(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "XC6SLX100-CSG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX100-CSG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 100 XC6SLX100-CSG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX100-CSG484_1_1"
			(pin bidirectional line
				(at -50.8 132.08 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 129.54 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L15P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L15N_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L16P_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L16N_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L46P_0")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L46N_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A18")
			)
			(pin power_in line
				(at -40.64 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B7")
			)
			(pin power_in line
				(at -35.56 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B11")
			)
			(pin power_in line
				(at -33.02 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -30.48 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E9")
			)
			(pin power_in line
				(at -27.94 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E13")
			)
			(pin power_in line
				(at -25.4 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -22.86 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at 10.16 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AA19")
			)
			(pin power_in line
				(at 12.7 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "B19")
			)
			(pin power_in line
				(at 15.24 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 17.78 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 20.32 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G14")
			)
			(pin power_in line
				(at 22.86 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 132.08 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 129.54 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L9P_1")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L9N_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L10P_1")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L10N_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L11P_1")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L11N_1")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L12P_1")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L12N_1")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L13P_1")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L13N_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L14P_1")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L14N_1")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L15P_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L15N_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L16P_1")
				(number "A19")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L16N_1")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L17P_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L17N_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L18P_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L18N_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21P_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L21N_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J21")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "AB21")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "AA21")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "Y19")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "R15")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -144.78 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -147.32 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -149.86 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "T20")
			)
		)
		(symbol "XC6SLX100-CSG484_2_1"
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L33P_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L33N_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L34P_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L34N_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AB5")
			)
			(pin power_in line
				(at -40.64 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -35.56 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -33.02 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -30.48 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -27.94 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -25.4 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -22.86 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at 10.16 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AA3")
			)
			(pin power_in line
				(at 12.7 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 15.24 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 17.78 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F6")
			)
			(pin power_in line
				(at 20.32 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 22.86 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 27.94 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 30.48 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 33.02 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 35.56 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 38.1 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin power_in line
				(at 40.64 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "T7")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L12P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L12N_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L13P_3")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L13N_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19P_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L19N_3")
				(number "R8")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "T5")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L73P_3")
				(number "G8")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L73N_3")
				(number "G7")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L74P_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L74N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L75P_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L75N_3")
				(number "E5")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L80P_3")
				(number "F8")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L80N_3")
				(number "F7")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L81P_3")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L81N_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L82P_3")
				(number "E6")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L82N_3")
				(number "D5")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "A3")
			)
			(pin bidirectional line
				(at 50.8 -144.78 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "A2")
			)
		)
		(symbol "XC6SLX100-CSG484_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "E14")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "E16")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "D14")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "U16")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "W18")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "T15")
			)
		)
		(symbol "XC6SLX100-CSG484_4_1"
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "RFUSE")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VBATT")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VFS")
				(number "U19")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D18")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "J20")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX100-FGG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX100-FGG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 100 XC6SLX100-FGG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX100-FGG484_1_1"
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L14P_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L14N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L15P_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L15N_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L16P_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L16N_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L17P_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L17N_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L18P_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L18N_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L43P_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L43N_0")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L44P_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L44N_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L45P_0")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L45N_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L46P_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L46N_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D17")
			)
			(pin power_in line
				(at -40.64 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B7")
			)
			(pin power_in line
				(at -35.56 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B11")
			)
			(pin power_in line
				(at -33.02 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -30.48 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -27.94 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E13")
			)
			(pin power_in line
				(at -22.86 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -20.32 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -17.78 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G14")
			)
			(pin power_in line
				(at 17.78 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 20.32 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 22.86 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L9P_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L9N_1")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L10P_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L10N_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L21P_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21N_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "T20")
			)
		)
		(symbol "XC6SLX100-FGG484_2_1"
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "T18")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "T17")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "W18")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L7P_2")
				(number "T16")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L7N_2")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L8P_2")
				(number "U17")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L8N_2")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L9P_2")
				(number "V19")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L9N_2")
				(number "V18")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L10P_2")
				(number "R16")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L10N_2")
				(number "R15")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L11P_2")
				(number "V17")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L11N_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L21P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L21N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L57P_2")
				(number "AA4")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L57N_2")
				(number "AB4")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "Y3")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "AB3")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L59P_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L59N_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L60P_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L60N_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W4")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "Y4")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "U6")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "V5")
			)
			(pin bidirectional line
				(at -50.8 -111.76 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA2")
			)
			(pin bidirectional line
				(at -50.8 -114.3 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AB2")
			)
			(pin bidirectional line
				(at -50.8 -116.84 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -119.38 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "T5")
			)
			(pin power_in line
				(at -40.64 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA3")
			)
			(pin power_in line
				(at -38.1 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -35.56 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -33.02 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -30.48 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA19")
			)
			(pin power_in line
				(at -27.94 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -25.4 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -22.86 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -20.32 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -17.78 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at -15.24 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at 15.24 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 17.78 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 20.32 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F6")
			)
			(pin power_in line
				(at 22.86 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 25.4 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 27.94 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 30.48 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 33.02 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 35.56 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "D5")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L80P_3")
				(number "G7")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L80N_3")
				(number "F7")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L81P_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L81N_3")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L82P_3")
				(number "E5")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L82N_3")
				(number "E6")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "A2")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "B3")
			)
		)
		(symbol "XC6SLX100-FGG484_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "A19")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "C18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "G15")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "Y22")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "N15")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "Y20")
			)
		)
		(symbol "XC6SLX100-FGG484_4_1"
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "RFUSE")
				(number "P15")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VBATT")
				(number "R17")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VFS")
				(number "P16")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D18")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX100-FGG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX100-FGG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 100 XC6SLX100-FGG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX100-FGG676_1_1"
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L12P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L12N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L13P_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L13N_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L14P_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L14N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L15P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L15N_0")
				(number "E9")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L16P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L16N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L17P_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L17N_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L18P_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L18N_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L19P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L19N_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L22P_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L22N_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L23P_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L23N_0")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L24P_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L24N_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L26P_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L26N_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L31P_0")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L31N_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L43P_0")
				(number "J14")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L43N_0")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L44P_0")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L44N_0")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L46P_0")
				(number "D16")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L46N_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "E17")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "J15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "H15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L52P_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L52N_0")
				(number "C18")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L54P_0")
				(number "E19")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L54N_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L55P_0")
				(number "H16")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L55N_0")
				(number "G17")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L56P_0")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L56N_0")
				(number "C20")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L57P_0")
				(number "F18")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L57N_0")
				(number "E18")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L58P_0")
				(number "E20")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L58N_0")
				(number "D20")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L59P_0")
				(number "J17")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L59N_0")
				(number "H17")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 -111.76 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 -114.3 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -116.84 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 -119.38 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A21")
			)
			(pin bidirectional line
				(at -50.8 -121.92 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 -124.46 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A22")
			)
			(pin power_in line
				(at -40.64 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B3")
			)
			(pin power_in line
				(at -38.1 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B7")
			)
			(pin power_in line
				(at -35.56 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B11")
			)
			(pin power_in line
				(at -33.02 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -30.48 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -27.94 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C22")
			)
			(pin power_in line
				(at -25.4 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D9")
			)
			(pin power_in line
				(at -22.86 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D17")
			)
			(pin power_in line
				(at -20.32 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E13")
			)
			(pin power_in line
				(at -17.78 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -15.24 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G18")
			)
			(pin power_in line
				(at -12.7 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H14")
			)
			(pin power_in line
				(at 20.32 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AB23")
			)
			(pin power_in line
				(at 22.86 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AD25")
			)
			(pin power_in line
				(at 25.4 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M20")
			)
			(pin power_in line
				(at 27.94 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "P23")
			)
			(pin power_in line
				(at 30.48 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "T25")
			)
			(pin power_in line
				(at 33.02 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 35.56 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "V21")
			)
			(pin power_in line
				(at 38.1 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W23")
			)
			(pin power_in line
				(at 40.64 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "L23")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "R24")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "V23")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "W24")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "U25")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "U26")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "W25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "W26")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "V24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "V26")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "Y24")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "AD24")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "AB24")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "AB26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "AC25")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "AC26")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "AA25")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "AA26")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "AE25")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "U24")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L55P_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L55N_1")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L56P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L56N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L57P_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L57N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "U23")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "U21")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "AA23")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "AA24")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AC23")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AC24")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "AE24")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "AF25")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "W18")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "W19")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L69P_1")
				(number "AB21")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L69N_VREF_1")
				(number "AB22")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "AE23")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "AF24")
			)
		)
		(symbol "XC6SLX100-FGG676_2_1"
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AF21")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AD20")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AF20")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AE19")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AF19")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "AC20")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "AA19")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L7P_2")
				(number "AC19")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L7N_2")
				(number "AD19")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L8P_2")
				(number "V16")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L8N_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L9P_2")
				(number "AD18")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L9N_2")
				(number "AF18")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L10P_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L10N_2")
				(number "AA17")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L11P_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L11N_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "AE17")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "AF17")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "AD16")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AF16")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AE15")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AF15")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AC17")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "AC15")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AD15")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "AC16")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "AD17")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "W16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AC14")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "AA15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L28P_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L28N_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "AD14")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "AF14")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AC13")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AD13")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AD12")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L33P_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L33N_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L34P_2")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L34N_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "V14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "AA11")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "V12")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AF11")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "AE9")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AD10")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L51P_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L51N_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L52P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L52N_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L53P_2")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L53N_2")
				(number "AF8")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L61P_2")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L61N_VREF_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "AE7")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AD6")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AF6")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AE5")
			)
			(pin bidirectional line
				(at -50.8 -111.76 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AF5")
			)
			(pin bidirectional line
				(at -50.8 -114.3 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "AE4")
			)
			(pin bidirectional line
				(at -50.8 -116.84 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AF4")
			)
			(pin power_in line
				(at -40.64 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AB14")
			)
			(pin power_in line
				(at -38.1 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC10")
			)
			(pin power_in line
				(at -35.56 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC18")
			)
			(pin power_in line
				(at -33.02 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC21")
			)
			(pin power_in line
				(at -30.48 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE8")
			)
			(pin power_in line
				(at -27.94 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE12")
			)
			(pin power_in line
				(at -25.4 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE16")
			)
			(pin power_in line
				(at -22.86 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE20")
			)
			(pin power_in line
				(at -20.32 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y12")
			)
			(pin power_in line
				(at -17.78 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y17")
			)
			(pin power_in line
				(at 17.78 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AC6")
			)
			(pin power_in line
				(at 20.32 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AD2")
			)
			(pin power_in line
				(at 22.86 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P4")
			)
			(pin power_in line
				(at 27.94 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P9")
			)
			(pin power_in line
				(at 30.48 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T2")
			)
			(pin power_in line
				(at 33.02 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T7")
			)
			(pin power_in line
				(at 35.56 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W4")
			)
			(pin power_in line
				(at 38.1 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W6")
			)
			(pin power_in line
				(at 40.64 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AC7")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AD7")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L3P_3")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L3N_3")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L4P_3")
				(number "AA8")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L4N_3")
				(number "AB8")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "AA7")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "AB7")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "Y9")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "Y8")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "AC5")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "AD5")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L15P_3")
				(number "W8")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L15N_3")
				(number "W7")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L16P_3")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L16N_3")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L17P_3")
				(number "V7")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L17N_VREF_3")
				(number "V6")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L19P_3")
				(number "W9")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L19N_3")
				(number "V8")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "W10")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "V10")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "T10")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "U9")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L27P_3")
				(number "R10")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L27N_3")
				(number "T9")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L28P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L28N_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L29P_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L29N_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L30P_3")
				(number "R5")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L30N_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "N8")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "P10")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "N5")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "M10")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "N9")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "M9")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "L7")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "L6")
			)
		)
		(symbol "XC6SLX100-FGG676_3_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L58P_4")
				(number "K8")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L58N_VREF_4")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L59P_M4DQ14_4")
				(number "N2")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L59N_M4DQ15_4")
				(number "N1")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L60P_M4DQ12_4")
				(number "M3")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L60N_M4DQ13_4")
				(number "M1")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L61P_M4UDQS_4")
				(number "L2")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L61N_M4UDQSN_4")
				(number "L1")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62P_M4DQ10_4")
				(number "K3")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L62N_M4DQ11_4")
				(number "K1")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63P_M4DQ8_4")
				(number "J2")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L63N_M4DQ9_4")
				(number "J1")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64P_M4DQ0_4")
				(number "H3")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L64N_M4DQ1_4")
				(number "H1")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65P_M4DQ2_4")
				(number "G2")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L65N_M4DQ3_4")
				(number "G1")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66P_M4LDQS_4")
				(number "F3")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L66N_M4LDQSN_4")
				(number "F1")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L67P_M4DQ6_4")
				(number "E2")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L67N_M4DQ7_4")
				(number "E1")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L68P_M4DQ4_4")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L68N_M4DQ5_4")
				(number "D1")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L69P_M4UDM_4")
				(number "J4")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L69N_M4LDM_4")
				(number "J3")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L70P_M4RASN_4")
				(number "K7")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L70N_M4CASN_4")
				(number "K6")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L71P_M4A5_4")
				(number "K5")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L71N_M4A6_4")
				(number "J5")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L72P_M4A3_4")
				(number "J7")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L72N_M4ODT_4")
				(number "H7")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L73P_M4CLK_4")
				(number "G4")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L73N_M4CLKN_4")
				(number "G3")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L74P_M4A0_4")
				(number "K10")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L74N_M4A1_4")
				(number "L9")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L75P_M4BA0_4")
				(number "H6")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L75N_M4BA1_4")
				(number "H5")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L76P_M4A7_4")
				(number "J10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L76N_M4A2_4")
				(number "K9")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L77P_M4WE_4")
				(number "E4")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L77N_M4BA2_4")
				(number "E3")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L78P_M4A10_4")
				(number "G6")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L78N_M4A4_4")
				(number "G5")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L79P_M4A8_4")
				(number "C2")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L79N_M4A9_4")
				(number "C1")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L80P_M4CKE_4")
				(number "F5")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L80N_M4A12_4")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L81P_M4RESET_4")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L81N_M4A11_4")
				(number "B1")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L82P_M4A13_4")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L82N_M4A14_4")
				(number "G7")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L83P_4")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L83N_VREF_4")
				(number "C3")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "D2")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "F4")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "H2")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "J6")
			)
			(pin power_in line
				(at -30.48 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "K4")
			)
			(pin power_in line
				(at -27.94 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "M2")
			)
			(pin power_in line
				(at 27.94 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "D25")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "F23")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "H25")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "J21")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "K23")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_A25_5")
				(number "B23")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_5")
				(number "A23")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L2P_M5A13_5")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L2N_M5A14_5")
				(number "G21")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L3P_M5RESET_5")
				(number "D23")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L3N_M5A11_5")
				(number "C24")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L4P_M5CKE_5")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L4N_M5A12_5")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L5P_M5A8_5")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L5N_M5A9_5")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L6P_M5A10_5")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L6N_M5A4_5")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L7P_M5WE_5")
				(number "E23")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L7N_M5BA2_5")
				(number "E24")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L8P_M5A7_5")
				(number "G23")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L8N_M5A2_5")
				(number "G24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L9P_M5BA0_5")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L9N_M5BA1_5")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L10P_M5A0_5")
				(number "B24")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L10N_M5A1_5")
				(number "A25")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L11P_M5CLK_5")
				(number "C25")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L11N_M5CLKN_5")
				(number "C26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L12P_M5A3_5")
				(number "B25")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L12N_M5ODT_5")
				(number "B26")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L13P_M5A5_5")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L13N_M5A6_5")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L14P_M5RASN_5")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L14N_M5CASN_5")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L15P_M5UDM_5")
				(number "J23")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L15N_M5LDM_5")
				(number "J24")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L16P_M5DQ4_5")
				(number "E25")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L16N_M5DQ5_5")
				(number "E26")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L17P_M5DQ6_5")
				(number "D24")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L17N_M5DQ7_5")
				(number "D26")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L18P_M5LDQS_5")
				(number "F24")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L18N_M5LDQSN_5")
				(number "F26")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L19P_M5DQ2_5")
				(number "H24")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L19N_M5DQ3_5")
				(number "H26")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L20P_M5DQ0_5")
				(number "G25")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L20N_M5DQ1_5")
				(number "G26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L21P_M5DQ8_5")
				(number "K24")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L21N_M5DQ9_5")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L22P_M5DQ10_5")
				(number "J25")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L22N_M5DQ11_5")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L23P_M5UDQS_5")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L23N_M5UDQSN_5")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L24P_M5DQ12_5")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L24N_M5DQ13_5")
				(number "L26")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L25P_M5DQ14_5")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L25N_M5DQ15_5")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L26P_5")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L26N_VREF_5")
				(number "L21")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L27P_5")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L27N_5")
				(number "J20")
			)
		)
		(symbol "XC6SLX100-FGG676_4_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "F20")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "A24")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "C23")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "E21")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AF23")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AF3")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "AD23")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "AC22")
			)
		)
		(symbol "XC6SLX100-FGG676_5_1"
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F6")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F21")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G15")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J18")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L22")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M17")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N10")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U6")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U14")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "Y19")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA6")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA10")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA16")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA21")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "RFUSE")
				(number "AA20")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VBATT")
				(number "W21")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VFS")
				(number "AB19")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B21")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F2")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F19")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "F25")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H11")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J19")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "K2")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "K16")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "K25")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "L15")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "M5")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "M16")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "M22")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "N15")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "P2")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "L16")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "R16")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "U16")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "P19")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T5")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "V2")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "W15")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "W20")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "Y7")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "Y11")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "Y23")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AB2")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AB12")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AB16")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AB20")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AB25")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AC8")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AE6")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AE10")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AE14")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AE18")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AF26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX100T-CSG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX100T-CSG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 100 XC6SLX100T-CSG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX100T-CSG484_1_1"
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "G7")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "C18")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D20")
			)
			(pin power_in line
				(at -40.64 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -35.56 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E10")
			)
			(pin power_in line
				(at -33.02 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -30.48 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F6")
			)
			(pin power_in line
				(at -27.94 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H8")
			)
			(pin power_in line
				(at 12.7 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AA19")
			)
			(pin power_in line
				(at 15.24 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 17.78 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 20.32 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 22.86 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 25.4 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 27.94 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 30.48 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 33.02 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R15")
			)
			(pin power_in line
				(at 35.56 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L15P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L15N_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L16P_1")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L16N_1")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L17P_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L17N_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L18P_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L18N_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "AA21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "R12")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "R13")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "T12")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "T13")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "AB21")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "Y19")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "T15")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "T20")
			)
		)
		(symbol "XC6SLX100T-CSG484_2_1"
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AB5")
			)
			(pin power_in line
				(at -40.64 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -35.56 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -33.02 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U14")
			)
			(pin power_in line
				(at -30.48 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -27.94 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -25.4 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at -22.86 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W16")
			)
			(pin power_in line
				(at 10.16 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AA3")
			)
			(pin power_in line
				(at 12.7 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 15.24 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 17.78 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 20.32 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 22.86 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 25.4 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 27.94 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 30.48 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 33.02 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R7")
			)
			(pin power_in line
				(at 35.56 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T9")
			)
			(pin power_in line
				(at 38.1 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "V11")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "U10")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L12P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L12N_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L13P_3")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L13N_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "T5")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "T7")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "U9")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "T11")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "T10")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "R8")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L69P_3")
				(number "A3")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L69N_3")
				(number "A2")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L70P_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L70N_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L71P_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L71N_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L72P_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L72N_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L73P_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L73N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L74P_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L74N_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L75P_3")
				(number "D4")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L75N_3")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "D3")
			)
		)
		(symbol "XC6SLX100T-CSG484_3_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C9")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "A10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "D11")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "C11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B14")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A14")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B16")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A16")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D13")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C13")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C15")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "B12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "A12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "F14")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "E14")
			)
		)
		(symbol "XC6SLX100T-CSG484_4_1"
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B9")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "D12")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C10")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "B13")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "E13")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "E15")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A7")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E11")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D14")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A15")
			)
		)
		(symbol "XC6SLX100T-CSG484_5_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "F17")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "H16")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "C19")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "U16")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "W18")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "U12")
			)
		)
		(symbol "XC6SLX100T-CSG484_6_1"
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F18")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R11")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "RFUSE")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VBATT")
				(number "R14")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VFS")
				(number "U19")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B15")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "E12")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "F15")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "G14")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "V16")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX100T-FGG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX100T-FGG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 100 XC6SLX100T-FGG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX100T-FGG484_1_1"
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "C3")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "D4")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "C18")
			)
			(pin power_in line
				(at -40.64 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -35.56 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -33.02 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F6")
			)
			(pin power_in line
				(at -30.48 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -27.94 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G14")
			)
			(pin power_in line
				(at 17.78 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 20.32 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 22.86 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L9P_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L9N_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L10P_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L10N_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L21P_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21N_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "R15")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "V20")
			)
		)
		(symbol "XC6SLX100T-FGG484_2_1"
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "V17")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "W18")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L21P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L21N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L22P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L22N_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L57P_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L57N_2")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L59P_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L59N_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L60P_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L60N_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "AB5")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AA4")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AB4")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "U6")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "Y4")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AA3")
			)
			(pin power_in line
				(at -40.64 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -35.56 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -33.02 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA19")
			)
			(pin power_in line
				(at -30.48 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AB3")
			)
			(pin power_in line
				(at -27.94 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -25.4 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -22.86 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -20.32 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -17.78 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at -15.24 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at 17.78 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 20.32 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 22.86 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 25.4 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 27.94 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 30.48 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 33.02 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 35.56 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "T5")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L80P_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L80N_3")
				(number "G7")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L81P_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L81N_3")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L82P_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L82N_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "B1")
			)
		)
		(symbol "XC6SLX100T-FGG484_3_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C9")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "A10")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "C11")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "D11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B14")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A14")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B16")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A16")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D13")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C13")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C15")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "A12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "B12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "E12")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "F12")
			)
		)
		(symbol "XC6SLX100T-FGG484_4_1"
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B9")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "D12")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C10")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "B13")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "E13")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "E10")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A7")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E8")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D14")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A15")
			)
		)
		(symbol "XC6SLX100T-FGG484_5_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "G17")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "D20")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A21")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AB2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "AA22")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "V18")
			)
		)
		(symbol "XC6SLX100T-FGG484_6_1"
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "RFUSE")
				(number "P15")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VBATT")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VFS")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B15")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX100T-FGG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX100T-FGG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 100 XC6SLX100T-FGG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX100T-FGG676_1_1"
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "H7")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "G7")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "F6")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "C3")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "G6")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "F5")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L13P_0")
				(number "H9")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L13N_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L14P_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L14N_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L15P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L15N_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L16P_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L16N_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L21P_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L21N_0")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L22P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L22N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L23P_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L23N_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L24P_0")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L24N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "K12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "J12")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L43P_0")
				(number "J15")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L43N_0")
				(number "H15")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "J16")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "J17")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "F18")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "E18")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L56P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L56N_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L57P_0")
				(number "F20")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L57N_0")
				(number "E20")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L58P_0")
				(number "H17")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L58N_0")
				(number "G17")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L59P_0")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L59N_0")
				(number "B21")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "H18")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "H19")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "G19")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "F19")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B23")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D22")
			)
			(pin power_in line
				(at -40.64 99.06 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B13")
			)
			(pin power_in line
				(at -38.1 99.06 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C4")
			)
			(pin power_in line
				(at -35.56 99.06 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C22")
			)
			(pin power_in line
				(at -33.02 99.06 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E21")
			)
			(pin power_in line
				(at -30.48 99.06 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F8")
			)
			(pin power_in line
				(at -27.94 99.06 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 99.06 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G18")
			)
			(pin power_in line
				(at -22.86 99.06 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H11")
			)
			(pin power_in line
				(at -20.32 99.06 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H16")
			)
			(pin power_in line
				(at -17.78 99.06 270)
				(length 6.35)
				(name "VCCO_0")
				(number "J14")
			)
			(pin power_in line
				(at 22.86 99.06 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AB23")
			)
			(pin power_in line
				(at 25.4 99.06 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AD25")
			)
			(pin power_in line
				(at 27.94 99.06 270)
				(length 6.35)
				(name "VCCO_1")
				(number "P18")
			)
			(pin power_in line
				(at 30.48 99.06 270)
				(length 6.35)
				(name "VCCO_1")
				(number "P23")
			)
			(pin power_in line
				(at 33.02 99.06 270)
				(length 6.35)
				(name "VCCO_1")
				(number "T25")
			)
			(pin power_in line
				(at 35.56 99.06 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin power_in line
				(at 38.1 99.06 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W23")
			)
			(pin power_in line
				(at 40.64 99.06 270)
				(length 6.35)
				(name "VCCO_1")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "L23")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "R24")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "U23")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "U24")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "V23")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "W24")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "U25")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "U26")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "V24")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "V26")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "W25")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "W26")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "AA25")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "AA26")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "AD24")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "AB24")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "AB26")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "AC25")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "AC26")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "Y24")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "AE25")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "U21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "AA23")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "AA24")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L69P_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L69N_VREF_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "AC23")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "AC24")
			)
		)
		(symbol "XC6SLX100T-FGG676_2_1"
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "AE24")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AF24")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "W20")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "V18")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "W19")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "W18")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AA17")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "V16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "AA19")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "W16")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L28P_2")
				(number "AA15")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L28N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "AE15")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "AF15")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AC14")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AD14")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AF14")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L33P_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L33N_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L34P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L34N_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AA11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "V10")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AD6")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AF6")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L51P_2")
				(number "AE5")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L51N_2")
				(number "AF5")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L52P_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L52N_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L53P_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L53N_2")
				(number "AC6")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L61P_2")
				(number "AC5")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L61N_VREF_2")
				(number "AD5")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "W7")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AD4")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AF4")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA7")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "AE3")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AF3")
			)
			(pin power_in line
				(at -40.64 99.06 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA14")
			)
			(pin power_in line
				(at -38.1 99.06 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA20")
			)
			(pin power_in line
				(at -35.56 99.06 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AB6")
			)
			(pin power_in line
				(at -33.02 99.06 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE4")
			)
			(pin power_in line
				(at -30.48 99.06 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE14")
			)
			(pin power_in line
				(at -27.94 99.06 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE23")
			)
			(pin power_in line
				(at -25.4 99.06 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W11")
			)
			(pin power_in line
				(at -22.86 99.06 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W15")
			)
			(pin power_in line
				(at -20.32 99.06 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y8")
			)
			(pin power_in line
				(at -17.78 99.06 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y18")
			)
			(pin power_in line
				(at 22.86 99.06 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AD2")
			)
			(pin power_in line
				(at 25.4 99.06 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P4")
			)
			(pin power_in line
				(at 27.94 99.06 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P9")
			)
			(pin power_in line
				(at 30.48 99.06 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T2")
			)
			(pin power_in line
				(at 33.02 99.06 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T7")
			)
			(pin power_in line
				(at 35.56 99.06 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W4")
			)
			(pin power_in line
				(at 38.1 99.06 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W6")
			)
			(pin power_in line
				(at 40.64 99.06 270)
				(length 6.35)
				(name "VCCO_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "V7")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "V6")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L17P_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L17N_VREF_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "U9")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "R8")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "R10")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "T9")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "R5")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "N8")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "N5")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "P10")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "N9")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "M10")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "M9")
			)
		)
		(symbol "XC6SLX100T-FGG676_3_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L58P_4")
				(number "M4")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L58N_VREF_4")
				(number "N3")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L59P_M4DQ14_4")
				(number "N2")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L59N_M4DQ15_4")
				(number "N1")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L60P_M4DQ12_4")
				(number "M3")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L60N_M4DQ13_4")
				(number "M1")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L61P_M4UDQS_4")
				(number "L2")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L61N_M4UDQSN_4")
				(number "L1")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62P_M4DQ10_4")
				(number "K3")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L62N_M4DQ11_4")
				(number "K1")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63P_M4DQ8_4")
				(number "J2")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L63N_M4DQ9_4")
				(number "J1")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64P_M4DQ0_4")
				(number "H3")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L64N_M4DQ1_4")
				(number "H1")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65P_M4DQ2_4")
				(number "G2")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L65N_M4DQ3_4")
				(number "G1")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66P_M4LDQS_4")
				(number "F3")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L66N_M4LDQSN_4")
				(number "F1")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L67P_M4DQ6_4")
				(number "E2")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L67N_M4DQ7_4")
				(number "E1")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L68P_M4DQ4_4")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L68N_M4DQ5_4")
				(number "D1")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L69P_M4UDM_4")
				(number "J4")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L69N_M4LDM_4")
				(number "J3")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L70P_M4RASN_4")
				(number "L9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L70N_M4CASN_4")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L71P_M4A5_4")
				(number "L4")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L71N_M4A6_4")
				(number "L3")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L72P_M4A3_4")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L72N_M4ODT_4")
				(number "M6")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L73P_M4CLK_4")
				(number "K5")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L73N_M4CLKN_4")
				(number "J5")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L74P_M4A0_4")
				(number "L7")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L74N_M4A1_4")
				(number "L6")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L75P_M4BA0_4")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L75N_M4BA1_4")
				(number "B1")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L76P_M4A7_4")
				(number "L10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L76N_M4A2_4")
				(number "K10")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L77P_M4WE_4")
				(number "G4")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L77N_M4BA2_4")
				(number "G3")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L78P_M4A10_4")
				(number "J9")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L78N_M4A4_4")
				(number "J7")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L79P_M4A8_4")
				(number "C2")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L79N_M4A9_4")
				(number "C1")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L80P_M4CKE_4")
				(number "K9")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L80N_M4A12_4")
				(number "K8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L81P_M4RESET_4")
				(number "E4")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L81N_M4A11_4")
				(number "E3")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L82P_M4A13_4")
				(number "K7")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L82N_M4A14_4")
				(number "K6")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L83P_4")
				(number "H6")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L83N_VREF_4")
				(number "H5")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "D2")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "F4")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "H2")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "J6")
			)
			(pin power_in line
				(at -30.48 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "K4")
			)
			(pin power_in line
				(at -27.94 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "M2")
			)
			(pin power_in line
				(at -25.4 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "D25")
			)
			(pin power_in line
				(at 27.94 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "G22")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "H25")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "J21")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "K23")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "M20")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_A25_5")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_5")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L2P_M5A13_5")
				(number "B24")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L2N_M5A14_5")
				(number "A25")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L3P_M5RESET_5")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L3N_M5A11_5")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L4P_M5CKE_5")
				(number "D23")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L4N_M5A12_5")
				(number "C24")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L5P_M5A8_5")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L5N_M5A9_5")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L6P_M5A10_5")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L6N_M5A4_5")
				(number "G23")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L7P_M5WE_5")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L7N_M5BA2_5")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L8P_M5A7_5")
				(number "E23")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L8N_M5A2_5")
				(number "E24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L9P_M5BA0_5")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L9N_M5BA1_5")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L10P_M5A0_5")
				(number "C25")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L10N_M5A1_5")
				(number "C26")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L11P_M5CLK_5")
				(number "B25")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L11N_M5CLKN_5")
				(number "B26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L12P_M5A3_5")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L12N_M5ODT_5")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L13P_M5A5_5")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L13N_M5A6_5")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L14P_M5RASN_5")
				(number "F23")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L14N_M5CASN_5")
				(number "G24")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L15P_M5UDM_5")
				(number "J23")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L15N_M5LDM_5")
				(number "J24")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L16P_M5DQ4_5")
				(number "E25")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L16N_M5DQ5_5")
				(number "E26")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L17P_M5DQ6_5")
				(number "D24")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L17N_M5DQ7_5")
				(number "D26")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L18P_M5LDQS_5")
				(number "F24")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L18N_M5LDQSN_5")
				(number "F26")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L19P_M5DQ2_5")
				(number "H24")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L19N_M5DQ3_5")
				(number "H26")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L20P_M5DQ0_5")
				(number "G25")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L20N_M5DQ1_5")
				(number "G26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L21P_M5DQ8_5")
				(number "K24")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L21N_M5DQ9_5")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L22P_M5DQ10_5")
				(number "J25")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L22N_M5DQ11_5")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L23P_M5UDQS_5")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L23N_M5UDQSN_5")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L24P_M5DQ12_5")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L24N_M5DQ13_5")
				(number "L26")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L25P_M5DQ14_5")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L25N_M5DQ15_5")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L26P_5")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L26N_VREF_5")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L27P_5")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L27N_5")
				(number "L21")
			)
		)
		(symbol "XC6SLX100T-FGG676_4_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C9")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "A10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "D11")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "C11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B18")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A18")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B20")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A20")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D17")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C17")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D19")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C19")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "C15")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "B16")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "A16")
			)
		)
		(symbol "XC6SLX100T-FGG676_5_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_245")
				(number "AE7")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_245")
				(number "AF7")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_245")
				(number "AE9")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_245")
				(number "AF9")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_245")
				(number "AC8")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_245")
				(number "AD8")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_245")
				(number "AC10")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_245")
				(number "AD10")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_245")
				(number "AE11")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_245")
				(number "AF11")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_245")
				(number "AC12")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_245")
				(number "AD12")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_267")
				(number "AE19")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_267")
				(number "AF19")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_267")
				(number "AE21")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_267")
				(number "AF21")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_267")
				(number "AC18")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_267")
				(number "AD18")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_267")
				(number "AC20")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_267")
				(number "AD20")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_267")
				(number "AC16")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_267")
				(number "AD16")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_267")
				(number "AE17")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_267")
				(number "AF17")
			)
		)
		(symbol "XC6SLX100T-FGG676_6_1"
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B11")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "C12")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C10")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "C14")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "B15")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "C16")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_245")
				(number "AE12")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_245")
				(number "AD13")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_245")
				(number "AD11")
			)
			(pin power_in line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTAVCCPLL0_267")
				(number "AD15")
			)
			(pin power_in line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTAVCCPLL1_267")
				(number "AE16")
			)
			(pin power_in line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTAVCC_267")
				(number "AD17")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A7")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E11")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D18")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A19")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTTRX_245")
				(number "AC9")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_245")
				(number "AF8")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTRCAL_245")
				(number "AB12")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTRREF_245")
				(number "AB10")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTTRX_267")
				(number "AC19")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTTTX_267")
				(number "AF20")
			)
		)
		(symbol "XC6SLX100T-FGG676_7_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "C23")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "G21")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "F21")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A24")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AF25")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AF2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "Y22")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "Y19")
			)
		)
		(symbol "XC6SLX100T-FGG676_8_1"
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D20")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E17")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J10")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J18")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L18")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L22")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M17")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N10")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R22")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U6")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U12")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U14")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U18")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V17")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "W13")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA5")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB8")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB18")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC7")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC21")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "RFUSE")
				(number "V19")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VBATT")
				(number "V22")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VFS")
				(number "W22")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A15")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A17")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A21")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "B19")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C18")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "C20")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "D12")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "D14")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "E19")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "F2")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "F25")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "G14")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J19")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "K2")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K16")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K25")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "L15")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "L17")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "M5")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "M22")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "P2")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "P7")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "L16")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "M16")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "R16")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "R17")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "U16")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "P20")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "T5")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "T10")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "T18")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "U17")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "V2")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "V8")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "Y7")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "Y10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "Y14")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "Y23")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AB2")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AB16")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AB20")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AB25")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AC11")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AC13")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AC15")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AC17")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AD9")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AD19")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AD21")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AE6")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AE8")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AE10")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AE18")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AE20")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AF10")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AF12")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AF16")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AF18")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AF26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX100T-FGG900"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX100T-FGG900"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 100 XC6SLX100T-FGG900"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX100T-FGG900_1_1"
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "H9")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "F6")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "J8")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "H7")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "G7")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "E7")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "M10")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "L10")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L9P_0")
				(number "K10")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L9N_0")
				(number "J10")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L10P_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L10N_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L11P_0")
				(number "L11")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L11N_0")
				(number "K11")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L13P_0")
				(number "B7")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L13N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L15P_0")
				(number "L12")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L15N_0")
				(number "K12")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L17P_0")
				(number "J12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L17N_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L19P_0")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L19N_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L20P_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L20N_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L21P_0")
				(number "M13")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L21N_0")
				(number "L13")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L23P_0")
				(number "L14")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L23N_0")
				(number "K14")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L25P_0")
				(number "M15")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L25N_0")
				(number "K15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "J14")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "E15")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "H15")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "D16")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "B17")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L43P_0")
				(number "L17")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L43N_0")
				(number "K17")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L44P_0")
				(number "H17")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L44N_0")
				(number "G17")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L45P_0")
				(number "H16")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L45N_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L46P_0")
				(number "G18")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L46N_0")
				(number "F18")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "M18")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "L18")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "K19")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "J19")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "F19")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "E19")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "M19")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "L19")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L52P_0")
				(number "H19")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L52N_0")
				(number "G19")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L53P_0")
				(number "J18")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L53N_0")
				(number "H18")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L54P_0")
				(number "G20")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L54N_0")
				(number "F20")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L55P_0")
				(number "K20")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L55N_0")
				(number "J20")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L59P_0")
				(number "L21")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L59N_0")
				(number "K21")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L60P_0")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L60N_0")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L61P_0")
				(number "H21")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L61N_0")
				(number "G21")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "F24")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "E24")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 -111.76 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 -114.3 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "J22")
			)
			(pin bidirectional line
				(at -50.8 -116.84 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "H22")
			)
			(pin bidirectional line
				(at -50.8 -119.38 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "E25")
			)
			(pin bidirectional line
				(at -50.8 -121.92 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D25")
			)
			(pin power_in line
				(at -40.64 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B16")
			)
			(pin power_in line
				(at -38.1 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C7")
			)
			(pin power_in line
				(at -35.56 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C25")
			)
			(pin power_in line
				(at -33.02 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F16")
			)
			(pin power_in line
				(at -30.48 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G8")
			)
			(pin power_in line
				(at -27.94 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G23")
			)
			(pin power_in line
				(at -22.86 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H10")
			)
			(pin power_in line
				(at -20.32 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H20")
			)
			(pin power_in line
				(at -17.78 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "J17")
			)
			(pin power_in line
				(at -15.24 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "K13")
			)
			(pin power_in line
				(at -12.7 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "L9")
			)
			(pin power_in line
				(at -10.16 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "L15")
			)
			(pin power_in line
				(at -7.62 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "M17")
			)
			(pin power_in line
				(at -5.08 129.54 270)
				(length 6.35)
				(name "VCCO_0")
				(number "M21")
			)
			(pin power_in line
				(at 7.62 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AA23")
			)
			(pin power_in line
				(at 10.16 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AC26")
			)
			(pin power_in line
				(at 12.7 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AD29")
			)
			(pin power_in line
				(at 15.24 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AH29")
			)
			(pin power_in line
				(at 17.78 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AJ27")
			)
			(pin power_in line
				(at 20.32 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N23")
			)
			(pin power_in line
				(at 22.86 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "P21")
			)
			(pin power_in line
				(at 25.4 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R23")
			)
			(pin power_in line
				(at 27.94 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R26")
			)
			(pin power_in line
				(at 30.48 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "T29")
			)
			(pin power_in line
				(at 33.02 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U23")
			)
			(pin power_in line
				(at 35.56 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W23")
			)
			(pin power_in line
				(at 38.1 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W26")
			)
			(pin power_in line
				(at 40.64 129.54 270)
				(length 6.35)
				(name "VCCO_1")
				(number "Y29")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "N29")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "N30")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "N27")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "N28")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "P28")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "P30")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "P27")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "R29")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "R30")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "R27")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "R28")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "T27")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "T28")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "T30")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "U29")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "U30")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "U27")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "U28")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "V28")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "V30")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "V26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "V27")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "W27")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "W28")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "AB28")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "AB30")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "W29")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "W30")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "Y28")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "Y30")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "AA29")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "AA30")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "AA27")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "AA28")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "Y27")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "AD28")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "AD30")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "AC27")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "AC28")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "AC29")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "AC30")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "AE29")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "AE30")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "AE27")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "AE28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "W24")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "W25")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L54P_1")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L54N_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L55P_1")
				(number "AF28")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L55N_1")
				(number "AF30")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L56P_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L56N_1")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L57P_1")
				(number "AG29")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L57N_1")
				(number "AG30")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "P25")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "AH30")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "AJ30")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "R24")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "AJ29")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "AK29")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "T25")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "AJ28")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "AK28")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "U24")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "U25")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AG27")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AG28")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "V23")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "V24")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "AD27")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L69P_1")
				(number "AH27")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L69N_VREF_1")
				(number "AK27")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "Y23")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "AE25")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "Y24")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "AG26")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "AH26")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "AA24")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "AA25")
			)
		)
		(symbol "XC6SLX100T-FGG900_2_1"
			(pin bidirectional line
				(at -50.8 134.62 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "AJ26")
			)
			(pin bidirectional line
				(at -50.8 132.08 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AK26")
			)
			(pin bidirectional line
				(at -50.8 129.54 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AD24")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AJ25")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AK25")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AB23")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AC23")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "AE24")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AF24")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L7P_2")
				(number "AE23")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L7N_2")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L8P_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L8N_2")
				(number "AC21")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L9P_2")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L9N_2")
				(number "AE22")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L10P_2")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L10N_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L11P_2")
				(number "AF25")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L11N_2")
				(number "AG25")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "AC20")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "AG24")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AH24")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AC19")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AD19")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AF21")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "AD20")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "AE20")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "W20")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AE19")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AF19")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "AA19")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L28P_2")
				(number "AE17")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L28N_2")
				(number "AF17")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "AC16")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "AD16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AF16")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AG16")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AH16")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AK16")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AJ17")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AK17")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L33P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L33N_2")
				(number "AA17")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L34P_2")
				(number "AJ15")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L34N_2")
				(number "AK15")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AD14")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AE14")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "AE15")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AF15")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "AC15")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "AD15")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AD12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AE12")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "AA15")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AC13")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AF11")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L51P_2")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L51N_2")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L52P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L52N_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L57P_2")
				(number "AE9")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L57N_2")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L59P_2")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L59N_2")
				(number "AG7")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L61P_2")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L61N_VREF_2")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "AH7")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "AK7")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AG6")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AH6")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "AJ6")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AK6")
			)
			(pin power_in line
				(at -40.64 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA12")
			)
			(pin power_in line
				(at -38.1 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA16")
			)
			(pin power_in line
				(at -35.56 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA20")
			)
			(pin power_in line
				(at -33.02 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC10")
			)
			(pin power_in line
				(at -30.48 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC18")
			)
			(pin power_in line
				(at -27.94 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AD13")
			)
			(pin power_in line
				(at -25.4 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AD21")
			)
			(pin power_in line
				(at -22.86 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AD23")
			)
			(pin power_in line
				(at -20.32 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE16")
			)
			(pin power_in line
				(at -17.78 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AF8")
			)
			(pin power_in line
				(at -15.24 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AH25")
			)
			(pin power_in line
				(at -12.7 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AJ7")
			)
			(pin power_in line
				(at -10.16 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AJ16")
			)
			(pin power_in line
				(at 7.62 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AA8")
			)
			(pin power_in line
				(at 10.16 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AC2")
			)
			(pin power_in line
				(at 12.7 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AD5")
			)
			(pin power_in line
				(at 15.24 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AG2")
			)
			(pin power_in line
				(at 17.78 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AJ3")
			)
			(pin power_in line
				(at 20.32 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M8")
			)
			(pin power_in line
				(at 22.86 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 27.94 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R8")
			)
			(pin power_in line
				(at 30.48 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T5")
			)
			(pin power_in line
				(at 33.02 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U8")
			)
			(pin power_in line
				(at 35.56 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin power_in line
				(at 38.1 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "Y5")
			)
			(pin power_in line
				(at 40.64 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "Y10")
			)
			(pin bidirectional line
				(at 50.8 134.62 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AA10")
			)
			(pin bidirectional line
				(at 50.8 132.08 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AA9")
			)
			(pin bidirectional line
				(at 50.8 129.54 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "AD7")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "AE7")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L3P_3")
				(number "Y9")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L3N_3")
				(number "Y8")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L4P_3")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L4N_3")
				(number "AF6")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L5P_3")
				(number "W11")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L5N_3")
				(number "Y11")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L6P_3")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L6N_3")
				(number "AG5")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "T7")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "AA7")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AA6")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "AH5")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "AK5")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "W10")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "W9")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L12P_3")
				(number "AB7")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L12N_3")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L13P_3")
				(number "W7")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L13N_3")
				(number "W6")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L14P_3")
				(number "AJ4")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L14N_3")
				(number "AK4")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L15P_3")
				(number "T9")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L15N_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L16P_3")
				(number "AH3")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L16N_3")
				(number "AK3")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L17P_3")
				(number "Y7")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L17N_VREF_3")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "AJ2")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "AK2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L19P_3")
				(number "AE4")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L19N_3")
				(number "AF4")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "AG3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "V8")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "V7")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "AH1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "AJ1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "V10")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "V9")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "AG4")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "AH4")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "N10")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "N9")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "AH2")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L27P_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L27N_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L28P_3")
				(number "AF1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L28N_3")
				(number "AG1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L29P_3")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L29N_3")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L30P_3")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L30N_3")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "N8")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "AC5")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "AD2")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "R5")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "N5")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 -144.78 180)
				(length 6.35)
				(name "IO_L56P_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 -147.32 180)
				(length 6.35)
				(name "IO_L56N_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 -149.86 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 -152.4 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "M6")
			)
		)
		(symbol "XC6SLX100T-FGG900_3_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L58P_4")
				(number "L7")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L58N_VREF_4")
				(number "L6")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L59P_M4DQ14_4")
				(number "M2")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L59N_M4DQ15_4")
				(number "M1")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L60P_M4DQ12_4")
				(number "L3")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L60N_M4DQ13_4")
				(number "L1")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L61P_M4UDQS_4")
				(number "K2")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L61N_M4UDQSN_4")
				(number "K1")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62P_M4DQ10_4")
				(number "L5")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L62N_M4DQ11_4")
				(number "L4")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63P_M4DQ8_4")
				(number "M4")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L63N_M4DQ9_4")
				(number "M3")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64P_M4DQ0_4")
				(number "H4")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L64N_M4DQ1_4")
				(number "H3")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65P_M4DQ2_4")
				(number "J3")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L65N_M4DQ3_4")
				(number "J1")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66P_M4LDQS_4")
				(number "J5")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L66N_M4LDQSN_4")
				(number "J4")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L67P_M4DQ6_4")
				(number "H2")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L67N_M4DQ7_4")
				(number "H1")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L68P_M4DQ4_4")
				(number "G3")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L68N_M4DQ5_4")
				(number "G1")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L69P_M4UDM_4")
				(number "K4")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L69N_M4LDM_4")
				(number "K3")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L70P_M4RASN_4")
				(number "C1")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L70N_M4CASN_4")
				(number "B1")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L71P_M4A5_4")
				(number "F2")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L71N_M4A6_4")
				(number "F1")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L72P_M4A3_4")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L72N_M4ODT_4")
				(number "E4")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L73P_M4CLK_4")
				(number "E3")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L73N_M4CLKN_4")
				(number "E1")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L74P_M4A0_4")
				(number "D4")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L74N_M4A1_4")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L75P_M4BA0_4")
				(number "D2")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L75N_M4BA1_4")
				(number "D1")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L76P_M4A7_4")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L76N_M4A2_4")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L77P_M4WE_4")
				(number "F4")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L77N_M4BA2_4")
				(number "F3")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L78P_M4A10_4")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L78N_M4A4_4")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L79P_M4A8_4")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L79N_M4A9_4")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L80P_M4CKE_4")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L80N_M4A12_4")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L81P_M4RESET_4")
				(number "G5")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L81N_M4A11_4")
				(number "G4")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L82P_M4A13_4")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L82N_M4A14_4")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L83P_4")
				(number "J6")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L83N_VREF_4")
				(number "H6")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "C2")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "G2")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "H5")
			)
			(pin power_in line
				(at -30.48 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "K6")
			)
			(pin power_in line
				(at -27.94 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "L2")
			)
			(pin power_in line
				(at -25.4 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "M5")
			)
			(pin power_in line
				(at 22.86 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "B28")
			)
			(pin power_in line
				(at 25.4 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "D29")
			)
			(pin power_in line
				(at 27.94 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "G26")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "H29")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "J25")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "K24")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "L26")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "M29")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_A25_5")
				(number "G25")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_5")
				(number "F25")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L2P_M5A13_5")
				(number "A28")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L2N_M5A14_5")
				(number "A29")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L3P_M5RESET_5")
				(number "C26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L3N_M5A11_5")
				(number "A26")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L4P_M5CKE_5")
				(number "B29")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L4N_M5A12_5")
				(number "B30")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L5P_M5A8_5")
				(number "B27")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L5N_M5A9_5")
				(number "A27")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L6P_M5A10_5")
				(number "F26")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L6N_M5A4_5")
				(number "F27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L7P_M5WE_5")
				(number "E26")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L7N_M5BA2_5")
				(number "D26")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L8P_M5A7_5")
				(number "C29")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L8N_M5A2_5")
				(number "C30")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L9P_M5BA0_5")
				(number "D27")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L9N_M5BA1_5")
				(number "C27")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L10P_M5A0_5")
				(number "D28")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L10N_M5A1_5")
				(number "D30")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L11P_M5CLK_5")
				(number "E27")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L11N_M5CLKN_5")
				(number "E28")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L12P_M5A3_5")
				(number "E29")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L12N_M5ODT_5")
				(number "E30")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L13P_M5A5_5")
				(number "H26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L13N_M5A6_5")
				(number "H27")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L14P_M5RASN_5")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L14N_M5CASN_5")
				(number "K27")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L15P_M5UDM_5")
				(number "J27")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L15N_M5LDM_5")
				(number "J28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L16P_M5DQ4_5")
				(number "G27")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L16N_M5DQ5_5")
				(number "G28")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L17P_M5DQ6_5")
				(number "F28")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L17N_M5DQ7_5")
				(number "F30")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L18P_M5LDQS_5")
				(number "J29")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L18N_M5LDQSN_5")
				(number "J30")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L19P_M5DQ2_5")
				(number "G29")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L19N_M5DQ3_5")
				(number "G30")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L20P_M5DQ0_5")
				(number "H28")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L20N_M5DQ1_5")
				(number "H30")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L21P_M5DQ8_5")
				(number "L27")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L21N_M5DQ9_5")
				(number "L28")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L22P_M5DQ10_5")
				(number "L29")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L22N_M5DQ11_5")
				(number "L30")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L23P_M5UDQS_5")
				(number "K28")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L23N_M5UDQSN_5")
				(number "K30")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L24P_M5DQ12_5")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L24N_M5DQ13_5")
				(number "M27")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L25P_M5DQ14_5")
				(number "M28")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L25N_M5DQ15_5")
				(number "M30")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L26P_5")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L26N_VREF_5")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L27P_5")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L27N_5")
				(number "L25")
			)
		)
		(symbol "XC6SLX100T-FGG900_4_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B9")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A9")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B11")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A11")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D10")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C10")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D12")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C12")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "B13")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "A13")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "D14")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "C14")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B21")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A21")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B23")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A23")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D20")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C20")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D22")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C22")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "D18")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "C18")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "B19")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "A19")
			)
		)
		(symbol "XC6SLX100T-FGG900_5_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_245")
				(number "AJ9")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_245")
				(number "AK9")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_245")
				(number "AJ11")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_245")
				(number "AK11")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_245")
				(number "AG10")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_245")
				(number "AH10")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_245")
				(number "AG12")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_245")
				(number "AH12")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_245")
				(number "AJ13")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_245")
				(number "AK13")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_245")
				(number "AG14")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_245")
				(number "AH14")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_267")
				(number "AJ21")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_267")
				(number "AK21")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_267")
				(number "AJ23")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_267")
				(number "AK23")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_267")
				(number "AG20")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_267")
				(number "AH20")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_267")
				(number "AG22")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_267")
				(number "AH22")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_267")
				(number "AG18")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_267")
				(number "AH18")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_267")
				(number "AJ19")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_267")
				(number "AK19")
			)
		)
		(symbol "XC6SLX100T-FGG900_6_1"
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B14")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "C15")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C13")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "C17")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "B18")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "C19")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_245")
				(number "AJ14")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_245")
				(number "AH15")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_245")
				(number "AH13")
			)
			(pin power_in line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTAVCCPLL0_267")
				(number "AH17")
			)
			(pin power_in line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTAVCCPLL1_267")
				(number "AJ18")
			)
			(pin power_in line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTAVCC_267")
				(number "AH19")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D11")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A10")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E14")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E12")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D21")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A22")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTTRX_245")
				(number "AG11")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_245")
				(number "AK10")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTRCAL_245")
				(number "AF14")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTRREF_245")
				(number "AF12")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTTRX_267")
				(number "AG21")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTTTX_267")
				(number "AK22")
			)
		)
		(symbol "XC6SLX100T-FGG900_7_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "J24")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "H25")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "K25")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "H23")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AD25")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "AB25")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "AC25")
			)
		)
		(symbol "XC6SLX100T-FGG900_8_1"
			(pin power_in line
				(at -25.4 134.62 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D9")
			)
			(pin power_in line
				(at -25.4 132.08 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D23")
			)
			(pin power_in line
				(at -25.4 129.54 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G6")
			)
			(pin power_in line
				(at -25.4 127 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H24")
			)
			(pin power_in line
				(at -25.4 124.46 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J7")
			)
			(pin power_in line
				(at -25.4 121.92 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 119.38 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 116.84 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J23")
			)
			(pin power_in line
				(at -25.4 114.3 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L22")
			)
			(pin power_in line
				(at -25.4 111.76 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M11")
			)
			(pin power_in line
				(at -25.4 109.22 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M14")
			)
			(pin power_in line
				(at -25.4 106.68 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M25")
			)
			(pin power_in line
				(at -25.4 104.14 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N6")
			)
			(pin power_in line
				(at -25.4 101.6 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T21")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U10")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V21")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V25")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 6.35)
				(name "VCCAUX")
				(number "W13")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX")
				(number "W15")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX")
				(number "W17")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX")
				(number "Y18")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB24")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC7")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AG9")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AG23")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "RFUSE")
				(number "AB27")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VBATT")
				(number "AB26")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VFS")
				(number "AF27")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "A8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "A12")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "A14")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "A18")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "A20")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A24")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "A30")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "B8")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "B10")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "B12")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "B20")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "B22")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "B24")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "B26")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "C9")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "C11")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "C21")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "C23")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "C28")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D15")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D17")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D19")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E10")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "E18")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E20")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "F5")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "F29")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G24")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J16")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "J26")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "K5")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "K16")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "K18")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "K22")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K23")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K29")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "L16")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "L23")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "M16")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "M22")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "N18")
			)
			(pin power_in line
				(at -25.4 -101.6 0)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at -25.4 -104.14 0)
				(length 6.35)
				(name "GND")
				(number "N22")
			)
			(pin power_in line
				(at -25.4 -106.68 0)
				(length 6.35)
				(name "GND")
				(number "N26")
			)
			(pin power_in line
				(at -25.4 -109.22 0)
				(length 6.35)
				(name "GND")
				(number "P5")
			)
			(pin power_in line
				(at -25.4 -111.76 0)
				(length 6.35)
				(name "GND")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 -114.3 0)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 -116.84 0)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at -25.4 -119.38 0)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 -121.92 0)
				(length 6.35)
				(name "GND")
				(number "P17")
			)
			(pin power_in line
				(at -25.4 -124.46 0)
				(length 6.35)
				(name "GND")
				(number "P18")
			)
			(pin power_in line
				(at -25.4 -127 0)
				(length 6.35)
				(name "GND")
				(number "P20")
			)
			(pin power_in line
				(at -25.4 -129.54 0)
				(length 6.35)
				(name "GND")
				(number "P29")
			)
			(pin power_in line
				(at -25.4 -132.08 0)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 -134.62 0)
				(length 6.35)
				(name "GND")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 134.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 132.08 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 129.54 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 127 180)
				(length 6.35)
				(name "VCCINT")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 124.46 180)
				(length 6.35)
				(name "VCCINT")
				(number "N19")
			)
			(pin power_in line
				(at 25.4 121.92 180)
				(length 6.35)
				(name "VCCINT")
				(number "N20")
			)
			(pin power_in line
				(at 25.4 119.38 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 116.84 180)
				(length 6.35)
				(name "VCCINT")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 114.3 180)
				(length 6.35)
				(name "VCCINT")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 111.76 180)
				(length 6.35)
				(name "VCCINT")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 109.22 180)
				(length 6.35)
				(name "VCCINT")
				(number "P19")
			)
			(pin power_in line
				(at 25.4 106.68 180)
				(length 6.35)
				(name "VCCINT")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 104.14 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 101.6 180)
				(length 6.35)
				(name "VCCINT")
				(number "R17")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "T18")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "U15")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "U16")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "U19")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "U20")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "V11")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "V12")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "V15")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "V16")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "V19")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "V20")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "R16")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "R19")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "R20")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "T10")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "T19")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "T20")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "T22")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "T23")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "U9")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "U13")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "U17")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "U22")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "U26")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "V5")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "V13")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "V17")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "V22")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "V29")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "W8")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "W18")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AA26")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AB5")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AB15")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AB29")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AC8")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AC17")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AE2")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AF5")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AF10")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AF18")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AF20")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AF22")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AF26")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AF29")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AG13")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AG15")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AG17")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AG19")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AH9")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AH11")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AH21")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AH23")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AH28")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "AJ5")
			)
			(pin power_in line
				(at 25.4 -101.6 180)
				(length 6.35)
				(name "GND")
				(number "AJ8")
			)
			(pin power_in line
				(at 25.4 -104.14 180)
				(length 6.35)
				(name "GND")
				(number "AJ10")
			)
			(pin power_in line
				(at 25.4 -106.68 180)
				(length 6.35)
				(name "GND")
				(number "AJ12")
			)
			(pin power_in line
				(at 25.4 -109.22 180)
				(length 6.35)
				(name "GND")
				(number "AJ20")
			)
			(pin power_in line
				(at 25.4 -111.76 180)
				(length 6.35)
				(name "GND")
				(number "AJ22")
			)
			(pin power_in line
				(at 25.4 -114.3 180)
				(length 6.35)
				(name "GND")
				(number "AJ24")
			)
			(pin power_in line
				(at 25.4 -116.84 180)
				(length 6.35)
				(name "GND")
				(number "AK1")
			)
			(pin power_in line
				(at 25.4 -119.38 180)
				(length 6.35)
				(name "GND")
				(number "AK8")
			)
			(pin power_in line
				(at 25.4 -121.92 180)
				(length 6.35)
				(name "GND")
				(number "AK12")
			)
			(pin power_in line
				(at 25.4 -124.46 180)
				(length 6.35)
				(name "GND")
				(number "AK14")
			)
			(pin power_in line
				(at 25.4 -127 180)
				(length 6.35)
				(name "GND")
				(number "AK18")
			)
			(pin power_in line
				(at 25.4 -129.54 180)
				(length 6.35)
				(name "GND")
				(number "AK20")
			)
			(pin power_in line
				(at 25.4 -132.08 180)
				(length 6.35)
				(name "GND")
				(number "AK24")
			)
			(pin power_in line
				(at 25.4 -134.62 180)
				(length 6.35)
				(name "GND")
				(number "AK30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX150-CSG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX150-CSG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 150 XC6SLX150-CSG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX150-CSG484_1_1"
			(pin bidirectional line
				(at -50.8 132.08 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 129.54 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L15P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L15N_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L16P_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L16N_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L46P_0")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L46N_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A18")
			)
			(pin power_in line
				(at -40.64 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B7")
			)
			(pin power_in line
				(at -35.56 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B11")
			)
			(pin power_in line
				(at -33.02 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -30.48 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E9")
			)
			(pin power_in line
				(at -27.94 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E13")
			)
			(pin power_in line
				(at -25.4 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -22.86 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at 10.16 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AA19")
			)
			(pin power_in line
				(at 12.7 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "B19")
			)
			(pin power_in line
				(at 15.24 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 17.78 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 20.32 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G14")
			)
			(pin power_in line
				(at 22.86 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 132.08 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 129.54 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L9P_1")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L9N_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L10P_1")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L10N_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L11P_1")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L11N_1")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L12P_1")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L12N_1")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L13P_1")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L13N_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L14P_1")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L14N_1")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L15P_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L15N_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L16P_1")
				(number "A19")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L16N_1")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L17P_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L17N_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L18P_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L18N_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21P_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L21N_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J21")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "AB21")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "AA21")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "Y19")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "R15")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -144.78 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -147.32 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -149.86 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "T20")
			)
		)
		(symbol "XC6SLX150-CSG484_2_1"
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L33P_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L33N_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L34P_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L34N_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AB5")
			)
			(pin power_in line
				(at -40.64 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -35.56 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -33.02 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -30.48 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -27.94 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -25.4 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -22.86 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at 10.16 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AA3")
			)
			(pin power_in line
				(at 12.7 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 15.24 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 17.78 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F6")
			)
			(pin power_in line
				(at 20.32 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 22.86 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 27.94 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 30.48 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 33.02 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 35.56 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 38.1 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin power_in line
				(at 40.64 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "T7")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L12P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L12N_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L13P_3")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L13N_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19P_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L19N_3")
				(number "R8")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "T5")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L73P_3")
				(number "G8")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L73N_3")
				(number "G7")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L74P_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L74N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L75P_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L75N_3")
				(number "E5")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L80P_3")
				(number "F8")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L80N_3")
				(number "F7")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L81P_3")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L81N_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L82P_3")
				(number "E6")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L82N_3")
				(number "D5")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "A3")
			)
			(pin bidirectional line
				(at 50.8 -144.78 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "A2")
			)
		)
		(symbol "XC6SLX150-CSG484_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "E14")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "E16")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "D14")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "U16")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "W18")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "T15")
			)
		)
		(symbol "XC6SLX150-CSG484_4_1"
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "RFUSE")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VBATT")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VFS")
				(number "U19")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D18")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "J20")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX150-FGG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX150-FGG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 150 XC6SLX150-FGG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX150-FGG484_1_1"
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L14P_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L14N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L15P_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L15N_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L16P_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L16N_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L17P_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L17N_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L18P_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L18N_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L43P_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L43N_0")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L44P_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L44N_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L45P_0")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L45N_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L46P_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L46N_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D17")
			)
			(pin power_in line
				(at -40.64 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B7")
			)
			(pin power_in line
				(at -35.56 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B11")
			)
			(pin power_in line
				(at -33.02 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -30.48 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -27.94 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E13")
			)
			(pin power_in line
				(at -22.86 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -20.32 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -17.78 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G14")
			)
			(pin power_in line
				(at 17.78 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 20.32 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 22.86 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L9P_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L9N_1")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L10P_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L10N_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L21P_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21N_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "T20")
			)
		)
		(symbol "XC6SLX150-FGG484_2_1"
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "T18")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "T17")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "W18")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L7P_2")
				(number "T16")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L7N_2")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L8P_2")
				(number "U17")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L8N_2")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L9P_2")
				(number "V19")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L9N_2")
				(number "V18")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L10P_2")
				(number "R16")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L10N_2")
				(number "R15")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L11P_2")
				(number "V17")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L11N_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L21P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L21N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L22P_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L22N_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L51P_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L51N_2")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L52P_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L52N_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L53P_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L53N_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L54P_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L54N_2")
				(number "AB5")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L57P_2")
				(number "AA4")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L57N_2")
				(number "AB4")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "Y3")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "AB3")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L59P_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L59N_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -111.76 0)
				(length 6.35)
				(name "IO_L60P_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -114.3 0)
				(length 6.35)
				(name "IO_L60N_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 -116.84 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W4")
			)
			(pin bidirectional line
				(at -50.8 -119.38 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "Y4")
			)
			(pin bidirectional line
				(at -50.8 -121.92 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "U6")
			)
			(pin bidirectional line
				(at -50.8 -124.46 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "V5")
			)
			(pin bidirectional line
				(at -50.8 -127 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA2")
			)
			(pin bidirectional line
				(at -50.8 -129.54 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AB2")
			)
			(pin bidirectional line
				(at -50.8 -132.08 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -134.62 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "T5")
			)
			(pin power_in line
				(at -40.64 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA3")
			)
			(pin power_in line
				(at -38.1 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -35.56 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -33.02 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -30.48 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA19")
			)
			(pin power_in line
				(at -27.94 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -25.4 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -22.86 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -20.32 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -17.78 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at -15.24 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at 15.24 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 17.78 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 20.32 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F6")
			)
			(pin power_in line
				(at 22.86 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 25.4 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 27.94 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 30.48 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 33.02 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 35.56 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "D5")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L80P_3")
				(number "G7")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L80N_3")
				(number "F7")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L81P_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L81N_3")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L82P_3")
				(number "E5")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L82N_3")
				(number "E6")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "A2")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "B3")
			)
		)
		(symbol "XC6SLX150-FGG484_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "A19")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "C18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "G15")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "Y22")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "N15")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "Y20")
			)
		)
		(symbol "XC6SLX150-FGG484_4_1"
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "RFUSE")
				(number "P15")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VBATT")
				(number "R17")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VFS")
				(number "P16")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D18")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX150-FGG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX150-FGG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 150 XC6SLX150-FGG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX150-FGG676_1_1"
			(pin bidirectional line
				(at -50.8 129.54 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L9P_0")
				(number "K12")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L9N_0")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L11P_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L11N_0")
				(number "H9")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L12P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L12N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L13P_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L13N_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L14P_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L14N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L15P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L15N_0")
				(number "E9")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L16P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L16N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L17P_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L17N_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L18P_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L18N_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L19P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L19N_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L21P_0")
				(number "J12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L21N_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L22P_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L22N_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L23P_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L23N_0")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L24P_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L24N_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L25P_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L25N_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L26P_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L26N_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L30P_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L30N_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L31P_0")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L31N_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L43P_0")
				(number "J14")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L43N_0")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L44P_0")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L44N_0")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L45P_0")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L45N_0")
				(number "K14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L46P_0")
				(number "D16")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L46N_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "E17")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "J15")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "H15")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L52P_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L52N_0")
				(number "C18")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L53P_0")
				(number "K15")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L53N_0")
				(number "J16")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L54P_0")
				(number "E19")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L54N_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L55P_0")
				(number "H16")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L55N_0")
				(number "G17")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L56P_0")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L56N_0")
				(number "C20")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L57P_0")
				(number "F18")
			)
			(pin bidirectional line
				(at -50.8 -111.76 0)
				(length 6.35)
				(name "IO_L57N_0")
				(number "E18")
			)
			(pin bidirectional line
				(at -50.8 -114.3 0)
				(length 6.35)
				(name "IO_L58P_0")
				(number "E20")
			)
			(pin bidirectional line
				(at -50.8 -116.84 0)
				(length 6.35)
				(name "IO_L58N_0")
				(number "D20")
			)
			(pin bidirectional line
				(at -50.8 -119.38 0)
				(length 6.35)
				(name "IO_L59P_0")
				(number "J17")
			)
			(pin bidirectional line
				(at -50.8 -121.92 0)
				(length 6.35)
				(name "IO_L59N_0")
				(number "H17")
			)
			(pin bidirectional line
				(at -50.8 -124.46 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -127 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -129.54 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -132.08 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 -134.62 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 -137.16 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -139.7 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 -142.24 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A21")
			)
			(pin bidirectional line
				(at -50.8 -144.78 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 -147.32 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A22")
			)
			(pin power_in line
				(at -40.64 149.86 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B3")
			)
			(pin power_in line
				(at -38.1 149.86 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B7")
			)
			(pin power_in line
				(at -35.56 149.86 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B11")
			)
			(pin power_in line
				(at -33.02 149.86 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -30.48 149.86 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -27.94 149.86 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C22")
			)
			(pin power_in line
				(at -25.4 149.86 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D9")
			)
			(pin power_in line
				(at -22.86 149.86 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D17")
			)
			(pin power_in line
				(at -20.32 149.86 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E13")
			)
			(pin power_in line
				(at -17.78 149.86 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -15.24 149.86 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G18")
			)
			(pin power_in line
				(at -12.7 149.86 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H14")
			)
			(pin power_in line
				(at 20.32 149.86 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AB23")
			)
			(pin power_in line
				(at 22.86 149.86 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AD25")
			)
			(pin power_in line
				(at 25.4 149.86 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M20")
			)
			(pin power_in line
				(at 27.94 149.86 270)
				(length 6.35)
				(name "VCCO_1")
				(number "P23")
			)
			(pin power_in line
				(at 30.48 149.86 270)
				(length 6.35)
				(name "VCCO_1")
				(number "T25")
			)
			(pin power_in line
				(at 33.02 149.86 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 35.56 149.86 270)
				(length 6.35)
				(name "VCCO_1")
				(number "V21")
			)
			(pin power_in line
				(at 38.1 149.86 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W23")
			)
			(pin power_in line
				(at 40.64 149.86 270)
				(length 6.35)
				(name "VCCO_1")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 129.54 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "L23")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "R24")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "V23")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "W24")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "U25")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "U26")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "W25")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "W26")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "V24")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "V26")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "Y24")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "AD24")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "AB24")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "AB26")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "AC25")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "AC26")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "AA25")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "AA26")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "AE25")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "U24")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L55P_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L55N_1")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L56P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L56N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L57P_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L57N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "U23")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "U21")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "AA23")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "AA24")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AC23")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AC24")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "AE24")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "AF25")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "W18")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "W19")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L69P_1")
				(number "AB21")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L69N_VREF_1")
				(number "AB22")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "AE23")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "AF24")
			)
		)
		(symbol "XC6SLX150-FGG676_2_1"
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AF21")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AD20")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AF20")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AE19")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AF19")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "AC20")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "AA19")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L7P_2")
				(number "AC19")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L7N_2")
				(number "AD19")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L8P_2")
				(number "V16")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L8N_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L9P_2")
				(number "AD18")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L9N_2")
				(number "AF18")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L10P_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L10N_2")
				(number "AA17")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L11P_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L11N_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "AE17")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "AF17")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "AD16")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AF16")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AE15")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AF15")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AC17")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "AC15")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AD15")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "AC16")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "AD17")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "W16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AC14")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "AA15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L28P_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L28N_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "AD14")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "AF14")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AC13")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AD13")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AD12")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L33P_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L33N_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L34P_2")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L34N_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "V14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "AA11")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "V12")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AF11")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "AE9")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AD10")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L51P_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L51N_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L52P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L52N_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L53P_2")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L53N_2")
				(number "AF8")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L61P_2")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L61N_VREF_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "AE7")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AD6")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AF6")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AE5")
			)
			(pin bidirectional line
				(at -50.8 -111.76 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AF5")
			)
			(pin bidirectional line
				(at -50.8 -114.3 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "AE4")
			)
			(pin bidirectional line
				(at -50.8 -116.84 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AF4")
			)
			(pin power_in line
				(at -40.64 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AB14")
			)
			(pin power_in line
				(at -38.1 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC10")
			)
			(pin power_in line
				(at -35.56 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC18")
			)
			(pin power_in line
				(at -33.02 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC21")
			)
			(pin power_in line
				(at -30.48 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE8")
			)
			(pin power_in line
				(at -27.94 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE12")
			)
			(pin power_in line
				(at -25.4 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE16")
			)
			(pin power_in line
				(at -22.86 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE20")
			)
			(pin power_in line
				(at -20.32 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y12")
			)
			(pin power_in line
				(at -17.78 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y17")
			)
			(pin power_in line
				(at 17.78 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AC6")
			)
			(pin power_in line
				(at 20.32 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AD2")
			)
			(pin power_in line
				(at 22.86 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P4")
			)
			(pin power_in line
				(at 27.94 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P9")
			)
			(pin power_in line
				(at 30.48 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T2")
			)
			(pin power_in line
				(at 33.02 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T7")
			)
			(pin power_in line
				(at 35.56 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W4")
			)
			(pin power_in line
				(at 38.1 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W6")
			)
			(pin power_in line
				(at 40.64 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AC7")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AD7")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L3P_3")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L3N_3")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L4P_3")
				(number "AA8")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L4N_3")
				(number "AB8")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "AA7")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "AB7")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "Y9")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "Y8")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "AC5")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "AD5")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L15P_3")
				(number "W8")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L15N_3")
				(number "W7")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L16P_3")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L16N_3")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L17P_3")
				(number "V7")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L17N_VREF_3")
				(number "V6")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L19P_3")
				(number "W9")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L19N_3")
				(number "V8")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "W10")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "V10")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "T10")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "U9")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L27P_3")
				(number "R10")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L27N_3")
				(number "T9")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L28P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L28N_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L29P_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L29N_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L30P_3")
				(number "R5")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L30N_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "N8")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "P10")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "N5")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "M10")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "N9")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "M9")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "L7")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "L6")
			)
		)
		(symbol "XC6SLX150-FGG676_3_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L58P_4")
				(number "K8")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L58N_VREF_4")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L59P_M4DQ14_4")
				(number "N2")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L59N_M4DQ15_4")
				(number "N1")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L60P_M4DQ12_4")
				(number "M3")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L60N_M4DQ13_4")
				(number "M1")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L61P_M4UDQS_4")
				(number "L2")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L61N_M4UDQSN_4")
				(number "L1")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62P_M4DQ10_4")
				(number "K3")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L62N_M4DQ11_4")
				(number "K1")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63P_M4DQ8_4")
				(number "J2")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L63N_M4DQ9_4")
				(number "J1")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64P_M4DQ0_4")
				(number "H3")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L64N_M4DQ1_4")
				(number "H1")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65P_M4DQ2_4")
				(number "G2")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L65N_M4DQ3_4")
				(number "G1")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66P_M4LDQS_4")
				(number "F3")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L66N_M4LDQSN_4")
				(number "F1")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L67P_M4DQ6_4")
				(number "E2")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L67N_M4DQ7_4")
				(number "E1")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L68P_M4DQ4_4")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L68N_M4DQ5_4")
				(number "D1")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L69P_M4UDM_4")
				(number "J4")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L69N_M4LDM_4")
				(number "J3")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L70P_M4RASN_4")
				(number "K7")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L70N_M4CASN_4")
				(number "K6")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L71P_M4A5_4")
				(number "K5")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L71N_M4A6_4")
				(number "J5")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L72P_M4A3_4")
				(number "J7")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L72N_M4ODT_4")
				(number "H7")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L73P_M4CLK_4")
				(number "G4")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L73N_M4CLKN_4")
				(number "G3")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L74P_M4A0_4")
				(number "K10")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L74N_M4A1_4")
				(number "L9")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L75P_M4BA0_4")
				(number "H6")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L75N_M4BA1_4")
				(number "H5")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L76P_M4A7_4")
				(number "J10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L76N_M4A2_4")
				(number "K9")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L77P_M4WE_4")
				(number "E4")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L77N_M4BA2_4")
				(number "E3")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L78P_M4A10_4")
				(number "G6")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L78N_M4A4_4")
				(number "G5")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L79P_M4A8_4")
				(number "C2")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L79N_M4A9_4")
				(number "C1")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L80P_M4CKE_4")
				(number "F5")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L80N_M4A12_4")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L81P_M4RESET_4")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L81N_M4A11_4")
				(number "B1")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L82P_M4A13_4")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L82N_M4A14_4")
				(number "G7")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L83P_4")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L83N_VREF_4")
				(number "C3")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "D2")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "F4")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "H2")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "J6")
			)
			(pin power_in line
				(at -30.48 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "K4")
			)
			(pin power_in line
				(at -27.94 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "M2")
			)
			(pin power_in line
				(at 27.94 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "D25")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "F23")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "H25")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "J21")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "K23")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_A25_5")
				(number "B23")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_5")
				(number "A23")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L2P_M5A13_5")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L2N_M5A14_5")
				(number "G21")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L3P_M5RESET_5")
				(number "D23")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L3N_M5A11_5")
				(number "C24")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L4P_M5CKE_5")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L4N_M5A12_5")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L5P_M5A8_5")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L5N_M5A9_5")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L6P_M5A10_5")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L6N_M5A4_5")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L7P_M5WE_5")
				(number "E23")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L7N_M5BA2_5")
				(number "E24")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L8P_M5A7_5")
				(number "G23")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L8N_M5A2_5")
				(number "G24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L9P_M5BA0_5")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L9N_M5BA1_5")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L10P_M5A0_5")
				(number "B24")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L10N_M5A1_5")
				(number "A25")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L11P_M5CLK_5")
				(number "C25")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L11N_M5CLKN_5")
				(number "C26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L12P_M5A3_5")
				(number "B25")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L12N_M5ODT_5")
				(number "B26")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L13P_M5A5_5")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L13N_M5A6_5")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L14P_M5RASN_5")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L14N_M5CASN_5")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L15P_M5UDM_5")
				(number "J23")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L15N_M5LDM_5")
				(number "J24")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L16P_M5DQ4_5")
				(number "E25")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L16N_M5DQ5_5")
				(number "E26")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L17P_M5DQ6_5")
				(number "D24")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L17N_M5DQ7_5")
				(number "D26")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L18P_M5LDQS_5")
				(number "F24")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L18N_M5LDQSN_5")
				(number "F26")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L19P_M5DQ2_5")
				(number "H24")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L19N_M5DQ3_5")
				(number "H26")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L20P_M5DQ0_5")
				(number "G25")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L20N_M5DQ1_5")
				(number "G26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L21P_M5DQ8_5")
				(number "K24")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L21N_M5DQ9_5")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L22P_M5DQ10_5")
				(number "J25")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L22N_M5DQ11_5")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L23P_M5UDQS_5")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L23N_M5UDQSN_5")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L24P_M5DQ12_5")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L24N_M5DQ13_5")
				(number "L26")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L25P_M5DQ14_5")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L25N_M5DQ15_5")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L26P_5")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L26N_VREF_5")
				(number "L21")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L27P_5")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L27N_5")
				(number "J20")
			)
		)
		(symbol "XC6SLX150-FGG676_4_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "F20")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "A24")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "C23")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "E21")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AF23")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AF3")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "AD23")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "AC22")
			)
		)
		(symbol "XC6SLX150-FGG676_5_1"
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F6")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F21")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G15")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J18")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L22")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M17")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N10")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U6")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U14")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "Y19")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA6")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA10")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA16")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA21")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "RFUSE")
				(number "AA20")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VBATT")
				(number "W21")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VFS")
				(number "AB19")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B21")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F2")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F19")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "F25")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H11")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J19")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "K2")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "K16")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "K25")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "L15")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "M5")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "M16")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "M22")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "N15")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "P2")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "L16")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "R16")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "U16")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "P19")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T5")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "V2")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "W15")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "W20")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "Y7")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "Y11")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "Y23")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AB2")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AB12")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AB16")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AB20")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AB25")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AC8")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AE6")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AE10")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AE14")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AE18")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AF26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX150-FGG900"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX150-FGG900"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 150 XC6SLX150-FGG900"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX150-FGG900_1_1"
			(pin bidirectional line
				(at -50.8 157.48 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 154.94 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 152.4 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "G7")
			)
			(pin bidirectional line
				(at -50.8 149.86 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 147.32 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "G6")
			)
			(pin bidirectional line
				(at -50.8 144.78 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "F6")
			)
			(pin bidirectional line
				(at -50.8 142.24 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 139.7 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 137.16 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 134.62 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 132.08 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 129.54 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "J10")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L9P_0")
				(number "B7")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L9N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L10P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L10N_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L11P_0")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L11N_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L12P_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L12N_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L13P_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L13N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L14P_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L14N_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L15P_0")
				(number "K12")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L15N_0")
				(number "J12")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L16P_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L16N_0")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L17P_0")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L17N_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L18P_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L18N_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L19P_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L19N_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L20P_0")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L20N_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L21P_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L21N_0")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L22P_0")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L22N_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L23P_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L23N_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L24P_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L24N_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L25P_0")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L25N_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L26P_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L26N_0")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L27P_0")
				(number "K14")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L27N_0")
				(number "J14")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L28P_0")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L28N_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L29P_0")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L29N_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L30P_0")
				(number "B13")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L30N_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L31P_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L31N_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "J15")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "H15")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "C18")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "B17")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L39P_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L39N_0")
				(number "D16")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L40P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L40N_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L41P_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L41N_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L42P_0")
				(number "G17")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L42N_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L43P_0")
				(number "J17")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L43N_0")
				(number "H17")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L44P_0")
				(number "B19")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L44N_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L45P_0")
				(number "E18")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L45N_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L46P_0")
				(number "G18")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L46N_0")
				(number "F18")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "C20")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "G19")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "F19")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "B21")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A21")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "J19")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "H19")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L52P_0")
				(number "E20")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L52N_0")
				(number "D20")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L53P_0")
				(number "C22")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L53N_0")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 -111.76 0)
				(length 6.35)
				(name "IO_L54P_0")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 -114.3 0)
				(length 6.35)
				(name "IO_L54N_0")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 -116.84 0)
				(length 6.35)
				(name "IO_L55P_0")
				(number "E22")
			)
			(pin bidirectional line
				(at -50.8 -119.38 0)
				(length 6.35)
				(name "IO_L55N_0")
				(number "D22")
			)
			(pin bidirectional line
				(at -50.8 -121.92 0)
				(length 6.35)
				(name "IO_L56P_0")
				(number "B23")
			)
			(pin bidirectional line
				(at -50.8 -124.46 0)
				(length 6.35)
				(name "IO_L56N_0")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 -127 0)
				(length 6.35)
				(name "IO_L57P_0")
				(number "J20")
			)
			(pin bidirectional line
				(at -50.8 -129.54 0)
				(length 6.35)
				(name "IO_L57N_0")
				(number "G20")
			)
			(pin bidirectional line
				(at -50.8 -132.08 0)
				(length 6.35)
				(name "IO_L58P_0")
				(number "G21")
			)
			(pin bidirectional line
				(at -50.8 -134.62 0)
				(length 6.35)
				(name "IO_L58N_0")
				(number "F21")
			)
			(pin bidirectional line
				(at -50.8 -137.16 0)
				(length 6.35)
				(name "IO_L59P_0")
				(number "D23")
			)
			(pin bidirectional line
				(at -50.8 -139.7 0)
				(length 6.35)
				(name "IO_L59N_0")
				(number "C23")
			)
			(pin bidirectional line
				(at -50.8 -142.24 0)
				(length 6.35)
				(name "IO_L60P_0")
				(number "G22")
			)
			(pin bidirectional line
				(at -50.8 -144.78 0)
				(length 6.35)
				(name "IO_L60N_0")
				(number "F22")
			)
			(pin bidirectional line
				(at -50.8 -147.32 0)
				(length 6.35)
				(name "IO_L61P_0")
				(number "E24")
			)
			(pin bidirectional line
				(at -50.8 -149.86 0)
				(length 6.35)
				(name "IO_L61N_0")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 -152.4 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "G23")
			)
			(pin bidirectional line
				(at -50.8 -154.94 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 -157.48 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 -160.02 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 -162.56 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 -165.1 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A24")
			)
			(pin bidirectional line
				(at -50.8 -167.64 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "J21")
			)
			(pin bidirectional line
				(at -50.8 -170.18 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "H21")
			)
			(pin bidirectional line
				(at -50.8 -172.72 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D25")
			)
			(pin bidirectional line
				(at -50.8 -175.26 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "C25")
			)
			(pin power_in line
				(at -40.64 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B8")
			)
			(pin power_in line
				(at -38.1 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B12")
			)
			(pin power_in line
				(at -35.56 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B16")
			)
			(pin power_in line
				(at -33.02 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B20")
			)
			(pin power_in line
				(at -30.48 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B24")
			)
			(pin power_in line
				(at -27.94 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E11")
			)
			(pin power_in line
				(at -22.86 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E15")
			)
			(pin power_in line
				(at -20.32 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E19")
			)
			(pin power_in line
				(at -17.78 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E23")
			)
			(pin power_in line
				(at -15.24 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H7")
			)
			(pin power_in line
				(at -12.7 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H10")
			)
			(pin power_in line
				(at -10.16 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H14")
			)
			(pin power_in line
				(at -7.62 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H18")
			)
			(pin power_in line
				(at -5.08 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H22")
			)
			(pin power_in line
				(at -2.54 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "J16")
			)
			(pin power_in line
				(at 0 177.8 270)
				(length 6.35)
				(name "VCCO_0")
				(number "K11")
			)
			(pin power_in line
				(at 7.62 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AA23")
			)
			(pin power_in line
				(at 10.16 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AC26")
			)
			(pin power_in line
				(at 12.7 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AD29")
			)
			(pin power_in line
				(at 15.24 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AH29")
			)
			(pin power_in line
				(at 17.78 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AJ27")
			)
			(pin power_in line
				(at 20.32 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N23")
			)
			(pin power_in line
				(at 22.86 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "P21")
			)
			(pin power_in line
				(at 25.4 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R23")
			)
			(pin power_in line
				(at 27.94 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R26")
			)
			(pin power_in line
				(at 30.48 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "T29")
			)
			(pin power_in line
				(at 33.02 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U23")
			)
			(pin power_in line
				(at 35.56 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "V21")
			)
			(pin power_in line
				(at 38.1 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W26")
			)
			(pin power_in line
				(at 40.64 177.8 270)
				(length 6.35)
				(name "VCCO_1")
				(number "Y29")
			)
			(pin bidirectional line
				(at 50.8 157.48 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 154.94 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 152.4 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "N29")
			)
			(pin bidirectional line
				(at 50.8 149.86 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "N30")
			)
			(pin bidirectional line
				(at 50.8 147.32 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "N27")
			)
			(pin bidirectional line
				(at 50.8 144.78 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "N28")
			)
			(pin bidirectional line
				(at 50.8 142.24 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "P28")
			)
			(pin bidirectional line
				(at 50.8 139.7 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "P30")
			)
			(pin bidirectional line
				(at 50.8 137.16 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 134.62 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "P27")
			)
			(pin bidirectional line
				(at 50.8 132.08 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "R29")
			)
			(pin bidirectional line
				(at 50.8 129.54 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "R30")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "R27")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "R28")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "T27")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "T28")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "T30")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "U29")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "U30")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "U27")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "U28")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "V28")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "V30")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "V26")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "V27")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "W27")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "W28")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "AB28")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "AB30")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "W29")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "W30")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "Y28")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "Y30")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "AA29")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "AA30")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "AA27")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "AA28")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "Y27")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "AD28")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "AD30")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "AC27")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "AC28")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "AC29")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "AC30")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "AE29")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "AE30")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "AE27")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "AE28")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "W24")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "W25")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L54P_1")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L54N_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L55P_1")
				(number "AF28")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L55N_1")
				(number "AF30")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L56P_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L56N_1")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L57P_1")
				(number "AG29")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L57N_1")
				(number "AG30")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "P25")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "AH30")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "AJ30")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "R24")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "AJ29")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "AK29")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "T25")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "AJ28")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "AK28")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "U24")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "U25")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AG27")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AG28")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "V23")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "V24")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "AD27")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L69P_1")
				(number "AH27")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L69N_VREF_1")
				(number "AK27")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "Y23")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "AE25")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "Y24")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "AG26")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "AH26")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "AA24")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "AA25")
			)
		)
		(symbol "XC6SLX150-FGG900_2_1"
			(pin bidirectional line
				(at -50.8 154.94 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "AJ26")
			)
			(pin bidirectional line
				(at -50.8 152.4 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AK26")
			)
			(pin bidirectional line
				(at -50.8 149.86 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AD24")
			)
			(pin bidirectional line
				(at -50.8 147.32 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AE24")
			)
			(pin bidirectional line
				(at -50.8 144.78 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AH25")
			)
			(pin bidirectional line
				(at -50.8 142.24 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AK25")
			)
			(pin bidirectional line
				(at -50.8 139.7 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AF25")
			)
			(pin bidirectional line
				(at -50.8 137.16 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AG25")
			)
			(pin bidirectional line
				(at -50.8 134.62 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "AG24")
			)
			(pin bidirectional line
				(at -50.8 132.08 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AH24")
			)
			(pin bidirectional line
				(at -50.8 129.54 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "AE23")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L7P_2")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L7N_2")
				(number "AE22")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L8P_2")
				(number "AC21")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L8N_2")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L9P_2")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L9N_2")
				(number "AG23")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L10P_2")
				(number "AD20")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L10N_2")
				(number "AE20")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L11P_2")
				(number "AJ24")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L11N_2")
				(number "AK24")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "AH23")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "AK23")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "AJ22")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AK22")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AH21")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AK21")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AG22")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AH22")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "AJ20")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AK20")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "AF21")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "AG21")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "AC20")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AD19")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AE19")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "AG20")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "AH20")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L21P_2")
				(number "AD18")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L21N_2")
				(number "AE18")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L22P_2")
				(number "AA19")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L22N_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "AF19")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "AG19")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L24P_2")
				(number "AG18")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L24N_VREF_2")
				(number "AH18")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L25P_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L25N_2")
				(number "AC18")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L26P_2")
				(number "AF17")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L26N_2")
				(number "AG17")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L27P_2")
				(number "AD17")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L27N_2")
				(number "AE17")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L28P_2")
				(number "AD16")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L28N_2")
				(number "AE16")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "AH19")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "AK19")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AJ18")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AK18")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AJ16")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AK16")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AH17")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AK17")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L33P_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L33N_2")
				(number "AC16")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L34P_2")
				(number "AF15")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L34N_2")
				(number "AG15")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L35P_2")
				(number "AG16")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L35N_2")
				(number "AH16")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L36P_2")
				(number "AD15")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L36N_2")
				(number "AE15")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L37P_2")
				(number "AA15")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L37N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L38P_2")
				(number "AH15")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L38N_2")
				(number "AK15")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L39P_2")
				(number "AJ14")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L39N_2")
				(number "AK14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "AC14")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AH13")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AK13")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "AD14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "AE14")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AG13")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "AG14")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "AH14")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AG12")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AH12")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "AD13")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "AD12")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AE12")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "AH11")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AK11")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AJ12")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AK12")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L51P_2")
				(number "AF11")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L51N_2")
				(number "AG11")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L52P_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L52N_2")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L53P_2")
				(number "AJ10")
			)
			(pin bidirectional line
				(at -50.8 -111.76 0)
				(length 6.35)
				(name "IO_L53N_2")
				(number "AK10")
			)
			(pin bidirectional line
				(at -50.8 -114.3 0)
				(length 6.35)
				(name "IO_L54P_2")
				(number "AH9")
			)
			(pin bidirectional line
				(at -50.8 -116.84 0)
				(length 6.35)
				(name "IO_L54N_2")
				(number "AK9")
			)
			(pin bidirectional line
				(at -50.8 -119.38 0)
				(length 6.35)
				(name "IO_L55P_2")
				(number "AG10")
			)
			(pin bidirectional line
				(at -50.8 -121.92 0)
				(length 6.35)
				(name "IO_L55N_2")
				(number "AH10")
			)
			(pin bidirectional line
				(at -50.8 -124.46 0)
				(length 6.35)
				(name "IO_L56P_2")
				(number "AD10")
			)
			(pin bidirectional line
				(at -50.8 -127 0)
				(length 6.35)
				(name "IO_L56N_2")
				(number "AE10")
			)
			(pin bidirectional line
				(at -50.8 -129.54 0)
				(length 6.35)
				(name "IO_L57P_2")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 -132.08 0)
				(length 6.35)
				(name "IO_L57N_2")
				(number "AG9")
			)
			(pin bidirectional line
				(at -50.8 -134.62 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "AG8")
			)
			(pin bidirectional line
				(at -50.8 -137.16 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "AH8")
			)
			(pin bidirectional line
				(at -50.8 -139.7 0)
				(length 6.35)
				(name "IO_L59P_2")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 -142.24 0)
				(length 6.35)
				(name "IO_L59N_2")
				(number "AG7")
			)
			(pin bidirectional line
				(at -50.8 -144.78 0)
				(length 6.35)
				(name "IO_L60P_2")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 -147.32 0)
				(length 6.35)
				(name "IO_L60N_2")
				(number "AE9")
			)
			(pin bidirectional line
				(at -50.8 -149.86 0)
				(length 6.35)
				(name "IO_L61P_2")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 -152.4 0)
				(length 6.35)
				(name "IO_L61N_VREF_2")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 -154.94 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "AJ8")
			)
			(pin bidirectional line
				(at -50.8 -157.48 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "AK8")
			)
			(pin bidirectional line
				(at -50.8 -160.02 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AG6")
			)
			(pin bidirectional line
				(at -50.8 -162.56 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AH6")
			)
			(pin bidirectional line
				(at -50.8 -165.1 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AH7")
			)
			(pin bidirectional line
				(at -50.8 -167.64 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AK7")
			)
			(pin bidirectional line
				(at -50.8 -170.18 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "AJ6")
			)
			(pin bidirectional line
				(at -50.8 -172.72 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AK6")
			)
			(pin power_in line
				(at -40.64 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA14")
			)
			(pin power_in line
				(at -38.1 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA18")
			)
			(pin power_in line
				(at -35.56 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC9")
			)
			(pin power_in line
				(at -33.02 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC11")
			)
			(pin power_in line
				(at -30.48 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC15")
			)
			(pin power_in line
				(at -27.94 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC19")
			)
			(pin power_in line
				(at -25.4 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC22")
			)
			(pin power_in line
				(at -22.86 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AF8")
			)
			(pin power_in line
				(at -20.32 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AF12")
			)
			(pin power_in line
				(at -17.78 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AF16")
			)
			(pin power_in line
				(at -15.24 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AF20")
			)
			(pin power_in line
				(at -12.7 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AF24")
			)
			(pin power_in line
				(at -10.16 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AJ7")
			)
			(pin power_in line
				(at -7.62 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AJ11")
			)
			(pin power_in line
				(at -5.08 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AJ15")
			)
			(pin power_in line
				(at -2.54 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AJ19")
			)
			(pin power_in line
				(at 0 175.26 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AJ23")
			)
			(pin power_in line
				(at 7.62 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AA8")
			)
			(pin power_in line
				(at 10.16 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AC2")
			)
			(pin power_in line
				(at 12.7 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AD5")
			)
			(pin power_in line
				(at 15.24 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AG2")
			)
			(pin power_in line
				(at 17.78 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AJ3")
			)
			(pin power_in line
				(at 20.32 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L8")
			)
			(pin power_in line
				(at 22.86 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P8")
			)
			(pin power_in line
				(at 27.94 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 30.48 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T5")
			)
			(pin power_in line
				(at 33.02 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U8")
			)
			(pin power_in line
				(at 35.56 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin power_in line
				(at 38.1 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "Y5")
			)
			(pin power_in line
				(at 40.64 175.26 270)
				(length 6.35)
				(name "VCCO_3")
				(number "Y10")
			)
			(pin bidirectional line
				(at 50.8 154.94 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AA10")
			)
			(pin bidirectional line
				(at 50.8 152.4 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AA9")
			)
			(pin bidirectional line
				(at 50.8 149.86 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "AD7")
			)
			(pin bidirectional line
				(at 50.8 147.32 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "AE7")
			)
			(pin bidirectional line
				(at 50.8 144.78 180)
				(length 6.35)
				(name "IO_L3P_3")
				(number "Y9")
			)
			(pin bidirectional line
				(at 50.8 142.24 180)
				(length 6.35)
				(name "IO_L3N_3")
				(number "Y8")
			)
			(pin bidirectional line
				(at 50.8 139.7 180)
				(length 6.35)
				(name "IO_L4P_3")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 137.16 180)
				(length 6.35)
				(name "IO_L4N_3")
				(number "AF6")
			)
			(pin bidirectional line
				(at 50.8 134.62 180)
				(length 6.35)
				(name "IO_L5P_3")
				(number "AA12")
			)
			(pin bidirectional line
				(at 50.8 132.08 180)
				(length 6.35)
				(name "IO_L5N_3")
				(number "AA11")
			)
			(pin bidirectional line
				(at 50.8 129.54 180)
				(length 6.35)
				(name "IO_L6P_3")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L6N_3")
				(number "AG5")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "T7")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "AA7")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AA6")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "AH5")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "AK5")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "W10")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "W9")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L12P_3")
				(number "AB7")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L12N_3")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L13P_3")
				(number "W7")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L13N_3")
				(number "W6")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L14P_3")
				(number "AJ4")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L14N_3")
				(number "AK4")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L15P_3")
				(number "T9")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L15N_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L16P_3")
				(number "AH3")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L16N_3")
				(number "AK3")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L17P_3")
				(number "Y7")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L17N_VREF_3")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "AJ2")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "AK2")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L19P_3")
				(number "AE4")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L19N_3")
				(number "AF4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "AG3")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "V8")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "V7")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "AH1")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "AJ1")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "V10")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "V9")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "AG4")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "AH4")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "N10")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "N9")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "AH2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L27P_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L27N_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L28P_3")
				(number "AF1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L28N_3")
				(number "AG1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L29P_3")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L29N_3")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L30P_3")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L30N_3")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "N8")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "AC5")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "AD2")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "R5")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "N5")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L56P_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L56N_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "M6")
			)
		)
		(symbol "XC6SLX150-FGG900_3_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L58P_4")
				(number "L7")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L58N_VREF_4")
				(number "L6")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L59P_M4DQ14_4")
				(number "M2")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L59N_M4DQ15_4")
				(number "M1")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L60P_M4DQ12_4")
				(number "L3")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L60N_M4DQ13_4")
				(number "L1")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L61P_M4UDQS_4")
				(number "K2")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L61N_M4UDQSN_4")
				(number "K1")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62P_M4DQ10_4")
				(number "L5")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L62N_M4DQ11_4")
				(number "L4")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63P_M4DQ8_4")
				(number "M4")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L63N_M4DQ9_4")
				(number "M3")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64P_M4DQ0_4")
				(number "H4")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L64N_M4DQ1_4")
				(number "H3")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65P_M4DQ2_4")
				(number "J3")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L65N_M4DQ3_4")
				(number "J1")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66P_M4LDQS_4")
				(number "J5")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L66N_M4LDQSN_4")
				(number "J4")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L67P_M4DQ6_4")
				(number "H2")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L67N_M4DQ7_4")
				(number "H1")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L68P_M4DQ4_4")
				(number "G3")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L68N_M4DQ5_4")
				(number "G1")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L69P_M4UDM_4")
				(number "K4")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L69N_M4LDM_4")
				(number "K3")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L70P_M4RASN_4")
				(number "C1")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L70N_M4CASN_4")
				(number "B1")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L71P_M4A5_4")
				(number "F2")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L71N_M4A6_4")
				(number "F1")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L72P_M4A3_4")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L72N_M4ODT_4")
				(number "E4")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L73P_M4CLK_4")
				(number "E3")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L73N_M4CLKN_4")
				(number "E1")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L74P_M4A0_4")
				(number "D4")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L74N_M4A1_4")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L75P_M4BA0_4")
				(number "D2")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L75N_M4BA1_4")
				(number "D1")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L76P_M4A7_4")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L76N_M4A2_4")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L77P_M4WE_4")
				(number "F4")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L77N_M4BA2_4")
				(number "F3")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L78P_M4A10_4")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L78N_M4A4_4")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L79P_M4A8_4")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L79N_M4A9_4")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L80P_M4CKE_4")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L80N_M4A12_4")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L81P_M4RESET_4")
				(number "G5")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L81N_M4A11_4")
				(number "G4")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L82P_M4A13_4")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L82N_M4A14_4")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L83P_4")
				(number "J6")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L83N_VREF_4")
				(number "H6")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "C2")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "G2")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "H5")
			)
			(pin power_in line
				(at -30.48 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "K6")
			)
			(pin power_in line
				(at -27.94 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "L2")
			)
			(pin power_in line
				(at -25.4 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "M5")
			)
			(pin power_in line
				(at 22.86 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "B28")
			)
			(pin power_in line
				(at 25.4 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "D29")
			)
			(pin power_in line
				(at 27.94 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "G26")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "H29")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "J25")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "K24")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "L26")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "M29")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_A25_5")
				(number "G25")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_5")
				(number "F25")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L2P_M5A13_5")
				(number "A28")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L2N_M5A14_5")
				(number "A29")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L3P_M5RESET_5")
				(number "C26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L3N_M5A11_5")
				(number "A26")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L4P_M5CKE_5")
				(number "B29")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L4N_M5A12_5")
				(number "B30")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L5P_M5A8_5")
				(number "B27")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L5N_M5A9_5")
				(number "A27")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L6P_M5A10_5")
				(number "F26")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L6N_M5A4_5")
				(number "F27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L7P_M5WE_5")
				(number "E26")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L7N_M5BA2_5")
				(number "D26")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L8P_M5A7_5")
				(number "C29")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L8N_M5A2_5")
				(number "C30")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L9P_M5BA0_5")
				(number "D27")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L9N_M5BA1_5")
				(number "C27")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L10P_M5A0_5")
				(number "D28")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L10N_M5A1_5")
				(number "D30")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L11P_M5CLK_5")
				(number "E27")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L11N_M5CLKN_5")
				(number "E28")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L12P_M5A3_5")
				(number "E29")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L12N_M5ODT_5")
				(number "E30")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L13P_M5A5_5")
				(number "H26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L13N_M5A6_5")
				(number "H27")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L14P_M5RASN_5")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L14N_M5CASN_5")
				(number "K27")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L15P_M5UDM_5")
				(number "J27")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L15N_M5LDM_5")
				(number "J28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L16P_M5DQ4_5")
				(number "G27")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L16N_M5DQ5_5")
				(number "G28")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L17P_M5DQ6_5")
				(number "F28")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L17N_M5DQ7_5")
				(number "F30")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L18P_M5LDQS_5")
				(number "J29")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L18N_M5LDQSN_5")
				(number "J30")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L19P_M5DQ2_5")
				(number "G29")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L19N_M5DQ3_5")
				(number "G30")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L20P_M5DQ0_5")
				(number "H28")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L20N_M5DQ1_5")
				(number "H30")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L21P_M5DQ8_5")
				(number "L27")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L21N_M5DQ9_5")
				(number "L28")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L22P_M5DQ10_5")
				(number "L29")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L22N_M5DQ11_5")
				(number "L30")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L23P_M5UDQS_5")
				(number "K28")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L23N_M5UDQSN_5")
				(number "K30")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L24P_M5DQ12_5")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L24N_M5DQ13_5")
				(number "M27")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L25P_M5DQ14_5")
				(number "M28")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L25N_M5DQ15_5")
				(number "M30")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L26P_5")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L26N_VREF_5")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L27P_5")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L27N_5")
				(number "L25")
			)
		)
		(symbol "XC6SLX150-FGG900_4_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "H25")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "G24")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "K25")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "F24")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AD25")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "AB25")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "AC25")
			)
		)
		(symbol "XC6SLX150-FGG900_5_1"
			(pin power_in line
				(at -25.4 134.62 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F10")
			)
			(pin power_in line
				(at -25.4 132.08 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F20")
			)
			(pin power_in line
				(at -25.4 129.54 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H24")
			)
			(pin power_in line
				(at -25.4 127 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J8")
			)
			(pin power_in line
				(at -25.4 124.46 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J23")
			)
			(pin power_in line
				(at -25.4 121.92 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K9")
			)
			(pin power_in line
				(at -25.4 119.38 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 116.84 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K17")
			)
			(pin power_in line
				(at -25.4 114.3 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L22")
			)
			(pin power_in line
				(at -25.4 111.76 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M25")
			)
			(pin power_in line
				(at -25.4 109.22 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N6")
			)
			(pin power_in line
				(at -25.4 106.68 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N21")
			)
			(pin power_in line
				(at -25.4 104.14 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 101.6 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T21")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U10")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V25")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA21")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB9")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB13")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB17")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC7")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC24")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AE11")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AE21")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "RFUSE")
				(number "AB27")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VBATT")
				(number "AB26")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VFS")
				(number "AF27")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "A30")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "B6")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "B10")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "B14")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "B18")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "B22")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "B26")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "C28")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "E13")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "E17")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "E25")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "F5")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "F29")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "H12")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "H16")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "H20")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "J7")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "J18")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "J22")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "J24")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "J26")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "K5")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "K16")
			)
			(pin power_in line
				(at -25.4 -101.6 0)
				(length 6.35)
				(name "GND")
				(number "K18")
			)
			(pin power_in line
				(at -25.4 -104.14 0)
				(length 6.35)
				(name "GND")
				(number "K21")
			)
			(pin power_in line
				(at -25.4 -106.68 0)
				(length 6.35)
				(name "GND")
				(number "K22")
			)
			(pin power_in line
				(at -25.4 -109.22 0)
				(length 6.35)
				(name "GND")
				(number "K23")
			)
			(pin power_in line
				(at -25.4 -111.76 0)
				(length 6.35)
				(name "GND")
				(number "K29")
			)
			(pin power_in line
				(at -25.4 -114.3 0)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at -25.4 -116.84 0)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at -25.4 -119.38 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -121.92 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -124.46 0)
				(length 6.35)
				(name "GND")
				(number "L14")
			)
			(pin power_in line
				(at -25.4 -127 0)
				(length 6.35)
				(name "GND")
				(number "L17")
			)
			(pin power_in line
				(at -25.4 -129.54 0)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at -25.4 -132.08 0)
				(length 6.35)
				(name "GND")
				(number "L21")
			)
			(pin power_in line
				(at -25.4 -134.62 0)
				(length 6.35)
				(name "GND")
				(number "L23")
			)
			(pin power_in line
				(at 25.4 134.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "K15")
			)
			(pin power_in line
				(at 25.4 132.08 180)
				(length 6.35)
				(name "VCCINT")
				(number "K19")
			)
			(pin power_in line
				(at 25.4 129.54 180)
				(length 6.35)
				(name "VCCINT")
				(number "K20")
			)
			(pin power_in line
				(at 25.4 127 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 124.46 180)
				(length 6.35)
				(name "VCCINT")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 121.92 180)
				(length 6.35)
				(name "VCCINT")
				(number "L16")
			)
			(pin power_in line
				(at 25.4 119.38 180)
				(length 6.35)
				(name "VCCINT")
				(number "L19")
			)
			(pin power_in line
				(at 25.4 116.84 180)
				(length 6.35)
				(name "VCCINT")
				(number "L20")
			)
			(pin power_in line
				(at 25.4 114.3 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 111.76 180)
				(length 6.35)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 109.22 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 106.68 180)
				(length 6.35)
				(name "VCCINT")
				(number "M16")
			)
			(pin power_in line
				(at 25.4 104.14 180)
				(length 6.35)
				(name "VCCINT")
				(number "M19")
			)
			(pin power_in line
				(at 25.4 101.6 180)
				(length 6.35)
				(name "VCCINT")
				(number "M20")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "N18")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "P17")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "P18")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "R16")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "R19")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "R20")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "T10")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "T12")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "T19")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "T20")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "U13")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "U17")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "V13")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "V17")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "V18")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "W11")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "W12")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "W15")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "W20")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y12")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y15")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y16")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y19")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "VCCINT")
				(number "Y20")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "VCCINT")
				(number "AA16")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "M17")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "M18")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "M21")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "M22")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "N19")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "N20")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "N22")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "N26")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "P5")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "P19")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "P20")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "P29")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "R17")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "T18")
			)
			(pin power_in line
				(at 25.4 -101.6 180)
				(length 6.35)
				(name "GND")
				(number "T22")
			)
			(pin power_in line
				(at 25.4 -104.14 180)
				(length 6.35)
				(name "GND")
				(number "T23")
			)
			(pin power_in line
				(at 25.4 -106.68 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -109.22 180)
				(length 6.35)
				(name "GND")
				(number "U9")
			)
			(pin power_in line
				(at 25.4 -111.76 180)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 -114.3 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -116.84 180)
				(length 6.35)
				(name "GND")
				(number "U15")
			)
			(pin power_in line
				(at 25.4 -119.38 180)
				(length 6.35)
				(name "GND")
				(number "U16")
			)
			(pin power_in line
				(at 25.4 -121.92 180)
				(length 6.35)
				(name "GND")
				(number "U19")
			)
			(pin power_in line
				(at 25.4 -124.46 180)
				(length 6.35)
				(name "GND")
				(number "U20")
			)
			(pin power_in line
				(at 25.4 -127 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -129.54 180)
				(length 6.35)
				(name "GND")
				(number "U22")
			)
			(pin power_in line
				(at 25.4 -132.08 180)
				(length 6.35)
				(name "GND")
				(number "U26")
			)
			(pin power_in line
				(at 25.4 -134.62 180)
				(length 6.35)
				(name "GND")
				(number "V5")
			)
		)
		(symbol "XC6SLX150-FGG900_6_1"
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "V11")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "V12")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "V15")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "V16")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "V19")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "V20")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "V22")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "V29")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "W8")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "W13")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "W14")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "W17")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "W18")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "W23")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "Y11")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "Y13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "Y14")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "Y17")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "Y18")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "Y21")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "AA20")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "AA22")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "AA26")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "AB5")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "AB10")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "AB21")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "AB23")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "AB24")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "AB29")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "AC8")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "AC10")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "AC13")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "AC17")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "AC23")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "AE2")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "AF5")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "AF10")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "AF14")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "AF18")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "AF22")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "AF26")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "AF29")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "AH28")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "AJ5")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "AJ9")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "AJ13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "AJ17")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "AJ21")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "AJ25")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "AK1")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "AK30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX150T-CSG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX150T-CSG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 150 XC6SLX150T-CSG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX150T-CSG484_1_1"
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "G7")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "C18")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D20")
			)
			(pin power_in line
				(at -40.64 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -35.56 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E10")
			)
			(pin power_in line
				(at -33.02 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -30.48 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F6")
			)
			(pin power_in line
				(at -27.94 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H8")
			)
			(pin power_in line
				(at 12.7 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AA19")
			)
			(pin power_in line
				(at 15.24 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 17.78 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 20.32 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 22.86 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 25.4 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 27.94 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 30.48 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 33.02 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R15")
			)
			(pin power_in line
				(at 35.56 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L15P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L15N_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L16P_1")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L16N_1")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L17P_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L17N_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L18P_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L18N_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "AA21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "R12")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "R13")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "T12")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "T13")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "AB21")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "Y19")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "T15")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "T20")
			)
		)
		(symbol "XC6SLX150T-CSG484_2_1"
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AB5")
			)
			(pin power_in line
				(at -40.64 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -35.56 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -33.02 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U14")
			)
			(pin power_in line
				(at -30.48 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -27.94 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -25.4 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at -22.86 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W16")
			)
			(pin power_in line
				(at 10.16 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AA3")
			)
			(pin power_in line
				(at 12.7 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 15.24 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 17.78 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 20.32 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 22.86 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 25.4 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 27.94 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 30.48 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 33.02 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R7")
			)
			(pin power_in line
				(at 35.56 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T9")
			)
			(pin power_in line
				(at 38.1 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "V11")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "U10")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L12P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L12N_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L13P_3")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L13N_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "T5")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "T7")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "U9")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "T11")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "T10")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "R8")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L69P_3")
				(number "A3")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L69N_3")
				(number "A2")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L70P_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L70N_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L71P_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L71N_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L72P_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L72N_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L73P_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L73N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L74P_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L74N_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L75P_3")
				(number "D4")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L75N_3")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "D3")
			)
		)
		(symbol "XC6SLX150T-CSG484_3_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C9")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "A10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "D11")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "C11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B14")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A14")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B16")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A16")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D13")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C13")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C15")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "B12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "A12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "F14")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "E14")
			)
		)
		(symbol "XC6SLX150T-CSG484_4_1"
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B9")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "D12")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C10")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "B13")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "E13")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "E15")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A7")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E11")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D14")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A15")
			)
		)
		(symbol "XC6SLX150T-CSG484_5_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "F17")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "H16")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "C19")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "U16")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "W18")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "U12")
			)
		)
		(symbol "XC6SLX150T-CSG484_6_1"
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F18")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R11")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "RFUSE")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VBATT")
				(number "R14")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VFS")
				(number "U19")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B15")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "E12")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "F15")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "G14")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "V16")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX150T-FGG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX150T-FGG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 150 XC6SLX150T-FGG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX150T-FGG484_1_1"
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "C3")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "D4")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "C18")
			)
			(pin power_in line
				(at -40.64 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -35.56 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -33.02 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F6")
			)
			(pin power_in line
				(at -30.48 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -27.94 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G14")
			)
			(pin power_in line
				(at 17.78 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 20.32 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 22.86 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L9P_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L9N_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L10P_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L10N_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L21P_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21N_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "R15")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "V20")
			)
		)
		(symbol "XC6SLX150T-FGG484_2_1"
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "V17")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "W18")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L21P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L21N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L22P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L22N_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L57P_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L57N_2")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L59P_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L59N_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L60P_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L60N_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "AB5")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AA4")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AB4")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "U6")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "Y4")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AA3")
			)
			(pin power_in line
				(at -40.64 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -35.56 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -33.02 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA19")
			)
			(pin power_in line
				(at -30.48 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AB3")
			)
			(pin power_in line
				(at -27.94 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -25.4 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -22.86 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -20.32 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -17.78 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at -15.24 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at 17.78 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 20.32 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 22.86 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 25.4 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 27.94 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 30.48 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 33.02 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 35.56 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "T5")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L80P_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L80N_3")
				(number "G7")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L81P_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L81N_3")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L82P_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L82N_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "B1")
			)
		)
		(symbol "XC6SLX150T-FGG484_3_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C9")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "A10")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "C11")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "D11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B14")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A14")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B16")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A16")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D13")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C13")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C15")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "A12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "B12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "E12")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "F12")
			)
		)
		(symbol "XC6SLX150T-FGG484_4_1"
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B9")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "D12")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C10")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "B13")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "E13")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "E10")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A7")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E8")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D14")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A15")
			)
		)
		(symbol "XC6SLX150T-FGG484_5_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "G17")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "D20")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A21")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AB2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "AA22")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "V18")
			)
		)
		(symbol "XC6SLX150T-FGG484_6_1"
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "RFUSE")
				(number "P15")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VBATT")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VFS")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B15")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX150T-FGG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX150T-FGG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 150 XC6SLX150T-FGG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX150T-FGG676_1_1"
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "H7")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "G7")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "F6")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "C3")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "G6")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "F5")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L13P_0")
				(number "H9")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L13N_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L14P_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L14N_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L15P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L15N_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L16P_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L16N_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L21P_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L21N_0")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L22P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L22N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L23P_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L23N_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L24P_0")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L24N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L30P_0")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L30N_0")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L31P_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L31N_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "K12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "J12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L39P_0")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L39N_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L40P_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L40N_0")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L41P_0")
				(number "K14")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L41N_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L43P_0")
				(number "J15")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L43N_0")
				(number "H15")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "J16")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "J17")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "F18")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "E18")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L56P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L56N_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L57P_0")
				(number "F20")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L57N_0")
				(number "E20")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L58P_0")
				(number "H17")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L58N_0")
				(number "G17")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L59P_0")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L59N_0")
				(number "B21")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "H18")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "H19")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "G19")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "F19")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B23")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D22")
			)
			(pin power_in line
				(at -40.64 111.76 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B13")
			)
			(pin power_in line
				(at -38.1 111.76 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C4")
			)
			(pin power_in line
				(at -35.56 111.76 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C22")
			)
			(pin power_in line
				(at -33.02 111.76 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E21")
			)
			(pin power_in line
				(at -30.48 111.76 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F8")
			)
			(pin power_in line
				(at -27.94 111.76 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 111.76 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G18")
			)
			(pin power_in line
				(at -22.86 111.76 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H11")
			)
			(pin power_in line
				(at -20.32 111.76 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H16")
			)
			(pin power_in line
				(at -17.78 111.76 270)
				(length 6.35)
				(name "VCCO_0")
				(number "J14")
			)
			(pin power_in line
				(at 22.86 111.76 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AB23")
			)
			(pin power_in line
				(at 25.4 111.76 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AD25")
			)
			(pin power_in line
				(at 27.94 111.76 270)
				(length 6.35)
				(name "VCCO_1")
				(number "P18")
			)
			(pin power_in line
				(at 30.48 111.76 270)
				(length 6.35)
				(name "VCCO_1")
				(number "P23")
			)
			(pin power_in line
				(at 33.02 111.76 270)
				(length 6.35)
				(name "VCCO_1")
				(number "T25")
			)
			(pin power_in line
				(at 35.56 111.76 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin power_in line
				(at 38.1 111.76 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W23")
			)
			(pin power_in line
				(at 40.64 111.76 270)
				(length 6.35)
				(name "VCCO_1")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "L23")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "R24")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "U23")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "U24")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "V23")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "W24")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "U25")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "U26")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "V24")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "V26")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "W25")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "W26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "AA25")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "AA26")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "AD24")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "AB24")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "AB26")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "AC25")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "AC26")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "Y24")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "AE25")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "U21")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "AA23")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "AA24")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L69P_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L69N_VREF_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "AC23")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "AC24")
			)
		)
		(symbol "XC6SLX150T-FGG676_2_1"
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "AE24")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AF24")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "W20")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "V18")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "W19")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "W18")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AA17")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "V16")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "AA19")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "W16")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L24P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L24N_VREF_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L26P_2")
				(number "V14")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L26N_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L27P_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L27N_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L28P_2")
				(number "AA15")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L28N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "AE15")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "AF15")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AC14")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AD14")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AF14")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L33P_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L33N_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L34P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L34N_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L35P_2")
				(number "V12")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L35N_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L36P_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L36N_2")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AA11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "V10")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AD6")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AF6")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L51P_2")
				(number "AE5")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L51N_2")
				(number "AF5")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L52P_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L52N_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L53P_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L53N_2")
				(number "AC6")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L61P_2")
				(number "AC5")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L61N_VREF_2")
				(number "AD5")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "W7")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AD4")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AF4")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA7")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "AE3")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AF3")
			)
			(pin power_in line
				(at -40.64 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA14")
			)
			(pin power_in line
				(at -38.1 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA20")
			)
			(pin power_in line
				(at -35.56 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AB6")
			)
			(pin power_in line
				(at -33.02 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE4")
			)
			(pin power_in line
				(at -30.48 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE14")
			)
			(pin power_in line
				(at -27.94 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE23")
			)
			(pin power_in line
				(at -25.4 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W11")
			)
			(pin power_in line
				(at -22.86 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W15")
			)
			(pin power_in line
				(at -20.32 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y8")
			)
			(pin power_in line
				(at -17.78 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y18")
			)
			(pin power_in line
				(at 22.86 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AD2")
			)
			(pin power_in line
				(at 25.4 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P4")
			)
			(pin power_in line
				(at 27.94 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P9")
			)
			(pin power_in line
				(at 30.48 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T2")
			)
			(pin power_in line
				(at 33.02 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T7")
			)
			(pin power_in line
				(at 35.56 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W4")
			)
			(pin power_in line
				(at 38.1 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W6")
			)
			(pin power_in line
				(at 40.64 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "V7")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "V6")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L17P_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L17N_VREF_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "U9")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "R8")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "R10")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "T9")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "R5")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "N8")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "N5")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "P10")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "N9")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "M10")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "M9")
			)
		)
		(symbol "XC6SLX150T-FGG676_3_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L58P_4")
				(number "M4")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L58N_VREF_4")
				(number "N3")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L59P_M4DQ14_4")
				(number "N2")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L59N_M4DQ15_4")
				(number "N1")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L60P_M4DQ12_4")
				(number "M3")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L60N_M4DQ13_4")
				(number "M1")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L61P_M4UDQS_4")
				(number "L2")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L61N_M4UDQSN_4")
				(number "L1")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62P_M4DQ10_4")
				(number "K3")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L62N_M4DQ11_4")
				(number "K1")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63P_M4DQ8_4")
				(number "J2")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L63N_M4DQ9_4")
				(number "J1")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64P_M4DQ0_4")
				(number "H3")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L64N_M4DQ1_4")
				(number "H1")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65P_M4DQ2_4")
				(number "G2")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L65N_M4DQ3_4")
				(number "G1")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66P_M4LDQS_4")
				(number "F3")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L66N_M4LDQSN_4")
				(number "F1")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L67P_M4DQ6_4")
				(number "E2")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L67N_M4DQ7_4")
				(number "E1")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L68P_M4DQ4_4")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L68N_M4DQ5_4")
				(number "D1")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L69P_M4UDM_4")
				(number "J4")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L69N_M4LDM_4")
				(number "J3")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L70P_M4RASN_4")
				(number "L9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L70N_M4CASN_4")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L71P_M4A5_4")
				(number "L4")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L71N_M4A6_4")
				(number "L3")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L72P_M4A3_4")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L72N_M4ODT_4")
				(number "M6")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L73P_M4CLK_4")
				(number "K5")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L73N_M4CLKN_4")
				(number "J5")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L74P_M4A0_4")
				(number "L7")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L74N_M4A1_4")
				(number "L6")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L75P_M4BA0_4")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L75N_M4BA1_4")
				(number "B1")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L76P_M4A7_4")
				(number "L10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L76N_M4A2_4")
				(number "K10")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L77P_M4WE_4")
				(number "G4")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L77N_M4BA2_4")
				(number "G3")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L78P_M4A10_4")
				(number "J9")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L78N_M4A4_4")
				(number "J7")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L79P_M4A8_4")
				(number "C2")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L79N_M4A9_4")
				(number "C1")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L80P_M4CKE_4")
				(number "K9")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L80N_M4A12_4")
				(number "K8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L81P_M4RESET_4")
				(number "E4")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L81N_M4A11_4")
				(number "E3")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L82P_M4A13_4")
				(number "K7")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L82N_M4A14_4")
				(number "K6")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L83P_4")
				(number "H6")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L83N_VREF_4")
				(number "H5")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "D2")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "F4")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "H2")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "J6")
			)
			(pin power_in line
				(at -30.48 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "K4")
			)
			(pin power_in line
				(at -27.94 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "M2")
			)
			(pin power_in line
				(at -25.4 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "D25")
			)
			(pin power_in line
				(at 27.94 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "G22")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "H25")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "J21")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "K23")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "M20")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_A25_5")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_5")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L2P_M5A13_5")
				(number "B24")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L2N_M5A14_5")
				(number "A25")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L3P_M5RESET_5")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L3N_M5A11_5")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L4P_M5CKE_5")
				(number "D23")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L4N_M5A12_5")
				(number "C24")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L5P_M5A8_5")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L5N_M5A9_5")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L6P_M5A10_5")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L6N_M5A4_5")
				(number "G23")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L7P_M5WE_5")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L7N_M5BA2_5")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L8P_M5A7_5")
				(number "E23")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L8N_M5A2_5")
				(number "E24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L9P_M5BA0_5")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L9N_M5BA1_5")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L10P_M5A0_5")
				(number "C25")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L10N_M5A1_5")
				(number "C26")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L11P_M5CLK_5")
				(number "B25")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L11N_M5CLKN_5")
				(number "B26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L12P_M5A3_5")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L12N_M5ODT_5")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L13P_M5A5_5")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L13N_M5A6_5")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L14P_M5RASN_5")
				(number "F23")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L14N_M5CASN_5")
				(number "G24")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L15P_M5UDM_5")
				(number "J23")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L15N_M5LDM_5")
				(number "J24")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L16P_M5DQ4_5")
				(number "E25")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L16N_M5DQ5_5")
				(number "E26")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L17P_M5DQ6_5")
				(number "D24")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L17N_M5DQ7_5")
				(number "D26")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L18P_M5LDQS_5")
				(number "F24")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L18N_M5LDQSN_5")
				(number "F26")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L19P_M5DQ2_5")
				(number "H24")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L19N_M5DQ3_5")
				(number "H26")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L20P_M5DQ0_5")
				(number "G25")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L20N_M5DQ1_5")
				(number "G26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L21P_M5DQ8_5")
				(number "K24")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L21N_M5DQ9_5")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L22P_M5DQ10_5")
				(number "J25")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L22N_M5DQ11_5")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L23P_M5UDQS_5")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L23N_M5UDQSN_5")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L24P_M5DQ12_5")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L24N_M5DQ13_5")
				(number "L26")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L25P_M5DQ14_5")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L25N_M5DQ15_5")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L26P_5")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L26N_VREF_5")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L27P_5")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L27N_5")
				(number "L21")
			)
		)
		(symbol "XC6SLX150T-FGG676_4_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C9")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "A10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "D11")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "C11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B18")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A18")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B20")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A20")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D17")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C17")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D19")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C19")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "C15")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "B16")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "A16")
			)
		)
		(symbol "XC6SLX150T-FGG676_5_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_245")
				(number "AE7")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_245")
				(number "AF7")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_245")
				(number "AE9")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_245")
				(number "AF9")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_245")
				(number "AC8")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_245")
				(number "AD8")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_245")
				(number "AC10")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_245")
				(number "AD10")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_245")
				(number "AE11")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_245")
				(number "AF11")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_245")
				(number "AC12")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_245")
				(number "AD12")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_267")
				(number "AE19")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_267")
				(number "AF19")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_267")
				(number "AE21")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_267")
				(number "AF21")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_267")
				(number "AC18")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_267")
				(number "AD18")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_267")
				(number "AC20")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_267")
				(number "AD20")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_267")
				(number "AC16")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_267")
				(number "AD16")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_267")
				(number "AE17")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_267")
				(number "AF17")
			)
		)
		(symbol "XC6SLX150T-FGG676_6_1"
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B11")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "C12")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C10")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "C14")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "B15")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "C16")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_245")
				(number "AE12")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_245")
				(number "AD13")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_245")
				(number "AD11")
			)
			(pin power_in line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTAVCCPLL0_267")
				(number "AD15")
			)
			(pin power_in line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTAVCCPLL1_267")
				(number "AE16")
			)
			(pin power_in line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTAVCC_267")
				(number "AD17")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A7")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E11")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D18")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A19")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTTRX_245")
				(number "AC9")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_245")
				(number "AF8")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTRCAL_245")
				(number "AB12")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTRREF_245")
				(number "AB10")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTTRX_267")
				(number "AC19")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTTTX_267")
				(number "AF20")
			)
		)
		(symbol "XC6SLX150T-FGG676_7_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "C23")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "G21")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "F21")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A24")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AF25")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AF2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "Y22")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "Y19")
			)
		)
		(symbol "XC6SLX150T-FGG676_8_1"
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D20")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E17")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J10")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J18")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L18")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L22")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M17")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N10")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R22")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U6")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U12")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U14")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U18")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V17")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "W13")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA5")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB8")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB18")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC7")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC21")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "RFUSE")
				(number "V19")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VBATT")
				(number "V22")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VFS")
				(number "W22")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A15")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A17")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A21")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "B19")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C18")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "C20")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "D12")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "D14")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "E19")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "F2")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "F25")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "G14")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J19")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "K2")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K16")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K25")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "L15")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "L17")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "M5")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "M22")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "P2")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "P7")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "L16")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "M16")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "R16")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "R17")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "U16")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "P20")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "T5")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "T10")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "T18")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "U17")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "V2")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "V8")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "Y7")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "Y10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "Y14")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "Y23")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AB2")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AB16")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AB20")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AB25")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AC11")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AC13")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AC15")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AC17")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AD9")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AD19")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AD21")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AE6")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AE8")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AE10")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AE18")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AE20")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AF10")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AF12")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AF16")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AF18")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AF26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX150T-FGG900"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX150T-FGG900"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 150 XC6SLX150T-FGG900"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX150T-FGG900_1_1"
			(pin bidirectional line
				(at -50.8 134.62 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "H9")
			)
			(pin bidirectional line
				(at -50.8 132.08 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 129.54 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "F6")
			)
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "J8")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "H7")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "G7")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "E7")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "M10")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "L10")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L9P_0")
				(number "K10")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L9N_0")
				(number "J10")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L10P_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L10N_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L11P_0")
				(number "L11")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L11N_0")
				(number "K11")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L12P_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L12N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L13P_0")
				(number "B7")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L13N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L14P_0")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L14N_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L15P_0")
				(number "L12")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L15N_0")
				(number "K12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L16P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L16N_0")
				(number "E9")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L17P_0")
				(number "J12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L17N_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L18P_0")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L18N_0")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L19P_0")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L19N_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L20P_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L20N_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L21P_0")
				(number "M13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L21N_0")
				(number "L13")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L22P_0")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L22N_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L23P_0")
				(number "L14")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L23N_0")
				(number "K14")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L24P_0")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L24N_0")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L25P_0")
				(number "M15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L25N_0")
				(number "K15")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L26P_0")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L26N_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "J14")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "E15")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "H15")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "D16")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "B17")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L43P_0")
				(number "L17")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L43N_0")
				(number "K17")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L44P_0")
				(number "H17")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L44N_0")
				(number "G17")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L45P_0")
				(number "H16")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L45N_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L46P_0")
				(number "G18")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L46N_0")
				(number "F18")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "M18")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "L18")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "E17")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "K19")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "J19")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "F19")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "E19")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "M19")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "L19")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L52P_0")
				(number "H19")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L52N_0")
				(number "G19")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L53P_0")
				(number "J18")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L53N_0")
				(number "H18")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L54P_0")
				(number "G20")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L54N_0")
				(number "F20")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L55P_0")
				(number "K20")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L55N_0")
				(number "J20")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L56P_0")
				(number "F21")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L56N_0")
				(number "E21")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L57P_0")
				(number "M20")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L57N_0")
				(number "L20")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L58P_0")
				(number "G22")
			)
			(pin bidirectional line
				(at -50.8 -111.76 0)
				(length 6.35)
				(name "IO_L58N_0")
				(number "F22")
			)
			(pin bidirectional line
				(at -50.8 -114.3 0)
				(length 6.35)
				(name "IO_L59P_0")
				(number "L21")
			)
			(pin bidirectional line
				(at -50.8 -116.84 0)
				(length 6.35)
				(name "IO_L59N_0")
				(number "K21")
			)
			(pin bidirectional line
				(at -50.8 -119.38 0)
				(length 6.35)
				(name "IO_L60P_0")
				(number "F23")
			)
			(pin bidirectional line
				(at -50.8 -121.92 0)
				(length 6.35)
				(name "IO_L60N_0")
				(number "E23")
			)
			(pin bidirectional line
				(at -50.8 -124.46 0)
				(length 6.35)
				(name "IO_L61P_0")
				(number "H21")
			)
			(pin bidirectional line
				(at -50.8 -127 0)
				(length 6.35)
				(name "IO_L61N_0")
				(number "G21")
			)
			(pin bidirectional line
				(at -50.8 -129.54 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "F24")
			)
			(pin bidirectional line
				(at -50.8 -132.08 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "E24")
			)
			(pin bidirectional line
				(at -50.8 -134.62 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B25")
			)
			(pin bidirectional line
				(at -50.8 -137.16 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A25")
			)
			(pin bidirectional line
				(at -50.8 -139.7 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "D24")
			)
			(pin bidirectional line
				(at -50.8 -142.24 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "C24")
			)
			(pin bidirectional line
				(at -50.8 -144.78 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "J22")
			)
			(pin bidirectional line
				(at -50.8 -147.32 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "H22")
			)
			(pin bidirectional line
				(at -50.8 -149.86 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "E25")
			)
			(pin bidirectional line
				(at -50.8 -152.4 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D25")
			)
			(pin power_in line
				(at -40.64 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B16")
			)
			(pin power_in line
				(at -38.1 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C7")
			)
			(pin power_in line
				(at -35.56 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C25")
			)
			(pin power_in line
				(at -33.02 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F16")
			)
			(pin power_in line
				(at -30.48 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G8")
			)
			(pin power_in line
				(at -27.94 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G23")
			)
			(pin power_in line
				(at -22.86 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H10")
			)
			(pin power_in line
				(at -20.32 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H20")
			)
			(pin power_in line
				(at -17.78 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "J17")
			)
			(pin power_in line
				(at -15.24 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "K13")
			)
			(pin power_in line
				(at -12.7 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "L9")
			)
			(pin power_in line
				(at -10.16 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "L15")
			)
			(pin power_in line
				(at -7.62 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "M17")
			)
			(pin power_in line
				(at -5.08 154.94 270)
				(length 6.35)
				(name "VCCO_0")
				(number "M21")
			)
			(pin power_in line
				(at 7.62 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AA23")
			)
			(pin power_in line
				(at 10.16 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AC26")
			)
			(pin power_in line
				(at 12.7 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AD29")
			)
			(pin power_in line
				(at 15.24 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AH29")
			)
			(pin power_in line
				(at 17.78 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AJ27")
			)
			(pin power_in line
				(at 20.32 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N23")
			)
			(pin power_in line
				(at 22.86 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "P21")
			)
			(pin power_in line
				(at 25.4 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R23")
			)
			(pin power_in line
				(at 27.94 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R26")
			)
			(pin power_in line
				(at 30.48 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "T29")
			)
			(pin power_in line
				(at 33.02 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U23")
			)
			(pin power_in line
				(at 35.56 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W23")
			)
			(pin power_in line
				(at 38.1 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W26")
			)
			(pin power_in line
				(at 40.64 154.94 270)
				(length 6.35)
				(name "VCCO_1")
				(number "Y29")
			)
			(pin bidirectional line
				(at 50.8 134.62 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 132.08 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 129.54 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "N29")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "N30")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "N27")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "N28")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "P28")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "P30")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "P27")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "R29")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "R30")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "R27")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "R28")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "T27")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "T28")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "T30")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "U29")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "U30")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "U27")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "U28")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "V28")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "V30")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "V26")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "V27")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "W27")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "W28")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "AB28")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "AB30")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "W29")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "W30")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "Y28")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "Y30")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "AA29")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "AA30")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "AA27")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "AA28")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "Y27")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "AD28")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "AD30")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "AC27")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "AC28")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "AC29")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "AC30")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "AE29")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "AE30")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "AE27")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "AE28")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "W24")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "W25")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L54P_1")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L54N_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L55P_1")
				(number "AF28")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L55N_1")
				(number "AF30")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L56P_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L56N_1")
				(number "P23")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L57P_1")
				(number "AG29")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L57N_1")
				(number "AG30")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "P25")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "AH30")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "AJ30")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "R24")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "AJ29")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "AK29")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "T25")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "AJ28")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "AK28")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "U24")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "U25")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AG27")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AG28")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "V23")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "V24")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "AD27")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L69P_1")
				(number "AH27")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L69N_VREF_1")
				(number "AK27")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "Y23")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "AE25")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "Y24")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "AG26")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "AH26")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "AA24")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "AA25")
			)
		)
		(symbol "XC6SLX150T-FGG900_2_1"
			(pin bidirectional line
				(at -50.8 134.62 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "AJ26")
			)
			(pin bidirectional line
				(at -50.8 132.08 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AK26")
			)
			(pin bidirectional line
				(at -50.8 129.54 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AC24")
			)
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AD24")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AJ25")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AK25")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AB23")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AC23")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "AE24")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AF24")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L7P_2")
				(number "AE23")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L7N_2")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L8P_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L8N_2")
				(number "AC21")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L9P_2")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L9N_2")
				(number "AE22")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L10P_2")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L10N_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L11P_2")
				(number "AF25")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L11N_2")
				(number "AG25")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "AC20")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "AG24")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AH24")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AC19")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AD19")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AF21")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "AD20")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "AE20")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "W20")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AE19")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AF19")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "AA19")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L21P_2")
				(number "AD18")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L21N_2")
				(number "AE18")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L22P_2")
				(number "W19")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L22N_2")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "AD17")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L28P_2")
				(number "AE17")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L28N_2")
				(number "AF17")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "AC16")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "AD16")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AF16")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AG16")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AH16")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AK16")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AJ17")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AK17")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L33P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L33N_2")
				(number "AA17")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L34P_2")
				(number "AJ15")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L34N_2")
				(number "AK15")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "AC14")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AD14")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AE14")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "AE15")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AF15")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "AC15")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "AD15")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AD12")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AE12")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "AA15")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AC13")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AF11")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L51P_2")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L51N_2")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L52P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L52N_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L53P_2")
				(number "AD10")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L53N_2")
				(number "AE10")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L54P_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L54N_2")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L55P_2")
				(number "AG8")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L55N_2")
				(number "AH8")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L56P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L56N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L57P_2")
				(number "AE9")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L57N_2")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "AA11")
			)
			(pin bidirectional line
				(at -50.8 -111.76 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -114.3 0)
				(length 6.35)
				(name "IO_L59P_2")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 -116.84 0)
				(length 6.35)
				(name "IO_L59N_2")
				(number "AG7")
			)
			(pin bidirectional line
				(at -50.8 -119.38 0)
				(length 6.35)
				(name "IO_L60P_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -121.92 0)
				(length 6.35)
				(name "IO_L60N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -124.46 0)
				(length 6.35)
				(name "IO_L61P_2")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 -127 0)
				(length 6.35)
				(name "IO_L61N_VREF_2")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 -129.54 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "AH7")
			)
			(pin bidirectional line
				(at -50.8 -132.08 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "AK7")
			)
			(pin bidirectional line
				(at -50.8 -134.62 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 -137.16 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AE8")
			)
			(pin bidirectional line
				(at -50.8 -139.7 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AG6")
			)
			(pin bidirectional line
				(at -50.8 -142.24 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AH6")
			)
			(pin bidirectional line
				(at -50.8 -144.78 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "AJ6")
			)
			(pin bidirectional line
				(at -50.8 -147.32 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AK6")
			)
			(pin power_in line
				(at -40.64 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA12")
			)
			(pin power_in line
				(at -38.1 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA16")
			)
			(pin power_in line
				(at -35.56 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA20")
			)
			(pin power_in line
				(at -33.02 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC10")
			)
			(pin power_in line
				(at -30.48 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC18")
			)
			(pin power_in line
				(at -27.94 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AD13")
			)
			(pin power_in line
				(at -25.4 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AD21")
			)
			(pin power_in line
				(at -22.86 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AD23")
			)
			(pin power_in line
				(at -20.32 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE16")
			)
			(pin power_in line
				(at -17.78 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AF8")
			)
			(pin power_in line
				(at -15.24 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AH25")
			)
			(pin power_in line
				(at -12.7 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AJ7")
			)
			(pin power_in line
				(at -10.16 154.94 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AJ16")
			)
			(pin power_in line
				(at 7.62 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AA8")
			)
			(pin power_in line
				(at 10.16 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AC2")
			)
			(pin power_in line
				(at 12.7 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AD5")
			)
			(pin power_in line
				(at 15.24 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AG2")
			)
			(pin power_in line
				(at 17.78 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AJ3")
			)
			(pin power_in line
				(at 20.32 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M8")
			)
			(pin power_in line
				(at 22.86 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 27.94 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R8")
			)
			(pin power_in line
				(at 30.48 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T5")
			)
			(pin power_in line
				(at 33.02 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U8")
			)
			(pin power_in line
				(at 35.56 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin power_in line
				(at 38.1 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "Y5")
			)
			(pin power_in line
				(at 40.64 154.94 270)
				(length 6.35)
				(name "VCCO_3")
				(number "Y10")
			)
			(pin bidirectional line
				(at 50.8 134.62 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AA10")
			)
			(pin bidirectional line
				(at 50.8 132.08 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AA9")
			)
			(pin bidirectional line
				(at 50.8 129.54 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "AD7")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "AE7")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L3P_3")
				(number "Y9")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L3N_3")
				(number "Y8")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L4P_3")
				(number "AE6")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L4N_3")
				(number "AF6")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L5P_3")
				(number "W11")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L5N_3")
				(number "Y11")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L6P_3")
				(number "AE5")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L6N_3")
				(number "AG5")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "T7")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "AA7")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AA6")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "AC6")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "AD6")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "AH5")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "AK5")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "W10")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "W9")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L12P_3")
				(number "AB7")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L12N_3")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L13P_3")
				(number "W7")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L13N_3")
				(number "W6")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L14P_3")
				(number "AJ4")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L14N_3")
				(number "AK4")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L15P_3")
				(number "T9")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L15N_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L16P_3")
				(number "AH3")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L16N_3")
				(number "AK3")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L17P_3")
				(number "Y7")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L17N_VREF_3")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "AJ2")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "AK2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L19P_3")
				(number "AE4")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L19N_3")
				(number "AF4")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "AF3")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "AG3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "V8")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "V7")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "AH1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "AJ1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "V10")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "V9")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "AG4")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "AH4")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "N10")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "N9")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "AH2")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L27P_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L27N_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L28P_3")
				(number "AF1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L28N_3")
				(number "AG1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L29P_3")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L29N_3")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L30P_3")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L30N_3")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "N8")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "AC5")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "AD2")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "R5")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "N5")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 -144.78 180)
				(length 6.35)
				(name "IO_L56P_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 -147.32 180)
				(length 6.35)
				(name "IO_L56N_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 -149.86 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 -152.4 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "M6")
			)
		)
		(symbol "XC6SLX150T-FGG900_3_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L58P_4")
				(number "L7")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L58N_VREF_4")
				(number "L6")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L59P_M4DQ14_4")
				(number "M2")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L59N_M4DQ15_4")
				(number "M1")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L60P_M4DQ12_4")
				(number "L3")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L60N_M4DQ13_4")
				(number "L1")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L61P_M4UDQS_4")
				(number "K2")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L61N_M4UDQSN_4")
				(number "K1")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62P_M4DQ10_4")
				(number "L5")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L62N_M4DQ11_4")
				(number "L4")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63P_M4DQ8_4")
				(number "M4")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L63N_M4DQ9_4")
				(number "M3")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64P_M4DQ0_4")
				(number "H4")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L64N_M4DQ1_4")
				(number "H3")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65P_M4DQ2_4")
				(number "J3")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L65N_M4DQ3_4")
				(number "J1")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66P_M4LDQS_4")
				(number "J5")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L66N_M4LDQSN_4")
				(number "J4")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L67P_M4DQ6_4")
				(number "H2")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L67N_M4DQ7_4")
				(number "H1")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L68P_M4DQ4_4")
				(number "G3")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L68N_M4DQ5_4")
				(number "G1")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L69P_M4UDM_4")
				(number "K4")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L69N_M4LDM_4")
				(number "K3")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L70P_M4RASN_4")
				(number "C1")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L70N_M4CASN_4")
				(number "B1")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L71P_M4A5_4")
				(number "F2")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L71N_M4A6_4")
				(number "F1")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L72P_M4A3_4")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L72N_M4ODT_4")
				(number "E4")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L73P_M4CLK_4")
				(number "E3")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L73N_M4CLKN_4")
				(number "E1")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L74P_M4A0_4")
				(number "D4")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L74N_M4A1_4")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L75P_M4BA0_4")
				(number "D2")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L75N_M4BA1_4")
				(number "D1")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L76P_M4A7_4")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L76N_M4A2_4")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L77P_M4WE_4")
				(number "F4")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L77N_M4BA2_4")
				(number "F3")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L78P_M4A10_4")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L78N_M4A4_4")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L79P_M4A8_4")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L79N_M4A9_4")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L80P_M4CKE_4")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L80N_M4A12_4")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L81P_M4RESET_4")
				(number "G5")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L81N_M4A11_4")
				(number "G4")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L82P_M4A13_4")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L82N_M4A14_4")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L83P_4")
				(number "J6")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L83N_VREF_4")
				(number "H6")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "C2")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "G2")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "H5")
			)
			(pin power_in line
				(at -30.48 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "K6")
			)
			(pin power_in line
				(at -27.94 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "L2")
			)
			(pin power_in line
				(at -25.4 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "M5")
			)
			(pin power_in line
				(at 22.86 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "B28")
			)
			(pin power_in line
				(at 25.4 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "D29")
			)
			(pin power_in line
				(at 27.94 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "G26")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "H29")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "J25")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "K24")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "L26")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "M29")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_A25_5")
				(number "G25")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_5")
				(number "F25")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L2P_M5A13_5")
				(number "A28")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L2N_M5A14_5")
				(number "A29")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L3P_M5RESET_5")
				(number "C26")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L3N_M5A11_5")
				(number "A26")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L4P_M5CKE_5")
				(number "B29")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L4N_M5A12_5")
				(number "B30")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L5P_M5A8_5")
				(number "B27")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L5N_M5A9_5")
				(number "A27")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L6P_M5A10_5")
				(number "F26")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L6N_M5A4_5")
				(number "F27")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L7P_M5WE_5")
				(number "E26")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L7N_M5BA2_5")
				(number "D26")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L8P_M5A7_5")
				(number "C29")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L8N_M5A2_5")
				(number "C30")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L9P_M5BA0_5")
				(number "D27")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L9N_M5BA1_5")
				(number "C27")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L10P_M5A0_5")
				(number "D28")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L10N_M5A1_5")
				(number "D30")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L11P_M5CLK_5")
				(number "E27")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L11N_M5CLKN_5")
				(number "E28")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L12P_M5A3_5")
				(number "E29")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L12N_M5ODT_5")
				(number "E30")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L13P_M5A5_5")
				(number "H26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L13N_M5A6_5")
				(number "H27")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L14P_M5RASN_5")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L14N_M5CASN_5")
				(number "K27")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L15P_M5UDM_5")
				(number "J27")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L15N_M5LDM_5")
				(number "J28")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L16P_M5DQ4_5")
				(number "G27")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L16N_M5DQ5_5")
				(number "G28")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L17P_M5DQ6_5")
				(number "F28")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L17N_M5DQ7_5")
				(number "F30")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L18P_M5LDQS_5")
				(number "J29")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L18N_M5LDQSN_5")
				(number "J30")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L19P_M5DQ2_5")
				(number "G29")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L19N_M5DQ3_5")
				(number "G30")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L20P_M5DQ0_5")
				(number "H28")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L20N_M5DQ1_5")
				(number "H30")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L21P_M5DQ8_5")
				(number "L27")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L21N_M5DQ9_5")
				(number "L28")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L22P_M5DQ10_5")
				(number "L29")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L22N_M5DQ11_5")
				(number "L30")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L23P_M5UDQS_5")
				(number "K28")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L23N_M5UDQSN_5")
				(number "K30")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L24P_M5DQ12_5")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L24N_M5DQ13_5")
				(number "M27")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L25P_M5DQ14_5")
				(number "M28")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L25N_M5DQ15_5")
				(number "M30")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L26P_5")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L26N_VREF_5")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L27P_5")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L27N_5")
				(number "L25")
			)
		)
		(symbol "XC6SLX150T-FGG900_4_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B9")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A9")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B11")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A11")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D10")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C10")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D12")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C12")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "B13")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "A13")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "D14")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "C14")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B21")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A21")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B23")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A23")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D20")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C20")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D22")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C22")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "D18")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "C18")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "B19")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "A19")
			)
		)
		(symbol "XC6SLX150T-FGG900_5_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_245")
				(number "AJ9")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_245")
				(number "AK9")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_245")
				(number "AJ11")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_245")
				(number "AK11")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_245")
				(number "AG10")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_245")
				(number "AH10")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_245")
				(number "AG12")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_245")
				(number "AH12")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_245")
				(number "AJ13")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_245")
				(number "AK13")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_245")
				(number "AG14")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_245")
				(number "AH14")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_267")
				(number "AJ21")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_267")
				(number "AK21")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_267")
				(number "AJ23")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_267")
				(number "AK23")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_267")
				(number "AG20")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_267")
				(number "AH20")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_267")
				(number "AG22")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_267")
				(number "AH22")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_267")
				(number "AG18")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_267")
				(number "AH18")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_267")
				(number "AJ19")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_267")
				(number "AK19")
			)
		)
		(symbol "XC6SLX150T-FGG900_6_1"
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B14")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "C15")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C13")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "C17")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "B18")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "C19")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_245")
				(number "AJ14")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_245")
				(number "AH15")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_245")
				(number "AH13")
			)
			(pin power_in line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTAVCCPLL0_267")
				(number "AH17")
			)
			(pin power_in line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTAVCCPLL1_267")
				(number "AJ18")
			)
			(pin power_in line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTAVCC_267")
				(number "AH19")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D11")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A10")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E14")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E12")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D21")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A22")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTTRX_245")
				(number "AG11")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_245")
				(number "AK10")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTRCAL_245")
				(number "AF14")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTRREF_245")
				(number "AF12")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTTRX_267")
				(number "AG21")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTTTX_267")
				(number "AK22")
			)
		)
		(symbol "XC6SLX150T-FGG900_7_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "J24")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "H25")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "K25")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "H23")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AD25")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "AB25")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "AC25")
			)
		)
		(symbol "XC6SLX150T-FGG900_8_1"
			(pin power_in line
				(at -25.4 134.62 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D9")
			)
			(pin power_in line
				(at -25.4 132.08 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D23")
			)
			(pin power_in line
				(at -25.4 129.54 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G6")
			)
			(pin power_in line
				(at -25.4 127 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H24")
			)
			(pin power_in line
				(at -25.4 124.46 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J7")
			)
			(pin power_in line
				(at -25.4 121.92 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 119.38 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 116.84 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J23")
			)
			(pin power_in line
				(at -25.4 114.3 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L22")
			)
			(pin power_in line
				(at -25.4 111.76 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M11")
			)
			(pin power_in line
				(at -25.4 109.22 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M14")
			)
			(pin power_in line
				(at -25.4 106.68 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M25")
			)
			(pin power_in line
				(at -25.4 104.14 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N6")
			)
			(pin power_in line
				(at -25.4 101.6 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 99.06 0)
				(length 6.35)
				(name "VCCAUX")
				(number "T21")
			)
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U10")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V21")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V25")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 6.35)
				(name "VCCAUX")
				(number "W13")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX")
				(number "W15")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX")
				(number "W17")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX")
				(number "Y18")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB24")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC7")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AG9")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AG23")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "RFUSE")
				(number "AB27")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VBATT")
				(number "AB26")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VFS")
				(number "AF27")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "GND")
				(number "A8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "GND")
				(number "A12")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "GND")
				(number "A14")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "GND")
				(number "A18")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "GND")
				(number "A20")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "GND")
				(number "A24")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "GND")
				(number "A30")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "GND")
				(number "B8")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "GND")
				(number "B10")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "GND")
				(number "B12")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "GND")
				(number "B20")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "GND")
				(number "B22")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "B24")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "B26")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "C9")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "C11")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "C21")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "C23")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "C28")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D15")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D17")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D19")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E10")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "E18")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E20")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "F5")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "F29")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G24")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J16")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "J26")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "K5")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "K16")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "K18")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "K22")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K23")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K29")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "L16")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "L23")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "M9")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "M16")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "M22")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at -25.4 -99.06 0)
				(length 6.35)
				(name "GND")
				(number "N18")
			)
			(pin power_in line
				(at -25.4 -101.6 0)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at -25.4 -104.14 0)
				(length 6.35)
				(name "GND")
				(number "N22")
			)
			(pin power_in line
				(at -25.4 -106.68 0)
				(length 6.35)
				(name "GND")
				(number "N26")
			)
			(pin power_in line
				(at -25.4 -109.22 0)
				(length 6.35)
				(name "GND")
				(number "P5")
			)
			(pin power_in line
				(at -25.4 -111.76 0)
				(length 6.35)
				(name "GND")
				(number "P8")
			)
			(pin power_in line
				(at -25.4 -114.3 0)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 -116.84 0)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at -25.4 -119.38 0)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 -121.92 0)
				(length 6.35)
				(name "GND")
				(number "P17")
			)
			(pin power_in line
				(at -25.4 -124.46 0)
				(length 6.35)
				(name "GND")
				(number "P18")
			)
			(pin power_in line
				(at -25.4 -127 0)
				(length 6.35)
				(name "GND")
				(number "P20")
			)
			(pin power_in line
				(at -25.4 -129.54 0)
				(length 6.35)
				(name "GND")
				(number "P29")
			)
			(pin power_in line
				(at -25.4 -132.08 0)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at -25.4 -134.62 0)
				(length 6.35)
				(name "GND")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 134.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 132.08 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 129.54 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 127 180)
				(length 6.35)
				(name "VCCINT")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 124.46 180)
				(length 6.35)
				(name "VCCINT")
				(number "N19")
			)
			(pin power_in line
				(at 25.4 121.92 180)
				(length 6.35)
				(name "VCCINT")
				(number "N20")
			)
			(pin power_in line
				(at 25.4 119.38 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 116.84 180)
				(length 6.35)
				(name "VCCINT")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 114.3 180)
				(length 6.35)
				(name "VCCINT")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 111.76 180)
				(length 6.35)
				(name "VCCINT")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 109.22 180)
				(length 6.35)
				(name "VCCINT")
				(number "P19")
			)
			(pin power_in line
				(at 25.4 106.68 180)
				(length 6.35)
				(name "VCCINT")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 104.14 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 101.6 180)
				(length 6.35)
				(name "VCCINT")
				(number "R17")
			)
			(pin power_in line
				(at 25.4 99.06 180)
				(length 6.35)
				(name "VCCINT")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "T18")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "U15")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "U16")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "U19")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "U20")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "V11")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "V12")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "V15")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "V16")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "V19")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "V20")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "GND")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "GND")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "GND")
				(number "R16")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "GND")
				(number "R19")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "GND")
				(number "R20")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "GND")
				(number "T10")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "GND")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "GND")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "GND")
				(number "T19")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "GND")
				(number "T20")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "GND")
				(number "T22")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "GND")
				(number "T23")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "U9")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "U13")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "U14")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "U17")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "U18")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "U22")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "U26")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "V5")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "V13")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "V17")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "V22")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "V29")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "W8")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "W18")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "AA2")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AA26")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AB5")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AB15")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AB29")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AC8")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AC17")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AE2")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AF5")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AF10")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AF18")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AF20")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AF22")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AF26")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AF29")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AG13")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AG15")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AG17")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AG19")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AH9")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AH11")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AH21")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AH23")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AH28")
			)
			(pin power_in line
				(at 25.4 -99.06 180)
				(length 6.35)
				(name "GND")
				(number "AJ5")
			)
			(pin power_in line
				(at 25.4 -101.6 180)
				(length 6.35)
				(name "GND")
				(number "AJ8")
			)
			(pin power_in line
				(at 25.4 -104.14 180)
				(length 6.35)
				(name "GND")
				(number "AJ10")
			)
			(pin power_in line
				(at 25.4 -106.68 180)
				(length 6.35)
				(name "GND")
				(number "AJ12")
			)
			(pin power_in line
				(at 25.4 -109.22 180)
				(length 6.35)
				(name "GND")
				(number "AJ20")
			)
			(pin power_in line
				(at 25.4 -111.76 180)
				(length 6.35)
				(name "GND")
				(number "AJ22")
			)
			(pin power_in line
				(at 25.4 -114.3 180)
				(length 6.35)
				(name "GND")
				(number "AJ24")
			)
			(pin power_in line
				(at 25.4 -116.84 180)
				(length 6.35)
				(name "GND")
				(number "AK1")
			)
			(pin power_in line
				(at 25.4 -119.38 180)
				(length 6.35)
				(name "GND")
				(number "AK8")
			)
			(pin power_in line
				(at 25.4 -121.92 180)
				(length 6.35)
				(name "GND")
				(number "AK12")
			)
			(pin power_in line
				(at 25.4 -124.46 180)
				(length 6.35)
				(name "GND")
				(number "AK14")
			)
			(pin power_in line
				(at 25.4 -127 180)
				(length 6.35)
				(name "GND")
				(number "AK18")
			)
			(pin power_in line
				(at 25.4 -129.54 180)
				(length 6.35)
				(name "GND")
				(number "AK20")
			)
			(pin power_in line
				(at 25.4 -132.08 180)
				(length 6.35)
				(name "GND")
				(number "AK24")
			)
			(pin power_in line
				(at 25.4 -134.62 180)
				(length 6.35)
				(name "GND")
				(number "AK30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX16-CPG196"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX16-CPG196"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 16 XC6SLX16-CPG196"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX16-CPG196_1_1"
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B7")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "C11")
			)
			(pin power_in line
				(at -40.64 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C4")
			)
			(pin power_in line
				(at -38.1 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C5")
			)
			(pin power_in line
				(at -35.56 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C9")
			)
			(pin power_in line
				(at -33.02 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C10")
			)
			(pin power_in line
				(at 27.94 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "D12")
			)
			(pin power_in line
				(at 30.48 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E12")
			)
			(pin power_in line
				(at 33.02 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G11")
			)
			(pin power_in line
				(at 35.56 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G12")
			)
			(pin power_in line
				(at 38.1 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "K11")
			)
			(pin power_in line
				(at 40.64 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L1P_1")
				(number "C12")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L1N_VREF_1")
				(number "C13")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L32P_1")
				(number "D13")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L32N_1")
				(number "D14")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L33P_1")
				(number "E13")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L33N_1")
				(number "E14")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L34P_1")
				(number "F11")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L34N_1")
				(number "F12")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_1")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_1")
				(number "H11")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45P_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45N_1")
				(number "J14")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46P_1")
				(number "J11")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46N_1")
				(number "J12")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47P_1")
				(number "K13")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L47N_1")
				(number "K14")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "L13")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "M14")
			)
		)
		(symbol "XC6SLX16-CPG196_2_1"
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "N13")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "P13")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "P12")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "N10")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "P10")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "P9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "P8")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "N7")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "P6")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "P5")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "L4")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "M4")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "N4")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "P4")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "N3")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "P3")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "N2")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "P2")
			)
			(pin power_in line
				(at -40.64 45.72 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M5")
			)
			(pin power_in line
				(at -38.1 45.72 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M6")
			)
			(pin power_in line
				(at -35.56 45.72 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M9")
			)
			(pin power_in line
				(at -33.02 45.72 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M10")
			)
			(pin power_in line
				(at 27.94 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "E3")
			)
			(pin power_in line
				(at 30.48 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "E4")
			)
			(pin power_in line
				(at 33.02 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G3")
			)
			(pin power_in line
				(at 35.56 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "K3")
			)
			(pin power_in line
				(at 40.64 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L36P_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L36N_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L37P_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L37N_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_3")
				(number "J2")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_3")
				(number "G2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L49P_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L49N_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L50P_3")
				(number "E2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L50N_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L51P_3")
				(number "D4")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L51N_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L52P_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L52N_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "B1")
			)
		)
		(symbol "XC6SLX16-CPG196_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "A13")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "C14")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "B14")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "B13")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "N14")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "N1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "L12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "M12")
			)
		)
		(symbol "XC6SLX16-CPG196_4_1"
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G9")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H5")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H6")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A14")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "C2")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C7")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D5")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "D9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E8")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "G4")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "G6")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "G7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "E5")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "E6")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "E9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "E10")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "F5")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "F6")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "F9")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "F10")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "J6")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "K5")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "K6")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "H10")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "J7")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "L3")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "L6")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "M3")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "P1")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX16-CSG225"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX16-CSG225"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 16 XC6SLX16-CSG225"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX16-CSG225_1_1"
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "E7")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B7")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L39P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L39N_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L40P_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L40N_0")
				(number "E9")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B13")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A12")
			)
			(pin power_in line
				(at -40.64 60.96 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 60.96 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B8")
			)
			(pin power_in line
				(at -35.56 60.96 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B12")
			)
			(pin power_in line
				(at -33.02 60.96 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D9")
			)
			(pin power_in line
				(at 33.02 60.96 270)
				(length 6.35)
				(name "VCCO_1")
				(number "D14")
			)
			(pin power_in line
				(at 35.56 60.96 270)
				(length 6.35)
				(name "VCCO_1")
				(number "H14")
			)
			(pin power_in line
				(at 38.1 60.96 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J12")
			)
			(pin power_in line
				(at 40.64 60.96 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M14")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "B14")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "B15")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "G11")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "G12")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "F11")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "F12")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "H10")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "H11")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "C14")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "C15")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "D13")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "D15")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "J11")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "E14")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "K10")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "K11")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "L12")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "J14")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "J15")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K13")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M15")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "P14")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "P15")
			)
		)
		(symbol "XC6SLX16-CSG225_2_1"
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "R12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "P13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "M11")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N10")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "R10")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "L9")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "M10")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "M9")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "N9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "P9")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "N7")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "K8")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "L7")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "M6")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "R6")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "P5")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "R5")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "L6")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "L5")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "N4")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "R4")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "M5")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "P3")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "R3")
			)
			(pin power_in line
				(at -40.64 63.5 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M7")
			)
			(pin power_in line
				(at -38.1 63.5 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P4")
			)
			(pin power_in line
				(at -35.56 63.5 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P8")
			)
			(pin power_in line
				(at -33.02 63.5 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P12")
			)
			(pin power_in line
				(at 33.02 63.5 270)
				(length 6.35)
				(name "VCCO_3")
				(number "D2")
			)
			(pin power_in line
				(at 35.56 63.5 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G4")
			)
			(pin power_in line
				(at 38.1 63.5 270)
				(length 6.35)
				(name "VCCO_3")
				(number "H2")
			)
			(pin power_in line
				(at 40.64 63.5 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J2")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "G2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "J5")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "G5")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "E5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "E2")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "D4")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "C1")
			)
		)
		(symbol "XC6SLX16-CSG225_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E10")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "D12")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "E13")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A14")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "R14")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "R2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "L13")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "L10")
			)
		)
		(symbol "XC6SLX16-CSG225_4_1"
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B1")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E12")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J6")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K9")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L4")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "A15")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B6")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B10")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C13")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "F2")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F6")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F14")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G7")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G9")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "F9")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "G6")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "G8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "H7")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "K7")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "J7")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "K2")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "K6")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N3")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P6")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX16-CSG324"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX16-CSG324"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 16 XC6SLX16-CSG324"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX16-CSG324_1_1"
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "D4")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L9P_0")
				(number "E7")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L9N_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L10P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L10N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L11P_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L11N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L39P_0")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L39N_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L40P_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L40N_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L41P_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L41N_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L42P_0")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L42N_0")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A16")
			)
			(pin power_in line
				(at -40.64 86.36 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B5")
			)
			(pin power_in line
				(at -38.1 86.36 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B10")
			)
			(pin power_in line
				(at -35.56 86.36 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -33.02 86.36 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D7")
			)
			(pin power_in line
				(at -30.48 86.36 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D13")
			)
			(pin power_in line
				(at -27.94 86.36 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E10")
			)
			(pin power_in line
				(at 27.94 86.36 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E17")
			)
			(pin power_in line
				(at 30.48 86.36 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G15")
			)
			(pin power_in line
				(at 33.02 86.36 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J14")
			)
			(pin power_in line
				(at 35.56 86.36 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J17")
			)
			(pin power_in line
				(at 38.1 86.36 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M15")
			)
			(pin power_in line
				(at 40.64 86.36 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "K13")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "K14")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "L12")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "L13")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "L16")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "U18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "M14")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "P16")
			)
		)
		(symbol "XC6SLX16-CSG324_2_1"
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "R15")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "V16")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "T13")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "V14")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "P12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "M11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "V12")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "N10")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L22P_2")
				(number "M10")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L22N_2")
				(number "N9")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "U11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "R10")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "V10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "T9")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "U7")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "N7")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "P8")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "V6")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "R5")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "T5")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "U5")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "V5")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "R3")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "T3")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "T4")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "V4")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "P6")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "U3")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "V3")
			)
			(pin power_in line
				(at -40.64 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P9")
			)
			(pin power_in line
				(at -38.1 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R6")
			)
			(pin power_in line
				(at -35.56 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R12")
			)
			(pin power_in line
				(at -33.02 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U4")
			)
			(pin power_in line
				(at -30.48 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U9")
			)
			(pin power_in line
				(at -27.94 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U14")
			)
			(pin power_in line
				(at 27.94 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "E2")
			)
			(pin power_in line
				(at 30.48 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G4")
			)
			(pin power_in line
				(at 33.02 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J2")
			)
			(pin power_in line
				(at 35.56 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 38.1 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M4")
			)
			(pin power_in line
				(at 40.64 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "L5")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "L7")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "H7")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "F6")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "C1")
			)
		)
		(symbol "XC6SLX16-CSG324_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "D16")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "B18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A17")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "V17")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "V2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "R16")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "P13")
			)
		)
		(symbol "XC6SLX16-CSG324_4_1"
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B1")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M9")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P5")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A18")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D5")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "G2")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G17")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "H10")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J4")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "G7")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "H11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "L8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "M2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "M6")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M17")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "R4")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U6")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "V1")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX16-FTG256"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX16-FTG256"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 16 XC6SLX16-FTG256"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX16-FTG256_1_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "E7")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L39P_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L39N_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L40P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L40N_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D12")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B9")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B13")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D7")
			)
			(pin power_in line
				(at -30.48 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D10")
			)
			(pin power_in line
				(at 27.94 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "D15")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G13")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J15")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "K13")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N15")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R13")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "E13")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "E12")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "B15")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "B16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F12")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "G11")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D14")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "C15")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "G12")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "H11")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "J11")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "J12")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K14")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "K11")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "J14")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "M15")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "L16")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R15")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "R14")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T15")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "T14")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "T13")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "R12")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "T12")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "L12")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "L13")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "M14")
			)
		)
		(symbol "XC6SLX16-FTG256_2_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "M12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "M11")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "P10")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "P12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "N9")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "P9")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "L10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "M10")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "T9")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "M9")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "P8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "M7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "P6")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "R5")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "T5")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "P5")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "L7")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "P4")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "T4")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "M6")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "R3")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "T3")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_2")
				(number "N7")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_2")
				(number "N10")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R4")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R8")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "D2")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G4")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J2")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "K4")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "L5")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "E2")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "G5")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "A2")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "F6")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "B3")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "A3")
			)
		)
		(symbol "XC6SLX16-FTG256_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "C12")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "E14")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "A15")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "C14")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "P13")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "T2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "P14")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "L11")
			)
		)
		(symbol "XC6SLX16-FTG256_4_1"
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H6")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L6")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L9")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "A16")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "G2")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "G15")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H12")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "G7")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "G9")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "H10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "J7")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "L2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "R6")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "T1")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX25-CSG324"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX25-CSG324"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 25 XC6SLX25-CSG324"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX25-CSG324_1_1"
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "D4")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L10P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L10N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L11P_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L11N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L39P_0")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L39N_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L40P_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L40N_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L41P_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L41N_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L42P_0")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L42N_0")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A16")
			)
			(pin power_in line
				(at -40.64 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B5")
			)
			(pin power_in line
				(at -38.1 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B10")
			)
			(pin power_in line
				(at -35.56 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -33.02 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D7")
			)
			(pin power_in line
				(at -30.48 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D13")
			)
			(pin power_in line
				(at -27.94 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E10")
			)
			(pin power_in line
				(at 27.94 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E17")
			)
			(pin power_in line
				(at 30.48 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G15")
			)
			(pin power_in line
				(at 33.02 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J14")
			)
			(pin power_in line
				(at 35.56 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J17")
			)
			(pin power_in line
				(at 38.1 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M15")
			)
			(pin power_in line
				(at 40.64 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "K13")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "K14")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "L12")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "L13")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "L16")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "U18")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "M14")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "P16")
			)
		)
		(symbol "XC6SLX25-CSG324_2_1"
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "R15")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "V16")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "T13")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "V14")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "P12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "M11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "V12")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "N10")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L22P_2")
				(number "M10")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L22N_2")
				(number "N9")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "U11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "R10")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "V10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "T9")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "U7")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "N7")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "P8")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "V6")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "R5")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "T5")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "U5")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "V5")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "R3")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "T3")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "T4")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "V4")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "P6")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "U3")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "V3")
			)
			(pin power_in line
				(at -40.64 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P9")
			)
			(pin power_in line
				(at -38.1 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R6")
			)
			(pin power_in line
				(at -35.56 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R12")
			)
			(pin power_in line
				(at -33.02 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U4")
			)
			(pin power_in line
				(at -30.48 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U9")
			)
			(pin power_in line
				(at -27.94 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U14")
			)
			(pin power_in line
				(at 27.94 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "E2")
			)
			(pin power_in line
				(at 30.48 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G4")
			)
			(pin power_in line
				(at 33.02 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J2")
			)
			(pin power_in line
				(at 35.56 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 38.1 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M4")
			)
			(pin power_in line
				(at 40.64 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "L5")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "L7")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "H7")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "F6")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "C1")
			)
		)
		(symbol "XC6SLX25-CSG324_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "D16")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "B18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A17")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "V17")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "V2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "R16")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "P13")
			)
		)
		(symbol "XC6SLX25-CSG324_4_1"
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B1")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M9")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P5")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A18")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D5")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "G2")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G17")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "H10")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J4")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "G7")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "H11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "L8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "M2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "M6")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M17")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "R4")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U6")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "V1")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX25-FGG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX25-FGG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 25 XC6SLX25-FGG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX25-FGG484_1_1"
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L43P_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L43N_0")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L44P_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L44N_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L45P_0")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L45N_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L46P_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L46N_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D17")
			)
			(pin power_in line
				(at -40.64 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B7")
			)
			(pin power_in line
				(at -35.56 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B11")
			)
			(pin power_in line
				(at -33.02 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -30.48 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -27.94 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E13")
			)
			(pin power_in line
				(at -22.86 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -20.32 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -17.78 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G14")
			)
			(pin power_in line
				(at 17.78 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 20.32 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 22.86 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "T20")
			)
		)
		(symbol "XC6SLX25-FGG484_2_1"
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "W18")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L21P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L21N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L53P_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L53N_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L54P_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L54N_2")
				(number "AB5")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L57P_2")
				(number "AA4")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L57N_2")
				(number "AB4")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "Y3")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "AB3")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L59P_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L59N_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L60P_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L60N_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W4")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "Y4")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "U6")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "V5")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA2")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AB2")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "T5")
			)
			(pin power_in line
				(at -40.64 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA3")
			)
			(pin power_in line
				(at -38.1 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -35.56 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -33.02 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -30.48 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA19")
			)
			(pin power_in line
				(at -27.94 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -25.4 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -22.86 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -20.32 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -17.78 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at -15.24 111.76 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at 15.24 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 17.78 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 20.32 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F6")
			)
			(pin power_in line
				(at 22.86 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 25.4 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 27.94 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 30.48 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 33.02 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 35.56 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 111.76 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "A2")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "B3")
			)
		)
		(symbol "XC6SLX25-FGG484_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "A19")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "C18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "G15")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "Y22")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "N15")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "Y20")
			)
		)
		(symbol "XC6SLX25-FGG484_4_1"
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D18")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX25-FTG256"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX25-FTG256"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 25 XC6SLX25-FTG256"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX25-FTG256_1_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "E7")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L39P_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L39N_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L40P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L40N_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D12")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B9")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B13")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D7")
			)
			(pin power_in line
				(at -30.48 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D10")
			)
			(pin power_in line
				(at 27.94 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "D15")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G13")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J15")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "K13")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N15")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R13")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "E13")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "E12")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "B15")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "B16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F12")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "G11")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D14")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "C15")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "G12")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "H11")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "J11")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "J12")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K14")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "K11")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "J14")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "M15")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "L16")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R15")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "R14")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T15")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "T14")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "T13")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "R12")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "T12")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "L12")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "L13")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "M14")
			)
		)
		(symbol "XC6SLX25-FTG256_2_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "M12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "M11")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "P10")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "P12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "N9")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "P9")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "L10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "M10")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "T9")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "M9")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "P8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "M7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "P6")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "R5")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "T5")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "P5")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "L7")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "P4")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "T4")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "M6")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "R3")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "T3")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_2")
				(number "N7")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_2")
				(number "N10")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R4")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R8")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "D2")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G4")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J2")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "K4")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "L5")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "E2")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "G5")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "A2")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "F6")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "B3")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "A3")
			)
		)
		(symbol "XC6SLX25-FTG256_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "C12")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "E14")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "A15")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "C14")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "P13")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "T2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "P14")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "L11")
			)
		)
		(symbol "XC6SLX25-FTG256_4_1"
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H6")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L6")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L9")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "A16")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "G2")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "G15")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H12")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "G7")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "G9")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "H10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "J7")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "L2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "R6")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "T1")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX25T-CSG324"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX25T-CSG324"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 25 XC6SLX25T-CSG324"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX25T-CSG324_1_1"
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D15")
			)
			(pin power_in line
				(at -40.64 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -38.1 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C3")
			)
			(pin power_in line
				(at -35.56 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F8")
			)
			(pin power_in line
				(at -33.02 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G12")
			)
			(pin power_in line
				(at 27.94 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E17")
			)
			(pin power_in line
				(at 30.48 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G15")
			)
			(pin power_in line
				(at 33.02 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J14")
			)
			(pin power_in line
				(at 35.56 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J17")
			)
			(pin power_in line
				(at 38.1 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M15")
			)
			(pin power_in line
				(at 40.64 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "K13")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "K14")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "L12")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "L13")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "L16")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "U18")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "M14")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "P16")
			)
		)
		(symbol "XC6SLX25T-CSG324_2_1"
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "R15")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "V16")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "T13")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "V14")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "P12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "M11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "V12")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "N10")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L22P_2")
				(number "M10")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L22N_2")
				(number "N9")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "U11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "R10")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "V10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "T9")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "U7")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "N7")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "P8")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "V6")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "R5")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "T5")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "U5")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "V5")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "R3")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "T3")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "T4")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "V4")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "P6")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "U3")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "V3")
			)
			(pin power_in line
				(at -40.64 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P9")
			)
			(pin power_in line
				(at -38.1 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R6")
			)
			(pin power_in line
				(at -35.56 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R12")
			)
			(pin power_in line
				(at -33.02 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U4")
			)
			(pin power_in line
				(at -30.48 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U9")
			)
			(pin power_in line
				(at -27.94 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U14")
			)
			(pin power_in line
				(at 27.94 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "E2")
			)
			(pin power_in line
				(at 30.48 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G4")
			)
			(pin power_in line
				(at 33.02 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J2")
			)
			(pin power_in line
				(at 35.56 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 38.1 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M4")
			)
			(pin power_in line
				(at 40.64 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "L5")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "L7")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "H7")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "F6")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "C1")
			)
		)
		(symbol "XC6SLX25T-CSG324_3_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B4")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A4")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D5")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "C9")
			)
		)
		(symbol "XC6SLX25T-CSG324_4_1"
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B7")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "D10")
			)
			(pin power_in line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C8")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D6")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A5")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E5")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E7")
			)
		)
		(symbol "XC6SLX25T-CSG324_5_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "F13")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "D16")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "B18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A17")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "V17")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "V2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "R16")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "P13")
			)
		)
		(symbol "XC6SLX25T-CSG324_6_1"
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B1")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D14")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M9")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P5")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A7")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A18")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C4")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D8")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "E13")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "F9")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "G2")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "G17")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "G7")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "H11")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "L8")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "H10")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "J4")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "M2")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M6")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "M17")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R4")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U6")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V1")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX25T-FGG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX25T-FGG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 25 XC6SLX25T-FGG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX25T-FGG484_1_1"
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "C3")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "D4")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "C18")
			)
			(pin power_in line
				(at -40.64 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -35.56 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -33.02 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F6")
			)
			(pin power_in line
				(at -30.48 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -27.94 91.44 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G14")
			)
			(pin power_in line
				(at 17.78 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 20.32 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 22.86 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 91.44 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "V20")
			)
		)
		(symbol "XC6SLX25T-FGG484_2_1"
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "V17")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "W18")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L21P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L21N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L57P_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L57N_2")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L59P_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L59N_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L60P_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L60N_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "AB5")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AA4")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AB4")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "U6")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "Y4")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AA3")
			)
			(pin power_in line
				(at -40.64 106.68 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 106.68 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -35.56 106.68 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -33.02 106.68 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA19")
			)
			(pin power_in line
				(at -30.48 106.68 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AB3")
			)
			(pin power_in line
				(at -27.94 106.68 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -25.4 106.68 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -22.86 106.68 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -20.32 106.68 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -17.78 106.68 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at -15.24 106.68 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at 17.78 106.68 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 20.32 106.68 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 22.86 106.68 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 25.4 106.68 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 27.94 106.68 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 30.48 106.68 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 33.02 106.68 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 35.56 106.68 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 106.68 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 106.68 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "B1")
			)
		)
		(symbol "XC6SLX25T-FGG484_3_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C9")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "A10")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "C11")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "D11")
			)
		)
		(symbol "XC6SLX25T-FGG484_4_1"
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B9")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "D12")
			)
			(pin power_in line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C10")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A7")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E8")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E9")
			)
		)
		(symbol "XC6SLX25T-FGG484_5_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "G17")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "D20")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A21")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AB2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "AA22")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "V18")
			)
		)
		(symbol "XC6SLX25T-FGG484_6_1"
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B15")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX4-CPG196"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX4-CPG196"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 4 XC6SLX4-CPG196"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX4-CPG196_1_1"
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B7")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "C11")
			)
			(pin power_in line
				(at -40.64 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C4")
			)
			(pin power_in line
				(at -38.1 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C5")
			)
			(pin power_in line
				(at -35.56 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C9")
			)
			(pin power_in line
				(at -33.02 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C10")
			)
			(pin power_in line
				(at 27.94 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "D12")
			)
			(pin power_in line
				(at 30.48 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E12")
			)
			(pin power_in line
				(at 33.02 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G11")
			)
			(pin power_in line
				(at 35.56 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G12")
			)
			(pin power_in line
				(at 38.1 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "K11")
			)
			(pin power_in line
				(at 40.64 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L1P_1")
				(number "C12")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L1N_VREF_1")
				(number "C13")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L32P_1")
				(number "D13")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L32N_1")
				(number "D14")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L33P_1")
				(number "E13")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L33N_1")
				(number "E14")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L34P_1")
				(number "F11")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L34N_1")
				(number "F12")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_1")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_1")
				(number "H11")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45P_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45N_1")
				(number "J14")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46P_1")
				(number "J11")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46N_1")
				(number "J12")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47P_1")
				(number "K13")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L47N_1")
				(number "K14")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "L13")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "M14")
			)
		)
		(symbol "XC6SLX4-CPG196_2_1"
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "N13")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "P13")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "P12")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "N10")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "P10")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "P9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "P8")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "N7")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "P6")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "P5")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "L4")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "M4")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "N4")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "P4")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "N3")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "P3")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "N2")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "P2")
			)
			(pin power_in line
				(at -40.64 45.72 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M5")
			)
			(pin power_in line
				(at -38.1 45.72 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M6")
			)
			(pin power_in line
				(at -35.56 45.72 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M9")
			)
			(pin power_in line
				(at -33.02 45.72 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M10")
			)
			(pin power_in line
				(at 27.94 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "E3")
			)
			(pin power_in line
				(at 30.48 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "E4")
			)
			(pin power_in line
				(at 33.02 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G3")
			)
			(pin power_in line
				(at 35.56 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "K3")
			)
			(pin power_in line
				(at 40.64 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L36P_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L36N_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L37P_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L37N_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_3")
				(number "J2")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_3")
				(number "G2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L49P_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L49N_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L50P_3")
				(number "E2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L50N_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L51P_3")
				(number "D4")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L51N_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L52P_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L52N_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "B1")
			)
		)
		(symbol "XC6SLX4-CPG196_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "A13")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "C14")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "B14")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "B13")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "N14")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "N1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "L12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "M12")
			)
		)
		(symbol "XC6SLX4-CPG196_4_1"
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G9")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H5")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H6")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A14")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "C2")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C7")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D5")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "D9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E8")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "G4")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "G6")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "G7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "E5")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "E6")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "E9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "E10")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "F5")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "F6")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "F9")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "F10")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "J6")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "K5")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "K6")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "H10")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "J7")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "L3")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "L6")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "M3")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "P1")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX4-CSG225"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX4-CSG225"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 4 XC6SLX4-CSG225"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX4-CSG225_1_1"
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "E7")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B7")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L39P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L39N_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L40P_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L40N_0")
				(number "E9")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B13")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A12")
			)
			(pin power_in line
				(at -40.64 53.34 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 53.34 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B8")
			)
			(pin power_in line
				(at -35.56 53.34 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B12")
			)
			(pin power_in line
				(at -33.02 53.34 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D9")
			)
			(pin power_in line
				(at 33.02 53.34 270)
				(length 6.35)
				(name "VCCO_1")
				(number "D14")
			)
			(pin power_in line
				(at 35.56 53.34 270)
				(length 6.35)
				(name "VCCO_1")
				(number "H14")
			)
			(pin power_in line
				(at 38.1 53.34 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J12")
			)
			(pin power_in line
				(at 40.64 53.34 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M14")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L1P_1")
				(number "B14")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L1N_VREF_1")
				(number "B15")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L33P_1")
				(number "C14")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L33N_1")
				(number "C15")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35P_1")
				(number "D13")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L35N_1")
				(number "D15")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36P_1")
				(number "J11")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L36N_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37P_1")
				(number "E14")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L37N_1")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38P_1")
				(number "K10")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L38N_1")
				(number "K11")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39P_1")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L39N_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_1")
				(number "L12")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_1")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_1")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_1")
				(number "J14")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_1")
				(number "J15")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44P_1")
				(number "K13")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L44N_1")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45P_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L45N_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46P_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L46N_1")
				(number "M15")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47P_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L47N_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "P14")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "P15")
			)
		)
		(symbol "XC6SLX4-CSG225_2_1"
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "R12")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "P13")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "M11")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N10")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "R10")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "L9")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "M10")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "P9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "N7")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "K8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "R6")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "P5")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "R5")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "L6")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "L5")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "N4")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "R4")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "M5")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "P3")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "R3")
			)
			(pin power_in line
				(at -40.64 53.34 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M7")
			)
			(pin power_in line
				(at -38.1 53.34 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P4")
			)
			(pin power_in line
				(at -35.56 53.34 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P8")
			)
			(pin power_in line
				(at -33.02 53.34 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P12")
			)
			(pin power_in line
				(at 33.02 53.34 270)
				(length 6.35)
				(name "VCCO_3")
				(number "D2")
			)
			(pin power_in line
				(at 35.56 53.34 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G4")
			)
			(pin power_in line
				(at 38.1 53.34 270)
				(length 6.35)
				(name "VCCO_3")
				(number "H2")
			)
			(pin power_in line
				(at 40.64 53.34 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L37P_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L37N_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L38P_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L38N_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L39P_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L39N_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L40P_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L40N_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_3")
				(number "J2")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_3")
				(number "G2")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45P_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45N_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46P_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46N_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L52P_3")
				(number "E2")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L52N_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L53P_3")
				(number "D4")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L53N_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L54P_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L54N_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "C1")
			)
		)
		(symbol "XC6SLX4-CSG225_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E10")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "D12")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "E13")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A14")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "R14")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "R2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "L13")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "L10")
			)
		)
		(symbol "XC6SLX4-CSG225_4_1"
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B1")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E12")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J6")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K9")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L4")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "A15")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B6")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B10")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C13")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "F2")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F6")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F14")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G7")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G9")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "F9")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "G6")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "G8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "H7")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "K7")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "J7")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "K2")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "K6")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N3")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P6")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX4-TQG144"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX4-TQG144"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 4 XC6SLX4-TQG144"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX4-TQG144_1_1"
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "144")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "143")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "142")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "141")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "140")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "139")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "138")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "137")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "134")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "133")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "132")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "131")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "127")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "126")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "124")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "123")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "121")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "120")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "119")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "118")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "117")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "116")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "115")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "114")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "112")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "111")
			)
			(pin power_in line
				(at -40.64 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "122")
			)
			(pin power_in line
				(at -38.1 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "125")
			)
			(pin power_in line
				(at -35.56 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "135")
			)
			(pin power_in line
				(at 35.56 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "76")
			)
			(pin power_in line
				(at 38.1 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "86")
			)
			(pin power_in line
				(at 40.64 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "103")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L1P_1")
				(number "105")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L1N_VREF_1")
				(number "104")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L32P_1")
				(number "102")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L32N_1")
				(number "101")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L33P_1")
				(number "100")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L33N_1")
				(number "99")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L34P_1")
				(number "98")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L34N_1")
				(number "97")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_1")
				(number "95")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_1")
				(number "94")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_1")
				(number "93")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_1")
				(number "92")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_1")
				(number "88")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_1")
				(number "87")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_1")
				(number "85")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_1")
				(number "84")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45P_1")
				(number "83")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45N_1")
				(number "82")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46P_1")
				(number "81")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46N_1")
				(number "80")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47P_1")
				(number "79")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L47N_1")
				(number "78")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "75")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "74")
			)
		)
		(symbol "XC6SLX4-TQG144_2_1"
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "70")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "69")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "67")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "66")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "65")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "64")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "62")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "61")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "60")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "59")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "58")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "57")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "56")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "55")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "51")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "50")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "48")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "47")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "46")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "45")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "44")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "43")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "41")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "40")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "39")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "38")
			)
			(pin power_in line
				(at -40.64 43.18 270)
				(length 6.35)
				(name "VCCO_2")
				(number "42")
			)
			(pin power_in line
				(at -38.1 43.18 270)
				(length 6.35)
				(name "VCCO_2")
				(number "63")
			)
			(pin power_in line
				(at 35.56 43.18 270)
				(length 6.35)
				(name "VCCO_3")
				(number "4")
			)
			(pin power_in line
				(at 38.1 43.18 270)
				(length 6.35)
				(name "VCCO_3")
				(number "18")
			)
			(pin power_in line
				(at 40.64 43.18 270)
				(length 6.35)
				(name "VCCO_3")
				(number "31")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "35")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "34")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "33")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "32")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L36P_3")
				(number "30")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L36N_3")
				(number "29")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L37P_3")
				(number "27")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L37N_3")
				(number "26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_3")
				(number "24")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_3")
				(number "23")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_3")
				(number "22")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_3")
				(number "21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_3")
				(number "17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_3")
				(number "16")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_3")
				(number "15")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_3")
				(number "14")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L49P_3")
				(number "12")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L49N_3")
				(number "11")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L50P_3")
				(number "10")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L50N_3")
				(number "9")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L51P_3")
				(number "8")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L51N_3")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L52P_3")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L52N_3")
				(number "5")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "2")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "1")
			)
		)
		(symbol "XC6SLX4-TQG144_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "110")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "106")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "107")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "109")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "71")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "37")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "73")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "72")
			)
		)
		(symbol "XC6SLX4-TQG144_4_1"
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "20")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "VCCAUX")
				(number "36")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "VCCAUX")
				(number "53")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "VCCAUX")
				(number "90")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "VCCAUX")
				(number "129")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "54")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "68")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "77")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "19")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "28")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "52")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "89")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "VCCINT")
				(number "128")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "91")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "96")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "108")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "113")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "130")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "136")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX45-CSG324"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX45-CSG324"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 45 XC6SLX45-CSG324"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX45-CSG324_1_1"
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "D4")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L10P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L10N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L11P_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L11N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L39P_0")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L39N_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L41P_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L41N_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A16")
			)
			(pin power_in line
				(at -40.64 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B5")
			)
			(pin power_in line
				(at -38.1 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B10")
			)
			(pin power_in line
				(at -35.56 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -33.02 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D7")
			)
			(pin power_in line
				(at -30.48 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D13")
			)
			(pin power_in line
				(at -27.94 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E10")
			)
			(pin power_in line
				(at 27.94 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E17")
			)
			(pin power_in line
				(at 30.48 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G15")
			)
			(pin power_in line
				(at 33.02 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J14")
			)
			(pin power_in line
				(at 35.56 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J17")
			)
			(pin power_in line
				(at 38.1 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M15")
			)
			(pin power_in line
				(at 40.64 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "K13")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "K14")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "L12")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "L13")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "L16")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "U18")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "M14")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "P16")
			)
		)
		(symbol "XC6SLX45-CSG324_2_1"
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "R15")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "V16")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "T13")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "V14")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "P12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "M11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "V12")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "N10")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L22P_2")
				(number "M10")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L22N_2")
				(number "N9")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "U11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "R10")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "V10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "T9")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "U7")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "N7")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "P8")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "V6")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "R5")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "T5")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "U5")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "V5")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "R3")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "T3")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "T4")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "V4")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "P6")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "U3")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "V3")
			)
			(pin power_in line
				(at -40.64 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P9")
			)
			(pin power_in line
				(at -38.1 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R6")
			)
			(pin power_in line
				(at -35.56 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R12")
			)
			(pin power_in line
				(at -33.02 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U4")
			)
			(pin power_in line
				(at -30.48 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U9")
			)
			(pin power_in line
				(at -27.94 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U14")
			)
			(pin power_in line
				(at 27.94 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "E2")
			)
			(pin power_in line
				(at 30.48 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G4")
			)
			(pin power_in line
				(at 33.02 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J2")
			)
			(pin power_in line
				(at 35.56 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 38.1 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M4")
			)
			(pin power_in line
				(at 40.64 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "L5")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "L7")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "H7")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "F6")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "C1")
			)
		)
		(symbol "XC6SLX45-CSG324_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "D16")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "B18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A17")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "V17")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "V2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "R16")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "P13")
			)
		)
		(symbol "XC6SLX45-CSG324_4_1"
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B1")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M9")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P5")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A18")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D5")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "G2")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G17")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "H10")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J4")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "G7")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "H11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "L8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "M2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "M6")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M17")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "R4")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U6")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "V1")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX45-CSG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX45-CSG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 45 XC6SLX45-CSG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX45-CSG484_1_1"
			(pin bidirectional line
				(at -50.8 132.08 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 129.54 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L46P_0")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L46N_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A18")
			)
			(pin power_in line
				(at -40.64 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B7")
			)
			(pin power_in line
				(at -35.56 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B11")
			)
			(pin power_in line
				(at -33.02 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -30.48 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E9")
			)
			(pin power_in line
				(at -27.94 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E13")
			)
			(pin power_in line
				(at -25.4 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -22.86 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at 10.16 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AA19")
			)
			(pin power_in line
				(at 12.7 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "B19")
			)
			(pin power_in line
				(at 15.24 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 17.78 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 20.32 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G14")
			)
			(pin power_in line
				(at 22.86 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 132.08 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 129.54 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L9P_1")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L9N_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L10P_1")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L10N_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L11P_1")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L11N_1")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L12P_1")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L12N_1")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L13P_1")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L13N_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L14P_1")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L14N_1")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L15P_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L15N_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L16P_1")
				(number "A19")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L16N_1")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L17P_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L17N_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L18P_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L18N_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21P_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L21N_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J21")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "AB21")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "AA21")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "Y19")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "R15")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -144.78 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -147.32 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -149.86 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "T20")
			)
		)
		(symbol "XC6SLX45-CSG484_2_1"
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AB5")
			)
			(pin power_in line
				(at -40.64 142.24 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 142.24 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -35.56 142.24 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -33.02 142.24 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -30.48 142.24 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -27.94 142.24 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -25.4 142.24 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -22.86 142.24 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at 10.16 142.24 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AA3")
			)
			(pin power_in line
				(at 12.7 142.24 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 15.24 142.24 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 17.78 142.24 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F6")
			)
			(pin power_in line
				(at 20.32 142.24 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 22.86 142.24 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 142.24 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 27.94 142.24 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 30.48 142.24 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 33.02 142.24 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 35.56 142.24 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 38.1 142.24 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin power_in line
				(at 40.64 142.24 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "T7")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L12P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L12N_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L13P_3")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L13N_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L73P_3")
				(number "G8")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L73N_3")
				(number "G7")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L74P_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L74N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L75P_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L75N_3")
				(number "E5")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L80P_3")
				(number "F8")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L80N_3")
				(number "F7")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L81P_3")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L81N_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L82P_3")
				(number "E6")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L82N_3")
				(number "D5")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "A3")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "A2")
			)
		)
		(symbol "XC6SLX45-CSG484_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "E14")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "E16")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "D14")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "U16")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "W18")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "T15")
			)
		)
		(symbol "XC6SLX45-CSG484_4_1"
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D18")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "J20")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX45-FGG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX45-FGG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 45 XC6SLX45-FGG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX45-FGG484_1_1"
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D17")
			)
			(pin power_in line
				(at -40.64 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B7")
			)
			(pin power_in line
				(at -35.56 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B11")
			)
			(pin power_in line
				(at -33.02 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -30.48 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -27.94 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E13")
			)
			(pin power_in line
				(at -22.86 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -20.32 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -17.78 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G14")
			)
			(pin power_in line
				(at 17.78 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 20.32 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 22.86 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L9P_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L9N_1")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L10P_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L10N_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L21P_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21N_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "T20")
			)
		)
		(symbol "XC6SLX45-FGG484_2_1"
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "T18")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "T17")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "W18")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L7P_2")
				(number "T16")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L7N_2")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L8P_2")
				(number "U17")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L8N_2")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L9P_2")
				(number "V19")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L9N_2")
				(number "V18")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L10P_2")
				(number "R16")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L10N_2")
				(number "R15")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L11P_2")
				(number "V17")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L11N_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L21P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L21N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L22P_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L22N_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L51P_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L51N_2")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L52P_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L52N_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L53P_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L53N_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L54P_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L54N_2")
				(number "AB5")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L57P_2")
				(number "AA4")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L57N_2")
				(number "AB4")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "Y3")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "AB3")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L59P_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 -109.22 0)
				(length 6.35)
				(name "IO_L59N_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -111.76 0)
				(length 6.35)
				(name "IO_L60P_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -114.3 0)
				(length 6.35)
				(name "IO_L60N_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 -116.84 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W4")
			)
			(pin bidirectional line
				(at -50.8 -119.38 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "Y4")
			)
			(pin bidirectional line
				(at -50.8 -121.92 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "U6")
			)
			(pin bidirectional line
				(at -50.8 -124.46 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "V5")
			)
			(pin bidirectional line
				(at -50.8 -127 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA2")
			)
			(pin bidirectional line
				(at -50.8 -129.54 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AB2")
			)
			(pin bidirectional line
				(at -50.8 -132.08 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -134.62 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "T5")
			)
			(pin power_in line
				(at -40.64 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA3")
			)
			(pin power_in line
				(at -38.1 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -35.56 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -33.02 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -30.48 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA19")
			)
			(pin power_in line
				(at -27.94 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -25.4 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -22.86 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -20.32 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -17.78 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at -15.24 137.16 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at 15.24 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 17.78 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 20.32 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F6")
			)
			(pin power_in line
				(at 22.86 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 25.4 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 27.94 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 30.48 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 33.02 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 35.56 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 137.16 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "D5")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L80P_3")
				(number "G7")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L80N_3")
				(number "F7")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L81P_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L81N_3")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L82P_3")
				(number "E5")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L82N_3")
				(number "E6")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "A2")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "B3")
			)
		)
		(symbol "XC6SLX45-FGG484_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "A19")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "C18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "G15")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "Y22")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "N15")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "Y20")
			)
		)
		(symbol "XC6SLX45-FGG484_4_1"
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D18")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX45-FGG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX45-FGG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 45 XC6SLX45-FGG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX45-FGG676_1_1"
			(pin bidirectional line
				(at -50.8 132.08 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 129.54 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L12P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L12N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L16P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L16N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L17P_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L17N_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L24P_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L24N_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L26P_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L26N_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L52P_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L52N_0")
				(number "C18")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L56P_0")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L56N_0")
				(number "C20")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A21")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A22")
			)
			(pin power_in line
				(at -40.64 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B3")
			)
			(pin power_in line
				(at -38.1 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B7")
			)
			(pin power_in line
				(at -35.56 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B11")
			)
			(pin power_in line
				(at -33.02 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -30.48 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -27.94 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C22")
			)
			(pin power_in line
				(at -25.4 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D9")
			)
			(pin power_in line
				(at -22.86 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D17")
			)
			(pin power_in line
				(at -20.32 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E13")
			)
			(pin power_in line
				(at -17.78 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -15.24 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G18")
			)
			(pin power_in line
				(at -12.7 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H14")
			)
			(pin power_in line
				(at 5.08 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AB23")
			)
			(pin power_in line
				(at 7.62 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AD25")
			)
			(pin power_in line
				(at 10.16 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "D25")
			)
			(pin power_in line
				(at 12.7 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "F23")
			)
			(pin power_in line
				(at 15.24 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "H25")
			)
			(pin power_in line
				(at 17.78 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J21")
			)
			(pin power_in line
				(at 20.32 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "K23")
			)
			(pin power_in line
				(at 22.86 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M20")
			)
			(pin power_in line
				(at 25.4 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M25")
			)
			(pin power_in line
				(at 27.94 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "P23")
			)
			(pin power_in line
				(at 30.48 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "T25")
			)
			(pin power_in line
				(at 33.02 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 35.56 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "V21")
			)
			(pin power_in line
				(at 38.1 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W23")
			)
			(pin power_in line
				(at 40.64 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 132.08 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "B23")
			)
			(pin bidirectional line
				(at 50.8 129.54 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "A23")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L10P_1")
				(number "B24")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L10N_1")
				(number "A25")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L11P_1")
				(number "C25")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L11N_1")
				(number "C26")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L12P_1")
				(number "B25")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L12N_1")
				(number "B26")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L16P_1")
				(number "E25")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L16N_1")
				(number "E26")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L17P_1")
				(number "D24")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L17N_1")
				(number "D26")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L18P_1")
				(number "F24")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L18N_1")
				(number "F26")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "H24")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "H26")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "G25")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "G26")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L21P_1")
				(number "K24")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L21N_1")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L22P_1")
				(number "J25")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L22N_1")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L23P_1")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L23N_1")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L24P_1")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L24N_1")
				(number "L26")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L25P_1")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L25N_1")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "L23")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "R24")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "V23")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "W24")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "U25")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "U26")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "W25")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "W26")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "V24")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "V26")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "Y24")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "AD24")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "AB24")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "AB26")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "AC25")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "AC26")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "AA25")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "AA26")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "AE25")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "U24")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L57P_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L57N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "U23")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "U21")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "AA23")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "AA24")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AC23")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AC24")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "AE24")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "AF25")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "W18")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "W19")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -144.78 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 -147.32 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "AE23")
			)
			(pin bidirectional line
				(at 50.8 -149.86 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "AF24")
			)
		)
		(symbol "XC6SLX45-FGG676_2_1"
			(pin bidirectional line
				(at -50.8 132.08 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 129.54 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AF21")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AD20")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AF20")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AE19")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AF19")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "AC20")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AD21")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "AA19")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L7P_2")
				(number "AC19")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L7N_2")
				(number "AD19")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L8P_2")
				(number "V16")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L8N_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L9P_2")
				(number "AD18")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L9N_2")
				(number "AF18")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L10P_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L10N_2")
				(number "AA17")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L11P_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L11N_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "AE17")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "AF17")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "AD16")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AF16")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AE15")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AF15")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AC17")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "AC15")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AD15")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "AC16")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "AD17")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "W16")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AC14")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "AA15")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L28P_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L28N_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "AD14")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "AF14")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AC13")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AD13")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AD12")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L34P_2")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L34N_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "V14")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "AA11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AC11")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AD11")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "V12")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AF11")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "AE9")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AD10")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L51P_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L51N_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L52P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L52N_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "AC9")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "AD9")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L53P_2")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L53N_2")
				(number "AF8")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "AE7")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AD6")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AF6")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AE5")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AF5")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "AE4")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AF4")
			)
			(pin power_in line
				(at -40.64 152.4 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AB14")
			)
			(pin power_in line
				(at -38.1 152.4 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC10")
			)
			(pin power_in line
				(at -35.56 152.4 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC18")
			)
			(pin power_in line
				(at -33.02 152.4 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC21")
			)
			(pin power_in line
				(at -30.48 152.4 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE8")
			)
			(pin power_in line
				(at -27.94 152.4 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE12")
			)
			(pin power_in line
				(at -25.4 152.4 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE16")
			)
			(pin power_in line
				(at -22.86 152.4 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE20")
			)
			(pin power_in line
				(at -20.32 152.4 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y12")
			)
			(pin power_in line
				(at -17.78 152.4 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y17")
			)
			(pin power_in line
				(at 2.54 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AC6")
			)
			(pin power_in line
				(at 5.08 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AD2")
			)
			(pin power_in line
				(at 7.62 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "D2")
			)
			(pin power_in line
				(at 10.16 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 12.7 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "H2")
			)
			(pin power_in line
				(at 15.24 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J6")
			)
			(pin power_in line
				(at 17.78 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "K4")
			)
			(pin power_in line
				(at 20.32 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M2")
			)
			(pin power_in line
				(at 22.86 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P4")
			)
			(pin power_in line
				(at 27.94 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P9")
			)
			(pin power_in line
				(at 30.48 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T2")
			)
			(pin power_in line
				(at 33.02 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T7")
			)
			(pin power_in line
				(at 35.56 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W4")
			)
			(pin power_in line
				(at 38.1 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W6")
			)
			(pin power_in line
				(at 40.64 152.4 270)
				(length 6.35)
				(name "VCCO_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 132.08 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AC7")
			)
			(pin bidirectional line
				(at 50.8 129.54 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AD7")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L3P_3")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L3N_3")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "AA7")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "AB7")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "AC5")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "AD5")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L16P_3")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L16N_3")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L15P_3")
				(number "W8")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L15N_3")
				(number "W7")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L28P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L28N_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L29P_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L29N_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L30P_3")
				(number "R5")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L30N_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "N8")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "P10")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "N5")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "M10")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "N9")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "M9")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "L7")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L61P_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L61N_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L62P_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L62N_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L63P_3")
				(number "J2")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L63N_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L64P_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L64N_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L65P_3")
				(number "G2")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L65N_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L66P_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L66N_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L67P_3")
				(number "E2")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L67N_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L68P_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L68N_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L77P_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L77N_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L79P_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L79N_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L81P_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -144.78 180)
				(length 6.35)
				(name "IO_L81N_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -147.32 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -149.86 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "C3")
			)
		)
		(symbol "XC6SLX45-FGG676_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "F20")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "A24")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "C23")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "E21")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AF23")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AF3")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "AD23")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "AC22")
			)
		)
		(symbol "XC6SLX45-FGG676_4_1"
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F6")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F21")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G15")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J18")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L22")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M17")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N10")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U6")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U14")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "Y19")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA6")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA10")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA16")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA21")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B21")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F2")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F19")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "F25")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H11")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J19")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "K2")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "K16")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "K25")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "L15")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "M5")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "M16")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "M22")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "N15")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "P2")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "L16")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "R16")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "U16")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "P19")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T5")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "V2")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "W15")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "W20")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "Y7")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "Y11")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "Y23")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AB2")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AB12")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AB16")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AB20")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AB25")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AC8")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AE6")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AE10")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AE14")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AE18")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AF26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX45T-CSG324"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX45T-CSG324"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 45 XC6SLX45T-CSG324"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX45T-CSG324_1_1"
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D15")
			)
			(pin power_in line
				(at -40.64 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -38.1 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C3")
			)
			(pin power_in line
				(at -35.56 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F8")
			)
			(pin power_in line
				(at -33.02 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G12")
			)
			(pin power_in line
				(at 27.94 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E17")
			)
			(pin power_in line
				(at 30.48 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G15")
			)
			(pin power_in line
				(at 33.02 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J14")
			)
			(pin power_in line
				(at 35.56 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J17")
			)
			(pin power_in line
				(at 38.1 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M15")
			)
			(pin power_in line
				(at 40.64 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "K13")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "K14")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "L12")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "L13")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "L16")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "U18")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "M14")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "P16")
			)
		)
		(symbol "XC6SLX45T-CSG324_2_1"
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "R15")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "V16")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "T13")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "V14")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "P12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "M11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "V12")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "N10")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L22P_2")
				(number "M10")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L22N_2")
				(number "N9")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "U11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "R10")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "V10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "T9")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "U7")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "N7")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "P8")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "V6")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "R5")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "T5")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "U5")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "V5")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "R3")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "T3")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "T4")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "V4")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "P6")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "U3")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "V3")
			)
			(pin power_in line
				(at -40.64 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P9")
			)
			(pin power_in line
				(at -38.1 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R6")
			)
			(pin power_in line
				(at -35.56 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R12")
			)
			(pin power_in line
				(at -33.02 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U4")
			)
			(pin power_in line
				(at -30.48 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U9")
			)
			(pin power_in line
				(at -27.94 86.36 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U14")
			)
			(pin power_in line
				(at 27.94 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "E2")
			)
			(pin power_in line
				(at 30.48 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G4")
			)
			(pin power_in line
				(at 33.02 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J2")
			)
			(pin power_in line
				(at 35.56 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 38.1 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M4")
			)
			(pin power_in line
				(at 40.64 86.36 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "L5")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "L7")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "H7")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "F6")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "C1")
			)
		)
		(symbol "XC6SLX45T-CSG324_3_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B4")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A4")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D5")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C5")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "C9")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B12")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A12")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B14")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A14")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D11")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C11")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D13")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C13")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "B10")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "A10")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "F10")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "E10")
			)
		)
		(symbol "XC6SLX45T-CSG324_4_1"
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B7")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "D10")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C8")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "B11")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "E11")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D6")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A5")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E5")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E7")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D12")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A13")
			)
		)
		(symbol "XC6SLX45T-CSG324_5_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "F13")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "D16")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "B18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A17")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "V17")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "V2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "R16")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "P13")
			)
		)
		(symbol "XC6SLX45T-CSG324_6_1"
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B1")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D14")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M9")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P5")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A7")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A18")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C4")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C10")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D8")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "E13")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "F9")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "G2")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "G17")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "G7")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "H11")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "L8")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "H10")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "J4")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "M2")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M6")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "M17")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R4")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U6")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V1")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX45T-CSG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX45T-CSG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 45 XC6SLX45T-CSG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX45T-CSG484_1_1"
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "G7")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "C18")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D20")
			)
			(pin power_in line
				(at -40.64 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -35.56 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E10")
			)
			(pin power_in line
				(at -33.02 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -30.48 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F6")
			)
			(pin power_in line
				(at -27.94 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H8")
			)
			(pin power_in line
				(at 12.7 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AA19")
			)
			(pin power_in line
				(at 15.24 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 17.78 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 20.32 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 22.86 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 25.4 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 27.94 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 30.48 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 33.02 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R15")
			)
			(pin power_in line
				(at 35.56 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L15P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L15N_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L16P_1")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L16N_1")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L17P_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L17N_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L18P_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L18N_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "AA21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "R12")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "R13")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "T12")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "T13")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "AB21")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "Y19")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "T15")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "T20")
			)
		)
		(symbol "XC6SLX45T-CSG484_2_1"
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AB5")
			)
			(pin power_in line
				(at -40.64 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -35.56 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -33.02 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U14")
			)
			(pin power_in line
				(at -30.48 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -27.94 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -25.4 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at -22.86 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W16")
			)
			(pin power_in line
				(at 10.16 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AA3")
			)
			(pin power_in line
				(at 12.7 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 15.24 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 17.78 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 20.32 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 22.86 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 25.4 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 27.94 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 30.48 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 33.02 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R7")
			)
			(pin power_in line
				(at 35.56 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T9")
			)
			(pin power_in line
				(at 38.1 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "V11")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "U10")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L12P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L12N_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L13P_3")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L13N_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "T5")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "T7")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "U9")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "T11")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "T10")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "R8")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L69P_3")
				(number "A3")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L69N_3")
				(number "A2")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L70P_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L70N_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L71P_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L71N_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L72P_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L72N_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L73P_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L73N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L74P_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L74N_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L75P_3")
				(number "D4")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L75N_3")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "D3")
			)
		)
		(symbol "XC6SLX45T-CSG484_3_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C9")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "A10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "D11")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "C11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B14")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A14")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B16")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A16")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D13")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C13")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C15")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "B12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "A12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "F14")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "E14")
			)
		)
		(symbol "XC6SLX45T-CSG484_4_1"
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B9")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "D12")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C10")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "B13")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "E13")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "E15")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A7")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E11")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D14")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A15")
			)
		)
		(symbol "XC6SLX45T-CSG484_5_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "F17")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "H16")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "C19")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "U16")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "W18")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "U12")
			)
		)
		(symbol "XC6SLX45T-CSG484_6_1"
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F18")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R11")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B15")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "E12")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "F15")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "G14")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "V16")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX45T-FGG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX45T-FGG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 45 XC6SLX45T-FGG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX45T-FGG484_1_1"
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "C3")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "D4")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "C18")
			)
			(pin power_in line
				(at -40.64 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -35.56 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -33.02 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F6")
			)
			(pin power_in line
				(at -30.48 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -27.94 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G14")
			)
			(pin power_in line
				(at 17.78 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 20.32 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 22.86 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L9P_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L9N_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L10P_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L10N_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L21P_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21N_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "R15")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "V20")
			)
		)
		(symbol "XC6SLX45T-FGG484_2_1"
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "V17")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "W18")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L18P_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L18N_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L21P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L21N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L22P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L22N_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L44P_2")
				(number "W10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L44N_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L50P_2")
				(number "U9")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L50N_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L57P_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L57N_2")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 6.35)
				(name "IO_L59P_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 -81.28 0)
				(length 6.35)
				(name "IO_L59N_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -83.82 0)
				(length 6.35)
				(name "IO_L60P_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 -86.36 0)
				(length 6.35)
				(name "IO_L60N_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 -88.9 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -91.44 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "AB5")
			)
			(pin bidirectional line
				(at -50.8 -93.98 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AA4")
			)
			(pin bidirectional line
				(at -50.8 -96.52 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AB4")
			)
			(pin bidirectional line
				(at -50.8 -99.06 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -101.6 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "U6")
			)
			(pin bidirectional line
				(at -50.8 -104.14 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "Y4")
			)
			(pin bidirectional line
				(at -50.8 -106.68 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AA3")
			)
			(pin power_in line
				(at -40.64 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -35.56 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -33.02 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA19")
			)
			(pin power_in line
				(at -30.48 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AB3")
			)
			(pin power_in line
				(at -27.94 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -25.4 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -22.86 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -20.32 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -17.78 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at -15.24 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at 17.78 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 20.32 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 22.86 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 25.4 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 27.94 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 30.48 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 33.02 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 35.56 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "T5")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L80P_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L80N_3")
				(number "G7")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L81P_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L81N_3")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L82P_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L82N_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "B1")
			)
		)
		(symbol "XC6SLX45T-FGG484_3_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C9")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "A10")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "C11")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "D11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B14")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A14")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B16")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A16")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D13")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C13")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C15")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "A12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "B12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "E12")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "F12")
			)
		)
		(symbol "XC6SLX45T-FGG484_4_1"
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B9")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "D12")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C10")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "B13")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "E13")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "E10")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A7")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E8")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D14")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A15")
			)
		)
		(symbol "XC6SLX45T-FGG484_5_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "G17")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "D20")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A21")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AB2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "AA22")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "V18")
			)
		)
		(symbol "XC6SLX45T-FGG484_6_1"
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B15")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX75-CSG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX75-CSG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 75 XC6SLX75-CSG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX75-CSG484_1_1"
			(pin bidirectional line
				(at -50.8 132.08 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 129.54 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L15P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L15N_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L16P_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L16N_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L46P_0")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L46N_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A18")
			)
			(pin power_in line
				(at -40.64 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B7")
			)
			(pin power_in line
				(at -35.56 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B11")
			)
			(pin power_in line
				(at -33.02 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -30.48 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E9")
			)
			(pin power_in line
				(at -27.94 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E13")
			)
			(pin power_in line
				(at -25.4 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -22.86 152.4 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at 10.16 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AA19")
			)
			(pin power_in line
				(at 12.7 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "B19")
			)
			(pin power_in line
				(at 15.24 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 17.78 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 20.32 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G14")
			)
			(pin power_in line
				(at 22.86 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 152.4 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 132.08 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 129.54 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L9P_1")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L9N_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L10P_1")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L10N_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L11P_1")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L11N_1")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L12P_1")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L12N_1")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L13P_1")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L13N_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L14P_1")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L14N_1")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L15P_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L15N_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L16P_1")
				(number "A19")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L16N_1")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L17P_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L17N_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L18P_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L18N_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21P_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L21N_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J21")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "AB21")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "AA21")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "Y19")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "R15")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -144.78 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -147.32 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -149.86 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "T20")
			)
		)
		(symbol "XC6SLX75-CSG484_2_1"
			(pin bidirectional line
				(at -50.8 127 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L33P_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L33N_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L34P_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L34N_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AB5")
			)
			(pin power_in line
				(at -40.64 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -35.56 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -33.02 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -30.48 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -27.94 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -25.4 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -22.86 147.32 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at 10.16 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AA3")
			)
			(pin power_in line
				(at 12.7 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 15.24 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 17.78 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F6")
			)
			(pin power_in line
				(at 20.32 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 22.86 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 27.94 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 30.48 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 33.02 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 35.56 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 38.1 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin power_in line
				(at 40.64 147.32 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 127 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "T7")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L12P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L12N_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L13P_3")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L13N_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19P_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L19N_3")
				(number "R8")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "T5")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L73P_3")
				(number "G8")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L73N_3")
				(number "G7")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L74P_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L74N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L75P_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L75N_3")
				(number "E5")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L80P_3")
				(number "F8")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L80N_3")
				(number "F7")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L81P_3")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L81N_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L82P_3")
				(number "E6")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L82N_3")
				(number "D5")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "A3")
			)
			(pin bidirectional line
				(at 50.8 -144.78 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "A2")
			)
		)
		(symbol "XC6SLX75-CSG484_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "E14")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "E16")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "D14")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "U16")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "W18")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "T15")
			)
		)
		(symbol "XC6SLX75-CSG484_4_1"
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "RFUSE")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VBATT")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VFS")
				(number "U19")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D18")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "J20")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX75-FGG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX75-FGG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 75 XC6SLX75-FGG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX75-FGG484_1_1"
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L43P_0")
				(number "E12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L43N_0")
				(number "D12")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L45P_0")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L45N_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L46P_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L46N_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L47P_0")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L47N_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D17")
			)
			(pin power_in line
				(at -40.64 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B7")
			)
			(pin power_in line
				(at -35.56 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B11")
			)
			(pin power_in line
				(at -33.02 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -30.48 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -27.94 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E13")
			)
			(pin power_in line
				(at -22.86 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -20.32 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -17.78 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G14")
			)
			(pin power_in line
				(at 17.78 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 20.32 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 22.86 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "C19")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "B20")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L9P_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L9N_1")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L10P_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L10N_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L21P_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21N_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "D19")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "D20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "T20")
			)
		)
		(symbol "XC6SLX75-FGG484_2_1"
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "T18")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "T17")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L21P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L21N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L58P_2")
				(number "Y3")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L58N_2")
				(number "AB3")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W4")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "Y4")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L57P_2")
				(number "AA4")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L57N_2")
				(number "AB4")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA2")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AB2")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "T5")
			)
			(pin power_in line
				(at -40.64 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA3")
			)
			(pin power_in line
				(at -38.1 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -35.56 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -33.02 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -30.48 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA19")
			)
			(pin power_in line
				(at -27.94 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -25.4 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -22.86 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -20.32 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -17.78 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at -15.24 121.92 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at 15.24 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 17.78 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 20.32 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F6")
			)
			(pin power_in line
				(at 22.86 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 25.4 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 27.94 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 30.48 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 33.02 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 35.56 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 121.92 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "D5")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L80P_3")
				(number "G7")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L80N_3")
				(number "F7")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L81P_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L81N_3")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L82P_3")
				(number "E5")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L82N_3")
				(number "E6")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "A2")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "B3")
			)
		)
		(symbol "XC6SLX75-FGG484_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "A19")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "C18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "G15")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "Y22")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "N15")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "Y20")
			)
		)
		(symbol "XC6SLX75-FGG484_4_1"
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "RFUSE")
				(number "P15")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VBATT")
				(number "R17")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VFS")
				(number "P16")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D18")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX75-FGG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX75-FGG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 75 XC6SLX75-FGG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX75-FGG676_1_1"
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L12P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L12N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L16P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L16N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L17P_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L17N_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L22P_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L22N_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L24P_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L24N_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L26P_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L26N_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "A16")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "E17")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "J15")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "H15")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L52P_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L52N_0")
				(number "C18")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L56P_0")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L56N_0")
				(number "C20")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A21")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A22")
			)
			(pin power_in line
				(at -40.64 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B3")
			)
			(pin power_in line
				(at -38.1 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B7")
			)
			(pin power_in line
				(at -35.56 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B11")
			)
			(pin power_in line
				(at -33.02 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -30.48 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -27.94 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C22")
			)
			(pin power_in line
				(at -25.4 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D9")
			)
			(pin power_in line
				(at -22.86 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D17")
			)
			(pin power_in line
				(at -20.32 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E13")
			)
			(pin power_in line
				(at -17.78 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -15.24 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G18")
			)
			(pin power_in line
				(at -12.7 127 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H14")
			)
			(pin power_in line
				(at 20.32 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AB23")
			)
			(pin power_in line
				(at 22.86 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AD25")
			)
			(pin power_in line
				(at 25.4 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M20")
			)
			(pin power_in line
				(at 27.94 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "P23")
			)
			(pin power_in line
				(at 30.48 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "T25")
			)
			(pin power_in line
				(at 33.02 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 35.56 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "V21")
			)
			(pin power_in line
				(at 38.1 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W23")
			)
			(pin power_in line
				(at 40.64 127 270)
				(length 6.35)
				(name "VCCO_1")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "L23")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "R24")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "V23")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "W24")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "U25")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "U26")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "W25")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "W26")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "V24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "V26")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "Y24")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "AD24")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "AB24")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "AB26")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "AC25")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "AC26")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "AA25")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "AA26")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "AE25")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "U24")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L55P_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L55N_1")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L56P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L56N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L57P_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L57N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "U23")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "U21")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "AA23")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "AA24")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AC23")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AC24")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "AE24")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "AF25")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "W18")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "W19")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L69P_1")
				(number "AB21")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L69N_VREF_1")
				(number "AB22")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "AE23")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "AF24")
			)
		)
		(symbol "XC6SLX75-FGG676_2_1"
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AE21")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AF21")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AD20")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AF20")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AE19")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AF19")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L9P_2")
				(number "AD18")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L9N_2")
				(number "AF18")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "AE17")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "AF17")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "AD16")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AF16")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AE15")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AF15")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AC17")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "AC15")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AD15")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AC14")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "AA15")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "AD14")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "AF14")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AC13")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AD13")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AD12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AF12")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "V12")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L34P_2")
				(number "AA13")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L34N_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AC12")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L53P_2")
				(number "AD8")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L53N_2")
				(number "AF8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "AE11")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AF11")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "AE9")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AF9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AD10")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AF10")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L61P_2")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L61N_VREF_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "AE7")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "AF7")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AD6")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AF6")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AE5")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AF5")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "AE4")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AF4")
			)
			(pin power_in line
				(at -40.64 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AB14")
			)
			(pin power_in line
				(at -38.1 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC10")
			)
			(pin power_in line
				(at -35.56 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC18")
			)
			(pin power_in line
				(at -33.02 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AC21")
			)
			(pin power_in line
				(at -30.48 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE8")
			)
			(pin power_in line
				(at -27.94 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE12")
			)
			(pin power_in line
				(at -25.4 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE16")
			)
			(pin power_in line
				(at -22.86 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE20")
			)
			(pin power_in line
				(at -20.32 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y12")
			)
			(pin power_in line
				(at -17.78 134.62 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y17")
			)
			(pin power_in line
				(at 17.78 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AC6")
			)
			(pin power_in line
				(at 20.32 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AD2")
			)
			(pin power_in line
				(at 22.86 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P4")
			)
			(pin power_in line
				(at 27.94 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P9")
			)
			(pin power_in line
				(at 30.48 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T2")
			)
			(pin power_in line
				(at 33.02 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T7")
			)
			(pin power_in line
				(at 35.56 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W4")
			)
			(pin power_in line
				(at 38.1 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W6")
			)
			(pin power_in line
				(at 40.64 134.62 270)
				(length 6.35)
				(name "VCCO_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AC7")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AD7")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "AE3")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "AF2")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L3P_3")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L3N_3")
				(number "AD4")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L4P_3")
				(number "AA8")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L4N_3")
				(number "AB8")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "AA7")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "AB7")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AB6")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "Y9")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "Y8")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "AC5")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "AD5")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L15P_3")
				(number "W8")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L15N_3")
				(number "W7")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L16P_3")
				(number "AA5")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L16N_3")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L17P_3")
				(number "V7")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L17N_VREF_3")
				(number "V6")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L19P_3")
				(number "W9")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L19N_3")
				(number "V8")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "W10")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "V10")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "T10")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "U9")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L27P_3")
				(number "R10")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L27N_3")
				(number "T9")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L28P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L28N_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L29P_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L29N_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L30P_3")
				(number "R5")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L30N_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "N8")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "P10")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "N5")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "M10")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "N9")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "M9")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "L7")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "L6")
			)
		)
		(symbol "XC6SLX75-FGG676_3_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L58P_4")
				(number "K8")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L58N_VREF_4")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L59P_M4DQ14_4")
				(number "N2")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L59N_M4DQ15_4")
				(number "N1")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L60P_M4DQ12_4")
				(number "M3")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L60N_M4DQ13_4")
				(number "M1")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L61P_M4UDQS_4")
				(number "L2")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L61N_M4UDQSN_4")
				(number "L1")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62P_M4DQ10_4")
				(number "K3")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L62N_M4DQ11_4")
				(number "K1")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63P_M4DQ8_4")
				(number "J2")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L63N_M4DQ9_4")
				(number "J1")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64P_M4DQ0_4")
				(number "H3")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L64N_M4DQ1_4")
				(number "H1")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65P_M4DQ2_4")
				(number "G2")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L65N_M4DQ3_4")
				(number "G1")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66P_M4LDQS_4")
				(number "F3")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L66N_M4LDQSN_4")
				(number "F1")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L67P_M4DQ6_4")
				(number "E2")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L67N_M4DQ7_4")
				(number "E1")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L68P_M4DQ4_4")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L68N_M4DQ5_4")
				(number "D1")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L69P_M4UDM_4")
				(number "J4")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L69N_M4LDM_4")
				(number "J3")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L70P_M4RASN_4")
				(number "K7")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L70N_M4CASN_4")
				(number "K6")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L71P_M4A5_4")
				(number "K5")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L71N_M4A6_4")
				(number "J5")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L72P_M4A3_4")
				(number "J7")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L72N_M4ODT_4")
				(number "H7")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L73P_M4CLK_4")
				(number "G4")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L73N_M4CLKN_4")
				(number "G3")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L74P_M4A0_4")
				(number "K10")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L74N_M4A1_4")
				(number "L9")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L75P_M4BA0_4")
				(number "H6")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L75N_M4BA1_4")
				(number "H5")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L76P_M4A7_4")
				(number "J10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L76N_M4A2_4")
				(number "K9")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L77P_M4WE_4")
				(number "E4")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L77N_M4BA2_4")
				(number "E3")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L78P_M4A10_4")
				(number "G6")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L78N_M4A4_4")
				(number "G5")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L79P_M4A8_4")
				(number "C2")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L79N_M4A9_4")
				(number "C1")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L80P_M4CKE_4")
				(number "F5")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L80N_M4A12_4")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L81P_M4RESET_4")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L81N_M4A11_4")
				(number "B1")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L82P_M4A13_4")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L82N_M4A14_4")
				(number "G7")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L83P_4")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L83N_VREF_4")
				(number "C3")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "D2")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "F4")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "H2")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "J6")
			)
			(pin power_in line
				(at -30.48 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "K4")
			)
			(pin power_in line
				(at -27.94 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "M2")
			)
			(pin power_in line
				(at 27.94 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "D25")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "F23")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "H25")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "J21")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "K23")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_A25_5")
				(number "B23")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_5")
				(number "A23")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L2P_M5A13_5")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L2N_M5A14_5")
				(number "G21")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L3P_M5RESET_5")
				(number "D23")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L3N_M5A11_5")
				(number "C24")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L4P_M5CKE_5")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L4N_M5A12_5")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L5P_M5A8_5")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L5N_M5A9_5")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L6P_M5A10_5")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L6N_M5A4_5")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L7P_M5WE_5")
				(number "E23")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L7N_M5BA2_5")
				(number "E24")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L8P_M5A7_5")
				(number "G23")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L8N_M5A2_5")
				(number "G24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L9P_M5BA0_5")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L9N_M5BA1_5")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L10P_M5A0_5")
				(number "B24")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L10N_M5A1_5")
				(number "A25")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L11P_M5CLK_5")
				(number "C25")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L11N_M5CLKN_5")
				(number "C26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L12P_M5A3_5")
				(number "B25")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L12N_M5ODT_5")
				(number "B26")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L13P_M5A5_5")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L13N_M5A6_5")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L14P_M5RASN_5")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L14N_M5CASN_5")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L15P_M5UDM_5")
				(number "J23")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L15N_M5LDM_5")
				(number "J24")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L16P_M5DQ4_5")
				(number "E25")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L16N_M5DQ5_5")
				(number "E26")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L17P_M5DQ6_5")
				(number "D24")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L17N_M5DQ7_5")
				(number "D26")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L18P_M5LDQS_5")
				(number "F24")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L18N_M5LDQSN_5")
				(number "F26")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L19P_M5DQ2_5")
				(number "H24")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L19N_M5DQ3_5")
				(number "H26")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L20P_M5DQ0_5")
				(number "G25")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L20N_M5DQ1_5")
				(number "G26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L21P_M5DQ8_5")
				(number "K24")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L21N_M5DQ9_5")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L22P_M5DQ10_5")
				(number "J25")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L22N_M5DQ11_5")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L23P_M5UDQS_5")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L23N_M5UDQSN_5")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L24P_M5DQ12_5")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L24N_M5DQ13_5")
				(number "L26")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L25P_M5DQ14_5")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L25N_M5DQ15_5")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L26P_5")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L26N_VREF_5")
				(number "L21")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L27P_5")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L27N_5")
				(number "J20")
			)
		)
		(symbol "XC6SLX75-FGG676_4_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "F20")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "A24")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "C23")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "E21")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AF23")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AF3")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "AD23")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "AC22")
			)
		)
		(symbol "XC6SLX75-FGG676_5_1"
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F6")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F21")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G15")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J18")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L22")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M17")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N10")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U6")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U14")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "Y19")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA6")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA10")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA16")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA21")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "RFUSE")
				(number "AA20")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VBATT")
				(number "W21")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VFS")
				(number "AB19")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B21")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F2")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F19")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "F25")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H11")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J19")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "K2")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "K16")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "K25")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "L15")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "M5")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "M16")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "M22")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "N15")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "P2")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "L16")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "R16")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "U16")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "P19")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "R8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T5")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "V2")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "W15")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "W20")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "Y7")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "Y11")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "Y23")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AB2")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AB12")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AB16")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AB20")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AB25")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AC8")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AE6")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AE10")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AE14")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AE18")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AF26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX75T-CSG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX75T-CSG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 75 XC6SLX75T-CSG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX75T-CSG484_1_1"
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "G7")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "G10")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "F11")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "G12")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "F12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "C18")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D20")
			)
			(pin power_in line
				(at -40.64 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -35.56 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E10")
			)
			(pin power_in line
				(at -33.02 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -30.48 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F6")
			)
			(pin power_in line
				(at -27.94 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G13")
			)
			(pin power_in line
				(at -25.4 134.62 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H8")
			)
			(pin power_in line
				(at 12.7 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AA19")
			)
			(pin power_in line
				(at 15.24 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 17.78 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 20.32 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 22.86 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 25.4 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 27.94 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 30.48 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 33.02 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R15")
			)
			(pin power_in line
				(at 35.56 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 134.62 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "G17")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L15P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L15N_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L16P_1")
				(number "A20")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L16N_1")
				(number "A21")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L17P_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L17N_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L18P_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L18N_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "AA21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "AA22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "R12")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "R13")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "T12")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "T13")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "AA20")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "AB21")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L62P_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L62N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L63P_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L63N_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L64P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L64N_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L65P_1")
				(number "AB19")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L65N_1")
				(number "AB20")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "Y19")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "Y20")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "T15")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "V17")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "V18")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "T20")
			)
		)
		(symbol "XC6SLX75T-CSG484_2_1"
			(pin bidirectional line
				(at -50.8 124.46 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 121.92 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "Y18")
			)
			(pin bidirectional line
				(at -50.8 119.38 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 116.84 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 114.3 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 111.76 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 109.22 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 106.68 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 104.14 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 101.6 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "W13")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "W15")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "Y16")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "Y14")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L20P_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L20N_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "W11")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "Y10")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L42P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L42N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W6")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "Y6")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AB5")
			)
			(pin power_in line
				(at -40.64 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -35.56 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -33.02 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U14")
			)
			(pin power_in line
				(at -30.48 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -27.94 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -25.4 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at -22.86 144.78 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W16")
			)
			(pin power_in line
				(at 10.16 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AA3")
			)
			(pin power_in line
				(at 12.7 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 15.24 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 17.78 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 20.32 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 22.86 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 25.4 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 27.94 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 30.48 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 33.02 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R7")
			)
			(pin power_in line
				(at 35.56 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T9")
			)
			(pin power_in line
				(at 38.1 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 144.78 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 124.46 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 121.92 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AB2")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "Y4")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L11P_3")
				(number "V11")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L11N_3")
				(number "U10")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L12P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L12N_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L13P_3")
				(number "U6")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L13N_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L20P_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L20N_3")
				(number "T5")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L21P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L21N_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L22P_3")
				(number "T7")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L22N_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "U9")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "T11")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "T10")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "R8")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L69P_3")
				(number "A3")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L69N_3")
				(number "A2")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L70P_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L70N_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L71P_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L71N_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -119.38 180)
				(length 6.35)
				(name "IO_L72P_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -121.92 180)
				(length 6.35)
				(name "IO_L72N_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -124.46 180)
				(length 6.35)
				(name "IO_L73P_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -127 180)
				(length 6.35)
				(name "IO_L73N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -129.54 180)
				(length 6.35)
				(name "IO_L74P_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -132.08 180)
				(length 6.35)
				(name "IO_L74N_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -134.62 180)
				(length 6.35)
				(name "IO_L75P_3")
				(number "D4")
			)
			(pin bidirectional line
				(at 50.8 -137.16 180)
				(length 6.35)
				(name "IO_L75N_3")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -139.7 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -142.24 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "D3")
			)
		)
		(symbol "XC6SLX75T-CSG484_3_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C9")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "A10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "D11")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "C11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B14")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A14")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B16")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A16")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D13")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C13")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C15")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "B12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "A12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "F14")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "E14")
			)
		)
		(symbol "XC6SLX75T-CSG484_4_1"
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B9")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "D12")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C10")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "B13")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "E13")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "E15")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A7")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E11")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D14")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A15")
			)
		)
		(symbol "XC6SLX75T-CSG484_5_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "F17")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "H16")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "C19")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "U16")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AA1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "W18")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "U12")
			)
		)
		(symbol "XC6SLX75T-CSG484_6_1"
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F18")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R11")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "RFUSE")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VBATT")
				(number "R14")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VFS")
				(number "U19")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B15")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "E12")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "F15")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "G14")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "V16")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX75T-FGG484"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX75T-FGG484"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 75 XC6SLX75T-FGG484"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX75T-FGG484_1_1"
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "C3")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "D4")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "H10")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "H11")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "H13")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L49P_0")
				(number "H14")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L49N_0")
				(number "G15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L50P_0")
				(number "C17")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L50N_0")
				(number "A17")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L51P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L51N_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "D18")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "D19")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B18")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A18")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C19")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A19")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B20")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A20")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D17")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "C18")
			)
			(pin power_in line
				(at -40.64 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B19")
			)
			(pin power_in line
				(at -35.56 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E17")
			)
			(pin power_in line
				(at -33.02 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F6")
			)
			(pin power_in line
				(at -30.48 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G10")
			)
			(pin power_in line
				(at -27.94 114.3 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G14")
			)
			(pin power_in line
				(at 17.78 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "C21")
			)
			(pin power_in line
				(at 20.32 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E19")
			)
			(pin power_in line
				(at 22.86 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G21")
			)
			(pin power_in line
				(at 25.4 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J18")
			)
			(pin power_in line
				(at 27.94 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L16")
			)
			(pin power_in line
				(at 30.48 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "L21")
			)
			(pin power_in line
				(at 33.02 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N18")
			)
			(pin power_in line
				(at 35.56 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R21")
			)
			(pin power_in line
				(at 38.1 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "U18")
			)
			(pin power_in line
				(at 40.64 114.3 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F19")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L9P_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L9N_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L10P_1")
				(number "B21")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L10N_1")
				(number "B22")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L19P_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L19N_1")
				(number "J17")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L20P_1")
				(number "C20")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L20N_1")
				(number "C22")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L21P_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L21N_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "D21")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "D22")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "G19")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "F20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "H19")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "F21")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "E20")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "E22")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "J19")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "G22")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "M20")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "P20")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "L22")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "M22")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "R22")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "T21")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "V22")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "W20")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "W22")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "Y21")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "Y22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L58P_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L58N_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L59P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L59N_1")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L60P_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L60N_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "M17")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L70P_1")
				(number "R15")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L70N_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L71P_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L71N_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L72P_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L72N_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L73P_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L73N_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "V19")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "V20")
			)
		)
		(symbol "XC6SLX75T-FGG484_2_1"
			(pin bidirectional line
				(at -50.8 99.06 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 96.52 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 93.98 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "V17")
			)
			(pin bidirectional line
				(at -50.8 91.44 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "W18")
			)
			(pin bidirectional line
				(at -50.8 88.9 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AA20")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AB20")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "V15")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 6.35)
				(name "IO_L6P_2")
				(number "AA14")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L6N_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "Y19")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AB19")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "AA18")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "AB18")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB17")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "U14")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L21P_2")
				(number "Y15")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L21N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L19P_2")
				(number "AA16")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L19N_2")
				(number "AB16")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "T12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "U12")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AB13")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AB12")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L40P_2")
				(number "W12")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L40N_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "Y7")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AB7")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AB10")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "AA8")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "AB8")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "Y9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "W9")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "Y8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AB6")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "Y5")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "AB5")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AA4")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AB4")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "U6")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "Y4")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AA3")
			)
			(pin power_in line
				(at -40.64 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA7")
			)
			(pin power_in line
				(at -38.1 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA11")
			)
			(pin power_in line
				(at -35.56 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA15")
			)
			(pin power_in line
				(at -33.02 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA19")
			)
			(pin power_in line
				(at -30.48 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AB3")
			)
			(pin power_in line
				(at -27.94 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T9")
			)
			(pin power_in line
				(at -25.4 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "T13")
			)
			(pin power_in line
				(at -22.86 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V8")
			)
			(pin power_in line
				(at -20.32 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V12")
			)
			(pin power_in line
				(at -17.78 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "V16")
			)
			(pin power_in line
				(at -15.24 119.38 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W5")
			)
			(pin power_in line
				(at 17.78 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "C2")
			)
			(pin power_in line
				(at 20.32 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "F4")
			)
			(pin power_in line
				(at 22.86 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G2")
			)
			(pin power_in line
				(at 25.4 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 27.94 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L2")
			)
			(pin power_in line
				(at 30.48 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "L7")
			)
			(pin power_in line
				(at 33.02 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N5")
			)
			(pin power_in line
				(at 35.56 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin power_in line
				(at 38.1 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "U5")
			)
			(pin power_in line
				(at 40.64 119.38 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "W4")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "T5")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L23P_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L23N_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L24P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L24N_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L25P_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L25N_3")
				(number "P7")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L26P_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L26N_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "M7")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M8")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "V2")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "M6")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "K7")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "K8")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L58P_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L58N_3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L59P_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L59N_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L60P_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 6.35)
				(name "IO_L60N_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 6.35)
				(name "IO_L80P_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 6.35)
				(name "IO_L80N_3")
				(number "G7")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 6.35)
				(name "IO_L81P_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 6.35)
				(name "IO_L81N_3")
				(number "H8")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 6.35)
				(name "IO_L82P_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -111.76 180)
				(length 6.35)
				(name "IO_L82N_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -114.3 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -116.84 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "B1")
			)
		)
		(symbol "XC6SLX75T-FGG484_3_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C9")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "A10")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "C11")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "D11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B14")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A14")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B16")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A16")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D13")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C13")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C15")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "A12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "B12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "E12")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "F12")
			)
		)
		(symbol "XC6SLX75T-FGG484_4_1"
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B9")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "D12")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C10")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "B13")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "E13")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "E10")
			)
			(pin power_in line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A7")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E8")
			)
			(pin power_in line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D14")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A15")
			)
		)
		(symbol "XC6SLX75T-FGG484_5_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E18")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "G17")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "D20")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A21")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AB2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "AA22")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "V18")
			)
		)
		(symbol "XC6SLX75T-FGG484_6_1"
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H15")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L8")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M15")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N8")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R6")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R10")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R12")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U11")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V6")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "RFUSE")
				(number "P15")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VBATT")
				(number "T16")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VFS")
				(number "U17")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A13")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A22")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "B5")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B15")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C12")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C14")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "E2")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "E21")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "G18")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "J2")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J13")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "J21")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "K12")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "J12")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "J14")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "K13")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "M9")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "N10")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "N14")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "P9")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "L18")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "M10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "N2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "N9")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N17")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "N21")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "R5")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U2")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "U7")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "U21")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "V4")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "V10")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "V14")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "W7")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "W16")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "W19")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AA5")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AA9")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AA13")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AA17")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AB1")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AB22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX75T-FGG676"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX75T-FGG676"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LXT 75 XC6SLX75T-FGG676"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX75T-FGG676_1_1"
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "H7")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "G7")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "H8")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "G8")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "F6")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "C3")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "G6")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "F5")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L13P_0")
				(number "H9")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L13N_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L14P_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L14N_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "E5")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L22P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L22N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L24P_0")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L24N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L32P_0")
				(number "J11")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L32N_0")
				(number "G11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "H12")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "D13")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "K12")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "J12")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L43P_0")
				(number "J15")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L43N_0")
				(number "H15")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L48P_0")
				(number "J16")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L48N_0")
				(number "J17")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L56P_0")
				(number "G16")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L56N_0")
				(number "F17")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L57P_0")
				(number "F20")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L57N_0")
				(number "E20")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L58P_0")
				(number "H17")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L58N_0")
				(number "G17")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L59P_0")
				(number "C21")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L59N_0")
				(number "B21")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "H18")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "H19")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B22")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A22")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "G19")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "F19")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B23")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A23")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D21")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D22")
			)
			(pin power_in line
				(at -40.64 88.9 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B13")
			)
			(pin power_in line
				(at -38.1 88.9 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C4")
			)
			(pin power_in line
				(at -35.56 88.9 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C22")
			)
			(pin power_in line
				(at -33.02 88.9 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E21")
			)
			(pin power_in line
				(at -30.48 88.9 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F8")
			)
			(pin power_in line
				(at -27.94 88.9 270)
				(length 6.35)
				(name "VCCO_0")
				(number "F13")
			)
			(pin power_in line
				(at -25.4 88.9 270)
				(length 6.35)
				(name "VCCO_0")
				(number "G18")
			)
			(pin power_in line
				(at -22.86 88.9 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H11")
			)
			(pin power_in line
				(at -20.32 88.9 270)
				(length 6.35)
				(name "VCCO_0")
				(number "H16")
			)
			(pin power_in line
				(at -17.78 88.9 270)
				(length 6.35)
				(name "VCCO_0")
				(number "J14")
			)
			(pin power_in line
				(at 22.86 88.9 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AB23")
			)
			(pin power_in line
				(at 25.4 88.9 270)
				(length 6.35)
				(name "VCCO_1")
				(number "AD25")
			)
			(pin power_in line
				(at 27.94 88.9 270)
				(length 6.35)
				(name "VCCO_1")
				(number "P18")
			)
			(pin power_in line
				(at 30.48 88.9 270)
				(length 6.35)
				(name "VCCO_1")
				(number "P23")
			)
			(pin power_in line
				(at 33.02 88.9 270)
				(length 6.35)
				(name "VCCO_1")
				(number "T25")
			)
			(pin power_in line
				(at 35.56 88.9 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W21")
			)
			(pin power_in line
				(at 38.1 88.9 270)
				(length 6.35)
				(name "VCCO_1")
				(number "W23")
			)
			(pin power_in line
				(at 40.64 88.9 270)
				(length 6.35)
				(name "VCCO_1")
				(number "Y25")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L28P_1")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L28N_VREF_1")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "L23")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "L24")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "N19")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "N20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "N21")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "N22")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "P19")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "N23")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "N24")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "R18")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "R19")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "P21")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "P22")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "R20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "R21")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "P24")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "P26")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "R23")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "R24")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "T22")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "T23")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "U23")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "U24")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "R25")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "R26")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "V23")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "W24")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "U25")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "U26")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "T24")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "T26")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "V24")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "V26")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "W25")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "W26")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "AA25")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "AA26")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "AD24")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "AD26")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "AB24")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "AB26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "AC25")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "AC26")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "Y24")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "Y26")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "AE25")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "AE26")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "U21")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "U22")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L66P_1")
				(number "T19")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L66N_1")
				(number "T20")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L67P_1")
				(number "AA23")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L67N_1")
				(number "AA24")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L68P_1")
				(number "U19")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L68N_1")
				(number "U20")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L69P_1")
				(number "V20")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L69N_VREF_1")
				(number "V21")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "AC23")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "AC24")
			)
		)
		(symbol "XC6SLX75T-FGG676_2_1"
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "AE24")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "AF24")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "Y21")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "AA22")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "AD23")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "AF23")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L4P_2")
				(number "W20")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L4N_VREF_2")
				(number "Y20")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L5P_2")
				(number "AB22")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L5N_2")
				(number "AC22")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "V18")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "W19")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "AD22")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "AF22")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "W17")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "W18")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "AA21")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "AB21")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "Y17")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "AA17")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L17P_2")
				(number "U15")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L17N_2")
				(number "V16")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L28P_2")
				(number "AA15")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L28N_2")
				(number "AB15")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "AE15")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "AF15")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "AB14")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "AC14")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "AE13")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "AF13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "AD14")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "AF14")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L33P_2")
				(number "Y12")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L33N_2")
				(number "AA12")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L34P_2")
				(number "W14")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L34N_2")
				(number "Y13")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "Y11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "AA11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "V10")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "AA9")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "AB9")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "AA10")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "AB11")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "AD6")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "AF6")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L61P_2")
				(number "AC5")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L61N_VREF_2")
				(number "AD5")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "W8")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "W7")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "AD4")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "AF4")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "AA7")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "AA6")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "AE3")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "AF3")
			)
			(pin power_in line
				(at -40.64 96.52 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA14")
			)
			(pin power_in line
				(at -38.1 96.52 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AA20")
			)
			(pin power_in line
				(at -35.56 96.52 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AB6")
			)
			(pin power_in line
				(at -33.02 96.52 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE4")
			)
			(pin power_in line
				(at -30.48 96.52 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE14")
			)
			(pin power_in line
				(at -27.94 96.52 270)
				(length 6.35)
				(name "VCCO_2")
				(number "AE23")
			)
			(pin power_in line
				(at -25.4 96.52 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W11")
			)
			(pin power_in line
				(at -22.86 96.52 270)
				(length 6.35)
				(name "VCCO_2")
				(number "W15")
			)
			(pin power_in line
				(at -20.32 96.52 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y8")
			)
			(pin power_in line
				(at -17.78 96.52 270)
				(length 6.35)
				(name "VCCO_2")
				(number "Y18")
			)
			(pin power_in line
				(at 22.86 96.52 270)
				(length 6.35)
				(name "VCCO_3")
				(number "AD2")
			)
			(pin power_in line
				(at 25.4 96.52 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P4")
			)
			(pin power_in line
				(at 27.94 96.52 270)
				(length 6.35)
				(name "VCCO_3")
				(number "P9")
			)
			(pin power_in line
				(at 30.48 96.52 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T2")
			)
			(pin power_in line
				(at 33.02 96.52 270)
				(length 6.35)
				(name "VCCO_3")
				(number "T7")
			)
			(pin power_in line
				(at 35.56 96.52 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W4")
			)
			(pin power_in line
				(at 38.1 96.52 270)
				(length 6.35)
				(name "VCCO_3")
				(number "W6")
			)
			(pin power_in line
				(at 40.64 96.52 270)
				(length 6.35)
				(name "VCCO_3")
				(number "Y2")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "AB5")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "AC4")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "AA4")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "AA3")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 6.35)
				(name "IO_L7P_3")
				(number "Y6")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 6.35)
				(name "IO_L7N_3")
				(number "Y5")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L8P_3")
				(number "AB4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L8N_3")
				(number "AC3")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L9P_3")
				(number "V7")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L9N_3")
				(number "V6")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L10P_3")
				(number "U4")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L10N_3")
				(number "U3")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L17P_3")
				(number "V5")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L17N_VREF_3")
				(number "W5")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L18P_3")
				(number "U9")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L18N_3")
				(number "U8")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "U7")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "AB3")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "AB1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "AD3")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "AD1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "AC2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "AC1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "AE2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "AE1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "AA2")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "AA1")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "Y3")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "Y1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "W2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "W1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "V3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "V1")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "T3")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "V4")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "W3")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "R7")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "R8")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "T8")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "U5")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "T4")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "R10")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "T9")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "N6")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "P5")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "R5")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "N8")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "N7")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "R4")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "R3")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "R9")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "P8")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "N5")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "P10")
			)
			(pin bidirectional line
				(at 50.8 -88.9 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "N9")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 6.35)
				(name "IO_L57P_3")
				(number "M10")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 6.35)
				(name "IO_L57N_VREF_3")
				(number "M9")
			)
		)
		(symbol "XC6SLX75T-FGG676_3_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L58P_4")
				(number "M4")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L58N_VREF_4")
				(number "N3")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L59P_M4DQ14_4")
				(number "N2")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L59N_M4DQ15_4")
				(number "N1")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L60P_M4DQ12_4")
				(number "M3")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L60N_M4DQ13_4")
				(number "M1")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L61P_M4UDQS_4")
				(number "L2")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L61N_M4UDQSN_4")
				(number "L1")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L62P_M4DQ10_4")
				(number "K3")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L62N_M4DQ11_4")
				(number "K1")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L63P_M4DQ8_4")
				(number "J2")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L63N_M4DQ9_4")
				(number "J1")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L64P_M4DQ0_4")
				(number "H3")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L64N_M4DQ1_4")
				(number "H1")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L65P_M4DQ2_4")
				(number "G2")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L65N_M4DQ3_4")
				(number "G1")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L66P_M4LDQS_4")
				(number "F3")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L66N_M4LDQSN_4")
				(number "F1")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L67P_M4DQ6_4")
				(number "E2")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L67N_M4DQ7_4")
				(number "E1")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L68P_M4DQ4_4")
				(number "D3")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L68N_M4DQ5_4")
				(number "D1")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L69P_M4UDM_4")
				(number "J4")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L69N_M4LDM_4")
				(number "J3")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L70P_M4RASN_4")
				(number "L9")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L70N_M4CASN_4")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L71P_M4A5_4")
				(number "L4")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L71N_M4A6_4")
				(number "L3")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L72P_M4A3_4")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L72N_M4ODT_4")
				(number "M6")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L73P_M4CLK_4")
				(number "K5")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L73N_M4CLKN_4")
				(number "J5")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L74P_M4A0_4")
				(number "L7")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L74N_M4A1_4")
				(number "L6")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L75P_M4BA0_4")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L75N_M4BA1_4")
				(number "B1")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L76P_M4A7_4")
				(number "L10")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L76N_M4A2_4")
				(number "K10")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L77P_M4WE_4")
				(number "G4")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L77N_M4BA2_4")
				(number "G3")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L78P_M4A10_4")
				(number "J9")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L78N_M4A4_4")
				(number "J7")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L79P_M4A8_4")
				(number "C2")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L79N_M4A9_4")
				(number "C1")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L80P_M4CKE_4")
				(number "K9")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L80N_M4A12_4")
				(number "K8")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L81P_M4RESET_4")
				(number "E4")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 6.35)
				(name "IO_L81N_M4A11_4")
				(number "E3")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 6.35)
				(name "IO_L82P_M4A13_4")
				(number "K7")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 6.35)
				(name "IO_L82N_M4A14_4")
				(number "K6")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 6.35)
				(name "IO_L83P_4")
				(number "H6")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 6.35)
				(name "IO_L83N_VREF_4")
				(number "H5")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "D2")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "F4")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "H2")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "J6")
			)
			(pin power_in line
				(at -30.48 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "K4")
			)
			(pin power_in line
				(at -27.94 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "M2")
			)
			(pin power_in line
				(at -25.4 78.74 270)
				(length 6.35)
				(name "VCCO_4")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "D25")
			)
			(pin power_in line
				(at 27.94 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "G22")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "H25")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "J21")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "K23")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "M20")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_5")
				(number "M25")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_A25_5")
				(number "H20")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_5")
				(number "G20")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L2P_M5A13_5")
				(number "B24")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L2N_M5A14_5")
				(number "A25")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L3P_M5RESET_5")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L3N_M5A11_5")
				(number "K19")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L4P_M5CKE_5")
				(number "D23")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L4N_M5A12_5")
				(number "C24")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L5P_M5A8_5")
				(number "H21")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L5N_M5A9_5")
				(number "H22")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L6P_M5A10_5")
				(number "F22")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L6N_M5A4_5")
				(number "G23")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L7P_M5WE_5")
				(number "J20")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L7N_M5BA2_5")
				(number "J22")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L8P_M5A7_5")
				(number "E23")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L8N_M5A2_5")
				(number "E24")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L9P_M5BA0_5")
				(number "L19")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L9N_M5BA1_5")
				(number "K20")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L10P_M5A0_5")
				(number "C25")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L10N_M5A1_5")
				(number "C26")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L11P_M5CLK_5")
				(number "B25")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L11N_M5CLKN_5")
				(number "B26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L12P_M5A3_5")
				(number "K21")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L12N_M5ODT_5")
				(number "K22")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L13P_M5A5_5")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L13N_M5A6_5")
				(number "M19")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L14P_M5RASN_5")
				(number "F23")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L14N_M5CASN_5")
				(number "G24")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L15P_M5UDM_5")
				(number "J23")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L15N_M5LDM_5")
				(number "J24")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L16P_M5DQ4_5")
				(number "E25")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L16N_M5DQ5_5")
				(number "E26")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L17P_M5DQ6_5")
				(number "D24")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L17N_M5DQ7_5")
				(number "D26")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L18P_M5LDQS_5")
				(number "F24")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L18N_M5LDQSN_5")
				(number "F26")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L19P_M5DQ2_5")
				(number "H24")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L19N_M5DQ3_5")
				(number "H26")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L20P_M5DQ0_5")
				(number "G25")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L20N_M5DQ1_5")
				(number "G26")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L21P_M5DQ8_5")
				(number "K24")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L21N_M5DQ9_5")
				(number "K26")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L22P_M5DQ10_5")
				(number "J25")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L22N_M5DQ11_5")
				(number "J26")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L23P_M5UDQS_5")
				(number "M24")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L23N_M5UDQSN_5")
				(number "M26")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L24P_M5DQ12_5")
				(number "L25")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L24N_M5DQ13_5")
				(number "L26")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L25P_M5DQ14_5")
				(number "N25")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L25N_M5DQ15_5")
				(number "N26")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L26P_5")
				(number "M21")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L26N_VREF_5")
				(number "M23")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L27P_5")
				(number "L20")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L27N_5")
				(number "L21")
			)
		)
		(symbol "XC6SLX75T-FGG676_4_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_101")
				(number "B6")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_101")
				(number "A6")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_101")
				(number "B8")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_101")
				(number "A8")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_101")
				(number "D7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_101")
				(number "C7")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_101")
				(number "D9")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_101")
				(number "C9")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_101")
				(number "B10")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_101")
				(number "A10")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_101")
				(number "D11")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_101")
				(number "C11")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_123")
				(number "B18")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_123")
				(number "A18")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_123")
				(number "B20")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_123")
				(number "A20")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_123")
				(number "D17")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_123")
				(number "C17")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_123")
				(number "D19")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_123")
				(number "C19")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_123")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_123")
				(number "C15")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_123")
				(number "B16")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_123")
				(number "A16")
			)
		)
		(symbol "XC6SLX75T-FGG676_5_1"
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTTXP0_245")
				(number "AE7")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTTXN0_245")
				(number "AF7")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTTXP1_245")
				(number "AE9")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 6.35)
				(name "MGTTXN1_245")
				(number "AF9")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTRXP0_245")
				(number "AC8")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTRXN0_245")
				(number "AD8")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 6.35)
				(name "MGTRXP1_245")
				(number "AC10")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTRXN1_245")
				(number "AD10")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTREFCLK0P_245")
				(number "AE11")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 6.35)
				(name "MGTREFCLK0N_245")
				(number "AF11")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTREFCLK1P_245")
				(number "AC12")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTREFCLK1N_245")
				(number "AD12")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTTXP0_267")
				(number "AE19")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTTXN0_267")
				(number "AF19")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTTXP1_267")
				(number "AE21")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTTXN1_267")
				(number "AF21")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTRXP0_267")
				(number "AC18")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTRXN0_267")
				(number "AD18")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "MGTRXP1_267")
				(number "AC20")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTRXN1_267")
				(number "AD20")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTREFCLK0P_267")
				(number "AC16")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTREFCLK0N_267")
				(number "AD16")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "MGTREFCLK1P_267")
				(number "AE17")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTREFCLK1N_267")
				(number "AF17")
			)
		)
		(symbol "XC6SLX75T-FGG676_6_1"
			(pin power_in line
				(at -38.1 17.78 0)
				(length 6.35)
				(name "MGTAVCCPLL0_101")
				(number "B11")
			)
			(pin power_in line
				(at -38.1 15.24 0)
				(length 6.35)
				(name "MGTAVCCPLL1_101")
				(number "C12")
			)
			(pin power_in line
				(at -38.1 12.7 0)
				(length 6.35)
				(name "MGTAVCC_101")
				(number "C10")
			)
			(pin power_in line
				(at -38.1 7.62 0)
				(length 6.35)
				(name "MGTAVCCPLL0_123")
				(number "C14")
			)
			(pin power_in line
				(at -38.1 5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_123")
				(number "B15")
			)
			(pin power_in line
				(at -38.1 2.54 0)
				(length 6.35)
				(name "MGTAVCC_123")
				(number "C16")
			)
			(pin power_in line
				(at -38.1 -2.54 0)
				(length 6.35)
				(name "MGTAVCCPLL0_245")
				(number "AE12")
			)
			(pin power_in line
				(at -38.1 -5.08 0)
				(length 6.35)
				(name "MGTAVCCPLL1_245")
				(number "AD13")
			)
			(pin power_in line
				(at -38.1 -7.62 0)
				(length 6.35)
				(name "MGTAVCC_245")
				(number "AD11")
			)
			(pin power_in line
				(at -38.1 -12.7 0)
				(length 6.35)
				(name "MGTAVCCPLL0_267")
				(number "AD15")
			)
			(pin power_in line
				(at -38.1 -15.24 0)
				(length 6.35)
				(name "MGTAVCCPLL1_267")
				(number "AE16")
			)
			(pin power_in line
				(at -38.1 -17.78 0)
				(length 6.35)
				(name "MGTAVCC_267")
				(number "AD17")
			)
			(pin power_in line
				(at 38.1 17.78 180)
				(length 6.35)
				(name "MGTAVTTRX_101")
				(number "D8")
			)
			(pin power_in line
				(at 38.1 15.24 180)
				(length 6.35)
				(name "MGTAVTTTX_101")
				(number "A7")
			)
			(pin power_in line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "MGTAVTTRCAL_101")
				(number "E11")
			)
			(pin power_in line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "MGTRREF_101")
				(number "E9")
			)
			(pin power_in line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "MGTAVTTRX_123")
				(number "D18")
			)
			(pin power_in line
				(at 38.1 2.54 180)
				(length 6.35)
				(name "MGTAVTTTX_123")
				(number "A19")
			)
			(pin power_in line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "MGTAVTTRX_245")
				(number "AC9")
			)
			(pin power_in line
				(at 38.1 -5.08 180)
				(length 6.35)
				(name "MGTAVTTTX_245")
				(number "AF8")
			)
			(pin power_in line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "MGTAVTTRCAL_245")
				(number "AB12")
			)
			(pin power_in line
				(at 38.1 -10.16 180)
				(length 6.35)
				(name "MGTRREF_245")
				(number "AB10")
			)
			(pin power_in line
				(at 38.1 -15.24 180)
				(length 6.35)
				(name "MGTAVTTRX_267")
				(number "AC19")
			)
			(pin power_in line
				(at 38.1 -17.78 180)
				(length 6.35)
				(name "MGTAVTTTX_267")
				(number "AF20")
			)
		)
		(symbol "XC6SLX75T-FGG676_7_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "C23")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "G21")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "F21")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A24")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "AF25")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "AF2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "Y22")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "Y19")
			)
		)
		(symbol "XC6SLX75T-FGG676_8_1"
			(pin power_in line
				(at -25.4 96.52 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 93.98 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D20")
			)
			(pin power_in line
				(at -25.4 91.44 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E17")
			)
			(pin power_in line
				(at -25.4 88.9 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 86.36 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J10")
			)
			(pin power_in line
				(at -25.4 83.82 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J18")
			)
			(pin power_in line
				(at -25.4 81.28 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K13")
			)
			(pin power_in line
				(at -25.4 78.74 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K15")
			)
			(pin power_in line
				(at -25.4 76.2 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L5")
			)
			(pin power_in line
				(at -25.4 73.66 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L18")
			)
			(pin power_in line
				(at -25.4 71.12 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L22")
			)
			(pin power_in line
				(at -25.4 68.58 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M17")
			)
			(pin power_in line
				(at -25.4 66.04 0)
				(length 6.35)
				(name "VCCAUX")
				(number "N10")
			)
			(pin power_in line
				(at -25.4 63.5 0)
				(length 6.35)
				(name "VCCAUX")
				(number "R22")
			)
			(pin power_in line
				(at -25.4 60.96 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U6")
			)
			(pin power_in line
				(at -25.4 58.42 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U12")
			)
			(pin power_in line
				(at -25.4 55.88 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U14")
			)
			(pin power_in line
				(at -25.4 53.34 0)
				(length 6.35)
				(name "VCCAUX")
				(number "U18")
			)
			(pin power_in line
				(at -25.4 50.8 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V9")
			)
			(pin power_in line
				(at -25.4 48.26 0)
				(length 6.35)
				(name "VCCAUX")
				(number "V17")
			)
			(pin power_in line
				(at -25.4 45.72 0)
				(length 6.35)
				(name "VCCAUX")
				(number "W13")
			)
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AA5")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB8")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AB18")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC7")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "AC21")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "RFUSE")
				(number "V19")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VBATT")
				(number "V22")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VFS")
				(number "W22")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "GND")
				(number "A9")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "GND")
				(number "A11")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "GND")
				(number "A15")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A17")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A21")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "A26")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B9")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "B19")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "C8")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "C18")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "C20")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "D12")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "D14")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "D16")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "E19")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "E22")
			)
			(pin power_in line
				(at -25.4 -45.72 0)
				(length 6.35)
				(name "GND")
				(number "F2")
			)
			(pin power_in line
				(at -25.4 -48.26 0)
				(length 6.35)
				(name "GND")
				(number "F25")
			)
			(pin power_in line
				(at -25.4 -50.8 0)
				(length 6.35)
				(name "GND")
				(number "G14")
			)
			(pin power_in line
				(at -25.4 -53.34 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at -25.4 -55.88 0)
				(length 6.35)
				(name "GND")
				(number "H23")
			)
			(pin power_in line
				(at -25.4 -58.42 0)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at -25.4 -60.96 0)
				(length 6.35)
				(name "GND")
				(number "J19")
			)
			(pin power_in line
				(at -25.4 -63.5 0)
				(length 6.35)
				(name "GND")
				(number "K2")
			)
			(pin power_in line
				(at -25.4 -66.04 0)
				(length 6.35)
				(name "GND")
				(number "K16")
			)
			(pin power_in line
				(at -25.4 -68.58 0)
				(length 6.35)
				(name "GND")
				(number "K25")
			)
			(pin power_in line
				(at -25.4 -71.12 0)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at -25.4 -73.66 0)
				(length 6.35)
				(name "GND")
				(number "L13")
			)
			(pin power_in line
				(at -25.4 -76.2 0)
				(length 6.35)
				(name "GND")
				(number "L15")
			)
			(pin power_in line
				(at -25.4 -78.74 0)
				(length 6.35)
				(name "GND")
				(number "L17")
			)
			(pin power_in line
				(at -25.4 -81.28 0)
				(length 6.35)
				(name "GND")
				(number "M5")
			)
			(pin power_in line
				(at -25.4 -83.82 0)
				(length 6.35)
				(name "GND")
				(number "M22")
			)
			(pin power_in line
				(at -25.4 -86.36 0)
				(length 6.35)
				(name "GND")
				(number "N11")
			)
			(pin power_in line
				(at -25.4 -88.9 0)
				(length 6.35)
				(name "GND")
				(number "N14")
			)
			(pin power_in line
				(at -25.4 -91.44 0)
				(length 6.35)
				(name "GND")
				(number "P2")
			)
			(pin power_in line
				(at -25.4 -93.98 0)
				(length 6.35)
				(name "GND")
				(number "P7")
			)
			(pin power_in line
				(at -25.4 -96.52 0)
				(length 6.35)
				(name "GND")
				(number "P13")
			)
			(pin power_in line
				(at 25.4 96.52 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 93.98 180)
				(length 6.35)
				(name "VCCINT")
				(number "K17")
			)
			(pin power_in line
				(at 25.4 91.44 180)
				(length 6.35)
				(name "VCCINT")
				(number "L12")
			)
			(pin power_in line
				(at 25.4 88.9 180)
				(length 6.35)
				(name "VCCINT")
				(number "L14")
			)
			(pin power_in line
				(at 25.4 86.36 180)
				(length 6.35)
				(name "VCCINT")
				(number "L16")
			)
			(pin power_in line
				(at 25.4 83.82 180)
				(length 6.35)
				(name "VCCINT")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 81.28 180)
				(length 6.35)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 78.74 180)
				(length 6.35)
				(name "VCCINT")
				(number "M13")
			)
			(pin power_in line
				(at 25.4 76.2 180)
				(length 6.35)
				(name "VCCINT")
				(number "M14")
			)
			(pin power_in line
				(at 25.4 73.66 180)
				(length 6.35)
				(name "VCCINT")
				(number "M15")
			)
			(pin power_in line
				(at 25.4 71.12 180)
				(length 6.35)
				(name "VCCINT")
				(number "M16")
			)
			(pin power_in line
				(at 25.4 68.58 180)
				(length 6.35)
				(name "VCCINT")
				(number "N12")
			)
			(pin power_in line
				(at 25.4 66.04 180)
				(length 6.35)
				(name "VCCINT")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 63.5 180)
				(length 6.35)
				(name "VCCINT")
				(number "N15")
			)
			(pin power_in line
				(at 25.4 60.96 180)
				(length 6.35)
				(name "VCCINT")
				(number "N16")
			)
			(pin power_in line
				(at 25.4 58.42 180)
				(length 6.35)
				(name "VCCINT")
				(number "P11")
			)
			(pin power_in line
				(at 25.4 55.88 180)
				(length 6.35)
				(name "VCCINT")
				(number "P12")
			)
			(pin power_in line
				(at 25.4 53.34 180)
				(length 6.35)
				(name "VCCINT")
				(number "P14")
			)
			(pin power_in line
				(at 25.4 50.8 180)
				(length 6.35)
				(name "VCCINT")
				(number "P15")
			)
			(pin power_in line
				(at 25.4 48.26 180)
				(length 6.35)
				(name "VCCINT")
				(number "R11")
			)
			(pin power_in line
				(at 25.4 45.72 180)
				(length 6.35)
				(name "VCCINT")
				(number "R12")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "R13")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "R15")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "R16")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "R17")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "T11")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "T13")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "T15")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "T17")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "U10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "U16")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "GND")
				(number "P16")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "GND")
				(number "P20")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "GND")
				(number "P25")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "GND")
				(number "T5")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "T10")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "T12")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "T14")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "T18")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "T21")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "U11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "U17")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "V2")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "V8")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "V25")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "Y4")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "Y7")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "Y10")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "Y14")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "Y23")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "AB2")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "AB16")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "AB20")
			)
			(pin power_in line
				(at 25.4 -45.72 180)
				(length 6.35)
				(name "GND")
				(number "AB25")
			)
			(pin power_in line
				(at 25.4 -48.26 180)
				(length 6.35)
				(name "GND")
				(number "AC11")
			)
			(pin power_in line
				(at 25.4 -50.8 180)
				(length 6.35)
				(name "GND")
				(number "AC13")
			)
			(pin power_in line
				(at 25.4 -53.34 180)
				(length 6.35)
				(name "GND")
				(number "AC15")
			)
			(pin power_in line
				(at 25.4 -55.88 180)
				(length 6.35)
				(name "GND")
				(number "AC17")
			)
			(pin power_in line
				(at 25.4 -58.42 180)
				(length 6.35)
				(name "GND")
				(number "AD7")
			)
			(pin power_in line
				(at 25.4 -60.96 180)
				(length 6.35)
				(name "GND")
				(number "AD9")
			)
			(pin power_in line
				(at 25.4 -63.5 180)
				(length 6.35)
				(name "GND")
				(number "AD19")
			)
			(pin power_in line
				(at 25.4 -66.04 180)
				(length 6.35)
				(name "GND")
				(number "AD21")
			)
			(pin power_in line
				(at 25.4 -68.58 180)
				(length 6.35)
				(name "GND")
				(number "AE6")
			)
			(pin power_in line
				(at 25.4 -71.12 180)
				(length 6.35)
				(name "GND")
				(number "AE8")
			)
			(pin power_in line
				(at 25.4 -73.66 180)
				(length 6.35)
				(name "GND")
				(number "AE10")
			)
			(pin power_in line
				(at 25.4 -76.2 180)
				(length 6.35)
				(name "GND")
				(number "AE18")
			)
			(pin power_in line
				(at 25.4 -78.74 180)
				(length 6.35)
				(name "GND")
				(number "AE20")
			)
			(pin power_in line
				(at 25.4 -81.28 180)
				(length 6.35)
				(name "GND")
				(number "AE22")
			)
			(pin power_in line
				(at 25.4 -83.82 180)
				(length 6.35)
				(name "GND")
				(number "AF1")
			)
			(pin power_in line
				(at 25.4 -86.36 180)
				(length 6.35)
				(name "GND")
				(number "AF10")
			)
			(pin power_in line
				(at 25.4 -88.9 180)
				(length 6.35)
				(name "GND")
				(number "AF12")
			)
			(pin power_in line
				(at 25.4 -91.44 180)
				(length 6.35)
				(name "GND")
				(number "AF16")
			)
			(pin power_in line
				(at 25.4 -93.98 180)
				(length 6.35)
				(name "GND")
				(number "AF18")
			)
			(pin power_in line
				(at 25.4 -96.52 180)
				(length 6.35)
				(name "GND")
				(number "AF26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX9-CPG196"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX9-CPG196"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 9 XC6SLX9-CPG196"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX9-CPG196_1_1"
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B7")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "C11")
			)
			(pin power_in line
				(at -40.64 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C4")
			)
			(pin power_in line
				(at -38.1 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C5")
			)
			(pin power_in line
				(at -35.56 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C9")
			)
			(pin power_in line
				(at -33.02 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "C10")
			)
			(pin power_in line
				(at 27.94 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "D12")
			)
			(pin power_in line
				(at 30.48 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E12")
			)
			(pin power_in line
				(at 33.02 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G11")
			)
			(pin power_in line
				(at 35.56 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G12")
			)
			(pin power_in line
				(at 38.1 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "K11")
			)
			(pin power_in line
				(at 40.64 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L1P_1")
				(number "C12")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L1N_VREF_1")
				(number "C13")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L32P_1")
				(number "D13")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L32N_1")
				(number "D14")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L33P_1")
				(number "E13")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L33N_1")
				(number "E14")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L34P_1")
				(number "F11")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L34N_1")
				(number "F12")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_1")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_1")
				(number "H11")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45P_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45N_1")
				(number "J14")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46P_1")
				(number "J11")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46N_1")
				(number "J12")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47P_1")
				(number "K13")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L47N_1")
				(number "K14")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "L13")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "M14")
			)
		)
		(symbol "XC6SLX9-CPG196_2_1"
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "N13")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "P13")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "P12")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "N10")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "P10")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "P9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "P8")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "N7")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "P6")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "P5")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "L4")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "M4")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "N4")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "P4")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "N3")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "P3")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "N2")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "P2")
			)
			(pin power_in line
				(at -40.64 45.72 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M5")
			)
			(pin power_in line
				(at -38.1 45.72 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M6")
			)
			(pin power_in line
				(at -35.56 45.72 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M9")
			)
			(pin power_in line
				(at -33.02 45.72 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M10")
			)
			(pin power_in line
				(at 27.94 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "E3")
			)
			(pin power_in line
				(at 30.48 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "E4")
			)
			(pin power_in line
				(at 33.02 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G3")
			)
			(pin power_in line
				(at 35.56 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "H3")
			)
			(pin power_in line
				(at 38.1 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "K3")
			)
			(pin power_in line
				(at 40.64 45.72 270)
				(length 6.35)
				(name "VCCO_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L36P_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L36N_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L37P_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L37N_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_3")
				(number "J2")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_3")
				(number "G2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L49P_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L49N_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L50P_3")
				(number "E2")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L50N_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L51P_3")
				(number "D4")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L51N_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L52P_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L52N_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "B1")
			)
		)
		(symbol "XC6SLX9-CPG196_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "A13")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "C14")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "B14")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "B13")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "N14")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "N1")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "L12")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "M12")
			)
		)
		(symbol "XC6SLX9-CPG196_4_1"
			(pin power_in line
				(at -25.4 43.18 0)
				(length 6.35)
				(name "VCCAUX")
				(number "D7")
			)
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E7")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G9")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H5")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H6")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L7")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A14")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "C2")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C7")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D5")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "D6")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "D9")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "E8")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "G4")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "G6")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "G7")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -25.4 -43.18 0)
				(length 6.35)
				(name "GND")
				(number "H4")
			)
			(pin power_in line
				(at 25.4 43.18 180)
				(length 6.35)
				(name "VCCINT")
				(number "E5")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "E6")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "E9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "E10")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "F5")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "F6")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "F9")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "F10")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "J6")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "K5")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "K6")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "H10")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "J7")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "L3")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "L5")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "L6")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "M3")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "M11")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "P1")
			)
			(pin power_in line
				(at 25.4 -43.18 180)
				(length 6.35)
				(name "GND")
				(number "P14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX9-CSG225"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX9-CSG225"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 9 XC6SLX9-CSG225"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX9-CSG225_1_1"
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "E7")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B7")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "F8")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L39P_0")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L39N_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L40P_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L40N_0")
				(number "E9")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B13")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "C12")
			)
			(pin bidirectional line
				(at -50.8 -58.42 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A12")
			)
			(pin power_in line
				(at -40.64 60.96 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 60.96 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B8")
			)
			(pin power_in line
				(at -35.56 60.96 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B12")
			)
			(pin power_in line
				(at -33.02 60.96 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D9")
			)
			(pin power_in line
				(at 33.02 60.96 270)
				(length 6.35)
				(name "VCCO_1")
				(number "D14")
			)
			(pin power_in line
				(at 35.56 60.96 270)
				(length 6.35)
				(name "VCCO_1")
				(number "H14")
			)
			(pin power_in line
				(at 38.1 60.96 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J12")
			)
			(pin power_in line
				(at 40.64 60.96 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M14")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "B14")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "B15")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "G11")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "G12")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "F11")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "F12")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "H10")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "H11")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "C14")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "C15")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "D13")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "D15")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "J11")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "E14")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "K10")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "K11")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "L12")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "J14")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "J15")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K13")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M15")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "P14")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "P15")
			)
		)
		(symbol "XC6SLX9-CSG225_2_1"
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "R12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "P13")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "M11")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N10")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "R10")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "L9")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "M10")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L15P_2")
				(number "M9")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L15N_2")
				(number "N9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "P9")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "M8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "N7")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "K8")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "L7")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "M6")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "R6")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "P5")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "R5")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "L6")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "L5")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "N4")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "R4")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "M5")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "P3")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "R3")
			)
			(pin power_in line
				(at -40.64 63.5 270)
				(length 6.35)
				(name "VCCO_2")
				(number "M7")
			)
			(pin power_in line
				(at -38.1 63.5 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P4")
			)
			(pin power_in line
				(at -35.56 63.5 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P8")
			)
			(pin power_in line
				(at -33.02 63.5 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P12")
			)
			(pin power_in line
				(at 33.02 63.5 270)
				(length 6.35)
				(name "VCCO_3")
				(number "D2")
			)
			(pin power_in line
				(at 35.56 63.5 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G4")
			)
			(pin power_in line
				(at 38.1 63.5 270)
				(length 6.35)
				(name "VCCO_3")
				(number "H2")
			)
			(pin power_in line
				(at 40.64 63.5 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "J2")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "G2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "J5")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "G5")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "E5")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "E2")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "D4")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "C1")
			)
		)
		(symbol "XC6SLX9-CSG225_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "E10")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "D12")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "E13")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A14")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "R14")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "R2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "L13")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "L10")
			)
		)
		(symbol "XC6SLX9-CSG225_4_1"
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B1")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E12")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F7")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J6")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K9")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L4")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M12")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "A15")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B6")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B10")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "C13")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E11")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "F2")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "F6")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "F14")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G7")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G9")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "F9")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "G6")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "G8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "H7")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "K7")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "J7")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "K2")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "K6")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "K14")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N3")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "P6")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "P10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX9-CSG324"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX9-CSG324"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 9 XC6SLX9-CSG324"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX9-CSG324_1_1"
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "D4")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A2")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B3")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "B4")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L10P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L10N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L8P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L8N_VREF_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L11P_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L11N_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "G9")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L39P_0")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L39N_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L41P_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L41N_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "A15")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "A16")
			)
			(pin power_in line
				(at -40.64 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B5")
			)
			(pin power_in line
				(at -38.1 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B10")
			)
			(pin power_in line
				(at -35.56 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B15")
			)
			(pin power_in line
				(at -33.02 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D7")
			)
			(pin power_in line
				(at -30.48 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D13")
			)
			(pin power_in line
				(at -27.94 81.28 270)
				(length 6.35)
				(name "VCCO_0")
				(number "E10")
			)
			(pin power_in line
				(at 27.94 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "E17")
			)
			(pin power_in line
				(at 30.48 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G15")
			)
			(pin power_in line
				(at 33.02 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J14")
			)
			(pin power_in line
				(at 35.56 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J17")
			)
			(pin power_in line
				(at 38.1 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "M15")
			)
			(pin power_in line
				(at 40.64 81.28 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R17")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "C17")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "C18")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D17")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D18")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "H12")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "G13")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "E18")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "K13")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "F17")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "F18")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "G18")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "K14")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "L12")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "L13")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "L16")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "H17")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "H18")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "J18")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "K17")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "K18")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "L17")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "L18")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "M18")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "N17")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "N18")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "P17")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "P18")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "T17")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "T18")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "U17")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "U18")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "M14")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L61P_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L61N_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "P16")
			)
		)
		(symbol "XC6SLX9-CSG324_2_1"
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "R15")
			)
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "T15")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "U16")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "V16")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "R13")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "T13")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "T14")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "V14")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "P12")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "U13")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "V13")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "U11")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "V11")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "R10")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "U10")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "V10")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "R8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "T9")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "V9")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L45P_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L45N_2")
				(number "V6")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L41P_2")
				(number "U8")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L41N_VREF_2")
				(number "V8")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L43P_2")
				(number "U7")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L43N_2")
				(number "V7")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L46P_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L46N_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "R5")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "T5")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "U5")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "V5")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "R3")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "T3")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "T4")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "V4")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "P6")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "U3")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "V3")
			)
			(pin power_in line
				(at -40.64 81.28 270)
				(length 6.35)
				(name "VCCO_2")
				(number "P9")
			)
			(pin power_in line
				(at -38.1 81.28 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R6")
			)
			(pin power_in line
				(at -35.56 81.28 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R12")
			)
			(pin power_in line
				(at -33.02 81.28 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U4")
			)
			(pin power_in line
				(at -30.48 81.28 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U9")
			)
			(pin power_in line
				(at -27.94 81.28 270)
				(length 6.35)
				(name "VCCO_2")
				(number "U14")
			)
			(pin power_in line
				(at 27.94 81.28 270)
				(length 6.35)
				(name "VCCO_3")
				(number "E2")
			)
			(pin power_in line
				(at 30.48 81.28 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G4")
			)
			(pin power_in line
				(at 33.02 81.28 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J2")
			)
			(pin power_in line
				(at 35.56 81.28 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J5")
			)
			(pin power_in line
				(at 38.1 81.28 270)
				(length 6.35)
				(name "VCCO_3")
				(number "M4")
			)
			(pin power_in line
				(at 40.64 81.28 270)
				(length 6.35)
				(name "VCCO_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "P4")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "P3")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L31P_3")
				(number "L6")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L31N_VREF_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "U2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "U1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "T2")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "T1")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "K4")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "L5")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "L7")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "J7")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "H6")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "H7")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "F6")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "C1")
			)
		)
		(symbol "XC6SLX9-CSG324_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "D15")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "D16")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "B18")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "A17")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "V17")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "V2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "R16")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "P13")
			)
		)
		(symbol "XC6SLX9-CSG324_4_1"
			(pin power_in line
				(at -25.4 40.64 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B1")
			)
			(pin power_in line
				(at -25.4 38.1 0)
				(length 6.35)
				(name "VCCAUX")
				(number "B17")
			)
			(pin power_in line
				(at -25.4 35.56 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 33.02 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 30.48 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E14")
			)
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J12")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "K7")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "M9")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P5")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "VCCAUX")
				(number "P14")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A18")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "C3")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "C16")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D5")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "D10")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "E15")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "G2")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "G12")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "G17")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 6.35)
				(name "GND")
				(number "H10")
			)
			(pin power_in line
				(at -25.4 -33.02 0)
				(length 6.35)
				(name "GND")
				(number "J4")
			)
			(pin power_in line
				(at -25.4 -35.56 0)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 6.35)
				(name "GND")
				(number "J11")
			)
			(pin power_in line
				(at -25.4 -40.64 0)
				(length 6.35)
				(name "GND")
				(number "J15")
			)
			(pin power_in line
				(at 25.4 40.64 180)
				(length 6.35)
				(name "VCCINT")
				(number "G7")
			)
			(pin power_in line
				(at 25.4 38.1 180)
				(length 6.35)
				(name "VCCINT")
				(number "H9")
			)
			(pin power_in line
				(at 25.4 35.56 180)
				(length 6.35)
				(name "VCCINT")
				(number "H11")
			)
			(pin power_in line
				(at 25.4 33.02 180)
				(length 6.35)
				(name "VCCINT")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 30.48 180)
				(length 6.35)
				(name "VCCINT")
				(number "J10")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "K11")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "L8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "L10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "M7")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "M12")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "L9")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "M2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "M6")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M17")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "R1")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "R4")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R9")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "R14")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "R18")
			)
			(pin power_in line
				(at 25.4 -30.48 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 25.4 -33.02 180)
				(length 6.35)
				(name "GND")
				(number "U6")
			)
			(pin power_in line
				(at 25.4 -35.56 180)
				(length 6.35)
				(name "GND")
				(number "U12")
			)
			(pin power_in line
				(at 25.4 -38.1 180)
				(length 6.35)
				(name "GND")
				(number "V1")
			)
			(pin power_in line
				(at 25.4 -40.64 180)
				(length 6.35)
				(name "GND")
				(number "V18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX9-FTG256"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX9-FTG256"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 9 XC6SLX9-FTG256"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX9-FTG256_1_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "C4")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "A4")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "B5")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "A5")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "D5")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "C5")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "B6")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "A6")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L5P_0")
				(number "F7")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L5N_0")
				(number "E6")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L6P_0")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L6N_0")
				(number "A7")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L7P_0")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L7N_0")
				(number "C6")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L33P_0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L33N_0")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "E7")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "E8")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "E10")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "C10")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L38P_0")
				(number "D8")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L38N_VREF_0")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L39P_0")
				(number "C11")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L39N_0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L40P_0")
				(number "F9")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L40N_0")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "B12")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "A12")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "C13")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "A13")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "F10")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "E11")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "B14")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "A14")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "D11")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "D12")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B4")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B9")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "B13")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D7")
			)
			(pin power_in line
				(at -30.48 78.74 270)
				(length 6.35)
				(name "VCCO_0")
				(number "D10")
			)
			(pin power_in line
				(at 27.94 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "D15")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "G13")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "J15")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "K13")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "N15")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_1")
				(number "R13")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_A25_1")
				(number "E13")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_A24_VREF_1")
				(number "E12")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L29P_A23_M1A13_1")
				(number "B15")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L29N_A22_M1A14_1")
				(number "B16")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L30P_A21_M1RESET_1")
				(number "F12")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L30N_A20_M1A11_1")
				(number "G11")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L31P_A19_M1CKE_1")
				(number "D14")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L31N_A18_M1A12_1")
				(number "D16")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L32P_A17_M1A8_1")
				(number "F13")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L32N_A16_M1A9_1")
				(number "F14")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L33P_A15_M1A10_1")
				(number "C15")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L33N_A14_M1A4_1")
				(number "C16")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L34P_A13_M1WE_1")
				(number "E15")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L34N_A12_M1BA2_1")
				(number "E16")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L35P_A11_M1A7_1")
				(number "F15")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L35N_A10_M1A2_1")
				(number "F16")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L36P_A9_M1BA0_1")
				(number "G14")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L36N_A8_M1BA1_1")
				(number "G16")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L37P_A7_M1A0_1")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L37N_A6_M1A1_1")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L38P_A5_M1CLK_1")
				(number "G12")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L38N_A4_M1CLKN_1")
				(number "H11")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L39P_M1A3_1")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L39N_M1ODT_1")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_M1A5_1")
				(number "J11")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_M1A6_1")
				(number "J12")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_M1RASN_1")
				(number "J13")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_M1CASN_1")
				(number "K14")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_M1UDM_1")
				(number "K12")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_M1LDM_1")
				(number "K11")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_M1DQ4_1")
				(number "J14")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_M1DQ5_1")
				(number "J16")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L44P_A3_M1DQ6_1")
				(number "K15")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L44N_A2_M1DQ7_1")
				(number "K16")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L45P_A1_M1LDQS_1")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L45N_A0_M1LDQSN_1")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L46P_FCS_B_M1DQ2_1")
				(number "M15")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L46N_FOE_B_M1DQ3_1")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L47P_FWE_B_M1DQ0_1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L47N_LDC_M1DQ1_1")
				(number "L16")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L48P_HDC_M1DQ8_1")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L48N_M1DQ9_1")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L49P_M1DQ10_1")
				(number "R15")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L49N_M1DQ11_1")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L50P_M1UDQS_1")
				(number "R14")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L50N_M1UDQSN_1")
				(number "T15")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L51P_M1DQ12_1")
				(number "T14")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L51N_M1DQ13_1")
				(number "T13")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L52P_M1DQ14_1")
				(number "R12")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L52N_M1DQ15_1")
				(number "T12")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L53P_1")
				(number "L12")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L53N_VREF_1")
				(number "L13")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "M13")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "M14")
			)
		)
		(symbol "XC6SLX9-FTG256_2_1"
			(pin bidirectional line
				(at -50.8 58.42 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "R11")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "T11")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "M12")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "M11")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "P10")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "T10")
			)
			(pin bidirectional line
				(at -50.8 43.18 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "N12")
			)
			(pin bidirectional line
				(at -50.8 40.64 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "P12")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "N11")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "P11")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "N9")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "P9")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 6.35)
				(name "IO_L23P_2")
				(number "R9")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 6.35)
				(name "IO_L23N_2")
				(number "T9")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L16P_2")
				(number "L10")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L16N_VREF_2")
				(number "M10")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L29P_GCLK3_2")
				(number "M9")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L29N_GCLK2_2")
				(number "N8")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "P8")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "T8")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "M7")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L32P_GCLK29_2")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L32N_GCLK28_2")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L47P_2")
				(number "P6")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L47N_2")
				(number "T6")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "R5")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "T5")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "N5")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "P5")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "L8")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "L7")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L63P_2")
				(number "P4")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L63N_2")
				(number "T4")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "M6")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "R3")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "T3")
			)
			(pin power_in line
				(at -40.64 78.74 270)
				(length 6.35)
				(name "VCCO_2")
				(number "N7")
			)
			(pin power_in line
				(at -38.1 78.74 270)
				(length 6.35)
				(name "VCCO_2")
				(number "N10")
			)
			(pin power_in line
				(at -35.56 78.74 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R4")
			)
			(pin power_in line
				(at -33.02 78.74 270)
				(length 6.35)
				(name "VCCO_2")
				(number "R8")
			)
			(pin power_in line
				(at 30.48 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "D2")
			)
			(pin power_in line
				(at 33.02 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "G4")
			)
			(pin power_in line
				(at 35.56 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "J2")
			)
			(pin power_in line
				(at 38.1 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "K4")
			)
			(pin power_in line
				(at 40.64 78.74 270)
				(length 6.35)
				(name "VCCO_3")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "M5")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "N4")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 6.35)
				(name "IO_L32P_M3DQ14_3")
				(number "R2")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 6.35)
				(name "IO_L32N_M3DQ15_3")
				(number "R1")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 6.35)
				(name "IO_L33P_M3DQ12_3")
				(number "P2")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 6.35)
				(name "IO_L33N_M3DQ13_3")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 6.35)
				(name "IO_L34P_M3UDQS_3")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 6.35)
				(name "IO_L34N_M3UDQSN_3")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 6.35)
				(name "IO_L35P_M3DQ10_3")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 6.35)
				(name "IO_L35N_M3DQ11_3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 6.35)
				(name "IO_L36P_M3DQ8_3")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 6.35)
				(name "IO_L36N_M3DQ9_3")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L37P_M3DQ0_3")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L37N_M3DQ1_3")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L38P_M3DQ2_3")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L38N_M3DQ3_3")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L39P_M3LDQS_3")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L39N_M3LDQSN_3")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L40P_M3DQ6_3")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L40N_M3DQ7_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_M3DQ4_3")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_M3DQ5_3")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_M3UDM_3")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_M3LDM_3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_M3RASN_3")
				(number "J6")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_M3CASN_3")
				(number "H5")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_M3A5_3")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_M3A6_3")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45P_M3A3_3")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45N_M3ODT_3")
				(number "L5")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46P_M3CLK_3")
				(number "E2")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46N_M3CLKN_3")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47P_M3A0_3")
				(number "K5")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L47N_M3A1_3")
				(number "K6")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L48P_M3BA0_3")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L48N_M3BA1_3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L49P_M3A7_3")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L49N_M3A2_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 6.35)
				(name "IO_L50P_M3WE_3")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 6.35)
				(name "IO_L50N_M3BA2_3")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 6.35)
				(name "IO_L51P_M3A10_3")
				(number "G6")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 6.35)
				(name "IO_L51N_M3A4_3")
				(number "G5")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 6.35)
				(name "IO_L52P_M3A8_3")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 6.35)
				(name "IO_L52N_M3A9_3")
				(number "A2")
			)
			(pin bidirectional line
				(at 50.8 -58.42 180)
				(length 6.35)
				(name "IO_L53P_M3CKE_3")
				(number "F4")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 6.35)
				(name "IO_L53N_M3A12_3")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 6.35)
				(name "IO_L54P_M3RESET_3")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 6.35)
				(name "IO_L54N_M3A11_3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 6.35)
				(name "IO_L55P_M3A13_3")
				(number "F6")
			)
			(pin bidirectional line
				(at 50.8 -71.12 180)
				(length 6.35)
				(name "IO_L55N_M3A14_3")
				(number "F5")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "B3")
			)
			(pin bidirectional line
				(at 50.8 -76.2 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "A3")
			)
		)
		(symbol "XC6SLX9-FTG256_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "C12")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "E14")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "A15")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "C14")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "P13")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "T2")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "P14")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "L11")
			)
		)
		(symbol "XC6SLX9-FTG256_4_1"
			(pin power_in line
				(at -25.4 27.94 0)
				(length 6.35)
				(name "VCCAUX")
				(number "E5")
			)
			(pin power_in line
				(at -25.4 25.4 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F8")
			)
			(pin power_in line
				(at -25.4 22.86 0)
				(length 6.35)
				(name "VCCAUX")
				(number "F11")
			)
			(pin power_in line
				(at -25.4 20.32 0)
				(length 6.35)
				(name "VCCAUX")
				(number "G10")
			)
			(pin power_in line
				(at -25.4 17.78 0)
				(length 6.35)
				(name "VCCAUX")
				(number "H6")
			)
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "J10")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L6")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "VCCAUX")
				(number "L9")
			)
			(pin power_in line
				(at -25.4 2.54 0)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "A16")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "B11")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "D4")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "D13")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "E9")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "G2")
			)
			(pin power_in line
				(at -25.4 -17.78 0)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -25.4 -20.32 0)
				(length 6.35)
				(name "GND")
				(number "G15")
			)
			(pin power_in line
				(at -25.4 -22.86 0)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at -25.4 -27.94 0)
				(length 6.35)
				(name "GND")
				(number "H12")
			)
			(pin power_in line
				(at 25.4 27.94 180)
				(length 6.35)
				(name "VCCINT")
				(number "G7")
			)
			(pin power_in line
				(at 25.4 25.4 180)
				(length 6.35)
				(name "VCCINT")
				(number "G9")
			)
			(pin power_in line
				(at 25.4 22.86 180)
				(length 6.35)
				(name "VCCINT")
				(number "H8")
			)
			(pin power_in line
				(at 25.4 20.32 180)
				(length 6.35)
				(name "VCCINT")
				(number "H10")
			)
			(pin power_in line
				(at 25.4 17.78 180)
				(length 6.35)
				(name "VCCINT")
				(number "J7")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "J9")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "K8")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "K10")
			)
			(pin power_in line
				(at 25.4 2.54 180)
				(length 6.35)
				(name "GND")
				(number "J5")
			)
			(pin power_in line
				(at 25.4 0 180)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "L2")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "L15")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "M8")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "N13")
			)
			(pin power_in line
				(at 25.4 -17.78 180)
				(length 6.35)
				(name "GND")
				(number "P3")
			)
			(pin power_in line
				(at 25.4 -20.32 180)
				(length 6.35)
				(name "GND")
				(number "R6")
			)
			(pin power_in line
				(at 25.4 -22.86 180)
				(length 6.35)
				(name "GND")
				(number "R10")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 6.35)
				(name "GND")
				(number "T1")
			)
			(pin power_in line
				(at 25.4 -27.94 180)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XC6SLX9-TQG144"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "XC6SLX9-TQG144"
			(at 0 -1.27 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Spartan 6 LX 9 XC6SLX9-TQG144"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "FPGA"
			(at 0 0 0)
		)
		(symbol "XC6SLX9-TQG144_1_1"
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L1P_HSWAPEN_0")
				(number "144")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L1N_VREF_0")
				(number "143")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L2P_0")
				(number "142")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L2N_0")
				(number "141")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L3P_0")
				(number "140")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L3N_0")
				(number "139")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L4P_0")
				(number "138")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L4N_0")
				(number "137")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L34P_GCLK19_0")
				(number "134")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L34N_GCLK18_0")
				(number "133")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L35P_GCLK17_0")
				(number "132")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L35N_GCLK16_0")
				(number "131")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L36P_GCLK15_0")
				(number "127")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L36N_GCLK14_0")
				(number "126")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L37P_GCLK13_0")
				(number "124")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L37N_GCLK12_0")
				(number "123")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L62P_0")
				(number "121")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L62N_VREF_0")
				(number "120")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L63P_SCP7_0")
				(number "119")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L63N_SCP6_0")
				(number "118")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L64P_SCP5_0")
				(number "117")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L64N_SCP4_0")
				(number "116")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L65P_SCP3_0")
				(number "115")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L65N_SCP2_0")
				(number "114")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L66P_SCP1_0")
				(number "112")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L66N_SCP0_0")
				(number "111")
			)
			(pin power_in line
				(at -40.64 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "122")
			)
			(pin power_in line
				(at -38.1 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "125")
			)
			(pin power_in line
				(at -35.56 43.18 270)
				(length 6.35)
				(name "VCCO_0")
				(number "135")
			)
			(pin power_in line
				(at 35.56 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "76")
			)
			(pin power_in line
				(at 38.1 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "86")
			)
			(pin power_in line
				(at 40.64 43.18 270)
				(length 6.35)
				(name "VCCO_1")
				(number "103")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L1P_1")
				(number "105")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L1N_VREF_1")
				(number "104")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L32P_1")
				(number "102")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L32N_1")
				(number "101")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L33P_1")
				(number "100")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L33N_1")
				(number "99")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L34P_1")
				(number "98")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L34N_1")
				(number "97")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L40P_GCLK11_1")
				(number "95")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L40N_GCLK10_1")
				(number "94")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK9_IRDY1_1")
				(number "93")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L41N_GCLK8_1")
				(number "92")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L42P_GCLK7_1")
				(number "88")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L42N_GCLK6_TRDY1_1")
				(number "87")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L43P_GCLK5_1")
				(number "85")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L43N_GCLK4_1")
				(number "84")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L45P_1")
				(number "83")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L45N_1")
				(number "82")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L46P_1")
				(number "81")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L46N_1")
				(number "80")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L47P_1")
				(number "79")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L47N_1")
				(number "78")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L74P_AWAKE_1")
				(number "75")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L74N_DOUT_BUSY_1")
				(number "74")
			)
		)
		(symbol "XC6SLX9-TQG144_2_1"
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 6.35)
				(name "IO_L1P_CCLK_2")
				(number "70")
			)
			(pin bidirectional line
				(at -50.8 20.32 0)
				(length 6.35)
				(name "IO_L1N_M0_CMPMISO_2")
				(number "69")
			)
			(pin bidirectional line
				(at -50.8 17.78 0)
				(length 6.35)
				(name "IO_L2P_CMPCLK_2")
				(number "67")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 6.35)
				(name "IO_L2N_CMPMOSI_2")
				(number "66")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 6.35)
				(name "IO_L3P_D0_DIN_MISO_MISO1_2")
				(number "65")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 6.35)
				(name "IO_L3N_MOSI_CSI_B_MISO0_2")
				(number "64")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 6.35)
				(name "IO_L12P_D1_MISO2_2")
				(number "62")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 6.35)
				(name "IO_L12N_D2_MISO3_2")
				(number "61")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 6.35)
				(name "IO_L13P_M1_2")
				(number "60")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 6.35)
				(name "IO_L13N_D10_2")
				(number "59")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 6.35)
				(name "IO_L14P_D11_2")
				(number "58")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 6.35)
				(name "IO_L14N_D12_2")
				(number "57")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 6.35)
				(name "IO_L30P_GCLK1_D13_2")
				(number "56")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 6.35)
				(name "IO_L30N_GCLK0_USERCCLK_2")
				(number "55")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 6.35)
				(name "IO_L31P_GCLK31_D14_2")
				(number "51")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 6.35)
				(name "IO_L31N_GCLK30_D15_2")
				(number "50")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 6.35)
				(name "IO_L48P_D7_2")
				(number "48")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 6.35)
				(name "IO_L48N_RDWR_B_VREF_2")
				(number "47")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 6.35)
				(name "IO_L49P_D3_2")
				(number "46")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 6.35)
				(name "IO_L49N_D4_2")
				(number "45")
			)
			(pin bidirectional line
				(at -50.8 -27.94 0)
				(length 6.35)
				(name "IO_L62P_D5_2")
				(number "44")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 6.35)
				(name "IO_L62N_D6_2")
				(number "43")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 6.35)
				(name "IO_L64P_D8_2")
				(number "41")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 6.35)
				(name "IO_L64N_D9_2")
				(number "40")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 6.35)
				(name "IO_L65P_INIT_B_2")
				(number "39")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 6.35)
				(name "IO_L65N_CSO_B_2")
				(number "38")
			)
			(pin power_in line
				(at -40.64 43.18 270)
				(length 6.35)
				(name "VCCO_2")
				(number "42")
			)
			(pin power_in line
				(at -38.1 43.18 270)
				(length 6.35)
				(name "VCCO_2")
				(number "63")
			)
			(pin power_in line
				(at 35.56 43.18 270)
				(length 6.35)
				(name "VCCO_3")
				(number "4")
			)
			(pin power_in line
				(at 38.1 43.18 270)
				(length 6.35)
				(name "VCCO_3")
				(number "18")
			)
			(pin power_in line
				(at 40.64 43.18 270)
				(length 6.35)
				(name "VCCO_3")
				(number "31")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 6.35)
				(name "IO_L1P_3")
				(number "35")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 6.35)
				(name "IO_L1N_VREF_3")
				(number "34")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 6.35)
				(name "IO_L2P_3")
				(number "33")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 6.35)
				(name "IO_L2N_3")
				(number "32")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 6.35)
				(name "IO_L36P_3")
				(number "30")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 6.35)
				(name "IO_L36N_3")
				(number "29")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 6.35)
				(name "IO_L37P_3")
				(number "27")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 6.35)
				(name "IO_L37N_3")
				(number "26")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 6.35)
				(name "IO_L41P_GCLK27_3")
				(number "24")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 6.35)
				(name "IO_L41N_GCLK26_3")
				(number "23")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 6.35)
				(name "IO_L42P_GCLK25_TRDY2_3")
				(number "22")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 6.35)
				(name "IO_L42N_GCLK24_3")
				(number "21")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 6.35)
				(name "IO_L43P_GCLK23_3")
				(number "17")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 6.35)
				(name "IO_L43N_GCLK22_IRDY2_3")
				(number "16")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 6.35)
				(name "IO_L44P_GCLK21_3")
				(number "15")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 6.35)
				(name "IO_L44N_GCLK20_3")
				(number "14")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 6.35)
				(name "IO_L49P_3")
				(number "12")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 6.35)
				(name "IO_L49N_3")
				(number "11")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 6.35)
				(name "IO_L50P_3")
				(number "10")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 6.35)
				(name "IO_L50N_3")
				(number "9")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 6.35)
				(name "IO_L51P_3")
				(number "8")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 6.35)
				(name "IO_L51N_3")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 6.35)
				(name "IO_L52P_3")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 6.35)
				(name "IO_L52N_3")
				(number "5")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 6.35)
				(name "IO_L83P_3")
				(number "2")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 6.35)
				(name "IO_L83N_VREF_3")
				(number "1")
			)
		)
		(symbol "XC6SLX9-TQG144_3_1"
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 6.35)
				(name "TDI")
				(number "110")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 6.35)
				(name "TDO")
				(number "106")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 6.35)
				(name "TMS")
				(number "107")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 6.35)
				(name "TCK")
				(number "109")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 6.35)
				(name "DONE_2")
				(number "71")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 6.35)
				(name "PROGRAM_B_2")
				(number "37")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 6.35)
				(name "SUSPEND")
				(number "73")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 6.35)
				(name "CMPCS_B_2")
				(number "72")
			)
		)
		(symbol "XC6SLX9-TQG144_4_1"
			(pin power_in line
				(at -25.4 15.24 0)
				(length 6.35)
				(name "VCCAUX")
				(number "20")
			)
			(pin power_in line
				(at -25.4 12.7 0)
				(length 6.35)
				(name "VCCAUX")
				(number "36")
			)
			(pin power_in line
				(at -25.4 10.16 0)
				(length 6.35)
				(name "VCCAUX")
				(number "53")
			)
			(pin power_in line
				(at -25.4 7.62 0)
				(length 6.35)
				(name "VCCAUX")
				(number "90")
			)
			(pin power_in line
				(at -25.4 5.08 0)
				(length 6.35)
				(name "VCCAUX")
				(number "129")
			)
			(pin power_in line
				(at -25.4 0 0)
				(length 6.35)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at -25.4 -2.54 0)
				(length 6.35)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at -25.4 -5.08 0)
				(length 6.35)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at -25.4 -7.62 0)
				(length 6.35)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at -25.4 -10.16 0)
				(length 6.35)
				(name "GND")
				(number "54")
			)
			(pin power_in line
				(at -25.4 -12.7 0)
				(length 6.35)
				(name "GND")
				(number "68")
			)
			(pin power_in line
				(at -25.4 -15.24 0)
				(length 6.35)
				(name "GND")
				(number "77")
			)
			(pin power_in line
				(at 25.4 15.24 180)
				(length 6.35)
				(name "VCCINT")
				(number "19")
			)
			(pin power_in line
				(at 25.4 12.7 180)
				(length 6.35)
				(name "VCCINT")
				(number "28")
			)
			(pin power_in line
				(at 25.4 10.16 180)
				(length 6.35)
				(name "VCCINT")
				(number "52")
			)
			(pin power_in line
				(at 25.4 7.62 180)
				(length 6.35)
				(name "VCCINT")
				(number "89")
			)
			(pin power_in line
				(at 25.4 5.08 180)
				(length 6.35)
				(name "VCCINT")
				(number "128")
			)
			(pin power_in line
				(at 25.4 -2.54 180)
				(length 6.35)
				(name "GND")
				(number "91")
			)
			(pin power_in line
				(at 25.4 -5.08 180)
				(length 6.35)
				(name "GND")
				(number "96")
			)
			(pin power_in line
				(at 25.4 -7.62 180)
				(length 6.35)
				(name "GND")
				(number "108")
			)
			(pin power_in line
				(at 25.4 -10.16 180)
				(length 6.35)
				(name "GND")
				(number "113")
			)
			(pin power_in line
				(at 25.4 -12.7 180)
				(length 6.35)
				(name "GND")
				(number "130")
			)
			(pin power_in line
				(at 25.4 -15.24 180)
				(length 6.35)
				(name "GND")
				(number "136")
			)
		)
		(embedded_fonts no)
	)
)
