(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AFBR-1624Z"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -7.62 8.89 0)
		)
		(property "Value" "AFBR-1624Z"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-4369EN"
			(at 5.08 0 0)
		)
		(property "Description" "Versatile Link Fiber Optic Transmitter"
			(at 0 0 0)
		)
		(property "ki_keywords" "Fiber optic transmitter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Broadcom*AFBR*16xxZ*"
			(at 0 0 0)
		)
		(symbol "AFBR-1624Z_0_0"
			(text "TX"
				(at 5.08 0 0)
			)
		)
		(symbol "AFBR-1624Z_0_1")
		(symbol "AFBR-1624Z_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "Data_in")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "HP")
				(number "5")
			)
			(pin passive line
				(at -2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "HP")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCCT")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VEET")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AFBR-2624Z"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -6.35 8.89 0)
		)
		(property "Value" "AFBR-2624Z"
			(at 1.27 8.89 0)
		)
		(property "Footprint" ""
			(at -2.54 -12.7 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-4369EN"
			(at -2.54 0 0)
		)
		(property "Description" "Versatile Link Fiber Optic Receiver"
			(at 0 0 0)
		)
		(property "ki_keywords" "fiber optic receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Broadcom*AFBR*16xxZ*"
			(at 0 0 0)
		)
		(symbol "AFBR-2624Z_0_1")
		(symbol "AFBR-2624Z_1_1"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCCR")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VEER")
				(number "2")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "HP")
				(number "5")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "HP")
				(number "8")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Data_Out")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
)
