(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "0850BM14E0016"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at -6.35 -6.35 0)
		)
		(property "Value" "0850BM14E0016"
			(at 0 6.35 0)
		)
		(property "Footprint" "RF_Converter:Balun_Johanson_1.6x0.8mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.johansontechnology.com/datasheets/0850BM14E0016/0850BM14E0016.pdf"
			(at -24.13 15.24 0)
		)
		(property "Description" "Sub-GHz Impedance Matched Balun + LPF integrated Passive"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sub-GHz Balun"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Balun*Johanson*1.6x0.8mm*"
			(at 0 0 0)
		)
		(symbol "0850BM14E0016_0_0"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RF_P")
				(number "4")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "RF_N")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RX/TX")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "UBP")
				(number "1")
			)
		)
		(symbol "0850BM14E0016_0_1")
		(embedded_fonts no)
	)
	(symbol "0900FM15K0039"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at -6.35 -6.35 0)
		)
		(property "Value" "0900FM15K0039"
			(at 0 6.35 0)
		)
		(property "Footprint" "RF_Converter:Balun_Johanson_0900FM15K0039"
			(at 0 -9.525 0)
		)
		(property "Datasheet" "https://www.johansontechnology.com/datasheets/0900FM15K0039/0900FM15K0039.pdf"
			(at 0.635 -11.43 0)
		)
		(property "Description" "868MHz/915MHz Sub-GHz Impedance Matched Filter integrated passive for Semtech SX1261, SX1262, LLCC68"
			(at 0 0 0)
		)
		(property "ki_keywords" "Sub-GHz filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Balun*Johanson*0900FM15K0039*"
			(at 0 0 0)
		)
		(symbol "0900FM15K0039_0_0"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RFO")
				(number "1")
			)
			(pin passive line
				(at -10.16 0 0)
				(length 2.54)
				(name "RFI_N")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "RFI_P")
				(number "4")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SW_RFO")
				(number "8")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "SW_RFI")
				(number "6")
			)
		)
		(symbol "0900FM15K0039_0_1")
		(embedded_fonts no)
	)
	(symbol "1FP45-0R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "1FP45-0R"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_FILTERCON_1FPxx"
			(at 0 0 0)
		)
		(property "Datasheet" "https://filtercon.com.pl/wp-content/uploads/2019/07/Karta-katalogowa-FP-12-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.5A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*FILTERCON*1FPxx*"
			(at 0 0 0)
		)
		(symbol "1FP45-0R_1_1"
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "P")
				(number "1")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "N")
				(number "3")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "P'")
				(number "2")
			)
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "N'")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "B39162B8813P810"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 2.54 -6.35 0)
		)
		(property "Value" "B39162B8813P810"
			(at 0 6.35 0)
		)
		(property "Footprint" "Filter:Filter_1109-5_1.1x0.9mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://product.tdk.com/search-template/en/documents/data_sheet/40/ds/mc/B9482.pdf"
			(at -1.778 0.762 0)
		)
		(property "Description" "1582.47MHz SAW filter, SMD 1109"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*1109*1.1x0.9mm*"
			(at 0 0 0)
		)
		(symbol "B39162B8813P810_0_1")
		(symbol "B39162B8813P810_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BNX025"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at -6.35 5.08 0)
		)
		(property "Value" "BNX025"
			(at 7.62 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Murata_BNX025"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.murata.com/en-us/products/productdetail.aspx?cate=luNoiseSupprFilteBlockType&partno=BNX025H01%23"
			(at -0.635 -0.635 90)
		)
		(property "Description" "EMI Filter SMD, Murata BNX025"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI Filter SMD Murata"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Murata*BNX025*"
			(at 0 0 0)
		)
		(symbol "BNX025_0_1")
		(symbol "BNX025_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "PSG")
				(number "3")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "CB")
				(number "2")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CG")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Choke_CommonMode_FerriteCore_1234"
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 4.445 0)
		)
		(property "Value" "Choke_CommonMode_FerriteCore_1234"
			(at 0 -4.445 0)
		)
		(property "Footprint" ""
			(at 0 -6.35 0)
		)
		(property "Datasheet" "~"
			(at 0 -8.255 0)
		)
		(property "Description" "Generic common-mode choke, ferrite core, 1234 pin order"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal line filter"
			(at 0 0 0)
		)
		(symbol "Choke_CommonMode_FerriteCore_1234_0_1")
		(symbol "Choke_CommonMode_FerriteCore_1234_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Choke_CommonMode_FerriteCore_1243"
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 4.445 0)
		)
		(property "Value" "Choke_CommonMode_FerriteCore_1243"
			(at 0 -4.445 0)
		)
		(property "Footprint" ""
			(at 0 -6.35 0)
		)
		(property "Datasheet" "~"
			(at 0 -8.255 0)
		)
		(property "Description" "Generic common-mode choke, ferrite core, 1243 pin order"
			(at 4.064 -0.762 0)
		)
		(property "ki_keywords" "signal line filter"
			(at 0 0 0)
		)
		(symbol "Choke_CommonMode_FerriteCore_1243_0_1")
		(symbol "Choke_CommonMode_FerriteCore_1243_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Choke_CommonMode_FerriteCore_1324"
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 4.445 0)
		)
		(property "Value" "Choke_CommonMode_FerriteCore_1324"
			(at 0 -4.445 0)
		)
		(property "Footprint" ""
			(at 0 -6.35 0)
		)
		(property "Datasheet" "~"
			(at 0 -8.255 0)
		)
		(property "Description" "Generic common-mode choke, ferrite core, 1324 pin order"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal line filter"
			(at 0 0 0)
		)
		(symbol "Choke_CommonMode_FerriteCore_1324_0_1")
		(symbol "Choke_CommonMode_FerriteCore_1324_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Choke_CommonMode_FerriteCore_1342"
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 4.445 0)
		)
		(property "Value" "Choke_CommonMode_FerriteCore_1342"
			(at 0 -4.445 0)
		)
		(property "Footprint" ""
			(at 0 -6.35 0)
		)
		(property "Datasheet" "~"
			(at 0 -8.255 0)
		)
		(property "Description" "Generic common-mode choke, ferrite core, 1342 pin order"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal line filter"
			(at 0 0 0)
		)
		(symbol "Choke_CommonMode_FerriteCore_1342_0_1")
		(symbol "Choke_CommonMode_FerriteCore_1342_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Choke_CommonMode_FerriteCore_1423"
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 4.445 0)
		)
		(property "Value" "Choke_CommonMode_FerriteCore_1423"
			(at 0 -4.445 0)
		)
		(property "Footprint" ""
			(at 0 -6.35 0)
		)
		(property "Datasheet" "~"
			(at 0 -8.255 0)
		)
		(property "Description" "Generic common-mode choke, ferrite core, 1423 pin order"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal line filter"
			(at 0 0 0)
		)
		(symbol "Choke_CommonMode_FerriteCore_1423_0_1")
		(symbol "Choke_CommonMode_FerriteCore_1423_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Choke_CommonMode_PulseElectronics_PH9455x105NL"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_CommonMode_PulseElectronics_PH9455x105NL"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:L_CommonMode_PulseElectronics_PH9455x105NL_1"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseelectronics.com/api/open/product-attachments/datasheet/ph9455.105nl"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 22A, 380VAC, 1mH, 2.1 mOhm, PH9455x105NL"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonMode*PulseElectronics*PH9455x105NL?1*"
			(at 0 0 0)
		)
		(symbol "Choke_CommonMode_PulseElectronics_PH9455x105NL_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Choke_Schaffner_RN102-0.3-02-22M"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_Schaffner_RN102-0.3-02-22M"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:Choke_Schaffner_RN102-04-14.0x14.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/rn-series-common-mode-chokes-new/"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 300mA, 300VAC, 22mH, 1.3 ohm, RN-102"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Choke*Schaffner*RN102*"
			(at 0 0 0)
		)
		(symbol "Choke_Schaffner_RN102-0.3-02-22M_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "4")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Choke_Wurth_WE-CNSW_744232090"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "L"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_Wurth_WE-CNSW_744232090"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_SMD:L_CommonMode_Wurth_WE-CNSW-1206"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.we-online.com/components/products/datasheet/744232090.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "Common mode choke, 370 mA, 125VDC, USB2.0, 111 nH"
			(at 0 0 0)
		)
		(property "ki_keywords" "common mode choke emi usb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonMode*Wurth*WE*CNSW*1206*"
			(at 0 0 0)
		)
		(symbol "Choke_Wurth_WE-CNSW_744232090_1_1"
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "")
				(number "1")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "")
				(number "4")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "")
				(number "2")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FN405-0.5-02"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN405-0.5-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN405"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/de/produkte/download/product/datasheet/fn-405-pcb-mounting-filter/"
			(at 2.54 0 0)
		)
		(property "Description" "0.5A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN405*"
			(at 0 0 0)
		)
		(symbol "FN405-0.5-02_0_1")
		(symbol "FN405-0.5-02_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "P")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "N")
				(number "1")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "P'")
				(number "4")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "E")
				(number "3")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "N'")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FN406-0.5-02"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN406-0.5-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN406"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/fn-406-ultra-compact-emc-filter/"
			(at 0 0 0)
		)
		(property "Description" "0.5A ultra compact EMI Filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI mains"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN406*"
			(at 0 0 0)
		)
		(symbol "FN406-0.5-02_0_1")
		(symbol "FN406-0.5-02_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "P")
				(number "1")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "PE")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "N")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "P'")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "N'")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1562xxG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 17.78 0)
		)
		(property "Value" "LTC1562xxG"
			(at 7.62 17.78 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1562fa.pdf"
			(at 5.08 -20.32 0)
		)
		(property "Description" "Active RC Quad Universal Filter, 10kHz to 150kHz, Low Noise, Low Distortion, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "filter opamp quad"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC1562xxG_0_1")
		(symbol "LTC1562xxG_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INV_B")
				(number "1")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "V1_B")
				(number "2")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "V2_B")
				(number "3")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "V2_A")
				(number "8")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "V1_A")
				(number "9")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "INV_A")
				(number "10")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "SHDN")
				(number "6")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "V+")
				(number "5")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "V-")
				(number "16")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "17")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "4")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "V-")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "AGND")
				(number "15")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "INV_C")
				(number "20")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "V1_C")
				(number "19")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V2_C")
				(number "18")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "V2_D")
				(number "13")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "V1_D")
				(number "12")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "INV_D")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "P300PL104M275xC222"
		(pin_names
			(offset 0.254)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 0 7.366 0)
		)
		(property "Value" "P300PL104M275xC222"
			(at 0 5.334 0)
		)
		(property "Footprint" "Filter:Filter_KEMET_PZB300_24.0x12.5mm_P10.0mm"
			(at 2.286 4.699 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_F3019_PZB300X2_2XY2_275.pdf"
			(at -0.254 2.032 0)
		)
		(property "Description" "EMI suppression capacitor PZB300 series, metallized paper, X2 and Y2 classes, 275 VAC, Cx 0.10uF, Cy 2.2nF, legacy P/N: PZB300MC11xxx"
			(at 0 2.032 0)
		)
		(property "ki_keywords" "suppressor filter cap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*PZB300*"
			(at 0 0 0)
		)
		(symbol "P300PL104M275xC222_0_1")
		(symbol "P300PL104M275xC222_1_1"
			(text "Cy"
				(at -1.778 1.016 0)
			)
			(text "Cx"
				(at 1.524 3.302 0)
			)
			(text "Cy"
				(at 1.778 1.016 0)
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "1")
				(number "1")
			)
			(pin passive line
				(at 0 -2.54 90)
				(length 2.54)
				(name "3")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "2")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SF14-1575F5UUA1"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "FL"
			(at 2.54 -6.35 0)
		)
		(property "Value" "SF14-1575F5UUA1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Filter:Filter_1411-5_1.4x1.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://global.kyocera.com/prdct/electro/product/pdf/sf14_gnss.pdf"
			(at 0 0 0)
		)
		(property "Description" "1575MHz SAW filter, SMD 1411"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*1411*1.4x1.1mm*"
			(at 0 0 0)
		)
		(symbol "SF14-1575F5UUA1_0_1")
		(symbol "SF14-1575F5UUA1_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "0603USB-142"
		(extends "Choke_CommonMode_FerriteCore_1243")
		(property "Reference" "FL"
			(at 0 4.445 0)
		)
		(property "Value" "0603USB-142"
			(at 0 -4.445 0)
		)
		(property "Footprint" "Inductor_SMD:L_CommonModeChoke_Coilcraft_0603USB"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.coilcraft.com/pdfs/0603usb.pdf"
			(at 0 -8.255 0)
		)
		(property "Description" "Coilcraft common mode choke, 500mA, 250VAC, 98nH, 174mohm, 1.9Ghz"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonModeChoke*Coilcraft*0603USB*"
			(at 0 0 0)
		)
	)
	(symbol "0603USB-222"
		(extends "Choke_CommonMode_FerriteCore_1243")
		(property "Reference" "FL"
			(at 0 4.445 0)
		)
		(property "Value" "0603USB-222"
			(at 0 -4.445 0)
		)
		(property "Footprint" "Inductor_SMD:L_CommonModeChoke_Coilcraft_0603USB"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.coilcraft.com/pdfs/0603usb.pdf"
			(at 0 -8.255 0)
		)
		(property "Description" "Coilcraft common mode choke, 500mA, 250VAC, 150nH, 209mohm, 0.96Ghz"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonModeChoke*Coilcraft*0603USB*"
			(at 0 0 0)
		)
	)
	(symbol "0603USB-251"
		(extends "Choke_CommonMode_FerriteCore_1243")
		(property "Reference" "FL"
			(at 0 4.445 0)
		)
		(property "Value" "0603USB-251"
			(at 0 -4.445 0)
		)
		(property "Footprint" "Inductor_SMD:L_CommonModeChoke_Coilcraft_0603USB"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.coilcraft.com/pdfs/0603usb.pdf"
			(at 0 -8.255 0)
		)
		(property "Description" "Coilcraft common mode choke, 500mA, 250VAC, 18nH, 77 mohm, 3.8Ghz"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonModeChoke*Coilcraft*0603USB*"
			(at 0 0 0)
		)
	)
	(symbol "0603USB-601"
		(extends "Choke_CommonMode_FerriteCore_1243")
		(property "Reference" "FL"
			(at 0 4.445 0)
		)
		(property "Value" "0603USB-601"
			(at 0 -4.445 0)
		)
		(property "Footprint" "Inductor_SMD:L_CommonModeChoke_Coilcraft_0603USB"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.coilcraft.com/pdfs/0603usb.pdf"
			(at 0 -8.255 0)
		)
		(property "Description" "Coilcraft common mode choke, 500mA, 250VAC, 37nH, 109mohm, 3.4Ghz"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonModeChoke*Coilcraft*0603USB*"
			(at 0 0 0)
		)
	)
	(symbol "0603USB-951"
		(extends "Choke_CommonMode_FerriteCore_1243")
		(property "Reference" "FL"
			(at 0 4.445 0)
		)
		(property "Value" "0603USB-951"
			(at 0 -4.445 0)
		)
		(property "Footprint" "Inductor_SMD:L_CommonModeChoke_Coilcraft_0603USB"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.coilcraft.com/pdfs/0603usb.pdf"
			(at 0 -8.255 0)
		)
		(property "Description" "Coilcraft common mode choke, 500mA, 250VAC, 63nH, 142mohm, 2.8Ghz"
			(at 0 0 0)
		)
		(property "ki_keywords" "signal line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonModeChoke*Coilcraft*0603USB*"
			(at 0 0 0)
		)
	)
	(symbol "1FP41-4R"
		(extends "1FP45-0R")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "1FP41-4R"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_FILTERCON_1FPxx"
			(at 0 0 0)
		)
		(property "Datasheet" "https://filtercon.com.pl/wp-content/uploads/2019/07/Karta-katalogowa-FP-12-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*FILTERCON*1FPxx*"
			(at 0 0 0)
		)
	)
	(symbol "1FP42-3R"
		(extends "1FP45-0R")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "1FP42-3R"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_FILTERCON_1FPxx"
			(at 0 0 0)
		)
		(property "Datasheet" "https://filtercon.com.pl/wp-content/uploads/2019/07/Karta-katalogowa-FP-12-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*FILTERCON*1FPxx*"
			(at 0 0 0)
		)
	)
	(symbol "1FP44-2R"
		(extends "1FP45-0R")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "1FP44-2R"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_FILTERCON_1FPxx"
			(at 0 0 0)
		)
		(property "Datasheet" "https://filtercon.com.pl/wp-content/uploads/2019/07/Karta-katalogowa-FP-12-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*FILTERCON*1FPxx*"
			(at 0 0 0)
		)
	)
	(symbol "1FP45-1R"
		(extends "1FP45-0R")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "1FP45-1R"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_FILTERCON_1FPxx"
			(at 0 0 0)
		)
		(property "Datasheet" "https://filtercon.com.pl/wp-content/uploads/2019/07/Karta-katalogowa-FP-12-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*FILTERCON*1FPxx*"
			(at 0 0 0)
		)
	)
	(symbol "1FP61-4R"
		(extends "1FP45-0R")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "1FP61-4R"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_FILTERCON_1FPxx"
			(at 0 0 0)
		)
		(property "Datasheet" "https://filtercon.com.pl/wp-content/uploads/2019/07/Karta-katalogowa-FP-12-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "4A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*FILTERCON*1FPxx*"
			(at 0 0 0)
		)
	)
	(symbol "1FP62-3R"
		(extends "1FP45-0R")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "1FP62-3R"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_FILTERCON_1FPxx"
			(at 0 0 0)
		)
		(property "Datasheet" "https://filtercon.com.pl/wp-content/uploads/2019/07/Karta-katalogowa-FP-12-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "3A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*FILTERCON*1FPxx*"
			(at 0 0 0)
		)
	)
	(symbol "1FP64-2R"
		(extends "1FP45-0R")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "1FP64-2R"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_FILTERCON_1FPxx"
			(at 0 0 0)
		)
		(property "Datasheet" "https://filtercon.com.pl/wp-content/uploads/2019/07/Karta-katalogowa-FP-12-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "2A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*FILTERCON*1FPxx*"
			(at 0 0 0)
		)
	)
	(symbol "1FP65-0R"
		(extends "1FP45-0R")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "1FP65-0R"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_FILTERCON_1FPxx"
			(at 0 0 0)
		)
		(property "Datasheet" "https://filtercon.com.pl/wp-content/uploads/2019/07/Karta-katalogowa-FP-12-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "0.5A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*FILTERCON*1FPxx*"
			(at 0 0 0)
		)
	)
	(symbol "1FP65-1R"
		(extends "1FP45-0R")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "1FP65-1R"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_FILTERCON_1FPxx"
			(at 0 0 0)
		)
		(property "Datasheet" "https://filtercon.com.pl/wp-content/uploads/2019/07/Karta-katalogowa-FP-12-1.pdf"
			(at 0 0 0)
		)
		(property "Description" "1A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*FILTERCON*1FPxx*"
			(at 0 0 0)
		)
	)
	(symbol "Choke_CommonMode_PulseElectronics_PH9455x155NL"
		(extends "Choke_CommonMode_PulseElectronics_PH9455x105NL")
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_CommonMode_PulseElectronics_PH9455x155NL"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:L_CommonMode_PulseElectronics_PH9455x155NL_1"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseelectronics.com/api/open/product-attachments/datasheet/ph9455.105nl"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 19A, 380VAC, 1.62mH, 3.2 mOhm, PH9455x155NL"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonMode*PulseElectronics*PH9455x155NL?1*"
			(at 0 0 0)
		)
	)
	(symbol "Choke_CommonMode_PulseElectronics_PH9455x156NL"
		(extends "Choke_CommonMode_PulseElectronics_PH9455x105NL")
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_CommonMode_PulseElectronics_PH9455x156NL"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:L_CommonMode_PulseElectronics_PH9455xxx6NL_2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseelectronics.com/api/open/product-attachments/datasheet/ph9455.105nl"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 6A, 380VAC, 15mH, 30 mOhm, PH9455x156NL"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonMode*PulseElectronics*PH9455xxx6NL?2*"
			(at 0 0 0)
		)
	)
	(symbol "Choke_CommonMode_PulseElectronics_PH9455x205NL"
		(extends "Choke_CommonMode_PulseElectronics_PH9455x105NL")
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_CommonMode_PulseElectronics_PH9455x205NL"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:L_CommonMode_PulseElectronics_PH9455x205NL_1"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseelectronics.com/api/open/product-attachments/datasheet/ph9455.105nl"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 16A, 380VAC, 2.2mH, 4.5 mOhm, PH9455x205NL"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonMode*PulseElectronics*PH9455x205NL?1*"
			(at 0 0 0)
		)
	)
	(symbol "Choke_CommonMode_PulseElectronics_PH9455x356NL"
		(extends "Choke_CommonMode_PulseElectronics_PH9455x105NL")
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_CommonMode_PulseElectronics_PH9455x356NL"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:L_CommonMode_PulseElectronics_PH9455xxx6NL_2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseelectronics.com/api/open/product-attachments/datasheet/ph9455.105nl"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 4A, 380VAC, 35mH, 80 mOhm, PH9455x356NL"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonMode*PulseElectronics*PH9455xxx6NL?2*"
			(at 0 0 0)
		)
	)
	(symbol "Choke_CommonMode_PulseElectronics_PH9455x405NL"
		(extends "Choke_CommonMode_PulseElectronics_PH9455x105NL")
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_CommonMode_PulseElectronics_PH9455x405NL"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:L_CommonMode_PulseElectronics_PH9455x405NL_1"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseelectronics.com/api/open/product-attachments/datasheet/ph9455.105nl"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 12A, 380VAC, 4.5mH, 8.5 mOhm, PH9455x405NL"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonMode*PulseElectronics*PH9455x405NL?1*"
			(at 0 0 0)
		)
	)
	(symbol "Choke_CommonMode_PulseElectronics_PH9455x705NL"
		(extends "Choke_CommonMode_PulseElectronics_PH9455x105NL")
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_CommonMode_PulseElectronics_PH9455x705NL"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:L_CommonMode_PulseElectronics_PH9455x705NL_1"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseelectronics.com/api/open/product-attachments/datasheet/ph9455.105nl"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 9A, 380VAC, 6.5mH, 14 mOhm, PH9455x705NL"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonMode*PulseElectronics*PH9455x705NL?1*"
			(at 0 0 0)
		)
	)
	(symbol "Choke_CommonMode_PulseElectronics_PH9455x826NL"
		(extends "Choke_CommonMode_PulseElectronics_PH9455x105NL")
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_CommonMode_PulseElectronics_PH9455x826NL"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:L_CommonMode_PulseElectronics_PH9455xxx6NL_2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://productfinder.pulseelectronics.com/api/open/product-attachments/datasheet/ph9455.105nl"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 3A, 380VAC, 82mH, 150 mOhm, PH9455x826NL"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "L*CommonMode*PulseElectronics*PH9455xxx6NL?2*"
			(at 0 0 0)
		)
	)
	(symbol "Choke_Schaffner_RN102-0.3-02-12M"
		(extends "Choke_Schaffner_RN102-0.3-02-22M")
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_Schaffner_RN102-0.3-02-12M"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:Choke_Schaffner_RN102-04-14.0x14.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/rn-series-common-mode-chokes-new/"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 300mA, 300VAC, 12mH, 1.1 ohm, RN-102"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Choke*Schaffner*RN102*"
			(at 0 0 0)
		)
	)
	(symbol "Choke_Schaffner_RN102-0.6-02-4M4"
		(extends "Choke_Schaffner_RN102-0.3-02-22M")
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_Schaffner_RN102-0.6-02-4M4"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:Choke_Schaffner_RN102-04-14.0x14.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/rn-series-common-mode-chokes-new/"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 600mA, 300VAC, 4.4mH, 380mohm, RN-102"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Choke*Schaffner*RN102*"
			(at 0 0 0)
		)
	)
	(symbol "Choke_Schaffner_RN102-1-02-3M0"
		(extends "Choke_Schaffner_RN102-0.3-02-22M")
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_Schaffner_RN102-1-02-3M0"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:Choke_Schaffner_RN102-04-14.0x14.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/rn-series-common-mode-chokes-new/"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 1A, 300VAC, 3mH, 210mohm, RN-102"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Choke*Schaffner*RN102*"
			(at 0 0 0)
		)
	)
	(symbol "Choke_Schaffner_RN102-1.5-02-1M6"
		(extends "Choke_Schaffner_RN102-0.3-02-22M")
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_Schaffner_RN102-1.5-02-1M6"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:Choke_Schaffner_RN102-04-14.0x14.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/rn-series-common-mode-chokes-new/"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 1.5A, 300VAC, 1.6mH, 94mohm, RN-102"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Choke*Schaffner*RN102*"
			(at 0 0 0)
		)
	)
	(symbol "Choke_Schaffner_RN102-2-02-1M1"
		(extends "Choke_Schaffner_RN102-0.3-02-22M")
		(property "Reference" "FL"
			(at 0 5.08 0)
		)
		(property "Value" "Choke_Schaffner_RN102-2-02-1M1"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Inductor_THT:Choke_Schaffner_RN102-04-14.0x14.0mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/rn-series-common-mode-chokes-new/"
			(at 0 0 0)
		)
		(property "Description" "Common mode choke, 2A, 300VAC, 1.1mH, 70mohm, RN-102"
			(at 0 0 0)
		)
		(property "ki_keywords" "common-mode common mode choke powerline power line filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Choke*Schaffner*RN102*"
			(at 0 0 0)
		)
	)
	(symbol "FN405-1-02"
		(extends "FN405-0.5-02")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN405-1-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN405"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/de/produkte/download/product/datasheet/fn-405-pcb-mounting-filter/"
			(at 2.54 0 0)
		)
		(property "Description" "1A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN405*"
			(at 0 0 0)
		)
	)
	(symbol "FN405-10-02"
		(extends "FN405-0.5-02")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN405-10-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN405"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/de/produkte/download/product/datasheet/fn-405-pcb-mounting-filter/"
			(at 2.54 0 0)
		)
		(property "Description" "10A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN405*"
			(at 0 0 0)
		)
	)
	(symbol "FN405-3-02"
		(extends "FN405-0.5-02")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN405-3-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN405"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/de/produkte/download/product/datasheet/fn-405-pcb-mounting-filter/"
			(at 2.54 0 0)
		)
		(property "Description" "3A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN405*"
			(at 0 0 0)
		)
	)
	(symbol "FN405-6-02"
		(extends "FN405-0.5-02")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN405-6-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN405"
			(at 2.54 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/de/produkte/download/product/datasheet/fn-405-pcb-mounting-filter/"
			(at 2.54 0 0)
		)
		(property "Description" "6A, 250VAC, 50/60Hz line filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN405*"
			(at 0 0 0)
		)
	)
	(symbol "FN406-1-02"
		(extends "FN406-0.5-02")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN406-1-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN406"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/fn-406-ultra-compact-emc-filter/"
			(at 0 0 0)
		)
		(property "Description" "1A ultra compact EMI Filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI mains"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN406*"
			(at 0 0 0)
		)
	)
	(symbol "FN406-3-02"
		(extends "FN406-0.5-02")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN406-3-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN406"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/fn-406-ultra-compact-emc-filter/"
			(at 0 0 0)
		)
		(property "Description" "3A ultra compact EMI Filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI mains"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN406*"
			(at 0 0 0)
		)
	)
	(symbol "FN406-6-02"
		(extends "FN406-0.5-02")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN406-6-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN406"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/fn-406-ultra-compact-emc-filter/"
			(at 0 0 0)
		)
		(property "Description" "6A ultra compact EMI Filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI mains"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN406*"
			(at 0 0 0)
		)
	)
	(symbol "FN406-8.4-02"
		(extends "FN406-0.5-02")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN406-8.4-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN406"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/fn-406-ultra-compact-emc-filter/"
			(at 0 0 0)
		)
		(property "Description" "8.4A ultra compact EMI Filter"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI mains"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN406*"
			(at 0 0 0)
		)
	)
	(symbol "FN406B-0.5-02"
		(extends "FN406-0.5-02")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN406B-0.5-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN406"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/fn-406-ultra-compact-emc-filter/"
			(at 0 0 0)
		)
		(property "Description" "0.5A ultra compact EMI Filter, medical version"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI mains"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN406*"
			(at 0 0 0)
		)
	)
	(symbol "FN406B-1-02"
		(extends "FN406-0.5-02")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN406B-1-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN406"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/fn-406-ultra-compact-emc-filter/"
			(at 0 0 0)
		)
		(property "Description" "1A ultra compact EMI Filter, medical version"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI mains"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN406*"
			(at 0 0 0)
		)
	)
	(symbol "FN406B-3-02"
		(extends "FN406-0.5-02")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN406B-3-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN406"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/fn-406-ultra-compact-emc-filter/"
			(at 0 0 0)
		)
		(property "Description" "3A ultra compact EMI Filter, medical version"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI mains"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN406*"
			(at 0 0 0)
		)
	)
	(symbol "FN406B-6-02"
		(extends "FN406-0.5-02")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN406B-6-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN406"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/fn-406-ultra-compact-emc-filter/"
			(at 0 0 0)
		)
		(property "Description" "6A ultra compact EMI Filter, medical version"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI mains"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN406*"
			(at 0 0 0)
		)
	)
	(symbol "FN406B-8.4-02"
		(extends "FN406-0.5-02")
		(property "Reference" "FL"
			(at 0 7.62 0)
		)
		(property "Value" "FN406B-8.4-02"
			(at 0 5.08 0)
		)
		(property "Footprint" "Filter:Filter_Schaffner_FN406"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.schaffner.com/products/download/product/datasheet/fn-406-ultra-compact-emc-filter/"
			(at 0 0 0)
		)
		(property "Description" "8.4A ultra compact EMI Filter, medical version"
			(at 0 0 0)
		)
		(property "ki_keywords" "EMI mains"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*Schaffner*FN406*"
			(at 0 0 0)
		)
	)
	(symbol "LTC1562xG-2"
		(extends "LTC1562xxG")
		(property "Reference" "U"
			(at -7.62 17.78 0)
		)
		(property "Value" "LTC1562xG-2"
			(at 7.62 17.78 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/15622fa.pdf"
			(at 5.08 -20.32 0)
		)
		(property "Description" "Active RC Quad Universal Filter, 20kHz to 300kHz, Low Noise, Low Distortion, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "filter opamp quad"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "P300PL104M275xC332"
		(extends "P300PL104M275xC222")
		(property "Reference" "FL"
			(at 0 7.366 0)
		)
		(property "Value" "P300PL104M275xC332"
			(at 0 5.334 0)
		)
		(property "Footprint" "Filter:Filter_KEMET_PZB300_24.0x12.5mm_P10.0mm"
			(at 2.286 4.699 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_F3019_PZB300X2_2XY2_275.pdf"
			(at -0.254 2.032 0)
		)
		(property "Description" "EMI suppression capacitor PZB300 series, metallized paper, X2 and Y2 classes, 275 VAC, Cx 0.10uF, Cy 3.3nF, legacy P/N: PZB300MC12xxx"
			(at 0 2.032 0)
		)
		(property "ki_keywords" "suppressor filter cap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*PZB300*"
			(at 0 0 0)
		)
	)
	(symbol "P300PL104M275xC472"
		(extends "P300PL104M275xC222")
		(property "Reference" "FL"
			(at 0 7.366 0)
		)
		(property "Value" "P300PL104M275xC472"
			(at 0 5.334 0)
		)
		(property "Footprint" "Filter:Filter_KEMET_PZB300_24.0x12.5mm_P10.0mm"
			(at 2.286 4.699 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_F3019_PZB300X2_2XY2_275.pdf"
			(at -0.254 2.032 0)
		)
		(property "Description" "EMI suppression capacitor PZB300 series, metallized paper, X2 and Y2 classes, 275 VAC, Cx 0.10uF, Cy 4.7nF, legacy P/N: PZB300MC13xxx"
			(at 0 2.032 0)
		)
		(property "ki_keywords" "suppressor filter cap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*PZB300*"
			(at 0 0 0)
		)
	)
	(symbol "P300PL154M275xC222"
		(extends "P300PL104M275xC222")
		(property "Reference" "FL"
			(at 0 7.366 0)
		)
		(property "Value" "P300PL154M275xC222"
			(at 0 5.334 0)
		)
		(property "Footprint" "Filter:Filter_KEMET_PZB300_24.0x12.5mm_P10.0mm"
			(at 2.286 4.699 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_F3019_PZB300X2_2XY2_275.pdf"
			(at -0.254 2.032 0)
		)
		(property "Description" "EMI suppression capacitor PZB300 series, metallized paper, X2 and Y2 classes, 275 VAC, Cx 0.15uF, Cy 2.2nF, legacy P/N: PZB300MC21xxx"
			(at 0 2.032 0)
		)
		(property "ki_keywords" "suppressor filter cap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*PZB300*"
			(at 0 0 0)
		)
	)
	(symbol "P300PL154M275xC332"
		(extends "P300PL104M275xC222")
		(property "Reference" "FL"
			(at 0 7.366 0)
		)
		(property "Value" "P300PL154M275xC332"
			(at 0 5.334 0)
		)
		(property "Footprint" "Filter:Filter_KEMET_PZB300_24.0x12.5mm_P10.0mm"
			(at 2.286 4.699 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_F3019_PZB300X2_2XY2_275.pdf"
			(at -0.254 2.032 0)
		)
		(property "Description" "EMI suppression capacitor PZB300 series, metallized paper, X2 and Y2 classes, 275 VAC, Cx 0.15uF, Cy 3.3nF, legacy P/N: PZB300MC22xxx"
			(at 0 2.032 0)
		)
		(property "ki_keywords" "suppressor filter cap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*PZB300*"
			(at 0 0 0)
		)
	)
	(symbol "P300PL154M275xC472"
		(extends "P300PL104M275xC222")
		(property "Reference" "FL"
			(at 0 7.366 0)
		)
		(property "Value" "P300PL154M275xC472"
			(at 0 5.334 0)
		)
		(property "Footprint" "Filter:Filter_KEMET_PZB300_24.0x12.5mm_P10.0mm"
			(at 2.286 4.699 0)
		)
		(property "Datasheet" "https://content.kemet.com/datasheets/KEM_F3019_PZB300X2_2XY2_275.pdf"
			(at -0.254 2.032 0)
		)
		(property "Description" "EMI suppression capacitor PZB300 series, metallized paper, X2 and Y2 classes, 275 VAC, Cx 0.15uF, Cy 4.7nF, legacy P/N: PZB300MC23xxx"
			(at 0 2.032 0)
		)
		(property "ki_keywords" "suppressor filter cap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*PZB300*"
			(at 0 0 0)
		)
	)
	(symbol "SAFFA1G58KA0F0A"
		(extends "SF14-1575F5UUA1")
		(property "Reference" "FL"
			(at 2.54 -6.35 0)
		)
		(property "Value" "SAFFA1G58KA0F0A"
			(at 0 6.35 0)
		)
		(property "Footprint" "Filter:Filter_1411-5_1.4x1.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.murata.com/~/media/webrenewal/support/library/catalog/products/filter/rf/p73e.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Murata 1575.42/1602MHz SAW filter, SMD 1411"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*1411*1.4x1.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "SAFFA1G96FN0F0A"
		(extends "SF14-1575F5UUA1")
		(property "Reference" "FL"
			(at 2.54 -6.35 0)
		)
		(property "Value" "SAFFA1G96FN0F0A"
			(at 0 6.35 0)
		)
		(property "Footprint" "Filter:Filter_1411-5_1.4x1.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.murata.com/~/media/webrenewal/support/library/catalog/products/filter/rf/p73e.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Murata 1960MHz SAW filter, SMD 1411"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*1411*1.4x1.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "SAFFA2G14FA0F0A"
		(extends "SF14-1575F5UUA1")
		(property "Reference" "FL"
			(at 2.54 -6.35 0)
		)
		(property "Value" "SAFFA2G14FA0F0A"
			(at 0 6.35 0)
		)
		(property "Footprint" "Filter:Filter_1411-5_1.4x1.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.murata.com/~/media/webrenewal/support/library/catalog/products/filter/rf/p73e.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Murata 2140MHz SAW filter, SMD 1411"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*1411*1.4x1.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "SAFFA881MFL0F0A"
		(extends "SF14-1575F5UUA1")
		(property "Reference" "FL"
			(at 2.54 -6.35 0)
		)
		(property "Value" "SAFFA881MFL0F0A"
			(at 0 6.35 0)
		)
		(property "Footprint" "Filter:Filter_1411-5_1.4x1.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.murata.com/~/media/webrenewal/support/library/catalog/products/filter/rf/p73e.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Murata 881.5MHz SAW filter, SMD 1411"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*1411*1.4x1.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "SAFFA942MFM0F0A"
		(extends "SF14-1575F5UUA1")
		(property "Reference" "FL"
			(at 2.54 -6.35 0)
		)
		(property "Value" "SAFFA942MFM0F0A"
			(at 0 6.35 0)
		)
		(property "Footprint" "Filter:Filter_1411-5_1.4x1.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.murata.com/~/media/webrenewal/support/library/catalog/products/filter/rf/p73e.ashx?la=en"
			(at 0 0 0)
		)
		(property "Description" "Murata 942.5MHz SAW filter, SMD 1411"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*1411*1.4x1.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "SAFFB1G58KA0F0A"
		(extends "B39162B8813P810")
		(property "Reference" "FL"
			(at 2.54 -6.35 0)
		)
		(property "Value" "SAFFB1G58KA0F0A"
			(at 0 6.35 0)
		)
		(property "Footprint" "Filter:Filter_1109-5_1.1x0.9mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.murata.com/~/media/webrenewal/support/library/catalog/products/filter/rf/p73e.ashx?la=en"
			(at -1.778 0.762 0)
		)
		(property "Description" "Murata 1575.42/1602MHz SAW filter, SMD 1109"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*1109*1.1x0.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "SAFFB1G96FN0F0A"
		(extends "B39162B8813P810")
		(property "Reference" "FL"
			(at 2.54 -6.35 0)
		)
		(property "Value" "SAFFB1G96FN0F0A"
			(at 0 6.35 0)
		)
		(property "Footprint" "Filter:Filter_1109-5_1.1x0.9mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.murata.com/~/media/webrenewal/support/library/catalog/products/filter/rf/p73e.ashx?la=en"
			(at -1.778 0.762 0)
		)
		(property "Description" "Murata 1960MHz SAW filter, SMD 1109"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*1109*1.1x0.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "SAFFB2G14FA0F0A"
		(extends "B39162B8813P810")
		(property "Reference" "FL"
			(at 2.54 -6.35 0)
		)
		(property "Value" "SAFFB2G14FA0F0A"
			(at 0 6.35 0)
		)
		(property "Footprint" "Filter:Filter_1109-5_1.1x0.9mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.murata.com/~/media/webrenewal/support/library/catalog/products/filter/rf/p73e.ashx?la=en"
			(at -1.778 0.762 0)
		)
		(property "Description" "Murata 2140MHz SAW filter, SMD 1109"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*1109*1.1x0.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "SAFFB881MFL0F0A"
		(extends "B39162B8813P810")
		(property "Reference" "FL"
			(at 2.54 -6.35 0)
		)
		(property "Value" "SAFFB881MFL0F0A"
			(at 0 6.35 0)
		)
		(property "Footprint" "Filter:Filter_1109-5_1.1x0.9mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.murata.com/~/media/webrenewal/support/library/catalog/products/filter/rf/p73e.ashx?la=en"
			(at -1.778 0.762 0)
		)
		(property "Description" "Murata 881.5MHz SAW filter, SMD 1109"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*1109*1.1x0.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "SAFFB942MFM0F0A"
		(extends "B39162B8813P810")
		(property "Reference" "FL"
			(at 2.54 -6.35 0)
		)
		(property "Value" "SAFFB942MFM0F0A"
			(at 0 6.35 0)
		)
		(property "Footprint" "Filter:Filter_1109-5_1.1x0.9mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.murata.com/~/media/webrenewal/support/library/catalog/products/filter/rf/p73e.ashx?la=en"
			(at -1.778 0.762 0)
		)
		(property "Description" "Murata 942.5MHz SAW filter, SMD 1109"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*1109*1.1x0.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "SF14-1575F5UUC1"
		(extends "SF14-1575F5UUA1")
		(property "Reference" "FL"
			(at 2.54 -6.35 0)
		)
		(property "Value" "SF14-1575F5UUC1"
			(at 0 6.35 0)
		)
		(property "Footprint" "Filter:Filter_1411-5_1.4x1.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://global.kyocera.com/prdct/electro/product/pdf/sf14_gnss.pdf"
			(at 0 0 0)
		)
		(property "Description" "1575MHz SAW filter, SMD 1411"
			(at 0 0 0)
		)
		(property "ki_keywords" "SAW filter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Filter*1411*1.4x1.1mm*"
			(at 0 0 0)
		)
	)
)
