(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "MC6845"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 34.29 0)
		)
		(property "Value" "MC6845"
			(at 12.7 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 -34.29 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet_pdf/motorola/MC6845L_and_MC6845P.pdf"
			(at 0 0 0)
		)
		(property "Description" "CRT Controller 1MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "CRT controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "MC6845_0_1")
		(symbol "MC6845_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "D0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "D1")
				(number "32")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "D2")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "D3")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "D4")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "D5")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "D6")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "D7")
				(number "26")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "R/~{W}")
				(number "22")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "25")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RS")
				(number "24")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "E")
				(number "23")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "2")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "CLK")
				(number "21")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "LPSTB")
				(number "3")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "MA0")
				(number "4")
			)
			(pin output line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "MA1")
				(number "5")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "MA2")
				(number "6")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "MA3")
				(number "7")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "MA4")
				(number "8")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "MA5")
				(number "9")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "MA6")
				(number "10")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "MA7")
				(number "11")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "MA8")
				(number "12")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "MA9")
				(number "13")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "MA10")
				(number "14")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "MA11")
				(number "15")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "MA12")
				(number "16")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "MA13")
				(number "17")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "RA0")
				(number "38")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "RA1")
				(number "37")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "RA2")
				(number "36")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RA3")
				(number "35")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "RA4")
				(number "34")
			)
			(pin output line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "DE")
				(number "18")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "HS")
				(number "39")
			)
			(pin output line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "VS")
				(number "40")
			)
			(pin output line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "CURSOR")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC68A45"
		(extends "MC6845")
		(property "Reference" "U"
			(at -10.16 34.29 0)
		)
		(property "Value" "MC68A45"
			(at 12.7 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 -34.29 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet_pdf/motorola/MC6845L_and_MC6845P.pdf"
			(at 0 0 0)
		)
		(property "Description" "CRT Controller 1.5MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "CRT controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68B45"
		(extends "MC6845")
		(property "Reference" "U"
			(at -10.16 34.29 0)
		)
		(property "Value" "MC68B45"
			(at 12.7 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 -34.29 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet_pdf/motorola/MC6845L_and_MC6845P.pdf"
			(at 0 0 0)
		)
		(property "Description" "CRT Controller 2MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "CRT controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
)
