(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "5PB1108PGxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "5PB1108PGxx"
			(at 10.16 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/5pb11xx-family-datasheet"
			(at -60.96 15.24 0)
		)
		(property "Description" "1:8 LVCMOS High-Performance Clock Buffer, 1.8V to 3.3V, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "clock buffer lvcmos"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "5PB1108PGxx_0_1")
		(symbol "5PB1108PGxx_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CLKIN")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "1G")
				(number "2")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "10")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "Y0")
				(number "3")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "Y1")
				(number "16")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Y2")
				(number "13")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Y3")
				(number "15")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Y4")
				(number "6")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Y5")
				(number "11")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Y6")
				(number "8")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "6821"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 34.29 0)
		)
		(property "Value" "6821"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 -34.29 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/6821.pdf"
			(at 0 0 0)
		)
		(property "Description" "Peripheral Interface Adapter 1MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "PIA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "6821_0_1")
		(symbol "6821_1_1"
			(pin bidirectional line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "D0")
				(number "33")
			)
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "D1")
				(number "32")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "D2")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "D3")
				(number "30")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D4")
				(number "29")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D5")
				(number "28")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D6")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D7")
				(number "26")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RS0")
				(number "36")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RS1")
				(number "35")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CS0")
				(number "22")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CS1")
				(number "24")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{CS2}")
				(number "23")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "R/~{W}")
				(number "21")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "ENABLE")
				(number "25")
			)
			(pin open_collector line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "~{IRQA}")
				(number "38")
			)
			(pin open_collector line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "~{IRQB}")
				(number "37")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "~{RESET}")
				(number "34")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "9")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "CA1")
				(number "40")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CA2")
				(number "39")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin input line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "CB1")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "CB2")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "68230"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "68230"
			(at 0 -3.81 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "PIT Interface parallele et Timer"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(symbol "68230_0_1")
		(symbol "68230_1_1"
			(pin tri_state line
				(at -25.4 38.1 0)
				(length 7.62)
				(name "D0")
				(number "44")
			)
			(pin tri_state line
				(at -25.4 35.56 0)
				(length 7.62)
				(name "D1")
				(number "45")
			)
			(pin tri_state line
				(at -25.4 33.02 0)
				(length 7.62)
				(name "D2")
				(number "46")
			)
			(pin tri_state line
				(at -25.4 30.48 0)
				(length 7.62)
				(name "D3")
				(number "47")
			)
			(pin tri_state line
				(at -25.4 27.94 0)
				(length 7.62)
				(name "D4")
				(number "48")
			)
			(pin tri_state line
				(at -25.4 25.4 0)
				(length 7.62)
				(name "D5")
				(number "1")
			)
			(pin tri_state line
				(at -25.4 22.86 0)
				(length 7.62)
				(name "D6")
				(number "2")
			)
			(pin tri_state line
				(at -25.4 20.32 0)
				(length 7.62)
				(name "D7")
				(number "3")
			)
			(pin input line
				(at -25.4 15.24 0)
				(length 7.62)
				(name "RS1")
				(number "29")
			)
			(pin input line
				(at -25.4 12.7 0)
				(length 7.62)
				(name "RS2")
				(number "28")
			)
			(pin input line
				(at -25.4 10.16 0)
				(length 7.62)
				(name "RS3")
				(number "27")
			)
			(pin input line
				(at -25.4 7.62 0)
				(length 7.62)
				(name "RS4")
				(number "26")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 7.62)
				(name "RS5")
				(number "25")
			)
			(pin input inverted
				(at -25.4 0 0)
				(length 7.62)
				(name "CS")
				(number "41")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 7.62)
				(name "R/W")
				(number "43")
			)
			(pin input line
				(at -25.4 -10.16 0)
				(length 7.62)
				(name "CLK")
				(number "40")
			)
			(pin input inverted
				(at -25.4 -15.24 0)
				(length 7.62)
				(name "RESET")
				(number "39")
			)
			(pin open_collector inverted
				(at -25.4 -20.32 0)
				(length 7.62)
				(name "DTACK")
				(number "42")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 7.62)
				(name "PA0")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 7.62)
				(name "PA1")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 7.62)
				(name "PA2")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 7.62)
				(name "PA3")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 7.62)
				(name "PA4")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 7.62)
				(name "PA5")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 7.62)
				(name "PA6")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 7.62)
				(name "PA7")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 7.62)
				(name "PB0")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 7.62)
				(name "PB1")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 7.62)
				(name "PB2")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 7.62)
				(name "PB3")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 7.62)
				(name "PB4")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 7.62)
				(name "PB5")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 7.62)
				(name "PB6")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 7.62)
				(name "PB7")
				(number "24")
			)
			(pin input line
				(at 25.4 -7.62 180)
				(length 7.62)
				(name "H1")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 7.62)
				(name "H2")
				(number "14")
			)
			(pin input line
				(at 25.4 -12.7 180)
				(length 7.62)
				(name "H3")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 7.62)
				(name "H4")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 7.62)
				(name "PC0")
				(number "30")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 7.62)
				(name "PC1")
				(number "31")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 7.62)
				(name "TIN/PC2")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 7.62)
				(name "PC3/TOUT")
				(number "33")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 7.62)
				(name "DMAREQ/PC4")
				(number "34")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 7.62)
				(name "PC5/PIRQ")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 7.62)
				(name "PC6/PIACK")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 7.62)
				(name "PC7/TIACK")
				(number "37")
			)
		)
		(embedded_fonts no)
	)
	(symbol "68681"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 3.81 0)
		)
		(property "Value" "68681"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Interface serie 2 voies + 1 port parallele"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(symbol "68681_0_1")
		(symbol "68681_1_1"
			(pin input line
				(at -25.4 30.48 0)
				(length 7.62)
				(name "X1/CLK")
				(number "32")
			)
			(pin input line
				(at -25.4 27.94 0)
				(length 7.62)
				(name "X2")
				(number "33")
			)
			(pin tri_state line
				(at -25.4 22.86 0)
				(length 7.62)
				(name "D0")
				(number "25")
			)
			(pin tri_state line
				(at -25.4 20.32 0)
				(length 7.62)
				(name "D1")
				(number "16")
			)
			(pin tri_state line
				(at -25.4 17.78 0)
				(length 7.62)
				(name "D2")
				(number "24")
			)
			(pin tri_state line
				(at -25.4 15.24 0)
				(length 7.62)
				(name "D3")
				(number "17")
			)
			(pin tri_state line
				(at -25.4 12.7 0)
				(length 7.62)
				(name "D4")
				(number "23")
			)
			(pin tri_state line
				(at -25.4 10.16 0)
				(length 7.62)
				(name "D5")
				(number "18")
			)
			(pin tri_state line
				(at -25.4 7.62 0)
				(length 7.62)
				(name "D6")
				(number "22")
			)
			(pin tri_state line
				(at -25.4 5.08 0)
				(length 7.62)
				(name "D7")
				(number "19")
			)
			(pin input line
				(at -25.4 0 0)
				(length 7.62)
				(name "RS1")
				(number "1")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 7.62)
				(name "RS2")
				(number "3")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 7.62)
				(name "RS3")
				(number "5")
			)
			(pin input line
				(at -25.4 -7.62 0)
				(length 7.62)
				(name "RS4")
				(number "6")
			)
			(pin input line
				(at -25.4 -12.7 0)
				(length 7.62)
				(name "CS")
				(number "35")
			)
			(pin input line
				(at -25.4 -15.24 0)
				(length 7.62)
				(name "R/W")
				(number "8")
			)
			(pin input inverted
				(at -25.4 -17.78 0)
				(length 7.62)
				(name "IACK")
				(number "37")
			)
			(pin input inverted
				(at -25.4 -20.32 0)
				(length 7.62)
				(name "RESET")
				(number "34")
			)
			(pin open_collector inverted
				(at -25.4 -25.4 0)
				(length 7.62)
				(name "DTACK")
				(number "9")
			)
			(pin output inverted
				(at -25.4 -27.94 0)
				(length 7.62)
				(name "IRQ")
				(number "21")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin output line
				(at 25.4 30.48 180)
				(length 7.62)
				(name "TXDA")
				(number "30")
			)
			(pin input line
				(at 25.4 27.94 180)
				(length 7.62)
				(name "RXDA")
				(number "31")
			)
			(pin output line
				(at 25.4 22.86 180)
				(length 7.62)
				(name "TXDB")
				(number "11")
			)
			(pin input line
				(at 25.4 20.32 180)
				(length 7.62)
				(name "RXDB")
				(number "10")
			)
			(pin output line
				(at 25.4 15.24 180)
				(length 7.62)
				(name "OP0")
				(number "29")
			)
			(pin output line
				(at 25.4 12.7 180)
				(length 7.62)
				(name "OP1")
				(number "12")
			)
			(pin output line
				(at 25.4 10.16 180)
				(length 7.62)
				(name "OP2")
				(number "28")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 7.62)
				(name "OP3")
				(number "13")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 7.62)
				(name "OP4")
				(number "27")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 7.62)
				(name "OP5")
				(number "14")
			)
			(pin output line
				(at 25.4 0 180)
				(length 7.62)
				(name "OP6")
				(number "26")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 7.62)
				(name "OP7")
				(number "15")
			)
			(pin input line
				(at 25.4 -7.62 180)
				(length 7.62)
				(name "IP0")
				(number "7")
			)
			(pin input line
				(at 25.4 -10.16 180)
				(length 7.62)
				(name "IP1")
				(number "4")
			)
			(pin input line
				(at 25.4 -12.7 180)
				(length 7.62)
				(name "IP2")
				(number "36")
			)
			(pin input line
				(at 25.4 -15.24 180)
				(length 7.62)
				(name "IP3")
				(number "2")
			)
			(pin input line
				(at 25.4 -17.78 180)
				(length 7.62)
				(name "IP4")
				(number "39")
			)
			(pin input line
				(at 25.4 -20.32 180)
				(length 7.62)
				(name "IP5")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "68901_PLCC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "68901_PLCC"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Parallel Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(symbol "68901_PLCC_0_1")
		(symbol "68901_PLCC_1_1"
			(pin input clock
				(at -22.86 35.56 0)
				(length 7.62)
				(name "X1")
				(number "19")
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 7.62)
				(name "X2")
				(number "20")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 7.62)
				(name "TAI")
				(number "22")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 7.62)
				(name "TBI")
				(number "23")
			)
			(pin input clock
				(at -22.86 17.78 0)
				(length 7.62)
				(name "CLK")
				(number "39")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 7.62)
				(name "R/W")
				(number "2")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 7.62)
				(name "CS")
				(number "52")
			)
			(pin input inverted
				(at -22.86 10.16 0)
				(length 7.62)
				(name "DS")
				(number "51")
			)
			(pin input inverted
				(at -22.86 7.62 0)
				(length 7.62)
				(name "RESET")
				(number "24")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 7.62)
				(name "RS1")
				(number "3")
			)
			(pin input line
				(at -22.86 0 0)
				(length 7.62)
				(name "RS2")
				(number "4")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 7.62)
				(name "RS3")
				(number "5")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 7.62)
				(name "RS4")
				(number "6")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 7.62)
				(name "RS5")
				(number "7")
			)
			(pin input inverted
				(at -22.86 -12.7 0)
				(length 7.62)
				(name "IACK")
				(number "49")
			)
			(pin input inverted
				(at -22.86 -15.24 0)
				(length 7.62)
				(name "IEI")
				(number "38")
			)
			(pin output inverted
				(at -22.86 -17.78 0)
				(length 7.62)
				(name "IRQ")
				(number "36")
			)
			(pin output inverted
				(at -22.86 -20.32 0)
				(length 7.62)
				(name "DTACK")
				(number "50")
			)
			(pin output inverted
				(at -22.86 -22.86 0)
				(length 7.62)
				(name "IEO")
				(number "37")
			)
			(pin input line
				(at -22.86 -30.48 0)
				(length 7.62)
				(name "MPX")
				(number "13")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 3.81)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 3.81)
				(name "GND")
				(number "40")
			)
			(pin output line
				(at 22.86 35.56 180)
				(length 7.62)
				(name "TAO")
				(number "15")
			)
			(pin output line
				(at 22.86 33.02 180)
				(length 7.62)
				(name "TBO")
				(number "16")
			)
			(pin output line
				(at 22.86 30.48 180)
				(length 7.62)
				(name "TCO")
				(number "17")
			)
			(pin output line
				(at 22.86 27.94 180)
				(length 7.62)
				(name "TDO")
				(number "18")
			)
			(pin input line
				(at 22.86 22.86 180)
				(length 7.62)
				(name "SI")
				(number "10")
			)
			(pin output line
				(at 22.86 20.32 180)
				(length 7.62)
				(name "SO")
				(number "9")
			)
			(pin input clock
				(at 22.86 17.78 180)
				(length 7.62)
				(name "RC")
				(number "11")
			)
			(pin input clock
				(at 22.86 15.24 180)
				(length 7.62)
				(name "TC")
				(number "8")
			)
			(pin output inverted
				(at 22.86 10.16 180)
				(length 7.62)
				(name "TR")
				(number "34")
			)
			(pin output inverted
				(at 22.86 7.62 180)
				(length 7.62)
				(name "RR")
				(number "35")
			)
			(pin input line
				(at 22.86 2.54 180)
				(length 7.62)
				(name "I0")
				(number "25")
			)
			(pin input line
				(at 22.86 0 180)
				(length 7.62)
				(name "I1")
				(number "26")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 7.62)
				(name "I2")
				(number "27")
			)
			(pin input line
				(at 22.86 -5.08 180)
				(length 7.62)
				(name "I3")
				(number "28")
			)
			(pin input line
				(at 22.86 -7.62 180)
				(length 7.62)
				(name "I4")
				(number "29")
			)
			(pin input line
				(at 22.86 -10.16 180)
				(length 7.62)
				(name "I5")
				(number "30")
			)
			(pin input line
				(at 22.86 -12.7 180)
				(length 7.62)
				(name "I6")
				(number "31")
			)
			(pin input line
				(at 22.86 -15.24 180)
				(length 7.62)
				(name "I7")
				(number "32")
			)
			(pin input line
				(at 22.86 -20.32 180)
				(length 7.62)
				(name "D0")
				(number "41")
			)
			(pin input line
				(at 22.86 -22.86 180)
				(length 7.62)
				(name "D1")
				(number "42")
			)
			(pin input line
				(at 22.86 -25.4 180)
				(length 7.62)
				(name "D2")
				(number "43")
			)
			(pin input line
				(at 22.86 -27.94 180)
				(length 7.62)
				(name "D3")
				(number "44")
			)
			(pin input line
				(at 22.86 -30.48 180)
				(length 7.62)
				(name "D4")
				(number "45")
			)
			(pin input line
				(at 22.86 -33.02 180)
				(length 7.62)
				(name "D5")
				(number "46")
			)
			(pin input line
				(at 22.86 -35.56 180)
				(length 7.62)
				(name "D6")
				(number "47")
			)
			(pin input line
				(at 22.86 -38.1 180)
				(length 7.62)
				(name "D7")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8237"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 38.1 0)
		)
		(property "Value" "8237"
			(at 8.89 38.1 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "https://pdos.csail.mit.edu/6.828/2012/readings/hardware/8237A.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "Programmable DMA Controller, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "8237 DMA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "8237_1_1"
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "A0")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 3.81)
				(name "A1")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "A2")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 3.81)
				(name "A3")
				(number "35")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "~{CS}")
				(number "11")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "READY")
				(number "6")
			)
			(pin input clock
				(at -17.78 15.24 0)
				(length 3.81)
				(name "CLK")
				(number "12")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "HLDA")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "~{IOR}")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "~{IOW}")
				(number "2")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "DREQ0")
				(number "19")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "DREQ1")
				(number "18")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "DREQ2")
				(number "17")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "DREQ3")
				(number "16")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "RESET")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "DB0")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "DB1")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "DB2")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "DB3")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 3.81)
				(name "DB4")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 3.81)
				(name "DB5")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 3.81)
				(name "DB6")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 3.81)
				(name "DB7")
				(number "21")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 3.81)
				(name "Vcc")
				(number "31")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 3.81)
				(name "Vss")
				(number "20")
			)
			(pin input line
				(at 2.54 40.64 270)
				(length 3.81)
				(name "PIN5")
				(number "5")
			)
			(pin tri_state line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "A4")
				(number "37")
			)
			(pin tri_state line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "A5")
				(number "38")
			)
			(pin tri_state line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "A6")
				(number "39")
			)
			(pin tri_state line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "A7")
				(number "40")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "HRQ")
				(number "10")
			)
			(pin tri_state line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "~{MEMR}")
				(number "3")
			)
			(pin tri_state line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "~{MEMW}")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "~{EOP}")
				(number "36")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "DACK0")
				(number "25")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "DACK1")
				(number "24")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "DACK2")
				(number "14")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "DACK3")
				(number "15")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "ADSTB")
				(number "8")
			)
			(pin output line
				(at 17.78 -33.02 180)
				(length 3.81)
				(name "AEN")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8255"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 38.1 0)
		)
		(property "Value" "8255"
			(at 8.89 38.1 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://aturing.umcs.maine.edu/~meadow/courses/cos335/Intel8255A.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "Programmable Peripheral Interface, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "8255 PPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "8255_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "RESET")
				(number "35")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 3.81)
				(name "~{CS}")
				(number "6")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "~{RD}")
				(number "5")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "~{WR}")
				(number "36")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "A0")
				(number "9")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "A1")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "D0")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "D1")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "D2")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "D3")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "D4")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "D5")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "D6")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "D7")
				(number "27")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 3.81)
				(name "VCC")
				(number "26")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "PA0")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "PA1")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "PA2")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "PA4")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "PA5")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "PA6")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "PA7")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PB0")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PB1")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PB3")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "PB4")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PB5")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PB6")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "PB7")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "PC0")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "PC1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "PC2")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "PC3")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "PC4")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "PC5")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "PC6")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "PC7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8259"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 25.4 0)
		)
		(property "Value" "8259"
			(at 8.89 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://pdos.csail.mit.edu/6.828/2005/readings/hardware/8259A.pdf"
			(at 0 0 0)
		)
		(property "Description" "8259, Programmable Interrupt Controller, PDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "PIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "8259_0_1")
		(symbol "8259_1_1"
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 3.81)
				(name "D0")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "D1")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "D2")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "D3")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "D4")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "D5")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "D6")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "D7")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "A0")
				(number "27")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "~{WR}")
				(number "2")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "~{RD}")
				(number "3")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 3.81)
				(name "INT")
				(number "17")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 3.81)
				(name "~{INTA}")
				(number "26")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "GND")
				(number "14")
			)
			(pin input line
				(at 15.24 20.32 180)
				(length 3.81)
				(name "IR7")
				(number "25")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 3.81)
				(name "IR6")
				(number "24")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "IR5")
				(number "23")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "IR4")
				(number "22")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "IR3")
				(number "21")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "IR2")
				(number "20")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "IR1")
				(number "19")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "IR0")
				(number "18")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "CAS0")
				(number "12")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "CAS1")
				(number "13")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "CAS2")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "~{SP}/~{EN}")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8288"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 20.32 0)
		)
		(property "Value" "8288"
			(at 8.89 20.32 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.datasheets360.com/pdf/7208679415653955300"
			(at -13.97 20.32 0)
		)
		(property "Description" "Bus Controller for Intel 8086/8088/80186/80188 microprocessors, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bus Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "8288_0_0")
		(symbol "8288_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "~{S0}")
				(number "19")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "~{S1}")
				(number "3")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "~{S2}")
				(number "18")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{AEN}")
				(number "6")
			)
			(pin input clock
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "CLK")
				(number "2")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "IOB")
				(number "1")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "CEN")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin tri_state line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "~{AIOWC}")
				(number "12")
			)
			(pin tri_state line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "~{AMWC}")
				(number "8")
			)
			(pin tri_state line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "~{IOWC}")
				(number "11")
			)
			(pin tri_state line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "~{MWTC}")
				(number "9")
			)
			(pin tri_state line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "~{MRDC}")
				(number "7")
			)
			(pin tri_state line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "~{IORC}")
				(number "13")
			)
			(pin tri_state line
				(at 17.78 0 180)
				(length 3.81)
				(name "~{INTA}")
				(number "14")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "DT/~{R}")
				(number "4")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "ALE")
				(number "5")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "MCE/~{PDEN}")
				(number "17")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "DEN")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "82C55A_PLCC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 38.1 0)
		)
		(property "Value" "82C55A_PLCC"
			(at 8.89 38.1 0)
		)
		(property "Footprint" "Package_LCC:PLCC-44"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://jap.hu/electronic/8255.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "CHMOS Programmable Peripheral Interface, PLCC-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "8255 PPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*PLCC?44*"
			(at 0 0 0)
		)
		(symbol "82C55A_PLCC_1_1"
			(pin input line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "RESET")
				(number "39")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 3.81)
				(name "~{CS}")
				(number "7")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "~{RD}")
				(number "6")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "~{WR}")
				(number "40")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "A0")
				(number "10")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "A1")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "D0")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "D1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "D2")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "D3")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "D4")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "D5")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "D6")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "D7")
				(number "30")
			)
			(pin no_connect line
				(at -13.97 -22.86 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -13.97 -25.4 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -13.97 -27.94 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at -13.97 -30.48 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 3.81)
				(name "VCC")
				(number "29")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "PA0")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "PA1")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "PA3")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "PA4")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "PA5")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "PA6")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "PA7")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PB0")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PB1")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PB2")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PB3")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "PB4")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PB5")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PB6")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "PB7")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "PC4")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "PC5")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "PC6")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "PC7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "88SE9125C0-NAA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 36.83 0)
		)
		(property "Value" "88SE9125C0-NAA"
			(at 20.32 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-76-1EP_9x9mm_P0.4mm_EP3.8x3.8mm"
			(at -2.54 48.26 0)
		)
		(property "Datasheet" "https://www.marvell.com/documents/bqcwxsoiqfjkcjdjhkvc/"
			(at -31.75 0 0)
		)
		(property "Description" "One-Lane PCIe SATA Two-Ports Controller, QFN-76"
			(at 0 0 0)
		)
		(property "ki_keywords" "PCIe2.0 SATA3.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "88SE9125C0-NAA_0_0"
			(text "PCIe"
				(at 0 1.27 0)
			)
		)
		(symbol "88SE9125C0-NAA_0_1")
		(symbol "88SE9125C0-NAA_1_0"
			(text "SATA"
				(at 0 -1.27 0)
			)
		)
		(symbol "88SE9125C0-NAA_1_1"
			(pin output line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "PTXP")
				(number "40")
			)
			(pin output line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PTXN")
				(number "39")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PRXP")
				(number "44")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PRXN")
				(number "43")
			)
			(pin input line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "CLKP")
				(number "45")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "CLKN")
				(number "46")
			)
			(pin open_collector line
				(at -22.86 0 0)
				(length 2.54)
				(name "~{WAKE}")
				(number "52")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "~{PERST}")
				(number "53")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "TP")
				(number "22")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "XTLIN_OSC")
				(number "35")
			)
			(pin output line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "XTLOUT")
				(number "36")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "TESTMODE")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "ISET")
				(number "37")
			)
			(pin no_connect line
				(at -20.32 27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "62")
			)
			(pin no_connect line
				(at -20.32 20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "61")
			)
			(pin no_connect line
				(at -20.32 12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "60")
			)
			(pin no_connect line
				(at -20.32 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "59")
			)
			(pin no_connect line
				(at -20.32 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "58")
			)
			(pin no_connect line
				(at -20.32 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -20.32 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -20.32 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "55")
			)
			(pin no_connect line
				(at -20.32 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -20.32 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at -20.32 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at -20.32 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin power_in line
				(at -17.78 38.1 270)
				(length 2.54)
				(name "AVDD")
				(number "42")
			)
			(pin power_in line
				(at -15.24 38.1 270)
				(length 2.54)
				(name "AVDDT")
				(number "41")
			)
			(pin no_connect line
				(at -12.7 35.56 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "72")
			)
			(pin no_connect line
				(at -12.7 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "68")
			)
			(pin power_in line
				(at -10.16 38.1 270)
				(length 2.54)
				(name "VAA2_0")
				(number "31")
			)
			(pin no_connect line
				(at -10.16 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "67")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VAA2_1")
				(number "25")
			)
			(pin no_connect line
				(at -7.62 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "66")
			)
			(pin no_connect line
				(at -5.08 35.56 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "76")
			)
			(pin no_connect line
				(at -5.08 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "65")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VAA1")
				(number "34")
			)
			(pin no_connect line
				(at -2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "63")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "28")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "77")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDIO")
				(number "9")
			)
			(pin no_connect line
				(at 2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "69")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDDIO")
				(number "57")
			)
			(pin no_connect line
				(at 5.08 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VDDIO")
				(number "73")
			)
			(pin no_connect line
				(at 7.62 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "70")
			)
			(pin passive line
				(at 10.16 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 10.16 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 12.7 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "21")
			)
			(pin power_in line
				(at 15.24 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 17.78 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "64")
			)
			(pin passive line
				(at 17.78 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "71")
			)
			(pin no_connect line
				(at 20.32 30.48 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "56")
			)
			(pin no_connect line
				(at 20.32 25.4 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 20.32 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 20.32 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 20.32 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 20.32 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 20.32 -22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin output line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "VCONT_10")
				(number "38")
			)
			(pin output line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "TXP_0")
				(number "33")
			)
			(pin output line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "TXN_0")
				(number "32")
			)
			(pin input line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "RXP_0")
				(number "29")
			)
			(pin input line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "RXN_0")
				(number "30")
			)
			(pin output line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "TXP_1")
				(number "27")
			)
			(pin output line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "TXN_1")
				(number "26")
			)
			(pin input line
				(at 22.86 0 180)
				(length 2.54)
				(name "RXP_1")
				(number "23")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "RXN_1")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "GPIO0")
				(number "54")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "GPIO1")
				(number "74")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "GPIO2")
				(number "75")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "GPIO3")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "GPIO4")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "GPIO5")
				(number "19")
			)
			(pin output line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "SPI_CS")
				(number "48")
			)
			(pin output line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "SPI_CLK")
				(number "50")
			)
			(pin output line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "SPI_DO")
				(number "47")
			)
			(pin input line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "SPI_DI")
				(number "49")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9833xRM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 11.43 0)
		)
		(property "Value" "AD9833xRM"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad9833.pdf"
			(at -1.27 7.62 0)
		)
		(property "Description" "10 bit 25 MHz Programmable Waveform Generator, 2.3V to 5.5V, 12.65mW, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "Direct Digital Synthesizer DDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD9833xRM_0_1")
		(symbol "AD9833xRM_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SCLK")
				(number "7")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SDATA")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "~{FSYNC}")
				(number "8")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "MCLK")
				(number "5")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "CAP/2.5V")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -12.7 90)
				(length 2.54)
				(name "DGND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 2.54)
				(name "AGND")
				(number "9")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "COMP")
				(number "1")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "VOUT")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9834"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "AD9834"
			(at 5.334 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD9834.pdf"
			(at -76.2 0 0)
		)
		(property "Description" "10 bit 75 MHz Complete Direct Digital Synthesizer, 2.3V to 5.5V, 20mW, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Direct Digital Synthesizer DDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD9834_0_1")
		(symbol "AD9834_1_1"
			(pin input clock
				(at -15.24 12.7 0)
				(length 2.54)
				(name "SCLK")
				(number "14")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SDATA")
				(number "13")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{FSYNC}")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RESET")
				(number "11")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "SLEEP")
				(number "12")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PSELECT")
				(number "10")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "FSELECT")
				(number "9")
			)
			(pin input clock
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "MCLK")
				(number "8")
			)
			(pin passive line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "CAP/2.5V")
				(number "6")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "DVDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "DGND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "AVDD")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "AGND")
				(number "18")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "COMP")
				(number "3")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "REFOUT")
				(number "2")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "FS_ADJUST")
				(number "1")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "SIGNBITOUT")
				(number "16")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "IOUTB")
				(number "20")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IOUT")
				(number "19")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "VIN")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9850"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 19.05 0)
		)
		(property "Value" "AD9850"
			(at 12.7 19.05 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD9850.pdf"
			(at -7.62 -25.4 0)
		)
		(property "Description" "CMOS, 125 MHz, Complete DDS Synthesizer, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "DDS direct digital synthesizer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD9850_0_1")
		(symbol "AD9850_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "D0")
				(number "4")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "D1")
				(number "3")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "D2")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "D3")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "D4")
				(number "28")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "D5")
				(number "27")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "D6")
				(number "26")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "D7")
				(number "25")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "W_CLK")
				(number "7")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "FQ_UD")
				(number "8")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RESET")
				(number "22")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "CLKIN")
				(number "9")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "AVDD")
				(number "11")
			)
			(pin passive line
				(at -2.54 20.32 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "10")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "19")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "DVDD")
				(number "23")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "24")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "DVDD")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "5")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IOUT")
				(number "21")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "IOUTB")
				(number "20")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "VINP")
				(number "16")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "VINN")
				(number "15")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "QOUT")
				(number "14")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "QOUTB")
				(number "13")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RSET")
				(number "12")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "DACBL")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9851"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 19.05 0)
		)
		(property "Value" "AD9851"
			(at 12.7 19.05 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD9851.pdf"
			(at -7.62 -25.4 0)
		)
		(property "Description" "CMOS, 180 MHz, DDS/DAC Synthesizer, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "DDS direct digital synthesizer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AD9851_0_1")
		(symbol "AD9851_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "D0")
				(number "4")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "D1")
				(number "3")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "D2")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "D3")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "D4")
				(number "28")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "D5")
				(number "27")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "D6")
				(number "26")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "D7")
				(number "25")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "W_CLK")
				(number "7")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "FQ_UD")
				(number "8")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RESET")
				(number "22")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "REFCLK")
				(number "9")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "AVDD")
				(number "11")
			)
			(pin passive line
				(at -2.54 20.32 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "10")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "19")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "DVDD")
				(number "23")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "24")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "PVCC")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "PGND")
				(number "5")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IOUT")
				(number "21")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "IOUTB")
				(number "20")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "VINP")
				(number "16")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "VINN")
				(number "15")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "VOUTP")
				(number "14")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "VOUTN")
				(number "13")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RSET")
				(number "12")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "DACBP")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9910"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 62.23 0)
		)
		(property "Value" "AD9910"
			(at 20.32 62.23 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100-1EP_14x14mm_P0.5mm_EP5x5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/AD9910.pdf"
			(at 0 0 0)
		)
		(property "Description" "1 GSPS, 14-Bit, 3.3V CMOS, Direct Digital Synthesizer, QFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "dds direct digital synthesizer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*1EP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD9910_0_0"
			(text "HIGH SPEED"
				(at -15.875 0 900)
			)
			(text "SERIAL"
				(at -15.24 -32.385 900)
			)
			(text "PARALLEL DATA"
				(at -13.335 0 900)
			)
			(text "DATA"
				(at -12.7 -33.02 900)
			)
			(text "INTERFACE"
				(at -10.795 0 900)
			)
			(text "INTERFACE"
				(at -10.16 -33.02 900)
			)
			(text "1024-"
				(at 3.81 12.7 0)
			)
			(text "ELEMENT"
				(at 3.81 10.16 0)
			)
			(text "RAM"
				(at 3.81 7.62 0)
			)
			(text "LINEAR"
				(at 3.81 -1.27 0)
			)
			(text "RAMP"
				(at 3.81 -3.81 0)
			)
			(text "GENERATOR"
				(at 3.81 -6.35 0)
			)
			(text "1GBPS"
				(at 3.81 -16.51 0)
			)
			(text "DDS"
				(at 3.81 -19.05 0)
			)
			(text "CORE"
				(at 3.81 -21.59 0)
			)
			(text "TIMING"
				(at 3.81 -30.48 0)
			)
			(text "AND"
				(at 3.81 -33.02 0)
			)
			(text "CONTROL"
				(at 3.81 -35.56 0)
			)
			(text "REFCLK"
				(at 3.81 -46.99 0)
			)
			(text "MULTIPLIER"
				(at 3.81 -49.53 0)
			)
			(text "DAC"
				(at 16.51 -20.32 0)
			)
		)
		(symbol "AD9910_0_1")
		(symbol "AD9910_1_0"
			(text "14-BIT"
				(at 16.51 -17.78 0)
			)
		)
		(symbol "AD9910_1_1"
			(pin input line
				(at -30.48 58.42 0)
				(length 2.54)
				(name "SYNC_IN+")
				(number "7")
			)
			(pin input line
				(at -30.48 55.88 0)
				(length 2.54)
				(name "SYNC_IN-")
				(number "8")
			)
			(pin input line
				(at -30.48 50.8 0)
				(length 2.54)
				(name "MASTER_RESET")
				(number "14")
			)
			(pin input line
				(at -30.48 48.26 0)
				(length 2.54)
				(name "EXT_PWR_DWN")
				(number "18")
			)
			(pin input line
				(at -30.48 43.18 0)
				(length 2.54)
				(name "PROFILE0")
				(number "54")
			)
			(pin input line
				(at -30.48 40.64 0)
				(length 2.54)
				(name "PROFILE1")
				(number "53")
			)
			(pin input line
				(at -30.48 38.1 0)
				(length 2.54)
				(name "PROFILE2")
				(number "52")
			)
			(pin input line
				(at -30.48 33.02 0)
				(length 2.54)
				(name "OSK")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 2.54)
				(name "I/O_UPDATE")
				(number "59")
			)
			(pin input line
				(at -30.48 22.86 0)
				(length 2.54)
				(name "TxENABLE")
				(number "41")
			)
			(pin input line
				(at -30.48 20.32 0)
				(length 2.54)
				(name "F0")
				(number "50")
			)
			(pin input line
				(at -30.48 17.78 0)
				(length 2.54)
				(name "F1")
				(number "49")
			)
			(pin input line
				(at -30.48 15.24 0)
				(length 2.54)
				(name "D0")
				(number "48")
			)
			(pin input line
				(at -30.48 12.7 0)
				(length 2.54)
				(name "D1")
				(number "44")
			)
			(pin input line
				(at -30.48 10.16 0)
				(length 2.54)
				(name "D2")
				(number "43")
			)
			(pin input line
				(at -30.48 7.62 0)
				(length 2.54)
				(name "D3")
				(number "42")
			)
			(pin input line
				(at -30.48 5.08 0)
				(length 2.54)
				(name "D4")
				(number "39")
			)
			(pin input line
				(at -30.48 2.54 0)
				(length 2.54)
				(name "D5")
				(number "38")
			)
			(pin input line
				(at -30.48 0 0)
				(length 2.54)
				(name "D6")
				(number "37")
			)
			(pin input line
				(at -30.48 -2.54 0)
				(length 2.54)
				(name "D7")
				(number "36")
			)
			(pin input line
				(at -30.48 -5.08 0)
				(length 2.54)
				(name "D8")
				(number "35")
			)
			(pin input line
				(at -30.48 -7.62 0)
				(length 2.54)
				(name "D9")
				(number "34")
			)
			(pin input line
				(at -30.48 -10.16 0)
				(length 2.54)
				(name "D10")
				(number "33")
			)
			(pin input line
				(at -30.48 -12.7 0)
				(length 2.54)
				(name "D11")
				(number "32")
			)
			(pin input line
				(at -30.48 -15.24 0)
				(length 2.54)
				(name "D12")
				(number "31")
			)
			(pin input line
				(at -30.48 -17.78 0)
				(length 2.54)
				(name "D13")
				(number "27")
			)
			(pin input line
				(at -30.48 -20.32 0)
				(length 2.54)
				(name "D14")
				(number "26")
			)
			(pin input line
				(at -30.48 -22.86 0)
				(length 2.54)
				(name "D15")
				(number "25")
			)
			(pin input line
				(at -30.48 -27.94 0)
				(length 2.54)
				(name "SCLK")
				(number "69")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 2.54)
				(name "SDIO")
				(number "67")
			)
			(pin output line
				(at -30.48 -33.02 0)
				(length 2.54)
				(name "SDO")
				(number "68")
			)
			(pin input line
				(at -30.48 -35.56 0)
				(length 2.54)
				(name "~{CS}")
				(number "70")
			)
			(pin input line
				(at -30.48 -38.1 0)
				(length 2.54)
				(name "I/O_RESET")
				(number "71")
			)
			(pin input line
				(at -30.48 -43.18 0)
				(length 2.54)
				(name "DRCTL")
				(number "62")
			)
			(pin input line
				(at -30.48 -45.72 0)
				(length 2.54)
				(name "DRHOLD")
				(number "63")
			)
			(pin input line
				(at -30.48 -50.8 0)
				(length 2.54)
				(name "PLL_LOOP_FILTER")
				(number "2")
			)
			(pin input line
				(at -30.48 -53.34 0)
				(length 2.54)
				(name "REF_CLK")
				(number "90")
			)
			(pin input line
				(at -30.48 -55.88 0)
				(length 2.54)
				(name "~{REF_CLK}")
				(number "91")
			)
			(pin input line
				(at -30.48 -58.42 0)
				(length 2.54)
				(name "XTAL_SEL")
				(number "95")
			)
			(pin power_in line
				(at -10.16 63.5 270)
				(length 2.54)
				(name "AVDD_3V3")
				(number "74")
			)
			(pin passive line
				(at -10.16 63.5 270)
				(length 2.54)
				(hide yes)
				(name "AVDD_3V3")
				(number "75")
			)
			(pin passive line
				(at -10.16 63.5 270)
				(length 2.54)
				(hide yes)
				(name "AVDD_3V3")
				(number "76")
			)
			(pin passive line
				(at -10.16 63.5 270)
				(length 2.54)
				(hide yes)
				(name "AVDD_3V3")
				(number "77")
			)
			(pin passive line
				(at -10.16 63.5 270)
				(length 2.54)
				(hide yes)
				(name "AVDD_3V3")
				(number "83")
			)
			(pin power_in line
				(at -5.08 63.5 270)
				(length 2.54)
				(name "AVDD_1V8")
				(number "89")
			)
			(pin passive line
				(at -5.08 63.5 270)
				(length 2.54)
				(hide yes)
				(name "AVDD_1V8")
				(number "92")
			)
			(pin power_in line
				(at -5.08 -63.5 90)
				(length 2.54)
				(name "AGND")
				(number "4")
			)
			(pin passive line
				(at -5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "5")
			)
			(pin passive line
				(at -5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "73")
			)
			(pin passive line
				(at -5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "78")
			)
			(pin passive line
				(at -5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "79")
			)
			(pin passive line
				(at -5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "82")
			)
			(pin passive line
				(at -5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "85")
			)
			(pin passive line
				(at -5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "88")
			)
			(pin passive line
				(at -5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "96")
			)
			(pin power_in line
				(at -2.54 63.5 270)
				(length 2.54)
				(name "AVDD_1V8")
				(number "3")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 2.54)
				(name "AVDD_1V8")
				(number "6")
			)
			(pin power_in line
				(at 0 -63.5 90)
				(length 2.54)
				(name "EP")
				(number "101")
			)
			(pin power_in line
				(at 5.08 63.5 270)
				(length 2.54)
				(name "DVDD_1V8")
				(number "17")
			)
			(pin passive line
				(at 5.08 63.5 270)
				(length 2.54)
				(hide yes)
				(name "DVDD_1V8")
				(number "23")
			)
			(pin passive line
				(at 5.08 63.5 270)
				(length 2.54)
				(hide yes)
				(name "DVDD_1V8")
				(number "30")
			)
			(pin passive line
				(at 5.08 63.5 270)
				(length 2.54)
				(hide yes)
				(name "DVDD_1V8")
				(number "47")
			)
			(pin passive line
				(at 5.08 63.5 270)
				(length 2.54)
				(hide yes)
				(name "DVDD_1V8")
				(number "57")
			)
			(pin passive line
				(at 5.08 63.5 270)
				(length 2.54)
				(hide yes)
				(name "DVDD_1V8")
				(number "64")
			)
			(pin power_in line
				(at 5.08 -63.5 90)
				(length 2.54)
				(name "DGND")
				(number "13")
			)
			(pin passive line
				(at 5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "16")
			)
			(pin passive line
				(at 5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "22")
			)
			(pin passive line
				(at 5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "29")
			)
			(pin passive line
				(at 5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "46")
			)
			(pin passive line
				(at 5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "51")
			)
			(pin passive line
				(at 5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "58")
			)
			(pin passive line
				(at 5.08 -63.5 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "65")
			)
			(pin power_in line
				(at 10.16 63.5 270)
				(length 2.54)
				(name "DVDD_IO_3V3")
				(number "11")
			)
			(pin passive line
				(at 10.16 63.5 270)
				(length 2.54)
				(hide yes)
				(name "DVDD_IO_3V3")
				(number "15")
			)
			(pin passive line
				(at 10.16 63.5 270)
				(length 2.54)
				(hide yes)
				(name "DVDD_IO_3V3")
				(number "21")
			)
			(pin passive line
				(at 10.16 63.5 270)
				(length 2.54)
				(hide yes)
				(name "DVDD_IO_3V3")
				(number "28")
			)
			(pin passive line
				(at 10.16 63.5 270)
				(length 2.54)
				(hide yes)
				(name "DVDD_IO_3V3")
				(number "45")
			)
			(pin passive line
				(at 10.16 63.5 270)
				(length 2.54)
				(hide yes)
				(name "DVDD_IO_3V3")
				(number "56")
			)
			(pin passive line
				(at 10.16 63.5 270)
				(length 2.54)
				(hide yes)
				(name "DVDD_IO_3V3")
				(number "66")
			)
			(pin no_connect line
				(at 27.94 48.26 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 27.94 45.72 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at 27.94 43.18 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "72")
			)
			(pin no_connect line
				(at 27.94 40.64 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "86")
			)
			(pin no_connect line
				(at 27.94 38.1 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "87")
			)
			(pin no_connect line
				(at 27.94 35.56 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "93")
			)
			(pin no_connect line
				(at 27.94 33.02 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "97")
			)
			(pin no_connect line
				(at 27.94 27.94 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "98")
			)
			(pin no_connect line
				(at 27.94 25.4 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "99")
			)
			(pin no_connect line
				(at 27.94 22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "100")
			)
			(pin output line
				(at 30.48 55.88 180)
				(length 2.54)
				(name "SYNC_OUT+")
				(number "9")
			)
			(pin output line
				(at 30.48 53.34 180)
				(length 2.54)
				(name "SYNC_OUT-")
				(number "10")
			)
			(pin output line
				(at 30.48 50.8 180)
				(length 2.54)
				(name "SYNC_SMP_ERR")
				(number "12")
			)
			(pin output line
				(at 30.48 30.48 180)
				(length 2.54)
				(name "RAM_SWP_OVR")
				(number "24")
			)
			(pin output line
				(at 30.48 5.08 180)
				(length 2.54)
				(name "DROVER")
				(number "61")
			)
			(pin output line
				(at 30.48 -2.54 180)
				(length 2.54)
				(name "PDCLK")
				(number "40")
			)
			(pin output line
				(at 30.48 -17.78 180)
				(length 2.54)
				(name "~{IOUT}")
				(number "80")
			)
			(pin output line
				(at 30.48 -20.32 180)
				(length 2.54)
				(name "IOUT")
				(number "81")
			)
			(pin output line
				(at 30.48 -33.02 180)
				(length 2.54)
				(name "DAC_RSET")
				(number "84")
			)
			(pin output line
				(at 30.48 -48.26 180)
				(length 2.54)
				(name "PLL_LOCK")
				(number "19")
			)
			(pin output line
				(at 30.48 -53.34 180)
				(length 2.54)
				(name "SYNC_CLK")
				(number "55")
			)
			(pin output line
				(at 30.48 -58.42 180)
				(length 2.54)
				(name "REFCLK_OUT")
				(number "94")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9912"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 24.13 0)
		)
		(property "Value" "AD9912"
			(at 11.43 24.13 0)
		)
		(property "Footprint" "Package_CSP:LFCSP-64-1EP_9x9mm_P0.5mm_EP5.21x5.21mm"
			(at -2.54 38.1 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ad9912.pdf"
			(at -12.7 -2.54 0)
		)
		(property "Description" "1 GSPS, 14-bit DAC, Direct Digital Synthesizer, LFCSP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Direct Digital Synthesizer DDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LFCSP*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD9912_0_1")
		(symbol "AD9912_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{CSB}")
				(number "61")
			)
			(pin output line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "SDO")
				(number "62")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SDIO")
				(number "63")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "SCLK")
				(number "64")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SYSCLK")
				(number "27")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SYSCLK_B")
				(number "28")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "CLKMODESEL")
				(number "32")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PWRDOWN")
				(number "58")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "RESET")
				(number "59")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "IO_UPDATE")
				(number "60")
			)
			(pin tri_state line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "S1")
				(number "9")
			)
			(pin tri_state line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "S2")
				(number "10")
			)
			(pin tri_state line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "S3")
				(number "54")
			)
			(pin tri_state line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "S4")
				(number "55")
			)
			(pin no_connect line
				(at -12.7 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -10.16 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin power_in line
				(at -7.62 25.4 270)
				(length 2.54)
				(name "DVDD_I/O")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "DVDD")
				(number "3")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "DVDD")
				(number "5")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "DVDD")
				(number "7")
			)
			(pin no_connect line
				(at -5.08 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "AVDD3")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "DVSS")
				(number "2")
			)
			(pin passive line
				(at -2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "DVSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "DVSS")
				(number "56")
			)
			(pin passive line
				(at -2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "DVSS")
				(number "57")
			)
			(pin passive line
				(at -2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "DVSS")
				(number "6")
			)
			(pin passive line
				(at -2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "DVSS")
				(number "8")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "AVDD3")
				(number "37")
			)
			(pin no_connect line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "AVDD3")
				(number "46")
			)
			(pin passive line
				(at 2.54 25.4 270)
				(length 2.54)
				(hide yes)
				(name "AVDD3")
				(number "47")
			)
			(pin passive line
				(at 2.54 25.4 270)
				(length 2.54)
				(hide yes)
				(name "AVDD3")
				(number "49")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "AVSS")
				(number "33")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "AVSS")
				(number "39")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "AVSS")
				(number "43")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "AVSS")
				(number "52")
			)
			(pin passive line
				(at 2.54 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "AVSS")
				(number "65")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "11")
			)
			(pin passive line
				(at 5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "19")
			)
			(pin passive line
				(at 5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "23")
			)
			(pin passive line
				(at 5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "24")
			)
			(pin passive line
				(at 5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "36")
			)
			(pin passive line
				(at 5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "42")
			)
			(pin passive line
				(at 5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "44")
			)
			(pin passive line
				(at 5.08 25.4 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "45")
			)
			(pin no_connect line
				(at 5.08 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin power_in line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "53")
			)
			(pin no_connect line
				(at 7.62 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin power_in line
				(at 10.16 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "25")
			)
			(pin passive line
				(at 10.16 25.4 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "26")
			)
			(pin passive line
				(at 10.16 25.4 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "29")
			)
			(pin passive line
				(at 10.16 25.4 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "30")
			)
			(pin no_connect line
				(at 10.16 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 12.7 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "LOOP_FILTER")
				(number "31")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "OUT_CMOS")
				(number "38")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "OUT")
				(number "35")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "34")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "FDBK_IN")
				(number "41")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "FDBK_INB")
				(number "40")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "DAC_OUT")
				(number "50")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "DAC_OUTB")
				(number "51")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "DAC_RSET")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9951"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 27.94 0)
		)
		(property "Value" "AD9951"
			(at -13.97 25.4 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP3.5x3.5mm"
			(at 33.02 -29.21 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD9951.pdf"
			(at 39.37 -31.75 0)
		)
		(property "Description" "14-Bit Direct Digital Synthesizer with 400MSPS DAC, 1.8V, TQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Direct Digital Synthesizer DDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD9951_0_1")
		(symbol "AD9951_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "RESET")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "I/OUPDATE")
				(number "1")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "SYNC_CLK")
				(number "45")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "OSC/REFCLK")
				(number "9")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "~{OSC/REFCLK}")
				(number "8")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "CLKMODESELECT")
				(number "11")
			)
			(pin output line
				(at -17.78 0 0)
				(length 3.81)
				(name "CRYSTALOUT")
				(number "10")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "SDO")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "SDIO")
				(number "41")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "SCLK")
				(number "40")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "~{CS}")
				(number "39")
			)
			(pin output line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "IOSYNC")
				(number "37")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "DVDD_I/O")
				(number "43")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "DGND")
				(number "3")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "DGND")
				(number "33")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "DGND")
				(number "42")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "DGND")
				(number "47")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "DGND")
				(number "48")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "DVDD")
				(number "2")
			)
			(pin passive line
				(at 2.54 27.94 270)
				(length 3.81)
				(hide yes)
				(name "DVDD")
				(number "34")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "14")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "15")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "17")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "22")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "26")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "28")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "30")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "31")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "32")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "49")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "AGND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "7")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "13")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "16")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "18")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "19")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "25")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "27")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "29")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 3.81)
				(name "AVDD")
				(number "4")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "6")
			)
			(pin input line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "DAC_R_{SET}")
				(number "24")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "IOUT")
				(number "21")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "~{IOUT}")
				(number "20")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "LOOP_FILTER")
				(number "12")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "DACBP")
				(number "23")
			)
			(pin power_in line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "SYNC_IN")
				(number "44")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "OSK")
				(number "46")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "PWRDWNCTL")
				(number "35")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AD9954"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 27.94 0)
		)
		(property "Value" "AD9954"
			(at -13.97 25.4 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP3.5x3.5mm"
			(at 33.02 -29.21 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/AD9954.pdf"
			(at 39.37 -31.75 0)
		)
		(property "Description" "14-Bit Direct Digital Synthesizer with 400MSPS DAC, 1.8V, TQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Direct Digital Synthesizer DDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AD9954_0_1")
		(symbol "AD9954_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "RESET")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "I/OUPDATE")
				(number "1")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "SYNC_CLK")
				(number "45")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "OSC/REFCLK")
				(number "9")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "~{OSC/REFCLK}")
				(number "8")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "CLKMODESELECT")
				(number "11")
			)
			(pin output line
				(at -17.78 0 0)
				(length 3.81)
				(name "CRYSTALOUT")
				(number "10")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "SDO")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "SDIO")
				(number "41")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "SCLK")
				(number "40")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "~{CS}")
				(number "39")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "IOSYNC")
				(number "37")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "DVDD_I/O")
				(number "43")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "DGND")
				(number "3")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "DGND")
				(number "33")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "DGND")
				(number "42")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "DVDD")
				(number "2")
			)
			(pin passive line
				(at 2.54 27.94 270)
				(length 3.81)
				(hide yes)
				(name "DVDD")
				(number "34")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "14")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "15")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "17")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "22")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "26")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "32")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "49")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "AGND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "7")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "13")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "16")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "18")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "19")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "25")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "27")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "29")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 3.81)
				(name "AVDD")
				(number "4")
			)
			(pin passive line
				(at 5.08 27.94 270)
				(length 3.81)
				(hide yes)
				(name "AVDD")
				(number "6")
			)
			(pin input line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "DAC_R_{SET}")
				(number "24")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "IOUT")
				(number "21")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "~{IOUT}")
				(number "20")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "COMP_IN")
				(number "30")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "~{COMP_IN}")
				(number "31")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "COMP_OUT")
				(number "28")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "LOOP_FILTER")
				(number "12")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "DACBP")
				(number "23")
			)
			(pin power_in line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "SYNC_IN")
				(number "44")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "OSK")
				(number "46")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "PWRDWNCTL")
				(number "35")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "PS0")
				(number "47")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "PS1")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AM26LS31CD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "AM26LS31CD"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 25.4 -24.13 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/am26ls31.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "32Mbps 3.3V RS485 Quad Line Drivers, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver rs485 rs422 differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AM26LS31CD_0_1")
		(symbol "AM26LS31CD_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "1A")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "2A")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{G}")
				(number "12")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "3A")
				(number "9")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "4A")
				(number "15")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "1Y")
				(number "2")
			)
			(pin tri_state line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "1Z")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "2Y")
				(number "6")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "2Z")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "3Y")
				(number "10")
			)
			(pin tri_state line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "3Z")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "4Y")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "4Z")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AM26LV32xD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "AM26LV32xD"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 25.4 -24.13 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/am26lv32.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "32Mbps 3.3V RS485 Quad Line Receivers, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "receiver rs485 rs422 differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AM26LV32xD_0_1")
		(symbol "AM26LV32xD_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "1A")
				(number "2")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "1B")
				(number "1")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "2A")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "2B")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{G}")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "3A")
				(number "10")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "3B")
				(number "9")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "4A")
				(number "14")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "4B")
				(number "15")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "1Y")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "2Y")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "3Y")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "4Y")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AM26LV32xNS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "AM26LV32xNS"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_5.3x10.2mm_P1.27mm"
			(at 25.4 -24.13 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/am26lv32.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "32Mbps 3.3V RS485 Quad Line Receivers, SO-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "receiver rs485 rs422 differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AM26LV32xNS_0_1")
		(symbol "AM26LV32xNS_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "1A")
				(number "2")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "1B")
				(number "1")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "2A")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "2B")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "G")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{G}")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "3A")
				(number "10")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "3B")
				(number "9")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "4A")
				(number "14")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "4B")
				(number "15")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "1Y")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "2Y")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "3Y")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "4Y")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CDCLVP1102RGT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 12.7 0)
		)
		(property "Value" "CDCLVP1102RGT"
			(at 7.62 12.7 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.6x1.6mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/cdclvp1102.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Two-LVPECL Output, High-Performance Clock Buffer, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Clock Buffer LVDS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CDCLVP1102RGT_0_0"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "INP")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "INN")
				(number "7")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUTP0")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUTN0")
				(number "10")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUTP1")
				(number "11")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUTN1")
				(number "12")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VAC_REF")
				(number "8")
			)
		)
		(symbol "CDCLVP1102RGT_0_1")
		(embedded_fonts no)
	)
	(symbol "CH376T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 20.32 0)
		)
		(property "Value" "CH376T"
			(at 6.35 20.32 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.mpja.com/download/ch376ds1.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "File Management USB Flash Card SD Interface, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Mass-Storage SD Card Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CH376T_0_1")
		(symbol "CH376T_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "RSTI")
				(number "2")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "SDI")
				(number "15")
			)
			(pin tri_state line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "SDO")
				(number "16")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "SCK")
				(number "14")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "~{SCS}")
				(number "13")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "~{SPI}")
				(number "3")
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "~{INT}")
				(number "1")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "RXD")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "TXD")
				(number "4")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 3.81)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 2.54 22.86 270)
				(length 3.81)
				(name "V3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "UD+")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "UD-")
				(number "9")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "SD_DI")
				(number "6")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "SD_DO")
				(number "18")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "SD_CK")
				(number "19")
			)
			(pin open_collector line
				(at 15.24 0 180)
				(length 3.81)
				(name "SD_CS")
				(number "17")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "XI")
				(number "11")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 3.81)
				(name "XO")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS90C124"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.478 34.29 0)
		)
		(property "Value" "DS90C124"
			(at 14.478 34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 0 -48.26 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ds90c241.pdf"
			(at -43.18 2.54 0)
		)
		(property "Description" "DC-Balanced 24-Bit FPD-Link II Deserializer, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC-Balanced 24-Bit FPD-Link II Deserializer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "DS90C124_0_1")
		(symbol "DS90C124_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "RIN+")
				(number "41")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "RIN-")
				(number "42")
			)
			(pin input clock
				(at -17.78 12.7 0)
				(length 2.54)
				(name "RRFB")
				(number "43")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "RPWDNB")
				(number "1")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "REN")
				(number "48")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RESRVD")
				(number "2")
			)
			(pin power_in line
				(at -12.7 -38.1 90)
				(length 2.54)
				(name "VSSIR")
				(number "40")
			)
			(pin power_in line
				(at -10.16 35.56 270)
				(length 2.54)
				(name "VDDIR")
				(number "39")
			)
			(pin power_in line
				(at -10.16 -38.1 90)
				(length 2.54)
				(name "VSSPR0")
				(number "46")
			)
			(pin power_in line
				(at -7.62 35.56 270)
				(length 2.54)
				(name "VDDPR0")
				(number "47")
			)
			(pin power_in line
				(at -7.62 -38.1 90)
				(length 2.54)
				(name "VSSPR1")
				(number "44")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 2.54)
				(name "VDDPR1")
				(number "45")
			)
			(pin power_in line
				(at -5.08 -38.1 90)
				(length 2.54)
				(name "VSSOR1")
				(number "29")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "VDDOR1")
				(number "30")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "VSSOR2")
				(number "19")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDDOR2")
				(number "20")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VDDOR3")
				(number "7")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "VSSOR3")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSSR0")
				(number "35")
			)
			(pin power_in line
				(at 5.08 35.56 270)
				(length 2.54)
				(name "VDDR0")
				(number "36")
			)
			(pin power_in line
				(at 5.08 -38.1 90)
				(length 2.54)
				(name "VSSR1")
				(number "38")
			)
			(pin power_in line
				(at 7.62 35.56 270)
				(length 2.54)
				(name "VDDR1")
				(number "37")
			)
			(pin output line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "ROUT0")
				(number "34")
			)
			(pin output line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "ROUT1")
				(number "33")
			)
			(pin output line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "ROUT2")
				(number "32")
			)
			(pin output line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "ROUT3")
				(number "31")
			)
			(pin output line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "ROUT4")
				(number "28")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "ROUT5")
				(number "27")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "ROUT6")
				(number "26")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "ROUT7")
				(number "25")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "ROUT8")
				(number "24")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "ROUT9")
				(number "23")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "ROUT10")
				(number "22")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "ROUT11")
				(number "21")
			)
			(pin output line
				(at 20.32 0 180)
				(length 2.54)
				(name "ROUT12")
				(number "16")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "ROUT13")
				(number "15")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "ROUT14")
				(number "14")
			)
			(pin output line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "ROUT15")
				(number "13")
			)
			(pin output line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "ROUT16")
				(number "12")
			)
			(pin output line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "ROUT17")
				(number "11")
			)
			(pin output line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "ROUT18")
				(number "10")
			)
			(pin output line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "ROUT19")
				(number "9")
			)
			(pin output line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "ROUT20")
				(number "6")
			)
			(pin output line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "ROUT21")
				(number "5")
			)
			(pin output line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "ROUT22")
				(number "4")
			)
			(pin output line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "ROUT23")
				(number "3")
			)
			(pin output clock
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "RCLK")
				(number "18")
			)
			(pin output line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "LOCK")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS90C241"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.764 29.21 0)
		)
		(property "Value" "DS90C241"
			(at 13.97 29.21 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 0 -45.72 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ds90c241.pdf"
			(at -7.62 -5.08 0)
		)
		(property "Description" "DC-Balanced 24-Bit FPD-Link II Serializer, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC-Balanced 24-Bit FPD-Link II Serializer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "DS90C241_0_1")
		(symbol "DS90C241_1_1"
			(pin input line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "DIN0")
				(number "25")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "DIN1")
				(number "26")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "DIN2")
				(number "27")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "DIN3")
				(number "28")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "DIN4")
				(number "29")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "DIN5")
				(number "32")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "DIN6")
				(number "33")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "DIN7")
				(number "34")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "DIN8")
				(number "35")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "DIN9")
				(number "36")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "DIN10")
				(number "37")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "DIN11")
				(number "38")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "DIN12")
				(number "39")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "DIN13")
				(number "40")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "DIN14")
				(number "41")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "DIN15")
				(number "44")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "DIN16")
				(number "45")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "DIN17")
				(number "46")
			)
			(pin input line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "DIN18")
				(number "47")
			)
			(pin input line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "DIN19")
				(number "48")
			)
			(pin input line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "DIN20")
				(number "1")
			)
			(pin input line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "DIN21")
				(number "2")
			)
			(pin input line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "DIN22")
				(number "3")
			)
			(pin input line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "DIN23")
				(number "4")
			)
			(pin power_in line
				(at -7.62 30.48 270)
				(length 2.54)
				(name "VDDIT")
				(number "42")
			)
			(pin power_in line
				(at -7.62 -38.1 90)
				(length 2.54)
				(name "VSSIT")
				(number "43")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "VDDPT0")
				(number "16")
			)
			(pin power_in line
				(at -5.08 -38.1 90)
				(length 2.54)
				(name "VSSPT0")
				(number "17")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDDPT1")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "VSSPT1")
				(number "15")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "24")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDDT")
				(number "30")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "VSST")
				(number "31")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "VDDL")
				(number "7")
			)
			(pin power_in line
				(at 5.08 -38.1 90)
				(length 2.54)
				(name "VSSL")
				(number "6")
			)
			(pin power_in line
				(at 7.62 30.48 270)
				(length 2.54)
				(name "VDDDR")
				(number "22")
			)
			(pin power_in line
				(at 7.62 -38.1 90)
				(length 2.54)
				(name "VSSDR")
				(number "21")
			)
			(pin output line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "DOUT+")
				(number "20")
			)
			(pin output line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "DOUT-")
				(number "19")
			)
			(pin input clock
				(at 20.32 20.32 180)
				(length 2.54)
				(name "TCLK")
				(number "10")
			)
			(pin input clock
				(at 20.32 17.78 180)
				(length 2.54)
				(name "TRFB")
				(number "11")
			)
			(pin input line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "VODSEL")
				(number "12")
			)
			(pin input line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "DEN")
				(number "18")
			)
			(pin input line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PRE")
				(number "23")
			)
			(pin input line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "TPWDNB")
				(number "9")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "DCAOFF")
				(number "5")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "DCBOFF")
				(number "8")
			)
			(pin input line
				(at 20.32 0 180)
				(length 2.54)
				(name "RESRVD")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS90C402"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "DS90C402"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ds90c402.pdf"
			(at -17.78 -21.59 0)
		)
		(property "Description" "Dual LVDS Receiver, >155Mbps, 5V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LVDS Receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DS90C402_0_1")
		(symbol "DS90C402_1_0"
			(text "R"
				(at -0.635 5.08 0)
			)
			(text "R"
				(at -0.635 -5.08 0)
			)
		)
		(symbol "DS90C402_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "RI1+")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RI1-")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RI2+")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RI2-")
				(number "8")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RO1")
				(number "2")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "RO2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS90LV011A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "DS90LV011A"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ds90lv011a.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "LVDS Single High Speed Differential Driver, 400Mbps, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "DS90LV011A_1_0"
			(text "D"
				(at -1.905 0 0)
			)
		)
		(symbol "DS90LV011A_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "OUT+")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "OUT-")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS90LV027A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "DS90LV027A"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ds90lv027a.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "LVDS Dual High Speed Differential Driver, >600MBps, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual LVDS Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DS90LV027A_1_0"
			(text "D1"
				(at -1.905 5.08 0)
			)
			(text "D2"
				(at -1.905 -5.08 0)
			)
		)
		(symbol "DS90LV027A_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DI1")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DI2")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DO+1")
				(number "7")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DO-1")
				(number "8")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DO+2")
				(number "6")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DO-2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FD1771"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "FD1771"
			(at 8.382 24.384 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://amaus.net/static/S100/western%20digital/datasheet/Western%20Digital%20FD1771%20Specification%20197710.pdf"
			(at 0 0 0)
		)
		(property "Description" "Floppy disk controller, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Floppy disk controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "FD1771_0_1")
		(symbol "FD1771_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "~{WE}")
				(number "2")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "~{CS}")
				(number "3")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{RE}")
				(number "4")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin tri_state line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "DI0")
				(number "7")
			)
			(pin tri_state line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DI1")
				(number "8")
			)
			(pin tri_state line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DI2")
				(number "9")
			)
			(pin tri_state line
				(at -12.7 0 0)
				(length 2.54)
				(name "DI3")
				(number "10")
			)
			(pin tri_state line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DI4")
				(number "11")
			)
			(pin tri_state line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DI5")
				(number "12")
			)
			(pin tri_state line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "DI6")
				(number "13")
			)
			(pin tri_state line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DI7")
				(number "14")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{PH1}/STEP")
				(number "15")
			)
			(pin output line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "~{PH2}/DIRC")
				(number "16")
			)
			(pin output line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "PH3")
				(number "17")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "~{3PM}")
				(number "18")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "~{MR}")
				(number "19")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "40")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "VBB")
				(number "1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "INTRQ")
				(number "39")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DRQ")
				(number "38")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{DINT}")
				(number "37")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{WPRT}")
				(number "36")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{IP}")
				(number "35")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{TR00}")
				(number "34")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{WF}")
				(number "33")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "READY")
				(number "32")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "WD")
				(number "31")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "WG")
				(number "30")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "TG43")
				(number "29")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "FDDATA")
				(number "27")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "FDCLK")
				(number "26")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{XTDS}")
				(number "25")
			)
			(pin input clock
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "CLK")
				(number "24")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "HLT")
				(number "23")
			)
			(pin input line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "~{TEST}")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FIN1019M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "FIN1019M"
			(at -10.16 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FIN1019-D.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "3.3V LVDS High Speed Differential Driver/Receiver, 400Mbps, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "lvds driver receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "FIN1019M_0_0"
			(text "D"
				(at -1.905 -5.08 0)
			)
			(text "R"
				(at 0 5.08 0)
			)
		)
		(symbol "FIN1019M_0_1")
		(symbol "FIN1019M_1_1"
			(pin tri_state line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RO")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{RE}")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "2")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DE")
				(number "1")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin no_connect line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 12.7 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 12.7 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 12.7 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "RI+")
				(number "10")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "RI-")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DO+")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DO-")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FIN1019MTC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "FIN1019MTC"
			(at -11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at -1.27 -16.51 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FIN1019-D.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "3.3V LVDS High Speed Differential Driver/Receiver, 400Mbps, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "lvds driver receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "FIN1019MTC_0_0"
			(text "D"
				(at -1.905 -5.08 0)
			)
			(text "R"
				(at 0 5.08 0)
			)
		)
		(symbol "FIN1019MTC_0_1")
		(symbol "FIN1019MTC_1_1"
			(pin tri_state line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RO")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{RE}")
				(number "8")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "2")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DE")
				(number "1")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin no_connect line
				(at 0 12.7 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 12.7 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 12.7 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 12.7 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "RI+")
				(number "10")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "RI-")
				(number "9")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DO+")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DO-")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HT12D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "HT12D"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_SO:SOP-20_7.5x12.8mm_P1.27mm"
			(at 15.24 20.32 0)
		)
		(property "Datasheet" "https://www.holtek.com/documents/10179/116711/2_12dv120.pdf"
			(at 17.78 15.24 0)
		)
		(property "Description" "2^12 serial decoder, SOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Serial Decoder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HT12D_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "DIN")
				(number "15")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A6")
				(number "8")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A7")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "10")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "VT")
				(number "18")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "D8")
				(number "11")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "D9")
				(number "12")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "D10")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "D11")
				(number "14")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OSC1")
				(number "17")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "OSC2")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HT12E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "HT12E"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_SO:SOP-20_7.5x12.8mm_P1.27mm"
			(at 15.24 20.32 0)
		)
		(property "Datasheet" "https://www.holtek.com/documents/10179/116711/2_12ev120.pdf"
			(at 17.78 15.24 0)
		)
		(property "Description" "2^12 serial encoder, SOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Serial Encoder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HT12E_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "~{TE}")
				(number "15")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A6")
				(number "8")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A7")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "10")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at 7.62 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "DOUT")
				(number "18")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "AD8")
				(number "11")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "AD9")
				(number "12")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "AD10")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "AD11")
				(number "14")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OSC1")
				(number "17")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "OSC2")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1518"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "LTC1518"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 25.4 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/15189fa.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "52Mbps Precision Delay RS485 Quad Line Receivers"
			(at 0 0 0)
		)
		(property "ki_keywords" "receiver rs485 rs422 differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*16*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC1518_0_1")
		(symbol "LTC1518_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "B1")
				(number "1")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A2")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "B2")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A3")
				(number "10")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "B3")
				(number "9")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A4")
				(number "14")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "B4")
				(number "15")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin tri_state line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "Out1")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "Out2")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "Out3")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "Out4")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1519"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "LTC1519"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/15189fa.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "52Mbps Precision Delay RS485 Quad Line Receivers"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "receiver rs485 rs422 differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*16*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC1519_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "B1")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A2")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "B2")
				(number "7")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "EN12")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "Out1")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "Out2")
				(number "5")
			)
		)
		(symbol "LTC1519_2_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A3")
				(number "10")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "B3")
				(number "9")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A4")
				(number "14")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "B4")
				(number "15")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "EN34")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "Out3")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "Out4")
				(number "13")
			)
		)
		(symbol "LTC1519_3_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
		)
		(symbol "LTC1519_3_3")
		(embedded_fonts no)
	)
	(symbol "LTC1688"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "LTC1688"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 25.4 -21.59 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/16889fa.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "100Mbps RS485 Hot Swapable Quad Drivers"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver rs485 rs422 differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*16*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC1688_0_1")
		(symbol "LTC1688_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "DI1")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "DI2")
				(number "7")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{EN}")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "DI3")
				(number "9")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "DI4")
				(number "15")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "DO1A")
				(number "2")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DO1B")
				(number "3")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DO2A")
				(number "6")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DO2B")
				(number "5")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DO3A")
				(number "10")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "DO3B")
				(number "11")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "DO4A")
				(number "14")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "DO4B")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC1689"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "LTC1689"
			(at 6.35 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/16889fa.pdf"
			(at 5.08 -7.62 0)
		)
		(property "Description" "100Mbps RS485 Hot Swapable Quad Drivers"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "driver rs485 rs422 differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*16*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC1689_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DI1")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DI2")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "EN12")
				(number "4")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DO1A")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DO1B")
				(number "3")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "DO2A")
				(number "6")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DO2B")
				(number "5")
			)
		)
		(symbol "LTC1689_2_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DI3")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DI4")
				(number "15")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "EN34")
				(number "12")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DO3A")
				(number "10")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DO3B")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "DO4A")
				(number "14")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DO4B")
				(number "13")
			)
		)
		(symbol "LTC1689_3_1"
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6957xDD-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -13.97 0)
		)
		(property "Value" "LTC6957xDD-1"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x3mm_P0.45mm_EP1.65x2.38mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6957fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Phase Noise, Dual Output Buffer/Driver/Logic Converter, LVPECL, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "LTC clock converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "LTC6957xDD-1_0_1")
		(symbol "LTC6957xDD-1_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN-")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "FILTA")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FILTB")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SD1")
				(number "12")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SD2")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V+")
				(number "2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin open_emitter line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT1-")
				(number "10")
			)
			(pin open_emitter line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1+")
				(number "11")
			)
			(pin open_emitter line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2-")
				(number "9")
			)
			(pin open_emitter line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUT2+")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6957xDD-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -13.97 0)
		)
		(property "Value" "LTC6957xDD-2"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x3mm_P0.45mm_EP1.65x2.38mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6957fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Phase Noise, Dual Output Buffer/Driver/Logic Converter, LVDS, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "LTC clock converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "LTC6957xDD-2_0_1")
		(symbol "LTC6957xDD-2_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN-")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "FILTA")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FILTB")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SD1")
				(number "12")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SD2")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V+")
				(number "2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT1-")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1+")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2-")
				(number "9")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUT2+")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6957xDD-3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -13.97 0)
		)
		(property "Value" "LTC6957xDD-3"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x3mm_P0.45mm_EP1.65x2.38mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6957fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Phase Noise, Dual Output Buffer/Driver/Logic Converter, CMOS In-Phase Outputs, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "LTC clock converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "LTC6957xDD-3_0_1")
		(symbol "LTC6957xDD-3_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN-")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "FILTA")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FILTB")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SD1")
				(number "12")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SD2")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V+")
				(number "2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin output line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDOUT")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6957xMS-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -13.97 0)
		)
		(property "Value" "LTC6957xMS-1"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-12_3x4.039mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6957fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Phase Noise, Dual Output Buffer/Driver/Logic Converter, LVPECL, MSOP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "LTC clock converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC6957xMS-1_0_1")
		(symbol "LTC6957xMS-1_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN-")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "FILTA")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FILTB")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SD1")
				(number "12")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SD2")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin open_emitter line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT1-")
				(number "10")
			)
			(pin open_emitter line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1+")
				(number "11")
			)
			(pin open_emitter line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2-")
				(number "9")
			)
			(pin open_emitter line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUT2+")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6957xMS-2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -13.97 0)
		)
		(property "Value" "LTC6957xMS-2"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-12_3x4.039mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6957fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Phase Noise, Dual Output Buffer/Driver/Logic Converter, LVDS, MSOP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "LTC clock converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC6957xMS-2_0_1")
		(symbol "LTC6957xMS-2_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN-")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "FILTA")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FILTB")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SD1")
				(number "12")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SD2")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUT1-")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1+")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2-")
				(number "9")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUT2+")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC6957xMS-3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 -13.97 0)
		)
		(property "Value" "LTC6957xMS-3"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-12_3x4.039mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6957fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Phase Noise, Dual Output Buffer/Driver/Logic Converter, CMOS In-Phase Outputs, MSOP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "LTC clock converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC6957xMS-3_0_1")
		(symbol "LTC6957xMS-3_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "IN+")
				(number "3")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "IN-")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "FILTA")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "FILTB")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "SD1")
				(number "12")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "SD2")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "V+")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin output line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDOUT")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT1")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX6816"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 8.89 0)
		)
		(property "Value" "MAX6816"
			(at 5.08 -8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-143"
			(at 16.51 -11.43 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/1896.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single Switch  Debouncer, SOT-143"
			(at 0 0 0)
		)
		(property "ki_keywords" "Switch Debouncer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*143*"
			(at 0 0 0)
		)
		(symbol "MAX6816_0_1")
		(symbol "MAX6816_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC100EPT22D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "MC100EPT22D"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -24.13 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC100EPT22-D.PDF"
			(at 1.27 -10.16 0)
		)
		(property "Description" "3.3 V Dual LVTTL/LVCMOS to Differential LVPECL Translator, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "PECL buffer interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC100EPT22D_0_1")
		(symbol "MC100EPT22D_1_0")
		(symbol "MC100EPT22D_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D0")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "D1")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Q0")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{Q0}")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Q1")
				(number "3")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{Q1}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC100EPT22DT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "MC100EPT22DT"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at -2.54 -24.13 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC100EPT22-D.PDF"
			(at 1.27 -10.16 0)
		)
		(property "Description" "3.3 V Dual LVTTL/LVCMOS to Differential LVPECL Translator, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "PECL buffer interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC100EPT22DT_0_1")
		(symbol "MC100EPT22DT_1_0")
		(symbol "MC100EPT22DT_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D0")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "D1")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Q0")
				(number "1")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{Q0}")
				(number "2")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Q1")
				(number "3")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{Q1}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC6840"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 28.575 0)
		)
		(property "Value" "MC6840"
			(at -2.54 26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 1.27 -27.94 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC6840.pdf"
			(at 1.27 -30.48 0)
		)
		(property "Description" "Motorola Programmable Timer Module, 1.0MHz, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "PTM MC6800"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "MC6840_0_1")
		(symbol "MC6840_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "D0")
				(number "25")
			)
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D1")
				(number "24")
			)
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D2")
				(number "23")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D3")
				(number "22")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D4")
				(number "21")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D5")
				(number "20")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D6")
				(number "19")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D7")
				(number "18")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "R/~{W}")
				(number "13")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RS0")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RS1")
				(number "11")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RS2")
				(number "12")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{CS0}")
				(number "15")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "CS1")
				(number "16")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "E")
				(number "17")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "~{RESET}")
				(number "8")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "~{IRQ}")
				(number "9")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "~{G1}")
				(number "26")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{C1}")
				(number "28")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "O1")
				(number "27")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{G2}")
				(number "2")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{C2}")
				(number "4")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "O2")
				(number "3")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{G3}")
				(number "5")
			)
			(pin input line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{C3}")
				(number "7")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "O3")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC6843"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 34.29 0)
		)
		(property "Value" "MC6843"
			(at 10.414 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 -31.75 0)
		)
		(property "Datasheet" "http://www.datasheetarchive.com/pdf/download.php?id=355f4f5379c550317997643252fd5cac1bb08e&type=M&query=MC6843P"
			(at 0 0 0)
		)
		(property "Description" "Floppy Disc Controller, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FDC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "MC6843_0_1")
		(symbol "MC6843_1_1"
			(pin output line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "TxRQ")
				(number "36")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "TxAck")
				(number "21")
			)
			(pin output line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "BD")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D0")
				(number "33")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D1")
				(number "32")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D2")
				(number "31")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D3")
				(number "30")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D4")
				(number "29")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D5")
				(number "28")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D6")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "D7")
				(number "26")
			)
			(pin open_collector line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "37")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CLK")
				(number "12")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "7")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "R/~{W}")
				(number "22")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "E")
				(number "23")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "RS0")
				(number "19")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "RS1")
				(number "18")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "RS2")
				(number "17")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "~{CS}")
				(number "24")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin no_connect line
				(at 10.16 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin input line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "DCK")
				(number "9")
			)
			(pin output line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "VFOC")
				(number "14")
			)
			(pin input line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "RDT")
				(number "38")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "WDT")
				(number "39")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "WGT")
				(number "6")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "HDR")
				(number "8")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "STP")
				(number "15")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "HLD")
				(number "16")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "LCT")
				(number "10")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "FIR")
				(number "3")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "FI")
				(number "4")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "WPT")
				(number "5")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "IDX")
				(number "11")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TRZ")
				(number "40")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "RDY")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC6844"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.382 34.544 0)
		)
		(property "Value" "MC6844"
			(at 12.7 34.544 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 -31.75 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets/560/501527_DS.pdf"
			(at 0 0 0)
		)
		(property "Description" "Direct Memory Access Controller 1MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Direct Memory Access Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "MC6844_0_1")
		(symbol "MC6844_1_1"
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "D0")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "D1")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "D2")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "D3")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "D4")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "D5")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "D6")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "D7")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "A0")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "A1")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "A2")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "A3")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "A4")
				(number "8")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "R/~{W}")
				(number "3")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "E")
				(number "40")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "Tx_RQ0")
				(number "32")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "Tx_RQ1")
				(number "31")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "Tx_RQ2")
				(number "30")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "Tx_RQ3")
				(number "29")
			)
			(pin input line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "DGRNT")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "~{CS}/Tx_AKB")
				(number "2")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "A5")
				(number "9")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "A6")
				(number "10")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "A7")
				(number "11")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "A8")
				(number "12")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "A9")
				(number "13")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "A10")
				(number "14")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "A11")
				(number "15")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "A12")
				(number "16")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "A13")
				(number "17")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "A14")
				(number "18")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "A15")
				(number "19")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "~{IRQ}/~{DEND}")
				(number "33")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "~{Tx_STB}")
				(number "34")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "Tx_AKA")
				(number "35")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "~{DRQ1}")
				(number "37")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "~{DRQ2}")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NB3N551MN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "NB3N551MN"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NB3N551-D.PDF"
			(at -6.35 8.89 0)
		)
		(property "Description" "1:4 Low Skew Clock Buffer, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "clock buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "NB3N551MN_0_1")
		(symbol "NB3N551MN_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "ICLK")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OE")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "EP")
				(number "9")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Q1")
				(number "2")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Q2")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "Q3")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Q4")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ONET1191PRGT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "ONET1191PRGT"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-16-1EP_3x3mm_P0.5mm_EP1.68x1.68mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/onet1191p.pdf"
			(at 0 8.89 0)
		)
		(property "Description" "11.3-Gbps Limiting Amplifier, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "limiting amplifier gigabit ethernet sfp sfp+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ONET1191PRGT_0_1")
		(symbol "ONET1191PRGT_1_1"
			(pin passive line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "COC-")
				(number "5")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "COC+")
				(number "6")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DIN+")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DIN-")
				(number "8")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DISABLE")
				(number "11")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "TH")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DOUT+")
				(number "15")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DOUT-")
				(number "14")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "VAR")
				(number "12")
			)
			(pin open_collector line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "LOS")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9306"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "PCA9306"
			(at 5.08 11.43 0)
		)
		(property "Footprint" ""
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pca9306.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "Dual bidirectional I2C Bus and SMBus voltage level translator"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual bidirectional I2C Bus and SMBus voltage level translator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*2.95x2.8mm*P0.65mm* VSSOP*2.3x2mm*P0.5mm* X2SON*1.4x1mm*P0.35mm*"
			(at 0 0 0)
		)
		(symbol "PCA9306_0_1")
		(symbol "PCA9306_1_1"
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCL1")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SDA1")
				(number "4")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VREF1")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VREF2")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "EN")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL2")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SDA2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9600D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "PCA9600D"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9600.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "Dual bidirectional bus buffer, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PCA9600D_0_1")
		(symbol "PCA9600D_1_1"
			(pin bidirectional line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "SX")
				(number "1")
			)
			(pin bidirectional line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "SY")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "TX")
				(number "3")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "RX")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "TY")
				(number "5")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "RY")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9600DP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 8.89 0)
		)
		(property "Value" "PCA9600DP"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9600.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "Dual bidirectional bus buffer, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCA9600DP_0_1")
		(symbol "PCA9600DP_1_1"
			(pin bidirectional line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "SX")
				(number "1")
			)
			(pin bidirectional line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "SY")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "TX")
				(number "3")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "RX")
				(number "2")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "TY")
				(number "5")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "RY")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9615DP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "PCA9615DP"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9615.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "Dual bidirectional hot-swap multipoint bus buffer, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Differential SMBus/I2C buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PCA9615DP_0_1")
		(symbol "PCA9615DP_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "EN")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "SDA")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCL")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "V_{DD(A)}")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{DD(B)}")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "V_{SS}")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DSDAP")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DSDAM")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DSCLP")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DSCLM")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCI9030-PQFP176"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.304 125.73 0)
		)
		(property "Value" "PCI9030-PQFP176"
			(at 14.224 125.73 0)
		)
		(property "Footprint" "Package_QFP:LQFP-176_24x24mm_P0.5mm"
			(at 0 -139.7 0)
		)
		(property "Datasheet" "http://lhcb-online.web.cern.ch/lhcb-online/ecs/ccpc/docs/plc-9030-databook.pdf"
			(at 0 0 0)
		)
		(property "Description" "PCI SMARTarget I/O Accelerator"
			(at 0 0 0)
		)
		(property "ki_keywords" "PCI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*24x24mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PCI9030-PQFP176_1_1"
			(pin output line
				(at -27.94 119.38 0)
				(length 7.62)
				(name "EECS")
				(number "158")
			)
			(pin output line
				(at -27.94 116.84 0)
				(length 7.62)
				(name "EESK")
				(number "160")
			)
			(pin output line
				(at -27.94 114.3 0)
				(length 7.62)
				(name "EEDI")
				(number "161")
			)
			(pin input line
				(at -27.94 111.76 0)
				(length 7.62)
				(name "EEDO")
				(number "159")
			)
			(pin input clock
				(at -27.94 106.68 0)
				(length 7.62)
				(name "TCK")
				(number "165")
			)
			(pin input line
				(at -27.94 104.14 0)
				(length 7.62)
				(name "TMS")
				(number "166")
			)
			(pin input line
				(at -27.94 101.6 0)
				(length 7.62)
				(name "TDI")
				(number "168")
			)
			(pin input line
				(at -27.94 99.06 0)
				(length 7.62)
				(name "TRST#")
				(number "164")
			)
			(pin output line
				(at -27.94 96.52 0)
				(length 7.62)
				(name "TDO")
				(number "167")
			)
			(pin input line
				(at -27.94 93.98 0)
				(length 7.62)
				(name "BD-SEL#/TST")
				(number "112")
			)
			(pin bidirectional line
				(at -27.94 88.9 0)
				(length 7.62)
				(name "AD0")
				(number "50")
			)
			(pin bidirectional line
				(at -27.94 86.36 0)
				(length 7.62)
				(name "AD1")
				(number "49")
			)
			(pin bidirectional line
				(at -27.94 83.82 0)
				(length 7.62)
				(name "AD2")
				(number "48")
			)
			(pin bidirectional line
				(at -27.94 81.28 0)
				(length 7.62)
				(name "AD3")
				(number "47")
			)
			(pin bidirectional line
				(at -27.94 78.74 0)
				(length 7.62)
				(name "AD4")
				(number "46")
			)
			(pin bidirectional line
				(at -27.94 76.2 0)
				(length 7.62)
				(name "AD5")
				(number "43")
			)
			(pin bidirectional line
				(at -27.94 73.66 0)
				(length 7.62)
				(name "AD6")
				(number "42")
			)
			(pin bidirectional line
				(at -27.94 71.12 0)
				(length 7.62)
				(name "AD7")
				(number "41")
			)
			(pin bidirectional line
				(at -27.94 68.58 0)
				(length 7.62)
				(name "AD8")
				(number "39")
			)
			(pin bidirectional line
				(at -27.94 66.04 0)
				(length 7.62)
				(name "AD9")
				(number "38")
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 7.62)
				(name "AD10")
				(number "37")
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 7.62)
				(name "AD11")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 7.62)
				(name "AD12")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 7.62)
				(name "AD13")
				(number "34")
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 7.62)
				(name "AD14")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 7.62)
				(name "AD15")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 7.62)
				(name "AD16")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 45.72 0)
				(length 7.62)
				(name "AD17")
				(number "17")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 7.62)
				(name "AD18")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 7.62)
				(name "AD19")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "AD20")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 7.62)
				(name "AD21")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "AD22")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "AD23")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 7.62)
				(name "AD24")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "AD25")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 7.62)
				(name "AD26")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "AD27")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 7.62)
				(name "AD28")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "AD29")
				(number "175")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "AD30")
				(number "174")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "AD31")
				(number "173")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "C/BE0#")
				(number "40")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "C/BE1#")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 7.62)
				(name "C/BE2#")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "C/BE3#")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "PAR")
				(number "28")
			)
			(pin input clock
				(at -27.94 -7.62 0)
				(length 7.62)
				(name "PCLK")
				(number "172")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "RST#")
				(number "171")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "FRAME#")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "IRDY#")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "TRDY#")
				(number "22")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 7.62)
				(name "STOP#")
				(number "24")
			)
			(pin input line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "LOCK#")
				(number "25")
			)
			(pin input line
				(at -27.94 -27.94 0)
				(length 7.62)
				(name "IDSEL")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 7.62)
				(name "DEVSEL#")
				(number "23")
			)
			(pin output line
				(at -27.94 -33.02 0)
				(length 7.62)
				(name "PME#")
				(number "169")
			)
			(pin output line
				(at -27.94 -35.56 0)
				(length 7.62)
				(name "PERR#")
				(number "26")
			)
			(pin output line
				(at -27.94 -38.1 0)
				(length 7.62)
				(name "SERR#")
				(number "27")
			)
			(pin output line
				(at -27.94 -40.64 0)
				(length 7.62)
				(name "INTA#")
				(number "170")
			)
			(pin output line
				(at -27.94 -43.18 0)
				(length 7.62)
				(name "ENUM#")
				(number "51")
			)
			(pin output line
				(at -27.94 -45.72 0)
				(length 7.62)
				(name "LEDON#")
				(number "52")
			)
			(pin input line
				(at -27.94 -48.26 0)
				(length 7.62)
				(name "CPCISW")
				(number "54")
			)
			(pin power_in line
				(at -27.94 -53.34 0)
				(length 7.62)
				(name "VI/O")
				(number "53")
			)
			(pin power_in line
				(at -17.78 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "13")
			)
			(pin power_in line
				(at -15.24 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -12.7 132.08 270)
				(length 7.62)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -12.7 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "44")
			)
			(pin power_in line
				(at -10.16 132.08 270)
				(length 7.62)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at -10.16 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "57")
			)
			(pin power_in line
				(at -7.62 132.08 270)
				(length 7.62)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at -7.62 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "66")
			)
			(pin power_in line
				(at -5.08 132.08 270)
				(length 7.62)
				(name "VDD")
				(number "45")
			)
			(pin power_in line
				(at -5.08 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "78")
			)
			(pin power_in line
				(at -2.54 132.08 270)
				(length 7.62)
				(name "VDD")
				(number "56")
			)
			(pin power_in line
				(at -2.54 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "88")
			)
			(pin power_in line
				(at 0 132.08 270)
				(length 7.62)
				(name "VDD")
				(number "70")
			)
			(pin power_in line
				(at 0 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "101")
			)
			(pin power_in line
				(at 2.54 132.08 270)
				(length 7.62)
				(name "VDD")
				(number "85")
			)
			(pin power_in line
				(at 2.54 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "113")
			)
			(pin power_in line
				(at 5.08 132.08 270)
				(length 7.62)
				(name "VDD")
				(number "100")
			)
			(pin power_in line
				(at 5.08 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "122")
			)
			(pin power_in line
				(at 7.62 132.08 270)
				(length 7.62)
				(name "VDD")
				(number "117")
			)
			(pin power_in line
				(at 7.62 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "132")
			)
			(pin power_in line
				(at 10.16 132.08 270)
				(length 7.62)
				(name "VDD")
				(number "133")
			)
			(pin power_in line
				(at 10.16 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "146")
			)
			(pin power_in line
				(at 12.7 132.08 270)
				(length 7.62)
				(name "VDD")
				(number "162")
			)
			(pin power_in line
				(at 12.7 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "163")
			)
			(pin power_in line
				(at 15.24 -134.62 90)
				(length 7.62)
				(name "VSS")
				(number "176")
			)
			(pin input clock
				(at 27.94 121.92 180)
				(length 7.62)
				(name "LCLK")
				(number "145")
			)
			(pin output line
				(at 27.94 116.84 180)
				(length 7.62)
				(name "LRESETo#")
				(number "149")
			)
			(pin output clock
				(at 27.94 114.3 180)
				(length 7.62)
				(name "BCLKo")
				(number "71")
			)
			(pin input line
				(at 27.94 109.22 180)
				(length 7.62)
				(name "LREQ")
				(number "151")
			)
			(pin output line
				(at 27.94 106.68 180)
				(length 7.62)
				(name "LGNT")
				(number "150")
			)
			(pin input line
				(at 27.94 104.14 180)
				(length 7.62)
				(name "LINTi1")
				(number "152")
			)
			(pin input line
				(at 27.94 101.6 180)
				(length 7.62)
				(name "LINTi2")
				(number "153")
			)
			(pin input line
				(at 27.94 96.52 180)
				(length 7.62)
				(name "MODE")
				(number "76")
			)
			(pin input line
				(at 27.94 93.98 180)
				(length 7.62)
				(name "LPMESET")
				(number "103")
			)
			(pin output line
				(at 27.94 91.44 180)
				(length 7.62)
				(name "LPMINT#")
				(number "126")
			)
			(pin output line
				(at 27.94 86.36 180)
				(length 7.62)
				(name "CS0#")
				(number "147")
			)
			(pin output line
				(at 27.94 83.82 180)
				(length 7.62)
				(name "CS1#")
				(number "148")
			)
			(pin bidirectional line
				(at 27.94 81.28 180)
				(length 7.62)
				(name "GPIO2/CS2#")
				(number "156")
			)
			(pin bidirectional line
				(at 27.94 78.74 180)
				(length 7.62)
				(name "GPIO3/CS3#")
				(number "157")
			)
			(pin bidirectional line
				(at 27.94 76.2 180)
				(length 7.62)
				(name "GPIO1/LLOCKo#")
				(number "155")
			)
			(pin bidirectional line
				(at 27.94 73.66 180)
				(length 7.62)
				(name "GPIO0/WAITo#")
				(number "154")
			)
			(pin bidirectional line
				(at 27.94 68.58 180)
				(length 7.62)
				(name "GPIO8")
				(number "94")
			)
			(pin output line
				(at 27.94 66.04 180)
				(length 7.62)
				(name "ADS#")
				(number "138")
			)
			(pin output line
				(at 27.94 63.5 180)
				(length 7.62)
				(name "ALE")
				(number "75")
			)
			(pin output line
				(at 27.94 60.96 180)
				(length 7.62)
				(name "BLAST#")
				(number "139")
			)
			(pin input line
				(at 27.94 58.42 180)
				(length 7.62)
				(name "BTERM#")
				(number "144")
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 7.62)
				(name "GPIO4/LA27")
				(number "137")
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 7.62)
				(name "GPIO5/LA26")
				(number "136")
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "GPIO6/LA25")
				(number "135")
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "GPIO7/LA24")
				(number "134")
			)
			(pin output line
				(at 27.94 43.18 180)
				(length 7.62)
				(name "LA23")
				(number "131")
			)
			(pin output line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "LA22")
				(number "130")
			)
			(pin output line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "LA21")
				(number "129")
			)
			(pin output line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "LA20")
				(number "128")
			)
			(pin output line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "LA19")
				(number "127")
			)
			(pin output line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "LA18")
				(number "125")
			)
			(pin output line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "LA17")
				(number "124")
			)
			(pin output line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "LA16")
				(number "123")
			)
			(pin output line
				(at 27.94 22.86 180)
				(length 7.62)
				(name "LA15")
				(number "121")
			)
			(pin output line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "LA14")
				(number "120")
			)
			(pin output line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "LA13")
				(number "119")
			)
			(pin output line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "LA12")
				(number "118")
			)
			(pin output line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "LA11")
				(number "116")
			)
			(pin input line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "LA10")
				(number "115")
			)
			(pin output line
				(at 27.94 7.62 180)
				(length 7.62)
				(name "LA9")
				(number "114")
			)
			(pin output line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "LA8")
				(number "111")
			)
			(pin output line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "LA7")
				(number "110")
			)
			(pin output line
				(at 27.94 0 180)
				(length 7.62)
				(name "LA6")
				(number "109")
			)
			(pin output line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "LA5")
				(number "108")
			)
			(pin output line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "LA4")
				(number "107")
			)
			(pin output line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "LA3")
				(number "106")
			)
			(pin output line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "LA2")
				(number "105")
			)
			(pin output line
				(at 27.94 -15.24 180)
				(length 7.62)
				(name "LBE0#")
				(number "60")
			)
			(pin output line
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "LBE1#")
				(number "59")
			)
			(pin output line
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "LBE2#")
				(number "58")
			)
			(pin output line
				(at 27.94 -22.86 180)
				(length 7.62)
				(name "LBE3#")
				(number "55")
			)
			(pin output line
				(at 27.94 -27.94 180)
				(length 7.62)
				(name "LW/R#")
				(number "142")
			)
			(pin output line
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "WR#")
				(number "140")
			)
			(pin output line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "RD#")
				(number "141")
			)
			(pin input line
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "READY#")
				(number "143")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 7.62)
				(name "LD0")
				(number "104")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "LD1")
				(number "102")
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "LD2")
				(number "99")
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "LD3")
				(number "98")
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 7.62)
				(name "LD4")
				(number "97")
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 7.62)
				(name "LD5")
				(number "96")
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 7.62)
				(name "LD6")
				(number "95")
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 7.62)
				(name "LD7")
				(number "93")
			)
			(pin bidirectional line
				(at 27.94 -60.96 180)
				(length 7.62)
				(name "LD8")
				(number "92")
			)
			(pin bidirectional line
				(at 27.94 -63.5 180)
				(length 7.62)
				(name "LD9")
				(number "91")
			)
			(pin bidirectional line
				(at 27.94 -66.04 180)
				(length 7.62)
				(name "LD10")
				(number "90")
			)
			(pin bidirectional line
				(at 27.94 -68.58 180)
				(length 7.62)
				(name "LD11")
				(number "89")
			)
			(pin bidirectional line
				(at 27.94 -71.12 180)
				(length 7.62)
				(name "LD12")
				(number "87")
			)
			(pin bidirectional line
				(at 27.94 -73.66 180)
				(length 7.62)
				(name "LD13")
				(number "86")
			)
			(pin bidirectional line
				(at 27.94 -76.2 180)
				(length 7.62)
				(name "LD14")
				(number "84")
			)
			(pin bidirectional line
				(at 27.94 -78.74 180)
				(length 7.62)
				(name "LD15")
				(number "83")
			)
			(pin bidirectional line
				(at 27.94 -81.28 180)
				(length 7.62)
				(name "LD16")
				(number "82")
			)
			(pin bidirectional line
				(at 27.94 -83.82 180)
				(length 7.62)
				(name "LD17")
				(number "81")
			)
			(pin bidirectional line
				(at 27.94 -86.36 180)
				(length 7.62)
				(name "LD18")
				(number "80")
			)
			(pin bidirectional line
				(at 27.94 -88.9 180)
				(length 7.62)
				(name "LD19")
				(number "79")
			)
			(pin bidirectional line
				(at 27.94 -91.44 180)
				(length 7.62)
				(name "LD20")
				(number "77")
			)
			(pin bidirectional line
				(at 27.94 -93.98 180)
				(length 7.62)
				(name "LD21")
				(number "74")
			)
			(pin bidirectional line
				(at 27.94 -96.52 180)
				(length 7.62)
				(name "LD22")
				(number "73")
			)
			(pin bidirectional line
				(at 27.94 -99.06 180)
				(length 7.62)
				(name "LD23")
				(number "72")
			)
			(pin bidirectional line
				(at 27.94 -101.6 180)
				(length 7.62)
				(name "LD24")
				(number "69")
			)
			(pin bidirectional line
				(at 27.94 -104.14 180)
				(length 7.62)
				(name "LD25")
				(number "68")
			)
			(pin bidirectional line
				(at 27.94 -106.68 180)
				(length 7.62)
				(name "LD26")
				(number "67")
			)
			(pin bidirectional line
				(at 27.94 -109.22 180)
				(length 7.62)
				(name "LD27")
				(number "65")
			)
			(pin bidirectional line
				(at 27.94 -111.76 180)
				(length 7.62)
				(name "LD28")
				(number "64")
			)
			(pin bidirectional line
				(at 27.94 -114.3 180)
				(length 7.62)
				(name "LD29")
				(number "63")
			)
			(pin bidirectional line
				(at 27.94 -116.84 180)
				(length 7.62)
				(name "LD30")
				(number "62")
			)
			(pin bidirectional line
				(at 27.94 -119.38 180)
				(length 7.62)
				(name "LD31")
				(number "61")
			)
		)
		(embedded_fonts no)
	)
	(symbol "S5933_PQ160"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 107.95 0)
		)
		(property "Value" "S5933_PQ160"
			(at 11.684 107.95 0)
		)
		(property "Footprint" "Package_QFP:PQFP-160_28x28mm_P0.65mm"
			(at 0 -114.3 0)
		)
		(property "Datasheet" "http://datasheet.datasheetarchive.com/originals/distributors/Datasheets-35/DSA-684194.pdf"
			(at 0 0 0)
		)
		(property "Description" "PCI 2.1 Compliant Master/Slave Device, PQFP-160"
			(at 0 0 0)
		)
		(property "ki_keywords" "PCI 2.1 Compliant Master/Slave Device"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PQFP*28x28mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "S5933_PQ160_0_0"
			(pin power_in line
				(at -7.62 111.76 270)
				(length 5.08)
				(name "VCC")
				(number "31")
			)
			(pin power_in line
				(at -5.08 111.76 270)
				(length 5.08)
				(name "VCC")
				(number "51")
			)
			(pin power_in line
				(at -5.08 -111.76 90)
				(length 5.08)
				(name "VSS")
				(number "150")
			)
			(pin power_in line
				(at -2.54 -111.76 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin power_in line
				(at 0 111.76 270)
				(length 5.08)
				(name "VCC")
				(number "71")
			)
			(pin power_in line
				(at 0 -111.76 90)
				(length 5.08)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 2.54 111.76 270)
				(length 5.08)
				(name "VCC")
				(number "91")
			)
			(pin power_in line
				(at 2.54 -111.76 90)
				(length 5.08)
				(name "VSS")
				(number "70")
			)
			(pin power_in line
				(at 5.08 111.76 270)
				(length 5.08)
				(name "VCC")
				(number "111")
			)
			(pin power_in line
				(at 5.08 -111.76 90)
				(length 5.08)
				(name "VSS")
				(number "50")
			)
			(pin power_in line
				(at 7.62 111.76 270)
				(length 5.08)
				(name "VCC")
				(number "131")
			)
			(pin power_in line
				(at 7.62 -111.76 90)
				(length 5.08)
				(name "VSS")
				(number "90")
			)
			(pin power_in line
				(at 10.16 111.76 270)
				(length 5.08)
				(name "VCC")
				(number "151")
			)
			(pin power_in line
				(at 10.16 -111.76 90)
				(length 5.08)
				(name "VSS")
				(number "110")
			)
			(pin power_in line
				(at 12.7 -111.76 90)
				(length 5.08)
				(name "VSS")
				(number "130")
			)
		)
		(symbol "S5933_PQ160_0_1")
		(symbol "S5933_PQ160_1_0"
			(pin power_in line
				(at -2.54 111.76 270)
				(length 5.08)
				(name "VCC")
				(number "11")
			)
		)
		(symbol "S5933_PQ160_1_1"
			(pin bidirectional line
				(at -27.94 101.6 0)
				(length 7.62)
				(name "AD0")
				(number "56")
			)
			(pin bidirectional line
				(at -27.94 99.06 0)
				(length 7.62)
				(name "AD1")
				(number "55")
			)
			(pin bidirectional line
				(at -27.94 96.52 0)
				(length 7.62)
				(name "AD2")
				(number "54")
			)
			(pin bidirectional line
				(at -27.94 93.98 0)
				(length 7.62)
				(name "AD3")
				(number "52")
			)
			(pin bidirectional line
				(at -27.94 91.44 0)
				(length 7.62)
				(name "AD4")
				(number "48")
			)
			(pin bidirectional line
				(at -27.94 88.9 0)
				(length 7.62)
				(name "AD5")
				(number "47")
			)
			(pin bidirectional line
				(at -27.94 86.36 0)
				(length 7.62)
				(name "AD6")
				(number "46")
			)
			(pin bidirectional line
				(at -27.94 83.82 0)
				(length 7.62)
				(name "AD7")
				(number "44")
			)
			(pin bidirectional line
				(at -27.94 81.28 0)
				(length 7.62)
				(name "AD8")
				(number "42")
			)
			(pin bidirectional line
				(at -27.94 78.74 0)
				(length 7.62)
				(name "AD9")
				(number "40")
			)
			(pin bidirectional line
				(at -27.94 76.2 0)
				(length 7.62)
				(name "AD10")
				(number "39")
			)
			(pin bidirectional line
				(at -27.94 73.66 0)
				(length 7.62)
				(name "AD11")
				(number "38")
			)
			(pin bidirectional line
				(at -27.94 71.12 0)
				(length 7.62)
				(name "AD12")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 68.58 0)
				(length 7.62)
				(name "AD13")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 66.04 0)
				(length 7.62)
				(name "AD14")
				(number "34")
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 7.62)
				(name "AD15")
				(number "32")
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 7.62)
				(name "AD16")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 7.62)
				(name "AD17")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 7.62)
				(name "AD18")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 7.62)
				(name "AD19")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 7.62)
				(name "AD20")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 7.62)
				(name "AD21")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 45.72 0)
				(length 7.62)
				(name "AD22")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 7.62)
				(name "AD23")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 7.62)
				(name "AD24")
				(number "158")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "AD25")
				(number "156")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 7.62)
				(name "AD26")
				(number "155")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "AD27")
				(number "154")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "AD28")
				(number "152")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 7.62)
				(name "AD29")
				(number "148")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "AD30")
				(number "147")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 7.62)
				(name "AD31")
				(number "146")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "C/BE0#")
				(number "43")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 7.62)
				(name "C/BE1#")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "C/BE2#")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "C/BE3#")
				(number "159")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "PAR")
				(number "27")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "CLK")
				(number "142")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "RST#")
				(number "139")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 7.62)
				(name "FRAME#")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "IRDY#")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "TRDY#")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 7.62)
				(name "STOP#")
				(number "22")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "LOCK#")
				(number "23")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "IDSEL")
				(number "160")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "DEVSEL#")
				(number "20")
			)
			(pin output line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "REQ#")
				(number "144")
			)
			(pin input line
				(at -27.94 -22.86 0)
				(length 7.62)
				(name "GNT#")
				(number "143")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "PERR#")
				(number "24")
			)
			(pin output line
				(at -27.94 -27.94 0)
				(length 7.62)
				(name "SERR#")
				(number "26")
			)
			(pin output line
				(at -27.94 -33.02 0)
				(length 7.62)
				(name "INTA#")
				(number "58")
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 7.62)
				(name "EA0")
				(number "57")
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 7.62)
				(name "EA1")
				(number "61")
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 7.62)
				(name "EA2")
				(number "69")
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 7.62)
				(name "EA3")
				(number "73")
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 7.62)
				(name "EA4")
				(number "81")
			)
			(pin bidirectional line
				(at -27.94 -53.34 0)
				(length 7.62)
				(name "EA5")
				(number "89")
			)
			(pin bidirectional line
				(at -27.94 -55.88 0)
				(length 7.62)
				(name "EA6")
				(number "97")
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 7.62)
				(name "EA7")
				(number "101")
			)
			(pin bidirectional line
				(at -27.94 -60.96 0)
				(length 7.62)
				(name "EA8")
				(number "109")
			)
			(pin output line
				(at -27.94 -63.5 0)
				(length 7.62)
				(name "EA9")
				(number "113")
			)
			(pin output line
				(at -27.94 -66.04 0)
				(length 7.62)
				(name "EA10")
				(number "121")
			)
			(pin output line
				(at -27.94 -68.58 0)
				(length 7.62)
				(name "EA11")
				(number "129")
			)
			(pin output line
				(at -27.94 -71.12 0)
				(length 7.62)
				(name "EA12")
				(number "137")
			)
			(pin output line
				(at -27.94 -73.66 0)
				(length 7.62)
				(name "EA13")
				(number "141")
			)
			(pin bidirectional line
				(at -27.94 -76.2 0)
				(length 7.62)
				(name "EA14/FWE")
				(number "149")
			)
			(pin bidirectional line
				(at -27.94 -78.74 0)
				(length 7.62)
				(name "EA15/FRF")
				(number "153")
			)
			(pin bidirectional line
				(at -27.94 -81.28 0)
				(length 7.62)
				(name "EQ0")
				(number "1")
			)
			(pin bidirectional line
				(at -27.94 -83.82 0)
				(length 7.62)
				(name "EQ1")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 -86.36 0)
				(length 7.62)
				(name "EQ2")
				(number "17")
			)
			(pin bidirectional line
				(at -27.94 -88.9 0)
				(length 7.62)
				(name "EQ3")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 -91.44 0)
				(length 7.62)
				(name "EQ4/FWC#")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 -93.98 0)
				(length 7.62)
				(name "EQ5/FRC#")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 -96.52 0)
				(length 7.62)
				(name "EQ6/AMREN")
				(number "41")
			)
			(pin bidirectional line
				(at -27.94 -99.06 0)
				(length 7.62)
				(name "EQ7/AMWEN")
				(number "49")
			)
			(pin output line
				(at -27.94 -101.6 0)
				(length 7.62)
				(name "ERD#/SCL")
				(number "128")
			)
			(pin bidirectional line
				(at -27.94 -104.14 0)
				(length 7.62)
				(name "EWR#/SDA")
				(number "127")
			)
			(pin bidirectional line
				(at 27.94 101.6 180)
				(length 7.62)
				(name "DQ0")
				(number "100")
			)
			(pin bidirectional line
				(at 27.94 99.06 180)
				(length 7.62)
				(name "DQ1")
				(number "99")
			)
			(pin bidirectional line
				(at 27.94 96.52 180)
				(length 7.62)
				(name "DQ2")
				(number "98")
			)
			(pin bidirectional line
				(at 27.94 93.98 180)
				(length 7.62)
				(name "DQ3")
				(number "96")
			)
			(pin bidirectional line
				(at 27.94 91.44 180)
				(length 7.62)
				(name "DQ4")
				(number "95")
			)
			(pin bidirectional line
				(at 27.94 88.9 180)
				(length 7.62)
				(name "DQ5")
				(number "94")
			)
			(pin bidirectional line
				(at 27.94 86.36 180)
				(length 7.62)
				(name "DQ6")
				(number "92")
			)
			(pin bidirectional line
				(at 27.94 83.82 180)
				(length 7.62)
				(name "DQ7")
				(number "88")
			)
			(pin bidirectional line
				(at 27.94 81.28 180)
				(length 7.62)
				(name "DQ8")
				(number "86")
			)
			(pin bidirectional line
				(at 27.94 78.74 180)
				(length 7.62)
				(name "DQ9")
				(number "84")
			)
			(pin bidirectional line
				(at 27.94 76.2 180)
				(length 7.62)
				(name "DQ10")
				(number "83")
			)
			(pin bidirectional line
				(at 27.94 73.66 180)
				(length 7.62)
				(name "DQ11")
				(number "82")
			)
			(pin bidirectional line
				(at 27.94 71.12 180)
				(length 7.62)
				(name "DQ12")
				(number "80")
			)
			(pin bidirectional line
				(at 27.94 68.58 180)
				(length 7.62)
				(name "DQ13")
				(number "79")
			)
			(pin bidirectional line
				(at 27.94 66.04 180)
				(length 7.62)
				(name "DQ14")
				(number "78")
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 7.62)
				(name "DQ15")
				(number "76")
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 7.62)
				(name "DQ16")
				(number "157")
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 7.62)
				(name "DQ17")
				(number "145")
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 7.62)
				(name "DQ18")
				(number "133")
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 7.62)
				(name "DQ19")
				(number "125")
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 7.62)
				(name "DQ20")
				(number "117")
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "DQ21")
				(number "105")
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "DQ22")
				(number "93")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 7.62)
				(name "DQ23")
				(number "85")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "DQ24")
				(number "77")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "DQ25")
				(number "65")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "DQ26")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "DQ27")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "DQ28")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "DQ29")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "DQ30")
				(number "13")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 7.62)
				(name "DQ31")
				(number "5")
			)
			(pin output line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "PTATN#")
				(number "114")
			)
			(pin input line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "PTRDY#")
				(number "115")
			)
			(pin output line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "PTNUM0")
				(number "123")
			)
			(pin output line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "PTNUM1")
				(number "122")
			)
			(pin output line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "PTBE0#")
				(number "116")
			)
			(pin output line
				(at 27.94 7.62 180)
				(length 7.62)
				(name "PTBE1#")
				(number "118")
			)
			(pin output line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "PTBE2#")
				(number "119")
			)
			(pin output line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "PTBE3#")
				(number "120")
			)
			(pin input line
				(at 27.94 0 180)
				(length 7.62)
				(name "PTADR#")
				(number "107")
			)
			(pin output line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "PTWR")
				(number "108")
			)
			(pin output line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "PTBURST#")
				(number "112")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "ADR2")
				(number "68")
			)
			(pin input line
				(at 27.94 -12.7 180)
				(length 7.62)
				(name "ADR3")
				(number "67")
			)
			(pin input line
				(at 27.94 -15.24 180)
				(length 7.62)
				(name "ADR4")
				(number "66")
			)
			(pin input line
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "ADR5")
				(number "64")
			)
			(pin input line
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "ADR6")
				(number "132")
			)
			(pin input line
				(at 27.94 -22.86 180)
				(length 7.62)
				(name "BE0#")
				(number "87")
			)
			(pin input line
				(at 27.94 -25.4 180)
				(length 7.62)
				(name "BE1#")
				(number "63")
			)
			(pin input line
				(at 27.94 -27.94 180)
				(length 7.62)
				(name "BE2#")
				(number "62")
			)
			(pin input line
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "BE3#")
				(number "60")
			)
			(pin input line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "MODE_16/32")
				(number "59")
			)
			(pin input line
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "SELECT#")
				(number "75")
			)
			(pin input line
				(at 27.94 -38.1 180)
				(length 7.62)
				(name "WR#")
				(number "74")
			)
			(pin input line
				(at 27.94 -40.64 180)
				(length 7.62)
				(name "RD#")
				(number "72")
			)
			(pin input line
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "WRFIFO#")
				(number "102")
			)
			(pin input line
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "RDFIFO#")
				(number "104")
			)
			(pin output line
				(at 27.94 -53.34 180)
				(length 7.62)
				(name "WRFULL")
				(number "103")
			)
			(pin output line
				(at 27.94 -55.88 180)
				(length 7.62)
				(name "RDEMPTY")
				(number "106")
			)
			(pin input line
				(at 27.94 -58.42 180)
				(length 7.62)
				(name "FLT#")
				(number "138")
			)
			(pin input line
				(at 27.94 -60.96 180)
				(length 7.62)
				(name "SNV")
				(number "135")
			)
			(pin output line
				(at 27.94 -63.5 180)
				(length 7.62)
				(name "IRQ#")
				(number "124")
			)
			(pin output line
				(at 27.94 -66.04 180)
				(length 7.62)
				(name "BPCLK")
				(number "140")
			)
			(pin output line
				(at 27.94 -68.58 180)
				(length 7.62)
				(name "SYSRST#")
				(number "126")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SI9986"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 12.7 0)
		)
		(property "Value" "SI9986"
			(at 10.16 10.16 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/70007/si9986.pdf"
			(at 0 0 0)
		)
		(property "Description" "Integrated, buffered H-bridge with TTL compatible inputs, 1A, 12V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "integrated, buffered H-bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SI9986_0_1")
		(symbol "SI9986_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 5.08)
				(name "INA")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 5.08)
				(name "INB")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -12.7 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 3.81)
				(name "PWR")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 5.08)
				(name "SB")
				(number "4")
			)
			(pin power_in line
				(at 10.16 -12.7 90)
				(length 5.08)
				(name "SA")
				(number "1")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 7.62)
				(name "OUTA")
				(number "8")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 7.62)
				(name "OUTB")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SLB9660xT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.652 16.51 0)
		)
		(property "Value" "SLB9660xT"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 2.54 -16.51 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-data-sheet-SLB9660_1.2_Rev1.2-DS-v01_02-EN.pdf?fileId=5546d462689a790c016929d1cb874fe5"
			(at 2.54 -19.05 0)
		)
		(property "Description" "Trusted Platform Module 1.2 with Low Pin Count interface, TSSOP-28"
			(at 2.54 -21.59 0)
		)
		(property "ki_keywords" "TPM LPC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SLB9660xT_0_0"
			(pin tri_state line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "LAD0")
				(number "26")
			)
			(pin tri_state line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "LAD1")
				(number "23")
			)
			(pin tri_state line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "LAD2")
				(number "20")
			)
			(pin tri_state line
				(at -12.7 0 0)
				(length 2.54)
				(name "LAD3")
				(number "17")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "LCLK")
				(number "21")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{LFRAME}")
				(number "22")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{LRESET}")
				(number "16")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "NC")
				(number "9")
			)
			(pin tri_state line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SERIRQ")
				(number "27")
			)
			(pin no_connect line
				(at -10.16 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin no_connect line
				(at 10.16 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PP")
				(number "7")
			)
		)
		(symbol "SLB9660xT_1_0"
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "GPIO")
				(number "6")
			)
		)
		(symbol "SLB9660xT_1_1")
		(embedded_fonts no)
	)
	(symbol "SN65LVDS047D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "SN65LVDS047D"
			(at 1.27 21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65lvds047.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Quad LVDS Differential Line Driver, 400Mbps, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad LVDS Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65LVDS047D_0_1")
		(symbol "SN65LVDS047D_1_0"
			(text "D1"
				(at -0.889 13.97 0)
			)
			(text "D2"
				(at -0.889 6.35 0)
			)
			(text "D3"
				(at -0.889 -1.27 0)
			)
			(text "D4"
				(at -0.889 -8.89 0)
			)
		)
		(symbol "SN65LVDS047D_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "DIN1")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DIN2")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIN3")
				(number "6")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DIN4")
				(number "7")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "~{EN}")
				(number "8")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "DOUT1+")
				(number "15")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "DOUT1-")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DOUT2+")
				(number "14")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DOUT2-")
				(number "13")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "DOUT3+")
				(number "11")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DOUT3-")
				(number "12")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DOUT4+")
				(number "10")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DOUT4-")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65LVDS047PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "SN65LVDS047PW"
			(at 1.27 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at -2.54 -24.13 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65lvds047.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "Quad LVDS Differential Line Driver, 400Mbps, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad LVDS Driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SN65LVDS047PW_0_1")
		(symbol "SN65LVDS047PW_1_0"
			(text "D1"
				(at -0.889 13.97 0)
			)
			(text "D2"
				(at -0.889 6.35 0)
			)
			(text "D3"
				(at -0.889 -1.27 0)
			)
			(text "D4"
				(at -0.889 -8.89 0)
			)
		)
		(symbol "SN65LVDS047PW_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "DIN1")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DIN2")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "DIN3")
				(number "6")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DIN4")
				(number "7")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "~{EN}")
				(number "8")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "DOUT1+")
				(number "15")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "DOUT1-")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DOUT2+")
				(number "14")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DOUT2-")
				(number "13")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "DOUT3+")
				(number "11")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DOUT3-")
				(number "12")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DOUT4+")
				(number "10")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DOUT4-")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65LVDS1D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "SN65LVDS1D"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65lvds1.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Differential Line Driver, 630Mbps, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS Driver TI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65LVDS1D_1_0"
			(text "D"
				(at -1.905 0 0)
			)
		)
		(symbol "SN65LVDS1D_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "D")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{CC}")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "5")
			)
			(pin passive line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "6")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "Y")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65LVDS1DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "SN65LVDS1DBV"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65lvds1.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Differential Line Driver, 630Mbps, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS Driver TI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "SN65LVDS1DBV_1_0"
			(text "D"
				(at -1.905 0 0)
			)
		)
		(symbol "SN65LVDS1DBV_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{CC}")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "Y")
				(number "4")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65LVDS2D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "SN65LVDS2D"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn65lvds2.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Differential Line Receiver, 630Mbps, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS Receiver TI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65LVDS2D_1_0"
			(text "R"
				(at 0 -0.127 0)
			)
		)
		(symbol "SN65LVDS2D_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{CC}")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "R")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65LVDS2DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "SN65LVDS2DBV"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn65lvds2.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Differential Line Receiver, 630Mbps, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS Receiver TI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "SN65LVDS2DBV_1_0"
			(text "R"
				(at 0 -0.127 0)
			)
		)
		(symbol "SN65LVDS2DBV_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "B")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{CC}")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "R")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65LVDT2D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "SN65LVDT2D"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn65lvdt2.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Differential Line Receiver, 110 Ω Terminated, 630Mbps, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS Receiver TI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65LVDT2D_0_1")
		(symbol "SN65LVDT2D_1_0"
			(text "R"
				(at 0 -0.127 0)
			)
		)
		(symbol "SN65LVDT2D_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "B")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{CC}")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 5.08 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at 7.62 -10.16 90)
				(length 2.54)
				(name "NC")
				(number "6")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "R")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65LVDT2DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "SN65LVDT2DBV"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn65lvdt2.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed Differential Line Receiver, 110 Ω Terminated, 630Mbps, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS Receiver TI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "SN65LVDT2DBV_0_1")
		(symbol "SN65LVDT2DBV_1_0"
			(text "R"
				(at 0 -0.127 0)
			)
		)
		(symbol "SN65LVDT2DBV_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "B")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V_{CC}")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "R")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74LV8153N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "SN74LV8153N"
			(at 10.16 15.24 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lv8153.pdf"
			(at 0 0 0)
		)
		(property "Description" "UART, Single wire input, Output 40mA, Open Collector or Push Pull, PDIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "serial to parallel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SN74LV8153N_0_1")
		(symbol "SN74LV8153N_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "D")
				(number "5")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "~{OE}")
				(number "8")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUTSEL")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A0")
				(number "2")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "V_{CC1}")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "V_{CC2}")
				(number "20")
			)
			(pin open_collector line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "Y0")
				(number "19")
			)
			(pin open_collector line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "Y1")
				(number "18")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Y2")
				(number "17")
			)
			(pin open_collector line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Y3")
				(number "16")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "Y4")
				(number "15")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Y5")
				(number "14")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Y6")
				(number "13")
			)
			(pin open_collector line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y7")
				(number "12")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "SOUT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN75160BDW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 19.05 0)
		)
		(property "Value" "SN75160BDW"
			(at -8.89 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75160b.pdf"
			(at -1.27 8.89 0)
		)
		(property "Description" "Octal general-purpose interface bus transceiver, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "gpib bidirectional bus transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN75160BDW_0_1")
		(symbol "SN75160BDW_1_1"
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "D1")
				(number "19")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "D2")
				(number "18")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "D3")
				(number "17")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "D4")
				(number "16")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D5")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "D6")
				(number "14")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "D7")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "D8")
				(number "12")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "TE")
				(number "1")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "~{PE}")
				(number "11")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "B1")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "B2")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B3")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B4")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B5")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B6")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B7")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B8")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN75160BN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 19.05 0)
		)
		(property "Value" "SN75160BN"
			(at -7.62 16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75160b.pdf"
			(at -20.32 5.08 0)
		)
		(property "Description" "Octal general-purpose interface bus transceiver, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "gpib bidirectional bus transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SN75160BN_1_1"
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "D1")
				(number "19")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "D2")
				(number "18")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "D3")
				(number "17")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "D4")
				(number "16")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D5")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "D6")
				(number "14")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "D7")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "D8")
				(number "12")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "TE")
				(number "1")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "~{PE}")
				(number "11")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "B1")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "B2")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B3")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B4")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B5")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B6")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B7")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B8")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TB5D1MD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "TB5D1MD"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tb5d2h.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad differential PECL driver"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential PECL driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27*"
			(at 0 0 0)
		)
		(symbol "TB5D1MD_0_1")
		(symbol "TB5D1MD_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AI")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "BI")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CI")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "DI")
				(number "15")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "E1")
				(number "4")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "E2")
				(number "12")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "AO")
				(number "2")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{AO}")
				(number "3")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "BO")
				(number "6")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{BO}")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "CO")
				(number "10")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CO}")
				(number "11")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DO")
				(number "14")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{DO}")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TB5D1MDW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "TB5D1MDW"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 25.4 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tb5d2h.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad differential PECL driver"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential PECL driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27*"
			(at 0 0 0)
		)
		(symbol "TB5D1MDW_0_1")
		(symbol "TB5D1MDW_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AI")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "BI")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CI")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "DI")
				(number "15")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "E1")
				(number "4")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "E2")
				(number "12")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "AO")
				(number "2")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{AO}")
				(number "3")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "BO")
				(number "6")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{BO}")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "CO")
				(number "10")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CO}")
				(number "11")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DO")
				(number "14")
			)
			(pin output line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{DO}")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TB5R1D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "TB5R1D"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tb5r1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad differential PECL reciver"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential PECL reciver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27*"
			(at 0 0 0)
		)
		(symbol "TB5R1D_0_1")
		(symbol "TB5R1D_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AI")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{AI}")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "BI")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{BI}")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CI")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{CI}")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "DI")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{DI}")
				(number "15")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "E1")
				(number "4")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "~{E2}")
				(number "12")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "AO")
				(number "3")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "BO")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "CO")
				(number "11")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DO")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TB5R1DW"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "TB5R1DW"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 25.4 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tb5r1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad differential PECL reciver"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential PECL reciver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27*"
			(at 0 0 0)
		)
		(symbol "TB5R1DW_0_1")
		(symbol "TB5R1DW_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "AI")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{AI}")
				(number "1")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "BI")
				(number "6")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{BI}")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CI")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{CI}")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "DI")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{DI}")
				(number "15")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "E1")
				(number "4")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "~{E2}")
				(number "12")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "AO")
				(number "3")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "BO")
				(number "5")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "CO")
				(number "11")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DO")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9406DC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TCA9406DC"
			(at 5.08 11.43 0)
		)
		(property "Footprint" ""
			(at -10.16 8.89 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/tca9406.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "2-Bit Bidirectional 1-MHz, I2C Bus and SMBus Voltage-Level Translator With 8-kV HBM ESD"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bidirectional 1-MHz I2C SMBus Voltage-Level Translator 8kV HBM ESD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*2.95x2.8mm*P0.65mm* VSSOP*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TCA9406DC_0_1")
		(symbol "TCA9406DC_1_1"
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SCL_A")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SDA_A")
				(number "4")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "7")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OE")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SCL_B")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SDA_B")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9800"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TCA9800"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 22.86 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9800.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "Level-Translating I2C Bus Buffer/Repeater 0.54mA Current Source, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C buffer repeater"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TCA9800_0_1")
		(symbol "TCA9800_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SCLA")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDAA")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SCLB")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SDAB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "U2270B"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 8.89 0)
		)
		(property "Value" "U2270B"
			(at 7.366 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 1.27 -24.13 0)
		)
		(property "Datasheet" "http://www.farnell.com/datasheets/94393.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "IDIC read/write base stations in contactless identification and immobilizer systems, SO-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "IDIC read/write base stations in contactless identification and immobilizer systems"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "U2270B_0_1")
		(symbol "U2270B_1_1"
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "~{OE}")
				(number "3")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "INPUT")
				(number "4")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "MS")
				(number "5")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "CFE")
				(number "6")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "STANDBY")
				(number "13")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "RF")
				(number "15")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "HIPASS")
				(number "16")
			)
			(pin power_in line
				(at -5.08 10.16 270)
				(length 2.54)
				(name "VEXT")
				(number "10")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "DVS")
				(number "11")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBATT")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "DGND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VS")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin open_collector line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "OUTPUT")
				(number "2")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "COIL1")
				(number "9")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "COIL2")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WD2791"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 44.45 0)
		)
		(property "Value" "WD2791"
			(at 6.35 44.45 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 16.51 -41.91 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets2/12/1229802_1.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "Floppy disk controller, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Floppy disk controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "WD2791_0_1")
		(symbol "WD2791_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "~{WE}")
				(number "2")
			)
			(pin input line
				(at -12.7 38.1 0)
				(length 2.54)
				(name "~{CS}")
				(number "3")
			)
			(pin input line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "~{RE}")
				(number "4")
			)
			(pin input line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "CLK")
				(number "24")
			)
			(pin input line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "~{MR}")
				(number "19")
			)
			(pin tri_state line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "~{DAL0}")
				(number "7")
			)
			(pin tri_state line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "~{DAL1}")
				(number "8")
			)
			(pin tri_state line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{DAL2}")
				(number "9")
			)
			(pin tri_state line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{DAL3}")
				(number "10")
			)
			(pin tri_state line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{DAL4}")
				(number "11")
			)
			(pin tri_state line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{DAL5}")
				(number "12")
			)
			(pin tri_state line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{DAL6}")
				(number "13")
			)
			(pin tri_state line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{DAL7}")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ENP")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RPW")
				(number "18")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{5}/8")
				(number "17")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{TEST}")
				(number "22")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "VCO")
				(number "26")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "WPW")
				(number "33")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "~{DDEN}")
				(number "37")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "~{RAW_READ}")
				(number "27")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "READY")
				(number "32")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "~{TR00}")
				(number "34")
			)
			(pin input line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "~{IP}")
				(number "35")
			)
			(pin input line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "~{WPRT}")
				(number "36")
			)
			(pin input line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "HLT")
				(number "40")
			)
			(pin input line
				(at -12.7 -38.1 0)
				(length 2.54)
				(name "~{ENMF}")
				(number "25")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin output line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "INTRQ")
				(number "39")
			)
			(pin output line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "DRQ")
				(number "38")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "STEP")
				(number "15")
			)
			(pin output line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "DIRC")
				(number "16")
			)
			(pin output line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "WD")
				(number "31")
			)
			(pin output line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "WG")
				(number "30")
			)
			(pin output line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "TG43")
				(number "29")
			)
			(pin output line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "HLD")
				(number "28")
			)
			(pin output line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PUMP")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WD2793"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 44.45 0)
		)
		(property "Value" "WD2793"
			(at 6.35 44.45 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 16.51 -41.91 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets2/12/1229802_1.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "Floppy disk controller, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Floppy disk controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "WD2793_0_1")
		(symbol "WD2793_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "~{WE}")
				(number "2")
			)
			(pin input line
				(at -12.7 38.1 0)
				(length 2.54)
				(name "~{CS}")
				(number "3")
			)
			(pin input line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "~{RE}")
				(number "4")
			)
			(pin input line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "CLK")
				(number "24")
			)
			(pin input line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "~{MR}")
				(number "19")
			)
			(pin tri_state line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "DAL0")
				(number "7")
			)
			(pin tri_state line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "DAL1")
				(number "8")
			)
			(pin tri_state line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "DAL2")
				(number "9")
			)
			(pin tri_state line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "DAL3")
				(number "10")
			)
			(pin tri_state line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "DAL4")
				(number "11")
			)
			(pin tri_state line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "DAL5")
				(number "12")
			)
			(pin tri_state line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DAL6")
				(number "13")
			)
			(pin tri_state line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DAL7")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ENP")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RPW")
				(number "18")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{5}/8")
				(number "17")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{TEST}")
				(number "22")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "VCO")
				(number "26")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "WPW")
				(number "33")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "~{DDEN}")
				(number "37")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "~{RAW_READ}")
				(number "27")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "READY")
				(number "32")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "~{TR00}")
				(number "34")
			)
			(pin input line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "~{IP}")
				(number "35")
			)
			(pin input line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "~{WPRT}")
				(number "36")
			)
			(pin input line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "HLT")
				(number "40")
			)
			(pin input line
				(at -12.7 -38.1 0)
				(length 2.54)
				(name "~{ENMF}")
				(number "25")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin output line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "INTRQ")
				(number "39")
			)
			(pin output line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "DRQ")
				(number "38")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "STEP")
				(number "15")
			)
			(pin output line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "DIRC")
				(number "16")
			)
			(pin output line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "WD")
				(number "31")
			)
			(pin output line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "WG")
				(number "30")
			)
			(pin output line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "TG43")
				(number "29")
			)
			(pin output line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "HLD")
				(number "28")
			)
			(pin output line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PUMP")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WD2795"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 44.45 0)
		)
		(property "Value" "WD2795"
			(at 6.35 44.45 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 16.51 -41.91 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets2/12/1229802_1.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "Floppy disk controller, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Floppy disk controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "WD2795_0_1")
		(symbol "WD2795_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "~{WE}")
				(number "2")
			)
			(pin input line
				(at -12.7 38.1 0)
				(length 2.54)
				(name "~{CS}")
				(number "3")
			)
			(pin input line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "~{RE}")
				(number "4")
			)
			(pin input line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "CLK")
				(number "24")
			)
			(pin input line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "~{MR}")
				(number "19")
			)
			(pin tri_state line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "~{DAL0}")
				(number "7")
			)
			(pin tri_state line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "~{DAL1}")
				(number "8")
			)
			(pin tri_state line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{DAL2}")
				(number "9")
			)
			(pin tri_state line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{DAL3}")
				(number "10")
			)
			(pin tri_state line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{DAL4}")
				(number "11")
			)
			(pin tri_state line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "~{DAL5}")
				(number "12")
			)
			(pin tri_state line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{DAL6}")
				(number "13")
			)
			(pin tri_state line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{DAL7}")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ENP")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RPW")
				(number "18")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{5}/8")
				(number "17")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{TEST}")
				(number "22")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "VCO")
				(number "26")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "WPW")
				(number "33")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "~{DDEN}")
				(number "37")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "~{RAW_READ}")
				(number "27")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "READY")
				(number "32")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "~{TR00}")
				(number "34")
			)
			(pin input line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "~{IP}")
				(number "35")
			)
			(pin input line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "~{WPRT}")
				(number "36")
			)
			(pin input line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "HLT")
				(number "40")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin output line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "INTRQ")
				(number "39")
			)
			(pin output line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "DRQ")
				(number "38")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "STEP")
				(number "15")
			)
			(pin output line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "DIRC")
				(number "16")
			)
			(pin output line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "WD")
				(number "31")
			)
			(pin output line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "WG")
				(number "30")
			)
			(pin output line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "TG43")
				(number "29")
			)
			(pin output line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "HLD")
				(number "28")
			)
			(pin output line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PUMP")
				(number "23")
			)
			(pin output line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "SSO")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WD2797"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 44.45 0)
		)
		(property "Value" "WD2797"
			(at 6.35 44.45 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 16.51 -41.91 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets2/12/1229802_1.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "Floppy disk controller, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Floppy disk controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "WD2797_0_1")
		(symbol "WD2797_1_1"
			(pin input line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "~{WE}")
				(number "2")
			)
			(pin input line
				(at -12.7 38.1 0)
				(length 2.54)
				(name "~{CS}")
				(number "3")
			)
			(pin input line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "~{RE}")
				(number "4")
			)
			(pin input line
				(at -12.7 33.02 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "CLK")
				(number "24")
			)
			(pin input line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "~{MR}")
				(number "19")
			)
			(pin tri_state line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "DAL0")
				(number "7")
			)
			(pin tri_state line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "DAL1")
				(number "8")
			)
			(pin tri_state line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "DAL2")
				(number "9")
			)
			(pin tri_state line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "DAL3")
				(number "10")
			)
			(pin tri_state line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "DAL4")
				(number "11")
			)
			(pin tri_state line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "DAL5")
				(number "12")
			)
			(pin tri_state line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DAL6")
				(number "13")
			)
			(pin tri_state line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DAL7")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ENP")
				(number "1")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RPW")
				(number "18")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{5}/8")
				(number "17")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{TEST}")
				(number "22")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "VCO")
				(number "26")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "WPW")
				(number "33")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "~{DDEN}")
				(number "37")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "~{RAW_READ}")
				(number "27")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "READY")
				(number "32")
			)
			(pin input line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "~{TR00}")
				(number "34")
			)
			(pin input line
				(at -12.7 -30.48 0)
				(length 2.54)
				(name "~{IP}")
				(number "35")
			)
			(pin input line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "~{WPRT}")
				(number "36")
			)
			(pin input line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "HLT")
				(number "40")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin output line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "INTRQ")
				(number "39")
			)
			(pin output line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "DRQ")
				(number "38")
			)
			(pin output line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "STEP")
				(number "15")
			)
			(pin output line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "DIRC")
				(number "16")
			)
			(pin output line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "WD")
				(number "31")
			)
			(pin output line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "WG")
				(number "30")
			)
			(pin output line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "TG43")
				(number "29")
			)
			(pin output line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "HLD")
				(number "28")
			)
			(pin output line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "PUMP")
				(number "23")
			)
			(pin output line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "SSO")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Z8420"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 31.75 0)
		)
		(property "Value" "Z8420"
			(at 3.81 31.75 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.zilog.com/appnotes_download.php?FromPage=DirectLink&dn=PS0180&ft=Product%20Specification%20(Data%20Sheet)%20%20&f=YUhSMGNEb3ZMM2QzZHk1NmFXeHZaeTVqYjIwdlpHOWpjeTk2T0RBdmNITXdNVGd3TG5Ca1pnPT0="
			(at -1.27 -40.64 0)
		)
		(property "Description" "Parallel I/O, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Z80 PIO parallel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "Z8420_1_0")
		(symbol "Z8420_1_1"
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "D0")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "D1")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "D2")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D3")
				(number "40")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D4")
				(number "39")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D5")
				(number "38")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D6")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D7")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "B/~{A}")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "C/~{D}")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{CE}")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{M1}")
				(number "37")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{IORQ}")
				(number "36")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{RD}")
				(number "35")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "CLK")
				(number "25")
			)
			(pin open_collector line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "~{INT}")
				(number "23")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "IEI")
				(number "24")
			)
			(pin output line
				(at -12.7 -27.94 0)
				(length 2.54)
				(name "IEO")
				(number "22")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "26")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "PA0")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "PA1")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "PA2")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA3")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA4")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "7")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "ARDY")
				(number "18")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{ASTB}")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "28")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "29")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "32")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "33")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "34")
			)
			(pin output line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "BRDY")
				(number "21")
			)
			(pin input line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "~{BSTB}")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "6822"
		(extends "6821")
		(property "Reference" "U"
			(at -7.62 34.29 0)
		)
		(property "Value" "6822"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 -34.29 0)
		)
		(property "Datasheet" "http://pdf1.alldatasheet.com/datasheet-pdf/view/135452/MOTOROLA/MC6822.html"
			(at 0 0 0)
		)
		(property "Description" "Peripheral Interface Adapter 1MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "PIA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "8255A"
		(extends "8255")
		(property "Reference" "U"
			(at -13.97 38.1 0)
		)
		(property "Value" "8255A"
			(at 8.89 38.1 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://aturing.umcs.maine.edu/~meadow/courses/cos335/Intel8255A.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "Programmable Peripheral Interface, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "8255 PPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "8259A"
		(extends "8259")
		(property "Reference" "U"
			(at -10.16 25.4 0)
		)
		(property "Value" "8259A"
			(at 8.89 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://pdos.csail.mit.edu/6.828/2005/readings/hardware/8259A.pdf"
			(at 0 0 0)
		)
		(property "Description" "8259, Programmable Interrupt Controller, PDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "PIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "8259A-2"
		(extends "8259")
		(property "Reference" "U"
			(at -10.16 25.4 0)
		)
		(property "Value" "8259A-2"
			(at 8.89 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://pdos.csail.mit.edu/6.828/2005/readings/hardware/8259A.pdf"
			(at 0 0 0)
		)
		(property "Description" "8259, Programmable Interrupt Controller, PDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "PIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "82C55A"
		(extends "8255")
		(property "Reference" "U"
			(at -13.97 38.1 0)
		)
		(property "Value" "82C55A"
			(at 8.89 38.1 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://jap.hu/electronic/8255.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "CHMOS Programmable Peripheral Interface, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "8255 PPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "AM26LS31CDB"
		(extends "AM26LS31CD")
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "AM26LS31CDB"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_5.3x6.2mm_P0.65mm"
			(at 25.4 -24.13 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/am26ls31.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "32Mbps 3.3V RS485 Quad Line Drivers, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver rs485 rs422 differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x6.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AM26LS31CN"
		(extends "AM26LS31CD")
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "AM26LS31CN"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 25.4 -24.13 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/am26ls31.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "32Mbps 3.3V RS485 Quad Line Drivers, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver rs485 rs422 differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AM26LS31MJ"
		(extends "AM26LS31CD")
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "AM26LS31MJ"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 25.4 -24.13 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/am26ls31.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "32Mbps 3.3V RS485 Quad Line Drivers, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver rs485 rs422 differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AM26LS31xNS"
		(extends "AM26LS31CD")
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "AM26LS31xNS"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_SO:SO-16_5.3x10.2mm_P1.27mm"
			(at 25.4 -24.13 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/am26ls31.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "32Mbps 3.3V RS485 Quad Line Drivers, SO-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "driver rs485 rs422 differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*5.3x10.2mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6957xDD-4"
		(extends "LTC6957xDD-3")
		(property "Reference" "U"
			(at 7.62 -13.97 0)
		)
		(property "Value" "LTC6957xDD-4"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-12-1EP_3x3mm_P0.45mm_EP1.65x2.38mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6957fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Phase Noise, Dual Output Buffer/Driver/Logic Converter, CMOS Complementary Outputs, DFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "LTC clock converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC6957xMS-4"
		(extends "LTC6957xMS-3")
		(property "Reference" "U"
			(at 7.62 -13.97 0)
		)
		(property "Value" "LTC6957xMS-4"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-12_3x4.039mm_P0.65mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/6957fb.pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Phase Noise, Dual Output Buffer/Driver/Logic Converter, CMOS Complementary Outputs, MSOP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "LTC clock converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x4.039mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC100LVELT22D"
		(extends "MC100EPT22D")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "MC100LVELT22D"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -2.54 -24.13 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC100LVELT22-D.PDF"
			(at 1.27 -10.16 0)
		)
		(property "Description" "3.3 V Dual LVTTL/LVCMOS to Differential LVPECL Translator, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "PECL buffer interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC100LVELT22DT"
		(extends "MC100EPT22DT")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "MC100LVELT22DT"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at -2.54 -24.13 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MC100LVELT22-D.PDF"
			(at 1.27 -10.16 0)
		)
		(property "Description" "3.3 V Dual LVTTL/LVCMOS to Differential LVPECL Translator, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "PECL buffer interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68A21"
		(extends "6821")
		(property "Reference" "U"
			(at -7.62 34.29 0)
		)
		(property "Value" "MC68A21"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 -34.29 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/6821.pdf"
			(at 0 0 0)
		)
		(property "Description" "Peripheral Interface Adapter 1.5MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "PIA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68A40"
		(extends "MC6840")
		(property "Reference" "U"
			(at -7.62 34.29 0)
		)
		(property "Value" "MC68A40"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 1.27 -27.94 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC6840.pdf"
			(at 1.27 -30.48 0)
		)
		(property "Description" "Motorola Programmable Timer Module, 1.5MHz, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "PTM MC6800"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68A44"
		(extends "MC6844")
		(property "Reference" "U"
			(at -8.382 34.544 0)
		)
		(property "Value" "MC68A44"
			(at 12.7 34.544 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 -31.75 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets/560/501527_DS.pdf"
			(at 0 0 0)
		)
		(property "Description" "Direct Memory Access Controller 1.5MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Direct Memory Access Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68B21"
		(extends "6821")
		(property "Reference" "U"
			(at -7.62 34.29 0)
		)
		(property "Value" "MC68B21"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 -34.29 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/6821.pdf"
			(at 0 0 0)
		)
		(property "Description" "Peripheral Interface Adapter 2MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "PIA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68B40"
		(extends "MC6840")
		(property "Reference" "U"
			(at -7.62 34.29 0)
		)
		(property "Value" "MC68B40"
			(at 10.16 34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 1.27 -27.94 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC6840.pdf"
			(at 1.27 -30.48 0)
		)
		(property "Description" "Motorola Programmable Timer Module, 2.0MHz, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "PTM MC6800"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68B44"
		(extends "MC6844")
		(property "Reference" "U"
			(at -8.382 34.544 0)
		)
		(property "Value" "MC68B44"
			(at 12.7 34.544 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 -31.75 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets/560/501527_DS.pdf"
			(at 0 0 0)
		)
		(property "Description" "Direct Memory Access Controller 2MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Direct Memory Access Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCA9306D"
		(extends "PCA9306")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "PCA9306D"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9306.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "Dual bidirectional I2C Bus and SMBus voltage level translator, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C SMBus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCA9306DC"
		(extends "PCA9306")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "PCA9306DC"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9306.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "Dual bidirectional I2C Bus and SMBus voltage level translator, VSSOP-8, Discontinued"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C SMBus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCA9306DC1"
		(extends "PCA9306")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "PCA9306DC1"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9306.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "Dual bidirectional I2C Bus and SMBus voltage level translator, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C SMBus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCA9306DP"
		(extends "PCA9306")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "PCA9306DP"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9306.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "Dual bidirectional I2C Bus and SMBus voltage level translator, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C SMBus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "SLB9665xT"
		(extends "SLB9660xT")
		(property "Reference" "U"
			(at -9.652 16.51 0)
		)
		(property "Value" "SLB9665xT"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 1.27 -16.51 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-data-sheet-SLB9665_2.0_Rev1.2-DS-v01_02-EN.pdf?fileId=5546d462689a790c016929d1d3054feb"
			(at 1.27 -19.05 0)
		)
		(property "Description" "Trusted Platform Module 2.0 with Low Pin Count interface, TSSOP-28"
			(at -0.508 0 0)
		)
		(property "ki_keywords" "TPM LPC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LV8153PW"
		(extends "SN74LV8153N")
		(property "Reference" "U"
			(at -7.62 15.24 0)
		)
		(property "Value" "SN74LV8153PW"
			(at 10.16 15.24 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lv8153.pdf"
			(at 0 0 0)
		)
		(property "Description" "UART, Single wire input, Output 40mA, Open Collector or Push Pull, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "serial to parallel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TB5D2H"
		(extends "TB5D1MD")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "TB5D2H"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tb5d2h.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad differential PECL driver"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential PECL driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27*"
			(at 0 0 0)
		)
	)
	(symbol "TB5D2HDW"
		(extends "TB5D1MDW")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "TB5D2HDW"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 25.4 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tb5d2h.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad differential PECL driver"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential PECL driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27*"
			(at 0 0 0)
		)
	)
	(symbol "TB5R2D"
		(extends "TB5R1D")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "TB5R2D"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tb5r1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad differential PECL reciver"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential PECL reciver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27*"
			(at 0 0 0)
		)
	)
	(symbol "TB5R2DW"
		(extends "TB5R1DW")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "TB5R2DW"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 25.4 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tb5r1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad differential PECL reciver"
			(at 0 0 0)
		)
		(property "ki_keywords" "differential PECL reciver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27*"
			(at 0 0 0)
		)
	)
	(symbol "TCA9801"
		(extends "TCA9800")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TCA9801"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 22.86 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9801.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "Level-Translating I2C Bus Buffer/Repeater 1.1mA Current Source, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C buffer repeater"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCA9802"
		(extends "TCA9800")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TCA9802"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 22.86 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9802.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "Level-Translating I2C Bus Buffer/Repeater 2.2mA Current Source, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C buffer repeater"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCA9803"
		(extends "TCA9800")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TCA9803"
			(at 5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 22.86 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9803.pdf"
			(at -7.62 11.43 0)
		)
		(property "Description" "Level-Translating I2C Bus Buffer/Repeater 3.3mA Current Source, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C buffer repeater"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "Z84C20"
		(extends "Z8420")
		(property "Reference" "U"
			(at -10.16 31.75 0)
		)
		(property "Value" "Z84C20"
			(at 3.81 31.75 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.zilog.com/appnotes_download.php?FromPage=DirectLink&dn=PS0180&ft=Product%20Specification%20(Data%20Sheet)%20%20&f=YUhSMGNEb3ZMM2QzZHk1NmFXeHZaeTVqYjIwdlpHOWpjeTk2T0RBdmNITXdNVGd3TG5Ca1pnPT0="
			(at -1.27 -40.64 0)
		)
		(property "Description" "Parallel I/O, CMOS, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Z80 PIO parallel"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
)
