(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ADM3053"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "ADM3053"
			(at 10.16 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 5.08 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM3053.pdf"
			(at 5.08 -20.32 0)
		)
		(property "Description" "Isolated CAN Transceiver, integrated isolated DC-DC converter, 1Mbps"
			(at 0 0 0)
		)
		(property "ki_keywords" "protected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADM3053_0_1")
		(symbol "ADM3053_1_1"
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIO")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "TXD")
				(number "5")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "1")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "10")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "3")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "7")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "9")
			)
			(pin no_connect line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VISOIN")
				(number "19")
			)
			(pin power_out line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VISOOUT")
				(number "12")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VREF")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANH")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "CANL")
				(number "15")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "RS")
				(number "18")
			)
			(pin power_in line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "13")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "16")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM3057ExRW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ADM3057ExRW"
			(at 13.97 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM3055E-3057E.pdf"
			(at -7.62 17.78 0)
		)
		(property "Description" "Isolated CAN FD Transceiver, integrated isolated DC-DC converter, 12Mbps, SOIC-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transceiver isolated protected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADM3057ExRW_0_1")
		(symbol "ADM3057ExRW_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "TXD")
				(number "7")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RXD")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "AUXIN")
				(number "9")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "STBY")
				(number "8")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SILENT")
				(number "6")
			)
			(pin power_in line
				(at -7.62 17.78 270)
				(length 2.54)
				(name "VIO")
				(number "4")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "GND1")
				(number "1")
			)
			(pin passive line
				(at -5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "10")
			)
			(pin passive line
				(at -5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VISOIN")
				(number "16")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VISOOUT")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "CANH")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "CANL")
				(number "13")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "AUXOUT")
				(number "17")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RS")
				(number "12")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GNDISO")
				(number "18")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GNDISO")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO1044BD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "ISO1044BD"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso1044.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "Isolated CAN FD Transceiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN-FD Isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO1044BD_0_1")
		(symbol "ISO1044BD_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "RXD")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "TXD")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VCC2")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "CANH")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "5")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND2")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO1050DUB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "ISO1050DUB"
			(at 2.54 6.35 0)
		)
		(property "Footprint" "Package_SO:SOP-8_6.62x9.15mm_P2.54mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/iso1050.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Isolated CAN Transceiver, SOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN Isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*6.62x9.15mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "ISO1050DUB_0_1")
		(symbol "ISO1050DUB_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "RXD")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "TXD")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VCC2")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISOW1044"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ISOW1044"
			(at 13.97 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/isow1044.pdf"
			(at 0 30.48 0)
		)
		(property "Description" "Isolated CAN FD Transceiver, Integrated DC-DC Converter, 5Mbps, Reinforced Isolation,  SOIC-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transceiver isolated protected integrated isolated supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISOW1044_0_1")
		(symbol "ISOW1044_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "TXD")
				(number "3")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RXD")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "STB")
				(number "4")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "EN/FLT")
				(number "8")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -7.62 17.78 270)
				(length 2.54)
				(name "VIO")
				(number "1")
			)
			(pin power_in line
				(at -7.62 -17.78 90)
				(length 2.54)
				(name "GNDIO")
				(number "6")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "GND1")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VISOIN")
				(number "20")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VSIN")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GISOIN")
				(number "15")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GISOIN")
				(number "16")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GISOIN")
				(number "17")
			)
			(pin power_out line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VISOOUT")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "CANH")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "CANL")
				(number "18")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUT")
				(number "14")
			)
			(pin power_out line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2875-DD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LTC2875-DD"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2875f.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 4Mbps, 3.3V or 5V supply, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2875-DD_0_1")
		(symbol "LTC2875-DD_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RS")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SPLIT")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2875-S8"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "LTC2875-S8"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/2875f.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 4Mbps, 3.3V or 5V supply, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC2875-S8_0_1")
		(symbol "LTC2875-S8_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RS")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "SPLIT")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2021A-xxxxMD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.811 8.763 0)
		)
		(property "Value" "MCP2021A-xxxxMD"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_4x4mm_P0.8mm_EP2.5x3.6mm"
			(at 0 1.905 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002298C.pdf"
			(at 0.635 1.905 0)
		)
		(property "Description" "LIN Transceiver with Voltage Regulator, 3.3V/5V, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN Transceiver regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MCP2021A-xxxxMD_0_1")
		(symbol "MCP2021A-xxxxMD_1_1"
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RXD")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "TXD")
				(number "4")
			)
			(pin open_collector line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "LBUS")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBB")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "9")
			)
			(pin power_out line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VREG")
				(number "3")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "CS/LWAKE")
				(number "2")
			)
			(pin open_collector line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{FAULT}/TXE")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2021A-xxxxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.811 8.763 0)
		)
		(property "Value" "MCP2021A-xxxxP"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0.635 1.905 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002298C.pdf"
			(at 0.635 1.905 0)
		)
		(property "Description" "LIN Transceiver with Voltage Regulator, 3.3V/5V, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN Transceiver regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP2021A-xxxxP_0_1")
		(symbol "MCP2021A-xxxxP_1_1"
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RXD")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "TXD")
				(number "4")
			)
			(pin open_collector line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "LBUS")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBB")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_out line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VREG")
				(number "3")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "CS/LWAKE")
				(number "2")
			)
			(pin open_collector line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{FAULT}/TXE")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2021A-xxxxSN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.811 8.763 0)
		)
		(property "Value" "MCP2021A-xxxxSN"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0.635 1.905 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002298C.pdf"
			(at 0.635 1.905 0)
		)
		(property "Description" "LIN Transceiver with Voltage Regulator, 3.3V/5V, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN Transceiver regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP2021A-xxxxSN_0_1")
		(symbol "MCP2021A-xxxxSN_1_1"
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RXD")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "TXD")
				(number "4")
			)
			(pin open_collector line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "LBUS")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBB")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_out line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VREG")
				(number "3")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "CS/LWAKE")
				(number "2")
			)
			(pin open_collector line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{FAULT}/TXE")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2022A-xxxxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.811 8.763 0)
		)
		(property "Value" "MCP2022A-xxxxP"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0.635 1.905 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002298C.pdf"
			(at 0.635 1.905 0)
		)
		(property "Description" "LIN Transceiver with Voltage Regulator, 3.3V/5V, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN Transceiver regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP2022A-xxxxP_0_1")
		(symbol "MCP2022A-xxxxP_1_1"
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RXD")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "TXD")
				(number "4")
			)
			(pin open_collector line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "LBUS")
				(number "12")
			)
			(pin no_connect line
				(at -10.16 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBB")
				(number "13")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "11")
			)
			(pin power_out line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VREG")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "CS/LWAKE")
				(number "2")
			)
			(pin open_collector line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{FAULT}/TXE")
				(number "14")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2022A-xxxxSL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.811 8.763 0)
		)
		(property "Value" "MCP2022A-xxxxSL"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0.635 1.905 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002298C.pdf"
			(at 0.635 1.905 0)
		)
		(property "Description" "LIN Transceiver with Voltage Regulator, 3.3V/5V, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN Transceiver regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP2022A-xxxxSL_0_1")
		(symbol "MCP2022A-xxxxSL_1_1"
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RXD")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "TXD")
				(number "4")
			)
			(pin open_collector line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "LBUS")
				(number "12")
			)
			(pin no_connect line
				(at -10.16 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBB")
				(number "13")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "11")
			)
			(pin power_out line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VREG")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "CS/LWAKE")
				(number "2")
			)
			(pin open_collector line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{FAULT}/TXE")
				(number "14")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2022A-xxxxST"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.811 8.763 0)
		)
		(property "Value" "MCP2022A-xxxxST"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0.635 1.905 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20002298C.pdf"
			(at 0.635 1.905 0)
		)
		(property "Description" "LIN Transceiver with Voltage Regulator, 3.3V/5V, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN Transceiver regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2022A-xxxxST_0_1")
		(symbol "MCP2022A-xxxxST_1_1"
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RXD")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "TXD")
				(number "4")
			)
			(pin open_collector line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "LBUS")
				(number "12")
			)
			(pin no_connect line
				(at -10.16 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBB")
				(number "13")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "11")
			)
			(pin power_out line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VREG")
				(number "3")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "CS/LWAKE")
				(number "2")
			)
			(pin open_collector line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{FAULT}/TXE")
				(number "14")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2050-330-EMQ"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 -13.97 0)
		)
		(property "Value" "MCP2050-330-EMQ"
			(at -22.86 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_5x5mm_P0.65mm_EP3.35x3.35mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22299B.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "LIN Transceiver with Voltage Regulator, 3.3V, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN transceiver regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2050-330-EMQ_0_1")
		(symbol "MCP2050-330-EMQ_1_1"
			(pin open_collector line
				(at -25.4 0 0)
				(length 2.54)
				(name "LBUS")
				(number "7")
			)
			(pin no_connect line
				(at -22.86 12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -22.86 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -22.86 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -22.86 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at -22.86 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -22.86 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -22.86 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at -22.86 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "PAD")
				(number "21")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VBB")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_out line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VREG")
				(number "3")
			)
			(pin input line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "TXD")
				(number "4")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "RXD")
				(number "1")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "VBAT_RATIO")
				(number "18")
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "CS/LWAKE")
				(number "2")
			)
			(pin open_collector line
				(at 25.4 0 180)
				(length 2.54)
				(name "FAULT/TXE")
				(number "13")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "~{WWDTTRIG}")
				(number "15")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "~{WWDTRESET}")
				(number "17")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin input line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "WWDTSELECT")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2050-330-EP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 -13.97 0)
		)
		(property "Value" "MCP2050-330-EP"
			(at -22.86 16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22299B.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "LIN Transceiver with Voltage Regulator, 3.3V, PDIP"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN transceiver regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP2050-330-EP_0_1")
		(symbol "MCP2050-330-EP_1_1"
			(pin open_collector line
				(at -25.4 0 0)
				(length 2.54)
				(name "LBUS")
				(number "9")
			)
			(pin no_connect line
				(at -22.86 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VBB")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_out line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VREG")
				(number "4")
			)
			(pin input line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "TXD")
				(number "5")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "RXD")
				(number "2")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "VBAT_RATIO")
				(number "1")
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "CS/LWAKE")
				(number "3")
			)
			(pin open_collector line
				(at 25.4 0 180)
				(length 2.54)
				(name "FAULT/TXE")
				(number "11")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "~{WWDTTRIG}")
				(number "13")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "~{WWDTRESET}")
				(number "14")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "~{RESET}")
				(number "6")
			)
			(pin input line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "WWDTSELECT")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2050-330-ESL"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 -13.97 0)
		)
		(property "Value" "MCP2050-330-ESL"
			(at -22.86 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22299B.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "LIN Transceiver with Voltage Regulator, 3.3V, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN transceiver regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP2050-330-ESL_0_1")
		(symbol "MCP2050-330-ESL_1_1"
			(pin open_collector line
				(at -25.4 0 0)
				(length 2.54)
				(name "LBUS")
				(number "9")
			)
			(pin no_connect line
				(at -22.86 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VBB")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_out line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VREG")
				(number "4")
			)
			(pin input line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "TXD")
				(number "5")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "RXD")
				(number "2")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "VBAT_RATIO")
				(number "1")
			)
			(pin input line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "CS/LWAKE")
				(number "3")
			)
			(pin open_collector line
				(at 25.4 0 180)
				(length 2.54)
				(name "FAULT/TXE")
				(number "11")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "~{WWDTTRIG}")
				(number "13")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "~{WWDTRESET}")
				(number "14")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "~{RESET}")
				(number "6")
			)
			(pin input line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "WWDTSELECT")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2515-xSO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.685 0)
		)
		(property "Value" "MCP2515-xSO"
			(at 19.05 20.32 0)
		)
		(property "Footprint" "Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21801e.pdf"
			(at 2.54 -20.32 0)
		)
		(property "Description" "Stand-Alone CAN Controller with SPI Interface, SOIC-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN Controller SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x11.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP2515-xSO_0_1")
		(symbol "MCP2515-xSO_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "SI")
				(number "14")
			)
			(pin output line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "SO")
				(number "15")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{CS}")
				(number "16")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SCK")
				(number "13")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "OSC2")
				(number "7")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "OSC1")
				(number "8")
			)
			(pin output line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CLKOUT/SOF")
				(number "3")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "RXCAN")
				(number "2")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "TXCAN")
				(number "1")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "~{INT}")
				(number "12")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{RX0BF}")
				(number "11")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RX1BF}")
				(number "10")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{TX0RTS}")
				(number "4")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "~{TX1RTS}")
				(number "5")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{TX2RTS}")
				(number "6")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2515-xST"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.685 0)
		)
		(property "Value" "MCP2515-xST"
			(at 19.05 20.32 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21801e.pdf"
			(at 2.54 -20.32 0)
		)
		(property "Description" "Stand-Alone CAN Controller with SPI Interface, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN Controller SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2515-xST_0_1")
		(symbol "MCP2515-xST_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "SI")
				(number "16")
			)
			(pin output line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "SO")
				(number "17")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{CS}")
				(number "18")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SCK")
				(number "14")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "OSC2")
				(number "8")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "OSC1")
				(number "9")
			)
			(pin output line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "CLKOUT/SOF")
				(number "3")
			)
			(pin no_connect line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "10")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "RXCAN")
				(number "2")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "TXCAN")
				(number "1")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "~{INT}")
				(number "13")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{RX0BF}")
				(number "12")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RX1BF}")
				(number "11")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{TX0RTS}")
				(number "4")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "~{TX1RTS}")
				(number "5")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{TX2RTS}")
				(number "7")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2517FD-xJHA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 12.7 0)
		)
		(property "Value" "MCP2517FD-xJHA"
			(at 2.54 12.7 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x4.5mm_P0.65mm_EP1.65x4.25mm"
			(at 5.08 -20.32 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MCP2517FD-External-CAN-FD-Controller-with-SPI-Interface-20005688B.pdf"
			(at 5.08 -17.78 0)
		)
		(property "Description" "External CAN FD Controller with SPI Interface, VDFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD Controller SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x4.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2517FD-xJHA_0_1")
		(symbol "MCP2517FD-xJHA_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SDI")
				(number "11")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SDO")
				(number "12")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "13")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "SCK")
				(number "10")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "OSC2")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "OSC1")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RXCAN")
				(number "2")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "TXCAN")
				(number "1")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CLKO/SOF")
				(number "3")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{INT}")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{INT0}/GPIO0/XSTBY")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{INT1}/GPIO1")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2517FD-xSL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 12.7 0)
		)
		(property "Value" "MCP2517FD-xSL"
			(at 2.54 12.7 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 5.08 -20.32 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/MCP2517FD-External-CAN-FD-Controller-with-SPI-Interface-20005688B.pdf"
			(at 5.08 -17.78 0)
		)
		(property "Description" "External CAN FD Controller with SPI Interface, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD Controller SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP2517FD-xSL_0_1")
		(symbol "MCP2517FD-xSL_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SDI")
				(number "11")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SDO")
				(number "12")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "~{CS}")
				(number "13")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "SCK")
				(number "10")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "OSC2")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "OSC1")
				(number "6")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RXCAN")
				(number "2")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "TXCAN")
				(number "1")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CLKO/SOF")
				(number "3")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{INT}")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{INT0}/GPIO0/XSTBY")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{INT1}/GPIO1")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP251863T-E-9PX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 19.304 0)
		)
		(property "Value" "MCP251863T-E-9PX"
			(at 4.572 19.304 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-28-1EP_5x5mm_P0.5mm_EP3.25x3.25mm"
			(at 5.08 -26.67 0)
		)
		(property "Datasheet" "https://cz.mouser.com/datasheet/2/268/MCP251863_External_CAN_FD_Controller_with_Integrat-3442054.pdf"
			(at 5.08 -24.13 0)
		)
		(property "Description" "External CAN FD Controller with Integrated Transceiver, VQFN-28"
			(at 32.258 -21.844 0)
		)
		(property "ki_keywords" "CAN FD Controller Transceiver SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP251863T-E-9PX_0_1")
		(symbol "MCP251863T-E-9PX_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "STBY")
				(number "18")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SDI")
				(number "23")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SDO")
				(number "24")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "25")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCK")
				(number "22")
			)
			(pin output line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "~{INT}")
				(number "3")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "~{INT0}")
				(number "9")
				(alternate "GPIO0" bidirectional line)
				(alternate "XSTBY" input line)
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{INT1}")
				(number "8")
				(alternate "GPIO1" bidirectional line)
			)
			(pin output line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "OSC2")
				(number "4")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "OSC1")
				(number "5")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "VIO")
				(number "14")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin no_connect line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "7")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "13")
			)
			(pin no_connect line
				(at 5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin no_connect line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "CANH")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "CANL")
				(number "16")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "TXD")
				(number "20")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RXD")
				(number "11")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "RXCAN")
				(number "1")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "TXCAN")
				(number "28")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "CLKO")
				(number "2")
				(alternate "SOF" output line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP251863T-H-SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 19.304 0)
		)
		(property "Value" "MCP251863T-H-SS"
			(at 4.572 19.304 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 5.08 -26.67 0)
		)
		(property "Datasheet" "https://cz.mouser.com/datasheet/2/268/MCP251863_External_CAN_FD_Controller_with_Integrat-3442054.pdf"
			(at 5.08 -24.13 0)
		)
		(property "Description" "External CAN FD Controller with Integrated Transceiver, SSOP-28"
			(at 32.258 -21.844 0)
		)
		(property "ki_keywords" "CAN FD Controller Transceiver SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP251863T-H-SS_0_1")
		(symbol "MCP251863T-H-SS_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "STBY")
				(number "5")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SDI")
				(number "10")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SDO")
				(number "11")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "~{CS}")
				(number "13")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCK")
				(number "9")
			)
			(pin output line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "~{INT}")
				(number "19")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "~{INT0}")
				(number "7")
				(alternate "GPIO0" bidirectional line)
				(alternate "XSTBY" input line)
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{INT1}")
				(number "6")
				(alternate "GPIO1" bidirectional line)
			)
			(pin output line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "OSC2")
				(number "20")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "OSC1")
				(number "21")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "VIO")
				(number "1")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "24")
			)
			(pin no_connect line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "22")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "25")
			)
			(pin no_connect line
				(at 5.08 17.78 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "CANH")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "CANL")
				(number "3")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "TXD")
				(number "23")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RXD")
				(number "28")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "RXCAN")
				(number "16")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "TXCAN")
				(number "15")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "CLKO")
				(number "18")
				(alternate "SOF" output line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2542FDxMF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2542FDxMF"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP2542FD-4FD-MCP2542WFD-4WFD-Data-Sheet20005514B.pdf"
			(at 0 0 0)
		)
		(property "Description" "CAN-FD Transceiver, Wake-Up on CAN activity, 8Mbps, 5V supply, STBY pin, 3x3 DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2542FDxMF_0_1")
		(symbol "MCP2542FDxMF_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STBY")
				(number "8")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2551-I-P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2551-I-P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21667d.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP2551-I-P_0_1")
		(symbol "MCP2551-I-P_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_out line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Vref")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "Rs")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2551-I-SN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2551-I-SN"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/21667d.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP2551-I-SN_0_1")
		(symbol "MCP2551-I-SN_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_out line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Vref")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "Rs")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2557FD-xMF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 10.16 0)
		)
		(property "Value" "MCP2557FD-xMF"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/20005533A.pdf"
			(at 0 0 0)
		)
		(property "Description" "CAN FD Transceiver with Silent Mode, up to 8 Mbps, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2557FD-xMF_0_1")
		(symbol "MCP2557FD-xMF_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2557FD-xMNY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 10.16 0)
		)
		(property "Value" "MCP2557FD-xMNY"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8-1EP_3x2mm_P0.5mm_EP1.80x1.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/20005533A.pdf"
			(at 0 0 0)
		)
		(property "Description" "CAN FD Transceiver with Silent Mode, up to 8 Mbps, TDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP2557FD-xMNY_0_1")
		(symbol "MCP2557FD-xMNY_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2557FD-xSN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 10.16 0)
		)
		(property "Value" "MCP2557FD-xSN"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/20005533A.pdf"
			(at 0 0 0)
		)
		(property "Description" "CAN FD Transceiver with Silent Mode, up to 8 Mbps, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP2557FD-xSN_0_1")
		(symbol "MCP2557FD-xSN_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2558FD-xMF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 10.16 0)
		)
		(property "Value" "MCP2558FD-xMF"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/20005533A.pdf"
			(at 0 0 0)
		)
		(property "Description" "CAN FD Transceiver with Silent Mode, up to 8 Mbps, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2558FD-xMF_0_1")
		(symbol "MCP2558FD-xMF_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2558FD-xMNY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 10.16 0)
		)
		(property "Value" "MCP2558FD-xMNY"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8-1EP_3x2mm_P0.5mm_EP1.80x1.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/20005533A.pdf"
			(at 0 0 0)
		)
		(property "Description" "CAN FD Transceiver with Silent Mode, up to 8 Mbps, TDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP2558FD-xMNY_0_1")
		(symbol "MCP2558FD-xMNY_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2558FD-xSN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 10.16 0)
		)
		(property "Value" "MCP2558FD-xSN"
			(at 2.54 10.16 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/20005533A.pdf"
			(at 0 0 0)
		)
		(property "Description" "CAN FD Transceiver with Silent Mode, up to 8 Mbps, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP2558FD-xSN_0_1")
		(symbol "MCP2558FD-xSN_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2561-E-MF"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2561-E-MF"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 5.08 -17.78 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 5.08 -15.24 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, SPLIT pin, -40C to +125C, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2561-E-MF_0_1")
		(symbol "MCP2561-E-MF_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STBY")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "SPLIT")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2561-E-P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2561-E-P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, SPLIT pin, -40C to +125C, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP2561-E-P_0_1")
		(symbol "MCP2561-E-P_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STBY")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "SPLIT")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2561-E-SN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2561-E-SN"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, SPLIT pin, -40C to +125C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP2561-E-SN_0_1")
		(symbol "MCP2561-E-SN_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STBY")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "SPLIT")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2562-E-MF"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2562-E-MF"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +125C, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2562-E-MF_0_1")
		(symbol "MCP2562-E-MF_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Vio")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SHDN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "PAD")
				(number "9")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2562-E-P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2562-E-P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +125C, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP2562-E-P_0_1")
		(symbol "MCP2562-E-P_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Vio")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STBY")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2562-E-SN"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2562-E-SN"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +125C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP2562-E-SN_0_1")
		(symbol "MCP2562-E-SN_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Vio")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STBY")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP25625-x-SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 26.67 0)
		)
		(property "Value" "MCP25625-x-SS"
			(at 15.24 26.67 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 2.54 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005282B.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "Stand-Alone CAN Controller with SPI Interface and integated Transceiver, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN Controller SPI Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP25625-x-SS_0_1")
		(symbol "MCP25625-x-SS_1_1"
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "STBY")
				(number "5")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "SCK")
				(number "14")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "SI")
				(number "15")
			)
			(pin output line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "SO")
				(number "16")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{CS}")
				(number "17")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "18")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "~{Tx0RTS}")
				(number "23")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "~{Tx1RTS}")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "~{Tx2RTS}")
				(number "7")
			)
			(pin output line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "~{Rx0BF}")
				(number "12")
			)
			(pin output line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "~{Rx1BF}")
				(number "11")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "~{INT}")
				(number "13")
			)
			(pin output line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "CLKOUT")
				(number "22")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VIO")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VDDA")
				(number "27")
			)
			(pin power_in line
				(at 5.08 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "26")
			)
			(pin no_connect line
				(at 12.7 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at 12.7 -17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "CANH")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "CANL")
				(number "3")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "RXD")
				(number "28")
			)
			(pin input line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "TXD")
				(number "24")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "TxCAN")
				(number "20")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RxCAN")
				(number "21")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OSC2")
				(number "8")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "OSC1")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA82C251"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 13.97 0)
		)
		(property "Value" "PCA82C251"
			(at -5.08 11.43 0)
		)
		(property "Footprint" "Package_SO:SO-8_3.9x4.9mm_P1.27mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCA82C251.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "CAN Transceiver for 24V Systems, SO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "BUS CAN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PCA82C251_0_1"
			(text "Volt"
				(at 1.27 7.62 0)
			)
		)
		(symbol "PCA82C251_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 5.08)
				(name "VCC")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 5.08)
				(name "TxD")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 5.08)
				(name "Rsl")
				(number "8")
			)
			(pin output line
				(at -10.16 -7.62 0)
				(length 5.08)
				(name "RxD")
				(number "4")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 5.08)
				(name "Vref")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 5.08)
				(name "CAN+")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 5.08)
				(name "CAN-")
				(number "6")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 5.08)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65HVD1050D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "SN65HVD1050D"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65hvd1050.pdf"
			(at -2.54 10.16 0)
		)
		(property "Description" "CAN Bus Transceiver, EMC optimised, 5.0V, 1Mbps, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transceiver ti canbus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65HVD1050D_0_1")
		(symbol "SN65HVD1050D_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin passive line
				(at 12.7 0 180)
				(length 2.54)
				(name "VREF")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65HVD230"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 10.16 0)
		)
		(property "Value" "SN65HVD230"
			(at -2.54 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65hvd230.pdf"
			(at -2.54 10.16 0)
		)
		(property "Description" "CAN Bus Transceivers, 3.3V, 1Mbps, Low-Power capabilities, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transeiver ti low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65HVD230_0_1")
		(symbol "SN65HVD230_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "R")
				(number "4")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "Vref")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Rs")
				(number "8")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65HVD232"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 10.16 0)
		)
		(property "Value" "SN65HVD232"
			(at -2.54 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65hvd230.pdf"
			(at -2.54 10.16 0)
		)
		(property "Description" "CAN Bus Transceivers, 3.3V, 1Mbps, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transeiver ti"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65HVD232_0_1")
		(symbol "SN65HVD232_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "R")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65HVD233"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 10.16 0)
		)
		(property "Value" "SN65HVD233"
			(at -2.54 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65hvd234.pdf"
			(at -2.54 10.16 0)
		)
		(property "Description" "CAN Bus Transceiver, 3.3V, 1Mbps, Loopback feature, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transeiver ti"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65HVD233_0_1")
		(symbol "SN65HVD233_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "R")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "LBK")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Rs")
				(number "8")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65HVD234"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 10.16 0)
		)
		(property "Value" "SN65HVD234"
			(at -2.54 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65hvd234.pdf"
			(at -2.54 10.16 0)
		)
		(property "Description" "CAN Bus Transceiver, 3.3V, 1Mbps, Enable feature, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transeiver ti"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65HVD234_0_1")
		(symbol "SN65HVD234_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "R")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Rs")
				(number "8")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65HVD235"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 10.16 0)
		)
		(property "Value" "SN65HVD235"
			(at -2.54 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65hvd234.pdf"
			(at -2.54 10.16 0)
		)
		(property "Description" "CAN Bus Transceiver, 3.3V, 1Mbps, Autobaud feature, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transeiver ti"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65HVD235_0_1")
		(symbol "SN65HVD235_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D")
				(number "1")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "R")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "AB")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "Rs")
				(number "8")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65HVD255D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "SN65HVD255D"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn65hvd257.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "CAN Bus Transceiver with Fast Loop Times for Highly Loaded Networks, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transceiver ti canbus 5.0V 1Mbps SOIC-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65HVD255D_0_1")
		(symbol "SN65HVD255D_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65HVD256D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "SN65HVD256D"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn65hvd257.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "CAN Bus Transceiver with Fast Loop Times for Highly Loaded Networks, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transceiver ti canbus 5.0V 1Mbps SOIC-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65HVD256D_0_1")
		(symbol "SN65HVD256D_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VRXD")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65HVD257D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "SN65HVD257D"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn65hvd257.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "CAN Bus Transceiver with Fast Loop Times for Highly Loaded Networks, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transceiver ti canbus 5.0V 1Mbps SOIC-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65HVD257D_0_1")
		(symbol "SN65HVD257D_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin open_collector line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "FAULT")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCAN1043xDxQ1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "TCAN1043xDxQ1"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tcan1043-q1.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "High-speed CAN-FD Transceiver with Sleep Mode, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD High Speed CAN Transceiver Sleep VIO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TCAN1043xDxQ1_0_1")
		(symbol "TCAN1043xDxQ1_1_1"
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{STB}")
				(number "14")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "WAKE")
				(number "9")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VSUP")
				(number "10")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CANH")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "CANL")
				(number "12")
			)
			(pin open_emitter line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "INH")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCAN330"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TCAN330"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tcan337.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 3.3V supply, silent mode, shutdown mode, SOT-23-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOT?23* *SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TCAN330_0_1")
		(symbol "TCAN330_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin tri_state line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SHDN")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCAN332"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TCAN332"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tcan337.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 3.3V supply, SOT-23-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOT?23* *SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TCAN332_0_1")
		(symbol "TCAN332_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin tri_state line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCAN334"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TCAN334"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tcan337.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 3.3V supply, low power standby mode, shutdown mode, SOT-23-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOT?23* *SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TCAN334_0_1")
		(symbol "TCAN334_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin tri_state line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SHDN")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STB")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCAN337"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TCAN337"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tcan337.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 3.3V supply, silent mode, fault output, SOT-23-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOT?23* *SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TCAN337_0_1")
		(symbol "TCAN337_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin tri_state line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin open_collector line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "FAULT")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCAN4550RGY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 -24.13 0)
		)
		(property "Value" "TCAN4550RGY"
			(at 2.54 -24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGY_R-PVQFN-N20_EP2.05x3.05mm"
			(at 7.62 -30.48 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tcan4550.pdf"
			(at 7.62 -27.94 0)
		)
		(property "Description" "CAN-FD controller with integrated transceiver, 5Mbps, 3.3V to 5V supply, SPI interface, VQFN-20"
			(at 7.62 -33.02 0)
		)
		(property "ki_keywords" "M_CAN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*RGY*PVQFN*"
			(at 0 0 0)
		)
		(symbol "TCAN4550RGY_0_1")
		(symbol "TCAN4550RGY_1_0"
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "GPO2")
				(number "9")
			)
			(pin output line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "OSC2")
				(number "20")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "RST")
				(number "19")
			)
			(pin power_out line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "V_{IO}")
				(number "17")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "V_{SUP}")
				(number "14")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "V_{CCOUT}")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "CANL")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "CANH")
				(number "11")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "INH")
				(number "15")
			)
			(pin input line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "WAKE")
				(number "12")
			)
			(pin output line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "FLTR")
				(number "18")
			)
		)
		(symbol "TCAN4550RGY_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "SCLK")
				(number "4")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SDI")
				(number "5")
			)
			(pin output line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "SDO")
				(number "6")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{CS}")
				(number "7")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{INT}")
				(number "8")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{WKRQ}")
				(number "2")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "GPO1")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "OSC1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCAN4551RGYRQ1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 -24.13 0)
		)
		(property "Value" "TCAN4551RGYRQ1"
			(at 2.54 -24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGY_R-PVQFN-N20_EP2.05x3.05mm"
			(at 7.62 -30.48 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tcan4551-q1.pdf"
			(at 7.62 -27.94 0)
		)
		(property "Description" "CAN-FD controller with integrated transceiver, 5Mbps, 3.3V to 5V supply, SPI interface, VQFN-20"
			(at 7.62 -33.02 0)
		)
		(property "ki_keywords" "M_CAN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*RGY*PVQFN*"
			(at 0 0 0)
		)
		(symbol "TCAN4551RGYRQ1_0_1")
		(symbol "TCAN4551RGYRQ1_1_0"
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "GPO2")
				(number "9")
			)
			(pin output line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "OSC2")
				(number "20")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "RST")
				(number "19")
			)
			(pin power_out line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "V_{IO}")
				(number "17")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "V_{SUP}")
				(number "14")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin output line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "V_{CCFLTR}")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "CANL")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "CANH")
				(number "11")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "INH")
				(number "15")
			)
			(pin input line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "WAKE")
				(number "12")
			)
			(pin output line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "FLTR")
				(number "18")
			)
		)
		(symbol "TCAN4551RGYRQ1_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "SCLK")
				(number "4")
			)
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SDI")
				(number "5")
			)
			(pin output line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "SDO")
				(number "6")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{CS}")
				(number "7")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{INT}")
				(number "8")
			)
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{WKRQ}")
				(number "2")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "GPO1")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "OSC1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1021T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1021T"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1021.pdf"
			(at -10.16 11.43 0)
		)
		(property "Description" "LIN 2.1/SAE J2602 transceiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN 2.1 SAE J2602 Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TJA1021T_0_1")
		(symbol "TJA1021T_1_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RXD")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{SLP}")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{WAKE}")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "INH")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "LIN")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1021TK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1021TK"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1021.pdf"
			(at 0 0 0)
		)
		(property "Description" "LIN 2.1/SAE J2602 transceiver, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN 2.1 SAE J2602 Transceiver HVSON-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TJA1021TK_0_1")
		(symbol "TJA1021TK_1_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RXD")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{SLP}")
				(number "2")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{WAKE}")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "INH")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "LIN")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1029T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1029T"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1029.pdf"
			(at 0 0 0)
		)
		(property "Description" "LIN 2.2A/SAE J2602 transceiver with TXD dominant timeout, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN 2.2A/SAE J2602 Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TJA1029T_0_1")
		(symbol "TJA1029T_1_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RXD")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{SLP}")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "LIN")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1029TK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1029TK"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1029.pdf"
			(at 0 0 0)
		)
		(property "Description" "LIN 2.2A/SAE J2602 transceiver with TXD dominant timeout, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN 2.2A/SAE J2602 Transceiver HVSON-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TJA1029TK_0_1")
		(symbol "TJA1029TK_1_1"
			(pin open_collector line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RXD")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "TXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{SLP}")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBAT")
				(number "7")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "LIN")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1043T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "TJA1043T"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TJA1043.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "High-speed CAN-FD Transceiver with Sleep Mode, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD High Speed CAN Transceiver Sleep Split-Pin VIO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TJA1043T_0_1")
		(symbol "TJA1043T_1_1"
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{STB}")
				(number "14")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{ERR}")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "WAKE")
				(number "9")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VBAT")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CANH")
				(number "13")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SPLIT")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "CANL")
				(number "12")
			)
			(pin open_emitter line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "INH")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1043TK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "TJA1043TK"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x4.5mm_P0.65mm_EP1.65x4.25mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TJA1043.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "High-speed CAN-FD Transceiver with Sleep Mode, HVSON-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD High Speed CAN Transceiver Sleep Split-Pin VIO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x4.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TJA1043TK_0_1")
		(symbol "TJA1043TK_1_1"
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "EN")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{STB}")
				(number "14")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{ERR}")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "WAKE")
				(number "9")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VBAT")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CANH")
				(number "13")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SPLIT")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "CANL")
				(number "12")
			)
			(pin open_emitter line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "INH")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1049T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1049T"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1049.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, standby mode, split pin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TJA1049T_0_1")
		(symbol "TJA1049T_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STB")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "SPLIT")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1049T-3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1049T-3"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1049.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, separate VIO, standby mode, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TJA1049T-3_0_1")
		(symbol "TJA1049T-3_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STB")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1049TK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1049TK"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1049.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, standby mode, DFN-8-1EP"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver HVSON-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm* HVSON*"
			(at 0 0 0)
		)
		(symbol "TJA1049TK_0_1")
		(symbol "TJA1049TK_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STB")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "SPLIT")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1049TK-3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1049TK-3"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1049.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, separate VIO, standby mode, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver HVSON-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm* HVSON*"
			(at 0 0 0)
		)
		(symbol "TJA1049TK-3_0_1")
		(symbol "TJA1049TK-3_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "STB")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1051T"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1051T"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1051.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, silent mode, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TJA1051T_0_1")
		(symbol "TJA1051T_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1051T-3"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1051T-3"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1051.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, separate VIO, silent mode, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TJA1051T-3_0_1")
		(symbol "TJA1051T-3_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1051T-E"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1051T-E"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1051.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, enable pin, silent mode, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TJA1051T-E_0_1")
		(symbol "TJA1051T-E_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1051TK-3"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1051TK-3"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1051.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, separate VIO, silent mode, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver HVSON-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TJA1051TK-3_0_1")
		(symbol "TJA1051TK-3_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin power_in line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1052i-1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "TJA1052i-1"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TJA1052I.pdf"
			(at -7.62 15.24 0)
		)
		(property "Description" "Isolated CAN Transceiver 1.0kV, up to 5Mbps"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transceiver isolated protected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TJA1052i-1_0_1")
		(symbol "TJA1052i-1_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "3")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RXD")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "7")
			)
			(pin passive line
				(at -5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin passive line
				(at 5.08 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VDD2")
				(number "11")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin passive line
				(at 5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "10")
			)
			(pin passive line
				(at 5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "CANH")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "12")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "STB")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1145T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "TJA1145T"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TJA1145.pdf"
			(at -10.16 13.97 0)
		)
		(property "Description" "High-speed CAN transceiver for partial networking, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD High Speed CAN Transceiver Sleep VIO Partial Networking SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TJA1145T_0_1")
		(symbol "TJA1145T_1_1"
			(pin output line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDO")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SCK")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDI")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{SCS}")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "WAKE")
				(number "9")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "BAT")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "12")
			)
			(pin open_emitter line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "INH")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TJA1145TK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "TJA1145TK"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x4.5mm_P0.65mm_EP1.65x4.25mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TJA1145.pdf"
			(at -10.16 13.97 0)
		)
		(property "Description" "High-speed CAN transceiver for partial networking, DFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD High Speed CAN Transceiver Sleep VIO Partial Networking SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x4.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TJA1145TK_0_1")
		(symbol "TJA1145TK_1_1"
			(pin output line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDO")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SCK")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDI")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{SCS}")
				(number "14")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "WAKE")
				(number "9")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "BAT")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "12")
			)
			(pin open_emitter line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "INH")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CA-IF1042LVS"
		(extends "TJA1049T-3")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "CA-IF1042LVS"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2401191740_Chipanalog-CA-IF1042LS-Q1_C20598901.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver up to 5 Mbps, separate VIO, standby mode, ±30V bus common mode voltage, 5V supply, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "chipanalog"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2050-500-EMQ"
		(extends "MCP2050-330-EMQ")
		(property "Reference" "U"
			(at -22.86 -13.97 0)
		)
		(property "Value" "MCP2050-500-EMQ"
			(at -22.86 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_5x5mm_P0.65mm_EP3.35x3.35mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22299B.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "LIN Transceiver with Voltage Regulator, 5V, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN transceiver regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2050-500-EP"
		(extends "MCP2050-330-EP")
		(property "Reference" "U"
			(at -22.86 -13.97 0)
		)
		(property "Value" "MCP2050-500-EP"
			(at -22.86 16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22299B.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "LIN Transceiver with Voltage Regulator, 5V, PDIP"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN transceiver regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2050-500-ESL"
		(extends "MCP2050-330-ESL")
		(property "Reference" "U"
			(at -22.86 -13.97 0)
		)
		(property "Value" "MCP2050-500-ESL"
			(at -22.86 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22299B.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "LIN Transceiver with Voltage Regulator, 5V, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "LIN transceiver regulator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2518FD-xQBB"
		(extends "MCP2517FD-xJHA")
		(property "Reference" "U"
			(at 8.89 13.97 0)
		)
		(property "Value" "MCP2518FD-xQBB"
			(at -3.81 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x4.5mm_P0.65mm_EP1.65x4.25mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/External-CAN-FD-Controller-with-SPI-Interface-DS20006027B.pdf"
			(at 1.27 -16.51 0)
		)
		(property "Description" "CAN FD Controller with SPI Interface, up to 8 Mbps, Vdd 2.7..5.5V,  functional safety ready, VDFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "microchip"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x4.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2542WFDxMF"
		(extends "MCP2542FDxMF")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2542WFDxMF"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP2542FD-4FD-MCP2542WFD-4WFD-Data-Sheet20005514B.pdf"
			(at 0 0 0)
		)
		(property "Description" "CAN-FD Transceiver, Wake-Up on CAN Pattern, 8Mbps, 5V supply, STBY pin, 3x3 DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN transceiver WUP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2561-H-MF"
		(extends "MCP2561-E-MF")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2561-H-MF"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, SPLIT pin, -40C to +150C, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2561-H-P"
		(extends "MCP2561-E-P")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2561-H-P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, SPLIT pin, -40C to +150C, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2561-H-SN"
		(extends "MCP2561-E-SN")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2561-H-SN"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, SPLIT pin, -40C to +150C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2562-H-MF"
		(extends "MCP2562-E-MF")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2562-H-MF"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +150C, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2562-H-P"
		(extends "MCP2562-E-P")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2562-H-P"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +150C, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2562-H-SN"
		(extends "MCP2562-E-SN")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MCP2562-H-SN"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/25167A.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 5V supply, Vio pin, -40C to +150C, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN65HVD231"
		(extends "SN65HVD230")
		(property "Reference" "U"
			(at -2.54 10.16 0)
		)
		(property "Value" "SN65HVD231"
			(at -2.54 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65hvd230.pdf"
			(at -2.54 10.16 0)
		)
		(property "Description" "CAN Bus Transceivers, 3.3V, 1Mbps,Ultra Low-Power capabilities, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transeiver ti ulp low-power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCAN330G"
		(extends "TCAN330")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TCAN330G"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tcan337.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver with CAN FD, 5Mbps, 3.3V supply, silent mode, shutdown mode, SOT-23-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOT?23* *SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCAN332G"
		(extends "TCAN332")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TCAN332G"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tcan337.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver with CAN FD, 5Mbps, 3.3V supply, SOT-23-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOT?23* *SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCAN334G"
		(extends "TCAN334")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TCAN334G"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tcan337.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver with CAN FD, 5Mbps, 3.3V supply, low power standby mode, shutdown mode, SOT-23-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOT?23* *SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCAN337G"
		(extends "TCAN337")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TCAN337G"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tcan337.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver with CAN FD, 5Mbps, 3.3V supply, silent mode, fault output, SOT-23-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSOT?23* *SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TJA1042T"
		(extends "TJA1049T")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1042T"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1042.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, standby mode, split pin, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TJA1042T-3"
		(extends "TJA1049T-3")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1042T-3"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1042.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, separate VIO, standby mode, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TJA1042TK-3"
		(extends "TJA1049TK-3")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "TJA1042TK-3"
			(at 1.27 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.65mm_EP1.55x2.4mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/TJA1042.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, separate VIO, standby mode, DFN-8-1EP"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver HVSON-8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.65mm* HVSON*"
			(at 0 0 0)
		)
	)
	(symbol "TJA1052i-2"
		(extends "TJA1052i-1")
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "TJA1052i-2"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TJA1052I.pdf"
			(at -7.62 15.24 0)
		)
		(property "Description" "Isolated CAN Transceiver 2.5kV, up to 5Mbps"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transceiver isolated protected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TJA1052i-5"
		(extends "TJA1052i-1")
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "TJA1052i-5"
			(at 17.78 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TJA1052I.pdf"
			(at -7.62 15.24 0)
		)
		(property "Description" "Isolated CAN Transceiver 5.0kV, up to 5Mbps"
			(at 0 0 0)
		)
		(property "ki_keywords" "can transceiver isolated protected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TJA1145T-FD"
		(extends "TJA1145T")
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "TJA1145T-FD"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TJA1145.pdf"
			(at -10.16 13.97 0)
		)
		(property "Description" "High-speed CAN transceiver for partial networking with FD-passive function, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD High Speed CAN Transceiver Sleep VIO Partial Networking SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TJA1145TK-FD"
		(extends "TJA1145TK")
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "TJA1145TK-FD"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x4.5mm_P0.65mm_EP1.65x4.25mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/TJA1145.pdf"
			(at -10.16 13.97 0)
		)
		(property "Description" "High-speed CAN transceiver for partial networking with FD-passive function, DFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "CAN FD High Speed CAN Transceiver Sleep VIO Partial Networking SPI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x4.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
)
