(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "DP83848C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 39.37 0)
		)
		(property "Value" "DP83848C"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 25.4 -39.37 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dp83848c.pdf"
			(at 0 0 0)
		)
		(property "Description" "MII/RMII Single 10/100Mbps Ethernet Physical Layer Transceiver, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ethernet PHY MII RMII 10/100Mpbs"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "DP83848C_0_1")
		(symbol "DP83848C_1_1"
			(pin input line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "TXD_0")
				(number "3")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "TXD_1")
				(number "4")
			)
			(pin input line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "TXD_2")
				(number "5")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "TXD_3/SNI_MODE")
				(number "6")
			)
			(pin output line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "TX_CLK")
				(number "1")
			)
			(pin input line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "TX_EN")
				(number "2")
			)
			(pin output line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "RXD_0/PHY_AD1")
				(number "43")
			)
			(pin output line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "RXD_1/PHY_AD2")
				(number "44")
			)
			(pin output line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "RXD_2/PHY_AD3")
				(number "45")
			)
			(pin output line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "RXD_3/PHY_AD4")
				(number "46")
			)
			(pin output line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "RX_CLK")
				(number "38")
			)
			(pin output line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "RX_ER/MDIX_EN")
				(number "41")
			)
			(pin output line
				(at -25.4 0 0)
				(length 2.54)
				(name "RX_DV/MII_MODE")
				(number "39")
			)
			(pin output line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "COL/PHY_AD0")
				(number "42")
			)
			(pin output line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "CRS/CRS_DV/LED_CFG")
				(number "40")
			)
			(pin input line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "MDC")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "MDIO")
				(number "30")
			)
			(pin input line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "29")
			)
			(pin input line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PWR_DOWN/INT")
				(number "7")
			)
			(pin output line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "25M_OUT")
				(number "25")
			)
			(pin input line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "X1")
				(number "34")
			)
			(pin output line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "X2")
				(number "33")
			)
			(pin power_in line
				(at -5.08 -40.64 90)
				(length 2.54)
				(name "IOGND")
				(number "35")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "IOVDD33")
				(number "32")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 2.54)
				(name "IOGND")
				(number "47")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "IOVDD33")
				(number "48")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "DGND")
				(number "36")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "AVDD33")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "AGND")
				(number "15")
			)
			(pin power_in line
				(at 5.08 -40.64 90)
				(length 2.54)
				(name "AGND")
				(number "19")
			)
			(pin passive line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "TD+")
				(number "17")
			)
			(pin passive line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "TD-")
				(number "16")
			)
			(pin passive line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "RD+")
				(number "14")
			)
			(pin passive line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "RD-")
				(number "13")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "AN0/LED_LINK")
				(number "28")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "AN1/LED_SPEED")
				(number "27")
			)
			(pin output line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "AN_EN/LED_ACT/COL")
				(number "26")
			)
			(pin passive line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "RESERVED")
				(number "20")
			)
			(pin passive line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "RESERVED")
				(number "21")
			)
			(pin passive line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "RBIAS")
				(number "24")
			)
			(pin passive line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PFBOUT")
				(number "23")
			)
			(pin passive line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "PFBIN1")
				(number "18")
			)
			(pin passive line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "PFBIN2")
				(number "37")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ENC28J60x-ML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "ENC28J60x-ML"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 30.48 -24.13 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/39662e.pdf"
			(at 0 0 0)
		)
		(property "Description" "ENC28J60 Single Chip Ethernet Interface,QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "ENC Ethernet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*28*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ENC28J60x-ML_0_1")
		(symbol "ENC28J60x-ML_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{RESET}")
				(number "6")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SI")
				(number "3")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "SO")
				(number "2")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SCK")
				(number "4")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "5")
			)
			(pin output line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "~{INT}")
				(number "28")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "~{WOL}")
				(number "1")
			)
			(pin power_in line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "VDDOSC")
				(number "21")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "OSC1")
				(number "19")
			)
			(pin output line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "OSC2")
				(number "20")
			)
			(pin power_in line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "VSSOSC")
				(number "18")
			)
			(pin output line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "CLKOUT")
				(number "27")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "26")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDPLL")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSPLL")
				(number "17")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "LEDA")
				(number "23")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "LEDB")
				(number "22")
			)
			(pin power_in line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "VDDRX")
				(number "15")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "TPIN+")
				(number "9")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "TPIN-")
				(number "8")
			)
			(pin power_out line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "VSSRX")
				(number "7")
			)
			(pin power_in line
				(at 17.78 0 180)
				(length 2.54)
				(name "VDDTX")
				(number "11")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "TPOUT+")
				(number "13")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "TPOUT-")
				(number "12")
			)
			(pin power_out line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "VSSTX")
				(number "14")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "RBIAS")
				(number "10")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "VCAP")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ENC28J60x-SO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "ENC28J60x-SO"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 29.21 -24.13 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/39662e.pdf"
			(at 0 0 0)
		)
		(property "Description" "ENC28J60 Single Chip Ethernet Interface, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "ENC Ethernet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*28*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ENC28J60x-SO_0_1")
		(symbol "ENC28J60x-SO_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{RESET}")
				(number "10")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SI")
				(number "7")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "SO")
				(number "6")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SCK")
				(number "8")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "9")
			)
			(pin output line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "~{INT}")
				(number "4")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "~{WOL}")
				(number "5")
			)
			(pin power_in line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "VDDOSC")
				(number "25")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "OSC1")
				(number "23")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "OSC2")
				(number "24")
			)
			(pin power_in line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "VSSOSC")
				(number "22")
			)
			(pin output line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "CLKOUT")
				(number "3")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDPLL")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSPLL")
				(number "21")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "LEDA")
				(number "27")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "LEDB")
				(number "26")
			)
			(pin power_in line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "VDDRX")
				(number "19")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "TPIN+")
				(number "13")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "TPIN-")
				(number "12")
			)
			(pin power_in line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "VSSRX")
				(number "11")
			)
			(pin power_in line
				(at 17.78 0 180)
				(length 2.54)
				(name "VDDTX")
				(number "15")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "TPOUT+")
				(number "17")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "TPOUT-")
				(number "16")
			)
			(pin power_in line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "VSSTX")
				(number "18")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "RBIAS")
				(number "14")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "VCAP")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ENC28J60x-SP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "ENC28J60x-SP"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 19.05 -24.13 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/39662e.pdf"
			(at 0 0 0)
		)
		(property "Description" "ENC28J60 Single Chip Ethernet Interface, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "ENC Ethernet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*28*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ENC28J60x-SP_0_1")
		(symbol "ENC28J60x-SP_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{RESET}")
				(number "10")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SI")
				(number "7")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "SO")
				(number "6")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SCK")
				(number "8")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "9")
			)
			(pin output line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "~{INT}")
				(number "4")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "~{WOL}")
				(number "5")
			)
			(pin power_in line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "VDDOSC")
				(number "25")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "OSC1")
				(number "23")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "OSC2")
				(number "24")
			)
			(pin power_in line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "VSSOSC")
				(number "22")
			)
			(pin output line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "CLKOUT")
				(number "3")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDPLL")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSPLL")
				(number "21")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "LEDA")
				(number "27")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "LEDB")
				(number "26")
			)
			(pin power_in line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "VDDRX")
				(number "19")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "TPIN+")
				(number "13")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "TPIN-")
				(number "12")
			)
			(pin power_in line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "VSSRX")
				(number "11")
			)
			(pin power_in line
				(at 17.78 0 180)
				(length 2.54)
				(name "VDDTX")
				(number "15")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "TPOUT+")
				(number "17")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "TPOUT-")
				(number "16")
			)
			(pin power_in line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "VSSTX")
				(number "18")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "RBIAS")
				(number "14")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "VCAP")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ENC28J60x-SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 24.13 0)
		)
		(property "Value" "ENC28J60x-SS"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 29.21 -24.13 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/39662e.pdf"
			(at 0 0 0)
		)
		(property "Description" "ENC28J60 Single Chip Ethernet Interface, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "ENC Ethernet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*28*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ENC28J60x-SS_0_1")
		(symbol "ENC28J60x-SS_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{RESET}")
				(number "10")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "SI")
				(number "7")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "SO")
				(number "6")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SCK")
				(number "8")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "~{CS}")
				(number "9")
			)
			(pin output line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "~{INT}")
				(number "4")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "~{WOL}")
				(number "5")
			)
			(pin power_in line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "VDDOSC")
				(number "25")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "OSC1")
				(number "23")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "OSC2")
				(number "24")
			)
			(pin power_in line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "VSSOSC")
				(number "22")
			)
			(pin output line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "CLKOUT")
				(number "3")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDPLL")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "VSSPLL")
				(number "21")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "LEDA")
				(number "27")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "LEDB")
				(number "26")
			)
			(pin power_in line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "VDDRX")
				(number "19")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "TPIN+")
				(number "13")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "TPIN-")
				(number "12")
			)
			(pin power_in line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "VSSRX")
				(number "11")
			)
			(pin power_in line
				(at 17.78 0 180)
				(length 2.54)
				(name "VDDTX")
				(number "15")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "TPOUT+")
				(number "17")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "TPOUT-")
				(number "16")
			)
			(pin power_in line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "VSSTX")
				(number "18")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "RBIAS")
				(number "14")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "VCAP")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ENC424J600-ML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 34.29 0)
		)
		(property "Value" "ENC424J600-ML"
			(at 7.62 34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 41.91 -34.29 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39935c.pdf"
			(at 1.27 20.32 0)
		)
		(property "Description" "Stand-Alone 10/100 Ethernet Controller with SPI or Parallel Interface, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "ENC Ethernet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*44*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ENC424J600-ML_0_1")
		(symbol "ENC424J600-ML_1_1"
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "~{INT}/SPISEL")
				(number "24")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "~{CS}/CS")
				(number "34")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "SO/WR/EN")
				(number "35")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "SI/RD/R~{W}")
				(number "36")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "SCK/AL")
				(number "37")
			)
			(pin input line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PSPCFG0")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "AD0")
				(number "38")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "AD1")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "AD2")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "AD3")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "AD4")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "AD5")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "AD6")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "AD7")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "AD8")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "AD9")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "AD10")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "AD11")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "AD12")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "AD13")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "AD14")
				(number "31")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 2.54)
				(name "VDDOSC")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -35.56 90)
				(length 2.54)
				(name "VSSOSC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "VDDPLL")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "VSSPLL")
				(number "13")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDDRX")
				(number "15")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSSRX")
				(number "14")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "VDDTX")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "VSSTX")
				(number "19")
			)
			(pin passive line
				(at 2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSTX")
				(number "22")
			)
			(pin power_in line
				(at 5.08 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at 5.08 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin passive line
				(at 5.08 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "42")
			)
			(pin power_in line
				(at 7.62 -35.56 90)
				(length 2.54)
				(name "EP")
				(number "45")
			)
			(pin output line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "TPOUT+")
				(number "20")
			)
			(pin output line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "TPOUT-")
				(number "21")
			)
			(pin input line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "TPIN+")
				(number "16")
			)
			(pin input line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "TPIN-")
				(number "17")
			)
			(pin output line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "LEDA")
				(number "10")
			)
			(pin output line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "LEDB")
				(number "9")
			)
			(pin output line
				(at 22.86 0 180)
				(length 2.54)
				(name "CLKOUT")
				(number "23")
			)
			(pin input line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "OSC1")
				(number "3")
			)
			(pin output line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "OSC2")
				(number "2")
			)
			(pin input line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "RBIAS")
				(number "11")
			)
			(pin input line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "VCAP")
				(number "43")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ENC424J600-PT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 34.29 0)
		)
		(property "Value" "ENC424J600-PT"
			(at 7.62 34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 26.67 -34.29 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39935c.pdf"
			(at 1.27 20.32 0)
		)
		(property "Description" "Stand-Alone 10/100 Ethernet Controller with SPI or Parallel Interface, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "ENC Ethernet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*44*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ENC424J600-PT_0_1")
		(symbol "ENC424J600-PT_1_1"
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "~{INT}/SPISEL")
				(number "24")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "~{CS}/CS")
				(number "34")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "SO/WR/EN")
				(number "35")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "SI/RD/R~{W}")
				(number "36")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "SCK/AL")
				(number "37")
			)
			(pin input line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PSPCFG0")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "AD0")
				(number "38")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "AD1")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "AD2")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "AD3")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "AD4")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "AD5")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "AD6")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "AD7")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "AD8")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "AD9")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "AD10")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "AD11")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "AD12")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "AD13")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "AD14")
				(number "31")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 2.54)
				(name "VDDOSC")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -35.56 90)
				(length 2.54)
				(name "VSSOSC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "VDDPLL")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "VSSPLL")
				(number "13")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDDRX")
				(number "15")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSSRX")
				(number "14")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "VDDTX")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "VSSTX")
				(number "19")
			)
			(pin passive line
				(at 2.54 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSSTX")
				(number "22")
			)
			(pin power_in line
				(at 5.08 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at 5.08 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin passive line
				(at 5.08 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "42")
			)
			(pin output line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "TPOUT+")
				(number "20")
			)
			(pin output line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "TPOUT-")
				(number "21")
			)
			(pin input line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "TPIN+")
				(number "16")
			)
			(pin input line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "TPIN-")
				(number "17")
			)
			(pin output line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "LEDA")
				(number "10")
			)
			(pin output line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "LEDB")
				(number "9")
			)
			(pin output line
				(at 22.86 0 180)
				(length 2.54)
				(name "CLKOUT")
				(number "23")
			)
			(pin input line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "OSC1")
				(number "3")
			)
			(pin output line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "OSC2")
				(number "2")
			)
			(pin input line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "RBIAS")
				(number "11")
			)
			(pin input line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "VCAP")
				(number "43")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KSZ8081MLX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 -33.02 0)
		)
		(property "Value" "KSZ8081MLX"
			(at 15.24 -35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at -1.27 -21.59 90)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/KSZ8081MLX.pdf"
			(at 8.89 -24.13 0)
		)
		(property "Description" "10BASE-T/100BASE-TX PHY with RMII Support, 25 MHz input clock, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "ETH PHY RMII MII"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP?48*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "KSZ8081MLX_1_1"
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "TXEN")
				(number "34")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "TXD0")
				(number "35")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "TXD1")
				(number "36")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "TXD2")
				(number "38")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "TXD3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "COL/CONFIG0")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "CRS/CONFIG1")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "TXC")
				(number "33")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RXD0/DUPLEX")
				(number "23")
			)
			(pin output line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "RXD1/PHYAD2")
				(number "22")
			)
			(pin output line
				(at -17.78 0 0)
				(length 2.54)
				(name "RXD2/PHYAD1")
				(number "21")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "RXD3/PHYAD0")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "RXDV/CONFIG2")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "RXC/B-CAST_OFF")
				(number "28")
			)
			(pin output line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "RXER/ISO")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "MDIO")
				(number "18")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "MDC")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "INTRP/NAND_Tree#")
				(number "32")
			)
			(pin input line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "~{RST}")
				(number "47")
			)
			(pin power_out line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VDD_1.2")
				(number "4")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD_1.2")
				(number "31")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDDA_3.3")
				(number "7")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VDDIO")
				(number "25")
			)
			(pin no_connect line
				(at 15.24 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at 15.24 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 15.24 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 15.24 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin no_connect line
				(at 15.24 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "45")
			)
			(pin no_connect line
				(at 15.24 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "46")
			)
			(pin no_connect line
				(at 15.24 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "TEST/NC")
				(number "44")
			)
			(pin passive line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "RXP")
				(number "10")
			)
			(pin passive line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "RXM")
				(number "9")
			)
			(pin passive line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "TXP")
				(number "12")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "TXM")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "LED0/NWAYEN")
				(number "42")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "LED1/SPEED")
				(number "43")
			)
			(pin passive line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "REXT")
				(number "16")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "XO")
				(number "14")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "XI")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KSZ8081RNA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.035 0)
		)
		(property "Value" "KSZ8081RNA"
			(at 3.81 26.035 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 35.56 -25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00002199A.pdf"
			(at -57.15 5.08 0)
		)
		(property "Description" "10BASE-T/100BASE-TX PHY with RMII Support, 25 MHz input clock/50 MHz output, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ETH PHY RMII"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "KSZ8081RNA_0_1")
		(symbol "KSZ8081RNA_1_1"
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "TXEN")
				(number "19")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "TXD0")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "TXD1")
				(number "21")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "RXD0")
				(number "13")
			)
			(pin output line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "RXD1")
				(number "12")
			)
			(pin output line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "CRS_DV/PHYAD[1:0]")
				(number "15")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "REF_CLK")
				(number "16")
			)
			(pin output line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "RXER")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "MDIO")
				(number "10")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "MDC")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "INTRP")
				(number "18")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "~{RST}")
				(number "24")
			)
			(pin output line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "XO")
				(number "7")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "XI")
				(number "8")
			)
			(pin power_out line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VDD_1.2")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDDA_3.3")
				(number "2")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDIO")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "RXM")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "RXP")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "TXM")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "TXP")
				(number "6")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "LED0/ANEN_SPEED")
				(number "23")
			)
			(pin passive line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "REXT")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KSZ9031RNXCA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 39.37 0)
		)
		(property "Value" "KSZ9031RNXCA"
			(at 39.37 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 11.43 -39.37 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00002117C.pdf"
			(at 0 -41.91 0)
		)
		(property "Description" "10/100/1000Mbps Ethernet Transceiver with RGMII Interface, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "ETHERNET PHY RGMII WOL IEEE 802.3 MICROCHIP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "KSZ9031RNXCA_0_1")
		(symbol "KSZ9031RNXCA_1_1"
			(pin input line
				(at -33.02 25.4 0)
				(length 2.54)
				(name "MDC")
				(number "36")
			)
			(pin input line
				(at -33.02 22.86 0)
				(length 2.54)
				(name "MDIO")
				(number "37")
			)
			(pin input line
				(at -33.02 17.78 0)
				(length 2.54)
				(name "TX_EN")
				(number "25")
			)
			(pin input line
				(at -33.02 15.24 0)
				(length 2.54)
				(name "TXD0")
				(number "19")
			)
			(pin input line
				(at -33.02 12.7 0)
				(length 2.54)
				(name "TXD1")
				(number "20")
			)
			(pin input line
				(at -33.02 10.16 0)
				(length 2.54)
				(name "TXD2")
				(number "21")
			)
			(pin input line
				(at -33.02 7.62 0)
				(length 2.54)
				(name "TXD3")
				(number "22")
			)
			(pin input line
				(at -33.02 5.08 0)
				(length 2.54)
				(name "GTX_CLK")
				(number "24")
			)
			(pin input line
				(at -33.02 0 0)
				(length 2.54)
				(name "RX_DV/CLK125_EN")
				(number "33")
			)
			(pin input line
				(at -33.02 -2.54 0)
				(length 2.54)
				(name "RXD0/MODE0")
				(number "32")
			)
			(pin input line
				(at -33.02 -5.08 0)
				(length 2.54)
				(name "RXD1/MODE1")
				(number "31")
			)
			(pin input line
				(at -33.02 -7.62 0)
				(length 2.54)
				(name "RXD2/MODE2")
				(number "28")
			)
			(pin input line
				(at -33.02 -10.16 0)
				(length 2.54)
				(name "RXD3/MODE3")
				(number "27")
			)
			(pin input line
				(at -33.02 -12.7 0)
				(length 2.54)
				(name "RX_CLK/PHYAD2")
				(number "35")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 2.54)
				(name "LED2/PHYAD1")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 2.54)
				(name "LED1/PHAD0/PME_N1")
				(number "17")
			)
			(pin input line
				(at -33.02 -22.86 0)
				(length 2.54)
				(name "INT_N/PME_N2")
				(number "38")
			)
			(pin input line
				(at -33.02 -27.94 0)
				(length 2.54)
				(name "CLK125_NDO/LED_MODE")
				(number "41")
			)
			(pin input line
				(at -33.02 -30.48 0)
				(length 2.54)
				(name "RESET_N")
				(number "42")
			)
			(pin power_in line
				(at -20.32 40.64 270)
				(length 2.54)
				(name "DVDDH")
				(number "40")
			)
			(pin power_in line
				(at -17.78 40.64 270)
				(length 2.54)
				(name "DVDDH")
				(number "34")
			)
			(pin power_in line
				(at -15.24 40.64 270)
				(length 2.54)
				(name "DVDDH")
				(number "16")
			)
			(pin power_in line
				(at -10.16 40.64 270)
				(length 2.54)
				(name "AVDDH")
				(number "12")
			)
			(pin power_in line
				(at -7.62 40.64 270)
				(length 2.54)
				(name "AVDDH")
				(number "1")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "DVDDL")
				(number "39")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "DVDDL")
				(number "30")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "DVDDL")
				(number "26")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 2.54)
				(name "PAD_GND")
				(number "49")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 2.54)
				(name "DVDDL")
				(number "23")
			)
			(pin power_in line
				(at 7.62 40.64 270)
				(length 2.54)
				(name "DVDDL")
				(number "18")
			)
			(pin power_in line
				(at 10.16 40.64 270)
				(length 2.54)
				(name "DVDDL")
				(number "14")
			)
			(pin output line
				(at 10.16 -40.64 90)
				(length 2.54)
				(name "ISET")
				(number "48")
			)
			(pin power_in line
				(at 15.24 40.64 270)
				(length 2.54)
				(name "AVDDL")
				(number "9")
			)
			(pin power_in line
				(at 17.78 40.64 270)
				(length 2.54)
				(name "AVDDL")
				(number "4")
			)
			(pin power_in line
				(at 22.86 40.64 270)
				(length 2.54)
				(name "AVDDL_PLL")
				(number "44")
			)
			(pin no_connect line
				(at 30.48 12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 30.48 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "47")
			)
			(pin input line
				(at 33.02 20.32 180)
				(length 2.54)
				(name "LDO_O")
				(number "43")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 2.54)
				(name "TXRXM_D")
				(number "11")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 2.54)
				(name "TXRXP_D")
				(number "10")
			)
			(pin input line
				(at 33.02 -2.54 180)
				(length 2.54)
				(name "TXRXM_C")
				(number "8")
			)
			(pin input line
				(at 33.02 -5.08 180)
				(length 2.54)
				(name "TXRXP_C")
				(number "7")
			)
			(pin input line
				(at 33.02 -10.16 180)
				(length 2.54)
				(name "TXRXM_B")
				(number "6")
			)
			(pin input line
				(at 33.02 -12.7 180)
				(length 2.54)
				(name "TXRXP_B")
				(number "5")
			)
			(pin input line
				(at 33.02 -17.78 180)
				(length 2.54)
				(name "TXRXM_A")
				(number "3")
			)
			(pin input line
				(at 33.02 -20.32 180)
				(length 2.54)
				(name "TXRXP_A")
				(number "2")
			)
			(pin input line
				(at 33.02 -27.94 180)
				(length 2.54)
				(name "XI")
				(number "46")
			)
			(pin input line
				(at 33.02 -30.48 180)
				(length 2.54)
				(name "XO")
				(number "45")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KSZ9563RNX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -34.29 36.83 0)
		)
		(property "Value" "KSZ9563RNX"
			(at 29.21 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_8x8mm_P0.4mm_EP6.5x6.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/KSZ9563R-Data-Sheet-DS00002419C.pdf"
			(at 0 0 0)
		)
		(property "Description" "3-Port Gigabit Ethernet Switch with RGMII/MII/RMII Interface and IEEE 1588v2, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gigabit Ethernet Switch RGMII MII RMII ieee1588v2"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "KSZ9563RNX_0_1")
		(symbol "KSZ9563RNX_1_1"
			(pin output line
				(at -38.1 33.02 0)
				(length 2.54)
				(name "XO")
				(number "57")
			)
			(pin input line
				(at -38.1 30.48 0)
				(length 2.54)
				(name "XI")
				(number "58")
			)
			(pin output line
				(at -38.1 25.4 0)
				(length 2.54)
				(name "SDO")
				(number "47")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 2.54)
				(name "SDI/SDA/MDIO")
				(number "48")
			)
			(pin input line
				(at -38.1 20.32 0)
				(length 2.54)
				(name "~{SCS}")
				(number "49")
			)
			(pin input line
				(at -38.1 17.78 0)
				(length 2.54)
				(name "SCL/MDC")
				(number "50")
			)
			(pin output line
				(at -38.1 12.7 0)
				(length 2.54)
				(name "~{PME}")
				(number "44")
			)
			(pin open_collector line
				(at -38.1 10.16 0)
				(length 2.54)
				(name "~{INTRP}")
				(number "45")
			)
			(pin input line
				(at -38.1 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "46")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 2.54)
				(name "TX_CLK/REFCLKI")
				(number "33")
			)
			(pin input line
				(at -38.1 0 0)
				(length 2.54)
				(name "TXD0")
				(number "32")
			)
			(pin input line
				(at -38.1 -2.54 0)
				(length 2.54)
				(name "TXD1")
				(number "31")
			)
			(pin input line
				(at -38.1 -5.08 0)
				(length 2.54)
				(name "TXD2")
				(number "30")
			)
			(pin input line
				(at -38.1 -7.62 0)
				(length 2.54)
				(name "TXD3")
				(number "29")
			)
			(pin input line
				(at -38.1 -10.16 0)
				(length 2.54)
				(name "TX_EN/TX_CTL")
				(number "35")
			)
			(pin input line
				(at -38.1 -12.7 0)
				(length 2.54)
				(name "TX_ER")
				(number "36")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 2.54)
				(name "RX_CLK/REFCLKO")
				(number "25")
			)
			(pin output line
				(at -38.1 -20.32 0)
				(length 2.54)
				(name "RXD0")
				(number "24")
			)
			(pin output line
				(at -38.1 -22.86 0)
				(length 2.54)
				(name "RXD1")
				(number "23")
			)
			(pin output line
				(at -38.1 -25.4 0)
				(length 2.54)
				(name "RXD2")
				(number "22")
			)
			(pin output line
				(at -38.1 -27.94 0)
				(length 2.54)
				(name "RXD3")
				(number "21")
			)
			(pin output line
				(at -38.1 -30.48 0)
				(length 2.54)
				(name "RX_DV/CRS_DV/RX_CTL")
				(number "27")
			)
			(pin output line
				(at -38.1 -33.02 0)
				(length 2.54)
				(name "RX_ER")
				(number "28")
			)
			(pin power_in line
				(at -25.4 38.1 270)
				(length 2.54)
				(name "VDDIO")
				(number "26")
			)
			(pin power_in line
				(at -22.86 38.1 270)
				(length 2.54)
				(name "VDDIO")
				(number "38")
			)
			(pin power_in line
				(at -20.32 38.1 270)
				(length 2.54)
				(name "VDDIO")
				(number "54")
			)
			(pin power_in line
				(at -15.24 38.1 270)
				(length 2.54)
				(name "DVDDL")
				(number "20")
			)
			(pin power_in line
				(at -12.7 38.1 270)
				(length 2.54)
				(name "DVDDL")
				(number "34")
			)
			(pin power_in line
				(at -10.16 38.1 270)
				(length 2.54)
				(name "DVDDL")
				(number "37")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "DVDDL")
				(number "41")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "DVDDL")
				(number "51")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "DVDDL")
				(number "55")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVDDH")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "AVDDH")
				(number "19")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "AVDDH")
				(number "61")
			)
			(pin power_in line
				(at 12.7 38.1 270)
				(length 2.54)
				(name "AVDDL")
				(number "5")
			)
			(pin power_in line
				(at 15.24 38.1 270)
				(length 2.54)
				(name "AVDDL")
				(number "11")
			)
			(pin power_in line
				(at 17.78 38.1 270)
				(length 2.54)
				(name "AVDDL")
				(number "16")
			)
			(pin power_in line
				(at 20.32 38.1 270)
				(length 2.54)
				(name "AVDDL")
				(number "56")
			)
			(pin power_in line
				(at 22.86 38.1 270)
				(length 2.54)
				(name "AVDDL")
				(number "64")
			)
			(pin passive line
				(at 38.1 33.02 180)
				(length 2.54)
				(name "TXRX1P_A")
				(number "62")
			)
			(pin passive line
				(at 38.1 30.48 180)
				(length 2.54)
				(name "TXRX1M_A")
				(number "63")
			)
			(pin passive line
				(at 38.1 27.94 180)
				(length 2.54)
				(name "TXRX1P_B")
				(number "1")
			)
			(pin passive line
				(at 38.1 25.4 180)
				(length 2.54)
				(name "TXRX1M_B")
				(number "2")
			)
			(pin passive line
				(at 38.1 22.86 180)
				(length 2.54)
				(name "TXRX1P_C")
				(number "3")
			)
			(pin passive line
				(at 38.1 20.32 180)
				(length 2.54)
				(name "TXRX1M_C")
				(number "4")
			)
			(pin passive line
				(at 38.1 17.78 180)
				(length 2.54)
				(name "TXRX1P_D")
				(number "6")
			)
			(pin passive line
				(at 38.1 15.24 180)
				(length 2.54)
				(name "TXRX1M_D")
				(number "7")
			)
			(pin output line
				(at 38.1 10.16 180)
				(length 2.54)
				(name "LED1_0")
				(number "52")
			)
			(pin output line
				(at 38.1 7.62 180)
				(length 2.54)
				(name "LED1_1")
				(number "53")
			)
			(pin passive line
				(at 38.1 0 180)
				(length 2.54)
				(name "TXRX2P_A")
				(number "9")
			)
			(pin passive line
				(at 38.1 -2.54 180)
				(length 2.54)
				(name "TXRX2M_A")
				(number "10")
			)
			(pin passive line
				(at 38.1 -5.08 180)
				(length 2.54)
				(name "TXRX2P_B")
				(number "12")
			)
			(pin passive line
				(at 38.1 -7.62 180)
				(length 2.54)
				(name "TXRX2M_B")
				(number "13")
			)
			(pin passive line
				(at 38.1 -10.16 180)
				(length 2.54)
				(name "TXRX2P_C")
				(number "14")
			)
			(pin passive line
				(at 38.1 -12.7 180)
				(length 2.54)
				(name "TXRX2M_C")
				(number "15")
			)
			(pin passive line
				(at 38.1 -15.24 180)
				(length 2.54)
				(name "TXRX2P_D")
				(number "17")
			)
			(pin passive line
				(at 38.1 -17.78 180)
				(length 2.54)
				(name "TXRX2M_D")
				(number "18")
			)
			(pin output line
				(at 38.1 -22.86 180)
				(length 2.54)
				(name "LED2_0")
				(number "42")
			)
			(pin output line
				(at 38.1 -25.4 180)
				(length 2.54)
				(name "LED2_1")
				(number "43")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 2.54)
				(name "GPIO_1")
				(number "39")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 2.54)
				(name "GPIO_2")
				(number "40")
			)
			(pin passive line
				(at 38.1 -33.02 180)
				(length 2.54)
				(name "ISET")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "KSZ9893RNX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -34.29 36.83 0)
		)
		(property "Value" "KSZ9893RNX"
			(at 29.21 36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_8x8mm_P0.4mm_EP6.5x6.5mm"
			(at 0 48.26 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/KSZ9893R-Data-Sheet-DS00002420C.pdf"
			(at -2.54 38.1 0)
		)
		(property "Description" "3-Port Gigabit Ethernet Switch with RGMII/MII/RMII Interface, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gigabit Ethernet Switch RGMII MII RMII"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "KSZ9893RNX_0_1")
		(symbol "KSZ9893RNX_1_1"
			(pin output line
				(at -38.1 33.02 0)
				(length 2.54)
				(name "XO")
				(number "57")
			)
			(pin input line
				(at -38.1 30.48 0)
				(length 2.54)
				(name "XI")
				(number "58")
			)
			(pin output line
				(at -38.1 25.4 0)
				(length 2.54)
				(name "SDO")
				(number "47")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 2.54)
				(name "SDI/SDA/MDIO")
				(number "48")
			)
			(pin input line
				(at -38.1 20.32 0)
				(length 2.54)
				(name "~{SCS}")
				(number "49")
			)
			(pin input line
				(at -38.1 17.78 0)
				(length 2.54)
				(name "SCL/MDC")
				(number "50")
			)
			(pin output line
				(at -38.1 12.7 0)
				(length 2.54)
				(name "~{PME}")
				(number "44")
			)
			(pin output line
				(at -38.1 10.16 0)
				(length 2.54)
				(name "~{INTRP}")
				(number "45")
			)
			(pin input line
				(at -38.1 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "46")
			)
			(pin input line
				(at -38.1 2.54 0)
				(length 2.54)
				(name "TX_CLK/REFCLKI")
				(number "33")
			)
			(pin input line
				(at -38.1 0 0)
				(length 2.54)
				(name "TXD0")
				(number "32")
			)
			(pin input line
				(at -38.1 -2.54 0)
				(length 2.54)
				(name "TXD1")
				(number "31")
			)
			(pin input line
				(at -38.1 -5.08 0)
				(length 2.54)
				(name "TXD2")
				(number "30")
			)
			(pin input line
				(at -38.1 -7.62 0)
				(length 2.54)
				(name "TXD3")
				(number "29")
			)
			(pin input line
				(at -38.1 -10.16 0)
				(length 2.54)
				(name "TX_EN/TX_CTL")
				(number "35")
			)
			(pin input line
				(at -38.1 -12.7 0)
				(length 2.54)
				(name "TX_ER")
				(number "36")
			)
			(pin output line
				(at -38.1 -17.78 0)
				(length 2.54)
				(name "RX_CLK/REFCLKO")
				(number "25")
			)
			(pin output line
				(at -38.1 -20.32 0)
				(length 2.54)
				(name "RXD0")
				(number "24")
			)
			(pin output line
				(at -38.1 -22.86 0)
				(length 2.54)
				(name "RXD1")
				(number "23")
			)
			(pin output line
				(at -38.1 -25.4 0)
				(length 2.54)
				(name "RXD2")
				(number "22")
			)
			(pin output line
				(at -38.1 -27.94 0)
				(length 2.54)
				(name "RXD3")
				(number "21")
			)
			(pin output line
				(at -38.1 -30.48 0)
				(length 2.54)
				(name "RX_DV/CRS_DV/RX_CTL")
				(number "27")
			)
			(pin output line
				(at -38.1 -33.02 0)
				(length 2.54)
				(name "RX_ER")
				(number "28")
			)
			(pin power_in line
				(at -25.4 38.1 270)
				(length 2.54)
				(name "VDDIO")
				(number "26")
			)
			(pin power_in line
				(at -22.86 38.1 270)
				(length 2.54)
				(name "VDDIO")
				(number "38")
			)
			(pin power_in line
				(at -20.32 38.1 270)
				(length 2.54)
				(name "VDDIO")
				(number "54")
			)
			(pin power_in line
				(at -15.24 38.1 270)
				(length 2.54)
				(name "DVDDL")
				(number "20")
			)
			(pin power_in line
				(at -12.7 38.1 270)
				(length 2.54)
				(name "DVDDL")
				(number "34")
			)
			(pin power_in line
				(at -10.16 38.1 270)
				(length 2.54)
				(name "DVDDL")
				(number "37")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "DVDDL")
				(number "41")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "DVDDL")
				(number "51")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "DVDDL")
				(number "55")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVDDH")
				(number "8")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "AVDDH")
				(number "19")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "AVDDH")
				(number "61")
			)
			(pin power_in line
				(at 12.7 38.1 270)
				(length 2.54)
				(name "AVDDL")
				(number "5")
			)
			(pin power_in line
				(at 15.24 38.1 270)
				(length 2.54)
				(name "AVDDL")
				(number "11")
			)
			(pin power_in line
				(at 17.78 38.1 270)
				(length 2.54)
				(name "AVDDL")
				(number "16")
			)
			(pin power_in line
				(at 20.32 38.1 270)
				(length 2.54)
				(name "AVDDL")
				(number "56")
			)
			(pin power_in line
				(at 22.86 38.1 270)
				(length 2.54)
				(name "AVDDL")
				(number "64")
			)
			(pin no_connect line
				(at 35.56 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin no_connect line
				(at 35.56 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "39")
			)
			(pin passive line
				(at 38.1 33.02 180)
				(length 2.54)
				(name "TXRX1P_A")
				(number "62")
			)
			(pin passive line
				(at 38.1 30.48 180)
				(length 2.54)
				(name "TXRX1M_A")
				(number "63")
			)
			(pin passive line
				(at 38.1 27.94 180)
				(length 2.54)
				(name "TXRX1P_B")
				(number "1")
			)
			(pin passive line
				(at 38.1 25.4 180)
				(length 2.54)
				(name "TXRX1M_B")
				(number "2")
			)
			(pin passive line
				(at 38.1 22.86 180)
				(length 2.54)
				(name "TXRX1P_C")
				(number "3")
			)
			(pin passive line
				(at 38.1 20.32 180)
				(length 2.54)
				(name "TXRX1M_C")
				(number "4")
			)
			(pin passive line
				(at 38.1 17.78 180)
				(length 2.54)
				(name "TXRX1P_D")
				(number "6")
			)
			(pin passive line
				(at 38.1 15.24 180)
				(length 2.54)
				(name "TXRX1M_D")
				(number "7")
			)
			(pin output line
				(at 38.1 10.16 180)
				(length 2.54)
				(name "LED1_0")
				(number "52")
			)
			(pin output line
				(at 38.1 7.62 180)
				(length 2.54)
				(name "LED1_1")
				(number "53")
			)
			(pin passive line
				(at 38.1 0 180)
				(length 2.54)
				(name "TXRX2P_A")
				(number "9")
			)
			(pin passive line
				(at 38.1 -2.54 180)
				(length 2.54)
				(name "TXRX2M_A")
				(number "10")
			)
			(pin passive line
				(at 38.1 -5.08 180)
				(length 2.54)
				(name "TXRX2P_B")
				(number "12")
			)
			(pin passive line
				(at 38.1 -7.62 180)
				(length 2.54)
				(name "TXRX2M_B")
				(number "13")
			)
			(pin passive line
				(at 38.1 -10.16 180)
				(length 2.54)
				(name "TXRX2P_C")
				(number "14")
			)
			(pin passive line
				(at 38.1 -12.7 180)
				(length 2.54)
				(name "TXRX2M_C")
				(number "15")
			)
			(pin passive line
				(at 38.1 -15.24 180)
				(length 2.54)
				(name "TXRX2P_D")
				(number "17")
			)
			(pin passive line
				(at 38.1 -17.78 180)
				(length 2.54)
				(name "TXRX2M_D")
				(number "18")
			)
			(pin output line
				(at 38.1 -22.86 180)
				(length 2.54)
				(name "LED2_0")
				(number "42")
			)
			(pin output line
				(at 38.1 -25.4 180)
				(length 2.54)
				(name "LED2_1")
				(number "43")
			)
			(pin passive line
				(at 38.1 -33.02 180)
				(length 2.54)
				(name "ISET")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LAN7500-ABJZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 -29.21 0)
		)
		(property "Value" "LAN7500-ABJZ"
			(at -17.78 -31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_8x8mm_P0.5mm_EP5.9x5.9mm"
			(at 31.75 -29.21 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00001734B.pdf"
			(at 2.54 -19.05 0)
		)
		(property "Description" "Hi-Speed USB 2.0 to 10/100/1000 Ethernet Controller, QFN-56"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Ethernet 10/100/1000"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LAN7500-ABJZ_1_1"
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "~{RESET}")
				(number "42")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TMS")
				(number "3")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "TDI")
				(number "1")
			)
			(pin output line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "TDO")
				(number "4")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "TCK")
				(number "2")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "TEST")
				(number "39")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "EEDI")
				(number "27")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "EEDO")
				(number "28")
			)
			(pin output line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "EECS")
				(number "29")
			)
			(pin output line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "EECLK")
				(number "26")
			)
			(pin output line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "XO")
				(number "6")
			)
			(pin input line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "XI")
				(number "5")
			)
			(pin power_in line
				(at -15.24 30.48 270)
				(length 2.54)
				(name "VDD33A")
				(number "15")
			)
			(pin passive line
				(at -10.16 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDDVARIO")
				(number "19")
			)
			(pin passive line
				(at -10.16 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDDVARIO")
				(number "24")
			)
			(pin passive line
				(at -10.16 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDDVARIO")
				(number "37")
			)
			(pin power_in line
				(at -10.16 30.48 270)
				(length 2.54)
				(name "VDDVARIO")
				(number "7")
			)
			(pin passive line
				(at -5.08 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD12CORE")
				(number "11")
			)
			(pin passive line
				(at -5.08 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD12CORE")
				(number "20")
			)
			(pin passive line
				(at -5.08 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD12CORE")
				(number "23")
			)
			(pin passive line
				(at -5.08 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD12CORE")
				(number "30")
			)
			(pin passive line
				(at -5.08 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD12CORE")
				(number "36")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "VDD12CORE")
				(number "8")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD12A")
				(number "45")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD12A")
				(number "48")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD12A")
				(number "53")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD12A")
				(number "56")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "57")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "VDD12USBPLL")
				(number "17")
			)
			(pin power_in line
				(at 10.16 30.48 270)
				(length 2.54)
				(name "VDD12BIAS")
				(number "49")
			)
			(pin power_in line
				(at 15.24 30.48 270)
				(length 2.54)
				(name "VDD12PLL")
				(number "50")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "GPIO0")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "GPIO1")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "GPIO2")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "GPIO3")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "GPIO4")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "GPIO5")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "GPIO6")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "GPIO7")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "GPIO8")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "GPIO9")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "GPIO10")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "GPIO11")
				(number "25")
			)
			(pin output line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "SW_MODE")
				(number "9")
			)
		)
		(symbol "LAN7500-ABJZ_2_1"
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "USBDP")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "USBDM")
				(number "12")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VBUS_DET")
				(number "14")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "USBRBIAS")
				(number "16")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "ETHRBIAS")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "TR0N")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "TR0P")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "TR1N")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "TR1P")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "TR2N")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "TR2P")
				(number "52")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "TR3N")
				(number "54")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "TR3P")
				(number "55")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LAN8710A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 34.29 0)
		)
		(property "Value" "LAN8710A"
			(at 17.78 34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.3x3.3mm_ThermalVias"
			(at 3.81 -34.29 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/8710a.pdf"
			(at -2.54 -24.13 0)
		)
		(property "Description" "LAN8710 Ethernet PHY with MII/RMII interface, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "ETH PHY MII RMII"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LAN8710A_0_1")
		(symbol "LAN8710A_1_1"
			(pin input line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "TXD0")
				(number "22")
			)
			(pin input line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "TXD1")
				(number "23")
			)
			(pin input line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "TXD2")
				(number "24")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "TXD3")
				(number "25")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "TXEN")
				(number "21")
			)
			(pin output line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "TXCLK")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RXD0/~{MODE0}")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RXD1/~{MODE1}")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RXD2/~{RMIISEL}")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RXD3/~{PHYAD2}")
				(number "8")
			)
			(pin output line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RXDV")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "RXCLK/~{PHYAD1}")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RXER/RXD4/~{PHYAD0}")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "COL/CRS_DV/~{MODE2}")
				(number "15")
			)
			(pin output line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "CRS")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "MDIO")
				(number "16")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "MDC")
				(number "17")
			)
			(pin input line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "~{RST}")
				(number "19")
			)
			(pin input line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "XTAL1/CLKIN")
				(number "5")
			)
			(pin output line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "XTAL2")
				(number "4")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 2.54)
				(name "VDDIO")
				(number "12")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "VDDCR")
				(number "6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDD1A")
				(number "27")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "VDD2A")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "TXP")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "TXN")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "RXP")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RXN")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "LED1/~{REGOFF}")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "LED2/~{INTSEL}")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "~{INT}/TXER/TXD4")
				(number "18")
			)
			(pin passive line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "RBIAS")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LAN8720A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 29.21 0)
		)
		(property "Value" "LAN8720A"
			(at 15.24 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm_ThermalVias"
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/8720a.pdf"
			(at -5.08 -24.13 0)
		)
		(property "Description" "LAN8720 Ethernet PHY with RMII interface, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ETH PHY RMII"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LAN8720A_0_0"
			(text "RMII"
				(at -5.08 -3.81 0)
			)
		)
		(symbol "LAN8720A_0_1")
		(symbol "LAN8720A_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "TXD0")
				(number "17")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "TXD1")
				(number "18")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "TXEN")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RXD0/MODE0")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RXD1/MODE1")
				(number "7")
			)
			(pin output line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RXER/PHYAD0")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "CRS_DV/MODE2")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "MDIO")
				(number "12")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "MDC")
				(number "13")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "~{RST}")
				(number "15")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "~{INT}/REFCLKO")
				(number "14")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "XTAL1/CLKIN")
				(number "5")
			)
			(pin output line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "XTAL2")
				(number "4")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "VDDIO")
				(number "9")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDDCR")
				(number "6")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD1A")
				(number "19")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "25")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDD2A")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "TXP")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "TXN")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "RXP")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "RXN")
				(number "22")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "RBIAS")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "LED1/REGOFF")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "LED2/~{INTSEL}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LAN8742A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 29.21 0)
		)
		(property "Value" "LAN8742A"
			(at 15.24 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm_ThermalVias"
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/8742a.pdf"
			(at 0 -39.37 0)
		)
		(property "Description" "LAN8720 Ethernet PHY with RMII interface, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ETH PHY RMII"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LAN8742A_0_0"
			(text "RMII"
				(at -5.08 -3.81 0)
			)
		)
		(symbol "LAN8742A_0_1")
		(symbol "LAN8742A_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "TXD0")
				(number "17")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "TXD1")
				(number "18")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "TXEN")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RXD0/MODE0")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RXD1/MODE1")
				(number "7")
			)
			(pin output line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RXER/PHYAD0")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "CRS_DV/MODE2")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "MDIO")
				(number "12")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "MDC")
				(number "13")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "~{RST}")
				(number "15")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "~{INT}/REFCLKO")
				(number "14")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "XTAL1/CLKIN")
				(number "5")
			)
			(pin output line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "XTAL2")
				(number "4")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "VDDIO")
				(number "9")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDDCR")
				(number "6")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD1A")
				(number "19")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "25")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VDD2A")
				(number "1")
			)
			(pin passive line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "TXP")
				(number "21")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "TXN")
				(number "20")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "RXP")
				(number "23")
			)
			(pin passive line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "RXN")
				(number "22")
			)
			(pin passive line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "RBIAS")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "LED1/REGOFF")
				(number "3")
				(alternate "~{INT}/REGOFF" bidirectional line)
				(alternate "~{PME}/REGOFF" bidirectional line)
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "LED2/~{INTSEL}")
				(number "2")
				(alternate "~{INT}/~{INTSEL}" output line)
				(alternate "~{PME}/~{INTSEL}" output line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "LAN9303"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 44.704 0)
		)
		(property "Value" "LAN9303"
			(at 19.812 44.704 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_8x8mm_P0.5mm_EP5.9x5.9mm_ThermalVias"
			(at 2.54 -45.72 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/9303.pdf"
			(at -33.02 -45.72 0)
		)
		(property "Description" "3-port managed Ethernet switch with dual PHY and RMII interface, QFN-56"
			(at -5.08 0 0)
		)
		(property "ki_keywords" "ETH PHY RMII switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LAN9303_0_1")
		(symbol "LAN9303_1_1"
			(pin passive line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "P0_INCLK")
				(number "8")
			)
			(pin passive line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "P0_INER")
				(number "7")
			)
			(pin input line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "P0_INDV")
				(number "6")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "P0_IND0")
				(number "5")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "P0_IND1")
				(number "4")
			)
			(pin passive line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "P0_IND2")
				(number "3")
			)
			(pin passive line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "P0_IND3")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "P0_OUTCLK")
				(number "17")
			)
			(pin output line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "P0_OUTDV")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "P0_OUTD0/~{P0_MODE0}")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "P0_OUTD1/~{P0_MODE1}")
				(number "13")
			)
			(pin passive line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "P0_OUTD2/~{P0_MODE2}")
				(number "12")
			)
			(pin passive line
				(at -22.86 0 0)
				(length 2.54)
				(name "P0_OUTD3/~{DUPLEX_POL_0}")
				(number "11")
			)
			(pin passive line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "P0_COL")
				(number "18")
			)
			(pin passive line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "P0_CRS")
				(number "19")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "P0_DUPLEX")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "MDIO")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "MDC")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "EE_SDA/SDA")
				(number "35")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "EE_SCL/SCL")
				(number "36")
			)
			(pin passive line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "~{RST}")
				(number "37")
			)
			(pin passive line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "IRQ")
				(number "38")
			)
			(pin input line
				(at -22.86 -35.56 0)
				(length 2.54)
				(name "XI")
				(number "39")
			)
			(pin passive line
				(at -22.86 -38.1 0)
				(length 2.54)
				(name "XO")
				(number "40")
			)
			(pin passive line
				(at -10.16 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "15")
			)
			(pin passive line
				(at -10.16 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "23")
			)
			(pin passive line
				(at -10.16 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "30")
			)
			(pin passive line
				(at -10.16 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "32")
			)
			(pin passive line
				(at -10.16 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "33")
			)
			(pin power_in line
				(at -10.16 45.72 270)
				(length 2.54)
				(name "VDD33IO")
				(number "9")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDD33BIAS")
				(number "50")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDD33A1")
				(number "44")
			)
			(pin passive line
				(at -5.08 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A1")
				(number "47")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD33A2")
				(number "52")
			)
			(pin passive line
				(at -2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A2")
				(number "55")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "34")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "57")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD18CORE")
				(number "10")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD18CORE")
				(number "31")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDD18PLL")
				(number "41")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDD18TX1")
				(number "48")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 2.54)
				(name "VDD18TX2")
				(number "51")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "TXP1")
				(number "43")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "TXN1")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "RXP1")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "RXN1")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "TXP2")
				(number "56")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "TXN2")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "RXP2")
				(number "53")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "RXN2")
				(number "54")
			)
			(pin passive line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "LED0/GPIO0/~{AMDIX1}")
				(number "29")
			)
			(pin passive line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "LED1/GPIO1/~{AMDIX2}")
				(number "28")
			)
			(pin passive line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "LED2/GPIO2/~{E2PSIZE}")
				(number "27")
			)
			(pin passive line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "LED3/GPIO3/~{MNGT0}")
				(number "26")
			)
			(pin passive line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "LED4/GPIO4/~{MNGT1}")
				(number "25")
			)
			(pin passive line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "LED5/GPIO5/~{PHYADDR}")
				(number "24")
			)
			(pin passive line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "EXRES")
				(number "49")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LAN9512"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "LAN9512"
			(at 15.24 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.3x7.3mm"
			(at 31.75 -31.75 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00002304A.pdf"
			(at 2.54 -7.62 0)
		)
		(property "Description" "Two USB 2.0 hub with an integrated 10/100 Ethernet controller (0°C to +70°C), QFN-48"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "USB HUB Ethernet 10/100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP?9x9mm?P0.5mm?EP7.3x7.3mm*"
			(at 0 0 0)
		)
		(symbol "LAN9512_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "12")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{TRST}")
				(number "28")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "TMS")
				(number "29")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "TDI")
				(number "30")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "TDO")
				(number "31")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "TCK")
				(number "32")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "TEST1")
				(number "13")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "TEST2")
				(number "34")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "TEST3")
				(number "40")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "TEST4")
				(number "47")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "CLK24_EN")
				(number "44")
			)
			(pin output line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "CLK24_OUT")
				(number "45")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "XO")
				(number "60")
			)
			(pin input line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "XI")
				(number "61")
			)
			(pin power_in line
				(at -10.16 33.02 270)
				(length 2.54)
				(name "VDD33IO")
				(number "19")
			)
			(pin passive line
				(at -10.16 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "27")
			)
			(pin passive line
				(at -10.16 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "33")
			)
			(pin passive line
				(at -10.16 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "39")
			)
			(pin passive line
				(at -10.16 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "46")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "10")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "49")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VDD33A")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "51")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "54")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "57")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "64")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD18CORE")
				(number "15")
			)
			(pin passive line
				(at 0 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD18CORE")
				(number "38")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "VDD18ETHPLL")
				(number "48")
			)
			(pin power_in line
				(at 10.16 33.02 270)
				(length 2.54)
				(name "VDD18USBPLL")
				(number "62")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "EECLK")
				(number "23")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "EECS")
				(number "24")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "EEDO")
				(number "25")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "EEDI")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{FDX_LED}/GPIO0")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{LNKA_LED}/GPIO1")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "~{SPD_LED}/GPIO2")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "GPIO3")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "GPIO4")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "GPIO5")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "GPIO6")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "GPIO7")
				(number "43")
			)
		)
		(symbol "LAN9512_2_1"
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "USBDP0")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "USBDM0")
				(number "58")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "VBUS_DET")
				(number "11")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "USBRBIAS")
				(number "63")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "AUTOMDIX_EN")
				(number "41")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "EXRES")
				(number "50")
			)
			(pin no_connect line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 12.7 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "USBDP2")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "USBDM2")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PRTCTL2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "USBDP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "USBDM3")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PRTCTL3")
				(number "16")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "TXP")
				(number "55")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "TXN")
				(number "56")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "RXP")
				(number "52")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "RXN")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LAN9513"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "LAN9513"
			(at 15.24 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.3x7.3mm"
			(at 31.75 -31.75 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00002305A.pdf"
			(at 2.54 -7.62 0)
		)
		(property "Description" "Three USB 2.0 hub with an integrated 10/100 Ethernet controller (0°C to +70°C), QFN-48"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "USB HUB Ethernet 10/100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP?9x9mm?P0.5mm?EP7.3x7.3mm*"
			(at 0 0 0)
		)
		(symbol "LAN9513_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "12")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{TRST}")
				(number "28")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "TMS")
				(number "29")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "TDI")
				(number "30")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "TDO")
				(number "31")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "TCK")
				(number "32")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "TEST1")
				(number "13")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "TEST2")
				(number "34")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "TEST3")
				(number "40")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "TEST4")
				(number "47")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "CLK24_EN")
				(number "44")
			)
			(pin output line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "CLK24_OUT")
				(number "45")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "XO")
				(number "60")
			)
			(pin input line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "XI")
				(number "61")
			)
			(pin power_in line
				(at -10.16 33.02 270)
				(length 2.54)
				(name "VDD33IO")
				(number "19")
			)
			(pin passive line
				(at -10.16 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "27")
			)
			(pin passive line
				(at -10.16 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "33")
			)
			(pin passive line
				(at -10.16 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "39")
			)
			(pin passive line
				(at -10.16 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "46")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "10")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "49")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VDD33A")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "51")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "54")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "57")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "64")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD18CORE")
				(number "15")
			)
			(pin passive line
				(at 0 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD18CORE")
				(number "38")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "VDD18ETHPLL")
				(number "48")
			)
			(pin power_in line
				(at 10.16 33.02 270)
				(length 2.54)
				(name "VDD18USBPLL")
				(number "62")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "EECLK")
				(number "23")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "EECS")
				(number "24")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "EEDO")
				(number "25")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "EEDI")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{FDX_LED}/GPIO0")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{LNKA_LED}/GPIO1")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "~{SPD_LED}/GPIO2")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "GPIO3")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "GPIO4")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "GPIO5")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "GPIO6")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "GPIO7")
				(number "43")
			)
		)
		(symbol "LAN9513_2_1"
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "USBDP0")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "USBDM0")
				(number "58")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "VBUS_DET")
				(number "11")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "USBRBIAS")
				(number "63")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "AUTOMDIX_EN")
				(number "41")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "EXRES")
				(number "50")
			)
			(pin no_connect line
				(at 12.7 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 12.7 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "USBDP2")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "USBDM2")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PRTCTL2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "USBDP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "USBDM3")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PRTCTL3")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "USBDP4")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "USBDM4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PRTCTL4")
				(number "17")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "TXP")
				(number "55")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "TXN")
				(number "56")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "RXP")
				(number "52")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "RXN")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LAN9514"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "LAN9514"
			(at 15.24 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.3x7.3mm"
			(at 31.75 -31.75 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00002306A.pdf"
			(at 2.54 -7.62 0)
		)
		(property "Description" "Four USB 2.0 hub with an integrated 10/100 Ethernet controller (0°C to +70°C), QFN-48"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "USB HUB Ethernet 10/100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP?9x9mm?P0.5mm?EP7.3x7.3mm*"
			(at 0 0 0)
		)
		(symbol "LAN9514_1_1"
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "12")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{TRST}")
				(number "28")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "TMS")
				(number "29")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "TDI")
				(number "30")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "TDO")
				(number "31")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "TCK")
				(number "32")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "TEST1")
				(number "13")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "TEST2")
				(number "34")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "TEST3")
				(number "40")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "TEST4")
				(number "47")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "CLK24_EN")
				(number "44")
			)
			(pin output line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "CLK24_OUT")
				(number "45")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "XO")
				(number "60")
			)
			(pin input line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "XI")
				(number "61")
			)
			(pin power_in line
				(at -10.16 33.02 270)
				(length 2.54)
				(name "VDD33IO")
				(number "19")
			)
			(pin passive line
				(at -10.16 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "27")
			)
			(pin passive line
				(at -10.16 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "33")
			)
			(pin passive line
				(at -10.16 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "39")
			)
			(pin passive line
				(at -10.16 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33IO")
				(number "46")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "10")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "49")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VDD33A")
				(number "5")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "51")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "54")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "57")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD33A")
				(number "64")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD18CORE")
				(number "15")
			)
			(pin passive line
				(at 0 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD18CORE")
				(number "38")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "VDD18ETHPLL")
				(number "48")
			)
			(pin power_in line
				(at 10.16 33.02 270)
				(length 2.54)
				(name "VDD18USBPLL")
				(number "62")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "EECLK")
				(number "23")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "EECS")
				(number "24")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "EEDO")
				(number "25")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "EEDI")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{FDX_LED}/GPIO0")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{LNKA_LED}/GPIO1")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "~{SPD_LED}/GPIO2")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "GPIO3")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "GPIO4")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "GPIO5")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "GPIO6")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "GPIO7")
				(number "43")
			)
		)
		(symbol "LAN9514_2_1"
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "USBDP0")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "USBDM0")
				(number "58")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "VBUS_DET")
				(number "11")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "USBRBIAS")
				(number "63")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "AUTOMDIX_EN")
				(number "41")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "EXRES")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "USBDP2")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "USBDM2")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PRTCTL2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "USBDP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "USBDM3")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PRTCTL3")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "USBDP4")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "USBDM4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PRTCTL4")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "USBDP5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "USBDM5")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PRTCTL5")
				(number "18")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "TXP")
				(number "55")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "TXN")
				(number "56")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "RXP")
				(number "52")
			)
			(pin input line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "RXN")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RTL8211EG-VB-CG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 22.86 -58.42 0)
		)
		(property "Value" "RTL8211EG-VB-CG"
			(at -15.24 -58.42 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP3.8x3.8mm"
			(at -15.24 10.16 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/szlcsc/Realtek-Semicon-RTL8211EG-VB-CG_C69264.pdf"
			(at 17.78 -5.08 0)
		)
		(property "Description" "10/100/1000Mbps Ethernet Transceiver with RGMII/GMII/MII/RMII Interface, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ethernet Phy Gigabit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "RTL8211EG-VB-CG_0_1")
		(symbol "RTL8211EG-VB-CG_1_1"
			(pin input line
				(at -27.94 43.18 0)
				(length 2.54)
				(name "ENSWREG")
				(number "57")
			)
			(pin input line
				(at -27.94 38.1 0)
				(length 2.54)
				(name "GTX_CLK")
				(number "34")
			)
			(pin output line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "TXCLK")
				(number "42")
			)
			(pin input line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "TXD0")
				(number "36")
			)
			(pin input line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "TXD1")
				(number "39")
			)
			(pin input line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "TXD2")
				(number "40")
			)
			(pin input line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "TXD3")
				(number "41")
			)
			(pin input line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "TXD4")
				(number "43")
			)
			(pin input line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "TXD5")
				(number "44")
			)
			(pin input line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "TXD6")
				(number "45")
			)
			(pin input line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "TXD7")
				(number "46")
			)
			(pin input line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "TXEN")
				(number "35")
			)
			(pin input line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "TXER")
				(number "47")
			)
			(pin output line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "RXC")
				(number "24")
			)
			(pin output line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "RXD0")
				(number "19")
			)
			(pin output line
				(at -27.94 0 0)
				(length 2.54)
				(name "RXD1")
				(number "21")
			)
			(pin output line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "RXD2")
				(number "22")
			)
			(pin output line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "RXD3")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "RXD4/SELRGV")
				(number "25")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "RXD5/TXDLY")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "RXD6/RXDLY")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "RXD7/AN0")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "RXDV/PHY_AD2")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "RXER/AN1")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "COL/MODE")
				(number "31")
			)
			(pin output line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "CRS")
				(number "32")
			)
			(pin input line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "CKXTAL1")
				(number "61")
			)
			(pin output line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "CKXTAL2")
				(number "62")
			)
			(pin output line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "CLK125")
				(number "1")
			)
			(pin input line
				(at -27.94 -40.64 0)
				(length 2.54)
				(name "~{PHYRST}")
				(number "38")
			)
			(pin input line
				(at -27.94 -45.72 0)
				(length 2.54)
				(name "MDC")
				(number "53")
			)
			(pin bidirectional line
				(at -27.94 -48.26 0)
				(length 2.54)
				(name "MDIO")
				(number "54")
			)
			(pin open_collector line
				(at -27.94 -50.8 0)
				(length 2.54)
				(name "~{PME}")
				(number "55")
			)
			(pin open_collector line
				(at -27.94 -53.34 0)
				(length 2.54)
				(name "~{INT}")
				(number "56")
			)
			(pin power_in line
				(at -22.86 55.88 270)
				(length 2.54)
				(name "VDDREG")
				(number "64")
			)
			(pin power_in line
				(at -17.78 55.88 270)
				(length 2.54)
				(name "AVDD33")
				(number "10")
			)
			(pin power_in line
				(at -15.24 55.88 270)
				(length 2.54)
				(name "AVDD33")
				(number "60")
			)
			(pin power_in line
				(at -10.16 55.88 270)
				(length 2.54)
				(name "DVDD33")
				(number "49")
			)
			(pin power_in line
				(at -5.08 55.88 270)
				(length 2.54)
				(name "DVDD33")
				(number "20")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 2.54)
				(name "DVDD33")
				(number "26")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 2.54)
				(name "DVDD33")
				(number "37")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_out line
				(at 5.08 55.88 270)
				(length 2.54)
				(name "REG_OUT")
				(number "3")
			)
			(pin power_in line
				(at 10.16 55.88 270)
				(length 2.54)
				(name "AVDD10")
				(number "7")
			)
			(pin power_in line
				(at 12.7 55.88 270)
				(length 2.54)
				(name "AVDD10")
				(number "13")
			)
			(pin power_in line
				(at 15.24 55.88 270)
				(length 2.54)
				(name "AVDD10")
				(number "59")
			)
			(pin power_in line
				(at 20.32 55.88 270)
				(length 2.54)
				(name "DVDD10")
				(number "33")
			)
			(pin power_in line
				(at 22.86 55.88 270)
				(length 2.54)
				(name "DVDD10")
				(number "48")
			)
			(pin no_connect line
				(at 25.4 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at 25.4 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 2.54)
				(name "MDI[0]+")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 2.54)
				(name "MDI[0]-")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "MDI[1]+")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 2.54)
				(name "MDI[1]-")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "MDI[2]+")
				(number "11")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "MDI[2]-")
				(number "12")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 2.54)
				(name "MDI[3]+")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "MDI[3]-")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "LED0/PHY_AD0")
				(number "50")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "LED1/PHY_AD1")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "LED2")
				(number "52")
			)
			(pin passive line
				(at 27.94 -53.34 180)
				(length 2.54)
				(name "RSET")
				(number "58")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VSC8541XMV-0x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.764 64.516 0)
		)
		(property "Value" "VSC8541XMV-0x"
			(at 19.304 64.77 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-68-1EP_8x8mm_P0.4mm_EP5.2x5.2mm"
			(at 0 -67.31 0)
		)
		(property "Datasheet" "https://ethernet.microsemi.com/products/download.php?fid=7978&number=vsc8541"
			(at 32.004 -64.77 0)
		)
		(property "Description" "Single Port Gigabit Ethernet, GMII/RGMII/MII/RMII Interfaces, QFN-68"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gigabit Ethernet PHY GMII RGMII MII RMII"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN?68*1EP*8x8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "VSC8541XMV-0x_0_1"
			(pin input line
				(at -20.32 48.26 0)
				(length 2.54)
				(name "XTAL1")
				(number "63")
			)
			(pin output line
				(at -20.32 43.18 0)
				(length 2.54)
				(name "XTAL2")
				(number "64")
			)
			(pin output line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "LED0")
				(number "60")
			)
			(pin output line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "LED1")
				(number "59")
			)
			(pin passive line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "P0_D0P")
				(number "13")
			)
			(pin passive line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "P0_D0N")
				(number "12")
			)
			(pin passive line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "P0_D1P")
				(number "10")
			)
			(pin passive line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "P0_D1N")
				(number "9")
			)
			(pin passive line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "P0_D2P")
				(number "7")
			)
			(pin passive line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "P0_D2N")
				(number "6")
			)
			(pin passive line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "P0_D3P")
				(number "4")
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "P0_D3N")
				(number "3")
			)
			(pin passive line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "THERMDA")
				(number "15")
			)
			(pin passive line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "THERMDC_VSS")
				(number "16")
			)
			(pin passive line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "REF_FILT")
				(number "67")
			)
			(pin passive line
				(at -20.32 -48.26 0)
				(length 2.54)
				(name "REF_REXT")
				(number "1")
			)
			(pin output line
				(at -20.32 -53.34 0)
				(length 2.54)
				(name "RCVRD_CLK")
				(number "55")
			)
			(pin input line
				(at -20.32 -58.42 0)
				(length 2.54)
				(name "REFCLK_SEL_0")
				(number "62")
			)
			(pin input line
				(at -20.32 -60.96 0)
				(length 2.54)
				(name "REFCLK_SEL_1")
				(number "61")
			)
			(pin no_connect line
				(at -17.78 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED_0")
				(number "66")
			)
			(pin no_connect line
				(at -17.78 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "RESERVED_1")
				(number "65")
			)
			(pin power_in line
				(at -12.7 66.04 270)
				(length 2.54)
				(name "VDD25A")
				(number "2")
			)
			(pin power_in line
				(at -10.16 66.04 270)
				(length 2.54)
				(name "VDD25A")
				(number "8")
			)
			(pin power_in line
				(at -7.62 66.04 270)
				(length 2.54)
				(name "VDD25A")
				(number "11")
			)
			(pin power_in line
				(at -5.08 66.04 270)
				(length 2.54)
				(name "VDD1A")
				(number "5")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 2.54)
				(name "VDD1A")
				(number "14")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 2.54)
				(name "VDD1A")
				(number "68")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 2.54)
				(name "VSS")
				(number "69")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 2.54)
				(name "VDD1")
				(number "17")
			)
			(pin passive line
				(at 2.54 66.04 270)
				(length 2.54)
				(hide yes)
				(name "VDD1")
				(number "34")
			)
			(pin power_in line
				(at 5.08 66.04 270)
				(length 2.54)
				(name "VDDIO")
				(number "58")
			)
			(pin power_in line
				(at 7.62 66.04 270)
				(length 2.54)
				(name "VDDMAC")
				(number "22")
			)
			(pin passive line
				(at 7.62 66.04 270)
				(length 2.54)
				(hide yes)
				(name "VDDMAC")
				(number "28")
			)
			(pin passive line
				(at 7.62 66.04 270)
				(length 2.54)
				(hide yes)
				(name "VDDMAC")
				(number "39")
			)
			(pin passive line
				(at 7.62 66.04 270)
				(length 2.54)
				(hide yes)
				(name "VDDMAC")
				(number "44")
			)
			(pin power_in line
				(at 10.16 66.04 270)
				(length 2.54)
				(name "VDDMDIO")
				(number "49")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 2.54)
				(name "RX_CLK")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 2.54)
				(name "RX_ER")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 2.54)
				(name "RX_DV/RX_CTL")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "RXD0")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "RXD1")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "RXD2")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "RXD3")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "RXD4")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "RXD5")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "RXD6")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "RXD7")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "CRS")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "COL")
				(number "18")
			)
			(pin input line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "TXD0")
				(number "38")
			)
			(pin input line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "TXD1")
				(number "40")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "TXD2")
				(number "41")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "TXD3")
				(number "42")
			)
			(pin input line
				(at 20.32 0 180)
				(length 2.54)
				(name "TXD4")
				(number "43")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "TXD5")
				(number "45")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "TXD6")
				(number "46")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "TXD7")
				(number "47")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "TX_EN/TX_CTL")
				(number "33")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "GTX_CLK")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "MII_TXCLK")
				(number "36")
			)
			(pin input line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "TX_ER")
				(number "35")
			)
			(pin input line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "MDC")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "MDIO")
				(number "50")
			)
			(pin input line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "NRESET")
				(number "53")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "COMA_MODE")
				(number "56")
			)
			(pin output line
				(at 20.32 -40.64 180)
				(length 2.54)
				(name "MDINT")
				(number "51")
			)
			(pin output line
				(at 20.32 -43.18 180)
				(length 2.54)
				(name "FASTLINK_FAIL")
				(number "52")
			)
			(pin input line
				(at 20.32 -53.34 180)
				(length 2.54)
				(name "CLK_SQUELCH_IN")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 2.54)
				(name "CLKOUT")
				(number "54")
			)
		)
		(embedded_fonts no)
	)
	(symbol "W5100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 49.53 0)
		)
		(property "Value" "W5100"
			(at 15.24 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_10x10mm_P0.4mm"
			(at 3.81 -49.53 0)
		)
		(property "Datasheet" "http://www.wiznet.io/wp-content/uploads/wiznethome/Chip/W5100/Document/W5100_Datasheet_v1.2.7.pdf"
			(at -92.71 80.01 0)
		)
		(property "Description" "10/100Mb Ethernet controller with TCP/IP stack, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Wiznet Ethernet controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "W5100_0_1")
		(symbol "W5100_1_1"
			(pin input line
				(at -17.78 45.72 0)
				(length 2.54)
				(name "~{RESET}")
				(number "59")
			)
			(pin output line
				(at -17.78 43.18 0)
				(length 2.54)
				(name "~{INT}")
				(number "56")
			)
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "SEN")
				(number "31")
			)
			(pin input line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "SCLK")
				(number "30")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "~{SCS}")
				(number "29")
			)
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "MOSI")
				(number "28")
			)
			(pin output line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "MISO")
				(number "27")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "~{CS}")
				(number "55")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{WR}")
				(number "57")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "~{RD}")
				(number "58")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "ADDR0")
				(number "54")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "ADDR1")
				(number "53")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "ADDR2")
				(number "52")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "ADDR3")
				(number "51")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "ADDR4")
				(number "50")
			)
			(pin input line
				(at -17.78 0 0)
				(length 2.54)
				(name "ADDR5")
				(number "49")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "ADDR6")
				(number "48")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "ADDR7")
				(number "47")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "ADDR8")
				(number "46")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "ADDR9")
				(number "45")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "ADDR10")
				(number "42")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "ADDR11")
				(number "41")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "ADDR12")
				(number "40")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "ADDR13")
				(number "39")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "ADDR14")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "DATA0")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "DATA1")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "DATA2")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "DATA3")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "DATA4")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "DATA5")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "DATA6")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -45.72 0)
				(length 2.54)
				(name "DATA7")
				(number "19")
			)
			(pin power_out line
				(at -5.08 50.8 270)
				(length 2.54)
				(name "1V8_OUT")
				(number "11")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "VCC1V8A")
				(number "7")
			)
			(pin passive line
				(at -2.54 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC1V8A")
				(number "74")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC1V8D")
				(number "15")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC1V8D")
				(number "16")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC1V8D")
				(number "33")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC1V8D")
				(number "69")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "10")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GNDA")
				(number "4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "77")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 2.54)
				(name "GNDD")
				(number "13")
			)
			(pin passive line
				(at 2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "14")
			)
			(pin passive line
				(at 2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "17")
			)
			(pin passive line
				(at 2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "32")
			)
			(pin passive line
				(at 2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "43")
			)
			(pin passive line
				(at 2.54 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GNDD")
				(number "68")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 2.54)
				(name "VCC3V3A")
				(number "2")
			)
			(pin power_in line
				(at 7.62 50.8 270)
				(length 2.54)
				(name "VCC3V3D")
				(number "12")
			)
			(pin passive line
				(at 7.62 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC3V3D")
				(number "18")
			)
			(pin passive line
				(at 7.62 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC3V3D")
				(number "44")
			)
			(pin no_connect line
				(at 15.24 -30.48 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 15.24 -33.02 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "60")
			)
			(pin no_connect line
				(at 15.24 -35.56 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "61")
			)
			(pin no_connect line
				(at 15.24 -38.1 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "62")
			)
			(pin no_connect line
				(at 15.24 -40.64 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "78")
			)
			(pin no_connect line
				(at 15.24 -43.18 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "79")
			)
			(pin no_connect line
				(at 15.24 -45.72 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "80")
			)
			(pin output line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "TXOP")
				(number "8")
			)
			(pin output line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "TXON")
				(number "9")
			)
			(pin input line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "RXIP")
				(number "5")
			)
			(pin input line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "RXIN")
				(number "6")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "LINKLED")
				(number "66")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "SPDLED")
				(number "67")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "FDXLED")
				(number "70")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "COLLED")
				(number "71")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "RXLED")
				(number "72")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "TXLED")
				(number "73")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "XTLP")
				(number "76")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "XTLN")
				(number "75")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "OPMODE0")
				(number "63")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "OPMODE1")
				(number "64")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "OPMODE2")
				(number "65")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "TEST_MODE0")
				(number "37")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "TEST_MODE1")
				(number "36")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "TEST_MODE2")
				(number "35")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "TEST_MODE3")
				(number "34")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "RSET_BG")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "W5100S-L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 -30.48 0)
		)
		(property "Value" "W5100S-L"
			(at 15.24 -33.02 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "https://docs.wiznet.io/img/products/w5100s/w5100s-ds-v128e.pdf"
			(at 0 -45.72 0)
		)
		(property "Description" "10/100Mb Ethernet controller with TCP/IP stack, LQFP-48"
			(at 0 -48.26 0)
		)
		(property "Manufacturer" "WIZnet"
			(at 0 -50.8 0)
		)
		(property "ki_keywords" "Wiznet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "W5100S-L_0_1")
		(symbol "W5100S-L_1_0"
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "~{RST}")
				(number "48")
			)
		)
		(symbol "W5100S-L_1_1"
			(pin output line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "~{INT}")
				(number "47")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "SCLK")
				(number "30")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "~{CS}")
				(number "29")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "MOSI")
				(number "32")
				(alternate "ADDR0" input line)
			)
			(pin output line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "MISO")
				(number "33")
				(alternate "ADDR1" input line)
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "~{WR}")
				(number "35")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "~{RD}")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DATA0")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DATA1")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "DATA2")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "DATA3")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "DATA4")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "DATA5")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "DATA6")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "DATA7")
				(number "44")
			)
			(pin output line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "RSET_BG")
				(number "9")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "1V2A")
				(number "4")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "1V2D")
				(number "13")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "1V2D")
				(number "22")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "1V2D")
				(number "31")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "1V2D")
				(number "45")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 2.54)
				(name "GNDA")
				(number "1")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "16")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "7")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "3V3A")
				(number "15")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "3V3A")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "3V3D")
				(number "24")
			)
			(pin passive line
				(at 5.08 30.48 270)
				(length 2.54)
				(hide yes)
				(name "3V3D")
				(number "36")
			)
			(pin power_out line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "1V2O")
				(number "14")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "TXOP")
				(number "3")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "TXON")
				(number "2")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "RXIP")
				(number "6")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "RXIN")
				(number "5")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "~{LNK}")
				(number "17")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "~{SPD}")
				(number "18")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "~{DPX}")
				(number "19")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "~{ACT}")
				(number "20")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "~{COL}")
				(number "21")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "XSCO")
				(number "11")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "XSCI")
				(number "12")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "MOD[0]")
				(number "25")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "MOD[1]")
				(number "26")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "MOD[2]")
				(number "27")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "MOD[3]")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "W5100S-Q"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 -30.48 0)
		)
		(property "Value" "W5100S-Q"
			(at 15.24 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "https://docs.wiznet.io/img/products/w5100s/w5100s-ds-v128e.pdf"
			(at 0 -45.72 0)
		)
		(property "Description" "10/100Mb Ethernet controller with TCP/IP stack, QFN-48"
			(at 0 -48.26 0)
		)
		(property "Manufacturer" "WIZnet"
			(at 0 -50.8 0)
		)
		(property "ki_keywords" "Wiznet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.5mm*EP5.3x5.3mm*"
			(at 0 0 0)
		)
		(symbol "W5100S-Q_0_1")
		(symbol "W5100S-Q_1_0"
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "~{RST}")
				(number "48")
			)
		)
		(symbol "W5100S-Q_1_1"
			(pin output line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "~{INT}")
				(number "47")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "SCLK")
				(number "30")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "~{CS}")
				(number "29")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "MOSI")
				(number "32")
				(alternate "ADDR0" input line)
			)
			(pin output line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "MISO")
				(number "33")
				(alternate "ADDR1" input line)
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "~{WR}")
				(number "35")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "~{RD}")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DATA0")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DATA1")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "DATA2")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "DATA3")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "DATA4")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "DATA5")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "DATA6")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "DATA7")
				(number "44")
			)
			(pin output line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "RSET_BG")
				(number "9")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "1V2A")
				(number "4")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "1V2D")
				(number "13")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "1V2D")
				(number "22")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "1V2D")
				(number "31")
			)
			(pin passive line
				(at -2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "1V2D")
				(number "45")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 2.54)
				(name "GNDA")
				(number "1")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "16")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GNDA")
				(number "7")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(name "EP")
				(number "49")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "3V3A")
				(number "15")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "3V3A")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "3V3D")
				(number "24")
			)
			(pin passive line
				(at 5.08 30.48 270)
				(length 2.54)
				(hide yes)
				(name "3V3D")
				(number "36")
			)
			(pin power_out line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "1V2O")
				(number "14")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "TXOP")
				(number "3")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "TXON")
				(number "2")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "RXIP")
				(number "6")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "RXIN")
				(number "5")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "~{LNK}")
				(number "17")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "~{SPD}")
				(number "18")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "~{DPX}")
				(number "19")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "~{ACT}")
				(number "20")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "~{COL}")
				(number "21")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "XSCO")
				(number "11")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "XSCI")
				(number "12")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "MOD[0]")
				(number "25")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "MOD[1]")
				(number "26")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "MOD[2]")
				(number "27")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "MOD[3]")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "W5500"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 29.21 0)
		)
		(property "Value" "W5500"
			(at 8.89 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 41.91 0)
		)
		(property "Datasheet" "http://wizwiki.net/wiki/lib/exe/fetch.php/products:w5500:w5500_ds_v109e.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "10/100Mb SPI Ethernet controller with TCP/IP stack, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "WIZnet Ethernet controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "W5500_0_1")
		(symbol "W5500_1_1"
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "~{SCS}")
				(number "32")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "SCLK")
				(number "33")
			)
			(pin output line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "MISO")
				(number "34")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "MOSI")
				(number "35")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "~{INT}")
				(number "36")
			)
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "~{RST}")
				(number "37")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PMODE0")
				(number "45")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PMODE1")
				(number "44")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PMODE2")
				(number "43")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "XI/CLKIN")
				(number "30")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "XO")
				(number "31")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RSVD")
				(number "38")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RSVD")
				(number "39")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "RSVD")
				(number "40")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "RSVD")
				(number "41")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "RSVD")
				(number "42")
			)
			(pin input line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "RSVD")
				(number "23")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "11")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "15")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "17")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "21")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "AVDD")
				(number "4")
			)
			(pin passive line
				(at 2.54 30.48 270)
				(length 2.54)
				(hide yes)
				(name "AVDD")
				(number "8")
			)
			(pin passive line
				(at 2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "14")
			)
			(pin passive line
				(at 2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "16")
			)
			(pin passive line
				(at 2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "19")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "AGND")
				(number "3")
			)
			(pin passive line
				(at 2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "48")
			)
			(pin passive line
				(at 2.54 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "9")
			)
			(pin no_connect line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "DNC")
				(number "7")
			)
			(pin no_connect line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 12.7 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 12.7 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "46")
			)
			(pin no_connect line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "47")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "TXN")
				(number "1")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "TXP")
				(number "2")
			)
			(pin input line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "RXN")
				(number "5")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "RXP")
				(number "6")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "SPDLED")
				(number "24")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "LINKLED")
				(number "25")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DUPLED")
				(number "26")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "ACTLED")
				(number "27")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "EXRES1")
				(number "10")
			)
			(pin passive line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "VBG")
				(number "18")
			)
			(pin passive line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "TOCAP")
				(number "20")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "1V2O")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WGI210AT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 44.45 0)
		)
		(property "Value" "WGI210AT"
			(at 25.4 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP3.4x3.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intel.com/content/www/us/en/ethernet-controllers/i210-ethernet-controller-datasheet.html"
			(at 0 0 0)
		)
		(property "Description" "10/100/1000Mbps Ethernet transceiver with GMII/Serdes/PCIe interface, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Gigabit ethernet PHY PCIe"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "WGI210AT_0_1"
			(pin input line
				(at -33.02 40.64 0)
				(length 2.54)
				(name "~{DEV_OFF}")
				(number "28")
			)
			(pin input line
				(at -33.02 35.56 0)
				(length 2.54)
				(name "LAN_PWR_GOOD")
				(number "1")
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 2.54)
				(name "SDP0")
				(number "63")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 2.54)
				(name "SDP1")
				(number "61")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 2.54)
				(name "SDP2")
				(number "62")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 2.54)
				(name "SDP3")
				(number "60")
			)
			(pin input line
				(at -33.02 17.78 0)
				(length 2.54)
				(name "PECLKp")
				(number "26")
			)
			(pin input line
				(at -33.02 15.24 0)
				(length 2.54)
				(name "PECLKn")
				(number "25")
			)
			(pin output line
				(at -33.02 12.7 0)
				(length 2.54)
				(name "PE_Tp")
				(number "21")
			)
			(pin output line
				(at -33.02 10.16 0)
				(length 2.54)
				(name "PE_Tn")
				(number "20")
			)
			(pin input line
				(at -33.02 7.62 0)
				(length 2.54)
				(name "PE_Rp")
				(number "24")
			)
			(pin input line
				(at -33.02 5.08 0)
				(length 2.54)
				(name "PE_Rn")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 2.54)
				(name "~{PE_WAKE}")
				(number "16")
			)
			(pin input line
				(at -33.02 0 0)
				(length 2.54)
				(name "~{PE_RST}")
				(number "17")
			)
			(pin output line
				(at -33.02 -5.08 0)
				(length 2.54)
				(name "NVM_SI")
				(number "12")
			)
			(pin input line
				(at -33.02 -7.62 0)
				(length 2.54)
				(name "NVM_SO")
				(number "14")
			)
			(pin output line
				(at -33.02 -10.16 0)
				(length 2.54)
				(name "NVM_SK")
				(number "13")
			)
			(pin output line
				(at -33.02 -12.7 0)
				(length 2.54)
				(name "~{NVM_CS}")
				(number "15")
			)
			(pin input line
				(at -33.02 -17.78 0)
				(length 2.54)
				(name "NC_SI_CLK_IN")
				(number "2")
			)
			(pin output line
				(at -33.02 -20.32 0)
				(length 2.54)
				(name "NC_SI_CRS_DV")
				(number "3")
			)
			(pin output line
				(at -33.02 -22.86 0)
				(length 2.54)
				(name "NC_SI_RXD0")
				(number "6")
			)
			(pin output line
				(at -33.02 -25.4 0)
				(length 2.54)
				(name "NC_SI_RXD1")
				(number "5")
			)
			(pin input line
				(at -33.02 -27.94 0)
				(length 2.54)
				(name "NC_SI_TX_EN")
				(number "7")
			)
			(pin input line
				(at -33.02 -30.48 0)
				(length 2.54)
				(name "NC_SI_TXD0")
				(number "9")
			)
			(pin input line
				(at -33.02 -33.02 0)
				(length 2.54)
				(name "NC_SI_ARB_IN")
				(number "43")
			)
			(pin output line
				(at -33.02 -35.56 0)
				(length 2.54)
				(name "NC_SI_ARB_OUT")
				(number "44")
			)
			(pin input line
				(at -33.02 -38.1 0)
				(length 2.54)
				(name "NC_SI_TXD1")
				(number "8")
			)
			(pin power_in line
				(at -12.7 45.72 270)
				(length 2.54)
				(name "VDD3p3")
				(number "10")
			)
			(pin passive line
				(at -12.7 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD3p3")
				(number "27")
			)
			(pin passive line
				(at -12.7 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD3p3")
				(number "41")
			)
			(pin passive line
				(at -12.7 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD3p3")
				(number "64")
			)
			(pin power_in line
				(at -10.16 45.72 270)
				(length 2.54)
				(name "VDD3p3")
				(number "51")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDD0p9")
				(number "11")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD0p9")
				(number "32")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD0p9")
				(number "42")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD0p9")
				(number "59")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDD1p5")
				(number "47")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 2.54)
				(name "VDD1p5")
				(number "56")
			)
			(pin power_in line
				(at 15.24 45.72 270)
				(length 2.54)
				(name "NC/Vext")
				(number "22")
			)
			(pin power_out line
				(at 20.32 45.72 270)
				(length 2.54)
				(name "VDD0p9_OUT")
				(number "38")
			)
			(pin power_out line
				(at 22.86 45.72 270)
				(length 2.54)
				(name "VDD1p5_OUT")
				(number "39")
			)
			(pin passive line
				(at 33.02 40.64 180)
				(length 2.54)
				(name "CBOT")
				(number "37")
			)
			(pin passive line
				(at 33.02 38.1 180)
				(length 2.54)
				(name "CTOP")
				(number "40")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 2.54)
				(name "SMB_DATA")
				(number "36")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 2.54)
				(name "SMB_CLK")
				(number "34")
			)
			(pin output line
				(at 33.02 22.86 180)
				(length 2.54)
				(name "~{SMB_ALRT}")
				(number "35")
			)
			(pin input line
				(at 33.02 17.78 180)
				(length 2.54)
				(name "JTAG_TDI")
				(number "29")
			)
			(pin input line
				(at 33.02 15.24 180)
				(length 2.54)
				(name "JTAG_CLK")
				(number "19")
			)
			(pin input line
				(at 33.02 12.7 180)
				(length 2.54)
				(name "JTAG_TMS")
				(number "18")
			)
			(pin output line
				(at 33.02 10.16 180)
				(length 2.54)
				(name "JTAG_TDO")
				(number "4")
			)
			(pin output line
				(at 33.02 5.08 180)
				(length 2.54)
				(name "LED0")
				(number "31")
			)
			(pin output line
				(at 33.02 2.54 180)
				(length 2.54)
				(name "LED1")
				(number "30")
			)
			(pin output line
				(at 33.02 0 180)
				(length 2.54)
				(name "LED2")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 2.54)
				(name "MDI_PLUS[0]/NC")
				(number "58")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 2.54)
				(name "MDI_MINUS[0]/SFP_I2C_DATA")
				(number "57")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 2.54)
				(name "MDI_PLUS[1]/SFP_I2C_CLK")
				(number "55")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 2.54)
				(name "MDI_MINUS[1]/SRDS_SIG_DET")
				(number "54")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 2.54)
				(name "MDI_PLUS[2]")
				(number "53")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 2.54)
				(name "MDI_MINUS[2]/SET_N")
				(number "52")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 2.54)
				(name "MDI_PLUS[3]/SER_P")
				(number "50")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 2.54)
				(name "MDI_MINUS[3]/SER_N")
				(number "49")
			)
			(pin input line
				(at 33.02 -27.94 180)
				(length 2.54)
				(name "XTAL1")
				(number "46")
			)
			(pin output line
				(at 33.02 -30.48 180)
				(length 2.54)
				(name "XTAL2")
				(number "45")
			)
			(pin passive line
				(at 33.02 -35.56 180)
				(length 2.54)
				(name "RSET")
				(number "48")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DP83848I"
		(extends "DP83848C")
		(property "Reference" "U"
			(at -21.59 39.37 0)
		)
		(property "Value" "DP83848I"
			(at 12.7 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 25.4 -39.37 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/dp83848c.pdf"
			(at 0 0 0)
		)
		(property "Description" "MII/RMII Single 10/100Mbps Ethernet Physical Layer Transceiver, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Ethernet PHY MII RMII 10/100Mpbs"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "KSZ8081RND"
		(extends "KSZ8081RNA")
		(property "Reference" "U"
			(at -15.24 26.035 0)
		)
		(property "Value" "KSZ8081RND"
			(at 3.81 26.035 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 35.56 -25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00002199A.pdf"
			(at -57.15 5.08 0)
		)
		(property "Description" "10BASE-T/100BASE-TX PHY with RMII Support, 50 MHz input clock, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ETH PHY RMII"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LAN9303i"
		(extends "LAN9303")
		(property "Reference" "U"
			(at 20.32 -38.1 0)
		)
		(property "Value" "LAN9303i"
			(at 22.86 -40.64 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_8x8mm_P0.5mm_EP5.9x5.9mm_ThermalVias"
			(at 2.54 -45.72 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/9303.pdf"
			(at -33.02 -45.72 0)
		)
		(property "Description" "3-port managed Ethernet switch with dual PHY and RMII interface, QFN-56, industrial version"
			(at 0 0 0)
		)
		(property "ki_keywords" "ETH PHY RMII switch industrial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LAN9512i"
		(extends "LAN9512")
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "LAN9512i"
			(at 15.24 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.3x7.3mm"
			(at 31.75 -31.75 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00002304A.pdf"
			(at 2.54 -7.62 0)
		)
		(property "Description" "Two USB 2.0 hub with an integrated 10/100 Ethernet controller (-40° to 85°C), QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB HUB Ethernet 10/100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP?9x9mm?P0.5mm?EP7.3x7.3mm*"
			(at 0 0 0)
		)
	)
	(symbol "LAN9513i"
		(extends "LAN9513")
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "LAN9513i"
			(at 15.24 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.3x7.3mm"
			(at 31.75 -31.75 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00002305A.pdf"
			(at 2.54 -7.62 0)
		)
		(property "Description" "Three USB 2.0 hub with an integrated 10/100 Ethernet controller (-40° to 85°C), QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB HUB Ethernet 10/100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP?9x9mm?P0.5mm?EP7.3x7.3mm*"
			(at 0 0 0)
		)
	)
	(symbol "LAN9514i"
		(extends "LAN9514")
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "LAN9514i"
			(at 15.24 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.3x7.3mm"
			(at 31.75 -31.75 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00002306A.pdf"
			(at 2.54 -7.62 0)
		)
		(property "Description" "Four USB 2.0 hub with an integrated 10/100 Ethernet controller (-40° to 85°C), QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB HUB Ethernet 10/100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP?9x9mm?P0.5mm?EP7.3x7.3mm*"
			(at 0 0 0)
		)
	)
	(symbol "W6100-L"
		(extends "W5100S-L")
		(property "Reference" "U"
			(at 15.24 -30.48 0)
		)
		(property "Value" "W6100-L"
			(at 15.24 -33.02 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 -50.8 0)
		)
		(property "Datasheet" "https://docs.wiznet.io/img/products/w6100/w6100_ds_v105e.pdf"
			(at 0 -45.72 0)
		)
		(property "Description" "10/100Mb Ethernet controller with TCP/IP stack, IPv4/IPv6, LQFP-48"
			(at 0 -48.26 0)
		)
		(property "ki_keywords" "Wiznet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "W6100-Q"
		(extends "W5100S-Q")
		(property "Reference" "U"
			(at 15.24 -30.48 0)
		)
		(property "Value" "W6100-Q"
			(at 15.24 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm"
			(at 0 -50.8 0)
		)
		(property "Datasheet" "https://docs.wiznet.io/img/products/w6100/w6100_ds_v105e.pdf"
			(at 0 -45.72 0)
		)
		(property "Description" "10/100Mb Ethernet controller with TCP/IP stack, IPv4/IPv6, QFN-48"
			(at 0 -48.26 0)
		)
		(property "ki_keywords" "Wiznet"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.5mm*EP5.3x5.3mm*"
			(at 0 0 0)
		)
	)
)
