(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AS1115-BQFT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "AS1115-BQFT"
			(at 2.54 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-24-1EP_4x4mm_P0.5mm_EP2.8x2.8mm_PullBack_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/36005/AS1115_DS000206_1-00.pdf/3d3e6d35-b184-1329-adf9-2d769eb2404f"
			(at 0 0 0)
		)
		(property "Description" "64 LEDs, I2C Interfaced LED Driver with Keyscan, TQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "led driver i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*1EP*4x4mm*P0.5mm*PullBack*"
			(at 0 0 0)
		)
		(symbol "AS1115-BQFT_0_1")
		(symbol "AS1115-BQFT_1_1"
			(pin passive line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "ISET")
				(number "10")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "22")
			)
			(pin open_collector line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IRQ")
				(number "21")
			)
			(pin passive line
				(at -2.54 -30.48 90)
				(length 2.54)
				(name "EP")
				(number "25")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "SEGA")
				(number "12")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "SEGB")
				(number "14")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "SEGC")
				(number "17")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "SEGD")
				(number "20")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "SEGE")
				(number "18")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SEGF")
				(number "13")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SEGG")
				(number "15")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "SEGDP")
				(number "19")
			)
			(pin open_collector line
				(at 15.24 0 180)
				(length 2.54)
				(name "DIG0")
				(number "23")
			)
			(pin open_collector line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DIG1")
				(number "24")
			)
			(pin open_collector line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DIG2")
				(number "1")
			)
			(pin open_collector line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DIG3")
				(number "2")
			)
			(pin open_collector line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DIG4")
				(number "4")
			)
			(pin open_collector line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "DIG5")
				(number "5")
			)
			(pin open_collector line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "DIG6")
				(number "6")
			)
			(pin open_collector line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "DIG7")
				(number "7")
			)
			(pin open_collector line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "KEYA")
				(number "8")
			)
			(pin open_collector line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "KEYB")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AS1115-BSST"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 29.21 0)
		)
		(property "Value" "AS1115-BSST"
			(at 2.54 29.21 0)
		)
		(property "Footprint" "Package_SO:QSOP-24_3.9x8.7mm_P0.635mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ams.com/documents/20143/36005/AS1115_DS000206_1-00.pdf/3d3e6d35-b184-1329-adf9-2d769eb2404f"
			(at 0 0 0)
		)
		(property "Description" "64 LEDs, I2C Interfaced LED Driver with Keyscan, QSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "led driver i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x8.7m*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "AS1115-BSST_0_1")
		(symbol "AS1115-BSST_1_1"
			(pin passive line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "ISET")
				(number "13")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin open_collector line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IRQ")
				(number "24")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "SEGA")
				(number "15")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "SEGB")
				(number "17")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "SEGC")
				(number "20")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "SEGD")
				(number "23")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "SEGE")
				(number "21")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "SEGF")
				(number "16")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "SEGG")
				(number "18")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "SEGDP")
				(number "22")
			)
			(pin open_collector line
				(at 15.24 0 180)
				(length 2.54)
				(name "DIG0")
				(number "2")
			)
			(pin open_collector line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DIG1")
				(number "3")
			)
			(pin open_collector line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DIG2")
				(number "4")
			)
			(pin open_collector line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DIG3")
				(number "5")
			)
			(pin open_collector line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DIG4")
				(number "7")
			)
			(pin open_collector line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "DIG5")
				(number "8")
			)
			(pin open_collector line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "DIG6")
				(number "9")
			)
			(pin open_collector line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "DIG7")
				(number "10")
			)
			(pin open_collector line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "KEYA")
				(number "11")
			)
			(pin open_collector line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "KEYB")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AW9523B"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 26.67 0)
		)
		(property "Value" "AW9523B"
			(at 6.35 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 34.29 -26.67 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4886/AW9523+English+Datasheet.pdf"
			(at 44.45 -29.21 0)
		)
		(property "Description" "16 multi-function led driver and gpio controller with i2c interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "Port-Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*EP2.7x2.7mm*"
			(at 0 0 0)
		)
		(symbol "AW9523B_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "SCL")
				(number "19")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "SDA")
				(number "20")
			)
			(pin open_collector line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{INT}")
				(number "22")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RST}")
				(number "23")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "AD0")
				(number "18")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "AD1")
				(number "24")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "P0_0")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "P0_1")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "P0_2")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "P0_3")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "P0_4")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "P0_5")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "P0_6")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "P0_7")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "P1_0")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "P1_1")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "P1_2")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "P1_3")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "P1_4")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "P1_5")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "P1_6")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "P1_7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4314xGN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "LTC4314xGN"
			(at 11.43 -20.32 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_3.9x8.7mm_P0.635mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4314f.pdf"
			(at -33.02 69.85 0)
		)
		(property "Description" "Pin-Selectable, 4-Channel, 2-Wire Multiplexer with Bus Buffers, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Multiplexer Buffer Level Shifter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "LTC4314xGN_0_0"
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "SCLOUT1")
				(number "3")
			)
		)
		(symbol "LTC4314xGN_0_1")
		(symbol "LTC4314xGN_1_1"
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SCLIN")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SDAIN")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "ENABLE1")
				(number "12")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "ENABLE2")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "ENABLE3")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ENABLE4")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{ACC}")
				(number "20")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DISCEN")
				(number "1")
			)
			(pin open_collector line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "15")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VCC2")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SDAOUT1")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SCLOUT2")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SDAOUT2")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SCLOUT3")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SDAOUT3")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SCLOUT4")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SDAOUT4")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4314xUDC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "LTC4314xUDC"
			(at 11.43 -20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x4mm_P0.5mm_EP1.65x2.65mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4314f.pdf"
			(at -33.02 69.85 0)
		)
		(property "Description" "Pin-Selectable, 4-Channel, 2-Wire Multiplexer with Bus Buffers, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Multiplexer Buffer Level Shifter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4314xUDC_0_0"
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "SCLOUT1")
				(number "1")
			)
		)
		(symbol "LTC4314xUDC_0_1")
		(symbol "LTC4314xUDC_1_1"
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "SCLIN")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SDAIN")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "ENABLE1")
				(number "10")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "ENABLE2")
				(number "9")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "ENABLE3")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "ENABLE4")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{ACC}")
				(number "18")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DISCEN")
				(number "19")
			)
			(pin open_collector line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "~{FAULT}")
				(number "13")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "EP")
				(number "21")
			)
			(pin power_in line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VCC2")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SDAOUT1")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SCLOUT2")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SDAOUT2")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SCLOUT3")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SDAOUT3")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SCLOUT4")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SDAOUT4")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4316xDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "LTC4316xDD"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4316fa.pdf"
			(at -15.24 41.91 0)
		)
		(property "Description" "Single I2C/SMBus Address-Translator, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Translator 4kV-ESD Level-Shifter Hot-Swap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4316xDD_0_1")
		(symbol "LTC4316xDD_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "ENABLE")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCLIN")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDAIN")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "XORH")
				(number "2")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "XORL")
				(number "3")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "V_{CC}")
				(number "4")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "EP")
				(number "11")
			)
			(pin open_collector line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "READY")
				(number "6")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SCLOUT")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SDAOUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC4317"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "LTC4317"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-16-1EP_3x5mm_P0.5mm_EP1.66x4.4mm"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/4317fa.pdf"
			(at -15.24 41.91 0)
		)
		(property "Description" "Dual I2C/SMBus Address-Translator, DFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Translator 4kV-ESD Level-Shifter Hot-Swap"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC4317_0_1")
		(symbol "LTC4317_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "ENABLE1")
				(number "8")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "ENABLE2")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCLIN")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDAIN")
				(number "12")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "XORH1")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "XORH2")
				(number "3")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "XORL1")
				(number "6")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "XORL2")
				(number "4")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "EP")
				(number "17")
			)
			(pin open_collector line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "READY1")
				(number "10")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "READY2")
				(number "9")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SCLOUT1")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SDAOUT1")
				(number "13")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SCLOUT2")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SDAOUT2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX31910xUI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "MAX31910xUI"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.85x6.7mm"
			(at 0 39.37 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max31910.pdf"
			(at 0 36.83 0)
		)
		(property "Description" "Ultra-Low Power Industrial, Octal, Digital Input Translator/Serializer, SPI interface, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI digital input serializer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*1EP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX31910xUI_0_1")
		(symbol "MAX31910xUI_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "IN1")
				(number "3")
			)
			(pin output line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "RT1")
				(number "4")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "IN2")
				(number "5")
			)
			(pin output line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "RT2")
				(number "6")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IN3")
				(number "7")
			)
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "RT3")
				(number "8")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IN4")
				(number "9")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RT4")
				(number "10")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN5")
				(number "11")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RT5")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN6")
				(number "18")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RT6")
				(number "17")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "IN7")
				(number "20")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RT7")
				(number "19")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "IN8")
				(number "22")
			)
			(pin output line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "RT8")
				(number "21")
			)
			(pin passive line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "RIREF")
				(number "13")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "V_{CC24V}")
				(number "14")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_out line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "5VOUT")
				(number "15")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "DB0")
				(number "1")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "DB1")
				(number "2")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "MODESEL")
				(number "26")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "16")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{CS}")
				(number "24")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "CLK")
				(number "25")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "SOUT")
				(number "23")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "SIN")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX7325AEG+"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "MAX7325AEG+"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_SO:QSOP-24_3.9x8.7mm_P0.635mm"
			(at 26.67 -25.4 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX7325.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Port Expander with 8 Push-Pull and 8 Open-Drain I/Os, QSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Expander I2C Parallel Port GPIO Maxim"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x8.7*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "MAX7325AEG+_0_1")
		(symbol "MAX7325AEG+_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "SCL")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SDA")
				(number "23")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "~{RST}")
				(number "2")
			)
			(pin open_collector line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "~{INT}")
				(number "1")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "AD0")
				(number "21")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "AD2")
				(number "3")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "V+")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin open_collector line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "O15")
				(number "20")
			)
			(pin open_collector line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "O14")
				(number "19")
			)
			(pin open_collector line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "O13")
				(number "18")
			)
			(pin open_collector line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "O12")
				(number "17")
			)
			(pin open_collector line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "O11")
				(number "16")
			)
			(pin open_collector line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "O10")
				(number "15")
			)
			(pin open_collector line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "O9")
				(number "14")
			)
			(pin open_collector line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "O8")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "P7")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "P6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "P5")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "P4")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "P3")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "P2")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "P1")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "P0")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP23008-xML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "MCP23008-xML"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 0 -26.67 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP23008-MCP23S08-Data-Sheet-20001919F.pdf"
			(at 33.02 -30.48 0)
		)
		(property "Description" "8-bit I/O expander, I2C, interrupts, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C parallel port expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCP23008-xML_0_1")
		(symbol "MCP23008-xML_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "20")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "INT")
				(number "7")
				(alternate "INT" open_collector line)
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A2")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A0")
				(number "3")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "17")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "GP0")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "GP1")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "GP2")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "GP3")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "GP4")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "GP5")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GP6")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "GP7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP23008-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "MCP23008-xP"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-18_W7.62mm"
			(at 0 -26.67 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP23008-MCP23S08-Data-Sheet-20001919F.pdf"
			(at 33.02 -30.48 0)
		)
		(property "Description" "8-bit I/O expander, I2C, interrupts, PDIP-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C parallel port expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP23008-xP_0_1")
		(symbol "MCP23008-xP_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "2")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "INT")
				(number "8")
				(alternate "INT" open_collector line)
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "GP0")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "GP1")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "GP2")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "GP3")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "GP4")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "GP5")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GP6")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "GP7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP23008-xSO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "MCP23008-xSO"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm"
			(at 0 -26.67 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP23008-MCP23S08-Data-Sheet-20001919F.pdf"
			(at 33.02 -30.48 0)
		)
		(property "Description" "8-bit I/O expander, I2C, interrupts, SOIC-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C parallel port expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x11.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP23008-xSO_0_1")
		(symbol "MCP23008-xSO_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "2")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "INT")
				(number "8")
				(alternate "INT" open_collector line)
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "GP0")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "GP1")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "GP2")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "GP3")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "GP4")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "GP5")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GP6")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "GP7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP23008-xSS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "MCP23008-xSS"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -26.67 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/MCP23008-MCP23S08-Data-Sheet-20001919F.pdf"
			(at 33.02 -30.48 0)
		)
		(property "Description" "8-bit I/O expander, I2C, interrupts, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C parallel port expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP23008-xSS_0_1")
		(symbol "MCP23008-xSS_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "6")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "2")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "INT")
				(number "8")
				(alternate "INT" open_collector line)
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "GP0")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "GP1")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "GP2")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "GP3")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "GP4")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "GP5")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GP6")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "GP7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP23017_ML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "MCP23017_ML"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 5.08 -25.4 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MCP23017-Data-Sheet-DS20001952.pdf"
			(at 5.08 -27.94 0)
		)
		(property "Description" "16-bit I/O expander, I2C, interrupts, w pull-ups, GPA/B7 output only (https://microchip.my.site.com/s/article/GPA7---GPB7-Cannot-Be-Used-as-Inputs-In-MCP23017), QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C parallel port expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP23017_ML_0_1")
		(symbol "MCP23017_ML_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "SDA")
				(number "9")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCK")
				(number "8")
			)
			(pin tri_state line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "INTB")
				(number "15")
			)
			(pin tri_state line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "INTA")
				(number "16")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "~{RESET}")
				(number "14")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A2")
				(number "13")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A1")
				(number "12")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "A0")
				(number "11")
			)
			(pin no_connect line
				(at -12.7 15.24 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -12.7 12.7 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "EP")
				(number "29")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "GPB0")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "GPB1")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "GPB2")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "GPB3")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "GPB4")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "GPB5")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "GPB6")
				(number "3")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "GPB7")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "GPA0")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "GPA1")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "GPA2")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "GPA3")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "GPA4")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "GPA5")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "GPA6")
				(number "23")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "GPA7")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP23017_SO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "MCP23017_SO"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 5.08 -25.4 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MCP23017-Data-Sheet-DS20001952.pdf"
			(at 5.08 -27.94 0)
		)
		(property "Description" "16-bit I/O expander, I2C, interrupts, w pull-ups, GPA/B7 output only (https://microchip.my.site.com/s/article/GPA7---GPB7-Cannot-Be-Used-as-Inputs-In-MCP23017),  SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C parallel port expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP23017_SO_0_1")
		(symbol "MCP23017_SO_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "SDA")
				(number "13")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCK")
				(number "12")
			)
			(pin tri_state line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "INTB")
				(number "19")
			)
			(pin tri_state line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "INTA")
				(number "20")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "~{RESET}")
				(number "18")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A2")
				(number "17")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A1")
				(number "16")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "A0")
				(number "15")
			)
			(pin no_connect line
				(at -12.7 15.24 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at -12.7 12.7 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "GPB0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "GPB1")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "GPB2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "GPB3")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "GPB4")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "GPB5")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "GPB6")
				(number "7")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "GPB7")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "GPA0")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "GPA1")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "GPA2")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "GPA3")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "GPA4")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "GPA5")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "GPA6")
				(number "27")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "GPA7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP23S17_ML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "MCP23S17_ML"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 5.08 -25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001952C.pdf"
			(at 5.08 -27.94 0)
		)
		(property "Description" "16-bit I/O expander, SPI, interrupts, w pull-ups, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI parallel port expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP23S17_ML_0_1")
		(symbol "MCP23S17_ML_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "~{CS}")
				(number "7")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCK")
				(number "8")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "SI")
				(number "9")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "SO")
				(number "10")
			)
			(pin tri_state line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "INTB")
				(number "15")
			)
			(pin tri_state line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "INTA")
				(number "16")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "~{RESET}")
				(number "14")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A2")
				(number "13")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A1")
				(number "12")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "A0")
				(number "11")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "EP")
				(number "29")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "GPB0")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "GPB1")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "GPB2")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "GPB3")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "GPB4")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "GPB5")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "GPB6")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "GPB7")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "GPA0")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "GPA1")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "GPA2")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "GPA3")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "GPA4")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "GPA5")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "GPA6")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "GPA7")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP23S17_SO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "MCP23S17_SO"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 5.08 -25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001952C.pdf"
			(at 5.08 -27.94 0)
		)
		(property "Description" "16-bit I/O expander, SPI, interrupts, w pull-ups, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI parallel port expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP23S17_SO_0_1")
		(symbol "MCP23S17_SO_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "~{CS}")
				(number "11")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCK")
				(number "12")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "SI")
				(number "13")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "SO")
				(number "14")
			)
			(pin tri_state line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "INTB")
				(number "19")
			)
			(pin tri_state line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "INTA")
				(number "20")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "~{RESET}")
				(number "18")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A2")
				(number "17")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A1")
				(number "16")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "A0")
				(number "15")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "GPB0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "GPB1")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "GPB2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "GPB3")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "GPB4")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "GPB5")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "GPB6")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "GPB7")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "GPA0")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "GPA1")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "GPA2")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "GPA3")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "GPA4")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "GPA5")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "GPA6")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "GPA7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP23S17_SP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "MCP23S17_SP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 5.08 -25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001952C.pdf"
			(at 5.08 -27.94 0)
		)
		(property "Description" "16-bit I/O expander, SPI, interrupts, w pull-ups, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "microchip i2c parallel port expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP23S17_SP_0_1")
		(symbol "MCP23S17_SP_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "~{CS}")
				(number "11")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCK")
				(number "12")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "SI")
				(number "13")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "SO")
				(number "14")
			)
			(pin tri_state line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "INTB")
				(number "19")
			)
			(pin tri_state line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "INTA")
				(number "20")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "~{RESET}")
				(number "18")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A2")
				(number "17")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A1")
				(number "16")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "A0")
				(number "15")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "GPB0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "GPB1")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "GPB2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "GPB3")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "GPB4")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "GPB5")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "GPB6")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "GPB7")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "GPA0")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "GPA1")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "GPA2")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "GPA3")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "GPA4")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "GPA5")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "GPA6")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "GPA7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP23S17_SS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "MCP23S17_SS"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 5.08 -25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20001952C.pdf"
			(at 5.08 -27.94 0)
		)
		(property "Description" "16-bit I/O expander, I2C, interrupts, w pull-ups, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI parallel port expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP23S17_SS_0_1")
		(symbol "MCP23S17_SS_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "~{CS}")
				(number "11")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCK")
				(number "12")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "SI")
				(number "13")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 5.08)
				(name "SO")
				(number "14")
			)
			(pin tri_state line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "INTB")
				(number "19")
			)
			(pin tri_state line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "INTA")
				(number "20")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "~{RESET}")
				(number "18")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A2")
				(number "17")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A1")
				(number "16")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "A0")
				(number "15")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "GPB0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "GPB1")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "GPB2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "GPB3")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "GPB4")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "GPB5")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "GPB6")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "GPB7")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "GPA0")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "GPA1")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "GPA2")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "GPA3")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "GPA4")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "GPA5")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "GPA6")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "GPA7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "P82B96"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 12.7 0)
		)
		(property "Value" "P82B96"
			(at 5.08 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/P82B96.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual I2C Bus Buffer, DIP8/SO8/TSSOP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Bus Buffer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SOIC* SO* TSSOP*"
			(at 0 0 0)
		)
		(symbol "P82B96_0_1")
		(symbol "P82B96_1_1"
			(pin power_in line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin power_in line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "TXD-SDA")
				(number "3")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RXD-SDA")
				(number "2")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "TXD-SCL")
				(number "5")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "RXD-SCL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9506BS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 59.69 0)
		)
		(property "Value" "PCA9506BS"
			(at 6.35 59.69 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_8x8mm_P0.5mm_EP4.3x4.3mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9505_9506.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "IO expander 40 GPIO, I2C 400kHz, Interrupt, Reset, OE, 2.3 - 5.5V, HVQFN-56"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C TWI IO expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*EP*8x8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PCA9506BS_0_1")
		(symbol "PCA9506BS_1_1"
			(pin input line
				(at -12.7 55.88 0)
				(length 2.54)
				(name "SCL")
				(number "51")
			)
			(pin bidirectional line
				(at -12.7 53.34 0)
				(length 2.54)
				(name "SDA")
				(number "50")
			)
			(pin input line
				(at -12.7 50.8 0)
				(length 2.54)
				(name "~{RESET}")
				(number "49")
			)
			(pin open_collector line
				(at -12.7 48.26 0)
				(length 2.54)
				(name "~{INT}")
				(number "48")
			)
			(pin input line
				(at -12.7 45.72 0)
				(length 2.54)
				(name "~{OE}")
				(number "23")
			)
			(pin input line
				(at -12.7 -48.26 0)
				(length 2.54)
				(name "A0")
				(number "20")
			)
			(pin input line
				(at -12.7 -50.8 0)
				(length 2.54)
				(name "A1")
				(number "21")
			)
			(pin input line
				(at -12.7 -53.34 0)
				(length 2.54)
				(name "A2")
				(number "22")
			)
			(pin power_in line
				(at 0 60.96 270)
				(length 2.54)
				(name "V_{DD}")
				(number "11")
			)
			(pin passive line
				(at 0 60.96 270)
				(length 2.54)
				(hide yes)
				(name "V_{DD}")
				(number "39")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "16")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "27")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "32")
			)
			(pin power_in line
				(at 0 -58.42 90)
				(length 2.54)
				(name "V_{SS}")
				(number "4")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "44")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "55")
			)
			(pin passive line
				(at 0 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "57")
			)
			(pin bidirectional line
				(at 12.7 55.88 180)
				(length 2.54)
				(name "IO0_0")
				(number "52")
			)
			(pin bidirectional line
				(at 12.7 53.34 180)
				(length 2.54)
				(name "IO0_1")
				(number "53")
			)
			(pin bidirectional line
				(at 12.7 50.8 180)
				(length 2.54)
				(name "IO0_2")
				(number "54")
			)
			(pin bidirectional line
				(at 12.7 48.26 180)
				(length 2.54)
				(name "IO0_3")
				(number "56")
			)
			(pin bidirectional line
				(at 12.7 45.72 180)
				(length 2.54)
				(name "IO0_4")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 43.18 180)
				(length 2.54)
				(name "IO0_5")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "IO0_6")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "IO0_7")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "IO1_0")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "IO1_1")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "IO1_2")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "IO1_3")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "IO1_4")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "IO1_5")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "IO1_6")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "IO1_7")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IO2_0")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "IO2_1")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "IO2_2")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IO2_3")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "IO2_4")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "IO2_5")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IO2_6")
				(number "26")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "IO2_7")
				(number "28")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "IO3_0")
				(number "29")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "IO3_1")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "IO3_2")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "IO3_3")
				(number "33")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "IO3_4")
				(number "34")
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "IO3_5")
				(number "35")
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "IO3_6")
				(number "36")
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "IO3_7")
				(number "37")
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "IO4_0")
				(number "38")
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "IO4_1")
				(number "40")
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "IO4_2")
				(number "41")
			)
			(pin bidirectional line
				(at 12.7 -43.18 180)
				(length 2.54)
				(name "IO4_3")
				(number "42")
			)
			(pin bidirectional line
				(at 12.7 -45.72 180)
				(length 2.54)
				(name "IO4_4")
				(number "43")
			)
			(pin bidirectional line
				(at 12.7 -48.26 180)
				(length 2.54)
				(name "IO4_5")
				(number "45")
			)
			(pin bidirectional line
				(at 12.7 -50.8 180)
				(length 2.54)
				(name "IO4_6")
				(number "46")
			)
			(pin bidirectional line
				(at 12.7 -53.34 180)
				(length 2.54)
				(name "IO4_7")
				(number "47")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9516"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "PCA9516"
			(at 3.81 17.78 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCA9518.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "5 channels I2C Hub, SO/TSSOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Hub"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO* SOIC* TSSOP*"
			(at 0 0 0)
		)
		(symbol "PCA9516_0_1")
		(symbol "PCA9516_1_1"
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "SCL0")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "SDA0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "SCL1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 3.81)
				(name "SDA1")
				(number "4")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "EN1")
				(number "5")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "EN2")
				(number "9")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "EN3")
				(number "12")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "EN4")
				(number "15")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "SCL2")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "SDA2")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "SCL3")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "SDA3")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "SCL4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "SDA4")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9536D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "PCA9536D"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 25.4 -8.89 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCA9536.pdf"
			(at -5.08 -43.18 0)
		)
		(property "Description" "4-bit I2C-bus and SMBus IO port, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "i2c io port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PCA9536D_0_1")
		(symbol "PCA9536D_1_1"
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IO0")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "IO1")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "IO2")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IO3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9536DP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "PCA9536DP"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at 25.4 -8.89 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCA9536.pdf"
			(at -5.08 -43.18 0)
		)
		(property "Description" "4-bit I2C-bus and SMBus IO port, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "i2c io port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCA9536DP_0_1")
		(symbol "PCA9536DP_1_1"
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IO0")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "IO1")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "IO2")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IO3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9537"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "PCA9537"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:TSSOP-10_3x3mm_P0.5mm"
			(at 25.4 -8.89 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9537.pdf"
			(at -5.08 -43.18 0)
		)
		(property "Description" "4-bit I2C-bus and SMBus IO port with interrupt and reset, TSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "i2c io port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PCA9537_0_1")
		(symbol "PCA9537_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "6")
			)
			(pin open_collector line
				(at -12.7 0 0)
				(length 2.54)
				(name "~{INT}")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCL")
				(number "8")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IO0")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "IO1")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "IO2")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IO3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9544AD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "PCA9544AD"
			(at 6.35 21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 25.4 -21.59 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCA9544A.pdf"
			(at -5.08 -27.94 0)
		)
		(property "Description" "4-channel I2C-bus multiplexer with interrupt logic, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "i2c multiplexer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PCA9544AD_0_1")
		(symbol "PCA9544AD_1_1"
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "19")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCL")
				(number "18")
			)
			(pin open_collector line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{INT}")
				(number "17")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "SD0")
				(number "5")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "SC0")
				(number "6")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{INT0}")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SD1")
				(number "8")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SC1")
				(number "9")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{INT1}")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SD2")
				(number "12")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SC2")
				(number "13")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{INT2}")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SD3")
				(number "15")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "SC3")
				(number "16")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "~{INT3}")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9544APW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "PCA9544APW"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 27.94 -21.59 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCA9544A.pdf"
			(at -5.08 -27.94 0)
		)
		(property "Description" "4-channel I2C-bus multiplexer with interrupt logic, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "i2c multiplexer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCA9544APW_0_1")
		(symbol "PCA9544APW_1_1"
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDA")
				(number "19")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SCL")
				(number "18")
			)
			(pin open_collector line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{INT}")
				(number "17")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "SD0")
				(number "5")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "SC0")
				(number "6")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{INT0}")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SD1")
				(number "8")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SC1")
				(number "9")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{INT1}")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SD2")
				(number "12")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SC2")
				(number "13")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{INT2}")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SD3")
				(number "15")
			)
			(pin output line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "SC3")
				(number "16")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "~{INT3}")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9547BS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "PCA9547BS"
			(at 1.016 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:HVQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9547.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Low voltage 8-channel I2C switch with reset, HVQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low voltage 8-channel I2C switch with reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVQFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PCA9547BS_0_1")
		(symbol "PCA9547BS_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "SCL")
				(number "19")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SDA")
				(number "20")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "24")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A2")
				(number "18")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A1")
				(number "23")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A0")
				(number "22")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "SC0")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SD0")
				(number "1")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SC1")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SD1")
				(number "3")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SC2")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SD2")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SC3")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SD3")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SC4")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SD4")
				(number "10")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "SC5")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "SD5")
				(number "12")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "SC6")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "SD6")
				(number "14")
			)
			(pin output line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "SC7")
				(number "17")
			)
			(pin bidirectional line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "SD7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9548ADB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "PCA9548ADB"
			(at 1.016 21.59 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pca9548a.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Low voltage 8-channel I2C switch with reset, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low voltage 8-channel I2C switch with reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCA9548ADB_0_1")
		(symbol "PCA9548ADB_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "SCL")
				(number "22")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SDA")
				(number "23")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A2")
				(number "21")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin output line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "SC0")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SD0")
				(number "4")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SC1")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SD1")
				(number "6")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SC2")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SD2")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SC3")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SD3")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SC4")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SD4")
				(number "13")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "SC5")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "SD5")
				(number "15")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "SC6")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "SD6")
				(number "17")
			)
			(pin output line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "SC7")
				(number "20")
			)
			(pin bidirectional line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "SD7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9548ADW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "PCA9548ADW"
			(at 1.016 21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pca9548a.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Low voltage 8-channel I2C switch with reset, SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low voltage 8-channel I2C switch with reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x15.4mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PCA9548ADW_0_1")
		(symbol "PCA9548ADW_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "SCL")
				(number "22")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SDA")
				(number "23")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A2")
				(number "21")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin output line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "SC0")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SD0")
				(number "4")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SC1")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SD1")
				(number "6")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SC2")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SD2")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SC3")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SD3")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SC4")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SD4")
				(number "13")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "SC5")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "SD5")
				(number "15")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "SC6")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "SD6")
				(number "17")
			)
			(pin output line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "SC7")
				(number "20")
			)
			(pin bidirectional line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "SD7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9555D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "PCA9555D"
			(at 6.35 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 24.13 -25.4 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9555.pdf"
			(at 0 0 0)
		)
		(property "Description" "IO expander 16 GPIO, I2C 400kHz, Interrupt, 2.3 - 5.5V, SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C TWI IO expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x15.4mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PCA9555D_0_1")
		(symbol "PCA9555D_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "SDA")
				(number "23")
			)
			(pin open_collector line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{INT}")
				(number "1")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A0")
				(number "21")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "IO0_0")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "IO0_1")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "IO0_2")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "IO0_3")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IO0_4")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "IO0_5")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "IO0_6")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IO0_7")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "IO1_0")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IO1_1")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "IO1_2")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "IO1_3")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "IO1_4")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "IO1_5")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "IO1_6")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "IO1_7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9555DB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "PCA9555DB"
			(at 6.35 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 22.86 -25.4 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9555.pdf"
			(at 0 0 0)
		)
		(property "Description" "IO expander 16 GPIO, I2C 400kHz, Interrupt, 2.3 - 5.5V, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C TWI IO expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCA9555DB_0_1")
		(symbol "PCA9555DB_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "SDA")
				(number "23")
			)
			(pin open_collector line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{INT}")
				(number "1")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A0")
				(number "21")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "IO0_0")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "IO0_1")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "IO0_2")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "IO0_3")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IO0_4")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "IO0_5")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "IO0_6")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IO0_7")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "IO1_0")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IO1_1")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "IO1_2")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "IO1_3")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "IO1_4")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "IO1_5")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "IO1_6")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "IO1_7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9555PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "PCA9555PW"
			(at 6.35 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9555.pdf"
			(at 0 0 0)
		)
		(property "Description" "IO expander 16 GPIO, I2C 400kHz, Interrupt, 2.3 - 5.5V, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C TWI IO expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCA9555PW_0_1")
		(symbol "PCA9555PW_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "SDA")
				(number "23")
			)
			(pin open_collector line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{INT}")
				(number "1")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "A0")
				(number "21")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "IO0_0")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "IO0_1")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "IO0_2")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "IO0_3")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IO0_4")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "IO0_5")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "IO0_6")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "IO0_7")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "IO1_0")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IO1_1")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "IO1_2")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "IO1_3")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "IO1_4")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "IO1_5")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "IO1_6")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "IO1_7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9557BS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "PCA9557BS"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:HVQFN-16-1EP_3x3mm_P0.5mm_EP1.5x1.5mm"
			(at 24.13 -13.97 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9557.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit I2C-bus and SMBus I/O port with reset, HVQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMBUS I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PCA9557BS_0_1")
		(symbol "PCA9557BS_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "IO0")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "IO1")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "IO2")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "IO3")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IO4")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "IO5")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "IO6")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "IO7")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9557D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "PCA9557D"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SO-16_3.9x9.9mm_P1.27mm"
			(at 24.13 -13.97 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9557.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit I2C-bus and SMBus I/O port with reset, SO-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMBUS I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PCA9557D_0_1")
		(symbol "PCA9557D_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "15")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A0")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "IO0")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "IO1")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "IO2")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "IO3")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IO4")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "IO5")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "IO6")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "IO7")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9557PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "PCA9557PW"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 24.13 -13.97 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9557.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit I2C-bus and SMBus I/O port with reset, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMBUS I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCA9557PW_0_1")
		(symbol "PCA9557PW_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RESET}")
				(number "15")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A0")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "4")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A2")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "IO0")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "IO1")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "IO2")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "IO3")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IO4")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "IO5")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "IO6")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "IO7")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCA9847PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "PCA9847PW"
			(at 3.556 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9847.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Ultra low voltage 8-channel I2C switch with reset, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "mux i2c switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCA9847PW_0_1")
		(symbol "PCA9847PW_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "SCL")
				(number "22")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SDA")
				(number "23")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A1")
				(number "21")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A0")
				(number "2")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "V_{DD1}")
				(number "1")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "V_{SS}")
				(number "12")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "V_{DD2}")
				(number "24")
			)
			(pin output line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "SC0")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SD0")
				(number "4")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SC1")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SD1")
				(number "6")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SC2")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SD2")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SC3")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SD3")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SC4")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SD4")
				(number "13")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "SC5")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "SD5")
				(number "15")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "SC6")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "SD6")
				(number "17")
			)
			(pin output line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "SC7")
				(number "20")
			)
			(pin bidirectional line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "SD7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCAL6416AHF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "PCAL6416AHF"
			(at 3.81 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:HVQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCAL6416A.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "IO expander 16 GPIO, I2C 400kHz, Interrupt, 1.65 - 5.5V, HWQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C TWI IO expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PCAL6416AHF_0_1")
		(symbol "PCAL6416AHF_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "SDA")
				(number "20")
			)
			(pin open_collector line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{INT}")
				(number "22")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "24")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "ADDR")
				(number "18")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "V_{DD(I2C-bus)}")
				(number "23")
			)
			(pin passive line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "EP")
				(number "25")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "V_{SS}")
				(number "9")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "V_{DD(P)}")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "P0_0")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "P0_1")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "P0_2")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "P0_3")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "P0_4")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "P0_5")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "P0_6")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "P0_7")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "P1_0")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "P1_1")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "P1_2")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "P1_3")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "P1_4")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "P1_5")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "P1_6")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "P1_7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCAL6416APW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "PCAL6416APW"
			(at 3.81 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCAL6416A.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "IO expander 16 GPIO, I2C 400kHz, Interrupt, 1.65 - 5.5V, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C TWI IO expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCAL6416APW_0_1")
		(symbol "PCAL6416APW_1_1"
			(pin input line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "SDA")
				(number "23")
			)
			(pin open_collector line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{INT}")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "ADDR")
				(number "21")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD_I2C")
				(number "2")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDD_P")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "P0_0")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "P0_1")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "P0_2")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "P0_3")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "P0_4")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "P0_5")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "P0_6")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "P0_7")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "P1_0")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "P1_1")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "P1_2")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "P1_3")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "P1_4")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "P1_5")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "P1_6")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "P1_7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCAL6534EV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 49.53 0)
		)
		(property "Value" "PCAL6534EV"
			(at 3.81 49.53 0)
		)
		(property "Footprint" "Package_BGA:NXP_VFBGA-42_2.6x3mm_Layout6x7_P0.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCAL6534.pdf"
			(at 0 0 0)
		)
		(property "Description" "Ultra low-voltage translating 34-bit Fm+ I2C-bus/SMBus I/O expander with Agile I/O features, interrupt output and reset"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C TWI IO expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NXP*VFBGA*2.6x3mm*Layout6x7*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "PCAL6534EV_0_1")
		(symbol "PCAL6534EV_1_1"
			(pin input line
				(at -12.7 45.72 0)
				(length 2.54)
				(name "SCL")
				(number "A3")
			)
			(pin bidirectional line
				(at -12.7 43.18 0)
				(length 2.54)
				(name "SDA")
				(number "A2")
			)
			(pin open_collector line
				(at -12.7 40.64 0)
				(length 2.54)
				(name "~{INT}")
				(number "B1")
			)
			(pin input line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "~{RESET}")
				(number "A5")
			)
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "ADDR")
				(number "A4")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "V_{DD(I2C-bus)}")
				(number "A1")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 2.54)
				(name "V_{SS}")
				(number "B6")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "V_{DD(P)}")
				(number "A6")
			)
			(pin bidirectional line
				(at 12.7 45.72 180)
				(length 2.54)
				(name "P0_0")
				(number "C1")
			)
			(pin bidirectional line
				(at 12.7 43.18 180)
				(length 2.54)
				(name "P0_1")
				(number "B2")
			)
			(pin bidirectional line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "P0_2")
				(number "B3")
			)
			(pin bidirectional line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "P0_3")
				(number "D1")
			)
			(pin bidirectional line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "P0_4")
				(number "C2")
			)
			(pin bidirectional line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "P0_5")
				(number "C3")
			)
			(pin bidirectional line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "P0_6")
				(number "E1")
			)
			(pin bidirectional line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "P0_7")
				(number "D2")
			)
			(pin bidirectional line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "P1_0")
				(number "D3")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "P1_1")
				(number "F1")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "P1_2")
				(number "E2")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "P1_3")
				(number "G1")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "P1_4")
				(number "G2")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "P1_5")
				(number "F2")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "P1_6")
				(number "G3")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "P1_7")
				(number "F3")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "P2_0")
				(number "E3")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "P2_1")
				(number "F4")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "P2_2")
				(number "G4")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "P2_3")
				(number "G5")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "P2_4")
				(number "G6")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "P2_5")
				(number "F6")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "P2_6")
				(number "F5")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "P2_7")
				(number "E5")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "P3_0")
				(number "E6")
			)
			(pin bidirectional line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "P3_1")
				(number "E4")
			)
			(pin bidirectional line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "P3_2")
				(number "D5")
			)
			(pin bidirectional line
				(at 12.7 -30.48 180)
				(length 2.54)
				(name "P3_3")
				(number "D6")
			)
			(pin bidirectional line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "P3_4")
				(number "D4")
			)
			(pin bidirectional line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "P3_5")
				(number "C5")
			)
			(pin bidirectional line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "P3_6")
				(number "C6")
			)
			(pin bidirectional line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "P3_7")
				(number "C4")
			)
			(pin bidirectional line
				(at 12.7 -45.72 180)
				(length 2.54)
				(name "P4_0")
				(number "B5")
			)
			(pin bidirectional line
				(at 12.7 -48.26 180)
				(length 2.54)
				(name "P4_1")
				(number "B4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF8574TS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "PCF8574TS"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCF8574_PCF8574A.pdf"
			(at 0 0 0)
		)
		(property "Description" "8 Bit Port/Expander to I2C Bus, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCF8574TS_0_1")
		(symbol "PCF8574TS_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A0")
				(number "6")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A1")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "9")
			)
			(pin open_collector output_low
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "~{INT}")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -10.16 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "15")
			)
			(pin no_connect line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 10.16 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "P0")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "P1")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "P2")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "P3")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "P4")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "P5")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "P6")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "P7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF8575DBR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 24.13 0)
		)
		(property "Value" "PCF8575DBR"
			(at 7.62 -24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcf8575.pdf"
			(at 0 0 0)
		)
		(property "Description" "16 Bits Port/Expander to I2C Bus, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PCF8575DBR_0_1")
		(symbol "PCF8575DBR_1_1"
			(pin input line
				(at -10.16 20.32 0)
				(length 2.54)
				(name "SCL")
				(number "22")
			)
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "SDA")
				(number "23")
			)
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A0")
				(number "21")
			)
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin open_collector output_low
				(at -10.16 0 0)
				(length 2.54)
				(name "~{INT}")
				(number "1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 20.32 180)
				(length 2.54)
				(name "P0")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "P1")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "P2")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "P3")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "P4")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "P5")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "P6")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "P7")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "P10")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "P11")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "P12")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "P13")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "P14")
				(number "17")
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "P15")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "P16")
				(number "19")
			)
			(pin bidirectional line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "P17")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF8584"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 22.86 0)
		)
		(property "Value" "PCF8584"
			(at 3.81 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCF8584.pdf"
			(at 0 0 0)
		)
		(property "Description" "I2C Bus Controller, DIP/SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Bus"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SOIC*"
			(at 0 0 0)
		)
		(symbol "PCF8584_0_1")
		(symbol "PCF8584_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "A0")
				(number "6")
			)
			(pin tri_state line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "D0")
				(number "7")
			)
			(pin tri_state line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "D1")
				(number "8")
			)
			(pin tri_state line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "D2")
				(number "9")
			)
			(pin tri_state line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "D3")
				(number "11")
			)
			(pin tri_state line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "D4")
				(number "12")
			)
			(pin tri_state line
				(at -15.24 0 0)
				(length 3.81)
				(name "D5")
				(number "13")
			)
			(pin tri_state line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "D6")
				(number "14")
			)
			(pin tri_state line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "D7")
				(number "15")
			)
			(pin input input_low
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "~{CS}")
				(number "17")
			)
			(pin passive input_low
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "~{RD}")
				(number "16")
			)
			(pin input input_low
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "~{WR}")
				(number "18")
			)
			(pin input clock
				(at -15.24 -17.78 0)
				(length 3.81)
				(name "CLK")
				(number "1")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "SDA")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "SCL")
				(number "3")
			)
			(pin input input_low
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "~{IACK}")
				(number "4")
			)
			(pin output output_low
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "~{INT}")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 3.81)
				(name "~{RST}")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PCF8591"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 17.78 0)
		)
		(property "Value" "PCF8591"
			(at 3.81 17.78 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCF8591.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "4ch ADC, 1 DAC, I2C Bus Interface, DIP/SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C ADC DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SOIC*"
			(at 0 0 0)
		)
		(symbol "PCF8591_0_1")
		(symbol "PCF8591_1_1"
			(pin passive line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "AIN0")
				(number "1")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "AIN1")
				(number "2")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "AIN2")
				(number "3")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "AIN3")
				(number "4")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "SCL")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "SDA")
				(number "9")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "A0")
				(number "5")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "A1")
				(number "6")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "A2")
				(number "7")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "AOUT")
				(number "15")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "VREF")
				(number "14")
			)
			(pin power_out line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "AGND")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "OSC")
				(number "11")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "EXT")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STMPE1600"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.144 21.336 0)
		)
		(property "Value" "STMPE1600"
			(at 6.096 21.336 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 7.62 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/stmpe1600.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "IO expander 16 GPIO, I2C 400kHz, Interrupt, 1.65 - 3.6V, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "IO expander 16 GPIO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STMPE1600_0_1")
		(symbol "STMPE1600_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "SCL")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "SDA")
				(number "20")
			)
			(pin output line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "INT")
				(number "22")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A0")
				(number "18")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A1")
				(number "23")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "A2")
				(number "24")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "GPIO_0")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "GPIO_1")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "GPIO_2")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "GPIO_3")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "GPIO_4")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "GPIO_5")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "GPIO_6")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "GPIO_7")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "GPIO_8")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GPIO_9")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "GPIO_10")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "GPIO_11")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "GPIO_12")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "GPIO_13")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "GPIO_14")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "GPIO_15")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9534"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 12.7 0)
		)
		(property "Value" "TCA9534"
			(at 2.54 12.7 0)
		)
		(property "Footprint" ""
			(at 24.13 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9534.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8 Bit Port/Expander, I2C SMBUS, Interrupt output, TSSOP-16, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMBUS I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm* SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TCA9534_0_1")
		(symbol "TCA9534_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 3.81)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 3.81)
				(name "SDA")
				(number "15")
			)
			(pin open_collector line
				(at -10.16 2.54 0)
				(length 3.81)
				(name "~{INT}")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 3.81)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 3.81)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 3.81)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 3.81)
				(name "P0")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 3.81)
				(name "P1")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "P2")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 3.81)
				(name "P3")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "P4")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 3.81)
				(name "P5")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 3.81)
				(name "P6")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 3.81)
				(name "P7")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9535DBR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TCA9535DBR"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9535.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/o pull-ups, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ti parallel port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TCA9535DBR_0_1")
		(symbol "TCA9535DBR_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "SDA")
				(number "23")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCL")
				(number "22")
			)
			(pin open_collector line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "~{INT}")
				(number "1")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "A0")
				(number "21")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "P00")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "P01")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "P02")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "P03")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "P04")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "P05")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "P06")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "P07")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "P10")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "P11")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "P12")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "P13")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "P14")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "P15")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "P16")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "P17")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9535PWR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TCA9535PWR"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9535.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/o pull-ups, TSSOP-24 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "ti parallel port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TCA9535PWR_0_1")
		(symbol "TCA9535PWR_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "SDA")
				(number "23")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCL")
				(number "22")
			)
			(pin open_collector line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "~{INT}")
				(number "1")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "A0")
				(number "21")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "P00")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "P01")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "P02")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "P03")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "P04")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "P05")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "P06")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "P07")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "P10")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "P11")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "P12")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "P13")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "P14")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "P15")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "P16")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "P17")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9535RGER"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TCA9535RGER"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at 30.48 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9535.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/o pull-ups, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ti parallel port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TCA9535RGER_0_1")
		(symbol "TCA9535RGER_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "SDA")
				(number "20")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCL")
				(number "19")
			)
			(pin open_collector line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "~{INT}")
				(number "22")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A2")
				(number "24")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A1")
				(number "23")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "A0")
				(number "18")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "EPAD")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "P00")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "P01")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "P02")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "P03")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "P04")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "P05")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "P06")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "P07")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "P10")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "P11")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "P12")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "P13")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "P14")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "P15")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "P16")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "P17")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9535RTWR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TCA9535RTWR"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at 30.48 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9535.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/o pull-ups, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ti parallel port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TCA9535RTWR_0_1")
		(symbol "TCA9535RTWR_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "SDA")
				(number "20")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCL")
				(number "19")
			)
			(pin open_collector line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "~{INT}")
				(number "22")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A2")
				(number "24")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A1")
				(number "23")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "A0")
				(number "18")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "EPAD")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "P00")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "P01")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "P02")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "P03")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "P04")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "P05")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "P06")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "P07")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "P10")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "P11")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "P12")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "P13")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "P14")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "P15")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "P16")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "P17")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9544A"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 20.32 0)
		)
		(property "Value" "TCA9544A"
			(at 2.54 20.32 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 25.4 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9544a.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "I2C Hub, 4 Channels, Interrupts, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Hub"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TCA9544A_0_1")
		(symbol "TCA9544A_1_1"
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 3.81)
				(name "SCL")
				(number "18")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 3.81)
				(name "SDA")
				(number "19")
			)
			(pin open_collector line
				(at -10.16 12.7 0)
				(length 3.81)
				(name "~{INT}")
				(number "17")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 3.81)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 -15.24 0)
				(length 3.81)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -17.78 0)
				(length 3.81)
				(name "A0")
				(number "1")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 3.81)
				(name "SC0")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "SD0")
				(number "5")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "~{INT0}")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "SC1")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "SD1")
				(number "8")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "~{INT1}")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "SC2")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "SD2")
				(number "12")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "~{INT2}")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 3.81)
				(name "SC3")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 3.81)
				(name "SD3")
				(number "15")
			)
			(pin input line
				(at 12.7 -17.78 180)
				(length 3.81)
				(name "~{INT3}")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9548AMRGER"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "TCA9548AMRGER"
			(at 1.016 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024C_VQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9548a.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Low voltage 8-channel I2C switch with reset, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low voltage 8-channel I2C switch with reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024C*"
			(at 0 0 0)
		)
		(symbol "TCA9548AMRGER_0_1")
		(symbol "TCA9548AMRGER_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "SCL")
				(number "19")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SDA")
				(number "20")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "24")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A2")
				(number "18")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A1")
				(number "23")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A0")
				(number "22")
			)
			(pin no_connect line
				(at -7.62 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "1EP")
				(number "25")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "SC0")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SD0")
				(number "1")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SC1")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SD1")
				(number "3")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SC2")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SD2")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SC3")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SD3")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SC4")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SD4")
				(number "10")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "SC5")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "SD5")
				(number "12")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "SC6")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "SD6")
				(number "14")
			)
			(pin output line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "SC7")
				(number "17")
			)
			(pin bidirectional line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "SD7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9548APWR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "TCA9548APWR"
			(at 1.016 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9548a.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Low voltage 8-channel I2C switch with reset, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low voltage 8-channel I2C switch with reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TCA9548APWR_0_1")
		(symbol "TCA9548APWR_1_1"
			(pin input line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "SCL")
				(number "22")
			)
			(pin bidirectional line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "SDA")
				(number "23")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A2")
				(number "21")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin output line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "SC0")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SD0")
				(number "4")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SC1")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SD1")
				(number "6")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "SC2")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SD2")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SC3")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SD3")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SC4")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SD4")
				(number "13")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "SC5")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "SD5")
				(number "15")
			)
			(pin output line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "SC6")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "SD6")
				(number "17")
			)
			(pin output line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "SC7")
				(number "20")
			)
			(pin bidirectional line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "SD7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9554DB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TCA9554DB"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_5.3x6.2mm_P0.65mm"
			(at 24.13 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9554.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8 Bit Port/Expander, I2C SMBUS, Interrupt output, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMBUS I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x6.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TCA9554DB_0_1")
		(symbol "TCA9554DB_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "15")
			)
			(pin open_collector line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{INT}")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "P0")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "P1")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "P2")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "P3")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "P4")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "P5")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "P6")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "P7")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9554DBQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TCA9554DBQ"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 24.13 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9554.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8 Bit Port/Expander, I2C SMBUS, Interrupt output, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMBUS I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "TCA9554DBQ_0_1")
		(symbol "TCA9554DBQ_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "15")
			)
			(pin open_collector line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{INT}")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "P0")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "P1")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "P2")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "P3")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "P4")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "P5")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "P6")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "P7")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9554DW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TCA9554DW"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 24.13 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9554.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8 Bit Port/Expander, I2C SMBUS, Interrupt output, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMBUS I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TCA9554DW_0_1")
		(symbol "TCA9554DW_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "15")
			)
			(pin open_collector line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{INT}")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "P0")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "P1")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "P2")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "P3")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "P4")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "P5")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "P6")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "P7")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9554PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TCA9554PW"
			(at 2.54 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 24.13 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9554.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8 Bit Port/Expander, I2C SMBUS, Interrupt output, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SMBUS I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TCA9554PW_0_1")
		(symbol "TCA9554PW_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "15")
			)
			(pin open_collector line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{INT}")
				(number "13")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "P0")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "P1")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "P2")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "P3")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "P4")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "P5")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "P6")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "P7")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPIC6595"
		(pin_names
			(offset 0.381)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "TPIC6595"
			(at 6.35 13.97 0)
		)
		(property "Footprint" ""
			(at 16.51 -16.51 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpic6595.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Power Logic 8-bit Shift Register, DIP-8/SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "shift register 8bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TPIC6595_0_1")
		(symbol "TPIC6595_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SER_IN")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SRCK")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{SRCLR}")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RCLK")
				(number "12")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{G}")
				(number "9")
			)
			(pin power_in line
				(at -7.62 -17.78 90)
				(length 2.54)
				(name "LGND")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "PGND")
				(number "1")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "10")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "11")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "PGND")
				(number "20")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "DRAIN0")
				(number "4")
			)
			(pin open_collector line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DRAIN1")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DRAIN2")
				(number "6")
			)
			(pin open_collector line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DRAIN3")
				(number "7")
			)
			(pin open_collector line
				(at 12.7 0 180)
				(length 2.54)
				(name "DRAIN4")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DRAIN5")
				(number "15")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DRAIN6")
				(number "16")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "DRAIN7")
				(number "17")
			)
			(pin output line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SER_OUT")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XRA1201IG24"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "XRA1201IG24"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 26.67 -25.4 0)
		)
		(property "Datasheet" "https://maxlinear-assets.azureedge.net/web/documents/xra1201.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/ optional pull-ups, TSSOP-24 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "IO expander i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "XRA1201IG24_0_1")
		(symbol "XRA1201IG24_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "SDA")
				(number "23")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCL")
				(number "22")
			)
			(pin open_collector line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "~{INT}")
				(number "1")
				(alternate "~{IRQ}" open_collector line)
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "A0")
				(number "21")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "P0")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "P1")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "P2")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "P3")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "P4")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "P5")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "P6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "P7")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "P8")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "P9")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "P10")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "P11")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "P12")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "P13")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "P14")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "P15")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XRA1201IL24"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "XRA1201IL24"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at 26.67 -25.4 0)
		)
		(property "Datasheet" "https://maxlinear-assets.azureedge.net/web/documents/xra1201.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/ optional pull-ups, QFN-24 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "IO expander i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "XRA1201IL24_0_1")
		(symbol "XRA1201IL24_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 5.08)
				(name "SDA")
				(number "23")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 5.08)
				(name "SCL")
				(number "22")
			)
			(pin open_collector line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "~{INT}")
				(number "1")
				(alternate "~{IRQ}" open_collector line)
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 5.08)
				(name "A0")
				(number "21")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "EPAD")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "P0")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "P1")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "P2")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "P3")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "P4")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "P5")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "P6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "P7")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "P8")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "P9")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "P10")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "P11")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "P12")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "P13")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "P14")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "P15")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX31911xUI"
		(extends "MAX31910xUI")
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "MAX31911xUI"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.85x6.7mm"
			(at 0 39.37 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max31911.pdf"
			(at -13.97 24.13 0)
		)
		(property "Description" "Industrial, Octal, Digital Input Translator/Serializer, SPI interface, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI digital input serializer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*1EP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX31912xUI"
		(extends "MAX31910xUI")
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "MAX31912xUI"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.85x6.7mm"
			(at 0 39.37 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max31912.pdf"
			(at -13.97 24.13 0)
		)
		(property "Description" "Ultra-Low Power Industrial, Octal, Digital Input Translator/Serializer, 8 integrated energy-less LED drivers, SPI interface, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI digital input serializer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*1EP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX31913xUI"
		(extends "MAX31910xUI")
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "MAX31913xUI"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28-1EP_4.4x9.7mm_P0.65mm_EP2.85x6.7mm"
			(at 0 39.37 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/max31913.pdf"
			(at -13.97 24.13 0)
		)
		(property "Description" "Industrial, Octal, Digital Input Translator/Serializer, 8 integrated energy-less LED drivers, SPI interface, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "SPI digital input serializer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*1EP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP23017_SP"
		(extends "MCP23017_SO")
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "MCP23017_SP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 5.08 -25.4 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MCP23017-Data-Sheet-DS20001952.pdf"
			(at 5.08 -27.94 0)
		)
		(property "Description" "16-bit I/O expander, I2C, interrupts, w pull-ups, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C parallel port expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP23017_SS"
		(extends "MCP23017_SO")
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "MCP23017_SS"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 5.08 -25.4 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/APID/ProductDocuments/DataSheets/MCP23017-Data-Sheet-DS20001952.pdf"
			(at 5.08 -27.94 0)
		)
		(property "Description" "16-bit I/O expander, I2C, interrupts, w pull-ups, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C parallel port expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCA9547D"
		(extends "PCA9548ADB")
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "PCA9547D"
			(at 1.016 21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9547.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Low voltage 8-channel I2C switch with reset, SO-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low voltage 8-channel I2C switch with reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x15.4mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCA9547PW"
		(extends "PCA9548ADB")
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "PCA9547PW"
			(at 1.016 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/PCA9547.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Low voltage 8-channel I2C switch with reset, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low voltage 8-channel I2C switch with reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCA9548APW"
		(extends "TCA9548APWR")
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "PCA9548APW"
			(at 1.016 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pca9548a.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Low voltage 8-channel I2C switch with reset, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low voltage 8-channel I2C switch with reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCA9548ARGE"
		(extends "TCA9548AMRGER")
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "PCA9548ARGE"
			(at 1.016 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024C_VQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pca9548a.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Low voltage 8-channel I2C switch with reset, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low voltage 8-channel I2C switch with reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024C*"
			(at 0 0 0)
		)
	)
	(symbol "PCF8574AP"
		(extends "TCA9534")
		(property "Reference" "U"
			(at -6.35 12.954 0)
		)
		(property "Value" "PCF8574AP"
			(at 3.048 12.954 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCF8574_PCF8574A.pdf"
			(at 0 0 0)
		)
		(property "Description" "8 Bit Port/Expander to I2C Bus, fixed address bits 0b0111, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCF8574AT"
		(extends "TCA9534")
		(property "Reference" "U"
			(at -6.35 12.954 0)
		)
		(property "Value" "PCF8574AT"
			(at 3.048 12.954 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCF8574_PCF8574A.pdf"
			(at 0 0 0)
		)
		(property "Description" "8 Bit Port/Expander to I2C Bus, fixed address bits 0b0111, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCF8574ATS"
		(extends "PCF8574TS")
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "PCF8574ATS"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCF8574_PCF8574A.pdf"
			(at 0 0 0)
		)
		(property "Description" "8 Bit Port/Expander to I2C Bus, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCF8574P"
		(extends "TCA9534")
		(property "Reference" "U"
			(at -6.35 12.954 0)
		)
		(property "Value" "PCF8574P"
			(at 3.048 12.954 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCF8574_PCF8574A.pdf"
			(at 0 0 0)
		)
		(property "Description" "8 Bit Port/Expander to I2C Bus, fixed address bits 0b0100, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PCF8574T"
		(extends "TCA9534")
		(property "Reference" "U"
			(at -6.35 12.954 0)
		)
		(property "Value" "PCF8574T"
			(at 3.048 12.954 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/PCF8574_PCF8574A.pdf"
			(at 0 0 0)
		)
		(property "Description" "8 Bit Port/Expander to I2C Bus, fixed address bits 0b0100, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C Expander"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCA9535DBT"
		(extends "TCA9535DBR")
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TCA9535DBT"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9535.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/o pull-ups, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ti parallel port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCA9535MRGER"
		(extends "TCA9535RGER")
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TCA9535MRGER"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at 30.48 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9535.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/o pull-ups, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ti parallel port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCA9548ARGER"
		(extends "TCA9548AMRGER")
		(property "Reference" "U"
			(at -7.62 21.59 0)
		)
		(property "Value" "TCA9548ARGER"
			(at 1.016 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGE0024C_VQFN-24-1EP_4x4mm_P0.5mm_EP2.1x2.1mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9548a.pdf"
			(at 1.27 6.35 0)
		)
		(property "Description" "Low voltage 8-channel I2C switch with reset, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low voltage 8-channel I2C switch with reset"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*RGE0024C*"
			(at 0 0 0)
		)
	)
	(symbol "TCA9555DBR"
		(extends "TCA9535DBR")
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TCA9555DBR"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9555.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/ pull-ups, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ti parallel port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCA9555DBT"
		(extends "TCA9535DBR")
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TCA9555DBT"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9555.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/ pull-ups, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ti parallel port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCA9555PWR"
		(extends "TCA9535PWR")
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TCA9555PWR"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 26.67 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9555.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/ pull-ups, TSSOP-24 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "ti parallel port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCA9555RGER"
		(extends "TCA9535RGER")
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TCA9555RGER"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at 30.48 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9555.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/ pull-ups, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ti parallel port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCA9555RTWR"
		(extends "TCA9535RTWR")
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TCA9555RTWR"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at 30.48 -25.4 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tca9555.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/ pull-ups, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "ti parallel port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "XRA1201PIG24"
		(extends "XRA1201IG24")
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "XRA1201PIG24"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 26.67 -25.4 0)
		)
		(property "Datasheet" "https://maxlinear-assets.azureedge.net/web/documents/xra1201.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/ pull-ups, TSSOP-24 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "IO expander i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "XRA1201PIL24"
		(extends "XRA1201IL24")
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "XRA1201PIL24"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm"
			(at 30.48 -25.4 0)
		)
		(property "Datasheet" "https://maxlinear-assets.azureedge.net/web/documents/xra1201.pdf"
			(at -12.7 22.86 0)
		)
		(property "Description" "16-bit I/O expander, I2C and SMBus interface, interrupts, w/ pull-ups, QFN-24 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "IO expander i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
