(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ADV7611"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 49.53 0)
		)
		(property "Value" "ADV7611"
			(at 30.48 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64-1EP_10x10mm_P0.5mm_EP5x5mm"
			(at 1.27 0 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adv7611.pdf"
			(at 31.75 -10.16 0)
		)
		(property "Description" "Low Power 165MHz HDMI Receiver, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "hdmi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*1EP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ADV7611_0_1")
		(symbol "ADV7611_1_1"
			(pin input line
				(at -33.02 43.18 0)
				(length 2.54)
				(name "RXA_2+")
				(number "13")
			)
			(pin input line
				(at -33.02 40.64 0)
				(length 2.54)
				(name "RXA_2-")
				(number "12")
			)
			(pin input line
				(at -33.02 38.1 0)
				(length 2.54)
				(name "RXA_1+")
				(number "10")
			)
			(pin input line
				(at -33.02 35.56 0)
				(length 2.54)
				(name "RXA_1-")
				(number "9")
			)
			(pin input line
				(at -33.02 33.02 0)
				(length 2.54)
				(name "RXA_0+")
				(number "7")
			)
			(pin input line
				(at -33.02 30.48 0)
				(length 2.54)
				(name "RXA_0-")
				(number "6")
			)
			(pin input line
				(at -33.02 27.94 0)
				(length 2.54)
				(name "RXA_C+")
				(number "4")
			)
			(pin input line
				(at -33.02 25.4 0)
				(length 2.54)
				(name "RXA_C-")
				(number "3")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 2.54)
				(name "CEC")
				(number "61")
			)
			(pin input line
				(at -33.02 20.32 0)
				(length 2.54)
				(name "DDCA_SCL")
				(number "62")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 2.54)
				(name "DDCA_SDA")
				(number "63")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 2.54)
				(name "HPA_A/INT2")
				(number "1")
			)
			(pin input line
				(at -33.02 12.7 0)
				(length 2.54)
				(name "RXA_5V")
				(number "64")
			)
			(pin input line
				(at -33.02 7.62 0)
				(length 2.54)
				(name "SCL")
				(number "53")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 2.54)
				(name "SDA")
				(number "54")
			)
			(pin input line
				(at -33.02 0 0)
				(length 2.54)
				(name "~{RESET}")
				(number "56")
			)
			(pin input line
				(at -33.02 -5.08 0)
				(length 2.54)
				(name "XTALP")
				(number "58")
			)
			(pin input line
				(at -33.02 -7.62 0)
				(length 2.54)
				(name "XTALN")
				(number "59")
			)
			(pin power_in line
				(at -20.32 50.8 270)
				(length 2.54)
				(name "CVDD")
				(number "2")
			)
			(pin power_in line
				(at -17.78 50.8 270)
				(length 2.54)
				(name "CVDD")
				(number "14")
			)
			(pin power_in line
				(at -12.7 50.8 270)
				(length 2.54)
				(name "DVDD")
				(number "24")
			)
			(pin power_in line
				(at -10.16 50.8 270)
				(length 2.54)
				(name "DVDD")
				(number "40")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 2.54)
				(name "DVDD")
				(number "52")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 2.54)
				(name "DVDD")
				(number "60")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "PVDD")
				(number "57")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 2.54)
				(name "TVDD")
				(number "5")
			)
			(pin power_in line
				(at 7.62 50.8 270)
				(length 2.54)
				(name "TVDD")
				(number "8")
			)
			(pin power_in line
				(at 10.16 50.8 270)
				(length 2.54)
				(name "TVDD")
				(number "11")
			)
			(pin power_in line
				(at 15.24 50.8 270)
				(length 2.54)
				(name "DVDDIO")
				(number "23")
			)
			(pin power_in line
				(at 17.78 50.8 270)
				(length 2.54)
				(name "DVDDIO")
				(number "34")
			)
			(pin power_in line
				(at 20.32 50.8 270)
				(length 2.54)
				(name "DVDDIO")
				(number "44")
			)
			(pin output line
				(at 33.02 43.18 180)
				(length 2.54)
				(name "P23")
				(number "15")
			)
			(pin output line
				(at 33.02 40.64 180)
				(length 2.54)
				(name "P22")
				(number "16")
			)
			(pin output line
				(at 33.02 38.1 180)
				(length 2.54)
				(name "P21")
				(number "17")
			)
			(pin output line
				(at 33.02 35.56 180)
				(length 2.54)
				(name "P20")
				(number "18")
			)
			(pin output line
				(at 33.02 33.02 180)
				(length 2.54)
				(name "P19")
				(number "19")
			)
			(pin output line
				(at 33.02 30.48 180)
				(length 2.54)
				(name "P18")
				(number "20")
			)
			(pin output line
				(at 33.02 27.94 180)
				(length 2.54)
				(name "P17")
				(number "21")
			)
			(pin output line
				(at 33.02 25.4 180)
				(length 2.54)
				(name "P16")
				(number "22")
			)
			(pin output line
				(at 33.02 22.86 180)
				(length 2.54)
				(name "P15")
				(number "26")
			)
			(pin output line
				(at 33.02 20.32 180)
				(length 2.54)
				(name "P14")
				(number "27")
			)
			(pin output line
				(at 33.02 17.78 180)
				(length 2.54)
				(name "P13")
				(number "28")
			)
			(pin output line
				(at 33.02 15.24 180)
				(length 2.54)
				(name "P12")
				(number "29")
			)
			(pin output line
				(at 33.02 12.7 180)
				(length 2.54)
				(name "P11")
				(number "30")
			)
			(pin output line
				(at 33.02 10.16 180)
				(length 2.54)
				(name "P10")
				(number "31")
			)
			(pin output line
				(at 33.02 7.62 180)
				(length 2.54)
				(name "P9")
				(number "32")
			)
			(pin output line
				(at 33.02 5.08 180)
				(length 2.54)
				(name "P8")
				(number "33")
			)
			(pin output line
				(at 33.02 2.54 180)
				(length 2.54)
				(name "P7")
				(number "35")
			)
			(pin output line
				(at 33.02 0 180)
				(length 2.54)
				(name "P6")
				(number "36")
			)
			(pin output line
				(at 33.02 -2.54 180)
				(length 2.54)
				(name "P5")
				(number "37")
			)
			(pin output line
				(at 33.02 -5.08 180)
				(length 2.54)
				(name "P4")
				(number "38")
			)
			(pin output line
				(at 33.02 -7.62 180)
				(length 2.54)
				(name "P3")
				(number "39")
			)
			(pin output line
				(at 33.02 -10.16 180)
				(length 2.54)
				(name "P2")
				(number "41")
			)
			(pin output line
				(at 33.02 -12.7 180)
				(length 2.54)
				(name "P1")
				(number "42")
			)
			(pin output line
				(at 33.02 -15.24 180)
				(length 2.54)
				(name "P0")
				(number "43")
			)
			(pin output line
				(at 33.02 -20.32 180)
				(length 2.54)
				(name "DE")
				(number "45")
			)
			(pin output line
				(at 33.02 -22.86 180)
				(length 2.54)
				(name "HS")
				(number "46")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 2.54)
				(name "VS/FIELD/ALSB")
				(number "47")
			)
			(pin output line
				(at 33.02 -27.94 180)
				(length 2.54)
				(name "LLC")
				(number "25")
			)
			(pin output line
				(at 33.02 -33.02 180)
				(length 2.54)
				(name "AP")
				(number "48")
			)
			(pin output line
				(at 33.02 -35.56 180)
				(length 2.54)
				(name "SCLK/INT2")
				(number "49")
			)
			(pin output line
				(at 33.02 -38.1 180)
				(length 2.54)
				(name "LRCLK")
				(number "50")
			)
			(pin output line
				(at 33.02 -40.64 180)
				(length 2.54)
				(name "MCLK/INT2")
				(number "51")
			)
			(pin output line
				(at 33.02 -43.18 180)
				(length 2.54)
				(name "INT1")
				(number "55")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPD12S520DBT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 26.67 0)
		)
		(property "Value" "TPD12S520DBT"
			(at 17.78 26.67 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_4.4x9.7mm_P0.5mm"
			(at -3.81 -6.35 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tpd12s520.pdf"
			(at -3.81 -6.35 0)
		)
		(property "Description" "HDMI Receiver Port Protection and Interface Device, TSSOP-38"
			(at 0 0 0)
		)
		(property "ki_keywords" "hdmi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPD12S520DBT_0_1")
		(symbol "TPD12S520DBT_1_1"
			(pin passive line
				(at -20.32 22.86 0)
				(length 2.54)
				(hide yes)
				(name "TMDS_D2+")
				(number "35")
			)
			(pin passive line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "TMDS_D2+")
				(number "4")
			)
			(pin passive line
				(at -20.32 20.32 0)
				(length 2.54)
				(hide yes)
				(name "TMDS_D2-")
				(number "33")
			)
			(pin passive line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "TMDS_D2-")
				(number "6")
			)
			(pin passive line
				(at -20.32 17.78 0)
				(length 2.54)
				(hide yes)
				(name "TMDS_D1+")
				(number "32")
			)
			(pin passive line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "TMDS_D1+")
				(number "7")
			)
			(pin passive line
				(at -20.32 15.24 0)
				(length 2.54)
				(hide yes)
				(name "TMDS_D1-")
				(number "30")
			)
			(pin passive line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "TMDS_D1-")
				(number "9")
			)
			(pin passive line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "TMDS_D0+")
				(number "10")
			)
			(pin passive line
				(at -20.32 12.7 0)
				(length 2.54)
				(hide yes)
				(name "TMDS_D0+")
				(number "29")
			)
			(pin passive line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "TMDS_D0-")
				(number "12")
			)
			(pin passive line
				(at -20.32 10.16 0)
				(length 2.54)
				(hide yes)
				(name "TMDS_D0-")
				(number "27")
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "TMDS_CK+")
				(number "13")
			)
			(pin passive line
				(at -20.32 7.62 0)
				(length 2.54)
				(hide yes)
				(name "TMDS_CK+")
				(number "26")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "TMDS_CK-")
				(number "15")
			)
			(pin passive line
				(at -20.32 5.08 0)
				(length 2.54)
				(hide yes)
				(name "TMDS_CK-")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "CE_REMOTE_IN")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "DDC_CLK_IN")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "DDC_DAT_IN")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "HOTPLUG_DET_IN")
				(number "19")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "5V_SUPPLY")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "LV_SUPPLY")
				(number "2")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "TMDS_GND")
				(number "11")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "TMDS_GND")
				(number "14")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "TMDS_GND")
				(number "25")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "TMDS_GND")
				(number "28")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "TMDS_GND")
				(number "31")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "TMDS_GND")
				(number "34")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "TMDS_GND")
				(number "5")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "TMDS_GND")
				(number "8")
			)
			(pin no_connect line
				(at 17.78 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "38")
			)
			(pin passive line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "ESD_BYP")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "CE_REMOTE_OUT")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "DDC_CLK_OUT")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "DDC_DAT_OUT")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "HOTPLUG_DET_OUT")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
)
