(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "JoyWarrior24A10L"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 -24.13 0)
		)
		(property "Value" "JoyWarrior24A10L"
			(at 17.78 26.67 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "http://codemercs.com/downloads/joywarrior/JW_Datasheet.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "JoyWarrior 10bit, 3 axis, joystick controller, DIP-24/SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "joystick controller 10bit 3-axis"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x15.4mm*P1.27mm* DIP*7.62mm*"
			(at 0 0 0)
		)
		(symbol "JoyWarrior24A10L_0_1")
		(symbol "JoyWarrior24A10L_1_1"
			(pin input line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "Direct")
				(number "12")
			)
			(pin power_out line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "VREG")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "D+")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "D-")
				(number "15")
			)
			(pin no_connect line
				(at -17.78 22.86 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at -7.62 30.48 270)
				(length 5.08)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -7.62 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "PullToGnd")
				(number "10")
			)
			(pin input line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "X0/B0")
				(number "1")
			)
			(pin input line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "X1/B1")
				(number "2")
			)
			(pin input line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "X2/B2")
				(number "3")
			)
			(pin input line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "X3/B3")
				(number "4")
			)
			(pin input line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "Y0/B4")
				(number "24")
			)
			(pin input line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "Y1/B5")
				(number "23")
			)
			(pin input line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "Y2/B6")
				(number "22")
			)
			(pin input line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "Y3/B7")
				(number "21")
			)
			(pin output line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "~{CS}")
				(number "5")
			)
			(pin output line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "SCLK")
				(number "20")
			)
			(pin input line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "Din")
				(number "6")
			)
			(pin output line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "Dout")
				(number "19")
			)
			(pin output line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "Aux0")
				(number "7")
			)
			(pin output line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "Aux1")
				(number "18")
			)
			(pin output line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "Aux2")
				(number "8")
			)
			(pin output line
				(at 22.86 -20.32 180)
				(length 5.08)
				(name "Aux3")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SpinWarrior24A3"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 -24.13 0)
		)
		(property "Value" "SpinWarrior24A3"
			(at 12.7 26.67 0)
		)
		(property "Footprint" ""
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.codemercs.com/downloads/spinwarrior/SW_Datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "SpinWarrior, 3 16bit absolute position rotary encoders, 6 digital inputs, DIP-24/SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "16bit absolute position USB rotary encoder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm* SOIC*7.5x15.4mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SpinWarrior24A3_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "Power")
				(number "12")
			)
			(pin power_out line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "Vreg")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "D+")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "D-")
				(number "15")
			)
			(pin no_connect line
				(at -12.7 22.86 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 5.08)
				(name "Vcc")
				(number "14")
			)
			(pin input line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "PullToGND")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "B0")
				(number "2")
			)
			(pin input line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "N0")
				(number "22")
			)
			(pin input line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "B1")
				(number "4")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "N1")
				(number "21")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "A2")
				(number "24")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "B2")
				(number "23")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "N2")
				(number "8")
			)
			(pin open_collector line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "~{EN}")
				(number "17")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "In0")
				(number "5")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "In1")
				(number "20")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "In2")
				(number "6")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "In3")
				(number "19")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "In4")
				(number "7")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "In5")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SpinWarrior24R4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 -24.13 0)
		)
		(property "Value" "SpinWarrior24R4"
			(at 12.7 26.67 0)
		)
		(property "Footprint" ""
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.codemercs.com/downloads/spinwarrior/SW_Datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "SpinWarrior, 4 8bit relative position rotary encoders, 7 switches, DIP-24/SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit relative position USB rotary encoder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm* SOIC*7.5x15.4mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SpinWarrior24R4_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "Power")
				(number "12")
			)
			(pin power_out line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "Vreg")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "D+")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "D-")
				(number "15")
			)
			(pin no_connect line
				(at -12.7 22.86 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 5.08)
				(name "Vcc")
				(number "14")
			)
			(pin input line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "PullToGND")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "B0")
				(number "2")
			)
			(pin input line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "B1")
				(number "4")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "A2")
				(number "24")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "B2")
				(number "23")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "A3")
				(number "22")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "B3")
				(number "21")
			)
			(pin open_collector line
				(at 17.78 0 180)
				(length 5.08)
				(name "~{EN}")
				(number "17")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "Sw0")
				(number "5")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 5.08)
				(name "Sw1")
				(number "20")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "Sw2")
				(number "6")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 5.08)
				(name "Sw3")
				(number "19")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "Sw4")
				(number "7")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "Sw5")
				(number "18")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "Sw6")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SpinWarrior24R6"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 -24.13 0)
		)
		(property "Value" "SpinWarrior24R6"
			(at 12.7 26.67 0)
		)
		(property "Footprint" ""
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://www.codemercs.com/downloads/spinwarrior/SW_Datasheet.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "SpinWarrior, 6 8bit relative position rotary encoders, 3 switches, DIP-24/SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "8bit relative position USB rotary encoder"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm* SOIC*7.5x15.4mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SpinWarrior24R6_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 5.08)
				(name "Power")
				(number "12")
			)
			(pin power_out line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "Vreg")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 5.08)
				(name "D+")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 5.08)
				(name "D-")
				(number "15")
			)
			(pin no_connect line
				(at -12.7 22.86 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 5.08)
				(name "Vcc")
				(number "14")
			)
			(pin input line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "PullToGND")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 17.78 22.86 180)
				(length 5.08)
				(name "A0")
				(number "1")
			)
			(pin input line
				(at 17.78 20.32 180)
				(length 5.08)
				(name "B0")
				(number "2")
			)
			(pin input line
				(at 17.78 17.78 180)
				(length 5.08)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at 17.78 15.24 180)
				(length 5.08)
				(name "B1")
				(number "4")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 5.08)
				(name "A2")
				(number "24")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 5.08)
				(name "B2")
				(number "23")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "A3")
				(number "22")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "B3")
				(number "21")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "A4")
				(number "19")
			)
			(pin input line
				(at 17.78 0 180)
				(length 5.08)
				(name "B4")
				(number "7")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "A5")
				(number "18")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "B5")
				(number "8")
			)
			(pin open_collector line
				(at 17.78 -10.16 180)
				(length 5.08)
				(name "~{EN}")
				(number "17")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 5.08)
				(name "Sw0")
				(number "5")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 5.08)
				(name "Sw1")
				(number "20")
			)
			(pin input line
				(at 17.78 -20.32 180)
				(length 5.08)
				(name "Sw2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "JoyWarrior24A8L"
		(extends "JoyWarrior24A10L")
		(property "Reference" "U"
			(at 17.78 -24.13 0)
		)
		(property "Value" "JoyWarrior24A8L"
			(at 17.78 26.67 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "http://codemercs.com/downloads/joywarrior/JW_Datasheet.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "JoyWarrior 8bit, 4 axis, joystick controller, DIP-24/SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "joystick controller, 8 bit, 4 axis"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x15.4mm*P1.27mm* DIP*7.62mm*"
			(at 0 0 0)
		)
	)
)
