(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "DS7820"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 8.89 0)
		)
		(property "Value" "DS7820"
			(at 14.224 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://pdf1.alldatasheet.com/datasheet-pdf/view/942427/NSC/DS7820.html"
			(at -57.15 7.112 0)
		)
		(property "Description" "Dual line receiver, VDD +5V, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual line receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DS7820_0_1")
		(symbol "DS7820_1_1"
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "INPUT")
				(number "1")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "TERMINATION")
				(number "2")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "INPUT")
				(number "3")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "STROBE")
				(number "4")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RESPONSE_TIME")
				(number "5")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "OUTPUT")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "INPUT")
				(number "13")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "TERMINATION")
				(number "12")
			)
			(pin input line
				(at 20.32 0 180)
				(length 2.54)
				(name "INPUT")
				(number "11")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "STROBE")
				(number "10")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RESPONSE_TIME")
				(number "9")
			)
			(pin output line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "OUTPUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS7830"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -18.542 9.398 0)
		)
		(property "Value" "DS7830"
			(at 16.51 9.398 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://pdf1.alldatasheet.com/datasheet-pdf/view/8473/NSC/DS7830J.html"
			(at -40.64 5.08 0)
		)
		(property "Description" "Dual differential line driver and dual four-input NAND or dual four-input AND function, VDD +5V, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual differential line driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "DS7830_0_1")
		(symbol "DS7830_1_1"
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "A_1")
				(number "1")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "A_2")
				(number "2")
			)
			(pin input line
				(at -22.86 0 0)
				(length 2.54)
				(name "A_3")
				(number "3")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "A_4")
				(number "4")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "A_AND_OUTPUT")
				(number "5")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "A_NAND_OUTPUT")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "B_1")
				(number "13")
			)
			(pin input line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "B_2")
				(number "12")
			)
			(pin input line
				(at 22.86 0 180)
				(length 2.54)
				(name "B_3")
				(number "11")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "B_4")
				(number "10")
			)
			(pin input line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "B_AND_OUTPUT")
				(number "9")
			)
			(pin input line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "B_NAND_OUTPUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS89C21"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "DS89C21"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ds89c21.pdf"
			(at 0 0 0)
		)
		(property "Description" "Differential CMOS Line Driver and Receiver Pair, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs422 tranciever"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "DS89C21_0_0"
			(text "D"
				(at -1.27 -5.08 0)
			)
			(text "R"
				(at 1.27 5.08 0)
			)
		)
		(symbol "DS89C21_0_1")
		(symbol "DS89C21_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "RI")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{RI}")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DO")
				(number "6")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{DO}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EL7242C"
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.922 8.89 0)
		)
		(property "Value" "EL7242C"
			(at 11.176 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/elantec/EL7242CN.pdf"
			(at 0 0 0)
		)
		(property "Description" "Translateur TTL->VMOS. Double driver VMOS"
			(at 0 0 0)
		)
		(property "ki_keywords" "Translateur TTL->VMOS. Double driver VMOS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "EL7242C_0_0"
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
		)
		(symbol "EL7242C_0_1")
		(symbol "EL7242C_1_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "1")
			)
			(pin input inverted
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "OUT")
				(number "7")
			)
		)
		(symbol "EL7242C_2_1"
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "IN1")
				(number "3")
			)
			(pin input inverted
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "IN")
				(number "4")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "OUT")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC3486N"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 7.62 0)
		)
		(property "Value" "MC3486N"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/mc3486.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quadruple differential line receiver, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quadruple differential line receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MC3486N_0_1")
		(symbol "MC3486N_1_1"
			(pin input inverted
				(at -12.7 2.54 0)
				(length 6.35)
				(name "E-")
				(number "1")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 6.35)
				(name "E+")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ENABLE")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 6.35)
				(name "OUT")
				(number "3")
			)
		)
		(symbol "MC3486N_2_1"
			(pin input inverted
				(at -12.7 2.54 0)
				(length 6.35)
				(name "E-")
				(number "7")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 6.35)
				(name "E+")
				(number "6")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ENABLE")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 6.35)
				(name "OUT")
				(number "5")
			)
		)
		(symbol "MC3486N_3_1"
			(pin input inverted
				(at -12.7 2.54 0)
				(length 6.35)
				(name "E-")
				(number "9")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 6.35)
				(name "E+")
				(number "10")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ENABLE")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 6.35)
				(name "OUT")
				(number "11")
			)
		)
		(symbol "MC3486N_4_1"
			(pin input inverted
				(at -12.7 2.54 0)
				(length 6.35)
				(name "E-")
				(number "15")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 6.35)
				(name "E+")
				(number "14")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ENABLE")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 6.35)
				(name "OUT")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC3487DX"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "MC3487DX"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/mc3487.pdf"
			(at 0 0 0)
		)
		(property "Description" "Four independent differential line drivers, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Four independent differential line drivers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC3487DX_0_1")
		(symbol "MC3487DX_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 6.35)
				(name "INPUT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ENABLE")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "OUT-")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "OUT+")
				(number "2")
			)
		)
		(symbol "MC3487DX_2_1"
			(pin input line
				(at -12.7 0 0)
				(length 6.35)
				(name "INPUT")
				(number "7")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ENABLE")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "OUT-")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "OUT+")
				(number "6")
			)
		)
		(symbol "MC3487DX_3_1"
			(pin input line
				(at -12.7 0 0)
				(length 6.35)
				(name "INPUT")
				(number "9")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ENABLE")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "OUT-")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "OUT+")
				(number "10")
			)
		)
		(symbol "MC3487DX_4_1"
			(pin input line
				(at -12.7 0 0)
				(length 6.35)
				(name "INPUT")
				(number "15")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ENABLE")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "OUT-")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "OUT+")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC3487N"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 7.62 0)
		)
		(property "Value" "MC3487N"
			(at 5.08 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/mc3487.pdf"
			(at 0 0 0)
		)
		(property "Description" "Four independent differential line drivers, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Four independent differential line drivers"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MC3487N_0_1")
		(symbol "MC3487N_1_1"
			(pin input line
				(at -12.7 0 0)
				(length 6.35)
				(name "INPUT")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ENABLE")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "OUT-")
				(number "3")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "OUT+")
				(number "2")
			)
		)
		(symbol "MC3487N_2_1"
			(pin input line
				(at -12.7 0 0)
				(length 6.35)
				(name "INPUT")
				(number "7")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ENABLE")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "OUT-")
				(number "5")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "OUT+")
				(number "6")
			)
		)
		(symbol "MC3487N_3_1"
			(pin input line
				(at -12.7 0 0)
				(length 6.35)
				(name "INPUT")
				(number "9")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ENABLE")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "OUT-")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "OUT+")
				(number "10")
			)
		)
		(symbol "MC3487N_4_1"
			(pin input line
				(at -12.7 0 0)
				(length 6.35)
				(name "INPUT")
				(number "15")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 3.81)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -7.62 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 0 -7.62 90)
				(length 2.54)
				(name "ENABLE")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 7.62)
				(name "OUT-")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 7.62)
				(name "OUT+")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UA9637"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "UA9637"
			(at 5.08 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheets2/28/284473_1.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual differential line receiver, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual differential line receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "UA9637_0_1"
			(text "+"
				(at -4.064 1.8034 0)
			)
			(text "-"
				(at -4.064 -3.2766 0)
			)
		)
		(symbol "UA9637_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "IN+")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "IN-")
				(number "7")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "OUT")
				(number "2")
			)
		)
		(symbol "UA9637_2_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 7.62)
				(name "IN+")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 7.62)
				(name "IN-")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 12.7 0 180)
				(length 7.62)
				(name "OUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UA9638CD"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "UA9638CD"
			(at 5.08 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ua9638.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual high-speed differential line driver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual high-speed differential line driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "UA9638CD_0_1")
		(symbol "UA9638CD_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 7.62)
				(name "OUTB")
				(number "8")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 7.62)
				(name "OUTA")
				(number "7")
			)
		)
		(symbol "UA9638CD_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 7.62)
				(name "OUTB")
				(number "6")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 7.62)
				(name "OUTA")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UA9638CP"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "UA9638CP"
			(at 2.54 7.62 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ua9638.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual high-speed differential line driver, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual high-speed differential line driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "UA9638CP_0_1")
		(symbol "UA9638CP_1_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 7.62)
				(name "OUTB")
				(number "8")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 7.62)
				(name "OUTA")
				(number "7")
			)
		)
		(symbol "UA9638CP_2_1"
			(pin input line
				(at -15.24 0 0)
				(length 7.62)
				(name "IN")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 7.62)
				(name "OUTB")
				(number "6")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 7.62)
				(name "OUTA")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DS8830"
		(extends "DS7830")
		(property "Reference" "U"
			(at -18.542 9.398 0)
		)
		(property "Value" "DS8830"
			(at 16.51 9.398 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://pdf1.alldatasheet.com/datasheet-pdf/view/8473/NSC/DS7830J.html"
			(at -40.64 5.08 0)
		)
		(property "Description" "Dual differential line driver and dual four-input NAND or dual four-input AND function, VDD +5V, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual differential line driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "UA9638CDE4"
		(extends "UA9638CD")
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "UA9638CDE4"
			(at 5.08 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ua9638.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual high-speed differential line driver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual high-speed differential line driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "UA9638CDG4"
		(extends "UA9638CD")
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "UA9638CDG4"
			(at 5.08 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ua9638.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual high-speed differential line driver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual high-speed differential line driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "UA9638CDR"
		(extends "UA9638CD")
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "UA9638CDR"
			(at 5.08 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ua9638.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual high-speed differential line driver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual high-speed differential line driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "UA9638CDRG4"
		(extends "UA9638CD")
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "UA9638CDRG4"
			(at 5.08 7.62 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ua9638.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual high-speed differential line driver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual high-speed differential line driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "UA9638CPE4"
		(extends "UA9638CP")
		(property "Reference" "U"
			(at -7.62 10.16 0)
		)
		(property "Value" "UA9638CPE4"
			(at 2.54 7.62 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/ua9638.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual high-speed differential line driver, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual high-speed differential line driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
)
