(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "IRM-H6xxT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "IRM-H6xxT"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Everlight_IRM-H6xxT"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "https://en.everlight.com/wp-content/plugins/ItemRelationship/product_files/pdf/DMO-0000004-IRM-H6XX-TR2_Series_Datasheet_V4.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for remote controls"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Everlight*IRM?H6xxT*"
			(at 0 0 0)
		)
		(symbol "IRM-H6xxT_0_0"
			(text "DEMOD"
				(at -3.175 0.254 900)
			)
		)
		(symbol "IRM-H6xxT_0_1")
		(symbol "IRM-H6xxT_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vcc")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS471F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.065 7.62 0)
		)
		(property "Value" "IS471F"
			(at 7.62 7.62 0)
		)
		(property "Footprint" "OptoDevice:Sharp_IS471F"
			(at -2.54 -10.16 0)
		)
		(property "Datasheet" "http://www.micropik.com/PDF/tsop17xx.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Modules for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sharp*IS471F*"
			(at 0 0 0)
		)
		(symbol "IS471F_0_0"
			(text "DEMOD"
				(at -4.953 1.397 900)
			)
			(text "OSC"
				(at -4.953 -5.588 0)
			)
		)
		(symbol "IS471F_0_1")
		(symbol "IS471F_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vs")
				(number "1")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GLo")
				(number "4")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GND")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS485"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "IS485"
			(at 7.62 7.62 0)
		)
		(property "Footprint" "OptoDevice:Sharp_IS485"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Sharp%20PDFs/is485,486_e.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Built-in Amplifier Type OPIC Light Detector"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto receiver amplifier light detector OPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sharp*IS485*"
			(at 0 0 0)
		)
		(symbol "IS485_0_0")
		(symbol "IS485_0_1")
		(symbol "IS485_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vs")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IS486"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "IS486"
			(at 7.62 7.62 0)
		)
		(property "Footprint" "OptoDevice:Sharp_IS485"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://media.digikey.com/pdf/Data%20Sheets/Sharp%20PDFs/is485,486_e.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Built-in Amplifier Type OPIC Light Detector"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto receiver amplifier light detector OPIC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sharp*IS485*"
			(at 0 0 0)
		)
		(symbol "IS486_0_0")
		(symbol "IS486_0_1")
		(symbol "IS486_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vs")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "2")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "QSE159"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "QSE159"
			(at -7.62 -6.35 0)
		)
		(property "Footprint" "OptoDevice:ONSemi_QSE15x"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/QSE159-D.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Plastic Silicon Photosensor"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QSE15*"
			(at 0 0 0)
		)
		(symbol "QSE159_0_0"
			(text "TRIG"
				(at -1.651 3.048 0)
			)
		)
		(symbol "QSE159_0_1")
		(symbol "QSE159_1_1"
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "Vcc")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "Out")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -8.89 16.51 0)
		)
		(property "Value" "SFP"
			(at 11.43 16.51 0)
		)
		(property "Footprint" ""
			(at 0 -21.59 0)
		)
		(property "Datasheet" "http://www.10gtek.com/templates/wzten/pdf/INF-8074.pdf"
			(at -11.43 16.51 0)
		)
		(property "Description" "Connector for Small Form Factor Pluggable (SFP) module, 1 Gbit/s, serial-to-serial data-agnostic optical transceiver"
			(at 0 0 0)
		)
		(property "ki_keywords" "SFP transceiver gigabit ethernet INF-8074i"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SFP*"
			(at 0 0 0)
		)
		(symbol "SFP_0_0")
		(symbol "SFP_1_1"
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MOD_DEF2")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MOD_DEF1")
				(number "5")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "MOD_DEF0")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RATE_SELECT")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "TX_DISABLE")
				(number "3")
			)
			(pin passive line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "CAGE")
				(number "CAGE")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VccT")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "VeeT")
				(number "1")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VeeT")
				(number "17")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VeeT")
				(number "20")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VccR")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VeeR")
				(number "10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VeeR")
				(number "11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VeeR")
				(number "14")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VeeR")
				(number "9")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "RX_LOS")
				(number "8")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RD+")
				(number "13")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "RD-")
				(number "12")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TD+")
				(number "18")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "TD-")
				(number "19")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "TX_FAULT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFP+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "J"
			(at -8.89 16.51 0)
		)
		(property "Value" "SFP+"
			(at 11.43 16.51 0)
		)
		(property "Footprint" ""
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://members.snia.org/document/dl/25892"
			(at -11.43 16.51 0)
		)
		(property "Description" "Connector for Small Form Factor Pluggable (SFP+) module, 10 Gbit/s, serial-to-serial data-agnostic optical transceiver"
			(at 0 0 0)
		)
		(property "ki_keywords" "SFP transceiver gigabit ethernet SFF-8432"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SFP*"
			(at 0 0 0)
		)
		(symbol "SFP+_0_0")
		(symbol "SFP+_1_1"
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "SDA")
				(number "4")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SCL")
				(number "5")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "MOD_ABS")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RS0")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RS1")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "TX_DISABLE")
				(number "3")
			)
			(pin passive line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "CAGE")
				(number "CAGE")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VccT")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "VeeT")
				(number "1")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VeeT")
				(number "17")
			)
			(pin passive line
				(at -2.54 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VeeT")
				(number "20")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VccR")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VeeR")
				(number "10")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VeeR")
				(number "11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VeeR")
				(number "14")
			)
			(pin open_collector line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "RX_LOS")
				(number "8")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RD+")
				(number "13")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "RD-")
				(number "12")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TD+")
				(number "18")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "TD-")
				(number "19")
			)
			(pin open_collector line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "TX_FAULT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSDP341xx"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSDP341xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82667/tsdp341.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Data Transmission"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
		(symbol "TSDP341xx_0_0"
			(text "DEMOD"
				(at -3.175 0.254 900)
			)
		)
		(symbol "TSDP341xx_0_1")
		(symbol "TSDP341xx_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vs")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSMP58138"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSMP58138"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINICAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82486/tsmp58138.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Module (Repeater) for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR repeater receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINICAST*"
			(at 0 0 0)
		)
		(symbol "TSMP58138_0_0"
			(text "CONDITION"
				(at -2.921 0 900)
			)
		)
		(symbol "TSMP58138_0_1")
		(symbol "TSMP58138_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vs")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSOP17xx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP17xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_CAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.micropik.com/PDF/tsop17xx.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Modules for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*CAST*"
			(at 0 0 0)
		)
		(symbol "TSOP17xx_0_0"
			(text "DEMOD"
				(at -3.175 0.254 900)
			)
		)
		(symbol "TSOP17xx_0_1")
		(symbol "TSOP17xx_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vs")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSOP32S40F"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP32S40F"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82669/tsop32s40f.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
		(symbol "TSOP32S40F_0_0"
			(text "DEMOD"
				(at -3.175 0.254 900)
			)
		)
		(symbol "TSOP32S40F_0_1")
		(symbol "TSOP32S40F_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vs")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSOP331xx"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP331xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINIMOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82742/tsop331.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINIMOLD*"
			(at 0 0 0)
		)
		(symbol "TSOP331xx_0_0"
			(text "DEMOD"
				(at -3.175 0.254 900)
			)
		)
		(symbol "TSOP331xx_0_1")
		(symbol "TSOP331xx_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vs")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSOP34S40F"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP34S40F"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82669/tsop32s40f.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
		(symbol "TSOP34S40F_0_0"
			(text "DEMOD"
				(at -3.175 0.254 900)
			)
		)
		(symbol "TSOP34S40F_0_1")
		(symbol "TSOP34S40F_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vs")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSOP581xx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP581xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINICAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82462/tsop581.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Modules for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINICAST*"
			(at 0 0 0)
		)
		(symbol "TSOP581xx_0_0"
			(text "DEMOD"
				(at -3.175 0.254 900)
			)
		)
		(symbol "TSOP581xx_0_1")
		(symbol "TSOP581xx_1_1"
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "Vs")
				(number "3")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT")
				(number "1")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TSDP343xx"
		(extends "TSDP341xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSDP343xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82667/tsdp341.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Data Transmission"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSMP58000"
		(extends "TSMP58138")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSMP58000"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINICAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82485/tsmp58000.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Module (Amplify&Condition) for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINICAST*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP21xx"
		(extends "TSOP32S40F")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP21xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82460/tsop45.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP23xx"
		(extends "TSOP32S40F")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP23xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82460/tsop45.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP25xx"
		(extends "TSOP32S40F")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP25xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82460/tsop45.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP312xx"
		(extends "TSOP17xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP312xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_CAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82492/tsop312.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Modules for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*CAST*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP314xx"
		(extends "TSOP17xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP314xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_CAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82492/tsop312.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Modules for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*CAST*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP321xx"
		(extends "TSOP32S40F")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP321xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82490/tsop321.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP323xx"
		(extends "TSOP32S40F")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP323xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82490/tsop321.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP325xx"
		(extends "TSOP32S40F")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP325xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82490/tsop321.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP333xx"
		(extends "TSOP331xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP333xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINIMOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82742/tsop331.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINIMOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP335xx"
		(extends "TSOP331xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP335xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINIMOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82742/tsop331.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINIMOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP341xx"
		(extends "TSDP341xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP341xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82490/tsop321.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP343xx"
		(extends "TSDP341xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP343xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82490/tsop321.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP345xx"
		(extends "TSDP341xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP345xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82490/tsop321.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP348xx"
		(extends "TSDP341xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP348xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/82489/tsop322.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP382xx"
		(extends "TSOP581xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP382xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINICAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82491/tsop382.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Modules for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINICAST*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP384xx"
		(extends "TSOP581xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP384xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINICAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82491/tsop382.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Modules for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINICAST*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP38G36"
		(extends "TSOP581xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP38G36"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINICAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82731/tsop38g36.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Modules for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINICAST*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP41xx"
		(extends "TSDP341xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP41xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82460/tsop45.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP43xx"
		(extends "TSDP341xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP43xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82460/tsop45.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP45xx"
		(extends "TSDP341xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP45xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82460/tsop45.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP531xx"
		(extends "TSOP331xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP531xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINIMOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82745/tsop531.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINIMOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP533xx"
		(extends "TSOP331xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP533xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINIMOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82745/tsop531.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINIMOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP535xx"
		(extends "TSOP331xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP535xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINIMOLD-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82745/tsop531.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "IR Receiver Modules for Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINIMOLD*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP582xx"
		(extends "TSOP581xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP582xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINICAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82461/tsop582.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Modules for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINICAST*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP583xx"
		(extends "TSOP581xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP583xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINICAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82462/tsop581.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Modules for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINICAST*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP584xx"
		(extends "TSOP581xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP584xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINICAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82461/tsop582.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Modules for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINICAST*"
			(at 0 0 0)
		)
	)
	(symbol "TSOP585xx"
		(extends "TSOP581xx")
		(property "Reference" "U"
			(at -10.16 7.62 0)
		)
		(property "Value" "TSOP585xx"
			(at -10.16 -7.62 0)
		)
		(property "Footprint" "OptoDevice:Vishay_MINICAST-3Pin"
			(at -1.27 -9.525 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/82462/tsop581.pdf"
			(at 16.51 7.62 0)
		)
		(property "Description" "Photo Modules for PCM Remote Control Systems"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Vishay*MINICAST*"
			(at 0 0 0)
		)
	)
)
