(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "FX614"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 20.32 0)
		)
		(property "Value" "FX614"
			(at 6.35 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.cmlmicro.com/wp-content/uploads/2017/06/FX614_ds.pdf"
			(at 0 0 0)
		)
		(property "Description" "Bell 202 Compatible Modem, DIP-16/SO-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Bell Modem"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
		(symbol "FX614_0_1")
		(symbol "FX614_1_1"
			(pin output line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "RXFB")
				(number "6")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "RXIN")
				(number "5")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "TXOP")
				(number "7")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "XTAL/CLK")
				(number "2")
			)
			(pin output line
				(at -15.24 -15.24 0)
				(length 3.81)
				(name "XTALN")
				(number "1")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "RXEQ")
				(number "10")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "RXD")
				(number "13")
			)
			(pin input clock
				(at 15.24 7.62 180)
				(length 3.81)
				(name "CLK")
				(number "12")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "~{RDYN}")
				(number "15")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "TXD")
				(number "11")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "DET")
				(number "14")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "M0")
				(number "3")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "M1")
				(number "4")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 3.81)
				(name "VBIAS")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HT9170D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "HT9170D"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm"
			(at 0 -16.51 0)
		)
		(property "Datasheet" "http://www.holtek.com/documents/10179/116711/9170v111.pdf"
			(at -2.54 17.78 0)
		)
		(property "Description" "DTMF receiver with 4 bit output, SOIC-18"
			(at 0 0 0)
		)
		(property "ki_keywords" "DTMF Receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x11.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HT9170D_0_1")
		(symbol "HT9170D_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "VP")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VN")
				(number "2")
			)
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "GS")
				(number "3")
			)
			(pin power_out line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VREF")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "INH")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PWDN")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "OE")
				(number "10")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "X1")
				(number "7")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "X2")
				(number "8")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "RT/GT")
				(number "17")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "EST")
				(number "16")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DV")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "D3")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 2.54)
				(name "D2")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "D1")
				(number "12")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "D0")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si3210"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 36.195 0)
		)
		(property "Value" "Si3210"
			(at -13.97 34.29 0)
		)
		(property "Footprint" "Package_SO:TSSOP-38_4.4x9.7mm_P0.5mm"
			(at 6.35 35.56 0)
		)
		(property "Datasheet" "http://www.mouser.com/ds/2/368/si3210-38974.pdf"
			(at 88.9 -67.31 0)
		)
		(property "Description" "ProSLIC Programmable cmos slic/codec with ringing/battery voltage generation"
			(at 0 0 0)
		)
		(property "ki_keywords" "ProSLIC slic"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*"
			(at 0 0 0)
		)
		(symbol "Si3210_0_1")
		(symbol "Si3210_1_1"
			(pin input line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "TEST")
				(number "32")
			)
			(pin input line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "STIPDC")
				(number "15")
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "STIPAC")
				(number "20")
			)
			(pin input line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "ITIPN")
				(number "29")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "IRINGN")
				(number "25")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "ITIPP")
				(number "28")
			)
			(pin input line
				(at -25.4 0 0)
				(length 5.08)
				(name "IRINGP")
				(number "26")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "STIPE")
				(number "17")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "SRINGE")
				(number "19")
			)
			(pin input line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "SVBAT")
				(number "18")
			)
			(pin input line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "SRINGAC")
				(number "21")
			)
			(pin input line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "SRINGDC")
				(number "16")
			)
			(pin output line
				(at -10.16 -40.64 90)
				(length 5.08)
				(name "SDCL")
				(number "9")
			)
			(pin output line
				(at -7.62 -40.64 90)
				(length 5.08)
				(name "SDCH")
				(number "8")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 5.08)
				(name "VDDA1")
				(number "10")
			)
			(pin output line
				(at -5.08 -40.64 90)
				(length 5.08)
				(name "DCDRV")
				(number "34")
			)
			(pin output line
				(at -2.54 -40.64 90)
				(length 5.08)
				(name "DCFF")
				(number "33")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 5.08)
				(name "VDDA2")
				(number "27")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 5.08)
				(name "GNDD")
				(number "31")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 5.08)
				(name "VDDD")
				(number "30")
			)
			(pin power_in line
				(at 7.62 -40.64 90)
				(length 5.08)
				(name "GNDA")
				(number "23")
			)
			(pin input line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "SCLK")
				(number "38")
			)
			(pin input line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "SDI")
				(number "37")
			)
			(pin output line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "SDITHRU")
				(number "35")
			)
			(pin output line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "SDO")
				(number "36")
			)
			(pin input line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "~{CS}")
				(number "1")
			)
			(pin input line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "FSYNC")
				(number "6")
			)
			(pin input line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PCLK")
				(number "3")
			)
			(pin input line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "DRX")
				(number "4")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "DTX")
				(number "5")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "~{INT}")
				(number "2")
			)
			(pin input line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "~{RESET}")
				(number "7")
			)
			(pin output line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "IGMP")
				(number "24")
			)
			(pin output line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "IGMN")
				(number "22")
			)
			(pin output line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "IREF")
				(number "11")
			)
			(pin output line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "CAPP")
				(number "12")
			)
			(pin output line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "CAPM")
				(number "14")
			)
			(pin power_in line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "QGND")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
)
