(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "16450"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 40.64 0)
		)
		(property "Value" "16450"
			(at 15.24 40.64 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "PC16450, Universal Asynchronous Receiver/Transmitter, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "1ch UART"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "16450_0_1")
		(symbol "16450_1_1"
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "D0")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "D1")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "D2")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "D3")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "D4")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "D5")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "D6")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "D7")
				(number "8")
			)
			(pin input line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "A0")
				(number "28")
			)
			(pin input line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "A1")
				(number "27")
			)
			(pin input line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "A2")
				(number "26")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "CS0")
				(number "12")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "CS1")
				(number "13")
			)
			(pin input line
				(at -25.4 0 0)
				(length 3.81)
				(name "~{CS2}")
				(number "14")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "XIN")
				(number "16")
			)
			(pin output line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "XOUT")
				(number "17")
			)
			(pin input line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "~{WR}")
				(number "18")
			)
			(pin input line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "WR")
				(number "19")
			)
			(pin input line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "RD")
				(number "22")
			)
			(pin input line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "~{RD}")
				(number "21")
			)
			(pin input line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "~{ADS}")
				(number "25")
			)
			(pin output line
				(at -25.4 -33.02 0)
				(length 3.81)
				(name "INTR")
				(number "30")
			)
			(pin input line
				(at -25.4 -35.56 0)
				(length 3.81)
				(name "MR")
				(number "35")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin input line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "~{RI}")
				(number "39")
			)
			(pin input line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "~{DCD}")
				(number "38")
			)
			(pin input line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "~{DSR}")
				(number "37")
			)
			(pin input line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "~{CTS}")
				(number "36")
			)
			(pin output line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "~{OUT1}")
				(number "34")
			)
			(pin output line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "~{DTR}")
				(number "33")
			)
			(pin output line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "~{RTS}")
				(number "32")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "~{OUT2}")
				(number "31")
			)
			(pin input line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "SIN")
				(number "10")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "SOUT")
				(number "11")
			)
			(pin output line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "CSOUT")
				(number "24")
			)
			(pin output line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "DDIS")
				(number "23")
			)
			(pin output line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "~{BAUDOUT}")
				(number "15")
			)
			(pin input line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "RCLK")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "16550"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 40.64 0)
		)
		(property "Value" "16550"
			(at 15.24 40.64 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/pc16550d.pdf"
			(at 0 0 0)
		)
		(property "Description" "PC16550D, Universal Asynchronous Receiver/Transmitter with FIFOs, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "1ch UART FIFO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "16550_0_1")
		(symbol "16550_1_1"
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "D0")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "D1")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "D2")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "D3")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "D4")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "D5")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "D6")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "D7")
				(number "8")
			)
			(pin input line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "A0")
				(number "28")
			)
			(pin input line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "A1")
				(number "27")
			)
			(pin input line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "A2")
				(number "26")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "CS0")
				(number "12")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "CS1")
				(number "13")
			)
			(pin input line
				(at -25.4 0 0)
				(length 3.81)
				(name "~{CS2}")
				(number "14")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "XIN")
				(number "16")
			)
			(pin output line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "XOUT")
				(number "17")
			)
			(pin input line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "~{WR}")
				(number "18")
			)
			(pin input line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "WR")
				(number "19")
			)
			(pin input line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "RD")
				(number "22")
			)
			(pin input line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "~{RD}")
				(number "21")
			)
			(pin input line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "~{ADS}")
				(number "25")
			)
			(pin output line
				(at -25.4 -33.02 0)
				(length 3.81)
				(name "INTR")
				(number "30")
			)
			(pin input line
				(at -25.4 -35.56 0)
				(length 3.81)
				(name "MR")
				(number "35")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin input line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "~{RI}")
				(number "39")
			)
			(pin input line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "~{DCD}")
				(number "38")
			)
			(pin input line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "~{DSR}")
				(number "37")
			)
			(pin input line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "~{CTS}")
				(number "36")
			)
			(pin output line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "~{OUT1}")
				(number "34")
			)
			(pin output line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "~{DTR}")
				(number "33")
			)
			(pin output line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "~{RTS}")
				(number "32")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "~{OUT2}")
				(number "31")
			)
			(pin input line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "SIN")
				(number "10")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "SOUT")
				(number "11")
			)
			(pin output line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "~{RXRDY}")
				(number "29")
			)
			(pin output line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "~{TXRDY}")
				(number "24")
			)
			(pin output line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "DDIS")
				(number "23")
			)
			(pin output line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "~{BAUDOUT}")
				(number "15")
			)
			(pin input line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "RCLK")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "68C681"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 2.54 0)
		)
		(property "Value" "68C681"
			(at -1.27 -2.54 0)
		)
		(property "Footprint" ""
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.elektronik.ropla.eu/pdf/stock/exa/xr68c681.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "CMOS Dual Channel UART"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART serial"
			(at 0 0 0)
		)
		(symbol "68C681_0_1")
		(symbol "68C681_1_1"
			(pin input line
				(at -22.86 33.02 0)
				(length 7.62)
				(name "A1")
				(number "1")
			)
			(pin input line
				(at -22.86 30.48 0)
				(length 7.62)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -22.86 27.94 0)
				(length 7.62)
				(name "A3")
				(number "5")
			)
			(pin input line
				(at -22.86 25.4 0)
				(length 7.62)
				(name "A4")
				(number "6")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 7.62)
				(name "IP0")
				(number "7")
			)
			(pin input line
				(at -22.86 17.78 0)
				(length 7.62)
				(name "IP1")
				(number "4")
			)
			(pin input line
				(at -22.86 15.24 0)
				(length 7.62)
				(name "IP2")
				(number "36")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 7.62)
				(name "IP3")
				(number "2")
			)
			(pin input line
				(at -22.86 10.16 0)
				(length 7.62)
				(name "IP4")
				(number "39")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 7.62)
				(name "IP5")
				(number "38")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 7.62)
				(name "D0")
				(number "25")
			)
			(pin input line
				(at -22.86 0 0)
				(length 7.62)
				(name "D1")
				(number "16")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 7.62)
				(name "D2")
				(number "24")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 7.62)
				(name "D3")
				(number "17")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 7.62)
				(name "D4")
				(number "23")
			)
			(pin input line
				(at -22.86 -10.16 0)
				(length 7.62)
				(name "D5")
				(number "18")
			)
			(pin input line
				(at -22.86 -12.7 0)
				(length 7.62)
				(name "D6")
				(number "22")
			)
			(pin input line
				(at -22.86 -15.24 0)
				(length 7.62)
				(name "D7")
				(number "19")
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 7.62)
				(name "RWN")
				(number "8")
			)
			(pin input line
				(at -22.86 -22.86 0)
				(length 7.62)
				(name "CSN")
				(number "35")
			)
			(pin input line
				(at -22.86 -25.4 0)
				(length 7.62)
				(name "RESETN")
				(number "34")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 7.62)
				(name "IACKN")
				(number "37")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 7.62)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 7.62)
				(name "GND")
				(number "20")
			)
			(pin input line
				(at 20.32 33.02 180)
				(length 7.62)
				(name "X1/CLK")
				(number "32")
			)
			(pin output line
				(at 20.32 25.4 180)
				(length 7.62)
				(name "X2")
				(number "33")
			)
			(pin output line
				(at 20.32 20.32 180)
				(length 7.62)
				(name "OP0")
				(number "29")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 7.62)
				(name "OP1")
				(number "12")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 7.62)
				(name "OP2")
				(number "28")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 7.62)
				(name "OP3")
				(number "13")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 7.62)
				(name "OP4")
				(number "27")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 7.62)
				(name "OP5")
				(number "14")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 7.62)
				(name "OP6")
				(number "26")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 7.62)
				(name "OP7")
				(number "15")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 7.62)
				(name "RXDA")
				(number "31")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 7.62)
				(name "TXDA")
				(number "30")
			)
			(pin input line
				(at 20.32 -10.16 180)
				(length 7.62)
				(name "RXDB")
				(number "10")
			)
			(pin output line
				(at 20.32 -12.7 180)
				(length 7.62)
				(name "TXDB")
				(number "11")
			)
			(pin output line
				(at 20.32 -20.32 180)
				(length 7.62)
				(name "DTACKN")
				(number "9")
			)
			(pin output line
				(at 20.32 -25.4 180)
				(length 7.62)
				(name "INTRN")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8252"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 25.4 0)
		)
		(property "Value" "8252"
			(at 8.89 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Universal Asynchronous Receiver/Transmitter, PDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART Serial Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "8252_0_1")
		(symbol "8252_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "D0")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "D1")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "D2")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "D3")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "D4")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "D5")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "D6")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "D7")
				(number "10")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "~{RD}")
				(number "1")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{WR}")
				(number "2")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "A0")
				(number "11")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "A1")
				(number "12")
			)
			(pin input inverted
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "CS0")
				(number "28")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "RST")
				(number "23")
			)
			(pin output line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "INTR")
				(number "24")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "IX")
				(number "13")
			)
			(pin output line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "OX")
				(number "14")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "VCC")
				(number "27")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "GND")
				(number "16")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "TBRE")
				(number "22")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "DR")
				(number "26")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "(TXD)SDO")
				(number "15")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "(RXD)SDI")
				(number "25")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "~{DSR}")
				(number "18")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "~{CTS}")
				(number "17")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "~{DTR}")
				(number "19")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "~{RTS}")
				(number "20")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "CO")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM101E"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 26.67 0)
		)
		(property "Value" "ADM101E"
			(at 12.7 26.67 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM101E.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Single RS232 driver/receiver, 5V supply, 460kb/s"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver line-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*"
			(at 0 0 0)
		)
		(symbol "ADM101E_0_0"
			(text "LOGIC"
				(at -11.43 -22.86 0)
			)
			(text "RS232"
				(at 11.43 -22.86 0)
			)
		)
		(symbol "ADM101E_0_1")
		(symbol "ADM101E_1_1"
			(pin passive line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "C1+")
				(number "9")
			)
			(pin passive line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "C1-")
				(number "2")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "SD")
				(number "8")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "T1IN")
				(number "4")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "R1OUT")
				(number "5")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 5.08)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin power_out line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "VS-")
				(number "3")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "T1OUT")
				(number "7")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "R1IN")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM1491EBR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "ADM1491EBR"
			(at -11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM1490E_1491E.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 full duplex 16Mbps transceiver, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADM1491EBR_0_1")
		(symbol "ADM1491EBR_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RE}")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "DE")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "13")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A")
				(number "12")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "10")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM205"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.732 32.512 0)
		)
		(property "Value" "ADM205"
			(at 14.732 32.512 0)
		)
		(property "Footprint" "Package_DIP:DIP-24_W15.24mm"
			(at 0.254 15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/obsolete-data-sheets/17659925ADM205.PDF"
			(at 0 1.524 0)
		)
		(property "Description" "0.1 μF, 5V powered CMOS RS-232 120kb/s transceiver with 5 drivers and 5 receivers (tx/rx: 5/5), shutdown / enable pins, DIP-24 (600 mil)"
			(at 0 -1.27 0)
		)
		(property "ki_keywords" "UART RS232 Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W15.*"
			(at 0 0 0)
		)
		(symbol "ADM205_0_1")
		(symbol "ADM205_1_0"
			(text "LOGIC"
				(at -14.732 -30.48 0)
			)
			(text "RS232"
				(at 14.732 -30.48 0)
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "T3IN")
				(number "15")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "T4IN")
				(number "16")
			)
			(pin input line
				(at -20.32 0 0)
				(length 5.08)
				(name "T5IN")
				(number "22")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "T3OUT")
				(number "2")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "T4OUT")
				(number "1")
			)
			(pin output line
				(at 20.32 0 180)
				(length 5.08)
				(name "T5OUT")
				(number "19")
			)
		)
		(symbol "ADM205_1_1"
			(pin input line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "~{EN}")
				(number "20")
			)
			(pin input line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "SD")
				(number "21")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "T1IN")
				(number "8")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "T2IN")
				(number "7")
			)
			(pin tri_state line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "R1OUT")
				(number "9")
			)
			(pin tri_state line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "R2OUT")
				(number "6")
			)
			(pin tri_state line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "R3OUT")
				(number "23")
			)
			(pin tri_state line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "R4OUT")
				(number "17")
			)
			(pin tri_state line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "R5OUT")
				(number "14")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 5.08)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 5.08)
				(name "GND")
				(number "11")
			)
			(pin output line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "T1OUT")
				(number "3")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "T2OUT")
				(number "4")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "R1IN")
				(number "10")
			)
			(pin input line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "R2IN")
				(number "5")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "R3IN")
				(number "24")
			)
			(pin input line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "R4IN")
				(number "18")
			)
			(pin input line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "R5IN")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM206"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.732 32.512 0)
		)
		(property "Value" "ADM206"
			(at 15.24 32.512 0)
		)
		(property "Footprint" ""
			(at 0.254 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM206_207_208_211_213.pdf"
			(at 0 4.064 0)
		)
		(property "Description" "0.1 μF, 5V powered CMOS RS-232 120kb/s transceiver with 4 drivers and 3 receivers (tx/rx: 4/3), shutdown / enable pins, DIP-24 (300 mil) / SOIC-24 / SSOP-24"
			(at 0 1.27 0)
		)
		(property "ki_keywords" "UART RS232"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62* *SOIC*7.*15.*P1.27mm* *SSOP*5.3*8.*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADM206_0_1")
		(symbol "ADM206_1_0"
			(text "LOGIC"
				(at -14.732 -27.94 0)
			)
			(text "RS232"
				(at 14.732 -27.94 0)
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "T3IN")
				(number "18")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "T4IN")
				(number "19")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "T3OUT")
				(number "1")
			)
			(pin output line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "T4OUT")
				(number "24")
			)
		)
		(symbol "ADM206_1_1"
			(pin passive line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "C1+")
				(number "10")
			)
			(pin passive line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "C1-")
				(number "12")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "~{EN}")
				(number "20")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "SD")
				(number "21")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "T1IN")
				(number "7")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "T2IN")
				(number "6")
			)
			(pin tri_state line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "R1OUT")
				(number "5")
			)
			(pin tri_state line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "R2OUT")
				(number "22")
			)
			(pin tri_state line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "R3OUT")
				(number "17")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 5.08)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "C2+")
				(number "13")
			)
			(pin passive line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "C2-")
				(number "14")
			)
			(pin power_out line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "V+")
				(number "11")
			)
			(pin power_out line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "V-")
				(number "15")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "T1OUT")
				(number "2")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "T2OUT")
				(number "3")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "R1IN")
				(number "4")
			)
			(pin input line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "R2IN")
				(number "23")
			)
			(pin input line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "R3IN")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM207"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.732 35.052 0)
		)
		(property "Value" "ADM207"
			(at 15.24 35.052 0)
		)
		(property "Footprint" ""
			(at 0.254 5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM206_207_208_211_213.pdf"
			(at 0 4.064 0)
		)
		(property "Description" "0.1 μF, 5V powered CMOS RS-232 120kb/s transceiver with 5 drivers and 3 receivers (tx/rx: 5/3), DIP-24 (300 mil) / SOIC-24 / SSOP-24"
			(at 0 1.27 0)
		)
		(property "ki_keywords" "UART RS232"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62* *SOIC*7.*15.*P1.27mm* *SSOP*5.3*8.*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADM207_0_1")
		(symbol "ADM207_1_0"
			(text "LOGIC"
				(at -14.732 -30.48 0)
			)
			(text "RS232"
				(at 14.732 -30.48 0)
			)
			(pin input line
				(at -20.32 0 0)
				(length 5.08)
				(name "T3IN")
				(number "18")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "T4IN")
				(number "19")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "T5IN")
				(number "21")
			)
			(pin output line
				(at 20.32 0 180)
				(length 5.08)
				(name "T3OUT")
				(number "1")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "T4OUT")
				(number "24")
			)
			(pin output line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "T5OUT")
				(number "20")
			)
		)
		(symbol "ADM207_1_1"
			(pin passive line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "C1+")
				(number "10")
			)
			(pin passive line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "C1-")
				(number "12")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "T1IN")
				(number "7")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "T2IN")
				(number "6")
			)
			(pin output line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "R1OUT")
				(number "5")
			)
			(pin output line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "R2OUT")
				(number "22")
			)
			(pin output line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "R3OUT")
				(number "17")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 5.08)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "C2+")
				(number "13")
			)
			(pin passive line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "C2-")
				(number "14")
			)
			(pin power_out line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "V+")
				(number "11")
			)
			(pin power_out line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "V-")
				(number "15")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "T1OUT")
				(number "2")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "T2OUT")
				(number "3")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "R1IN")
				(number "4")
			)
			(pin input line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "R2IN")
				(number "23")
			)
			(pin input line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "R3IN")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM208"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.732 35.052 0)
		)
		(property "Value" "ADM208"
			(at 15.24 35.052 0)
		)
		(property "Footprint" ""
			(at 0.254 5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM206_207_208_211_213.pdf"
			(at 0 4.064 0)
		)
		(property "Description" "0.1 μF, 5V powered CMOS RS-232 120kb/s transceiver with 4 drivers and 4 receivers (tx/rx: 4/4), DIP-24 (300 mil) / SOIC-24 / SSOP-24"
			(at 0 1.27 0)
		)
		(property "ki_keywords" "UART RS232"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62* *SOIC*7.*15.*P1.27mm* *SSOP*5.3*8.*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADM208_0_1")
		(symbol "ADM208_1_0"
			(text "LOGIC"
				(at -14.732 -30.48 0)
			)
			(text "RS232"
				(at 14.732 -30.48 0)
			)
			(pin input line
				(at -20.32 0 0)
				(length 5.08)
				(name "T3IN")
				(number "19")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "T4IN")
				(number "21")
			)
			(pin output line
				(at 20.32 0 180)
				(length 5.08)
				(name "T3OUT")
				(number "24")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "T4OUT")
				(number "20")
			)
		)
		(symbol "ADM208_1_1"
			(pin passive line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "C1+")
				(number "10")
			)
			(pin passive line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "C1-")
				(number "12")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "T1IN")
				(number "5")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "T2IN")
				(number "18")
			)
			(pin output line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "R1OUT")
				(number "6")
			)
			(pin output line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "R2OUT")
				(number "4")
			)
			(pin output line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "R3OUT")
				(number "22")
			)
			(pin output line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "R4OUT")
				(number "17")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 5.08)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "C2+")
				(number "13")
			)
			(pin passive line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "C2-")
				(number "14")
			)
			(pin power_out line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "V+")
				(number "11")
			)
			(pin power_out line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "V-")
				(number "15")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "T1OUT")
				(number "2")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "T2OUT")
				(number "1")
			)
			(pin input line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "R1IN")
				(number "7")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "R2IN")
				(number "3")
			)
			(pin input line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "R3IN")
				(number "23")
			)
			(pin input line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "R4IN")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM209"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.224 32.512 0)
		)
		(property "Value" "ADM209"
			(at 14.986 32.512 0)
		)
		(property "Footprint" ""
			(at 0.254 5.08 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/obsolete-data-sheets/17659925ADM205.PDF"
			(at 0 1.524 0)
		)
		(property "Description" "0.1 μF, 5V powered CMOS RS-232 120kb/s transceiver with 3 drivers and 5 receivers (tx/rx: 3/5), enable pin, external 9 V to 13.2 V supply, DIP-24 (300 mil) / SOIC-24 / SSOP-24"
			(at 0 -1.27 0)
		)
		(property "ki_keywords" "UART RS232 Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DIP*W7.62* *SOIC*7.*15.*P1.27mm* *SSOP*5.3*8.*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADM209_0_1")
		(symbol "ADM209_1_0"
			(text "LOGIC"
				(at -14.732 -30.48 0)
			)
			(text "RS232"
				(at 14.732 -30.48 0)
			)
			(pin input line
				(at -20.32 0 0)
				(length 5.08)
				(name "T3IN")
				(number "16")
			)
			(pin tri_state line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "R5OUT")
				(number "10")
			)
			(pin no_connect line
				(at 15.24 22.86 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin output line
				(at 20.32 0 180)
				(length 5.08)
				(name "T3OUT")
				(number "13")
			)
			(pin input line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "R5IN")
				(number "9")
			)
		)
		(symbol "ADM209_1_1"
			(pin passive line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "C+")
				(number "6")
			)
			(pin passive line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "C-")
				(number "7")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "~{EN}")
				(number "14")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "T1IN")
				(number "24")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "T2IN")
				(number "23")
			)
			(pin tri_state line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "R1OUT")
				(number "1")
			)
			(pin tri_state line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "R2OUT")
				(number "22")
			)
			(pin tri_state line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "R3OUT")
				(number "17")
			)
			(pin tri_state line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "R4OUT")
				(number "11")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 5.08)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "V+")
				(number "5")
			)
			(pin power_out line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "V-")
				(number "8")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "T1OUT")
				(number "19")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "T2OUT")
				(number "20")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "R1IN")
				(number "2")
			)
			(pin input line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "R2IN")
				(number "21")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "R3IN")
				(number "18")
			)
			(pin input line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "R4IN")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM211"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.732 37.592 0)
		)
		(property "Value" "ADM211"
			(at 14.732 37.592 0)
		)
		(property "Footprint" ""
			(at 0.254 7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM206_207_208_211_213.pdf"
			(at 0 4.064 0)
		)
		(property "Description" "0.1 μF, 5V powered CMOS RS-232 120kb/s transceiver with 4 drivers and 5 receivers (tx/rx: 4/5), shutdown / enable pins, SOIC-28 / SSOP-28"
			(at 0 1.27 0)
		)
		(property "ki_keywords" "UART RS232"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*7.*17.*P1.27mm* *SSOP*5.3*10.*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADM211_0_1")
		(symbol "ADM211_1_0"
			(text "LOGIC"
				(at -14.732 -33.02 0)
			)
			(text "RS232"
				(at 14.732 -33.02 0)
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "T3IN")
				(number "20")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "T4IN")
				(number "21")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "T3OUT")
				(number "1")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "T4OUT")
				(number "28")
			)
		)
		(symbol "ADM211_1_1"
			(pin passive line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "C1+")
				(number "12")
			)
			(pin passive line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "C1-")
				(number "14")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "~{EN}")
				(number "24")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "SD")
				(number "25")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "T1IN")
				(number "7")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "T2IN")
				(number "6")
			)
			(pin tri_state line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "R1OUT")
				(number "8")
			)
			(pin tri_state line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "R2OUT")
				(number "5")
			)
			(pin tri_state line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "R3OUT")
				(number "26")
			)
			(pin tri_state line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "R4OUT")
				(number "22")
			)
			(pin tri_state line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "R5OUT")
				(number "19")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 5.08)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "C2+")
				(number "15")
			)
			(pin passive line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "C2-")
				(number "16")
			)
			(pin power_out line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "V+")
				(number "13")
			)
			(pin power_out line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "V-")
				(number "17")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "T1OUT")
				(number "2")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "T2OUT")
				(number "3")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "R1IN")
				(number "9")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "R2IN")
				(number "4")
			)
			(pin input line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "R3IN")
				(number "27")
			)
			(pin input line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "R4IN")
				(number "23")
			)
			(pin input line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "R5IN")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM213"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -14.732 37.592 0)
		)
		(property "Value" "ADM213"
			(at 14.732 37.592 0)
		)
		(property "Footprint" ""
			(at 0.254 7.62 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM206_207_208_211_213.pdf"
			(at 0 4.064 0)
		)
		(property "Description" "0.1 μF, 5V powered CMOS RS-232 120kb/s transceiver with 4 drivers and 5 receivers (tx/rx: 4/5; 2 receivers active in shutdown), shutdown / enable pins, SOIC-28 / SSOP-28"
			(at 0 1.27 0)
		)
		(property "ki_keywords" "UART RS232"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*7.*17.*P1.27mm* *SSOP*5.3*10.*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADM213_0_1")
		(symbol "ADM213_1_0"
			(text "LOGIC"
				(at -14.732 -33.02 0)
			)
			(text "RS232"
				(at 14.732 -33.02 0)
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "T3IN")
				(number "20")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "T4IN")
				(number "21")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "T3OUT")
				(number "1")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "T4OUT")
				(number "28")
			)
		)
		(symbol "ADM213_1_1"
			(pin passive line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "C1+")
				(number "12")
			)
			(pin passive line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "C1-")
				(number "14")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "EN")
				(number "24")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "~{SD}")
				(number "25")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "T1IN")
				(number "7")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "T2IN")
				(number "6")
			)
			(pin tri_state line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "R1OUT")
				(number "8")
			)
			(pin tri_state line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "R2OUT")
				(number "5")
			)
			(pin tri_state line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "R3OUT")
				(number "26")
			)
			(pin tri_state line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "R4OUT")
				(number "22")
			)
			(pin tri_state line
				(at -20.32 -27.94 0)
				(length 5.08)
				(name "R5OUT")
				(number "19")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 5.08)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 5.08)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "C2+")
				(number "15")
			)
			(pin passive line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "C2-")
				(number "16")
			)
			(pin power_out line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "V+")
				(number "13")
			)
			(pin power_out line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "V-")
				(number "17")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 5.08)
				(name "T1OUT")
				(number "2")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "T2OUT")
				(number "3")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "R1IN")
				(number "9")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "R2IN")
				(number "4")
			)
			(pin input line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "R3IN")
				(number "27")
			)
			(pin input line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "R4IN")
				(number "23")
			)
			(pin input line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "R5IN")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM242"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 26.67 0)
		)
		(property "Value" "ADM242"
			(at 12.7 26.67 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM222_232A_242.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Dual RS232 driver/receiver, 5V supply, 200kb/s, separate shutdown/enable pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ADM242_0_0"
			(text "LOGIC"
				(at -11.43 -22.86 0)
			)
			(text "RS232"
				(at 11.43 -22.86 0)
			)
		)
		(symbol "ADM242_0_1")
		(symbol "ADM242_1_1"
			(pin passive line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "C1+")
				(number "2")
			)
			(pin passive line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "C1-")
				(number "4")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "~{EN}")
				(number "1")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "~{SHDN}")
				(number "18")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "T1IN")
				(number "12")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "T2IN")
				(number "11")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "R1OUT")
				(number "13")
			)
			(pin output line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "R2OUT")
				(number "10")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 5.08)
				(name "VCC")
				(number "17")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 5.08)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "C2+")
				(number "5")
			)
			(pin passive line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "C2-")
				(number "6")
			)
			(pin power_out line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "V+")
				(number "3")
			)
			(pin power_out line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "V-")
				(number "7")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "T1OUT")
				(number "15")
			)
			(pin output line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "T2OUT")
				(number "8")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "R1IN")
				(number "14")
			)
			(pin input line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "R2IN")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM2481xRW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ADM2481xRW"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adm2481.pdf"
			(at -19.05 1.27 0)
		)
		(property "Description" "Isolated RS485/RS422 Transceiver, Half-Duplex, 500kbps, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs-485 rs-422 eia485 eia-485 eia422 eia-422 serial differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADM2481xRW_0_0")
		(symbol "ADM2481xRW_0_1")
		(symbol "ADM2481xRW_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DE")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "TxD")
				(number "6")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RxD")
				(number "3")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{RE}")
				(number "4")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "7")
			)
			(pin passive line
				(at -5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
			(pin no_connect line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 12.7 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "A")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "B")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM2483xRW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ADM2483xRW"
			(at 6.35 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adm2483.pdf"
			(at -19.05 1.27 0)
		)
		(property "Description" "Isolated RS485/RS422 Transceiver, Half-Duplex, 500kbps, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs-485 rs-422 eia485 eia-485 eia422 eia-422 serial differential"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADM2483xRW_0_0")
		(symbol "ADM2483xRW_0_1")
		(symbol "ADM2483xRW_1_1"
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DE")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "TxD")
				(number "6")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RxD")
				(number "3")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{RE}")
				(number "4")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PV")
				(number "7")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 5.08 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 12.7 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "A")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "B")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM2484E"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 19.05 0)
		)
		(property "Value" "ADM2484E"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM2484E.pdf"
			(at -19.05 1.27 0)
		)
		(property "Description" "Isolated RS485/RS422 Transceiver, Half-/Full-Duplex, 500kbps,SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 Transceiver RS422 Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADM2484E_0_0")
		(symbol "ADM2484E_0_1")
		(symbol "ADM2484E_1_1"
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DE")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "TxD")
				(number "6")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RxD")
				(number "3")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{RE}")
				(number "4")
			)
			(pin power_in line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 12.7 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin power_in line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "Y")
				(number "11")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "Z")
				(number "12")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "A")
				(number "14")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin power_in line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM2587E"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 21.59 0)
		)
		(property "Value" "ADM2587E"
			(at 0 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "www.analog.com/media/en/technical-documentation/data-sheets/ADM2582E_2587E.pdf"
			(at -20.32 0 0)
		)
		(property "Description" "Isolated RS485/RS422 Transceiver,Integrated Isolated DC-DC Converter, 500kbps,SO-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 Transceiver,RS422 Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADM2587E_0_0"
			(text "DECODE"
				(at -4.445 7.62 0)
			)
			(text "ENCODE"
				(at -4.445 2.54 0)
			)
			(text "ENCODE"
				(at -4.445 0 0)
			)
			(text "ISOLATED DC-DC"
				(at -0.127 15.24 0)
			)
			(text "ENCODE"
				(at 4.445 7.62 0)
			)
			(text "DECODE"
				(at 4.445 0 0)
			)
		)
		(symbol "ADM2587E_0_1")
		(symbol "ADM2587E_1_1"
			(pin power_in line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RxD")
				(number "4")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "~{RE}")
				(number "5")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DE")
				(number "6")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "TxD")
				(number "7")
			)
			(pin power_in line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "GND1")
				(number "1")
			)
			(pin power_in line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "GND1")
				(number "3")
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "9")
			)
			(pin power_in line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "10")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "Visoout")
				(number "12")
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "Visoin")
				(number "19")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "A")
				(number "18")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "B")
				(number "17")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "Y")
				(number "13")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "Z")
				(number "15")
			)
			(pin power_in line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
			(pin power_in line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "GND2")
				(number "14")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "16")
			)
			(pin power_in line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM2682E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "ADM2682E"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x12.8mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM2682E_2687E.pdf"
			(at 0 18.415 0)
		)
		(property "Description" "Isolated RS485/RS422 Transceiver, Integrated Isolated DC-DC Converter, 16Mbps, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 Transceiver, RS422 Transceiver, Isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADM2682E_0_0"
			(text "D"
				(at 8.128 -1.27 0)
			)
			(text "R"
				(at 8.509 -6.35 0)
			)
		)
		(symbol "ADM2682E_0_1")
		(symbol "ADM2682E_1_0"
			(text "OSCILLATOR"
				(at -4.953 8.255 0)
			)
			(text "ENCODE"
				(at -3.81 0 0)
			)
			(text "ENCODE"
				(at -3.81 -2.54 0)
			)
			(text "DECODE"
				(at -3.81 -5.08 0)
			)
			(text "DECODE"
				(at 3.81 0 0)
			)
			(text "DECODE"
				(at 3.81 -2.54 0)
			)
			(text "ENCODE"
				(at 3.81 -5.08 0)
			)
			(text "RECTIFIER"
				(at 4.826 8.255 0)
			)
			(text "REGULATOR"
				(at 4.826 5.715 0)
			)
		)
		(symbol "ADM2682E_1_1"
			(pin power_in line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "7")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "TXD")
				(number "6")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DE")
				(number "5")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RXD")
				(number "3")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{RE}")
				(number "4")
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "1")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "VISOOUT")
				(number "10")
			)
			(pin power_in line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VISOIN")
				(number "15")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "Y")
				(number "11")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "12")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "A")
				(number "14")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "16")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADM3490ExR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "ADM3490ExR"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM3483E_3486E_3488E_3490E_3491E.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 full duplex 12 Mbps transceiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADM3490ExR_0_1")
		(symbol "ADM3490ExR_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "6")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AZ75232M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 29.21 0)
		)
		(property "Value" "AZ75232M"
			(at 15.24 26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ75232.pdf"
			(at 63.5 3.81 0)
		)
		(property "Description" "RS232 interface IC, 3 drivers, 5 receivers, 3.3V/5V Vcc supply, bipolar Vdd/Vss supply, 120kb/s, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver line-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AZ75232M_0_0"
			(text "RS232"
				(at -6.985 -24.13 0)
			)
			(text "LOGIC"
				(at 7.62 -24.13 0)
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "V_{CC}")
				(number "20")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "RY1")
				(number "19")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "RY2")
				(number "18")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "RY3")
				(number "17")
			)
		)
		(symbol "AZ75232M_0_1")
		(symbol "AZ75232M_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "RA1")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "RA2")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "RA3")
				(number "4")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DY1")
				(number "5")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DY2")
				(number "6")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RA4")
				(number "7")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "DY3")
				(number "8")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "RA5")
				(number "9")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "V_{DD}")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "V_{SS}")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DA1")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DA2")
				(number "15")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "RY4")
				(number "14")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "DA3")
				(number "13")
			)
			(pin output line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "RY5")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL3280ExHZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ISL3280ExHZ"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 2.54 13.97 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/www/doc/datasheet/isl3280e-81e-82e-83e-84e-85e.pdf"
			(at -22.86 17.78 0)
		)
		(property "Description" "RS485, RS422, 20Mbps Transceiver, 3.0V to 5.5V, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "Interface Driver Receiver Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ISL3280ExHZ_0_1")
		(symbol "ISL3280ExHZ_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "B")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL3281ExHZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ISL3281ExHZ"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 2.54 13.97 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/www/doc/datasheet/isl3280e-81e-82e-83e-84e-85e.pdf"
			(at 0 0 0)
		)
		(property "Description" "RS485, RS422, 20Mbps Transceiver, 3.0V to 5.5V, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Interface - Driver Receiver Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ISL3281ExHZ_0_1")
		(symbol "ISL3281ExHZ_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "B")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RO")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "RE")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL3282ExRHZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ISL3282ExRHZ"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8-1EP_3x2mm_P0.5mm_EP1.80x1.65mm"
			(at 2.54 13.97 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/www/doc/datasheet/isl3280e-81e-82e-83e-84e-85e.pdf"
			(at 0 0 0)
		)
		(property "Description" "RS485, RS422, 20Mbps Transceiver, 3.0V to 5.5V, TDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Interface Driver Receiver Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ISL3282ExRHZ_0_1")
		(symbol "ISL3282ExRHZ_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "B")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VL")
				(number "6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RO")
				(number "1")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RE}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL3283ExHZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ISL3283ExHZ"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 2.54 13.97 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/www/doc/datasheet/isl3280e-81e-82e-83e-84e-85e.pdf"
			(at 0 0 0)
		)
		(property "Description" "RS485, RS422, 20Mbps Transceiver, 3.0V to 5.5V, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Interface Driver Receiver Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ISL3283ExHZ_0_1")
		(symbol "ISL3283ExHZ_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "B")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RO")
				(number "3")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RE}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL3284ExHZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 11.43 0)
		)
		(property "Value" "ISL3284ExHZ"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 2.54 13.97 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/www/doc/datasheet/isl3280e-81e-82e-83e-84e-85e.pdf"
			(at 0 0 0)
		)
		(property "Description" "RS485, RS422, 20Mbps Transceiver, 3.0V to 5.5V, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Interface Driver Receiver Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ISL3284ExHZ_0_1")
		(symbol "ISL3284ExHZ_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "B")
				(number "4")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "RO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL3295xxH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 11.43 0)
		)
		(property "Value" "ISL3295xxH"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "https://www.renesas.com/sg/en/www/doc/datasheet/isl3295e-98e.pdf"
			(at -5.08 11.43 0)
		)
		(property "Description" "RS485, RS422, 20Mbps Transceiver, 3.0V to 7V, Low-Power, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "ISL3295xxH_0_1")
		(symbol "ISL3295xxH_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DI")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DE")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Z")
				(number "4")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Y")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL3298xxRT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 12.7 0)
		)
		(property "Value" "ISL3298xxRT"
			(at -10.16 10.16 0)
		)
		(property "Footprint" "Package_DFN_QFN:TDFN-8-1EP_3x2mm_P0.5mm_EP1.80x1.65mm"
			(at 5.08 -20.32 0)
		)
		(property "Datasheet" "https://www.renesas.com/sg/en/www/doc/datasheet/isl3295e-98e.pdf"
			(at -7.62 12.7 0)
		)
		(property "Description" "RS485, RS422, 20Mbps Transceiver, 3.0V to 7V, Low-Power, TDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TDFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ISL3298xxRT_0_1")
		(symbol "ISL3298xxRT_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DE")
				(number "2")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VL")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "Z")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Y")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISL83491"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 -15.24 0)
		)
		(property "Value" "ISL83491"
			(at 0 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/isl8/isl83483-85-88-90-91.pdf"
			(at 0 0 0)
		)
		(property "Description" "10Mbps RS485/RS422 transceiver, full duplex, receiver/driver enable, low power shutdown"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ISL83491_0_0"
			(text "D"
				(at -1.27 -5.08 0)
			)
			(text "R"
				(at 1.27 7.62 0)
			)
		)
		(symbol "ISL83491_0_1")
		(symbol "ISL83491_1_1"
			(pin output line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "RO")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "~{RE}")
				(number "3")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "DI")
				(number "5")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "DE")
				(number "4")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "13")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "A")
				(number "12")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "~{B}")
				(number "11")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "Y")
				(number "9")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "~{Z}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO1500"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "ISO1500"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/iso1500.pdf"
			(at 0 0 0)
		)
		(property "Description" "Half duplex RS-485/RS-422 transceiver, 3-kVRMS Isolated, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS-485 RS422 transceiver isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ISO1500_0_1")
		(symbol "ISO1500_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "R")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RE}")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "DE")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin no_connect line
				(at 0 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VCC2")
				(number "10")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "VCC2")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "A")
				(number "12")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO3082DW"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 19.05 0)
		)
		(property "Value" "ISO3082DW"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/iso3082.pdf"
			(at -5.08 -19.05 0)
		)
		(property "Description" "200 kbps, Isolated 5-V Half-Duplex RS-485 transceiver, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS-485"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO3082DW_0_0"
			(text "GALVANIC ISOLATION"
				(at -1.27 0.508 900)
			)
		)
		(symbol "ISO3082DW_0_1")
		(symbol "ISO3082DW_1_0")
		(symbol "ISO3082DW_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DE")
				(number "5")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "D")
				(number "6")
			)
			(pin output line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "R")
				(number "3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "~{RE}")
				(number "4")
			)
			(pin power_in line
				(at -10.16 -17.78 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at -7.62 17.78 270)
				(length 2.54)
				(name "Vcc1")
				(number "1")
			)
			(pin power_in line
				(at -7.62 -17.78 90)
				(length 2.54)
				(name "GND1")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin power_in line
				(at 7.62 17.78 270)
				(length 2.54)
				(name "Vcc2")
				(number "16")
			)
			(pin power_in line
				(at 7.62 -17.78 90)
				(length 2.54)
				(name "GND2")
				(number "10")
			)
			(pin power_in line
				(at 10.16 -17.78 90)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin no_connect line
				(at 12.7 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 12.7 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "B")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "A")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1080"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 26.67 0)
		)
		(property "Value" "LT1080"
			(at 12.7 26.67 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/10801fe.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Dual RS232 driver/receiver, 5V supply, 120kb/s"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO* DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LT1080_0_0"
			(text "LOGIC"
				(at -11.43 -22.86 0)
			)
			(text "RS232"
				(at 11.43 -22.86 0)
			)
		)
		(symbol "LT1080_0_1")
		(symbol "LT1080_1_1"
			(pin passive line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "C1+")
				(number "2")
			)
			(pin passive line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "C1-")
				(number "4")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "ON/~{OFF}")
				(number "18")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "T1IN")
				(number "12")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "T2IN")
				(number "11")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "R1OUT")
				(number "13")
			)
			(pin output line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "R2OUT")
				(number "10")
			)
			(pin no_connect line
				(at -15.24 5.08 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 5.08)
				(name "VCC")
				(number "17")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 5.08)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "C2+")
				(number "5")
			)
			(pin passive line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "C2-")
				(number "6")
			)
			(pin power_out line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "V+")
				(number "3")
			)
			(pin power_out line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "V-")
				(number "7")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "T1OUT")
				(number "15")
			)
			(pin output line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "T2OUT")
				(number "8")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "R1IN")
				(number "14")
			)
			(pin input line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "R2IN")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LT1791xN8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LT1791xN8"
			(at 6.985 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285012fe.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 250kbps transceiver, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LT1791xN8_0_1")
		(symbol "LT1791xN8_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RE}")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "DE")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A")
				(number "12")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "10")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2850xDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2850xDD"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285012fe.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Half duplex 20Mbps transceiver, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2850xDD_0_1")
		(symbol "LTC2850xDD_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RE}")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "DE")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2850xS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2850xS8"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285012fe.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Half-duplex 20Mbps transceiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC2850xS8_0_1")
		(symbol "LTC2850xS8_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RE}")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "DE")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2851xDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2851xDD"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285012fe.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 20Mbps transceiver, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2851xDD_0_1")
		(symbol "LTC2851xDD_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "6")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2851xMS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2851xMS8"
			(at 8.255 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285012fe.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 20Mbps transceiver, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LTC2851xMS8_0_1")
		(symbol "LTC2851xMS8_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "6")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2851xS8"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2851xS8"
			(at 6.985 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285012fe.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 20Mbps transceiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC2851xS8_0_1")
		(symbol "LTC2851xS8_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "6")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2852xDD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2852xDD"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285012fe.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 20Mbps transceiver, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2852xDD_0_1")
		(symbol "LTC2852xDD_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RE}")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "DE")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "8")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "7")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2852xMS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2852xMS"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285012fe.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 20Mbps transceiver, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LTC2852xMS_0_1")
		(symbol "LTC2852xMS_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RE}")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "DE")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "8")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "7")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2852xS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2852xS"
			(at 6.985 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285012fe.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 20Mbps transceiver, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTC2852xS_0_1")
		(symbol "LTC2852xS_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "RO")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RE}")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "DE")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A")
				(number "12")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "10")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTC2861"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "LTC2861"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "linear-tec\\ltc2859-2861.pdf"
			(at 0 0 0)
		)
		(property "Description" "20Mbps RS485 transceiver with tntegrated switchable termination"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "LTC2861_0_1")
		(symbol "LTC2861_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A")
				(number "15")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "TE")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{B}")
				(number "14")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "DE")
				(number "3")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "Y")
				(number "12")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{Z}")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "RO")
				(number "1")
			)
			(pin input inverted
				(at 12.7 2.54 180)
				(length 3.81)
				(name "RE")
				(number "2")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DI")
				(number "4")
			)
			(pin input inverted
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SLO")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX13432EESD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "MAX13432EESD"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX13430E-MAX13433E.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "RS485 transceiver, full duplex, dual supply, receiver/driver enable, 500kbps, SOIC-14 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs485 transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX13432EESD_0_0"
			(text "D"
				(at -1.27 -5.08 0)
			)
			(text "R"
				(at 1.27 7.62 0)
			)
		)
		(symbol "MAX13432EESD_0_1")
		(symbol "MAX13432EESD_1_1"
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "Vlogic")
				(number "1")
			)
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "RO")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{RE}")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "5")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DE")
				(number "3")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "A")
				(number "12")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{B}")
				(number "11")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "Y")
				(number "9")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{Z}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX13432EETD"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "MAX13432EETD"
			(at 2.54 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x3mm_P0.4mm_EP1.78x2.35mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX13430E-MAX13433E.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "RS485 transceiver, full duplex, dual supply, receiver/driver enable, 500kbps, DFN-14 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs485 transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MAX13432EETD_0_0"
			(text "D"
				(at -1.27 -5.08 0)
			)
			(text "R"
				(at 1.27 7.62 0)
			)
		)
		(symbol "MAX13432EETD_0_1")
		(symbol "MAX13432EETD_1_1"
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "Vlogic")
				(number "1")
			)
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "RO")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{RE}")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "5")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "DE")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "EP")
				(number "15")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "A")
				(number "12")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{B}")
				(number "11")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "Y")
				(number "9")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{Z}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX14783ExS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.096 11.43 0)
		)
		(property "Value" "MAX14783ExS"
			(at 0.762 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX14783E.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "High-Speed 3.3V/5V RS-485/RS-422 Transceiver with ±35kV HBM ESD Protection, SOIC8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed 3.3V/5V RS-485/RS-422 Transceiver ESD 42Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX14783ExS_0_1")
		(symbol "MAX14783ExS_1_1"
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RO")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{RE}")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DE")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX14830"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 46.99 0)
		)
		(property "Value" "MAX14830"
			(at 8.89 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:TQFN-48-1EP_7x7mm_P0.5mm_EP5.1x5.1mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX14830.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad UART with I2C/SPI interface, 128 Word FIFOs, IrDA SIR built-in support, TQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART I2C/SPI 128W FIFO IrDA SIR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAX14830_0_1")
		(symbol "MAX14830_1_1"
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "LDOEN")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SPI/~{I2C}")
				(number "1")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "MOSI/A1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "MISO/SDA")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "~{CS}/A0")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SCLK/SCL")
				(number "4")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "~{RST}")
				(number "8")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "7")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "XOUT")
				(number "44")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "XIN")
				(number "45")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 2.54)
				(name "VL")
				(number "9")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VA")
				(number "47")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VEXT")
				(number "43")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "AGND")
				(number "46")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "49")
			)
			(pin power_out line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "V18")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "DGND")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "GPIO0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "GPIO1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "GPIO2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "GPIO3")
				(number "14")
			)
			(pin input line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "RX0")
				(number "17")
			)
			(pin input line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "~{CTS0}")
				(number "16")
			)
			(pin output line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "~{RTS0}")
				(number "15")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "TX0")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "GPIO4")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "GPIO5")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "GPIO6")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "GPIO7")
				(number "22")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "RX1")
				(number "25")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "~{CTS1}")
				(number "24")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "~{RTS1}")
				(number "23")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "TX1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "GPIO8")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "GPIO9")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "GPIO10")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GPIO11")
				(number "30")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "RX2")
				(number "33")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{CTS2}")
				(number "32")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "~{RTS2}")
				(number "31")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "TX2")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "GPIO12")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "GPIO13")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "GPIO14")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "GPIO15")
				(number "38")
			)
			(pin input line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "RX3")
				(number "41")
			)
			(pin input line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "~{CTS3}")
				(number "40")
			)
			(pin output line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "~{RTS3}")
				(number "39")
			)
			(pin output line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "TX3")
				(number "42")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX232"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 28.575 0)
		)
		(property "Value" "MAX232"
			(at -2.54 26.67 0)
		)
		(property "Footprint" ""
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/max232.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Dual RS232 driver/receiver, 5V supply, 120kb/s, 0C-70C"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver line-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX232_0_0"
			(text "LOGIC"
				(at -11.43 -22.86 0)
			)
			(text "RS232"
				(at 11.43 -22.86 0)
			)
		)
		(symbol "MAX232_0_1")
		(symbol "MAX232_1_1"
			(pin passive line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "C1+")
				(number "1")
			)
			(pin passive line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "C1-")
				(number "3")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "T1IN")
				(number "11")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "T2IN")
				(number "10")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "R1OUT")
				(number "12")
			)
			(pin output line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "R2OUT")
				(number "9")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 5.08)
				(name "VCC")
				(number "16")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 5.08)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "C2+")
				(number "4")
			)
			(pin passive line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "C2-")
				(number "5")
			)
			(pin power_out line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "VS+")
				(number "2")
			)
			(pin power_out line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "VS-")
				(number "6")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "T1OUT")
				(number "14")
			)
			(pin output line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "T2OUT")
				(number "7")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "R1IN")
				(number "13")
			)
			(pin input line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "R2IN")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX238xWG+"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.858 41.148 0)
		)
		(property "Value" "MAX238xWG+"
			(at -2.54 39.37 0)
		)
		(property "Footprint" "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 1.27 -39.37 0)
		)
		(property "Datasheet" "https://eu.mouser.com/datasheet/2/609/MAX220_MAX249-3127785.pdf"
			(at 0 -36.83 0)
		)
		(property "Description" "Quad RS232 driver/receiver, 5V supply, 120kb/s, SOIC-24W"
			(at 0 12.7 0)
		)
		(property "ki_keywords" "rs232 uart transceiver line-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX238xWG+_0_0"
			(text "LOGIC"
				(at -11.43 -35.56 0)
			)
			(text "RS232"
				(at 11.43 -35.56 0)
			)
		)
		(symbol "MAX238xWG+_0_1")
		(symbol "MAX238xWG+_1_1"
			(pin passive line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "C1+")
				(number "10")
			)
			(pin passive line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "C1-")
				(number "12")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "T1IN")
				(number "5")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "T2IN")
				(number "18")
			)
			(pin input line
				(at -20.32 0 0)
				(length 5.08)
				(name "T1IN")
				(number "19")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "T2IN")
				(number "21")
			)
			(pin output line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "R1OUT")
				(number "6")
			)
			(pin output line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "R2OUT")
				(number "4")
			)
			(pin output line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "R1OUT")
				(number "22")
			)
			(pin output line
				(at -20.32 -25.4 0)
				(length 5.08)
				(name "R2OUT")
				(number "17")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 5.08)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "C2+")
				(number "13")
			)
			(pin passive line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "C2-")
				(number "14")
			)
			(pin power_out line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "VS+")
				(number "11")
			)
			(pin power_out line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "VS-")
				(number "15")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "T1OUT")
				(number "2")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "T2OUT")
				(number "1")
			)
			(pin output line
				(at 20.32 0 180)
				(length 5.08)
				(name "T1OUT")
				(number "24")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "T2OUT")
				(number "20")
			)
			(pin input line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "R1IN")
				(number "7")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "R2IN")
				(number "3")
			)
			(pin input line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "R1IN")
				(number "23")
			)
			(pin input line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "R2IN")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX3051"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "MAX3051"
			(at 2.54 8.89 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://datasheets.maximintegrated.com/en/ds/MAX3051.pdf"
			(at 0 0 0)
		)
		(property "Description" "High-Speed CAN Transceiver, 1Mbps, 3.3V supply"
			(at 0 0 0)
		)
		(property "ki_keywords" "High-Speed CAN Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23* SOIC*"
			(at 0 0 0)
		)
		(symbol "MAX3051_0_1")
		(symbol "MAX3051_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SHDN")
				(number "5")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RS")
				(number "8")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "CANH")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CANL")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX3218"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "MAX3218"
			(at 12.7 24.13 0)
		)
		(property "Footprint" ""
			(at 1.27 -21.59 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX3218.pdf"
			(at -3.81 5.08 0)
		)
		(property "Description" "Dual RS-232 Transceiver, 1.8V to 4.25V, AutoShutdown, DIP-20/SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "1μA Supply Current"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX3218_0_1")
		(symbol "MAX3218_1_1"
			(pin passive line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "C1+")
				(number "18")
			)
			(pin passive line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "C1-")
				(number "16")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "T1IN")
				(number "7")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "T2IN")
				(number "8")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "R1OUT")
				(number "9")
			)
			(pin output line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "R2OUT")
				(number "10")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "FORCEON")
				(number "3")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "~{FORCEOFF}")
				(number "4")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin passive line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "LX")
				(number "1")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "V+")
				(number "19")
			)
			(pin power_out line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "V-")
				(number "15")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "T1OUT")
				(number "14")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "T2OUT")
				(number "13")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "R1IN")
				(number "12")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "R2IN")
				(number "11")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{INVALID}")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX3221"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 21.59 0)
		)
		(property "Value" "MAX3221"
			(at 12.7 21.59 0)
		)
		(property "Footprint" ""
			(at 1.27 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/max3221.pdf"
			(at 0 24.13 0)
		)
		(property "Description" "RS232 transceiver with 15kV ESD protection"
			(at 0 0 0)
		)
		(property "ki_keywords" "serial UART RS232"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP* TSSOP*"
			(at 0 0 0)
		)
		(symbol "MAX3221_0_1")
		(symbol "MAX3221_1_1"
			(pin passive line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "C1+")
				(number "2")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "C1-")
				(number "4")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "C2+")
				(number "5")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "C2-")
				(number "6")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "DIN")
				(number "11")
			)
			(pin output line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "ROUT")
				(number "9")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "~{EN}")
				(number "1")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "FORCEON")
				(number "12")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin power_out line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "V+")
				(number "3")
			)
			(pin power_out line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "V-")
				(number "7")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DOUT")
				(number "13")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "RIN")
				(number "8")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{INVALID}")
				(number "10")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "~{FORCEOFF}")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX3226"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 26.67 0)
		)
		(property "Value" "MAX3226"
			(at 12.7 26.67 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_5.3x6.2mm_P0.65mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX3224-MAX3245.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Single RS232 driver/receiver, 3.0V to 5V supply, 250kb/s, AutoShutdown Plus, SSOP-16 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x6.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MAX3226_0_0"
			(text "LOGIC"
				(at -11.43 -22.86 0)
			)
			(text "RS232"
				(at 11.43 -22.86 0)
			)
		)
		(symbol "MAX3226_0_1")
		(symbol "MAX3226_1_1"
			(pin passive line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "C1+")
				(number "2")
			)
			(pin passive line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "C1-")
				(number "4")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "T1IN")
				(number "11")
			)
			(pin output line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "R1OUT")
				(number "9")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "FORCEON")
				(number "12")
			)
			(pin input line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "~{FORCEOFF}")
				(number "16")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 5.08)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 5.08)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "C2+")
				(number "5")
			)
			(pin passive line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "C2-")
				(number "6")
			)
			(pin power_out line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "V+")
				(number "3")
			)
			(pin power_out line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "V-")
				(number "7")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "T1OUT")
				(number "13")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "R1IN")
				(number "8")
			)
			(pin output line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "READY")
				(number "1")
			)
			(pin output line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "~{INVALID}")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX3284E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 8.89 0)
		)
		(property "Value" "MAX3284E"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX3280E-MAX3284E.pdf"
			(at -0.254 -1.27 0)
		)
		(property "Description" "±15kV ESD-Protected 52Mbps, 3V to 5.5V RS-485/RS-422 True Fail-Safe Receivers, SOT23"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS-485 RS-422 True Fail-Safe Receivers 1/4 unit load receiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "MAX3284E_0_1")
		(symbol "MAX3284E_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "B")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VL")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "RO")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX489E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.096 11.43 0)
		)
		(property "Value" "MAX489E"
			(at 0.762 11.43 0)
		)
		(property "Footprint" ""
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1487E-MAX491E.pdf"
			(at 1.27 0.635 0)
		)
		(property "Description" "Full duplex RS-485/RS-422, 0.25 Mbps, ±15kV electro-static discharge (ESD) protection, slew-rate limited, no low-power shutdown, with with receiver/driver enable, 32 receiver drive capability, 0 to +70 degree Celsius, DIP-14 and SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MAX489E_0_1")
		(symbol "MAX489E_1_1"
			(pin output line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "RO")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "~{RE}")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DE")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DI")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at 7.62 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "A")
				(number "12")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "B")
				(number "11")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "10")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "Y")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC6850"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.366 31.75 0)
		)
		(property "Value" "MC6850"
			(at 10.414 31.75 0)
		)
		(property "Footprint" "Package_DIP:DIP-24_W15.24mm"
			(at 1.27 -29.21 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC6850.pdf"
			(at 0 0 0)
		)
		(property "Description" "Asynchronous Communications Interface Adapter 1MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "ACIA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "MC6850_1_1"
			(pin bidirectional line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "D0")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 25.4 0)
				(length 2.54)
				(name "D1")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "D2")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D3")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D4")
				(number "18")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D5")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D6")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D7")
				(number "15")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "R/~{W}")
				(number "13")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "RS")
				(number "11")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "CS0")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "CS1")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CS2")
				(number "9")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "E")
				(number "14")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "Rx_CLK")
				(number "3")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "Tx_CLK")
				(number "4")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "Rx_Data")
				(number "2")
			)
			(pin input line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "~{DCD}")
				(number "23")
			)
			(pin input line
				(at -12.7 -25.4 0)
				(length 2.54)
				(name "~{CTS}")
				(number "24")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin output line
				(at 10.16 22.86 180)
				(length 2.54)
				(name "~{IRQ}")
				(number "7")
			)
			(pin output line
				(at 10.16 -20.32 180)
				(length 2.54)
				(name "Tx_Data")
				(number "6")
			)
			(pin output line
				(at 10.16 -22.86 180)
				(length 2.54)
				(name "~{RTS}")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SC16IS740"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "SC16IS740"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SC16IS740_750_760.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Single UART with I2C/SPI interface, 64 bytes of transmit and receive FIFOs, IrDA SIR built-in support, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART I2C/SPI 64B FIFO IrDA SIR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SC16IS740_0_1")
		(symbol "SC16IS740_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "~{RESET}")
				(number "14")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "I2C/~{SPI}")
				(number "8")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A0/~{CS}")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A1/SI")
				(number "3")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "SO")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCL/SCLK")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SDA")
				(number "6")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "XTAL1")
				(number "15")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "XTAL2")
				(number "16")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "RX")
				(number "13")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{CTS}")
				(number "11")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{RTS}")
				(number "10")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "TX")
				(number "12")
			)
			(pin open_collector line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{IRQ}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SC16IS750xBS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 21.59 0)
		)
		(property "Value" "SC16IS750xBS"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:HVQFN-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SC16IS740_750_760.pdf"
			(at -2.54 3.81 0)
		)
		(property "Description" "Single UART with I2C/SPI interface, 64 bytes of transmit and receive FIFOs, IrDA SIR built-in support, HVQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART I2C/SPI 64B FIFO IrDA SIR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SC16IS750xBS_0_1")
		(symbol "SC16IS750xBS_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "I2C/~{SPI}")
				(number "5")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "A0/~{CS}")
				(number "6")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "A1/SI")
				(number "7")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SO")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCL/SCLK")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "SDA")
				(number "10")
			)
			(pin open_collector line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "11")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "XTAL1")
				(number "2")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "XTAL2")
				(number "3")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "GPIO0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "GPIO1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "GPIO2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "GPIO3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "GPIO4/~{DSR}")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "GPIO5/~{DTR}")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "GPIO6/~{CD}")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "GPIO7/~{RI}")
				(number "20")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "RX")
				(number "24")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{CTS}")
				(number "22")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RTS}")
				(number "21")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "TX")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SC16IS750xPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 21.59 0)
		)
		(property "Value" "SC16IS750xPW"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SC16IS740_750_760.pdf"
			(at 53.34 8.89 0)
		)
		(property "Description" "Single UART with I2C/SPI interface, 64 bytes of transmit and receive FIFOs, IrDA SIR built-in support, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART I2C/SPI 64B FIFO IrDA SIR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SC16IS750xPW_0_1")
		(symbol "SC16IS750xPW_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "I2C/~{SPI}")
				(number "8")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "A0/~{CS}")
				(number "9")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "A1/SI")
				(number "10")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SO")
				(number "11")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SCL/SCLK")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "SDA")
				(number "13")
			)
			(pin open_collector line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "14")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "XTAL1")
				(number "5")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "XTAL2")
				(number "6")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "GPIO0")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "GPIO1")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "GPIO2")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "GPIO3")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "GPIO4/~{DSR}")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "GPIO5/~{DTR}")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "GPIO6/~{CD}")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "GPIO7/~{RI}")
				(number "23")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "RX")
				(number "3")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{CTS}")
				(number "1")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RTS}")
				(number "24")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "TX")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SC16IS752IBS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "SC16IS752IBS"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SC16IS752_SC16IS762.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Dual UART with I2C/SPI interface, 64 bytes of transmit and receive FIFOs, IrDA SIR built-in support, HVQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART I2C/SPI 64B FIFO IrDA SIR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SC16IS752IBS_0_1")
		(symbol "SC16IS752IBS_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "2")
			)
			(pin open_collector line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "14")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "A0/~{CS}")
				(number "7")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A1/SI")
				(number "8")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "n.c./SO")
				(number "9")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SCL/SCLK")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SDA/VSS")
				(number "11")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "I2C/~{SPI}")
				(number "6")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "XTAL1")
				(number "3")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "XTAL2")
				(number "4")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "13")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "12")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "21")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "29")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "GPIO7/~{RIA}")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "GPIO6/~{CDA}")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "GPIO5/~{DTRA}")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "GPIO4/~{DSRA}")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "GPIO3/~{RIB}")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "GPIO2/~{CDB}")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "GPIO1/~{DTRB}")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "GPIO0/~{DSRB}")
				(number "17")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "TXA")
				(number "32")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RXA")
				(number "1")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RTSA}")
				(number "30")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "~{CTSA}")
				(number "31")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "TXB")
				(number "22")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RXB")
				(number "23")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "~{RTSB}")
				(number "16")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "~{CTSB}")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SC16IS752IPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "SC16IS752IPW"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 0 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SC16IS752_SC16IS762.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Dual UART with I2C/SPI interface, 64 bytes of transmit and receive FIFOs, IrDA SIR built-in support, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART I2C/SPI 64B FIFO IrDA SIR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SC16IS752IPW_0_1")
		(symbol "SC16IS752IPW_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "5")
			)
			(pin open_collector line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{IRQ}")
				(number "15")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "A0/~{CS}")
				(number "10")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "A1/SI")
				(number "11")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "n.c./SO")
				(number "12")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "SCL/SCLK")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "SDA/VSS")
				(number "14")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "I2C/~{SPI}")
				(number "9")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "XTAL1")
				(number "6")
			)
			(pin output line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "XTAL2")
				(number "7")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "GPIO7/~{RIA}")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "GPIO6/~{CDA}")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "GPIO5/~{DTRA}")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "GPIO4/~{DSRA}")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "GPIO3/~{RIB}")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "GPIO2/~{CDB}")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "GPIO1/~{DTRB}")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "GPIO0/~{DSRB}")
				(number "18")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "TXA")
				(number "3")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RXA")
				(number "4")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RTSA}")
				(number "1")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "~{CTSA}")
				(number "2")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "TXB")
				(number "23")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RXB")
				(number "24")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "~{RTSB}")
				(number "17")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "~{CTSB}")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN65HVD11HD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 12.7 0)
		)
		(property "Value" "SN65HVD11HD"
			(at 2.54 12.7 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn65hvd11-ht.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "3.3V, RS-485 Transceiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs485 transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN65HVD11HD_0_1")
		(symbol "SN65HVD11HD_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "R")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~{RE}")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DE")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN75LBC176D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.318 8.89 0)
		)
		(property "Value" "SN75LBC176D"
			(at 1.016 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75lbc176.pdf"
			(at 40.64 -5.08 0)
		)
		(property "Description" "Differential bus transceiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Differential bus transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "SN75LBC176D_0_1")
		(symbol "SN75LBC176D_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "DE")
				(number "3")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{RE}")
				(number "2")
			)
			(pin output line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "R")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "B")
				(number "7")
			)
			(pin bidirectional line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN75LBC176P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.318 8.89 0)
		)
		(property "Value" "SN75LBC176P"
			(at 1.016 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75lbc176.pdf"
			(at 40.64 -5.08 0)
		)
		(property "Description" "Differential bus transceiver, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Differential bus transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SN75LBC176P_0_1")
		(symbol "SN75LBC176P_1_1"
			(pin input line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "DE")
				(number "3")
			)
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~{RE}")
				(number "2")
			)
			(pin output line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "R")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "B")
				(number "7")
			)
			(pin bidirectional line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THVD1451D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "THVD1451D"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/thvd1451.pdf"
			(at 0 0 0)
		)
		(property "Description" "RS485 transceiver, 3.3-V to 5-V, 18-kV IEC ESD Protection, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs485 transceiver line driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "THVD1451D_0_1")
		(symbol "THVD1451D_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "R")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "D")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "Z")
				(number "6")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "Y")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "THVD8000"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "THVD8000"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-8"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/thvd8000.pdf"
			(at -1.27 -1.27 0)
		)
		(property "Description" "RS-485 500 kbps Transceiver with OOK Modulation for Power Line Communication, 3V-5.5V supply, -7 to +12V common mode range, SOT-23-8"
			(at 0.635 1.27 0)
		)
		(property "ki_keywords" "RS485 half-duplex power-line-communication PLC powerline"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "THVD8000_0_1")
		(symbol "THVD8000_1_1"
			(pin output line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "R")
				(number "1")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "MODE")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "D")
				(number "4")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "F_SET")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Z8530"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 35.56 0)
		)
		(property "Value" "Z8530"
			(at 10.16 35.56 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "SCC Serial Communication Controller, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "SCC Serial Communication"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "Z8530_0_1")
		(symbol "Z8530_1_1"
			(pin input line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "D0")
				(number "40")
			)
			(pin input line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "D1")
				(number "1")
			)
			(pin input line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "D2")
				(number "39")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "D3")
				(number "2")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "D4")
				(number "38")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "D5")
				(number "3")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "D6")
				(number "37")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "D7")
				(number "4")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "~{RD}")
				(number "36")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "~{WR}")
				(number "35")
			)
			(pin input line
				(at -20.32 0 0)
				(length 3.81)
				(name "~{CE}")
				(number "33")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "A/~{B}")
				(number "34")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "D/~{C}")
				(number "32")
			)
			(pin open_collector line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "~{INT}")
				(number "5")
			)
			(pin output line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "IEO")
				(number "6")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "IEI")
				(number "7")
			)
			(pin input line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "~{INTACK}")
				(number "8")
			)
			(pin input clock
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "PCLK")
				(number "20")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "31")
			)
			(pin output line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "TXDA")
				(number "15")
			)
			(pin input line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "RXDA")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "~{TRXCA}")
				(number "14")
			)
			(pin input line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "~{RTXCA}")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "~{SYNCA}")
				(number "11")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "~{W/REQA}")
				(number "10")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "~{DTR/REQA}")
				(number "16")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "~{RTSA}")
				(number "17")
			)
			(pin input line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "~{CTSA}")
				(number "18")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "~{DCDA}")
				(number "19")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "TXDB")
				(number "25")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "RXDB")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "~{TRXCB}")
				(number "26")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "~{RTXCB}")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "~{SYNCB}")
				(number "29")
			)
			(pin output line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "~{W/REQB}")
				(number "30")
			)
			(pin output line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "~{DTR/REQB}")
				(number "24")
			)
			(pin output line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "~{RTSB}")
				(number "23")
			)
			(pin input line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "~{CTSB}")
				(number "22")
			)
			(pin input line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "~{DCDB}")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8250"
		(extends "16450")
		(property "Reference" "U"
			(at -21.59 40.64 0)
		)
		(property "Value" "8250"
			(at 15.24 40.64 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "PC8250A, Universal Asynchronous Receiver/Transmitter, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "1ch UART"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADM222"
		(extends "LT1080")
		(property "Reference" "U"
			(at -13.97 26.67 0)
		)
		(property "Value" "ADM222"
			(at 12.7 26.67 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM222_232A_242.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Dual RS232 driver/receiver, 5V supply, 200kb/s"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO* DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADM232A"
		(extends "MAX232")
		(property "Reference" "U"
			(at -2.54 28.575 0)
		)
		(property "Value" "ADM232A"
			(at -2.54 26.67 0)
		)
		(property "Footprint" ""
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM222_232A_242.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Dual RS232 driver/receiver, 5V supply, 200kb/s"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver line-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADM2582E"
		(extends "ADM2587E")
		(property "Reference" "U"
			(at 0 21.59 0)
		)
		(property "Value" "ADM2582E"
			(at 0 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "www.analog.com/media/en/technical-documentation/data-sheets/ADM2582E_2587E.pdf"
			(at -20.32 0 0)
		)
		(property "Description" "Isolated RS485/RS422 Transceiver,Integrated Isolated DC-DC Converter, 16Mbps,SO-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 Transceiver,RS422 Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADM2687E"
		(extends "ADM2682E")
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "ADM2687E"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x12.8mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM2682E_2687E.pdf"
			(at 0 18.415 0)
		)
		(property "Description" "Isolated RS485/RS422 Transceiver, Integrated Isolated DC-DC Converter, 500kbps, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 Transceiver, RS422 Transceiver, Isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADM3488ExR"
		(extends "ADM3490ExR")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "ADM3488ExR"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM3483E_3486E_3488E_3490E_3491E.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 full duplex 250 kbps transceiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADM3491ExR"
		(extends "ADM1491EBR")
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "ADM3491ExR"
			(at -11.43 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADM3483E_3486E_3488E_3490E_3491E.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 full duplex 12 Mbps transceiver, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AZ75232G"
		(extends "AZ75232M")
		(property "Reference" "U"
			(at 15.24 29.21 0)
		)
		(property "Value" "AZ75232G"
			(at 15.24 26.67 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ75232.pdf"
			(at 63.5 3.81 0)
		)
		(property "Description" "RS232 interface IC, 3 drivers, 5 receivers, 3.3V/5V Vcc supply, bipolar Vdd/Vss supply, 120kb/s, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver line-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AZ75232GS"
		(extends "AZ75232M")
		(property "Reference" "U"
			(at 15.24 29.21 0)
		)
		(property "Value" "AZ75232GS"
			(at 15.24 26.67 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AZ75232.pdf"
			(at 63.5 3.81 0)
		)
		(property "Description" "RS232 interface IC, 3 drivers, 5 receivers, 3.3V/5V Vcc supply, bipolar Vdd/Vss supply, 120kb/s, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver line-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "GD65232DB"
		(extends "AZ75232M")
		(property "Reference" "U"
			(at 8.89 29.21 0)
		)
		(property "Value" "GD65232DB"
			(at 3.81 26.67 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/gd75232.pdf"
			(at -12.7 0 0)
		)
		(property "Description" "Multiple RS-232 Driver and Receiver, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS232 UART Driver Receiver Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "GD65232DW"
		(extends "AZ75232M")
		(property "Reference" "U"
			(at 8.89 29.21 0)
		)
		(property "Value" "GD65232DW"
			(at 3.81 26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/gd75232.pdf"
			(at -12.7 0 0)
		)
		(property "Description" "Multiple RS-232 Driver and Receiver, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS232 UART Driver Receiver Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "GD65232PW"
		(extends "AZ75232M")
		(property "Reference" "U"
			(at 8.89 29.21 0)
		)
		(property "Value" "GD65232PW"
			(at 3.81 26.67 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/gd75232.pdf"
			(at -12.7 0 0)
		)
		(property "Description" "Multiple RS-232 Driver and Receiver, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS232 UART Driver Receiver Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "GD75232DB"
		(extends "AZ75232M")
		(property "Reference" "U"
			(at 8.89 29.21 0)
		)
		(property "Value" "GD75232DB"
			(at 3.81 26.67 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/gd75232.pdf"
			(at -12.7 0 0)
		)
		(property "Description" "Multiple RS-232 Driver and Receiver, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS232 UART Driver Receiver Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "GD75232DW"
		(extends "AZ75232M")
		(property "Reference" "U"
			(at 8.89 29.21 0)
		)
		(property "Value" "GD75232DW"
			(at 3.81 26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/gd75232.pdf"
			(at -12.7 0 0)
		)
		(property "Description" "Multiple RS-232 Driver and Receiver, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS232 UART Driver Receiver Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "GD75232N"
		(extends "AZ75232M")
		(property "Reference" "U"
			(at 7.62 29.21 0)
		)
		(property "Value" "GD75232N"
			(at 3.81 26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/gd75232.pdf"
			(at -12.7 0 0)
		)
		(property "Description" "Multiple RS-232 Driver and Receiver, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS232 UART Driver Receiver Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "GD75232PW"
		(extends "AZ75232M")
		(property "Reference" "U"
			(at 8.89 29.21 0)
		)
		(property "Value" "GD75232PW"
			(at 3.81 26.67 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/gd75232.pdf"
			(at -12.7 0 0)
		)
		(property "Description" "Multiple RS-232 Driver and Receiver, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS232 UART Driver Receiver Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "ICL3232"
		(extends "MAX232")
		(property "Reference" "U"
			(at -2.54 28.575 0)
		)
		(property "Value" "ICL3232"
			(at -2.54 26.67 0)
		)
		(property "Footprint" ""
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "http://www.intersil.com/content/dam/Intersil/documents/icl3/icl3221-22-23-32-41-43.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "3.0V to 5.5V, Low-Power, up to 250kbps, True RS-232 Transceivers Using Four 0.1μF External Capacitors"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver line-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISL3172E"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "ISL3172E"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.renesas.com/en/document/dst/isl3170e-isl3171e-isl3172e-isl3173e-isl3174e-isl3175e-isl3176e-isl3177e-isl3178e-datasheet"
			(at 0 -27.94 0)
		)
		(property "Description" "250kbps, 3.3V RS-485 transceiver, ±15-kV IEC ESD protection, -7V..+12V common mode voltage, slew-rate limit, SO-8"
			(at 2.54 -25.4 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half-duplex renesas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISL3175E"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "ISL3175E"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.renesas.com/en/document/dst/isl3170e-isl3171e-isl3172e-isl3173e-isl3174e-isl3175e-isl3176e-isl3177e-isl3178e-datasheet"
			(at 0 -27.94 0)
		)
		(property "Description" "500kbps, 3.3V RS-485 transceiver, ±15-kV IEC ESD protection, -7V..+12V common mode voltage, slew-rate limit, SO-8"
			(at 2.54 -25.4 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half-duplex renesas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISL3178E"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "ISL3178E"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.renesas.com/en/document/dst/isl3170e-isl3171e-isl3172e-isl3173e-isl3174e-isl3175e-isl3176e-isl3177e-isl3178e-datasheet"
			(at 0 -27.94 0)
		)
		(property "Description" "20Mbps, 3.3V RS-485 transceiver, ±15-kV IEC ESD protection, -7V..+12V common mode voltage, SO-8"
			(at 2.54 -25.4 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half-duplex renesas"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISO3088DW"
		(extends "ISO3082DW")
		(property "Reference" "U"
			(at 0 19.05 0)
		)
		(property "Value" "ISO3088DW"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/iso3082.pdf"
			(at -5.08 -19.05 0)
		)
		(property "Description" "20 Mbps, Isolated 5-V Half-Duplex RS-485 transceiver, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS-485"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1785AxS8"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LT1785AxS8"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1785-1785A-1791-1791A.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Half duplex 250kbps transceiver, fail-safe receiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1785xN8"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LT1785xN8"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1785-1785A-1791-1791A.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Half duplex 250kbps transceiver, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1785xS8"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LT1785xS8"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1785-1785A-1791-1791A.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Half duplex 250kbps transceiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1791AxN8"
		(extends "LT1791xN8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LT1791AxN8"
			(at 6.985 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1785-1785A-1791-1791A.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 250kbps transceiver, fail-safe receiver, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1791AxS"
		(extends "LTC2852xS")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LT1791AxS"
			(at 6.985 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1785-1785A-1791-1791A.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 250kbps transceiver, fail-safe receiver, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1791xS"
		(extends "LTC2852xS")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LT1791xS"
			(at 6.985 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1785-1785A-1791-1791A.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 250kbps transceiver, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2850xMS8"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2850xMS8"
			(at 8.255 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285012fe.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Half duplex 20Mbps transceiver, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2856xDD-1"
		(extends "LTC2850xDD")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2856xDD-1"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285678fg.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Half duplex 20Mbps transceiver, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2856xDD-2"
		(extends "LTC2850xDD")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2856xDD-2"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285678fg.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Half duplex 250kbps transceiver, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2857xDD-1"
		(extends "LTC2851xDD")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2857xDD-1"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285678fg.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 250kbps transceiver, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2857xDD-2"
		(extends "LTC2851xDD")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2857xDD-2"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x3mm_P0.5mm_EP1.66x2.38mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285012fe.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 250kbps transceiver, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2857xMS8-1"
		(extends "LTC2851xMS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2857xMS8-1"
			(at 8.255 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285678fg.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 20Mbps transceiver, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2857xMS8-2"
		(extends "LTC2851xMS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2857xMS8-2"
			(at 8.255 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285678fg.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 250kbps transceiver, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2858xDD-1"
		(extends "LTC2852xDD")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2858xDD-1"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285678fg.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 20Mbps transceiver, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2858xDD-2"
		(extends "LTC2852xDD")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2858xDD-2"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.65x2.38mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285678fg.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 250kbps transceiver, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2858xMS-1"
		(extends "LTC2852xMS")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2858xMS-1"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285678fg.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 20Mbps transceiver, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2858xMS-2"
		(extends "LTC2852xMS")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2858xMS-2"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285678fg.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Full duplex 250kbps transceiver, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver full duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX13433EESD"
		(extends "MAX13432EESD")
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "MAX13433EESD"
			(at 2.54 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -25.4 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX13430E-MAX13433E.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "RS485 transceiver, full duplex, dual supply, receiver/driver enable, 16Mbps, SOIC-14 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs485 transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX13433EETD"
		(extends "MAX13432EETD")
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "MAX13433EETD"
			(at 2.54 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-14-1EP_3x3mm_P0.4mm_EP1.78x2.35mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX13430E-MAX13433E.pdf"
			(at 0 20.32 0)
		)
		(property "Description" "RS485 transceiver, full duplex, dual supply, receiver/driver enable, 16Mbps, DFN-14 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs485 transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX202"
		(extends "MAX232")
		(property "Reference" "U"
			(at -2.54 28.575 0)
		)
		(property "Value" "MAX202"
			(at -2.54 26.67 0)
		)
		(property "Footprint" ""
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/max202.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Dual RS232 driver/receiver, 5V supply, 120kb/s, 0C-70C"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver line-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX232I"
		(extends "MAX232")
		(property "Reference" "U"
			(at -2.54 28.575 0)
		)
		(property "Value" "MAX232I"
			(at -2.54 26.67 0)
		)
		(property "Footprint" ""
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/max232.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Dual RS232 driver/receiver, 5V supply, 120kb/s, -40C-80C"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver line-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX238xNG+"
		(extends "MAX238xWG+")
		(property "Reference" "U"
			(at -6.858 41.148 0)
		)
		(property "Value" "MAX238xNG+"
			(at -2.54 39.37 0)
		)
		(property "Footprint" "Package_DIP:DIP-24_W7.62mm"
			(at 1.27 -39.37 0)
		)
		(property "Datasheet" "https://eu.mouser.com/datasheet/2/609/MAX220_MAX249-3127785.pdf"
			(at 0 -36.83 0)
		)
		(property "Description" "Quad RS232 driver/receiver, 5V supply, 120kb/s, DIP-24"
			(at 0 12.7 0)
		)
		(property "ki_keywords" "rs232 uart transceiver line-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX3072E"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "MAX3072E"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 26.67 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX3070E-MAX3079E.pdf"
			(at 0 0 0)
		)
		(property "Description" "+3.3V, ±15kV ESD-Protected, Fail-Safe, Hot-Swap, RS-485/RS-422 Transceivers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power Half-Duplex RS-485 RS-422 Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX3227"
		(extends "MAX3226")
		(property "Reference" "U"
			(at -13.97 26.67 0)
		)
		(property "Value" "MAX3227"
			(at 12.7 26.67 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_5.3x6.2mm_P0.65mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX3224-MAX3245.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "Single RS232 driver/receiver, 3.0V to 5V supply, 1Mb/s, AutoShutdown Plus, SSOP-16 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x6.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX3232"
		(extends "MAX232")
		(property "Reference" "U"
			(at -2.54 28.575 0)
		)
		(property "Value" "MAX3232"
			(at -2.54 26.67 0)
		)
		(property "Footprint" ""
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX3222-MAX3241.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "3.0V to 5.5V, Low-Power, up to 1Mbps, True RS-232 Transceivers Using Four 0.1μF External Capacitors"
			(at 0 0 0)
		)
		(property "ki_keywords" "rs232 uart transceiver line-driver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*P1.27mm* DIP*W7.62mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX3485"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "MAX3485"
			(at 1.905 13.97 0)
		)
		(property "Footprint" ""
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX3483-MAX3491.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "True RS-485/RS-422, 10Mbps, Slew-Rate Limited, with low-power shutdown, with receiver/driver enable, 32 receiver drive capacitity, DIP-8 and SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS-485 RS-422 UART line-driver transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX3488xPA"
		(extends "ADM3490ExR")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "MAX3488xPA"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX3483-MAX3491.pdf"
			(at -6.096 11.43 0)
		)
		(property "Description" "Full duplex RS-485/RS-422, 0.25 Mbps, slew-rate limited, no low-power shutdown, no with receiver/driver enable, 32 receiver drive capability, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX3488xSA"
		(extends "ADM3490ExR")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "MAX3488xSA"
			(at 0.762 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX3483-MAX3491.pdf"
			(at -6.096 11.43 0)
		)
		(property "Description" "Full duplex RS-485/RS-422, 0.25 Mbps, slew-rate limited, no low-power shutdown, no with receiver/driver enable, 32 receiver drive capability, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX3490xPA"
		(extends "ADM3490ExR")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "MAX3490xPA"
			(at 0.762 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX3483-MAX3491.pdf"
			(at -6.096 11.43 0)
		)
		(property "Description" "Full duplex RS-485/RS-422, 10 Mbps, slew-rate limited, no low-power shutdown, no with receiver/driver enable, 32 receiver drive capability, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX3490xSA"
		(extends "ADM3490ExR")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "MAX3490xSA"
			(at 0.762 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/MAX3483-MAX3491.pdf"
			(at -6.096 11.43 0)
		)
		(property "Description" "Full duplex RS-485/RS-422, 10Mbps, slew-rate limited, no low-power shutdown, no with receiver/driver enable, 32 receiver drive capability, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX481E"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "MAX481E"
			(at 1.905 13.97 0)
		)
		(property "Footprint" ""
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1487E-MAX491E.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Half duplex RS-485/RS-422, 2.5 Mbps, ±15kV electro-static discharge (ESD) protection, no slew-rate, with low-power shutdown, with receiver/driver enable, 32 receiver drive capability, DIP-8 and SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX488E"
		(extends "ADM3490ExR")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "MAX488E"
			(at 0.762 13.97 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1487E-MAX491E.pdf"
			(at -6.096 11.43 0)
		)
		(property "Description" "Full duplex RS-485/RS-422, 0.25 Mbps, ±15kV electro-static discharge (ESD) protection, slew-rate limited, no low-power shutdown, no with receiver/driver enable, 32 receiver drive capability, 0 to +70 degree Celsius, DIP-8 and SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX490E"
		(extends "ADM3490ExR")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "MAX490E"
			(at 0.762 13.97 0)
		)
		(property "Footprint" ""
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1487E-MAX491E.pdf"
			(at -6.096 11.43 0)
		)
		(property "Description" "Full duplex RS-485/RS-422, 2.5 Mbps, ±15kV electro-static discharge (ESD) protection, no slew-rate limited, no low-power shutdown, no with receiver/driver enable, 32 receiver drive capability, -40 to +85 degree Celsius, DIP-8 and SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX491E"
		(extends "MAX489E")
		(property "Reference" "U"
			(at -6.096 11.43 0)
		)
		(property "Value" "MAX491E"
			(at 0.762 11.43 0)
		)
		(property "Footprint" ""
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1487E-MAX491E.pdf"
			(at 1.27 0.635 0)
		)
		(property "Description" "Full duplex RS-485/RS-422, 2.5 Mbps, ±15kV electro-static discharge (ESD) protection, no slew-rate limited, no low-power shutdown, with receiver/driver enable, 32 receiver drive capability, 0 to +70 degree Celsius, DIP-14 and SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68A50"
		(extends "MC6850")
		(property "Reference" "U"
			(at -7.366 31.75 0)
		)
		(property "Value" "MC68A50"
			(at 10.414 31.75 0)
		)
		(property "Footprint" "Package_DIP:DIP-24_W15.24mm"
			(at 1.27 -29.21 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC6850.pdf"
			(at 0 0 0)
		)
		(property "Description" "Asynchronous Communications Interface Adapter 1.5MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "ACIA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC68B50"
		(extends "MC6850")
		(property "Reference" "U"
			(at -7.366 31.75 0)
		)
		(property "Value" "MC68B50"
			(at 10.414 31.75 0)
		)
		(property "Footprint" "Package_DIP:DIP-24_W15.24mm"
			(at 1.27 -29.21 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/motorola/MC6850.pdf"
			(at 0 0 0)
		)
		(property "Description" "Asynchronous Communications Interface Adapter 2MHz, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "ACIA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "SC16IS760xBS"
		(extends "SC16IS750xBS")
		(property "Reference" "U"
			(at -11.43 21.59 0)
		)
		(property "Value" "SC16IS760xBS"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:HVQFN-24-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SC16IS740_750_760.pdf"
			(at -2.54 3.81 0)
		)
		(property "Description" "Single UART with I2C/SPI interface, 64 bytes of transmit and receive FIFOs, IrDA SIR built-in support, HVQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART I2C/SPI 64B FIFO IrDA SIR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SC16IS760xPW"
		(extends "SC16IS750xPW")
		(property "Reference" "U"
			(at -11.43 21.59 0)
		)
		(property "Value" "SC16IS760xPW"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SC16IS740_750_760.pdf"
			(at 53.34 8.89 0)
		)
		(property "Description" "Single UART with I2C/SPI interface, 64 bytes of transmit and receive FIFOs, IrDA SIR built-in support, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART I2C/SPI 64B FIFO IrDA SIR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "SC16IS762IBS"
		(extends "SC16IS752IBS")
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "SC16IS762IBS"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SC16IS752_SC16IS762.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Dual UART with I2C/SPI interface, 64 bytes of transmit and receive FIFOs, IrDA SIR built-in support, HVQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART I2C/SPI 64B FIFO IrDA SIR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SC16IS762IPW"
		(extends "SC16IS752IPW")
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "SC16IS762IPW"
			(at 7.62 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 0 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/SC16IS752_SC16IS762.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "Dual UART with I2C/SPI interface, 64 bytes of transmit and receive FIFOs, IrDA SIR built-in support, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART I2C/SPI 64B FIFO IrDA SIR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN65LBC176D"
		(extends "SN75LBC176D")
		(property "Reference" "U"
			(at -4.318 8.89 0)
		)
		(property "Value" "SN65LBC176D"
			(at 1.016 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75lbc176.pdf"
			(at 40.64 -5.08 0)
		)
		(property "Description" "Differential bus transceiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Differential bus transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN65LBC176P"
		(extends "SN75LBC176P")
		(property "Reference" "U"
			(at -4.318 8.89 0)
		)
		(property "Value" "SN65LBC176P"
			(at 1.016 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75lbc176.pdf"
			(at 40.64 -5.08 0)
		)
		(property "Description" "Differential bus transceiver, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Differential bus transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN65LBC176QD"
		(extends "SN75LBC176D")
		(property "Reference" "U"
			(at -4.318 8.89 0)
		)
		(property "Value" "SN65LBC176QD"
			(at 1.016 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75lbc176.pdf"
			(at 40.64 -5.08 0)
		)
		(property "Description" "Differential bus transceiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Differential bus transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN65LBC176QDR"
		(extends "SN75LBC176D")
		(property "Reference" "U"
			(at -4.318 8.89 0)
		)
		(property "Value" "SN65LBC176QDR"
			(at 1.016 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75lbc176.pdf"
			(at 40.64 -5.08 0)
		)
		(property "Description" "Differential bus transceiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Differential bus transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN75176AD"
		(extends "SN75LBC176D")
		(property "Reference" "U"
			(at -4.318 8.89 0)
		)
		(property "Value" "SN75176AD"
			(at 1.016 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75176a.pdf"
			(at 40.64 -5.08 0)
		)
		(property "Description" "Differential RS-422/RS-485 bus transceiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Differential bus transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN75176AP"
		(extends "SN75LBC176P")
		(property "Reference" "U"
			(at -4.318 8.89 0)
		)
		(property "Value" "SN75176AP"
			(at 1.016 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75176a.pdf"
			(at 40.64 -5.08 0)
		)
		(property "Description" "Differential RS-422/RS-485 bus transceiver, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Differential bus transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SNJ55LBC176JG"
		(extends "SN75LBC176P")
		(property "Reference" "U"
			(at -4.318 8.89 0)
		)
		(property "Value" "SNJ55LBC176JG"
			(at 1.016 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn75lbc176.pdf"
			(at 40.64 -5.08 0)
		)
		(property "Description" "Differential bus transceiver, ceramic DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Differential bus transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SP3481CN"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "SP3481CN"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 26.67 -8.89 0)
		)
		(property "Datasheet" "http://www.icbase.com/pdf/SPX/SPX00480106.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V Low Power Half-Duplex RS-485 Transceiver 10Mbps, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power Half-Duplex RS-485 Transceiver 10Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SP3481CP"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "SP3481CP"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.icbase.com/pdf/SPX/SPX00480106.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V Low Power Half-Duplex RS-485 Transceiver 10Mbps, DIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power Half-Duplex RS-485 Transceiver 10Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SP3485CN"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "SP3485CN"
			(at 1.905 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 26.67 -8.89 0)
		)
		(property "Datasheet" "http://www.icbase.com/pdf/SPX/SPX00480106.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V Low Power Half-Duplex RS-485 Transceiver 10Mbps, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power Half-Duplex RS-485 Transceiver 10Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SP3485CP"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "SP3485CP"
			(at 1.905 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.icbase.com/pdf/SPX/SPX00480106.pdf"
			(at 0 0 0)
		)
		(property "Description" "3.3V Low Power Half-Duplex RS-485 Transceiver 10Mbps, DIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power Half-Duplex RS-485 Transceiver 10Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SP3485EN"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "SP3485EN"
			(at 1.905 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 26.67 -8.89 0)
		)
		(property "Datasheet" "http://www.icbase.com/pdf/SPX/SPX00480106.pdf"
			(at 0 0 0)
		)
		(property "Description" "Industrial 3.3V Low Power Half-Duplex RS-485 Transceiver 10Mbps, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power Half-Duplex RS-485 Transceiver 10Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SP3485EP"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "SP3485EP"
			(at 1.905 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.icbase.com/pdf/SPX/SPX00480106.pdf"
			(at 0 0 0)
		)
		(property "Description" "Industrial 3.3V Low Power Half-Duplex RS-485 Transceiver 10Mbps, DIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power Half-Duplex RS-485 Transceiver 10Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SSP3085"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "SSP3085"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.lcsc.com/datasheet/lcsc_datasheet_2404071515_Shanghai-Siproin-Microelectronics-SSP3085_C410986.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Half duplex 500kbps transceiver, 15kV ESD protected, 5V operating voltage, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half duplex Siproin"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ST202ExD"
		(extends "MAX232")
		(property "Reference" "U"
			(at -2.54 28.575 0)
		)
		(property "Value" "ST202ExD"
			(at -2.54 26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/st202eb.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "+/-15 kV ESD-protected 5V powered RS-232 dual transceiver (tx/rx: 2/2), 230kbps, 0.1uF capacitors operation, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART RS232"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*3.9*9.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ST485E"
		(extends "LTC2850xS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "ST485E"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.st.com/resource/en/datasheet/st485eb.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Half duplex RS-485/RS-422, 5 Mbps, ±15kV ESD, 5V supply, 256 bus load, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ST-Microelectronics half-duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LT1785AxN8"
		(extends "LT1785xN8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LT1785AxN8"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/LT1785-1785A-1791-1791A.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Half duplex 250kbps transceiver, fail-safe receiver, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2856xMS8-1"
		(extends "LTC2850xMS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2856xMS8-1"
			(at 8.255 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285678fg.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Half duplex 20Mbps transceiver, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTC2856xMS8-2"
		(extends "LTC2850xMS8")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "LTC2856xMS8-2"
			(at 8.255 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/285678fg.pdf"
			(at -12.7 2.54 0)
		)
		(property "Description" "RS-485, RS-422 Half duplex 250kbps transceiver, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS485 RS422 transceiver half duplex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX1487E"
		(extends "MAX481E")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "MAX1487E"
			(at 1.905 13.97 0)
		)
		(property "Footprint" ""
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1487E-MAX491E.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Half duplex RS-485/RS-422, 2.5 Mbps, ±15kV electro-static discharge (ESD) protection, no slew-rate, no low-power shutdown, with receiver/driver enable, 128 receiver drive capability, DIP-8 and SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX3075E"
		(extends "SP3481CN")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "MAX3075E"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 26.67 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX3070E-MAX3079E.pdf"
			(at 0 0 0)
		)
		(property "Description" "+3.3V, ±15kV ESD-Protected, Fail-Safe, Hot-Swap, RS-485/RS-422 Transceivers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power Half-Duplex RS-485 RS-422 Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX3078E"
		(extends "SP3481CN")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "MAX3078E"
			(at 1.905 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 26.67 -8.89 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX3070E-MAX3079E.pdf"
			(at 0 0 0)
		)
		(property "Description" "+3.3V, ±15kV ESD-Protected, Fail-Safe, Hot-Swap, RS-485/RS-422 Transceivers, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power Half-Duplex RS-485 RS-422 Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX3483"
		(extends "MAX481E")
		(property "Reference" "U"
			(at -6.096 11.43 0)
		)
		(property "Value" "MAX3483"
			(at 0.762 11.43 0)
		)
		(property "Footprint" ""
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX3483-MAX3491.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "True RS-485/RS-422, 0.25Mbps, Slew-Rate Limited, with low-power shutdown, with receiver/driver enable, 32 receiver drive capacitity, DIP-8 and SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS-485 RS-422 UART line-driver transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX3486"
		(extends "MAX481E")
		(property "Reference" "U"
			(at -6.096 11.43 0)
		)
		(property "Value" "MAX3486"
			(at 0.762 11.43 0)
		)
		(property "Footprint" ""
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX3483-MAX3491.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "True RS-485/RS-422, 2.5Mbps, Slew-Rate Limited, with low-power shutdown, with receiver/driver enable, 32 receiver drive capacitity, DIP-8 and SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "RS-485 RS-422 UART line-driver transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX483E"
		(extends "MAX481E")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "MAX483E"
			(at 1.905 13.97 0)
		)
		(property "Footprint" ""
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1487E-MAX491E.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Half duplex RS-485/RS-422, 0.25 Mbps, ±15kV electro-static discharge (ESD) protection, with slew-rate, with low-power shutdown, with receiver/driver enable, 32 receiver drive capability, DIP-8 and SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX485E"
		(extends "MAX481E")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "MAX485E"
			(at 1.905 13.97 0)
		)
		(property "Footprint" ""
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1487E-MAX491E.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Half duplex RS-485/RS-422, 2.5 Mbps, ±15kV electro-static discharge (ESD) protection, no slew-rate, no low-power shutdown, with receiver/driver enable, 32 receiver drive capability, DIP-8 and SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX487E"
		(extends "MAX481E")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "MAX487E"
			(at 1.27 13.97 0)
		)
		(property "Footprint" ""
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1487E-MAX491E.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Half duplex RS-485/RS-422, 0.25 Mbps, ±15kV electro-static discharge (ESD) protection, with slew-rate, with low-power shutdown, with receiver/driver enable, 128 receiver drive capability, DIP-8 and SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SP3481EN"
		(extends "SP3481CN")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "SP3481EN"
			(at 1.905 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 26.67 -8.89 0)
		)
		(property "Datasheet" "http://www.icbase.com/pdf/SPX/SPX00480106.pdf"
			(at 0 0 0)
		)
		(property "Description" "Industrial 3.3V Low Power Half-Duplex RS-485 Transceiver 10Mbps, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power Half-Duplex RS-485 Transceiver 10Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "SP3481EP"
		(extends "SP3481CP")
		(property "Reference" "U"
			(at -7.62 13.97 0)
		)
		(property "Value" "SP3481EP"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.icbase.com/pdf/SPX/SPX00480106.pdf"
			(at 0 0 0)
		)
		(property "Description" "Industrial 3.3V Low Power Half-Duplex RS-485 Transceiver 10Mbps, DIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Low Power Half-Duplex RS-485 Transceiver 10Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ST232ExD"
		(extends "ST202ExD")
		(property "Reference" "U"
			(at -2.54 28.575 0)
		)
		(property "Value" "ST232ExD"
			(at -2.54 26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/st202eb.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "+/-15 kV ESD-protected 5V powered RS-232 dual transceiver (tx/rx: 2/2), 230kbps, 1uF capacitors operation, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "UART RS232"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SO*3.9*9.*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "THVD1400D"
		(extends "MAX481E")
		(property "Reference" "U"
			(at -6.096 11.43 0)
		)
		(property "Value" "THVD1400D"
			(at 0.762 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/thvd1420.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Half duplex RS-485/RS-422, 500 Kbps, 3V - 5.5V supply, ±12kV electro-static discharge (ESD) protection, with receiver/driver enable, 32 receiver drive capacity, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half duplex 3.3V 5V RS-485 RS-422"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "THVD1420D"
		(extends "MAX481E")
		(property "Reference" "U"
			(at -6.096 11.43 0)
		)
		(property "Value" "THVD1420D"
			(at 0.762 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/thvd1420.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Half duplex RS-485/RS-422, 12 Mbps, 3V - 5.5V supply, ±12kV electro-static discharge (ESD) protection, with receiver/driver enable, 32 receiver drive capacity, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half duplex 3.3V 5V RS-485 RS-422"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "THVD1450D"
		(extends "MAX481E")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "THVD1450D"
			(at 1.905 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/thvd1450.pdf"
			(at 0 -33.02 0)
		)
		(property "Description" "3.3-V to 5-V RS-485 transceiver with ±18-kV IEC ESD protection, SOIC-8"
			(at 0 -27.94 0)
		)
		(property "Manufacturer" "Texas Instruments"
			(at 0 0 0)
		)
		(property "ki_keywords" "tranceiver rs485 esd"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "THVD1500"
		(extends "MAX481E")
		(property "Reference" "U"
			(at -6.096 11.43 0)
		)
		(property "Value" "THVD1500"
			(at 0.762 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/thvd1500.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Half duplex RS-485, 500 Kbps, 4.5V - 5.5V supply, ±8kV electro-static discharge (ESD) protection, with receiver/driver enable, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Half duplex 4.5V 5.5V RS-485"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "THVD1450DR"
		(extends "THVD1450D")
		(property "Reference" "U"
			(at -6.985 13.97 0)
		)
		(property "Value" "THVD1450DR"
			(at 1.905 13.97 0)
		)
		(property "Footprint" "Package_SON:VSON-8-1EP_3x3mm_P0.65mm_EP1.6x2.4mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/thvd1450.pdf"
			(at 0 -33.02 0)
		)
		(property "Description" "3.3-V to 5-V RS-485 transceiver with ±18-kV IEC ESD protection, VSON-8"
			(at 0 -27.94 0)
		)
		(property "ki_keywords" "tranceiver rs485 esd"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*VSON*3x3mm*P0.65mm*EP1.6x2.4mm*"
			(at 0 0 0)
		)
	)
)
