(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ADUM4160"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "ADUM4160"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM4160.pdf"
			(at -5.08 0 0)
		)
		(property "Description" "Full/Low Speed, iCoupler USB Digital Isolator, 5kV protection, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb isolation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADUM4160_0_0"
			(text "Logic"
				(at 8.89 -12.065 900)
			)
		)
		(symbol "ADUM4160_0_1")
		(symbol "ADUM4160_1_0"
			(text "USB"
				(at -8.89 -12.065 900)
			)
		)
		(symbol "ADUM4160_1_1"
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "UD+")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "UD-")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PDEN")
				(number "4")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "SPU")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VBUS1")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VBUS2")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "14")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PIN")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DD+")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "DD-")
				(number "11")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SPD")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AP33771"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "AP33771"
			(at 7.62 -19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 0 -31.75 0)
		)
		(property "Datasheet" "https://www.diodes.com/assets/Datasheets/AP33771.pdf"
			(at 0 -34.29 0)
		)
		(property "Description" "USB Type-C PD Sink Controller, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Type C PD Sink"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AP33771_1_1"
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "ISENP")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "CC1")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "CC2")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VSEL0")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "VSEL1")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VSEL2")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PSEL")
				(number "13")
			)
			(pin no_connect line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -10.16 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "5")
			)
			(pin no_connect line
				(at -10.16 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -10.16 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin no_connect line
				(at -7.62 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -7.62 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -7.62 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "24")
			)
			(pin passive line
				(at 0 -20.32 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PWR_EN")
				(number "23")
			)
			(pin power_in line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VBUS")
				(number "22")
			)
			(pin power_out line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "V3VD")
				(number "12")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "V5V")
				(number "20")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VFB")
				(number "14")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "IFB")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "GPIO1")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "GPIO4")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "BQ24392"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "BQ24392"
			(at 5.08 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_R-PUQFN-N10"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/bq24392.pdf"
			(at -12.7 -2.54 0)
		)
		(property "Description" "Dual SPST USB 2.0 High Speed Switch with USB Battery Charging Specification Revision 1.2 Detection, UQFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB BC detector charger"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*R*PUQFN*"
			(at 0 0 0)
		)
		(symbol "BQ24392_0_1")
		(symbol "BQ24392_1_1"
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "DP_CON")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DM_CON")
				(number "8")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VBUS")
				(number "9")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "DP_HOST")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DM_HOST")
				(number "2")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "GOOD_BAT")
				(number "5")
			)
			(pin open_collector line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SW_OPEN")
				(number "1")
			)
			(pin open_collector line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{CHG_AL}")
				(number "4")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "CHG_DET")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH224K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.874 -8.89 0)
		)
		(property "Value" "CH224K"
			(at 3.048 -8.89 0)
		)
		(property "Footprint" "Package_SO:SSOP-10-1EP_3.9x4.9mm_P1mm_EP2.1x3.3mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.wch.cn/downloads/file/301.html"
			(at 0 13.97 0)
		)
		(property "Description" "100W USB Type-C PD3.0/2.0, BC1.2 Sink Controller, SSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB-C WCH powered-device"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P1mm*EP2.1x3.3mm*"
			(at 0 0 0)
		)
		(symbol "CH224K_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CC1")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CC2")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "DM")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DP")
				(number "4")
			)
			(pin passive line
				(at 0 10.16 270)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "PG")
				(number "10")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "CFG1")
				(number "9")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "CFG2")
				(number "2")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "CFG3")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH236D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 20.32 0)
		)
		(property "Value" "CH236D"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm"
			(at 2.54 -20.32 0)
		)
		(property "Datasheet" "https://wch-ic.com/downloads/file/313.html"
			(at -2.54 33.02 0)
		)
		(property "Description" "USB fast charging interface PD2.0/3.0, PPS, BC1.2 , QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB PD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "CH236D_0_1")
		(symbol "CH236D_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{NMOS}")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "UD+")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "UD-")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "CC1")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "CC2")
				(number "11")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -7.62 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -7.62 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VBUS")
				(number "19")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "0")
			)
			(pin power_out line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "FBO")
				(number "20")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "GATEP")
				(number "4")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "GATEN")
				(number "5")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VHV")
				(number "2")
			)
			(pin passive line
				(at 10.16 0 180)
				(length 2.54)
				(name "FBOX")
				(number "1")
			)
			(pin passive line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "VFB")
				(number "17")
			)
			(pin passive line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "IFB")
				(number "18")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "IS-")
				(number "15")
			)
			(pin passive line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "IS+")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH246D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 20.32 0)
		)
		(property "Value" "CH246D"
			(at 5.08 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.4mm_EP1.65x1.65mm"
			(at 2.54 -20.32 0)
		)
		(property "Datasheet" "https://wch-ic.com/downloads/file/307.html"
			(at -2.54 33.02 0)
		)
		(property "Description" "USB QII wireless charging interface PD2.0, BC1.2, QII 5W, 7.5W, 10W, 15W, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB PD QII"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "CH246D_0_1")
		(symbol "CH246D_1_1"
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "UDP")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "UDM")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CC1")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CC0")
				(number "11")
			)
			(pin open_emitter line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "LED1")
				(number "17")
			)
			(pin output line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "LED0")
				(number "20")
			)
			(pin no_connect line
				(at -7.62 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -7.62 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VHV")
				(number "2")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "0")
			)
			(pin output line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "HV1")
				(number "3")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "HV0P")
				(number "4")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "HV0N")
				(number "5")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OSC")
				(number "19")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "NTC")
				(number "18")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "QII")
				(number "16")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "LV0")
				(number "12")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "LV1")
				(number "13")
			)
			(pin passive line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "IS-")
				(number "15")
			)
			(pin passive line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "IS+")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH330N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "CH330N"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -3.81 19.05 0)
		)
		(property "Datasheet" "http://www.wch.cn/downloads/file/240.html"
			(at -2.54 5.08 0)
		)
		(property "Description" "USB serial converter, UART, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb uart wch serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CH330N_0_1")
		(symbol "CH330N_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "V3")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "UD+")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "UD-")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "TXD")
				(number "6")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "RXD")
				(number "7")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{RTS}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH334R"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 20.32 0)
		)
		(property "Value" "CH334R"
			(at 2.54 20.32 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 2.54 -22.86 0)
		)
		(property "Datasheet" "https://www.wch-ic.com/downloads/file/327.html"
			(at 0 33.02 0)
		)
		(property "Description" "USB HUB controller, UART, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB HUB Controller Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "CH334R_0_1")
		(symbol "CH334R_1_1"
			(pin passive line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "VDD33")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "DPU+")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DMU-")
				(number "10")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{RESET}/CDP")
				(number "9")
			)
			(pin passive line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "XO")
				(number "15")
			)
			(pin passive line
				(at -10.16 -15.24 0)
				(length 2.54)
				(name "XI")
				(number "16")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "V5")
				(number "12")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "DM4-")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "DP4+")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "DM3-")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DP3+")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DM2-")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "DP2+")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "DM1-")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "DP1+")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH340C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 13.97 0)
		)
		(property "Value" "CH340C"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at -18.542 30.226 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/szlcsc/Jiangsu-Qin-Heng-CH340C_C84681.pdf"
			(at -6.604 33.274 0)
		)
		(property "Description" "USB serial converter, crystal-less, UART, SOIC-16"
			(at -1.524 36.068 0)
		)
		(property "ki_keywords" "USB UART Serial Converter Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CH340C_0_1")
		(symbol "CH340C_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "R232")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "UD+")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "UD-")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_out line
				(at 0 15.24 270)
				(length 2.54)
				(name "V3")
				(number "4")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "TXD")
				(number "2")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "RXD")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{CTS}")
				(number "9")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{DSR}")
				(number "10")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RI}")
				(number "11")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{DCD}")
				(number "12")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{DTR}")
				(number "13")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{RTS}")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH340E"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 13.97 0)
		)
		(property "Value" "CH340E"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "https://www.mpja.com/download/35227cpdata.pdf"
			(at -8.89 20.32 0)
		)
		(property "Description" "USB serial converter, UART, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Serial Converter Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CH340E_0_1")
		(symbol "CH340E_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "UD+")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "UD-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_out line
				(at 0 15.24 270)
				(length 2.54)
				(name "V3")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "TXD")
				(number "8")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "RXD")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{CTS}")
				(number "5")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "TNOW")
				(number "6")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{RTS}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH340G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 13.97 0)
		)
		(property "Value" "CH340G"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.datasheet5.com/pdf-local-2195953"
			(at -8.89 20.32 0)
		)
		(property "Description" "USB serial converter, UART, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Serial Converter Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CH340G_0_1")
		(symbol "CH340G_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "R232")
				(number "15")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "UD+")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "UD-")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "XI")
				(number "7")
			)
			(pin output line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "XO")
				(number "8")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "16")
			)
			(pin power_out line
				(at 0 15.24 270)
				(length 2.54)
				(name "V3")
				(number "4")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "TXD")
				(number "2")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "RXD")
				(number "3")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{CTS}")
				(number "9")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{DSR}")
				(number "10")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RI}")
				(number "11")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{DCD}")
				(number "12")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{DTR}")
				(number "13")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{RTS}")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH340K"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.858 13.97 0)
		)
		(property "Value" "CH340K"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:SSOP-10-1EP_3.9x4.9mm_P1mm_EP2.1x3.3mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "https://cdn.sparkfun.com/assets/5/0/a/8/5/CH340DS1.PDF"
			(at -8.89 20.32 0)
		)
		(property "Description" "USB serial converter, UART, SSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Serial Converter Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*1EP*3.9x4.9mm*P1mm*"
			(at 0 0 0)
		)
		(symbol "CH340K_0_1")
		(symbol "CH340K_1_0"
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
		)
		(symbol "CH340K_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "UD+")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "UD-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 15.24 270)
				(length 2.54)
				(name "V3")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "TXD")
				(number "8")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "RXD")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{CTS}")
				(number "5")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{DTR}")
				(number "4")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{RTS}")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH340T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 22.86 0)
		)
		(property "Value" "CH340T"
			(at 7.62 22.86 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 22.86 -20.32 0)
		)
		(property "Datasheet" "https://cdn.sparkfun.com/datasheets/Dev/Arduino/Other/CH340DS1.PDF"
			(at -6.35 21.59 0)
		)
		(property "Description" "USB serial converter, UART, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Serial Converter Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CH340T_1_1"
			(pin input line
				(at -10.16 15.24 0)
				(length 2.54)
				(name "R232")
				(number "18")
			)
			(pin bidirectional line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "UD+")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "UD-")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "XI")
				(number "9")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "XO")
				(number "10")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "19")
			)
			(pin power_out line
				(at 0 22.86 270)
				(length 2.54)
				(name "V3")
				(number "5")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin output line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "TXD")
				(number "3")
			)
			(pin input line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "RXD")
				(number "4")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "~{CTS}")
				(number "11")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "~{DSR}")
				(number "12")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{RI}")
				(number "13")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{DCD}")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{DTR}")
				(number "15")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RTS}")
				(number "16")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "CKOH")
				(number "1")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "CKOL")
				(number "2")
			)
			(pin input line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "~{NOS}")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH340X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 13.97 0)
		)
		(property "Value" "CH340X"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "https://cdn.sparkfun.com/assets/5/0/a/8/5/CH340DS1.PDF"
			(at -8.89 20.32 0)
		)
		(property "Description" "USB serial converter, 5V-tolerant IO, UART, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Serial Converter Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CH340X_0_1")
		(symbol "CH340X_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "UD+")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "UD-")
				(number "2")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_out line
				(at 0 15.24 270)
				(length 2.54)
				(name "V3")
				(number "10")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "TXD")
				(number "8")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "RXD")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{CTS}")
				(number "5")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "TNOW/~{DTR}")
				(number "6")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{RTS}")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH343G"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "CH343G"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 5.08 -15.24 0)
		)
		(property "Datasheet" "https://www.wch-ic.com/downloads/CH343DS1_PDF.html"
			(at 5.08 -17.78 0)
		)
		(property "Description" "High-Speed USB serial converter, up to 6Mbps, 3.3V or 5V supply, UART, SOIC-16"
			(at 22.86 -20.32 0)
		)
		(property "ki_keywords" "UART Interface crystalless"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CH343G_0_1")
		(symbol "CH343G_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VBUS")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "UD+")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "UD-")
				(number "6")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD5")
				(number "16")
			)
			(pin power_out line
				(at 0 15.24 270)
				(length 2.54)
				(name "V3")
				(number "4")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VIO")
				(number "15")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "TXD")
				(number "2")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "RXD")
				(number "3")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{ACT}")
				(number "8")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{CTS}")
				(number "13")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{DSR}")
				(number "12")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RI}")
				(number "14")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{DCD}")
				(number "9")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{DTR}")
				(number "10")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{RTS}")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH343P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "CH343P"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:WCH_QFN-16-1EP_3x3mm_P0.5mm_EP1.8x1.8mm"
			(at 5.08 -15.24 0)
		)
		(property "Datasheet" "https://www.wch-ic.com/downloads/CH343DS1_PDF.html"
			(at 5.08 -17.78 0)
		)
		(property "Description" "High-Speed USB serial converter, up to 6Mbps, 3.3V or 5V supply, UART, QFN-16"
			(at 36.83 -20.32 0)
		)
		(property "ki_keywords" "UART Interface crystalless Winchip WCH"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*3x3mm*P0.5mm*EP1.8x1.8mm*"
			(at 0 0 0)
		)
		(symbol "CH343P_0_1")
		(symbol "CH343P_1_0"
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND_EPAD")
				(number "17")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
		)
		(symbol "CH343P_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VBUS")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "UD+")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "UD-")
				(number "8")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD5")
				(number "3")
			)
			(pin power_out line
				(at 0 15.24 270)
				(length 2.54)
				(name "V3_{OUT}")
				(number "6")
				(alternate "V3_{IN}" power_in line)
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VIO")
				(number "1")
			)
			(pin output line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "TXD")
				(number "4")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "RXD")
				(number "5")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "~{ACT}")
				(number "10")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~{CTS}")
				(number "15")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "~{DSR}")
				(number "14")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~{RI}")
				(number "16")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{DCD}")
				(number "11")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "~{DTR}")
				(number "12")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "~{RTS}")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH344Q"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 44.45 0)
		)
		(property "Value" "CH344Q"
			(at 22.86 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 7.62 -43.18 0)
		)
		(property "Datasheet" "https://www.wch-ic.com/downloads/file/299.html"
			(at 7.62 -45.72 0)
		)
		(property "Description" "USB to Quad Serial Ports Chip, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Quad UART Serial Converter Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CH344Q_0_1")
		(symbol "CH344Q_1_0"
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "~{DTR2}/TNOW2/GPIO9")
				(number "19")
			)
		)
		(symbol "CH344Q_1_1"
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "UD+")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "UD-")
				(number "42")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "XI")
				(number "5")
			)
			(pin output line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "XO")
				(number "6")
			)
			(pin input line
				(at -25.4 -17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "~{ACT}/~{CFG}/~{DCD3}")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "TX_S/~{RI3}")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "RX_S/~{DSR3}")
				(number "16")
			)
			(pin input line
				(at -25.4 -38.1 0)
				(length 2.54)
				(name "TEST")
				(number "44")
			)
			(pin no_connect line
				(at -22.86 38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "36")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -43.18 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin power_in line
				(at 0 -43.18 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "48")
			)
			(pin output line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "TXD0")
				(number "30")
			)
			(pin input line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "RXD0")
				(number "31")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "~{CTS0}/GPIO0")
				(number "41")
			)
			(pin input line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "~{DSR0}/GPIO14")
				(number "29")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "~{RI0}/GPIO13")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "~{DCD0}/GPIO12")
				(number "33")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "~{DTR0}/TNOW0/GPIO8")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "~{RTS0}/GPIO1")
				(number "40")
			)
			(pin output line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "TXD1")
				(number "12")
			)
			(pin input line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "RXD1")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "~{CTS1}/GPIO2")
				(number "10")
			)
			(pin input line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "~{DSR1}")
				(number "17")
			)
			(pin input line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "~{RI1}")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "~{DCD1}/GPIO15")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "~{DTR1}/TNOW1/GPIO9")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "~{RTS1}/GPIO3")
				(number "11")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "TXD2")
				(number "21")
			)
			(pin input line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "RXD2")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "~{CTS2}/GPIO4")
				(number "26")
			)
			(pin input line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "~{DSR2}")
				(number "2")
			)
			(pin input line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "~{RI2}")
				(number "3")
			)
			(pin input line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "~{DCD2}")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "~{RTS2}/GPIO5")
				(number "27")
			)
			(pin output line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "TXD3")
				(number "37")
			)
			(pin input line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "RXD3")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "~{CTS3}/GPIO6")
				(number "46")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "~{DTR3}/TNOW3/GPIO11")
				(number "34")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "~{RTS3}/GPIO7")
				(number "45")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CH9102F"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 29.21 0)
		)
		(property "Value" "CH9102F"
			(at 12.7 29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 1.27 -29.21 0)
		)
		(property "Datasheet" "http://www.wch-ic.com/downloads/CH9102DS1_PDF.html"
			(at 0 0 0)
		)
		(property "Description" "WCH-IC, Single-Chip USB-to-UART Bridge, USB 2.0 Full-Speed, 4Mbps UART, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "uart usb bridge interface transceiver CH9102F"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CH9102F_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D-")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D+")
				(number "3")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VDD5")
				(number "7")
			)
			(pin power_out line
				(at 0 30.48 270)
				(length 2.54)
				(name "V3")
				(number "6")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "TXD")
				(number "21")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "RXD")
				(number "20")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "~{RTS}")
				(number "19")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{CTS}")
				(number "18")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{DSR}")
				(number "22")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{DTR}")
				(number "23")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{DCD}")
				(number "24")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{RI}")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "SUSPEND")
				(number "17")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{SUSPEND}")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "TXS/GPIO0")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "RXS/GPIO1")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "TNOW/GPIO2")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{WAKEUP}/GPIO3")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "GPIO4")
				(number "16")
			)
			(pin output line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "~{ACT}")
				(number "10")
			)
			(pin input line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "~{RST}")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP2102N-Axx-xQFN20"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 26.67 0)
		)
		(property "Value" "CP2102N-Axx-xQFN20"
			(at 12.7 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:SiliconLabs_QFN-20-1EP_3x3mm_P0.5mm"
			(at 31.75 -26.67 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/cp2102n-datasheet.pdf"
			(at 1.27 -19.05 0)
		)
		(property "Description" "USB to UART master bridge, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SiliconLabs*QFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CP2102N-Axx-xQFN20_0_1")
		(symbol "CP2102N-Axx-xQFN20_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "~{RST}")
				(number "9")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D-")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D+")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VREGIN")
				(number "7")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "TXD")
				(number "18")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "RXD")
				(number "17")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "~{RTS}")
				(number "16")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{CTS}")
				(number "15")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{WAKEUP}")
				(number "13")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "SUSPEND")
				(number "14")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{SUSPEND}")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "CLK/GPIO.0")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "RS485/GPIO.1")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "~{TXT}/GPIO.2")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{RXT}/GPIO.3")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP2102N-Axx-xQFN24"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 26.67 0)
		)
		(property "Value" "CP2102N-Axx-xQFN24"
			(at 13.97 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 31.75 -26.67 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/cp2102n-datasheet.pdf"
			(at 1.27 -19.05 0)
		)
		(property "Description" "USB to UART master bridge, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CP2102N-Axx-xQFN24_0_1")
		(symbol "CP2102N-Axx-xQFN24_1_1"
			(pin input line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "~{RST}")
				(number "9")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D-")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D+")
				(number "3")
			)
			(pin no_connect line
				(at -10.16 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VREGIN")
				(number "7")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 -22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "TXD")
				(number "21")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "RXD")
				(number "20")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "~{RTS}")
				(number "19")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{CTS}")
				(number "18")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{DSR}")
				(number "22")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{DTR}")
				(number "23")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{DCD}")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{RI}/CLK")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "SUSPEND")
				(number "17")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{SUSPEND}")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{TXT}/GPIO.0")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{RXT}/GPIO.1")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "RS485/GPIO.2")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "~{WAKEUP}/GPIO.3")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP2102N-Axx-xQFN28"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 31.75 0)
		)
		(property "Value" "CP2102N-Axx-xQFN28"
			(at 12.7 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_5x5mm_P0.5mm_EP3.35x3.35mm"
			(at 33.02 -31.75 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/cp2102n-datasheet.pdf"
			(at 1.27 -19.05 0)
		)
		(property "Description" "USB to UART master bridge, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CP2102N-Axx-xQFN28_0_1")
		(symbol "CP2102N-Axx-xQFN28_1_1"
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "~{RST}")
				(number "9")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D-")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D+")
				(number "4")
			)
			(pin no_connect line
				(at -10.16 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VREGIN")
				(number "7")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "TXD")
				(number "26")
			)
			(pin input line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "RXD")
				(number "25")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "~{RTS}")
				(number "24")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "~{CTS}")
				(number "23")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "~{DSR}")
				(number "27")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{DTR}")
				(number "28")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{DCD}")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{RI}/CLK")
				(number "2")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SUSPEND")
				(number "12")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{SUSPEND}")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{TXT}/GPIO.0")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "~{RXT}/GPIO.1")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "RS485/GPIO.2")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "~{WAKEUP}/GPIO.3")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "GPIO.4")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "GPIO.5")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "GPIO.6")
				(number "20")
			)
			(pin output line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "CHREN")
				(number "13")
			)
			(pin output line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "CHR0")
				(number "15")
			)
			(pin output line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "CHR1")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP2104"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 28.575 0)
		)
		(property "Value" "CP2104"
			(at -5.08 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 29.21 -52.07 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/cp2104.pdf"
			(at 105.41 10.16 0)
		)
		(property "Description" "Single-Chip USB-to-UART Bridge, USB 2.0 Full-Speed, 2Mbps UART, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "uart usb bridge interface transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CP2104_1_1"
			(pin bidirectional line
				(at -12.7 22.86 0)
				(length 2.54)
				(name "~{RST}")
				(number "9")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D-")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D+")
				(number "3")
			)
			(pin passive line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "VPP")
				(number "16")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "REGIN")
				(number "7")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VIO")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "TXD")
				(number "21")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "RXD")
				(number "20")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "~{RTS}")
				(number "19")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{CTS}")
				(number "18")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{DSR}")
				(number "22")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{DTR}")
				(number "23")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "~{DCD}")
				(number "24")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "~{RI}")
				(number "1")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "SUSPEND")
				(number "17")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{SUSPEND}")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "TXT/GPIO.0")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "RXT/GPIO.1")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "RS485/GPIO.2")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "GPIO.3")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP2108-xxx-xM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 53.34 0)
		)
		(property "Value" "CP2108-xxx-xM"
			(at 19.05 53.34 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.1x4.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/cp2108-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed Quad Channel USB UART/FIFO, integrated clock and EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Quad UART FIFO bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CP2108-xxx-xM_0_1")
		(symbol "CP2108-xxx-xM_1_1"
			(pin power_in line
				(at -30.48 48.26 0)
				(length 3.81)
				(name "VREGIN")
				(number "60")
			)
			(pin input line
				(at -30.48 27.94 0)
				(length 3.81)
				(name "VBUS")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "D-")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "D+")
				(number "62")
			)
			(pin input line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "~{RESET}")
				(number "64")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "GPIO0")
				(number "41")
				(alternate "UART0_TX_TOGGLE" output line)
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "GPIO1")
				(number "40")
				(alternate "UART0_RX_TOGGLE" output line)
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "GPIO2")
				(number "38")
				(alternate "UART0_RS485" output line)
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "GPIO3")
				(number "37")
				(alternate "CLK0" output line)
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "GPIO4")
				(number "34")
				(alternate "UART1_TX_TOGGLE" output line)
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "GPIO5")
				(number "33")
				(alternate "UART1_RX_TOGGLE" output line)
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "GPIO6")
				(number "32")
				(alternate "UART1_RS485" output line)
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "GPIO7")
				(number "31")
				(alternate "CLK1" output line)
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "GPIO8")
				(number "30")
				(alternate "UART2_TX_TOGGLE" output line)
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "GPIO9")
				(number "29")
				(alternate "UART2_RX_TOGGLE" output line)
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 3.81)
				(name "GPIO10")
				(number "28")
				(alternate "UART2_RS485" output line)
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 3.81)
				(name "GPIO11")
				(number "27")
				(alternate "CLK2" output line)
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 3.81)
				(name "GPIO12")
				(number "26")
				(alternate "UART3_TX_TOGGLE" output line)
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 3.81)
				(name "GPIO13")
				(number "23")
				(alternate "UART2_RX_TOGGLE" output line)
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 3.81)
				(name "GPIO14")
				(number "22")
				(alternate "UART2_RS485" output line)
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 3.81)
				(name "GPIO15")
				(number "21")
				(alternate "CLK3" output line)
			)
			(pin no_connect line
				(at -26.67 43.18 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at -26.67 40.64 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 3.81)
				(name "VSSHD")
				(number "2")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 3.81)
				(name "VDD")
				(number "58")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 3.81)
				(name "VSS")
				(number "25")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "59")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "65")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 3.81)
				(name "VIO")
				(number "24")
			)
			(pin passive line
				(at 5.08 55.88 270)
				(length 3.81)
				(hide yes)
				(name "VIO")
				(number "39")
			)
			(pin power_in line
				(at 10.16 55.88 270)
				(length 3.81)
				(name "VIOHD")
				(number "3")
			)
			(pin output line
				(at 30.48 48.26 180)
				(length 3.81)
				(name "TX0")
				(number "57")
			)
			(pin input line
				(at 30.48 45.72 180)
				(length 3.81)
				(name "RX0")
				(number "56")
			)
			(pin output line
				(at 30.48 43.18 180)
				(length 3.81)
				(name "~{RTS0}")
				(number "55")
			)
			(pin input line
				(at 30.48 40.64 180)
				(length 3.81)
				(name "~{CTS0}")
				(number "54")
			)
			(pin output line
				(at 30.48 38.1 180)
				(length 3.81)
				(name "~{DTR0}")
				(number "53")
			)
			(pin input line
				(at 30.48 35.56 180)
				(length 3.81)
				(name "~{DSR0}")
				(number "52")
			)
			(pin input line
				(at 30.48 33.02 180)
				(length 3.81)
				(name "~{DCD0}")
				(number "51")
			)
			(pin input line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "~{RI0}")
				(number "50")
			)
			(pin output line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "TX1")
				(number "49")
			)
			(pin input line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "RX1")
				(number "48")
			)
			(pin output line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "~{RTS1}")
				(number "47")
			)
			(pin input line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "~{CTS1}")
				(number "46")
			)
			(pin output line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "~{DTR1}")
				(number "45")
			)
			(pin input line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "~{DSR1}")
				(number "44")
			)
			(pin input line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "~{DCD1}")
				(number "43")
			)
			(pin input line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "~{RI1}")
				(number "42")
			)
			(pin output line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "TX2")
				(number "16")
			)
			(pin input line
				(at 30.48 0 180)
				(length 3.81)
				(name "RX2")
				(number "15")
			)
			(pin output line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "~{RTS2}")
				(number "14")
			)
			(pin input line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "~{CTS2}")
				(number "13")
			)
			(pin output line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "~{DTR2}")
				(number "18")
			)
			(pin input line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "~{DSR2}")
				(number "17")
			)
			(pin input line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "~{DCD2}")
				(number "12")
			)
			(pin input line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "~{RI2}")
				(number "11")
			)
			(pin output line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "TX3")
				(number "4")
			)
			(pin input line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "RX3")
				(number "1")
			)
			(pin output line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "~{RTS3}")
				(number "6")
			)
			(pin input line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "~{CTS3}")
				(number "5")
			)
			(pin output line
				(at 30.48 -30.48 180)
				(length 3.81)
				(name "~{DTR3}")
				(number "10")
			)
			(pin input line
				(at 30.48 -33.02 180)
				(length 3.81)
				(name "~{DSR3}")
				(number "9")
			)
			(pin input line
				(at 30.48 -35.56 180)
				(length 3.81)
				(name "~{DCD3}")
				(number "8")
			)
			(pin input line
				(at 30.48 -38.1 180)
				(length 3.81)
				(name "~{RI3}")
				(number "7")
			)
			(pin output line
				(at 30.48 -43.18 180)
				(length 3.81)
				(name "SUSPEND")
				(number "20")
			)
			(pin output line
				(at 30.48 -45.72 180)
				(length 3.81)
				(name "~{SUSPEND}")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP2112"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 19.685 0)
		)
		(property "Value" "CP2112"
			(at -2.54 17.78 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 11.43 -17.78 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/cp2112-datasheet.pdf"
			(at 1.27 -25.4 0)
		)
		(property "Description" "HID USB to SMBUS master bridge"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB SMBUS bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CP2112_0_1")
		(symbol "CP2112_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "~{RST}")
				(number "9")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "~{SUSPEND}")
				(number "17")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "SUSPEND")
				(number "11")
			)
			(pin power_in line
				(at -15.24 0 0)
				(length 3.81)
				(name "VPP")
				(number "16")
			)
			(pin power_in line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "REGIN")
				(number "7")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "VBUS")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "D+")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "D-")
				(number "4")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 3.81)
				(name "VIO")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 -16.51 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at 7.62 -16.51 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at 10.16 -16.51 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "SDA")
				(number "1")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "SCL")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "GPIO.0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "GPIO.1")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "GPIO.2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "GPIO.3")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "GPIO.4")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "GPIO.5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "GPIO.6")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "GPIO.7")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CP2615-xx-xM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 27.94 0)
		)
		(property "Value" "CP2615-xx-xM"
			(at 2.54 -27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.3x3.3mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/cp2615-datasheet.pdf"
			(at -15.24 27.94 0)
		)
		(property "Description" "USB to I2S bridge, USB 1.0 Audio Class, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb i2s i2c uart audio bridge hid gpio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CP2615-xx-xM_0_0"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{RST}")
				(number "9")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "~{CFGMODE}")
				(number "21")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "D+")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "D-")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "GPIO.10/~{RESETOUT}")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "GPIO.11/RTS")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "GPIO.12/CLKOUT")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "GPIO.13/TX")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "GPIO.14/RX")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "GPIO.15/CTS")
				(number "31")
			)
			(pin no_connect line
				(at -15.24 15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "REGIN")
				(number "7")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "I2C_SCL")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "I2C_SDA")
				(number "30")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "I2S_MCLK")
				(number "26")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "I2S_LRCLK")
				(number "28")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "I2S_SCLK")
				(number "2")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "I2S_SDOUT")
				(number "32")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "I2S_SDIN")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "GPIO.6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "GPIO.7")
				(number "11")
			)
		)
		(symbol "CP2615-xx-xM_0_1")
		(symbol "CP2615-xx-xM_1_1"
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "GPIO.8/ADC")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "GPIO.9/BUTTONS")
				(number "19")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GPIO.0")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "GPIO.1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "GPIO.2")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "GPIO.3")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "GPIO.4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "GPIO.5")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY7C65211-24LTXI"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.716 16.51 0)
		)
		(property "Value" "CY7C65211-24LTXI"
			(at 3.302 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/139886/download"
			(at -40.64 21.59 0)
		)
		(property "Description" "USB-Serial single channel bridge with capsense and BCD, +1.71V to +5.5V VDD, UART/I2C/SPI/RS232/RS422, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB-Serial single channel bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CY7C65211-24LTXI_0_1")
		(symbol "CY7C65211-24LTXI_1_1"
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "~{XRES}")
				(number "14")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "WAKEUP")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SCB_0/GPIO_6")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "SCB_4/GPIO_5")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "SCB_2/GPIO_3")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "SCB_3/GPIO_4")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "SCB_1/GPIO_2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "SCB_5/GPIO_7")
				(number "2")
			)
			(pin power_in line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "VCCD")
				(number "12")
			)
			(pin no_connect line
				(at -15.24 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "1EP")
				(number "25")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "VSSD")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "VSSD")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSSD")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "VSSA")
				(number "17")
			)
			(pin power_out line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "VBUS")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "USBDP")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "USBDM")
				(number "11")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "SUSPEND")
				(number "8")
			)
			(pin tri_state line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GPIO_11")
				(number "7")
			)
			(pin tri_state line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "GPIO_10")
				(number "6")
			)
			(pin tri_state line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "GPIO_9")
				(number "5")
			)
			(pin tri_state line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "GPIO_8")
				(number "4")
			)
			(pin tri_state line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "GPIO_0")
				(number "18")
			)
			(pin tri_state line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "GPIO_1")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY7C65213-28PVXI"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "CY7C65213-28PVXI"
			(at 3.556 19.05 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/139881/download"
			(at -63.5 12.7 0)
		)
		(property "Description" "USB-UART LP Bridge Controller, full speed 12Mbps, +1.71V to 5.5V VDD, UART/RS232/RS422, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB-UART LP Bridge Controller, full speed 12Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "CY7C65213-28PVXI_0_1")
		(symbol "CY7C65213-28PVXI_1_1"
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "19")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "RXD")
				(number "5")
			)
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "TXD")
				(number "1")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "RTS")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "CTS")
				(number "11")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "DTR")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DSR")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DCD")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "RI")
				(number "6")
			)
			(pin passive line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "VCCD")
				(number "17")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "DNU")
				(number "26")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCCIO")
				(number "4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin no_connect line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin no_connect line
				(at 12.7 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "USBDP")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "USBDM")
				(number "16")
			)
			(pin tri_state line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "GPIO7")
				(number "28")
			)
			(pin tri_state line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "GPIO6")
				(number "27")
			)
			(pin tri_state line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "GPIO5")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "GPIO4")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "GPIO3")
				(number "14")
			)
			(pin tri_state line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "GPIO2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "GPIO1")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GPIO0")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY7C65213-32LTXI"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.922 19.05 0)
		)
		(property "Value" "CY7C65213-32LTXI"
			(at 3.556 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/139881/download"
			(at -63.5 12.7 0)
		)
		(property "Description" "USB-UART LP Bridge Controller, full speed 12Mbps, +1.71V to 5.5V VDD, UART/RS232/RS422, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB-UART LP Bridge Controller, full speed 12Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CY7C65213-32LTXI_0_1")
		(symbol "CY7C65213-32LTXI_1_1"
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "~{RESET}")
				(number "18")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RXD")
				(number "2")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "TXD")
				(number "30")
			)
			(pin output line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RTS")
				(number "32")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CTS")
				(number "8")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "DTR")
				(number "31")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DSR")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DCD")
				(number "7")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RI")
				(number "3")
			)
			(pin passive line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "DNU")
				(number "23")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "DNU")
				(number "25")
			)
			(pin passive line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "DNU")
				(number "26")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "1EP")
				(number "33")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VCCIO")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VCC")
				(number "19")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "VCCD")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 5.08 -25.4 90)
				(length 2.54)
				(name "AGND")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "USBDP")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "USBDM")
				(number "15")
			)
			(pin tri_state line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "GPIO7")
				(number "13")
			)
			(pin tri_state line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "GPIO6")
				(number "12")
			)
			(pin tri_state line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "GPIO5")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "GPIO4")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "GPIO3")
				(number "11")
			)
			(pin tri_state line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "GPIO2")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "GPIO1")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GPIO0")
				(number "22")
			)
			(pin passive line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "DNU")
				(number "29")
			)
			(pin passive line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "DNU")
				(number "28")
			)
			(pin passive line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "DNU")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY7C65215-32LTXI"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.462 21.844 0)
		)
		(property "Value" "CY7C65215-32LTXI"
			(at 7.112 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/129956/download"
			(at -40.64 26.67 0)
		)
		(property "Description" "USB-Serial Dual Channel Bridge with CapSense Full-Speed 12 Mbps, +1.71V to +5.5V VDD, UART/I2C/SPI/RS232/RS422/JTAG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB-Serial single channel bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CY7C65215-32LTXI_0_1")
		(symbol "CY7C65215-32LTXI_1_1"
			(pin input line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "~{XRES}")
				(number "18")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "WAKEUP")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "SCB0_0/GPIO_8")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SCB0_1/GPIO_2")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SCB0_2/GPIO_3")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "SCB0_3/GPIO_4")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "SCB0_4/GPIO_5")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "SCB0_5/GPIO_9")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "SCB1_0/GPIO_10")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "SCB1_1/GPIO_11")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "SCB1_2/GPIO_12")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "SCB1_3/GPIO_13")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "SCB1_4/GPIO_14")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "SCB1_5/GPIO_15")
				(number "10")
			)
			(pin no_connect line
				(at -15.24 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "1EP")
				(number "33")
			)
			(pin power_in line
				(at -5.08 -30.48 90)
				(length 2.54)
				(name "VSSD")
				(number "20")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VDDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 2.54)
				(name "VSSD")
				(number "4")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDDD")
				(number "23")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "VSSD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VCCD")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "VSSA")
				(number "24")
			)
			(pin power_out line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "VBUS")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "USBDP")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "USBDM")
				(number "15")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SUSPEND")
				(number "11")
			)
			(pin tri_state line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "GPIO_18")
				(number "22")
			)
			(pin tri_state line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "GPIO_17")
				(number "21")
			)
			(pin tri_state line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "GPIO_16")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "GPIO_7")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "GPIO_6")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "GPIO_1")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "GPIO_0")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CYPD3171-24LQXQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 26.67 0)
		)
		(property "Value" "CYPD3171-24LQXQ"
			(at 10.16 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.75x2.75mm"
			(at 0 35.56 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-EZ-PD(TM)_CCG3PA_Datasheet_USB_Type-C_Port_Controller-DataSheet-v09_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ee438366ac0"
			(at 4.572 41.402 0)
		)
		(property "Description" "USB Type-C port controller, Cortex®-M0 processor, UFP CC bootloader, QFN-24"
			(at 3.556 38.354 0)
		)
		(property "ki_keywords" "USBPD Quickcharge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*EP2.75x2.75mm*"
			(at 0 0 0)
		)
		(symbol "CYPD3171-24LQXQ_1_1"
			(pin power_in line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "VDDD")
				(number "23")
			)
			(pin power_out line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "VCCD")
				(number "24")
			)
			(pin output line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "FB")
				(number "20")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "COMP")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "P0.0/SWD_DAT_0")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "P0.1/SWD_CLK_0")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "DP1/P1.2")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "DM1/P1.3")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "P2.0/AXRES")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "P2.1")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "P2.2")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "P2.3")
				(number "13")
			)
			(pin input line
				(at -7.62 27.94 270)
				(length 2.54)
				(name "VBUS_IN_DIS")
				(number "18")
			)
			(pin power_in line
				(at -7.62 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at -7.62 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin output line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VBUS_P_CTRL")
				(number "3")
			)
			(pin output line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VBUS_C_CTRL")
				(number "4")
			)
			(pin input line
				(at 7.62 27.94 270)
				(length 2.54)
				(name "VBUS_C_MON_DIS")
				(number "11")
			)
			(pin input line
				(at 7.62 -27.94 90)
				(length 2.54)
				(name "CSP")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "CC1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "CC2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "DP0/P3.0")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "DM0/P3.1")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CYPD3174-16SXQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 17.78 0)
		)
		(property "Value" "CYPD3174-16SXQ"
			(at 8.89 17.78 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 33.02 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-EZ-PD(TM)_CCG3PA_Datasheet_USB_Type-C_Port_Controller-DataSheet-v09_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ee438366ac0"
			(at 5.08 30.48 0)
		)
		(property "Description" "USB Type-C port controller, Cortex®-M0 processor, DFP CC with opto coupler feedback bootloader, SOIC-16"
			(at 5.08 27.94 0)
		)
		(property "ki_keywords" "USBPD quickcharge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "CYPD3174-16SXQ_1_1"
			(pin power_in line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "VDDD")
				(number "3")
			)
			(pin power_out line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "VCCD")
				(number "4")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "FB")
				(number "1")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "COMP")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "P0.0/SWD_DAT_0")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "P0.1/SWD_CLK_0")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "P2.0/AXRES")
				(number "8")
			)
			(pin input line
				(at -7.62 17.78 270)
				(length 2.54)
				(name "VBUS_IN_DIS")
				(number "14")
			)
			(pin power_in line
				(at -7.62 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin output line
				(at 0 17.78 270)
				(length 2.54)
				(name "VBUS_P_CTRL")
				(number "5")
			)
			(pin input line
				(at 7.62 17.78 270)
				(length 2.54)
				(name "VBUS_C_MON_DIS")
				(number "9")
			)
			(pin input line
				(at 7.62 -17.78 90)
				(length 2.54)
				(name "CSP")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "CC1")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "CC2")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "DP0/P3.0")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "DM0/P3.1")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CYPD3177-24LQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 21.59 0)
		)
		(property "Value" "CYPD3177-24LQ"
			(at 10.16 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.75x2.75mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-EZ-PD_BCR_Datasheet_USB_Type-C_Port_Controller_for_Power_Sinks-DataSheet-v03_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ee7ce9d70ad"
			(at 0 0 0)
		)
		(property "Description" "Stand-alone USB PD controller (with sink Auto-run mode), QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb pd type csink"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP?4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CYPD3177-24LQ_0_1")
		(symbol "CYPD3177-24LQ_1_1"
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "VBUS_MAX")
				(number "2")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "VBUS_MIN")
				(number "1")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "ISNK_COARSE")
				(number "5")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "ISNK_FINE")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "CC1")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "CC2")
				(number "14")
			)
			(pin no_connect line
				(at -15.24 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -15.24 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin power_out line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VCCD")
				(number "24")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VBUS_IN")
				(number "18")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_out line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VDDD")
				(number "23")
			)
			(pin no_connect line
				(at 15.24 17.78 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at 15.24 15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "FLIP")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "HPI_SCL")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "HPI_SDA")
				(number "12")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "~{HPI_INT}")
				(number "7")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "VBUS_FET_EN")
				(number "3")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "SAFE_PWR_EN")
				(number "4")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "FAULT")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "GPIO_1")
				(number "8")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "VDC_OUT")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FE1.1s"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 26.67 0)
		)
		(property "Value" "FE1.1s"
			(at 12.7 27.94 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_3.9x9.9mm_P0.635mm"
			(at 26.67 -38.1 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2991/FE1.1s+Data+Sheet+(Rev.+1.0).pdf"
			(at 0 0 0)
		)
		(property "Description" "USB 2.0 High Speed 4-Port Hub Controller, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "4-Port, EEPROM, High Speed, Hub, USB2.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x9.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "FE1.1s_0_1")
		(symbol "FE1.1s_1_1"
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "VBUSM")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "DPU")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "DMU")
				(number "15")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "~{XRSTJ}")
				(number "17")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "BUSJ")
				(number "19")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "OVCJ")
				(number "26")
			)
			(pin output line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "XOUT")
				(number "2")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "XIN")
				(number "3")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "REXT")
				(number "14")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 2.54)
				(name "VDD5")
				(number "20")
			)
			(pin power_out line
				(at 0 27.94 270)
				(length 2.54)
				(name "VD33_O")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VD33")
				(number "13")
			)
			(pin power_out line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VD18_O")
				(number "12")
			)
			(pin power_in line
				(at 7.62 27.94 270)
				(length 2.54)
				(name "VD18")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "DP1")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "DM1")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "DP2")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "DM2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DP3")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DM3")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "DP4")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "DM4")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "TESTJ/EESDA")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "LED1/EESCL")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "LED2")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "DRV")
				(number "22")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PWRJ")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FSUSB30MUX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 8.89 0)
		)
		(property "Value" "FSUSB30MUX"
			(at 7.62 -8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 21.59 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/fsusb30-d.pdf"
			(at 0 -20.32 0)
		)
		(property "Description" "Low-Power, Two-Port, High-Speed, USB2.0 (480Mbps) Switch, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB 2.0 High Speed Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FSUSB30MUX_0_1")
		(symbol "FSUSB30MUX_1_1"
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D+")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "D-")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "~{OE}")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "HSD1+")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "HSD1-")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "HSD2+")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "HSD2-")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FSUSB42MUX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "FSUSB42MUX"
			(at 7.62 8.89 0)
		)
		(property "Footprint" "Package_SO:MSOP-10_3x3mm_P0.5mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FSUSB42-D.PDF"
			(at 0 -2.54 0)
		)
		(property "Description" "Low-Power, Two-Port, High-Speed, USB2.0 (480Mbps) or UART Switch, MSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB 2.0 UART High Speed Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FSUSB42MUX_0_1")
		(symbol "FSUSB42MUX_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "D+")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D-")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{OE}")
				(number "10")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "SEL")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "HSD2+")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "HSD2-")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "HSD1+")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "HSD1-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT200XD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 12.7 0)
		)
		(property "Value" "FT200XD"
			(at 7.62 12.7 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.55x2.48mm"
			(at 35.56 -12.7 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT200XD.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to I2C Bridge, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB I2C Interface Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FT200XD_0_1")
		(symbol "FT200XD_1_1"
			(pin power_out line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "3V3OUT")
				(number "3")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "USBDM")
				(number "1")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "USBDP")
				(number "10")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "~{RESET}")
				(number "2")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 3.81)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 3.81)
				(name "VCCIO")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "SCL")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "SDA")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "CBUS0")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT201XQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "FT201XQ"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
			(at 34.29 -15.24 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT201X.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to I2C Bridge, QFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB I2C interface Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "FT201XQ_0_1")
		(symbol "FT201XQ_1_1"
			(pin power_out line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "3V3OUT")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "USBDM")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "USBDP")
				(number "6")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{RESET}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VCCIO")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "SCL")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "SDA")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "CBUS0")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "CBUS1")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "CBUS2")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "CBUS3")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "CBUS4")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "CBUS5")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT201XS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "FT201XS"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 25.4 -15.24 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT201X.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to I2C Bridge, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB I2C Interface Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "FT201XS_0_1")
		(symbol "FT201XS_1_1"
			(pin power_out line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "3V3OUT")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "USBDM")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "USBDP")
				(number "8")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{RESET}")
				(number "11")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VCCIO")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "13")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "SCL")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "SDA")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "CBUS0")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "CBUS1")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "CBUS2")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "CBUS3")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "CBUS4")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "CBUS5")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT220XQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "FT220XQ"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
			(at 34.29 -15.24 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT220X.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to 4-Bit SPI / FT1248 Bridge, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB SPI FT1248 Interface Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "FT220XQ_0_1")
		(symbol "FT220XQ_1_1"
			(pin power_out line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "3V3OUT")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "USBDM")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "USBDP")
				(number "6")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{RESET}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VCCIO")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "MIOSI0")
				(number "15")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "MIOSI1")
				(number "2")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "MIOSI2")
				(number "16")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "MIOSI3")
				(number "4")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "CLK")
				(number "12")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "~{CS}")
				(number "11")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "MISO")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "CBUS3")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT220XS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "FT220XS"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 25.4 -15.24 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT220X.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to 4-Bit SPI / FT1248 Bridge, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB SPI FT1248 Interface Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "FT220XS_0_1")
		(symbol "FT220XS_1_1"
			(pin power_out line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "3V3OUT")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "USBDM")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "USBDP")
				(number "8")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{RESET}")
				(number "11")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VCCIO")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "13")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "MIOSI0")
				(number "1")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "MIOSI1")
				(number "4")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "MIOSI2")
				(number "2")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "MIOSI3")
				(number "6")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "CLK")
				(number "15")
			)
			(pin input line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "~{CS}")
				(number "14")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "MISO")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "CBUS3")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT221XQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 20.32 0)
		)
		(property "Value" "FT221XQ"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 34.29 -20.32 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT221X.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to 8-Bit SPI / FT1248 Bridge, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB SPI FT1248 interface converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FT221XQ_0_1")
		(symbol "FT221XQ_1_1"
			(pin power_out line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "3V3OUT")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "USBDM")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "USBDP")
				(number "8")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "~{RESET}")
				(number "11")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 3.81)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 3.81)
				(name "VCCIO")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "21")
			)
			(pin input line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "MIOSI0")
				(number "17")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "MIOSI1")
				(number "1")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "MIOSI2")
				(number "19")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "MIOSI3")
				(number "6")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "MIOSI4")
				(number "18")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "MIOSI5")
				(number "4")
			)
			(pin input line
				(at 17.78 0 180)
				(length 3.81)
				(name "MIOSI6")
				(number "5")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "MIOSI7")
				(number "2")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "CLK")
				(number "15")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "~{CS}")
				(number "14")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "MISO")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "CBUS3")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT221XS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 20.32 0)
		)
		(property "Value" "FT221XS"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_3.9x8.7mm_P0.635mm"
			(at 25.4 -20.32 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT221X.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to 8-Bit SPI / FT1248 Bridge, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB SPI FT1248 interface converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "FT221XS_0_1")
		(symbol "FT221XS_1_1"
			(pin power_out line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "3V3OUT")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "USBDM")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "USBDP")
				(number "11")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "~{RESET}")
				(number "14")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 3.81)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 3.81)
				(name "VCCIO")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "16")
			)
			(pin input line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "MIOSI0")
				(number "20")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "MIOSI1")
				(number "4")
			)
			(pin input line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "MIOSI2")
				(number "2")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "MIOSI3")
				(number "9")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "MIOSI4")
				(number "1")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "MIOSI5")
				(number "7")
			)
			(pin input line
				(at 17.78 0 180)
				(length 3.81)
				(name "MIOSI6")
				(number "8")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "MIOSI7")
				(number "5")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "CLK")
				(number "18")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "~{CS}")
				(number "17")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "MISO")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "CBUS3")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT2232D"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 44.45 0)
		)
		(property "Value" "FT2232D"
			(at 13.97 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 25.4 -41.91 0)
		)
		(property "Datasheet" "http://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT2232D.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed Double Channel USB UART/FIFO, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Double UART FIFO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FT2232D_0_1")
		(symbol "FT2232D_1_1"
			(pin power_out line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "3V3OUT")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "USBDM")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "USBDP")
				(number "7")
			)
			(pin output line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "~{RSTOUT}")
				(number "5")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "XTIN")
				(number "43")
			)
			(pin output line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "XTOUT")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "EECS")
				(number "48")
			)
			(pin output line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "EECLK")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "EEDATA")
				(number "2")
			)
			(pin input line
				(at -22.86 -33.02 0)
				(length 5.08)
				(name "TEST")
				(number "47")
			)
			(pin power_in line
				(at -10.16 48.26 270)
				(length 5.08)
				(name "AVCC")
				(number "46")
			)
			(pin power_in line
				(at -7.62 -45.72 90)
				(length 5.08)
				(name "AGND")
				(number "45")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 5.08)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 5.08)
				(name "VCC")
				(number "42")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 5.08)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 5.08)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 5.08)
				(name "VCCIOA")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 5.08)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 5.08)
				(name "VCCIOB")
				(number "31")
			)
			(pin power_in line
				(at 5.08 -45.72 90)
				(length 5.08)
				(name "GND")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "ADBUS0")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "ADBUS1")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "ADBUS2")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "ADBUS3")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "ADBUS4")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "ADBUS5")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 5.08)
				(name "ADBUS6")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "ADBUS7")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "ACBUS0")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "ACBUS1")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "ACBUS2")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "ACBUS3")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "SI/WUA")
				(number "10")
			)
			(pin output line
				(at 22.86 0 180)
				(length 5.08)
				(name "BDBUS0")
				(number "40")
			)
			(pin output line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "BDBUS1")
				(number "39")
			)
			(pin output line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "BDBUS2")
				(number "38")
			)
			(pin output line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "BDBUS3")
				(number "37")
			)
			(pin output line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "BDBUS4")
				(number "36")
			)
			(pin output line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "BDBUS5")
				(number "35")
			)
			(pin output line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "BDBUS6")
				(number "33")
			)
			(pin output line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "BDBUS7")
				(number "32")
			)
			(pin output line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "BCBUS0")
				(number "30")
			)
			(pin output line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "BCBUS1")
				(number "29")
			)
			(pin output line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "BCBUS2")
				(number "28")
			)
			(pin output line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "BCBUS3")
				(number "27")
			)
			(pin output line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "SI/WUB")
				(number "26")
			)
			(pin output line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "~{PWREN}")
				(number "41")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT2232HL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 53.34 0)
		)
		(property "Value" "FT2232HL"
			(at 19.05 53.34 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT2232H.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hi Speed Double Channel USB UART/FIFO, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Double UART FIFO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FT2232HL_0_1")
		(symbol "FT2232HL_1_1"
			(pin power_in line
				(at -30.48 48.26 0)
				(length 3.81)
				(name "VREGIN")
				(number "50")
			)
			(pin power_out line
				(at -30.48 43.18 0)
				(length 3.81)
				(name "VREGOUT")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "DM")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "DP")
				(number "8")
			)
			(pin output line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "REF")
				(number "6")
			)
			(pin input line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "~{RESET}")
				(number "14")
			)
			(pin output line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "EECS")
				(number "63")
			)
			(pin output line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "EECLK")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "EEDATA")
				(number "61")
			)
			(pin input line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "OSCI")
				(number "2")
			)
			(pin output line
				(at -30.48 -40.64 0)
				(length 3.81)
				(name "OSCO")
				(number "3")
			)
			(pin input line
				(at -30.48 -45.72 0)
				(length 3.81)
				(name "TEST")
				(number "13")
			)
			(pin power_in line
				(at -15.24 -55.88 90)
				(length 3.81)
				(name "AGND")
				(number "10")
			)
			(pin power_in line
				(at -12.7 55.88 270)
				(length 3.81)
				(name "VPHY")
				(number "4")
			)
			(pin input line
				(at -10.16 55.88 270)
				(length 3.81)
				(name "VPLL")
				(number "9")
			)
			(pin power_in line
				(at -10.16 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -7.62 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at -5.08 55.88 270)
				(length 3.81)
				(name "VCORE")
				(number "12")
			)
			(pin power_in line
				(at -5.08 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 3.81)
				(name "VCORE")
				(number "37")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 3.81)
				(name "VCORE")
				(number "64")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "35")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "20")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "47")
			)
			(pin power_in line
				(at 7.62 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "31")
			)
			(pin power_in line
				(at 7.62 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "51")
			)
			(pin power_in line
				(at 10.16 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "42")
			)
			(pin power_in line
				(at 12.7 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 3.81)
				(name "ADBUS0")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 3.81)
				(name "ADBUS1")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 3.81)
				(name "ADBUS2")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 3.81)
				(name "ADBUS3")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 3.81)
				(name "ADBUS4")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 3.81)
				(name "ADBUS5")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 3.81)
				(name "ADBUS6")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "ADBUS7")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "ACBUS0")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "ACBUS1")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "ACBUS2")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "ACBUS3")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "ACBUS4")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "ACBUS5")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "ACBUS6")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "ACBUS7")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "BDBUS0")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "BDBUS1")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "BDBUS2")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "BDBUS3")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "BDBUS4")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "BDBUS5")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "BDBUS6")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "BDBUS7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "BCBUS0")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "BCBUS1")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "BCBUS2")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "BCBUS3")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 3.81)
				(name "BCBUS4")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 3.81)
				(name "BCBUS5")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 3.81)
				(name "BCBUS6")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 3.81)
				(name "BCBUS7")
				(number "59")
			)
			(pin output line
				(at 30.48 -43.18 180)
				(length 3.81)
				(name "~{PWREN}")
				(number "60")
			)
			(pin output line
				(at 30.48 -45.72 180)
				(length 3.81)
				(name "~{SUSPEND}")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT2232HQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 53.34 0)
		)
		(property "Value" "FT2232HQ"
			(at 19.05 53.34 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.35x4.35mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT2232H.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hi Speed Double Channel USB UART/FIFO, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Double UART FIFO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FT2232HQ_0_1")
		(symbol "FT2232HQ_1_1"
			(pin power_in line
				(at -30.48 48.26 0)
				(length 3.81)
				(name "VREGIN")
				(number "50")
			)
			(pin power_out line
				(at -30.48 43.18 0)
				(length 3.81)
				(name "VREGOUT")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "DM")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "DP")
				(number "8")
			)
			(pin output line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "REF")
				(number "6")
			)
			(pin input line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "~{RESET}")
				(number "14")
			)
			(pin output line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "EECS")
				(number "63")
			)
			(pin output line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "EECLK")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "EEDATA")
				(number "61")
			)
			(pin input line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "OSCI")
				(number "2")
			)
			(pin output line
				(at -30.48 -40.64 0)
				(length 3.81)
				(name "OSCO")
				(number "3")
			)
			(pin input line
				(at -30.48 -45.72 0)
				(length 3.81)
				(name "TEST")
				(number "13")
			)
			(pin power_in line
				(at -15.24 -55.88 90)
				(length 3.81)
				(name "AGND")
				(number "10")
			)
			(pin power_in line
				(at -12.7 55.88 270)
				(length 3.81)
				(name "VPHY")
				(number "4")
			)
			(pin input line
				(at -10.16 55.88 270)
				(length 3.81)
				(name "VPLL")
				(number "9")
			)
			(pin power_in line
				(at -10.16 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -7.62 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at -5.08 55.88 270)
				(length 3.81)
				(name "VCORE")
				(number "12")
			)
			(pin power_in line
				(at -5.08 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 3.81)
				(name "VCORE")
				(number "37")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 3.81)
				(name "VCORE")
				(number "64")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "35")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "20")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "47")
			)
			(pin power_in line
				(at 7.62 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "31")
			)
			(pin power_in line
				(at 7.62 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "51")
			)
			(pin power_in line
				(at 10.16 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "42")
			)
			(pin power_in line
				(at 10.16 -55.88 90)
				(length 3.81)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 12.7 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 3.81)
				(name "ADBUS0")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 3.81)
				(name "ADBUS1")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 3.81)
				(name "ADBUS2")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 3.81)
				(name "ADBUS3")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 3.81)
				(name "ADBUS4")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 3.81)
				(name "ADBUS5")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 3.81)
				(name "ADBUS6")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "ADBUS7")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "ACBUS0")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "ACBUS1")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "ACBUS2")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "ACBUS3")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "ACBUS4")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "ACBUS5")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "ACBUS6")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "ACBUS7")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "BDBUS0")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "BDBUS1")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "BDBUS2")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "BDBUS3")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "BDBUS4")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "BDBUS5")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "BDBUS6")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "BDBUS7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "BCBUS0")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "BCBUS1")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "BCBUS2")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "BCBUS3")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 3.81)
				(name "BCBUS4")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 3.81)
				(name "BCBUS5")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 3.81)
				(name "BCBUS6")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 3.81)
				(name "BCBUS7")
				(number "59")
			)
			(pin output line
				(at 30.48 -43.18 180)
				(length 3.81)
				(name "~{PWREN}")
				(number "60")
			)
			(pin output line
				(at 30.48 -45.72 180)
				(length 3.81)
				(name "~{SUSPEND}")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT230XQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "FT230XQ"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.1x2.1mm"
			(at 34.29 -15.24 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT230X.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to Basic UART, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB UART interface converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "FT230XQ_0_1")
		(symbol "FT230XQ_1_1"
			(pin power_out line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "3V3OUT")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "USBDM")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "USBDP")
				(number "6")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{RESET}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VCCIO")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "TXD")
				(number "15")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "RXD")
				(number "2")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "~{RTS}")
				(number "16")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "~{CTS}")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "CBUS0")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "CBUS1")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "CBUS2")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "CBUS3")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT230XS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 15.24 0)
		)
		(property "Value" "FT230XS"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 25.4 -15.24 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT230X.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to Basic UART, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB UART interface converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "FT230XS_0_1")
		(symbol "FT230XS_1_1"
			(pin power_out line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "3V3OUT")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "USBDM")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "USBDP")
				(number "8")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{RESET}")
				(number "11")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VCCIO")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "13")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "TXD")
				(number "1")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "RXD")
				(number "4")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "~{RTS}")
				(number "2")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "~{CTS}")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "CBUS0")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "CBUS1")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "CBUS2")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "CBUS3")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT231XQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 20.32 0)
		)
		(property "Value" "FT231XQ"
			(at 6.35 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 34.29 -20.32 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT231X.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to Full Handshake UART, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB UART interface converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FT231XQ_0_1")
		(symbol "FT231XQ_1_1"
			(pin power_out line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "3V3OUT")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "USBDM")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "USBDP")
				(number "8")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "~{RESET}")
				(number "11")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 3.81)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 3.81)
				(name "VCCIO")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "21")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "TXD")
				(number "17")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "RXD")
				(number "1")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "~{RTS}")
				(number "19")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "~{CTS}")
				(number "6")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "~{DTR}")
				(number "18")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "~{DSR}")
				(number "4")
			)
			(pin input line
				(at 17.78 0 180)
				(length 3.81)
				(name "~{DCD}")
				(number "5")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "~{RI}")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "CBUS0")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "CBUS1")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "CBUS2")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "CBUS3")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT231XS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 20.32 0)
		)
		(property "Value" "FT231XS"
			(at 7.62 20.32 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_3.9x8.7mm_P0.635mm"
			(at 25.4 -20.32 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT231X.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to Full Handshake UART, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB UART interface converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "FT231XS_0_1")
		(symbol "FT231XS_1_1"
			(pin power_out line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "3V3OUT")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "USBDM")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "USBDP")
				(number "11")
			)
			(pin input line
				(at -17.78 0 0)
				(length 3.81)
				(name "~{RESET}")
				(number "14")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 3.81)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 3.81)
				(name "VCCIO")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 3.81)
				(name "GND")
				(number "16")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "TXD")
				(number "20")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "RXD")
				(number "4")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "~{RTS}")
				(number "2")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "~{CTS}")
				(number "9")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "~{DTR}")
				(number "1")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "~{DSR}")
				(number "7")
			)
			(pin input line
				(at 17.78 0 180)
				(length 3.81)
				(name "~{DCD}")
				(number "8")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "~{RI}")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "CBUS0")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "CBUS1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "CBUS2")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "CBUS3")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT232BM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 30.48 0)
		)
		(property "Value" "FT232BM"
			(at 11.43 30.48 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 25.4 -30.48 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT232BM.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hi Speed Single Channel USB UART/FIFO, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB Single UART FIFO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "FT232BM_0_1")
		(symbol "FT232BM_1_1"
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "D0/TXD")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "D1/RXD")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "D2/~{RST}")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "D3/~{CTS}")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "D4/~{DTR}")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "D5/~{DSR}")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "D6/~{DCD}")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "D7/~{RI}")
				(number "18")
			)
			(pin output line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "TXDEN")
				(number "16")
			)
			(pin output line
				(at -22.86 0 0)
				(length 3.81)
				(name "~{PWREN}")
				(number "15")
			)
			(pin input line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "PWRCTL")
				(number "14")
			)
			(pin open_collector line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "~{TXLED}")
				(number "12")
			)
			(pin open_collector line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "~{RXLED}")
				(number "11")
			)
			(pin output line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "~{SLEEP}")
				(number "10")
			)
			(pin power_in line
				(at -7.62 33.02 270)
				(length 3.81)
				(name "VCCIO")
				(number "13")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 3.81)
				(name "VCC")
				(number "26")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 3.81)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 3.81)
				(name "AVCC")
				(number "30")
			)
			(pin power_in line
				(at 5.08 -33.02 90)
				(length 3.81)
				(name "AGND")
				(number "29")
			)
			(pin power_out line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "3V3OUT")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "USBDM")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "USBDP")
				(number "7")
			)
			(pin output line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "~{RSTOUT}")
				(number "5")
			)
			(pin input line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "XTIN")
				(number "27")
			)
			(pin output line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "XTOUT")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "EECS")
				(number "32")
			)
			(pin output line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "EESK")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "EEDATA")
				(number "2")
			)
			(pin input line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "TEST")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT232H"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 35.56 0)
		)
		(property "Value" "FT232H"
			(at 12.7 35.56 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT232H.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hi Speed Single Channel USB UART/FIFO, LQFP/QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB Single UART FIFO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.5mm* LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FT232H_0_1")
		(symbol "FT232H_1_1"
			(pin power_in line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "VREGIN")
				(number "40")
			)
			(pin power_in line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "VCCD")
				(number "39")
			)
			(pin power_out line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "VCCCORE")
				(number "38")
			)
			(pin power_out line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "VCCA")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "DM")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "DP")
				(number "7")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "~{RESET}")
				(number "34")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "REF")
				(number "5")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "EECS")
				(number "45")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "EECLK")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "EEDATA")
				(number "43")
			)
			(pin input line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "XCSI")
				(number "1")
			)
			(pin output line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "XCSO")
				(number "2")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "TEST")
				(number "42")
			)
			(pin power_in line
				(at -10.16 -38.1 90)
				(length 3.81)
				(name "AGND")
				(number "4")
			)
			(pin power_in line
				(at -7.62 -38.1 90)
				(length 3.81)
				(name "AGND")
				(number "9")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 3.81)
				(name "VPHY")
				(number "3")
			)
			(pin power_in line
				(at -5.08 -38.1 90)
				(length 3.81)
				(name "AGND")
				(number "41")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 3.81)
				(name "VPLL")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "VCCIO")
				(number "12")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 3.81)
				(name "VCCIO")
				(number "24")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "22")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 3.81)
				(name "VCCIO")
				(number "46")
			)
			(pin power_in line
				(at 5.08 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "23")
			)
			(pin power_in line
				(at 7.62 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "35")
			)
			(pin power_in line
				(at 10.16 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "36")
			)
			(pin power_in line
				(at 12.7 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "47")
			)
			(pin power_in line
				(at 15.24 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "ADBUS0")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "ADBUS1")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "ADBUS2")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "ADBUS3")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "ADBUS4")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "ADBUS5")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "ADBUS6")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "ADBUS7")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "ACBUS0")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "ACBUS1")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "ACBUS2")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "ACBUS3")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "ACBUS4")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "ACBUS5")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "ACBUS6")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "ACBUS7")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "ACBUS8")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "ACBUS9")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT232RL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 22.86 0)
		)
		(property "Value" "FT232RL"
			(at 10.16 22.86 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 27.94 -22.86 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT232R.pdf"
			(at 0 0 0)
		)
		(property "Description" "USB to Serial Interface, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB Serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "FT232RL_0_1")
		(symbol "FT232RL_1_1"
			(pin power_out line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "3V3OUT")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "USBD+")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "USBD-")
				(number "16")
			)
			(pin input line
				(at -20.32 0 0)
				(length 3.81)
				(name "~{RESET}")
				(number "19")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "OSCI")
				(number "27")
			)
			(pin output line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "OSCO")
				(number "28")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "TEST")
				(number "26")
			)
			(pin power_in line
				(at -5.08 -25.4 90)
				(length 3.81)
				(name "AGND")
				(number "25")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 3.81)
				(name "VCCIO")
				(number "4")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 3.81)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 5.08 -25.4 90)
				(length 3.81)
				(name "GND")
				(number "21")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "TXD")
				(number "1")
			)
			(pin input line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "RXD")
				(number "5")
			)
			(pin output output_low
				(at 20.32 12.7 180)
				(length 3.81)
				(name "RTS")
				(number "3")
			)
			(pin input input_low
				(at 20.32 10.16 180)
				(length 3.81)
				(name "CTS")
				(number "11")
			)
			(pin output output_low
				(at 20.32 7.62 180)
				(length 3.81)
				(name "DTR")
				(number "2")
			)
			(pin input input_low
				(at 20.32 5.08 180)
				(length 3.81)
				(name "DCR")
				(number "9")
			)
			(pin input input_low
				(at 20.32 2.54 180)
				(length 3.81)
				(name "DCD")
				(number "10")
			)
			(pin input input_low
				(at 20.32 0 180)
				(length 3.81)
				(name "RI")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "CBUS0")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "CBUS1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "CBUS2")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "CBUS3")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "CBUS4")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT234XD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.494 14.986 0)
		)
		(property "Value" "FT234XD"
			(at -15.494 12.954 0)
		)
		(property "Footprint" "Package_DFN_QFN:WDFN-12-1EP_3x3mm_P0.45mm_EP1.7x2.5mm"
			(at -1.27 -19.812 0)
		)
		(property "Datasheet" "https://ftdichip.com/wp-content/uploads/2024/05/DS_FT234XD.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Full Speed USB to Basic UART, WDFN-12"
			(at -1.27 0 0)
		)
		(property "ki_keywords" "FTDI Serial"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WDFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "FT234XD_0_0")
		(symbol "FT234XD_1_0"
			(pin power_out line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "3V3OUT")
				(number "3")
				(alternate "3V3IN" power_in line)
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "USBDP")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "USBDM")
				(number "1")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "2")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCCIO")
				(number "9")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "TXD/D0")
				(number "7")
				(alternate "D0" bidirectional line)
				(alternate "TXD" output line)
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "RXD/D1")
				(number "10")
				(alternate "D1" bidirectional line)
				(alternate "RXD" input line)
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "~{RTS}/D2")
				(number "8")
				(alternate "D2" bidirectional line)
				(alternate "~{RTS}" output line)
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "~{CTS}/D3")
				(number "11")
				(alternate "D3" bidirectional line)
				(alternate "~{CTS}" input line)
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "CBUS0")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT240XQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 25.4 0)
		)
		(property "Value" "FT240XQ"
			(at 6.35 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 34.29 -25.4 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT240X.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to 8-Bit FIFO, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB FIFO interface converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FT240XQ_0_1")
		(symbol "FT240XQ_1_1"
			(pin power_out line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "3V3OUT")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "USBDM")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "USBDP")
				(number "10")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "~{RESET}")
				(number "13")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin power_out line
				(at 0 27.94 270)
				(length 3.81)
				(name "VCORE")
				(number "14")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "VCCIO")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "DATA0")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "DATA1")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "DATA2")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "DATA3")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "DATA4")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "DATA5")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "DATA6")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "DATA7")
				(number "2")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "~{RXF}")
				(number "18")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "~{TXE}")
				(number "17")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "~{RD}")
				(number "8")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "~{WR}")
				(number "9")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "~{SI/WU}")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "CBUS5")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "CBUS6")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT240XS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 25.4 0)
		)
		(property "Value" "FT240XS"
			(at 7.62 25.4 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_3.9x8.7mm_P0.635mm"
			(at 25.4 -25.4 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT240X.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to 8-Bit FIFO, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB FIFO interface converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "FT240XS_0_1")
		(symbol "FT240XS_1_1"
			(pin power_out line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "3V3OUT")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "USBDM")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "USBDP")
				(number "13")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "~{RESET}")
				(number "16")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "VCC")
				(number "18")
			)
			(pin passive line
				(at -2.54 -27.94 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 0 27.94 270)
				(length 3.81)
				(name "VCORE")
				(number "17")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "VCCIO")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "DATA0")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "DATA1")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "DATA2")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "DATA3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "DATA4")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "DATA5")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "DATA6")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "DATA7")
				(number "5")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "~{RXF}")
				(number "21")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "~{TXE}")
				(number "20")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "~{RD}")
				(number "11")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "~{WR}")
				(number "12")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "~{SI/WU}")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "CBUS5")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "CBUS6")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT245BM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 27.94 0)
		)
		(property "Value" "FT245BM"
			(at 11.43 27.94 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 22.86 -27.94 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT245BM.pdf"
			(at 0 0 0)
		)
		(property "Description" "Full Speed USB to 8-Bit FIFO, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB FIFO Interface Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "FT245BM_0_1")
		(symbol "FT245BM_1_1"
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "D0")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "D1")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "D2")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "D3")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "D4")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "D5")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "D6")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "D7")
				(number "18")
			)
			(pin input line
				(at -22.86 0 0)
				(length 3.81)
				(name "~{RD}")
				(number "16")
			)
			(pin input line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "WR")
				(number "15")
			)
			(pin output line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "~{TXE}")
				(number "14")
			)
			(pin output line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "~{RXF}")
				(number "12")
			)
			(pin input line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "SI/WU")
				(number "11")
			)
			(pin output line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "~{PWREN}")
				(number "10")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 3.81)
				(name "VCCIO")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VCC")
				(number "26")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 3.81)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 3.81)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 7.62 30.48 270)
				(length 3.81)
				(name "AVCC")
				(number "30")
			)
			(pin power_out line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "3V3OUT")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "USBDM")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "USBDP")
				(number "7")
			)
			(pin output line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "~{RSTOUT}")
				(number "5")
			)
			(pin input line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "XTIN")
				(number "27")
			)
			(pin output line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "XTOUT")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "EECS")
				(number "32")
			)
			(pin output line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "EESK")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "EEDATA")
				(number "2")
			)
			(pin input line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "TEST")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT4222HQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 21.59 0)
		)
		(property "Value" "FT4222HQ"
			(at 10.16 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 36.83 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT4222H.pdf"
			(at -13.97 21.59 0)
		)
		(property "Description" "USB 2.0 to Quad SPI or I2C Bridge, VQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB SPI I2C FTDI Bridge Converter Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FT4222HQ_0_1")
		(symbol "FT4222HQ_1_1"
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "DEBUGGER")
				(number "1")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "~{STEST_RST}")
				(number "2")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "DCNF0")
				(number "4")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "DCNF1")
				(number "5")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "XSCI")
				(number "18")
			)
			(pin output line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "XSCO")
				(number "19")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RREF")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "DM")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "DP")
				(number "23")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "VBUS_DET")
				(number "30")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VCCIO")
				(number "7")
			)
			(pin passive line
				(at -5.08 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "DGND")
				(number "28")
			)
			(pin power_in line
				(at -5.08 -22.86 90)
				(length 2.54)
				(name "DGND")
				(number "6")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VCCIN")
				(number "26")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "UGND")
				(number "20")
			)
			(pin passive line
				(at -2.54 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "UGND")
				(number "24")
			)
			(pin unspecified line
				(at 0 22.86 270)
				(length 2.54)
				(name "VOUT3V3")
				(number "25")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "27")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VPP")
				(number "29")
			)
			(pin power_in line
				(at 2.54 -22.86 90)
				(length 2.54)
				(name "EP")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "SCK")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "MOSI")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "MISO")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "IO2")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "IO3")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "GPIO0")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "GPIO1")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "GPIO2")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "GPIO3")
				(number "16")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "~{SS0O}")
				(number "17")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "~{SS}")
				(number "32")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "BCD_DET")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT4232H"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 53.34 0)
		)
		(property "Value" "FT4232H"
			(at 19.05 53.34 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.ftdichip.com/Support/Documents/DataSheets/ICs/DS_FT4232H.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hi Speed Quad Channel USB UART/FIFO, LQFP/QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB Quad UART FIFO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm* LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FT4232H_0_1")
		(symbol "FT4232H_1_1"
			(pin power_in line
				(at -30.48 48.26 0)
				(length 3.81)
				(name "VREGIN")
				(number "50")
			)
			(pin power_out line
				(at -30.48 43.18 0)
				(length 3.81)
				(name "VREGOUT")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "DM")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "DP")
				(number "8")
			)
			(pin input line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "REF")
				(number "6")
			)
			(pin input line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "~{RESET}")
				(number "14")
			)
			(pin output line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "EECS")
				(number "63")
			)
			(pin output line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "EECLK")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "EEDATA")
				(number "61")
			)
			(pin input line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "OSCI")
				(number "2")
			)
			(pin output line
				(at -30.48 -40.64 0)
				(length 3.81)
				(name "OSCO")
				(number "3")
			)
			(pin input line
				(at -30.48 -45.72 0)
				(length 3.81)
				(name "TEST")
				(number "13")
			)
			(pin power_in line
				(at -15.24 -53.34 90)
				(length 3.81)
				(name "AGND")
				(number "10")
			)
			(pin power_in line
				(at -12.7 55.88 270)
				(length 3.81)
				(name "VPHY")
				(number "4")
			)
			(pin power_in line
				(at -10.16 55.88 270)
				(length 3.81)
				(name "VPLL")
				(number "9")
			)
			(pin power_in line
				(at -10.16 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -7.62 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at -5.08 55.88 270)
				(length 3.81)
				(name "VCORE")
				(number "12")
			)
			(pin power_in line
				(at -5.08 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 3.81)
				(name "VCORE")
				(number "37")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 3.81)
				(name "VCORE")
				(number "64")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "35")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "20")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "47")
			)
			(pin power_in line
				(at 7.62 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "31")
			)
			(pin power_in line
				(at 7.62 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "51")
			)
			(pin power_in line
				(at 10.16 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "42")
			)
			(pin power_in line
				(at 12.7 55.88 270)
				(length 3.81)
				(name "VCCIO")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 3.81)
				(name "ADBUS0")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 3.81)
				(name "ADBUS1")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 3.81)
				(name "ADBUS2")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 3.81)
				(name "ADBUS3")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 3.81)
				(name "ADBUS4")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 3.81)
				(name "ADBUS5")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 3.81)
				(name "ADBUS6")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "ADBUS7")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "BDBUS0")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "BDBUS1")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "BDBUS2")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "BDBUS3")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "BDBUS4")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "BDBUS5")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "BDBUS6")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "BDBUS7")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "CDBUS0")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "CDBUS1")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "CDBUS2")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "CDBUS3")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "CDBUS4")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "CDBUS5")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "CDBUS6")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "CDBUS7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "DDBUS0")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "DDBUS1")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "DDBUS2")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "DDBUS3")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 3.81)
				(name "DDBUS4")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 3.81)
				(name "DDBUS5")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 3.81)
				(name "DDBUS6")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 3.81)
				(name "DDBUS7")
				(number "59")
			)
			(pin output line
				(at 30.48 -43.18 180)
				(length 3.81)
				(name "~{PWREN}")
				(number "60")
			)
			(pin output line
				(at 30.48 -45.72 180)
				(length 3.81)
				(name "~{SUSPEND}")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FT601Q"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 62.23 0)
		)
		(property "Value" "FT601Q"
			(at 16.51 62.23 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-76-1EP_9x9mm_P0.4mm_EP5.81x6.31mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ftdichip.com/wp-content/uploads/2020/07/DS_FT600Q-FT601Q-IC-Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "USB 3.0 Super-Speed to 32 bits Sync FIFO, QFN-76"
			(at 0 0 0)
		)
		(property "ki_keywords" "FTDI USB 3.0 FIFO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*1EP*9x9mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "FT601Q_0_1")
		(symbol "FT601Q_1_1"
			(pin input line
				(at -22.86 58.42 0)
				(length 2.54)
				(name "~{SIWU}")
				(number "10")
			)
			(pin input line
				(at -22.86 53.34 0)
				(length 2.54)
				(name "~{RESET}")
				(number "15")
			)
			(pin input line
				(at -22.86 48.26 0)
				(length 2.54)
				(name "~{WR}")
				(number "11")
			)
			(pin input line
				(at -22.86 45.72 0)
				(length 2.54)
				(name "~{RD}")
				(number "12")
			)
			(pin input line
				(at -22.86 43.18 0)
				(length 2.54)
				(name "~{OE}")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "~{WAKEUP}")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "GPIO0")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "GPIO1")
				(number "18")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "DM")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "DP")
				(number "23")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "RIDN")
				(number "34")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "RIDP")
				(number "35")
			)
			(pin output line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "TODN")
				(number "31")
			)
			(pin output line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "TODP")
				(number "32")
			)
			(pin power_out line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "DV10")
				(number "39")
			)
			(pin power_in line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "VD10")
				(number "3")
			)
			(pin passive line
				(at -22.86 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "VD10")
				(number "30")
			)
			(pin passive line
				(at -22.86 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "VD10")
				(number "33")
			)
			(pin passive line
				(at -22.86 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "VD10")
				(number "48")
			)
			(pin power_in line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "AVDD")
				(number "2")
			)
			(pin input line
				(at -22.86 -40.64 0)
				(length 2.54)
				(name "XI")
				(number "21")
			)
			(pin output line
				(at -22.86 -43.18 0)
				(length 2.54)
				(name "XO")
				(number "22")
			)
			(pin input line
				(at -22.86 -50.8 0)
				(length 2.54)
				(name "RREF")
				(number "27")
			)
			(pin no_connect line
				(at -20.32 -48.26 0)
				(length 2.54)
				(hide yes)
				(name "Reserved")
				(number "19")
			)
			(pin power_in line
				(at -7.62 63.5 270)
				(length 2.54)
				(name "VBUS")
				(number "37")
			)
			(pin power_in line
				(at -2.54 63.5 270)
				(length 2.54)
				(name "VCC33")
				(number "20")
			)
			(pin passive line
				(at -2.54 63.5 270)
				(length 2.54)
				(hide yes)
				(name "VCC33")
				(number "24")
			)
			(pin passive line
				(at -2.54 63.5 270)
				(length 2.54)
				(hide yes)
				(name "VCC33")
				(number "38")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 2.54)
				(name "VDDA")
				(number "28")
			)
			(pin power_in line
				(at 0 -60.96 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -60.96 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -60.96 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -60.96 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at 0 -60.96 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "77")
			)
			(pin power_in line
				(at 7.62 63.5 270)
				(length 2.54)
				(name "VCCIO")
				(number "14")
			)
			(pin passive line
				(at 7.62 63.5 270)
				(length 2.54)
				(hide yes)
				(name "VCCIO")
				(number "49")
			)
			(pin passive line
				(at 7.62 63.5 270)
				(length 2.54)
				(hide yes)
				(name "VCCIO")
				(number "59")
			)
			(pin passive line
				(at 7.62 63.5 270)
				(length 2.54)
				(hide yes)
				(name "VCCIO")
				(number "68")
			)
			(pin output line
				(at 22.86 58.42 180)
				(length 2.54)
				(name "CLK")
				(number "58")
			)
			(pin output line
				(at 22.86 53.34 180)
				(length 2.54)
				(name "~{TXE}")
				(number "8")
			)
			(pin output line
				(at 22.86 50.8 180)
				(length 2.54)
				(name "~{RXF}")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 2.54)
				(name "DATA_0")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "DATA_1")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "DATA_2")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "DATA_3")
				(number "43")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "DATA_4")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "DATA_5")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "DATA_6")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "DATA_7")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "DATA_8")
				(number "50")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "DATA_9")
				(number "51")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "DATA_10")
				(number "52")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "DATA_11")
				(number "53")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "DATA_12")
				(number "54")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "DATA_13")
				(number "55")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "DATA_14")
				(number "56")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "DATA_15")
				(number "57")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "DATA_16")
				(number "60")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "DATA_17")
				(number "61")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "DATA_18")
				(number "62")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "DATA_19")
				(number "63")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "DATA_20")
				(number "64")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "DATA_21")
				(number "65")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "DATA_22")
				(number "66")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "DATA_23")
				(number "67")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "DATA_24")
				(number "69")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "DATA_25")
				(number "70")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "DATA_26")
				(number "71")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "DATA_27")
				(number "72")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "DATA_28")
				(number "73")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "DATA_29")
				(number "74")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "DATA_30")
				(number "75")
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 2.54)
				(name "DATA_31")
				(number "76")
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 2.54)
				(name "BE_0")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 2.54)
				(name "BE_1")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 2.54)
				(name "BE_2")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 2.54)
				(name "BE_3")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FUSB302BMPX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "FUSB302BMPX"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-14-1EP_2.5x2.5mm_P0.5mm_EP1.45x1.45mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FUSB302B-D.PDF"
			(at 2.54 -10.16 0)
		)
		(property "Description" "Programmable USB Type-C Controller w/PD, I2C address 0x22, WQFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB USB-C PD Power Delivery PHY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FUSB302BMPX_0_1")
		(symbol "FUSB302BMPX_1_1"
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "SCL")
				(number "6")
			)
			(pin open_collector line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "INT_N")
				(number "5")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at -2.54 10.16 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCONN")
				(number "12")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VCONN")
				(number "13")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VBUS")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "CC1")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(hide yes)
				(name "CC1")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "CC2")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "CC2")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FUSB303BTMX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "FUSB303BTMX"
			(at 7.62 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_X2QFN-12_1.6x1.6mm_P0.4mm"
			(at 3.302 -24.638 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/fusb303b-d.pdf"
			(at 3.302 -19.304 0)
		)
		(property "Description" "USB Type-C port controller with I2C and GPIO control, X2QFN-12"
			(at 3.302 -21.844 0)
		)
		(property "ki_keywords" "usb type-c controller i2c gpio source sink drp"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*X2QFN*1.6x1.6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "FUSB303BTMX_0_1")
		(symbol "FUSB303BTMX_1_1"
			(pin input line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "~{EN}")
				(number "11")
			)
			(pin open_collector line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "INT_N/OUT3")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "SDA/OUT1")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "SCL/OUT2")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "ADDR/ORIENT")
				(number "5")
			)
			(pin open_collector line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "ID")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "VBUS_DET")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "CC1")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CC2")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PORT/~{DEBUG}")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FUSB307BMPX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 13.97 0)
		)
		(property "Value" "FUSB307BMPX"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-16-1EP_3x3mm_P0.5mm_EP1.75x1.75mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FUSB307B-D.PDF"
			(at 0 -15.24 0)
		)
		(property "Description" "USB Type-C Port Controller with USB-PD, WQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB USB-C PD Power Delivery PHY TCPC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FUSB307BMPX_0_1")
		(symbol "FUSB307BMPX_1_1"
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "SDA1/SCL2")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "SCL1/SDA2")
				(number "11")
			)
			(pin open_collector line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "INT_N")
				(number "10")
			)
			(pin tri_state line
				(at -17.78 0 0)
				(length 2.54)
				(name "ORIENT/I2C_ADDR")
				(number "4")
			)
			(pin open_collector line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DBG_N")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "GPIO1")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "GPIO2")
				(number "9")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCONN")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VBUS")
				(number "6")
			)
			(pin power_out line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "LDO")
				(number "5")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "SRC")
				(number "13")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "SNK")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "CC1")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "CC2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IP2721"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 -10.16 0)
		)
		(property "Value" "IP2721"
			(at 7.62 -12.7 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2006111335_INJOINIC-IP2721_C603176.pdf"
			(at 0 0 0)
		)
		(property "Description" "USB TYPEC  PD Controller Interface, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB TYPEC PD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*16*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "IP2721_0_1")
		(symbol "IP2721_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "CC1")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "CC2")
				(number "12")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -5.08 7.62 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -2.54 7.62 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VIN")
				(number "2")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 2.54 7.62 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 2.54 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 5.08 7.62 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VBUSG")
				(number "1")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VBUS")
				(number "16")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "SEL")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MA8601"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "MA8601"
			(at 13.97 27.94 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_3.9x9.9mm_P0.635mm"
			(at 26.67 -38.1 0)
		)
		(property "Datasheet" "https://datasheetspdf.com/pdf-file/1312067/Prolific/MA8601/1"
			(at 0 0 0)
		)
		(property "Description" "USB 2.0 High Speed 4-Port Hub Controller, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "4-Port, EEPROM, High Speed, Hub, USB2.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x9.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "MA8601_0_1")
		(symbol "MA8601_1_1"
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "DPU")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "DMU")
				(number "15")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "~{SRST}")
				(number "17")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PSELF")
				(number "19")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "OVCJ")
				(number "26")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "VBUS_IN")
				(number "18")
			)
			(pin output line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "XO")
				(number "2")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "XI")
				(number "3")
			)
			(pin passive line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "REXT")
				(number "14")
			)
			(pin power_in line
				(at -7.62 27.94 270)
				(length 2.54)
				(name "VDD5")
				(number "20")
			)
			(pin power_out line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDDR33")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDD33")
				(number "13")
			)
			(pin power_out line
				(at 5.08 27.94 270)
				(length 2.54)
				(name "VDDR12")
				(number "12")
			)
			(pin power_in line
				(at 7.62 27.94 270)
				(length 2.54)
				(name "VDD12")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "DP1")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "DM1")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "DP2")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "DM2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "DP3")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DM3")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "DP4")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "DM4")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "TEST/EESDA")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "LED1/EESCL")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "LED2/GLEDEN")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "DRV")
				(number "22")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "~{PWRJ}")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2200-I-MQ"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 -19.05 0)
		)
		(property "Value" "MCP2200-I-MQ"
			(at -20.32 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_5x5mm_P0.65mm_EP3.35x3.35mm"
			(at 27.94 -20.32 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/200022228D.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "USB 2.0 to UART Protocol Converter with GPIO, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*20*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2200-I-MQ_0_1")
		(symbol "MCP2200-I-MQ_1_1"
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "RST")
				(number "1")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "RX")
				(number "9")
			)
			(pin output line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "TX")
				(number "7")
			)
			(pin output line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "RTS")
				(number "8")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "CTS")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "GP0/SSPND")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "GP1/USB-CFG")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "GP2")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "GP3")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "GP4")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "GP5")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "GP6/RxLED")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "GP7/TxLED")
				(number "2")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "17")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "V_USB")
				(number "14")
			)
			(pin no_connect line
				(at 20.32 0 180)
				(length 2.54)
				(hide yes)
				(name "EP")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "D+")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "D-")
				(number "15")
			)
			(pin input line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "OSC1")
				(number "19")
			)
			(pin output line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "OSC2")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2200-I-SO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 -19.05 0)
		)
		(property "Value" "MCP2200-I-SO"
			(at -20.32 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/200022228D.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "USB 2.0 to UART Protocol Converter with GPIO, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*20*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP2200-I-SO_0_1")
		(symbol "MCP2200-I-SO_1_1"
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "RST")
				(number "4")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "RX")
				(number "12")
			)
			(pin output line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "TX")
				(number "10")
			)
			(pin output line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "RTS")
				(number "11")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "CTS")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "GP0/SSPND")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "GP1/USB-CFG")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "GP2")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "GP3")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "GP4")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "GP5")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "GP6/RxLED")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "GP7/TxLED")
				(number "5")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "V_USB")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "D+")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "D-")
				(number "18")
			)
			(pin input line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "OSC1")
				(number "2")
			)
			(pin output line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "OSC2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2200-I-SS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 -19.05 0)
		)
		(property "Value" "MCP2200-I-SS"
			(at -20.32 19.05 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/200022228D.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "USB 2.0 to UART Protocol Converter with GPIO, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*20*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2200-I-SS_0_1")
		(symbol "MCP2200-I-SS_1_1"
			(pin input line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "RST")
				(number "4")
			)
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "RX")
				(number "12")
			)
			(pin output line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "TX")
				(number "10")
			)
			(pin output line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "RTS")
				(number "11")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "CTS")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "GP0/SSPND")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "GP1/USB-CFG")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "GP2")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "GP3")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "GP4")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "GP5")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "GP6/RxLED")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "GP7/TxLED")
				(number "5")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "V_USB")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "D+")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "D-")
				(number "18")
			)
			(pin input line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "OSC1")
				(number "2")
			)
			(pin output line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "OSC2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2210x-MQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "MCP2210x-MQ"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_5x5mm_P0.65mm_EP3.35x3.35mm"
			(at 0 25.4 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/22288A.pdf"
			(at -2.54 20.32 0)
		)
		(property "Description" "USB to SPI Protocol Converter with GPIO, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB SPI Master Converter Bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2210x-MQ_0_1")
		(symbol "MCP2210x-MQ_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{RST}")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D+")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D-")
				(number "15")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "OSC1")
				(number "19")
			)
			(pin output line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "OSC2")
				(number "20")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin passive line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "EP")
				(number "21")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 2.54)
				(name "VUSB")
				(number "14")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "17")
			)
			(pin output line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SCK")
				(number "8")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "MOSI")
				(number "6")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "MISO")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "GP0")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "GP1")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "GP2")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GP3")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GP4")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GP5")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GP6")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "GP7")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "GP8")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2210x-SO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "MCP2210x-SO"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 27.94 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/22288A.pdf"
			(at -2.54 20.32 0)
		)
		(property "Description" "USB to SPI Protocol Converter with GPIO, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB SPI Master Converter Bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP2210x-SO_0_1")
		(symbol "MCP2210x-SO_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D+")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D-")
				(number "18")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "OSC1")
				(number "2")
			)
			(pin output line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "OSC2")
				(number "3")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 2.54)
				(name "VUSB")
				(number "17")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin output line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SCK")
				(number "11")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "MOSI")
				(number "9")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "MISO")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "GP0")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "GP2")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GP3")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GP4")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GP5")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GP6")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "GP7")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "GP8")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2210x-SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "MCP2210x-SS"
			(at 10.16 19.05 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 25.4 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/22288A.pdf"
			(at -2.54 20.32 0)
		)
		(property "Description" "USB to SPI Protocol Converter with GPIO, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB SPI Master Converter Bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2210x-SS_0_1")
		(symbol "MCP2210x-SS_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D+")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D-")
				(number "18")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "OSC1")
				(number "2")
			)
			(pin output line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "OSC2")
				(number "3")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 2.54)
				(name "VUSB")
				(number "17")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin output line
				(at 10.16 15.24 180)
				(length 2.54)
				(name "SCK")
				(number "11")
			)
			(pin output line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "MOSI")
				(number "9")
			)
			(pin input line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "MISO")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "GP0")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "GP2")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GP3")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GP4")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GP5")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GP6")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "GP7")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -15.24 180)
				(length 2.54)
				(name "GP8")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2221AxML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "MCP2221AxML"
			(at 12.7 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_4x4mm_P0.65mm_EP2.5x2.5mm"
			(at 0 25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005565B.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "USB to I2C/UART Protocol Converter with GPIO, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB I2C UART Converter Bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2221AxML_0_1")
		(symbol "MCP2221AxML_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "~{RST}")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D+")
				(number "12")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "D-")
				(number "11")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "13")
			)
			(pin passive line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VUSB")
				(number "10")
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "9")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "URx")
				(number "4")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "UTx")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GP0")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GP1")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GP2")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GP3")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2221AxP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "MCP2221AxP"
			(at 12.7 16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005565B.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "USB to I2C/UART Protocol Converter with GPIO, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB I2C UART Converter Bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MCP2221AxP_0_1")
		(symbol "MCP2221AxP_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D+")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "D-")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VUSB")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "10")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "URx")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "UTx")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GP0")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GP1")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GP2")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GP3")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2221AxSL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "MCP2221AxSL"
			(at 12.7 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005565B.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "USB to I2C/UART Protocol Converter with GPIO, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB I2C UART Converter Bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MCP2221AxSL_0_1")
		(symbol "MCP2221AxSL_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D+")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "D-")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VUSB")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "10")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "URx")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "UTx")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GP0")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GP1")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GP2")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GP3")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCP2221AxST"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 16.51 0)
		)
		(property "Value" "MCP2221AxST"
			(at 12.7 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005565B.pdf"
			(at 0 17.78 0)
		)
		(property "Description" "USB to I2C/UART Protocol Converter with GPIO, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB I2C UART Converter Bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MCP2221AxST_0_1")
		(symbol "MCP2221AxST_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "~{RST}")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D+")
				(number "13")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "D-")
				(number "12")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VUSB")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "SDA")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "SCL")
				(number "10")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "URx")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "UTx")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "GP0")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GP1")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GP2")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GP3")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MP5034GJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 7.62 0)
		)
		(property "Value" "MP5034GJ"
			(at 5.08 -6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-8"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.monolithicpower.com/en/documentview/productdocument/index/version/2/document_type/Datasheet/lang/en/sku/MP5034/"
			(at 0 -10.16 0)
		)
		(property "Description" "USB charging port controller integrating QC 2.0/3.0 anc BC1.2 Protocol, TSOT-23-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Quick Charge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSOT?23*"
			(at 0 0 0)
		)
		(symbol "MP5034GJ_0_1")
		(symbol "MP5034GJ_1_1"
			(pin power_in line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "IN")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "ADJ")
				(number "5")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "DP")
				(number "8")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "DM")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STULPI01A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "STULPI01A"
			(at 8.89 24.13 0)
		)
		(property "Footprint" "Package_BGA:ST_uTFBGA-36_3.6x3.6mm_Layout6x6_P0.5mm"
			(at 2.54 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stulpi01a.pdf"
			(at -2.54 -1.27 0)
		)
		(property "Description" "High-speed USB On-The-Go ULPI transceiver"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB OTG HS PHY ULPI Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*uTFBGA*3.6x3.6mm*Layout6x6*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STULPI01A_0_1")
		(symbol "STULPI01A_1_1"
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D0")
				(number "B1")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D1")
				(number "A1")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D2")
				(number "A2")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D3")
				(number "A3")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D4")
				(number "A5")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D5")
				(number "A6")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "D6")
				(number "B6")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "D7")
				(number "C6")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CLK")
				(number "A4")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "STP")
				(number "D6")
			)
			(pin output line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "NXT")
				(number "D5")
			)
			(pin output line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "DIR")
				(number "E5")
			)
			(pin input line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "~{CS}/PWRDN")
				(number "C3")
			)
			(pin input line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "~{RESET}")
				(number "C4")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "F1")
			)
			(pin no_connect line
				(at -10.16 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "F2")
			)
			(pin passive line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "1V2V")
				(number "E6")
			)
			(pin passive line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "3V3V")
				(number "E3")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDVIO")
				(number "B2")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VDVIO")
				(number "B3")
			)
			(pin passive line
				(at 0 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VDVIO")
				(number "B5")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C5")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E1")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E4")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VBAT")
				(number "F3")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "XI")
				(number "F5")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "XO")
				(number "F6")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "ID")
				(number "D3")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DP")
				(number "D1")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "DM")
				(number "C1")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VBUS")
				(number "F4")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "~{PSW}")
				(number "D4")
			)
			(pin input line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "VB_REF_FAULT")
				(number "E2")
			)
			(pin passive line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "RREF")
				(number "C2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "STUSB4500QTR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "STUSB4500QTR"
			(at 8.89 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.7x2.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stusb4500.pdf"
			(at 0 0 0)
		)
		(property "Description" "Stand-alone USB PD controller (with sink Auto-run mode), QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB PD Type C Sink"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "STUSB4500QTR_0_1")
		(symbol "STUSB4500QTR_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "RESET")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "CC1")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "CC1DB")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "CC2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CC2DB")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "VBUS_VS_DISCH")
				(number "18")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SCL")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "SDA")
				(number "8")
			)
			(pin open_collector line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "ALERT")
				(number "19")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "ADDR0")
				(number "12")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "ADDR1")
				(number "13")
			)
			(pin no_connect line
				(at -12.7 15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VSYS")
				(number "22")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_out line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VREG_1V2")
				(number "21")
			)
			(pin power_out line
				(at 7.62 22.86 270)
				(length 2.54)
				(name "VREG_2V7")
				(number "23")
			)
			(pin open_collector line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VBUS_EN_SNK")
				(number "16")
			)
			(pin open_collector line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "POWER_OK2")
				(number "20")
			)
			(pin open_collector line
				(at 15.24 0 180)
				(length 2.54)
				(name "POWER_OK3")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DISCH")
				(number "9")
			)
			(pin open_collector line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "A_B_SIDE")
				(number "17")
			)
			(pin open_collector line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "ATTACH")
				(number "11")
			)
			(pin open_collector line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "GPIO")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2500DRC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 -11.43 0)
		)
		(property "Value" "TPS2500DRC"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2500.pdf"
			(at -2.54 -7.62 0)
		)
		(property "Description" "Integrated USB power Switch with Boost Converter, High-Efficiency Eco-mode Control Scheme, Texas S-PVSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB switch boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PVSON*N10*"
			(at 0 0 0)
		)
		(symbol "TPS2500DRC_0_1")
		(symbol "TPS2500DRC_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SW")
				(number "1")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "EN")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "ENUSB")
				(number "7")
			)
			(pin passive line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "ILIM")
				(number "6")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_out line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "USB")
				(number "9")
			)
			(pin power_out line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "AUX")
				(number "10")
			)
			(pin open_collector line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "~{FAULT}")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2513"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -7.62 0)
		)
		(property "Value" "TPS2513"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2513.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "USB Dedicated Charging Port Controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Charge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS2513_0_1")
		(symbol "TPS2513_1_1"
			(pin power_in line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin power_in line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "DP1")
				(number "1")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "DM1")
				(number "6")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "DP2")
				(number "3")
			)
			(pin input line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "DM2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2514"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 -7.62 0)
		)
		(property "Value" "TPS2514"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2513.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "USB Dedicated Charging Port Controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Charge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TPS2514_0_1")
		(symbol "TPS2514_1_1"
			(pin power_in line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "IN")
				(number "5")
			)
			(pin power_in line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 5.08 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin input line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "DP1")
				(number "1")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "DM1")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2560"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 12.7 0)
		)
		(property "Value" "TPS2560"
			(at -5.08 12.7 0)
		)
		(property "Footprint" "Package_SON:VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm_ThermalVias"
			(at 5.08 12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2560.pdf"
			(at -10.16 12.7 0)
		)
		(property "Description" "Dual channel precision adjustable current-limited power switches"
			(at 0 0 0)
		)
		(property "ki_keywords" "power switche current limited usb port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS2560_0_1")
		(symbol "TPS2560_1_1"
			(pin power_in line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "IN")
				(number "3")
			)
			(pin input inverted
				(at -15.24 0 0)
				(length 5.08)
				(name "EN1")
				(number "4")
			)
			(pin input inverted
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "EN2")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 5.08)
				(name "PAD")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "OUT1")
				(number "9")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "~{FAULT1}")
				(number "10")
			)
			(pin output line
				(at 15.24 0 180)
				(length 5.08)
				(name "OUT2")
				(number "8")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "~{FAULT2}")
				(number "6")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "ILM")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS2561"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 12.7 0)
		)
		(property "Value" "TPS2561"
			(at -5.08 12.7 0)
		)
		(property "Footprint" "Package_SON:VSON-10-1EP_3x3mm_P0.5mm_EP1.65x2.4mm_ThermalVias"
			(at 5.08 12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2561.pdf"
			(at -10.16 12.7 0)
		)
		(property "Description" "Dual channel precision adjustable current-limited power switches"
			(at 0 0 0)
		)
		(property "ki_keywords" "power switche current limited usb port"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSON*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TPS2561_0_1")
		(symbol "TPS2561_1_1"
			(pin power_in line
				(at -15.24 7.62 0)
				(length 5.08)
				(name "IN")
				(number "2")
			)
			(pin power_in line
				(at -15.24 5.08 0)
				(length 5.08)
				(name "IN")
				(number "3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 5.08)
				(name "EN1")
				(number "4")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "EN2")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 5.08)
				(name "PAD")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 5.08)
				(name "OUT1")
				(number "9")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 5.08)
				(name "~{FAULT1}")
				(number "10")
			)
			(pin output line
				(at 15.24 0 180)
				(length 5.08)
				(name "OUT2")
				(number "8")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "~{FAULT2}")
				(number "6")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 5.08)
				(name "ILM")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TPS25730D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.192 26.924 0)
		)
		(property "Value" "TPS25730D"
			(at 7.874 -26.924 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_REF0038A_WQFN-38-2EP_6x4mm_P0.4"
			(at 3.81 -53.34 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tps25730.pdf"
			(at 0.508 -39.116 0)
		)
		(property "Description" "USB Type-C and USB PD Controller, Integrated Power Switches, QFN-38"
			(at 0.254 -42.164 0)
		)
		(property "ki_keywords" "USB CC PD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*REF0038A*WQFN*38*"
			(at 0 0 0)
		)
		(symbol "TPS25730D_1_1"
			(pin power_in line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "VBUS_IN")
				(number "23")
			)
			(pin power_in line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "VBUS")
				(number "32")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "CC1")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "CC2")
				(number "29")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DRAIN")
				(number "15")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DRAIN")
				(number "30")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DRAIN")
				(number "40")
			)
			(pin power_in line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "VIN_3V3")
				(number "38")
			)
			(pin power_out line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "LDO_3V3")
				(number "1")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "ADCIN1")
				(number "2")
			)
			(pin input line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "ADCIN2")
				(number "3")
			)
			(pin input line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "ADCIN3")
				(number "5")
			)
			(pin input line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "ADCIN4")
				(number "7")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PPHV")
				(number "20")
			)
			(pin output line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "LDO_1V5")
				(number "4")
			)
			(pin open_collector line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "CAP_MIS")
				(number "6")
			)
			(pin open_collector line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "~{SINK_EN}")
				(number "19")
			)
			(pin open_collector line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PLUG_EVENT")
				(number "37")
			)
			(pin open_collector line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DBG_ACC")
				(number "10")
			)
			(pin open_collector line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PLUG_FLIP")
				(number "13")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{FAULT_IN}")
				(number "18")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "I2Ct_SCL")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "I2Ct_SDA")
				(number "8")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RESERVED")
				(number "26")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "RESERVED")
				(number "27")
			)
			(pin input line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "RESERVED")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS3USB30EDGSR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TS3USB30EDGSR"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_SO:VSSOP-10_3x3mm_P0.5mm"
			(at 20.32 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ts3usb30e.pdf"
			(at 0 0 0)
		)
		(property "Description" "ESD-Protected, High-Speed USB 2.0 (480-Mbps) 1:2 Multiplexer/Demultiplexer Switch With Single Enable, VSSOP-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb mux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TS3USB30EDGSR_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "D+")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D-")
				(number "6")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{OE}")
				(number "9")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S")
				(number "1")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "D1+")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "D1-")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "D2+")
				(number "3")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "D2-")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS3USB30ERSWR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TS3USB30ERSWR"
			(at 8.89 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-10_1.4x1.8mm_P0.4mm"
			(at 24.13 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/ts3usb30e.pdf"
			(at 0 0 0)
		)
		(property "Description" "ESD-Protected, High-Speed USB 2.0 (480-Mbps) 1:2 Multiplexer/Demultiplexer Switch With Single Enable, UQFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb mux"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1.4x1.8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TS3USB30ERSWR_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "D+")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "D-")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~{OE}")
				(number "8")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S")
				(number "10")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "D1+")
				(number "1")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "D1-")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "D2+")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "D2-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TS3USBCA410"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 24.13 0)
		)
		(property "Value" "TS3USBCA410"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-16_1.8x2.6mm_P0.4mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/ts3usbca4"
			(at 0 -31.75 0)
		)
		(property "Description" "USB Type-C, SBU 3:1 multiplexer, 500MHz bandwidth, UQFN-16"
			(at 0 -36.83 0)
		)
		(property "ki_keywords" "Texas usb-c mux i2c aux analog audio microphone uart debug"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1.8x2.6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TS3USBCA410_0_0"
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "LnBp")
				(number "7")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "LnBn")
				(number "8")
			)
		)
		(symbol "TS3USBCA410_1_0"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SBU1")
				(number "11")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SBU2")
				(number "10")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "FLIP")
				(number "14")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{OE}")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SEL0/SDA")
				(number "6")
				(alternate "SDA" bidirectional line)
				(alternate "SEL0" input line)
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SEL1/SCL")
				(number "5")
				(alternate "SCL" input line)
				(alternate "SEL1" input line)
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "I2C_EN")
				(number "12")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "MIC_GND1/Ln1")
				(number "2")
				(alternate "Ln1" passive line)
				(alternate "MIC_GND1" passive line)
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "MIC_GND2/Ln2")
				(number "3")
				(alternate "Ln2" passive line)
				(alternate "MIC_GND2" passive line)
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LnAp")
				(number "16")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "LnAn")
				(number "15")
			)
		)
		(symbol "TS3USBCA410_1_1")
		(embedded_fonts no)
	)
	(symbol "TS3USBCA420"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 24.13 0)
		)
		(property "Value" "TS3USBCA420"
			(at 2.54 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-16_1.8x2.6mm_P0.4mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/ts3usbca4"
			(at 0 -31.75 0)
		)
		(property "Description" "USB Type-C, SBU 4:1 multiplexer, 500MHz bandwidth, UQFN-16"
			(at 0 -36.83 0)
		)
		(property "ki_keywords" "Texas usb-c mux i2c aux analog audio microphone uart debug"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1.8x2.6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TS3USBCA420_0_0"
			(pin passive line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "LnBp")
				(number "7")
			)
			(pin passive line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "LnBn")
				(number "8")
			)
			(pin passive line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "LnCp")
				(number "14")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "LnCn")
				(number "13")
			)
		)
		(symbol "TS3USBCA420_1_0"
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SBU1")
				(number "11")
			)
			(pin passive line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SBU2")
				(number "10")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "~{OE}")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "SEL0/SDA")
				(number "6")
				(alternate "SDA" bidirectional line)
				(alternate "SEL0" input line)
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "SEL1/SCL")
				(number "5")
				(alternate "SCL" input line)
				(alternate "SEL1" input line)
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "I2C_EN")
				(number "12")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "MIC_GND1/Ln1")
				(number "2")
				(alternate "Ln1" passive line)
				(alternate "MIC_GND1" passive line)
			)
			(pin passive line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "MIC_GND2/Ln2")
				(number "3")
				(alternate "Ln2" passive line)
				(alternate "MIC_GND2" passive line)
			)
			(pin passive line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "LnAp")
				(number "16")
			)
			(pin passive line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "LnAn")
				(number "15")
			)
		)
		(symbol "TS3USBCA420_1_1")
		(embedded_fonts no)
	)
	(symbol "TUSB2036"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 36.83 0)
		)
		(property "Value" "TUSB2036"
			(at 0 0 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 26.67 -38.1 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tusb2036.pdf"
			(at 0 0 0)
		)
		(property "Description" "2- or 3-Port USB1.1 HUB with optional serial EEPROM"
			(at 0 0 0)
		)
		(property "ki_keywords" "2-Port, 3-Port, 3.3V, EEPROM, Full Speed, Hub, Texas Instruments, USB1.1"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "TUSB2036_0_1")
		(symbol "TUSB2036_1_1"
			(pin input line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "~{RESET}")
				(number "4")
			)
			(pin output line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "DP0PUR")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "DP0")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "DM0")
				(number "2")
			)
			(pin input line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "~{BUSPWR}")
				(number "8")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "~{OCPROT}/~{PWRSW}")
				(number "21")
			)
			(pin input line
				(at -25.4 0 0)
				(length 5.08)
				(name "~{NP3}")
				(number "24")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "NPINT0")
				(number "22")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "NPINT1")
				(number "23")
			)
			(pin tri_state line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "EECLK")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "EEDATA/~{GANGED}")
				(number "6")
			)
			(pin input line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "~{EXTMEM}")
				(number "26")
			)
			(pin input line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "MODE")
				(number "31")
			)
			(pin input line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "XTAL1/CLK48")
				(number "30")
			)
			(pin output line
				(at -25.4 -30.48 0)
				(length 5.08)
				(name "XTAL2")
				(number "29")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 5.08)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 5.08)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 5.08)
				(name "VCC")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 5.08)
				(name "GND")
				(number "28")
			)
			(pin output line
				(at 25.4 30.48 180)
				(length 5.08)
				(name "SUSPND")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "DP1")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "DM1")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "DP2")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "DM2")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "DP3")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "DM3")
				(number "19")
			)
			(pin input line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "~{OVRCUR1}")
				(number "10")
			)
			(pin input line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "~{OVRCUR2}")
				(number "14")
			)
			(pin input line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "~{OVRCUR3}")
				(number "18")
			)
			(pin output line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "~{PWRON1}")
				(number "9")
			)
			(pin output line
				(at 25.4 -27.94 180)
				(length 5.08)
				(name "~{PWRON2}")
				(number "13")
			)
			(pin output line
				(at 25.4 -30.48 180)
				(length 5.08)
				(name "~{PWRON3}")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TUSB320"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 11.43 0)
		)
		(property "Value" "TUSB320"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_X2QFN-12_1.6x1.6mm_P0.4mm"
			(at 5.08 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tusb320.pdf"
			(at 0 0 0)
		)
		(property "Description" "USB Type-C Configuration Channel Logic and Port Control, X2QFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB PD CC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?X2QFN*1.6x1.6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TUSB320_0_1")
		(symbol "TUSB320_1_1"
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SDA/OUT1")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SCL/OUT2")
				(number "8")
			)
			(pin open_collector line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "~{INT}/OUT3")
				(number "6")
			)
			(pin open_collector line
				(at -15.24 0 0)
				(length 2.54)
				(name "ID")
				(number "9")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "~{EN}")
				(number "11")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VBUS_DET")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CC1")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "CC2")
				(number "2")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PORT")
				(number "3")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "ADDR")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TUSB321"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 11.43 0)
		)
		(property "Value" "TUSB321"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_X2QFN-12_1.6x1.6mm_P0.4mm"
			(at 5.08 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tusb321.pdf"
			(at 0 0 0)
		)
		(property "Description" "USB Type-C Configuration Channel Logic and Port Control with VCONN, X2QFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB CC PD VCONN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?X2QFN*1.6x1.6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TUSB321_1_1"
			(pin open_collector line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "OUT1")
				(number "7")
			)
			(pin open_collector line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "OUT2")
				(number "8")
			)
			(pin open_collector line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "~{VCONN_FAULT}")
				(number "6")
			)
			(pin open_collector line
				(at -15.24 0 0)
				(length 2.54)
				(name "ID")
				(number "9")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CURRENT_MODE")
				(number "3")
			)
			(pin open_collector line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DIR")
				(number "11")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VBUS_DET")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CC1")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "CC2")
				(number "2")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PORT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TUSB322I"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 11.43 0)
		)
		(property "Value" "TUSB322I"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_X2QFN-12_1.6x1.6mm_P0.4mm"
			(at 6.35 -13.97 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/tusb322i.pdf"
			(at 7.62 -22.86 0)
		)
		(property "Description" "USB Type-C Configuration Channel Logic and Port Control with VCONN, X2QFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB VCONN PD CC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?X2QFN*1.6x1.6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TUSB322I_1_1"
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "SDA/OUT1")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "SCL/OUT2")
				(number "8")
			)
			(pin open_collector line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "~{INT}/OUT3")
				(number "6")
			)
			(pin open_collector line
				(at -15.24 0 0)
				(length 2.54)
				(name "ID")
				(number "9")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "~{EN}")
				(number "11")
			)
			(pin open_collector line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DIR")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VBUS_DET")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CC1")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "CC2")
				(number "2")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "ADDR")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TUSB4041I"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 53.34 0)
		)
		(property "Value" "TUSB4041I"
			(at 15.24 50.8 0)
		)
		(property "Footprint" "Package_QFP:HTQFP-64-1EP_10x10mm_P0.5mm_EP8x8mm_Mask4.4x4.4mm_ThermalVias"
			(at 30.48 50.8 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tusb4041i.pdf"
			(at -7.62 5.08 0)
		)
		(property "Description" "four port USB 2.0 Hub"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB2.0 hub"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HTQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TUSB4041I_0_1")
		(symbol "TUSB4041I_1_1"
			(pin input line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "USB_VBUS")
				(number "16")
			)
			(pin input line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "GRSTz")
				(number "18")
			)
			(pin input line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "XI")
				(number "30")
			)
			(pin output line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "XO")
				(number "29")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "USB_DP_UP")
				(number "21")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "USB_DM_UP")
				(number "22")
			)
			(pin input line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "USB_R1")
				(number "32")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "SCL/SMBCLK")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "SDA/SMBDAT")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "SMBUSz")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "FULLPWRMGMTz/SMBA1")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PWRCTL_POL")
				(number "9")
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "GANGED/SMBA2/HS_UP")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "AUTOENz/HS_SUSPEND")
				(number "13")
			)
			(pin input line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "TEST")
				(number "17")
			)
			(pin no_connect line
				(at -27.94 7.62 0)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "44")
			)
			(pin no_connect line
				(at -27.94 5.08 0)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "46")
			)
			(pin no_connect line
				(at -27.94 2.54 0)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "47")
			)
			(pin no_connect line
				(at -27.94 0 0)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "51")
			)
			(pin no_connect line
				(at -27.94 -2.54 0)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "52")
			)
			(pin no_connect line
				(at -27.94 -5.08 0)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "54")
			)
			(pin no_connect line
				(at -27.94 -7.62 0)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "55")
			)
			(pin no_connect line
				(at -27.94 -10.16 0)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "58")
			)
			(pin no_connect line
				(at -27.94 -12.7 0)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "59")
			)
			(pin no_connect line
				(at -27.94 -15.24 0)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "61")
			)
			(pin no_connect line
				(at -27.94 -17.78 0)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "62")
			)
			(pin power_in line
				(at -22.86 53.34 270)
				(length 5.08)
				(name "VDD33")
				(number "48")
			)
			(pin power_in line
				(at -20.32 53.34 270)
				(length 5.08)
				(name "VDD33")
				(number "31")
			)
			(pin power_in line
				(at -17.78 53.34 270)
				(length 5.08)
				(name "VDD33")
				(number "20")
			)
			(pin power_in line
				(at -15.24 53.34 270)
				(length 5.08)
				(name "VDD33")
				(number "2")
			)
			(pin power_in line
				(at -10.16 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "63")
			)
			(pin power_in line
				(at -7.62 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "60")
			)
			(pin power_in line
				(at -5.08 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "53")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "45")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "37")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "65")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "25")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "19")
			)
			(pin no_connect line
				(at 27.94 -17.78 180)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "23")
			)
			(pin no_connect line
				(at 27.94 -20.32 180)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "24")
			)
			(pin no_connect line
				(at 27.94 -22.86 180)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "26")
			)
			(pin no_connect line
				(at 27.94 -25.4 180)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "27")
			)
			(pin no_connect line
				(at 27.94 -27.94 180)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "35")
			)
			(pin no_connect line
				(at 27.94 -30.48 180)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "36")
			)
			(pin no_connect line
				(at 27.94 -33.02 180)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "38")
			)
			(pin no_connect line
				(at 27.94 -35.56 180)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "39")
			)
			(pin no_connect line
				(at 27.94 -38.1 180)
				(length 5.08)
				(hide yes)
				(name "RSVD")
				(number "43")
			)
			(pin no_connect line
				(at 27.94 -43.18 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at 27.94 -45.72 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "40")
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "USB_DP_DN1")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "USB_DM_DN1")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PWRCTL1/BATEN1")
				(number "4")
			)
			(pin input line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "OVERCUR1z")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "USB_DP_DN2")
				(number "41")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "USB_DM_DN2")
				(number "42")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PWRCTL2/BATEN2")
				(number "3")
			)
			(pin input line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "OVERCUR2z")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "USB_DP_DN3")
				(number "49")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "USB_DM_DN3")
				(number "50")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PWRCTL3/BATEN3")
				(number "1")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "OVERCUR3z")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "USB_DP_DN4")
				(number "56")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "USB_DM_DN4")
				(number "57")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PWRCTL4/BATEN4")
				(number "64")
			)
			(pin input line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "OVERCUR4z")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TUSB7340"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "TUSB7340"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_S-PWQFN-N100_EP5.5x5.5mm_ThermalVias"
			(at 58.42 -60.96 0)
		)
		(property "Datasheet" "http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=tusb7320&fileType=pdf"
			(at 76.2 -63.5 0)
		)
		(property "Description" "USB 3.0 xHCI Host Controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB HUB PCIE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S?PWQFN?N100*"
			(at 0 0 0)
		)
		(symbol "TUSB7340_0_1")
		(symbol "TUSB7340_1_1"
			(pin input line
				(at -63.5 45.72 0)
				(length 5.08)
				(name "GRST#")
				(number "A15")
			)
			(pin output line
				(at -63.5 40.64 0)
				(length 5.08)
				(name "PCIE_TXP")
				(number "B38")
			)
			(pin output line
				(at -63.5 38.1 0)
				(length 5.08)
				(name "PCIE_TXN")
				(number "A41")
			)
			(pin input line
				(at -63.5 35.56 0)
				(length 5.08)
				(name "PCIE_RXP")
				(number "B39")
			)
			(pin input line
				(at -63.5 33.02 0)
				(length 5.08)
				(name "PCIE_RXN")
				(number "A42")
			)
			(pin input clock
				(at -63.5 30.48 0)
				(length 5.08)
				(name "PCIE_REFCLKP")
				(number "A45")
			)
			(pin input clock
				(at -63.5 27.94 0)
				(length 5.08)
				(name "PCIE_REFCLKN")
				(number "B41")
			)
			(pin output line
				(at -63.5 25.4 0)
				(length 5.08)
				(name "WAKE#")
				(number "B35")
			)
			(pin input line
				(at -63.5 22.86 0)
				(length 5.08)
				(name "CLKREQ#")
				(number "B36")
			)
			(pin input line
				(at -63.5 20.32 0)
				(length 5.08)
				(name "PERST#")
				(number "A40")
			)
			(pin input line
				(at -63.5 15.24 0)
				(length 5.08)
				(name "XI")
				(number "A23")
			)
			(pin output line
				(at -63.5 12.7 0)
				(length 5.08)
				(name "XO")
				(number "A22")
			)
			(pin input line
				(at -63.5 10.16 0)
				(length 5.08)
				(name "VSS_OSC")
				(number "B21")
			)
			(pin input line
				(at -63.5 5.08 0)
				(length 5.08)
				(name "FREQSEL")
				(number "B14")
			)
			(pin input line
				(at -63.5 -2.54 0)
				(length 5.08)
				(name "JTAG_TCK")
				(number "A32")
			)
			(pin input line
				(at -63.5 -5.08 0)
				(length 5.08)
				(name "JTAG_TMS")
				(number "B30")
			)
			(pin output line
				(at -63.5 -7.62 0)
				(length 5.08)
				(name "JTAG_TDO")
				(number "B31")
			)
			(pin input line
				(at -63.5 -10.16 0)
				(length 5.08)
				(name "JTAG_RST#")
				(number "B32")
			)
			(pin input line
				(at -63.5 -12.7 0)
				(length 5.08)
				(name "JTAG_TDI")
				(number "A35")
			)
			(pin bidirectional line
				(at -63.5 -17.78 0)
				(length 5.08)
				(name "SDA")
				(number "A2")
			)
			(pin bidirectional line
				(at -63.5 -20.32 0)
				(length 5.08)
				(name "SCL")
				(number "B2")
			)
			(pin input line
				(at -63.5 -25.4 0)
				(length 5.08)
				(name "AUX_DET")
				(number "A52")
			)
			(pin bidirectional line
				(at -63.5 -30.48 0)
				(length 5.08)
				(name "R1EXT")
				(number "A24")
			)
			(pin bidirectional line
				(at -63.5 -33.02 0)
				(length 5.08)
				(name "R1EXTRTN")
				(number "B23")
			)
			(pin bidirectional line
				(at -63.5 -38.1 0)
				(length 5.08)
				(name "GPIO0")
				(number "A49")
			)
			(pin bidirectional line
				(at -63.5 -40.64 0)
				(length 5.08)
				(name "GPIO1")
				(number "B46")
			)
			(pin bidirectional line
				(at -63.5 -43.18 0)
				(length 5.08)
				(name "GPIO2")
				(number "B47")
			)
			(pin bidirectional line
				(at -63.5 -45.72 0)
				(length 5.08)
				(name "GPIO3")
				(number "B48")
			)
			(pin power_in line
				(at -43.18 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "A1")
			)
			(pin power_in line
				(at -40.64 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "B1")
			)
			(pin power_in line
				(at -38.1 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "A4")
			)
			(pin power_in line
				(at -35.56 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "A6")
			)
			(pin power_in line
				(at -33.02 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "A9")
			)
			(pin power_in line
				(at -30.48 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "A12")
			)
			(pin power_in line
				(at -27.94 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "A16")
			)
			(pin power_in line
				(at -25.4 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "B17")
			)
			(pin power_in line
				(at -22.86 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "B19")
			)
			(pin no_connect line
				(at -22.86 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B8")
			)
			(pin power_in line
				(at -20.32 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "B24")
			)
			(pin no_connect line
				(at -20.32 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B13")
			)
			(pin power_in line
				(at -17.78 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "A28")
			)
			(pin no_connect line
				(at -17.78 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A14")
			)
			(pin power_in line
				(at -15.24 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "A31")
			)
			(pin no_connect line
				(at -15.24 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A26")
			)
			(pin power_in line
				(at -12.7 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "A33")
			)
			(pin no_connect line
				(at -12.7 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B29")
			)
			(pin power_in line
				(at -10.16 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "A38")
			)
			(pin no_connect line
				(at -10.16 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A43")
			)
			(pin power_in line
				(at -7.62 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "B37")
			)
			(pin power_in line
				(at -5.08 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "B40")
			)
			(pin power_in line
				(at -2.54 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "B42")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "A50")
			)
			(pin power_in line
				(at 0 -63.5 90)
				(length 5.08)
				(name "VSS")
				(number "B20")
			)
			(pin power_in line
				(at 2.54 63.5 270)
				(length 5.08)
				(name "VDD11")
				(number "B44")
			)
			(pin power_in line
				(at 2.54 -63.5 90)
				(length 5.08)
				(name "VSS_EP")
				(number "A53")
			)
			(pin power_in line
				(at 5.08 -63.5 90)
				(length 5.08)
				(name "VSS")
				(number "C1")
			)
			(pin power_in line
				(at 7.62 63.5 270)
				(length 5.08)
				(name "VDD33")
				(number "A3")
			)
			(pin power_in line
				(at 7.62 -63.5 90)
				(length 5.08)
				(name "VSS")
				(number "C2")
			)
			(pin power_in line
				(at 10.16 63.5 270)
				(length 5.08)
				(name "VDD33")
				(number "A34")
			)
			(pin power_in line
				(at 10.16 -63.5 90)
				(length 5.08)
				(name "VSS")
				(number "C3")
			)
			(pin power_in line
				(at 12.7 63.5 270)
				(length 5.08)
				(name "VDD33")
				(number "A39")
			)
			(pin power_in line
				(at 12.7 -63.5 90)
				(length 5.08)
				(name "VSS")
				(number "C4")
			)
			(pin power_in line
				(at 15.24 63.5 270)
				(length 5.08)
				(name "VDD33")
				(number "A47")
			)
			(pin power_in line
				(at 17.78 63.5 270)
				(length 5.08)
				(name "VDD33")
				(number "A51")
			)
			(pin power_in line
				(at 22.86 63.5 270)
				(length 5.08)
				(name "VDDA_3P3")
				(number "B4")
			)
			(pin power_in line
				(at 25.4 63.5 270)
				(length 5.08)
				(name "VDDA_3P3")
				(number "B11")
			)
			(pin power_in line
				(at 27.94 63.5 270)
				(length 5.08)
				(name "VDDA_3P3")
				(number "A19")
			)
			(pin power_in line
				(at 30.48 63.5 270)
				(length 5.08)
				(name "VDDA_3P3")
				(number "A21")
			)
			(pin power_in line
				(at 33.02 63.5 270)
				(length 5.08)
				(name "VDDA_3P3")
				(number "B22")
			)
			(pin power_in line
				(at 35.56 63.5 270)
				(length 5.08)
				(name "VDDA_3P3")
				(number "A25")
			)
			(pin power_in line
				(at 38.1 63.5 270)
				(length 5.08)
				(name "VDDA_3P3")
				(number "B26")
			)
			(pin power_in line
				(at 40.64 63.5 270)
				(length 5.08)
				(name "VDDA_3P3")
				(number "A44")
			)
			(pin bidirectional line
				(at 63.5 45.72 180)
				(length 5.08)
				(name "USB_DP_DN1")
				(number "A20")
			)
			(pin bidirectional line
				(at 63.5 43.18 180)
				(length 5.08)
				(name "USB_DM_DN1")
				(number "B18")
			)
			(pin output line
				(at 63.5 40.64 180)
				(length 5.08)
				(name "USB_SSTXP_DN1")
				(number "A17")
			)
			(pin output line
				(at 63.5 38.1 180)
				(length 5.08)
				(name "USB_SSTXN_DN1")
				(number "B15")
			)
			(pin input line
				(at 63.5 35.56 180)
				(length 5.08)
				(name "USB_SSRXP_DN1")
				(number "A18")
			)
			(pin input line
				(at 63.5 33.02 180)
				(length 5.08)
				(name "USB_SSRXN_DN1")
				(number "B16")
			)
			(pin bidirectional line
				(at 63.5 27.94 180)
				(length 5.08)
				(name "USB_DP_DN2")
				(number "B12")
			)
			(pin bidirectional line
				(at 63.5 25.4 180)
				(length 5.08)
				(name "USB_DM_DN2")
				(number "A13")
			)
			(pin output line
				(at 63.5 22.86 180)
				(length 5.08)
				(name "USB_SSTXP_DN2")
				(number "A11")
			)
			(pin output line
				(at 63.5 20.32 180)
				(length 5.08)
				(name "USB_SSTXN_DN2")
				(number "B10")
			)
			(pin input line
				(at 63.5 17.78 180)
				(length 5.08)
				(name "USB_SSRXP_DN2")
				(number "B9")
			)
			(pin input line
				(at 63.5 15.24 180)
				(length 5.08)
				(name "USB_SSRXN_DN2")
				(number "A10")
			)
			(pin bidirectional line
				(at 63.5 10.16 180)
				(length 5.08)
				(name "USB_DP_DN3")
				(number "B25")
			)
			(pin bidirectional line
				(at 63.5 7.62 180)
				(length 5.08)
				(name "USB_DM_DN3")
				(number "A27")
			)
			(pin output line
				(at 63.5 5.08 180)
				(length 5.08)
				(name "USB_SSTXP_DN3")
				(number "B28")
			)
			(pin output line
				(at 63.5 2.54 180)
				(length 5.08)
				(name "USB_SSTXN_DN3")
				(number "A30")
			)
			(pin input line
				(at 63.5 0 180)
				(length 5.08)
				(name "USB_SSRXP_DN3")
				(number "B27")
			)
			(pin input line
				(at 63.5 -2.54 180)
				(length 5.08)
				(name "USB_SSRXN_DN3")
				(number "A29")
			)
			(pin bidirectional line
				(at 63.5 -7.62 180)
				(length 5.08)
				(name "USB_DP_DN4")
				(number "B5")
			)
			(pin bidirectional line
				(at 63.5 -10.16 180)
				(length 5.08)
				(name "USB_DM_DN4")
				(number "A5")
			)
			(pin input line
				(at 63.5 -12.7 180)
				(length 5.08)
				(name "USB_SSTXP_DN4")
				(number "B7")
			)
			(pin input line
				(at 63.5 -15.24 180)
				(length 5.08)
				(name "USB_SSTXN_DN4")
				(number "A8")
			)
			(pin input line
				(at 63.5 -17.78 180)
				(length 5.08)
				(name "USB_SSRXP_DN4")
				(number "B6")
			)
			(pin input line
				(at 63.5 -20.32 180)
				(length 5.08)
				(name "USB_SSRXN_DN4")
				(number "A7")
			)
			(pin output line
				(at 63.5 -25.4 180)
				(length 5.08)
				(name "PWRON1#")
				(number "B33")
			)
			(pin input line
				(at 63.5 -27.94 180)
				(length 5.08)
				(name "OVERCUR1#")
				(number "A36")
			)
			(pin output line
				(at 63.5 -30.48 180)
				(length 5.08)
				(name "PWRON2#")
				(number "B34")
			)
			(pin input line
				(at 63.5 -33.02 180)
				(length 5.08)
				(name "OVERCUR2#")
				(number "A37")
			)
			(pin output line
				(at 63.5 -35.56 180)
				(length 5.08)
				(name "PWRON3#")
				(number "A46")
			)
			(pin input line
				(at 63.5 -38.1 180)
				(length 5.08)
				(name "OVERCUR3#")
				(number "B43")
			)
			(pin output line
				(at 63.5 -40.64 180)
				(length 5.08)
				(name "PWRON4#")
				(number "A48")
			)
			(pin input line
				(at 63.5 -43.18 180)
				(length 5.08)
				(name "OVERCUR4#")
				(number "B45")
			)
			(pin output line
				(at 63.5 -48.26 180)
				(length 5.08)
				(name "SMI")
				(number "B3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TUSB8041"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 53.34 0)
		)
		(property "Value" "TUSB8041"
			(at 15.24 50.8 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP6x6mm_ThermalVias"
			(at 30.48 50.8 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tusb8041.pdf"
			(at -7.62 5.08 0)
		)
		(property "Description" "four port USB 3.0 Hub"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB3.0 hub"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TUSB8041_0_1")
		(symbol "TUSB8041_1_1"
			(pin input line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "USB_VBUS")
				(number "48")
			)
			(pin input line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "GRSTz")
				(number "50")
			)
			(pin input line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "XI")
				(number "62")
			)
			(pin output line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "XO")
				(number "61")
			)
			(pin output line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "USB_SSTXP_UP")
				(number "55")
			)
			(pin output line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "USB_SSTXM_UP")
				(number "56")
			)
			(pin input line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "USB_SSRXP_UP")
				(number "58")
			)
			(pin input line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "USB_SSRXM_UP")
				(number "59")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "USB_DP_UP")
				(number "53")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "USB_DM_UP")
				(number "54")
			)
			(pin input line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "USB_R1")
				(number "64")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "SCL/SMBCLK")
				(number "38")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "SDA/SMBDAT")
				(number "37")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "SMBUSz/SS_SUSPEND")
				(number "39")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "FULLPWRMGMTz/SMBA1/SS_UP")
				(number "40")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PWRCTL_POL")
				(number "41")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "GANGED/SMBA2/HS_UP")
				(number "42")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "AUTOENz/HS_SUSPEND")
				(number "45")
			)
			(pin input line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "TEST")
				(number "49")
			)
			(pin power_in line
				(at -22.86 53.34 270)
				(length 5.08)
				(name "VDD33")
				(number "63")
			)
			(pin power_in line
				(at -20.32 53.34 270)
				(length 5.08)
				(name "VDD33")
				(number "52")
			)
			(pin power_in line
				(at -17.78 53.34 270)
				(length 5.08)
				(name "VDD33")
				(number "34")
			)
			(pin power_in line
				(at -15.24 53.34 270)
				(length 5.08)
				(name "VDD33")
				(number "16")
			)
			(pin power_in line
				(at -10.16 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "57")
			)
			(pin power_in line
				(at -7.62 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at -5.08 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "21")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "65")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 7.62 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin no_connect line
				(at 27.94 -45.72 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "60")
			)
			(pin output line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "USB_SSTXP_DN1")
				(number "3")
			)
			(pin output line
				(at 33.02 43.18 180)
				(length 5.08)
				(name "USB_SSTXM_DN1")
				(number "4")
			)
			(pin input line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "USB_SSRXP_DN1")
				(number "6")
			)
			(pin input line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "USB_SSRXM_DN1")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "USB_DP_DN1")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "USB_DM_DN1")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PWRCTL1/BATEN1")
				(number "36")
			)
			(pin input line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "OVERCUR1z")
				(number "46")
			)
			(pin output line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "USB_SSTXP_DN2")
				(number "11")
			)
			(pin output line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "USB_SSTXM_DN2")
				(number "12")
			)
			(pin input line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "USB_SSRXP_DN2")
				(number "14")
			)
			(pin input line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "USB_SSRXM_DN2")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "USB_DP_DN2")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "USB_DM_DN2")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PWRCTL2/BATEN2")
				(number "35")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "OVERCUR2z")
				(number "47")
			)
			(pin output line
				(at 33.02 0 180)
				(length 5.08)
				(name "USB_SSTXP_DN3")
				(number "19")
			)
			(pin output line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "USB_SSTXM_DN3")
				(number "20")
			)
			(pin input line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "USB_SSRXP_DN3")
				(number "22")
			)
			(pin input line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "USB_SSRXM_DN3")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "USB_DP_DN3")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "USB_DM_DN3")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PWRCTL3/BATEN3")
				(number "33")
			)
			(pin input line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "OVERCUR3z")
				(number "44")
			)
			(pin output line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "USB_SSTXP_DN4")
				(number "26")
			)
			(pin output line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "USB_SSTXM_DN4")
				(number "27")
			)
			(pin input line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "USB_SSRXP_DN4")
				(number "29")
			)
			(pin input line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "USB_SSRXM_DN4")
				(number "30")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "USB_DP_DN4")
				(number "24")
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "USB_DM_DN4")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "PWRCTL4/BATEN4")
				(number "32")
			)
			(pin input line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "OVERCUR4z")
				(number "43")
			)
		)
		(embedded_fonts no)
	)
	(symbol "UPD720202K8-7x1-BAA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 34.29 0)
		)
		(property "Value" "UPD720202K8-7x1-BAA"
			(at 16.51 34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.7x5.7mm"
			(at 0 46.99 0)
		)
		(property "Datasheet" "https://www.renesas.com/us/en/document/dst/upd720201upd720202-datasheet"
			(at 0 49.53 0)
		)
		(property "Description" "PCIe to USB 3.0 Host Controller, 2 ports, QFN-48"
			(at 0 52.07 0)
		)
		(property "ki_keywords" "PCIe USB 3.0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*EP5.7x5.7mm*"
			(at 0 0 0)
		)
		(symbol "UPD720202K8-7x1-BAA_1_1"
			(pin input line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PECLKP")
				(number "1")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PECLKN")
				(number "2")
			)
			(pin output line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PETXP")
				(number "4")
			)
			(pin output line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PETXN")
				(number "5")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PERXP")
				(number "7")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PERXN")
				(number "8")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "~{PERST}")
				(number "47")
			)
			(pin open_collector line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "~{PEWAKE}")
				(number "48")
			)
			(pin open_collector line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "~{PECREQ}")
				(number "10")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "SPISCK")
				(number "15")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "~{SPICS}")
				(number "14")
			)
			(pin output line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "SPISI")
				(number "16")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "SPISO")
				(number "13")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PONRSTB")
				(number "11")
			)
			(pin open_collector line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "SMIB")
				(number "46")
			)
			(pin input line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "XT1")
				(number "24")
			)
			(pin output line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "XT2")
				(number "23")
			)
			(pin passive line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "RREF")
				(number "26")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "AVDD33")
				(number "25")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "AVDD33")
				(number "3")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDD33")
				(number "12")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD33")
				(number "22")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD33")
				(number "34")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD33")
				(number "43")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin passive line
				(at 2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD10")
				(number "21")
			)
			(pin passive line
				(at 2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD10")
				(number "30")
			)
			(pin passive line
				(at 2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD10")
				(number "33")
			)
			(pin passive line
				(at 2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD10")
				(number "39")
			)
			(pin passive line
				(at 2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD10")
				(number "42")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "VDD10")
				(number "6")
			)
			(pin passive line
				(at 2.54 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VDD10")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "U2DM1")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "U2DP1")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "U3RXDN1")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "U3RXDP1")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "U3TXDN1")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "U3TXDP1")
				(number "28")
			)
			(pin input line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "~{OCI1}")
				(number "19")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PPON1")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "U2DM2")
				(number "45")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "U2DP2")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "U3RXDN2")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "U3RXDP2")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "U3TXDN2")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "U3TXDP2")
				(number "37")
			)
			(pin input line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "~{OCI2}")
				(number "17")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PPON2")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB2504"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 44.45 0)
		)
		(property "Value" "USB2504"
			(at -19.05 -44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 21.59 -45.72 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/00002250A.pdf"
			(at 35.56 -46.99 0)
		)
		(property "Description" "USB 2.0 4-Port Hub Hi-Speed Hub Controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB2.0 Hi-Speed-USB-Hub Hub-Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "USB2504_0_1")
		(symbol "USB2504_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "~{RESET}")
				(number "49")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "VBUS_DET")
				(number "52")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "USBD0_P")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "USBD0_N")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "SDA/SMBDATA")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "SCL/SMBCLK")
				(number "35")
			)
			(pin input line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "TEST1")
				(number "48")
			)
			(pin input line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "TEST0")
				(number "31")
			)
			(pin input line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "CFG_SEL0")
				(number "36")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "CFG_SEL1")
				(number "50")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "CFG_SEL2")
				(number "59")
			)
			(pin input line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "CLKIN_EN")
				(number "47")
			)
			(pin input line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "XTAL1/CLKIN")
				(number "58")
			)
			(pin output line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "XTAL2")
				(number "57")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PRTPWR_POL")
				(number "23")
			)
			(pin input line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "SELF_PWR")
				(number "51")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "ATEST/REG_EN")
				(number "62")
			)
			(pin input line
				(at -25.4 -40.64 0)
				(length 2.54)
				(name "RBIAS")
				(number "63")
			)
			(pin no_connect line
				(at -22.86 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -22.86 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -22.86 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin no_connect line
				(at -22.86 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDDA33")
				(number "1")
			)
			(pin passive line
				(at -5.08 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDDA33")
				(number "13")
			)
			(pin passive line
				(at -5.08 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDDA33")
				(number "7")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD33")
				(number "28")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDDA33PLL")
				(number "61")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "10")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "16")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "41")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "53")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "55")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "64")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD18")
				(number "30")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD18")
				(number "42")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD18")
				(number "54")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDA18PLL")
				(number "60")
			)
			(pin no_connect line
				(at 22.86 -40.64 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "USBD1_P")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "USBD1_N")
				(number "5")
			)
			(pin output line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "PRTPWR1")
				(number "45")
			)
			(pin input line
				(at 25.4 33.02 180)
				(length 2.54)
				(name "~{OCS1}")
				(number "46")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "AM1/GANG_EN")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "GR1/NON_REM0")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "USBD2_P")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "USBD2_N")
				(number "9")
			)
			(pin output line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "PRTPWR2")
				(number "43")
			)
			(pin input line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "~{OCS2}")
				(number "44")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "AM2/MTT_EN")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "GR2/NON_REM1")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "USBD3_P")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "USBD3_N")
				(number "11")
			)
			(pin output line
				(at 25.4 0 180)
				(length 2.54)
				(name "PRTPWR3")
				(number "39")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "~{OCS3}")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "AM3")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "GR3/PRT_DIS0")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "USBD4_P")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "USBD4_N")
				(number "15")
			)
			(pin output line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "PRTPWR4")
				(number "37")
			)
			(pin input line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "~{OCS4}")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "AM4/LED_EN")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "GR4/PRT_DIS1")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB2514B_Bi"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 40.64 0)
		)
		(property "Value" "USB2514B_Bi"
			(at -20.32 38.1 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-36-1EP_6x6mm_P0.5mm_EP3.7x3.7mm"
			(at 33.02 -38.1 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00001692C.pdf"
			(at 40.64 -40.64 0)
		)
		(property "Description" "USB 2.0 Hi-Speed Hub Controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB2.0 Hi-Speed-USB-Hub Hub-Controller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*6x6mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "USB2514B_Bi_0_1")
		(symbol "USB2514B_Bi_1_1"
			(pin input line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "VBUS_DET")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "USBDM_UP")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "USBDP_UP")
				(number "31")
			)
			(pin input line
				(at -27.94 10.16 0)
				(length 2.54)
				(name "RESET_N")
				(number "26")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "TEST")
				(number "11")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "RBIAS")
				(number "35")
			)
			(pin input clock
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "XTALIN/CLKIN")
				(number "33")
			)
			(pin output line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "XTALOUT")
				(number "32")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "PLLFILT")
				(number "34")
			)
			(pin input line
				(at -27.94 -12.7 0)
				(length 2.54)
				(name "CRFILT")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "SCL/SMBCLK/CFG_SEL0")
				(number "24")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "SDA/SMBDATA/NON_REM1")
				(number "22")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "SUSP_IND/LOCAL_PWR/NON_REM0")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 2.54)
				(name "HS_IND/CFG_SEL1")
				(number "25")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VDDA33")
				(number "5")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDDA33")
				(number "10")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDDA33")
				(number "29")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDDA33")
				(number "36")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "37")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD33")
				(number "15")
			)
			(pin power_in line
				(at 7.62 38.1 270)
				(length 2.54)
				(name "VDD33")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "USBDM_DN1/PRT_DIS_M1")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 2.54)
				(name "USBDP_DN1/PRT_DIS_P1")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "PRTPWR1/BC_EN1")
				(number "12")
			)
			(pin input line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "OCS_N1")
				(number "13")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 2.54)
				(name "USBDM_DN2/PRT_DIS_M2")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 2.54)
				(name "USBDP_DN2/PRT_DIS_P2")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 2.54)
				(name "PRTPWR2/BC_EN2")
				(number "16")
			)
			(pin input line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "OCS_N2")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 2.54)
				(name "USBDM_DN3/PRT_DIS_M3")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 2.54)
				(name "USBDP_DN3/PRT_DIS_P3")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "PRTPWR3/BC_EN3")
				(number "18")
			)
			(pin input line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "OCS_N3")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "USBDM_DN4/PRT_DIS_M4")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 2.54)
				(name "USBDP_DN4/PRT_DIS_P4")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "PRTPWR4/BC_EN4")
				(number "20")
			)
			(pin input line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "OCS_N4")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB3250-ABZJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 31.75 0)
		)
		(property "Value" "USB3250-ABZJ"
			(at 13.97 31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_8x8mm_P0.5mm_EP4.3x4.3mm"
			(at 1.27 -36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00002142A.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hi-Speed USB Device Transceiver with UTMI Interface, QFN-56"
			(at 0 0 0)
		)
		(property "ki_keywords" "HS FS Device USB PHY UTMI"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "USB3250-ABZJ_0_1")
		(symbol "USB3250-ABZJ_1_1"
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "DATA0")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "DATA1")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "DATA2")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "DATA3")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "DATA4")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "DATA5")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "DATA6")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "DATA7")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "DATA8")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "DATA9")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "DATA10")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "DATA11")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "DATA12")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "DATA13")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "DATA14")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "DATA15")
				(number "25")
			)
			(pin output line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "CLKOUT")
				(number "49")
			)
			(pin input line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "XI")
				(number "10")
			)
			(pin output line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "XO")
				(number "11")
			)
			(pin passive line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "RBIAS")
				(number "6")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "VDDA3.3")
				(number "4")
			)
			(pin passive line
				(at -5.08 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDDA3.3")
				(number "7")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 2.54)
				(name "VDD3.3")
				(number "15")
			)
			(pin passive line
				(at -2.54 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD3.3")
				(number "28")
			)
			(pin passive line
				(at -2.54 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD3.3")
				(number "43")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "VSS")
				(number "14")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "33")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "48")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "55")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "56")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "EP")
				(number "57")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "VDD1.8")
				(number "16")
			)
			(pin passive line
				(at 2.54 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD1.8")
				(number "23")
			)
			(pin passive line
				(at 2.54 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD1.8")
				(number "38")
			)
			(pin passive line
				(at 2.54 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD1.8")
				(number "53")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "VSSA")
				(number "1")
			)
			(pin passive line
				(at 2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSSA")
				(number "5")
			)
			(pin passive line
				(at 2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSSA")
				(number "8")
			)
			(pin passive line
				(at 2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSSA")
				(number "9")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "VDDA1.8")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "DM")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "DP")
				(number "3")
			)
			(pin input line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "TXVALID")
				(number "45")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "TXREADY")
				(number "51")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "RXACTIVE")
				(number "50")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "RXVALID")
				(number "46")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "RXERROR")
				(number "52")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "VALIDH")
				(number "47")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DATABUS16_8")
				(number "54")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "XCVRSELECT")
				(number "17")
			)
			(pin input line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "TERMSELECT")
				(number "18")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "~{SUSPEND}")
				(number "13")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "RESET")
				(number "24")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "OPMODE0")
				(number "20")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "OPMODE1")
				(number "19")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "LINESTATE0")
				(number "22")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "LINESTATE1")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB3300-EZK"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "USB3300-EZK"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 33.02 -31.75 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00001783C.pdf"
			(at 0 0 0)
		)
		(property "Description" "Hi-Speed USB Host, Device or OTG PHY with ULPI Interface"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB OTG Hi-Speed PHY ULPI Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*32*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "USB3300-EZK_0_1")
		(symbol "USB3300-EZK_1_1"
			(pin power_in line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "VBUS")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "DM")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "DP")
				(number "7")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "ID")
				(number "5")
			)
			(pin output line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "XO")
				(number "27")
			)
			(pin input line
				(at -20.32 0 0)
				(length 3.81)
				(name "XI")
				(number "28")
			)
			(pin output line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "CPEN")
				(number "3")
			)
			(pin input line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "EXTVBUS")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "REG_EN")
				(number "31")
			)
			(pin passive line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "RBIAS")
				(number "32")
			)
			(pin power_in line
				(at -5.08 27.94 270)
				(length 3.81)
				(name "VDD3.3")
				(number "6")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "VDD3.3")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "VDD3.3")
				(number "25")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "VDD3.3")
				(number "30")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "GND")
				(number "33")
			)
			(pin power_out line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "VDD1.8")
				(number "15")
			)
			(pin power_out line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "VDD1.8")
				(number "26")
			)
			(pin power_out line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "VDDA1.8")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "DATA7")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "DATA6")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "DATA5")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "DATA4")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "DATA3")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "DATA2")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "DATA1")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "DATA0")
				(number "24")
			)
			(pin output line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "NXT")
				(number "11")
			)
			(pin output line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "DIR")
				(number "12")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "STP")
				(number "13")
			)
			(pin output line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "CLKOUT")
				(number "14")
			)
			(pin input line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "RESET")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB3341"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "USB3341"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 12.7 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/334x.pdf"
			(at 12.7 5.08 0)
		)
		(property "Description" "Hi-Speed USB ULPI Transceiver, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB ULPI Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "USB3341_0_1")
		(symbol "USB3341_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "~{RESETB}")
				(number "21")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VBUS")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DP")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DM")
				(number "14")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "ID")
				(number "18")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "REFCLK")
				(number "20")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "RBIAS")
				(number "19")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VBAT")
				(number "16")
			)
			(pin power_out line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD33")
				(number "15")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "25")
			)
			(pin power_out line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDD18")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "SPK_L")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "SPK_R")
				(number "12")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "CLKOUT")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DATA0")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DATA1")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DATA2")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "DATA3")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DATA4")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DATA5")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DATA6")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DATA7")
				(number "10")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "DIR")
				(number "24")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "STP")
				(number "23")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "NXT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB3343"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "USB3343"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 12.7 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/334x.pdf"
			(at 12.7 7.62 0)
		)
		(property "Description" "Hi-Speed USB ULPI Transceiver, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB ULPI Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "USB3343_0_1")
		(symbol "USB3343_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "~{RESETB}")
				(number "22")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VBUS")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DP")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DM")
				(number "14")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "ID")
				(number "18")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "XO")
				(number "20")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "REFCLK/XI")
				(number "21")
			)
			(pin passive line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "RBIAS")
				(number "19")
			)
			(pin power_in line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VBAT")
				(number "16")
			)
			(pin power_out line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD33")
				(number "15")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "25")
			)
			(pin power_out line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDD18")
				(number "23")
			)
			(pin power_in line
				(at 7.62 22.86 270)
				(length 2.54)
				(name "VDDIO")
				(number "9")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "CLKOUT")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DATA0")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DATA1")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "DATA2")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "DATA3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "DATA4")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DATA5")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DATA6")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DATA7")
				(number "12")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "DIR")
				(number "1")
			)
			(pin input line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "STP")
				(number "24")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "NXT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "USB3740B-AI2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "USB3740B-AI2"
			(at 10.16 8.89 0)
		)
		(property "Footprint" ""
			(at 30.48 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00001725D.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "USB 2.0 Switch with ESD Protection, UQFN-10 Pitch 0.4 mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB 2.0 High Speed Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1.3x1.8mm?P0.4mm* UQFN*1.6x2.1mm?P0.5mm*"
			(at 0 0 0)
		)
		(symbol "USB3740B-AI2_0_1")
		(symbol "USB3740B-AI2_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "DP")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "DM")
				(number "9")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OE_N")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "S")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "DP_2")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "DM_2")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "DP_1")
				(number "2")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "DM_1")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "XR21B1424"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 67.31 0)
		)
		(property "Value" "XR21B1424"
			(at 11.43 67.31 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 21.59 -67.31 0)
		)
		(property "Datasheet" "https://assets.maxlinear.com/web/documents/xr21b1424.pdf"
			(at 0 0 0)
		)
		(property "Description" "USB 2.0 up to 12Mbps, Quad Channel USB UART/FIFO, RS485 capability, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Quad UART FIFO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "XR21B1424_0_1")
		(symbol "XR21B1424_1_1"
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 2.54)
				(name "USB_D+")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 2.54)
				(name "USB_D-")
				(number "10")
			)
			(pin output line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "USB_STAT1")
				(number "25")
			)
			(pin output line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "USB_STAT2")
				(number "18")
			)
			(pin passive line
				(at -25.4 -60.96 0)
				(length 2.54)
				(name "~{TEST}")
				(number "32")
			)
			(pin passive line
				(at -25.4 -63.5 0)
				(length 2.54)
				(name "~{RESET}")
				(number "17")
			)
			(pin power_in line
				(at -5.08 68.58 270)
				(length 2.54)
				(name "VCC")
				(number "12")
			)
			(pin power_in line
				(at -2.54 68.58 270)
				(length 2.54)
				(name "VIO")
				(number "11")
			)
			(pin passive line
				(at -2.54 68.58 270)
				(length 2.54)
				(hide yes)
				(name "VIO")
				(number "38")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 2.54)
				(name "VCC_REG")
				(number "13")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin input line
				(at 2.54 68.58 270)
				(length 2.54)
				(name "VBUS_SENSE")
				(number "16")
			)
			(pin output line
				(at 25.4 63.5 180)
				(length 2.54)
				(name "TXA")
				(number "64")
			)
			(pin input line
				(at 25.4 60.96 180)
				(length 2.54)
				(name "RXA")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 58.42 180)
				(length 2.54)
				(name "GPIOA9/RXTA")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 55.88 180)
				(length 2.54)
				(name "GPIOA8/TXTA")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 53.34 180)
				(length 2.54)
				(name "GPIOA7/RS485A")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 50.8 180)
				(length 2.54)
				(name "GPIOA6/CLKA")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 48.26 180)
				(length 2.54)
				(name "GPIOA5/~{RTSA}/RS485A")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 2.54)
				(name "GPIOA4/~{CTSA}")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 2.54)
				(name "GPIOA3/~{DTRA}")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "GPIOA2/~{DSRA}")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "GPIOA1/~{CDA}")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "GPIOA0/~{RIA}/~{RWKA}")
				(number "7")
			)
			(pin output line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "TXB")
				(number "40")
			)
			(pin input line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "RXB")
				(number "41")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "GPIOB9/RXTB")
				(number "34")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "GPIOB8/TXTB")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "GPIOB7/RS485B")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "GPIOB6/CLKB")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "GPIOB5/~{RTSB}/RS485B")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "GPIOB4/~{CTSB}")
				(number "43")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "GPIOB3/~{DTRB}")
				(number "44")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "GPIOB2/~{DSRB}")
				(number "45")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "GPIOB1/~{CDB}")
				(number "46")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "GPIOB0/~{RIB}/~{RWKB}")
				(number "47")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "TXC")
				(number "24")
			)
			(pin input line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "RXC")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "GPIOC9/RXTC")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "GPIOC8/TXTC")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "GPIOC7/RS485C")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "GPIOC6/CLKC")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "GPIOC5/~{RTSC}/RS485C")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "GPIOC4/~{CTSC}")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "GPIOC3/~{DTRC}")
				(number "29")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "GPIOC2/~{DSRC}")
				(number "30")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "GPIOC1/~{CDC}")
				(number "31")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 2.54)
				(name "GPIOC0/~{RIC}/~{RWKC}")
				(number "33")
			)
			(pin output line
				(at 25.4 -35.56 180)
				(length 2.54)
				(name "TXD")
				(number "52")
			)
			(pin input line
				(at 25.4 -38.1 180)
				(length 2.54)
				(name "RXD")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 2.54)
				(name "GPIOD9/RXTD")
				(number "48")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 2.54)
				(name "GPIOD8/TXTD")
				(number "49")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 2.54)
				(name "GPIOD7/RS485D")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 -48.26 180)
				(length 2.54)
				(name "GPIOD6/CLKD")
				(number "51")
			)
			(pin bidirectional line
				(at 25.4 -50.8 180)
				(length 2.54)
				(name "GPIOD5/~{RTSD}/RS485D")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 -53.34 180)
				(length 2.54)
				(name "GPIOD4/~{CTSD}")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 -55.88 180)
				(length 2.54)
				(name "GPIOD3/~{DTRD}")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 -58.42 180)
				(length 2.54)
				(name "GPIOD2/~{DSRD}")
				(number "57")
			)
			(pin bidirectional line
				(at 25.4 -60.96 180)
				(length 2.54)
				(name "GPIOD1/~{CDD}")
				(number "58")
			)
			(pin bidirectional line
				(at 25.4 -63.5 180)
				(length 2.54)
				(name "GPIOD0/~{RID}/~{RWKD}")
				(number "59")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADUM3160"
		(extends "ADUM4160")
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "ADUM3160"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM3160.pdf"
			(at -5.08 0 0)
		)
		(property "Description" "Full/Low Speed, iCoupler USB Digital Isolator, 2.5kV protection"
			(at 0 0 0)
		)
		(property "ki_keywords" "usb isolation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CH340N"
		(extends "CH330N")
		(property "Reference" "U"
			(at -7.62 6.35 0)
		)
		(property "Value" "CH340N"
			(at 7.62 6.35 0)
		)
		(property "Footprint" "Package_SO:SOP-8_3.9x4.9mm_P1.27mm"
			(at -3.81 19.05 0)
		)
		(property "Datasheet" "https://aitendo3.sakura.ne.jp/aitendo_data/product_img/ic/inteface/CH340N/ch340n.pdf"
			(at -2.54 5.08 0)
		)
		(property "Description" "USB serial converter, 2Mbps, UART, SOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Serial Converter Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY7C65211A-24LTXI"
		(extends "CY7C65211-24LTXI")
		(property "Reference" "U"
			(at -13.716 16.51 0)
		)
		(property "Value" "CY7C65211A-24LTXI"
			(at 3.302 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/139886/download"
			(at -40.64 21.59 0)
		)
		(property "Description" "USB-Serial single channel bridge with capsense and BCD, +1.71V to +5.5V VDD, UART/I2C/SPI/RS232/RS422/RS485, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB-Serial single channel bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY7C65213A-28PVXI"
		(extends "CY7C65213-28PVXI")
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "CY7C65213A-28PVXI"
			(at 3.556 19.05 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/139881/download"
			(at -63.5 12.7 0)
		)
		(property "Description" "USB-UART LP Bridge Controller, full speed 12Mbps, +1.71V to 5.5V VDD, UART/RS232/RS422/RS485, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB-UART LP Bridge Controller, full speed 12Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY7C65213A-32LTXI"
		(extends "CY7C65213-32LTXI")
		(property "Reference" "U"
			(at -10.922 19.05 0)
		)
		(property "Value" "CY7C65213A-32LTXI"
			(at 3.556 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/139881/download"
			(at -63.5 12.7 0)
		)
		(property "Description" "USB-UART LP Bridge Controller, full speed 12Mbps, +1.71V to 5.5V VDD, UART/RS232/RS422/RS485, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB-UART LP Bridge Controller, full speed 12Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY7C65215A-32LTXI"
		(extends "CY7C65215-32LTXI")
		(property "Reference" "U"
			(at -13.462 21.844 0)
		)
		(property "Value" "CY7C65215A-32LTXI"
			(at 7.112 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/129956/download"
			(at -40.64 26.67 0)
		)
		(property "Description" "USB-Serial Dual Channel Bridge with CapSense, +1.71V to +5.5V VDD, UART/I2C/SPI/RS232/RS422/RS485/JTAG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB-Serial single channel bridge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CYPD3174-24LQXQ"
		(extends "CYPD3171-24LQXQ")
		(property "Reference" "U"
			(at -17.78 26.67 0)
		)
		(property "Value" "CYPD3174-24LQXQ"
			(at -17.78 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.75x2.75mm"
			(at -4.572 29.718 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-EZ-PD(TM)_CCG3PA_Datasheet_USB_Type-C_Port_Controller-DataSheet-v09_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ee438366ac0"
			(at 0 35.56 0)
		)
		(property "Description" "USB Type-C port controller, Cortex®-M0 processor, DFP CC with opto coupler feedback bootloader, QFN-24"
			(at -1.016 32.512 0)
		)
		(property "ki_keywords" "USBPD Quickcharge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*EP2.75x2.75mm*"
			(at 0 0 0)
		)
	)
	(symbol "CYPD3175-24LQXQ"
		(extends "CYPD3171-24LQXQ")
		(property "Reference" "U"
			(at -17.78 26.67 0)
		)
		(property "Value" "CYPD3175-24LQXQ"
			(at -17.78 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.75x2.75mm"
			(at -4.572 29.718 0)
		)
		(property "Datasheet" "https://www.infineon.com/dgdl/Infineon-EZ-PD(TM)_CCG3PA_Datasheet_USB_Type-C_Port_Controller-DataSheet-v09_00-EN.pdf?fileId=8ac78c8c7d0d8da4017d0ee438366ac0"
			(at 0 35.56 0)
		)
		(property "Description" "USB Type-C port controller, Cortex®-M0 processor, DFP CC with direct feedback bootloader, QFN-24"
			(at -1.016 32.512 0)
		)
		(property "ki_keywords" "USBPD Quickcharge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*EP2.75x2.75mm*"
			(at 0 0 0)
		)
	)
	(symbol "FUSB302B01MPX"
		(extends "FUSB302BMPX")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "FUSB302B01MPX"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-14-1EP_2.5x2.5mm_P0.5mm_EP1.45x1.45mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FUSB302B-D.PDF"
			(at 2.54 -10.16 0)
		)
		(property "Description" "Programmable USB Type-C Controller w/PD, I2C address 0x23, WQFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB USB-C PD Power Delivery PHY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "FUSB302B10MPX"
		(extends "FUSB302BMPX")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "FUSB302B10MPX"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-14-1EP_2.5x2.5mm_P0.5mm_EP1.45x1.45mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FUSB302B-D.PDF"
			(at 2.54 -10.16 0)
		)
		(property "Description" "Programmable USB Type-C Controller w/PD, I2C address 0x24, WQFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB USB-C PD Power Delivery PHY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "FUSB302B11MPX"
		(extends "FUSB302BMPX")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "FUSB302B11MPX"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-14-1EP_2.5x2.5mm_P0.5mm_EP1.45x1.45mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FUSB302B-D.PDF"
			(at 2.54 -10.16 0)
		)
		(property "Description" "Programmable USB Type-C Controller w/PD, I2C address 0x25, WQFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB USB-C PD Power Delivery PHY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*2.5x2.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2200-E-SS"
		(extends "MCP2200-I-SS")
		(property "Reference" "U"
			(at -20.32 -19.05 0)
		)
		(property "Value" "MCP2200-E-SS"
			(at -20.32 19.05 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/200022228D.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "USB 2.0 to UART Protocol Converter with GPIO, Extended Temperature Range, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*20*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2200T-E-SS"
		(extends "MCP2200-I-SS")
		(property "Reference" "U"
			(at -20.32 -19.05 0)
		)
		(property "Value" "MCP2200T-E-SS"
			(at -20.32 19.05 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/200022228D.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "USB 2.0 to UART Protocol Converter with GPIO, Extended Temperature Range, TnR, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*20*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2200T-I-MQ"
		(extends "MCP2200-I-MQ")
		(property "Reference" "U"
			(at -20.32 -19.05 0)
		)
		(property "Value" "MCP2200T-I-MQ"
			(at -20.32 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_5x5mm_P0.65mm_EP3.35x3.35mm"
			(at 27.94 -20.32 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/200022228D.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "USB 2.0 to UART Protocol Converter with GPIO, TnR, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*20*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2200T-I-SO"
		(extends "MCP2200-I-SO")
		(property "Reference" "U"
			(at -20.32 -19.05 0)
		)
		(property "Value" "MCP2200T-I-SO"
			(at -20.32 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/200022228D.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "USB 2.0 to UART Protocol Converter with GPIO,TnR,SOIC"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*20*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MCP2200T-I-SS"
		(extends "MCP2200-I-SS")
		(property "Reference" "U"
			(at -20.32 -19.05 0)
		)
		(property "Value" "MCP2200T-I-SS"
			(at -20.32 19.05 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/200022228D.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "USB 2.0 to UART Protocol Converter with GPIO, TnR, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB UART Converter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*20*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "STULPI01B"
		(extends "STULPI01A")
		(property "Reference" "U"
			(at -8.89 24.13 0)
		)
		(property "Value" "STULPI01B"
			(at 8.89 24.13 0)
		)
		(property "Footprint" "Package_BGA:ST_uTFBGA-36_3.6x3.6mm_Layout6x6_P0.5mm"
			(at 2.54 -25.4 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/stulpi01b.pdf"
			(at -2.54 -1.27 0)
		)
		(property "Description" "High-speed USB On-The-Go ULPI transceiver"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB OTG HS PHY ULPI Interface"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*uTFBGA*3.6x3.6mm*Layout6x6*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "TPS2501DRC"
		(extends "TPS2500DRC")
		(property "Reference" "U"
			(at -7.62 -11.43 0)
		)
		(property "Value" "TPS2501DRC"
			(at -7.62 8.89 0)
		)
		(property "Footprint" "Package_SON:Texas_S-PVSON-N10"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2500.pdf"
			(at -2.54 -7.62 0)
		)
		(property "Description" "Integrated USB power Switch with Boost Converter, Constant Frequency, Texas S-PVSON-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB switch boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PVSON*N10*"
			(at 0 0 0)
		)
	)
	(symbol "TPS2513A"
		(extends "TPS2513")
		(property "Reference" "U"
			(at -3.81 -7.62 0)
		)
		(property "Value" "TPS2513A"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2513.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "USB Dedicated Charging Port Controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Charge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TPS2514A"
		(extends "TPS2514")
		(property "Reference" "U"
			(at -3.81 -7.62 0)
		)
		(property "Value" "TPS2514A"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tps2513.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "USB Dedicated Charging Port Controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB Charge"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TUSB320I"
		(extends "TUSB320")
		(property "Reference" "U"
			(at -11.43 11.43 0)
		)
		(property "Value" "TUSB320I"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_X2QFN-12_1.6x1.6mm_P0.4mm"
			(at 5.08 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/tusb320.pdf"
			(at 0 0 0)
		)
		(property "Description" "USB Type-C Configuration Channel Logic and Port Control, industrial temperature range, X2QFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB PD CC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas?X2QFN*1.6x1.6mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "USB3346"
		(extends "USB3341")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "USB3346"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 12.7 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/334x.pdf"
			(at 12.7 5.08 0)
		)
		(property "Description" "Hi-Speed USB ULPI Transceiver, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB ULPI Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "USB3347"
		(extends "USB3341")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "USB3347"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 12.7 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/334x.pdf"
			(at 12.7 5.08 0)
		)
		(property "Description" "Hi-Speed USB ULPI Transceiver, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB ULPI Transceiver"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "USB3740B-AI9"
		(extends "USB3740B-AI2")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "USB3740B-AI9"
			(at 10.16 8.89 0)
		)
		(property "Footprint" ""
			(at 30.48 -8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/00001725D.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "USB 2.0 Switch with ESD Protection, UQFN-10 Pitch 0.5mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "USB 2.0 High Speed Switch"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1.3x1.8mm?P0.4mm* UQFN*1.6x2.1mm?P0.5mm*"
			(at 0 0 0)
		)
	)
)
