(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "4N25"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "4N25"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83725/4n25.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 30V, CTR 20%, Viso 2500V, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "4N25_0_1")
		(symbol "4N25_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "6N135"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "6N135"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -5.08 -7.62 0)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS70-2008-0032/6N135-L%206N136-L%20series.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Speed Optocoupler, TTL Compatible, CTR 18%, DIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Speed Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "6N135_0_1")
		(symbol "6N135_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "6N135S"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "6N135S"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-8_W9.53mm"
			(at -5.08 -7.62 0)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS70-2008-0032/6N135-L%206N136-L%20series.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Speed Optocoupler, TTL Compatible, CTR 18%, SMDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Speed Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm*"
			(at 0 0 0)
		)
		(symbol "6N135S_0_1")
		(symbol "6N135S_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "6N138"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "6N138"
			(at 2.286 8.89 0)
		)
		(property "Footprint" ""
			(at 7.366 -7.62 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/HCPL2731-D.pdf"
			(at 7.366 -7.62 0)
		)
		(property "Description" "Low Input Current high Gain Split Darlington Optocouplers, -0.5V to 7V VDD, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm*"
			(at 0 0 0)
		)
		(symbol "6N138_0_1")
		(symbol "6N138_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C1")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "VO1")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "VO2")
				(number "6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADN4650"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "ADN4650"
			(at 13.97 13.97 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adn4650-4651-4652.pdf"
			(at -8.89 17.78 0)
		)
		(property "Description" "Dual-Channel LVDS Isolators, 5 kV RMS/3.75 kV RMS, 600 Mbps, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS Isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADN4650_0_0"
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "9")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VDD2")
				(number "12")
			)
		)
		(symbol "ADN4650_0_1")
		(symbol "ADN4650_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DIN1+")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DIN1-")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DIN2+")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DIN2-")
				(number "8")
			)
			(pin power_in line
				(at -7.62 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "3")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VIN1")
				(number "1")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VIN2")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "17")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "19")
			)
			(pin power_in line
				(at 7.62 15.24 270)
				(length 2.54)
				(name "VDD2")
				(number "18")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DOUT1+")
				(number "16")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DOUT1-")
				(number "15")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DOUT2+")
				(number "14")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DOUT2-")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADN4651"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "ADN4651"
			(at 13.97 13.97 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adn4650-4651-4652.pdf"
			(at -8.89 17.78 0)
		)
		(property "Description" "Dual-Channel LVDS Isolators, 5 kV RMS/3.75 kV RMS, 600 Mbps, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS Isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADN4651_0_0"
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "9")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VDD2")
				(number "12")
			)
		)
		(symbol "ADN4651_0_1")
		(symbol "ADN4651_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DIN1+")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DIN1-")
				(number "6")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DOUT2+")
				(number "7")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DOUT2-")
				(number "8")
			)
			(pin power_in line
				(at -7.62 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "3")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VIN1")
				(number "1")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "10")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VIN2")
				(number "20")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "17")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "19")
			)
			(pin power_in line
				(at 7.62 15.24 270)
				(length 2.54)
				(name "VDD2")
				(number "18")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DOUT1+")
				(number "16")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DOUT1-")
				(number "15")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DIN2+")
				(number "14")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DIN2-")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADN4652"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 13.97 0)
		)
		(property "Value" "ADN4652"
			(at 13.97 13.97 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adn4650-4651-4652.pdf"
			(at -6.35 20.32 0)
		)
		(property "Description" "Dual-Channel LVDS Isolators, 5 kV RMS/3.75 kV RMS, 600 Mbps, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "LVDS Isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADN4652_0_0"
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "9")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VDD2")
				(number "12")
			)
		)
		(symbol "ADN4652_0_1")
		(symbol "ADN4652_1_1"
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "DOUT1+")
				(number "5")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "DOUT1-")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "DIN2+")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "DIN2-")
				(number "8")
			)
			(pin power_in line
				(at -7.62 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "3")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VIN1")
				(number "1")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "10")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VIN2")
				(number "20")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "11")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "17")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "19")
			)
			(pin power_in line
				(at 7.62 15.24 270)
				(length 2.54)
				(name "VDD2")
				(number "18")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DIN1+")
				(number "16")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DIN1-")
				(number "15")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "DOUT2+")
				(number "14")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "DOUT2-")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM1200AR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1200AR"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM1200_1201.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Dual-channel digital isolator, Bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM1200AR_0_1")
		(symbol "ADuM1200AR_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIA")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VIB")
				(number "3")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VDD2")
				(number "8")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOA")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VOB")
				(number "6")
			)
			(pin power_in line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GND2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM1201AR"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1201AR"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM1200_1201.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Dual-channel digital isolator, bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM1201AR_0_1")
		(symbol "ADuM1201AR_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VOA")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VIB")
				(number "3")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VDD2")
				(number "8")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VIA")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VOB")
				(number "6")
			)
			(pin power_in line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GND2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM120N"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM120N"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM120N_121N.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Dual-channel digital isolator,1.8 to 5V, 150Mbs, 3kV"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM120N_0_1")
		(symbol "ADuM120N_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIA")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VIB")
				(number "3")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VDD2")
				(number "8")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOA")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VOB")
				(number "6")
			)
			(pin power_in line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GND2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM121N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM121N"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM120N_121N.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Dual-channel digital isolator,1.8 to 5V, 150Mbs, 3kV"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM121N_0_1")
		(symbol "ADuM121N_1_1"
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VOA")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VIB")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VDD2")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND2")
				(number "5")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VIA")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VOB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM1250"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1250"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM1250_1251.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Dual-channel I2C digital isolator, Bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-channel digital isolator I2C"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM1250_0_1")
		(symbol "ADuM1250_1_1"
			(pin power_in line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SDA1")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCL1")
				(number "3")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VDD2")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SDA2")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SCL2")
				(number "6")
			)
			(pin power_in line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "GND2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM1300xRW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 19.05 0)
		)
		(property "Value" "ADuM1300xRW"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -14.605 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/adum1300_1301.pdf"
			(at 0 -16.51 0)
		)
		(property "Description" "Three Channel Digital Isolator, 10Mbps, SOICW-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM1300xRW_0_0"
			(text "ENCODE"
				(at -4.445 7.62 0)
			)
			(text "ENCODE"
				(at -4.445 5.08 0)
			)
			(text "ENCODE"
				(at -4.445 2.54 0)
			)
			(text "DECODE"
				(at 4.445 7.62 0)
			)
			(text "DECODE"
				(at 4.445 5.08 0)
			)
			(text "DECODE"
				(at 4.445 2.54 0)
			)
		)
		(symbol "ADuM1300xRW_0_1")
		(symbol "ADuM1300xRW_1_1"
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "V_{DD1}")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "V_{IA}")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "V_{IB}")
				(number "4")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "V_{IC}")
				(number "5")
			)
			(pin no_connect line
				(at -15.24 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -15.24 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GND_{1}")
				(number "2")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND_{1}")
				(number "8")
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "V_{DD2}")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "V_{OA}")
				(number "14")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "V_{OB}")
				(number "13")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "V_{OC}")
				(number "12")
			)
			(pin no_connect line
				(at 15.24 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "V_{E2}")
				(number "10")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND_{2}")
				(number "15")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GND_{2}")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM1400xRW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 19.05 0)
		)
		(property "Value" "ADuM1400xRW"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -14.605 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADUM1400_1401_1402.pdf"
			(at -20.32 0 0)
		)
		(property "Description" "Quad Channel Digital Isolator, 10Mbps, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM1400xRW_0_0"
			(text "ENCODE"
				(at -4.445 7.62 0)
			)
			(text "ENCODE"
				(at -4.445 5.08 0)
			)
			(text "ENCODE"
				(at -4.445 2.54 0)
			)
			(text "ENCODE"
				(at -4.445 0 0)
			)
			(text "DECODE"
				(at 4.445 7.62 0)
			)
			(text "DECODE"
				(at 4.445 5.08 0)
			)
			(text "DECODE"
				(at 4.445 2.54 0)
			)
			(text "DECODE"
				(at 4.445 0 0)
			)
		)
		(symbol "ADuM1400xRW_0_1")
		(symbol "ADuM1400xRW_1_1"
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VIC")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "VID")
				(number "6")
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "14")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "13")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VOC")
				(number "12")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "VOD")
				(number "11")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "VE2")
				(number "10")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM1401xRW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 19.05 0)
		)
		(property "Value" "ADuM1401xRW"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -14.605 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADUM1400_1401_1402.pdf"
			(at -20.32 0 0)
		)
		(property "Description" "Quad Channel Digital Isolator, 10Mbps, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM1401xRW_0_0"
			(text "ENCODE"
				(at -4.445 7.62 0)
			)
			(text "ENCODE"
				(at -4.445 5.08 0)
			)
			(text "ENCODE"
				(at -4.445 2.54 0)
			)
			(text "DECODE"
				(at -4.445 0 0)
			)
			(text "DECODE"
				(at 4.445 7.62 0)
			)
			(text "DECODE"
				(at 4.445 5.08 0)
			)
			(text "DECODE"
				(at 4.445 2.54 0)
			)
			(text "ENCODE"
				(at 4.445 0 0)
			)
		)
		(symbol "ADuM1401xRW_0_1")
		(symbol "ADuM1401xRW_1_1"
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VIC")
				(number "5")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "VOD")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "VE1")
				(number "7")
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "14")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "13")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VOC")
				(number "12")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "VID")
				(number "11")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "VE2")
				(number "10")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM1402xRW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 19.05 0)
		)
		(property "Value" "ADuM1402xRW"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -14.605 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADUM1400_1401_1402.pdf"
			(at -20.32 0 0)
		)
		(property "Description" "Quad Channel Digital Isolator, 10Mbps, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM1402xRW_0_0"
			(text "ENCODE"
				(at -4.445 7.62 0)
			)
			(text "ENCODE"
				(at -4.445 5.08 0)
			)
			(text "DECODE"
				(at -4.445 2.54 0)
			)
			(text "DECODE"
				(at -4.445 0 0)
			)
			(text "DECODE"
				(at 4.445 7.62 0)
			)
			(text "DECODE"
				(at 4.445 5.08 0)
			)
			(text "ENCODE"
				(at 4.445 2.54 0)
			)
			(text "ENCODE"
				(at 4.445 0 0)
			)
		)
		(symbol "ADuM1402xRW_0_1")
		(symbol "ADuM1402xRW_1_1"
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VOC")
				(number "5")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "VOD")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "VE1")
				(number "7")
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "14")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "13")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VIC")
				(number "12")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "VID")
				(number "11")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "VE2")
				(number "10")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM1410"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 19.05 0)
		)
		(property "Value" "ADuM1410"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADUM1410_1411_1412.pdf"
			(at -20.32 0 0)
		)
		(property "Description" "Quad Channel Digital Isolator,10Mbps,SO-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM1410_0_0"
			(text "ENCODE"
				(at -4.445 7.62 0)
			)
			(text "ENCODE"
				(at -4.445 5.08 0)
			)
			(text "ENCODE"
				(at -4.445 2.54 0)
			)
			(text "ENCODE"
				(at -4.445 0 0)
			)
			(text "DECODE"
				(at 4.445 7.62 0)
			)
			(text "DECODE"
				(at 4.445 5.08 0)
			)
			(text "DECODE"
				(at 4.445 2.54 0)
			)
			(text "DECODE"
				(at 4.445 0 0)
			)
		)
		(symbol "ADuM1410_0_1")
		(symbol "ADuM1410_1_1"
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VIC")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "VID")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DISABLE")
				(number "7")
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "14")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "13")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VOC")
				(number "12")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "VOD")
				(number "11")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "CTRL2")
				(number "10")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin power_in line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM1411"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 19.05 0)
		)
		(property "Value" "ADuM1411"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADUM1410_1411_1412.pdf"
			(at -20.32 0 0)
		)
		(property "Description" "Quad Channel Digital Isolator,10Mbps,SO-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM1411_0_0"
			(text "ENCODE"
				(at -4.445 7.62 0)
			)
			(text "ENCODE"
				(at -4.445 5.08 0)
			)
			(text "ENCODE"
				(at -4.445 2.54 0)
			)
			(text "DECODE"
				(at -4.445 0 0)
			)
			(text "DECODE"
				(at 4.445 7.62 0)
			)
			(text "DECODE"
				(at 4.445 5.08 0)
			)
			(text "DECODE"
				(at 4.445 2.54 0)
			)
			(text "ENCODE"
				(at 4.445 0 0)
			)
		)
		(symbol "ADuM1411_0_1")
		(symbol "ADuM1411_1_1"
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VIC")
				(number "5")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "VOD")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CTRL1")
				(number "7")
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "14")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "13")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VOC")
				(number "12")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "VID")
				(number "11")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "CTRL2")
				(number "10")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin power_in line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM1412"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 19.05 0)
		)
		(property "Value" "ADuM1412"
			(at 0 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADUM1410_1411_1412.pdf"
			(at -20.32 0 0)
		)
		(property "Description" "Quad Channel Digital Isolator,10Mbps,SO-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Digital Isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM1412_0_0"
			(text "ENCODE"
				(at -4.445 7.62 0)
			)
			(text "ENCODE"
				(at -4.445 5.08 0)
			)
			(text "DECODE"
				(at -4.445 2.54 0)
			)
			(text "DECODE"
				(at -4.445 0 0)
			)
			(text "DECODE"
				(at 4.445 7.62 0)
			)
			(text "DECODE"
				(at 4.445 5.08 0)
			)
			(text "ENCODE"
				(at 4.445 2.54 0)
			)
			(text "ENCODE"
				(at 4.445 0 0)
			)
		)
		(symbol "ADuM1412_0_1")
		(symbol "ADuM1412_1_1"
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin output line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VOC")
				(number "5")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "VOD")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "CTRL1")
				(number "7")
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "14")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "13")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VIC")
				(number "12")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "VID")
				(number "11")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "CTRL2")
				(number "10")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin power_in line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM260N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 16.51 0)
		)
		(property "Value" "ADuM260N"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x12.8mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.analog.com/media/en/technical-documentation/data-sheets/ADuM260N-261N-262N-263N.pdf"
			(at 0 19.05 0)
		)
		(property "Description" "5.0 kV RMS, 6-Channel Digital Isolator, 0 reverse channels, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator galvanic isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM260N_0_1")
		(symbol "ADuM260N_1_0"
			(text "ENCODE"
				(at -4.064 7.62 0)
			)
			(text "ENCODE"
				(at -4.064 5.08 0)
			)
			(text "ENCODE"
				(at -4.064 2.54 0)
			)
			(text "ENCODE"
				(at -4.064 0 0)
			)
			(text "ENCODE"
				(at -4.064 -2.54 0)
			)
			(text "ENCODE"
				(at -4.064 -5.08 0)
			)
			(text "DECODE"
				(at 4.064 7.62 0)
			)
			(text "DECODE"
				(at 4.064 5.08 0)
			)
			(text "DECODE"
				(at 4.064 2.54 0)
			)
			(text "DECODE"
				(at 4.064 0 0)
			)
			(text "DECODE"
				(at 4.064 -2.54 0)
			)
			(text "DECODE"
				(at 4.064 -5.08 0)
			)
		)
		(symbol "ADuM260N_1_1"
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VIC")
				(number "4")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "VID")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "VIE")
				(number "6")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "VIF")
				(number "7")
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "15")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "14")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VOC")
				(number "13")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "VOD")
				(number "12")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "VOE")
				(number "11")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "VOF")
				(number "10")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM261N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 16.51 0)
		)
		(property "Value" "ADuM261N"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x12.8mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.analog.com/media/en/technical-documentation/data-sheets/ADuM260N-261N-262N-263N.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "5.0 kV RMS, 6-Channel Digital Isolator, 1 reverse channels, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator galvanic isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM261N_1_0"
			(text "ENCODE"
				(at -4.064 7.62 0)
			)
			(text "ENCODE"
				(at -4.064 5.08 0)
			)
			(text "ENCODE"
				(at -4.064 2.54 0)
			)
			(text "ENCODE"
				(at -4.064 0 0)
			)
			(text "ENCODE"
				(at -4.064 -2.54 0)
			)
			(text "DECODE"
				(at -4.064 -5.08 0)
			)
			(text "DECODE"
				(at 4.064 7.62 0)
			)
			(text "DECODE"
				(at 4.064 5.08 0)
			)
			(text "DECODE"
				(at 4.064 2.54 0)
			)
			(text "DECODE"
				(at 4.064 0 0)
			)
			(text "DECODE"
				(at 4.064 -2.54 0)
			)
			(text "ENCODE"
				(at 4.064 -5.08 0)
			)
		)
		(symbol "ADuM261N_1_1"
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VIC")
				(number "4")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "VID")
				(number "5")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "VIE")
				(number "6")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "VOF")
				(number "7")
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "15")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "14")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VOC")
				(number "13")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "VOD")
				(number "12")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "VOE")
				(number "11")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "VIF")
				(number "10")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM262N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 16.51 0)
		)
		(property "Value" "ADuM262N"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x12.8mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.analog.com/media/en/technical-documentation/data-sheets/ADuM260N-261N-262N-263N.pdf"
			(at 0 27.94 0)
		)
		(property "Description" "5.0 kV RMS, 6-Channel Digital Isolator, 2 reverse channels, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator galvanic isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM262N_1_0"
			(text "ENCODE"
				(at -4.064 7.62 0)
			)
			(text "ENCODE"
				(at -4.064 5.08 0)
			)
			(text "ENCODE"
				(at -4.064 2.54 0)
			)
			(text "ENCODE"
				(at -4.064 0 0)
			)
			(text "DECODE"
				(at -4.064 -2.54 0)
			)
			(text "DECODE"
				(at -4.064 -5.08 0)
			)
			(text "DECODE"
				(at 4.064 7.62 0)
			)
			(text "DECODE"
				(at 4.064 5.08 0)
			)
			(text "DECODE"
				(at 4.064 2.54 0)
			)
			(text "DECODE"
				(at 4.064 0 0)
			)
			(text "ENCODE"
				(at 4.064 -2.54 0)
			)
			(text "ENCODE"
				(at 4.064 -5.08 0)
			)
		)
		(symbol "ADuM262N_1_1"
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VIC")
				(number "4")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "VID")
				(number "5")
			)
			(pin output line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "VOE")
				(number "6")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "VOF")
				(number "7")
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "15")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "14")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VOC")
				(number "13")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "VOD")
				(number "12")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "VIE")
				(number "11")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "VIF")
				(number "10")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM263N"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 16.51 0)
		)
		(property "Value" "ADuM263N"
			(at 7.62 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x12.8mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://www.analog.com/media/en/technical-documentation/data-sheets/ADuM260N-261N-262N-263N.pdf"
			(at 0 19.05 0)
		)
		(property "Description" "5.0 kV RMS, 6-Channel Digital Isolator, 3 reverse channels, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator galvanic isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM263N_1_0"
			(text "ENCODE"
				(at -4.064 7.62 0)
			)
			(text "ENCODE"
				(at -4.064 5.08 0)
			)
			(text "ENCODE"
				(at -4.064 2.54 0)
			)
			(text "ENCODE"
				(at -4.064 0 0)
			)
			(text "DECODE"
				(at -4.064 -2.54 0)
			)
			(text "DECODE"
				(at -4.064 -5.08 0)
			)
			(text "DECODE"
				(at 4.064 7.62 0)
			)
			(text "DECODE"
				(at 4.064 5.08 0)
			)
			(text "DECODE"
				(at 4.064 2.54 0)
			)
			(text "DECODE"
				(at 4.064 0 0)
			)
			(text "ENCODE"
				(at 4.064 -2.54 0)
			)
			(text "ENCODE"
				(at 4.064 -5.08 0)
			)
		)
		(symbol "ADuM263N_1_1"
			(pin power_in line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "2")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "3")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "VIC")
				(number "4")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "VOD")
				(number "5")
			)
			(pin output line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "VOE")
				(number "6")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "VOF")
				(number "7")
			)
			(pin power_in line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "15")
			)
			(pin output line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "14")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "VOC")
				(number "13")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "VID")
				(number "12")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "VIE")
				(number "11")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "VIF")
				(number "10")
			)
			(pin power_in line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM3151"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 17.78 0)
		)
		(property "Value" "ADuM3151"
			(at 10.16 15.24 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM3151_3152_3153.pdf"
			(at -24.13 29.21 0)
		)
		(property "Description" "3.75kV 7-Channel SPI Isolator, 1 Reverse Channel, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "spi isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADuM3151_0_0")
		(symbol "ADuM3151_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "MCLK")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MO")
				(number "4")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MI")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{MSS}")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "V_{IA}")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "V_{IB}")
				(number "8")
			)
			(pin output line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "V_{OC}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "V_{DD1}")
				(number "1")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND_{1}")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND_{1}")
				(number "2")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "V_{DD2}")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND_{2}")
				(number "11")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND_{2}")
				(number "19")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCLK")
				(number "18")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SI")
				(number "17")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SO")
				(number "16")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{SSS}")
				(number "15")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "V_{OA}")
				(number "14")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "V_{OB}")
				(number "13")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "V_{IC}")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM3152"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 17.78 0)
		)
		(property "Value" "ADuM3152"
			(at 10.16 15.24 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM3151_3152_3153.pdf"
			(at -24.13 29.21 0)
		)
		(property "Description" "3.75kV 7-Channel SPI Isolator, 2 Reverse Channels, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "spi isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADuM3152_0_0")
		(symbol "ADuM3152_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "MCLK")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MO")
				(number "4")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MI")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{MSS}")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "V_{IA}")
				(number "7")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "V_{OB}")
				(number "8")
			)
			(pin output line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "V_{OC}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "V_{DD1}")
				(number "1")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND_{1}")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND_{1}")
				(number "2")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "V_{DD2}")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND_{2}")
				(number "11")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND_{2}")
				(number "19")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCLK")
				(number "18")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SI")
				(number "17")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SO")
				(number "16")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{SSS}")
				(number "15")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "V_{OA}")
				(number "14")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "V_{IB}")
				(number "13")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "V_{IC}")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM3153"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 17.78 0)
		)
		(property "Value" "ADuM3153"
			(at 10.16 15.24 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM3151_3152_3153.pdf"
			(at -24.13 29.21 0)
		)
		(property "Description" "3.75kV 7-Channel SPI Isolator, 3 Reverse Channels, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "spi isolated"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADuM3153_0_0")
		(symbol "ADuM3153_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "MCLK")
				(number "3")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "MO")
				(number "4")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "MI")
				(number "5")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "~{MSS}")
				(number "6")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "V_{OA}")
				(number "7")
			)
			(pin output line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "V_{OB}")
				(number "8")
			)
			(pin output line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "V_{OC}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "V_{DD1}")
				(number "1")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND_{1}")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND_{1}")
				(number "2")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "V_{DD2}")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND_{2}")
				(number "11")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND_{2}")
				(number "19")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SCLK")
				(number "18")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SI")
				(number "17")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "SO")
				(number "16")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "~{SSS}")
				(number "15")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "V_{IA}")
				(number "14")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "V_{IB}")
				(number "13")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "V_{IC}")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM5211"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ADuM5211"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM5210_5211_5212.pdf"
			(at -11.43 7.62 0)
		)
		(property "Description" "Dual-Channel 2.5kV isolator with integrated dc-dc converter, 1 Input / 1 output, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator galvanic isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*20*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADuM5211_0_1")
		(symbol "ADuM5211_1_1"
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "V_{OA}")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "V_{IB}")
				(number "4")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PDIS")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "V_{DDP}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "V_{DD1}")
				(number "1")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND_{P}")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND_{P}")
				(number "2")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND_{P}")
				(number "5")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND_{P}")
				(number "6")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "V_{ISO}")
				(number "12")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND_{ISO}")
				(number "11")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND_{ISO}")
				(number "15")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND_{ISO}")
				(number "16")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND_{ISO}")
				(number "19")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "V_{DD2}")
				(number "20")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "V_{IA}")
				(number "18")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "V_{OB}")
				(number "17")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "V_{SEL}")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM5401"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "ADuM5401"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM5401_5402_5403_5404.pdf"
			(at -11.43 7.62 0)
		)
		(property "Description" "Quad-Channel 2.5kV isolator with integrated isoPower dc-dc converter, 3 Input / 1 output, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator galvanic isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM5401_0_1")
		(symbol "ADuM5401_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIC")
				(number "5")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "VOD")
				(number "6")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RCOUT")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VISO")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDISO")
				(number "9")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GNDISO")
				(number "15")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "13")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOC")
				(number "12")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "VID")
				(number "11")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VSEL")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM5402"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "ADuM5402"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM5401_5402_5403_5404.pdf"
			(at -11.43 7.62 0)
		)
		(property "Description" "Quad-Channel 2.5kV isolator with integrated isoPower dc-dc converter, 2 Input / 2 output, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator galvanic isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM5402_0_1")
		(symbol "ADuM5402_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VOC")
				(number "5")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "VOD")
				(number "6")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RCOUT")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VISO")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDISO")
				(number "9")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GNDISO")
				(number "15")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "13")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VIC")
				(number "12")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "VID")
				(number "11")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VSEL")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM5403"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "ADuM5403"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM5401_5402_5403_5404.pdf"
			(at -11.43 7.62 0)
		)
		(property "Description" "Quad-Channel 2.5kV isolator with integrated isoPower dc-dc converter, 1 Input / 3 output, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator galvanic isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM5403_0_1")
		(symbol "ADuM5403_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VOB")
				(number "4")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VOC")
				(number "5")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "VOD")
				(number "6")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RCOUT")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VISO")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDISO")
				(number "9")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GNDISO")
				(number "15")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "14")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VIB")
				(number "13")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VIC")
				(number "12")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "VID")
				(number "11")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VSEL")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM5404"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "ADuM5404"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM5401_5402_5403_5404.pdf"
			(at -11.43 7.62 0)
		)
		(property "Description" "Quad-Channel 2.5kV isolator with integrated isoPower dc-dc converter, 0 Input / 4 output, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator galvanic isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ADuM5404_0_1")
		(symbol "ADuM5404_1_1"
			(pin output line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VOA")
				(number "3")
			)
			(pin output line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VOB")
				(number "4")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VOC")
				(number "5")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "VOD")
				(number "6")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "RCOUT")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VISO")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDISO")
				(number "9")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GNDISO")
				(number "15")
			)
			(pin input line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VIA")
				(number "14")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VIB")
				(number "13")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VIC")
				(number "12")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "VID")
				(number "11")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VSEL")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM5410"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "ADuM5410"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM5410-5411-5412.pdf"
			(at -10.16 6.35 0)
		)
		(property "Description" "Quad-Channel 2.5kV isolator with integrated dc-dc converter, 4 Input / 0 output, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator galvanic isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADuM5410_0_1")
		(symbol "ADuM5410_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIC")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VID")
				(number "6")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PDIS")
				(number "10")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -10.16 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "VDDP")
				(number "11")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "9")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VDD2")
				(number "24")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDISO")
				(number "13")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GNDISO")
				(number "16")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GNDISO")
				(number "23")
			)
			(pin power_out line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VISO")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "22")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "21")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOC")
				(number "20")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "VOD")
				(number "19")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VE2")
				(number "18")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VSEL")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM5411"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "ADuM5411"
			(at 6.35 13.97 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 1.27 -29.21 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM5410-5411-5412.pdf"
			(at -12.7 6.35 0)
		)
		(property "Description" "Quad-Channel 2.5kV isolator with integrated dc-dc converter, 3 Input / 1 output, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator galvanic isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADuM5411_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIC")
				(number "5")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "VOD")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VE1")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PDIS")
				(number "10")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "VDDP")
				(number "11")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "9")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VDD2")
				(number "24")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDISO")
				(number "13")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GNDISO")
				(number "16")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GNDISO")
				(number "23")
			)
			(pin power_out line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VISO")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "22")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "21")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOC")
				(number "20")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "VID")
				(number "19")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VE2")
				(number "18")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VSEL")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM5412"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 13.97 0)
		)
		(property "Value" "ADuM5412"
			(at 6.604 14.224 0)
		)
		(property "Footprint" "Package_SO:SSOP-24_5.3x8.2mm_P0.65mm"
			(at 1.27 -29.21 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM5410-5411-5412.pdf"
			(at -12.7 8.89 0)
		)
		(property "Description" "Quad-Channel 2.5kV isolator with integrated dc-dc converter, 2 Input / 2 output, SSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator galvanic isopower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ADuM5412_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VOC")
				(number "5")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "VOD")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VE1")
				(number "7")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PDIS")
				(number "10")
			)
			(pin no_connect line
				(at -10.16 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "VDDP")
				(number "11")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "9")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VDD2")
				(number "24")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GNDISO")
				(number "13")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GNDISO")
				(number "16")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GNDISO")
				(number "23")
			)
			(pin power_out line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "VISO")
				(number "14")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "VOA")
				(number "22")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOB")
				(number "21")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VIC")
				(number "20")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "VID")
				(number "19")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VE2")
				(number "18")
			)
			(pin input line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VSEL")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM7640C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "ADuM7640C"
			(at -1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:QSOP-20_3.9x8.7mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM7640_7641_7642_7643.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Low Power Six-Channel 6/0 Digital Isolator, 25Mbps 6ns, Fail-Safe High, QSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "6-Channels Hex Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ADuM7640C_0_1")
		(symbol "ADuM7640C_1_1"
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "VDD1A")
				(number "1")
			)
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VDD1B")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VIC")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VID")
				(number "6")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VIE")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VIF")
				(number "9")
			)
			(pin power_in line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "10")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VDD2A")
				(number "20")
			)
			(pin power_in line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VDD2B")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOA")
				(number "18")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOB")
				(number "17")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "VOC")
				(number "16")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VOD")
				(number "15")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VOE")
				(number "13")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VOF")
				(number "12")
			)
			(pin power_in line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM7641C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "ADuM7641C"
			(at -1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:QSOP-20_3.9x8.7mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM7640_7641_7642_7643.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Low Power Six-Channel 5/1 Digital Isolator, 25Mbps 6ns, Fail-Safe High, QSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "6-Channels Hex Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ADuM7641C_0_1")
		(symbol "ADuM7641C_1_1"
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "VDD1A")
				(number "1")
			)
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VDD1B")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VIC")
				(number "5")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VID")
				(number "6")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VOE")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VIF")
				(number "9")
			)
			(pin power_in line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "10")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VDD2A")
				(number "20")
			)
			(pin power_in line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VDD2B")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOA")
				(number "18")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOB")
				(number "17")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "VOC")
				(number "16")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VOD")
				(number "15")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VIE")
				(number "13")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VOF")
				(number "12")
			)
			(pin power_in line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM7642C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "ADuM7642C"
			(at -1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:QSOP-20_3.9x8.7mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM7640_7641_7642_7643.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Low Power Six-Channel 4/2 Digital Isolator, 25Mbps 6ns, Fail-Safe High, QSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "6-Channels Hex Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ADuM7642C_0_1")
		(symbol "ADuM7642C_1_1"
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "VDD1A")
				(number "1")
			)
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VDD1B")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "VIC")
				(number "5")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VOD")
				(number "6")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VOE")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VIF")
				(number "9")
			)
			(pin power_in line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "10")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VDD2A")
				(number "20")
			)
			(pin power_in line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VDD2B")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOA")
				(number "18")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOB")
				(number "17")
			)
			(pin output line
				(at 12.7 0 180)
				(length 2.54)
				(name "VOC")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VID")
				(number "15")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VIE")
				(number "13")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VOF")
				(number "12")
			)
			(pin power_in line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ADuM7643C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "ADuM7643C"
			(at -1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:QSOP-20_3.9x8.7mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM7640_7641_7642_7643.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Low Power Six-Channel 3/3 Digital Isolator, 25Mbps 6ns, Fail-Safe High, QSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "6-Channels Hex Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ADuM7643C_0_1")
		(symbol "ADuM7643C_1_1"
			(pin power_in line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "VDD1A")
				(number "1")
			)
			(pin power_in line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "VDD1B")
				(number "7")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "VIA")
				(number "3")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "VIB")
				(number "4")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "VOC")
				(number "5")
			)
			(pin output line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "VOD")
				(number "6")
			)
			(pin output line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "VOE")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "VIF")
				(number "9")
			)
			(pin passive line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "10")
			)
			(pin power_in line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "VDD2A")
				(number "20")
			)
			(pin power_in line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "VDD2B")
				(number "14")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "VOA")
				(number "18")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "VOB")
				(number "17")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "VIC")
				(number "16")
			)
			(pin input line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "VID")
				(number "15")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "VIE")
				(number "13")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "VOF")
				(number "12")
			)
			(pin power_in line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
			(pin passive line
				(at 12.7 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CNY17-1"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "CNY17-1"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 40-80%, Viso 5000V (RMS), DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*"
			(at 0 0 0)
		)
		(symbol "CNY17-1_0_1")
		(symbol "CNY17-1_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "EL814"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "EL814"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.everlight.com/file/ProductFile/EL814.pdf"
			(at 0.635 0 0)
		)
		(property "Description" "AC/DC NPN Optocoupler, DIP4/SMD4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*"
			(at 0 0 0)
		)
		(symbol "EL814_0_1")
		(symbol "EL814_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FODM214"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FODM214"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FODM214-D.PDF"
			(at 0.635 0 0)
		)
		(property "Description" "AC/DC Optocoupler, Vce 80V, CTR 20-400%, SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC DC Phototransistor Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "FODM214_0_1")
		(symbol "FODM214_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FODM217A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FODM217A"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FODM214-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 80V, CTR 80-160%, SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC Phototransistor Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "FODM217A_0_1")
		(symbol "FODM217A_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "H11AA1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.334 4.953 0)
		)
		(property "Value" "H11AA1"
			(at 0.635 4.953 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at -12.446 -4.953 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83608/h11aa1.pdf"
			(at 19.304 16.002 0)
		)
		(property "Description" "AC/DC NPN Optocoupler, DIP-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "H11AA1_0_1")
		(symbol "H11AA1_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "H11L1"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "H11L1"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -2.286 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/H11L3M-D.PDF"
			(at -2.286 0 0)
		)
		(property "Description" "Schmitt Trigger Output Optocoupler, High Speed, DIP-6, 1.6mA turn on threshold"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Speed Schmitt Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*"
			(at 0 0 0)
		)
		(symbol "H11L1_0_1")
		(symbol "H11L1_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin output inverted
				(at 7.62 0 180)
				(length 3.81)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HCNW2201"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "HCNW2201"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W10.16mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0674EN"
			(at 0 0 0)
		)
		(property "Description" "Opto Coupler, 1kV/us, 50V CMR, Schmitt trigger output, WDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto coupler schmitt output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
		(symbol "HCNW2201_0_1")
		(symbol "HCNW2201_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HCPL-0201"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "HCPL-0201"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0674EN"
			(at 0.254 0 0)
		)
		(property "Description" "Opto Coupler, 1kV/us, 50V CMR, Schmitt trigger output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto coupler schmitt output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HCPL-0201_0_1")
		(symbol "HCPL-0201_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HCPL-061A"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "HCPL-061A"
			(at 0.254 -9.144 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://docs.avagotech.com/docs/AV02-0391EN"
			(at -21.59 15.24 0)
		)
		(property "Description" "Single High Speed HCMOS/LSTTL/TTL Compatible Optocoupler with enable, dV/dt 1000/us, VCM 50, -0.5V to 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HCPL-061A_0_1")
		(symbol "HCPL-061A_1_1"
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "6")
			)
			(pin power_in line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HCPL-063A"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "HCPL-063A"
			(at 7.874 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://docs.avagotech.com/docs/AV02-0391EN"
			(at -21.59 15.24 0)
		)
		(property "Description" "Dual High Speed HCMOS/LSTTL/TTL Compatible Optocoupler, dV/dt 1000/us, VCM 50, -0.5V to 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "HCPL-063A_0_1")
		(symbol "HCPL-063A_1_1"
			(pin passive line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C1")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VO1")
				(number "7")
			)
			(pin open_collector line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VO2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HCPL-2201"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "HCPL-2201"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0674EN"
			(at 0 0 0)
		)
		(property "Description" "Opto Coupler, 1kV/us, 50V CMR, Schmitt trigger output, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto coupler schmitt output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "HCPL-2201_0_1")
		(symbol "HCPL-2201_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HCPL-2202"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "HCPL-2202"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0674EN"
			(at 0 0 0)
		)
		(property "Description" "Opto Coupler, 1kV/us, 50V CMR, Schmitt trigger output, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto coupler schmitt output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "HCPL-2202_0_1")
		(symbol "HCPL-2202_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin no_connect line
				(at 5.08 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "~")
				(number "7")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HCPL-2601"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 8.89 0)
		)
		(property "Value" "HCPL-2601"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 17.78 0 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/doc/6N137-HCNW137-2601-2611-HCPL-0600-0601-0611-0630-0631-0661-2601-2611-2630-2631-4661-High-CMR-High-Speed-TTL-Compatible-Optocouplers-DS"
			(at 17.78 2.54 0)
		)
		(property "Description" "Single High Speed LSTTL/TTL Compatible Optocoupler with enable, dV/dt 10000V/us, VCM 1000, max 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "HCPL-2601_0_1")
		(symbol "HCPL-2601_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 7.62 0)
				(length 0)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -7.62 0)
				(length 0)
				(hide yes)
				(name "")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HCPL-261A"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -2.54 8.89 0)
		)
		(property "Value" "HCPL-261A"
			(at 2.54 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -10.16 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/doc/AV02-0391EN"
			(at 2.54 -12.7 0)
		)
		(property "Description" "Single High Speed HCMOS/LSTTL/TTL Compatible Optocoupler with enable, dV/dt 1000/us, VCM 50, -0.5V to 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "HCPL-261A_0_1")
		(symbol "HCPL-261A_1_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "NC")
				(number "1")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "EN")
				(number "7")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "VO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HCPL-263A"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "HCPL-263A"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -18.288 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/doc/AV02-0391EN"
			(at -10.16 8.89 0)
		)
		(property "Description" "Dual High Speed HCMOS/LSTTL/TTL Compatible Optocoupler, dV/dt 1000/us, VCM 50, -0.5V to 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "HCPL-263A_1_1"
			(pin passive line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C1")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin open_collector line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VO1")
				(number "7")
			)
			(pin open_collector line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VO2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HCPL-9000"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 8.89 0)
		)
		(property "Value" "HCPL-9000"
			(at 10.16 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -1.27 -17.78 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0137EN"
			(at -1.27 8.89 0)
		)
		(property "Description" "High Speed Digital Isolator, CMOS, excellent transient immunity, active-low logic output enable, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator, high speed"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "HCPL-9000_0_1")
		(symbol "HCPL-9000_1_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN1")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VDD2")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND2")
				(number "5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "V~{OE}")
				(number "7")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUT1")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HCPL2731"
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "HCPL2731"
			(at -5.08 -10.16 0)
		)
		(property "Footprint" ""
			(at -0.635 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/HCPL2731-D.pdf"
			(at -0.635 0 0)
		)
		(property "Description" "Low Input Current high Gain Split Darlington Optocouplers, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm*"
			(at 0 0 0)
		)
		(symbol "HCPL2731_0_1")
		(symbol "HCPL2731_1_1"
			(pin passive line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C1")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VO1")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VO2")
				(number "6")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "GND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ILD74"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ILD74"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83640/ild74.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual Optocoupler, NPN Phototransistor Output, TTL compatible, DIP8/SMD8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Dual Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*Clearance8mm*"
			(at 0 0 0)
		)
		(symbol "ILD74_0_1")
		(symbol "ILD74_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
		)
		(symbol "ILD74_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ILQ74"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ILQ74"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83640/ild74.pdf"
			(at 0 0 0)
		)
		(property "Description" "Quad Optocoupler, NPN Phototransistor Output, TTL compatible, DIP16/SMD16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Dual Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*Clearance8mm*"
			(at 0 0 0)
		)
		(symbol "ILQ74_0_1")
		(symbol "ILQ74_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
		)
		(symbol "ILQ74_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "ILQ74_3_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
		)
		(symbol "ILQ74_4_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO1211"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 6.35 0)
		)
		(property "Value" "ISO1211"
			(at 8.89 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/iso1211.pdf"
			(at -1.27 1.27 0)
		)
		(property "Description" "Isolated, 1 Channel, 24 to 60V Digital Input Receiver, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated digital input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO1211_0_1")
		(symbol "ISO1211_1_1"
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SENSE")
				(number "8")
			)
			(pin input line
				(at -12.7 0 0)
				(length 2.54)
				(name "IN")
				(number "7")
			)
			(pin passive line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SUB")
				(number "5")
			)
			(pin power_in line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "FGND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 2.54)
				(name "OUT")
				(number "3")
			)
			(pin input line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "EN")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO1212"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "ISO1212"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/iso1212.pdf"
			(at -1.27 8.89 0)
		)
		(property "Description" "Isolated, 2 Channels, 24 to 60V Digital Inputs Receiver, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated digital input"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ISO1212_0_1")
		(symbol "ISO1212_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "SENSE1")
				(number "16")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IN1")
				(number "15")
			)
			(pin passive line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "SUB1")
				(number "13")
			)
			(pin power_in line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "FGND1")
				(number "14")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SENSE2")
				(number "11")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "IN2")
				(number "10")
			)
			(pin passive line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "SUB2")
				(number "12")
			)
			(pin power_in line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "FGND2")
				(number "9")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VCC1")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "1")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUT1")
				(number "4")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "OUT2")
				(number "5")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "EN")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO1540"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "ISO1540"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/iso1541.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "I2C Isolator, 2.5 kVrms, Bidirectional clock and data, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO1540_0_1")
		(symbol "ISO1540_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCL1")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VCC2")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SDA2")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SCL2")
				(number "6")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO1541"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "ISO1541"
			(at 3.81 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/iso1541.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "I2C Isolator, 2.5 kVrms, Unidirectional Clock, Bidirectional data, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "digital isolator i2c"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO1541_0_1")
		(symbol "ISO1541_1_1"
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "SDA1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "SCL1")
				(number "3")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "VCC2")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "SDA2")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "SCL2")
				(number "6")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND2")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO1642DWR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 13.97 0)
		)
		(property "Value" "ISO1642DWR"
			(at 10.16 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at -2.54 -27.94 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso1642.pdf"
			(at -2.54 -30.48 0)
		)
		(property "Description" "I2C Isolator with Bidirectional Clock and Data and two 1/1 Auxiliary GPIOs, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "i2c isolator additional gpio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO1642DWR_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL1")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA1")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INA")
				(number "4")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OUTB")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VCC2")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 7.62 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCL2")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA2")
				(number "14")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "13")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "INB")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO1643DWR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 13.97 0)
		)
		(property "Value" "ISO1643DWR"
			(at 10.16 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at -2.54 -27.94 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso1643.pdf"
			(at -2.54 -30.48 0)
		)
		(property "Description" "I2C Isolator with Bidirectional Clock and Data and two 2/0 Auxiliary GPIOs, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "i2c isolator additional gpio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO1643DWR_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL1")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA1")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INA")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "INB")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -7.62 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VCC2")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at 7.62 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCL2")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA2")
				(number "14")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "13")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO1644DWR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 13.97 0)
		)
		(property "Value" "ISO1644DWR"
			(at 10.16 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at -2.54 -27.94 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso1644.pdf"
			(at -2.54 -30.48 0)
		)
		(property "Description" "I2C Isolator with Bidirectional Clock and Data and three 2/1 Auxiliary GPIOs, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "i2c isolator additional gpio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO1644DWR_1_1"
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "SCL1")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "SDA1")
				(number "3")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INA")
				(number "4")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "INB")
				(number "5")
			)
			(pin output line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "OUT")
				(number "7")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VCC2")
				(number "16")
			)
			(pin passive line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "SCL2")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "SDA2")
				(number "14")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "13")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "12")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "INC")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO6731"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO6731"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso6731.pdf"
			(at 5.715 -16.51 0)
		)
		(property "Description" "General-purpose, triple-channel, 2/1, digital isolator"
			(at 0 0 0)
		)
		(property "ki_keywords" "3 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO6731_0_1")
		(symbol "ISO6731_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INA")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "OUTC")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "EN1")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "V_{CC1}")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "V_{CC2}")
				(number "16")
			)
			(pin passive line
				(at 5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin no_connect line
				(at 7.62 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTA")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "13")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "INC")
				(number "12")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO6740"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO6740"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso6740.pdf"
			(at 5.715 -16.51 0)
		)
		(property "Description" "General-purpose, quad-channel, 4/0 digital isolator"
			(at 0 0 0)
		)
		(property "ki_keywords" "4 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO6740_0_1")
		(symbol "ISO6740_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INA")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "INC")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "IND")
				(number "6")
			)
			(pin no_connect line
				(at -7.62 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "V_{CC1}")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "V_{CC2}")
				(number "16")
			)
			(pin passive line
				(at 5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTA")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTC")
				(number "12")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTD")
				(number "11")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO6741"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO6741"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso6741.pdf"
			(at 5.715 -16.51 0)
		)
		(property "Description" "General-purpose, quad-channel, 3/1 digital isolator"
			(at 0 0 0)
		)
		(property "ki_keywords" "4 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO6741_0_1")
		(symbol "ISO6741_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INA")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "INC")
				(number "5")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUTD")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "EN1")
				(number "7")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "V_{CC1}")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "V_{CC2}")
				(number "16")
			)
			(pin passive line
				(at 5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTA")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTC")
				(number "12")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IND")
				(number "11")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO6742"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO6742"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso6742.pdf"
			(at 5.715 -16.51 0)
		)
		(property "Description" "General-purpose, quad-channel, 2/2 digital isolator"
			(at 0 0 0)
		)
		(property "ki_keywords" "4 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO6742_0_1")
		(symbol "ISO6742_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INA")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "OUTC")
				(number "5")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUTD")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "EN1")
				(number "7")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 2.54)
				(name "V_{CC1}")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 2.54)
				(name "V_{CC2}")
				(number "16")
			)
			(pin passive line
				(at 5.08 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTA")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "13")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "INC")
				(number "12")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "IND")
				(number "11")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7320C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.795 0)
		)
		(property "Value" "ISO7320C"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7320c&fileType=pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power Dual-Channel 2/0 Digital Isolator, 25Mbps 33ns, Fail-Safe High, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "ISO7320C_0_1")
		(symbol "ISO7320C_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "INB")
				(number "3")
			)
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VCC2")
				(number "8")
			)
			(pin power_in line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "GND2")
				(number "5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "7")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7321C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 10.795 0)
		)
		(property "Value" "ISO7321C"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7321c&fileType=pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power Dual-Channel 1/1 Digital Isolator, 25Mbps 33ns, Fail-Safe High, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "ISO7321C_0_1")
		(symbol "ISO7321C_1_1"
			(pin power_in line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin power_in line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUTA")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "INB")
				(number "3")
			)
			(pin power_in line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VCC2")
				(number "8")
			)
			(pin power_in line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "GND2")
				(number "5")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "INA")
				(number "7")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7330C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "ISO7330C"
			(at 8.382 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/iso7330-q1.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "Low Power Quad-Channel 3/0 Digital Isolator, 25Mbps 31ns, Fail-Safe High, SO16"
			(at 0 0 0)
		)
		(property "ki_keywords" "3Ch Quad Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO7330C_0_1")
		(symbol "ISO7330C_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INA")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INC")
				(number "5")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 0 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VCC2")
				(number "16")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "EN")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTB")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTC")
				(number "12")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7331C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "ISO7331C"
			(at 6.858 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/iso7331c.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low Power Quad-Channel 2/1 Digital Isolator, 25Mbps 31ns, Fail-Safe High, SO16"
			(at 0 0 0)
		)
		(property "ki_keywords" "3Ch Quad Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO7331C_0_1")
		(symbol "ISO7331C_1_1"
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "EN1")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INA")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUTC")
				(number "5")
			)
			(pin power_in line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin power_in line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin no_connect line
				(at 0 10.16 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin no_connect line
				(at 0 -10.16 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "VCC2")
				(number "16")
			)
			(pin input line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTB")
				(number "13")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "INC")
				(number "12")
			)
			(pin power_in line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin power_in line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7340C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ISO7340C"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7340c&fileType=pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low Power Quad-Channel 4/0 Digital Isolator, 25Mbps 31ns, Fail-Safe High, SO16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch Quad Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "ISO7340C_0_1")
		(symbol "ISO7340C_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INA")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "INC")
				(number "5")
			)
			(pin input line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "IND")
				(number "6")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VCC2")
				(number "16")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "EN")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "14")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "13")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OUTC")
				(number "12")
			)
			(pin output line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "OUTD")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7341C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ISO7341C"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7341c&fileType=pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low Power Quad-Channel 3/1 Digital Isolator, 25Mbps 31ns, Fail-Safe High, SO16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch Quad Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "ISO7341C_0_1")
		(symbol "ISO7341C_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN1")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INA")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "INC")
				(number "5")
			)
			(pin output line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "OUTD")
				(number "6")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VCC2")
				(number "16")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "14")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "13")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "OUTC")
				(number "12")
			)
			(pin input line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "IND")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7342C"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ISO7342C"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7342c&fileType=pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low Power Quad-Channel 2/2 Digital Isolator, 25Mbps 31ns, Fail-Safe High, SO16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch Quad Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "ISO7342C_0_1")
		(symbol "ISO7342C_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VCC1")
				(number "1")
			)
			(pin power_in line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "EN1")
				(number "7")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INA")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "INB")
				(number "4")
			)
			(pin output line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "OUTC")
				(number "5")
			)
			(pin output line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "OUTD")
				(number "6")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VCC2")
				(number "16")
			)
			(pin power_in line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTA")
				(number "14")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "13")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "INC")
				(number "12")
			)
			(pin input line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "IND")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7760DBQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7760DBQ"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default high, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ISO7760DBQ_0_1")
		(symbol "ISO7760DBQ_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INB")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INC")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IND")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INE")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "INF")
				(number "7")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "Vcc1")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "Vcc2")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUTA")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTC")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTD")
				(number "12")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTE")
				(number "11")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUTF")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7760DW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7760DW"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default high, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO7760DW_0_1")
		(symbol "ISO7760DW_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INB")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INC")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IND")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INE")
				(number "6")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "INF")
				(number "7")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "Vcc1")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "Vcc2")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUTA")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTC")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTD")
				(number "12")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTE")
				(number "11")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "OUTF")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7761DBQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7761DBQ"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default high, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ISO7761DBQ_0_1")
		(symbol "ISO7761DBQ_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INB")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INC")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IND")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INE")
				(number "6")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OUTF")
				(number "7")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "Vcc1")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "Vcc2")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUTA")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTC")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTD")
				(number "12")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTE")
				(number "11")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "INF")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7761DW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7761DW"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default high, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO7761DW_0_1")
		(symbol "ISO7761DW_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INB")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INC")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IND")
				(number "5")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "INE")
				(number "6")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OUTF")
				(number "7")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "Vcc1")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "Vcc2")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUTA")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTC")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTD")
				(number "12")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUTE")
				(number "11")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "INF")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7762DBQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7762DBQ"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default high, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ISO7762DBQ_0_1")
		(symbol "ISO7762DBQ_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INB")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INC")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IND")
				(number "5")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUTE")
				(number "6")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OUTF")
				(number "7")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "Vcc1")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "Vcc2")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUTA")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTC")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTD")
				(number "12")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "INE")
				(number "11")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "INF")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7762DW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7762DW"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default high, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO7762DW_0_1")
		(symbol "ISO7762DW_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INB")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INC")
				(number "4")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IND")
				(number "5")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUTE")
				(number "6")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OUTF")
				(number "7")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "Vcc1")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "Vcc2")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUTA")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTC")
				(number "13")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "OUTD")
				(number "12")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "INE")
				(number "11")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "INF")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7763DBQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7763DBQ"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default high, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "ISO7763DBQ_0_1")
		(symbol "ISO7763DBQ_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INB")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INC")
				(number "4")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "OUTD")
				(number "5")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUTE")
				(number "6")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OUTF")
				(number "7")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "Vcc1")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "Vcc2")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUTA")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTC")
				(number "13")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "IND")
				(number "12")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "INE")
				(number "11")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "INF")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISO7763DW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7763DW"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default high, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISO7763DW_0_1")
		(symbol "ISO7763DW_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "INB")
				(number "3")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "INC")
				(number "4")
			)
			(pin output line
				(at -10.16 0 0)
				(length 2.54)
				(name "OUTD")
				(number "5")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "OUTE")
				(number "6")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "OUTF")
				(number "7")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "Vcc1")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -15.24 90)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "Vcc2")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -15.24 90)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
			(pin output line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "OUTA")
				(number "15")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "OUTB")
				(number "14")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUTC")
				(number "13")
			)
			(pin input line
				(at 10.16 0 180)
				(length 2.54)
				(name "IND")
				(number "12")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "INE")
				(number "11")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "INF")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISOW7740"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "ISOW7740"
			(at 3.81 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/isow7741.pdf"
			(at 0 -36.83 0)
		)
		(property "Description" "Quad-Channel 4/0 Digital Isolator with Integrated Low-Emissions, Low-Noise DC-DC Converter, SOIC-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4-channel-digital-isolator integrated-isolated-supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISOW7740_0_1")
		(symbol "ISOW7740_1_1"
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "EN/FLT")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "EN_IO1")
				(number "7")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "INB")
				(number "3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "INC")
				(number "4")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "IND")
				(number "5")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "V_{IO}")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "GNDIO")
				(number "6")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND1")
				(number "10")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "V_{ISOIN}")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "GISOIN")
				(number "15")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "V_{ISOOUT}")
				(number "12")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VSEL")
				(number "13")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "EN_IO2")
				(number "14")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUTA")
				(number "19")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "18")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUTC")
				(number "17")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "OUTD")
				(number "16")
			)
			(pin power_out line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISOW7741"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "ISOW7741"
			(at 3.81 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/isow7741.pdf"
			(at 0 -36.83 0)
		)
		(property "Description" "Quad-Channel 3/1 Digital Isolator with Integrated Low-Emissions, Low-Noise DC-DC Converter, SOIC-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4-channel-digital-isolator integrated-isolated-supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISOW7741_0_1")
		(symbol "ISOW7741_1_1"
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "EN/FLT")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "EN_IO1")
				(number "7")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "INB")
				(number "3")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "INC")
				(number "4")
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "OUTD")
				(number "5")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "V_{IO}")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "GNDIO")
				(number "6")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND1")
				(number "10")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "V_{ISOIN}")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "GISOIN")
				(number "15")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "V_{ISOOUT}")
				(number "12")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VSEL")
				(number "13")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "EN_IO2")
				(number "14")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUTA")
				(number "19")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "18")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "OUTC")
				(number "17")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IND")
				(number "16")
			)
			(pin power_out line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISOW7742"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "ISOW7742"
			(at 3.81 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/isow7741.pdf"
			(at 0 -36.83 0)
		)
		(property "Description" "Quad-Channel 2/2 Digital Isolator with Integrated Low-Emissions, Low-Noise DC-DC Converter, SOIC-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4-channel-digital-isolator integrated-isolated-supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISOW7742_0_1")
		(symbol "ISOW7742_1_1"
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "EN/FLT")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "EN_IO1")
				(number "7")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "INB")
				(number "3")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "OUTC")
				(number "4")
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "OUTD")
				(number "5")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "V_{IO}")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "GNDIO")
				(number "6")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND1")
				(number "10")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "V_{ISOIN}")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "GISOIN")
				(number "15")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "V_{ISOOUT}")
				(number "12")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VSEL")
				(number "13")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "EN_IO2")
				(number "14")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUTA")
				(number "19")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "OUTB")
				(number "18")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "INC")
				(number "17")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IND")
				(number "16")
			)
			(pin power_out line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISOW7743"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "ISOW7743"
			(at 3.81 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/isow7741.pdf"
			(at 0 -36.83 0)
		)
		(property "Description" "Quad-Channel 1/3 Digital Isolator with Integrated Low-Emissions, Low-Noise DC-DC Converter, SOIC-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4-channel-digital-isolator integrated-isolated-supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISOW7743_0_1")
		(symbol "ISOW7743_1_1"
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "EN/FLT")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "EN_IO1")
				(number "7")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "INA")
				(number "2")
			)
			(pin output line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "OUTB")
				(number "3")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "OUTC")
				(number "4")
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "OUTD")
				(number "5")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "V_{IO}")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "GNDIO")
				(number "6")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND1")
				(number "10")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "V_{ISOIN}")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "GISOIN")
				(number "15")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "V_{ISOOUT}")
				(number "12")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VSEL")
				(number "13")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "EN_IO2")
				(number "14")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "OUTA")
				(number "19")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "INB")
				(number "18")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "INC")
				(number "17")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IND")
				(number "16")
			)
			(pin power_out line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ISOW7744"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "ISOW7744"
			(at 3.81 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/isow7741.pdf"
			(at 0 -36.83 0)
		)
		(property "Description" "Quad-Channel 0/4 Digital Isolator with Integrated Low-Emissions, Low-Noise DC-DC Converter, SOIC-20W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4-channel-digital-isolator integrated-isolated-supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ISOW7744_0_1")
		(symbol "ISOW7744_1_1"
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "EN/FLT")
				(number "8")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "EN_IO1")
				(number "7")
			)
			(pin output line
				(at -15.24 0 0)
				(length 2.54)
				(name "OUTA")
				(number "2")
			)
			(pin output line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "OUTB")
				(number "3")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "OUTC")
				(number "4")
			)
			(pin output line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "OUTD")
				(number "5")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 2.54)
				(name "V_{IO}")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -20.32 90)
				(length 2.54)
				(name "GNDIO")
				(number "6")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 2.54)
				(name "V_{DD}")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 2.54)
				(name "GND1")
				(number "10")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 2.54)
				(name "V_{ISOIN}")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 2.54)
				(name "GISOIN")
				(number "15")
			)
			(pin power_out line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "V_{ISOOUT}")
				(number "12")
			)
			(pin input line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "VSEL")
				(number "13")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "EN_IO2")
				(number "14")
			)
			(pin input line
				(at 15.24 0 180)
				(length 2.54)
				(name "INA")
				(number "19")
			)
			(pin input line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "INB")
				(number "18")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "INC")
				(number "17")
			)
			(pin input line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IND")
				(number "16")
			)
			(pin power_out line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "GND2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-247"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "LTV-247"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-16_4.4x10.4mm_P1.27mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS70-2009-0014/LTV-2X7%20sereis%20Mar17.PDF"
			(at 0 0 0)
		)
		(property "Description" "DC Quad Optocoupler, Vce 80V, CTR 100-600%, SOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Quad Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x10.4mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LTV-247_0_1")
		(symbol "LTV-247_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "LTV-247_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "LTV-247_3_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "LTV-247_4_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-352T"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 5.08 0)
		)
		(property "Value" "LTV-352T"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SO-4_4.4x3.6mm_P2.54mm"
			(at -7.62 -5.08 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS70-2001-002/S_110_LTV-352T%2020140520.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Darlington Optocoupler, Vce 300V, CTR 1000%, SO-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Darlington DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*4.4x3.6mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "LTV-352T_0_0")
		(symbol "LTV-352T_0_1")
		(symbol "LTV-352T_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-354T"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "LTV-354T"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SO-4_4.4x3.6mm_P2.54mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS70-2001-004/S_110_LTV-354T%2020140520.pdf"
			(at 0.635 0 0)
		)
		(property "Description" "AC/DC Optocoupler, Vce 35V, CTR 20%, SO-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*4.4x3.6mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "LTV-354T_0_1")
		(symbol "LTV-354T_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-355T"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "LTV-355T"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SO-4_4.4x3.6mm_P2.54mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS70-2001-006/S_110_LTV-355T%2020140520.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Darlington Optocoupler, Vce 35V, CTR 600%, SO-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Darlington DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*4.4x3.6mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "LTV-355T_0_1")
		(symbol "LTV-355T_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-356T"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "LTV-356T"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SO-4_4.4x3.6mm_P2.54mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS70-2001-010/S_110_LTV-356T%2020140520.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 80V, CTR 50%, SO-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*4.4x3.6mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "LTV-356T_0_1")
		(symbol "LTV-356T_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-814"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "LTV-814"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS-70-96-0013/LTV-8X4%20series%20201509.pdf"
			(at 1.905 0 0)
		)
		(property "Description" "AC/DC Optocoupler, Vce 35V, CTR 20%, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LTV-814_0_1")
		(symbol "LTV-814_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-817"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "LTV-817"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.us.liteon.com/downloads/LTV-817-827-847.PDF"
			(at 0 -2.54 0)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50%, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LTV-817_0_1")
		(symbol "LTV-817_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-817M"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "LTV-817M"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.us.liteon.com/downloads/LTV-817-827-847.PDF"
			(at -10.16 7.62 0)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50%, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
		(symbol "LTV-817M_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-817S"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "LTV-817S"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W9.53mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.us.liteon.com/downloads/LTV-817-827-847.PDF"
			(at -8.89 7.62 0)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50%, SMDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm*"
			(at 0 0 0)
		)
		(symbol "LTV-817S_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-824"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "LTV-824"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS-70-96-0013/S_110_LTV-814%20824%20844%20(M,%20S,%20S-TA,%20S-TA1,%20S-TP)%20Series.pdf"
			(at 0.635 0 0)
		)
		(property "Description" "Dual AC/DC Optocoupler, Vce 35V, CTR 20%, DIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual NPN AC DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LTV-824_0_1")
		(symbol "LTV-824_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LTV-824_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-827M"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "LTV-827M"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W10.16mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.us.liteon.com/downloads/LTV-817-827-847.PDF"
			(at -21.59 13.97 0)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50%, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
		(symbol "LTV-827M_0_1")
		(symbol "LTV-827M_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LTV-827M_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-827S"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "LTV-827S"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-8_W9.53mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.us.liteon.com/downloads/LTV-817-827-847.PDF"
			(at -20.32 13.97 0)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50%, SMDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm*"
			(at 0 0 0)
		)
		(symbol "LTV-827S_0_1")
		(symbol "LTV-827S_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "LTV-827S_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-844"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "LTV-844"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS-70-96-0013/S_110_LTV-814%20824%20844%20(M,%20S,%20S-TA,%20S-TA1,%20S-TP)%20Series.pdf"
			(at 0.635 0 0)
		)
		(property "Description" "Quad AC/DC Optocoupler, Vce 35V, CTR 20%, DIP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Quad NPN AC DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "LTV-844_0_1")
		(symbol "LTV-844_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "LTV-844_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "LTV-844_3_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "LTV-844_4_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-847M"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "LTV-847M"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W10.16mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.us.liteon.com/downloads/LTV-817-827-847.PDF"
			(at -11.43 10.16 0)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50%, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
		(symbol "LTV-847M_0_1")
		(symbol "LTV-847M_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "LTV-847M_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "LTV-847M_3_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "LTV-847M_4_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTV-847S"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "LTV-847S"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-16_W9.53mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.us.liteon.com/downloads/LTV-817-827-847.PDF"
			(at -15.24 11.43 0)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50%, SMDIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm*"
			(at 0 0 0)
		)
		(symbol "LTV-847S_0_1")
		(symbol "LTV-847S_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "LTV-847S_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "LTV-847S_3_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "LTV-847S_4_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAX14850AEE+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -9.525 16.51 0)
		)
		(property "Value" "MAX14850AEE+"
			(at 13.335 16.51 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX14850.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Six-channel digital isolator, bidirectional, 3V3, 5V, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "MAX14850AEE+_0_1")
		(symbol "MAX14850AEE+_1_1"
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "INA1")
				(number "2")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "INA2")
				(number "3")
			)
			(pin output line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "OUTA1")
				(number "4")
			)
			(pin output line
				(at -12.7 0 0)
				(length 2.54)
				(name "OUTA2")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "I/OA1")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "I/OA2")
				(number "7")
			)
			(pin power_in line
				(at -5.08 17.78 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "GNDA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "VCCB")
				(number "16")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "GNDB")
				(number "9")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "OUTB1")
				(number "15")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "OUTB2")
				(number "14")
			)
			(pin input line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "INB1")
				(number "13")
			)
			(pin input line
				(at 12.7 0 180)
				(length 2.54)
				(name "INB2")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "I/OB1")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "I/OB2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MID400"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.715 6.985 0)
		)
		(property "Value" "MID400"
			(at 5.715 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/MID400-D.pdf"
			(at 0 0 0)
		)
		(property "Description" "AC Line Monitor Logic-Out Device, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC line monitor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "MID400_0_1")
		(symbol "MID400_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "VIN1")
				(number "1")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "VIN2")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin no_connect line
				(at 7.62 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "AUX")
				(number "7")
			)
			(pin open_collector line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "VO")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MOCD207M"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOCD207M"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -21.082 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mocd217m-d.pdf"
			(at -34.29 0 0)
		)
		(property "Description" "8-pin SOIC Dual-Channel Phototransistor Output Optocoupler, VCEO 70V, VF 1.25-1.5V (IF 30mA), CTR 100-200%, SOIC8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Dual Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9*4.9*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MOCD207M_0_1")
		(symbol "MOCD207M_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "MOCD207M_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NSL-32"
		(pin_names
			(offset 0.762)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "NSL-32"
			(at 0 -5.08 0)
		)
		(property "Footprint" "OptoDevice:Luna_NSL-32"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://lunainc.com/wp-content/uploads/2016/06/NSL-32.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "Optocoupler, LED Input, Photocell Output"
			(at 0 0 0)
		)
		(property "ki_keywords" "optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Luna*NSL?32*"
			(at 0 0 0)
		)
		(symbol "NSL-32_0_1")
		(symbol "NSL-32_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "K")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "R")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "R")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PC3H4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "PC3H4"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.sharpsme.com/download/pc3h4-epdf"
			(at 0.635 0 0)
		)
		(property "Description" "AC/DC Optocoupler, Vce 70V, CTR 100-250%, SOP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PC3H4_0_1")
		(symbol "PC3H4_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PC817"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "PC817"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50-300%, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PC817_0_1")
		(symbol "PC817_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PC827"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "PC827"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS-70-96-0016/LTV-8X7%20series.PDF"
			(at 0 0 0)
		)
		(property "Description" "Dual DC Optocoupler, Vce 35V, CTR 50%, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Dual Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PC827_0_1")
		(symbol "PC827_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "PC827_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PC837"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "PC837"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-12_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Triple Optocoupler, Vce 35V, CTR 50-300%, DIP12"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Triple Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PC837_0_1")
		(symbol "PC837_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "PC837_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(symbol "PC837_3_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PC847"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "PC847"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.soselectronic.cz/a_info/resource/d/pc817.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Quad Optocoupler, Vce 35V, CTR 50-300%, DIP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Quad Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PC847_0_1")
		(symbol "PC847_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "PC847_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "PC847_3_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "PC847_4_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PS8802-1"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "PS8802-1"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_SO:SSOP-8_3.95x5.21x3.27mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.cel.com/pdf/datasheets/ps8802.pdf"
			(at 0 0 0)
		)
		(property "Description" "Single DC Optocoupler Base Connected, Vcc 35V, CTR 15%, Viso 2500V, SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.95x5.21x3.27mm?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PS8802-1_0_1")
		(symbol "PS8802-1_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin no_connect line
				(at -5.08 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -5.08 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "VO")
				(number "6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "GND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PS8802-2"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "PS8802-2"
			(at 0 10.16 0)
		)
		(property "Footprint" "Package_SO:SSOP-8_3.95x5.21x3.27mm_P1.27mm"
			(at -5.08 -10.16 0)
		)
		(property "Datasheet" "http://www.cel.com/pdf/datasheets/ps8802.pdf"
			(at -1.143 5.08 0)
		)
		(property "Description" "Dual DC Optocoupler Base Connected, Vcc 35V, CTR 15%, Viso 2500V, SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.95x5.21x3.27mm?P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PS8802-2_0_1")
		(symbol "PS8802-2_1_1"
			(pin passive line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "C1")
				(number "2")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "C2")
				(number "3")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin passive line
				(at 7.62 7.62 180)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "VO1")
				(number "7")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "VO2")
				(number "6")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "GND")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH617A-1X007T"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "SFH617A-1X007T"
			(at -5.08 -6.35 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80, -55 to +110 degree Celsius, UL, BSI, FIMKO, cUL, 8mm clearence SMD PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm*Clearance8mm*"
			(at 0 0 0)
		)
		(symbol "SFH617A-1X007T_0_1")
		(symbol "SFH617A-1X007T_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH617A-2X009T"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "SFH617A-2X009T"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W7.62mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at -8.89 7.62 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125, -55 to +110 degree Celsius, UL, BSI, FIMKO, SMD PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SFH617A-2X009T_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH620A-1"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH620A-1"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-125, UL, cUL, BSI, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-125"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "SFH620A-1_0_1")
		(symbol "SFH620A-1_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH620A-1X006"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH620A-1X006"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-125, UL, cUL, BSI, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-125"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
		(symbol "SFH620A-1X006_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH620A-2X007T"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH620A-2X007T"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200 UL, cUL, BSI, SMD-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm?Clearance8mm*"
			(at 0 0 0)
		)
		(symbol "SFH620A-2X007T_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8640BA-B-IU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8640BA-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 1.0kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "Si8640BA-B-IU_0_1")
		(symbol "Si8640BA-B-IU_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "12")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B4")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8640BB-B-IS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8640BB-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Si8640BB-B-IS_0_1")
		(symbol "Si8640BB-B-IS_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "12")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B4")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8640BB-B-IS1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8640BB-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Si8640BB-B-IS1_0_1")
		(symbol "Si8640BB-B-IS1_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "12")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B4")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8641BA-B-IU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8641BA-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 1.0kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 3In 1Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "Si8641BA-B-IU_0_1")
		(symbol "Si8641BA-B-IU_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN1")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "12")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B4")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8641BB-B-IS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8641BB-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 3In 1Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Si8641BB-B-IS_0_1")
		(symbol "Si8641BB-B-IS_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN1")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "12")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B4")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8641BB-B-IS1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8641BB-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 3In 1Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Si8641BB-B-IS1_0_1")
		(symbol "Si8641BB-B-IS1_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN1")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "12")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B4")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8642BA-B-IU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8642BA-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 1.0kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 2In 2Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "Si8642BA-B-IU_0_1")
		(symbol "Si8642BA-B-IU_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN1")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "13")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "12")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B4")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8642BB-B-IS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8642BB-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 2In 2Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Si8642BB-B-IS_0_1")
		(symbol "Si8642BB-B-IS_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN1")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "13")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "12")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B4")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8642BB-B-IS1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8642BB-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 2In 2Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Si8642BB-B-IS1_0_1")
		(symbol "Si8642BB-B-IS1_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "EN1")
				(number "7")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin input line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "EN2")
				(number "10")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "13")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "12")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B4")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8645BA-B-IU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8645BA-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 1.0kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "Si8645BA-B-IU_0_1")
		(symbol "Si8645BA-B-IU_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "12")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B4")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8645BB-B-IS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8645BB-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Si8645BB-B-IS_0_1")
		(symbol "Si8645BB-B-IS_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "12")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B4")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8645BB-B-IS1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8645BB-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Si8645BB-B-IS1_0_1")
		(symbol "Si8645BB-B-IS1_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin power_in line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "GND1")
				(number "2")
			)
			(pin passive line
				(at -10.16 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "GND1")
				(number "8")
			)
			(pin no_connect line
				(at -7.62 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 7.62 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "12")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B4")
				(number "11")
			)
			(pin power_in line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "GND2")
				(number "15")
			)
			(pin passive line
				(at 10.16 -10.16 180)
				(length 2.54)
				(hide yes)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8660BA-B-IS1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660BA-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 1kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Si8660BA-B-IS1_0_1")
		(symbol "Si8660BA-B-IS1_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A6")
				(number "7")
			)
			(pin power_in line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B1")
				(number "15")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B3")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B4")
				(number "12")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B5")
				(number "11")
			)
			(pin output line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B6")
				(number "10")
			)
			(pin power_in line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8661BB-B-IS1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661BB-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Si8661BB-B-IS1_0_1")
		(symbol "Si8661BB-B-IS1_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin output line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A6")
				(number "7")
			)
			(pin power_in line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B1")
				(number "15")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B3")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B4")
				(number "12")
			)
			(pin output line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B5")
				(number "11")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B6")
				(number "10")
			)
			(pin power_in line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8662BB-B-IS1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662BB-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Si8662BB-B-IS1_0_1")
		(symbol "Si8662BB-B-IS1_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin output line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A6")
				(number "7")
			)
			(pin power_in line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B1")
				(number "15")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B3")
				(number "13")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B4")
				(number "12")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B5")
				(number "11")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B6")
				(number "10")
			)
			(pin power_in line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Si8663BB-B-IS1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663BB-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "Si8663BB-B-IS1_0_1")
		(symbol "Si8663BB-B-IS1_1_1"
			(pin power_in line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin output line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin output line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin output line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A6")
				(number "7")
			)
			(pin power_in line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "GND1")
				(number "8")
			)
			(pin power_in line
				(at 10.16 10.16 180)
				(length 2.54)
				(name "VDD2")
				(number "16")
			)
			(pin output line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B1")
				(number "15")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "14")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B3")
				(number "13")
			)
			(pin input line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B4")
				(number "12")
			)
			(pin input line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B5")
				(number "11")
			)
			(pin input line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B6")
				(number "10")
			)
			(pin power_in line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "GND2")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCMT1100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TCMT1100"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83510/tcmt1100.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Vce 70V, CTR 50-600%, Viso 3750V (RMS), SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TCMT1100_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCMT4100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TCMT4100"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-16_4.4x10.4mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/84181/tcmt4100.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Quad Optocoupler, Vce 70V, CTR 50-600%, Viso 3750V (RMS), SOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x10.4mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TCMT4100_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "TCMT4100_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "TCMT4100_3_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "TCMT4100_4_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP127"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -4.826 5.08 0)
		)
		(property "Value" "TLP127"
			(at -5.207 -5.08 0)
		)
		(property "Footprint" "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=16902&prodName=TLP127"
			(at -1.778 0 0)
		)
		(property "Description" "DC Darlington Optocoupler, Vce 300V, CTR 1000%, MFSOP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Darlington DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MFSOP6*4.4x3.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP127_0_1")
		(symbol "TLP127_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin open_collector line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP130"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 4.826 0)
		)
		(property "Value" "TLP130"
			(at -5.08 -5.08 0)
		)
		(property "Footprint" "Package_SO:MFSOP6-5_4.4x3.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=16740&prodName=TLP130"
			(at 0.254 0 0)
		)
		(property "Description" "AC DC Optocoupler Base Connected, Vce 80V, CTR 50-100%, MFSOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MFSOP6*4.4x3.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP130_0_1")
		(symbol "TLP130_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP131"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.207 4.826 0)
		)
		(property "Value" "TLP131"
			(at -5.08 -5.08 0)
		)
		(property "Footprint" "Package_SO:MFSOP6-5_4.4x3.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=16742&prodName=TLP131"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 80V, CTR 50-200%, MFSOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MFSOP6*4.4x3.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP131_0_1")
		(symbol "TLP131_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP137"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 4.953 0)
		)
		(property "Value" "TLP137"
			(at -5.08 -5.08 0)
		)
		(property "Footprint" "Package_SO:MFSOP6-5_4.4x3.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=16744&prodName=TLP137"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 80V, CTR 100-200%, MFSOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MFSOP6*4.4x3.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP137_0_1")
		(symbol "TLP137_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin open_collector line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP184"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP184"
			(at -5.08 -5.08 0)
		)
		(property "Footprint" "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=11793&prodName=TLP184"
			(at 1.27 0 0)
		)
		(property "Description" "AC/DC Optocoupler, Vce 80V, CTR 50-100%, MFSOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MFSOP6*4.4x3.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP184_0_1")
		(symbol "TLP184_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP185"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP185"
			(at -5.08 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-4_4.55x3.7mm_P2.54mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=11791&prodName=TLP185"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 80V, CTR 50-100%, MFSOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*4.55x3.7mm*P2.54mm*"
			(at 0 0 0)
		)
		(symbol "TLP185_0_1")
		(symbol "TLP185_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP2310"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.112 8.89 0)
		)
		(property "Value" "TLP2310"
			(at 1.016 9.144 0)
		)
		(property "Footprint" "Package_SO:SO-5-6_4.55x3.7mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/TLP2310_datasheet_en_20220913.pdf?did=29657&prodName=TLP2310"
			(at 0 0 0)
		)
		(property "Description" "5-Mbps low-power non inverting photocouple, 3.75 kVrms, 2.7 - 5.5 Vdd, push-pull output"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler high-speed Toshiba"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*4.55x3.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP2310_0_1")
		(symbol "TLP2310_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP2703"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.4676 8.9408 0)
		)
		(property "Value" "TLP2703"
			(at 0.9652 8.9916 0)
		)
		(property "Footprint" "Package_SO:SO-6L_10x3.84mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=15216&prodName=TLP2703"
			(at 0 0 0)
		)
		(property "Description" "100 kbps, High-speed GaA&As, high-gain, 4.5 - 18 VCC, 5 kVrms, CTR 900%, SO-6L"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Darlington DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*6L*10x3.84mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP2703_0_1")
		(symbol "TLP2703_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 0 180)
				(length 2.54)
				(name "Out")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP2745"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.112 8.89 0)
		)
		(property "Value" "TLP2745"
			(at 1.016 9.144 0)
		)
		(property "Footprint" "Package_SO:SO-6L_10x3.84mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=29405&prodName=TLP2745"
			(at 0 0 0)
		)
		(property "Description" "10-Mbps low-power non inverting photocouple,5 kVrms, 4.5 - 30 Vdd, push-pull output"
			(at 0 0 0)
		)
		(property "ki_keywords" "Photocouple highspeed non inverting push-pull output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*6L*10x3.84mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP2745_0_1")
		(symbol "TLP2745_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP2748"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.112 8.89 0)
		)
		(property "Value" "TLP2748"
			(at 1.016 9.144 0)
		)
		(property "Footprint" "Package_SO:SO-6L_10x3.84mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=29407&prodName=TLP2748"
			(at 0 0 0)
		)
		(property "Description" "10-Mbps inverting photocouple,5 kVrms, 4.5 - 30 Vdd, push-pull output, SO-6L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Photocouple highspeed inverting push-pull output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*6L*10x3.84mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP2748_0_1")
		(symbol "TLP2748_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "VO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP2768A"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.112 8.89 0)
		)
		(property "Value" "TLP2768A"
			(at 1.016 9.144 0)
		)
		(property "Footprint" "Package_SO:SO-6L_10x3.84mm_P1.27mm"
			(at -17.78 -12.7 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=36717&prodName=TLP2768A"
			(at -3.7592 0 0)
		)
		(property "Description" "20-Mbps high speed inverting photocouple,5 kVrms, 2.7 - 5.5 Vdd, open collector, SO-6L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Photocouple highspeed inverting open collector output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*6L*10x3.84mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP2768A_0_1")
		(symbol "TLP2768A_1_1"
			(pin passive line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "K")
				(number "3")
			)
			(pin no_connect line
				(at -7.62 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin open_collector line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "VO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP290"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP290"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at -21.59 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=12882&prodName=TLP290"
			(at 0.635 0 0)
		)
		(property "Description" "AC/DC Phototransistor Optocoupler, Vce 80V, CTR 50-600%, not recommended for new designs, SOP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Phototransistor Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP290_0_1")
		(symbol "TLP290_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP290-4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP290-4"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-16_4.55x10.3mm_P1.27mm"
			(at -21.59 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=12855&prodName=TLP290-4"
			(at 0.635 0 0)
		)
		(property "Description" "Quad AC/DC Phototransistor Optocoupler, Vce 80V, CTR 50-600%, SOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Quad Phototransistor Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.55x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP290-4_0_1")
		(symbol "TLP290-4_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "TLP290-4_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "TLP290-4_3_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "TLP290-4_4_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP291"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP291"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-4_4.55x2.6mm_P1.27mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=12884&prodName=TLP291"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 80V, CTR 50-100%, SOP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*4.55x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP291_0_1")
		(symbol "TLP291_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP291-4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP291-4"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_4.55x10.3mm_P1.27mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=12858&prodName=TLP291-4"
			(at 0 0 0)
		)
		(property "Description" "Quad DC Optocoupler, Vce 80V, CTR 50-100%, SOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Quad Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*4.55x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TLP291-4_0_1")
		(symbol "TLP291-4_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "TLP291-4_2_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "TLP291-4_3_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "TLP291-4_4_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP3021"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP3021"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:Toshiba_11-7A9"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=1421&prodName=TLP3021(S)"
			(at -0.635 0 0)
		)
		(property "Description" "Photo-Triac, Vdrm 400V, Ift 15mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Photo-Triac Opto Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Toshiba*11?7A9*"
			(at 0 0 0)
		)
		(symbol "TLP3021_0_1")
		(symbol "TLP3021_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP627"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 5.08 0)
		)
		(property "Value" "TLP627"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -7.62 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=16914&prodName=TLP627"
			(at 0 0 0)
		)
		(property "Description" "DC Darlington Optocoupler, Vce 300V, CTR 1000%, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Darlington DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TLP627_0_1")
		(symbol "TLP627_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP627-2"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 5.08 0)
		)
		(property "Value" "TLP627-2"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -7.62 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=16914&prodName=TLP627"
			(at 0 0 0)
		)
		(property "Description" "DC Dual Darlington Optocoupler, Vce 300V, CTR 1000%, DIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Dual Darlington DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TLP627-2_0_1")
		(symbol "TLP627-2_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "7")
			)
		)
		(symbol "TLP627-2_2_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP627-4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 5.08 0)
		)
		(property "Value" "TLP627-4"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at -7.62 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=16914&prodName=TLP627"
			(at 0 0 0)
		)
		(property "Description" "DC Quad Darlington Optocoupler, Vce 300V, CTR 1000%, DIP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN Quad Darlington DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TLP627-4_0_1")
		(symbol "TLP627-4_1_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "16")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "15")
			)
		)
		(symbol "TLP627-4_2_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "14")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "13")
			)
		)
		(symbol "TLP627-4_3_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "5")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "12")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "11")
			)
		)
		(symbol "TLP627-4_4_1"
			(pin passive line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "~")
				(number "7")
			)
			(pin passive line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "~")
				(number "8")
			)
			(pin passive line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "~")
				(number "10")
			)
			(pin passive line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "~")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP785"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP785"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=10569&prodName=TLP785"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 80V, CTR 50-200%, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "TLP785_0_1")
		(symbol "TLP785_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TLP785F"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP785F"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=10569&prodName=TLP785F"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 80V, CTR 50-200%, DIP4F"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
		(symbol "TLP785F_0_1")
		(symbol "TLP785F_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VO615A"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "VO615A"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81753/vo615a.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 70V, CTR 50-600% @ 5mA, Viso 5000Vrms, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W7.62mm* SMDIP*W9.53mm* SMDIP*W11.48mm*"
			(at 0 0 0)
		)
		(symbol "VO615A_0_1")
		(symbol "VO615A_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VOA300"
		(pin_names
			(offset 0)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -3.81 11.43 0)
		)
		(property "Value" "VOA300"
			(at 0 -11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "https://mouser.com/pdfDocs/Vishay_VOA300_DS.pdf"
			(at -21.59 15.24 0)
		)
		(property "Description" "Linear Optocoupler, High Gain Stability, 5300VRMS isolation, 200 kHz Bandwidth, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "optically coupled gates automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "VOA300_0_1")
		(symbol "VOA300_1_1"
			(pin passive line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "C")
				(number "1")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin open_collector line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "C")
				(number "3")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin open_collector line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "C")
				(number "6")
			)
			(pin passive line
				(at 7.62 -7.62 180)
				(length 2.54)
				(name "A")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VTL5C"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "VTL5C"
			(at 0 -5.08 0)
		)
		(property "Footprint" "OptoDevice:PerkinElmer_VTL5C"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.qsl.net/wa1ion/vactrol/vactrol.pdf"
			(at 1.27 -6.35 0)
		)
		(property "Description" "Low Cost Axial Vactrols"
			(at 0 0 0)
		)
		(property "ki_keywords" "vactrol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PerkinElmer*VTL5C*"
			(at 0 0 0)
		)
		(symbol "VTL5C_0_1")
		(symbol "VTL5C_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VTL5Cx2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "VTL5Cx2"
			(at 0 -5.08 0)
		)
		(property "Footprint" "OptoDevice:PerkinElmer_VTL5Cx2"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.alliedelec.com/m/d/ecb1ed91959ae54d97cf67f5103d9b2b.pdf"
			(at 1.27 -6.35 0)
		)
		(property "Description" "Dual Element Axial Vactrols"
			(at 0 0 0)
		)
		(property "ki_keywords" "vactrol"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PerkinElmer*VTL5C*"
			(at 0 0 0)
		)
		(symbol "VTL5Cx2_0_1")
		(symbol "VTL5Cx2_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "-")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "+")
				(number "2")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "4N26"
		(extends "4N25")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "4N26"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83725/4n25.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 30V, CTR 20%, Viso 1500V, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "4N27"
		(extends "4N25")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "4N27"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83725/4n25.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 30V, CTR 10%, Viso 2500V, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "4N28"
		(extends "4N25")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "4N28"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83725/4n25.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 30V, CTR 10%, Viso 2500V, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "4N35"
		(extends "4N25")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "4N35"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/81181/4n35.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, with Base Connection, Vce 70V, CTR 100%, Viso 5000V, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "4N36"
		(extends "4N25")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "4N36"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/81181/4n35.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, with Base Connection, Vce 70V, CTR 100%, Viso 5000V, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "4N37"
		(extends "4N25")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "4N37"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/81181/4n35.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, with Base Connection, Vce 70V, CTR 100%, Viso 5000V, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "6N136"
		(extends "6N135")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "6N136"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -5.08 -7.62 0)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS70-2008-0032/6N135-L%206N136-L%20series.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Speed Optocoupler, TTL Compatible, CTR 24%, DIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Speed Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "6N136S"
		(extends "6N135S")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "6N136S"
			(at 0 7.62 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-8_W9.53mm"
			(at -5.08 -7.62 0)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS70-2008-0032/6N135-L%206N136-L%20series.pdf"
			(at 0 0 0)
		)
		(property "Description" "High Speed Optocoupler, TTL Compatible, CTR 18%, SMDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Speed Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm*"
			(at 0 0 0)
		)
	)
	(symbol "6N137"
		(extends "HCPL-261A")
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "6N137"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0940EN"
			(at -21.59 13.97 0)
		)
		(property "Description" "Single High Speed LSTTL/TTL Compatible Optocoupler with enable, dV/dt 1000/us, VCM 10, max 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "6N139"
		(extends "6N138")
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "6N139"
			(at 2.286 8.89 0)
		)
		(property "Footprint" ""
			(at 7.366 -7.62 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/HCPL2731-D.pdf"
			(at 7.366 -7.62 0)
		)
		(property "Description" "Low Input Current high Gain Split Darlington Optocouplers, -0.5V to 18V VDD, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACPL-214-500E"
		(extends "TLP290")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "ACPL-214-500E"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at -21.59 -5.08 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/doc/AV02-0469EN"
			(at 0.635 0 0)
		)
		(property "Description" "AC/DC Phototransistor Optocoupler, Vce 80V, CTR 20-400%, SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "npn ac dc ac-dc acdc phototransistor optocoupler optoisolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM1200BR"
		(extends "ADuM1200AR")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1200BR"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/ADuM1200_1201.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Dual-Channel Digital Isolator, 10Mbps 50ns, bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 10Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM1200CR"
		(extends "ADuM1200AR")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1200CR"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/ADuM1200_1201.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Dual-Channel Digital Isolator, 25Mbps 45ns, bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM1200WS"
		(extends "ADuM1200AR")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1200WS"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/ADuM1200_1201.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Dual-Channel Digital Isolator, 1Mbps 150ns, Highest Tem. Grade, bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 1Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM1200WT"
		(extends "ADuM1200AR")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1200WT"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/ADuM1200_1201.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Dual-Channel Digital Isolator, 10Mbps 50ns, Highest Tem. Grade, bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 10Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM1200WU"
		(extends "ADuM1200AR")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1200WU"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/ADuM1200_1201.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Dual-Channel Digital Isolator, 25Mbps 45ns, Highest Tem. Grade, bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM1201BR"
		(extends "ADuM1201AR")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1201BR"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/ADuM1200_1201.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Dual-Channel Digital Isolator, 10Mbps 50ns, bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 10Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM1201CR"
		(extends "ADuM1201AR")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1201CR"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/ADuM1200_1201.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Dual-Channel Digital Isolator, 25Mbps 45ns, bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM1201WS"
		(extends "ADuM1201AR")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1201WS"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/ADuM1200_1201.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Dual-Channel Digital Isolator, 1Mbps 150ns, Highest Temp. Grade, bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 1Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM1201WT"
		(extends "ADuM1201AR")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1201WT"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/ADuM1200_1201.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Dual-Channel Digital Isolator, 10Mbps 50ns, Hihgest Temp. Grade, bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 10Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM1201WU"
		(extends "ADuM1201AR")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1201WU"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/static/imported-files/data_sheets/ADuM1200_1201.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Dual-Channel Digital Isolator, 25Mbps 45ns, Highest Temp. Grade, bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM1281"
		(extends "ADuM1201AR")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "ADuM1281"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM1280_1281_1285_1286.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Dual-channel digital isolator, bidirectional communication, 3V/5V level translation, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM7640A"
		(extends "ADuM7640C")
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "ADuM7640A"
			(at -1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:QSOP-20_3.9x8.7mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM7640_7641_7642_7643.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Low Power Six-Channel 6/0 Digital Isolator, 1Mbps 25ns, Fail-Safe High, QSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "6-Channels Hex Digital Isolator 1Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM7641A"
		(extends "ADuM7641C")
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "ADuM7641A"
			(at -1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:QSOP-20_3.9x8.7mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM7640_7641_7642_7643.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Low Power Six-Channel 5/1 Digital Isolator, 1Mbps 25ns, Fail-Safe High, QSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "6-Channels Hex Digital Isolator 1Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM7642A"
		(extends "ADuM7642C")
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "ADuM7642A"
			(at -1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:QSOP-20_3.9x8.7mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM7640_7641_7642_7643.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Low Power Six-Channel 4/2 Digital Isolator, 1Mbps 25ns, Fail-Safe High, QSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "6-Channels Hex Digital Isolator 1Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ADuM7643A"
		(extends "ADuM7643C")
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "ADuM7643A"
			(at -1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:QSOP-20_3.9x8.7mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADuM7640_7641_7642_7643.pdf"
			(at 0 12.7 0)
		)
		(property "Description" "Low Power Six-Channel 3/3 Digital Isolator, 1Mbps 25ns, Fail-Safe High, QSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "6-Channels Hex Digital Isolator 1Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x8.7mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "CNY17-2"
		(extends "CNY17-1")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "CNY17-2"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 63-125%, Viso 5000V (RMS), DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*"
			(at 0 0 0)
		)
	)
	(symbol "CNY17-3"
		(extends "CNY17-1")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "CNY17-3"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 100-200%, Viso 5000V (RMS), DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*"
			(at 0 0 0)
		)
	)
	(symbol "CNY17-4"
		(extends "CNY17-1")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "CNY17-4"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83606/cny17.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler Base Connected, Vce 70V, CTR 160-320%, Viso 5000V (RMS), DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*"
			(at 0 0 0)
		)
	)
	(symbol "CPC-5002"
		(extends "HCPL-263A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "CPC-5002"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -18.288 0)
		)
		(property "Datasheet" "http://www.ixysic.com/home/pdfs.nsf/www/CPC5002.pdf"
			(at -10.16 8.89 0)
		)
		(property "Description" "Dual High Speed CMOS Compatible Optocoupler, dV/dt 5000/us, VCM 20, -0.3V to 6.5V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "EL817"
		(extends "PC817")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "EL817"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.everlight.com/file/ProductFile/EL817.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 35V, DIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "FODM214A"
		(extends "FODM214")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FODM214A"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FODM214-D.PDF"
			(at 0.635 0 0)
		)
		(property "Description" "AC/DC Optocoupler, Vce 80V, CTR 50-250%, SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "AC DC Phototransistor Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FODM217B"
		(extends "FODM217A")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FODM217B"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FODM214-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 80V, CTR 130-260%, SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC Phototransistor Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FODM217C"
		(extends "FODM217A")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FODM217C"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FODM214-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 80V, CTR 200-400%, SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC Phototransistor Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "FODM217D"
		(extends "FODM217A")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "FODM217D"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -5.08 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/FODM214-D.PDF"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 80V, CTR 300-600%, SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "DC Phototransistor Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "H11L2"
		(extends "H11L1")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "H11L2"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -2.286 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/H11L3M-D.PDF"
			(at -2.286 0 0)
		)
		(property "Description" "Schmitt Trigger Output Optocoupler, High Speed, DIP-6, 10mA turn on threshold"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Speed Schmitt Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*"
			(at 0 0 0)
		)
	)
	(symbol "H11L3"
		(extends "H11L1")
		(property "Reference" "U"
			(at 1.27 8.89 0)
		)
		(property "Value" "H11L3"
			(at 1.27 6.35 0)
		)
		(property "Footprint" ""
			(at -2.286 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/H11L3M-D.PDF"
			(at -2.286 0 0)
		)
		(property "Description" "Schmitt Trigger Output Optocoupler, High Speed, DIP-6, 5mA turn on threshold"
			(at 0 0 0)
		)
		(property "ki_keywords" "High Speed Schmitt Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W9.53mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCNW2211"
		(extends "HCNW2201")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "HCNW2211"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W10.16mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0674EN"
			(at 0 0 0)
		)
		(property "Description" "Opto Coupler, 10kV/us, 1kV CMR, Schmitt trigger output, WDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto coupler schmitt output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-0211"
		(extends "HCPL-0201")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "HCPL-0211"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0674EN"
			(at 0.254 0 0)
		)
		(property "Description" "Opto Coupler, 5kV/us, 300V CMR, Schmitt trigger output, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto coupler schmitt output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-0600"
		(extends "HCPL-061A")
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "HCPL-0600"
			(at 0.254 -9.144 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0940EN"
			(at -21.59 15.24 0)
		)
		(property "Description" "Single High Speed LSTTL/TTL Compatible Optocoupler with enable, dV/dt 5000/us, VCM 1000, max 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-0601"
		(extends "HCPL-061A")
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "HCPL-0601"
			(at 0.254 -9.144 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0940EN"
			(at -21.59 15.24 0)
		)
		(property "Description" "Single High Speed LSTTL/TTL Compatible Optocoupler with enable, dV/dt 10000/us, VCM 1000, max 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-0611"
		(extends "HCPL-061A")
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "HCPL-0611"
			(at 0.254 -9.144 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0940EN"
			(at -21.59 15.24 0)
		)
		(property "Description" "Single High Speed LSTTL/TTL Compatible Optocoupler with enable, dV/dt 15000/us, VCM 1000, max 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-061N"
		(extends "HCPL-061A")
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "HCPL-061N"
			(at 0.254 -9.144 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://docs.avagotech.com/docs/AV02-0391EN"
			(at -21.59 15.24 0)
		)
		(property "Description" "Single High Speed HCMOS/LSTTL/TTL Compatible Optocoupler with enable, dV/dt 1000/us, VCM 1000, -0.5V to 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-0630"
		(extends "HCPL-063A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "HCPL-0630"
			(at 7.874 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0940EN"
			(at -21.59 15.24 0)
		)
		(property "Description" "Dual High Speed LSTTL/TTL Compatible Optocoupler, dV/dt 5000/us, VCM 1000, max 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-0631"
		(extends "HCPL-063A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "HCPL-0631"
			(at 7.874 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0940EN"
			(at -21.59 15.24 0)
		)
		(property "Description" "Dual High Speed LSTTL/TTL Compatible Optocoupler, dV/dt 10000/us, VCM 1000, max 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-063N"
		(extends "HCPL-063A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "HCPL-063N"
			(at 7.874 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://docs.avagotech.com/docs/AV02-0391EN"
			(at -21.59 15.24 0)
		)
		(property "Description" "Dual High Speed HCMOS/LSTTL/TTL Compatible Optocoupler, dV/dt 1000/us, VCM 1000, -0.5V to 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-0661"
		(extends "HCPL-063A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "HCPL-0661"
			(at 7.874 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0940EN"
			(at -21.59 15.24 0)
		)
		(property "Description" "Dual High Speed LSTTL/TTL Compatible Optocoupler, dV/dt 15000/us, VCM 1000, max 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-2211"
		(extends "HCPL-2201")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "HCPL-2211"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0674EN"
			(at 0 0 0)
		)
		(property "Description" "Opto Coupler, 5kV/us, 300V CMR, Schmitt trigger output, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto coupler schmitt output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-2212"
		(extends "HCPL-2202")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "HCPL-2212"
			(at 6.35 6.35 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0674EN"
			(at 0 0 0)
		)
		(property "Description" "Opto Coupler, 5kV/us, 300V CMR, Schmitt trigger output, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto coupler schmitt output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-2611"
		(extends "HCPL-2601")
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "HCPL-2611"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 17.78 0 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/doc/6N137-HCNW137-2601-2611-HCPL-0600-0601-0611-0630-0631-0661-2601-2611-2630-2631-4661-High-CMR-High-Speed-TTL-Compatible-Optocouplers-DS"
			(at 17.78 2.54 0)
		)
		(property "Description" "Single High Speed LSTTL/TTL Compatible Optocoupler with enable, dV/dt 15000V/us, VCM 1000, max 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-261N"
		(extends "HCPL-261A")
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "HCPL-261N"
			(at 6.35 8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/doc/AV02-0391EN"
			(at -21.59 13.97 0)
		)
		(property "Description" "Single High Speed HCMOS/LSTTL/TTL Compatible Optocoupler with enable, dV/dt 1000/us, VCM 1000, -0.5V to 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-2630"
		(extends "HCPL-263A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "HCPL-2630"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -18.288 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0940EN"
			(at -10.16 8.89 0)
		)
		(property "Description" "Dual High Speed LSTTL/TTL Compatible Optocoupler, dV/dt 5000/us, VCM 1000, max 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-2631"
		(extends "HCPL-263A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "HCPL-2631"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -18.288 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0940EN"
			(at -10.16 8.89 0)
		)
		(property "Description" "Dual High Speed LSTTL/TTL Compatible Optocoupler, dV/dt 10000/us, VCM 1000, max 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-263N"
		(extends "HCPL-263A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "HCPL-263N"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -18.288 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/doc/AV02-0391EN"
			(at -10.16 8.89 0)
		)
		(property "Description" "Dual High Speed HCMOS/LSTTL/TTL Compatible Optocoupler, dV/dt 1000/us, VCM 1000, -0.5V to 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL-4661"
		(extends "HCPL-263A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "HCPL-4661"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -18.288 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-0940EN"
			(at -10.16 8.89 0)
		)
		(property "Description" "Dual High Speed LSTTL/TTL Compatible Optocoupler, dV/dt 15000/us, VCM 1000, max 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "HCPL2730"
		(extends "HCPL2731")
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "HCPL2730"
			(at -5.08 -10.16 0)
		)
		(property "Footprint" ""
			(at -0.635 0 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/HCPL2731-D.pdf"
			(at -0.635 0 0)
		)
		(property "Description" "Low Input Current high Gain Split Darlington Optocouplers"
			(at 0 0 0)
		)
		(property "ki_keywords" "darlington optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SMDIP*W9.53mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7320FC"
		(extends "ISO7320C")
		(property "Reference" "U"
			(at 0 10.795 0)
		)
		(property "Value" "ISO7320FC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7320fc&fileType=pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power Dual-Channel 2/0 Digital Isolator, 25Mbps 33ns, Fail-Safe Low, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7321FC"
		(extends "ISO7321C")
		(property "Reference" "U"
			(at 0 10.795 0)
		)
		(property "Value" "ISO7321FC"
			(at 0 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7321fc&fileType=pdf"
			(at 0 0 0)
		)
		(property "Description" "Low Power Dual-Channel 1/1 Digital Isolator, 25Mbps 33ns, Fail-Safe Low, SO8"
			(at 0 0 0)
		)
		(property "ki_keywords" "2Ch Dual Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7330FC"
		(extends "ISO7330C")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "ISO7330FC"
			(at 8.382 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/iso7330-q1.pdf"
			(at 0 7.62 0)
		)
		(property "Description" "Low Power Quad-Channel 3/0 Digital Isolator, 25Mbps 31ns, Fail-Safe Low, SO16"
			(at 0 0 0)
		)
		(property "ki_keywords" "3Ch Quad Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7331FC"
		(extends "ISO7331C")
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "ISO7331FC"
			(at 6.858 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7341c&fileType=pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low Power Quad-Channel 2/1 Digital Isolator, 25Mbps 31ns, Fail-Safe Low, SO16"
			(at 0 0 0)
		)
		(property "ki_keywords" "3Ch Quad Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7340FC"
		(extends "ISO7340C")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ISO7340FC"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7340fc&fileType=pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low Power Quad-Channel 4/0 Digital Isolator, 25Mbps 31ns, Fail-Safe Low, SO16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch Quad Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7341FC"
		(extends "ISO7341C")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ISO7341FC"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7341fc&fileType=pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low Power Quad-Channel 3/1 Digital Isolator, 25Mbps 31ns, Fail-Safe Low, SO16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch Quad Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7342FC"
		(extends "ISO7342C")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "ISO7342FC"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/general/docs/lit/getliterature.tsp?genericPartNumber=iso7342fc&fileType=pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low Power Quad-Channel 2/2 Digital Isolator, 25Mbps 31ns, Fail-Safe Low, SO16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch Quad Digital Isolator 25Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7760FDBQ"
		(extends "ISO7760DBQ")
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7760FDBQ"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf?ts=1596905577895"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default low, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7760FDW"
		(extends "ISO7760DW")
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7760FDW"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf?ts=1596905577895"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default low, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7761FDBQ"
		(extends "ISO7761DBQ")
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7761FDBQ"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf?ts=1596905577895"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default low, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7761FDW"
		(extends "ISO7761DW")
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7761FDW"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf?ts=1596905577895"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default low, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7762FDBQ"
		(extends "ISO7762DBQ")
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7762FDBQ"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf?ts=1596905577895"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default low, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7762FDW"
		(extends "ISO7762DW")
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7762FDW"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf?ts=1596905577895"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default low, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7763FDBQ"
		(extends "ISO7763DBQ")
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7763FDBQ"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SSOP-16_3.9x4.9mm_P0.635mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf?ts=1596905577895"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default low, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "ISO7763FDW"
		(extends "ISO7763DW")
		(property "Reference" "U"
			(at 8.255 14.605 0)
		)
		(property "Value" "ISO7763FDW"
			(at 8.255 12.065 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 5.715 -13.97 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/iso7763.pdf?ts=1596905577895"
			(at 10.16 -2.54 0)
		)
		(property "Description" "Default low, High-speed, robust EMC, reinforced, six-channel, digital, isolator, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTV-357T"
		(extends "LTV-356T")
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "LTV-357T"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SO-4_4.4x3.6mm_P2.54mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.buerklin.com/medias/sys_master/download/download/h91/ha0/8892020588574.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 35V, CTR 50%, SO-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*4.4x3.6mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTV-358T"
		(extends "LTV-356T")
		(property "Reference" "U"
			(at -5.334 4.826 0)
		)
		(property "Value" "LTV-358T"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SO-4_4.4x3.6mm_P2.54mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS70-2001-022/S_110_LTV-358T%2020140520.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 120V, CTR 50%, SO-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*4.4x3.6mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTV-827"
		(extends "PC827")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "LTV-827"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS-70-96-0016/LTV-8X7%20series%20201610%20.pdf"
			(at 0 0 0)
		)
		(property "Description" "Dual DC Optocoupler, Vce 35V, CTR 50%, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Dual Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LTV-847"
		(extends "PC847")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "LTV-847"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://optoelectronics.liteon.com/upload/download/DS-70-96-0016/LTV-8X7%20series.PDF"
			(at 0 0 0)
		)
		(property "Description" "Quad DC Optocoupler, Vce 35V, CTR 50%, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Quad Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MAX14850ASE+"
		(extends "MAX14850AEE+")
		(property "Reference" "U"
			(at -9.525 16.51 0)
		)
		(property "Value" "MAX14850ASE+"
			(at 13.335 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 1.27 0)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX14850.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Six-channel digital isolator, bidirectional, 3V3, 5V, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6 channel digital isolator bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOCD208M"
		(extends "MOCD207M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOCD208M"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -21.082 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mocd217m-d.pdf"
			(at -34.29 0 0)
		)
		(property "Description" "8-pin SOIC Dual-Channel Phototransistor Output Optocoupler, VCEO 70V, VF 1.25-1.5V (IF 30mA), CTR 40-125%, SOIC8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Dual Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9*4.9*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOCD211M"
		(extends "MOCD207M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOCD211M"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -21.082 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mocd217m-d.pdf"
			(at -34.29 0 0)
		)
		(property "Description" "8-pin SOIC Dual-Channel Phototransistor Output Optocoupler, VCEO 30V, VF 1.25-1.5V (IF 30mA), CTR 20%, SOIC8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Dual Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9*4.9*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOCD213M"
		(extends "MOCD207M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOCD213M"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -21.082 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mocd217m-d.pdf"
			(at -34.29 0 0)
		)
		(property "Description" "8-pin SOIC Dual-Channel Phototransistor Output Optocoupler, VCEO 70V, VF 1.15-1.5V (IF 10mA), CTR 100%, SOIC8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Dual Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9*4.9*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MOCD217M"
		(extends "MOCD207M")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "MOCD217M"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at -21.082 0 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/mocd217m-d.pdf"
			(at -34.29 0 0)
		)
		(property "Description" "8-pin SOIC Dual-Channel Phototransistor Output Optocoupler, VCEO 30V, VF 1.05-1.3V (IF 1mA), CTR 100%, SOIC8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Dual Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9*4.9*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PC3H4A"
		(extends "PC3H4")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "PC3H4A"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.sharpsma.com/webfm_send/395"
			(at 0.635 0 0)
		)
		(property "Description" "AC/DC Optocoupler, Vce 70V, CTR 100-250%, SOP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-1"
		(extends "TLP785")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-1"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80, -55 to +110 degree Celsius, UL, BSI, FIMKO, cUL, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-1X001"
		(extends "TLP785")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-1X001"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80, -55 to +110 degree Celsius, VDE, UL, BSI, FIMKO, cUL, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-1X006"
		(extends "TLP785F")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-1X006"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80, -55 to +110 degree Celsius, UL, BSI, FIMKO, cUL, wide THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-1X016"
		(extends "TLP785F")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-1X016"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80, -55 to +110 degree Celsius, VDE, UL, BSI, FIMKO, cUL, wide THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-2"
		(extends "TLP785")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-2"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125, -55 to +110 degree Celsius, UL, BSI, FIMKO, cUL, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-2X001"
		(extends "TLP785")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-2X001"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125, -55 to +110 degree Celsius, VDE, UL, BSI, FIMKO, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-2X006"
		(extends "TLP785F")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-2X006"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125, -55 to +110 degree Celsius, UL, BSI, FIMKO, cUL, wide THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-2X016"
		(extends "TLP785F")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-2X016"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125, -55 to +110 degree Celsius, VDE, UL, BSI, FIMKO, wide THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-2X017T"
		(extends "SFH617A-1X007T")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "SFH617A-2X017T"
			(at -5.08 -6.35 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125, -55 to +110 degree Celsius, VDE, UL, BSI, FIMKO, 8mm clearence SMD PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm*Clearance8mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-2X019T"
		(extends "SFH617A-2X009T")
		(property "Reference" "U"
			(at -3.81 5.08 0)
		)
		(property "Value" "SFH617A-2X019T"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W7.62mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at -8.89 7.62 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125, -55 to +110 degree Celsius, VDE, UL, BSI, FIMKO, SMD PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-125"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-3"
		(extends "TLP785")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-3"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-200, -55 to +110 degree Celsius, UL, BSI, FIMKO, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-3X001"
		(extends "TLP785")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-3X001"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-200, -55 to +110 degree Celsius, VDE, UL, BSI, FIMKO, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-3X006"
		(extends "TLP785F")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-3X006"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-200, -55 to +110 degree Celsius, VDE, UL, BSI, FIMKO, wide THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-3X007T"
		(extends "SFH617A-1X007T")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "SFH617A-3X007T"
			(at -5.08 -6.35 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80, -55 to +110 degree Celsius, UL, BSI, FIMKO, cUL, 8mm clearence SMD PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-80"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm*Clearance8mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-3X016"
		(extends "TLP785F")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-3X016"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-200, -55 to +110 degree Celsius, VDE, UL, BSI, FIMKO, wide THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-3X017T"
		(extends "SFH617A-1X007T")
		(property "Reference" "U"
			(at -5.08 6.35 0)
		)
		(property "Value" "SFH617A-3X017T"
			(at -5.08 -6.35 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-200, -55 to +110 degree Celsius, VDE, UL, BSI, FIMKO, 8mm clearence SMD PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm*Clearance8mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-4"
		(extends "TLP785")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-4"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 160-320, -55 to +110 degree Celsius, UL, BSI, FIMKO, cUL, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 160-320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-4X001"
		(extends "TLP785")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-4X001"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 160-320, -55 to +110 degree Celsius, VDE, UL, BSI, FIMKO, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 160-320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-4X006"
		(extends "TLP785F")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-4X006"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 160-320, -55 to +110 degree Celsius, UL, BSI, FIMKO, cUL, wide THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 160-320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH617A-4X016"
		(extends "TLP785F")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "SFH617A-4X016"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83740/sfh617a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 160-320, -55 to +110 degree Celsius, VDE, UL, BSI, FIMKO, wide THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 160-320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH6206-1T"
		(extends "SFH620A-2X007T")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH6206-1T"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-125, UL, cUL, BSI, SMD-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-125"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm?Clearance8mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH6206-2T"
		(extends "SFH620A-2X007T")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH6206-2T"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200, UL, cUL, BSI, SMD-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm?Clearance8mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH6206-2X001T"
		(extends "SFH620A-2X007T")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH6206-2X001T"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200, VDE, UL, CUL, BSI, SMD-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm?Clearance8mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH6206-3T"
		(extends "SFH620A-2X007T")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH6206-3T"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-320, UL, cUL, BSI, SMD-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm?Clearance8mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH6206-3X001T"
		(extends "SFH620A-2X007T")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH6206-3X001T"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-320, VDE, UL, CUL, BSI, SMD-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm?Clearance8mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH620A-1X001"
		(extends "SFH620A-1")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH620A-1X001"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-125 VDE, UL, CUL, BSI, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 40-125"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH620A-2"
		(extends "SFH620A-1")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH620A-2"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200 UL, cUL, BSI, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH620A-2X001"
		(extends "SFH620A-1")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH620A-2X001"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200 VDE, UL, CUL, BSI, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH620A-2X006"
		(extends "SFH620A-1X006")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH620A-2X006"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200 UL, cUL, BSI, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH620A-2X016"
		(extends "SFH620A-1X006")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH620A-2X016"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200 VDE, UL, CUL, BSI, SMD-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH620A-2X017T"
		(extends "SFH620A-2X007T")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH620A-2X017T"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:SMDIP-4_W9.53mm_Clearance8mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200 VDE, UL, CUL, BSI, SMD-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 63-200"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SMDIP*W9.53mm?Clearance8mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH620A-3"
		(extends "SFH620A-1")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH620A-3"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-320 UL, cUL, BSI, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH620A-3X001"
		(extends "SFH620A-1")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH620A-3X001"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W7.62mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-320 VDE, UL, CUL, BSI, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH620A-3X006"
		(extends "SFH620A-1X006")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH620A-3X006"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-320 UL, cUL, BSI, THT PDIP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH620A-3X016"
		(extends "SFH620A-1X006")
		(property "Reference" "U"
			(at -4.064 6.35 0)
		)
		(property "Value" "SFH620A-3X016"
			(at -5.334 -6.604 0)
		)
		(property "Footprint" "Package_DIP:DIP-4_W10.16mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83675/sfh620a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-320 VDE, UL, CUL, BSI, SMD-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optocoupler, Phototransistor Output, 5300 VRMS, VCEO 70V, CTR% 100-320"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W10.16mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8640BB-B-IU"
		(extends "Si8640BA-B-IU")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8640BB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8640BC-B-IS1"
		(extends "Si8640BB-B-IS1")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8640BC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8640BD-B-IS"
		(extends "Si8640BB-B-IS")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8640BD-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5.0kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8640BD-B-IS2"
		(extends "Si8640BB-B-IS")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8640BD-B-IS2"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5.0kV isolation, Fail-Safe Low, 8mm creepage, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8640EB-B-IU"
		(extends "Si8640BA-B-IU")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8640EB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe High, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8640EC-B-IS1"
		(extends "Si8640BB-B-IS1")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8640EC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe High, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8640ED-B-IS"
		(extends "Si8640BB-B-IS")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8640ED-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5.0kV isolation, Fail-Safe High, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8640ED-B-IS2"
		(extends "Si8640BB-B-IS")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8640ED-B-IS2"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5.0kV isolation, Fail-Safe High, 8mm creepage, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8641BB-B-IU"
		(extends "Si8641BA-B-IU")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8641BB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 3In 1Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8641BC-B-IS1"
		(extends "Si8641BB-B-IS1")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8641BC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 3In 1Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8641BD-B-IS"
		(extends "Si8641BB-B-IS")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8641BD-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5.0kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 3In 1Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8641BD-B-IS2"
		(extends "Si8641BB-B-IS")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8641BD-B-IS2"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5.0kV isolation, Fail-Safe Low, 8mm creepage, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 3In 1Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8641EB-B-IU"
		(extends "Si8641BA-B-IU")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8641EB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe High, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 3In 1Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8641EC-B-IS1"
		(extends "Si8641BB-B-IS1")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8641EC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe High, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 3In 1Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8641ED-B-IS"
		(extends "Si8641BB-B-IS")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8641ED-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5.0kV isolation, Fail-Safe High, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 3In 1Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8641ED-B-IS2"
		(extends "Si8641BB-B-IS")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8641ED-B-IS2"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5.0kV isolation, Fail-Safe High, 8mm creepage, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 3In 1Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8642BB-B-IU"
		(extends "Si8642BA-B-IU")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8642BB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 2In 2Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8642BC-B-IS1"
		(extends "Si8642BB-B-IS1")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8642BC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 2In 2Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8642BD-B-IS"
		(extends "Si8642BB-B-IS")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8642BD-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5.0kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 2In 2Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8642BD-B-IS2"
		(extends "Si8642BB-B-IS")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8642BD-B-IS2"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5.0kV isolation, Fail-Safe Low, 8mm creepage, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 2In 2Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8642EA-B-IU"
		(extends "Si8642BA-B-IU")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8642EA-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 1.0kV isolation, Fail-Safe High, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 2In 2Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8642EB-B-IU"
		(extends "Si8642BA-B-IU")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8642EB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe High, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 2In 2Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8642EC-B-IS1"
		(extends "Si8642BB-B-IS1")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8642EC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe High, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 2In 2Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8642ED-B-IS"
		(extends "Si8642BB-B-IS")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8642ED-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5.0kV isolation, Fail-Safe High, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 2In 2Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8642ED-B-IS2"
		(extends "Si8642BB-B-IS")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8642ED-B-IS2"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5.0kV isolation, Fail-Safe High, 8mm creepage, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 2In 2Out Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8645BB-B-IU"
		(extends "Si8645BA-B-IU")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8645BB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8645BC-B-IS1"
		(extends "Si8645BB-B-IS1")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8645BC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8645BD-B-IS"
		(extends "Si8645BB-B-IS")
		(property "Reference" "U"
			(at 0 15.875 0)
		)
		(property "Value" "Si8645BD-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "https://www.silabs.com/documents/public/data-sheets/si864x-datasheet.pdf"
			(at 0 10.16 0)
		)
		(property "Description" "Low-Power Quad-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5.0kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "4Ch 4In Quad Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660BA-AS1"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660BA-AS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 1kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660BB-AS1"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660BB-AS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660BB-AU"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660BB-AU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660BB-B-IS1"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660BB-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660BB-B-IU"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660BB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660BC-AS1"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660BC-AS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660BC-B-IS1"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660BC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660BD-AS"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660BD-AS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660BD-B-IS"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660BD-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660EB-AU"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660EB-AU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe High, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660EB-B-IU"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660EB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe High, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660EC-AS1"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660EC-AS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe High, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660EC-B-IS1"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660EC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe High, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660ED-AS"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660ED-AS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe High, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8660ED-B-IS"
		(extends "Si8660BA-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8660ED-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe High, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 6In Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661BB-AS1"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661BB-AS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661BB-AU"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661BB-AU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661BB-B-IU"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661BB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661BC-AS1"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661BC-AS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661BC-B-IS1"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661BC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661BD-AS"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661BD-AS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661BD-AS2"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661BD-AS2"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe Low, 8mm creepage, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661BD-B-IS"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661BD-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661BD-B-IS2"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661BD-B-IS2"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe Low, 8mm creepage, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661EB-AU"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661EB-AU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe High, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661EB-B-IU"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661EB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe High, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661EC-AS1"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661EC-AS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe High, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661EC-B-IS1"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661EC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe High, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661ED-AS"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661ED-AS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe High, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8661ED-B-IS"
		(extends "Si8661BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8661ED-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe High, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 5In 1Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8662BB-AS1"
		(extends "Si8662BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662BB-AS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8662BB-AU"
		(extends "Si8662BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662BB-AU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8662BB-B-IU"
		(extends "Si8662BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662BB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8662BC-AS1"
		(extends "Si8662BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662BC-AS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8662BC-B-IS1"
		(extends "Si8662BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662BC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8662BD-AS"
		(extends "Si8662BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662BD-AS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8662BD-B-IS"
		(extends "Si8662BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662BD-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8662EB-AU"
		(extends "Si8662BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662EB-AU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe High, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8662EB-B-IU"
		(extends "Si8662BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662EB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe High, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8662EC-AS1"
		(extends "Si8662BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662EC-AS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe High, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8662EC-B-IS1"
		(extends "Si8662BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662EC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe High, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8662ED-AS"
		(extends "Si8662BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662ED-AS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe High, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8662ED-B-IS"
		(extends "Si8662BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8662ED-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe High, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 4In 2Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8663BB-AS1"
		(extends "Si8663BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663BB-AS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8663BB-AU"
		(extends "Si8663BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663BB-AU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8663BB-B-IU"
		(extends "Si8663BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663BB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe Low, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8663BC-AS1"
		(extends "Si8663BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663BC-AS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8663BC-B-IS1"
		(extends "Si8663BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663BC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe Low, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8663BD-AS"
		(extends "Si8663BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663BD-AS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8663BD-B-IS"
		(extends "Si8663BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663BD-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe Low, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8663EB-AU"
		(extends "Si8663BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663EB-AU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe High, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8663EB-B-IU"
		(extends "Si8663BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663EB-B-IU"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:QSOP-16_3.9x4.9mm_P0.635mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 2.5kV isolation, Fail-Safe High, QSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QSOP*3.9x4.9mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8663EC-AS1"
		(extends "Si8663BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663EC-AS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe High, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8663EC-B-IS1"
		(extends "Si8663BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663EC-B-IS1"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_3.9x9.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 3.75kV isolation, Fail-Safe High, SOIC-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x9.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8663ED-AS"
		(extends "Si8663BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663ED-AS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe High, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps AEC-Q100"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "Si8663ED-B-IS"
		(extends "Si8663BB-B-IS1")
		(property "Reference" "U"
			(at 0 16.51 0)
		)
		(property "Value" "Si8663ED-B-IS"
			(at 0 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "https://www.skyworksinc.com/-/media/Skyworks/SL/documents/public/data-sheets/Si866x.pdf"
			(at 0 11.43 0)
		)
		(property "Description" "Low-Power Hex-Channel Digital Isolator, 150Mbps, 2.5-5.5V, 5kV isolation, Fail-Safe High, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "6Ch 3In 3Out Hex Digital Isolator 150Mbps"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCMT1101"
		(extends "TCMT1100")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TCMT1101"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83510/tcmt1100.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Vce 70V, CTR 40-80%, Viso 3750V (RMS), SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCMT1102"
		(extends "TCMT1100")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TCMT1102"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83510/tcmt1100.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Vce 70V, CTR 63-125%, Viso 3750V (RMS), SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCMT1103"
		(extends "TCMT1100")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TCMT1103"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83510/tcmt1100.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Vce 70V, CTR 100-200%, Viso 3750V (RMS), SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCMT1104"
		(extends "TCMT1100")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TCMT1104"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83510/tcmt1100.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Vce 70V, CTR 160-320%, Viso 3750V (RMS), SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCMT1105"
		(extends "TCMT1100")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TCMT1105"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83510/tcmt1100.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Vce 70V, CTR 50-150%, Viso 3750V (RMS), SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCMT1106"
		(extends "TCMT1100")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TCMT1106"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83510/tcmt1100.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Vce 70V, CTR 100-300%, Viso 3750V (RMS), SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCMT1107"
		(extends "TCMT1100")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TCMT1107"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83510/tcmt1100.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Vce 70V, CTR 80-160%, Viso 3750V (RMS), SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCMT1108"
		(extends "TCMT1100")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TCMT1108"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83510/tcmt1100.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Vce 70V, CTR 130-260%, Viso 3750V (RMS), SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCMT1109"
		(extends "TCMT1100")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TCMT1109"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83510/tcmt1100.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Optocoupler, Vce 70V, CTR 200-400%, Viso 3750V (RMS), SOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCMT1600"
		(extends "TLP290")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TCMT1600"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-4_4.4x2.6mm_P1.27mm"
			(at -21.59 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83512/tcmt1600.pdf"
			(at 0.635 0 0)
		)
		(property "Description" "AC/DC Phototransistor Optocoupler, Vce 70V, CTR 80-300%, SOP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Phototransistor Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCMT4106"
		(extends "TCMT4100")
		(property "Reference" "U"
			(at 0 5.08 0)
		)
		(property "Value" "TCMT4106"
			(at 0 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-16_4.4x10.4mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/84181/tcmt4100.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Quad Optocoupler, Vce 70V, CTR 100-300%, Viso 3750V (RMS), SOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.4x10.4mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCMT4600"
		(extends "TLP290-4")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TCMT4600"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-16_4.55x10.3mm_P1.27mm"
			(at -21.59 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83512/tcmt1600.pdf"
			(at 0.635 0 0)
		)
		(property "Description" "Quad AC/DC Phototransistor Optocoupler, Vce 70V, CTR 80-300%, SOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Quad Phototransistor Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.55x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TCMT4606"
		(extends "TLP290-4")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TCMT4606"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-16_4.55x10.3mm_P1.27mm"
			(at -21.59 -5.08 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83512/tcmt1600.pdf"
			(at 0.635 0 0)
		)
		(property "Description" "Quad AC/DC Phototransistor Optocoupler, Vce 70V, CTR 100-300%, SOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Quad Phototransistor Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.55x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TIL111"
		(extends "4N25")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TIL111"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:DIP-6_W7.62mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.egr.msu.edu/eceshop/Parts_Inventory/datasheets/til111.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Phototransistor NPN, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler Base Connected"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP184xSE"
		(extends "TLP184")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP184xSE"
			(at -5.08 -5.08 0)
		)
		(property "Footprint" "Package_SO:MFSOP6-4_4.4x3.6mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=14118&prodName=TLP184(SE"
			(at 1.27 0 0)
		)
		(property "Description" "AC/DC Optocoupler, Vce 80V, CTR 50-100%, MFSOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MFSOP6*4.4x3.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP185xSE"
		(extends "TLP185")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP185xSE"
			(at -5.08 -5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-4_4.55x3.7mm_P2.54mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=14111&prodName=TLP185(SE"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 80V, CTR 50-100%, MFSOP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*4.55x3.7mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP2761"
		(extends "TLP2748")
		(property "Reference" "U"
			(at -7.112 8.89 0)
		)
		(property "Value" "TLP2761"
			(at 1.016 9.144 0)
		)
		(property "Footprint" "Package_SO:SO-6L_10x3.84mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=28819&prodName=TLP2761"
			(at 0 0 0)
		)
		(property "Description" "15-Mbps inverting photocouple,5 kVrms, 2.7 - 5.5 Vdd, push-pull output"
			(at 0 0 0)
		)
		(property "ki_keywords" "Photocouple highspeed inverting push-pull output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*6L*10x3.84mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP2767"
		(extends "TLP2748")
		(property "Reference" "U"
			(at -7.112 8.89 0)
		)
		(property "Value" "TLP2767"
			(at 1.016 9.144 0)
		)
		(property "Footprint" "Package_SO:SO-6L_10x3.84mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=36717&prodName=TLP2767"
			(at 0 0 0)
		)
		(property "Description" "50-Mbps high speed inverting photocouple,5 kVrms, 2.7 - 5.5 Vdd, push-pull output"
			(at 0 0 0)
		)
		(property "ki_keywords" "Photocouple highspeed inverting push-pull output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*6L*10x3.84mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP2770"
		(extends "TLP2745")
		(property "Reference" "U"
			(at -7.112 8.89 0)
		)
		(property "Value" "TLP2770"
			(at 1.016 9.144 0)
		)
		(property "Footprint" "Package_SO:SO-6L_10x3.84mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=53548&prodName=TLP2770"
			(at 0 0 0)
		)
		(property "Description" "20-Mbps low-power non inverting photocouple,5 kVrms, 2.7 to 5.5 Vdd, push-pull output, SO-6L"
			(at 0 0 0)
		)
		(property "ki_keywords" "Photocouple highspeed non inverting push-pull output"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*6L*10x3.84mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP292"
		(extends "TLP290")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP292"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-4_4.55x2.6mm_P1.27mm"
			(at -21.59 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/TLP292_datasheet_en_20191129.pdf?did=14425&prodName=TLP292"
			(at 0 -7.62 0)
		)
		(property "Description" "AC/DC Phototransistor Optocoupler, Vce 80V, CTR 50-200%, SOP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Phototransistor Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*4.55x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP292-4"
		(extends "TLP290-4")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP292-4"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOP-16_4.55x10.3mm_P1.27mm"
			(at -21.59 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/TLP292-4_datasheet_en_20190520.pdf?did=15284&prodName=TLP292-4"
			(at 0 -7.62 0)
		)
		(property "Description" "Quad AC/DC Phototransistor Optocoupler, Vce 80V, CTR 50-200%, SOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN AC DC Quad Phototransistor Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOP*4.55x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP293"
		(extends "TLP291")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP293"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-4_4.55x2.6mm_P1.27mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/TLP293_datasheet_en_20191129.pdf?did=14419&prodName=TLP293"
			(at 0 -7.62 0)
		)
		(property "Description" "DC Optocoupler, Vce 80V, CTR 50-100%, SOP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*4.55x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP293-4"
		(extends "TLP291-4")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP293-4"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_SO:SOIC-16_4.55x10.3mm_P1.27mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/TLP293-4_datasheet_en_20190520.pdf?did=15287&prodName=TLP293-4"
			(at 0 -7.62 0)
		)
		(property "Description" "Quad DC Optocoupler, Vce 80V, CTR 50-100%, SOP16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Quad Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*4.55x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TLP3022"
		(extends "TLP3021")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP3022"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:Toshiba_11-7A9"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=1421&prodName=TLP3021(S)"
			(at -0.635 0 0)
		)
		(property "Description" "Photo-Triac, Vdrm 400V, Ift 10mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Photo-Triac Opto Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Toshiba*11?7A9*"
			(at 0 0 0)
		)
	)
	(symbol "TLP3023"
		(extends "TLP3021")
		(property "Reference" "U"
			(at -5.08 5.08 0)
		)
		(property "Value" "TLP3023"
			(at 0 5.08 0)
		)
		(property "Footprint" "Package_DIP:Toshiba_11-7A9"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://toshiba.semicon-storage.com/info/docget.jsp?did=1421&prodName=TLP3021(S)"
			(at -0.635 0 0)
		)
		(property "Description" "Photo-Triac, Vdrm 400V, Ift 5mA, DIP6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Photo-Triac Opto Triac"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Toshiba*11?7A9*"
			(at 0 0 0)
		)
	)
	(symbol "VO0600T"
		(extends "HCPL-061A")
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "VO0600T"
			(at 0.254 -9.144 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.vishay.com/doc?84607"
			(at -21.59 15.24 0)
		)
		(property "Description" "Single High Speed CMOS Compatible Optocoupler with enable, dV/dt 1000/us, VCM 10, max 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO0601T"
		(extends "HCPL-061A")
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "VO0601T"
			(at 0.254 -9.144 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.vishay.com/doc?84607"
			(at -21.59 15.24 0)
		)
		(property "Description" "Single High Speed CMOS Compatible Optocoupler with enable, dV/dt 5000/us, VCM 50, max 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO0611T"
		(extends "HCPL-061A")
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "VO0611T"
			(at 0.254 -9.144 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "http://www.vishay.com/doc?84607"
			(at -21.59 15.24 0)
		)
		(property "Description" "Single High Speed CMOS Compatible Optocoupler with enable, dV/dt 15000/us, VCM 1000, max 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO0630T"
		(extends "HCPL-063A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "VO0630T"
			(at 7.874 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.vishay.com/doc?84607"
			(at -21.59 15.24 0)
		)
		(property "Description" "Dual High Speed CMOS Compatible Optocoupler, dV/dt 1000/us, VCM 50, max 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO0631T"
		(extends "HCPL-063A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "VO0631T"
			(at 7.874 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.vishay.com/doc?84607"
			(at -21.59 15.24 0)
		)
		(property "Description" "Dual High Speed CMOS Compatible Optocoupler, dV/dt 5000/us, VCM 1000, max 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO0661T"
		(extends "HCPL-063A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "VO0661T"
			(at 7.874 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.vishay.com/doc?84607"
			(at -21.59 15.24 0)
		)
		(property "Description" "Dual High Speed CMOS Compatible Optocoupler, dV/dt 15000/us, VCM 1000, max 7V VCC, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm?P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO2601"
		(extends "HCPL-261A")
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "VO2601"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?84732"
			(at -21.59 13.97 0)
		)
		(property "Description" "Single High Speed CMOS Compatible Optocoupler with enable, dV/dt 5000/us, VCM 50, max 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO2611"
		(extends "HCPL-261A")
		(property "Reference" "U"
			(at -4.064 8.89 0)
		)
		(property "Value" "VO2611"
			(at 0 -8.89 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 -12.7 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?84732"
			(at -21.59 13.97 0)
		)
		(property "Description" "Single High Speed CMOS Compatible Optocoupler with enable, dV/dt 15000/us, VCM 1000, max 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates enable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO2630"
		(extends "HCPL-263A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "VO2630"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -18.288 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?84732"
			(at -10.16 8.89 0)
		)
		(property "Description" "Dual High Speed CMOS Compatible Optocoupler, dV/dt 1000/us, VCM 10, max 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO2631"
		(extends "HCPL-263A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "VO2631"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -18.288 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?84732"
			(at -10.16 8.89 0)
		)
		(property "Description" "Dual High Speed CMOS Compatible Optocoupler, dV/dt 5000/us, VCM 50, max 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO4661"
		(extends "HCPL-263A")
		(property "Reference" "U"
			(at -4.064 11.43 0)
		)
		(property "Value" "VO4661"
			(at 7.62 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -18.288 0)
		)
		(property "Datasheet" "https://www.vishay.com/doc?84732"
			(at -10.16 8.89 0)
		)
		(property "Description" "Dual High Speed CMOS Compatible Optocoupler, dV/dt 15000/us, VCM 1000, max 7V VCC, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "High speed optically coupled gates"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO615A-1"
		(extends "VO615A")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "VO615A-1"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81753/vo615a.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 70V, CTR 40-80% @ 10mA, Viso 5000Vrms, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W7.62mm* SMDIP*W9.53mm* SMDIP*W11.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO615A-2"
		(extends "VO615A")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "VO615A-2"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81753/vo615a.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 70V, CTR 63-125% @ 10mA, Viso 5000Vrms, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W7.62mm* SMDIP*W9.53mm* SMDIP*W11.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO615A-3"
		(extends "VO615A")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "VO615A-3"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81753/vo615a.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 70V, CTR 100-200% @ 10mA, Viso 5000Vrms, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W7.62mm* SMDIP*W9.53mm* SMDIP*W11.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO615A-4"
		(extends "VO615A")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "VO615A-4"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81753/vo615a.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 70V, CTR 160-320% @ 10mA, Viso 5000Vrms, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W7.62mm* SMDIP*W9.53mm* SMDIP*W11.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO615A-5"
		(extends "VO615A")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "VO615A-5"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81753/vo615a.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 70V, CTR 50-150% @ 5mA, Viso 5000Vrms, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W7.62mm* SMDIP*W9.53mm* SMDIP*W11.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO615A-6"
		(extends "VO615A")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "VO615A-6"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81753/vo615a.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 70V, CTR 100-300% @ 5mA, Viso 5000Vrms, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W7.62mm* SMDIP*W9.53mm* SMDIP*W11.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO615A-7"
		(extends "VO615A")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "VO615A-7"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81753/vo615a.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 70V, CTR 80-160% @ 5mA, Viso 5000Vrms, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W7.62mm* SMDIP*W9.53mm* SMDIP*W11.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO615A-8"
		(extends "VO615A")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "VO615A-8"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81753/vo615a.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 70V, CTR 130-260% @ 5mA, Viso 5000Vrms, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W7.62mm* SMDIP*W9.53mm* SMDIP*W11.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "VO615A-9"
		(extends "VO615A")
		(property "Reference" "U"
			(at 0 7.62 0)
		)
		(property "Value" "VO615A-9"
			(at 0 5.08 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81753/vo615a.pdf"
			(at 0 0 0)
		)
		(property "Description" "DC Optocoupler, Vce 70V, CTR 200-400% @ 5mA, Viso 5000Vrms, DIP4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W7.62mm* SMDIP*W9.53mm* SMDIP*W11.48mm*"
			(at 0 0 0)
		)
	)
	(symbol "VOS618A"
		(extends "TLP785")
		(property "Reference" "U"
			(at -5.08 7.62 0)
		)
		(property "Value" "VOS618A"
			(at -5.08 5.08 0)
		)
		(property "Footprint" "Package_SO:SSOP-4_4.4x2.6mm_P1.27mm"
			(at -5.08 -5.08 0)
		)
		(property "Datasheet" "https://www.vishay.com/docs/83465/vos618a.pdf"
			(at 0 0 0)
		)
		(property "Description" "Optocoupler, Phototransistor Output, Low Input Current, SSOP-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "NPN DC Optocoupler"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*4.4x2.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "π120U30"
		(extends "ADuM1200AR")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "π120U30"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.rpsemi.com/public/doc/2Pai_%CF%8012xUxx_20200416_EN.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Dual-channel digital isolator, 3V/5V level translation, Safe LOW, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-channel digital isolator pi120U30"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "π120U31"
		(extends "ADuM1200AR")
		(property "Reference" "U"
			(at -10.16 8.89 0)
		)
		(property "Value" "π120U31"
			(at -2.032 8.89 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -10.16 0)
		)
		(property "Datasheet" "http://www.rpsemi.com/public/doc/2Pai_%CF%8012xUxx_20200416_EN.pdf"
			(at -11.43 10.16 0)
		)
		(property "Description" "Dual-channel digital isolator, 3V/5V level translation, Safe HIGH, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual-channel digital isolator pi120U31"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
)
