(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ACPL-C790"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.795 0)
		)
		(property "Value" "ACPL-C790"
			(at -5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:SSO-8_6.8x5.9mm_P1.27mm_Clearance8mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://docs.avagotech.com/docs/AV02-2460EN"
			(at 1.143 0.127 0)
		)
		(property "Description" "Precision Isolation Amplifer, ±3% Gain Tolerance, Bandwidth 200kHz, SSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Isolation Amplifer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.8x5.9mm*P1.27mm*Clearance8mm*"
			(at 0 0 0)
		)
		(symbol "ACPL-C790_0_1")
		(symbol "ACPL-C790_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN+")
				(number "2")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "IN-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VDD2")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND2")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT+")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACPL-C870"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.795 0)
		)
		(property "Value" "ACPL-C870"
			(at -5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:SSO-8_6.8x5.9mm_P1.27mm_Clearance8mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "www.avagotech.com/docs/AV02-3563EN"
			(at 1.143 0.127 0)
		)
		(property "Description" "Precision Optycally Isolated Voltage Sensor, ±3% Gain Tolerance, Bandwidth 100kHz, SSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optycally Isolated Voltage Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.8x5.9mm*P1.27mm*Clearance8mm*"
			(at 0 0 0)
		)
		(symbol "ACPL-C870_0_0"
			(text "IN"
				(at -3.81 5.08 900)
			)
			(text "GND"
				(at -3.81 -4.699 900)
			)
			(text "SHDN"
				(at -3.048 0 0)
			)
		)
		(symbol "ACPL-C870_0_1")
		(symbol "ACPL-C870_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "IN")
				(number "2")
			)
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "IN-")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VDD1")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 2.54)
				(name "GND1")
				(number "4")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VDD2")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -10.16 90)
				(length 2.54)
				(name "GND2")
				(number "5")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "OUT+")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "OUT-")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AMC3330"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 22.86 0)
		)
		(property "Value" "AMC3330"
			(at 0 20.32 0)
		)
		(property "Footprint" "Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm"
			(at 31.75 41.91 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/amc3330.pdf"
			(at 33.02 39.37 0)
		)
		(property "Description" "Reinforced Isolated Amplifier With Integrated DC/DC Converter, SOIC-16W"
			(at 0 0 0)
		)
		(property "ki_keywords" "isolated analog amplifier integrated power supply"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x10.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AMC3330_0_1")
		(symbol "AMC3330_1_1"
			(pin power_out line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "DCDC_OUT")
				(number "1")
			)
			(pin power_out line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "DCDC_HGND")
				(number "2")
			)
			(pin power_in line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "HLDO_IN")
				(number "3")
			)
			(pin power_out line
				(at -17.78 0 0)
				(length 2.54)
				(name "HLDO_OUT")
				(number "5")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "INP")
				(number "6")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "INN")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -17.78 90)
				(length 2.54)
				(name "HGND")
				(number "8")
			)
			(pin power_in line
				(at 5.08 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 5.08 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_out line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "LDO_OUT")
				(number "13")
			)
			(pin power_in line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "DCDC_IN")
				(number "16")
			)
			(pin power_in line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "DCDC_GND")
				(number "15")
			)
			(pin output line
				(at 17.78 0 180)
				(length 2.54)
				(name "DIAG")
				(number "14")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "OUTP")
				(number "11")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "OUTN")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IL300"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "IL300"
			(at 0 10.16 0)
		)
		(property "Footprint" ""
			(at -7.62 7.62 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/83622/il300.pdf"
			(at -5.08 10.16 0)
		)
		(property "Description" "Isolated Linear Photocoupler, High Gain, Wideband, DIP8/SMD-DIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Vishay"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* DIP*W10.16mm* SMDIP*W7.62mm* SMDIP*W9.53mm* SMDIP*W11.48mm*"
			(at 0 0 0)
		)
		(symbol "IL300_0_1")
		(symbol "IL300_1_1"
			(pin passive line
				(at -7.62 7.62 0)
				(length 2.54)
				(name "~")
				(number "2")
			)
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~")
				(number "1")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "~")
				(number "3")
			)
			(pin passive line
				(at -7.62 -7.62 0)
				(length 2.54)
				(name "~")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 5.08 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "~")
				(number "6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "~")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ACPL-C79A"
		(extends "ACPL-C790")
		(property "Reference" "U"
			(at -5.08 10.795 0)
		)
		(property "Value" "ACPL-C79A"
			(at -5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:SSO-8_6.8x5.9mm_P1.27mm_Clearance8mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://docs.avagotech.com/docs/AV02-2460EN"
			(at 1.143 0.127 0)
		)
		(property "Description" "Precision Isolation Amplifer, ±1% Gain Tolerance, Bandwidth 200kHz, SSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Isolation Amplifer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.8x5.9mm*P1.27mm*Clearance8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACPL-C79B"
		(extends "ACPL-C790")
		(property "Reference" "U"
			(at -5.08 10.795 0)
		)
		(property "Value" "ACPL-C79B"
			(at -5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:SSO-8_6.8x5.9mm_P1.27mm_Clearance8mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "http://docs.avagotech.com/docs/AV02-2460EN"
			(at 1.143 0.127 0)
		)
		(property "Description" "Precision Isolation Amplifer, ±0.5% Gain Tolerance, Bandwidth 200kHz, SSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Isolation Amplifer"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.8x5.9mm*P1.27mm*Clearance8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACPL-C87A"
		(extends "ACPL-C870")
		(property "Reference" "U"
			(at -5.08 10.795 0)
		)
		(property "Value" "ACPL-C87A"
			(at -5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:SSO-8_6.8x5.9mm_P1.27mm_Clearance8mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "www.avagotech.com/docs/AV02-3563EN"
			(at 1.143 0.127 0)
		)
		(property "Description" "Precision Optycally Isolated Voltage Sensor, ±1% Gain Tolerance, Bandwidth 100kHz, SSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optycally Isolated Voltage Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.8x5.9mm*P1.27mm*Clearance8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ACPL-C87B"
		(extends "ACPL-C870")
		(property "Reference" "U"
			(at -5.08 10.795 0)
		)
		(property "Value" "ACPL-C87B"
			(at -5.08 8.89 0)
		)
		(property "Footprint" "Package_SO:SSO-8_6.8x5.9mm_P1.27mm_Clearance8mm"
			(at 3.81 -8.89 0)
		)
		(property "Datasheet" "www.avagotech.com/docs/AV02-3563EN"
			(at 1.143 0.127 0)
		)
		(property "Description" "Precision Optycally Isolated Voltage Sensor, ±0.5% Gain Tolerance, Bandwidth 100kHz, SSO-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Optycally Isolated Voltage Sensor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSO*6.8x5.9mm*P1.27mm*Clearance8mm*"
			(at 0 0 0)
		)
	)
	(symbol "LOC112"
		(extends "IL300")
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "LOC112"
			(at 0 10.16 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at -7.62 7.62 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=996c6e8f-cc1b-44f6-811e-251c6e004c56&filename=littelfuse-integrated-circuits-loc112-datasheet"
			(at -5.08 10.16 0)
		)
		(property "Description" "Isolated Linear Photocoupler, Wideband, DIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ixys littlefuse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "LOC112P"
		(extends "IL300")
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "LOC112P"
			(at 0 10.16 0)
		)
		(property "Footprint" "Package_DIP:IXYS_Flatpak-8_6.3x9.7mm_P2.54mm"
			(at -7.62 7.62 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=996c6e8f-cc1b-44f6-811e-251c6e004c56&filename=littelfuse-integrated-circuits-loc112-datasheet"
			(at -5.08 10.16 0)
		)
		(property "Description" "Isolated Linear Photocoupler, Wideband, Flatpak-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ixys littlefuse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Flatpak*6.3x9.7mm*P2.54mm*"
			(at 0 0 0)
		)
	)
	(symbol "LOC112S"
		(extends "IL300")
		(property "Reference" "U"
			(at -5.08 10.16 0)
		)
		(property "Value" "LOC112S"
			(at 0 10.16 0)
		)
		(property "Footprint" "Package_DIP:IXYS_SMD-8_6.3x9.7mm_P2.54mm"
			(at -7.62 7.62 0)
		)
		(property "Datasheet" "https://www.littelfuse.com/media?resourcetype=datasheets&itemid=996c6e8f-cc1b-44f6-811e-251c6e004c56&filename=littelfuse-integrated-circuits-loc112-datasheet"
			(at -5.08 10.16 0)
		)
		(property "Description" "Isolated Linear Photocoupler, Wideband, SMD-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "ixys littlefuse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SMD*6.3x9.7mm*P2.54mm*"
			(at 0 0 0)
		)
	)
)
