(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "Jumper_2_Bridged"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim yes)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "JP"
			(at 0 1.905 0)
		)
		(property "Value" "Jumper_2_Bridged"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Jumper, 2-pole, closed/bridged"
			(at 0 0 0)
		)
		(property "ki_keywords" "Jumper SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jumper* TestPoint*2Pads* TestPoint*Bridge*"
			(at 0 0 0)
		)
		(symbol "Jumper_2_Bridged_0_0")
		(symbol "Jumper_2_Bridged_0_1")
		(symbol "Jumper_2_Bridged_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "B")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Jumper_2_Open"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim yes)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "JP"
			(at 0 2.794 0)
		)
		(property "Value" "Jumper_2_Open"
			(at 0 -2.286 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Jumper, 2-pole, open"
			(at 0 0 0)
		)
		(property "ki_keywords" "Jumper SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jumper* TestPoint*2Pads* TestPoint*Bridge*"
			(at 0 0 0)
		)
		(symbol "Jumper_2_Open_0_0")
		(symbol "Jumper_2_Open_0_1")
		(symbol "Jumper_2_Open_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "B")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Jumper_2_Small_Bridged"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim yes)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "JP"
			(at 0 2.032 0)
		)
		(property "Value" "Jumper_2_Small_Bridged"
			(at 0 -2.286 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Jumper, 2-pole, small symbol, bridged"
			(at 0 0 0)
		)
		(property "ki_keywords" "Jumper SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jumper* TestPoint*2Pads* TestPoint*Bridge*"
			(at 0 0 0)
		)
		(symbol "Jumper_2_Small_Bridged_0_0")
		(symbol "Jumper_2_Small_Bridged_0_1")
		(symbol "Jumper_2_Small_Bridged_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.27)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.27)
				(name "B")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Jumper_2_Small_Open"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim yes)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "JP"
			(at 0 2.794 0)
		)
		(property "Value" "Jumper_2_Small_Open"
			(at 0 -2.286 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Jumper, 2-pole, small symbol, open"
			(at 0 0 0)
		)
		(property "ki_keywords" "Jumper SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jumper* TestPoint*2Pads* TestPoint*Bridge*"
			(at 0 0 0)
		)
		(symbol "Jumper_2_Small_Open_0_0")
		(symbol "Jumper_2_Small_Open_0_1")
		(symbol "Jumper_2_Small_Open_1_1"
			(pin passive line
				(at -2.54 0 0)
				(length 1.27)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 1.27)
				(name "B")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Jumper_3_Bridged12"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim yes)
		(in_bom no)
		(on_board yes)
		(property "Reference" "JP"
			(at -2.54 -2.54 0)
		)
		(property "Value" "Jumper_3_Bridged12"
			(at 0 2.794 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Jumper, 3-pole, pins 1+2 closed/bridged"
			(at 0 0 0)
		)
		(property "ki_keywords" "Jumper SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jumper* TestPoint*3Pads* TestPoint*Bridge*"
			(at 0 0 0)
		)
		(symbol "Jumper_3_Bridged12_0_0")
		(symbol "Jumper_3_Bridged12_0_1")
		(symbol "Jumper_3_Bridged12_1_1"
			(pin passive line
				(at -6.35 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 6.35 0 180)
				(length 2.54)
				(name "B")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Jumper_3_Open"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim yes)
		(in_bom no)
		(on_board yes)
		(property "Reference" "JP"
			(at -2.54 -2.54 0)
		)
		(property "Value" "Jumper_3_Open"
			(at 0 2.794 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Jumper, 3-pole, both open"
			(at 0 0 0)
		)
		(property "ki_keywords" "Jumper SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Jumper* TestPoint*3Pads* TestPoint*Bridge*"
			(at 0 0 0)
		)
		(symbol "Jumper_3_Open_0_0")
		(symbol "Jumper_3_Open_0_1")
		(symbol "Jumper_3_Open_1_1"
			(pin passive line
				(at -6.35 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 6.35 0 180)
				(length 2.54)
				(name "B")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SolderJumper_2_Bridged"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim yes)
		(in_bom no)
		(on_board yes)
		(property "Reference" "JP"
			(at 0 2.032 0)
		)
		(property "Value" "SolderJumper_2_Bridged"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Solder Jumper, 2-pole, closed/bridged"
			(at 0 0 0)
		)
		(property "ki_keywords" "solder jumper SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SolderJumper*Bridged*"
			(at 0 0 0)
		)
		(symbol "SolderJumper_2_Bridged_0_1")
		(symbol "SolderJumper_2_Bridged_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "B")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SolderJumper_2_Open"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim yes)
		(in_bom no)
		(on_board yes)
		(property "Reference" "JP"
			(at 0 2.032 0)
		)
		(property "Value" "SolderJumper_2_Open"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Solder Jumper, 2-pole, open"
			(at 0 0 0)
		)
		(property "ki_keywords" "solder jumper SPST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SolderJumper*Open*"
			(at 0 0 0)
		)
		(symbol "SolderJumper_2_Open_0_1")
		(symbol "SolderJumper_2_Open_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "B")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SolderJumper_3_Bridged12"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim yes)
		(in_bom no)
		(on_board yes)
		(property "Reference" "JP"
			(at -2.54 -2.54 0)
		)
		(property "Value" "SolderJumper_3_Bridged12"
			(at 0 2.794 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "3-pole Solder Jumper, pins 1+2 closed/bridged"
			(at 0 0 0)
		)
		(property "ki_keywords" "Solder Jumper SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SolderJumper*Bridged12*"
			(at 0 0 0)
		)
		(symbol "SolderJumper_3_Bridged12_0_1")
		(symbol "SolderJumper_3_Bridged12_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "B")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SolderJumper_3_Bridged123"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim yes)
		(in_bom no)
		(on_board yes)
		(property "Reference" "JP"
			(at -2.54 -2.54 0)
		)
		(property "Value" "SolderJumper_3_Bridged123"
			(at 0 2.794 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Solder Jumper, 3-pole, pins 1+2+3 closed/bridged"
			(at 0 0 0)
		)
		(property "ki_keywords" "Solder Jumper SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SolderJumper*Bridged123*"
			(at 0 0 0)
		)
		(symbol "SolderJumper_3_Bridged123_0_1")
		(symbol "SolderJumper_3_Bridged123_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "B")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SolderJumper_3_Open"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim yes)
		(in_bom no)
		(on_board yes)
		(property "Reference" "JP"
			(at -2.54 -2.54 0)
		)
		(property "Value" "SolderJumper_3_Open"
			(at 0 2.794 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
		)
		(property "Description" "Solder Jumper, 3-pole, open"
			(at 0 0 0)
		)
		(property "ki_keywords" "Solder Jumper SPDT"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SolderJumper*Open*"
			(at 0 0 0)
		)
		(symbol "SolderJumper_3_Open_0_1")
		(symbol "SolderJumper_3_Open_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 0 -3.81 90)
				(length 2.54)
				(name "C")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "B")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
)
