(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "APA-106-F5"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "APA-106-F5"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm-4_RGB"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://cdn.sparkfun.com/datasheets/Components/LED/COM-12877.pdf"
			(at 2.54 -9.525 0)
		)
		(property "Description" "RGB LED with integrated controller, 5mm Package"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED addressable 8bit pwm 5bit greyscale"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*D5.0mm*RGB*"
			(at 0 0 0)
		)
		(symbol "APA-106-F5_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "APA-106-F5_0_1")
		(symbol "APA-106-F5_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "DI")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "DO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APA102"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "APA102"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_RGB_5050-6"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "http://www.led-color.com/upload/201506/APA102%20LED.pdf"
			(at 2.54 -9.525 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED addressable 8bit pwm 5bit greyscale"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*RGB*5050*"
			(at 0 0 0)
		)
		(symbol "APA102_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "APA102_0_1")
		(symbol "APA102_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "DI")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "CI")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "DO")
				(number "6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "CO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APA102-2020"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "APA102-2020"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED-APA102-2020"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "http://www.led-color.com/upload/201604/APA102-2020%20SMD%20LED.pdf"
			(at 2.54 -9.525 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED addressable 8bit pwm 5bit greyscale"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*APA102*"
			(at 0 0 0)
		)
		(symbol "APA102-2020_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "APA102-2020_0_1")
		(symbol "APA102-2020_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "SDI")
				(number "4")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "CKI")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin output line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "SDO")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "CKO")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "APFA3010"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "APFA3010"
			(at 0 -10.16 0)
		)
		(property "Footprint" "LED_SMD:LED_Kingbright_APFA3010_3x1.5mm_Horizontal"
			(at 0 12.7 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/APFA3010LSEEZGKQBKC.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "LED RGB, Common Anode, SMD, 3.0x1.5mm, Horizontal"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED RGB SMD Kingbright APFA3010 Horizontal"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Kingbright*APFA3010*3x1.5mm*Horizontal*"
			(at 0 0 0)
		)
		(symbol "APFA3010_0_0"
			(text "R"
				(at -1.905 3.81 0)
			)
			(text "G"
				(at -1.905 -1.27 0)
			)
			(text "B"
				(at -1.905 -6.35 0)
			)
		)
		(symbol "APFA3010_0_1")
		(symbol "APFA3010_1_1"
			(pin input line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "R")
				(number "1")
			)
			(pin input line
				(at -5.08 0 0)
				(length 2.54)
				(name "G")
				(number "3")
			)
			(pin input line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "B")
				(number "4")
			)
			(pin power_in line
				(at 5.08 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ASMB-MTB0-0A3A2"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 10.16 0)
		)
		(property "Value" "ASMB-MTB0-0A3A2"
			(at 0 -10.16 0)
		)
		(property "Footprint" "LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW"
			(at 0 12.7 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-4186EN"
			(at 0 -11.43 0)
		)
		(property "Description" "Tricolor Black Surface LED, Common Anode Pin 1, PLCC-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "led rgb diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Avago*PLCC4*3.2x2.8mm*"
			(at 0 0 0)
		)
		(symbol "ASMB-MTB0-0A3A2_0_0"
			(text "R"
				(at -1.905 3.81 0)
			)
			(text "G"
				(at -1.905 -1.27 0)
			)
			(text "B"
				(at -1.905 -6.35 0)
			)
		)
		(symbol "ASMB-MTB0-0A3A2_0_1")
		(symbol "ASMB-MTB0-0A3A2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "RK")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "GK")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "BK")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ASMB-MTB1-0A3A2"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 12.7 0)
		)
		(property "Value" "ASMB-MTB1-0A3A2"
			(at 1.27 -11.43 0)
		)
		(property "Footprint" "LED_SMD:LED_Avago_PLCC4_3.2x2.8mm_CW"
			(at 0 15.24 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-4194EN"
			(at 0 -11.43 0)
		)
		(property "Description" "Tricolor Black Surface LED, Common Anode Pin 4, PLCC-4"
			(at 0 0 0)
		)
		(property "ki_keywords" "led rgb diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Avago*PLCC4*3.2x2.8mm*"
			(at 0 0 0)
		)
		(symbol "ASMB-MTB1-0A3A2_0_0"
			(text "R"
				(at -1.905 3.81 0)
			)
			(text "G"
				(at -1.905 -1.27 0)
			)
			(text "B"
				(at -1.905 -6.35 0)
			)
		)
		(symbol "ASMB-MTB1-0A3A2_0_1")
		(symbol "ASMB-MTB1-0A3A2_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "RK")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "GK")
				(number "2")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "BK")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "A")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ASMT-YTC2-0AA02"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at -5.08 6.35 0)
		)
		(property "Value" "ASMT-YTC2-0AA02"
			(at -5.08 -6.35 0)
		)
		(property "Footprint" "LED_SMD:LED_Avago_PLCC6_3x2.8mm"
			(at -5.08 -8.128 0)
		)
		(property "Datasheet" "http://www.avagotech.com/docs/AV02-2589EN"
			(at 3.81 0 0)
		)
		(property "Description" "Triple LED RVB (Avago Technology)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED RGB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED?Avago?PLCC6?3x2.8mm*"
			(at 0 0 0)
		)
		(symbol "ASMT-YTC2-0AA02_0_0"
			(text "B"
				(at -0.508 -3.4544 0)
			)
			(text "R"
				(at -0.381 1.8034 0)
			)
			(text "G"
				(at 4.5466 -0.8382 0)
			)
		)
		(symbol "ASMT-YTC2-0AA02_0_1")
		(symbol "ASMT-YTC2-0AA02_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "AR")
				(number "4")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "AG")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "AB")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "KR")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "KG")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "KB")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CLS6B-FKW"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at -5.08 6.35 0)
		)
		(property "Value" "CLS6B-FKW"
			(at -5.08 -6.35 0)
		)
		(property "Footprint" "LED_SMD:LED_Cree-PLCC6_4.7x1.5mm"
			(at -5.08 -8.128 0)
		)
		(property "Datasheet" "https://www.cree.com/led-components/media/documents/CLS6B-FKW.pdf"
			(at -5.08 -10.16 0)
		)
		(property "Description" "Cree PLCC6 3 in 1 SMD LED, PLCC-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED RGB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*Cree*PLCC*4.7x1.5mm*"
			(at 0 0 0)
		)
		(symbol "CLS6B-FKW_0_0"
			(text "R"
				(at -0.635 1.8034 0)
			)
			(text "B"
				(at -0.635 -3.3274 0)
			)
			(text "G"
				(at 4.4196 -0.7112 0)
			)
		)
		(symbol "CLS6B-FKW_0_1")
		(symbol "CLS6B-FKW_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "AR")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "AG")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "AB")
				(number "1")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "KR")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "KR")
				(number "6")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "KB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CLV1L-FKB"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 9.398 0)
		)
		(property "Value" "CLV1L-FKB"
			(at 0 -8.89 0)
		)
		(property "Footprint" "LED_SMD:LED_Cree-PLCC4_3.2x2.8mm_CCW"
			(at 0 -1.27 0)
		)
		(property "Datasheet" "http://www.cree.com/led-components/media/documents/CLV1L-FKB-1238.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "Cree PLCC4 3 in 1 SMD LED"
			(at 0 0 0)
		)
		(property "ki_keywords" "led rgb diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*Cree*PLCC4*3.2x2.8mm*"
			(at 0 0 0)
		)
		(symbol "CLV1L-FKB_0_0"
			(text "R"
				(at -1.905 3.81 0)
			)
			(text "G"
				(at -1.905 -1.27 0)
			)
			(text "B"
				(at -1.905 -6.35 0)
			)
		)
		(symbol "CLV1L-FKB_0_1")
		(symbol "CLV1L-FKB_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "RK")
				(number "2")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "GK")
				(number "3")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "BK")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "A")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-4830"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "BAR"
			(at 0 3.81 0)
		)
		(property "Value" "HDSP-4830"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Display:HDSP-4830"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1798EN"
			(at 0 0 0)
		)
		(property "Description" "10-element LED arrays, high efficient red"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?48*"
			(at 0 0 0)
		)
		(symbol "HDSP-4830_0_1")
		(symbol "HDSP-4830_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "20")
			)
		)
		(symbol "HDSP-4830_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "19")
			)
		)
		(symbol "HDSP-4830_3_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "18")
			)
		)
		(symbol "HDSP-4830_4_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "17")
			)
		)
		(symbol "HDSP-4830_5_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
		)
		(symbol "HDSP-4830_6_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "15")
			)
		)
		(symbol "HDSP-4830_7_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "14")
			)
		)
		(symbol "HDSP-4830_8_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "13")
			)
		)
		(symbol "HDSP-4830_9_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "12")
			)
		)
		(symbol "HDSP-4830_10_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-4830_2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "BAR"
			(at 0 15.24 0)
		)
		(property "Value" "HDSP-4830_2"
			(at 0 -17.78 0)
		)
		(property "Footprint" "Display:HDSP-4830"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1798EN"
			(at -50.8 5.08 0)
		)
		(property "Description" "BAR GRAPH 10 segment block, high efficiency red"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?48*"
			(at 0 0 0)
		)
		(symbol "HDSP-4830_2_0_1")
		(symbol "HDSP-4830_2_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 2.54)
				(name "K")
				(number "20")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "K")
				(number "19")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "K")
				(number "18")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "K")
				(number "17")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "K")
				(number "15")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "K")
				(number "14")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "K")
				(number "13")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "K")
				(number "12")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 2.54)
				(name "K")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-4832"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "BAR"
			(at 0 3.81 0)
		)
		(property "Value" "HDSP-4832"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Display:HDSP-4832"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1798EN"
			(at 0 0 0)
		)
		(property "Description" "10-element LED arrays, Mix of high efficient red, yellow and green"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?48*"
			(at 0 0 0)
		)
		(symbol "HDSP-4832_0_1")
		(symbol "HDSP-4832_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "20")
			)
		)
		(symbol "HDSP-4832_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "19")
			)
		)
		(symbol "HDSP-4832_3_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "18")
			)
		)
		(symbol "HDSP-4832_4_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "17")
			)
		)
		(symbol "HDSP-4832_5_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
		)
		(symbol "HDSP-4832_6_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "15")
			)
		)
		(symbol "HDSP-4832_7_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "14")
			)
		)
		(symbol "HDSP-4832_8_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "13")
			)
		)
		(symbol "HDSP-4832_9_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "12")
			)
		)
		(symbol "HDSP-4832_10_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-4832_2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "BAR"
			(at 0 15.24 0)
		)
		(property "Value" "HDSP-4832_2"
			(at 0 -17.78 0)
		)
		(property "Footprint" "Display:HDSP-4832"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1798EN"
			(at -50.8 5.08 0)
		)
		(property "Description" "BAR GRAPH 10 segment block, Mix of high efficiency red, yellow and green"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?48*"
			(at 0 0 0)
		)
		(symbol "HDSP-4832_2_0_1")
		(symbol "HDSP-4832_2_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 2.54)
				(name "K")
				(number "20")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "K")
				(number "19")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "K")
				(number "18")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "K")
				(number "17")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "K")
				(number "15")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "K")
				(number "14")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "K")
				(number "13")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "K")
				(number "12")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 2.54)
				(name "K")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-4836"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "BAR"
			(at 0 3.81 0)
		)
		(property "Value" "HDSP-4836"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Display:HDSP-4836"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1798EN"
			(at 0 0 0)
		)
		(property "Description" "10-element LED arrays, Mix of high efficient red, yellow and green"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?48*"
			(at 0 0 0)
		)
		(symbol "HDSP-4836_0_1")
		(symbol "HDSP-4836_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "20")
			)
		)
		(symbol "HDSP-4836_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "19")
			)
		)
		(symbol "HDSP-4836_3_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "18")
			)
		)
		(symbol "HDSP-4836_4_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "17")
			)
		)
		(symbol "HDSP-4836_5_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
		)
		(symbol "HDSP-4836_6_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "15")
			)
		)
		(symbol "HDSP-4836_7_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "14")
			)
		)
		(symbol "HDSP-4836_8_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "13")
			)
		)
		(symbol "HDSP-4836_9_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "12")
			)
		)
		(symbol "HDSP-4836_10_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-4836_2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "BAR"
			(at 0 15.24 0)
		)
		(property "Value" "HDSP-4836_2"
			(at 0 -17.78 0)
		)
		(property "Footprint" "Display:HDSP-4836"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1798EN"
			(at -50.8 5.08 0)
		)
		(property "Description" "BAR GRAPH 10 segment block, Mix of high efficiency red, yellow and green"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?48*"
			(at 0 0 0)
		)
		(symbol "HDSP-4836_2_0_1")
		(symbol "HDSP-4836_2_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 2.54)
				(name "K")
				(number "20")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "K")
				(number "19")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "K")
				(number "18")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "K")
				(number "17")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "K")
				(number "15")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "K")
				(number "14")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "K")
				(number "13")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "K")
				(number "12")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 2.54)
				(name "K")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-4840"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "BAR"
			(at 0 3.81 0)
		)
		(property "Value" "HDSP-4840"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Display:HDSP-4840"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1798EN"
			(at 0 0 0)
		)
		(property "Description" "10-element LED arrays, Yellow"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?48*"
			(at 0 0 0)
		)
		(symbol "HDSP-4840_0_1")
		(symbol "HDSP-4840_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "20")
			)
		)
		(symbol "HDSP-4840_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "19")
			)
		)
		(symbol "HDSP-4840_3_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "18")
			)
		)
		(symbol "HDSP-4840_4_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "17")
			)
		)
		(symbol "HDSP-4840_5_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
		)
		(symbol "HDSP-4840_6_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "15")
			)
		)
		(symbol "HDSP-4840_7_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "14")
			)
		)
		(symbol "HDSP-4840_8_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "13")
			)
		)
		(symbol "HDSP-4840_9_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "12")
			)
		)
		(symbol "HDSP-4840_10_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-4840_2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "BAR"
			(at 0 15.24 0)
		)
		(property "Value" "HDSP-4840_2"
			(at 0 -17.78 0)
		)
		(property "Footprint" "Display:HDSP-4840"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1798EN"
			(at -50.8 5.08 0)
		)
		(property "Description" "BAR GRAPH 10 segment block, yellow"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?48*"
			(at 0 0 0)
		)
		(symbol "HDSP-4840_2_0_1")
		(symbol "HDSP-4840_2_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 2.54)
				(name "K")
				(number "20")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "K")
				(number "19")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "K")
				(number "18")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "K")
				(number "17")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "K")
				(number "15")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "K")
				(number "14")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "K")
				(number "13")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "K")
				(number "12")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 2.54)
				(name "K")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-4850"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "BAR"
			(at 0 3.81 0)
		)
		(property "Value" "HDSP-4850"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Display:HDSP-4850"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1798EN"
			(at 0 0 0)
		)
		(property "Description" "10-element LED arrays, Green"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?48*"
			(at 0 0 0)
		)
		(symbol "HDSP-4850_0_1")
		(symbol "HDSP-4850_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "20")
			)
		)
		(symbol "HDSP-4850_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "19")
			)
		)
		(symbol "HDSP-4850_3_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "18")
			)
		)
		(symbol "HDSP-4850_4_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "17")
			)
		)
		(symbol "HDSP-4850_5_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
		)
		(symbol "HDSP-4850_6_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "15")
			)
		)
		(symbol "HDSP-4850_7_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "14")
			)
		)
		(symbol "HDSP-4850_8_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "13")
			)
		)
		(symbol "HDSP-4850_9_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "12")
			)
		)
		(symbol "HDSP-4850_10_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HDSP-4850_2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "BAR"
			(at 0 15.24 0)
		)
		(property "Value" "HDSP-4850_2"
			(at 0 -17.78 0)
		)
		(property "Footprint" "Display:HDSP-4850"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1798EN"
			(at -50.8 5.08 0)
		)
		(property "Description" "BAR GRAPH 10 segment block, green"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HDSP?48*"
			(at 0 0 0)
		)
		(symbol "HDSP-4850_2_0_1")
		(symbol "HDSP-4850_2_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 2.54)
				(name "K")
				(number "20")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "K")
				(number "19")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "K")
				(number "18")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "K")
				(number "17")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "K")
				(number "15")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "K")
				(number "14")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "K")
				(number "13")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "K")
				(number "12")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 2.54)
				(name "K")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HLCP-J100"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "BAR"
			(at 0 3.81 0)
		)
		(property "Value" "HLCP-J100"
			(at 0 -3.81 0)
		)
		(property "Footprint" "Display:HLCP-J100"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1798EN"
			(at 0 0 0)
		)
		(property "Description" "10-element LED arrays, AIGaAs Red"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HLCP*J100*"
			(at 0 0 0)
		)
		(symbol "HLCP-J100_0_1")
		(symbol "HLCP-J100_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "20")
			)
		)
		(symbol "HLCP-J100_2_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "19")
			)
		)
		(symbol "HLCP-J100_3_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "18")
			)
		)
		(symbol "HLCP-J100_4_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "17")
			)
		)
		(symbol "HLCP-J100_5_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
		)
		(symbol "HLCP-J100_6_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "15")
			)
		)
		(symbol "HLCP-J100_7_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "14")
			)
		)
		(symbol "HLCP-J100_8_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "13")
			)
		)
		(symbol "HLCP-J100_9_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "12")
			)
		)
		(symbol "HLCP-J100_10_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "HLCP-J100_2"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "BAR"
			(at 0 15.24 0)
		)
		(property "Value" "HLCP-J100_2"
			(at 0 -17.78 0)
		)
		(property "Footprint" "Display:HLCP-J100"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-1798EN"
			(at -50.8 5.08 0)
		)
		(property "Description" "BAR GRAPH 10 segment block, AlGaAs red"
			(at 0 0 0)
		)
		(property "ki_keywords" "display LED array"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HLCP?J100*"
			(at 0 0 0)
		)
		(symbol "HLCP-J100_2_0_1")
		(symbol "HLCP-J100_2_1_1"
			(pin passive line
				(at -5.08 10.16 0)
				(length 2.54)
				(name "A")
				(number "1")
			)
			(pin passive line
				(at -5.08 7.62 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin passive line
				(at -5.08 2.54 0)
				(length 2.54)
				(name "A")
				(number "4")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "A")
				(number "5")
			)
			(pin passive line
				(at -5.08 -2.54 0)
				(length 2.54)
				(name "A")
				(number "6")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "A")
				(number "7")
			)
			(pin passive line
				(at -5.08 -7.62 0)
				(length 2.54)
				(name "A")
				(number "8")
			)
			(pin passive line
				(at -5.08 -10.16 0)
				(length 2.54)
				(name "A")
				(number "9")
			)
			(pin passive line
				(at -5.08 -12.7 0)
				(length 2.54)
				(name "A")
				(number "10")
			)
			(pin passive line
				(at 5.08 10.16 180)
				(length 2.54)
				(name "K")
				(number "20")
			)
			(pin passive line
				(at 5.08 7.62 180)
				(length 2.54)
				(name "K")
				(number "19")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "K")
				(number "18")
			)
			(pin passive line
				(at 5.08 2.54 180)
				(length 2.54)
				(name "K")
				(number "17")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "K")
				(number "16")
			)
			(pin passive line
				(at 5.08 -2.54 180)
				(length 2.54)
				(name "K")
				(number "15")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "K")
				(number "14")
			)
			(pin passive line
				(at 5.08 -7.62 180)
				(length 2.54)
				(name "K")
				(number "13")
			)
			(pin passive line
				(at 5.08 -10.16 180)
				(length 2.54)
				(name "K")
				(number "12")
			)
			(pin passive line
				(at 5.08 -12.7 180)
				(length 2.54)
				(name "K")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IR26-21C_L110_TR8"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 2.54 0)
		)
		(property "Value" "IR26-21C_L110_TR8"
			(at 0 -3.81 0)
		)
		(property "Footprint" "LED_SMD:LED_1206_3216Metric"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://www.everlight.com/file/ProductFile/IR26-21C-L110-TR8.pdf"
			(at 0 0 0)
		)
		(property "Description" "940nm, 20 deg, Infrared LED, 1206"
			(at 0 0 0)
		)
		(property "ki_keywords" "IR LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*1206*3216Metric*"
			(at 0 0 0)
		)
		(symbol "IR26-21C_L110_TR8_0_1")
		(symbol "IR26-21C_L110_TR8_1_1"
			(pin passive line
				(at -3.81 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 3.81 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "IRL81A"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "IRL81A"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "LED_THT:LED_SideEmitter_Rectangular_W4.5mm_H1.6mm"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic0/00203825_0.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "850nm High Power Infrared Emitter, Side-Emitter package"
			(at 0 0 0)
		)
		(property "ki_keywords" "IR LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*SideEmitter*Rectangular*W4.5mm*H1.6mm*"
			(at 0 0 0)
		)
		(symbol "IRL81A_0_1")
		(symbol "IRL81A_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Inolux_IN-P55TATRGB"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at -5.08 6.35 0)
		)
		(property "Value" "Inolux_IN-P55TATRGB"
			(at -5.08 -6.35 0)
		)
		(property "Footprint" "LED_SMD:LED_Inolux_IN-P55TATRGB_PLCC6_5.0x5.5mm_P1.8mm"
			(at -5.08 -8.128 0)
		)
		(property "Datasheet" "https://www.inolux-corp.com/datasheet/SMDLED/RGB%20Top%20View/IN-P55TATRGB.pdf"
			(at -5.08 -10.16 0)
		)
		(property "Description" "Inolux RGB LED, PLCC-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED RGB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*Inolux*PLCC6*5.0x5.5mm*"
			(at 0 0 0)
		)
		(symbol "Inolux_IN-P55TATRGB_0_0"
			(text "B"
				(at -0.635 -3.3274 0)
			)
		)
		(symbol "Inolux_IN-P55TATRGB_0_1")
		(symbol "Inolux_IN-P55TATRGB_1_0"
			(text "G"
				(at -0.635 1.8034 0)
			)
			(text "R"
				(at 4.4196 -0.7112 0)
			)
		)
		(symbol "Inolux_IN-P55TATRGB_1_1"
			(pin passive line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "AG")
				(number "4")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "AR")
				(number "5")
			)
			(pin passive line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "AB")
				(number "6")
			)
			(pin passive line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "KG")
				(number "3")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "KR")
				(number "2")
			)
			(pin passive line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "KB")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Inolux_IN-PI554FCH"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "Inolux_IN-PI554FCH"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_Inolux_IN-PI554FCH_PLCC4_5.0x5.0mm_P3.2mm"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "http://www.inolux-corp.com/datasheet/SMDLED/Addressable%20LED/IN-PI554FCH.pdf"
			(at 2.54 -9.525 0)
		)
		(property "Description" "5050 RGB LED 4-Pin with integrated IC"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED NeoPixel addressable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*IN-PI554FCH*PLCC*5.0x5.0mm*P3.2mm*"
			(at 0 0 0)
		)
		(symbol "Inolux_IN-PI554FCH_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "Inolux_IN-PI554FCH_0_1")
		(symbol "Inolux_IN-PI554FCH_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DO")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Inolux_IN-PI556FCH"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "Inolux_IN-PI556FCH"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_WS2812_PLCC6_5.0x5.0mm_P1.6mm"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "http://www.inolux-corp.com/datasheet/SMDLED/Addressable%20LED/IN-PI556FCH.pdf"
			(at 2.54 -9.525 0)
		)
		(property "Description" "5050 RGB LED 6-Pin with integrated IC"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED NeoPixel addressable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*WS2812*PLCC*5.0x5.0mm*P1.6mm*"
			(at 0 0 0)
		)
		(symbol "Inolux_IN-PI556FCH_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "Inolux_IN-PI556FCH_0_1")
		(symbol "Inolux_IN-PI556FCH_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DO")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LD271"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "LD271"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm_IRGrey"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.alliedelec.com/m/d/40788c34903a719969df15f1fbea1056.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "940nm IR-LED, 5mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "IR LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*5.0mm*IRGrey*"
			(at 0 0 0)
		)
		(symbol "LD271_0_1")
		(symbol "LD271_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED_Cree_XHP50_12V"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 6.35 0)
		)
		(property "Value" "LED_Cree_XHP50_12V"
			(at 0 4.445 0)
		)
		(property "Footprint" "LED_SMD:LED_Cree-XHP50_12V"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.cree.com/%7E/media/Files/Cree/LED%20Components%20and%20Modules/XLamp/Data%20and%20Binning/ds%20XHP50.pdf"
			(at -5.08 0 0)
		)
		(property "Description" "XLamp® XHP50 LED, 12V footprint (all 4 LEDs in series)"
			(at 0 0 0)
		)
		(property "ki_keywords" "led diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED?Cree?XHP50?12V*"
			(at 0 0 0)
		)
		(symbol "LED_Cree_XHP50_12V_0_1")
		(symbol "LED_Cree_XHP50_12V_1_1"
			(pin passive line
				(at -8.89 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "PAD")
				(number "3")
			)
			(pin passive line
				(at 8.89 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED_Cree_XHP50_6V"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 11.43 0)
		)
		(property "Value" "LED_Cree_XHP50_6V"
			(at 0 9.525 0)
		)
		(property "Footprint" "LED_SMD:LED_Cree-XHP50_6V"
			(at 0 13.335 0)
		)
		(property "Datasheet" "http://www.cree.com/%7E/media/Files/Cree/LED%20Components%20and%20Modules/XLamp/Data%20and%20Binning/ds%20XHP50.pdf"
			(at -1.905 -2.54 0)
		)
		(property "Description" "XLamp® XHP50 LED, 6V footprint (2x2 serial LEDs in parallel)"
			(at 0 0 0)
		)
		(property "ki_keywords" "led diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED?Cree?XHP50?6V*"
			(at 0 0 0)
		)
		(symbol "LED_Cree_XHP50_6V_0_1")
		(symbol "LED_Cree_XHP50_6V_1_1"
			(pin passive line
				(at -6.35 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "PAD")
				(number "3")
			)
			(pin passive line
				(at 6.35 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED_Cree_XHP70_12V"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 6.35 0)
		)
		(property "Value" "LED_Cree_XHP70_12V"
			(at 0 4.445 0)
		)
		(property "Footprint" "LED_SMD:LED_Cree-XHP70_12V"
			(at 0 8.255 0)
		)
		(property "Datasheet" "http://www.cree.com/%7E/media/Files/Cree/LED%20Components%20and%20Modules/XLamp/Data%20and%20Binning/ds%20XHP70.pdf"
			(at -5.08 0 0)
		)
		(property "Description" "XLamp® XHP70 LED, 12V footprint (all 4 LEDs in series)"
			(at 0 0 0)
		)
		(property "ki_keywords" "led diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED?Cree?XHP70?12V*"
			(at 0 0 0)
		)
		(symbol "LED_Cree_XHP70_12V_0_1")
		(symbol "LED_Cree_XHP70_12V_1_1"
			(pin passive line
				(at -8.89 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 0 -5.08 90)
				(length 2.54)
				(name "PAD")
				(number "3")
			)
			(pin passive line
				(at 8.89 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LED_Cree_XHP70_6V"
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 11.43 0)
		)
		(property "Value" "LED_Cree_XHP70_6V"
			(at 0 9.525 0)
		)
		(property "Footprint" "LED_SMD:LED_Cree-XHP70_6V"
			(at 0 13.335 0)
		)
		(property "Datasheet" "http://www.cree.com/%7E/media/Files/Cree/LED%20Components%20and%20Modules/XLamp/Data%20and%20Binning/ds%20XHP70.pdf"
			(at -1.905 -2.54 0)
		)
		(property "Description" "XLamp® XHP70 LED, 6V footprint (2x2 serial LEDs in parallel)"
			(at 0 0 0)
		)
		(property "ki_keywords" "led diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED?Cree?XHP70?6V*"
			(at 0 0 0)
		)
		(symbol "LED_Cree_XHP70_6V_0_1")
		(symbol "LED_Cree_XHP70_6V_1_1"
			(pin passive line
				(at -6.35 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 0 -10.16 90)
				(length 2.54)
				(name "PAD")
				(number "3")
			)
			(pin passive line
				(at 6.35 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LTST-C235KGKRKT"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at -5.08 6.35 0)
		)
		(property "Value" "LTST-C235KGKRKT"
			(at 0 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_LiteOn_LTST-C235KGKRKT"
			(at 0.762 0 0)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS22-2009-0219/LTST-C235KGKRKT.pdf"
			(at 0.762 0 0)
		)
		(property "Description" "LED dual red/green, 4-pin, down-facing"
			(at 0 0 0)
		)
		(property "ki_keywords" "diode bicolor down-facing reverse"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LTST*C235K*"
			(at 0 0 0)
		)
		(symbol "LTST-C235KGKRKT_0_0"
			(text "R"
				(at -2.54 1.27 0)
			)
			(text "G"
				(at -2.54 -1.27 0)
			)
		)
		(symbol "LTST-C235KGKRKT_0_1")
		(symbol "LTST-C235KGKRKT_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "2")
			)
			(pin input line
				(at 7.62 2.54 180)
				(length 2.54)
				(name "K1")
				(number "4")
			)
			(pin input line
				(at 7.62 -2.54 180)
				(length 2.54)
				(name "K2")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LiteOn_LTST-E563C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "LiteOn_LTST-E563C"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_LiteOn_LTST-E563C_PLCC4_5.0x5.0mm_P3.2mm"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://optoelectronics.liteon.com/upload/download/DS35-2018-0092/LTST-E563CHEGBW-AW.PDF"
			(at 2.54 -9.525 0)
		)
		(property "Description" "5x5mm RGB LED with integrated controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED addressable 5050"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*LiteOn*LTST?E563C*PLCC4*5.0x5.0mm*P3.2mm*"
			(at 0 0 0)
		)
		(symbol "LiteOn_LTST-E563C_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "LiteOn_LTST-E563C_0_1")
		(symbol "LiteOn_LTST-E563C_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NeoPixel_THT"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "NeoPixel_THT"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" ""
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://www.adafruit.com/product/1938"
			(at 2.54 -9.525 0)
		)
		(property "Description" "RGB LED with integrated controller, 5mm/8mm LED package"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED NeoPixel addressable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*D5.0mm* LED*D8.0mm*"
			(at 0 0 0)
		)
		(symbol "NeoPixel_THT_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "NeoPixel_THT_0_1")
		(symbol "NeoPixel_THT_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIN")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "QLS6A-FKW"
		(pin_names
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at -5.08 8.89 0)
		)
		(property "Value" "QLS6A-FKW"
			(at 0 8.89 0)
		)
		(property "Footprint" "LED_SMD:LED_Cree-PLCC6_4.7x1.5mm"
			(at -5.08 -8.89 0)
		)
		(property "Datasheet" "https://www.cree.com/led-components/media/documents/1381-QLS6AFKW.pdf"
			(at -5.08 -13.97 0)
		)
		(property "Description" "Cree PLCC6 3 in 1 SMD LED with zener protection, PLCC-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED RGB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*Cree*PLCC*4.7x1.5mm*"
			(at 0 0 0)
		)
		(symbol "QLS6A-FKW_0_0"
			(text "R"
				(at -0.635 4.3434 0)
			)
			(text "G"
				(at -0.5334 -0.8382 0)
			)
			(text "B"
				(at -0.508 -5.9944 0)
			)
		)
		(symbol "QLS6A-FKW_0_1")
		(symbol "QLS6A-FKW_1_1"
			(pin passive line
				(at -7.62 5.08 0)
				(length 2.54)
				(name "AR")
				(number "3")
			)
			(pin passive line
				(at -7.62 0 0)
				(length 2.54)
				(name "AG")
				(number "5")
			)
			(pin passive line
				(at -7.62 -5.08 0)
				(length 2.54)
				(name "AB")
				(number "1")
			)
			(pin passive line
				(at 7.62 5.08 180)
				(length 2.54)
				(name "KR")
				(number "4")
			)
			(pin passive line
				(at 7.62 0 180)
				(length 2.54)
				(name "KR")
				(number "6")
			)
			(pin passive line
				(at 7.62 -5.08 180)
				(length 2.54)
				(name "KB")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH4356P"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH4356P"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "LED_THT:LED_D3.0mm_IRBlack"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic5/00181708_0.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Infrared LED , 3mm LED package"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*3.0mm*IRBlack*"
			(at 0 0 0)
		)
		(symbol "SFH4356P_0_1")
		(symbol "SFH4356P_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH460"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH460"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-2_Window"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic6/00029609_0.pdf/SFh%20460.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "GaAlAs Infrared LED, TO-18 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*Window*"
			(at 0 0 0)
		)
		(symbol "SFH460_0_1")
		(symbol "SFH460_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SFH482"
		(pin_numbers
			(hide yes)
		)
		(pin_names
			(offset 1.016)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH482"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-2_Window"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic2/00182155_0.pdf/SFH%20482%20E7800,%20Lead%20(Pb)%20Free%20Product%20-%20RoHS%20Compliant.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "GaAlAs Infrared LED (880 nm), TO-18 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*Window*"
			(at 0 0 0)
		)
		(symbol "SFH482_0_1")
		(symbol "SFH482_1_1"
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "K")
				(number "1")
			)
			(pin passive line
				(at 2.54 0 180)
				(length 2.54)
				(name "A")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SK6805"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "SK6805"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_SK6805_PLCC4_2.4x2.7mm_P1.3mm"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/3484/3484_Datasheet.pdf"
			(at 2.54 -9.525 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED NeoPixel Nano addressable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*SK6805*PLCC*2.4x2.7mm*P1.3mm*"
			(at 0 0 0)
		)
		(symbol "SK6805_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "SK6805_0_1")
		(symbol "SK6805_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIN")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SK6812"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "SK6812"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_SK6812_PLCC4_5.0x5.0mm_P3.2mm"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/1138/SK6812+LED+datasheet+.pdf"
			(at 2.54 -9.525 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED NeoPixel addressable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*SK6812*PLCC*5.0x5.0mm*P3.2mm*"
			(at 0 0 0)
		)
		(symbol "SK6812_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "SK6812_0_1")
		(symbol "SK6812_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "1")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DOUT")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SK6812MINI"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "SK6812MINI"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_SK6812MINI_PLCC4_3.5x3.5mm_P1.75mm"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/2686/SK6812MINI_REV.01-1-2.pdf"
			(at 2.54 -9.525 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED NeoPixel Mini addressable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*SK6812MINI*PLCC*3.5x3.5mm*P1.75mm*"
			(at 0 0 0)
		)
		(symbol "SK6812MINI_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "SK6812MINI_0_1")
		(symbol "SK6812MINI_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIN")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SMLVN6RGB"
		(pin_names
			(offset 0)
			(hide yes)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 0 12.7 0)
		)
		(property "Value" "SMLVN6RGB"
			(at 0 10.16 0)
		)
		(property "Footprint" "LED_SMD:LED_ROHM_SMLVN6"
			(at 0 -8.89 0)
		)
		(property "Datasheet" "https://www.rohm.com/datasheet/SMLVN6RGB1U"
			(at 0 -1.27 0)
		)
		(property "Description" "High Brightness Tri-Color LED, RGB, 3.5x2.8mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED RGB Diode"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*ROHM*SMLVN6*"
			(at 0 0 0)
		)
		(symbol "SMLVN6RGB_0_0"
			(text "B"
				(at 1.905 3.81 0)
			)
			(text "R"
				(at 1.905 -1.27 0)
			)
			(text "G"
				(at 1.905 -6.35 0)
			)
		)
		(symbol "SMLVN6RGB_0_1")
		(symbol "SMLVN6RGB_1_1"
			(pin passive line
				(at -5.08 5.08 0)
				(length 2.54)
				(name "BA")
				(number "1")
			)
			(pin passive line
				(at -5.08 0 0)
				(length 2.54)
				(name "RA")
				(number "2")
			)
			(pin passive line
				(at -5.08 -5.08 0)
				(length 2.54)
				(name "GA")
				(number "3")
			)
			(pin passive line
				(at 5.08 5.08 180)
				(length 2.54)
				(name "BK")
				(number "6")
			)
			(pin passive line
				(at 5.08 0 180)
				(length 2.54)
				(name "RK")
				(number "5")
			)
			(pin passive line
				(at 5.08 -5.08 180)
				(length 2.54)
				(name "GK")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WS2812B"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "WS2812B"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B_PLCC4_5.0x5.0mm_P3.2mm"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/WS2812B.pdf"
			(at 2.54 -9.525 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED NeoPixel addressable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*WS2812*PLCC*5.0x5.0mm*P3.2mm*"
			(at 0 0 0)
		)
		(symbol "WS2812B_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "WS2812B_0_1")
		(symbol "WS2812B_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIN")
				(number "4")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DOUT")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WS2812B-2020"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "WS2812B-2020"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_WS2812B-2020_PLCC4_2.0x2.0mm"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/product-files/4684/4684_WS2812B-2020_V1.3_EN.pdf"
			(at 2.54 -9.525 0)
		)
		(property "Description" "RGB LED with integrated controller, 2.0 x 2.0 mm, 12 mA"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED NeoPixel Nano addressable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*WS2812*-2020_PLCC4*"
			(at 0 0 0)
		)
		(symbol "WS2812B-2020_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "WS2812B-2020_0_1")
		(symbol "WS2812B-2020_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIN")
				(number "3")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WS2812S"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "WS2812S"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_WS2812_PLCC6_5.0x5.0mm_P1.6mm"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "http://www.world-semi.com/DownLoadFile/115"
			(at 2.54 -9.525 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED addressable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*WS2812*PLCC*5.0x5.0mm*P1.6mm*"
			(at 0 0 0)
		)
		(symbol "WS2812S_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "WS2812S_0_1")
		(symbol "WS2812S_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIN")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin no_connect line
				(at 5.08 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DOUT")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WS2813"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "WS2813"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_WS2812_PLCC6_5.0x5.0mm_P1.6mm"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "http://www.normandled.com/upload/201605/WS2813%20LED%20Datasheet.pdf"
			(at 2.54 -9.525 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED addressable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*WS2812*PLCC*5.0x5.0mm*P1.6mm*"
			(at 0 0 0)
		)
		(symbol "WS2813_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "WS2813_0_1")
		(symbol "WS2813_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "DIN")
				(number "4")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "BIN")
				(number "6")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "DOUT")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "WS2822S"
		(pin_names
			(offset 0.254)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "WS2822S"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_WS2812_PLCC6_5.0x5.0mm_P1.6mm"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "http://akizukidenshi.com/download/ds/worldsemi/WS2822S.pdf"
			(at 2.54 -9.525 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED addressable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*WS2812*PLCC*5.0x5.0mm*P1.6mm*"
			(at 0 0 0)
		)
		(symbol "WS2822S_0_0"
			(text "RGB"
				(at 2.286 -4.191 0)
			)
		)
		(symbol "WS2822S_0_1")
		(symbol "WS2822S_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "ADRI")
				(number "2")
			)
			(pin input line
				(at -7.62 -2.54 0)
				(length 2.54)
				(name "DAI")
				(number "1")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "ADRO")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ASMT-YTB7-0AA02"
		(extends "ASMT-YTC2-0AA02")
		(property "Reference" "D"
			(at -5.08 6.35 0)
		)
		(property "Value" "ASMT-YTB7-0AA02"
			(at -5.08 -6.35 0)
		)
		(property "Footprint" "LED_SMD:LED_Avago_PLCC6_3x2.8mm"
			(at -5.08 -8.128 0)
		)
		(property "Datasheet" "https://docs.broadcom.com/docs/AV02-3793EN"
			(at 3.81 0 0)
		)
		(property "Description" "Triple LED RVB (Avago Technology)"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED RGB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED?Avago?PLCC6?3x2.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "CLX6F-FKC"
		(extends "ASMT-YTC2-0AA02")
		(property "Reference" "D"
			(at -5.08 6.35 0)
		)
		(property "Value" "CLX6F-FKC"
			(at -5.08 -6.35 0)
		)
		(property "Footprint" "LED_SMD:LED_RGB_PLCC-6"
			(at -5.08 -8.128 0)
		)
		(property "Datasheet" "https://assets.cree-led.com/a/ds/h/HB-CLX6F-FKC.pdf"
			(at 3.81 0 0)
		)
		(property "Description" "RGB LED, PLCC-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED RGB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED?RGB?PLCC*"
			(at 0 0 0)
		)
	)
	(symbol "CQY99"
		(extends "LD271")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "CQY99"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm_IRGrey"
			(at 0 4.445 0)
		)
		(property "Datasheet" "https://www.prtice.info/IMG/pdf/CQY99.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "950nm IR-LED, 5mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "IR LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*5.0mm*IRGrey*"
			(at 0 0 0)
		)
	)
	(symbol "IR204A"
		(extends "SFH4356P")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "IR204A"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "LED_THT:LED_D3.0mm_IRBlack"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.everlight.com/file/ProductFile/IR204-A.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Infrared LED , 3mm LED package"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*3.0mm*IRBlack*"
			(at 0 0 0)
		)
	)
	(symbol "LD274"
		(extends "LD271")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "LD274"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm_IRGrey"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://pdf.datasheetcatalog.com/datasheet/siemens/LD274.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "950nm IR-LED, 5mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "IR LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*5.0mm*IRGrey*"
			(at 0 0 0)
		)
	)
	(symbol "QLS6B-FKW"
		(extends "CLS6B-FKW")
		(property "Reference" "D"
			(at -5.08 6.35 0)
		)
		(property "Value" "QLS6B-FKW"
			(at -5.08 -6.35 0)
		)
		(property "Footprint" "LED_SMD:LED_Cree-PLCC6_4.7x1.5mm"
			(at -5.08 -8.128 0)
		)
		(property "Datasheet" "https://www.cree.com/led-components/media/documents/1397-QLS6BFKW.pdf"
			(at -5.08 -10.16 0)
		)
		(property "Description" "Cree PLCC6 3 in 1 SMD LED, PLCC-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "LED RGB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*Cree*PLCC*4.7x1.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SFH4346"
		(extends "SFH4356P")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH4346"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "LED_THT:LED_D3.0mm_IRBlack"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://cdn-reichelt.de/documents/datenblatt/A500/SFH4346.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Infrared LED , 3mm LED package"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*3.0mm*IRBlack*"
			(at 0 0 0)
		)
	)
	(symbol "SFH4546"
		(extends "LD271")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH4546"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm_IRGrey"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic1/00101982_0.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "High-Power IR LED 940nm"
			(at 0 0 0)
		)
		(property "ki_keywords" "IR LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*5.0mm*IRGrey*"
			(at 0 0 0)
		)
	)
	(symbol "SFH4550"
		(extends "LD271")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH4550"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm_IRGrey"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic3/00116140_0.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "950nm High-Power IR-LED, 5mm"
			(at 0 0 0)
		)
		(property "ki_keywords" "IR LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*5.0mm*IRGrey*"
			(at 0 0 0)
		)
	)
	(symbol "SFH480"
		(extends "SFH482")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "SFH480"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "Package_TO_SOT_THT:TO-18-2_Window"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.osram-os.com/Graphics/XPic1/00083613_0.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "GaAlAs Infrared LED (880 nm), TO-18 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "IR LED Opto"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TO?18*Window*"
			(at 0 0 0)
		)
	)
	(symbol "TSAL4400"
		(extends "SFH4356P")
		(property "Reference" "D"
			(at 0.508 1.778 0)
		)
		(property "Value" "TSAL4400"
			(at -1.016 -2.794 0)
		)
		(property "Footprint" "LED_THT:LED_D3.0mm_IRBlack"
			(at 0 4.445 0)
		)
		(property "Datasheet" "http://www.vishay.com/docs/81006/tsal4400.pdf"
			(at -1.27 0 0)
		)
		(property "Description" "Infrared LED , 3mm LED package"
			(at 0 0 0)
		)
		(property "ki_keywords" "opto IR LED"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*3.0mm*IRBlack*"
			(at 0 0 0)
		)
	)
	(symbol "WS2812"
		(extends "WS2812S")
		(property "Reference" "D"
			(at 5.08 5.715 0)
		)
		(property "Value" "WS2812"
			(at 1.27 -5.715 0)
		)
		(property "Footprint" "LED_SMD:LED_WS2812_PLCC6_5.0x5.0mm_P1.6mm"
			(at 1.27 -7.62 0)
		)
		(property "Datasheet" "https://cdn-shop.adafruit.com/datasheets/WS2812.pdf"
			(at 2.54 -9.525 0)
		)
		(property "Description" "RGB LED with integrated controller"
			(at 0 0 0)
		)
		(property "ki_keywords" "RGB LED NeoPixel addressable"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LED*WS2812*PLCC*5.0x5.0mm*P1.6mm*"
			(at 0 0 0)
		)
	)
)
