(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "74LVC2T45DC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 -11.43 0)
		)
		(property "Value" "74LVC2T45DC"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74LVC_LVCH2T45.pdf"
			(at 6.35 -6.35 0)
		)
		(property "Description" "Dual supply translating transceiver, 3-state, 2-bit, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "74LVC2T45DC_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "1A")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "2A")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DIR")
				(number "5")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "1B")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "2B")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "FXMA108"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "FXMA108"
			(at 7.62 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-20-1EP_2.5x4.5mm_P0.5mm_EP1x2.9mm"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/FXMA108-D.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Dual-Supply, 8-Bit Signal Translator with Configurable Voltage Supplies and Signals Levels, 3-State Outputs and Auto Direction Sensing, WQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level shifter translator bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WQFN*1EP*2.5x4.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "FXMA108_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "~{OE}")
				(number "11")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A0")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A6")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A7")
				(number "9")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VCCB")
				(number "20")
			)
			(pin no_connect line
				(at 2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B0")
				(number "19")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B1")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "17")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B3")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B4")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B5")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B6")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "B7")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NCN4555MN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 11.43 0)
		)
		(property "Value" "NCN4555MN"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.75x1.75mm"
			(at 33.02 -11.43 0)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/NCN4555-D.PDF"
			(at -40.64 -5.08 0)
		)
		(property "Description" "SIM Card Power Supply and Level Shifter, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "SIM Card Level Shifter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "NCN4555MN_0_1")
		(symbol "NCN4555MN_1_1"
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "~{STOP}")
				(number "1")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "MOD_VCC")
				(number "2")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "RST")
				(number "14")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "CLK")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "I/O")
				(number "15")
			)
			(pin no_connect line
				(at -10.16 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VBAT")
				(number "5")
			)
			(pin no_connect line
				(at 10.16 7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin power_out line
				(at 12.7 0 180)
				(length 2.54)
				(name "SIM_VCC")
				(number "7")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SIM_RST")
				(number "9")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "SIM_CLK")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "SIM_I/O")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NLSV2T244D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "NLSV2T244D"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NLSV2T244-D.PDF"
			(at -22.86 -13.97 0)
		)
		(property "Description" "Dual-Bit Dual-Supply Non-Inverting Level Translator, Output Enable, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "NLSV2T244D_0_1")
		(symbol "NLSV2T244D_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{OE}")
				(number "4")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NLSV2T244DM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "NLSV2T244DM"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NLSV2T244-D.PDF"
			(at -22.86 -13.97 0)
		)
		(property "Description" "Dual-Bit Dual-Supply Non-Inverting Level Translator, Output Enable, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "NLSV2T244DM_0_1")
		(symbol "NLSV2T244DM_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{OE}")
				(number "4")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NLSV2T244MU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "NLSV2T244MU"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:OnSemi_UDFN-8_1.2x1.8mm_P0.4mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.onsemi.com/pub/Collateral/NLSV2T244-D.PDF"
			(at -22.86 -13.97 0)
		)
		(property "Description" "Dual-Bit Dual-Supply Non-Inverting Level Translator, Output Enable, UDFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "OnSemi*UDFN*1.2x1.8mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "NLSV2T244MU_0_1")
		(symbol "NLSV2T244MU_1_1"
			(pin input line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin input line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "~{OE}")
				(number "4")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "8")
			)
			(pin output line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "7")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74AUP1T34DCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 6.35 0)
		)
		(property "Value" "SN74AUP1T34DCK"
			(at 11.43 6.35 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -17.78 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74aup1t34.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "1-Bit Unidirectional Voltage-Level Translator, SC-70"
			(at 0 0 0)
		)
		(property "ki_keywords" "Noninverting"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*353*"
			(at 0 0 0)
		)
		(symbol "SN74AUP1T34DCK_0_1"
			(pin input line
				(at -10.16 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin power_in line
				(at -2.54 7.62 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 7.62 270)
				(length 2.54)
				(name "VCCB")
				(number "5")
			)
			(pin output line
				(at 10.16 0 180)
				(length 2.54)
				(name "B")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74AVC4T245PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "SN74AVC4T245PW"
			(at 12.7 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74avc4t245.pdf"
			(at -1.27 -6.35 0)
		)
		(property "Description" "4-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Noninverting Bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SN74AVC4T245PW_0_1")
		(symbol "SN74AVC4T245PW_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "1~{OE}")
				(number "15")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "2~{OE}")
				(number "14")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "1DIR")
				(number "2")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "2DIR")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "1A1")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "1A2")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "2A1")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "2A2")
				(number "7")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VCCB")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "1B1")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "1B2")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "2B1")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "2B2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74AVC8T245PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 13.97 0)
		)
		(property "Value" "SN74AVC8T245PW"
			(at 12.7 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-24_4.4x7.8mm_P0.65mm"
			(at 22.86 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74avc8t245.pdf"
			(at -1.27 -6.35 0)
		)
		(property "Description" "8-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs, TSSOP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Noninverting Bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x7.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SN74AVC8T245PW_0_1")
		(symbol "SN74AVC8T245PW_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "DIR")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A6")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A7")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A8")
				(number "10")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCCB")
				(number "24")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "VCCB")
				(number "23")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{OE}")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "B1")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "B2")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "B3")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "B4")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "B5")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "B6")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "B7")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "B8")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74LV1T125DCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "SN74LV1T125DCK"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lv1t125.pdf"
			(at 0 -21.59 0)
		)
		(property "Description" "Single Power Supply, Single Buffer Gate with 3-State Output, CMOS Logic Level Shifter Level Shifter, SC70-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single buffer level shift"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
		(symbol "SN74LV1T125DCK_0_1")
		(symbol "SN74LV1T125DCK_1_1"
			(pin input line
				(at -7.62 2.54 0)
				(length 2.54)
				(name "~{OE}")
				(number "1")
			)
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "Y")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74LV1T34DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "SN74LV1T34DBV"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 16.51 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lv1t34.pdf"
			(at -10.16 -5.08 0)
		)
		(property "Description" "Single Power Supply, Single Buffer GATE, CMOS Logic, Level Shifter, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single buffer level shift"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "SN74LV1T34DBV_0_1")
		(symbol "SN74LV1T34DBV_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "Y")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74LV1T34DCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "SN74LV1T34DCK"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-353_SC-70-5"
			(at 20.32 -6.35 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lv1t34.pdf"
			(at -10.16 -5.08 0)
		)
		(property "Description" "Single Power Supply, Single Buffer GATE, CMOS Logic, Level Shifter, SOT-353"
			(at 0 0 0)
		)
		(property "ki_keywords" "single buffer level shift"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?353*"
			(at 0 0 0)
		)
		(symbol "SN74LV1T34DCK_0_1")
		(symbol "SN74LV1T34DCK_1_1"
			(pin input line
				(at -7.62 0 0)
				(length 2.54)
				(name "A")
				(number "2")
			)
			(pin no_connect line
				(at -5.08 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 7.62 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -7.62 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin output line
				(at 7.62 0 180)
				(length 2.54)
				(name "Y")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74LVC1T45DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "SN74LVC1T45DBV"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1t45.pdf"
			(at -22.86 -16.51 0)
		)
		(property "Description" "Single-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "SN74LVC1T45DBV_0_1")
		(symbol "SN74LVC1T45DBV_1_1"
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DIR")
				(number "5")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VCCB")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74LVC1T45DCK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "SN74LVC1T45DCK"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1t45.pdf"
			(at -22.86 -16.51 0)
		)
		(property "Description" "Single-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70*"
			(at 0 0 0)
		)
		(symbol "SN74LVC1T45DCK_0_1")
		(symbol "SN74LVC1T45DCK_1_1"
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DIR")
				(number "5")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VCCB")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74LVC1T45DRL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "SN74LVC1T45DRL"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 0 -11.43 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1t45.pdf"
			(at -22.86 -16.51 0)
		)
		(property "Description" "Single-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOT?563*"
			(at 0 0 0)
		)
		(symbol "SN74LVC1T45DRL_0_1")
		(symbol "SN74LVC1T45DRL_1_1"
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin input line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "DIR")
				(number "5")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "VCCB")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74LVC245APW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 17.78 0)
		)
		(property "Value" "SN74LVC245APW"
			(at 10.16 17.78 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 22.86 -16.51 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/scas218x/scas218x.pdf"
			(at -1.27 -6.35 0)
		)
		(property "Description" "8-Bit Single-Supply Bus Transceiver With 5V tolerant input voltage and 3-State Outputs 24mA, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Noninverting Bidirectional"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "SN74LVC245APW_0_1")
		(symbol "SN74LVC245APW_1_1"
			(pin input line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "DIR")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "A6")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "A7")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "A8")
				(number "9")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "~{OE}")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "B1")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "B2")
				(number "17")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "B3")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "B4")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "B5")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "B6")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "B7")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "B8")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74LVC2T45DCUR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "SN74LVC2T45DCUR"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc2t45.pdf"
			(at -22.86 -13.97 0)
		)
		(property "Description" "Dual-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SN74LVC2T45DCUR_0_1")
		(symbol "SN74LVC2T45DCUR_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DIR")
				(number "5")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74LVC2T45YZP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "SN74LVC2T45YZP"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-8_0.9x1.9mm_Layout2x4_P0.5mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc2t45.pdf"
			(at -22.86 -13.97 0)
		)
		(property "Description" "Dual-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs, DSBGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*0.9x1.9mm*Layout2x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "SN74LVC2T45YZP_0_1")
		(symbol "SN74LVC2T45YZP_1_1"
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "B1")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "C1")
			)
			(pin input line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "DIR")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "A1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "D1")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "A2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "B2")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B2")
				(number "C2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "SN74LVC8T245"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 27.94 0)
		)
		(property "Value" "SN74LVC8T245"
			(at 3.81 27.94 0)
		)
		(property "Footprint" ""
			(at 20.32 -24.13 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lvc8t245.pdf"
			(at 0 -35.56 0)
		)
		(property "Description" "8-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs"
			(at 0 0 0)
		)
		(property "ki_keywords" "Dual Supply Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x8.2mm* SSOP*3.9x8.7mm* TSSOP*4.4x7.8mm* TVSOP*4.4x5.0mm* Texas*VQFN*RHL*"
			(at 0 0 0)
		)
		(symbol "SN74LVC8T245_0_1")
		(symbol "SN74LVC8T245_1_1"
			(pin bidirectional line
				(at -10.16 17.78 0)
				(length 2.54)
				(name "A1")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A3")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A4")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A6")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "A7")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 -17.78 0)
				(length 2.54)
				(name "A8")
				(number "10")
			)
			(pin input line
				(at -10.16 -20.32 0)
				(length 2.54)
				(name "~{OE}")
				(number "22")
			)
			(pin input line
				(at -10.16 -22.86 0)
				(length 2.54)
				(name "DIR")
				(number "2")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "V_{CCA}")
				(number "1")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "V_{CCB}")
				(number "23")
			)
			(pin passive line
				(at 2.54 27.94 270)
				(length 2.54)
				(hide yes)
				(name "V_{CCB}")
				(number "24")
			)
			(pin bidirectional line
				(at 10.16 17.78 180)
				(length 2.54)
				(name "B1")
				(number "21")
			)
			(pin bidirectional line
				(at 10.16 12.7 180)
				(length 2.54)
				(name "B2")
				(number "20")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B3")
				(number "19")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B4")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B5")
				(number "17")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B6")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -12.7 180)
				(length 2.54)
				(name "B7")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -17.78 180)
				(length 2.54)
				(name "B8")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TCA9517ADGK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "TCA9517ADGK"
			(at 1.27 -11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.7 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tca9517a.pdf"
			(at 0 -15.24 0)
		)
		(property "Description" "Level-Translating I2C Bus Buffer/Repeater, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "I2C buffer repeater"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TCA9517ADGK_1_1"
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SCLA")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SDAA")
				(number "3")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SCLB")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "SDAB")
				(number "6")
			)
			(pin passive line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "EN")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0101DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TXB0101DBV"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0101.pdf"
			(at 0 -0.762 0)
		)
		(property "Description" "1-Bit Bidirectional Voltage-Level Translator With Auto Direction Sensing and ±15-kV ESD Protection, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional voltage level translator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?6*"
			(at 0 0 0)
		)
		(symbol "TXB0101DBV_0_1")
		(symbol "TXB0101DBV_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "OE")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "V_{CCA}")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "V_{CCB}")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0101YZP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TXB0101YZP"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-6_0.9x1.4mm_Layout2x3_P0.5mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0101.pdf"
			(at 0 -0.762 0)
		)
		(property "Description" "1-Bit Bidirectional Voltage-Level Translator With Auto Direction Sensing and ±15-kV ESD Protection, DSBGA-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional voltage level translator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*DSBGA?6*"
			(at 0 0 0)
		)
		(symbol "TXB0101YZP_0_1")
		(symbol "TXB0101YZP_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "OE")
				(number "B2")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "A")
				(number "C1")
			)
			(pin power_in line
				(at -2.54 10.16 270)
				(length 2.54)
				(name "V_{CCA}")
				(number "A1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "GND")
				(number "B1")
			)
			(pin power_in line
				(at 2.54 10.16 270)
				(length 2.54)
				(name "V_{CCB}")
				(number "A2")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B")
				(number "C2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0102DCT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TXB0102DCT"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_3x3mm_P0.65mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0102.pdf"
			(at 0 -0.762 0)
		)
		(property "Description" "2-Bit Bidirectional Voltage-Level Translator With Auto Direction Sensing and ±15-kV ESD Protection, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TXB0102DCT_0_1")
		(symbol "TXB0102DCT_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "OE")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B2")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0102DCU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TXB0102DCU"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0102.pdf"
			(at 0 -0.762 0)
		)
		(property "Description" "2-Bit Bidirectional Voltage-Level Translator With Auto Direction Sensing and ±15-kV ESD Protection, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TXB0102DCU_0_1")
		(symbol "TXB0102DCU_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "OE")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B2")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0102YZP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TXB0102YZP"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-8_0.9x1.9mm_Layout2x4_P0.5mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0102.pdf"
			(at 0 -0.762 0)
		)
		(property "Description" "2-Bit Bidirectional Voltage-Level Translator With Auto Direction Sensing and ±15-kV ESD Protection, DSBGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*0.9x1.9mm*Layout2x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TXB0102YZP_0_1")
		(symbol "TXB0102YZP_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "OE")
				(number "C2")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "D2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "D1")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "C1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "B1")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "B2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "A2")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B2")
				(number "A1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0104D"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TXB0104D"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0104.pdf"
			(at 2.794 2.413 0)
		)
		(property "Description" "4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6V APort, 1.65 - 5.5V BPort, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*14*7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "TXB0104D_0_1")
		(symbol "TXB0104D_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "OE")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VCCB")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B1")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B4")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0104PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TXB0104PW"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0104.pdf"
			(at 2.794 2.413 0)
		)
		(property "Description" "4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6V APort, 1.65 - 5.5V BPort, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*14*5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TXB0104PW_0_1")
		(symbol "TXB0104PW_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "OE")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VCCB")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B1")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B4")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0104RGY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TXB0104RGY"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_S-PVQFN-N14"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0104.pdf"
			(at 2.794 2.413 0)
		)
		(property "Description" "4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6V APort, 1.65 - 5.5V BPort, Texas_PVGFN-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*S*PVQFN*N14*"
			(at 0 0 0)
		)
		(symbol "TXB0104RGY_0_1")
		(symbol "TXB0104RGY_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "OE")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin no_connect line
				(at -7.62 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VCCB")
				(number "14")
			)
			(pin input line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "Pad")
				(number "15")
			)
			(pin no_connect line
				(at 7.62 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B1")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B4")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0104RUT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TXB0104RUT"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_R-PUQFN-N12"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0104.pdf"
			(at 2.794 2.413 0)
		)
		(property "Description" "4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6V APort, 1.65 - 5.5V BPort, Texas_PUQFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*R*PUQFN*N12*"
			(at 0 0 0)
		)
		(symbol "TXB0104RUT_0_1")
		(symbol "TXB0104RUT_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "OE")
				(number "12")
			)
			(pin tri_state line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin tri_state line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin tri_state line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin tri_state line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VCCB")
				(number "11")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B1")
				(number "10")
			)
			(pin tri_state line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "9")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "8")
			)
			(pin tri_state line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B4")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0104YZT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TXB0104YZT"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-12_1.36x1.86mm_Layout3x4_P0.5mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0104.pdf"
			(at 2.794 2.413 0)
		)
		(property "Description" "4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6V APort, 1.65 - 5.5V BPort, DSBGA-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*1.36x1.86mm*Layout3x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TXB0104YZT_0_1")
		(symbol "TXB0104YZT_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "OE")
				(number "C2")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "A3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "B3")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "C3")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A4")
				(number "D3")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCCA")
				(number "B2")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "D2")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VCCB")
				(number "A2")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B1")
				(number "A1")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "B1")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "C1")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B4")
				(number "D1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0104ZXU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TXB0104ZXU"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_BGA:Texas_MicroStar_Junior_BGA-12_2.0x2.5mm_Layout4x3_P0.5mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0104.pdf"
			(at 2.794 2.413 0)
		)
		(property "Description" "4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6V APort, 1.65 - 5.5V BPort, Texas_Junior-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*Junior*BGA*2.0x2.5mm*Layout4x3*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TXB0104ZXU_0_1")
		(symbol "TXB0104ZXU_1_1"
			(pin input line
				(at -10.16 12.7 0)
				(length 2.54)
				(name "OE")
				(number "B3")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "A1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "A2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "A3")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A4")
				(number "A4")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCCA")
				(number "B2")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "B4")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VCCB")
				(number "B1")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B1")
				(number "C1")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "C2")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "C3")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B4")
				(number "C4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0106PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "TXB0106PW"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0106.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "6-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6V APort, 1.65 - 5.5V BPort, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional voltage level translator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TXB0106PW_0_1")
		(symbol "TXB0106PW_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "OE")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A6")
				(number "7")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "V_{CCA}")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "V_{CCB}")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B1")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B3")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B4")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B5")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B6")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0106RGY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "TXB0106RGY"
			(at 3.81 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGY_R-PVQFN-N16_EP2.05x2.55mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0106.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "6-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6V APort, 1.65 - 5.5V BPort, VQFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional voltage level translator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*RGY*PVQFN*"
			(at 0 0 0)
		)
		(symbol "TXB0106RGY_0_1")
		(symbol "TXB0106RGY_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "OE")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A6")
				(number "7")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 2.54)
				(name "V_{CCA}")
				(number "2")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 2.54)
				(name "V_{CCB}")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B1")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B3")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B4")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B5")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B6")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0108DQSR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TXB0108DQSR"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SON:USON-20_2x4mm_P0.4mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0108.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "8-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6V APort, 1.65 - 5.5V BPort, USON-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional voltage level translator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "USON*2x4mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "TXB0108DQSR_0_1")
		(symbol "TXB0108DQSR_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "OE")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A2")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A3")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "A4")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A5")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A6")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A7")
				(number "9")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A8")
				(number "10")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCCA")
				(number "5")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VCCB")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B1")
				(number "20")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B2")
				(number "19")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B3")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B4")
				(number "17")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B5")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B6")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B7")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "B8")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0108PW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TXB0108PW"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0108.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "8-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6V APort, 1.65 - 5.5V BPort, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional voltage level translator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TXB0108PW_0_1")
		(symbol "TXB0108PW_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "OE")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A6")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A7")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A8")
				(number "9")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "V_{CCA}")
				(number "2")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "V_{CCB}")
				(number "19")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B1")
				(number "20")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B2")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B3")
				(number "17")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B4")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B5")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B6")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B7")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "B8")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXB0108RGY"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TXB0108RGY"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_RGY_R-PVQFN-N20_EP2.05x3.05mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0108.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "8-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing and ±15-kV ESD Protection, 1.2 - 3.6V APort, 1.65 - 5.5V BPort, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional voltage level translator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*RGY*PVQFN*"
			(at 0 0 0)
		)
		(symbol "TXB0108RGY_0_1")
		(symbol "TXB0108RGY_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "OE")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A6")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A7")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A8")
				(number "9")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "V_{CCA}")
				(number "2")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "V_{CCB}")
				(number "19")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B1")
				(number "20")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B2")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B3")
				(number "17")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B4")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B5")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B6")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B7")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "B8")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXBN0304RUT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TXBN0304RUT"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_R-PUQFN-N12"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0304.pdf"
			(at 2.794 2.413 0)
		)
		(property "Description" "4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing, 0.9 - 3.6V APort, 0.9 - 3.6V BPort, Active Low Output Enable, Texas_PUQFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*R*PUQFN*N12*"
			(at 0 0 0)
		)
		(symbol "TXBN0304RUT_0_1")
		(symbol "TXBN0304RUT_1_1"
			(pin tri_state line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin tri_state line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin tri_state line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin tri_state line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin input line
				(at -10.16 -12.7 0)
				(length 2.54)
				(name "~{OE}")
				(number "12")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VCCB")
				(number "11")
			)
			(pin tri_state line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B1")
				(number "10")
			)
			(pin tri_state line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B2")
				(number "9")
			)
			(pin tri_state line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "8")
			)
			(pin tri_state line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B4")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXS0101DBV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TXS0101DBV"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/txs0101.pdf"
			(at 0 -24.13 0)
		)
		(property "Description" "1-Bit Bidirectional Voltage-Level Shifter for Open-Drain and Push-Pull Application, SOT-23"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
		(symbol "TXS0101DBV_0_1")
		(symbol "TXS0101DBV_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "OE")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A")
				(number "3")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "V_{CCA}")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "V_{CCB}")
				(number "6")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXS0101YZP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TXS0101YZP"
			(at 8.89 11.43 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-6_0.9x1.4mm_Layout2x3_P0.5mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/txs0101.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "1-Bit Bidirectional Voltage-Level Shifter for Open-Drain and Push-Pull Application, Texas DSBGA-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*0.9x1.4mm*Layout2x3*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TXS0101YZP_0_1")
		(symbol "TXS0101YZP_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "OE")
				(number "B2")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A")
				(number "C1")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "V_{CCA}")
				(number "A1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "B1")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "V_{CCB}")
				(number "A2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B")
				(number "C2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXS0102DCT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TXS0102DCT"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:SSOP-8_2.95x2.8mm_P0.65mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/txs0102"
			(at 0 -0.508 0)
		)
		(property "Description" "2-Bit Bidirectional Voltage-Level Shifter for Open-Drain and Push-Pull Application, SSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*2.95x2.8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TXS0102DCT_0_1")
		(symbol "TXS0102DCT_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "OE")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B2")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXS0102DCU"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TXS0102DCU"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/txs0102"
			(at 0 -0.508 0)
		)
		(property "Description" "2-Bit Bidirectional Voltage-Level Shifter for Open-Drain and Push-Pull Application, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TXS0102DCU_0_1")
		(symbol "TXS0102DCU_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "OE")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "4")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B2")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXS0102DQE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TXS0102DQE"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SON:X2SON-8_1.4x1mm_P0.35mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/txs0102"
			(at 0 -0.508 0)
		)
		(property "Description" "2-Bit Bidirectional Voltage-Level Shifter for Open-Drain and Push-Pull Application, X2SON-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "X2SON*1.4x1mm*P0.35mm*"
			(at 0 0 0)
		)
		(symbol "TXS0102DQE_0_1")
		(symbol "TXS0102DQE_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "OE")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "8")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "7")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B2")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXS0102YZP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 11.43 0)
		)
		(property "Value" "TXS0102YZP"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_BGA:Texas_DSBGA-8_0.9x1.9mm_Layout2x4_P0.5mm"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/gpn/txs0102"
			(at 0 -0.508 0)
		)
		(property "Description" "2-Bit Bidirectional Voltage-Level Shifter for Open-Drain and Push-Pull Application, DSBGA-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*DSBGA*0.9x1.9mm*Layout2x4*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "TXS0102YZP_0_1")
		(symbol "TXS0102YZP_1_1"
			(pin input line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "OE")
				(number "C2")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "D2")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A2")
				(number "D1")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "VCCA")
				(number "C1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "B1")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "VCCB")
				(number "B2")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "A2")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B2")
				(number "A1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXS0104EPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TXS0104EPW"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/txs0104e.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Bidirectional  level-shifting voltage translator, TSSOP-14"
			(at 1.27 -16.51 0)
		)
		(property "ki_keywords" "4-bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TXS0104EPW_0_1")
		(symbol "TXS0104EPW_1_0"
			(pin no_connect line
				(at -7.62 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 7.62 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
		)
		(symbol "TXS0104EPW_1_1"
			(pin input line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "OE")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A1")
				(number "2")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin power_in line
				(at -2.54 12.7 270)
				(length 2.54)
				(name "V_{CCA}")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 12.7 270)
				(length 2.54)
				(name "V_{CCB}")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B1")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B2")
				(number "12")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B3")
				(number "11")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B4")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXS0108EPW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TXS0108EPW"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/txs0108e.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Bidirectional  level-shifting voltage translator, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "TXS0108EPW_0_1")
		(symbol "TXS0108EPW_1_1"
			(pin input line
				(at -10.16 10.16 0)
				(length 2.54)
				(name "OE")
				(number "10")
			)
			(pin bidirectional line
				(at -10.16 7.62 0)
				(length 2.54)
				(name "A1")
				(number "1")
			)
			(pin bidirectional line
				(at -10.16 5.08 0)
				(length 2.54)
				(name "A2")
				(number "3")
			)
			(pin bidirectional line
				(at -10.16 2.54 0)
				(length 2.54)
				(name "A3")
				(number "4")
			)
			(pin bidirectional line
				(at -10.16 0 0)
				(length 2.54)
				(name "A4")
				(number "5")
			)
			(pin bidirectional line
				(at -10.16 -2.54 0)
				(length 2.54)
				(name "A5")
				(number "6")
			)
			(pin bidirectional line
				(at -10.16 -5.08 0)
				(length 2.54)
				(name "A6")
				(number "7")
			)
			(pin bidirectional line
				(at -10.16 -7.62 0)
				(length 2.54)
				(name "A7")
				(number "8")
			)
			(pin bidirectional line
				(at -10.16 -10.16 0)
				(length 2.54)
				(name "A8")
				(number "9")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VCCA")
				(number "2")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VCCB")
				(number "19")
			)
			(pin bidirectional line
				(at 10.16 7.62 180)
				(length 2.54)
				(name "B1")
				(number "20")
			)
			(pin bidirectional line
				(at 10.16 5.08 180)
				(length 2.54)
				(name "B2")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 2.54 180)
				(length 2.54)
				(name "B3")
				(number "17")
			)
			(pin bidirectional line
				(at 10.16 0 180)
				(length 2.54)
				(name "B4")
				(number "16")
			)
			(pin bidirectional line
				(at 10.16 -2.54 180)
				(length 2.54)
				(name "B5")
				(number "15")
			)
			(pin bidirectional line
				(at 10.16 -5.08 180)
				(length 2.54)
				(name "B6")
				(number "14")
			)
			(pin bidirectional line
				(at 10.16 -7.62 180)
				(length 2.54)
				(name "B7")
				(number "13")
			)
			(pin bidirectional line
				(at 10.16 -10.16 180)
				(length 2.54)
				(name "B8")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "TXS02612RTW"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 24.13 0)
		)
		(property "Value" "TXS02612RTW"
			(at 8.89 -24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:WQFN-24-1EP_4x4mm_P0.5mm_EP2.45x2.45mm_ThermalVias"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/gpn/TXS02612"
			(at 0 -38.1 0)
		)
		(property "Description" "SDIO port expander with voltage-level translation, 6:12 Demultiplexer/Multiplexer, 1.1V to 3.6V supply range, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "SDIO level translator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*WQFN*24*4x4mm*"
			(at 0 0 0)
		)
		(symbol "TXS02612RTW_1_1"
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "DAT0A")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DAT1A")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DAT2A")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DAT3A")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "CMDA")
				(number "4")
			)
			(pin input line
				(at -15.24 0 0)
				(length 2.54)
				(name "CLKA")
				(number "9")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "SEL")
				(number "24")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "V_{CCA}")
				(number "5")
			)
			(pin passive line
				(at -5.08 -25.4 90)
				(length 2.54)
				(name "EPAD")
				(number "25")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VCC_{B1}")
				(number "17")
			)
			(pin power_in line
				(at 7.62 25.4 270)
				(length 2.54)
				(name "VCC_{B0}")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "DAT0_{B0}")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "DAT1_{B0}")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "DAT2_{B0}")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "DAT3_{B0}")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "CMD_{B0}")
				(number "20")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "CLK_{B0}")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "DAT0_{B1}")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "DAT1_{B1}")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "DAT2_{B1}")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "DAT3_{B1}")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "CMD_{B1}")
				(number "12")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "CLK_{B1}")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "74LVCH2T45DC"
		(extends "74LVC2T45DC")
		(property "Reference" "U"
			(at 6.35 -11.43 0)
		)
		(property "Value" "74LVCH2T45DC"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_SO:VSSOP-8_2.3x2mm_P0.5mm"
			(at 0 -21.59 0)
		)
		(property "Datasheet" "https://assets.nexperia.com/documents/data-sheet/74LVC_LVCH2T45.pdf"
			(at 6.35 -6.35 0)
		)
		(property "Description" "Dual supply translating transceiver with bus-hold for unused/floating inputs, 3-state, 2-bit, VSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VSSOP*2.3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "SN74LV1T125DBV"
		(extends "SN74LV1T125DCK")
		(property "Reference" "U"
			(at 5.08 6.35 0)
		)
		(property "Value" "SN74LV1T125DBV"
			(at 5.08 3.81 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-5"
			(at 0 -24.13 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/sn74lv1t125.pdf"
			(at 0 -21.59 0)
		)
		(property "Description" "Single Power Supply, Single Buffer Gate with 3-State Output, CMOS Logic Level Shifter Level Shifter, SOT-23-5"
			(at 0 0 0)
		)
		(property "ki_keywords" "single buffer level shift"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23*"
			(at 0 0 0)
		)
	)
	(symbol "TCA9517D"
		(extends "TCA9517ADGK")
		(property "Reference" "U"
			(at -10.16 11.43 0)
		)
		(property "Value" "TCA9517D"
			(at 1.27 -11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/tca9517.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "Level-Translating I2C Bus Buffer/Repeater With Enable Function, SOIC-8"
			(at 0 -22.86 0)
		)
		(property "ki_keywords" "I2C buffer repeater"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*8*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "TXB0101DCK"
		(extends "TXB0101DBV")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TXB0101DCK"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0101.pdf"
			(at 0 -0.762 0)
		)
		(property "Description" "1-Bit Bidirectional Voltage-Level Translator With Auto Direction Sensing and ±15-kV ESD Protection, SC-70-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional voltage level translator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SC?70?6*"
			(at 0 0 0)
		)
	)
	(symbol "TXB0101DRL"
		(extends "TXB0101DBV")
		(property "Reference" "U"
			(at -6.35 8.89 0)
		)
		(property "Value" "TXB0101DRL"
			(at 3.81 8.89 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0101.pdf"
			(at 0 -0.762 0)
		)
		(property "Description" "1-Bit Bidirectional Voltage-Level Translator With Auto Direction Sensing and ±15-kV ESD Protection, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "bidirectional voltage level translator"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TXB0304RUT"
		(extends "TXB0104RUT")
		(property "Reference" "U"
			(at -6.35 16.51 0)
		)
		(property "Value" "TXB0304RUT"
			(at 3.81 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:Texas_R-PUQFN-N12"
			(at 0 -19.05 0)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/txb0304.pdf"
			(at 2.794 2.413 0)
		)
		(property "Description" "4-Bit Bidirectional Voltage-Level Translator, Auto Direction Sensing, 0.9 - 3.6V APort, 0.9 - 3.6V BPort, Active High Output Enable, Texas_PUQFN-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Texas*R*PUQFN*N12*"
			(at 0 0 0)
		)
	)
	(symbol "TXS0101DCK"
		(extends "TXS0101DBV")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "TXS0101DCK"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/txs0101.pdf"
			(at 0 -21.59 0)
		)
		(property "Description" "1-Bit Bidirectional Voltage-Level Shifter for Open-Drain and Push-Pull Application, SOT-363"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?363*"
			(at 0 0 0)
		)
	)
	(symbol "TXS0101DRL"
		(extends "TXS0101DBV")
		(property "Reference" "U"
			(at -6.35 13.97 0)
		)
		(property "Value" "TXS0101DRL"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-563"
			(at 1.27 -8.89 0)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/txs0101.pdf"
			(at 0 -21.59 0)
		)
		(property "Description" "1-Bit Bidirectional Voltage-Level Shifter for Open-Drain and Push-Pull Application, SOT-563"
			(at 0 0 0)
		)
		(property "ki_keywords" "Level-Shifter CMOS-TTL-Translation"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?563*"
			(at 0 0 0)
		)
	)
	(symbol "TXS0104ED"
		(extends "TXS0104EPW")
		(property "Reference" "U"
			(at -7.62 11.43 0)
		)
		(property "Value" "TXS0104ED"
			(at 3.81 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 1.27 -11.43 0)
		)
		(property "Datasheet" "www.ti.com/lit/ds/symlink/txs0104e.pdf"
			(at 1.27 -13.97 0)
		)
		(property "Description" "Bidirectional  level-shifting voltage translator, SOIC-14"
			(at 1.27 -16.51 0)
		)
		(property "ki_keywords" "4-bit"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
)
