(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "GAL16V8"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "GAL16V8"
			(at 1.27 16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Programmable Logic Array, DIP-20/SOIC-20/PLCC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "GAL PLD 16V8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SOIC* SO* PLCC*"
			(at 0 0 0)
		)
		(symbol "GAL16V8_0_0"
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
		)
		(symbol "GAL16V8_0_1")
		(symbol "GAL16V8_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "I1/CLK")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "I2")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "I3")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "I4")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "I5")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "I6")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "I7")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "I8")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "I9")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "I10/~{OE}")
				(number "11")
			)
			(pin tri_state line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "IO1")
				(number "19")
			)
			(pin tri_state line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "IO2")
				(number "18")
			)
			(pin tri_state line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "I03")
				(number "17")
			)
			(pin tri_state line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "IO4")
				(number "16")
			)
			(pin tri_state line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "IO5")
				(number "15")
			)
			(pin tri_state line
				(at 12.7 0 180)
				(length 3.81)
				(name "IO6")
				(number "14")
			)
			(pin tri_state line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "IO7")
				(number "13")
			)
			(pin tri_state line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "IO8")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAL16L8"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 16.51 0)
		)
		(property "Value" "PAL16L8"
			(at 1.27 16.51 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Programmable Logic Array, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "PAL PLD 16L8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PAL16L8_0_0"
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
		)
		(symbol "PAL16L8_0_1")
		(symbol "PAL16L8_1_1"
			(pin input line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "I1")
				(number "1")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "I2")
				(number "2")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "I3")
				(number "3")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "I4")
				(number "4")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "I5")
				(number "5")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "I6")
				(number "6")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "I7")
				(number "7")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "I8")
				(number "8")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "I9")
				(number "9")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "I10")
				(number "11")
			)
			(pin tri_state inverted
				(at 12.7 12.7 180)
				(length 5.08)
				(name "IO1")
				(number "19")
			)
			(pin tri_state inverted
				(at 12.7 10.16 180)
				(length 5.08)
				(name "IO2")
				(number "18")
			)
			(pin tri_state inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "I03")
				(number "17")
			)
			(pin tri_state inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "IO4")
				(number "16")
			)
			(pin tri_state inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "IO5")
				(number "15")
			)
			(pin tri_state inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "IO6")
				(number "14")
			)
			(pin tri_state inverted
				(at 12.7 -2.54 180)
				(length 5.08)
				(name "IO7")
				(number "13")
			)
			(pin tri_state inverted
				(at 12.7 -5.08 180)
				(length 5.08)
				(name "IO8")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAL20"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.684 16.51 0)
		)
		(property "Value" "PAL20"
			(at 10.16 16.51 0)
		)
		(property "Footprint" ""
			(at 0 1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 1.27 0)
		)
		(property "Description" "generic 20-pin Programmable Array Logic (PAL) device"
			(at 0 0 0)
		)
		(property "ki_keywords" "logic programmable PAL"
			(at 0 0 0)
		)
		(symbol "PAL20_0_1")
		(symbol "PAL20_1_1"
			(pin passive line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "OD/CLK")
				(number "1")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "I0")
				(number "2")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "I1")
				(number "3")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "I2")
				(number "4")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 3.81)
				(name "I3")
				(number "5")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "I4")
				(number "6")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "I5")
				(number "7")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "I6")
				(number "8")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "I7")
				(number "9")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 3.81)
				(name "VCC")
				(number "20")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "CLK/OD")
				(number "11")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "O0/LR")
				(number "19")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "O1/A0")
				(number "18")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "O2/A1")
				(number "17")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(name "O3/A2")
				(number "16")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "A0/O0")
				(number "15")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "A1/O1")
				(number "14")
			)
			(pin passive line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "A2/O2")
				(number "13")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "LR/O3")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAL20L8"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 21.59 0)
		)
		(property "Value" "PAL20L8"
			(at 1.27 21.59 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Programmable Logic Array, DIP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "PAL PLD 20L8"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PAL20L8_0_0"
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
		)
		(symbol "PAL20L8_0_1")
		(symbol "PAL20L8_1_1"
			(pin input line
				(at -12.7 17.78 0)
				(length 3.81)
				(name "I1")
				(number "1")
			)
			(pin input line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "I2")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "I3")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "I4")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "I5")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "I6")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "I7")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "I8")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "I9")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "I10")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "I11")
				(number "11")
			)
			(pin input line
				(at -12.7 -10.16 0)
				(length 3.81)
				(name "I13")
				(number "13")
			)
			(pin input line
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "I14")
				(number "14")
			)
			(pin input line
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "I23")
				(number "23")
			)
			(pin tri_state inverted
				(at 12.7 17.78 180)
				(length 5.08)
				(name "IO22")
				(number "22")
			)
			(pin tri_state inverted
				(at 12.7 15.24 180)
				(length 5.08)
				(name "IO21")
				(number "21")
			)
			(pin tri_state inverted
				(at 12.7 12.7 180)
				(length 5.08)
				(name "I020")
				(number "20")
			)
			(pin tri_state inverted
				(at 12.7 10.16 180)
				(length 5.08)
				(name "IO19")
				(number "19")
			)
			(pin tri_state inverted
				(at 12.7 7.62 180)
				(length 5.08)
				(name "IO18")
				(number "18")
			)
			(pin tri_state inverted
				(at 12.7 5.08 180)
				(length 5.08)
				(name "IO17")
				(number "17")
			)
			(pin tri_state inverted
				(at 12.7 2.54 180)
				(length 5.08)
				(name "IO16")
				(number "16")
			)
			(pin tri_state inverted
				(at 12.7 0 180)
				(length 5.08)
				(name "IO15")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAL20RS10"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -8.89 19.05 0)
		)
		(property "Value" "PAL20RS10"
			(at 5.08 19.05 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Programmable Logic Array, DIP-24 (Narrow)"
			(at 0 0 0)
		)
		(property "ki_keywords" "PAL PLD 20RS10"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PAL20RS10_0_1")
		(symbol "PAL20RS10_1_1"
			(pin input line
				(at -12.7 15.24 0)
				(length 3.81)
				(name "I0")
				(number "2")
			)
			(pin input line
				(at -12.7 12.7 0)
				(length 3.81)
				(name "I1")
				(number "3")
			)
			(pin input line
				(at -12.7 10.16 0)
				(length 3.81)
				(name "I2")
				(number "4")
			)
			(pin input line
				(at -12.7 7.62 0)
				(length 3.81)
				(name "I3")
				(number "5")
			)
			(pin input line
				(at -12.7 5.08 0)
				(length 3.81)
				(name "I4")
				(number "6")
			)
			(pin input line
				(at -12.7 2.54 0)
				(length 3.81)
				(name "I5")
				(number "7")
			)
			(pin input line
				(at -12.7 0 0)
				(length 3.81)
				(name "I6")
				(number "8")
			)
			(pin input line
				(at -12.7 -2.54 0)
				(length 3.81)
				(name "I7")
				(number "9")
			)
			(pin input line
				(at -12.7 -5.08 0)
				(length 3.81)
				(name "I8")
				(number "10")
			)
			(pin input line
				(at -12.7 -7.62 0)
				(length 3.81)
				(name "I9")
				(number "11")
			)
			(pin input clock
				(at -12.7 -12.7 0)
				(length 3.81)
				(name "CLK")
				(number "1")
			)
			(pin input inverted
				(at -12.7 -15.24 0)
				(length 3.81)
				(name "~{OE}")
				(number "13")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 3.81)
				(name "O0")
				(number "23")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 3.81)
				(name "O1")
				(number "22")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 3.81)
				(name "O2")
				(number "21")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 3.81)
				(name "O3")
				(number "20")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 3.81)
				(name "O4")
				(number "19")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 3.81)
				(name "O5")
				(number "18")
			)
			(pin output line
				(at 12.7 0 180)
				(length 3.81)
				(name "O6")
				(number "17")
			)
			(pin output line
				(at 12.7 -2.54 180)
				(length 3.81)
				(name "O7")
				(number "16")
			)
			(pin output line
				(at 12.7 -5.08 180)
				(length 3.81)
				(name "O8")
				(number "15")
			)
			(pin output line
				(at 12.7 -7.62 180)
				(length 3.81)
				(name "O9")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PAL24"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.938 17.526 0)
		)
		(property "Value" "PAL24"
			(at 9.906 17.526 0)
		)
		(property "Footprint" ""
			(at 0 -1.27 0)
		)
		(property "Datasheet" "~"
			(at 0 -1.27 0)
		)
		(property "Description" "generic 24-pin Programmable Array Logic (PAL) device"
			(at 0 0 0)
		)
		(property "ki_keywords" "logic programmable PAL"
			(at 0 0 0)
		)
		(symbol "PAL24_0_1")
		(symbol "PAL24_1_1"
			(pin passive line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "OD/CLK")
				(number "1")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "I0")
				(number "2")
			)
			(pin passive line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "I1")
				(number "3")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "I2")
				(number "4")
			)
			(pin passive line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "I3")
				(number "5")
			)
			(pin passive line
				(at -15.24 0 0)
				(length 3.81)
				(name "I4")
				(number "6")
			)
			(pin passive line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "I5")
				(number "7")
			)
			(pin passive line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "I6")
				(number "8")
			)
			(pin passive line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "I7")
				(number "9")
			)
			(pin passive line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "I8")
				(number "10")
			)
			(pin passive line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "I9")
				(number "11")
			)
			(pin passive line
				(at 0 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "24")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "CLK/OD")
				(number "13")
			)
			(pin passive line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "O0/LR")
				(number "23")
			)
			(pin passive line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "O1/A0")
				(number "22")
			)
			(pin passive line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "O2/A1")
				(number "21")
			)
			(pin passive line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "O3/A2")
				(number "20")
			)
			(pin passive line
				(at 15.24 0 180)
				(length 3.81)
				(name "O4/NC")
				(number "19")
			)
			(pin passive line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "NC/O0")
				(number "18")
			)
			(pin passive line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "A2/O1")
				(number "17")
			)
			(pin passive line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "A1/O2")
				(number "16")
			)
			(pin passive line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "A0/O3")
				(number "15")
			)
			(pin passive line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "LR/O4")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PEEL22CV10AP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "PEEL22CV10AP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DIP:DIP-24_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alldatasheet.com/datasheet-pdf/pdf/149182/ANACHIP/PEEL22CV10AP-15L.html"
			(at 0 0 0)
		)
		(property "Description" "Not in Production, CMOS Programmable Electrically Erasable Logic Device, DIP-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "PLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PEEL22CV10AP_1_0"
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VCC")
				(number "24")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "12")
			)
		)
		(symbol "PEEL22CV10AP_1_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "I1/CLK")
				(number "1")
			)
			(pin input line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "I2")
				(number "2")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "I3")
				(number "3")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "I4")
				(number "4")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "I5")
				(number "5")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "I6")
				(number "6")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "I7")
				(number "7")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "I8")
				(number "8")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "I9")
				(number "9")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "I10")
				(number "10")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "I11")
				(number "11")
			)
			(pin tri_state line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "IO23")
				(number "23")
			)
			(pin tri_state line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "IO22")
				(number "22")
			)
			(pin tri_state line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "IO21")
				(number "21")
			)
			(pin tri_state line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "IO20")
				(number "20")
			)
			(pin tri_state line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "IO19")
				(number "19")
			)
			(pin tri_state line
				(at 15.24 0 180)
				(length 3.81)
				(name "IO18")
				(number "18")
			)
			(pin tri_state line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "IO17")
				(number "17")
			)
			(pin tri_state line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "IO16")
				(number "16")
			)
			(pin tri_state line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "IO15")
				(number "15")
			)
			(pin tri_state line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "IO14")
				(number "14")
			)
			(pin input line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "I13")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PEEL22CV10AS"
		(extends "PEEL22CV10AP")
		(property "Reference" "U"
			(at 0 0 0)
		)
		(property "Value" "PEEL22CV10AS"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.alldatasheet.com/datasheet-pdf/download/149182/ANACHIP/PEEL22CV10AP-15L.html"
			(at 0 0 0)
		)
		(property "Description" "Not in Production, CMOS Programmable Electrically Erasable Logic Device, SOIC-24W"
			(at 0 0 0)
		)
		(property "ki_keywords" "PLD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*7.5x15.4mm*P1.27mm*"
			(at 0 0 0)
		)
	)
)
