(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "CY7C68013A-56LTX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 49.53 0)
		)
		(property "Value" "CY7C68013A-56LTX"
			(at 11.43 49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_8x8mm_P0.5mm_EP4.5x5.2mm_ThermalVias_TopTented"
			(at 0 -59.69 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/138911/download"
			(at 0 5.08 0)
		)
		(property "Description" "CYPRESS FX2LP USB Microcontroller, 48MHz 8051, 16KB RAM, USB 2.0, I2C, QFN-56"
			(at 0 0 0)
		)
		(property "ki_keywords" "FX2LP 8-bit USB MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CY7C68013A-56LTX_0_1")
		(symbol "CY7C68013A-56LTX_1_1"
			(pin output line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "XTALOUT")
				(number "4")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "XTALIN")
				(number "5")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "~{RESET}")
				(number "42")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "WAKEUP")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "D+")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "D-")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "SDA")
				(number "16")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "SCL")
				(number "15")
			)
			(pin input line
				(at -10.16 -50.8 90)
				(length 2.54)
				(name "RESERVED")
				(number "14")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "3")
			)
			(pin passive line
				(at -5.08 50.8 270)
				(length 2.54)
				(hide yes)
				(name "AVCC")
				(number "7")
			)
			(pin passive line
				(at -5.08 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "10")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 2.54)
				(name "AGND")
				(number "6")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "27")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "32")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "43")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "55")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "56")
			)
			(pin input line
				(at 5.08 -50.8 90)
				(length 2.54)
				(name "EP")
				(number "57")
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "PB0/FD0")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "PB1/FD1")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PB2/FD2")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PB3/FD3")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PB4/FD4")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB5/FD5")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB6/FD6")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB7/FD7")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PD0/FD8")
				(number "45")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PD1/FD9")
				(number "46")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PD2/FD10")
				(number "47")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PD3/FD11")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PD4/FD12")
				(number "49")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PD5/FD13")
				(number "50")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PD6/FD14")
				(number "51")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PD7/FD15")
				(number "52")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "RDY0/SLRD")
				(number "1")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "RDY1/SLWR")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "IFCLK")
				(number "13")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "CLKOUT")
				(number "54")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "CTL0/FLAGA")
				(number "29")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "CTL1/FLAGB")
				(number "30")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "CTL2/FLAGC")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PA0/~{INT0}")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PA1/~{INT1}")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PA2/SLOE")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PA3/WU2")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PA4/FIOADDR0")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PA5/FIOADDR1")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PA6/PKTEND")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PA7/FLAGD/~{SLCS}")
				(number "40")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY7C68013A-56PVX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 49.53 0)
		)
		(property "Value" "CY7C68013A-56PVX"
			(at 12.7 49.53 0)
		)
		(property "Footprint" "Package_SO:SSOP-56_7.5x18.5mm_P0.635mm"
			(at 0 -58.42 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/138911/download"
			(at 0 5.08 0)
		)
		(property "Description" "CYPRESS FX2LP USB Microcontroller, 48MHz 8051, 16KB RAM, USB 2.0, I2C, SSOP-56"
			(at 0 0 0)
		)
		(property "ki_keywords" "FX2LP 8-bit USB MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*7.5x18.5mm*P0.635mm*"
			(at 0 0 0)
		)
		(symbol "CY7C68013A-56PVX_0_1")
		(symbol "CY7C68013A-56PVX_1_1"
			(pin output line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "XTALOUT")
				(number "11")
			)
			(pin input line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "XTALIN")
				(number "12")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "~{RESET}")
				(number "49")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "WAKEUP")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "D+")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "D-")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "SDA")
				(number "23")
			)
			(pin input line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "SCL")
				(number "22")
			)
			(pin input line
				(at -10.16 -50.8 90)
				(length 2.54)
				(name "RESERVED")
				(number "21")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "10")
			)
			(pin passive line
				(at -5.08 50.8 270)
				(length 2.54)
				(hide yes)
				(name "AVCC")
				(number "14")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 2.54)
				(name "AGND")
				(number "13")
			)
			(pin passive line
				(at -5.08 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "AGND")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "18")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "24")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "34")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "39")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "50")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "48")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 2.54)
				(name "PB0/FD0")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "PB1/FD1")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PB2/FD2")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PB3/FD3")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PB4/FD4")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB5/FD5")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB6/FD6")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB7/FD7")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PD0/FD8")
				(number "52")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PD1/FD9")
				(number "53")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PD2/FD10")
				(number "54")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PD3/FD11")
				(number "55")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PD4/FD12")
				(number "56")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PD5/FD13")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PD6/FD14")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PD7/FD15")
				(number "3")
			)
			(pin input line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "RDY0/SLRD")
				(number "8")
			)
			(pin input line
				(at 17.78 0 180)
				(length 2.54)
				(name "RDY1/SLWR")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "IFCLK")
				(number "20")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "CLKOUT")
				(number "5")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "CTL0/FLAGA")
				(number "36")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "CTL1/FLAGB")
				(number "37")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "CTL2/FLAGC")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PA0/~{INT0}")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PA1/~{INT1}")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PA2/SLOE")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PA3/WU2")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PA4/FIOADDR0")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PA5/FIOADDR1")
				(number "45")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PA6/PKTEND")
				(number "46")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PA7/FLAGD/~{SLCS}")
				(number "47")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY8C4245AXI-M445"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 43.18 0)
		)
		(property "Value" "CY8C4245AXI-M445"
			(at 20.32 43.18 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "https://www.cypress.com/file/139956/download"
			(at -15.24 35.56 0)
		)
		(property "Description" "PSoC 4200M series, 48MHz CPU, 32KB Flash, 4KB SRAM, 64-TQFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cypress Microcontroller Arm CapSense LCD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "CY8C4245AXI-M445_0_1")
		(symbol "CY8C4245AXI-M445_1_1"
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "P0.0")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "P0.1")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "P0.2")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "P0.3")
				(number "42")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "P0.4")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "P0.5")
				(number "44")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "P0.6")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "P0.7")
				(number "46")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "P1.0")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "P1.1")
				(number "59")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "P1.2")
				(number "60")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "P1.3")
				(number "61")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "P1.4")
				(number "62")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "P1.5")
				(number "63")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "P1.6")
				(number "64")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "P1.7/VREF")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "P2.0")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "P2.1")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "P2.2")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "P2.3")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "P2.4")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "P2.5")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "P2.6")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "P2.7")
				(number "9")
			)
			(pin input line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "XRES")
				(number "47")
			)
			(pin power_out line
				(at -7.62 43.18 270)
				(length 2.54)
				(name "VCCD")
				(number "48")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDDD")
				(number "50")
			)
			(pin power_in line
				(at -2.54 -43.18 90)
				(length 2.54)
				(name "VSSD")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "56")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "57")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "11")
			)
			(pin power_in line
				(at 5.08 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "10")
			)
			(pin power_in line
				(at 10.16 43.18 270)
				(length 2.54)
				(name "VDDIO")
				(number "26")
			)
			(pin power_in line
				(at 10.16 -43.18 90)
				(length 2.54)
				(name "VSSIO")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "P3.0")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "P3.1")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "P3.2")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "P3.3")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "P3.4")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "P3.5")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "P3.6")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "P3.7")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "P4.0")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "P4.1")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "P4.2")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "P4.3")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "P4.4")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "P4.5")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "P4.6")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "P5.0")
				(number "51")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "P5.1")
				(number "52")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "P5.2")
				(number "53")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "P5.3")
				(number "54")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "P5.5")
				(number "55")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "P6.0")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "P6.1")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "P6.2")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "P6.4")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "P6.5")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "P7.0")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 2.54)
				(name "P7.1")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY8C4245AZI-M445"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 43.18 0)
		)
		(property "Value" "CY8C4245AZI-M445"
			(at 20.32 43.18 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "https://www.cypress.com/file/139956/download"
			(at -15.24 35.56 0)
		)
		(property "Description" "PSoC 4200M series, 48MHz CPU, 32KB Flash, 4KB SRAM, 64-TQFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cypress Microcontroller Arm CapSense LCD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "CY8C4245AZI-M445_0_1")
		(symbol "CY8C4245AZI-M445_1_1"
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "P0.0")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "P0.1")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "P0.2")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "P0.3")
				(number "42")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "P0.4")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "P0.5")
				(number "44")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "P0.6")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "P0.7")
				(number "46")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "P1.0")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "P1.1")
				(number "59")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "P1.2")
				(number "60")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "P1.3")
				(number "61")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "P1.4")
				(number "62")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "P1.5")
				(number "63")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "P1.6")
				(number "64")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "P1.7/VREF")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "P2.0")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "P2.1")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "P2.2")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "P2.3")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "P2.4")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "P2.5")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "P2.6")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "P2.7")
				(number "9")
			)
			(pin input line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "XRES")
				(number "47")
			)
			(pin power_out line
				(at -7.62 43.18 270)
				(length 2.54)
				(name "VCCD")
				(number "48")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 2.54)
				(name "VDDD")
				(number "50")
			)
			(pin power_in line
				(at -2.54 -43.18 90)
				(length 2.54)
				(name "VSSD")
				(number "49")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "56")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "57")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 2.54)
				(name "VDDA")
				(number "11")
			)
			(pin power_in line
				(at 5.08 -43.18 90)
				(length 2.54)
				(name "VSSA")
				(number "10")
			)
			(pin power_in line
				(at 10.16 43.18 270)
				(length 2.54)
				(name "VDDIO")
				(number "26")
			)
			(pin power_in line
				(at 10.16 -43.18 90)
				(length 2.54)
				(name "VSSIO")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "P3.0")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "P3.1")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "P3.2")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "P3.3")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "P3.4")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "P3.5")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "P3.6")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "P3.7")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "P4.0")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "P4.1")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "P4.2")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "P4.3")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "P4.4")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "P4.5")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "P4.6")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "P5.0")
				(number "51")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "P5.1")
				(number "52")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "P5.2")
				(number "53")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "P5.3")
				(number "54")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "P5.5")
				(number "55")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "P6.0")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "P6.1")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "P6.2")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "P6.4")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "P6.5")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "P7.0")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 2.54)
				(name "P7.1")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY8C4xx7LQI-4xx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 39.37 0)
		)
		(property "Value" "CY8C4xx7LQI-4xx"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/137466/download"
			(at 1.27 -2.54 0)
		)
		(property "Description" "Programmable System-on-Chip With Bluetooth Low Energy, 24/48-MHz ARM® Cortex®-M0 , 56-QFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PSOC BLE CY8 CY8C4 ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "CY8C4xx7LQI-4xx_1_0")
		(symbol "CY8C4xx7LQI-4xx_1_1"
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "P0.0")
				(number "19")
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "P0.1")
				(number "20")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "P0.2")
				(number "21")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "P0.3")
				(number "22")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "P0.4")
				(number "24")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "P0.5")
				(number "25")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "P0.6")
				(number "26")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "P0.7")
				(number "27")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "P1.0")
				(number "28")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "P1.1")
				(number "29")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "P1.2")
				(number "30")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "P1.3")
				(number "31")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "P1.4")
				(number "32")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "P1.5")
				(number "33")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "P1.6")
				(number "34")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "P1.7")
				(number "35")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "P2.0")
				(number "37")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "P2.1")
				(number "38")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "P2.2")
				(number "39")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "P2.3")
				(number "40")
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "P2.4")
				(number "41")
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "P2.5")
				(number "42")
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "P2.6")
				(number "43")
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "P2.7")
				(number "44")
			)
			(pin power_out line
				(at -15.24 43.18 270)
				(length 5.08)
				(name "VCCD")
				(number "56")
			)
			(pin power_in line
				(at -12.7 -43.18 90)
				(length 5.08)
				(name "VSSD")
				(number "9")
			)
			(pin power_in line
				(at -10.16 43.18 270)
				(length 5.08)
				(name "VDDD")
				(number "23")
			)
			(pin power_in line
				(at -10.16 -43.18 90)
				(length 5.08)
				(name "VSSA")
				(number "55")
			)
			(pin power_in line
				(at -7.62 43.18 270)
				(length 5.08)
				(name "VDDD")
				(number "1")
			)
			(pin power_in line
				(at -7.62 -43.18 90)
				(length 5.08)
				(name "GND_EP")
				(number "57")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 5.08)
				(name "VDDA")
				(number "46")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 5.08)
				(name "VDDA")
				(number "36")
			)
			(pin input line
				(at 0 -43.18 90)
				(length 5.08)
				(name "XTAL24I")
				(number "16")
			)
			(pin output line
				(at 2.54 -43.18 90)
				(length 5.08)
				(name "XTAL24O")
				(number "17")
			)
			(pin passive line
				(at 5.08 43.18 270)
				(length 5.08)
				(name "VREF")
				(number "45")
			)
			(pin power_in line
				(at 10.16 43.18 270)
				(length 5.08)
				(name "VDDR")
				(number "18")
			)
			(pin bidirectional line
				(at 10.16 -43.18 90)
				(length 5.08)
				(name "XTAL32O/P6.0")
				(number "2")
			)
			(pin power_in line
				(at 12.7 43.18 270)
				(length 5.08)
				(name "VDDR")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -43.18 90)
				(length 5.08)
				(name "XTAL32I/P6.1")
				(number "3")
			)
			(pin power_in line
				(at 15.24 43.18 270)
				(length 5.08)
				(name "VDDR")
				(number "14")
			)
			(pin power_in line
				(at 17.78 43.18 270)
				(length 5.08)
				(name "VDDR")
				(number "10")
			)
			(pin input inverted
				(at 35.56 25.4 180)
				(length 5.08)
				(name "XRES")
				(number "4")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "P5.1")
				(number "8")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "P5.0")
				(number "7")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "P4.1")
				(number "6")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "P4.0")
				(number "5")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "P3.7")
				(number "54")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "P3.6")
				(number "53")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "P3.5")
				(number "52")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "P3.4")
				(number "51")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "P3.3")
				(number "50")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "P3.2")
				(number "49")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "P3.1")
				(number "48")
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "P3.0")
				(number "47")
			)
			(pin output line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "ANT")
				(number "12")
			)
			(pin power_in line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "GANT2")
				(number "13")
			)
			(pin power_in line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "GANT1")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CYBL10563-68FNXIT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 39.37 0)
		)
		(property "Value" "CYBL10563-68FNXIT"
			(at 0 2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/documentation/datasheets/cybl10x6x-family-datasheet-programmable-radio-chip-bluetooth-low-energy"
			(at 1.27 -2.54 0)
		)
		(property "Description" "68-WLCSP, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, BLE 4.1, CAP-SENSE W/ GESTURES, 2 SCB, 4 TCPWM, I2S, 1 PWM , LCD, 1MSPS 12-BIT SAR"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PROC BLE CY8BL ARM CORTEX M0 BLUETOOTH WLCSP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*"
			(at 0 0 0)
		)
		(symbol "CYBL10563-68FNXIT_1_0")
		(symbol "CYBL10563-68FNXIT_1_1"
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "P0.0")
				(number "J2")
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "P0.1")
				(number "H2")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "P0.2")
				(number "G3")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "P0.3")
				(number "F3")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "P0.4")
				(number "J1")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "P0.5")
				(number "H1")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "P0.6")
				(number "G1")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "P0.7")
				(number "F2")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "P1.0")
				(number "F4")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "P1.1")
				(number "F5")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "P1.2")
				(number "E1")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "P1.3")
				(number "E2")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "P1.4")
				(number "E3")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "P1.5")
				(number "E4")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "P1.6")
				(number "E5")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "P1.7")
				(number "D1")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "P2.0")
				(number "D3")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "P2.1")
				(number "D4")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "P2.2")
				(number "C2")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "P2.3")
				(number "B1")
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "P2.4")
				(number "E6")
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "P2.5")
				(number "D5")
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "P2.6")
				(number "C3")
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "P2.7")
				(number "B3")
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 5.08)
				(name "XTAL32O/P6.0")
				(number "B8")
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 5.08)
				(name "XTAL32I/P6.1")
				(number "B7")
			)
			(pin power_in line
				(at -25.4 -55.88 90)
				(length 5.08)
				(name "VSSD")
				(number "A5")
			)
			(pin power_in line
				(at -22.86 -55.88 90)
				(length 5.08)
				(name "VSSD")
				(number "D6")
			)
			(pin power_in line
				(at -20.32 -55.88 90)
				(length 5.08)
				(name "VSSD")
				(number "E8")
			)
			(pin power_in line
				(at -17.78 -55.88 90)
				(length 5.08)
				(name "VSSD")
				(number "F1")
			)
			(pin power_out line
				(at -15.24 43.18 270)
				(length 5.08)
				(name "VCCD")
				(number "A7")
			)
			(pin power_in line
				(at -15.24 -55.88 90)
				(length 5.08)
				(name "VSSD")
				(number "G4")
			)
			(pin power_in line
				(at -10.16 43.18 270)
				(length 5.08)
				(name "VDDD")
				(number "A8")
			)
			(pin power_in line
				(at -7.62 43.18 270)
				(length 5.08)
				(name "VDDD")
				(number "G2")
			)
			(pin power_in line
				(at -7.62 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "A2")
			)
			(pin power_in line
				(at -5.08 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "A6")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 5.08)
				(name "VDDA")
				(number "D2")
			)
			(pin bidirectional line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "B2")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 5.08)
				(name "VDDA")
				(number "36")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "C1")
			)
			(pin passive line
				(at 5.08 43.18 270)
				(length 5.08)
				(name "VREF")
				(number "A1")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 5.08)
				(name "GND_EP")
				(number "57")
			)
			(pin power_in line
				(at 12.7 43.18 270)
				(length 5.08)
				(name "VDDR")
				(number "F8")
			)
			(pin power_in line
				(at 12.7 -55.88 90)
				(length 5.08)
				(name "VSSR")
				(number "F6")
			)
			(pin power_in line
				(at 15.24 43.18 270)
				(length 5.08)
				(name "VDDR")
				(number "J3")
			)
			(pin power_in line
				(at 15.24 -55.88 90)
				(length 5.08)
				(name "VSSR")
				(number "F7")
			)
			(pin power_in line
				(at 17.78 43.18 270)
				(length 5.08)
				(name "VDDR")
				(number "J4")
			)
			(pin power_in line
				(at 17.78 -55.88 90)
				(length 5.08)
				(name "VSSR")
				(number "G5")
			)
			(pin power_in line
				(at 20.32 -55.88 90)
				(length 5.08)
				(name "VSSR")
				(number "G6")
			)
			(pin power_in line
				(at 22.86 -55.88 90)
				(length 5.08)
				(name "VSSR")
				(number "G8")
			)
			(pin power_in line
				(at 25.4 -55.88 90)
				(length 5.08)
				(name "VSSR")
				(number "H5")
			)
			(pin power_in line
				(at 27.94 -55.88 90)
				(length 5.08)
				(name "VSSR")
				(number "H6")
			)
			(pin no_connect line
				(at 30.48 30.48 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "J7")
			)
			(pin input inverted
				(at 35.56 25.4 180)
				(length 5.08)
				(name "XRES")
				(number "C7")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "P3.7")
				(number "A4")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "P3.6")
				(number "B6")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "P3.5")
				(number "B5")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "P3.4")
				(number "B4")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "P3.3")
				(number "A3")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "P3.2")
				(number "C6")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "P3.1")
				(number "C5")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "P3.0")
				(number "C4")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "P5.1")
				(number "E7")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "P5.0")
				(number "D8")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "P4.1")
				(number "D7")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "P4.0")
				(number "C8")
			)
			(pin output line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "ANT")
				(number "H7")
			)
			(pin power_in line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "GANT2")
				(number "G7")
			)
			(pin power_in line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "GANT1")
				(number "11")
			)
			(pin output line
				(at 35.56 -38.1 180)
				(length 5.08)
				(name "XTAL24O")
				(number "H3")
			)
			(pin input line
				(at 35.56 -40.64 180)
				(length 5.08)
				(name "XTAL24I")
				(number "H4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CYBL10x6x-56LQxx"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 39.37 0)
		)
		(property "Value" "CYBL10x6x-56LQxx"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/documentation/datasheets/cybl10x6x-family-datasheet-programmable-radio-chip-bluetooth-low-energy"
			(at 1.27 -2.54 0)
		)
		(property "Description" "Programmable Radio-on-Chip With Bluetooth Low Energy, 48-MHz ARM® Cortex®-M0 , 56-QFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PROC BLE CY8BL ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "CYBL10x6x-56LQxx_1_0")
		(symbol "CYBL10x6x-56LQxx_1_1"
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 5.08)
				(name "P0.0")
				(number "19")
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 5.08)
				(name "P0.1")
				(number "20")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 5.08)
				(name "P0.2")
				(number "21")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "P0.3")
				(number "22")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "P0.4")
				(number "24")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "P0.5")
				(number "25")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "P0.6")
				(number "26")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "P0.7")
				(number "27")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "P1.0")
				(number "28")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "P1.1")
				(number "29")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "P1.2")
				(number "30")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "P1.3")
				(number "31")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "P1.4")
				(number "32")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "P1.5")
				(number "33")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "P1.6")
				(number "34")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "P1.7")
				(number "35")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "P2.0")
				(number "37")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "P2.1")
				(number "38")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "P2.2")
				(number "39")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "P2.3")
				(number "40")
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "P2.4")
				(number "41")
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 5.08)
				(name "P2.5")
				(number "42")
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 5.08)
				(name "P2.6")
				(number "43")
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 5.08)
				(name "P2.7")
				(number "44")
			)
			(pin power_out line
				(at -15.24 43.18 270)
				(length 5.08)
				(name "VCCD")
				(number "56")
			)
			(pin power_in line
				(at -12.7 -43.18 90)
				(length 5.08)
				(name "VSSD")
				(number "9")
			)
			(pin power_in line
				(at -10.16 43.18 270)
				(length 5.08)
				(name "VDDD")
				(number "23")
			)
			(pin power_in line
				(at -10.16 -43.18 90)
				(length 5.08)
				(name "VSSA")
				(number "55")
			)
			(pin power_in line
				(at -7.62 43.18 270)
				(length 5.08)
				(name "VDDD")
				(number "1")
			)
			(pin power_in line
				(at -7.62 -43.18 90)
				(length 5.08)
				(name "GND_EP")
				(number "57")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 5.08)
				(name "VDDA")
				(number "46")
			)
			(pin power_in line
				(at 0 43.18 270)
				(length 5.08)
				(name "VDDA")
				(number "36")
			)
			(pin input line
				(at 0 -43.18 90)
				(length 5.08)
				(name "XTAL24I")
				(number "16")
			)
			(pin output line
				(at 2.54 -43.18 90)
				(length 5.08)
				(name "XTAL24O")
				(number "17")
			)
			(pin passive line
				(at 5.08 43.18 270)
				(length 5.08)
				(name "VREF")
				(number "45")
			)
			(pin bidirectional line
				(at 10.16 -43.18 90)
				(length 5.08)
				(name "XTAL32O/P6.0")
				(number "2")
			)
			(pin power_in line
				(at 12.7 43.18 270)
				(length 5.08)
				(name "VDDR")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 -43.18 90)
				(length 5.08)
				(name "XTAL32I/P6.1")
				(number "3")
			)
			(pin power_in line
				(at 15.24 43.18 270)
				(length 5.08)
				(name "VDDR")
				(number "15")
			)
			(pin power_in line
				(at 17.78 43.18 270)
				(length 5.08)
				(name "VDDR")
				(number "14")
			)
			(pin power_in line
				(at 20.32 43.18 270)
				(length 5.08)
				(name "VDDR")
				(number "10")
			)
			(pin input inverted
				(at 35.56 25.4 180)
				(length 5.08)
				(name "XRES")
				(number "4")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "P5.1")
				(number "8")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "P5.0")
				(number "7")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "P4.1")
				(number "6")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "P4.0")
				(number "5")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "P3.7")
				(number "54")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "P3.6")
				(number "53")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "P3.5")
				(number "52")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "P3.4")
				(number "51")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "P3.3")
				(number "50")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "P3.2")
				(number "49")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "P3.1")
				(number "48")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "P3.0")
				(number "47")
			)
			(pin output line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "ANT")
				(number "12")
			)
			(pin power_in line
				(at 35.56 -27.94 180)
				(length 5.08)
				(name "GANT2")
				(number "13")
			)
			(pin power_in line
				(at 35.56 -30.48 180)
				(length 5.08)
				(name "GANT1")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CY7C68014A-56LTX"
		(extends "CY7C68013A-56LTX")
		(property "Reference" "U"
			(at -13.97 49.53 0)
		)
		(property "Value" "CY7C68014A-56LTX"
			(at 11.43 49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_8x8mm_P0.5mm_EP4.5x5.2mm_ThermalVias_TopTented"
			(at 0 -59.69 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/138911/download"
			(at 0 5.08 0)
		)
		(property "Description" "CYPRESS FX2LP USB Microcontroller, 48MHz 8051, 16KB RAM, USB 2.0, I2C, QFN-56"
			(at 0 0 0)
		)
		(property "ki_keywords" "FX2LP 8-bit USB MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY7C68014A-56PVX"
		(extends "CY7C68013A-56PVX")
		(property "Reference" "U"
			(at -13.97 49.53 0)
		)
		(property "Value" "CY7C68014A-56PVX"
			(at 12.7 49.53 0)
		)
		(property "Footprint" "Package_SO:SSOP-56_7.5x18.5mm_P0.635mm"
			(at 0 -58.42 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/138911/download"
			(at 0 5.08 0)
		)
		(property "Description" "CYPRESS FX2LP USB Microcontroller, 48MHz 8051, 16KB RAM, USB 2.0, I2C, SSOP-56"
			(at 0 0 0)
		)
		(property "ki_keywords" "FX2LP 8-bit USB MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*7.5x18.5mm*P0.635mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4127LQI-BL453"
		(extends "CY8C4xx7LQI-4xx")
		(property "Reference" "U"
			(at -29.21 39.37 0)
		)
		(property "Value" "CY8C4127LQI-BL453"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/137466/download"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 24-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, NO UDB, CAP-SENSE W/O GESTURE, NO LCD DRIVE"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PSOC BLE CY8 CY8C4 ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4127LQI-BL473"
		(extends "CY8C4xx7LQI-4xx")
		(property "Reference" "U"
			(at -29.21 39.37 0)
		)
		(property "Value" "CY8C4127LQI-BL473"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/137466/download"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 24-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, NO UDB, NO CAP-SENSE, NO LCD DRIVE"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PSOC BLE CY8 CY8C4 ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4127LQI-BL483"
		(extends "CY8C4xx7LQI-4xx")
		(property "Reference" "U"
			(at -29.21 39.37 0)
		)
		(property "Value" "CY8C4127LQI-BL483"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/137466/download"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 24-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, NO UDB, CAP-SENSE W/O GESTURE, LCD DRIVE"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PSOC BLE CY8 CY8C4 ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4127LQI-BL493"
		(extends "CY8C4xx7LQI-4xx")
		(property "Reference" "U"
			(at -29.21 39.37 0)
		)
		(property "Value" "CY8C4127LQI-BL493"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/137466/download"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 24-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, NO UDB, CAP-SENSE W/ GESTURE, LCD DRIVE"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PSOC BLE CY8 CY8C4 ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4246AXI-M445"
		(extends "CY8C4245AXI-M445")
		(property "Reference" "U"
			(at -15.24 43.18 0)
		)
		(property "Value" "CY8C4246AXI-M445"
			(at 20.32 43.18 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "https://www.cypress.com/file/139956/download"
			(at -15.24 35.56 0)
		)
		(property "Description" "PSoC 4200M series, 48MHz CPU, 64KB Flash, 8KB SRAM, 64-TQFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cypress Microcontroller Arm CapSense LCD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4246AZI-M445"
		(extends "CY8C4245AZI-M445")
		(property "Reference" "U"
			(at -15.24 43.18 0)
		)
		(property "Value" "CY8C4246AZI-M445"
			(at 20.32 43.18 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "https://www.cypress.com/file/139956/download"
			(at -15.24 35.56 0)
		)
		(property "Description" "PSoC 4200M series, 48MHz CPU, 64KB Flash, 8KB SRAM, 64-TQFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cypress Microcontroller Arm CapSense LCD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4246AZI-M475"
		(extends "CY8C4245AZI-M445")
		(property "Reference" "U"
			(at -15.24 43.18 0)
		)
		(property "Value" "CY8C4246AZI-M475"
			(at 20.32 43.18 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "https://www.cypress.com/file/139956/download"
			(at -15.24 35.56 0)
		)
		(property "Description" "PSoC 4200M series, 48MHz CPU, 64KB Flash, 8KB SRAM, 64-TQFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cypress Microcontroller Arm IDAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4247AXI-M485"
		(extends "CY8C4245AXI-M445")
		(property "Reference" "U"
			(at -15.24 43.18 0)
		)
		(property "Value" "CY8C4247AXI-M485"
			(at 20.32 43.18 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "https://www.cypress.com/file/139956/download"
			(at -15.24 35.56 0)
		)
		(property "Description" "PSoC 4200M series, 48MHz CPU, 128KB Flash, 16KB SRAM, 64-TQFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cypress Microcontroller Arm CapSense IDAC LCD CAN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4247AZI-M475"
		(extends "CY8C4245AZI-M445")
		(property "Reference" "U"
			(at -15.24 43.18 0)
		)
		(property "Value" "CY8C4247AZI-M475"
			(at 20.32 43.18 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "https://www.cypress.com/file/139956/download"
			(at -15.24 35.56 0)
		)
		(property "Description" "PSoC 4200M series, 48MHz CPU, 128KB Flash, 16KB SRAM, 64-TQFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cypress Microcontroller Arm IDAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4247AZI-M485"
		(extends "CY8C4245AZI-M445")
		(property "Reference" "U"
			(at -15.24 43.18 0)
		)
		(property "Value" "CY8C4247AZI-M485"
			(at 20.32 43.18 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 -53.34 0)
		)
		(property "Datasheet" "https://www.cypress.com/file/139956/download"
			(at -15.24 35.56 0)
		)
		(property "Description" "PSoC 4200M series, 48MHz CPU, 128KB Flash, 16KB SRAM, 64-TQFP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Cypress Microcontroller Arm CapSense IDAC LCD CAN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4247LQI-BL453"
		(extends "CY8C4xx7LQI-4xx")
		(property "Reference" "U"
			(at -29.21 39.37 0)
		)
		(property "Value" "CY8C4247LQI-BL453"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/137466/download"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, 4 UDB, CAP-SENSE W/O GESTURE, NO LCD DRIVE"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PSOC BLE CY8 CY8C4 ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4247LQI-BL463"
		(extends "CY8C4xx7LQI-4xx")
		(property "Reference" "U"
			(at -29.21 39.37 0)
		)
		(property "Value" "CY8C4247LQI-BL463"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/137466/download"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, 4 UDB, NO CAP-SENSE, LCD DRIVE"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PSOC BLE CY8 CY8C4 ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4247LQI-BL473"
		(extends "CY8C4xx7LQI-4xx")
		(property "Reference" "U"
			(at -29.21 39.37 0)
		)
		(property "Value" "CY8C4247LQI-BL473"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/137466/download"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, 4 UDB, NO CAP-SENSE, NO LCD DRIVE"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PSOC BLE CY8 CY8C4 ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4247LQI-BL483"
		(extends "CY8C4xx7LQI-4xx")
		(property "Reference" "U"
			(at -29.21 39.37 0)
		)
		(property "Value" "CY8C4247LQI-BL483"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/137466/download"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, 4 UDB, CAP-SENSE W/O GESTURES, LCD DRIVE"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PSOC BLE CY8 CY8C4 ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4247LQI-BL493"
		(extends "CY8C4xx7LQI-4xx")
		(property "Reference" "U"
			(at -29.21 39.37 0)
		)
		(property "Value" "CY8C4247LQI-BL493"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/137466/download"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, NO UDB, CAP-SENSE W/ GESTURE, LCD DRIVE"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PSOC BLE CY8 CY8C4 ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CY8C4247LQQ-BL483"
		(extends "CY8C4xx7LQI-4xx")
		(property "Reference" "U"
			(at -29.21 39.37 0)
		)
		(property "Value" "CY8C4247LQQ-BL483"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/file/137466/download"
			(at 1.27 -2.54 0)
		)
		(property "Description" "ENGR_SAMPLE,  56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, NO UDB, CAP-SENSE W/ GESTURE, LCD DRIVE"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PSOC BLE CY8 CY8C4 ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CYBL10161-56LQXI"
		(extends "CYBL10x6x-56LQxx")
		(property "Reference" "U"
			(at -27.94 39.37 0)
		)
		(property "Value" "CYBL10161-56LQXI"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/documentation/datasheets/cybl10x6x-family-datasheet-programmable-radio-chip-bluetooth-low-energy"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, BLE 4.1, NO CAP-SENSE, 1 SCB, 2 TCPWM, NO I2S, NO PWM , NO LCD, 1MSPS 12-BIT SAR"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PROC BLE CY8BL ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CYBL10162-56LQXI"
		(extends "CYBL10x6x-56LQxx")
		(property "Reference" "U"
			(at -27.94 39.37 0)
		)
		(property "Value" "CYBL10162-56LQXI"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/documentation/datasheets/cybl10x6x-family-datasheet-programmable-radio-chip-bluetooth-low-energy"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, BLE 4.1, NO CAP-SENSE, 2 SCB, 4 TCPWM, NO I2S, 4 PWM , NO LCD, 1MSPS 12-BIT SAR"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PROC BLE CY8BL ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CYBL10163-56LQXI"
		(extends "CYBL10x6x-56LQxx")
		(property "Reference" "U"
			(at -27.94 39.37 0)
		)
		(property "Value" "CYBL10163-56LQXI"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/documentation/datasheets/cybl10x6x-family-datasheet-programmable-radio-chip-bluetooth-low-energy"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, BLE 4.1, NO CAP-SENSE, 2 SCB, 4 TCPWM, 1 I2S, NO PWM , NO LCD, 1MSPS 12-BIT SAR"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PROC BLE CY8BL ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CYBL10461-56LQXI"
		(extends "CYBL10x6x-56LQxx")
		(property "Reference" "U"
			(at -27.94 39.37 0)
		)
		(property "Value" "CYBL10461-56LQXI"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/documentation/datasheets/cybl10x6x-family-datasheet-programmable-radio-chip-bluetooth-low-energy"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, BLE 4.1, CAP-SENSE, 2 SCB, 4 TCPWM, NO I2S, NO PWM , NO LCD, 1MSPS 12-BIT SAR"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PROC BLE CY8BL ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CYBL10462-56LQXI"
		(extends "CYBL10x6x-56LQxx")
		(property "Reference" "U"
			(at -27.94 39.37 0)
		)
		(property "Value" "CYBL10462-56LQXI"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/documentation/datasheets/cybl10x6x-family-datasheet-programmable-radio-chip-bluetooth-low-energy"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, BLE 4.1, CAP-SENSE, 2 SCB, 4 TCPWM, 1 I2S, NO PWM , NO LCD, 1MSPS 12-BIT SAR"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PROC BLE CY8BL ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CYBL10463-56LQXI"
		(extends "CYBL10x6x-56LQxx")
		(property "Reference" "U"
			(at -27.94 39.37 0)
		)
		(property "Value" "CYBL10463-56LQXI"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/documentation/datasheets/cybl10x6x-family-datasheet-programmable-radio-chip-bluetooth-low-energy"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, BLE 4.1, CAP-SENSE, 2 SCB, 4 TCPWM, NO I2S, NO PWM , LCD, 1MSPS 12-BIT SAR"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PROC BLE CY8BL ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CYBL10561-56LQXI"
		(extends "CYBL10x6x-56LQxx")
		(property "Reference" "U"
			(at -27.94 39.37 0)
		)
		(property "Value" "CYBL10561-56LQXI"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/documentation/datasheets/cybl10x6x-family-datasheet-programmable-radio-chip-bluetooth-low-energy"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, BLE 4.1, CAP-SENSE W/ GESTURES, 2 SCB, 4 TCPWM, NO I2S, NO PWM , NO LCD, 1MSPS 12-BIT SAR"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PROC BLE CY8BL ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CYBL10562-56LQXI"
		(extends "CYBL10x6x-56LQxx")
		(property "Reference" "U"
			(at -27.94 39.37 0)
		)
		(property "Value" "CYBL10562-56LQXI"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/documentation/datasheets/cybl10x6x-family-datasheet-programmable-radio-chip-bluetooth-low-energy"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, BLE 4.1, CAP-SENSE W/ GESTURES, 2 SCB, 4 TCPWM, I2S, 1 PWM , NO LCD, 1MSPS 12-BIT SAR"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PROC BLE CY8BL ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CYBL10563-56LQXI"
		(extends "CYBL10x6x-56LQxx")
		(property "Reference" "U"
			(at -27.94 39.37 0)
		)
		(property "Value" "CYBL10563-56LQXI"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/documentation/datasheets/cybl10x6x-family-datasheet-programmable-radio-chip-bluetooth-low-energy"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, BLE 4.1, CAP-SENSE W/ GESTURES, 2 SCB, 4 TCPWM, I2S, 1 PWM , LCD, 1MSPS 12-BIT SAR"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PROC BLE CY8BL ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CYBL10563-56LQXQ"
		(extends "CYBL10x6x-56LQxx")
		(property "Reference" "U"
			(at -27.94 39.37 0)
		)
		(property "Value" "CYBL10563-56LQXQ"
			(at 0 2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP5.6x5.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/documentation/datasheets/cybl10x6x-family-datasheet-programmable-radio-chip-bluetooth-low-energy"
			(at 1.27 -2.54 0)
		)
		(property "Description" "56-QFN, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, BLE 4.1, CAP-SENSE W/ GESTURES, 2 SCB, 4 TCPWM, I2S, 1 PWM , LCD, 1MSPS 12-BIT SAR"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PROC BLE CY8BL ARM CORTEX M0 BLUETOOTH QFN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "CYBL10563-68FLXIT"
		(extends "CYBL10563-68FNXIT")
		(property "Reference" "U"
			(at -29.21 39.37 0)
		)
		(property "Value" "CYBL10563-68FLXIT"
			(at 0 2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.cypress.com/documentation/datasheets/cybl10x6x-family-datasheet-programmable-radio-chip-bluetooth-low-energy"
			(at 1.27 -2.54 0)
		)
		(property "Description" "68-WLCSP, 48-MHz ARM® Cortex®-M0, 128KB Flash, 16kB SRAM, BLE 4.1, CAP-SENSE W/ GESTURES, 2 SCB, 4 TCPWM, I2S, 1 PWM , LCD, 1MSPS 12-BIT SAR"
			(at 0 0 0)
		)
		(property "ki_keywords" "CYPRESS PROC BLE CY8BL ARM CORTEX M0 BLUETOOTH WLCSP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*"
			(at 0 0 0)
		)
	)
)
