(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "DA14691"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "DA14691"
			(at 0 0 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-86_6x6mm_Layout10x10_P0.55mm"
			(at 0 69.85 0)
		)
		(property "Datasheet" "https://www.dialog-semiconductor.com/sites/default/files/da1469x_datasheet_3v1.pdf"
			(at -11.43 83.82 0)
		)
		(property "Description" "Multi-core BLE 5.1 SoC series, 96-MHz/32-bit ARM Cortex-M33, 128 kB ROM, 384 kB SRAM, 4 kB OTP Memory, 16 kB cache SRAM, VFBGA-86"
			(at 0 0 0)
		)
		(property "ki_keywords" "BLE MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*6x6mm*Layout10x10*P0.55mm*"
			(at 0 0 0)
		)
		(symbol "DA14691_1_1"
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 3.81)
				(name "RFIOP")
				(number "A8")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 3.81)
				(name "QSPIF_D0")
				(number "A2")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 3.81)
				(name "QSPIF_D1")
				(number "C2")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "QSPIF_D2")
				(number "C1")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "QSPIF_D3")
				(number "B2")
			)
			(pin output line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "QSPIF_CLK")
				(number "A1")
			)
			(pin output line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "QSPIF_CS")
				(number "B1")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "P0_14/USB_P")
				(number "K6")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "P0_15/USB_M")
				(number "K7")
			)
			(pin passive line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "LY")
				(number "J1")
			)
			(pin passive line
				(at -25.4 0 0)
				(length 3.81)
				(name "LX")
				(number "K1")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "P0_22/XTAL_32K_M")
				(number "H9")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "P0_23/XTAL_32K_P")
				(number "H10")
			)
			(pin output line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "XTAL32M_M")
				(number "F10")
			)
			(pin input line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "XTAL32M_P")
				(number "F9")
			)
			(pin input line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "~{RESET}")
				(number "B8")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "P0_10/M33_SWDIO")
				(number "A3")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 3.81)
				(name "P0_11/M33_SWCLK")
				(number "B3")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 3.81)
				(name "P0_12/CMAC_SWDIO")
				(number "A4")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 3.81)
				(name "P0_13/CMAC_SWCLK")
				(number "B4")
			)
			(pin no_connect line
				(at -20.32 -45.72 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "J4")
			)
			(pin no_connect line
				(at -20.32 -48.26 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "K4")
			)
			(pin power_out line
				(at -12.7 53.34 270)
				(length 3.81)
				(name "V18F")
				(number "G1")
			)
			(pin power_out line
				(at -10.16 53.34 270)
				(length 3.81)
				(name "V18P")
				(number "G2")
			)
			(pin power_in line
				(at -7.62 53.34 270)
				(length 3.81)
				(name "VBUS")
				(number "J5")
			)
			(pin passive line
				(at -7.62 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "J3")
			)
			(pin power_in line
				(at -7.62 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "K10")
			)
			(pin passive line
				(at -7.62 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K9")
			)
			(pin power_out line
				(at -5.08 53.34 270)
				(length 3.81)
				(name "V30")
				(number "J6")
			)
			(pin passive line
				(at -5.08 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "DGND")
				(number "F4")
			)
			(pin power_in line
				(at -5.08 -53.34 90)
				(length 3.81)
				(name "DGND")
				(number "G3")
			)
			(pin passive line
				(at -5.08 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "DGND")
				(number "G4")
			)
			(pin power_out line
				(at -2.54 53.34 270)
				(length 3.81)
				(name "V18")
				(number "H2")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 3.81)
				(name "AGND")
				(number "F5")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "AGND")
				(number "G5")
			)
			(pin power_out line
				(at 0 53.34 270)
				(length 3.81)
				(name "V14")
				(number "H1")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 3.81)
				(name "VSSIOQ")
				(number "F3")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 3.81)
				(name "VSUP_RF")
				(number "A5")
			)
			(pin passive line
				(at 2.54 -53.34 90)
				(length 3.81)
				(name "XTAL32M_GND")
				(number "E10")
			)
			(pin power_out line
				(at 5.08 53.34 270)
				(length 3.81)
				(name "V12")
				(number "J2")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 3.81)
				(name "BUCK_GND")
				(number "K3")
			)
			(pin passive line
				(at 7.62 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "RF_GND")
				(number "A10")
			)
			(pin passive line
				(at 7.62 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "RF_GND")
				(number "A6")
			)
			(pin power_in line
				(at 7.62 -53.34 90)
				(length 3.81)
				(name "RF_GND")
				(number "A7")
			)
			(pin passive line
				(at 7.62 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "RF_GND")
				(number "A9")
			)
			(pin passive line
				(at 7.62 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "RF_GND")
				(number "B7")
			)
			(pin passive line
				(at 7.62 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "RF_GND")
				(number "D10")
			)
			(pin passive line
				(at 7.62 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "RF_GND")
				(number "D9")
			)
			(pin power_out line
				(at 10.16 53.34 270)
				(length 3.81)
				(name "VBAT2")
				(number "K2")
			)
			(pin power_out line
				(at 12.7 53.34 270)
				(length 3.81)
				(name "VBAT1")
				(number "K5")
			)
			(pin bidirectional line
				(at 25.4 45.72 180)
				(length 3.81)
				(name "P0_00")
				(number "D2")
			)
			(pin bidirectional line
				(at 25.4 43.18 180)
				(length 3.81)
				(name "P0_01")
				(number "F2")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 3.81)
				(name "P0_02")
				(number "F1")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 3.81)
				(name "P0_03")
				(number "E2")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "P0_04")
				(number "E1")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "P0_05")
				(number "D1")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "P0_06")
				(number "B10")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "P0_07")
				(number "B9")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "P0_08")
				(number "D6")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "P0_09")
				(number "B5")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "P0_16")
				(number "C9")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "P0_17")
				(number "C8")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "P0_18")
				(number "G10")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "P0_19")
				(number "C6")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "P0_20")
				(number "G8")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "P0_21")
				(number "C4")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "P0_24")
				(number "J9")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "P0_25")
				(number "H8")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "P0_26")
				(number "H7")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "P0_27")
				(number "C10")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "P0_28")
				(number "H5")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "P0_29")
				(number "D5")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "P0_30")
				(number "C3")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "P0_31")
				(number "D3")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "P1_00")
				(number "E9")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "P1_01")
				(number "E8")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "P1_02")
				(number "J10")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "P1_03")
				(number "E6")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "P1_04")
				(number "H3")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "P1_05")
				(number "E4")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 3.81)
				(name "P1_06")
				(number "J8")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "P1_07")
				(number "F7")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 3.81)
				(name "P1_08")
				(number "J7")
			)
			(pin bidirectional line
				(at 25.4 -40.64 180)
				(length 3.81)
				(name "P1_09")
				(number "G9")
			)
			(pin bidirectional line
				(at 25.4 -43.18 180)
				(length 3.81)
				(name "P1_10")
				(number "K8")
			)
			(pin bidirectional line
				(at 25.4 -45.72 180)
				(length 3.81)
				(name "P1_11")
				(number "G6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "DA14695"
		(extends "DA14691")
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "DA14695"
			(at 0 0 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-86_6x6mm_Layout10x10_P0.55mm"
			(at 0 69.85 0)
		)
		(property "Datasheet" "https://www.dialog-semiconductor.com/sites/default/files/da1469x_datasheet_3v1.pdf"
			(at -11.43 83.82 0)
		)
		(property "Description" "Multi-core BLE 5.1 Soc series, 96-MHz/32-bit ARM Cortex-M33, 128 kB ROM, 512 kB SRAM, 4 kB OTP Memory, 16 kB cache SRAM, VFBGA-86"
			(at 0 0 0)
		)
		(property "ki_keywords" "BLE MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*6x6mm*Layout10x10*P0.55mm*"
			(at 0 0 0)
		)
	)
)
