(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ESP32-C3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.272 23.876 0)
		)
		(property "Value" "ESP32-C3"
			(at 16.256 23.876 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.7x3.7mm"
			(at 0.508 0 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-c3_datasheet_en.pdf"
			(at 0.508 0 0)
		)
		(property "Description" "RF Module, ESP32 SoC, RISC-V, WiFi 802.11b/n/g, Bluetooth LE 5, QFN32"
			(at 0.508 0 0)
		)
		(property "ki_keywords" "WiFi BLE ESP32 Espressif"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*EP3.7x3.7mm*"
			(at 0 0 0)
		)
		(symbol "ESP32-C3_1_1"
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "GPIO2")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "GPIO3")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "GPIO8")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "GPIO9")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "GPIO10")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "GPIO18")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "GPIO19")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "U0TXD")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "U0RXD")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "XTAL_32K_P")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "XTAL_32K_N")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "XTAL_N")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "XTAL_P")
				(number "30")
			)
			(pin power_in line
				(at -10.16 25.4 270)
				(length 2.54)
				(name "VDD3P3")
				(number "2")
			)
			(pin passive line
				(at -10.16 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VDD3P3")
				(number "3")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "VDD3P3_RTC")
				(number "11")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD3P3_CPU")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "VDD_SPI")
				(number "18")
			)
			(pin power_in line
				(at 10.16 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "31")
			)
			(pin passive line
				(at 10.16 25.4 270)
				(length 2.54)
				(hide yes)
				(name "VDDA")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "LNA_IN")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "CHIP_EN")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "MTMS")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "MTDI")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "MTCK")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "MTDO")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "SPIHD")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "SPIWP")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "SPICS0")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "SPICLK")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "SPID")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "SPIQ")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-PICO-D4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 39.37 0)
		)
		(property "Value" "ESP32-PICO-D4"
			(at 3.81 39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.3x5.3mm"
			(at 31.75 -39.37 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-pico-d4_datasheet_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "RF Module, ESP32 SoC, Wi-Fi 802.11b/g/n, Bluetooth, BLE, 32-bit, 2.7-3.6V, external antenna, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "RF Radio BT ESP ESP32 Espressif external antenna"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ESP32-PICO-D4_0_0"
			(pin input line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "EN")
				(number "9")
			)
			(pin input line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "SENSOR_VP")
				(number "5")
			)
			(pin input line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "SENSOR_CAPP")
				(number "6")
			)
			(pin input line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "SENSOR_CAPN")
				(number "7")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "SENSOR_VN")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "IO16")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "IO17")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "SD0")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "SD1")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "CLK")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "CMD")
				(number "30")
			)
			(pin no_connect line
				(at -17.78 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "XTAL_N_NC")
				(number "44")
			)
			(pin no_connect line
				(at -17.78 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "XTAL_P_NC")
				(number "45")
			)
			(pin no_connect line
				(at -17.78 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "CAP2_NC")
				(number "47")
			)
			(pin no_connect line
				(at -17.78 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "CAP1_NC")
				(number "48")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 2.54)
				(name "VDDA")
				(number "1")
			)
			(pin passive line
				(at -5.08 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VDDA")
				(number "43")
			)
			(pin passive line
				(at -5.08 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VDDA")
				(number "46")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 2.54)
				(name "VDDA3P3")
				(number "3")
			)
			(pin passive line
				(at -2.54 40.64 270)
				(length 2.54)
				(hide yes)
				(name "VDDA3P3")
				(number "4")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VDD3P3_RTC")
				(number "19")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "VDD3P3_CPU")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "LNA_IN")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "IO0")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "U0TXD/IO1")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "IO2")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "U0RXD/IO3")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "IO4")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "IO5")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "SD2/IO9")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "SD3/IO10")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "IO12")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "IO13")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "IO14")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "IO15")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "IO18")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "IO19")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "IO21")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "IO22")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "IO23")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "IO25")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "IO26")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "IO27")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "IO32")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "IO33")
				(number "13")
			)
			(pin input line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "IO34")
				(number "10")
			)
			(pin input line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "IO35")
				(number "11")
			)
			(pin power_out line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "VDD_SDIO")
				(number "26")
			)
		)
		(symbol "ESP32-PICO-D4_0_1")
		(embedded_fonts no)
	)
	(symbol "ESP32-S2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 12.7 -38.1 0)
		)
		(property "Value" "ESP32-S2"
			(at 16.51 -40.64 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP4x4mm"
			(at 2.54 -48.26 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s2_datasheet_en.pdf"
			(at 2.54 -45.72 0)
		)
		(property "Description" "Microcontroller, Wi-Fi 802.11b/g/n, Bluetooth, 32bit"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microcontroller Wi-Fi BT ESP ESP32 Espressif"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "ESP32-S2_0_1")
		(symbol "ESP32-S2_1_1"
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "GPIO0")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "GPIO1")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "GPIO2")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "GPIO3")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "GPIO4")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "GPIO5")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "GPIO6")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "GPIO7")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "GPIO8")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "GPIO9")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "GPIO10")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "GPIO11")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "GPIO12")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "GPIO13")
				(number "18")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "GPIO14")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "DAC_1")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "DAC_2")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "GPIO19/USB_D-")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "GPIO20/USB_D+")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "GPIO21")
				(number "28")
			)
			(pin input line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "XTAL_P")
				(number "53")
			)
			(pin output line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "XTAL_N")
				(number "52")
			)
			(pin passive line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "XTAL_32K_P")
				(number "21")
			)
			(pin passive line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "XTAL_32K_N")
				(number "22")
			)
			(pin power_in line
				(at -7.62 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "1")
			)
			(pin passive line
				(at -7.62 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDDA")
				(number "51")
			)
			(pin passive line
				(at -7.62 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDDA")
				(number "54")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDD3P3")
				(number "3")
			)
			(pin passive line
				(at -5.08 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDD3P3")
				(number "4")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD3P3_RTC")
				(number "20")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD3P3_RTC_IO")
				(number "27")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "57")
			)
			(pin power_out line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD_SPI")
				(number "30")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD3P3_CPU")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "SPICS1")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "SPIHD")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "SPIWP")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "SPICS0")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "SPICLK")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "SPIQ")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "SPID")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "GPIO33")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "GPIO34")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "GPIO35")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "GPIO36")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "GPIO38")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "GPIO37")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "MTCK")
				(number "43")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "MTD0")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "MDTI")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "MTMS")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "U0TXD")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "U0RXD")
				(number "49")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "GPIO45")
				(number "50")
			)
			(pin input line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "GPIO46")
				(number "55")
			)
			(pin input line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "CHIP_PU")
				(number "56")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "LNA_IN")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP32-S3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 10.16 -38.1 0)
		)
		(property "Value" "ESP32-S3"
			(at 13.97 -40.64 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP4x4mm"
			(at 0 -48.26 0)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s3_datasheet_en.pdf"
			(at 0 0 0)
		)
		(property "Description" "Microcontroller, Wi-Fi 802.11b/g/n, Bluetooth, 32bit"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microcontroller Wi-Fi BT ESP ESP32 Espressif"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "ESP32-S3_0_1")
		(symbol "ESP32-S3_1_0"
			(pin passive line
				(at -5.08 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDDA")
				(number "56")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "SPICLK_N")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "MTDO")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "GPIO45")
				(number "51")
			)
		)
		(symbol "ESP32-S3_1_1"
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "GPIO0")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "GPIO1")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "GPIO2")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "GPIO3")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "GPIO4")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "GPIO5")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "GPIO6")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "GPIO7")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "GPIO8")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "GPIO9")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "GPIO10")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "GPIO11")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "GPIO12")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "GPIO13")
				(number "18")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "GPIO14")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "GPIO17")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "GPIO18")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "GPIO19/USB_D-")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "GPIO20/USB_D+")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "GPIO21")
				(number "27")
			)
			(pin passive line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "XTAL_32K_P")
				(number "21")
			)
			(pin passive line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "XTAL_32K_N")
				(number "22")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "XTAL_P")
				(number "54")
			)
			(pin output line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "XTAL_N")
				(number "53")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "55")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD3P3")
				(number "2")
			)
			(pin passive line
				(at -2.54 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDD3P3")
				(number "3")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD3P3_RTC")
				(number "20")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "57")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD_SPI")
				(number "29")
			)
			(pin power_in line
				(at 5.08 38.1 270)
				(length 2.54)
				(name "VDD3P3_CPU")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "SPICS1")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "SPIHD")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "SPIWP")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "SPICS0")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "SPICLK")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "SPIQ")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "SPID")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "SPICLK_P")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "GPIO33")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "GPIO34")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "GPIO35")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "GPIO36")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "GPIO37")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "GPIO38")
				(number "43")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "MTCK")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "MTDI")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "MTMS")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "U0TXD")
				(number "49")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "U0RXD")
				(number "50")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "GPIO46")
				(number "52")
			)
			(pin input line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "CHIP_PU")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "LNA_IN")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ESP8266EX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "ESP8266EX"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "http://espressif.com/sites/default/files/documentation/0a-esp8266ex_datasheet_en.pdf"
			(at 2.54 -33.02 0)
		)
		(property "Description" "Highly integrated Wi-Fi SoC, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "wifi soc"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ESP8266EX_0_1")
		(symbol "ESP8266EX_1_1"
			(pin input line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "TOUT")
				(number "6")
			)
			(pin input line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "CHIP_PU")
				(number "7")
			)
			(pin input line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "RES12K")
				(number "31")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "~{EXT_RSTB}")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "XPD_DCDC")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "LNA")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "XTAL_OUT")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "XTAL_IN")
				(number "28")
			)
			(pin power_in line
				(at -12.7 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "1")
			)
			(pin power_in line
				(at -10.16 25.4 270)
				(length 2.54)
				(name "VDDA")
				(number "30")
			)
			(pin power_in line
				(at -7.62 25.4 270)
				(length 2.54)
				(name "VDD3P3")
				(number "3")
			)
			(pin power_in line
				(at -5.08 25.4 270)
				(length 2.54)
				(name "VDD3P3")
				(number "4")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDD_RTC")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDDPST")
				(number "11")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VDDPST")
				(number "17")
			)
			(pin power_in line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "VDDD")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "SDIO_CMD")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "SDIO_CLK")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "SDIO_DATA_0")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "SDIO_DATA_2")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "SDIO_DATA_3")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "U0RXD")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "U0TXD")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "GPIO0")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "SDIO_DATA_1")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "GPIO2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "MTCK")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "GPIO5")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "MTMS")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "MTDO")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "MTDI")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "GPIO4")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
)
