(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "80186"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 72.39 0)
		)
		(property "Value" "80186"
			(at 10.16 72.39 0)
		)
		(property "Footprint" ""
			(at 1.27 33.02 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/x86/8018x/datashts/27243002.PDF"
			(at 0 31.75 0)
		)
		(property "Description" "High-Integration 16-Bit Microprocessor"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC* PGA*Layout11x11*P2.54mm* LCC*"
			(at 0 0 0)
		)
		(symbol "80186_0_1")
		(symbol "80186_1_1"
			(pin input line
				(at -15.24 68.58 0)
				(length 2.54)
				(name "~{RES}")
				(number "24")
			)
			(pin input line
				(at -15.24 60.96 0)
				(length 2.54)
				(name "X1")
				(number "59")
			)
			(pin output line
				(at -15.24 55.88 0)
				(length 2.54)
				(name "X2")
				(number "58")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "ARDY")
				(number "55")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "SRDY")
				(number "49")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{TEST}")
				(number "47")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DRQ0")
				(number "18")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "DRQ1")
				(number "19")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "NMI")
				(number "46")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "INT0")
				(number "45")
			)
			(pin input line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "INT1/~{SELECT}")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "INT2/~{INTA0}")
				(number "42")
			)
			(pin bidirectional line
				(at -15.24 -45.72 0)
				(length 2.54)
				(name "INT3/~{INTA1}/IRQ")
				(number "41")
			)
			(pin input line
				(at -15.24 -60.96 0)
				(length 2.54)
				(name "TMR_IN_0")
				(number "20")
			)
			(pin input line
				(at -15.24 -63.5 0)
				(length 2.54)
				(name "TMR_IN_1")
				(number "21")
			)
			(pin input line
				(at -15.24 -68.58 0)
				(length 2.54)
				(name "HOLD")
				(number "50")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 2.54)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "60")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 2.54)
				(name "VCC")
				(number "43")
			)
			(pin output line
				(at 15.24 68.58 180)
				(length 2.54)
				(name "RESET")
				(number "57")
			)
			(pin output line
				(at 15.24 66.04 180)
				(length 2.54)
				(name "CLKOUT")
				(number "56")
			)
			(pin bidirectional line
				(at 15.24 58.42 180)
				(length 2.54)
				(name "AD0")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 55.88 180)
				(length 2.54)
				(name "AD1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 53.34 180)
				(length 2.54)
				(name "AD2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 50.8 180)
				(length 2.54)
				(name "AD3")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 48.26 180)
				(length 2.54)
				(name "AD4")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 45.72 180)
				(length 2.54)
				(name "AD5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "AD6")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "AD7")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "AD8")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "AD9")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "AD10")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "AD11")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "AD12")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "AD13")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "AD14")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "AD15")
				(number "1")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "A16/S3")
				(number "68")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "A17/S4")
				(number "67")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "A18/S5")
				(number "66")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "A19/S6")
				(number "65")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~{S0}")
				(number "52")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "~{S1}")
				(number "53")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{S2}")
				(number "54")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{LOCK}")
				(number "48")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RD}/~{QSMD}")
				(number "62")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "ALE/QS0")
				(number "61")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{WR}/QS1")
				(number "63")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{BHE}/S7")
				(number "64")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "DT/~{R}")
				(number "40")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "~{DEN}")
				(number "39")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "~{UCS}")
				(number "34")
			)
			(pin output line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "~{LCS}")
				(number "33")
			)
			(pin output line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "~{MCS0}")
				(number "38")
			)
			(pin output line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "~{MCS1}")
				(number "37")
			)
			(pin output line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "~{MCS2}")
				(number "36")
			)
			(pin output line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "~{MCS3}")
				(number "35")
			)
			(pin output line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "~{PCS0}")
				(number "25")
			)
			(pin output line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "~{PCS1}")
				(number "27")
			)
			(pin output line
				(at 15.24 -45.72 180)
				(length 2.54)
				(name "~{PCS2}")
				(number "28")
			)
			(pin output line
				(at 15.24 -48.26 180)
				(length 2.54)
				(name "~{PCS3}")
				(number "29")
			)
			(pin output line
				(at 15.24 -50.8 180)
				(length 2.54)
				(name "~{PCS4}")
				(number "30")
			)
			(pin output line
				(at 15.24 -53.34 180)
				(length 2.54)
				(name "~{PCS5}/A1")
				(number "31")
			)
			(pin output line
				(at 15.24 -55.88 180)
				(length 2.54)
				(name "~{PCS6}/A2")
				(number "32")
			)
			(pin output line
				(at 15.24 -60.96 180)
				(length 2.54)
				(name "TMR_OUT_0")
				(number "22")
			)
			(pin output line
				(at 15.24 -63.5 180)
				(length 2.54)
				(name "TMR_OUT_1")
				(number "23")
			)
			(pin output line
				(at 15.24 -68.58 180)
				(length 2.54)
				(name "HLDA")
				(number "51")
			)
		)
		(embedded_fonts no)
	)
	(symbol "80188"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 72.39 0)
		)
		(property "Value" "80188"
			(at 10.16 72.39 0)
		)
		(property "Footprint" ""
			(at 1.27 33.02 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/x86/8018x/datashts/27243002.PDF"
			(at 0 31.75 0)
		)
		(property "Description" "High-Integration 16-Bit Microprocessor"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC* PGA*Layout11x11*P2.54mm* LCC*"
			(at 0 0 0)
		)
		(symbol "80188_0_1")
		(symbol "80188_1_1"
			(pin input line
				(at -15.24 68.58 0)
				(length 2.54)
				(name "~{RES}")
				(number "24")
			)
			(pin input line
				(at -15.24 60.96 0)
				(length 2.54)
				(name "X1")
				(number "59")
			)
			(pin output line
				(at -15.24 55.88 0)
				(length 2.54)
				(name "X2")
				(number "58")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "ARDY")
				(number "55")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "SRDY")
				(number "49")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{TEST}")
				(number "47")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DRQ0")
				(number "18")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "DRQ1")
				(number "19")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "NMI")
				(number "46")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "INT0")
				(number "45")
			)
			(pin input line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "INT1/~{SELECT}")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "INT2/~{INTA0}")
				(number "42")
			)
			(pin bidirectional line
				(at -15.24 -45.72 0)
				(length 2.54)
				(name "INT3/~{INTA1}/IRQ")
				(number "41")
			)
			(pin input line
				(at -15.24 -60.96 0)
				(length 2.54)
				(name "TMR_IN_0")
				(number "20")
			)
			(pin input line
				(at -15.24 -63.5 0)
				(length 2.54)
				(name "TMR_IN_1")
				(number "21")
			)
			(pin input line
				(at -15.24 -68.58 0)
				(length 2.54)
				(name "HOLD")
				(number "50")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 2.54)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "60")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 2.54)
				(name "VCC")
				(number "43")
			)
			(pin output line
				(at 15.24 68.58 180)
				(length 2.54)
				(name "RESET")
				(number "57")
			)
			(pin output line
				(at 15.24 66.04 180)
				(length 2.54)
				(name "CLKOUT")
				(number "56")
			)
			(pin bidirectional line
				(at 15.24 60.96 180)
				(length 2.54)
				(name "AD0")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 58.42 180)
				(length 2.54)
				(name "AD1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 55.88 180)
				(length 2.54)
				(name "AD2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 53.34 180)
				(length 2.54)
				(name "AD3")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 50.8 180)
				(length 2.54)
				(name "AD4")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 48.26 180)
				(length 2.54)
				(name "AD5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 45.72 180)
				(length 2.54)
				(name "AD6")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "AD7")
				(number "2")
			)
			(pin output line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "A8")
				(number "16")
			)
			(pin output line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "A9")
				(number "14")
			)
			(pin output line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "A10")
				(number "12")
			)
			(pin output line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "A11")
				(number "10")
			)
			(pin output line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "A12")
				(number "7")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "A13")
				(number "5")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "A14")
				(number "3")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "A15")
				(number "1")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "A16/S3")
				(number "68")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "A17/S4")
				(number "67")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "A18/S5")
				(number "66")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "A19/S6")
				(number "65")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~{S0}")
				(number "52")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "~{S1}")
				(number "53")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{S2}")
				(number "54")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{LOCK}")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RD}/~{QSMD}")
				(number "62")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "ALE/QS0")
				(number "61")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{WR}/QS1")
				(number "63")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "S7")
				(number "64")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "DT/~{R}")
				(number "40")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "~{DEN}")
				(number "39")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "~{UCS}")
				(number "34")
			)
			(pin output line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "~{LCS}")
				(number "33")
			)
			(pin output line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "~{MCS0}")
				(number "38")
			)
			(pin output line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "~{MCS1}")
				(number "37")
			)
			(pin output line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "~{MCS2}")
				(number "36")
			)
			(pin output line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "~{MCS3}")
				(number "35")
			)
			(pin output line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "~{PCS0}")
				(number "25")
			)
			(pin output line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "~{PCS1}")
				(number "27")
			)
			(pin output line
				(at 15.24 -45.72 180)
				(length 2.54)
				(name "~{PCS2}")
				(number "28")
			)
			(pin output line
				(at 15.24 -48.26 180)
				(length 2.54)
				(name "~{PCS3}")
				(number "29")
			)
			(pin output line
				(at 15.24 -50.8 180)
				(length 2.54)
				(name "~{PCS4}")
				(number "30")
			)
			(pin output line
				(at 15.24 -53.34 180)
				(length 2.54)
				(name "~{PCS5}/A1")
				(number "31")
			)
			(pin output line
				(at 15.24 -55.88 180)
				(length 2.54)
				(name "~{PCS6}/A2")
				(number "32")
			)
			(pin output line
				(at 15.24 -60.96 180)
				(length 2.54)
				(name "TMR_OUT_0")
				(number "22")
			)
			(pin output line
				(at 15.24 -63.5 180)
				(length 2.54)
				(name "TMR_OUT_1")
				(number "23")
			)
			(pin output line
				(at 15.24 -68.58 180)
				(length 2.54)
				(name "HLDA")
				(number "51")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8035"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 35.56 0)
		)
		(property "Value" "8035"
			(at 8.89 35.56 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" ""
			(at 0 5.08 0)
		)
		(property "Description" "MCS-48 8-bit Microcontroller, No (EP)ROM, 64B RAM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCS-48 uC Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "8035_1_1"
			(pin input inverted
				(at -17.78 30.48 0)
				(length 3.81)
				(name "~{RESET}")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 3.81)
				(name "P1.0")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "P1.1")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "P1.2")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "P1.3")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "P1.4")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "P1.5")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "P1.6")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "P1.7")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "P2.0")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "P2.1")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "P2.2")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "P2.3")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "P2.4")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "P2.5")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "P2.6")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "P2.7")
				(number "38")
			)
			(pin output line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "PROG")
				(number "25")
			)
			(pin input line
				(at -17.78 -25.4 0)
				(length 3.81)
				(name "T0")
				(number "1")
			)
			(pin input line
				(at -17.78 -27.94 0)
				(length 3.81)
				(name "T1")
				(number "39")
			)
			(pin input inverted
				(at -17.78 -30.48 0)
				(length 3.81)
				(name "~{INT}")
				(number "6")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "VDD")
				(number "26")
			)
			(pin input line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "EA")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "DB.0")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "DB.1")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "DB.2")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "DB.3")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "DB.4")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "DB.5")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "DB.6")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "DB.7")
				(number "19")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "ALE")
				(number "11")
			)
			(pin output output_low
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "~{PSEN}")
				(number "9")
			)
			(pin output output_low
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "~{RD}")
				(number "8")
			)
			(pin output output_low
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "~{WR}")
				(number "10")
			)
			(pin input inverted
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "~{SS}")
				(number "5")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "X1")
				(number "2")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "X2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8080"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -7.62 44.45 0)
		)
		(property "Value" "8080"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 15.24 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/MCS-80/intel-8080.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "8-bit N-channel Microprocessor, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "cpu mpu microprocessor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24*"
			(at 0 0 0)
		)
		(symbol "8080_0_1")
		(symbol "8080_1_1"
			(pin input line
				(at -12.7 35.56 0)
				(length 2.54)
				(name "RESET")
				(number "12")
			)
			(pin input line
				(at -12.7 30.48 0)
				(length 2.54)
				(name "ϕ1")
				(number "22")
			)
			(pin input line
				(at -12.7 27.94 0)
				(length 2.54)
				(name "ϕ2")
				(number "15")
			)
			(pin input line
				(at -12.7 -33.02 0)
				(length 2.54)
				(name "HOLD")
				(number "13")
			)
			(pin input line
				(at -12.7 -35.56 0)
				(length 2.54)
				(name "READY")
				(number "23")
			)
			(pin input line
				(at -12.7 -38.1 0)
				(length 2.54)
				(name "INT")
				(number "14")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "+5V")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "+12V")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "-5V")
				(number "11")
			)
			(pin output line
				(at 12.7 40.64 180)
				(length 2.54)
				(name "A0")
				(number "25")
			)
			(pin output line
				(at 12.7 38.1 180)
				(length 2.54)
				(name "A1")
				(number "26")
			)
			(pin output line
				(at 12.7 35.56 180)
				(length 2.54)
				(name "A2")
				(number "27")
			)
			(pin output line
				(at 12.7 33.02 180)
				(length 2.54)
				(name "A3")
				(number "29")
			)
			(pin output line
				(at 12.7 30.48 180)
				(length 2.54)
				(name "A4")
				(number "30")
			)
			(pin output line
				(at 12.7 27.94 180)
				(length 2.54)
				(name "A5")
				(number "31")
			)
			(pin output line
				(at 12.7 25.4 180)
				(length 2.54)
				(name "A6")
				(number "32")
			)
			(pin output line
				(at 12.7 22.86 180)
				(length 2.54)
				(name "A7")
				(number "33")
			)
			(pin output line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "A8")
				(number "34")
			)
			(pin output line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "A9")
				(number "35")
			)
			(pin output line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "A10")
				(number "1")
			)
			(pin output line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "A11")
				(number "40")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "A12")
				(number "37")
			)
			(pin output line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "A13")
				(number "38")
			)
			(pin output line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A14")
				(number "39")
			)
			(pin output line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A15")
				(number "36")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "D0")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "D1")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "D2")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "D3")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "D4")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "D5")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "D6")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "D7")
				(number "6")
			)
			(pin output line
				(at 12.7 -25.4 180)
				(length 2.54)
				(name "DBIN")
				(number "17")
			)
			(pin output line
				(at 12.7 -27.94 180)
				(length 2.54)
				(name "~{WR}")
				(number "18")
			)
			(pin output line
				(at 12.7 -33.02 180)
				(length 2.54)
				(name "HLDA")
				(number "21")
			)
			(pin output line
				(at 12.7 -35.56 180)
				(length 2.54)
				(name "WAIT")
				(number "24")
			)
			(pin output line
				(at 12.7 -38.1 180)
				(length 2.54)
				(name "INTE")
				(number "16")
			)
			(pin output line
				(at 12.7 -40.64 180)
				(length 2.54)
				(name "SYNC")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8086_Max_Mode"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 43.18 0)
		)
		(property "Value" "8086_Max_Mode"
			(at 10.16 43.18 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 2.54 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/x86/808x/datashts/8086/231455-006.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "8086 (maximum mode), 16-Bit HMOS Microprocessor, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "8086_Max_Mode_0_1")
		(symbol "8086_Max_Mode_1_1"
			(pin input clock
				(at -17.78 38.1 0)
				(length 3.81)
				(name "CLK")
				(number "19")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "READY")
				(number "22")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "RESET")
				(number "21")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "NMI")
				(number "17")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "INTR")
				(number "18")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "~{TEST}")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "~{RQ}/~{GT1}")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{RQ}/~{GT0}")
				(number "31")
			)
			(pin input line
				(at -17.78 -38.1 0)
				(length 3.81)
				(name "MN/~{MX}")
				(number "33")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 3.81)
				(name "QS0")
				(number "25")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 3.81)
				(name "QS1")
				(number "24")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "~{BHE}/S7")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "AD0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "AD1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "AD2")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "AD3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "AD4")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "AD5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "AD6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "AD7")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "AD8")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "AD9")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "AD10")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "AD11")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "AD12")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "AD13")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "AD14")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "AD15")
				(number "39")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "A16/S3")
				(number "38")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "A17/S4")
				(number "37")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "A18/S5")
				(number "36")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "A19/S6")
				(number "35")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "~{S0}")
				(number "26")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "~{S1}")
				(number "27")
			)
			(pin output line
				(at 17.78 -33.02 180)
				(length 3.81)
				(name "~{S2}")
				(number "28")
			)
			(pin output line
				(at 17.78 -35.56 180)
				(length 3.81)
				(name "~{LOCK}")
				(number "29")
			)
			(pin output line
				(at 17.78 -38.1 180)
				(length 3.81)
				(name "~{RD}")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8086_Min_Mode"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 43.18 0)
		)
		(property "Value" "8086_Min_Mode"
			(at 10.16 43.18 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 2.54 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/x86/808x/datashts/8086/231455-006.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "8086 (minimum mode), 16-Bit HMOS Microprocessor, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "8086_Min_Mode_0_1")
		(symbol "8086_Min_Mode_1_1"
			(pin input clock
				(at -17.78 38.1 0)
				(length 3.81)
				(name "CLK")
				(number "19")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "READY")
				(number "22")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "RESET")
				(number "21")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "NMI")
				(number "17")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "INTR")
				(number "18")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "~{TEST}")
				(number "23")
			)
			(pin output line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "HLDA")
				(number "30")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "HOLD")
				(number "31")
			)
			(pin input line
				(at -17.78 -38.1 0)
				(length 3.81)
				(name "MN/~{MX}")
				(number "33")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 3.81)
				(name "DT/~{R}")
				(number "27")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 3.81)
				(name "~{DEN}")
				(number "26")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "ALE")
				(number "25")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "~{BHE}/S7")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "AD0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "AD1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "AD2")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "AD3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "AD4")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "AD5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "AD6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "AD7")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "AD8")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "AD9")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "AD10")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "AD11")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "AD12")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "AD13")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "AD14")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "AD15")
				(number "39")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "A16/S3")
				(number "38")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "A17/S4")
				(number "37")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "A18/S5")
				(number "36")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "A19/S6")
				(number "35")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "M/~{IO}")
				(number "28")
			)
			(pin output line
				(at 17.78 -33.02 180)
				(length 3.81)
				(name "~{WR}")
				(number "29")
			)
			(pin output line
				(at 17.78 -35.56 180)
				(length 3.81)
				(name "~{RD}")
				(number "32")
			)
			(pin output line
				(at 17.78 -38.1 180)
				(length 3.81)
				(name "~{INTA}")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8087"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 43.18 0)
		)
		(property "Value" "8087"
			(at 10.16 43.18 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 2.54 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/x86/808x/datashts/8087/205835-007.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "Math Coprocessor for Intel 8086/8088/80186/80188 microprocessors, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FPU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "8087_0_1")
		(symbol "8087_1_1"
			(pin input clock
				(at -17.78 38.1 0)
				(length 3.81)
				(name "CLK")
				(number "19")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "READY")
				(number "22")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "RESET")
				(number "21")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "QS0")
				(number "25")
			)
			(pin input line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "QS1")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "~{RQ}/~{GT0}")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "~{RQ}/~{GT1}")
				(number "33")
			)
			(pin no_connect line
				(at -13.97 -30.48 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -13.97 -33.02 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -13.97 -35.56 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin no_connect line
				(at -13.97 -38.1 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "30")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 3.81)
				(name "~{BHE}/S7")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "AD0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "AD1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "AD2")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "AD3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "AD4")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "AD5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "AD6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "AD7")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "AD8")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "AD9")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "AD10")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "AD11")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "AD12")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "AD13")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "AD14")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "AD15")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "A16/S3")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "A17/S4")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "A18/S5")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "A19/S6")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "~{S0}")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "~{S1}")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "~{S2}")
				(number "28")
			)
			(pin output line
				(at 17.78 -35.56 180)
				(length 3.81)
				(name "BUSY")
				(number "23")
			)
			(pin output line
				(at 17.78 -38.1 180)
				(length 3.81)
				(name "INT")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8088"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 43.18 0)
		)
		(property "Value" "8088"
			(at 10.16 43.18 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 2.54 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/x86/808x/datashts/8088/231456-006.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "8088 (minimum mode), 8-Bit HMOS Microprocessor, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "8088_0_1")
		(symbol "8088_1_1"
			(pin input clock
				(at -17.78 38.1 0)
				(length 3.81)
				(name "CLK")
				(number "19")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "READY")
				(number "22")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "RESET")
				(number "21")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "NMI")
				(number "17")
			)
			(pin input line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "INTR")
				(number "18")
			)
			(pin output line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "~{INTA}")
				(number "24")
			)
			(pin output line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "HLDA")
				(number "30")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "HOLD")
				(number "31")
			)
			(pin output line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "~{SSO}")
				(number "34")
			)
			(pin input line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "~{TEST}")
				(number "23")
			)
			(pin input line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "MN/~{MX}")
				(number "33")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 3.81)
				(name "DT/~{R}")
				(number "27")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 3.81)
				(name "DEN")
				(number "26")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "ALE")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "AD0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "AD1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "AD2")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "AD3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "AD4")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "AD5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "AD6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "AD7")
				(number "9")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "A8")
				(number "8")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "A9")
				(number "7")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "A10")
				(number "6")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "A11")
				(number "5")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "A12")
				(number "4")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "A13")
				(number "3")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "A14")
				(number "2")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "A15")
				(number "39")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "A16/S3")
				(number "38")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "A17/S4")
				(number "37")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "A18/S5")
				(number "36")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "A19/S6")
				(number "35")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "IO/~{M}")
				(number "28")
			)
			(pin output line
				(at 17.78 -33.02 180)
				(length 3.81)
				(name "WR")
				(number "29")
			)
			(pin output output_low
				(at 17.78 -35.56 180)
				(length 3.81)
				(name "~{RD}")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8088_Max_Mode"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 43.18 0)
		)
		(property "Value" "8088_Max_Mode"
			(at 10.16 43.18 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 2.54 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/x86/808x/datashts/8088/231456-006.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "8088 (maximum mode), 8-Bit HMOS Microprocessor, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "8088_Max_Mode_0_1")
		(symbol "8088_Max_Mode_1_1"
			(pin input clock
				(at -17.78 38.1 0)
				(length 3.81)
				(name "CLK")
				(number "19")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "READY")
				(number "22")
			)
			(pin input line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "RESET")
				(number "21")
			)
			(pin input line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "NMI")
				(number "17")
			)
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "INTR")
				(number "18")
			)
			(pin input line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "~{TEST}")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "~{RQ}/~{GT1}")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "~{RQ}/~{GT0}")
				(number "31")
			)
			(pin output line
				(at -17.78 -33.02 0)
				(length 3.81)
				(name "HIGH")
				(number "34")
			)
			(pin input line
				(at -17.78 -38.1 0)
				(length 3.81)
				(name "MN/~{MX}")
				(number "33")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 3.81)
				(name "QS0")
				(number "25")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 3.81)
				(name "QS1")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "AD0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "AD1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "AD2")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "AD3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "AD4")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "AD5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "AD6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "AD7")
				(number "9")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "A8")
				(number "8")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "A9")
				(number "7")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "A10")
				(number "6")
			)
			(pin output line
				(at 17.78 0 180)
				(length 3.81)
				(name "A11")
				(number "5")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "A12")
				(number "4")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "A13")
				(number "3")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "A14")
				(number "2")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "A15")
				(number "39")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "A16/S3")
				(number "38")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "A17/S4")
				(number "37")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "A18/S5")
				(number "36")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "A19/S6")
				(number "35")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "~{S0}")
				(number "26")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "~{S1}")
				(number "27")
			)
			(pin output line
				(at 17.78 -33.02 180)
				(length 3.81)
				(name "~{S2}")
				(number "28")
			)
			(pin output line
				(at 17.78 -35.56 180)
				(length 3.81)
				(name "~{LOCK}")
				(number "29")
			)
			(pin output output_low
				(at 17.78 -38.1 180)
				(length 3.81)
				(name "~{RD}")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "80C188"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 72.39 0)
		)
		(property "Value" "80C188"
			(at 10.16 72.39 0)
		)
		(property "Footprint" ""
			(at 1.27 33.02 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/x86/8018x/datashts/80188/intel-80c188.pdf"
			(at 0 31.75 0)
		)
		(property "Description" "CHMOS High-Integration 16-Bit Microprocessor"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC* PGA*Layout11x11*P2.54mm* LCC*"
			(at 0 0 0)
		)
		(symbol "80C188_0_1")
		(symbol "80C188_1_1"
			(pin input line
				(at -15.24 68.58 0)
				(length 2.54)
				(name "~{RES}")
				(number "24")
			)
			(pin input line
				(at -15.24 60.96 0)
				(length 2.54)
				(name "X1")
				(number "59")
			)
			(pin output line
				(at -15.24 55.88 0)
				(length 2.54)
				(name "X2")
				(number "58")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "ARDY")
				(number "55")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "SRDY")
				(number "49")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{TEST}")
				(number "47")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DRQ0")
				(number "18")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "DRQ1")
				(number "19")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "NMI")
				(number "46")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "INT0")
				(number "45")
			)
			(pin input line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "INT1/~{SELECT}")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "INT2/~{INTA0}")
				(number "42")
			)
			(pin bidirectional line
				(at -15.24 -45.72 0)
				(length 2.54)
				(name "INT3/~{INTA1}/IRQ")
				(number "41")
			)
			(pin input line
				(at -15.24 -60.96 0)
				(length 2.54)
				(name "TMR_IN_0")
				(number "20")
			)
			(pin input line
				(at -15.24 -63.5 0)
				(length 2.54)
				(name "TMR_IN_1")
				(number "21")
			)
			(pin input line
				(at -15.24 -68.58 0)
				(length 2.54)
				(name "HOLD")
				(number "50")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 2.54)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "60")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 2.54)
				(name "VCC")
				(number "43")
			)
			(pin output line
				(at 15.24 68.58 180)
				(length 2.54)
				(name "RESET")
				(number "57")
			)
			(pin output line
				(at 15.24 66.04 180)
				(length 2.54)
				(name "CLKOUT")
				(number "56")
			)
			(pin bidirectional line
				(at 15.24 60.96 180)
				(length 2.54)
				(name "AD0")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 58.42 180)
				(length 2.54)
				(name "AD1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 55.88 180)
				(length 2.54)
				(name "AD2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 53.34 180)
				(length 2.54)
				(name "AD3")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 50.8 180)
				(length 2.54)
				(name "AD4")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 48.26 180)
				(length 2.54)
				(name "AD5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 45.72 180)
				(length 2.54)
				(name "AD6")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "AD7")
				(number "2")
			)
			(pin output line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "A8")
				(number "16")
			)
			(pin output line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "A9")
				(number "14")
			)
			(pin output line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "A10")
				(number "12")
			)
			(pin output line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "A11")
				(number "10")
			)
			(pin output line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "A12")
				(number "7")
			)
			(pin output line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "A13")
				(number "5")
			)
			(pin output line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "A14")
				(number "3")
			)
			(pin output line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "A15")
				(number "1")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "A16/S3")
				(number "68")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "A17/S4")
				(number "67")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "A18/S5")
				(number "66")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "A19/S6")
				(number "65")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~{S0}")
				(number "52")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "~{S1}")
				(number "53")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{S2}")
				(number "54")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{LOCK}")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RD}/~{QSMD}")
				(number "62")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "ALE/QS0")
				(number "61")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{WR}/QS1")
				(number "63")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RFSH}")
				(number "64")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "DT/~{R}")
				(number "40")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "~{DEN}")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "~{UCS}")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "~{LCS}")
				(number "33")
			)
			(pin output line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "~{MCS0}")
				(number "38")
			)
			(pin output line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "~{MCS1}")
				(number "37")
			)
			(pin output line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "~{MCS2}")
				(number "36")
			)
			(pin output line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "~{MCS3}")
				(number "35")
			)
			(pin output line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "~{PCS0}")
				(number "25")
			)
			(pin output line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "~{PCS1}")
				(number "27")
			)
			(pin output line
				(at 15.24 -45.72 180)
				(length 2.54)
				(name "~{PCS2}")
				(number "28")
			)
			(pin output line
				(at 15.24 -48.26 180)
				(length 2.54)
				(name "~{PCS3}")
				(number "29")
			)
			(pin output line
				(at 15.24 -50.8 180)
				(length 2.54)
				(name "~{PCS4}")
				(number "30")
			)
			(pin output line
				(at 15.24 -53.34 180)
				(length 2.54)
				(name "~{PCS5}/A1")
				(number "31")
			)
			(pin output line
				(at 15.24 -55.88 180)
				(length 2.54)
				(name "~{PCS6}/A2")
				(number "32")
			)
			(pin output line
				(at 15.24 -60.96 180)
				(length 2.54)
				(name "TMR_OUT_0")
				(number "22")
			)
			(pin output line
				(at 15.24 -63.5 180)
				(length 2.54)
				(name "TMR_OUT_1")
				(number "23")
			)
			(pin output line
				(at 15.24 -68.58 180)
				(length 2.54)
				(name "HLDA")
				(number "51")
			)
		)
		(embedded_fonts no)
	)
	(symbol "8748"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 35.56 0)
		)
		(property "Value" "8748"
			(at 8.89 35.56 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" ""
			(at 0 5.08 0)
		)
		(property "Description" "i8748, MCS-48 8-bit Microcontroller with Internal EPROM, 1KB EPROM, 64B RAM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCS-48 uC Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "8748_1_1"
			(pin input inverted
				(at -17.78 30.48 0)
				(length 3.81)
				(name "~{RESET}")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 3.81)
				(name "P1.0")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "P1.1")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "P1.2")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "P1.3")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "P1.4")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "P1.5")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "P1.6")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "P1.7")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "P2.0")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "P2.1")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "P2.2")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "P2.3")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "P2.4")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "P2.5")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "P2.6")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "P2.7")
				(number "38")
			)
			(pin output line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "PROG")
				(number "25")
			)
			(pin input line
				(at -17.78 -25.4 0)
				(length 3.81)
				(name "T0")
				(number "1")
			)
			(pin input line
				(at -17.78 -27.94 0)
				(length 3.81)
				(name "T1")
				(number "39")
			)
			(pin input inverted
				(at -17.78 -30.48 0)
				(length 3.81)
				(name "~{INT}")
				(number "6")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "Vpp/VDD")
				(number "26")
			)
			(pin input line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "EA")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "DB.0")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "DB.1")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "DB.2")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "DB.3")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "DB.4")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "DB.5")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "DB.6")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "DB.7")
				(number "19")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "ALE")
				(number "11")
			)
			(pin output output_low
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "~{PSEN}")
				(number "9")
			)
			(pin output output_low
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "~{RD}")
				(number "8")
			)
			(pin output output_low
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "~{WR}")
				(number "10")
			)
			(pin input inverted
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "~{SS}")
				(number "5")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "X1")
				(number "2")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "X2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "I386EX_PQFP"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 83.82 0)
		)
		(property "Value" "I386EX_PQFP"
			(at 16.51 83.82 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Intel I386EX Embedded microprocessor, PQFP-132"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PQFP*"
			(at 0 0 0)
		)
		(symbol "I386EX_PQFP_1_1"
			(pin input inverted
				(at -33.02 78.74 0)
				(length 3.81)
				(name "BS8")
				(number "33")
			)
			(pin output inverted
				(at -33.02 76.2 0)
				(length 3.81)
				(name "ADS")
				(number "40")
			)
			(pin output inverted
				(at -33.02 73.66 0)
				(length 3.81)
				(name "BHE")
				(number "39")
			)
			(pin output inverted
				(at -33.02 71.12 0)
				(length 3.81)
				(name "BLE")
				(number "37")
			)
			(pin tri_state line
				(at -33.02 68.58 0)
				(length 3.81)
				(name "A1")
				(number "42")
			)
			(pin tri_state line
				(at -33.02 66.04 0)
				(length 3.81)
				(name "A2")
				(number "43")
			)
			(pin tri_state line
				(at -33.02 63.5 0)
				(length 3.81)
				(name "A3")
				(number "44")
			)
			(pin tri_state line
				(at -33.02 60.96 0)
				(length 3.81)
				(name "A4")
				(number "45")
			)
			(pin tri_state line
				(at -33.02 58.42 0)
				(length 3.81)
				(name "A5")
				(number "48")
			)
			(pin tri_state line
				(at -33.02 55.88 0)
				(length 3.81)
				(name "A6")
				(number "49")
			)
			(pin tri_state line
				(at -33.02 53.34 0)
				(length 3.81)
				(name "A7")
				(number "50")
			)
			(pin tri_state line
				(at -33.02 50.8 0)
				(length 3.81)
				(name "A8")
				(number "51")
			)
			(pin tri_state line
				(at -33.02 48.26 0)
				(length 3.81)
				(name "A9")
				(number "52")
			)
			(pin tri_state line
				(at -33.02 45.72 0)
				(length 3.81)
				(name "A10")
				(number "53")
			)
			(pin tri_state line
				(at -33.02 43.18 0)
				(length 3.81)
				(name "A11")
				(number "54")
			)
			(pin tri_state line
				(at -33.02 40.64 0)
				(length 3.81)
				(name "A12")
				(number "55")
			)
			(pin tri_state line
				(at -33.02 38.1 0)
				(length 3.81)
				(name "A13")
				(number "56")
			)
			(pin tri_state line
				(at -33.02 35.56 0)
				(length 3.81)
				(name "A14")
				(number "57")
			)
			(pin tri_state line
				(at -33.02 33.02 0)
				(length 3.81)
				(name "A15")
				(number "58")
			)
			(pin tri_state line
				(at -33.02 30.48 0)
				(length 3.81)
				(name "A16/CAS0")
				(number "59")
			)
			(pin tri_state line
				(at -33.02 27.94 0)
				(length 3.81)
				(name "A17/CAS1")
				(number "61")
			)
			(pin tri_state line
				(at -33.02 25.4 0)
				(length 3.81)
				(name "A18/CAS2")
				(number "62")
			)
			(pin tri_state line
				(at -33.02 22.86 0)
				(length 3.81)
				(name "A19")
				(number "63")
			)
			(pin tri_state line
				(at -33.02 20.32 0)
				(length 3.81)
				(name "A20")
				(number "65")
			)
			(pin tri_state line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "A21")
				(number "66")
			)
			(pin tri_state line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "A22")
				(number "67")
			)
			(pin tri_state line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "A23")
				(number "68")
			)
			(pin tri_state line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "A24")
				(number "70")
			)
			(pin tri_state line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "A25")
				(number "72")
			)
			(pin tri_state line
				(at -33.02 0 0)
				(length 3.81)
				(name "D0")
				(number "5")
			)
			(pin tri_state line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "D1")
				(number "6")
			)
			(pin tri_state line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "D2")
				(number "7")
			)
			(pin tri_state line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "D3")
				(number "8")
			)
			(pin tri_state line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "D4")
				(number "10")
			)
			(pin tri_state line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "D5")
				(number "11")
			)
			(pin tri_state line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "D6")
				(number "12")
			)
			(pin tri_state line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "D7")
				(number "13")
			)
			(pin tri_state line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "D8")
				(number "14")
			)
			(pin tri_state line
				(at -33.02 -22.86 0)
				(length 3.81)
				(name "D9")
				(number "16")
			)
			(pin tri_state line
				(at -33.02 -25.4 0)
				(length 3.81)
				(name "D10")
				(number "18")
			)
			(pin tri_state line
				(at -33.02 -27.94 0)
				(length 3.81)
				(name "D11")
				(number "19")
			)
			(pin tri_state line
				(at -33.02 -30.48 0)
				(length 3.81)
				(name "D12")
				(number "20")
			)
			(pin tri_state line
				(at -33.02 -33.02 0)
				(length 3.81)
				(name "D13")
				(number "21")
			)
			(pin tri_state line
				(at -33.02 -35.56 0)
				(length 3.81)
				(name "D14")
				(number "22")
			)
			(pin tri_state line
				(at -33.02 -38.1 0)
				(length 3.81)
				(name "D15")
				(number "23")
			)
			(pin input line
				(at -33.02 -43.18 0)
				(length 3.81)
				(name "RESET")
				(number "110")
			)
			(pin input clock
				(at -33.02 -45.72 0)
				(length 3.81)
				(name "CLK2")
				(number "115")
			)
			(pin input clock
				(at -33.02 -50.8 0)
				(length 3.81)
				(name "TCK")
				(number "76")
			)
			(pin input line
				(at -33.02 -53.34 0)
				(length 3.81)
				(name "TDI")
				(number "25")
			)
			(pin output line
				(at -33.02 -55.88 0)
				(length 3.81)
				(name "TDO")
				(number "24")
			)
			(pin input line
				(at -33.02 -58.42 0)
				(length 3.81)
				(name "TMS")
				(number "26")
			)
			(pin input inverted
				(at -33.02 -60.96 0)
				(length 3.81)
				(name "TRST")
				(number "119")
			)
			(pin input inverted_clock
				(at -33.02 -66.04 0)
				(length 3.81)
				(name "SMI")
				(number "73")
			)
			(pin output inverted
				(at -33.02 -68.58 0)
				(length 3.81)
				(name "SMIACT")
				(number "120")
			)
			(pin input inverted
				(at -33.02 -73.66 0)
				(length 3.81)
				(name "FLT")
				(number "99")
			)
			(pin input inverted
				(at -33.02 -78.74 0)
				(length 3.81)
				(name "NA")
				(number "41")
			)
			(pin power_in line
				(at -15.24 86.36 270)
				(length 3.81)
				(name "VCC")
				(number "28")
			)
			(pin power_in line
				(at -15.24 -86.36 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at -12.7 86.36 270)
				(length 3.81)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at -12.7 -86.36 90)
				(length 3.81)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at -10.16 86.36 270)
				(length 3.81)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at -10.16 -86.36 90)
				(length 3.81)
				(name "GND")
				(number "31")
			)
			(pin power_in line
				(at -7.62 86.36 270)
				(length 3.81)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at -7.62 -86.36 90)
				(length 3.81)
				(name "GND")
				(number "36")
			)
			(pin power_in line
				(at -5.08 86.36 270)
				(length 3.81)
				(name "VCC")
				(number "47")
			)
			(pin power_in line
				(at -5.08 -86.36 90)
				(length 3.81)
				(name "GND")
				(number "46")
			)
			(pin power_in line
				(at -2.54 86.36 270)
				(length 3.81)
				(name "VCC")
				(number "60")
			)
			(pin power_in line
				(at -2.54 -86.36 90)
				(length 3.81)
				(name "GND")
				(number "64")
			)
			(pin power_in line
				(at 0 86.36 270)
				(length 3.81)
				(name "VCC")
				(number "71")
			)
			(pin power_in line
				(at 0 -86.36 90)
				(length 3.81)
				(name "GND")
				(number "69")
			)
			(pin power_in line
				(at 2.54 86.36 270)
				(length 3.81)
				(name "VCC")
				(number "81")
			)
			(pin power_in line
				(at 2.54 -86.36 90)
				(length 3.81)
				(name "GND")
				(number "83")
			)
			(pin power_in line
				(at 5.08 86.36 270)
				(length 3.81)
				(name "VCC")
				(number "88")
			)
			(pin power_in line
				(at 5.08 -86.36 90)
				(length 3.81)
				(name "GND")
				(number "97")
			)
			(pin power_in line
				(at 7.62 86.36 270)
				(length 3.81)
				(name "VCC")
				(number "109")
			)
			(pin power_in line
				(at 7.62 -86.36 90)
				(length 3.81)
				(name "GND")
				(number "100")
			)
			(pin power_in line
				(at 10.16 86.36 270)
				(length 3.81)
				(name "VCC")
				(number "121")
			)
			(pin power_in line
				(at 10.16 -86.36 90)
				(length 3.81)
				(name "GND")
				(number "116")
			)
			(pin power_in line
				(at 12.7 86.36 270)
				(length 3.81)
				(name "VCC")
				(number "127")
			)
			(pin power_in line
				(at 12.7 -86.36 90)
				(length 3.81)
				(name "GND")
				(number "130")
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 3.81)
				(name "DCD0/P1.0")
				(number "101")
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 3.81)
				(name "RTS0/P1.1")
				(number "102")
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 3.81)
				(name "DTR0/P1.2")
				(number "104")
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 3.81)
				(name "DSR0/P1.3")
				(number "105")
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 3.81)
				(name "RI0/P1.4")
				(number "106")
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 3.81)
				(name "LOCK/P1.5")
				(number "107")
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 3.81)
				(name "HOLD/P1.6")
				(number "108")
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 3.81)
				(name "HLDA/P1.7")
				(number "111")
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 3.81)
				(name "CS0/P2.0")
				(number "122")
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 3.81)
				(name "CS1/P2.1")
				(number "123")
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 3.81)
				(name "CS2/P2.2")
				(number "124")
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 3.81)
				(name "CS3/P2.3")
				(number "125")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 3.81)
				(name "CS4/P2.4")
				(number "126")
			)
			(pin bidirectional line
				(at 33.02 43.18 180)
				(length 3.81)
				(name "RDX0/P2.5")
				(number "129")
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 3.81)
				(name "TXD0/P2.6")
				(number "131")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 3.81)
				(name "CTS0/P2.7")
				(number "132")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 3.81)
				(name "TMROUT0/P3.0")
				(number "74")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 3.81)
				(name "TMROUT1/P3.1")
				(number "75")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 3.81)
				(name "INT0/P3.2")
				(number "80")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "INT1/P3.3")
				(number "82")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 3.81)
				(name "INT2/P3.4")
				(number "84")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "INT3/P3.5")
				(number "85")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "PWRDWN/P3.6")
				(number "86")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "COMCLK/P3.7")
				(number "87")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "DRQ0/DCD1")
				(number "117")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "DRQ1/RXD1")
				(number "118")
			)
			(pin output inverted
				(at 33.02 0 180)
				(length 3.81)
				(name "DACK0/CS5")
				(number "128")
			)
			(pin output line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "DACK1/TXD1")
				(number "112")
			)
			(pin bidirectional inverted
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "EOP/CTS1")
				(number "113")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "SRXCLK/DTR1")
				(number "77")
			)
			(pin input line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "SSIORX/RI1")
				(number "78")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "SSIOTX/RST1")
				(number "79")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "STXCLK/DSR1")
				(number "98")
			)
			(pin output line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "WDTOUT")
				(number "114")
			)
			(pin input line
				(at 33.02 -27.94 180)
				(length 3.81)
				(name "PEREQ/TMRCLK2")
				(number "89")
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 3.81)
				(name "ERROR/TMROUT2")
				(number "91")
			)
			(pin input line
				(at 33.02 -33.02 180)
				(length 3.81)
				(name "BUSY/TMRGATE2")
				(number "92")
			)
			(pin input line
				(at 33.02 -35.56 180)
				(length 3.81)
				(name "INT4/TMRCLK0")
				(number "93")
			)
			(pin input line
				(at 33.02 -38.1 180)
				(length 3.81)
				(name "INT5/TMRGATE0")
				(number "94")
			)
			(pin input line
				(at 33.02 -40.64 180)
				(length 3.81)
				(name "INT6/TMRCLK1")
				(number "95")
			)
			(pin input line
				(at 33.02 -43.18 180)
				(length 3.81)
				(name "INT7/TMRGATE1")
				(number "96")
			)
			(pin input line
				(at 33.02 -48.26 180)
				(length 3.81)
				(name "NMI")
				(number "90")
			)
			(pin output inverted
				(at 33.02 -53.34 180)
				(length 3.81)
				(name "CS6/REFRESH")
				(number "2")
			)
			(pin output inverted
				(at 33.02 -55.88 180)
				(length 3.81)
				(name "UCS")
				(number "1")
			)
			(pin output inverted
				(at 33.02 -60.96 180)
				(length 3.81)
				(name "LBA")
				(number "4")
			)
			(pin bidirectional inverted
				(at 33.02 -63.5 180)
				(length 3.81)
				(name "READY")
				(number "32")
			)
			(pin output line
				(at 33.02 -66.04 180)
				(length 3.81)
				(name "M/IO")
				(number "27")
			)
			(pin output line
				(at 33.02 -68.58 180)
				(length 3.81)
				(name "D/C")
				(number "29")
			)
			(pin output inverted
				(at 33.02 -73.66 180)
				(length 3.81)
				(name "RD")
				(number "34")
			)
			(pin output inverted
				(at 33.02 -76.2 180)
				(length 3.81)
				(name "WR")
				(number "35")
			)
			(pin output line
				(at 33.02 -78.74 180)
				(length 3.81)
				(name "WR/RD")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M80C186"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 72.39 0)
		)
		(property "Value" "M80C186"
			(at 10.16 72.39 0)
		)
		(property "Footprint" ""
			(at 1.27 33.02 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/x86/8018x/datashts/80186/27050008.PDF"
			(at 0 31.75 0)
		)
		(property "Description" "CHMOS High-Integration 16-Bit Microprocessor"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC* PGA*Layout11x11*P2.54mm* LCC*"
			(at 0 0 0)
		)
		(symbol "M80C186_0_1")
		(symbol "M80C186_1_1"
			(pin input line
				(at -15.24 68.58 0)
				(length 2.54)
				(name "~{RES}")
				(number "24")
			)
			(pin input line
				(at -15.24 60.96 0)
				(length 2.54)
				(name "X1")
				(number "59")
			)
			(pin output line
				(at -15.24 55.88 0)
				(length 2.54)
				(name "X2")
				(number "58")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "ARDY")
				(number "55")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "SRDY")
				(number "49")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{TEST}/BUSY")
				(number "47")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DRQ0")
				(number "18")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "DRQ1")
				(number "19")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "NMI")
				(number "46")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "INT0")
				(number "45")
			)
			(pin input line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "INT1")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "INT2/~{INTA0}")
				(number "42")
			)
			(pin bidirectional line
				(at -15.24 -45.72 0)
				(length 2.54)
				(name "INT3/~{INTA1}")
				(number "41")
			)
			(pin input line
				(at -15.24 -60.96 0)
				(length 2.54)
				(name "TMR_IN_0")
				(number "20")
			)
			(pin input line
				(at -15.24 -63.5 0)
				(length 2.54)
				(name "TMR_IN_1")
				(number "21")
			)
			(pin input line
				(at -15.24 -68.58 0)
				(length 2.54)
				(name "HOLD")
				(number "50")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 2.54)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "60")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 2.54)
				(name "VCC")
				(number "43")
			)
			(pin output line
				(at 15.24 68.58 180)
				(length 2.54)
				(name "RESET")
				(number "57")
			)
			(pin output line
				(at 15.24 66.04 180)
				(length 2.54)
				(name "CLKOUT")
				(number "56")
			)
			(pin bidirectional line
				(at 15.24 58.42 180)
				(length 2.54)
				(name "AD0")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 55.88 180)
				(length 2.54)
				(name "AD1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 53.34 180)
				(length 2.54)
				(name "AD2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 50.8 180)
				(length 2.54)
				(name "AD3")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 48.26 180)
				(length 2.54)
				(name "AD4")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 45.72 180)
				(length 2.54)
				(name "AD5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "AD6")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "AD7")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "AD8")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "AD9")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "AD10")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "AD11")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "AD12")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "AD13")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "AD14")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "AD15")
				(number "1")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "A16/S3")
				(number "68")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "A17/S4")
				(number "67")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "A18/S5")
				(number "66")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "A19/S6")
				(number "65")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~{S0}")
				(number "52")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "~{S1}")
				(number "53")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{S2}")
				(number "54")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{LOCK}")
				(number "48")
			)
			(pin output line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RD}/~{QSMD}")
				(number "62")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "ALE/QS0")
				(number "61")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{WR}/QS1")
				(number "63")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{BHE}")
				(number "64")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "DT/~{R}")
				(number "40")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "~{DEN}")
				(number "39")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "~{UCS}")
				(number "34")
			)
			(pin output line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "~{LCS}")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "~{MCS0}/PEREQ")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "~{MCS1}/~{ERROR}")
				(number "37")
			)
			(pin output line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "~{MCS2}")
				(number "36")
			)
			(pin output line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "~{MCS3}/~{NPS}")
				(number "35")
			)
			(pin output line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "~{PCS0}")
				(number "25")
			)
			(pin output line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "~{PCS1}")
				(number "27")
			)
			(pin output line
				(at 15.24 -45.72 180)
				(length 2.54)
				(name "~{PCS2}")
				(number "28")
			)
			(pin output line
				(at 15.24 -48.26 180)
				(length 2.54)
				(name "~{PCS3}")
				(number "29")
			)
			(pin output line
				(at 15.24 -50.8 180)
				(length 2.54)
				(name "~{PCS4}")
				(number "30")
			)
			(pin output line
				(at 15.24 -53.34 180)
				(length 2.54)
				(name "~{PCS5}/A1")
				(number "31")
			)
			(pin output line
				(at 15.24 -55.88 180)
				(length 2.54)
				(name "~{PCS6}/A2")
				(number "32")
			)
			(pin output line
				(at 15.24 -60.96 180)
				(length 2.54)
				(name "TMR_OUT_0")
				(number "22")
			)
			(pin output line
				(at 15.24 -63.5 180)
				(length 2.54)
				(name "TMR_OUT_1")
				(number "23")
			)
			(pin output line
				(at 15.24 -68.58 180)
				(length 2.54)
				(name "HLDA")
				(number "51")
			)
		)
		(embedded_fonts no)
	)
	(symbol "M80C186XL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 72.39 0)
		)
		(property "Value" "M80C186XL"
			(at 10.16 72.39 0)
		)
		(property "Footprint" ""
			(at 1.27 33.02 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/x86/8018x/datashts/80186/27127602.pdf"
			(at 0 31.75 0)
		)
		(property "Description" "16-Bit High-Integration Embedded Processor"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC* PGA*Layout11x11*P2.54mm* LCC*"
			(at 0 0 0)
		)
		(symbol "M80C186XL_0_1")
		(symbol "M80C186XL_1_1"
			(pin input line
				(at -15.24 68.58 0)
				(length 2.54)
				(name "~{RES}")
				(number "24")
			)
			(pin input line
				(at -15.24 60.96 0)
				(length 2.54)
				(name "X1")
				(number "59")
			)
			(pin output line
				(at -15.24 55.88 0)
				(length 2.54)
				(name "X2")
				(number "58")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "ARDY")
				(number "55")
			)
			(pin input line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "SRDY")
				(number "49")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{TEST}/BUSY")
				(number "47")
			)
			(pin input line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "DRQ0")
				(number "18")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "DRQ1")
				(number "19")
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "NMI")
				(number "46")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "INT0")
				(number "45")
			)
			(pin input line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "INT1/~{SELECT}")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "INT2/~{INTA0}")
				(number "42")
			)
			(pin bidirectional line
				(at -15.24 -45.72 0)
				(length 2.54)
				(name "INT3/~{INTA1}/IRQ")
				(number "41")
			)
			(pin input line
				(at -15.24 -60.96 0)
				(length 2.54)
				(name "TMR_IN_0")
				(number "20")
			)
			(pin input line
				(at -15.24 -63.5 0)
				(length 2.54)
				(name "TMR_IN_1")
				(number "21")
			)
			(pin input line
				(at -15.24 -68.58 0)
				(length 2.54)
				(name "HOLD")
				(number "50")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 2.54)
				(name "VSS")
				(number "26")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "60")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 2.54)
				(name "VCC")
				(number "43")
			)
			(pin output line
				(at 15.24 68.58 180)
				(length 2.54)
				(name "RESET")
				(number "57")
			)
			(pin output line
				(at 15.24 66.04 180)
				(length 2.54)
				(name "CLKOUT")
				(number "56")
			)
			(pin bidirectional line
				(at 15.24 58.42 180)
				(length 2.54)
				(name "AD0")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 55.88 180)
				(length 2.54)
				(name "AD1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 53.34 180)
				(length 2.54)
				(name "AD2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 50.8 180)
				(length 2.54)
				(name "AD3")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 48.26 180)
				(length 2.54)
				(name "AD4")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 45.72 180)
				(length 2.54)
				(name "AD5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "AD6")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "AD7")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "AD8")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "AD9")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "AD10")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "AD11")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "AD12")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "AD13")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "AD14")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "AD15")
				(number "1")
			)
			(pin output line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "A16/S3")
				(number "68")
			)
			(pin output line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "A17/S4")
				(number "67")
			)
			(pin output line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "A18/S5")
				(number "66")
			)
			(pin output line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "A19/S6")
				(number "65")
			)
			(pin output line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~{S0}")
				(number "52")
			)
			(pin output line
				(at 15.24 0 180)
				(length 2.54)
				(name "~{S1}")
				(number "53")
			)
			(pin output line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "~{S2}")
				(number "54")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{LOCK}")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RD}/~{QSMD}")
				(number "62")
			)
			(pin output line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "ALE/QS0")
				(number "61")
			)
			(pin output line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{WR}/QS1")
				(number "63")
			)
			(pin output line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{BHE}")
				(number "64")
			)
			(pin output line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "DT/~{R}")
				(number "40")
			)
			(pin output line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "~{DEN}")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "~{UCS}")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "~{LCS}")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "~{MCS0}/PEREQ")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "~{MCS1}/~{ERROR}")
				(number "37")
			)
			(pin output line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "~{MCS2}")
				(number "36")
			)
			(pin output line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "~{MCS3}/~{NPS}")
				(number "35")
			)
			(pin output line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "~{PCS0}")
				(number "25")
			)
			(pin output line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "~{PCS1}")
				(number "27")
			)
			(pin output line
				(at 15.24 -45.72 180)
				(length 2.54)
				(name "~{PCS2}")
				(number "28")
			)
			(pin output line
				(at 15.24 -48.26 180)
				(length 2.54)
				(name "~{PCS3}")
				(number "29")
			)
			(pin output line
				(at 15.24 -50.8 180)
				(length 2.54)
				(name "~{PCS4}")
				(number "30")
			)
			(pin output line
				(at 15.24 -53.34 180)
				(length 2.54)
				(name "~{PCS5}/A1")
				(number "31")
			)
			(pin output line
				(at 15.24 -55.88 180)
				(length 2.54)
				(name "~{PCS6}/A2")
				(number "32")
			)
			(pin output line
				(at 15.24 -60.96 180)
				(length 2.54)
				(name "TMR_OUT_0")
				(number "22")
			)
			(pin output line
				(at 15.24 -63.5 180)
				(length 2.54)
				(name "TMR_OUT_1")
				(number "23")
			)
			(pin output line
				(at 15.24 -68.58 180)
				(length 2.54)
				(name "HLDA")
				(number "51")
			)
		)
		(embedded_fonts no)
	)
	(symbol "P8051AH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.684 35.052 0)
		)
		(property "Value" "P8051AH"
			(at 8.128 35.052 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.524 -43.688 0)
		)
		(property "Datasheet" "https://www.datasheetarchive.com/datasheet/MCS%2051/Intel"
			(at 0 -45.72 0)
		)
		(property "Description" "MCS-51 8-bit Control-Oriented Microcontrollers, 4K x 8 masked ROM, 128 x 8 RAM, 2x 16-bit timers / event counters, 12MHz, DIP-40"
			(at 1.524 -41.656 0)
		)
		(property "ki_keywords" "8051 NMOS HMOS Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24*"
			(at 0 0 0)
		)
		(symbol "P8051AH_1_0"
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "P1.2")
				(number "3")
			)
		)
		(symbol "P8051AH_1_1"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "RST")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "P1.5")
				(number "6")
				(alternate "MOSI" output line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "P1.6")
				(number "7")
				(alternate "MISO" input line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "P1.7")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "P3.0/RXD")
				(number "10")
				(alternate "RXD" input line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "P3.1/TXD")
				(number "11")
				(alternate "TXD" output line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "P3.2/~{INT0}")
				(number "12")
				(alternate "~{INT0}" input line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "P3.3/~{INT1}")
				(number "13")
				(alternate "~{INT1}" input line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "P3.4/T0")
				(number "14")
				(alternate "T0" input line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "P3.5/T1")
				(number "15")
				(alternate "T1" input line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "P3.6/~{WR}")
				(number "16")
				(alternate "~{WR}" output line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "P3.7/~{RD}")
				(number "17")
				(alternate "~{RD}" input line)
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "XTAL1")
				(number "19")
			)
			(pin output line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "XTAL2")
				(number "18")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "~{EA}")
				(number "31")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "P0.0/AD0")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "P0.1/AD1")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "P0.2/AD2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "P0.3/AD3")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "P0.4/AD4")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "P0.5/AD5")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "P0.6/AD6")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "P0.7/AD7")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "P2.0/A8")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "P2.1/A9")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "P2.2/A10")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "P2.3/A11")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "P2.4/A12")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "P2.5/A13")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "P2.6/A14")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "P2.7/A15")
				(number "28")
			)
			(pin output line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "~{PSEN}")
				(number "29")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "ALE")
				(number "30")
				(alternate "~{PROG}" input line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "P8052AH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.684 35.052 0)
		)
		(property "Value" "P8052AH"
			(at 8.128 35.052 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.524 -43.688 0)
		)
		(property "Datasheet" "https://www.datasheetarchive.com/datasheet/MCS%2051/Intel"
			(at 0 -45.72 0)
		)
		(property "Description" "MCS-51 8-bit Control-Oriented Microcontrollers, 8K x 8 masked ROM, 256 x 8 RAM, 3x 16-bit timers / event counters, 12MHz, DIP-40"
			(at 1.524 -41.656 0)
		)
		(property "ki_keywords" "8051 NMOS HMOS Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24*"
			(at 0 0 0)
		)
		(symbol "P8052AH_1_0"
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "P1.2")
				(number "3")
			)
		)
		(symbol "P8052AH_1_1"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "RST")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "P1.0/T2")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "P1.1/T2EX")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "P1.5")
				(number "6")
				(alternate "MOSI" output line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "P1.6")
				(number "7")
				(alternate "MISO" input line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "P1.7")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "P3.0/RXD")
				(number "10")
				(alternate "RXD" input line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "P3.1/TXD")
				(number "11")
				(alternate "TXD" output line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "P3.2/~{INT0}")
				(number "12")
				(alternate "~{INT0}" input line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "P3.3/~{INT1}")
				(number "13")
				(alternate "~{INT1}" input line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "P3.4/T0")
				(number "14")
				(alternate "T0" input line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "P3.5/T1")
				(number "15")
				(alternate "T1" input line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "P3.6/~{WR}")
				(number "16")
				(alternate "~{WR}" output line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "P3.7/~{RD}")
				(number "17")
				(alternate "~{RD}" input line)
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "XTAL1")
				(number "19")
			)
			(pin output line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "XTAL2")
				(number "18")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "~{EA}")
				(number "31")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "P0.0/AD0")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "P0.1/AD1")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "P0.2/AD2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "P0.3/AD3")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "P0.4/AD4")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "P0.5/AD5")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "P0.6/AD6")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "P0.7/AD7")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "P2.0/A8")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "P2.1/A9")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "P2.2/A10")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "P2.3/A11")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "P2.4/A12")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "P2.5/A13")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "P2.6/A14")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "P2.7/A15")
				(number "28")
			)
			(pin output line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "~{PSEN}")
				(number "29")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "ALE")
				(number "30")
				(alternate "~{PROG}" input line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "P8751BH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.684 35.052 0)
		)
		(property "Value" "P8751BH"
			(at 8.128 35.052 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.524 -43.688 0)
		)
		(property "Datasheet" "https://www.datasheetarchive.com/datasheet/MCS%2051/Intel"
			(at 0 -45.72 0)
		)
		(property "Description" "MCS-51 8-bit Control-Oriented Microcontrollers, 4K x 8 EPROM, 128 x 8 RAM, 2x 16-bit timers / event counters, 12MHz, DIP-40"
			(at 1.524 -41.656 0)
		)
		(property "ki_keywords" "8051 NMOS HMOS Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24*"
			(at 0 0 0)
		)
		(symbol "P8751BH_1_0"
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "P1.2")
				(number "3")
			)
		)
		(symbol "P8751BH_1_1"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "RST")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "P1.0")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "P1.1")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "P1.5")
				(number "6")
				(alternate "MOSI" output line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "P1.6")
				(number "7")
				(alternate "MISO" input line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "P1.7")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "P3.0/RXD")
				(number "10")
				(alternate "RXD" input line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "P3.1/TXD")
				(number "11")
				(alternate "TXD" output line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "P3.2/~{INT0}")
				(number "12")
				(alternate "~{INT0}" input line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "P3.3/~{INT1}")
				(number "13")
				(alternate "~{INT1}" input line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "P3.4/T0")
				(number "14")
				(alternate "T0" input line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "P3.5/T1")
				(number "15")
				(alternate "T1" input line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "P3.6/~{WR}")
				(number "16")
				(alternate "~{WR}" output line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "P3.7/~{RD}")
				(number "17")
				(alternate "~{RD}" input line)
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "XTAL1")
				(number "19")
			)
			(pin output line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "XTAL2")
				(number "18")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "~{EA}/VPP")
				(number "31")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "P0.0/AD0")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "P0.1/AD1")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "P0.2/AD2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "P0.3/AD3")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "P0.4/AD4")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "P0.5/AD5")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "P0.6/AD6")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "P0.7/AD7")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "P2.0/A8")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "P2.1/A9")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "P2.2/A10")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "P2.3/A11")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "P2.4/A12")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "P2.5/A13")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "P2.6/A14")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "P2.7/A15")
				(number "28")
			)
			(pin output line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "~{PSEN}")
				(number "29")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "ALE/~{PROG}")
				(number "30")
				(alternate "~{PROG}" input line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "P8752BH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.684 35.052 0)
		)
		(property "Value" "P8752BH"
			(at 8.128 35.052 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.524 -43.688 0)
		)
		(property "Datasheet" "https://www.datasheetarchive.com/datasheet/MCS%2051/Intel"
			(at 0 -45.72 0)
		)
		(property "Description" "MCS-51 8-bit Control-Oriented Microcontrollers, 8K x 8 EPROM, 256 x 8 RAM, 3x 16-bit timers / event counters, 12MHz, DIP-40"
			(at 1.524 -41.656 0)
		)
		(property "ki_keywords" "8051 NMOS HMOS Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24*"
			(at 0 0 0)
		)
		(symbol "P8752BH_1_0"
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "P1.2")
				(number "3")
			)
		)
		(symbol "P8752BH_1_1"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "RST")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "P1.0/T2")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "P1.1/T2EX")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "P1.3")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "P1.4")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "P1.5")
				(number "6")
				(alternate "MOSI" output line)
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "P1.6")
				(number "7")
				(alternate "MISO" input line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "P1.7")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "P3.0/RXD")
				(number "10")
				(alternate "RXD" input line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "P3.1/TXD")
				(number "11")
				(alternate "TXD" output line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "P3.2/~{INT0}")
				(number "12")
				(alternate "~{INT0}" input line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "P3.3/~{INT1}")
				(number "13")
				(alternate "~{INT1}" input line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "P3.4/T0")
				(number "14")
				(alternate "T0" input line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "P3.5/T1")
				(number "15")
				(alternate "T1" input line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "P3.6/~{WR}")
				(number "16")
				(alternate "~{WR}" output line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "P3.7/~{RD}")
				(number "17")
				(alternate "~{RD}" input line)
			)
			(pin input line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "XTAL1")
				(number "19")
			)
			(pin output line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "XTAL2")
				(number "18")
			)
			(pin input line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "~{EA}/VPP")
				(number "31")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "P0.0/AD0")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "P0.1/AD1")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "P0.2/AD2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "P0.3/AD3")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "P0.4/AD4")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "P0.5/AD5")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "P0.6/AD6")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "P0.7/AD7")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "P2.0/A8")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "P2.1/A9")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "P2.2/A10")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "P2.3/A11")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "P2.4/A12")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "P2.5/A13")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "P2.6/A14")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "P2.7/A15")
				(number "28")
			)
			(pin output line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "~{PSEN}")
				(number "29")
			)
			(pin output line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "ALE/~{PROG}")
				(number "30")
				(alternate "~{PROG}" input line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "8039"
		(extends "8035")
		(property "Reference" "U"
			(at -13.97 35.56 0)
		)
		(property "Value" "8039"
			(at 8.89 35.56 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" ""
			(at 0 5.08 0)
		)
		(property "Description" "MCS-48 8-bit Microcontroller, No (EP)ROM, 128B RAM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCS-48 uC Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "8040"
		(extends "8035")
		(property "Reference" "U"
			(at -13.97 35.56 0)
		)
		(property "Value" "8040"
			(at 8.89 35.56 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" ""
			(at 0 5.08 0)
		)
		(property "Description" "MCS-48 8-bit Microcontroller, No (EP)ROM, 256B RAM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCS-48 uC Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "8048"
		(extends "8035")
		(property "Reference" "U"
			(at -13.97 35.56 0)
		)
		(property "Value" "8048"
			(at 8.89 35.56 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" ""
			(at 0 5.08 0)
		)
		(property "Description" "MCS-48 8-bit Microcontroller, 1KB Mask ROM, 64B RAM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCS-48 uC Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "8049"
		(extends "8035")
		(property "Reference" "U"
			(at -13.97 35.56 0)
		)
		(property "Value" "8049"
			(at 8.89 35.56 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" ""
			(at 0 5.08 0)
		)
		(property "Description" "MCS-48 8-bit Microcontroller, 2KB Mask ROM, 128B RAM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCS-48 uC Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "8050"
		(extends "8035")
		(property "Reference" "U"
			(at -13.97 35.56 0)
		)
		(property "Value" "8050"
			(at 8.89 35.56 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" ""
			(at 0 5.08 0)
		)
		(property "Description" "MCS-48 8-bit Microcontroller, 4KB Mask ROM, 256B RAM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCS-48 uC Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "8080A"
		(extends "8080")
		(property "Reference" "U"
			(at -7.62 44.45 0)
		)
		(property "Value" "8080A"
			(at 7.62 44.45 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 15.24 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/MCS-80/intel-8080.pdf"
			(at 0 15.24 0)
		)
		(property "Description" "8-bit N-channel Microprocessor, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "cpu mpu microprocessor"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24*"
			(at 0 0 0)
		)
	)
	(symbol "8088_Min_Mode"
		(extends "8088")
		(property "Reference" "U"
			(at -12.7 43.18 0)
		)
		(property "Value" "8088_Min_Mode"
			(at 10.16 43.18 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.27 2.54 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/x86/808x/datashts/8088/231456-006.pdf"
			(at 0 1.27 0)
		)
		(property "Description" "8088 (minimum mode), 8-Bit HMOS Microprocessor, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "80C186XL"
		(extends "M80C186XL")
		(property "Reference" "U"
			(at -12.7 72.39 0)
		)
		(property "Value" "80C186XL"
			(at 10.16 72.39 0)
		)
		(property "Footprint" ""
			(at 1.27 33.02 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/x86/8018x/datashts/27243104.PDF"
			(at 0 31.75 0)
		)
		(property "Description" "16-Bit High-Integration Embedded Processor"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC* PGA*Layout11x11*P2.54mm* LCC*"
			(at 0 0 0)
		)
	)
	(symbol "80C188XL"
		(extends "80C188")
		(property "Reference" "U"
			(at -12.7 72.39 0)
		)
		(property "Value" "80C188XL"
			(at 10.16 72.39 0)
		)
		(property "Footprint" ""
			(at 1.27 33.02 0)
		)
		(property "Datasheet" "http://datasheets.chipdb.org/Intel/x86/8018x/datashts/27243104.PDF"
			(at 0 31.75 0)
		)
		(property "Description" "16-Bit High-Integration Embedded Processor"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC* PGA*Layout11x11*P2.54mm* LCC*"
			(at 0 0 0)
		)
	)
	(symbol "8749"
		(extends "8748")
		(property "Reference" "U"
			(at -13.97 35.56 0)
		)
		(property "Value" "8749"
			(at 8.89 35.56 0)
		)
		(property "Footprint" ""
			(at 0 5.08 0)
		)
		(property "Datasheet" ""
			(at 0 5.08 0)
		)
		(property "Description" "i8748, MCS-48 8-bit Microcontroller with Internal EPROM, 2KB EPROM, 128B RAM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCS-48 uC Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "IA186XLPLC68IR2"
		(extends "M80C186XL")
		(property "Reference" "U"
			(at -12.7 72.39 0)
		)
		(property "Value" "IA186XLPLC68IR2"
			(at 10.16 72.39 0)
		)
		(property "Footprint" ""
			(at 1.27 33.02 0)
		)
		(property "Datasheet" "http://www.innovasic.com/upload/products/Innovasic_IA186XL_IA188XL_Data_Sheet_20110706_2.pdf"
			(at 0 31.75 0)
		)
		(property "Description" "MCU Replacement for Intel 80C186XL"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC* PGA*Layout11x11*P2.54mm* LCC*"
			(at 0 0 0)
		)
	)
	(symbol "IA188XLPLC68IR2"
		(extends "80C188")
		(property "Reference" "U"
			(at -12.7 72.39 0)
		)
		(property "Value" "IA188XLPLC68IR2"
			(at 10.16 72.39 0)
		)
		(property "Footprint" ""
			(at 1.27 33.02 0)
		)
		(property "Datasheet" "http://www.innovasic.com/upload/products/Innovasic_IA186XL_IA188XL_Data_Sheet_20110706_2.pdf"
			(at 0 31.75 0)
		)
		(property "Description" "MCU Replacement for Intel 80C188XL"
			(at 0 0 0)
		)
		(property "ki_keywords" "MPRO"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC* PGA*Layout11x11*P2.54mm* LCC*"
			(at 0 0 0)
		)
	)
	(symbol "P8031AH"
		(extends "P8051AH")
		(property "Reference" "U"
			(at -11.684 35.052 0)
		)
		(property "Value" "P8031AH"
			(at 8.128 35.052 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 1.524 -42.672 0)
		)
		(property "Datasheet" "https://www.datasheetarchive.com/datasheet/MCS%2051/Intel"
			(at 0 -44.704 0)
		)
		(property "Description" "MCS-51 8-bit Control-Oriented Microcontrollers, ROMless, 128 x 8 RAM, 2x 16-bit timers / event counters, 12MHz, DIP-40"
			(at 1.524 -40.64 0)
		)
		(property "ki_keywords" "8051 NMOS HMOS Obsolete"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24*"
			(at 0 0 0)
		)
	)
)
