(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ATmega1281V-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega1281V-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 128kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega1281V-8A_0_1")
		(symbol "ATmega1281V-8A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "20")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PG5")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega1281V-8M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega1281V-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 128kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega1281V-8M_0_1")
		(symbol "ATmega1281V-8M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "20")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PG5")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega162V-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega162V-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2513-8-bit-AVR-Microntroller-ATmega162_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega162V-8A_0_1")
		(symbol "ATmega162V-8A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "15")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "26")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega162V-8M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega162V-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2513-8-bit-AVR-Microntroller-ATmega162_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega162V-8M_0_1")
		(symbol "ATmega162V-8M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "15")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "26")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega162V-8P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega162V-8P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2513-8-bit-AVR-Microntroller-ATmega162_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "ATmega162V-8P_0_1")
		(symbol "ATmega162V-8P_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "19")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "29")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega164A-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164A-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega164A-A_0_1")
		(symbol "ATmega164A-A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "8")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "7")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "29")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega164A-C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164A-C"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATmega164A-C_0_1")
		(symbol "ATmega164A-C_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "C2")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "E1")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "D2")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "C7")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "A5")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "C1")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "G3")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "A7")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D1")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D7")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G1")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G7")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "E7")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "B5")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "C5")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "A6")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "B6")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "D5")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "B7")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "C6")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "D6")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "B4")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "C4")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "A3")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "B3")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "A2")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "B2")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "B1")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "C3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "F4")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "G5")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "F5")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "G6")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "F6")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "E5")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "F7")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "E6")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "D3")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "E2")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "F1")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "F2")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "G2")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "E3")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "F3")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "E4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega164A-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164A-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega164A-M_0_1")
		(symbol "ATmega164A-M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "8")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "7")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "29")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega164A-MC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 50.8 0)
		)
		(property "Value" "ATmega164A-MC"
			(at 2.54 -50.8 0)
		)
		(property "Footprint" "Package_DFN_QFN:Microchip_DRQFN-44-1EP_5x5mm_P0.7mm_EP2.65x2.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, DRQFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Microchip*DRQFN*1EP*5x5mm*P0.7mm*"
			(at 0 0 0)
		)
		(symbol "ATmega164A-MC_0_1")
		(symbol "ATmega164A-MC_1_1"
			(pin input line
				(at -17.78 43.18 0)
				(length 3.81)
				(name "~{RESET}")
				(number "B2")
			)
			(pin input line
				(at -17.78 38.1 0)
				(length 3.81)
				(name "XTAL1")
				(number "B4")
			)
			(pin output line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "XTAL2")
				(number "A4")
			)
			(pin passive line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "AREF")
				(number "A16")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "A21")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 3.81)
				(name "VCC")
				(number "A3")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "B8")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "A10")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B13")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B18")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B3")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "EP")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 3.81)
				(name "AVCC")
				(number "A15")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 3.81)
				(name "PA0")
				(number "B17")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 3.81)
				(name "PA1")
				(number "A20")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 3.81)
				(name "PA2")
				(number "B16")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 3.81)
				(name "PA3")
				(number "A19")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "PA4")
				(number "A18")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "PA5")
				(number "B15")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "PA6")
				(number "A17")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "PA7")
				(number "B14")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "PB0")
				(number "A22")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "PB1")
				(number "B19")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "PB2")
				(number "A23")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "PB3")
				(number "B20")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PB4")
				(number "A24")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PB5")
				(number "A1")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PB6")
				(number "B1")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PB7")
				(number "A2")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PC0")
				(number "B9")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PC1")
				(number "A11")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "PC2")
				(number "B10")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "PC3")
				(number "A12")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "PC4")
				(number "A13")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "PC5")
				(number "B11")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "PC6")
				(number "A14")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "PC7")
				(number "B12")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "PD0")
				(number "A5")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "PD1")
				(number "B5")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "PD2")
				(number "A6")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 3.81)
				(name "PD3")
				(number "A7")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 3.81)
				(name "PD4")
				(number "B6")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 3.81)
				(name "PD5")
				(number "A8")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 3.81)
				(name "PD6")
				(number "B7")
			)
			(pin bidirectional line
				(at 17.78 -43.18 180)
				(length 3.81)
				(name "PD7")
				(number "A9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega164A-P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164A-P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "ATmega164A-P_0_1")
		(symbol "ATmega164A-P_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "13")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "12")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "32")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega164PV-10A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164PV-10A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42742-ATmega164P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega164PV-10A_0_1")
		(symbol "ATmega164PV-10A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "8")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "7")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "29")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega164PV-10M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164PV-10M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42742-ATmega164P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega164PV-10M_0_1")
		(symbol "ATmega164PV-10M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "8")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "7")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "29")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega164PV-10P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164PV-10P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42742-ATmega164P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "ATmega164PV-10P_0_1")
		(symbol "ATmega164PV-10P_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "13")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "12")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "32")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega165A-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega165A-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega165A-A_0_1")
		(symbol "ATmega165A-A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PG5/~{RESET}")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin no_connect line
				(at -12.7 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega165A-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega165A-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega165A-M_0_1")
		(symbol "ATmega165A-M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PG5/~{RESET}")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin no_connect line
				(at -12.7 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega165PV-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega165PV-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8019.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega165PV-8A_0_1")
		(symbol "ATmega165PV-8A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "20")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin no_connect line
				(at -12.7 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega165PV-8M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega165PV-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8019.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega165PV-8M_0_1")
		(symbol "ATmega165PV-8M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "20")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin no_connect line
				(at -12.7 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega169PV-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega169PV-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8018.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega169PV-8A_0_1")
		(symbol "ATmega169PV-8A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "LCDCAP")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PG5/~{RESET}")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega169PV-8M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega169PV-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8018.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega169PV-8M_0_1")
		(symbol "ATmega169PV-8M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "LCDCAP")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PG5/~{RESET}")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega169PV-8MC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 50.8 0)
		)
		(property "Value" "ATmega169PV-8MC"
			(at 2.54 -50.8 0)
		)
		(property "Footprint" "Package_DFN_QFN:Microchip_DRQFN-64-1EP_7x7mm_P0.65mm_EP4.1x4.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8018.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, DRQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Microchip*DRQFN*1EP*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATmega169PV-8MC_0_1")
		(symbol "ATmega169PV-8MC_1_1"
			(pin input line
				(at -17.78 43.18 0)
				(length 3.81)
				(name "XTAL1")
				(number "A13")
			)
			(pin output line
				(at -17.78 38.1 0)
				(length 3.81)
				(name "XTAL2")
				(number "B11")
			)
			(pin passive line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "AREF")
				(number "A33")
			)
			(pin passive line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "LCDCAP")
				(number "B1")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "PG0")
				(number "B16")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "PG1")
				(number "A18")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "PG2")
				(number "A23")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "PG3")
				(number "A10")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "PG4")
				(number "B9")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PG5/~{RESET}")
				(number "A11")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "PF0")
				(number "B29")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "PF1")
				(number "A32")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "PF2")
				(number "B28")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "PF3")
				(number "A31")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "PF4")
				(number "B27")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "PF5")
				(number "A30")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "PF6")
				(number "B26")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "PF7")
				(number "A29")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 3.81)
				(name "PE0")
				(number "A1")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 3.81)
				(name "PE1")
				(number "A2")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 3.81)
				(name "PE2")
				(number "B2")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 3.81)
				(name "PE3")
				(number "A3")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 3.81)
				(name "PE4")
				(number "B3")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 3.81)
				(name "PE5")
				(number "A4")
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 3.81)
				(name "PE6")
				(number "B4")
			)
			(pin bidirectional line
				(at -17.78 -43.18 0)
				(length 3.81)
				(name "PE7")
				(number "A5")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 3.81)
				(name "VCC")
				(number "A28")
			)
			(pin passive line
				(at 0 53.34 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "B10")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 3.81)
				(name "GND")
				(number "A12")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A34")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B25")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "EP")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 3.81)
				(name "AVCC")
				(number "B30")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 3.81)
				(name "PA0")
				(number "B24")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 3.81)
				(name "PA1")
				(number "A27")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 3.81)
				(name "PA2")
				(number "A26")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 3.81)
				(name "PA3")
				(number "B23")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "PA4")
				(number "B22")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "PA5")
				(number "A25")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "PA6")
				(number "A24")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "PA7")
				(number "B21")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "PB0")
				(number "B5")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "PB1")
				(number "A6")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "PB2")
				(number "B6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "PB3")
				(number "A7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PB4")
				(number "A8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PB5")
				(number "B7")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PB6")
				(number "B8")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PB7")
				(number "A9")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PC0")
				(number "A19")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PC1")
				(number "B17")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "PC2")
				(number "A20")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "PC3")
				(number "B18")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "PC4")
				(number "A21")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "PC5")
				(number "B19")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "PC6")
				(number "A22")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "PC7")
				(number "B20")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "PD0")
				(number "B12")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "PD1")
				(number "A14")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "PD2")
				(number "B13")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 3.81)
				(name "PD3")
				(number "A15")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 3.81)
				(name "PD4")
				(number "B14")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 3.81)
				(name "PD5")
				(number "A16")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 3.81)
				(name "PD6")
				(number "A17")
			)
			(pin bidirectional line
				(at 17.78 -43.18 180)
				(length 3.81)
				(name "PD7")
				(number "B15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega16L-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega16L-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2466.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega16L-8A_0_1")
		(symbol "ATmega16L-8A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "8")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "7")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "29")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega16L-8M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega16L-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2466.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega16L-8M_0_1")
		(symbol "ATmega16L-8M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "8")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "7")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "29")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega16L-8P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega16L-8P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2466.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "ATmega16L-8P_0_1")
		(symbol "ATmega16L-8P_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "13")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "12")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "32")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega16M1-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega16M1-A"
			(at 5.08 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8209-8-bit%20AVR%20ATmega16M1-32M1-64M1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, CAN, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega16M1-A_0_1")
		(symbol "ATmega16M1-A_1_1"
			(pin passive line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "AREF/ISRC")
				(number "21")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "19")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "AGND")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PB0")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PB1")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB3")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB4")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB5")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB6")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB7")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PC0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PC1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC2")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC4")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC5")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC7")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD0")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD1")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD2")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD4")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD5")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD6")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD7")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "~{RESET}/PE0")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "XTAL1/PE1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "XTAL2/PE2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega16M1-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega16M1-M"
			(at 5.08 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.65x4.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8209-8-bit%20AVR%20ATmega16M1-32M1-64M1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, CAN, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATmega16M1-M_0_1")
		(symbol "ATmega16M1-M_1_1"
			(pin passive line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "AREF/ISRC")
				(number "21")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "19")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "AGND")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PB0")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PB1")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB3")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB4")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB5")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB6")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB7")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PC0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PC1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC2")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC4")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC5")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC7")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD0")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD1")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD2")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD4")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD5")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD6")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD7")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "~{RESET}/PE0")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "XTAL1/PE1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "XTAL2/PE2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega16U4-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega16U4-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1.25kB SRAM, 512B EEPROM, USB 2.0, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega16U4-A_0_1")
		(symbol "ATmega16U4-A_1_1"
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "~{RESET}")
				(number "13")
			)
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL1")
				(number "17")
			)
			(pin output line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "XTAL2")
				(number "16")
			)
			(pin passive line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "AREF")
				(number "42")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "VBUS")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "D+")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "D-")
				(number "3")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "UCAP")
				(number "6")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "UVCC")
				(number "2")
			)
			(pin passive line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "UGND")
				(number "5")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "34")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "24")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "AVCC")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PB0")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PB1")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PB2")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB3")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB4")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB5")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB6")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB7")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PC6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PC7")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PD0")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PD1")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PD2")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PD3")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PD4")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PD5")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD7")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{HWB}/PE2")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PE6")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PF0")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PF1")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PF4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PF5")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PF6")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PF7")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega16U4-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega16U4-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1.25kB SRAM, 512B EEPROM, USB 2.0, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega16U4-M_0_1")
		(symbol "ATmega16U4-M_1_1"
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "~{RESET}")
				(number "13")
			)
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL1")
				(number "17")
			)
			(pin output line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "XTAL2")
				(number "16")
			)
			(pin passive line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "AREF")
				(number "42")
			)
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "VBUS")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "D+")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "D-")
				(number "3")
			)
			(pin passive line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "UCAP")
				(number "6")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "UVCC")
				(number "2")
			)
			(pin passive line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "UGND")
				(number "5")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "34")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "24")
			)
			(pin passive line
				(at 2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "AVCC")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PB0")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PB1")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PB2")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB3")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB4")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB5")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB6")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB7")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PC6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PC7")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PD0")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PD1")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PD2")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PD3")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PD4")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PD5")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD7")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{HWB}/PE2")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PE6")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PF0")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PF1")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PF4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PF5")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PF6")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PF7")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega3208-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATmega3208-A"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40002017A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 4kB SRAM, 256B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega3208-A_0_1")
		(symbol "ATmega3208-A_1_1"
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "UPDI")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF0/TOSC1")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PF1/TOSC2")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PF2")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF3")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF4")
				(number "24")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PF5")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PF6/~{RESET}")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PD0")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PD1")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PD2")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PD3")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PD4")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PD5")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PD6")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PD7")
				(number "17")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVDD")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "EXTCLK/PA0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC0")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC1")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC2")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC3")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega3208-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATmega3208-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40002017A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 4kB SRAM, 256B EEPROM, VQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega3208-M_0_1")
		(symbol "ATmega3208-M_1_1"
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "UPDI")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF0/TOSC1")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PF1/TOSC2")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PF2")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF3")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PF4")
				(number "24")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PF5")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PF6/~{RESET}")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PD0")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PD1")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PD2")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PD3")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PD4")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PD5")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PD6")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PD7")
				(number "17")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVDD")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "EXTCLK/PA0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC0")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC1")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC2")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC3")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega3208-X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATmega3208-X"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40002018A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 4kB SRAM, 256B EEPROM, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATmega3208-X_0_1")
		(symbol "ATmega3208-X_1_1"
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "UPDI")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF0/TOSC1")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PF1/TOSC2")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PF6/~{RESET}")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PD0")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PD1")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PD2")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PD3")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PD4")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PD7")
				(number "13")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVDD")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "EXTCLK/PA0")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA7")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC2")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega3209-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATmega3209-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40002016A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 4kB SRAM, 256B EEPROM, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega3209-A_0_1")
		(symbol "ATmega3209-A_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "UPDI")
				(number "41")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "36")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF3")
				(number "37")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PF4")
				(number "38")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PF5")
				(number "39")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF6/~{RESET}")
				(number "40")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PE2")
				(number "32")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PD5")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PD7")
				(number "27")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "42")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PC5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PC6")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PC7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega3209-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATmega3209-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-48-1EP_6x6mm_P0.4mm_EP4.62x4.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40002016A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 4kB SRAM, 256B EEPROM, UQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1EP*6x6mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "ATmega3209-M_0_1")
		(symbol "ATmega3209-M_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "UPDI")
				(number "41")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PF0")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PF1")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "36")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PF3")
				(number "37")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PF4")
				(number "38")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PF5")
				(number "39")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PF6/~{RESET}")
				(number "40")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PE2")
				(number "32")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PD5")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PD7")
				(number "27")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "14")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "42")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PC5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PC6")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PC7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega324PB-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega324PB-A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001908A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega324PB-A_0_1")
		(symbol "ATmega324PB-A_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PE0/XTAL2")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PE1/XTAL1")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PE2")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PE3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PE4/AREF")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PE5")
				(number "38")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PE6")
				(number "39")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PD0")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PD1")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PD2")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PD3")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PD4")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PD5")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PD6")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PD7")
				(number "16")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVCC")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PC7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega324PB-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega324PB-M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001908A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega324PB-M_0_1")
		(symbol "ATmega324PB-M_1_1"
			(pin input line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PE0/XTAL2")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PE1/XTAL1")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PE2")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PE3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PE4/AREF")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PE5")
				(number "38")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PE6")
				(number "39")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PD0")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PD1")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PD2")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PD3")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PD4")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PD5")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PD6")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PD7")
				(number "16")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVCC")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PC7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega3250V-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega3250V-8A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2570.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega3250V-8A_0_1")
		(symbol "ATmega3250V-8A_1_1"
			(pin input line
				(at -20.32 55.88 0)
				(length 3.81)
				(name "XTAL1")
				(number "34")
			)
			(pin output line
				(at -20.32 50.8 0)
				(length 3.81)
				(name "XTAL2")
				(number "33")
			)
			(pin passive line
				(at -20.32 45.72 0)
				(length 3.81)
				(name "AREF")
				(number "98")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 3.81)
				(name "PJ0")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "PJ1")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "PJ2")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "PJ3")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "PJ4")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "PJ5")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "PJ6")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "PH0")
				(number "63")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PH1")
				(number "64")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PH2")
				(number "65")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PH3")
				(number "66")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "PH4")
				(number "84")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "PH5")
				(number "85")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "PH6")
				(number "86")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "PH7")
				(number "87")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "PG0")
				(number "51")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "PG1")
				(number "52")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PG2")
				(number "70")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PG3")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "PG4")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PG5/~{RESET}")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 3.81)
				(name "PF0")
				(number "97")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "PF1")
				(number "96")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "PF2")
				(number "95")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "PF3")
				(number "94")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "PF4")
				(number "93")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "PF5")
				(number "92")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "PF6")
				(number "91")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "PF7")
				(number "90")
			)
			(pin no_connect line
				(at -15.24 40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -15.24 38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -15.24 35.56 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at -15.24 15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -15.24 12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -15.24 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -15.24 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at -15.24 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at -15.24 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at -15.24 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "42")
			)
			(pin no_connect line
				(at -12.7 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "59")
			)
			(pin no_connect line
				(at -10.16 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "60")
			)
			(pin no_connect line
				(at -7.62 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "61")
			)
			(pin no_connect line
				(at -5.08 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "62")
			)
			(pin no_connect line
				(at -2.54 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "67")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 3.81)
				(name "VCC")
				(number "10")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "31")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "80")
			)
			(pin power_in line
				(at 0 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin power_in line
				(at 2.54 63.5 270)
				(length 3.81)
				(name "AVCC")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -63.5 90)
				(length 3.81)
				(name "AGND")
				(number "99")
			)
			(pin no_connect line
				(at 5.08 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "79")
			)
			(pin no_connect line
				(at 7.62 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "82")
			)
			(pin no_connect line
				(at 10.16 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "83")
			)
			(pin no_connect line
				(at 12.7 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "88")
			)
			(pin no_connect line
				(at 15.24 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "89")
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 3.81)
				(name "PA0")
				(number "78")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "PA1")
				(number "77")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "PA2")
				(number "76")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "PA3")
				(number "75")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "PA4")
				(number "74")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "PA5")
				(number "73")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "PA6")
				(number "72")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "PA7")
				(number "71")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "PB0")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "PB1")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "PB2")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "PB3")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "PB4")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "PB5")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "PB6")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "PB7")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "PC0")
				(number "53")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "PC1")
				(number "54")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "PC2")
				(number "55")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "PC3")
				(number "56")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "PC4")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "PC5")
				(number "58")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "PC6")
				(number "68")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PC7")
				(number "69")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PD0")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PD1")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PD2")
				(number "45")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PD3")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "PD4")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "PD5")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "PD6")
				(number "49")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "PD7")
				(number "50")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 3.81)
				(name "PE7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega325V-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega325V-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2570.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega325V-8A_0_1")
		(symbol "ATmega325V-8A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PG5/~{RESET}")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin no_connect line
				(at -12.7 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega325V-8M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega325V-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2570.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega325V-8M_0_1")
		(symbol "ATmega325V-8M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PG5/~{RESET}")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin no_connect line
				(at -12.7 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega3290V-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega3290V-8A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2552.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega3290V-8A_0_1")
		(symbol "ATmega3290V-8A_1_1"
			(pin input line
				(at -20.32 55.88 0)
				(length 3.81)
				(name "XTAL1")
				(number "34")
			)
			(pin output line
				(at -20.32 50.8 0)
				(length 3.81)
				(name "XTAL2")
				(number "33")
			)
			(pin passive line
				(at -20.32 45.72 0)
				(length 3.81)
				(name "AREF")
				(number "98")
			)
			(pin passive line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "LCDCAP")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 3.81)
				(name "PJ0")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "PJ1")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "PJ2")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "PJ3")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "PJ4")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "PJ5")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "PJ6")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "PH0")
				(number "63")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PH1")
				(number "64")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PH2")
				(number "65")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PH3")
				(number "66")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "PH4")
				(number "84")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "PH5")
				(number "85")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "PH6")
				(number "86")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "PH7")
				(number "87")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "PG0")
				(number "51")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "PG1")
				(number "52")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PG2")
				(number "70")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PG3")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "PG4")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PG5/~{RESET}")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 3.81)
				(name "PF0")
				(number "97")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "PF1")
				(number "96")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "PF2")
				(number "95")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "PF3")
				(number "94")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "PF4")
				(number "93")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "PF5")
				(number "92")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "PF6")
				(number "91")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "PF7")
				(number "90")
			)
			(pin no_connect line
				(at -15.24 38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -15.24 35.56 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin no_connect line
				(at -15.24 15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -15.24 12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -15.24 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -15.24 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at -15.24 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "35")
			)
			(pin no_connect line
				(at -15.24 -33.02 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at -15.24 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "42")
			)
			(pin no_connect line
				(at -12.7 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "59")
			)
			(pin no_connect line
				(at -10.16 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "60")
			)
			(pin no_connect line
				(at -7.62 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "61")
			)
			(pin no_connect line
				(at -5.08 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "62")
			)
			(pin no_connect line
				(at -2.54 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "67")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 3.81)
				(name "VCC")
				(number "10")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "31")
			)
			(pin passive line
				(at 0 63.5 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "80")
			)
			(pin power_in line
				(at 0 -63.5 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -63.5 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin power_in line
				(at 2.54 63.5 270)
				(length 3.81)
				(name "AVCC")
				(number "100")
			)
			(pin power_in line
				(at 2.54 -63.5 90)
				(length 3.81)
				(name "AGND")
				(number "99")
			)
			(pin no_connect line
				(at 5.08 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "79")
			)
			(pin no_connect line
				(at 7.62 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "82")
			)
			(pin no_connect line
				(at 10.16 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "83")
			)
			(pin no_connect line
				(at 12.7 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "88")
			)
			(pin no_connect line
				(at 15.24 -58.42 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "89")
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 3.81)
				(name "PA0")
				(number "78")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "PA1")
				(number "77")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "PA2")
				(number "76")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "PA3")
				(number "75")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "PA4")
				(number "74")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "PA5")
				(number "73")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "PA6")
				(number "72")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "PA7")
				(number "71")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "PB0")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "PB1")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "PB2")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "PB3")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "PB4")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "PB5")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "PB6")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "PB7")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "PC0")
				(number "53")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "PC1")
				(number "54")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "PC2")
				(number "55")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "PC3")
				(number "56")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "PC4")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "PC5")
				(number "58")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "PC6")
				(number "68")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PC7")
				(number "69")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PD0")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PD1")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PD2")
				(number "45")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PD3")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "PD4")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "PD5")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "PD6")
				(number "49")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "PD7")
				(number "50")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 3.81)
				(name "PE7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega329V-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega329V-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2552.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega329V-8A_0_1")
		(symbol "ATmega329V-8A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "LCDCAP")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PG5/~{RESET}")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega329V-8M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega329V-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2552.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega329V-8M_0_1")
		(symbol "ATmega329V-8M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "LCDCAP")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PG5/~{RESET}")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega406-1AA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega406-1AA"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2548-8-bit-AVR-Microcontroller-Battery-Management-ATmega406_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "1MHz, 40kB Flash, 2kB SRAM, 512B EEPROM, JTAG, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR battery management"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega406-1AA_1_1"
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "BATT")
				(number "31")
			)
			(pin input line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "SCL")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "SDA")
				(number "24")
			)
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "~{RESET}")
				(number "13")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "XTAL1")
				(number "14")
			)
			(pin output line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "XTAL2")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PD0")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PD1")
				(number "28")
			)
			(pin open_collector line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PC0")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB0")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PB1")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PB2")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PB3")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PB4")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PB5")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PB6")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PB7")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PA0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PA1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PA2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PA3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PA4")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PA5")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PA6")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PA7")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "SGND")
				(number "1")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VFET")
				(number "34")
			)
			(pin output line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "OC")
				(number "33")
			)
			(pin output line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "OPC")
				(number "32")
			)
			(pin output line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "OD")
				(number "35")
			)
			(pin input line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PVT")
				(number "36")
			)
			(pin input line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PV4")
				(number "38")
			)
			(pin input line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PV3")
				(number "39")
			)
			(pin input line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PV2")
				(number "40")
			)
			(pin input line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PV1")
				(number "41")
			)
			(pin input line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "NV")
				(number "42")
			)
			(pin input line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PPI")
				(number "45")
			)
			(pin input line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PI")
				(number "46")
			)
			(pin input line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "NI")
				(number "47")
			)
			(pin input line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "NNI")
				(number "48")
			)
			(pin passive line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "VREF")
				(number "43")
			)
			(pin passive line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "VREFGND")
				(number "44")
			)
			(pin power_out line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "VREG")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega48A-CC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48A-CC"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-32_4.0x4.0mm_Layout6x6_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, UFBGA-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*4.0x4.0mm*Layout6x6*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega48A-CC_0_1")
		(symbol "ATmega48A-CC_1_1"
			(pin passive line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "AREF")
				(number "D5")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "ADC6")
				(number "D6")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "ADC7")
				(number "C5")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "D1")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "D2")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "C1")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C2")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVCC")
				(number "E5")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB0")
				(number "E3")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB1")
				(number "F4")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB2")
				(number "E4")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB3")
				(number "F5")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB4")
				(number "F6")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB5")
				(number "E6")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "XTAL1/PB6")
				(number "E1")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "XTAL2/PB7")
				(number "F1")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC0")
				(number "B6")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC1")
				(number "A6")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC2")
				(number "A5")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC3")
				(number "B5")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC4")
				(number "A4")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC5")
				(number "B4")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "A3")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD0")
				(number "B3")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD1")
				(number "A2")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD2")
				(number "A1")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD3")
				(number "B1")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD4")
				(number "B2")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD5")
				(number "F2")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD6")
				(number "E2")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD7")
				(number "F3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega48PB-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48PB-A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001909A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega48PB-A_0_1")
		(symbol "ATmega48PB-A_1_1"
			(pin passive line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "AREF")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PE0")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PE1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PE2")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PE3")
				(number "22")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "XTAL1/PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "XTAL2/PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega48PB-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48PB-M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001909A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega48PB-M_0_1")
		(symbol "ATmega48PB-M_1_1"
			(pin passive line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "AREF")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PE0")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PE1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PE2")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PE3")
				(number "22")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "XTAL1/PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "XTAL2/PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega48PV-10A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48PV-10A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 512B SRAM, 256B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega48PV-10A_0_1")
		(symbol "ATmega48PV-10A_1_1"
			(pin passive line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "AREF")
				(number "20")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "ADC6")
				(number "19")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "ADC7")
				(number "22")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "6")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "XTAL1/PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "XTAL2/PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega48PV-10M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48PV-10M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 512B SRAM, 256B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega48PV-10M_0_1")
		(symbol "ATmega48PV-10M_1_1"
			(pin passive line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "AREF")
				(number "20")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "ADC6")
				(number "19")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "ADC7")
				(number "22")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "6")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "XTAL1/PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "XTAL2/PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega48PV-10MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48PV-10MM"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 512B SRAM, 256B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "ATmega48PV-10MM_0_1")
		(symbol "ATmega48PV-10MM_1_1"
			(pin passive line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "AREF")
				(number "17")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVCC")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "XTAL1/PB6")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "XTAL2/PB7")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD5")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD6")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega48PV-10P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48PV-10P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 512B SRAM, 256B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ATmega48PV-10P_0_1")
		(symbol "ATmega48PV-10P_1_1"
			(pin passive line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "AREF")
				(number "21")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVCC")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB0")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB4")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB5")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "XTAL1/PB6")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "XTAL2/PB7")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD2")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD3")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega48V-10A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48V-10A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 512B SRAM, 256B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega48V-10A_0_1")
		(symbol "ATmega48V-10A_1_1"
			(pin passive line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "AREF")
				(number "20")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "ADC6")
				(number "19")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "ADC7")
				(number "22")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "6")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "XTAL1/PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "XTAL2/PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega48V-10M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48V-10M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 512B SRAM, 256B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega48V-10M_0_1")
		(symbol "ATmega48V-10M_1_1"
			(pin passive line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "AREF")
				(number "20")
			)
			(pin input line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "ADC6")
				(number "19")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "ADC7")
				(number "22")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "6")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "XTAL1/PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "XTAL2/PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega48V-10MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48V-10MM"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 512B SRAM, 256B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "ATmega48V-10MM_0_1")
		(symbol "ATmega48V-10MM_1_1"
			(pin passive line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "AREF")
				(number "17")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVCC")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "XTAL1/PB6")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "XTAL2/PB7")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD5")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD6")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega48V-10P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48V-10P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 512B SRAM, 256B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ATmega48V-10P_0_1")
		(symbol "ATmega48V-10P_1_1"
			(pin passive line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "AREF")
				(number "21")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "AVCC")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB0")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB4")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB5")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "XTAL1/PB6")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "XTAL2/PB7")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD2")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD3")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega640V-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega640V-8A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 64kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega640V-8A_0_1")
		(symbol "ATmega640V-8A_1_1"
			(pin input line
				(at -20.32 66.04 0)
				(length 3.81)
				(name "~{RESET}")
				(number "30")
			)
			(pin input line
				(at -20.32 60.96 0)
				(length 3.81)
				(name "XTAL1")
				(number "34")
			)
			(pin output line
				(at -20.32 55.88 0)
				(length 3.81)
				(name "XTAL2")
				(number "33")
			)
			(pin passive line
				(at -20.32 50.8 0)
				(length 3.81)
				(name "AREF")
				(number "98")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 3.81)
				(name "PL0")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "PL1")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "PL2")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "PL3")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 3.81)
				(name "PL4")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "PL5")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "PL6")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "PL7")
				(number "42")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "PK0")
				(number "89")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "PK1")
				(number "88")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "PK2")
				(number "87")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "PK3")
				(number "86")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "PK4")
				(number "85")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PK5")
				(number "84")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PK6")
				(number "83")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PK7")
				(number "82")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "PJ0")
				(number "63")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "PJ1")
				(number "64")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "PJ2")
				(number "65")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "PJ3")
				(number "66")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "PJ4")
				(number "67")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "PJ5")
				(number "68")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PJ6")
				(number "69")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PJ7")
				(number "79")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PH0")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "PH1")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "PH2")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "PH3")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 3.81)
				(name "PH4")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "PH5")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "PH6")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "PH7")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "PG0")
				(number "51")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "PG1")
				(number "52")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "PG2")
				(number "70")
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "PG3")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 -58.42 0)
				(length 3.81)
				(name "PG4")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 -60.96 0)
				(length 3.81)
				(name "PG5")
				(number "1")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 3.81)
				(name "VCC")
				(number "10")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "31")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "61")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "80")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "99")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 3.81)
				(name "AVCC")
				(number "100")
			)
			(pin bidirectional line
				(at 20.32 66.04 180)
				(length 3.81)
				(name "PA0")
				(number "78")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 3.81)
				(name "PA1")
				(number "77")
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 3.81)
				(name "PA2")
				(number "76")
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "PA3")
				(number "75")
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 3.81)
				(name "PA4")
				(number "74")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "PA5")
				(number "73")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "PA6")
				(number "72")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "PA7")
				(number "71")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "PB0")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "PB1")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "PB2")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "PB3")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "PB4")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "PB5")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "PB6")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "PB7")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "PC0")
				(number "53")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "PC1")
				(number "54")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "PC2")
				(number "55")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "PC3")
				(number "56")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "PC4")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "PC5")
				(number "58")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "PC6")
				(number "59")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "PC7")
				(number "60")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "PD0")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "PD1")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PD2")
				(number "45")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "PD3")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PD4")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PD5")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PD6")
				(number "49")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PD7")
				(number "50")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "PE7")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "PF0")
				(number "97")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "PF1")
				(number "96")
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 3.81)
				(name "PF2")
				(number "95")
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 3.81)
				(name "PF3")
				(number "94")
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 3.81)
				(name "PF4")
				(number "93")
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 3.81)
				(name "PF5")
				(number "92")
			)
			(pin bidirectional line
				(at 20.32 -63.5 180)
				(length 3.81)
				(name "PF6")
				(number "91")
			)
			(pin bidirectional line
				(at 20.32 -66.04 180)
				(length 3.81)
				(name "PF7")
				(number "90")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega640V-8C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega640V-8C"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_9.0x9.0mm_Layout10x10_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at -29.21 71.12 0)
		)
		(property "Description" "8MHz, 64kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*9.0x9.0mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega640V-8C_0_1")
		(symbol "ATmega640V-8C_1_1"
			(pin input line
				(at -20.32 66.04 0)
				(length 3.81)
				(name "~{RESET}")
				(number "H3")
			)
			(pin input line
				(at -20.32 60.96 0)
				(length 3.81)
				(name "XTAL1")
				(number "K5")
			)
			(pin output line
				(at -20.32 55.88 0)
				(length 3.81)
				(name "XTAL2")
				(number "J5")
			)
			(pin passive line
				(at -20.32 50.8 0)
				(length 3.81)
				(name "AREF")
				(number "A2")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 3.81)
				(name "PL0")
				(number "J4")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "PL1")
				(number "H4")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "PL2")
				(number "G5")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "PL3")
				(number "H5")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 3.81)
				(name "PL4")
				(number "F5")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "PL5")
				(number "K6")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "PL6")
				(number "J6")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "PL7")
				(number "H6")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "PK0")
				(number "A6")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "PK1")
				(number "B6")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "PK2")
				(number "C6")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "PK3")
				(number "A7")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "PK4")
				(number "B7")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PK5")
				(number "C7")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PK6")
				(number "A8")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PK7")
				(number "B8")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "PJ0")
				(number "F8")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "PJ1")
				(number "F7")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "PJ2")
				(number "E10")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "PJ3")
				(number "E9")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "PJ4")
				(number "E8")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "PJ5")
				(number "E7")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PJ6")
				(number "E6")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PJ7")
				(number "C8")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PH0")
				(number "E2")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "PH1")
				(number "E3")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "PH2")
				(number "D5")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "PH3")
				(number "E4")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 3.81)
				(name "PH4")
				(number "F2")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "PH5")
				(number "E5")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "PH6")
				(number "F3")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "PH7")
				(number "J1")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "PG0")
				(number "K10")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "PG1")
				(number "J10")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "PG2")
				(number "D10")
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "PG3")
				(number "J2")
			)
			(pin bidirectional line
				(at -20.32 -58.42 0)
				(length 3.81)
				(name "PG4")
				(number "K2")
			)
			(pin bidirectional line
				(at -20.32 -60.96 0)
				(length 3.81)
				(name "PG5")
				(number "B2")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 3.81)
				(name "VCC")
				(number "A10")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "F1")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "G10")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "K3")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "A1")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A9")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F10")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G1")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K4")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 3.81)
				(name "AVCC")
				(number "B1")
			)
			(pin bidirectional line
				(at 20.32 66.04 180)
				(length 3.81)
				(name "PA0")
				(number "B9")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 3.81)
				(name "PA1")
				(number "C9")
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 3.81)
				(name "PA2")
				(number "B10")
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "PA3")
				(number "C10")
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 3.81)
				(name "PA4")
				(number "D6")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "PA5")
				(number "D7")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "PA6")
				(number "D8")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "PA7")
				(number "D9")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "PB0")
				(number "F4")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "PB1")
				(number "G2")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "PB2")
				(number "G3")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "PB3")
				(number "H1")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "PB4")
				(number "H2")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "PB5")
				(number "G4")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "PB6")
				(number "J3")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "PB7")
				(number "K1")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "PC0")
				(number "J9")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "PC1")
				(number "J8")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "PC2")
				(number "H10")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "PC3")
				(number "H9")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "PC4")
				(number "H8")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "PC5")
				(number "G8")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "PC6")
				(number "G9")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "PC7")
				(number "F9")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "PD0")
				(number "G6")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "PD1")
				(number "F6")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PD2")
				(number "K7")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "PD3")
				(number "J7")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PD4")
				(number "H7")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PD5")
				(number "G7")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PD6")
				(number "K8")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PD7")
				(number "K9")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "PE0")
				(number "C2")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "PE1")
				(number "C3")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "PE2")
				(number "C1")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "PE3")
				(number "D1")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "PE4")
				(number "D2")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "PE5")
				(number "D3")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "PE6")
				(number "D4")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "PE7")
				(number "E1")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "PF0")
				(number "A3")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "PF1")
				(number "B3")
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 3.81)
				(name "PF2")
				(number "A4")
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 3.81)
				(name "PF3")
				(number "B4")
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 3.81)
				(name "PF4")
				(number "C4")
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 3.81)
				(name "PF5")
				(number "A5")
			)
			(pin bidirectional line
				(at 20.32 -63.5 180)
				(length 3.81)
				(name "PF6")
				(number "B5")
			)
			(pin bidirectional line
				(at 20.32 -66.04 180)
				(length 3.81)
				(name "PF7")
				(number "C5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega644V-10A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644V-10A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2593.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega644V-10A_0_1")
		(symbol "ATmega644V-10A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "8")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "7")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "29")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega644V-10M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644V-10M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2593.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega644V-10M_0_1")
		(symbol "ATmega644V-10M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "8")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "7")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "29")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega644V-10P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644V-10P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2593.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "ATmega644V-10P_0_1")
		(symbol "ATmega644V-10P_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "13")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "12")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "32")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega64L-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega64L-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2490-8-bit-avr-microcontroller-atmega64-l_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega64L-8A_0_1")
		(symbol "ATmega64L-8A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "20")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "~{PEN}")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega64L-8M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega64L-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2490-8-bit-avr-microcontroller-atmega64-l_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega64L-8M_0_1")
		(symbol "ATmega64L-8M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "20")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "~{PEN}")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega8515L-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8515L-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2512.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 8kB Flash, 512B SRAM, 512B EEPROM, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega8515L-8A_0_1")
		(symbol "ATmega8515L-8A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "15")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "26")
			)
			(pin no_connect line
				(at -12.7 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -12.7 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at -12.7 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "39")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega8515L-8J"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8515L-8J"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_LCC:PLCC-44"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2512.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 8kB Flash, 512B SRAM, 512B EEPROM, PLCC-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
		(symbol "ATmega8515L-8J_0_1")
		(symbol "ATmega8515L-8J_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "10")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "21")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "32")
			)
			(pin no_connect line
				(at -12.7 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -12.7 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -12.7 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at -12.7 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "44")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega8515L-8M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8515L-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2512.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 8kB Flash, 512B SRAM, 512B EEPROM, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega8515L-8M_0_1")
		(symbol "ATmega8515L-8M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "15")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "26")
			)
			(pin no_connect line
				(at -12.7 -38.1 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 -40.64 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -12.7 -43.18 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at -12.7 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "39")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega8515L-8P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8515L-8P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2512.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 8kB Flash, 512B SRAM, 512B EEPROM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "ATmega8515L-8P_0_1")
		(symbol "ATmega8515L-8P_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "19")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "29")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "40")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega8535L-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8535L-8A"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2502.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 8kB Flash, 512B SRAM, 512B EEPROM, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega8535L-8A_0_1")
		(symbol "ATmega8535L-8A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "8")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "7")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "29")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "27")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 2.54)
				(name "AGND")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega8535L-8J"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8535L-8J"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_LCC:PLCC-44"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2502.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 8kB Flash, 512B SRAM, 512B EEPROM, PLCC-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
		(symbol "ATmega8535L-8J_0_1")
		(symbol "ATmega8535L-8J_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "10")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "14")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "13")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "35")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "23")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "44")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "33")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 2.54)
				(name "AGND")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "22")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega8535L-8M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8535L-8M"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2502.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 8kB Flash, 512B SRAM, 512B EEPROM, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega8535L-8M_0_1")
		(symbol "ATmega8535L-8M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "4")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "8")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "7")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "29")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "17")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "38")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "27")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 2.54)
				(name "AGND")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega8535L-8P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8535L-8P"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2502.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 8kB Flash, 512B SRAM, 512B EEPROM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "ATmega8535L-8P_0_1")
		(symbol "ATmega8535L-8P_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "13")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "12")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "32")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "30")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 2.54)
				(name "AGND")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega8L-8A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATmega8L-8A"
			(at 5.08 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2486-8-bit-avr-microcontroller-atmega8_l_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega8L-8A_0_1")
		(symbol "ATmega8L-8A_1_1"
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PC6/~{RESET}")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PB6/XTAL1")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PB7/XTAL2")
				(number "8")
			)
			(pin passive line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "AREF")
				(number "20")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "ADC6")
				(number "19")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "ADC7")
				(number "22")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "AGND")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega8L-8M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATmega8L-8M"
			(at 5.08 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2486-8-bit-avr-microcontroller-atmega8_l_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega8L-8M_0_1")
		(symbol "ATmega8L-8M_1_1"
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PC6/~{RESET}")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PB6/XTAL1")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PB7/XTAL2")
				(number "8")
			)
			(pin passive line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "AREF")
				(number "20")
			)
			(pin input line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "ADC6")
				(number "19")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "ADC7")
				(number "22")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "AGND")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega8L-8P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATmega8L-8P"
			(at 5.08 -34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2486-8-bit-avr-microcontroller-atmega8_l_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ATmega8L-8P_0_1")
		(symbol "ATmega8L-8P_1_1"
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PC6/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PB6/XTAL1")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PB7/XTAL2")
				(number "10")
			)
			(pin passive line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "AREF")
				(number "21")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "AGND")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB0")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB4")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB5")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD2")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD3")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega8U2-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATmega8U2-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7799.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATmega8U2-A_0_1")
		(symbol "ATmega8U2-A_1_1"
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PC1/~{RESET}")
				(number "24")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "XTAL1")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0/XTAL2")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "D+")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "D-")
				(number "30")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "UCAP")
				(number "27")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "UVCC")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "UGND")
				(number "28")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB0")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PB1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB3")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB4")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB5")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB6")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB7")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PC2")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PC4")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PC5")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PC6")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PC7")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PD0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PD1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PD2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PD3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PD4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "~{HWB}/PD7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega8U2-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATmega8U2-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7799.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATmega8U2-M_0_1")
		(symbol "ATmega8U2-M_1_1"
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PC1/~{RESET}")
				(number "24")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "XTAL1")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0/XTAL2")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "D+")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "D-")
				(number "30")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "UCAP")
				(number "27")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "UVCC")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "UGND")
				(number "28")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB0")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PB1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB3")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB4")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB5")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB6")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB7")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PC2")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PC4")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PC5")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PC6")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PC7")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PD0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PD1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PD2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PD3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PD4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "~{HWB}/PD7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega128B3-MC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 48.26 0)
		)
		(property "Value" "ATxmega128B3-MC"
			(at 5.08 -48.26 0)
		)
		(property "Footprint" "Package_DFN_QFN:Microchip_DRQFN-64-1EP_7x7mm_P0.65mm_EP4.1x4.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8074-8-and-16-bit-AVR-Microcontroller-XMEGA-B-ATxmega64B3-ATxmega128B3_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, LCD, DRQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Microchip*DRQFN*1EP*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega128B3-MC_0_1")
		(symbol "ATxmega128B3-MC_1_1"
			(pin input line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "~{RESET}/PDI_CLK")
				(number "B6")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "PDI_DATA")
				(number "B7")
			)
			(pin passive line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "CAPH")
				(number "A26")
			)
			(pin passive line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "CAPL")
				(number "A25")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "PR0/XTAL2")
				(number "B25")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "PR1/XTAL1")
				(number "A29")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PB0/AREF")
				(number "A30")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PB1")
				(number "A31")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PB2")
				(number "B28")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "PB3")
				(number "A32")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "PB4")
				(number "B29")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "PB5")
				(number "A33")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "PB6")
				(number "A34")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "PB7")
				(number "B30")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "PC0")
				(number "A1")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PC1")
				(number "B1")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PC2")
				(number "A2")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "PC3")
				(number "B2")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PC4")
				(number "A3")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "PC5")
				(number "B3")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "PC6")
				(number "A4")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "PC7")
				(number "A5")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "PD0")
				(number "B5")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "PD1")
				(number "A7")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "A23")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "VCC")
				(number "A6")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "B8")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "A8")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B20")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "EP")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 3.81)
				(name "AVCC")
				(number "B27")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "AGND")
				(number "B26")
			)
			(pin output line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "COM0")
				(number "B23")
			)
			(pin output line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "COM1")
				(number "A27")
			)
			(pin output line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "COM2")
				(number "B24")
			)
			(pin output line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "COM3")
				(number "A28")
			)
			(pin output line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "SEG0")
				(number "A22")
			)
			(pin output line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "SEG1")
				(number "B19")
			)
			(pin output line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "SEG2")
				(number "A21")
			)
			(pin output line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "SEG3")
				(number "B18")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "SEG4")
				(number "A20")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "SEG5")
				(number "B17")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "SEG6")
				(number "A19")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "SEG7")
				(number "A18")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "SEG8")
				(number "B16")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "PM7/SEG9")
				(number "B15")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "PM6/SEG10")
				(number "A17")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "PM5/SEG11")
				(number "B14")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "PM4/SEG12")
				(number "A16")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "PM3/SEG13")
				(number "A15")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PM2/SEG14")
				(number "B13")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "PM1/SEG15")
				(number "A14")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PM0/SEG16")
				(number "B12")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PG7/SEG17")
				(number "A13")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PG6/SEG18")
				(number "B11")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PG5/SEG19")
				(number "A12")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "PG4/SEG20")
				(number "B10")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "PG3/SEG21")
				(number "A11")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "PG2/SEG22")
				(number "A10")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "PG1/SEG23")
				(number "B9")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "PG0/SEG24")
				(number "A9")
			)
			(pin power_out line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "VLCD")
				(number "B22")
			)
			(pin power_out line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "BIAS1")
				(number "B21")
			)
			(pin power_out line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "BIAS2")
				(number "A24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega16A4U-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega16A4U-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8387-8-and16-bit-AVR-Microcontroller-XMEGA-A4U_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 16kB Flash, 4kB Boot, 2kB SRAM, 1kB EEPROM, JTAG, USB, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega16A4U-A_0_1")
		(symbol "ATxmega16A4U-A_1_1"
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PE2")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "27")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "19")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "31")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA1")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA2")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA3")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA4")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega16A4U-C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega16A4U-C"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8387-8-and16-bit-AVR-Microcontroller-XMEGA-A4U_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 16kB Flash, 4kB Boot, 2kB SRAM, 1kB EEPROM, JTAG, USB, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega16A4U-C_0_1")
		(symbol "ATxmega16A4U-C_1_1"
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "B5")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "A6")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "A5")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "A4")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "D7")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "C6")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PE2")
				(number "B6")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "A7")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "F5")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "F6")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "G7")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "F7")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "E5")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "E6")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "E7")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "D6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "B7")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "F1")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "G6")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "A3")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C5")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C7")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D5")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E1")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E2")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E4")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "A2")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "B3")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA1")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA2")
				(number "C2")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA3")
				(number "A1")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA4")
				(number "B1")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "C1")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "C3")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "C4")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "D4")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB1")
				(number "D1")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB2")
				(number "D2")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB3")
				(number "D3")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "F2")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "G1")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "G2")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "E3")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "F3")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "G3")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "F4")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "G4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega16A4U-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega16A4U-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8387-8-and16-bit-AVR-Microcontroller-XMEGA-A4U_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 16kB Flash, 4kB Boot, 2kB SRAM, 1kB EEPROM, JTAG, USB, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega16A4U-M_0_1")
		(symbol "ATxmega16A4U-M_1_1"
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PE2")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "27")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "19")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "31")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA1")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA2")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA3")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA4")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega16C4-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega16C4-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8493-8-and-32-bit-AVR-XMEGA-Microcontrollers-ATxmega16C4-ATxmega32C4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 16kB Flash, 4kB Boot, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega16C4-A_0_1")
		(symbol "ATxmega16C4-A_1_1"
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PR0/XTAL1")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PR1/XTAL2")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PE2")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "27")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "19")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "31")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA1")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA2")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA3")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA4")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega16C4-C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega16C4-C"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8493-8-and-32-bit-AVR-XMEGA-Microcontrollers-ATxmega16C4-ATxmega32C4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 16kB Flash, 4kB Boot, 2kB SRAM, 1kB EEPROM, JTAG, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega16C4-C_0_1")
		(symbol "ATxmega16C4-C_1_1"
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "B5")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "A6")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PR0/XTAL1")
				(number "A5")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PR1/XTAL2")
				(number "A4")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "D7")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "C6")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PE2")
				(number "B6")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "A7")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "F5")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "F6")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "G7")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "F7")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "E5")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "E6")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "E7")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "D6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "B7")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "F1")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "G6")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "A3")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C5")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C7")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D5")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E1")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E2")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E4")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "A2")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "B3")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA1")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA2")
				(number "C2")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA3")
				(number "A1")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA4")
				(number "B1")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "C1")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "C3")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "C4")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "D4")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB1")
				(number "D1")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB2")
				(number "D2")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB3")
				(number "D3")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "F2")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "G1")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "G2")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "E3")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "F3")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "G3")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "F4")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "G4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega16C4-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega16C4-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8493-8-and-32-bit-AVR-XMEGA-Microcontrollers-ATxmega16C4-ATxmega32C4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 16kB Flash, 4kB Boot, 2kB SRAM, 1kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega16C4-M_0_1")
		(symbol "ATxmega16C4-M_1_1"
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PR0/XTAL1")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PR1/XTAL2")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PE2")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "27")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "19")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "31")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA1")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA2")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA3")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA4")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega16D4-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega16D4-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8135-8-and-16-bit-AVR-microcontroller-ATxmega16D4-32D4-64D4-128D4_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 16kB Flash, 4kB Boot, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega16D4-A_0_1")
		(symbol "ATxmega16D4-A_1_1"
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PE2")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "27")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "19")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "31")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA1")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA2")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA3")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA4")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "AREF/PB0")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega16D4-C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega16D4-C"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8135-8-and-16-bit-AVR-microcontroller-ATxmega16D4-32D4-64D4-128D4_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 16kB Flash, 4kB Boot, 2kB SRAM, 1kB EEPROM, JTAG, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega16D4-C_0_1")
		(symbol "ATxmega16D4-C_1_1"
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "B5")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "A6")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "A5")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "A4")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "D7")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "C6")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PE2")
				(number "B6")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "A7")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "F5")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "F6")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "G7")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "F7")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "E5")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "E6")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "E7")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "D6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "B7")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "F1")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "G6")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "A3")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "B4")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C5")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C7")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D5")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E1")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E2")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "E4")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "G5")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "A2")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "B3")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA1")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA2")
				(number "C2")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA3")
				(number "A1")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA4")
				(number "B1")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "C1")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "C3")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "C4")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "AREF/PB0")
				(number "D4")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB1")
				(number "D1")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB2")
				(number "D2")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB3")
				(number "D3")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "F2")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "G1")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "G2")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "E3")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "F3")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "G3")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "F4")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "G4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega16D4-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega16D4-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8135-8-and-16-bit-AVR-microcontroller-ATxmega16D4-32D4-64D4-128D4_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 16kB Flash, 4kB Boot, 2kB SRAM, 1kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega16D4-M_0_1")
		(symbol "ATxmega16D4-M_1_1"
			(pin input line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PE2")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PD7")
				(number "27")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "19")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "31")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA1")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA2")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA3")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA4")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA5")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA6")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA7")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "AREF/PB0")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega256A3B-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 49.53 0)
		)
		(property "Value" "ATxmega256A3B-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8116-8-and-16-bit-AVR-XMEGA-A3B-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 256kB Flash, 8kB Boot, 16kB SRAM, 4kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega256A3B-A_0_1")
		(symbol "ATxmega256A3B-A_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "56")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "TOSC1")
				(number "43")
			)
			(pin passive line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "TOSC2")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "50")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PF6")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PF7")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "VBAT")
				(number "51")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "35")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "45")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "AREF/PB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega256A3B-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 49.53 0)
		)
		(property "Value" "ATxmega256A3B-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8116-8-and-16-bit-AVR-XMEGA-A3B-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 256kB Flash, 8kB Boot, 16kB SRAM, 4kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega256A3B-M_0_1")
		(symbol "ATxmega256A3B-M_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "56")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "TOSC1")
				(number "43")
			)
			(pin passive line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "TOSC2")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "50")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PF6")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PF7")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "VBAT")
				(number "51")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "35")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "45")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "AREF/PB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega256A3BU-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 49.53 0)
		)
		(property "Value" "ATxmega256A3BU-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8362-8-and-16bit-AVR-microcontroller-ATxmega256A3BU_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 256kB Flash, 8kB Boot, 16kB SRAM, 4kB EEPROM, JTAG, USB, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega256A3BU-A_0_1")
		(symbol "ATxmega256A3BU-A_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "56")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "TOSC1")
				(number "43")
			)
			(pin passive line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "TOSC2")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "50")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PF6")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PF7")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "VBAT")
				(number "51")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "35")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "45")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "AREF/PB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega256A3BU-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 49.53 0)
		)
		(property "Value" "ATxmega256A3BU-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8362-8-and-16bit-AVR-microcontroller-ATxmega256A3BU_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 256kB Flash, 8kB Boot, 16kB SRAM, 4kB EEPROM, JTAG, USB, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega256A3BU-M_0_1")
		(symbol "ATxmega256A3BU-M_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "56")
			)
			(pin input line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "TOSC1")
				(number "43")
			)
			(pin passive line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "TOSC2")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "50")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PF6")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PF7")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "VBAT")
				(number "51")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "35")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "45")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "AREF/PB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega32C3-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega32C3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8492-8-and-16-bit-AVR-microcontroller-ATxmega32C3_64C3_128C3_192C3_256C3_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, JTAG, USB, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega32C3-A_0_1")
		(symbol "ATxmega32C3-A_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "56")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "50")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PF6")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PF7")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PE6")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PE7")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PD7")
				(number "33")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "35")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "45")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega32C3-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega32C3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8492-8-and-16-bit-AVR-microcontroller-ATxmega32C3_64C3_128C3_192C3_256C3_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, JTAG, USB, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega32C3-M_0_1")
		(symbol "ATxmega32C3-M_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "56")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "50")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PF6")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PF7")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PE6")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PE7")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PD7")
				(number "33")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "35")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "45")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega32D3-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega32D3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8134-8-16-bit-Atmel-XMEGA-D3-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega32D3-A_0_1")
		(symbol "ATxmega32D3-A_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "56")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "50")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PF6")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PF7")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PE6")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PE7")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PD7")
				(number "33")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "35")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "45")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega32D3-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega32D3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8134-8-16-bit-Atmel-XMEGA-D3-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega32D3-M_0_1")
		(symbol "ATxmega32D3-M_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "56")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "50")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PF6")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PF7")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PE6")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PE7")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PD7")
				(number "33")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "35")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "45")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64A1-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega64A1-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8067-8-and-16-bit-AVR-Microcontrollers-ATxmega64A1-ATxmega128A1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64A1-A_0_1")
		(symbol "ATxmega64A1-A_1_1"
			(pin input line
				(at -20.32 58.42 0)
				(length 3.81)
				(name "~{RESET}/PDI_CLK")
				(number "90")
			)
			(pin bidirectional line
				(at -20.32 55.88 0)
				(length 3.81)
				(name "PDI_DATA")
				(number "89")
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 3.81)
				(name "PR0/XTAL2")
				(number "91")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 3.81)
				(name "PR1/XTAL1")
				(number "92")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 3.81)
				(name "PQ0")
				(number "85")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "PQ1")
				(number "86")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "PQ2")
				(number "87")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "PQ3")
				(number "88")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "PK0")
				(number "75")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "PK1")
				(number "76")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "PK2")
				(number "77")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "PK3")
				(number "78")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "PK4")
				(number "79")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "PK5")
				(number "80")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "PK6")
				(number "81")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "PK7")
				(number "82")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PJ0")
				(number "65")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PJ1")
				(number "66")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PJ2")
				(number "67")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "PJ3")
				(number "68")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "PJ4")
				(number "69")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "PJ5")
				(number "70")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "PJ6")
				(number "71")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "PJ7")
				(number "72")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "PH0")
				(number "55")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PH1")
				(number "56")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PH2")
				(number "57")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "PH3")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PH4")
				(number "59")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "PH5")
				(number "60")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "PH6")
				(number "61")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "PH7")
				(number "62")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "PF0")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "PF1")
				(number "46")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "PF2")
				(number "47")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "PF3")
				(number "48")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "PF4")
				(number "49")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "PF5")
				(number "50")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "PF6")
				(number "51")
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "PF7")
				(number "52")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 3.81)
				(name "VCC")
				(number "14")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "24")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "34")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "44")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "54")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "64")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "74")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "83")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "84")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "93")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 3.81)
				(name "AVCC")
				(number "4")
			)
			(pin passive line
				(at 2.54 66.04 270)
				(length 3.81)
				(hide yes)
				(name "AVCC")
				(number "94")
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "AREF/PA0")
				(number "95")
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 3.81)
				(name "PA1")
				(number "96")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "PA2")
				(number "97")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "PA3")
				(number "98")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "PA4")
				(number "99")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "PA5")
				(number "100")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "PA6")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "PA7")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "AREF/PB0")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "PB1")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "PB2")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "PB3")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "PB4")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "PB5")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "PB6")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "PB7")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "PC0")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "PC1")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "PC2")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "PC3")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "PC4")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "PC5")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "PC6")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "PC7")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "PD7")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "PE0")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "PE1")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "PE2")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "PE3")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "PE4")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "PE5")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "PE6")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "PE7")
				(number "42")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64A1-C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega64A1-C"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_9.0x9.0mm_Layout10x10_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8067-8-and-16-bit-AVR-Microcontrollers-ATxmega64A1-ATxmega128A1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, TFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*9.0x9.0mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64A1-C_0_1")
		(symbol "ATxmega64A1-C_1_1"
			(pin input line
				(at -20.32 58.42 0)
				(length 3.81)
				(name "~{RESET}/PDI_CLK")
				(number "F3")
			)
			(pin bidirectional line
				(at -20.32 55.88 0)
				(length 3.81)
				(name "PDI_DATA")
				(number "F4")
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 3.81)
				(name "PR0/XTAL2")
				(number "F2")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 3.81)
				(name "PR1/XTAL1")
				(number "F1")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 3.81)
				(name "PQ0")
				(number "E1")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "PQ1")
				(number "E2")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "PQ2")
				(number "E3")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "PQ3")
				(number "F5")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "PK0")
				(number "A1")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "PK1")
				(number "B3")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "PK2")
				(number "B2")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "PK3")
				(number "B1")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "PK4")
				(number "C3")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "PK5")
				(number "C2")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "PK6")
				(number "D2")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "PK7")
				(number "D3")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PJ0")
				(number "C5")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PJ1")
				(number "D5")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PJ2")
				(number "E5")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "PJ3")
				(number "A4")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "PJ4")
				(number "B4")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "PJ5")
				(number "C4")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "PJ6")
				(number "D4")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "PJ7")
				(number "E4")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "PH0")
				(number "B8")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PH1")
				(number "A7")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PH2")
				(number "B7")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "PH3")
				(number "C7")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PH4")
				(number "B6")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "PH5")
				(number "C6")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "PH6")
				(number "D6")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "PH7")
				(number "B5")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "PF0")
				(number "D7")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "PF1")
				(number "D8")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "PF2")
				(number "C8")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "PF3")
				(number "C9")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "PF4")
				(number "D9")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "PF5")
				(number "B10")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "PF6")
				(number "B9")
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "PF7")
				(number "A10")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 3.81)
				(name "VCC")
				(number "A2")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "A5")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "A9")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "C1")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "C10")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "F10")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "K6")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "K8")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 3.81)
				(name "GND")
				(number "A3")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A6")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A8")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D1")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D10")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G1")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G10")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K3")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K7")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 3.81)
				(name "AVCC")
				(number "H1")
			)
			(pin passive line
				(at 2.54 66.04 270)
				(length 3.81)
				(hide yes)
				(name "AVCC")
				(number "K4")
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "AREF/PA0")
				(number "J1")
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 3.81)
				(name "PA1")
				(number "G2")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "PA2")
				(number "H2")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "PA3")
				(number "J2")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "PA4")
				(number "G3")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "PA5")
				(number "H3")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "PA6")
				(number "K1")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "PA7")
				(number "K2")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "AREF/PB0")
				(number "J3")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "PB1")
				(number "J4")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "PB2")
				(number "H4")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "PB3")
				(number "G4")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "PB4")
				(number "G5")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "PB5")
				(number "H5")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "PB6")
				(number "J5")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "PB7")
				(number "K5")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "PC0")
				(number "H6")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "PC1")
				(number "G6")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "PC2")
				(number "F6")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "PC3")
				(number "J6")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "PC4")
				(number "J7")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "PC5")
				(number "H7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "PC6")
				(number "G7")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "PC7")
				(number "J8")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "PD0")
				(number "K10")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PD1")
				(number "J10")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PD2")
				(number "J9")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PD3")
				(number "H10")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PD4")
				(number "H9")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "PD5")
				(number "H8")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "PD6")
				(number "G9")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "PD7")
				(number "G8")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "PE0")
				(number "F9")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "PE1")
				(number "F8")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "PE2")
				(number "F7")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "PE3")
				(number "E10")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "PE4")
				(number "E9")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "PE5")
				(number "E8")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "PE6")
				(number "E7")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "PE7")
				(number "E6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64A1-C7"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega64A1-C7"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-100_7.0x7.0mm_Layout10x10_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8067-8-and-16-bit-AVR-Microcontrollers-ATxmega64A1-ATxmega128A1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, VFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*7.0x7.0mm*Layout10x10*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64A1-C7_0_1")
		(symbol "ATxmega64A1-C7_1_1"
			(pin input line
				(at -20.32 58.42 0)
				(length 3.81)
				(name "~{RESET}/PDI_CLK")
				(number "F3")
			)
			(pin bidirectional line
				(at -20.32 55.88 0)
				(length 3.81)
				(name "PDI_DATA")
				(number "F4")
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 3.81)
				(name "PR0/XTAL2")
				(number "F2")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 3.81)
				(name "PR1/XTAL1")
				(number "F1")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 3.81)
				(name "PQ0")
				(number "E1")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "PQ1")
				(number "E2")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "PQ2")
				(number "E3")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "PQ3")
				(number "F5")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "PK0")
				(number "A1")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "PK1")
				(number "B3")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "PK2")
				(number "B2")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "PK3")
				(number "B1")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "PK4")
				(number "C3")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "PK5")
				(number "C2")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "PK6")
				(number "D2")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "PK7")
				(number "D3")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PJ0")
				(number "C5")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PJ1")
				(number "D5")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PJ2")
				(number "E5")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "PJ3")
				(number "A4")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "PJ4")
				(number "B4")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "PJ5")
				(number "C4")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "PJ6")
				(number "D4")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "PJ7")
				(number "E4")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "PH0")
				(number "B8")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PH1")
				(number "A7")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PH2")
				(number "B7")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "PH3")
				(number "C7")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PH4")
				(number "B6")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "PH5")
				(number "C6")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "PH6")
				(number "D6")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "PH7")
				(number "B5")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "PF0")
				(number "D7")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "PF1")
				(number "D8")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "PF2")
				(number "C8")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "PF3")
				(number "C9")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "PF4")
				(number "D9")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "PF5")
				(number "B10")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "PF6")
				(number "B9")
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "PF7")
				(number "A10")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 3.81)
				(name "VCC")
				(number "A2")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "A5")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "A9")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "C1")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "C10")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "F10")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "K6")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "K8")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 3.81)
				(name "GND")
				(number "A3")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A6")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A8")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D1")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D10")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G1")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G10")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K3")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K7")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 3.81)
				(name "AVCC")
				(number "H1")
			)
			(pin passive line
				(at 2.54 66.04 270)
				(length 3.81)
				(hide yes)
				(name "AVCC")
				(number "K4")
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "AREF/PA0")
				(number "J1")
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 3.81)
				(name "PA1")
				(number "G2")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "PA2")
				(number "H2")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "PA3")
				(number "J2")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "PA4")
				(number "G3")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "PA5")
				(number "H3")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "PA6")
				(number "K1")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "PA7")
				(number "K2")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "AREF/PB0")
				(number "J3")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "PB1")
				(number "J4")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "PB2")
				(number "H4")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "PB3")
				(number "G4")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "PB4")
				(number "G5")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "PB5")
				(number "H5")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "PB6")
				(number "J5")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "PB7")
				(number "K5")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "PC0")
				(number "H6")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "PC1")
				(number "G6")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "PC2")
				(number "F6")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "PC3")
				(number "J6")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "PC4")
				(number "J7")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "PC5")
				(number "H7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "PC6")
				(number "G7")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "PC7")
				(number "J8")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "PD0")
				(number "K10")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PD1")
				(number "J10")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PD2")
				(number "J9")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PD3")
				(number "H10")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PD4")
				(number "H9")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "PD5")
				(number "H8")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "PD6")
				(number "G9")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "PD7")
				(number "G8")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "PE0")
				(number "F9")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "PE1")
				(number "F8")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "PE2")
				(number "F7")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "PE3")
				(number "E10")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "PE4")
				(number "E9")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "PE5")
				(number "E8")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "PE6")
				(number "E7")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "PE7")
				(number "E6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64A1U-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega64A1U-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8385-8-and-16-bit-AVR-Microcontroller-ATxmega64A1U-ATxmega128A1U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64A1U-A_0_1")
		(symbol "ATxmega64A1U-A_1_1"
			(pin input line
				(at -20.32 58.42 0)
				(length 3.81)
				(name "~{RESET}/PDI_CLK")
				(number "90")
			)
			(pin bidirectional line
				(at -20.32 55.88 0)
				(length 3.81)
				(name "PDI_DATA")
				(number "89")
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 3.81)
				(name "PR0/XTAL2")
				(number "91")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 3.81)
				(name "PR1/XTAL1")
				(number "92")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 3.81)
				(name "PQ0")
				(number "85")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "PQ1")
				(number "86")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "PQ2")
				(number "87")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "PQ3")
				(number "88")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "PK0")
				(number "75")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "PK1")
				(number "76")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "PK2")
				(number "77")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "PK3")
				(number "78")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "PK4")
				(number "79")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "PK5")
				(number "80")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "PK6")
				(number "81")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "PK7")
				(number "82")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PJ0")
				(number "65")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PJ1")
				(number "66")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PJ2")
				(number "67")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "PJ3")
				(number "68")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "PJ4")
				(number "69")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "PJ5")
				(number "70")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "PJ6")
				(number "71")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "PJ7")
				(number "72")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "PH0")
				(number "55")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PH1")
				(number "56")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PH2")
				(number "57")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "PH3")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PH4")
				(number "59")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "PH5")
				(number "60")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "PH6")
				(number "61")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "PH7")
				(number "62")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "PF0")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "PF1")
				(number "46")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "PF2")
				(number "47")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "PF3")
				(number "48")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "PF4")
				(number "49")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "PF5")
				(number "50")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "PF6")
				(number "51")
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "PF7")
				(number "52")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 3.81)
				(name "VCC")
				(number "14")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "24")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "34")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "44")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "54")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "64")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "74")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "83")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 3.81)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "84")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "93")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 3.81)
				(name "AVCC")
				(number "4")
			)
			(pin passive line
				(at 2.54 66.04 270)
				(length 3.81)
				(hide yes)
				(name "AVCC")
				(number "94")
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "AREF/PA0")
				(number "95")
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 3.81)
				(name "PA1")
				(number "96")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "PA2")
				(number "97")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "PA3")
				(number "98")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "PA4")
				(number "99")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "PA5")
				(number "100")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "PA6")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "PA7")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "AREF/PB0")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "PB1")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "PB2")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "PB3")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "PB4")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "PB5")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "PB6")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "PB7")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "PC0")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "PC1")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "PC2")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "PC3")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "PC4")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "PC5")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "PC6")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "PC7")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "PD7")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "PE0")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "PE1")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "PE2")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "PE3")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "PE4")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "PE5")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "PE6")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "PE7")
				(number "42")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64A1U-C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega64A1U-C"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_9.0x9.0mm_Layout10x10_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8385-8-and-16-bit-AVR-Microcontroller-ATxmega64A1U-ATxmega128A1U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, TFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*9.0x9.0mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64A1U-C_0_1")
		(symbol "ATxmega64A1U-C_1_1"
			(pin input line
				(at -20.32 58.42 0)
				(length 3.81)
				(name "~{RESET}/PDI_CLK")
				(number "F3")
			)
			(pin bidirectional line
				(at -20.32 55.88 0)
				(length 3.81)
				(name "PDI_DATA")
				(number "F4")
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 3.81)
				(name "PR0/XTAL2")
				(number "F2")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 3.81)
				(name "PR1/XTAL1")
				(number "F1")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 3.81)
				(name "PQ0")
				(number "E1")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "PQ1")
				(number "E2")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "PQ2")
				(number "E3")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "PQ3")
				(number "F5")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "PK0")
				(number "A1")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "PK1")
				(number "B3")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "PK2")
				(number "B2")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "PK3")
				(number "B1")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "PK4")
				(number "C3")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "PK5")
				(number "C2")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "PK6")
				(number "D2")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "PK7")
				(number "D3")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PJ0")
				(number "C5")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PJ1")
				(number "D5")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PJ2")
				(number "E5")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "PJ3")
				(number "A4")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "PJ4")
				(number "B4")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "PJ5")
				(number "C4")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "PJ6")
				(number "D4")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "PJ7")
				(number "E4")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "PH0")
				(number "B8")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PH1")
				(number "A7")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PH2")
				(number "B7")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "PH3")
				(number "C7")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PH4")
				(number "B6")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "PH5")
				(number "C6")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "PH6")
				(number "D6")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "PH7")
				(number "B5")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "PF0")
				(number "D7")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "PF1")
				(number "D8")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "PF2")
				(number "C8")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "PF3")
				(number "C9")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "PF4")
				(number "D9")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "PF5")
				(number "B10")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "PF6")
				(number "B9")
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "PF7")
				(number "A10")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 3.81)
				(name "VCC")
				(number "A2")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "A5")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "A9")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "C1")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "C10")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "F10")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "K6")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "K8")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 3.81)
				(name "GND")
				(number "A3")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A6")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A8")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D1")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D10")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G1")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G10")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K3")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K7")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 3.81)
				(name "AVCC")
				(number "H1")
			)
			(pin passive line
				(at 2.54 66.04 270)
				(length 3.81)
				(hide yes)
				(name "AVCC")
				(number "K4")
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "AREF/PA0")
				(number "J1")
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 3.81)
				(name "PA1")
				(number "G2")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "PA2")
				(number "H2")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "PA3")
				(number "J2")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "PA4")
				(number "G3")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "PA5")
				(number "H3")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "PA6")
				(number "K1")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "PA7")
				(number "K2")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "AREF/PB0")
				(number "J3")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "PB1")
				(number "J4")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "PB2")
				(number "H4")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "PB3")
				(number "G4")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "PB4")
				(number "G5")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "PB5")
				(number "H5")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "PB6")
				(number "J5")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "PB7")
				(number "K5")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "PC0")
				(number "H6")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "PC1")
				(number "G6")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "PC2")
				(number "F6")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "PC3")
				(number "J6")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "PC4")
				(number "J7")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "PC5")
				(number "H7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "PC6")
				(number "G7")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "PC7")
				(number "J8")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "PD0")
				(number "K10")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PD1")
				(number "J10")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PD2")
				(number "J9")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PD3")
				(number "H10")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PD4")
				(number "H9")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "PD5")
				(number "H8")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "PD6")
				(number "G9")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "PD7")
				(number "G8")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "PE0")
				(number "F9")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "PE1")
				(number "F8")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "PE2")
				(number "F7")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "PE3")
				(number "E10")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "PE4")
				(number "E9")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "PE5")
				(number "E8")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "PE6")
				(number "E7")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "PE7")
				(number "E6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64A1U-C7"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega64A1U-C7"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-100_7.0x7.0mm_Layout10x10_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8385-8-and-16-bit-AVR-Microcontroller-ATxmega64A1U-ATxmega128A1U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, VFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*7.0x7.0mm*Layout10x10*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64A1U-C7_0_1")
		(symbol "ATxmega64A1U-C7_1_1"
			(pin input line
				(at -20.32 58.42 0)
				(length 3.81)
				(name "~{RESET}/PDI_CLK")
				(number "F3")
			)
			(pin bidirectional line
				(at -20.32 55.88 0)
				(length 3.81)
				(name "PDI_DATA")
				(number "F4")
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 3.81)
				(name "PR0/XTAL2")
				(number "F2")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 3.81)
				(name "PR1/XTAL1")
				(number "F1")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 3.81)
				(name "PQ0")
				(number "E1")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "PQ1")
				(number "E2")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "PQ2")
				(number "E3")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "PQ3")
				(number "F5")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "PK0")
				(number "A1")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "PK1")
				(number "B3")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "PK2")
				(number "B2")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "PK3")
				(number "B1")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "PK4")
				(number "C3")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "PK5")
				(number "C2")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "PK6")
				(number "D2")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "PK7")
				(number "D3")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PJ0")
				(number "C5")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PJ1")
				(number "D5")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PJ2")
				(number "E5")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "PJ3")
				(number "A4")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "PJ4")
				(number "B4")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "PJ5")
				(number "C4")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "PJ6")
				(number "D4")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "PJ7")
				(number "E4")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "PH0")
				(number "B8")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PH1")
				(number "A7")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PH2")
				(number "B7")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "PH3")
				(number "C7")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PH4")
				(number "B6")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "PH5")
				(number "C6")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "PH6")
				(number "D6")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "PH7")
				(number "B5")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "PF0")
				(number "D7")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "PF1")
				(number "D8")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "PF2")
				(number "C8")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "PF3")
				(number "C9")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "PF4")
				(number "D9")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "PF5")
				(number "B10")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "PF6")
				(number "B9")
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "PF7")
				(number "A10")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 3.81)
				(name "VCC")
				(number "A2")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "A5")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "A9")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "C1")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "C10")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "F10")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "K6")
			)
			(pin passive line
				(at 0 66.04 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "K8")
			)
			(pin power_in line
				(at 0 -66.04 90)
				(length 3.81)
				(name "GND")
				(number "A3")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A6")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "A8")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D1")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D10")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G1")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "G10")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K3")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K7")
			)
			(pin passive line
				(at 0 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 3.81)
				(name "AVCC")
				(number "H1")
			)
			(pin passive line
				(at 2.54 66.04 270)
				(length 3.81)
				(hide yes)
				(name "AVCC")
				(number "K4")
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "AREF/PA0")
				(number "J1")
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 3.81)
				(name "PA1")
				(number "G2")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "PA2")
				(number "H2")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "PA3")
				(number "J2")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "PA4")
				(number "G3")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "PA5")
				(number "H3")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "PA6")
				(number "K1")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "PA7")
				(number "K2")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "AREF/PB0")
				(number "J3")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "PB1")
				(number "J4")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "PB2")
				(number "H4")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "PB3")
				(number "G4")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "PB4")
				(number "G5")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "PB5")
				(number "H5")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "PB6")
				(number "J5")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "PB7")
				(number "K5")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "PC0")
				(number "H6")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "PC1")
				(number "G6")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "PC2")
				(number "F6")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "PC3")
				(number "J6")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "PC4")
				(number "J7")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "PC5")
				(number "H7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "PC6")
				(number "G7")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "PC7")
				(number "J8")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "PD0")
				(number "K10")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PD1")
				(number "J10")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PD2")
				(number "J9")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PD3")
				(number "H10")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PD4")
				(number "H9")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "PD5")
				(number "H8")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "PD6")
				(number "G9")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "PD7")
				(number "G8")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "PE0")
				(number "F9")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "PE1")
				(number "F8")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "PE2")
				(number "F7")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "PE3")
				(number "E10")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "PE4")
				(number "E9")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "PE5")
				(number "E8")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "PE6")
				(number "E7")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "PE7")
				(number "E6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64A3-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega64A3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8068-8-and16-bit-AVR-XMEGA-A3-Microcontrollers_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64A3-A_0_1")
		(symbol "ATxmega64A3-A_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "56")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "50")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PF6")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PF7")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PE6")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PE7")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PD7")
				(number "33")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "35")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "45")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64A3-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega64A3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8068-8-and16-bit-AVR-XMEGA-A3-Microcontrollers_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64A3-M_0_1")
		(symbol "ATxmega64A3-M_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "56")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "50")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PF6")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PF7")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PE6")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PE7")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PD7")
				(number "33")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "35")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "45")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64A3U-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega64A3U-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8386-8-and-16-bit-AVR-Microcontroller-ATxmega64A3U-128A3U-192A3U-256A3U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64A3U-A_0_1")
		(symbol "ATxmega64A3U-A_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "56")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "50")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PF6")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PF7")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PE6")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PE7")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PD7")
				(number "33")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "35")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "45")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64A3U-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega64A3U-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8386-8-and-16-bit-AVR-Microcontroller-ATxmega64A3U-128A3U-192A3U-256A3U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64A3U-M_0_1")
		(symbol "ATxmega64A3U-M_1_1"
			(pin input line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "56")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PF0")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PF1")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "50")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PF6")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PF7")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PE6")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PE7")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PD7")
				(number "33")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "25")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "35")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "45")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "53")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "52")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "AREFA/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "AREFB/PB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC4")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC5")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PC6")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PC7")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64B1-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega64B1-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8330-8-and-16-bit-AVR-Microcontroller-XMEGA-B-ATxmega64B1-ATxmega128B1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, LCD, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64B1-A_0_1")
		(symbol "ATxmega64B1-A_1_1"
			(pin input line
				(at -20.32 66.04 0)
				(length 3.81)
				(name "~{RESET}/PDI_CLK")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 63.5 0)
				(length 3.81)
				(name "PDI_DATA")
				(number "16")
			)
			(pin passive line
				(at -20.32 48.26 0)
				(length 3.81)
				(name "CAPH")
				(number "75")
			)
			(pin passive line
				(at -20.32 45.72 0)
				(length 3.81)
				(name "CAPL")
				(number "74")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "PR0/XTAL2")
				(number "80")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "PR1/XTAL1")
				(number "81")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 3.81)
				(name "PA0/AREF")
				(number "82")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "PA1")
				(number "83")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "PA2")
				(number "84")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "PA3")
				(number "85")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "PA4")
				(number "86")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "PA5")
				(number "87")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "PA6")
				(number "88")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "PA7")
				(number "89")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "PB0")
				(number "92")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PB1")
				(number "93")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PB2")
				(number "94")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PB3")
				(number "95")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "PB4")
				(number "96")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "PB5")
				(number "97")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "PB6")
				(number "98")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "PB7")
				(number "99")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "PC0")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "PC1")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PC2")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PC3")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "PC4")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PC5")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "PC6")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "PC7")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 3.81)
				(name "PD0")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "PD1")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "PD2")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "PE0")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "PE1")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "PE2")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "PE3")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "PE4")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 -58.42 0)
				(length 3.81)
				(name "PE5")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 -60.96 0)
				(length 3.81)
				(name "PE6")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 -63.5 0)
				(length 3.81)
				(name "PE7")
				(number "26")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "11")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "18")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "28")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "70")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "100")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "69")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 3.81)
				(name "AVCC")
				(number "91")
			)
			(pin power_in line
				(at 2.54 -73.66 90)
				(length 3.81)
				(name "AGND")
				(number "90")
			)
			(pin output line
				(at 20.32 66.04 180)
				(length 3.81)
				(name "COM0")
				(number "76")
			)
			(pin output line
				(at 20.32 63.5 180)
				(length 3.81)
				(name "COM1")
				(number "77")
			)
			(pin output line
				(at 20.32 60.96 180)
				(length 3.81)
				(name "COM2")
				(number "78")
			)
			(pin output line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "COM3")
				(number "79")
			)
			(pin output line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "SEG0")
				(number "68")
			)
			(pin output line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "SEG1")
				(number "67")
			)
			(pin output line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "SEG2")
				(number "66")
			)
			(pin output line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "SEG3")
				(number "65")
			)
			(pin output line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "SEG4")
				(number "64")
			)
			(pin output line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "SEG5")
				(number "63")
			)
			(pin output line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "SEG6")
				(number "62")
			)
			(pin output line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "SEG7")
				(number "61")
			)
			(pin output line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "SEG8")
				(number "60")
			)
			(pin output line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "SEG9")
				(number "59")
			)
			(pin output line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "SEG10")
				(number "58")
			)
			(pin output line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "SEG11")
				(number "57")
			)
			(pin output line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "SEG12")
				(number "56")
			)
			(pin output line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "SEG13")
				(number "55")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "SEG14")
				(number "54")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "SEG15")
				(number "53")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "SEG16")
				(number "52")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "SEG17")
				(number "51")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "SEG18")
				(number "50")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "SEG19")
				(number "49")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "SEG20")
				(number "48")
			)
			(pin output line
				(at 20.32 0 180)
				(length 3.81)
				(name "SEG21")
				(number "47")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "SEG22")
				(number "46")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "SEG23")
				(number "45")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PM7/SEG24")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "PM6/SEG25")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PM5/SEG26")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PM4/SEG27")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PM3/SEG28")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PM2/SEG29")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "PM1/SEG30")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "PM0/SEG31")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "PG7/SEG32")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "PG6/SEG33")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "PG5/SEG34")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "PG4/SEG35")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "PG3/SEG36")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "PG2/SEG37")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "PG1/SEG38")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "PG0/SEG39")
				(number "29")
			)
			(pin power_out line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "VLCD")
				(number "73")
			)
			(pin power_out line
				(at 20.32 -53.34 180)
				(length 3.81)
				(name "BIAS1")
				(number "71")
			)
			(pin power_out line
				(at 20.32 -55.88 180)
				(length 3.81)
				(name "BIAS2")
				(number "72")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64B1-C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega64B1-C"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-100_7.0x7.0mm_Layout10x10_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8330-8-and-16-bit-AVR-Microcontroller-XMEGA-B-ATxmega64B1-ATxmega128B1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, LCD, VFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*7.0x7.0mm*Layout10x10*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64B1-C_0_1")
		(symbol "ATxmega64B1-C_1_1"
			(pin input line
				(at -20.32 66.04 0)
				(length 3.81)
				(name "~{RESET}/PDI_CLK")
				(number "E2")
			)
			(pin bidirectional line
				(at -20.32 63.5 0)
				(length 3.81)
				(name "PDI_DATA")
				(number "F3")
			)
			(pin passive line
				(at -20.32 48.26 0)
				(length 3.81)
				(name "CAPH")
				(number "A10")
			)
			(pin passive line
				(at -20.32 45.72 0)
				(length 3.81)
				(name "CAPL")
				(number "B10")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "PR0/XTAL2")
				(number "B8")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "PR1/XTAL1")
				(number "A8")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 3.81)
				(name "PA0/AREF")
				(number "B7")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "PA1")
				(number "A7")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "PA2")
				(number "E6")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "PA3")
				(number "C6")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "PA4")
				(number "B6")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "PA5")
				(number "A6")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "PA6")
				(number "D6")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "PA7")
				(number "C5")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "PB0")
				(number "D5")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "PB1")
				(number "E5")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "PB2")
				(number "A4")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "PB3")
				(number "F5")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "PB4")
				(number "B4")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "PB5")
				(number "C4")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "PB6")
				(number "A3")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "PB7")
				(number "B3")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "PC0")
				(number "A1")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "PC1")
				(number "C3")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PC2")
				(number "D4")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PC3")
				(number "B1")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "PC4")
				(number "C2")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PC5")
				(number "C1")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "PC6")
				(number "E4")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "PC7")
				(number "F4")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 3.81)
				(name "PD0")
				(number "D3")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "PD1")
				(number "E3")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "PD2")
				(number "E1")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "PE0")
				(number "G4")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "PE1")
				(number "G2")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "PE2")
				(number "G1")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "PE3")
				(number "G3")
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "PE4")
				(number "G5")
			)
			(pin bidirectional line
				(at -20.32 -58.42 0)
				(length 3.81)
				(name "PE5")
				(number "H1")
			)
			(pin bidirectional line
				(at -20.32 -60.96 0)
				(length 3.81)
				(name "PE6")
				(number "H2")
			)
			(pin bidirectional line
				(at -20.32 -63.5 0)
				(length 3.81)
				(name "PE7")
				(number "J1")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 3.81)
				(name "VCC")
				(number "A2")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "D1")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "D10")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "F1")
			)
			(pin passive line
				(at 0 73.66 270)
				(length 3.81)
				(hide yes)
				(name "VCC")
				(number "K2")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 3.81)
				(name "GND")
				(number "B2")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D9")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "F2")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "K1")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 3.81)
				(name "AVCC")
				(number "A5")
			)
			(pin power_in line
				(at 2.54 -73.66 90)
				(length 3.81)
				(name "AGND")
				(number "B5")
			)
			(pin output line
				(at 20.32 66.04 180)
				(length 3.81)
				(name "COM0")
				(number "C8")
			)
			(pin output line
				(at 20.32 63.5 180)
				(length 3.81)
				(name "COM1")
				(number "B9")
			)
			(pin output line
				(at 20.32 60.96 180)
				(length 3.81)
				(name "COM2")
				(number "A9")
			)
			(pin output line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "COM3")
				(number "C7")
			)
			(pin output line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "SEG0")
				(number "D7")
			)
			(pin output line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "SEG1")
				(number "E7")
			)
			(pin output line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "SEG2")
				(number "E10")
			)
			(pin output line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "SEG3")
				(number "E9")
			)
			(pin output line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "SEG4")
				(number "E8")
			)
			(pin output line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "SEG5")
				(number "F10")
			)
			(pin output line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "SEG6")
				(number "F9")
			)
			(pin output line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "SEG7")
				(number "F8")
			)
			(pin output line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "SEG8")
				(number "G10")
			)
			(pin output line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "SEG9")
				(number "G9")
			)
			(pin output line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "SEG10")
				(number "F7")
			)
			(pin output line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "SEG11")
				(number "H10")
			)
			(pin output line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "SEG12")
				(number "H9")
			)
			(pin output line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "SEG13")
				(number "G8")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "SEG14")
				(number "J10")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "SEG15")
				(number "G7")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "SEG16")
				(number "J9")
			)
			(pin output line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "SEG17")
				(number "K10")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "SEG18")
				(number "H8")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "SEG19")
				(number "K9")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "SEG20")
				(number "J8")
			)
			(pin output line
				(at 20.32 0 180)
				(length 3.81)
				(name "SEG21")
				(number "H7")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "SEG22")
				(number "K8")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "SEG23")
				(number "G6")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PM7/SEG24")
				(number "J7")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "PM6/SEG25")
				(number "K7")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "PM5/SEG26")
				(number "H6")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PM4/SEG27")
				(number "J6")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PM3/SEG28")
				(number "K6")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "PM2/SEG29")
				(number "F6")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "PM1/SEG30")
				(number "J5")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "PM0/SEG31")
				(number "K5")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "PG7/SEG32")
				(number "H5")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "PG6/SEG33")
				(number "J4")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "PG5/SEG34")
				(number "K4")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "PG4/SEG35")
				(number "H4")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "PG3/SEG36")
				(number "J3")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "PG2/SEG37")
				(number "K3")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "PG1/SEG38")
				(number "H3")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "PG0/SEG39")
				(number "J2")
			)
			(pin power_out line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "VLCD")
				(number "D8")
			)
			(pin power_out line
				(at 20.32 -53.34 180)
				(length 3.81)
				(name "BIAS1")
				(number "C10")
			)
			(pin power_out line
				(at 20.32 -55.88 180)
				(length 3.81)
				(name "BIAS2")
				(number "C9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64B3-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "ATxmega64B3-A"
			(at 5.08 -46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8074-8-and-16-bit-AVR-Microcontroller-XMEGA-B-ATxmega64B3-ATxmega128B3_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, LCD, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64B3-A_0_1")
		(symbol "ATxmega64B3-A_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "14")
			)
			(pin passive line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "CAPH")
				(number "48")
			)
			(pin passive line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "CAPL")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PB0/AREF")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB3")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "61")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "62")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "63")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "64")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC0")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC1")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC2")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC3")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC4")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC5")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC6")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC7")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PD0")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PD1")
				(number "12")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "16")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "43")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "AVCC")
				(number "56")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "AGND")
				(number "55")
			)
			(pin output line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "COM0")
				(number "49")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "COM1")
				(number "50")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "COM2")
				(number "51")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "COM3")
				(number "52")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "SEG0")
				(number "41")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "SEG1")
				(number "40")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "SEG2")
				(number "39")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "SEG3")
				(number "38")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "SEG4")
				(number "37")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "SEG5")
				(number "36")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "SEG6")
				(number "35")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "SEG7")
				(number "34")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SEG8")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PM7/SEG9")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PM6/SEG10")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PM5/SEG11")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PM4/SEG12")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PM3/SEG13")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PM2/SEG14")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PM1/SEG15")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PM0/SEG16")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PG7/SEG17")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PG6/SEG18")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PG5/SEG19")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PG4/SEG20")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PG3/SEG21")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PG2/SEG22")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PG1/SEG23")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PG0/SEG24")
				(number "17")
			)
			(pin power_out line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "VLCD")
				(number "46")
			)
			(pin power_out line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "BIAS1")
				(number "44")
			)
			(pin power_out line
				(at 17.78 -43.18 180)
				(length 2.54)
				(name "BIAS2")
				(number "45")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega64B3-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "ATxmega64B3-M"
			(at 5.08 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8074-8-and-16-bit-AVR-Microcontroller-XMEGA-B-ATxmega64B3-ATxmega128B3_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, LCD, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega64B3-M_0_1")
		(symbol "ATxmega64B3-M_1_1"
			(pin input line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "14")
			)
			(pin passive line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "CAPH")
				(number "48")
			)
			(pin passive line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "CAPL")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PB0/AREF")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "59")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PB3")
				(number "60")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PB4")
				(number "61")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PB5")
				(number "62")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PB6")
				(number "63")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PB7")
				(number "64")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PC0")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PC1")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PC2")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PC3")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PC4")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PC5")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PC6")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PC7")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PD0")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PD1")
				(number "12")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "16")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "43")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "AVCC")
				(number "56")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "AGND")
				(number "55")
			)
			(pin output line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "COM0")
				(number "49")
			)
			(pin output line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "COM1")
				(number "50")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "COM2")
				(number "51")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "COM3")
				(number "52")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "SEG0")
				(number "41")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "SEG1")
				(number "40")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "SEG2")
				(number "39")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "SEG3")
				(number "38")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "SEG4")
				(number "37")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "SEG5")
				(number "36")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "SEG6")
				(number "35")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "SEG7")
				(number "34")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SEG8")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PM7/SEG9")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PM6/SEG10")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PM5/SEG11")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PM4/SEG12")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PM3/SEG13")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PM2/SEG14")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PM1/SEG15")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PM0/SEG16")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PG7/SEG17")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PG6/SEG18")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PG5/SEG19")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PG4/SEG20")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PG3/SEG21")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "PG2/SEG22")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PG1/SEG23")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PG0/SEG24")
				(number "17")
			)
			(pin power_out line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "VLCD")
				(number "46")
			)
			(pin power_out line
				(at 17.78 -40.64 180)
				(length 2.54)
				(name "BIAS1")
				(number "44")
			)
			(pin power_out line
				(at 17.78 -43.18 180)
				(length 2.54)
				(name "BIAS2")
				(number "45")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega8E5-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATxmega8E5-A"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8153-8-and-16-bit-AVR-Microcontroller-XMEGA-E-ATxmega8E5-ATxmega16E5-ATxmega32E5_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 8kB Flash, 2kB Boot, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega8E5-A_0_1")
		(symbol "ATxmega8E5-A_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PD0/AREF")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD2")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PD3")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PD5")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PD6")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PD7")
				(number "21")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "17")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega8E5-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATxmega8E5-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8153-8-and-16-bit-AVR-Microcontroller-XMEGA-E-ATxmega8E5-ATxmega16E5-ATxmega32E5_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 8kB Flash, 2kB Boot, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega8E5-M_0_1")
		(symbol "ATxmega8E5-M_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PD0/AREF")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD2")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PD3")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PD5")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PD6")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PD7")
				(number "21")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "17")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATxmega8E5-M4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATxmega8E5-M4"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_4x4mm_P0.4mm_EP2.9x2.9mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8153-8-and-16-bit-AVR-Microcontroller-XMEGA-E-ATxmega8E5-ATxmega16E5-ATxmega32E5_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 8kB Flash, 2kB Boot, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "ATxmega8E5-M4_0_1")
		(symbol "ATxmega8E5-M4_1_1"
			(pin input line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "~{RESET}/PDI_CLK")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PDI_DATA")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PR0/XTAL2")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PR1/XTAL1")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PD0/AREF")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PD2")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PD3")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PD5")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PD6")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PD7")
				(number "21")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "17")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATmega128-16A"
		(extends "ATmega64L-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega128-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2467.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 128kB Flash, 4kB SRAM, 4kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega128-16M"
		(extends "ATmega64L-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega128-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2467.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 128kB Flash, 4kB SRAM, 4kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega1280-16A"
		(extends "ATmega640V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega1280-16A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 128kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega1280-16C"
		(extends "ATmega640V-8C")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega1280-16C"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_9.0x9.0mm_Layout10x10_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at -29.21 71.12 0)
		)
		(property "Description" "16MHz, 128kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*9.0x9.0mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega1280V-8A"
		(extends "ATmega640V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega1280V-8A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 128kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega1280V-8C"
		(extends "ATmega640V-8C")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega1280V-8C"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_9.0x9.0mm_Layout10x10_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at -29.21 71.12 0)
		)
		(property "Description" "8MHz, 128kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*9.0x9.0mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega1281-16A"
		(extends "ATmega1281V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega1281-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 128kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega1281-16M"
		(extends "ATmega1281V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega1281-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 128kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega1284-A"
		(extends "ATmega164A-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega1284-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 128kB Flash, 16kB SRAM, 4kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega1284-M"
		(extends "ATmega164A-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega1284-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 128kB Flash, 16kB SRAM, 4kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega1284-P"
		(extends "ATmega164A-P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega1284-P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 128kB Flash, 16kB SRAM, 4kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega1284P-A"
		(extends "ATmega164A-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega1284P-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 128kB Flash, 16kB SRAM, 4kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega1284P-M"
		(extends "ATmega164A-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega1284P-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 128kB Flash, 16kB SRAM, 4kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega1284P-P"
		(extends "ATmega164A-P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega1284P-P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 128kB Flash, 16kB SRAM, 4kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega128A-A"
		(extends "ATmega64L-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega128A-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8151-8-bit-AVR-ATmega128A_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 128kB Flash, 4kB SRAM, 4kB EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega128A-M"
		(extends "ATmega64L-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega128A-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8151-8-bit-AVR-ATmega128A_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 128kB Flash, 4kB SRAM, 4kB EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega128L-8A"
		(extends "ATmega64L-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega128L-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2467.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 128kB Flash, 4kB SRAM, 4kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega128L-8M"
		(extends "ATmega64L-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega128L-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2467.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 128kB Flash, 4kB SRAM, 4kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega16-16A"
		(extends "ATmega16L-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega16-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2466.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega16-16M"
		(extends "ATmega16L-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega16-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2466.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega16-16P"
		(extends "ATmega16L-8P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega16-16P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2466.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega162-16A"
		(extends "ATmega162V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega162-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2513-8-bit-AVR-Microntroller-ATmega162_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega162-16M"
		(extends "ATmega162V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega162-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2513-8-bit-AVR-Microntroller-ATmega162_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega162-16P"
		(extends "ATmega162V-8P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega162-16P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2513-8-bit-AVR-Microntroller-ATmega162_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega164P-20A"
		(extends "ATmega164PV-10A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164P-20A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42742-ATmega164P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega164P-20M"
		(extends "ATmega164PV-10M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164P-20M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42742-ATmega164P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega164P-20P"
		(extends "ATmega164PV-10P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164P-20P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42742-ATmega164P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega164PA-A"
		(extends "ATmega164A-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164PA-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega164PA-C"
		(extends "ATmega164A-C")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164PA-C"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega164PA-M"
		(extends "ATmega164A-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164PA-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega164PA-MC"
		(extends "ATmega164A-MC")
		(property "Reference" "U"
			(at -13.97 50.8 0)
		)
		(property "Value" "ATmega164PA-MC"
			(at 2.54 -50.8 0)
		)
		(property "Footprint" "Package_DFN_QFN:Microchip_DRQFN-44-1EP_5x5mm_P0.7mm_EP2.65x2.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, DRQFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Microchip*DRQFN*1EP*5x5mm*P0.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega164PA-P"
		(extends "ATmega164A-P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega164PA-P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega165P-16A"
		(extends "ATmega165PV-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega165P-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8019.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega165P-16M"
		(extends "ATmega165PV-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega165P-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8019.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega165PA-A"
		(extends "ATmega165A-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega165PA-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega165PA-M"
		(extends "ATmega165A-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega165PA-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168-20A"
		(extends "ATmega48V-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168-20A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168-20M"
		(extends "ATmega48V-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168-20M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168-20P"
		(extends "ATmega48V-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168-20P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168A-A"
		(extends "ATmega48PV-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168A-A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168A-CC"
		(extends "ATmega48A-CC")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168A-CC"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-32_4.0x4.0mm_Layout6x6_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, UFBGA-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*4.0x4.0mm*Layout6x6*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168A-M"
		(extends "ATmega48PV-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168A-M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168A-MM"
		(extends "ATmega48PV-10MM")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168A-MM"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168A-P"
		(extends "ATmega48PV-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168A-P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168P-20A"
		(extends "ATmega48PV-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168P-20A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168P-20M"
		(extends "ATmega48PV-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168P-20M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168P-20P"
		(extends "ATmega48PV-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168P-20P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168PA-A"
		(extends "ATmega48PV-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168PA-A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168PA-CC"
		(extends "ATmega48A-CC")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168PA-CC"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-32_4.0x4.0mm_Layout6x6_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, UFBGA-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*4.0x4.0mm*Layout6x6*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168PA-M"
		(extends "ATmega48PV-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168PA-M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168PA-MM"
		(extends "ATmega48PV-10MM")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168PA-MM"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168PA-P"
		(extends "ATmega48PV-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168PA-P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168PB-A"
		(extends "ATmega48PB-A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168PB-A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001909A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168PB-M"
		(extends "ATmega48PB-M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168PB-M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001909A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168PV-10A"
		(extends "ATmega48PV-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168PV-10A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168PV-10M"
		(extends "ATmega48PV-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168PV-10M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168PV-10P"
		(extends "ATmega48PV-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168PV-10P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168V-10A"
		(extends "ATmega48V-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168V-10A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168V-10M"
		(extends "ATmega48V-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168V-10M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega168V-10P"
		(extends "ATmega48V-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega168V-10P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega169A-A"
		(extends "ATmega169PV-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega169A-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega169A-M"
		(extends "ATmega169PV-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega169A-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega169A-MC"
		(extends "ATmega169PV-8MC")
		(property "Reference" "U"
			(at -13.97 50.8 0)
		)
		(property "Value" "ATmega169A-MC"
			(at 2.54 -50.8 0)
		)
		(property "Footprint" "Package_DFN_QFN:Microchip_DRQFN-64-1EP_7x7mm_P0.65mm_EP4.1x4.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, DRQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Microchip*DRQFN*1EP*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega169P-16A"
		(extends "ATmega169PV-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega169P-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8018.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega169P-16M"
		(extends "ATmega169PV-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega169P-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8018.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega169P-16MC"
		(extends "ATmega169PV-8MC")
		(property "Reference" "U"
			(at -13.97 50.8 0)
		)
		(property "Value" "ATmega169P-16MC"
			(at 2.54 -50.8 0)
		)
		(property "Footprint" "Package_DFN_QFN:Microchip_DRQFN-64-1EP_7x7mm_P0.65mm_EP4.1x4.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8018.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, DRQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Microchip*DRQFN*1EP*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega169PA-A"
		(extends "ATmega169PV-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega169PA-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega169PA-M"
		(extends "ATmega169PV-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega169PA-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega169PA-MC"
		(extends "ATmega169PV-8MC")
		(property "Reference" "U"
			(at -13.97 50.8 0)
		)
		(property "Value" "ATmega169PA-MC"
			(at 2.54 -50.8 0)
		)
		(property "Footprint" "Package_DFN_QFN:Microchip_DRQFN-64-1EP_7x7mm_P0.65mm_EP4.1x4.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, DRQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Microchip*DRQFN*1EP*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega16A-A"
		(extends "ATmega16L-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega16A-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8154-8-bit-AVR-ATmega16A_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega16A-M"
		(extends "ATmega16L-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega16A-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8154-8-bit-AVR-ATmega16A_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega16A-P"
		(extends "ATmega16L-8P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega16A-P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8154-8-bit-AVR-ATmega16A_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1kB SRAM, 512B EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega16U2-A"
		(extends "ATmega8U2-A")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATmega16U2-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7799.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 512B SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega16U2-M"
		(extends "ATmega8U2-M")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATmega16U2-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7799.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 512B SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega16U4RC-A"
		(extends "ATmega16U4-A")
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega16U4RC-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1.25kB SRAM, 512B EEPROM, USB 2.0, RC Osc, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega16U4RC-M"
		(extends "ATmega16U4-M")
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega16U4RC-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 1.25kB SRAM, 512B EEPROM, USB 2.0, RC Osc, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega2560-16A"
		(extends "ATmega640V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega2560-16A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 256kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega2560-16C"
		(extends "ATmega640V-8C")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega2560-16C"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_9.0x9.0mm_Layout10x10_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at -29.21 71.12 0)
		)
		(property "Description" "16MHz, 256kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*9.0x9.0mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega2560V-8A"
		(extends "ATmega640V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega2560V-8A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 256kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega2560V-8C"
		(extends "ATmega640V-8C")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega2560V-8C"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_9.0x9.0mm_Layout10x10_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at -29.21 71.12 0)
		)
		(property "Description" "8MHz, 256kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*9.0x9.0mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega2561-16A"
		(extends "ATmega1281V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega2561-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 256kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega2561-16M"
		(extends "ATmega1281V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega2561-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 256kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega2561V-8A"
		(extends "ATmega1281V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega2561V-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 256kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega2561V-8M"
		(extends "ATmega1281V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega2561V-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 256kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32-16A"
		(extends "ATmega16L-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega32-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2503.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32-16M"
		(extends "ATmega16L-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega32-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2503.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32-16P"
		(extends "ATmega16L-8P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega32-16P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2503.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324A-A"
		(extends "ATmega164A-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324A-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324A-C"
		(extends "ATmega164A-C")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324A-C"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324A-M"
		(extends "ATmega164A-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324A-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324A-MC"
		(extends "ATmega164A-MC")
		(property "Reference" "U"
			(at -13.97 50.8 0)
		)
		(property "Value" "ATmega324A-MC"
			(at 2.54 -50.8 0)
		)
		(property "Footprint" "Package_DFN_QFN:Microchip_DRQFN-44-1EP_5x5mm_P0.7mm_EP2.65x2.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, DRQFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Microchip*DRQFN*1EP*5x5mm*P0.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324A-P"
		(extends "ATmega164A-P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324A-P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324P-20A"
		(extends "ATmega164PV-10A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324P-20A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42743-ATmega324P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324P-20M"
		(extends "ATmega164PV-10M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324P-20M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42743-ATmega324P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324P-20P"
		(extends "ATmega164PV-10P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324P-20P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42743-ATmega324P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324PA-A"
		(extends "ATmega164A-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324PA-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324PA-C"
		(extends "ATmega164A-C")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324PA-C"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324PA-M"
		(extends "ATmega164A-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324PA-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324PA-MC"
		(extends "ATmega164A-MC")
		(property "Reference" "U"
			(at -13.97 50.8 0)
		)
		(property "Value" "ATmega324PA-MC"
			(at 2.54 -50.8 0)
		)
		(property "Footprint" "Package_DFN_QFN:Microchip_DRQFN-44-1EP_5x5mm_P0.7mm_EP2.65x2.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, DRQFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Microchip*DRQFN*1EP*5x5mm*P0.7mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324PA-P"
		(extends "ATmega164A-P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324PA-P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324PV-10A"
		(extends "ATmega164PV-10A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324PV-10A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42743-ATmega324P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324PV-10M"
		(extends "ATmega164PV-10M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324PV-10M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42743-ATmega324P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega324PV-10P"
		(extends "ATmega164PV-10P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega324PV-10P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42743-ATmega324P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega325-16A"
		(extends "ATmega325V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega325-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2570.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega325-16M"
		(extends "ATmega325V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega325-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2570.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega3250-16A"
		(extends "ATmega3250V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega3250-16A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2570.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega3250A-A"
		(extends "ATmega3250V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega3250A-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega3250P-20A"
		(extends "ATmega3250V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega3250P-20A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8023.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega3250PA-A"
		(extends "ATmega3250V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega3250PA-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega3250PV-10A"
		(extends "ATmega3250V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega3250PV-10A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8023.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega325A-A"
		(extends "ATmega165A-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega325A-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega325A-M"
		(extends "ATmega165A-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega325A-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega325P-20A"
		(extends "ATmega325V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega325P-20A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8023.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega325P-20M"
		(extends "ATmega325V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega325P-20M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8023.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega325PA-A"
		(extends "ATmega165A-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega325PA-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega325PA-M"
		(extends "ATmega165A-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega325PA-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega325PV-10A"
		(extends "ATmega325V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega325PV-10A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8023.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega325PV-10M"
		(extends "ATmega325V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega325PV-10M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8023.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega328-A"
		(extends "ATmega48PV-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega328-A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega328_P%20AVR%20MCU%20with%20picoPower%20Technology%20Data%20Sheet%2040001984A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega328-M"
		(extends "ATmega48PV-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega328-M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega328_P%20AVR%20MCU%20with%20picoPower%20Technology%20Data%20Sheet%2040001984A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega328-MM"
		(extends "ATmega48PV-10MM")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega328-MM"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega328_P%20AVR%20MCU%20with%20picoPower%20Technology%20Data%20Sheet%2040001984A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega328-P"
		(extends "ATmega48PV-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega328-P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega328_P%20AVR%20MCU%20with%20picoPower%20Technology%20Data%20Sheet%2040001984A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega328P-A"
		(extends "ATmega48PV-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega328P-A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega328_P%20AVR%20MCU%20with%20picoPower%20Technology%20Data%20Sheet%2040001984A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega328P-M"
		(extends "ATmega48PV-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega328P-M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega328_P%20AVR%20MCU%20with%20picoPower%20Technology%20Data%20Sheet%2040001984A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega328P-MM"
		(extends "ATmega48PV-10MM")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega328P-MM"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega328_P%20AVR%20MCU%20with%20picoPower%20Technology%20Data%20Sheet%2040001984A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega328P-P"
		(extends "ATmega48PV-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega328P-P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega328_P%20AVR%20MCU%20with%20picoPower%20Technology%20Data%20Sheet%2040001984A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega328PB-A"
		(extends "ATmega48PB-A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega328PB-A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001906C.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega328PB-M"
		(extends "ATmega48PB-M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega328PB-M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001906C.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega329-16A"
		(extends "ATmega329V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega329-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2552.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega329-16M"
		(extends "ATmega329V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega329-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2552.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega3290-16A"
		(extends "ATmega3290V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega3290-16A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2552.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega3290A-A"
		(extends "ATmega3290V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega3290A-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega3290P-20A"
		(extends "ATmega3290V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega3290P-20A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8021-AVR-ATmega329P-3290P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega3290PA-A"
		(extends "ATmega3290V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega3290PA-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega3290PV-10A"
		(extends "ATmega3290V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega3290PV-10A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8021-AVR-ATmega329P-3290P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega329A-A"
		(extends "ATmega169PV-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega329A-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega329A-M"
		(extends "ATmega169PV-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega329A-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega329P-20A"
		(extends "ATmega329V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega329P-20A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8021-AVR-ATmega329P-3290P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega329P-20M"
		(extends "ATmega329V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega329P-20M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8021-AVR-ATmega329P-3290P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega329PA-A"
		(extends "ATmega169PV-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega329PA-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega329PA-M"
		(extends "ATmega169PV-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega329PA-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega329PV-10A"
		(extends "ATmega329V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega329PV-10A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8021-AVR-ATmega329P-3290P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega329PV-10M"
		(extends "ATmega329V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega329PV-10M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8021-AVR-ATmega329P-3290P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32A-A"
		(extends "ATmega16L-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega32A-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8155-8-bit-microcontroller-avr-atmega32a_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32A-M"
		(extends "ATmega16L-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega32A-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8155-8-bit-microcontroller-avr-atmega32a_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32A-P"
		(extends "ATmega16L-8P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega32A-P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8155-8-bit-microcontroller-avr-atmega32a_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32L-8A"
		(extends "ATmega16L-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega32L-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2503.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32L-8M"
		(extends "ATmega16L-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega32L-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2503.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32L-8P"
		(extends "ATmega16L-8P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega32L-8P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2503.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32M1-A"
		(extends "ATmega16M1-A")
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega32M1-A"
			(at 5.08 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8209-8-bit%20AVR%20ATmega16M1-32M1-64M1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, CAN, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32M1-M"
		(extends "ATmega16M1-M")
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega32M1-M"
			(at 5.08 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.65x4.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8209-8-bit%20AVR%20ATmega16M1-32M1-64M1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, CAN, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32U2-A"
		(extends "ATmega8U2-A")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATmega32U2-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7799.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 1kB SRAM, 1kB EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32U2-M"
		(extends "ATmega8U2-M")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATmega32U2-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7799.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 1kB SRAM, 1kB EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32U4-A"
		(extends "ATmega16U4-A")
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega32U4-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32U4-M"
		(extends "ATmega16U4-M")
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega32U4-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32U4RC-A"
		(extends "ATmega16U4-A")
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega32U4RC-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, RC Osc, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega32U4RC-M"
		(extends "ATmega16U4-M")
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega32U4RC-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-7766-8-bit-AVR-ATmega16U4-32U4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2.5kB SRAM, 1kB EEPROM, USB 2.0, RC Osc, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48-20A"
		(extends "ATmega48V-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48-20A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48-20M"
		(extends "ATmega48V-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48-20M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48-20MM"
		(extends "ATmega48V-10MM")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48-20MM"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48-20P"
		(extends "ATmega48V-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48-20P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega4808-A"
		(extends "ATmega3208-A")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATmega4808-A"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40002017A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 48kB Flash, 6kB SRAM, 256B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega4808-M"
		(extends "ATmega3208-M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATmega4808-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm_ThermalVias"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40002017A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 48kB Flash, 6kB SRAM, 256B EEPROM, VQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega4808-X"
		(extends "ATmega3208-X")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATmega4808-X"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40002018A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 48kB Flash, 6kB SRAM, 256B EEPROM, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega4809-A"
		(extends "ATmega3209-A")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATmega4809-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40002016A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 48kB Flash, 6kB SRAM, 256B EEPROM, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega4809-M"
		(extends "ATmega3209-M")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATmega4809-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-48-1EP_6x6mm_P0.4mm_EP4.62x4.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40002016A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 48kB Flash, 6kB SRAM, 256B EEPROM, UQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1EP*6x6mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48A-A"
		(extends "ATmega48PV-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48A-A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48A-M"
		(extends "ATmega48PV-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48A-M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48A-MM"
		(extends "ATmega48PV-10MM")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48A-MM"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48A-P"
		(extends "ATmega48PV-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48A-P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48P-20A"
		(extends "ATmega48PV-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48P-20A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48P-20M"
		(extends "ATmega48PV-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48P-20M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48P-20MM"
		(extends "ATmega48PV-10MM")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48P-20MM"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48P-20P"
		(extends "ATmega48PV-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48P-20P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48PA-A"
		(extends "ATmega48PV-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48PA-A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48PA-CC"
		(extends "ATmega48A-CC")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48PA-CC"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-32_4.0x4.0mm_Layout6x6_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, UFBGA-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*4.0x4.0mm*Layout6x6*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48PA-M"
		(extends "ATmega48PV-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48PA-M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48PA-MM"
		(extends "ATmega48PV-10MM")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48PA-MM"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega48PA-P"
		(extends "ATmega48PV-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega48PA-P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 256B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega64-16A"
		(extends "ATmega64L-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega64-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2490-8-bit-avr-microcontroller-atmega64-l_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega64-16M"
		(extends "ATmega64L-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega64-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2490-8-bit-avr-microcontroller-atmega64-l_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega640-16A"
		(extends "ATmega640V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega640-16A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega640-16C"
		(extends "ATmega640V-8C")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega640-16C"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_9.0x9.0mm_Layout10x10_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2549-8-bit-AVR-Microcontroller-ATmega640-1280-1281-2560-2561_datasheet.pdf"
			(at -29.21 71.12 0)
		)
		(property "Description" "16MHz, 64kB Flash, 8kB SRAM, 4kB EEPROM, JTAG, TFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*9.0x9.0mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644-20A"
		(extends "ATmega644V-10A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644-20A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2593.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644-20M"
		(extends "ATmega644V-10M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644-20M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2593.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644-20P"
		(extends "ATmega644V-10P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644-20P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2593.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644A-A"
		(extends "ATmega164A-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644A-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644A-M"
		(extends "ATmega164A-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644A-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644A-P"
		(extends "ATmega164A-P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644A-P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644P-20A"
		(extends "ATmega164PV-10A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644P-20A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42744-ATmega644P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644P-20M"
		(extends "ATmega164PV-10M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644P-20M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42744-ATmega644P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644P-20P"
		(extends "ATmega164PV-10P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644P-20P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42744-ATmega644P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644PA-A"
		(extends "ATmega164A-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644PA-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644PA-M"
		(extends "ATmega164A-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644PA-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644PA-P"
		(extends "ATmega164A-P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644PA-P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8272-8-bit-AVR-microcontroller-ATmega164A_PA-324A_PA-644A_PA-1284_P_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644PV-10A"
		(extends "ATmega164PV-10A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644PV-10A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42744-ATmega644P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644PV-10M"
		(extends "ATmega164PV-10M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644PV-10M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42744-ATmega644P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega644PV-10P"
		(extends "ATmega164PV-10P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega644PV-10P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42744-ATmega644P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega645-16A"
		(extends "ATmega325V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega645-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2570.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega645-16M"
		(extends "ATmega325V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega645-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2570.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega6450-16A"
		(extends "ATmega3250V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega6450-16A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2570.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega6450A-A"
		(extends "ATmega3250V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega6450A-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega6450P-A"
		(extends "ATmega3250V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega6450P-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega6450V-8A"
		(extends "ATmega3250V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega6450V-8A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2570.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega645A-A"
		(extends "ATmega165A-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega645A-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega645A-M"
		(extends "ATmega165A-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega645A-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega645P-A"
		(extends "ATmega165A-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega645P-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega645P-M"
		(extends "ATmega165A-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega645P-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8285-8-bit-avr-microcontroller-atmega165a_pa_325a_pa_3250a_pa_645a_p_6450a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega645V-8A"
		(extends "ATmega325V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega645V-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2570.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega645V-8M"
		(extends "ATmega325V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega645V-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2570.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega649-16A"
		(extends "ATmega329V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega649-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2552.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega649-16M"
		(extends "ATmega329V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega649-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2552.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega6490-16A"
		(extends "ATmega3290V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega6490-16A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2552.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega6490A-A"
		(extends "ATmega3290V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega6490A-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega6490P-A"
		(extends "ATmega3290V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega6490P-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega6490V-8A"
		(extends "ATmega3290V-8A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATmega6490V-8A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2552.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega649A-A"
		(extends "ATmega169PV-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega649A-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega649A-M"
		(extends "ATmega169PV-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega649A-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega649P-A"
		(extends "ATmega169PV-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega649P-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega649P-M"
		(extends "ATmega169PV-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega649P-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8284-8-bit-avr-microcontroller-atmega169a_pa_329a_pa_3290a_pa_649a_p_6490a_p_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR LCD PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega649V-8A"
		(extends "ATmega329V-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega649V-8A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2552.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega649V-8M"
		(extends "ATmega329V-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega649V-8M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2552.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega64A-A"
		(extends "ATmega64L-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega64A-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8160-8-bit-avr-microcontroller-atmega64a-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega64A-M"
		(extends "ATmega64L-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega64A-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8160-8-bit-avr-microcontroller-atmega64a-datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega64M1-A"
		(extends "ATmega16M1-A")
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega64M1-A"
			(at 5.08 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8209-8-bit%20AVR%20ATmega16M1-32M1-64M1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, CAN, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega64M1-M"
		(extends "ATmega16M1-M")
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATmega64M1-M"
			(at 5.08 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.65x4.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8209-8-bit%20AVR%20ATmega16M1-32M1-64M1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, CAN, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8-16A"
		(extends "ATmega8L-8A")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATmega8-16A"
			(at 5.08 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2486-8-bit-avr-microcontroller-atmega8_l_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8-16M"
		(extends "ATmega8L-8M")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATmega8-16M"
			(at 5.08 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2486-8-bit-avr-microcontroller-atmega8_l_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8-16P"
		(extends "ATmega8L-8P")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATmega8-16P"
			(at 5.08 -34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2486-8-bit-avr-microcontroller-atmega8_l_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8515-16A"
		(extends "ATmega8515L-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8515-16A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2512.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8515-16J"
		(extends "ATmega8515L-8J")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8515-16J"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_LCC:PLCC-44"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2512.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, PLCC-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8515-16M"
		(extends "ATmega8515L-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8515-16M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2512.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8515-16P"
		(extends "ATmega8515L-8P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8515-16P"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2512.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8535-16A"
		(extends "ATmega8535L-8A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8535-16A"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2502.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8535-16J"
		(extends "ATmega8535L-8J")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8535-16J"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_LCC:PLCC-44"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2502.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, PLCC-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8535-16M"
		(extends "ATmega8535L-8M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8535-16M"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2502.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8535-16P"
		(extends "ATmega8535L-8P")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "ATmega8535-16P"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2502.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88-20A"
		(extends "ATmega48V-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88-20A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88-20M"
		(extends "ATmega48V-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88-20M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88-20P"
		(extends "ATmega48V-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88-20P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88A-A"
		(extends "ATmega48PV-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88A-A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88A-CC"
		(extends "ATmega48A-CC")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88A-CC"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-32_4.0x4.0mm_Layout6x6_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, UFBGA-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*4.0x4.0mm*Layout6x6*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88A-M"
		(extends "ATmega48PV-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88A-M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88A-MM"
		(extends "ATmega48PV-10MM")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88A-MM"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88A-P"
		(extends "ATmega48PV-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88A-P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48A_88A_168A-Data-Sheet-40002007A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88P-20A"
		(extends "ATmega48PV-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88P-20A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88P-20M"
		(extends "ATmega48PV-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88P-20M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88P-20P"
		(extends "ATmega48PV-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88P-20P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88PA-A"
		(extends "ATmega48PV-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88PA-A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88PA-CC"
		(extends "ATmega48A-CC")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88PA-CC"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-32_4.0x4.0mm_Layout6x6_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, UFBGA-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*4.0x4.0mm*Layout6x6*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88PA-M"
		(extends "ATmega48PV-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88PA-M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88PA-MM"
		(extends "ATmega48PV-10MM")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88PA-MM"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88PA-P"
		(extends "ATmega48PV-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88PA-P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATmega48PA_88PA_168PA-Data-Sheet-40002011A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR PicoPower"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88PB-A"
		(extends "ATmega48PB-A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88PB-A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001909A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88PB-M"
		(extends "ATmega48PB-M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88PB-M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001909A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88PV-10A"
		(extends "ATmega48PV-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88PV-10A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88PV-10M"
		(extends "ATmega48PV-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88PV-10M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88PV-10P"
		(extends "ATmega48PV-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88PV-10P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8025-8-bit-AVR-Microcontroller-ATmega48P-88P-168P_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88V-10A"
		(extends "ATmega48V-10A")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88V-10A"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88V-10M"
		(extends "ATmega48V-10M")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88V-10M"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega88V-10P"
		(extends "ATmega48V-10P")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "ATmega88V-10P"
			(at 2.54 -36.83 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2545-8-bit-AVR-Microcontroller-ATmega48-88-168_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8A-A"
		(extends "ATmega8L-8A")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATmega8A-A"
			(at 5.08 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Microchip%208bit%20mcu%20AVR%20ATmega8A%20data%20sheet%2040001974A.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8A-M"
		(extends "ATmega8L-8M")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATmega8A-M"
			(at 5.08 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Microchip%208bit%20mcu%20AVR%20ATmega8A%20data%20sheet%2040001974A.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATmega8A-P"
		(extends "ATmega8L-8P")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATmega8A-P"
			(at 5.08 -34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Microchip%208bit%20mcu%20AVR%20ATmega8A%20data%20sheet%2040001974A.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 1kB SRAM, 512B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128A1-A"
		(extends "ATxmega64A1-A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega128A1-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8067-8-and-16-bit-AVR-Microcontrollers-ATxmega64A1-ATxmega128A1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128A1-C"
		(extends "ATxmega64A1-C")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega128A1-C"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_9.0x9.0mm_Layout10x10_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8067-8-and-16-bit-AVR-Microcontrollers-ATxmega64A1-ATxmega128A1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, TFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*9.0x9.0mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128A1-C7"
		(extends "ATxmega64A1-C7")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega128A1-C7"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-100_7.0x7.0mm_Layout10x10_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8067-8-and-16-bit-AVR-Microcontrollers-ATxmega64A1-ATxmega128A1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, VFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*7.0x7.0mm*Layout10x10*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128A1U-A"
		(extends "ATxmega64A1U-A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega128A1U-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8385-8-and-16-bit-AVR-Microcontroller-ATxmega64A1U-ATxmega128A1U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128A1U-C"
		(extends "ATxmega64A1U-C")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega128A1U-C"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:TFBGA-100_9.0x9.0mm_Layout10x10_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8385-8-and-16-bit-AVR-Microcontroller-ATxmega64A1U-ATxmega128A1U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, TFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TFBGA*9.0x9.0mm*Layout10x10*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128A1U-C7"
		(extends "ATxmega64A1U-C7")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega128A1U-C7"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-100_7.0x7.0mm_Layout10x10_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8385-8-and-16-bit-AVR-Microcontroller-ATxmega64A1U-ATxmega128A1U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, VFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*7.0x7.0mm*Layout10x10*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128A3-A"
		(extends "ATxmega64A3-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega128A3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8068-8-and16-bit-AVR-XMEGA-A3-Microcontrollers_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128A3-M"
		(extends "ATxmega64A3-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega128A3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8068-8-and16-bit-AVR-XMEGA-A3-Microcontrollers_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128A3U-A"
		(extends "ATxmega64A3U-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega128A3U-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8386-8-and-16-bit-AVR-Microcontroller-ATxmega64A3U-128A3U-192A3U-256A3U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128A3U-M"
		(extends "ATxmega64A3U-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega128A3U-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8386-8-and-16-bit-AVR-Microcontroller-ATxmega64A3U-128A3U-192A3U-256A3U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128A4U-A"
		(extends "ATxmega16A4U-A")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega128A4U-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8387-8-and16-bit-AVR-Microcontroller-XMEGA-A4U_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128A4U-C"
		(extends "ATxmega16A4U-C")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega128A4U-C"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8387-8-and16-bit-AVR-Microcontroller-XMEGA-A4U_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128A4U-M"
		(extends "ATxmega16A4U-M")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega128A4U-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8387-8-and16-bit-AVR-Microcontroller-XMEGA-A4U_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128B1-A"
		(extends "ATxmega64B1-A")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega128B1-A"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8330-8-and-16-bit-AVR-Microcontroller-XMEGA-B-ATxmega64B1-ATxmega128B1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, LCD, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128B1-C"
		(extends "ATxmega64B1-C")
		(property "Reference" "U"
			(at 0 1.27 0)
		)
		(property "Value" "ATxmega128B1-C"
			(at 0 -1.27 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-100_7.0x7.0mm_Layout10x10_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8330-8-and-16-bit-AVR-Microcontroller-XMEGA-B-ATxmega64B1-ATxmega128B1_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, LCD, VFBGA-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*7.0x7.0mm*Layout10x10*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128B3-A"
		(extends "ATxmega64B3-A")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "ATxmega128B3-A"
			(at 5.08 -46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8074-8-and-16-bit-AVR-Microcontroller-XMEGA-B-ATxmega64B3-ATxmega128B3_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, LCD, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128B3-M"
		(extends "ATxmega64B3-M")
		(property "Reference" "U"
			(at -15.24 46.99 0)
		)
		(property "Value" "ATxmega128B3-M"
			(at 5.08 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8074-8-and-16-bit-AVR-Microcontroller-XMEGA-B-ATxmega64B3-ATxmega128B3_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, LCD, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128C3-A"
		(extends "ATxmega32C3-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega128C3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8492-8-and-16-bit-AVR-microcontroller-ATxmega32C3_64C3_128C3_192C3_256C3_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128C3-M"
		(extends "ATxmega32C3-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega128C3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8492-8-and-16-bit-AVR-microcontroller-ATxmega32C3_64C3_128C3_192C3_256C3_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, USB, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128D3-A"
		(extends "ATxmega32D3-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega128D3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8134-8-16-bit-Atmel-XMEGA-D3-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128D3-M"
		(extends "ATxmega32D3-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega128D3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8134-8-16-bit-Atmel-XMEGA-D3-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128D4-A"
		(extends "ATxmega16D4-A")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega128D4-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8135-8-and-16-bit-AVR-microcontroller-ATxmega16D4-32D4-64D4-128D4_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128D4-C"
		(extends "ATxmega16D4-C")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega128D4-C"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8135-8-and-16-bit-AVR-microcontroller-ATxmega16D4-32D4-64D4-128D4_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega128D4-M"
		(extends "ATxmega16D4-M")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega128D4-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8135-8-and-16-bit-AVR-microcontroller-ATxmega16D4-32D4-64D4-128D4_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 128kB Flash, 8kB Boot, 8kB SRAM, 2kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega16E5-A"
		(extends "ATxmega8E5-A")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATxmega16E5-A"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8153-8-and-16-bit-AVR-Microcontroller-XMEGA-E-ATxmega8E5-ATxmega16E5-ATxmega32E5_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 16kB Flash, 4kB Boot, 2kB SRAM, 512B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega16E5-M"
		(extends "ATxmega8E5-M")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATxmega16E5-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8153-8-and-16-bit-AVR-Microcontroller-XMEGA-E-ATxmega8E5-ATxmega16E5-ATxmega32E5_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 16kB Flash, 4kB Boot, 2kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega16E5-M4"
		(extends "ATxmega8E5-M4")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATxmega16E5-M4"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_4x4mm_P0.4mm_EP2.9x2.9mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8153-8-and-16-bit-AVR-Microcontroller-XMEGA-E-ATxmega8E5-ATxmega16E5-ATxmega32E5_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 16kB Flash, 4kB Boot, 2kB SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega192A3-A"
		(extends "ATxmega64A3-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega192A3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8068-8-and16-bit-AVR-XMEGA-A3-Microcontrollers_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 192kB Flash, 8kB Boot, 16kB SRAM, 2kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega192A3-M"
		(extends "ATxmega64A3-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega192A3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8068-8-and16-bit-AVR-XMEGA-A3-Microcontrollers_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 192kB Flash, 8kB Boot, 16kB SRAM, 2kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega192A3U-A"
		(extends "ATxmega64A3U-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega192A3U-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8386-8-and-16-bit-AVR-Microcontroller-ATxmega64A3U-128A3U-192A3U-256A3U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 192kB Flash, 8kB Boot, 16kB SRAM, 2kB EEPROM, JTAG, USB, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega192A3U-M"
		(extends "ATxmega64A3U-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega192A3U-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8386-8-and-16-bit-AVR-Microcontroller-ATxmega64A3U-128A3U-192A3U-256A3U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 192kB Flash, 8kB Boot, 16kB SRAM, 2kB EEPROM, JTAG, USB, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega192C3-A"
		(extends "ATxmega32C3-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega192C3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8492-8-and-16-bit-AVR-microcontroller-ATxmega32C3_64C3_128C3_192C3_256C3_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 192kB Flash, 8kB Boot, 16kB SRAM, 2kB EEPROM, JTAG, USB, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega192C3-M"
		(extends "ATxmega32C3-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega192C3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8492-8-and-16-bit-AVR-microcontroller-ATxmega32C3_64C3_128C3_192C3_256C3_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 192kB Flash, 8kB Boot, 16kB SRAM, 2kB EEPROM, JTAG, USB, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega192D3-A"
		(extends "ATxmega32D3-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega192D3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8134-8-16-bit-Atmel-XMEGA-D3-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 192kB Flash, 8kB Boot, 16kB SRAM, 2kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega192D3-M"
		(extends "ATxmega32D3-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega192D3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8134-8-16-bit-Atmel-XMEGA-D3-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 192kB Flash, 8kB Boot, 16kB SRAM, 2kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega256A3-A"
		(extends "ATxmega64A3-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega256A3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8068-8-and16-bit-AVR-XMEGA-A3-Microcontrollers_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 256kB Flash, 8kB Boot, 16kB SRAM, 4kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega256A3-M"
		(extends "ATxmega64A3-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega256A3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8068-8-and16-bit-AVR-XMEGA-A3-Microcontrollers_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 256kB Flash, 8kB Boot, 16kB SRAM, 4kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega256A3U-A"
		(extends "ATxmega64A3U-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega256A3U-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8386-8-and-16-bit-AVR-Microcontroller-ATxmega64A3U-128A3U-192A3U-256A3U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 256kB Flash, 8kB Boot, 16kB SRAM, 4kB EEPROM, JTAG, USB, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega256A3U-M"
		(extends "ATxmega64A3U-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega256A3U-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8386-8-and-16-bit-AVR-Microcontroller-ATxmega64A3U-128A3U-192A3U-256A3U_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 256kB Flash, 8kB Boot, 16kB SRAM, 4kB EEPROM, JTAG, USB, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega256C3-A"
		(extends "ATxmega32C3-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega256C3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8492-8-and-16-bit-AVR-microcontroller-ATxmega32C3_64C3_128C3_192C3_256C3_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 256kB Flash, 8kB Boot, 16kB SRAM, 4kB EEPROM, JTAG, USB, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega256C3-M"
		(extends "ATxmega32C3-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega256C3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8492-8-and-16-bit-AVR-microcontroller-ATxmega32C3_64C3_128C3_192C3_256C3_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 256kB Flash, 8kB Boot, 16kB SRAM, 4kB EEPROM, JTAG, USB, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega256D3-A"
		(extends "ATxmega32D3-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega256D3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8134-8-16-bit-Atmel-XMEGA-D3-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 256kB Flash, 8kB Boot, 16kB SRAM, 4kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega256D3-M"
		(extends "ATxmega32D3-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega256D3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8134-8-16-bit-Atmel-XMEGA-D3-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 256kB Flash, 8kB Boot, 16kB SRAM, 4kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega32A4U-A"
		(extends "ATxmega16A4U-A")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega32A4U-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8387-8-and16-bit-AVR-Microcontroller-XMEGA-A4U_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, JTAG, USB, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega32A4U-C"
		(extends "ATxmega16A4U-C")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega32A4U-C"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8387-8-and16-bit-AVR-Microcontroller-XMEGA-A4U_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, JTAG, USB, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega32A4U-M"
		(extends "ATxmega16A4U-M")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega32A4U-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8387-8-and16-bit-AVR-Microcontroller-XMEGA-A4U_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, JTAG, USB, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega32C4-A"
		(extends "ATxmega16C4-A")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega32C4-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8493-8-and-32-bit-AVR-XMEGA-Microcontrollers-ATxmega16C4-ATxmega32C4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega32C4-C"
		(extends "ATxmega16C4-C")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega32C4-C"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8493-8-and-32-bit-AVR-XMEGA-Microcontrollers-ATxmega16C4-ATxmega32C4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, JTAG, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega32C4-M"
		(extends "ATxmega16C4-M")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega32C4-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8493-8-and-32-bit-AVR-XMEGA-Microcontrollers-ATxmega16C4-ATxmega32C4_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega32D4-A"
		(extends "ATxmega16D4-A")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega32D4-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8135-8-and-16-bit-AVR-microcontroller-ATxmega16D4-32D4-64D4-128D4_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega32D4-C"
		(extends "ATxmega16D4-C")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega32D4-C"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8135-8-and-16-bit-AVR-microcontroller-ATxmega16D4-32D4-64D4-128D4_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, JTAG, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega32D4-M"
		(extends "ATxmega16D4-M")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega32D4-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8135-8-and-16-bit-AVR-microcontroller-ATxmega16D4-32D4-64D4-128D4_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega32E5-A"
		(extends "ATxmega8E5-A")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATxmega32E5-A"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8153-8-and-16-bit-AVR-Microcontroller-XMEGA-E-ATxmega8E5-ATxmega16E5-ATxmega32E5_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega32E5-M"
		(extends "ATxmega8E5-M")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATxmega32E5-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8153-8-and-16-bit-AVR-Microcontroller-XMEGA-E-ATxmega8E5-ATxmega16E5-ATxmega32E5_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega32E5-M4"
		(extends "ATxmega8E5-M4")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATxmega32E5-M4"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_4x4mm_P0.4mm_EP2.9x2.9mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8153-8-and-16-bit-AVR-Microcontroller-XMEGA-E-ATxmega8E5-ATxmega16E5-ATxmega32E5_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 32kB Flash, 4kB Boot, 4kB SRAM, 1kB EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega384C3-A"
		(extends "ATxmega32C3-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega384C3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8361-8-and-16-bit-AVR-XMEGA-Microcontrollers-ATxmega384C3_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 384kB Flash, 8kB Boot, 32kB SRAM, 4kB EEPROM, JTAG, USB, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega384C3-M"
		(extends "ATxmega32C3-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega384C3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8361-8-and-16-bit-AVR-XMEGA-Microcontrollers-ATxmega384C3_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 384kB Flash, 8kB Boot, 32kB SRAM, 4kB EEPROM, JTAG, USB, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega384D3-A"
		(extends "ATxmega32D3-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega384D3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8134-8-16-bit-Atmel-XMEGA-D3-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 384kB Flash, 8kB Boot, 32kB SRAM, 4kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega384D3-M"
		(extends "ATxmega32D3-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega384D3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8134-8-16-bit-Atmel-XMEGA-D3-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 384kB Flash, 8kB Boot, 32kB SRAM, 4kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega64A4U-A"
		(extends "ATxmega16A4U-A")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega64A4U-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8387-8-and16-bit-AVR-Microcontroller-XMEGA-A4U_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega64A4U-C"
		(extends "ATxmega16A4U-C")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega64A4U-C"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8387-8-and16-bit-AVR-Microcontroller-XMEGA-A4U_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega64A4U-M"
		(extends "ATxmega16A4U-M")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega64A4U-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8387-8-and16-bit-AVR-Microcontroller-XMEGA-A4U_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega64C3-A"
		(extends "ATxmega32C3-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega64C3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8492-8-and-16-bit-AVR-microcontroller-ATxmega32C3_64C3_128C3_192C3_256C3_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega64C3-M"
		(extends "ATxmega32C3-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega64C3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8492-8-and-16-bit-AVR-microcontroller-ATxmega32C3_64C3_128C3_192C3_256C3_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, USB, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega64D3-A"
		(extends "ATxmega32D3-A")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega64D3-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8134-8-16-bit-Atmel-XMEGA-D3-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega64D3-M"
		(extends "ATxmega32D3-M")
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "ATxmega64D3-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.65x7.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8134-8-16-bit-Atmel-XMEGA-D3-Microcontroller_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega64D4-A"
		(extends "ATxmega16D4-A")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega64D4-A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8135-8-and-16-bit-AVR-microcontroller-ATxmega16D4-32D4-64D4-128D4_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega64D4-C"
		(extends "ATxmega16D4-C")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega64D4-C"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_BGA:VFBGA-49_5.0x5.0mm_Layout7x7_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8135-8-and-16-bit-AVR-microcontroller-ATxmega16D4-32D4-64D4-128D4_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, VFBGA-49"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VFBGA*5.0x5.0mm*Layout7x7*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATxmega64D4-M"
		(extends "ATxmega16D4-M")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "ATxmega64D4-M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_7x7mm_P0.5mm_EP5.2x5.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8135-8-and-16-bit-AVR-microcontroller-ATxmega16D4-32D4-64D4-128D4_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "32MHz, 64kB Flash, 4kB Boot, 4kB SRAM, 2kB EEPROM, JTAG, QFN-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8/16bit Microcontroller XMegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
