(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ATtiny102-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny102-M"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.3x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42505-8-bit-AVR-Microcontrollers-ATtiny102-ATtiny104_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 1kB Flash, 32B SRAM, No EEPROM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny102-M_0_1")
		(symbol "ATtiny102-M_1_1"
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~{RESET}/PA2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny102-SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny102-SS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42505-8-bit-AVR-Microcontrollers-ATtiny102-ATtiny104_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 1kB Flash, 32B SRAM, No EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny102-SS_0_1")
		(symbol "ATtiny102-SS_1_1"
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~{RESET}/PA2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny104-SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny104-SS"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42505-8-bit-AVR-Microcontrollers-ATtiny102-ATtiny104_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 1kB Flash, 32B SRAM, No EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny104-SS_0_1")
		(symbol "ATtiny104-SS_1_1"
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "~{RESET}/PA2")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA3")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA5")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA6")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny13V-10M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13V-10M"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny13V-10M_0_1")
		(symbol "ATtiny13V-10M_1_1"
			(pin no_connect line
				(at -12.7 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -12.7 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -12.7 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -7.62 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -5.08 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}/PB5")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny13V-10MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13V-10MM"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.75x2.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny13V-10MM_0_1")
		(symbol "ATtiny13V-10MM_1_1"
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "10")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}/PB5")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny13V-10P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13V-10P"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny13V-10P_0_1")
		(symbol "ATtiny13V-10P_1_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}/PB5")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny13V-10S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13V-10S"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny13V-10S_0_1")
		(symbol "ATtiny13V-10S_1_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}/PB5")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny13V-10SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13V-10SS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny13V-10SS_0_1")
		(symbol "ATtiny13V-10SS_1_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}/PB5")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny1634-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "ATtiny1634-M"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8303-8-bit-AVR-Microcontroller-tinyAVR-ATtiny1634_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 16kB Flash, 1kB SRAM, 256B EEPROM, ADC, ACI, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny1634-M_0_1")
		(symbol "ATtiny1634-M_1_1"
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA1")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA2")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA5")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA6")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA7")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB1")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC0")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC1")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "~{RESET}/PC3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "XTAL2/PC4")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "XTAL1/PC5")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny1634-S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "ATtiny1634-S"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8303-8-bit-AVR-Microcontroller-tinyAVR-ATtiny1634_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 16kB Flash, 1kB SRAM, 256B EEPROM, ADC, ACI, debugWIRE, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny1634-S_0_1")
		(symbol "ATtiny1634-S_1_1"
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA1")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA2")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA3")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA5")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA6")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA7")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC0")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC1")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC2")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "~{RESET}/PC3")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "XTAL2/PC4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "XTAL1/PC5")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny20-CC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny20-CC"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-15_3.0x3.0mm_Layout4x4_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8235-8-bit-avr-microcontroller-attiny20_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 2kB Flash, 128B SRAM, No EEPROM, UFBGA-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*3.0x3.0mm*Layout4x4*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny20-CC_0_1")
		(symbol "ATtiny20-CC_1_1"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "D4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "D1")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "C3")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "C2")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "C1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "B1")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "A2")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA6")
				(number "A3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "B2")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB0")
				(number "C4")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB1")
				(number "B3")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "A4")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "B4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny20-MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny20-MM"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.45mm_EP1.6x1.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8235-8-bit-avr-microcontroller-attiny20_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 2kB Flash, 128B SRAM, No EEPROM, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny20-MM_0_1")
		(symbol "ATtiny20-MM_1_1"
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -12.7 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny20-SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny20-SS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8235-8-bit-avr-microcontroller-attiny20_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 2kB Flash, 128B SRAM, No EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny20-SS_0_1")
		(symbol "ATtiny20-SS_1_1"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny20-U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny20-U"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-12_1.403x1.555mm_Layout6x4_P0.4mm_Stagger"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8235-8-bit-avr-microcontroller-attiny20_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 2kB Flash, 128B SRAM, No EEPROM, WLCSP-12"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*1.403x1.555mm*Layout6x4*P0.4mm*Stagger*"
			(at 0 0 0)
		)
		(symbol "ATtiny20-U_0_1")
		(symbol "ATtiny20-U_1_1"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "B6")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "B4")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "A3")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "A5")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "A1")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "C1")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA6")
				(number "B2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "C3")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB0")
				(number "D6")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB1")
				(number "C5")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "D2")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "D4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny20-X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny20-X"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8235-8-bit-avr-microcontroller-attiny20_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 2kB Flash, 128B SRAM, No EEPROM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny20-X_0_1")
		(symbol "ATtiny20-X_1_1"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA0")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny202-SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny202-SS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny202-402-AVR-MCU-with-Core-Independent-Peripherals_and-picoPower-40001969A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 64B EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny202-SS_0_1")
		(symbol "ATtiny202-SS_1_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "~{RESET}/PA0")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA1")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA2")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA6")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA7")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny204-SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny204-SS"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/50002687A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 64B EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny204-SS_0_1")
		(symbol "ATtiny204-SS_1_1"
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PB0")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PB1")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PB2")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PB3")
				(number "6")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "~{RESET}/PA0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny2313A-MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny2313A-MM"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.45mm_EP1.55x1.55mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8246.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny2313A-MM_0_1")
		(symbol "ATtiny2313A-MM_1_1"
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA2/~{RESET}")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA0/XTAL1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA1/XTAL2")
				(number "2")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "18")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PD1")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD2")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD3")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD5")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD6")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny2313V-10M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny2313V-10M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLF-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2543-AVR-ATtiny2313_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny2313V-10M_0_1")
		(symbol "ATtiny2313V-10M_1_1"
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA2/~{RESET}")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA0/XTAL1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA1/XTAL2")
				(number "2")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "18")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PD1")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD2")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD3")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD5")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD6")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny2313V-10P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny2313V-10P"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2543-AVR-ATtiny2313_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny2313V-10P_0_1")
		(symbol "ATtiny2313V-10P_1_1"
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA2/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA0/XTAL1")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA1/XTAL2")
				(number "4")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PD0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PD1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD2")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD4")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD6")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny2313V-10S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny2313V-10S"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2543-AVR-ATtiny2313_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny2313V-10S_0_1")
		(symbol "ATtiny2313V-10S_1_1"
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA2/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA0/XTAL1")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA1/XTAL2")
				(number "4")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PD0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PD1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD2")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD4")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD6")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny24A-CC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny24A-CC"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-15_3.0x3.0mm_Layout4x4_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, UFBGA-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*3.0x3.0mm*Layout4x4*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny24A-CC_0_1")
		(symbol "ATtiny24A-CC_1_1"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "D4")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "D2")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "D3")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "D1")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "C3")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "C2")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "C1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "B1")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "A2")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA6")
				(number "A3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "B2")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "XTAL1/PB0")
				(number "C4")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "XTAL2/PB1")
				(number "B3")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "A4")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "B4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny24A-MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny24A-MM"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.45mm_EP1.6x1.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny24A-MM_0_1")
		(symbol "ATtiny24A-MM_1_1"
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -12.7 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "XTAL1/PB0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "XTAL2/PB1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny24V-10M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny24V-10M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny24V-10M_0_1")
		(symbol "ATtiny24V-10M_1_1"
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -12.7 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "XTAL1/PB0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "XTAL2/PB1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny24V-10P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny24V-10P"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny24V-10P_0_1")
		(symbol "ATtiny24V-10P_1_1"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "XTAL1/PB0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "XTAL2/PB1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny24V-10SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny24V-10SS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny24V-10SS_0_1")
		(symbol "ATtiny24V-10SS_1_1"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "XTAL1/PB0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "XTAL2/PB1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny25V-10M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny25V-10M"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny25V-10M_0_1")
		(symbol "ATtiny25V-10M_1_1"
			(pin no_connect line
				(at -12.7 10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -12.7 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at -12.7 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -7.62 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -5.08 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -2.54 -12.7 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "AREF/PB0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "XTAL1/PB3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "XTAL2/PB4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}/PB5")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny25V-10P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny25V-10P"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny25V-10P_0_1")
		(symbol "ATtiny25V-10P_1_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "AREF/PB0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "XTAL1/PB3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "XTAL2/PB4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}/PB5")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny25V-10S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny25V-10S"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny25V-10S_0_1")
		(symbol "ATtiny25V-10S_1_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "AREF/PB0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "XTAL1/PB3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "XTAL2/PB4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}/PB5")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny25V-10SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny25V-10SS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny25V-10SS_0_1")
		(symbol "ATtiny25V-10SS_1_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "AREF/PB0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "XTAL1/PB3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "XTAL2/PB4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}/PB5")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny261A-X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny261A-X"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8197.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny261A-X_0_1")
		(symbol "ATtiny261A-X_1_1"
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "AREF/PA3")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "XTAL1/PB4")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "XTAL2/PB5")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "~{RESET}/PB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny26L-8M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny26L-8M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc1477.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 2kB Flash, 128B SRAM, 128B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny26L-8M_0_1")
		(symbol "ATtiny26L-8M_1_1"
			(pin no_connect line
				(at -12.7 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -12.7 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -12.7 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at -12.7 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at -12.7 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at -12.7 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "AREF/PA3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "XTAL1/PB4")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "XTAL2/PB5")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "~{RESET}/PB7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny26L-8P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny26L-8P"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc1477.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 2kB Flash, 128B SRAM, 128B EEPROM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny26L-8P_0_1")
		(symbol "ATtiny26L-8P_1_1"
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "AREF/PA3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "XTAL1/PB4")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "XTAL2/PB5")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "~{RESET}/PB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny26L-8S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny26L-8S"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc1477.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 2kB Flash, 128B SRAM, 128B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny26L-8S_0_1")
		(symbol "ATtiny26L-8S_1_1"
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "AREF/PA3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "XTAL1/PB4")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "XTAL2/PB5")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "~{RESET}/PB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny28V-1A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATtiny28V-1A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc1062.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.2MHz, 2kB Flash, No SRAM, No EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR IR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny28V-1A_0_1")
		(symbol "ATtiny28V-1A_1_1"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "~{RESET}")
				(number "29")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "XTAL1")
				(number "7")
			)
			(pin output line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "XTAL2")
				(number "8")
			)
			(pin no_connect line
				(at -12.7 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -12.7 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -12.7 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at -12.7 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "18")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA0")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA1")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB6")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB7")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny28V-1M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATtiny28V-1M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc1062.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.2MHz, 2kB Flash, No SRAM, No EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR IR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny28V-1M_0_1")
		(symbol "ATtiny28V-1M_1_1"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "~{RESET}")
				(number "29")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "XTAL1")
				(number "7")
			)
			(pin output line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "XTAL2")
				(number "8")
			)
			(pin no_connect line
				(at -12.7 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -12.7 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -12.7 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at -12.7 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "18")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA0")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA1")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB6")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB7")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny28V-1P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATtiny28V-1P"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc1062.pdf"
			(at 0 0 0)
		)
		(property "Description" "1.2MHz, 2kB Flash, No SRAM, No EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR IR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny28V-1P_0_1")
		(symbol "ATtiny28V-1P_1_1"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "XTAL1")
				(number "9")
			)
			(pin output line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "XTAL2")
				(number "10")
			)
			(pin no_connect line
				(at -12.7 -30.48 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "21")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA0")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA1")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB0")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB4")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB5")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB6")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB7")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PD0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PD1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD2")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD3")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny4-MA"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny4-MA"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8127-AVR-8-bit-Microcontroller-ATtiny4-ATtiny5-ATtiny9-ATtiny10_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 512B Flash, 32B SRAM, No EEPROM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny4-MA_0_1")
		(symbol "ATtiny4-MA_1_1"
			(pin no_connect line
				(at -12.7 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -12.7 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny4-TS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny4-TS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8127-AVR-8-bit-Microcontroller-ATtiny4-ATtiny5-ATtiny9-ATtiny10_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 512B Flash, 32B SRAM, No EEPROM, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?6*"
			(at 0 0 0)
		)
		(symbol "ATtiny4-TS_0_1")
		(symbol "ATtiny4-TS_1_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny40-MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "ATtiny40-MM"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.45mm_EP1.6x1.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8263-8-bit-avr-microcontroller-tinyavr-attiny40_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 4kB Flash, 256B SRAM, No EEPROM, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny40-MM_0_1")
		(symbol "ATtiny40-MM_1_1"
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA0")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA1")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA2")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA5")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA6")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA7")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB1")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC0")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC1")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "~{RESET}/PC3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC4")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PC5")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny40-S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "ATtiny40-S"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8263-8-bit-avr-microcontroller-tinyavr-attiny40_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 4kB Flash, 256B SRAM, No EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny40-S_0_1")
		(symbol "ATtiny40-S_1_1"
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA1")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA2")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA3")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA5")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA6")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA7")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC0")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC1")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC2")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "~{RESET}/PC3")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PC5")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny40-X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 31.75 0)
		)
		(property "Value" "ATtiny40-X"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-8263-8-bit-avr-microcontroller-tinyavr-attiny40_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 4kB Flash, 256B SRAM, No EEPROM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny40-X_0_1")
		(symbol "ATtiny40-X_1_1"
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "11")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PA1")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA2")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA3")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA5")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA6")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA7")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB2")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB3")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC0")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC1")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC2")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "~{RESET}/PC3")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PC5")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny406-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny406-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Microchip%208bit%20mcu%20AVR%20ATtiny406%20data%20sheet%2040001976A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 128B EEPROM, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny406-M_0_1")
		(symbol "ATtiny406-M_1_1"
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC0")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC1")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PC2")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC3")
				(number "18")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "~{RESET}/PA0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB3")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB4")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny406-S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny406-S"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Microchip%208bit%20mcu%20AVR%20ATtiny406%20data%20sheet%2040001976A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 128B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny406-S_0_1")
		(symbol "ATtiny406-S_1_1"
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC0")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC1")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PC2")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC3")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "~{RESET}/PA0")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB2")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB3")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB4")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB5")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny43U-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny43U-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8048.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 4kB Flash, 256B SRAM, 64B EEPROM, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR Battery Boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny43U-M_0_1")
		(symbol "ATtiny43U-M_1_1"
			(pin passive line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "LSW")
				(number "9")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VBAT")
				(number "10")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~{RESET}/PA7")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny43U-S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny43U-S"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8048.pdf"
			(at 0 0 0)
		)
		(property "Description" "8MHz, 4kB Flash, 256B SRAM, 64B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR Battery Boost"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny43U-S_0_1")
		(symbol "ATtiny43U-S_1_1"
			(pin passive line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "LSW")
				(number "11")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "VBAT")
				(number "12")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "~{RESET}/PA7")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny441-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny441-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8495-8-bit-AVR-Microcontrollers-ATtiny441-ATtiny841_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 4kB Flash, 256B SRAM, 256B EEPROM, ADC, ACI, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny441-M_0_1")
		(symbol "ATtiny441-M_1_1"
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -12.7 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "XTAL1/PB0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "XTAL2/PB1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny441-MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny441-MM"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.45mm_EP1.6x1.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8495-8-bit-AVR-Microcontrollers-ATtiny441-ATtiny841_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 4kB Flash, 256B SRAM, 256B EEPROM, ADC, ACI, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny441-MM_0_1")
		(symbol "ATtiny441-MM_1_1"
			(pin no_connect line
				(at -12.7 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -12.7 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -12.7 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -12.7 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -12.7 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -12.7 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "9")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "XTAL1/PB0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "XTAL2/PB1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny441-SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny441-SS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8495-8-bit-AVR-Microcontrollers-ATtiny441-ATtiny841_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 4kB Flash, 256B SRAM, 256B EEPROM, ADC, ACI, debugWIRE, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny441-SS_0_1")
		(symbol "ATtiny441-SS_1_1"
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "AREF/PA0")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "XTAL1/PB0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "XTAL2/PB1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB2")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "~{RESET}/PB3")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny45V-10X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny45V-10X"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny45V-10X_0_1")
		(symbol "ATtiny45V-10X_1_1"
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VCC")
				(number "8")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "AREF/PB0")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "XTAL1/PB3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "XTAL2/PB4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}/PB5")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny461V-10M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny461V-10M"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2588-8-bit-avr-microcontrollers-tinyavr-attiny261-attiny461-attiny861_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 256B SRAM, 256B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny461V-10M_0_1")
		(symbol "ATtiny461V-10M_1_1"
			(pin no_connect line
				(at -15.24 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -15.24 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -15.24 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -15.24 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -15.24 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -15.24 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -15.24 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin no_connect line
				(at -15.24 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at -15.24 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at -15.24 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "27")
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "28")
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "AREF/PA3")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "XTAL1/PB4")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "XTAL2/PB5")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "~{RESET}/PB7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny461V-10P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny461V-10P"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2588-8-bit-avr-microcontrollers-tinyavr-attiny261-attiny461-attiny861_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 256B SRAM, 256B EEPROM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny461V-10P_0_1")
		(symbol "ATtiny461V-10P_1_1"
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "AREF/PA3")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "XTAL1/PB4")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "XTAL2/PB5")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "~{RESET}/PB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny461V-10S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny461V-10S"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2588-8-bit-avr-microcontrollers-tinyavr-attiny261-attiny461-attiny861_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 256B SRAM, 256B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny461V-10S_0_1")
		(symbol "ATtiny461V-10S_1_1"
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "5")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "15")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "AREF/PA3")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "XTAL1/PB4")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "XTAL2/PB5")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "~{RESET}/PB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny48-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATtiny48-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8008.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 4kB Flash, 256B SRAM, 64B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny48-A_0_1")
		(symbol "ATtiny48-A_1_1"
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC7")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny48-CC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATtiny48-CC"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-32_4.0x4.0mm_Layout6x6_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8008.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 4kB Flash, 256B SRAM, 64B EEPROM, UFBGA-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*4.0x4.0mm*Layout6x6*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny48-CC_0_1")
		(symbol "ATtiny48-CC_1_1"
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "D1")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "C1")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C6")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "E5")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "D6")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "C5")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "C2")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "D2")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB0")
				(number "E3")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB1")
				(number "F4")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB2")
				(number "E4")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB3")
				(number "F5")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB4")
				(number "F6")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB5")
				(number "E6")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB6")
				(number "E1")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB7")
				(number "F1")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC0")
				(number "B6")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC1")
				(number "A6")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC2")
				(number "A5")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC3")
				(number "B5")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC4")
				(number "A4")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC5")
				(number "B4")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "A3")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC7")
				(number "D5")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD0")
				(number "B3")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD1")
				(number "A2")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD2")
				(number "A1")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD3")
				(number "B1")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD4")
				(number "B2")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD5")
				(number "F2")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD6")
				(number "E2")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD7")
				(number "F3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny48-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATtiny48-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8008.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 4kB Flash, 256B SRAM, 64B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny48-M_0_1")
		(symbol "ATtiny48-M_1_1"
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA1")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA3")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB1")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB3")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB4")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB5")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC7")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD0")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD1")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD2")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD5")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny48-MM"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "ATtiny48-MM"
			(at 2.54 -39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8008.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 4kB Flash, 256B SRAM, 64B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny48-MM_0_1")
		(symbol "ATtiny48-MM_1_1"
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VCC")
				(number "3")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "AVCC")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB6")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB7")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD3")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD4")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD5")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD6")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny48-P"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "ATtiny48-P"
			(at 2.54 -39.37 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8008.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 4kB Flash, 256B SRAM, 64B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny48-P_0_1")
		(symbol "ATtiny48-P_1_1"
			(pin power_in line
				(at 0 40.64 270)
				(length 2.54)
				(name "VCC")
				(number "7")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 2.54)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 2.54)
				(name "AVCC")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PB0")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB3")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB4")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB5")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB6")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB7")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PC0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PC1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PC3")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PC4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "~{RESET}/PC6")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC7")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PD0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PD1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PD2")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PD3")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "PD4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny807-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny807-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny807_1607-Data-Sheet-40002030A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 128B EEPROM, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny807-M_0_1")
		(symbol "ATtiny807-M_1_1"
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PC0")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC1")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC2")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PC3")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC4")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PC5")
				(number "22")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "~{RESET}/PA0")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny828-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny828-A"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8371.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 256B EEPROM, debugWIRE, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny828-A_0_1")
		(symbol "ATtiny828-A_1_1"
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PD0")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PD1")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PD2/~{RESET}")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PD3")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PC0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC1")
				(number "32")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC2")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PC3")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC4")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PC5")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PC6")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PC7")
				(number "8")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny828-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny828-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8371.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 256B EEPROM, debugWIRE, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny828-M_0_1")
		(symbol "ATtiny828-M_1_1"
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PD0")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PD1")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PD2/~{RESET}")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PD3")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PC0")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PC1")
				(number "32")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PC2")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PC3")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PC4")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PC5")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PC6")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PC7")
				(number "8")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PB7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny87-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny87-M"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8265-8-bit-AVR-Microcontroller-tinyAVR-ATtiny87-ATtiny167_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny87-M_0_1")
		(symbol "ATtiny87-M_1_1"
			(pin no_connect line
				(at -15.24 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin no_connect line
				(at -15.24 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "2")
			)
			(pin no_connect line
				(at -15.24 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -15.24 -2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -15.24 -5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -15.24 -7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -15.24 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -15.24 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -15.24 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at -15.24 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "23")
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "AREF/PA7")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "XTAL1/PB4")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "XTAL2/PB5")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "~{RESET}/PB7")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny87-S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny87-S"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8265-8-bit-AVR-Microcontroller-tinyAVR-ATtiny87-ATtiny167_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny87-S_0_1")
		(symbol "ATtiny87-S_1_1"
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "AREF/PA7")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "XTAL1/PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "XTAL2/PB5")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "~{RESET}/PB7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny87-X"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny87-X"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8265-8-bit-AVR-Microcontroller-tinyAVR-ATtiny87-ATtiny167_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "ATtiny87-X_0_1")
		(symbol "ATtiny87-X_1_1"
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VCC")
				(number "15")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "AVCC")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PA0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PA1")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "AREF/PA7")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB0")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB1")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB2")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB3")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "XTAL1/PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "XTAL2/PB5")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "~{RESET}/PB7")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATtiny10-MA"
		(extends "ATtiny4-MA")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny10-MA"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8127-AVR-8-bit-Microcontroller-ATtiny4-ATtiny5-ATtiny9-ATtiny10_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 1kB Flash, 32B SRAM, No EEPROM, ADC, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny10-TS"
		(extends "ATtiny4-TS")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny10-TS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8127-AVR-8-bit-Microcontroller-ATtiny4-ATtiny5-ATtiny9-ATtiny10_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 1kB Flash, 32B SRAM, No EEPROM, ADC, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny13-20M"
		(extends "ATtiny13V-10M")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13-20M"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny13-20MM"
		(extends "ATtiny13V-10MM")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13-20MM"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.75x2.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny13-20P"
		(extends "ATtiny13V-10P")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13-20P"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny13-20S"
		(extends "ATtiny13V-10S")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13-20S"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny13-20SS"
		(extends "ATtiny13V-10SS")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13-20SS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny13A-M"
		(extends "ATtiny13V-10M")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13A-M"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8126.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny13A-MM"
		(extends "ATtiny13V-10MM")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13A-MM"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-10-1EP_3x3mm_P0.5mm_EP1.75x2.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8126.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, DFN-10"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny13A-P"
		(extends "ATtiny13V-10P")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13A-P"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8126.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny13A-S"
		(extends "ATtiny13V-10S")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13A-S"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU08/ProductDocuments/DataSheets/ATtiny13A-Data-Sheet-DS40002307A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny13A-SS"
		(extends "ATtiny13V-10SS")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny13A-SS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8126.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 1kB Flash, 64B SRAM, 64B EEPROM, debugWIRE, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1604-SS"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny1604-SS"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny804_1604-Data-Sheet-40002028A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 256B EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1606-M"
		(extends "ATtiny406-M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny1606-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny806_1606_Data_Sheet_40002029A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 256B EEPROM, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1606-S"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny1606-S"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny806_1606_Data_Sheet_40002029A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 256B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1607-M"
		(extends "ATtiny807-M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny1607-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny807_1607-Data-Sheet-40002030A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 1kB SRAM, 256B EEPROM, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1614-SS"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny1614-SS"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny1614-data-sheet-40001995A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 2kB SRAM, 256B EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1616-M"
		(extends "ATtiny406-M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny1616-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny3216_ATtiny1616-data-sheet-40001997B.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 2kB SRAM, 256B EEPROM, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1616-S"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny1616-S"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny3216_ATtiny1616-data-sheet-40001997B.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 2kB SRAM, 256B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1617-M"
		(extends "ATtiny807-M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny1617-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny3217_1617-Data-Sheet-40001999B.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 2kB SRAM, 256B EEPROM, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1624-SS"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny1624-SS"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny1624-26-27-DataSheet-DS40002234A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 2kB SRAM, 256B EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1624-X"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny1624-X"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny1624-26-27-DataSheet-DS40002234A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 2kB SRAM, 256B EEPROM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1626-M"
		(extends "ATtiny406-M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny1626-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny1624-26-27-DataSheet-DS40002234A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 2kB SRAM, 256B EEPROM, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1626-S"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny1626-S"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny1624-26-27-DataSheet-DS40002234A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 2kB SRAM, 256B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1626-X"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny1626-X"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny1624-26-27-DataSheet-DS40002234A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 2kB SRAM, 256B EEPROM, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny1627-M"
		(extends "ATtiny807-M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny1627-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny1624-26-27-DataSheet-DS40002234A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 16kB Flash, 2kB SRAM, 256B EEPROM, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny167-M"
		(extends "ATtiny87-M")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny167-M"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8265-8-bit-AVR-Microcontroller-tinyAVR-ATtiny87-ATtiny167_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny167-S"
		(extends "ATtiny87-S")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny167-S"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8265-8-bit-AVR-Microcontroller-tinyAVR-ATtiny87-ATtiny167_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny167-X"
		(extends "ATtiny87-X")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny167-X"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8265-8-bit-AVR-Microcontroller-tinyAVR-ATtiny87-ATtiny167_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR Automotive"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny212-SS"
		(extends "ATtiny202-SS")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny212-SS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001911A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 64B EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny214-SS"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny214-SS"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001912A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 64B EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny2313-20M"
		(extends "ATtiny2313V-10M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny2313-20M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLF-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2543-AVR-ATtiny2313_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny2313-20P"
		(extends "ATtiny2313V-10P")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny2313-20P"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2543-AVR-ATtiny2313_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny2313-20S"
		(extends "ATtiny2313V-10S")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny2313-20S"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-2543-AVR-ATtiny2313_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny2313A-M"
		(extends "ATtiny2313V-10M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny2313A-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLF-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8246.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny2313A-P"
		(extends "ATtiny2313V-10P")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny2313A-P"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8246.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny2313A-S"
		(extends "ATtiny2313V-10S")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny2313A-S"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8246.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny24-20M"
		(extends "ATtiny24V-10M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny24-20M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny24-20P"
		(extends "ATtiny24V-10P")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny24-20P"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny24-20SS"
		(extends "ATtiny24V-10SS")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny24-20SS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny24A-M"
		(extends "ATtiny24V-10M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny24A-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny24A-P"
		(extends "ATtiny24V-10P")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny24A-P"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny24A-SS"
		(extends "ATtiny24V-10SS")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny24A-SS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny25-20M"
		(extends "ATtiny25V-10M")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny25-20M"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny25-20P"
		(extends "ATtiny25V-10P")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny25-20P"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny25-20S"
		(extends "ATtiny25V-10S")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny25-20S"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny25-20SS"
		(extends "ATtiny25V-10SS")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny25-20SS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, debugWIRE, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny26-16M"
		(extends "ATtiny26L-8M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny26-16M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc1477.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 2kB Flash, 128B SRAM, 128B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny26-16P"
		(extends "ATtiny26L-8P")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny26-16P"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc1477.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 2kB Flash, 128B SRAM, 128B EEPROM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny26-16S"
		(extends "ATtiny26L-8S")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny26-16S"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc1477.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 2kB Flash, 128B SRAM, 128B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny261A-M"
		(extends "ATtiny461V-10M")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny261A-M"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8197.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny261A-P"
		(extends "ATtiny461V-10P")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny261A-P"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8197.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny261A-S"
		(extends "ATtiny461V-10S")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny261A-S"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8197.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 2kB Flash, 128B SRAM, 128B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny28L-4A"
		(extends "ATtiny28V-1A")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATtiny28L-4A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc1062.pdf"
			(at 0 0 0)
		)
		(property "Description" "4MHz, 2kB Flash, No SRAM, No EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR IR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny28L-4M"
		(extends "ATtiny28V-1M")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATtiny28L-4M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc1062.pdf"
			(at 0 0 0)
		)
		(property "Description" "4MHz, 2kB Flash, No SRAM, No EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR IR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny28L-4P"
		(extends "ATtiny28V-1P")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "ATtiny28L-4P"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc1062.pdf"
			(at 0 0 0)
		)
		(property "Description" "4MHz, 2kB Flash, No SRAM, No EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR IR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny3216-M"
		(extends "ATtiny406-M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny3216-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny3216_ATtiny1616-data-sheet-40001997B.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 256B EEPROM, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny3216-S"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny3216-S"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny3216_ATtiny1616-data-sheet-40001997B.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 256B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny3217-M"
		(extends "ATtiny807-M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny3217-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny3217_1617-Data-Sheet-40001999B.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 2kB SRAM, 256B EEPROM, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny3224-SS"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny3224-SS"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny3224-3226-3227-Data-Sheet-DS40002345A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 3kB SRAM, 256B EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny3224-X"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny3224-X"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny3224-3226-3227-Data-Sheet-DS40002345A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 3kB SRAM, 256B EEPROM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny3226-M"
		(extends "ATtiny406-M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny3226-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny3224-3226-3227-Data-Sheet-DS40002345A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 3kB SRAM, 256B EEPROM, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny3226-S"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny3226-S"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny3224-3226-3227-Data-Sheet-DS40002345A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 3kB SRAM, 256B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny3226-X"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny3226-X"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny3224-3226-3227-Data-Sheet-DS40002345A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 3kB SRAM, 256B EEPROM, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny3227-M"
		(extends "ATtiny807-M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny3227-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny3224-3226-3227-Data-Sheet-DS40002345A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 32kB Flash, 3kB SRAM, 256B EEPROM, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny402-SS"
		(extends "ATtiny202-SS")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny402-SS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny202-402-AVR-MCU-with-Core-Independent-Peripherals_and-picoPower-40001969A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 128B EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny404-SS"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny404-SS"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/50002687A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 128B EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny412-SS"
		(extends "ATtiny202-SS")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny412-SS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001911A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 128B EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny414-SS"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny414-SS"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001912A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 128B EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny416-M"
		(extends "ATtiny406-M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny416-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001913A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 128B EEPROM, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny416-S"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny416-S"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001913A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 128B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny417-M"
		(extends "ATtiny807-M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny417-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001901B.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 128B EEPROM, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny424-SS"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny424-SS"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 128B EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny424-X"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny424-X"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 128B EEPROM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny426-M"
		(extends "ATtiny406-M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny426-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 128B EEPROM, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny426-S"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny426-S"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 128B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny426-X"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny426-X"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 128B EEPROM, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny427-M"
		(extends "ATtiny807-M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny427-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 512B SRAM, 128B EEPROM, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny4313-M"
		(extends "ATtiny2313V-10M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny4313-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:MLF-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8246.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny4313-MM"
		(extends "ATtiny2313A-MM")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny4313-MM"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.45mm_EP1.55x1.55mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8246.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny4313-P"
		(extends "ATtiny2313V-10P")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny4313-P"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8246.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny4313-S"
		(extends "ATtiny2313V-10S")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny4313-S"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8246.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny44-20M"
		(extends "ATtiny24V-10M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny44-20M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny44-20P"
		(extends "ATtiny24V-10P")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny44-20P"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny44-20SS"
		(extends "ATtiny24V-10SS")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny44-20SS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny44A-CC"
		(extends "ATtiny24A-CC")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny44A-CC"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-15_3.0x3.0mm_Layout4x4_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, UFBGA-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*3.0x3.0mm*Layout4x4*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny44A-M"
		(extends "ATtiny24V-10M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny44A-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny44A-MM"
		(extends "ATtiny24A-MM")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny44A-MM"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.45mm_EP1.6x1.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny44A-P"
		(extends "ATtiny24V-10P")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny44A-P"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny44A-SS"
		(extends "ATtiny24V-10SS")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny44A-SS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny44V-10M"
		(extends "ATtiny24V-10M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny44V-10M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny44V-10P"
		(extends "ATtiny24V-10P")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny44V-10P"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny44V-10SS"
		(extends "ATtiny24V-10SS")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny44V-10SS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny45-20M"
		(extends "ATtiny25V-10M")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny45-20M"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny45-20P"
		(extends "ATtiny25V-10P")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny45-20P"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny45-20S"
		(extends "ATtiny25V-10S")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny45-20S"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny45-20X"
		(extends "ATtiny45V-10X")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny45-20X"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-8_4.4x3mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, TSSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny45V-10M"
		(extends "ATtiny25V-10M")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny45V-10M"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny45V-10P"
		(extends "ATtiny25V-10P")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny45V-10P"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny45V-10S"
		(extends "ATtiny25V-10S")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny45V-10S"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 4kB Flash, 256B SRAM, 256B EEPROM, debugWIRE, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny461-20M"
		(extends "ATtiny461V-10M")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny461-20M"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2588-8-bit-avr-microcontrollers-tinyavr-attiny261-attiny461-attiny861_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny461-20P"
		(extends "ATtiny461V-10P")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny461-20P"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2588-8-bit-avr-microcontrollers-tinyavr-attiny261-attiny461-attiny861_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny461-20S"
		(extends "ATtiny461V-10S")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny461-20S"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2588-8-bit-avr-microcontrollers-tinyavr-attiny261-attiny461-attiny861_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny461A-M"
		(extends "ATtiny461V-10M")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny461A-M"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8197.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny461A-P"
		(extends "ATtiny461V-10P")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny461A-P"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8197.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny461A-S"
		(extends "ATtiny461V-10S")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny461A-S"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8197.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny461A-X"
		(extends "ATtiny261A-X")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny461A-X"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8197.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 4kB Flash, 256B SRAM, 256B EEPROM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny5-MA"
		(extends "ATtiny4-MA")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny5-MA"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8127-AVR-8-bit-Microcontroller-ATtiny4-ATtiny5-ATtiny9-ATtiny10_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 512B Flash, 32B SRAM, No EEPROM, ADC, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny5-TS"
		(extends "ATtiny4-TS")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny5-TS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8127-AVR-8-bit-Microcontroller-ATtiny4-ATtiny5-ATtiny9-ATtiny10_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 512B Flash, 32B SRAM, No EEPROM, ADC, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?6*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny804-SS"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny804-SS"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny804_1604-Data-Sheet-40002028A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 128B EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny806-M"
		(extends "ATtiny406-M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny806-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny806_1606_Data_Sheet_40002029A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 128B EEPROM, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny806-S"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny806-S"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny806_1606_Data_Sheet_40002029A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 128B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny814-SS"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny814-SS"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001912A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 128B EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny816-M"
		(extends "ATtiny406-M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny816-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001913A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 128B EEPROM, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny816-S"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny816-S"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001913A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 128B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny817-M"
		(extends "ATtiny807-M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny817-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001901B.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 128B EEPROM, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny824-SS"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny824-SS"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 128B EEPROM, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny824-X"
		(extends "ATtiny204-SS")
		(property "Reference" "U"
			(at -12.7 16.51 0)
		)
		(property "Value" "ATtiny824-X"
			(at 2.54 -16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 128B EEPROM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny826-M"
		(extends "ATtiny406-M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny826-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-20-1EP_3x3mm_P0.4mm_EP1.7x1.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 128B EEPROM, VQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*3x3mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny826-S"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny826-S"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 128B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny826-X"
		(extends "ATtiny406-S")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny826-X"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 128B EEPROM, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny827-M"
		(extends "ATtiny807-M")
		(property "Reference" "U"
			(at -12.7 26.67 0)
		)
		(property "Value" "ATtiny827-M"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/ATtiny424-426-427-824-826-827-DataSheet-DS40002311A.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 1kB SRAM, 128B EEPROM, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny84-20M"
		(extends "ATtiny24V-10M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny84-20M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny84-20P"
		(extends "ATtiny24V-10P")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny84-20P"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny84-20SS"
		(extends "ATtiny24V-10SS")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny84-20SS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny841-M"
		(extends "ATtiny441-M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny841-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8495-8-bit-AVR-Microcontrollers-ATtiny441-ATtiny841_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, ADC, ACI, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny841-MM"
		(extends "ATtiny441-MM")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny841-MM"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.45mm_EP1.6x1.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8495-8-bit-AVR-Microcontrollers-ATtiny441-ATtiny841_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, ADC, ACI, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny841-SS"
		(extends "ATtiny441-SS")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny841-SS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8495-8-bit-AVR-Microcontrollers-ATtiny441-ATtiny841_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, ADC, ACI, debugWIRE, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny84A-CC"
		(extends "ATtiny24A-CC")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny84A-CC"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-15_3.0x3.0mm_Layout4x4_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, UFBGA-15"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*3.0x3.0mm*Layout4x4*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny84A-M"
		(extends "ATtiny24V-10M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny84A-M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny84A-MM"
		(extends "ATtiny24A-MM")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny84A-MM"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_3x3mm_P0.45mm_EP1.6x1.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny84A-P"
		(extends "ATtiny24V-10P")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny84A-P"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny84A-SS"
		(extends "ATtiny24V-10SS")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny84A-SS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8183.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny84V-10M"
		(extends "ATtiny24V-10M")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny84V-10M"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny84V-10P"
		(extends "ATtiny24V-10P")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny84V-10P"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-14_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, DIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny84V-10SS"
		(extends "ATtiny24V-10SS")
		(property "Reference" "U"
			(at -12.7 21.59 0)
		)
		(property "Value" "ATtiny84V-10SS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8006.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny85-20M"
		(extends "ATtiny25V-10M")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny85-20M"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny85-20P"
		(extends "ATtiny25V-10P")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny85-20P"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny85-20S"
		(extends "ATtiny25V-10S")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny85-20S"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny85V-10M"
		(extends "ATtiny25V-10M")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny85V-10M"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny85V-10P"
		(extends "ATtiny25V-10P")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny85V-10P"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny85V-10S"
		(extends "ATtiny25V-10S")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny85V-10S"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny861-20M"
		(extends "ATtiny461V-10M")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny861-20M"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2588-8-bit-avr-microcontrollers-tinyavr-attiny261-attiny461-attiny861_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny861-20P"
		(extends "ATtiny461V-10P")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny861-20P"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2588-8-bit-avr-microcontrollers-tinyavr-attiny261-attiny461-attiny861_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny861-20S"
		(extends "ATtiny461V-10S")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny861-20S"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2588-8-bit-avr-microcontrollers-tinyavr-attiny261-attiny461-attiny861_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny861A-M"
		(extends "ATtiny461V-10M")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny861A-M"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8197.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny861A-P"
		(extends "ATtiny461V-10P")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny861A-P"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8197.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny861A-S"
		(extends "ATtiny461V-10S")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny861A-S"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8197.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny861A-X"
		(extends "ATtiny261A-X")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny861A-X"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8197.pdf"
			(at 0 0 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny861V-10M"
		(extends "ATtiny461V-10M")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny861V-10M"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2588-8-bit-avr-microcontrollers-tinyavr-attiny261-attiny461-attiny861_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 512B SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny861V-10P"
		(extends "ATtiny461V-10P")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny861V-10P"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2588-8-bit-avr-microcontrollers-tinyavr-attiny261-attiny461-attiny861_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 512B SRAM, 512B EEPROM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny861V-10S"
		(extends "ATtiny461V-10S")
		(property "Reference" "U"
			(at -15.24 26.67 0)
		)
		(property "Value" "ATtiny861V-10S"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2588-8-bit-avr-microcontrollers-tinyavr-attiny261-attiny461-attiny861_datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "10MHz, 8kB Flash, 512B SRAM, 512B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny88-A"
		(extends "ATtiny48-A")
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATtiny88-A"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8008.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 8kB Flash, 512B SRAM, 64B EEPROM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny88-CC"
		(extends "ATtiny48-CC")
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATtiny88-CC"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-32_4.0x4.0mm_Layout6x6_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8008.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 8kB Flash, 512B SRAM, 64B EEPROM, UFBGA-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*4.0x4.0mm*Layout6x6*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny88-M"
		(extends "ATtiny48-M")
		(property "Reference" "U"
			(at -12.7 44.45 0)
		)
		(property "Value" "ATtiny88-M"
			(at 2.54 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8008.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 8kB Flash, 512B SRAM, 64B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny88-MM"
		(extends "ATtiny48-MM")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "ATtiny88-MM"
			(at 2.54 -39.37 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.45mm_EP2.4x2.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8008.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 8kB Flash, 512B SRAM, 64B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.45mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny88-P"
		(extends "ATtiny48-P")
		(property "Reference" "U"
			(at -12.7 39.37 0)
		)
		(property "Value" "ATtiny88-P"
			(at 2.54 -39.37 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc8008.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 8kB Flash, 512B SRAM, 64B EEPROM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny9-MA"
		(extends "ATtiny4-MA")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny9-MA"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_2x2mm_P0.5mm_EP0.9x1.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8127-AVR-8-bit-Microcontroller-ATtiny4-ATtiny5-ATtiny9-ATtiny10_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 1kB Flash, 32B SRAM, No EEPROM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*2x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATtiny9-TS"
		(extends "ATtiny4-TS")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "ATtiny9-TS"
			(at 2.54 -13.97 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-8127-AVR-8-bit-Microcontroller-ATtiny4-ATtiny5-ATtiny9-ATtiny10_Datasheet.pdf"
			(at 0 0 0)
		)
		(property "Description" "12MHz, 1kB Flash, 32B SRAM, No EEPROM, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT?23?6*"
			(at 0 0 0)
		)
	)
)
