(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AT90CAN32-16A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90CAN32-16A"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7679.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, CAN, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "AT90CAN32-16A_0_1")
		(symbol "AT90CAN32-16A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "20")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin no_connect line
				(at -12.7 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 2.54)
				(name "AGND")
				(number "63")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT90CAN32-16M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90CAN32-16M"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.5x7.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7679.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 32kB Flash, 2kB SRAM, 1kB EEPROM, JTAG, CAN, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AT90CAN32-16M_0_1")
		(symbol "AT90CAN32-16M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "20")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PG0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PG1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PG2")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PG3")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PG4")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PE0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PE1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PE2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PE3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PE4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PE5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PE6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PE7")
				(number "9")
			)
			(pin no_connect line
				(at -12.7 -45.72 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 2.54)
				(name "AGND")
				(number "63")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT90PWM1-16M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "AT90PWM1-16M"
			(at 5.08 -31.75 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.65x4.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc4378.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller LightingAVR PWM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "AT90PWM1-16M_0_1")
		(symbol "AT90PWM1-16M_1_1"
			(pin passive line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "AREF")
				(number "21")
			)
			(pin no_connect line
				(at -15.24 -10.16 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at -15.24 -12.7 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at -15.24 -15.24 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at -15.24 -17.78 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "17")
			)
			(pin no_connect line
				(at -15.24 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at -15.24 -25.4 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "25")
			)
			(pin no_connect line
				(at -15.24 -27.94 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "30")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "5")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "AVCC")
				(number "19")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "AGND")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PB0")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PB1")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB3")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB4")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB5")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB6")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB7")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PD0")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PD1")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PD2")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PD3")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PD4")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PD5")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PD6")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PD7")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "~{RESET}/PE0")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "XTAL1/PE1")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "XTAL2/PE2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT90PWM1-16S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 31.75 0)
		)
		(property "Value" "AT90PWM1-16S"
			(at 5.08 -31.75 0)
		)
		(property "Footprint" "Package_SO:SOIC-24W_7.5x15.4mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc4378.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, SOIC-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller LightingAVR PWM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x15.4mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AT90PWM1-16S_0_1")
		(symbol "AT90PWM1-16S_1_1"
			(pin passive line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "AREF")
				(number "19")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VCC")
				(number "6")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 2.54)
				(name "AVCC")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "AGND")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PB0")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PB1")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB3")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB4")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB5")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB6")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB7")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PD0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PD1")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PD2")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PD3")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PD4")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PD5")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PD6")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PD7")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "~{RESET}/PE0")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "XTAL1/PE1")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "XTAL2/PE2")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT90USB162-16A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "AT90USB162-16A"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7707.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 512B SRAM, 512B EEPROM, USB 2.0, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "AT90USB162-16A_0_1")
		(symbol "AT90USB162-16A_1_1"
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PC1/~{RESET}")
				(number "24")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "XTAL1")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0/XTAL2")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "D+")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "D-")
				(number "30")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "UCAP")
				(number "27")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "UVCC")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "UGND")
				(number "28")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB0")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PB1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB3")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB4")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB5")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB6")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB7")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PC2")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PC4")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PC5")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PC6")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PC7")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PD0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PD1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PD2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PD3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PD4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "~{HWB}/PD7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT90USB646-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90USB646-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7593.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, USB 2.0, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "AT90USB646-A_0_1")
		(symbol "AT90USB646-A_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "20")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "D+")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "D-")
				(number "4")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "UCAP")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PE0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PE1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PE2/~{HWB}")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PE3")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PE4")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PE5")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PE6")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PE7")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "UVCC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 2.54)
				(name "UGND")
				(number "6")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT90USB646-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90USB646-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.5x7.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7593.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, USB 2.0, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AT90USB646-M_0_1")
		(symbol "AT90USB646-M_1_1"
			(pin input line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "20")
			)
			(pin input line
				(at -15.24 38.1 0)
				(length 2.54)
				(name "XTAL1")
				(number "24")
			)
			(pin output line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "XTAL2")
				(number "23")
			)
			(pin passive line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "AREF")
				(number "62")
			)
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "VBUS")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "D+")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "D-")
				(number "4")
			)
			(pin passive line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "UCAP")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PE0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PE1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PE2/~{HWB}")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PE3")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PE4")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PE5")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PE6")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PE7")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PF0")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PF1")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PF2")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PF3")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PF4")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "PF5")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "PF6")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "PF7")
				(number "54")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "UVCC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 2.54)
				(name "UGND")
				(number "6")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VCC")
				(number "21")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "53")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "AVCC")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "51")
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "PD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT90USB82-16M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "AT90USB82-16M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7707.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 8kB Flash, 512B SRAM, 512B EEPROM, USB 2.0, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AT90USB82-16M_0_1")
		(symbol "AT90USB82-16M_1_1"
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PC1/~{RESET}")
				(number "24")
			)
			(pin input line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "XTAL1")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PC0/XTAL2")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "D+")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "D-")
				(number "30")
			)
			(pin passive line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "UCAP")
				(number "27")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "UVCC")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "UGND")
				(number "28")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VCC")
				(number "4")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "AVCC")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB0")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PB1")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PB2")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB3")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB4")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB5")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB6")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB7")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PC2")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PC4")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PC5")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PC6")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PC7")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PD0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PD1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PD2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PD3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PD4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "~{HWB}/PD7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AT90CAN128-16A"
		(extends "AT90CAN32-16A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90CAN128-16A"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7679.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 128kB Flash, 4kB SRAM, 4kB EEPROM, JTAG, CAN, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT90CAN128-16M"
		(extends "AT90CAN32-16M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90CAN128-16M"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.5x7.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7679.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 128kB Flash, 4kB SRAM, 4kB EEPROM, JTAG, CAN, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT90CAN64-16A"
		(extends "AT90CAN32-16A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90CAN64-16A"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7679.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, CAN, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT90CAN64-16M"
		(extends "AT90CAN32-16M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90CAN64-16M"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.5x7.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7679.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, JTAG, CAN, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller MegaAVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT90USB1286-A"
		(extends "AT90USB646-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90USB1286-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7593.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 128kB Flash, 8kB SRAM, 4kB EEPROM, USB 2.0, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT90USB1286-M"
		(extends "AT90USB646-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90USB1286-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.5x7.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7593.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 128kB Flash, 8kB SRAM, 4kB EEPROM, USB 2.0, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT90USB1287-A"
		(extends "AT90USB646-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90USB1287-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7593.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 128kB Flash, 8kB SRAM, 4kB EEPROM, USB 2.0 OTG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT90USB1287-M"
		(extends "AT90USB646-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90USB1287-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.5x7.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7593.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 128kB Flash, 8kB SRAM, 4kB EEPROM, USB 2.0 OTG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT90USB162-16M"
		(extends "AT90USB82-16M")
		(property "Reference" "U"
			(at -15.24 34.29 0)
		)
		(property "Value" "AT90USB162-16M"
			(at 2.54 -34.29 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7707.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 16kB Flash, 512B SRAM, 512B EEPROM, USB 2.0, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT90USB647-A"
		(extends "AT90USB646-A")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90USB647-A"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7593.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, USB 2.0 OTG, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "AT90USB647-M"
		(extends "AT90USB646-M")
		(property "Reference" "U"
			(at -12.7 49.53 0)
		)
		(property "Value" "AT90USB647-M"
			(at 2.54 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.5x7.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/doc7593.pdf"
			(at 0 0 0)
		)
		(property "Description" "16MHz, 64kB Flash, 4kB SRAM, 2kB EEPROM, USB 2.0 OTG, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
