(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "AVR32DA28x-xSO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "AVR32DA28x-xSO"
			(at 2.54 -24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DA28-32-48-Data-Sheet-40002228B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Touch Sensing, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AVR32DA28x-xSO_0_1")
		(symbol "AVR32DA28x-xSO_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "UPDI")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "~{RESET}/PF6")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PD0")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD1")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD2")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD3")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD4")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "VREFA/PD7")
				(number "13")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "AVDD")
				(number "14")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA0")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA1")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA2")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA3")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA4")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA5")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA6")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA7")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PC0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PC1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PC2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PC3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR32DA32x-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 29.21 0)
		)
		(property "Value" "AVR32DA32x-xPT"
			(at 2.54 -29.21 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DA28-32-48-Data-Sheet-40002228B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Touch Sensing, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "AVR32DA32x-xPT_0_1")
		(symbol "AVR32DA32x-xPT_1_1"
			(pin input line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "UPDI")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PF2")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PF3")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PF4")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PF5")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "~{RESET}/PF6")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD0")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD1")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD2")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PD3")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PD4")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PD5")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PD6")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "VREFA/PD7")
				(number "17")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "AVDD")
				(number "18")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PC0")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PC1")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PC2")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PC3")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR32DA32x-xRXB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 29.21 0)
		)
		(property "Value" "AVR32DA32x-xRXB"
			(at 2.54 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DA28-32-48-Data-Sheet-40002228B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Touch Sensing, VQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*EP3.1x3.1mm*"
			(at 0 0 0)
		)
		(symbol "AVR32DA32x-xRXB_0_1")
		(symbol "AVR32DA32x-xRXB_1_1"
			(pin input line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "UPDI")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PF2")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PF3")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PF4")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PF5")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "~{RESET}/PF6")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD0")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD1")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD2")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PD3")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PD4")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PD5")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PD6")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "VREFA/PD7")
				(number "17")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "AVDD")
				(number "18")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA0")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA1")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA2")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PC0")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PC1")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PC2")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PC3")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR32DA48x-x6LX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "AVR32DA48x-x6LX"
			(at 5.08 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.2x4.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DA28-32-48-Data-Sheet-40002228B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Touch Sensing, VQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.4mm*EP4.2x4.2mm*"
			(at 0 0 0)
		)
		(symbol "AVR32DA48x-x6LX_0_1")
		(symbol "AVR32DA48x-x6LX_1_1"
			(pin input line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "UPDI")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PF3")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PF4")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PF5")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "~{RESET}/PF6")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PE2")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "VREFA/PD7")
				(number "27")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "AVDD")
				(number "28")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "42")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "45")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PC0")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PC1")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PC2")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PC4")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PC5")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PC6")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PC7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR32DA48x-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "AVR32DA48x-xPT"
			(at 5.08 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DA28-32-48-Data-Sheet-40002228B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Touch Sensing, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AVR32DA48x-xPT_0_1")
		(symbol "AVR32DA48x-xPT_1_1"
			(pin input line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "UPDI")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PF3")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PF4")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PF5")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "~{RESET}/PF6")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PE2")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "VREFA/PD7")
				(number "27")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "AVDD")
				(number "28")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "14")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "42")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "PA0")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "PA1")
				(number "45")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PC0")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PC1")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PC2")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PC4")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PC5")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PC6")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PC7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR32DB28x-xSO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 21.59 0)
		)
		(property "Value" "AVR32DB28x-xSO"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DB28-32-48-DataSheet-DS40002301A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "AVR32DB28x-xSO_0_1")
		(symbol "AVR32DB28x-xSO_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "UPDI")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "~{RESET}/PF6")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PD1")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PD2")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD3")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD4")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PD5")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PD6")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "VREFA/PD7")
				(number "13")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 2.54)
				(name "AVDD")
				(number "14")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 2.54)
				(name "AGND")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDIO2")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "XTALHF1/PA0")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "XTALHF2/PA1")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA2")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA3")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA4")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA5")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PA6")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PA7")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PC0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PC1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PC2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PC3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR32DB32x-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 26.67 0)
		)
		(property "Value" "AVR32DB32x-xPT"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DB28-32-48-DataSheet-DS40002301A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "AVR32DB32x-xPT_0_1")
		(symbol "AVR32DB32x-xPT_1_1"
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "UPDI")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "25")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "~{RESET}/PF6")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD1")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD2")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PD3")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PD4")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PD5")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PD6")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "VREFA/PD7")
				(number "17")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "AVDD")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "19")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDIO2")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "XTALHF1/PA0")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "XTALHF2/PA1")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR32DB32x-xRXB"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 26.67 0)
		)
		(property "Value" "AVR32DB32x-xRXB"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DB28-32-48-DataSheet-DS40002301A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, VQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*EP3.1x3.1mm*"
			(at 0 0 0)
		)
		(symbol "AVR32DB32x-xRXB_0_1")
		(symbol "AVR32DB32x-xRXB_1_1"
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "UPDI")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "25")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "~{RESET}/PF6")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "PD1")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD2")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PD3")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PD4")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PD5")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PD6")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "VREFA/PD7")
				(number "17")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 2.54)
				(name "AVDD")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "AGND")
				(number "19")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 2.54)
				(name "VDDIO2")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "XTALHF1/PA0")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "XTALHF2/PA1")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA2")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR32DB48x-x6LX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "AVR32DB48x-x6LX"
			(at 5.08 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.2x4.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DB28-32-48-DataSheet-DS40002301A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, VQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.4mm*EP4.2x4.2mm*"
			(at 0 0 0)
		)
		(symbol "AVR32DB48x-x6LX_0_1")
		(symbol "AVR32DB48x-x6LX_1_1"
			(pin input line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "UPDI")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PF3")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PF4")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PF5")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "~{RESET}/PF6")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PE2")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "VREFA/PD7")
				(number "27")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "AVDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "AGND")
				(number "29")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "42")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDIO2")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "XTALHF1/PA0")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "XTALHF2/PA1")
				(number "45")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PC0")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PC1")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PC2")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PC4")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PC5")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PC6")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PC7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR32DB48x-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "AVR32DB48x-xPT"
			(at 5.08 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DB28-32-48-DataSheet-DS40002301A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AVR32DB48x-xPT_0_1")
		(symbol "AVR32DB48x-xPT_1_1"
			(pin input line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "UPDI")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "PF2")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "PF3")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "PF4")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "PF5")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "~{RESET}/PF6")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "PE0")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PE1")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "PE2")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "PE3")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "PD0")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "PD1")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "PD2")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PD5")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "PD6")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "VREFA/PD7")
				(number "27")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "AVDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "AGND")
				(number "29")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "42")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDDIO2")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "XTALHF1/PA0")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "XTALHF2/PA1")
				(number "45")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "PA2")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "PA3")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "PA4")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "PA5")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "PA6")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "PA7")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PB0")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PB1")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PB2")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "PB3")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PB4")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "PB5")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "PC0")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "PC1")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "PC2")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "PC3")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "PC4")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "PC5")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "PC6")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "PC7")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR64DA64x-xMR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 49.53 0)
		)
		(property "Value" "AVR64DA64x-xMR"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DA28-32-48-64-Data-Sheet-40002233B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Touch Sensing, VQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*9x9mm*P0.5mm*EP7.15x7.15mm*"
			(at 0 0 0)
		)
		(symbol "AVR64DA64x-xMR_0_1")
		(symbol "AVR64DA64x-xMR_1_1"
			(pin input line
				(at -22.86 43.18 0)
				(length 2.54)
				(name "UPDI")
				(number "51")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "PG0")
				(number "52")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "PG1")
				(number "53")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "PG2")
				(number "54")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "PG3")
				(number "55")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "PG4")
				(number "58")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "PG5")
				(number "59")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PG6")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PG7")
				(number "61")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "46")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "47")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "48")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "49")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "~{RESET}/PF6_")
				(number "50")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PE6")
				(number "42")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PE7")
				(number "43")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "AVDD")
				(number "34")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "20")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "56")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 2.54)
				(name "VREFA/PD7")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR64DA64x-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 49.53 0)
		)
		(property "Value" "AVR64DA64x-xPT"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DA28-32-48-64-Data-Sheet-40002233B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Touch Sensing, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AVR64DA64x-xPT_0_1")
		(symbol "AVR64DA64x-xPT_1_1"
			(pin input line
				(at -22.86 43.18 0)
				(length 2.54)
				(name "UPDI")
				(number "51")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "PG0")
				(number "52")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "PG1")
				(number "53")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "PG2")
				(number "54")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "PG3")
				(number "55")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "PG4")
				(number "58")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "PG5")
				(number "59")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PG6")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PG7")
				(number "61")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "46")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "47")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "48")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "49")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "~{RESET}/PF6_")
				(number "50")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PE6")
				(number "42")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PE7")
				(number "43")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "AVDD")
				(number "34")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "20")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "56")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 2.54)
				(name "PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 2.54)
				(name "VREFA/PD7")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR64DB64x-xMR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 49.53 0)
		)
		(property "Value" "AVR64DB64x-xMR"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DB28-32-48-64-DataSheet-DS40002300A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, VQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*9x9mm*P0.5mm*EP7.15x7.15mm*"
			(at 0 0 0)
		)
		(symbol "AVR64DB64x-xMR_0_1")
		(symbol "AVR64DB64x-xMR_1_1"
			(pin input line
				(at -22.86 43.18 0)
				(length 2.54)
				(name "UPDI")
				(number "51")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "PG0")
				(number "52")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "PG1")
				(number "53")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "PG2")
				(number "54")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "PG3")
				(number "55")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "PG4")
				(number "58")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "PG5")
				(number "59")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PG6")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PG7")
				(number "61")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "46")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "47")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "48")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "49")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "~{RESET}/PF6")
				(number "50")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PE6")
				(number "42")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PE7")
				(number "43")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "AVDD")
				(number "34")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 2.54)
				(name "AGND")
				(number "35")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "56")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "VDDIO2")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 2.54)
				(name "XTALHF1/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "XTALHF2/PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 2.54)
				(name "VREFA/PD7")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR64DB64x-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 49.53 0)
		)
		(property "Value" "AVR64DB64x-xPT"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DB28-32-48-64-DataSheet-DS40002300A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "AVR64DB64x-xPT_0_1")
		(symbol "AVR64DB64x-xPT_1_1"
			(pin input line
				(at -22.86 43.18 0)
				(length 2.54)
				(name "UPDI")
				(number "51")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 2.54)
				(name "PG0")
				(number "52")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "PG1")
				(number "53")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "PG2")
				(number "54")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "PG3")
				(number "55")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "PG4")
				(number "58")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "PG5")
				(number "59")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PG6")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PG7")
				(number "61")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "XTAL32K1/PF0")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "XTAL32K2/PF1")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PF2")
				(number "46")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PF3")
				(number "47")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PF4")
				(number "48")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PF5")
				(number "49")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "~{RESET}/PF6")
				(number "50")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PE0")
				(number "36")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PE1")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PE2")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PE3")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PE4")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PE5")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PE6")
				(number "42")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PE7")
				(number "43")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "AVDD")
				(number "34")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 2.54)
				(name "AGND")
				(number "35")
			)
			(pin passive line
				(at 0 50.8 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "56")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 2.54)
				(name "VDD")
				(number "6")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 2.54)
				(name "VDDIO2")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 2.54)
				(name "XTALHF1/PA0")
				(number "62")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 2.54)
				(name "XTALHF2/PA1")
				(number "63")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PA2")
				(number "64")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PA3")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PA4")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PA5")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PA6")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PA7")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PB0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PB1")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PB3")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PB4")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PB5")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PB6")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PB7")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PC0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PC1")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PC2")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PC3")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PC4")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PC5")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PC6")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PC7")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PD0")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PD1")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 2.54)
				(name "PD2")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 2.54)
				(name "PD3")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "PD4")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 2.54)
				(name "PD5")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 2.54)
				(name "PD6")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 2.54)
				(name "VREFA/PD7")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "AVR128DA28x-xSO"
		(extends "AVR32DA28x-xSO")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "AVR128DA28x-xSO"
			(at 2.54 -24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DA28-32-48-64-DataSheet-DS40002183B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Touch Sensing, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DA28x-xSP"
		(extends "AVR32DA28x-xSO")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "AVR128DA28x-xSP"
			(at 2.54 -24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DA28-32-48-64-DataSheet-DS40002183B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Touch Sensing, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DA28x-xSS"
		(extends "AVR32DA28x-xSO")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "AVR128DA28x-xSS"
			(at 2.54 -24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DA28-32-48-64-DataSheet-DS40002183B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Touch Sensing, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DA32x-xPT"
		(extends "AVR32DA32x-xPT")
		(property "Reference" "U"
			(at -17.78 29.21 0)
		)
		(property "Value" "AVR128DA32x-xPT"
			(at 2.54 -29.21 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DA28-32-48-64-DataSheet-DS40002183B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Touch Sensing, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DA32x-xRXB"
		(extends "AVR32DA32x-xRXB")
		(property "Reference" "U"
			(at -17.78 29.21 0)
		)
		(property "Value" "AVR128DA32x-xRXB"
			(at 2.54 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DA28-32-48-64-DataSheet-DS40002183B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Touch Sensing, VQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*EP3.1x3.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DA48x-x6LX"
		(extends "AVR32DA48x-x6LX")
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "AVR128DA48x-x6LX"
			(at 5.08 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.2x4.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DA28-32-48-64-DataSheet-DS40002183B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Touch Sensing, VQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.4mm*EP4.2x4.2mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DA48x-xPT"
		(extends "AVR32DA48x-xPT")
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "AVR128DA48x-xPT"
			(at 5.08 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DA28-32-48-64-DataSheet-DS40002183B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Touch Sensing, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DA64x-xMR"
		(extends "AVR64DA64x-xMR")
		(property "Reference" "U"
			(at -20.32 49.53 0)
		)
		(property "Value" "AVR128DA64x-xMR"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DA28-32-48-64-DataSheet-DS40002183B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Touch Sensing, VQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*9x9mm*P0.5mm*EP7.15x7.15mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DA64x-xPT"
		(extends "AVR64DA64x-xPT")
		(property "Reference" "U"
			(at -20.32 49.53 0)
		)
		(property "Value" "AVR128DA64x-xPT"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DA28-32-48-64-DataSheet-DS40002183B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Touch Sensing, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DB28x-xSO"
		(extends "AVR32DB28x-xSO")
		(property "Reference" "U"
			(at -17.78 21.59 0)
		)
		(property "Value" "AVR128DB28x-xSO"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DB28-32-48-64-DataSheet-DS40002247A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DB28x-xSP"
		(extends "AVR32DB28x-xSO")
		(property "Reference" "U"
			(at -17.78 21.59 0)
		)
		(property "Value" "AVR128DB28x-xSP"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DB28-32-48-64-DataSheet-DS40002247A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DB28x-xSS"
		(extends "AVR32DB28x-xSO")
		(property "Reference" "U"
			(at -17.78 21.59 0)
		)
		(property "Value" "AVR128DB28x-xSS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DB28-32-48-64-DataSheet-DS40002247A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DB32x-xPT"
		(extends "AVR32DB32x-xPT")
		(property "Reference" "U"
			(at -17.78 26.67 0)
		)
		(property "Value" "AVR128DB32x-xPT"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DB28-32-48-64-DataSheet-DS40002247A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DB32x-xRXB"
		(extends "AVR32DB32x-xRXB")
		(property "Reference" "U"
			(at -17.78 26.67 0)
		)
		(property "Value" "AVR128DB32x-xRXB"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DB28-32-48-64-DataSheet-DS40002247A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, VQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*EP3.1x3.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DB48x-x6LX"
		(extends "AVR32DB48x-x6LX")
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "AVR128DB48x-x6LX"
			(at 5.08 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.2x4.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DB28-32-48-64-DataSheet-DS40002247A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, VQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.4mm*EP4.2x4.2mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DB48x-xPT"
		(extends "AVR32DB48x-xPT")
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "AVR128DB48x-xPT"
			(at 5.08 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DB28-32-48-64-DataSheet-DS40002247A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DB64x-xMR"
		(extends "AVR64DB64x-xMR")
		(property "Reference" "U"
			(at -20.32 49.53 0)
		)
		(property "Value" "AVR128DB64x-xMR"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DB28-32-48-64-DataSheet-DS40002247A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, VQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*1EP*9x9mm*P0.5mm*EP7.15x7.15mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR128DB64x-xPT"
		(extends "AVR64DB64x-xPT")
		(property "Reference" "U"
			(at -20.32 49.53 0)
		)
		(property "Value" "AVR128DB64x-xPT"
			(at 5.08 -49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DB28-32-48-64-DataSheet-DS40002247A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR32DA28x-xSP"
		(extends "AVR32DA28x-xSO")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "AVR32DA28x-xSP"
			(at 2.54 -24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DA28-32-48-Data-Sheet-40002228B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Touch Sensing, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR32DA28x-xSS"
		(extends "AVR32DA28x-xSO")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "AVR32DA28x-xSS"
			(at 2.54 -24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DA28-32-48-Data-Sheet-40002228B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Touch Sensing, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR32DB28x-xSP"
		(extends "AVR32DB28x-xSO")
		(property "Reference" "U"
			(at -17.78 21.59 0)
		)
		(property "Value" "AVR32DB28x-xSP"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DB28-32-48-DataSheet-DS40002301A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR32DB28x-xSS"
		(extends "AVR32DB28x-xSO")
		(property "Reference" "U"
			(at -17.78 21.59 0)
		)
		(property "Value" "AVR32DB28x-xSS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR32DB28-32-48-DataSheet-DS40002301A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 32kB Flash, 4kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DA28x-xSO"
		(extends "AVR32DA28x-xSO")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "AVR64DA28x-xSO"
			(at 2.54 -24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DA28-32-48-64-Data-Sheet-40002233B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Touch Sensing, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DA28x-xSP"
		(extends "AVR32DA28x-xSO")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "AVR64DA28x-xSP"
			(at 2.54 -24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DA28-32-48-64-Data-Sheet-40002233B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Touch Sensing, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DA28x-xSS"
		(extends "AVR32DA28x-xSO")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "AVR64DA28x-xSS"
			(at 2.54 -24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DA28-32-48-64-Data-Sheet-40002233B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Touch Sensing, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DA32x-xPT"
		(extends "AVR32DA32x-xPT")
		(property "Reference" "U"
			(at -17.78 29.21 0)
		)
		(property "Value" "AVR64DA32x-xPT"
			(at 2.54 -29.21 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DA28-32-48-64-Data-Sheet-40002233B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Touch Sensing, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DA32x-xRXB"
		(extends "AVR32DA32x-xRXB")
		(property "Reference" "U"
			(at -17.78 29.21 0)
		)
		(property "Value" "AVR64DA32x-xRXB"
			(at 2.54 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DA28-32-48-64-Data-Sheet-40002233B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Touch Sensing, VQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*EP3.1x3.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DA48x-x6LX"
		(extends "AVR32DA48x-x6LX")
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "AVR64DA48x-x6LX"
			(at 5.08 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.2x4.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DA28-32-48-64-Data-Sheet-40002233B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Touch Sensing, VQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.4mm*EP4.2x4.2mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DA48x-xPT"
		(extends "AVR32DA48x-xPT")
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "AVR64DA48x-xPT"
			(at 5.08 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DA28-32-48-64-Data-Sheet-40002233B.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Touch Sensing, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DB28x-xSO"
		(extends "AVR32DB28x-xSO")
		(property "Reference" "U"
			(at -17.78 21.59 0)
		)
		(property "Value" "AVR64DB28x-xSO"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DB28-32-48-64-DataSheet-DS40002300A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DB28x-xSP"
		(extends "AVR32DB28x-xSO")
		(property "Reference" "U"
			(at -17.78 21.59 0)
		)
		(property "Value" "AVR64DB28x-xSP"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DB28-32-48-64-DataSheet-DS40002300A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DB28x-xSS"
		(extends "AVR32DB28x-xSO")
		(property "Reference" "U"
			(at -17.78 21.59 0)
		)
		(property "Value" "AVR64DB28x-xSS"
			(at 2.54 -21.59 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DB28-32-48-64-DataSheet-DS40002300A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DB32x-xPT"
		(extends "AVR32DB32x-xPT")
		(property "Reference" "U"
			(at -17.78 26.67 0)
		)
		(property "Value" "AVR64DB32x-xPT"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DB28-32-48-64-DataSheet-DS40002300A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DB32x-xRXB"
		(extends "AVR32DB32x-xRXB")
		(property "Reference" "U"
			(at -17.78 26.67 0)
		)
		(property "Value" "AVR64DB32x-xRXB"
			(at 2.54 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.1x3.1mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DB28-32-48-64-DataSheet-DS40002300A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, VQFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*EP3.1x3.1mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DB48x-x6LX"
		(extends "AVR32DB48x-x6LX")
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "AVR64DB48x-x6LX"
			(at 5.08 -36.83 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.2x4.2mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DB28-32-48-64-DataSheet-DS40002300A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, VQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.4mm*EP4.2x4.2mm*"
			(at 0 0 0)
		)
	)
	(symbol "AVR64DB48x-xPT"
		(extends "AVR32DB48x-xPT")
		(property "Reference" "U"
			(at -17.78 36.83 0)
		)
		(property "Value" "AVR64DB48x-xPT"
			(at 5.08 -36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR64DB28-32-48-64-DataSheet-DS40002300A.pdf"
			(at 0 0 0)
		)
		(property "Description" "24MHz, 64kB Flash, 8kB SRAM, EEPROM with Op Amps and Multi-Voltage I/O, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "AVR 8bit Microcontroller AVR-DB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
