(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "PIC10F200-IMC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F200-IMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41239D.pdf"
			(at 0 0 0)
		)
		(property "Description" "256W Flash, 16B SRAM, DFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*8*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC10F200-IMC_0_1")
		(symbol "PIC10F200-IMC_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP1")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC10F200-IOT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F200-IOT"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41239D.pdf"
			(at 0 0 0)
		)
		(property "Description" "256W Flash, 16B SRAM, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*6*"
			(at 0 0 0)
		)
		(symbol "PIC10F200-IOT_0_1")
		(symbol "PIC10F200-IOT_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP1")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC10F200-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F200-IP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41239D.pdf"
			(at 0 0 0)
		)
		(property "Description" "256W Flash, 16B SRAM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*8*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC10F200-IP_0_1")
		(symbol "PIC10F200-IP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP1")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC10F204-IMC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F204-IMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41239D.pdf"
			(at 0 0 0)
		)
		(property "Description" "256W Flash, 16B SRAM, DFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*8*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC10F204-IMC_0_1")
		(symbol "PIC10F204-IMC_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP1")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC10F204-IOT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F204-IOT"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41239D.pdf"
			(at 0 0 0)
		)
		(property "Description" "256W Flash, 16B SRAM, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*6*"
			(at 0 0 0)
		)
		(symbol "PIC10F204-IOT_0_1")
		(symbol "PIC10F204-IOT_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP1")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC10F204-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F204-IP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41239D.pdf"
			(at 0 0 0)
		)
		(property "Description" "256W Flash, 16B SRAM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*8*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC10F204-IP_0_1")
		(symbol "PIC10F204-IP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP1")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC10F220-IMC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F220-IMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41270E.pdf"
			(at 0 0 0)
		)
		(property "Description" "256W Flash, 16B SRAM, DFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*8*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC10F220-IMC_0_1")
		(symbol "PIC10F220-IMC_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP1")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC10F220-IOT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F220-IOT"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41270E.pdf"
			(at 0 0 0)
		)
		(property "Description" "256W Flash, 16B SRAM, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*6*"
			(at 0 0 0)
		)
		(symbol "PIC10F220-IOT_0_1")
		(symbol "PIC10F220-IOT_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP1")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC10F220-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F220-IP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41270E.pdf"
			(at 0 0 0)
		)
		(property "Description" "256W Flash, 16B SRAM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*8*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC10F220-IP_0_1")
		(symbol "PIC10F220-IP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP1")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC10F320-IMC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F320-IMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41585A.pdf"
			(at 0 0 0)
		)
		(property "Description" "256W Flash, 64B SRAM, DFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*8*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC10F320-IMC_0_1")
		(symbol "PIC10F320-IMC_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "RA0")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "RA1")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "RA3")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "RA2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC10F320-IOT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F320-IOT"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41585A.pdf"
			(at 0 0 0)
		)
		(property "Description" "256W Flash, 64B SRAM, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*6*"
			(at 0 0 0)
		)
		(symbol "PIC10F320-IOT_0_1")
		(symbol "PIC10F320-IOT_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "RA0")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "RA1")
				(number "3")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "RA3")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "RA2")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC10F320-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F320-IP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41585A.pdf"
			(at 0 0 0)
		)
		(property "Description" "256W Flash, 64B SRAM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*8*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC10F320-IP_0_1")
		(symbol "PIC10F320-IP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "RA0")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "RA1")
				(number "4")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "7")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "RA3")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "RA2")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC10F202-IMC"
		(extends "PIC10F200-IMC")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F202-IMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41239D.pdf"
			(at 0 0 0)
		)
		(property "Description" "512W Flash, 24B SRAM, DFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*8*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC10F202-IOT"
		(extends "PIC10F200-IOT")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F202-IOT"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41239D.pdf"
			(at 0 0 0)
		)
		(property "Description" "512W Flash, 24B SRAM, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*6*"
			(at 0 0 0)
		)
	)
	(symbol "PIC10F202-IP"
		(extends "PIC10F200-IP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F202-IP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41239D.pdf"
			(at 0 0 0)
		)
		(property "Description" "512W Flash, 24B SRAM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*8*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC10F206-IMC"
		(extends "PIC10F204-IMC")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F206-IMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41239D.pdf"
			(at 0 0 0)
		)
		(property "Description" "512W Flash, 24B SRAM, DFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*8*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC10F206-IOT"
		(extends "PIC10F204-IOT")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F206-IOT"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41239D.pdf"
			(at 0 0 0)
		)
		(property "Description" "512W Flash, 24B SRAM, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*6*"
			(at 0 0 0)
		)
	)
	(symbol "PIC10F206-IP"
		(extends "PIC10F204-IP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F206-IP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41239D.pdf"
			(at 0 0 0)
		)
		(property "Description" "512W Flash, 24B SRAM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*8*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC10F222-IMC"
		(extends "PIC10F220-IMC")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F222-IMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41270E.pdf"
			(at 0 0 0)
		)
		(property "Description" "512W Flash, 24B SRAM, DFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*8*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC10F222-IOT"
		(extends "PIC10F220-IOT")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F222-IOT"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41270E.pdf"
			(at 0 0 0)
		)
		(property "Description" "512W Flash, 24B SRAM, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*6*"
			(at 0 0 0)
		)
	)
	(symbol "PIC10F222-IP"
		(extends "PIC10F220-IP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F222-IP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41270E.pdf"
			(at 0 0 0)
		)
		(property "Description" "512W Flash, 24B SRAM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*8*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC10F322-IMC"
		(extends "PIC10F320-IMC")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F322-IMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41585A.pdf"
			(at 0 0 0)
		)
		(property "Description" "512W Flash, 64B SRAM, DFN8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*8*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC10F322-IOT"
		(extends "PIC10F320-IOT")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F322-IOT"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41585A.pdf"
			(at 0 0 0)
		)
		(property "Description" "512W Flash, 64B SRAM, SOT-23-6"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOT*23*6*"
			(at 0 0 0)
		)
	)
	(symbol "PIC10F322-IP"
		(extends "PIC10F320-IP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC10F322-IP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 16.51 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41585A.pdf"
			(at 0 0 0)
		)
		(property "Description" "512W Flash, 64B SRAM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*8*W7.62mm*"
			(at 0 0 0)
		)
	)
)
