(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "PIC12C508-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C508-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "512W EPROM, 25B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12C508-xP_0_1")
		(symbol "PIC12C508-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12C508A-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C508A-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "512W EPROM, 25B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12C508A-xP_0_1")
		(symbol "PIC12C508A-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12C509-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C509-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W EPROM, 41B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12C509-xP_0_1")
		(symbol "PIC12C509-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12C509A-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C509A-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C509, 1024W EPROM, 41B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12C509A-xP_0_1")
		(symbol "PIC12C509A-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12C671-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C671-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/30561b.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W EPROM, 128B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12C671-xP_0_1")
		(symbol "PIC12C671-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12C672-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C672-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/30561b.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "2048W EPROM, 128B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12C672-xP_0_1")
		(symbol "PIC12C672-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12CE518-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CE518-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "512W EPROM, 25B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12CE518-xP_0_1")
		(symbol "PIC12CE518-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12CE519-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CE519-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W EPROM, 41B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12CE519-xP_0_1")
		(symbol "PIC12CE519-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12CE673-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CE673-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/30561b.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W EPROM, 128B SRAM, 128B EPROM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12CE673-xP_0_1")
		(symbol "PIC12CE673-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12CE674-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CE674-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/30561b.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "2048W EPROM, 128B SRAM, 128B EPROM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12CE674-xP_0_1")
		(symbol "PIC12CE674-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12CR509A-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CR509A-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W ROM, 41B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12CR509A-xP_0_1")
		(symbol "PIC12CR509A-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F1501-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F1501-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41615A.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W FLASH, 64B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F1501-xP_0_1")
		(symbol "PIC12F1501-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "RA0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "RA1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "RA2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "RA5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F1822-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F1822-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41413B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "2kW FLASH, 128B SRAM, 256 EEPROM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F1822-xP_0_1")
		(symbol "PIC12F1822-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "RA0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "RA1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "RA2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "RA5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F1840-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F1840-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41441B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "4kW FLASH, 256B SRAM, 256B EEPROM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F1840-xP_0_1")
		(symbol "PIC12F1840-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "RA0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "RA1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "RA2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "RA5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F508-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F508-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "512W Flash, 25B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F508-xP_0_1")
		(symbol "PIC12F508-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F509-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F509-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 41B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F509-xP_0_1")
		(symbol "PIC12F509-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F510-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F510-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41268D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W FLASH, 38B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F510-xP_0_1")
		(symbol "PIC12F510-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F519-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F519-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41319B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 41B SRAM, 64B EEPROM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F519-xP_0_1")
		(symbol "PIC12F519-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F609-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F609-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 64B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F609-xP_0_1")
		(symbol "PIC12F609-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F615-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F615-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 64B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F615-xP_0_1")
		(symbol "PIC12F615-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F617-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F617-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "2048W Flash, 128B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F617-xP_0_1")
		(symbol "PIC12F617-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F629-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F629-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41190G.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 64B SRAM, 128B EEPROM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F629-xP_0_1")
		(symbol "PIC12F629-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F635-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F635-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41232D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 64B SRAM, 128B EEPROM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F635-xP_0_1")
		(symbol "PIC12F635-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F675-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F675-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41190G.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 64B SRAM, 128B EEPROM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F675-xP_0_1")
		(symbol "PIC12F675-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F683-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F683-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41232D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "2048W Flash, 128B SRAM, 256B EEPROM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F683-xP_0_1")
		(symbol "PIC12F683-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12F752-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F752-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41576B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 64B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12F752-xP_0_1")
		(symbol "PIC12F752-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12HV609-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12HV609-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 64B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12HV609-xP_0_1")
		(symbol "PIC12HV609-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12HV615-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12HV615-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 64B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12HV615-xP_0_1")
		(symbol "PIC12HV615-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12HV752-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12HV752-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41576B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 64B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC12HV752-xP_0_1")
		(symbol "PIC12HV752-xP_1_1"
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 5.08)
				(name "GP0")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 5.08)
				(name "GP1")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 5.08)
				(name "GP2")
				(number "5")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin input line
				(at 15.24 2.54 180)
				(length 5.08)
				(name "GP3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 5.08)
				(name "GP4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 5.08)
				(name "GP5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12LF1840T48-xST"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 16.51 0)
		)
		(property "Value" "PIC12LF1840T48-xST"
			(at 1.27 13.97 0)
		)
		(property "Footprint" "Package_SO:TSSOP-14_4.4x5mm_P0.65mm"
			(at 1.27 -13.97 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/40001594C.pdf"
			(at 1.27 -16.51 0)
		)
		(property "Description" "PIC12LF1840T48, 4kW FLASH, 256B SRAM, 256B EEPROM, RF, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP RF Transmitter"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC12LF1840T48-xST_0_1")
		(symbol "PIC12LF1840T48-xST_1_1"
			(pin power_in line
				(at -17.78 7.62 0)
				(length 5.08)
				(name "VDDRF")
				(number "5")
			)
			(pin input line
				(at -17.78 5.08 0)
				(length 5.08)
				(name "CTRL")
				(number "6")
			)
			(pin input line
				(at -17.78 2.54 0)
				(length 5.08)
				(name "DATA")
				(number "9")
			)
			(pin input line
				(at -17.78 -2.54 0)
				(length 5.08)
				(name "XTAL")
				(number "10")
			)
			(pin input line
				(at -17.78 -5.08 0)
				(length 5.08)
				(name "RFOUT")
				(number "7")
			)
			(pin power_in line
				(at -17.78 -7.62 0)
				(length 5.08)
				(name "VSSRF")
				(number "8")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 5.08)
				(name "RA0")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 5.08)
				(name "RA1")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 5.08)
				(name "RA2")
				(number "11")
			)
			(pin input line
				(at 17.78 0 180)
				(length 5.08)
				(name "RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 5.08)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 5.08)
				(name "RA5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC12C508-xJW"
		(extends "PIC12C508-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C508-xJW"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:CERDIP-8_W7.62mm_SideBrazed"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C508, 512W EPROM, 25B SRAM, CERDIP-8 Windowed"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CERDIP*7.62mm*SideBrazed*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12C508-xSM"
		(extends "PIC12C508-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C508-xSM"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C508, 512W EPROM, 25B SRAM, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12C508A-xJW"
		(extends "PIC12C508A-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C508A-xJW"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:CERDIP-8_W7.62mm_SideBrazed"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C508A, 512W EPROM, 25B SRAM, CERDIP-8 Windowed"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CERDIP*7.62mm*SideBrazed*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12C508A-xSM"
		(extends "PIC12C508A-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C508A-xSM"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C508A, 512W EPROM, 25B SRAM, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12C508A-xSN"
		(extends "PIC12C508A-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C508A-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C508A, 512W EPROM, 25B SRAM, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12C509-xJW"
		(extends "PIC12C509-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C509-xJW"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:CERDIP-8_W7.62mm_SideBrazed"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C509, 1024W EPROM, 41B SRAM, CERDIP-8 Windowed"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CERDIP*7.62mm*SideBrazed*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12C509-xSM"
		(extends "PIC12C509-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C509-xSM"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C509, 1024W EPROM, 41B SRAM, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12C509A-xJW"
		(extends "PIC12C509A-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C509A-xJW"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:CERDIP-8_W7.62mm_SideBrazed"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C509A, 1024W EPROM, 41B SRAM, CERDIP-8 Windowed"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CERDIP*7.62mm*SideBrazed*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12C509A-xSM"
		(extends "PIC12C509A-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C509A-xSM"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C509A, 1024W EPROM, 41B SRAM, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12C509A-xSN"
		(extends "PIC12C509A-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C509A-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C509A, 1024W EPROM, 41B SRAM, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12C671-xJW"
		(extends "PIC12C671-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C671-xJW"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:CERDIP-8_W7.62mm_SideBrazed"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/30561b.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C671, 1024W EPROM, 128B SRAM, CERDIP-8 Windowed"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CERDIP*7.62mm*SideBrazed*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12C671-xSN"
		(extends "PIC12C671-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C671-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/30561b.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C671, 1024W EPROM, 128B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12C672-xJW"
		(extends "PIC12C672-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C672-xJW"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:CERDIP-8_W7.62mm_SideBrazed"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/30561b.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C672, 2048W EPROM, 128B SRAM, CERDIP-8 Windowed"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CERDIP*7.62mm*SideBrazed*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12C672-xSN"
		(extends "PIC12C672-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12C672-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/30561b.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12C672, 2048W EPROM, 128B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12CE518-xJW"
		(extends "PIC12CE518-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CE518-xJW"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:CERDIP-8_W7.62mm_SideBrazed"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12CE518, 512W EPROM, 25B SRAM, CERDIP-8 Windowed"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CERDIP*7.62mm*SideBrazed*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12CE518-xSM"
		(extends "PIC12CE518-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CE518-xSM"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12CE518, 512W EPROM, 25B SRAM, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12CE518-xSN"
		(extends "PIC12CE518-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CE518-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12CE518, 512W EPROM, 25B SRAM, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12CE519-xJW"
		(extends "PIC12CE519-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CE519-xJW"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:CERDIP-8_W7.62mm_SideBrazed"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12CE519, 1024W EPROM, 41B SRAM, CERDIP-8 Windowed"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CERDIP*7.62mm*SideBrazed*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12CE519-xSM"
		(extends "PIC12CE519-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CE519-xSM"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W EPROM, 41B SRAM, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12CE519-xSN"
		(extends "PIC12CE519-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CE519-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12CE519, 1024W EPROM, 41B SRAM, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12CE673-xJW"
		(extends "PIC12CE673-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CE673-xJW"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:CERDIP-8_W7.62mm_SideBrazed"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/30561b.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12CE673, 1024W EPROM, 128B SRAM, 128B EEPROM, CERDIP-8 Windowed"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CERDIP*7.62mm*SideBrazed*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12CE674-xJW"
		(extends "PIC12CE674-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CE674-xJW"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:CERDIP-8_W7.62mm_SideBrazed"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/30561b.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12CE674, 2048W EPROM, 128B SRAM, 128B EEPROM, CERDIP-8 Windowed"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "CERDIP*7.62mm*SideBrazed*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12CR509A-xSM"
		(extends "PIC12CR509A-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CR509A-xSM"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12CR509A, 1024W ROM, 41B SRAM, SOIC-8 (208 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*5.3x5.3mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12CR509A-xSN"
		(extends "PIC12CR509A-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12CR509A-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/devicedoc/40139e.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12CR509A, 1024W ROM, 41B SRAM, SOIC-8 (150 mil)"
			(at 0 0 0)
		)
		(property "ki_keywords" "8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F1501-xMC"
		(extends "PIC12F1501-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F1501-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41615A.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F1501, 1024W FLASH, 64B SRAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F1501-xMS"
		(extends "PIC12F1501-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F1501-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41615A.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F1501, 1024W FLASH, 64B SRAM, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F1501-xSN"
		(extends "PIC12F1501-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F1501-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41615A.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F1501, 1024W FLASH, 64B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F1822-xMC"
		(extends "PIC12F1822-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F1822-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41413B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F1822, 2kW FLASH, 128B SRAM, 256 EEPROM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F1822-xSN"
		(extends "PIC12F1822-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F1822-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41413B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F1822, 2kW FLASH, 128B SRAM, 256 EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F1840-xMC"
		(extends "PIC12F1840-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F1840-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41441B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F1840, 4kW FLASH, 256B SRAM, 256B EEPROM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F1840-xSN"
		(extends "PIC12F1840-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F1840-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41441B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F1840, 4kW FLASH, 256B SRAM, 256B EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F508-xMC"
		(extends "PIC12F508-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F508-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F508, 512W Flash, 25B SRAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F508-xMS"
		(extends "PIC12F508-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F508-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F508, 512W Flash, 25B SRAM, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F508-xSN"
		(extends "PIC12F508-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F508-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F508, 512W Flash, 25B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F509-xMC"
		(extends "PIC12F509-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F509-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F509, 1024W Flash, 41B SRAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F509-xMS"
		(extends "PIC12F509-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F509-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F509, 1024W Flash, 41B SRAM, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F509-xSN"
		(extends "PIC12F509-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F509-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F509, 1024W Flash, 41B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F510-xMC"
		(extends "PIC12F510-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F510-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41268D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F510, 1024W FLASH, 38B SRAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F510-xMS"
		(extends "PIC12F510-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F510-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41268D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F510, 1024W FLASH, 38B SRAM, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F510-xSN"
		(extends "PIC12F510-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F510-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41268D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F510, 1024W FLASH, 38B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F519-xMC"
		(extends "PIC12F519-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F519-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41319B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F519, 1024W Flash, 41B SRAM, 64B EEPROM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F519-xMS"
		(extends "PIC12F519-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F519-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41319B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F519, 1024W Flash, 41B SRAM, 64B EEPROM, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F519-xSN"
		(extends "PIC12F519-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F519-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41319B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F519, 1024W Flash, 41B SRAM, 64B EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F609-xMC"
		(extends "PIC12F609-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F609-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F609, 1024W Flash, 64B SRAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F609-xMS"
		(extends "PIC12F609-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F609-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F609, 1024W Flash, 64B SRAM, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F609-xSN"
		(extends "PIC12F609-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F609-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F609, 1024W Flash, 64B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F615-xMC"
		(extends "PIC12F615-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F615-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F615, 1024W Flash, 64B SRAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F615-xMS"
		(extends "PIC12F615-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F615-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F615, 1024W Flash, 64B SRAM, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F615-xSN"
		(extends "PIC12F615-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F615-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F615, 1024W Flash, 64B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F617-xMC"
		(extends "PIC12F617-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F617-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F617, 2048W Flash, 128B SRAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F617-xMS"
		(extends "PIC12F617-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F617-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F617, 2048W Flash, 128B SRAM, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F617-xSN"
		(extends "PIC12F617-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F617-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F617, 2048W Flash, 128B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F629-xMC"
		(extends "PIC12F629-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F629-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41190G.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F629, 1024W Flash, 64B SRAM, 128B EEPROM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F629-xMS"
		(extends "PIC12F629-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F629-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41190G.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 64B SRAM, 128B EEPROM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F629-xSN"
		(extends "PIC12F629-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F629-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41190G.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F629, 1024W Flash, 64B SRAM, 128B EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F635-xMC"
		(extends "PIC12F635-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F635-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41232D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F635, 1024W Flash, 64B SRAM, 128B EEPROM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F635-xMS"
		(extends "PIC12F635-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F635-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41232D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 64B SRAM, 128B EEPROM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F635-xSN"
		(extends "PIC12F635-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F635-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41232D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F635, 1024W Flash, 64B SRAM, 128B EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F675-xMC"
		(extends "PIC12F675-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F675-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41190G.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F675, 1024W Flash, 64B SRAM, 128B EEPROM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F675-xMS"
		(extends "PIC12F675-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F675-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41190G.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W Flash, 64B SRAM, 128B EEPROM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F675-xSN"
		(extends "PIC12F675-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F675-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41190G.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F675, 1024W Flash, 64B SRAM, 128B EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F683-xMC"
		(extends "PIC12F683-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F683-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41211D_.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F683, 2048W Flash, 128B SRAM, 256B EEPROM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F683-xMS"
		(extends "PIC12F683-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F683-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41232D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "2048W Flash, 128B SRAM, 256B EEPROM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F683-xSN"
		(extends "PIC12F683-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F683-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41211D_.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F683, 2048W Flash, 128B SRAM, 256B EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F752-xMC"
		(extends "PIC12F752-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F752-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41576B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F752, 1024W Flash, 64B SRAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12F752-xSN"
		(extends "PIC12F752-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12F752-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41576B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12F752, 1024W Flash, 64B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12HV609-xMC"
		(extends "PIC12HV609-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12HV609-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12HV609, 1024W Flash, 64B SRAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12HV609-xMS"
		(extends "PIC12HV609-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12HV609-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12HV609, 1024W Flash, 64B SRAM, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12HV609-xSN"
		(extends "PIC12HV609-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12HV609-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12HV609, 1024W Flash, 64B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12HV615-xMC"
		(extends "PIC12HV615-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12HV615-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12HV615, 1024W Flash, 64B SRAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12HV615-xMS"
		(extends "PIC12HV615-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12HV615-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12HV615, 1024W Flash, 64B SRAM, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12HV615-xSN"
		(extends "PIC12HV615-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12HV615-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41302D.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12HV615, 1024W Flash, 64B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12HV752-xMC"
		(extends "PIC12HV752-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12HV752-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41576B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12HV752, 1024W Flash, 64B SRAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12HV752-xSN"
		(extends "PIC12HV752-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12HV752-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41576B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12HV752, 1024W Flash, 64B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller High Voltage"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12LF1501-xMC"
		(extends "PIC12F1501-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12LF1501-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41615A.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12LF1501, 1024W FLASH, 64B SRAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12LF1501-xMS"
		(extends "PIC12F1501-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12LF1501-xMS"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:MSOP-8_3x3mm_P0.65mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41615A.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12LF1501, 1024W FLASH, 64B SRAM, MSOP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MSOP*3x3mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12LF1501-xP"
		(extends "PIC12F1501-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12LF1501-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41615A.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "1024W FLASH, 64B SRAM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12LF1501-xSN"
		(extends "PIC12F1501-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12LF1501-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41615A.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12LF1501, 1024W FLASH, 64B SRAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12LF1822-xMC"
		(extends "PIC12F1822-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12LF1822-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41413B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12LF1822, 2kW FLASH, 128B SRAM, 256 EEPROM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12LF1822-xP"
		(extends "PIC12F1822-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12LF1822-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41413B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "2kW FLASH, 128B SRAM, 256 EEPROM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12LF1822-xSN"
		(extends "PIC12F1822-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12LF1822-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41413B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12LF1822, 2kW FLASH, 128B SRAM, 256 EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12LF1840-xMC"
		(extends "PIC12F1840-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12LF1840-xMC"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_3x2mm_P0.5mm_EP1.7x1.4mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41441B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12LF1840, 4kW FLASH, 256B SRAM, 256B EEPROM, PDIP8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*1EP*3x2mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12LF1840-xP"
		(extends "PIC12F1840-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12LF1840-xP"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41441B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "4kW FLASH, 256B SRAM, 256B EEPROM, PDIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC12LF1840-xSN"
		(extends "PIC12F1840-xP")
		(property "Reference" "U"
			(at 1.27 13.97 0)
		)
		(property "Value" "PIC12LF1840-xSN"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 1.27 -12.065 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/41441B.pdf"
			(at 1.27 -14.605 0)
		)
		(property "Description" "PIC12LF1840, 4kW FLASH, 256B SRAM, 256B EEPROM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*"
			(at 0 0 0)
		)
	)
)
