(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "PIC16F1454-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -46.99 15.24 0)
		)
		(property "Value" "PIC16F1454-IML"
			(at -46.99 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41639A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1454, 8192W FLASH, 1024B SRAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F1454-IML_0_1")
		(symbol "PIC16F1454-IML_1_1"
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 3.81)
				(name "Vusb3v3")
				(number "10")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 3.81)
				(name "RA0/D+/ICSPDAT")
				(number "12")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 3.81)
				(name "RA1/D-/ICSPCLK")
				(number "11")
			)
			(pin input line
				(at -50.8 -2.54 0)
				(length 3.81)
				(name "RA3/T1G/~{SS}/~{MCLR}/Vpp")
				(number "3")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 3.81)
				(name "RA4/SOSCO/T1G/SDO/CLKOUT/OSC2/CLKR")
				(number "2")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 3.81)
				(name "RA5/SOSCI/T1CKI/PWM2/CLKIN/OSC1")
				(number "1")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "13")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 3.81)
				(name "ICSPDAT/SCK/SCL/RC0")
				(number "9")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 3.81)
				(name "ICSPCLK/SDI/SDA/RC1")
				(number "8")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 3.81)
				(name "SDO/RC2")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 3.81)
				(name "CLKR/~{SS}/PWM2/RC3")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 3.81)
				(name "CK/TX/RC4")
				(number "5")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 3.81)
				(name "PWM1/DT/RX/T0CKI/RC5")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1454-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -46.99 15.24 0)
		)
		(property "Value" "PIC16F1454-IP"
			(at -46.99 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41639A.pdf"
			(at 0 0 0)
		)
		(property "Description" "8192W FLASH, 1024B SRAM, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F1454-IP_0_1")
		(symbol "PIC16F1454-IP_1_1"
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 3.81)
				(name "Vusb3v3")
				(number "11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 3.81)
				(name "RA0/D+/ICSPDAT")
				(number "13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 3.81)
				(name "RA1/D-/ICSPCLK")
				(number "12")
			)
			(pin input line
				(at -50.8 -2.54 0)
				(length 3.81)
				(name "RA3/T1G/~{SS}/~{MCLR}/Vpp")
				(number "4")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 3.81)
				(name "RA4/SOSCO/T1G/SDO/CLKOUT/OSC2/CLKR")
				(number "3")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 3.81)
				(name "RA5/SOSCI/T1CKI/PWM2/CLKIN/OSC1")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 3.81)
				(name "ICSPDAT/SCK/SCL/RC0")
				(number "10")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 3.81)
				(name "ICSPCLK/SDI/SDA/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 3.81)
				(name "SDO/RC2")
				(number "8")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 3.81)
				(name "CLKR/~{SS}/PWM2/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 3.81)
				(name "CK/TX/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 3.81)
				(name "PWM1/DT/RX/T0CKI/RC5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1455-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -46.99 17.78 0)
		)
		(property "Value" "PIC16F1455-IML"
			(at -46.99 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41639A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1454, 8192W FLASH, 1024B SRAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F1455-IML_0_1")
		(symbol "PIC16F1455-IML_1_1"
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 3.81)
				(name "Vusb3v3")
				(number "10")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 3.81)
				(name "RA0/D+/ICSPDAT")
				(number "12")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 3.81)
				(name "RA1/D-/ICSPCLK")
				(number "11")
			)
			(pin input line
				(at -50.8 -2.54 0)
				(length 3.81)
				(name "RA3/T1G/~{SS}/~{MCLR}/Vpp")
				(number "3")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 3.81)
				(name "RA4/AN3/SOSCO/T1G/SDO/CLKOUT/OSC2/CLKR")
				(number "2")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 3.81)
				(name "RA5/SOSCI/T1CKI/PWM2/CLKIN/OSC1")
				(number "1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "13")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 3.81)
				(name "ICSPDAT/SCK/SCL/C2IN+/C1IN+/Vref+/AN4/RC0")
				(number "9")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 3.81)
				(name "ICSPCLK/SDI/SDA/~{CWGFLT}/C2IN-/C1IN-/AN5/RC1")
				(number "8")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 3.81)
				(name "SDO/C2IN2-/C1IN2-/DACOUT1/AN6/RC2")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 3.81)
				(name "CLKR/~{SS}/PWM2/C1IN3-/C2IN3-/DACOUT2/AN7/RC3")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 3.81)
				(name "CK/TX/CWG1B/C1OUT/C2OUT/RC4")
				(number "5")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 3.81)
				(name "PWM1/DT/RX/CWG1A/T0CKI/RC5")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1455-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -46.99 17.78 0)
		)
		(property "Value" "PIC16F1455-IP"
			(at -46.99 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41639A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1454, 8192W FLASH, 1024B SRAM, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F1455-IP_0_1")
		(symbol "PIC16F1455-IP_1_1"
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 3.81)
				(name "Vusb3v3")
				(number "11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 3.81)
				(name "RA0/D+/ICSPDAT")
				(number "13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 3.81)
				(name "RA1/D-/ICSPCLK")
				(number "12")
			)
			(pin input line
				(at -50.8 -2.54 0)
				(length 3.81)
				(name "RA3/T1G/~{SS}/~{MCLR}/Vpp")
				(number "4")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 3.81)
				(name "RA4/AN3/SOSCO/T1G/SDO/CLKOUT/OSC2/CLKR")
				(number "3")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 3.81)
				(name "RA5/SOSCI/T1CKI/PWM2/CLKIN/OSC1")
				(number "2")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 3.81)
				(name "ICSPDAT/SCK/SCL/C2IN+/C1IN+/Vref+/AN4/RC0")
				(number "10")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 3.81)
				(name "ICSPCLK/SDI/SDA/~{CWGFLT}/C2IN-/C1IN-/AN5/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 3.81)
				(name "SDO/C2IN2-/C1IN2-/DACOUT1/AN6/RC2")
				(number "8")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 3.81)
				(name "CLKR/~{SS}/PWM2/C1IN3-/C2IN3-/DACOUT2/AN7/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 3.81)
				(name "CK/TX/CWG1B/C1OUT/C2OUT/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 3.81)
				(name "PWM1/DT/RX/CWG1A/T0CKI/RC5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1459-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -46.99 17.78 0)
		)
		(property "Value" "PIC16F1459-IML"
			(at -46.99 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41639A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1454, 8192W FLASH, 1024B SRAM, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F1459-IML_0_1")
		(symbol "PIC16F1459-IML_1_1"
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 3.81)
				(name "Vusb3v3")
				(number "14")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 3.81)
				(name "RA0/D+/ICSPDAT")
				(number "16")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 3.81)
				(name "RA1/D-/ICSPCLK")
				(number "15")
			)
			(pin input line
				(at -50.8 0 0)
				(length 3.81)
				(name "RA3/T1G/~{SS}/~{MCLR}/Vpp")
				(number "1")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 3.81)
				(name "RA4/AN3/SOSCO/T1G/OSC2/CLKOUT/CLKR")
				(number "20")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 3.81)
				(name "RA5/SOSCI/T1CKI/OSC1/CLKIN")
				(number "19")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 3.81)
				(name "RB4/AN10/SDA/SDI")
				(number "10")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 3.81)
				(name "RB5/AN11/RX/DX")
				(number "9")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 3.81)
				(name "RB6/SCL/SCK")
				(number "8")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 3.81)
				(name "RB7/TX/CK")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "17")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 3.81)
				(name "ICSPDAT/C2IN+/C1IN+/Vref+/AN4/RC0")
				(number "13")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 3.81)
				(name "ICSPCLK/~{CWGFLT}/C2IN-/C1IN-/AN5/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 3.81)
				(name "C2IN2-/C1IN2-/DACOUT1/AN6/RC2")
				(number "11")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 3.81)
				(name "CLKR/C1IN3-/C2IN3-/DACOUT2/AN7/RC3")
				(number "4")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 3.81)
				(name "CWG1B/C1OUT/C2OUT/RC4")
				(number "3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 3.81)
				(name "PWM1/CWG1A/T0CKI/RC5")
				(number "2")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 3.81)
				(name "~{SS}/PWM2/AN8/RC6")
				(number "5")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 3.81)
				(name "SDO/AN9/RC7")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1459-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -46.99 17.78 0)
		)
		(property "Value" "PIC16F1459-IP"
			(at -46.99 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41639A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1454, 8192W FLASH, 1024B SRAM, PDIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F1459-IP_0_1")
		(symbol "PIC16F1459-IP_1_1"
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 3.81)
				(name "Vusb3v3")
				(number "17")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 3.81)
				(name "RA0/D+/ICSPDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 3.81)
				(name "RA1/D-/ICSPCLK")
				(number "18")
			)
			(pin input line
				(at -50.8 0 0)
				(length 3.81)
				(name "RA3/T1G/~{SS}/~{MCLR}/Vpp")
				(number "4")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 3.81)
				(name "RA4/AN3/SOSCO/T1G/OSC2/CLKOUT/CLKR")
				(number "3")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 3.81)
				(name "RA5/SOSCI/T1CKI/OSC1/CLKIN")
				(number "2")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 3.81)
				(name "RB4/AN10/SDA/SDI")
				(number "13")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 3.81)
				(name "RB5/AN11/RX/DX")
				(number "12")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 3.81)
				(name "RB6/SCL/SCK")
				(number "11")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 3.81)
				(name "RB7/TX/CK")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 3.81)
				(name "ICSPDAT/C2IN+/C1IN+/Vref+/AN4/RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 3.81)
				(name "ICSPCLK/~{CWGFLT}/C2IN-/C1IN-/AN5/RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 3.81)
				(name "C2IN2-/C1IN2-/DACOUT1/AN6/RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 3.81)
				(name "CLKR/C1IN3-/C2IN3-/DACOUT2/AN7/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 3.81)
				(name "CWG1B/C1OUT/C2OUT/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 3.81)
				(name "PWM1/CWG1A/T0CKI/RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 3.81)
				(name "~{SS}/PWM2/AN8/RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 3.81)
				(name "SDO/AN9/RC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1503-IMG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -46.99 15.24 0)
		)
		(property "Value" "PIC16F1503-IMG"
			(at -46.99 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41607A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1503, 2048W FLASH, 128B SRAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F1503-IMG_0_1")
		(symbol "PIC16F1503-IMG_1_1"
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 3.81)
				(name "RA0/AN0/DACOUT1/C1IN+/ICSPDAT")
				(number "12")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 3.81)
				(name "RA1/AN1/Vref+/C1IN0-/C2IN0-/ICSPCLK")
				(number "11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 3.81)
				(name "RA2/AN2/DACOUT2/C1OUT/T0CKI/~{CWG1FLT}/CLC1/PWM3/INT")
				(number "10")
			)
			(pin input line
				(at -50.8 0 0)
				(length 3.81)
				(name "RA3/T1G/CLC1IN0/~{SS}/~{MCLR}/Vpp")
				(number "3")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 3.81)
				(name "RA4/AN3/T1G/NCO1/SDO/CLKOUT")
				(number "2")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 3.81)
				(name "RA5/T1CKI/NCO1CLK/CLCIN1/CLKIN")
				(number "1")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "13")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 3.81)
				(name "SCK/SCL/CLC2/C2IN+/AN4/RC0")
				(number "9")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 3.81)
				(name "SDI/SDA/PWM4/NCO1/C2IN1-/C1IN1-/AN5/RC1")
				(number "8")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 3.81)
				(name "SDO/C2IN2-/C1IN2-/AN6/RC2")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 3.81)
				(name "~{SS}/PWM2/CLCIN0/C2IN3-/C1IN3-/AN7/RC3")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 3.81)
				(name "CLC2IN1/CWG1B/C2OUT/RC4")
				(number "5")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 3.81)
				(name "PWM1/CLC1/CWG1A/RC5")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1503-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -46.99 15.24 0)
		)
		(property "Value" "PIC16F1503-IP"
			(at -46.99 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41607A.pdf"
			(at 0 0 0)
		)
		(property "Description" "2048W FLASH, 128B SRAM, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F1503-IP_0_1")
		(symbol "PIC16F1503-IP_1_1"
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 3.81)
				(name "RA0/AN0/DACOUT1/C1IN+/ICSPDAT")
				(number "13")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 3.81)
				(name "RA1/AN1/Vref+/C1IN0-/C2IN0-/ICSPCLK")
				(number "12")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 3.81)
				(name "RA2/AN2/DACOUT2/C1OUT/T0CKI/~{CWG1FLT}/CLC1/PWM3/INT")
				(number "11")
			)
			(pin input line
				(at -50.8 0 0)
				(length 3.81)
				(name "RA3/T1G/CLC1IN0/~{SS}/~{MCLR}/Vpp")
				(number "4")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 3.81)
				(name "RA4/AN3/T1G/NCO1/SDO/CLKOUT")
				(number "3")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 3.81)
				(name "RA5/T1CKI/NCO1CLK/CLCIN1/CLKIN")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 3.81)
				(name "SCK/SCL/CLC2/C2IN+/AN4/RC0")
				(number "10")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 3.81)
				(name "SDI/SDA/PWM4/NCO1/C2IN1-/C1IN1-/AN5/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 3.81)
				(name "SDO/C2IN2-/C1IN2-/AN6/RC2")
				(number "8")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 3.81)
				(name "~{SS}/PWM2/CLCIN0/C2IN3-/C1IN3-/AN7/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 3.81)
				(name "CLC2IN1/CWG1B/C2OUT/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 3.81)
				(name "PWM1/CLC1/CWG1A/RC5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1507-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 20.32 0)
		)
		(property "Value" "PIC16F1507-IML"
			(at -29.21 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41586A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1507, 2048W FLASH, 128B SRAM, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*"
			(at 0 0 0)
		)
		(symbol "PIC16F1507-IML_0_1")
		(symbol "PIC16F1507-IML_1_1"
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "RA0/AN0/ICSPDAT")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "RA1/AN1/Vref+/ICSPCLK")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "RA2/AN2/~{CWG1FLT}/CLC1/T0CKI/PWM3")
				(number "14")
			)
			(pin input line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "RA3/CLC1IN0/~{MCLR}/Vpp")
				(number "1")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "RA4/AN3/~{T1G}/CLKOUT")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "RA5/NCO1CLK/T1CKI/CLKIN")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "RB4/AN10")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "RB5/AN11")
				(number "9")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "RB6")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "RB7")
				(number "7")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "CLC2/AN4/RC0")
				(number "13")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "PWM4/NCO1/AN5/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "AN6/RC2")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "PWM2/CLC2IN0/AN7/RC3")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "CLC2IN1/CWG1B/RC4")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "PWM1/CLC1/CWG1A/RC5")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "NCO1/AN8/RC6")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "CLCIN1/AN9/RC7")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1507-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 20.32 0)
		)
		(property "Value" "PIC16F1507-IP"
			(at -29.21 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41586A.pdf"
			(at 0 0 0)
		)
		(property "Description" "2048W FLASH, 128B SRAM, PDIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F1507-IP_0_1")
		(symbol "PIC16F1507-IP_1_1"
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "RA0/AN0/ICSPDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "RA1/AN1/Vref+/ICSPCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "RA2/AN2/~{CWG1FLT}/CLC1/T0CKI/PWM3")
				(number "17")
			)
			(pin input line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "RA3/CLC1IN0/~{MCLR}/Vpp")
				(number "4")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "RA4/AN3/~{T1G}/CLKOUT")
				(number "3")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "RA5/NCO1CLK/T1CKI/CLKIN")
				(number "2")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "RB4/AN10")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "RB5/AN11")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "RB7")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "CLC2/AN4/RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "PWM4/NCO1/AN5/RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "AN6/RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "PWM2/CLC2IN0/AN7/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "CLC2IN1/CWG1B/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "PWM1/CLC1/CWG1A/RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "NCO1/AN8/RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "CLCIN1/AN9/RC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1508-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -52.07 20.32 0)
		)
		(property "Value" "PIC16F1508-IML"
			(at -52.07 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41609A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1508, 4096W FLASH, 256B SRAM, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*"
			(at 0 0 0)
		)
		(symbol "PIC16F1508-IML_0_1")
		(symbol "PIC16F1508-IML_1_1"
			(pin bidirectional line
				(at -55.88 12.7 0)
				(length 3.81)
				(name "RA0/AN0/DACOUT1/C1IN+/ICSPDAT/ICDDAT")
				(number "16")
			)
			(pin bidirectional line
				(at -55.88 10.16 0)
				(length 3.81)
				(name "RA1/AN1/Vref+/C1IN0-/C2IN0-/CLC4IN1/ICSPCLK/ICDCLK")
				(number "15")
			)
			(pin bidirectional line
				(at -55.88 7.62 0)
				(length 3.81)
				(name "RA2/AN2/DACOUT2/C1OUT/T0CLKI/~{CWG1FLT}/CLC1/PWM3")
				(number "14")
			)
			(pin input line
				(at -55.88 5.08 0)
				(length 3.81)
				(name "RA3/T1G/~{SS}/CLC1IN0/~{MCLR}/Vpp")
				(number "1")
			)
			(pin bidirectional line
				(at -55.88 2.54 0)
				(length 3.81)
				(name "RA4/AN3/SOSCO/T1G/CLKOUT/OSC2")
				(number "20")
			)
			(pin bidirectional line
				(at -55.88 0 0)
				(length 3.81)
				(name "RA5/SOSCI/T1CKI/NCO1CLK/CLKIN/OSC1")
				(number "19")
			)
			(pin bidirectional line
				(at -55.88 -5.08 0)
				(length 3.81)
				(name "RB4/AN10/SDA/SDI/CLC3IN0")
				(number "10")
			)
			(pin bidirectional line
				(at -55.88 -7.62 0)
				(length 3.81)
				(name "RB5/AN11/RX/DT/CLC4IN0")
				(number "9")
			)
			(pin bidirectional line
				(at -55.88 -10.16 0)
				(length 3.81)
				(name "RB6/SCL/SCK")
				(number "8")
			)
			(pin bidirectional line
				(at -55.88 -12.7 0)
				(length 3.81)
				(name "RB7/TX/CK/CLC3")
				(number "7")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "17")
			)
			(pin bidirectional line
				(at 55.88 12.7 180)
				(length 3.81)
				(name "CLC2/C2IN+/AN4/RC0")
				(number "13")
			)
			(pin bidirectional line
				(at 55.88 10.16 180)
				(length 3.81)
				(name "PWM4/NCO1/C1IN1-/C2IN1-/AN5/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 55.88 7.62 180)
				(length 3.81)
				(name "C1IN2-/C2IN2-/AN6/RC2")
				(number "11")
			)
			(pin bidirectional line
				(at 55.88 5.08 180)
				(length 3.81)
				(name "PWM2/CLC2IN0/C1IN3-/AN7/RC3")
				(number "4")
			)
			(pin bidirectional line
				(at 55.88 2.54 180)
				(length 3.81)
				(name "CLC4/CLC2IN1/CWG1B/C2OUT/RC4")
				(number "3")
			)
			(pin bidirectional line
				(at 55.88 0 180)
				(length 3.81)
				(name "PWM1/CLC1/CWG1A/RC5")
				(number "2")
			)
			(pin bidirectional line
				(at 55.88 -2.54 180)
				(length 3.81)
				(name "CLC3IN1/NCO1/~{SS}/AN8/RC6")
				(number "5")
			)
			(pin bidirectional line
				(at 55.88 -5.08 180)
				(length 3.81)
				(name "CLC1IN1/SDO/AN9/RC7")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1508-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -52.07 20.32 0)
		)
		(property "Value" "PIC16F1508-IP"
			(at -52.07 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41609A.pdf"
			(at 0 0 0)
		)
		(property "Description" "4096W FLASH, 256B SRAM, PDIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F1508-IP_0_1")
		(symbol "PIC16F1508-IP_1_1"
			(pin bidirectional line
				(at -55.88 12.7 0)
				(length 3.81)
				(name "RA0/AN0/DACOUT1/C1IN+/ICSPDAT/ICDDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -55.88 10.16 0)
				(length 3.81)
				(name "RA1/AN1/Vref+/C1IN0-/C2IN0-/CLC4IN1/ICSPCLK/ICDCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -55.88 7.62 0)
				(length 3.81)
				(name "RA2/AN2/DACOUT2/C1OUT/T0CLKI/~{CWG1FLT}/CLC1/PWM3")
				(number "17")
			)
			(pin input line
				(at -55.88 5.08 0)
				(length 3.81)
				(name "RA3/T1G/~{SS}/CLC1IN0/~{MCLR}/Vpp")
				(number "4")
			)
			(pin bidirectional line
				(at -55.88 2.54 0)
				(length 3.81)
				(name "RA4/AN3/SOSCO/T1G/CLKOUT/OSC2")
				(number "3")
			)
			(pin bidirectional line
				(at -55.88 0 0)
				(length 3.81)
				(name "RA5/SOSCI/T1CKI/NCO1CLK/CLKIN/OSC1")
				(number "2")
			)
			(pin bidirectional line
				(at -55.88 -5.08 0)
				(length 3.81)
				(name "RB4/AN10/SDA/SDI/CLC3IN0")
				(number "13")
			)
			(pin bidirectional line
				(at -55.88 -7.62 0)
				(length 3.81)
				(name "RB5/AN11/RX/DT/CLC4IN0")
				(number "12")
			)
			(pin bidirectional line
				(at -55.88 -10.16 0)
				(length 3.81)
				(name "RB6/SCL/SCK")
				(number "11")
			)
			(pin bidirectional line
				(at -55.88 -12.7 0)
				(length 3.81)
				(name "RB7/TX/CK/CLC3")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 55.88 12.7 180)
				(length 3.81)
				(name "CLC2/C2IN+/AN4/RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 55.88 10.16 180)
				(length 3.81)
				(name "PWM4/NCO1/C1IN1-/C2IN1-/AN5/RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 55.88 7.62 180)
				(length 3.81)
				(name "C1IN2-/C2IN2-/AN6/RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 55.88 5.08 180)
				(length 3.81)
				(name "PWM2/CLC2IN0/C1IN3-/AN7/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 55.88 2.54 180)
				(length 3.81)
				(name "CLC4/CLC2IN1/CWG1B/C2OUT/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 55.88 0 180)
				(length 3.81)
				(name "PWM1/CLC1/CWG1A/RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 55.88 -2.54 180)
				(length 3.81)
				(name "CLC3IN1/NCO1/~{SS}/AN8/RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 55.88 -5.08 180)
				(length 3.81)
				(name "CLC1IN1/SDO/AN9/RC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1509-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -52.07 20.32 0)
		)
		(property "Value" "PIC16F1509-IML"
			(at -52.07 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41609A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1509, 9192W FLASH, 512B SRAM, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*"
			(at 0 0 0)
		)
		(symbol "PIC16F1509-IML_0_1")
		(symbol "PIC16F1509-IML_1_1"
			(pin bidirectional line
				(at -55.88 12.7 0)
				(length 3.81)
				(name "RA0/AN0/DACOUT1/C1IN+/ICSPDAT/ICDDAT")
				(number "16")
			)
			(pin bidirectional line
				(at -55.88 10.16 0)
				(length 3.81)
				(name "RA1/AN1/Vref+/C1IN0-/C2IN0-/CLC4IN1/ICSPCLK/ICDCLK")
				(number "15")
			)
			(pin bidirectional line
				(at -55.88 7.62 0)
				(length 3.81)
				(name "RA2/AN2/DACOUT2/C1OUT/T0CLKI/~{CWG1FLT}/CLC1/PWM3")
				(number "14")
			)
			(pin input line
				(at -55.88 5.08 0)
				(length 3.81)
				(name "RA3/T1G/~{SS}/CLC1IN0/~{MCLR}/Vpp")
				(number "1")
			)
			(pin bidirectional line
				(at -55.88 2.54 0)
				(length 3.81)
				(name "RA4/AN3/SOSCO/T1G/CLKOUT/OSC2")
				(number "20")
			)
			(pin bidirectional line
				(at -55.88 0 0)
				(length 3.81)
				(name "RA5/SOSCI/T1CKI/NCO1CLK/CLKIN/OSC1")
				(number "19")
			)
			(pin bidirectional line
				(at -55.88 -5.08 0)
				(length 3.81)
				(name "RB4/AN10/SDA/SDI/CLC3IN0")
				(number "10")
			)
			(pin bidirectional line
				(at -55.88 -7.62 0)
				(length 3.81)
				(name "RB5/AN11/RX/DT/CLC4IN0")
				(number "9")
			)
			(pin bidirectional line
				(at -55.88 -10.16 0)
				(length 3.81)
				(name "RB6/SCL/SCK")
				(number "8")
			)
			(pin bidirectional line
				(at -55.88 -12.7 0)
				(length 3.81)
				(name "RB7/TX/CK/CLC3")
				(number "7")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "17")
			)
			(pin bidirectional line
				(at 55.88 12.7 180)
				(length 3.81)
				(name "CLC2/C2IN+/AN4/RC0")
				(number "13")
			)
			(pin bidirectional line
				(at 55.88 10.16 180)
				(length 3.81)
				(name "PWM4/NCO1/C1IN1-/C2IN1-/AN5/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 55.88 7.62 180)
				(length 3.81)
				(name "C1IN2-/C2IN2-/AN6/RC2")
				(number "11")
			)
			(pin bidirectional line
				(at 55.88 5.08 180)
				(length 3.81)
				(name "PWM2/CLC2IN0/C1IN3-/AN7/RC3")
				(number "4")
			)
			(pin bidirectional line
				(at 55.88 2.54 180)
				(length 3.81)
				(name "CLC4/CLC2IN1/CWG1B/C2OUT/RC4")
				(number "3")
			)
			(pin bidirectional line
				(at 55.88 0 180)
				(length 3.81)
				(name "PWM1/CLC1/CWG1A/RC5")
				(number "2")
			)
			(pin bidirectional line
				(at 55.88 -2.54 180)
				(length 3.81)
				(name "CLC3IN1/NCO1/~{SS}/AN8/RC6")
				(number "5")
			)
			(pin bidirectional line
				(at 55.88 -5.08 180)
				(length 3.81)
				(name "CLC1IN1/SDO/AN9/RC7")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1509-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -52.07 20.32 0)
		)
		(property "Value" "PIC16F1509-IP"
			(at -52.07 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41609A.pdf"
			(at 0 0 0)
		)
		(property "Description" "8192W FLASH, 512B SRAM, PDIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F1509-IP_0_1")
		(symbol "PIC16F1509-IP_1_1"
			(pin bidirectional line
				(at -55.88 12.7 0)
				(length 3.81)
				(name "RA0/AN0/DACOUT1/C1IN+/ICSPDAT/ICDDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -55.88 10.16 0)
				(length 3.81)
				(name "RA1/AN1/Vref+/C1IN0-/C2IN0-/CLC4IN1/ICSPCLK/ICDCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -55.88 7.62 0)
				(length 3.81)
				(name "RA2/AN2/DACOUT2/C1OUT/T0CLKI/~{CWG1FLT}/CLC1/PWM3")
				(number "17")
			)
			(pin input line
				(at -55.88 5.08 0)
				(length 3.81)
				(name "RA3/T1G/~{SS}/CLC1IN0/~{MCLR}/Vpp")
				(number "4")
			)
			(pin bidirectional line
				(at -55.88 2.54 0)
				(length 3.81)
				(name "RA4/AN3/SOSCO/T1G/CLKOUT/OSC2")
				(number "3")
			)
			(pin bidirectional line
				(at -55.88 0 0)
				(length 3.81)
				(name "RA5/SOSCI/T1CKI/NCO1CLK/CLKIN/OSC1")
				(number "2")
			)
			(pin bidirectional line
				(at -55.88 -5.08 0)
				(length 3.81)
				(name "RB4/AN10/SDA/SDI/CLC3IN0")
				(number "13")
			)
			(pin bidirectional line
				(at -55.88 -7.62 0)
				(length 3.81)
				(name "RB5/AN11/RX/DT/CLC4IN0")
				(number "12")
			)
			(pin bidirectional line
				(at -55.88 -10.16 0)
				(length 3.81)
				(name "RB6/SCL/SCK")
				(number "11")
			)
			(pin bidirectional line
				(at -55.88 -12.7 0)
				(length 3.81)
				(name "RB7/TX/CK/CLC3")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 55.88 12.7 180)
				(length 3.81)
				(name "CLC2/C2IN+/AN4/RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 55.88 10.16 180)
				(length 3.81)
				(name "PWM4/NCO1/C1IN1-/C2IN1-/AN5/RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 55.88 7.62 180)
				(length 3.81)
				(name "C1IN2-/C2IN2-/AN6/RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 55.88 5.08 180)
				(length 3.81)
				(name "PWM2/CLC2IN0/C1IN3-/AN7/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 55.88 2.54 180)
				(length 3.81)
				(name "CLC4/CLC2IN1/CWG1B/C2OUT/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 55.88 0 180)
				(length 3.81)
				(name "PWM1/CLC1/CWG1A/RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 55.88 -2.54 180)
				(length 3.81)
				(name "CLC3IN1/NCO1/~{SS}/AN8/RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 55.88 -5.08 180)
				(length 3.81)
				(name "CLC1IN1/SDO/AN9/RC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1512-IMV"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 30.48 0)
		)
		(property "Value" "PIC16F1512-IMV"
			(at 6.35 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41624A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1512, 2048W FLASH, 128B SRAM, UQFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F1512-IMV_0_1")
		(symbol "PIC16F1512-IMV_1_1"
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA5/AN4/VCAP/~{SS}")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT/IOC")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/IOC")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/IOC")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/IOC")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/ADOUT/IOC")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RB5/AN13/T1G/IOC")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RB6/ADGRDA/IOC/ICSPCLK/ICDCLK")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RB7/ADGRDB/IOC/ICSPDAT/ICDDAT")
				(number "25")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "15")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1512-ISP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 30.48 0)
		)
		(property "Value" "PIC16F1512-ISP"
			(at 5.08 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41624A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1512, 2048W FLASH, 128B SRAM, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F1512-ISP_0_1")
		(symbol "PIC16F1512-ISP_1_1"
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA5/AN4/Vcap/~{SS}")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT/IOC")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/IOC")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/IOC")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/IOC")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/ADOUT/IOC")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RB5/AN13/T1G/IOC")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RB6/ADGRDA/IOC/ICSPCLK/ICDCLK")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RB7/ADGRDB/IOC/ICSPDAT/ICDDAT")
				(number "28")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "18")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1513-IMV"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 30.48 0)
		)
		(property "Value" "PIC16F1513-IMV"
			(at 5.08 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41624A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1513, 4096W FLASH, 256B SRAM, UQFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F1513-IMV_0_1")
		(symbol "PIC16F1513-IMV_1_1"
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA5/AN4/Vcap/~{SS}")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT/IOC")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/IOC")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/IOC")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/IOC")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/ADOUT/IOC")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RB5/AN13/T1G/IOC")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RB6/ADGRDA/IOC/ICSPCLK/ICDCLK")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RB7/ADGRDB/IOC/ICSPDAT/ICDDAT")
				(number "25")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "15")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1513-ISP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 30.48 0)
		)
		(property "Value" "PIC16F1513-ISP"
			(at 5.08 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41624A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1513, 4096W FLASH, 2568B SRAM, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F1513-ISP_0_1")
		(symbol "PIC16F1513-ISP_1_1"
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA5/AN4/Vcap/~{SS}")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT/IOC")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/IOC")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/IOC")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/IOC")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/ADOUT/IOC")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RB5/AN13/T1G/IOC")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RB6/ADGRDA/IOC/ICSPCLK/ICDCLK")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RB7/ADGRDB/IOC/ICSPDAT/ICDDAT")
				(number "28")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "18")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1516-IMV"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 30.48 0)
		)
		(property "Value" "PIC16F1516-IMV"
			(at 5.08 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1516, 8192W FLASH, 512B SRAM, UQFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F1516-IMV_0_1")
		(symbol "PIC16F1516-IMV_1_1"
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA5/AN4/Vcap/~{SS}")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT/IOC")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/IOC")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/IOC")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/IOC")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/ADOUT/IOC")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RB5/AN13/T1G/IOC")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RB6/ADGRDA/IOC/ICSPCLK/ICDCLK")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RB7/ADGRDB/IOC/ICSPDAT/ICDDAT")
				(number "25")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "15")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1516-ISP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 30.48 0)
		)
		(property "Value" "PIC16F1516-ISP"
			(at 5.08 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1516, 8192W FLASH, 512B SRAM, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F1516-ISP_0_1")
		(symbol "PIC16F1516-ISP_1_1"
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA5/AN4/Vcap/~{SS}")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT/IOC")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/IOC")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/IOC")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/IOC")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/ADOUT/IOC")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RB5/AN13/T1G/IOC")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RB6/ADGRDA/IOC/ICSPCLK/ICDCLK")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RB7/ADGRDB/IOC/ICSPDAT/ICDDAT")
				(number "28")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "18")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1517-IMV"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 35.56 0)
		)
		(property "Value" "PIC16F1517-IMV"
			(at 3.81 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1517, 8192W FLASH, 512B SRAM, UQFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F1517-IMV_0_1")
		(symbol "PIC16F1517-IMV_1_1"
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA5/AN4/VCAP/~{SS}")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RB0/AN12/INT")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RB1/AN10")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "RB2/AN8")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB3/AN9/CCP2")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB4/AN11")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB5/AN13/T1G")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB6/ICSPCLK/ICDCLK")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB7/ICSPDAT/ICDDAT")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RE0/AN5")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RE1/AN6")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "RE2/AN7")
				(number "25")
			)
			(pin input line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "RE3/~{MCLR}/Vpp")
				(number "16")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "30")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "31")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "33")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "AN20/RD0")
				(number "34")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "AN21/RD1")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "AN22/RD2")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "AN23/RD3")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "AN24/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "AN25/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "AN26/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "AN27/RD7")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1517-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 35.56 0)
		)
		(property "Value" "PIC16F1517-IP"
			(at 3.81 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "8192W FLASH, 512B SRAM, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F1517-IP_0_1")
		(symbol "PIC16F1517-IP_1_1"
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA5/AN4/VCAP/~{SS}")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RB0/AN12/INT")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RB1/AN10")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "RB2/AN8")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB3/AN9/CCP2")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB4/AN11")
				(number "37")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB5/AN13/T1G")
				(number "38")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB6/ICSPCLK/ICDCLK")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB7/ICSPDAT/ICDDAT")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RE0/AN5")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RE1/AN6")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "RE2/AN7")
				(number "10")
			)
			(pin input line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "RE3/~{MCLR}/Vpp")
				(number "1")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "AN20/RD0")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "AN21/RD1")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "AN22/RD2")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "AN23/RD3")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "AN24/RD4")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "AN25/RD5")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "AN26/RD6")
				(number "29")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "AN27/RD7")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1517-IPT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 35.56 0)
		)
		(property "Value" "PIC16F1517-IPT"
			(at 3.81 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1517, 8192W FLASH, 512B SRAM, TQFP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*"
			(at 0 0 0)
		)
		(symbol "PIC16F1517-IPT_0_1")
		(symbol "PIC16F1517-IPT_1_1"
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA5/AN4/VCAP/~{SS}")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RB0/AN12/INT")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RB1/AN10")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "RB2/AN8")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB3/AN9/CCP2")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB4/AN11")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB5/AN13/T1G")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB6/ICSPCLK/ICDCLK")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB7/ICSPDAT/ICDDAT")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RE0/AN5")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RE1/AN6")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "RE2/AN7")
				(number "27")
			)
			(pin input line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "RE3/~{MCLR}/Vpp")
				(number "18")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "AN20/RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "AN21/RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "AN22/RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "AN23/RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "AN24/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "AN25/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "AN26/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "AN27/RD7")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1518-IMV"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 30.48 0)
		)
		(property "Value" "PIC16F1518-IMV"
			(at 2.54 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1518, 16384W FLASH, 1204B SRAM, UQFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F1518-IMV_0_1")
		(symbol "PIC16F1518-IMV_1_1"
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "RA5/AN4/VCAP/~{SS}")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT/IOC")
				(number "18")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/IOC")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/IOC")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/IOC")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/ADOUT/IOC")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "RB5/AN13/T1G/IOC")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "RB6/ADGRDA/IOC/ICSPCLK/ICDCLK")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "RB7/ADGRDB/IOC/ICSPDAT/ICDDAT")
				(number "25")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "15")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1518-ISP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 30.48 0)
		)
		(property "Value" "PIC16F1518-ISP"
			(at 2.54 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1518, 16384W FLASH, 1024B SRAM, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F1518-ISP_0_1")
		(symbol "PIC16F1518-ISP_1_1"
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "RA5/AN4/VCAP/~{SS}")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT/IOC")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/IOC")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/IOC")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/IOC")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/ADOUT/IOC")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "RB5/AN13/T1G/IOC")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "RB6/ADGRDA/IOC/ICSPCLK/ICDCLK")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "RB7/ADGRDB/IOC/ICSPDAT/ICDDAT")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "18")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1519-IMV"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 35.56 0)
		)
		(property "Value" "PIC16F1519-IMV"
			(at 2.54 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1519, 16384W FLASH, 1024B SRAM, UQFN-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F1519-IMV_0_1")
		(symbol "PIC16F1519-IMV_1_1"
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA5/AN4/VCAP/~{SS}")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RB0/AN12/INT")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RB1/AN10")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "RB2/AN8")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB3/AN9/CCP2")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB4/AN11")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB5/AN13/T1G")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB6/ICSPCLK/ICDCLK")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB7/ICSPDAT/ICDDAT")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RE0/AN5")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RE1/AN6")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "RE2/AN7")
				(number "25")
			)
			(pin input line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "RE3/~{MCLR}/Vpp")
				(number "16")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "30")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "31")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "33")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "AN20/RD0")
				(number "34")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "AN21/RD1")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "AN22/RD2")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "AN23/RD3")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "AN24/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "AN25/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "AN26/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "AN27/RD7")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1519-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 35.56 0)
		)
		(property "Value" "PIC16F1519-IP"
			(at 2.54 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "16384W FLASH, 1024B SRAM, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F1519-IP_0_1")
		(symbol "PIC16F1519-IP_1_1"
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA5/AN4/VCAP/~{SS}")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RB0/AN12/INT")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RB1/AN10")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "RB2/AN8")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB3/AN9/CCP2")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB4/AN11")
				(number "37")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB5/AN13/T1G")
				(number "38")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB6/ICSPCLK/ICDCLK")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB7/ICSPDAT/ICDDAT")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RE0/AN5")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RE1/AN6")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "RE2/AN7")
				(number "10")
			)
			(pin input line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "RE3/~{MCLR}/Vpp")
				(number "1")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "AN20/RD0")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "AN21/RD1")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "AN22/RD2")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "AN23/RD3")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "AN24/RD4")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "AN25/RD5")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "AN26/RD6")
				(number "29")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "AN27/RD7")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1519-IPT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 35.56 0)
		)
		(property "Value" "PIC16F1519-IPT"
			(at 2.54 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1519, 16384W FLASH, 1024B SRAM, TQFP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*"
			(at 0 0 0)
		)
		(symbol "PIC16F1519-IPT_0_1")
		(symbol "PIC16F1519-IPT_1_1"
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "RA0/AN0/~{SS}")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA5/AN4/VCAP/~{SS}")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RB0/AN12/INT")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RB1/AN10")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "RB2/AN8")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB3/AN9/CCP2")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB4/AN11")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB5/AN13/T1G")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB6/ICSPCLK/ICDCLK")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB7/ICSPDAT/ICDDAT")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RE0/AN5")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RE1/AN6")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "RE2/AN7")
				(number "27")
			)
			(pin input line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "RE3/~{MCLR}/Vpp")
				(number "18")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "SOSCO/T1CKI/RC0")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "SOSCI/CCP2/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "CCP1/AN14/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "SCK/SCL/AN15/RC3")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SDI/SDA/AN16/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "SDO/AN17/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "TX/CK/AN18/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "RX/DT/AN19/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "AN20/RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "AN21/RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "AN22/RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "AN23/RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "AN24/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "AN25/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "AN26/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "AN27/RD7")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1526-IPT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 48.26 0)
		)
		(property "Value" "PIC16F1526-IPT"
			(at 5.08 45.72 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41458B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1526, 8192W FLASH, 768B SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP* QFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F1526-IPT_0_1")
		(symbol "PIC16F1526-IPT_1_1"
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "RA5/AN4/T3G")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA7/OSC1/CKLIN")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RB0/AN17/INT")
				(number "48")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RB1/AN18")
				(number "47")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RB2/AN19")
				(number "46")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RB3/AN20")
				(number "45")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RB4/AN21/T3CKI")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RB5/AN22/T1G/T3CKI")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RB6/ICSPLCK/ICDCLK")
				(number "42")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "RB7/ICSPDAT/ISCDAT")
				(number "37")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RC0/SOSCO/T1CKI")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RC1/SOSCI/CCP2")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RC2/CCP1")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RC3/SCK1/SCL1")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RC4/SDI1/SDA1")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RC5/SDO1")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RC6/TX1/CK1")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "RC7/RX1/DT1")
				(number "32")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "AVDD")
				(number "19")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 3.81)
				(name "AVSS")
				(number "20")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 3.81)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at -5.08 -48.26 90)
				(length 3.81)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 3.81)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 3.81)
				(name "VSS")
				(number "25")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 3.81)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 3.81)
				(name "VSS")
				(number "41")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 3.81)
				(name "VDD")
				(number "57")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 3.81)
				(name "VSS")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 3.81)
				(name "AN23/RD0")
				(number "58")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 3.81)
				(name "T5CKI/AN24/RD1")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "AN25/RD2")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "AN26/RD3")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "SDO2/RD4")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "SDI2/SDA2/RD5")
				(number "51")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "SCK2/SCL2/RD6")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "~{SS2}/RD7")
				(number "49")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "AN27/RE0")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "AN28/RE1")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "CCP10/AN29/RE2")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "CCP9/RE3")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "CCP8/RE4")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "CCP7/RE5")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "CCP6/RE6")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "CCP2/RE7")
				(number "59")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "VCAP/AN16/RF0")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "AN6/RF1")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "AN7/RF2")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "AN8/RF3")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "AN9/RF4")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "AN10/RF5")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "AN11/RF6")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "~{SS1}/AN5/RF7")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "CCP3/RG0")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "TX2/CK2/AN15/RG1")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 3.81)
				(name "RX2/DT2/AN14/RG2")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "CCP4/RG3")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 3.81)
				(name "CCP5/T5G/AN12/RG4")
				(number "8")
			)
			(pin input line
				(at 25.4 -40.64 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RG5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1527-IPT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 48.26 0)
		)
		(property "Value" "PIC16F1527-IPT"
			(at 5.08 45.72 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41458B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1527, 16384W FLASH, 1536B SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP* QFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F1527-IPT_0_1")
		(symbol "PIC16F1527-IPT_1_1"
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "RA2/AN2")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "RA5/AN4/T3G")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA7/OSC1/CKLIN")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RB0/AN17/INT")
				(number "48")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RB1/AN18")
				(number "47")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RB2/AN19")
				(number "46")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RB3/AN20")
				(number "45")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RB4/AN21/T3CKI")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RB5/AN22/T1G/T3CKI")
				(number "43")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RB6/ICSPLCK/ICDCLK")
				(number "42")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "RB7/ICSPDAT/ISCDAT")
				(number "37")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RC0/SOSCO/T1CKI")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RC1/SOSCI/CCP2")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RC2/CCP1")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RC3/SCK1/SCL1")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RC4/SDI1/SDA1")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RC5/SDO1")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RC6/TX1/CK1")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "RC7/RX1/DT1")
				(number "32")
			)
			(pin power_in line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "AVDD")
				(number "19")
			)
			(pin power_in line
				(at -25.4 -38.1 0)
				(length 3.81)
				(name "AVSS")
				(number "20")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 3.81)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at -5.08 -48.26 90)
				(length 3.81)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 3.81)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 3.81)
				(name "VSS")
				(number "25")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 3.81)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 3.81)
				(name "VSS")
				(number "41")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 3.81)
				(name "VDD")
				(number "57")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 3.81)
				(name "VSS")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 3.81)
				(name "AN23/RD0")
				(number "58")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 3.81)
				(name "T5CKI/AN24/RD1")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "AN25/RD2")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "AN26/RD3")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "SDO2/RD4")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "SDI2/SDA2/RD5")
				(number "51")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "SCK2/SCL2/RD6")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "~{SS2}/RD7")
				(number "49")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "AN27/RE0")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "AN28/RE1")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "CCP10/AN29/RE2")
				(number "64")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "CCP9/RE3")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "CCP8/RE4")
				(number "62")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "CCP7/RE5")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "CCP6/RE6")
				(number "60")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "CCP2/RE7")
				(number "59")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "VCAP/AN16/RF0")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "AN6/RF1")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "AN7/RF2")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "AN8/RF3")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "AN9/RF4")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "AN10/RF5")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "AN11/RF6")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "~{SS1}/AN5/RF7")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "CCP3/RG0")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "TX2/CK2/AN15/RG1")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -33.02 180)
				(length 3.81)
				(name "RX2/DT2/AN14/RG2")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "CCP4/RG3")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 -38.1 180)
				(length 3.81)
				(name "CCP5/T5G/AN12/RG4")
				(number "8")
			)
			(pin input line
				(at 25.4 -40.64 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RG5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F15323-xSL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.192 16.256 0)
		)
		(property "Value" "PIC16F15323-xSL"
			(at 9.652 -16.51 0)
		)
		(property "Footprint" "Package_SO:SO-14_3.9x8.65mm_P1.27mm"
			(at 1.016 -2.032 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/PIC16_L_F15313_23_Data_Sheet_40001897C.pdf"
			(at -0.254 2.032 0)
		)
		(property "Description" "8-bit Low Power Microcontroller, 2KB Flash, 256B SRAM, SOIC-14"
			(at 0 -4.064 0)
		)
		(property "ki_keywords" "8-bit microcontroller low power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*3.9x8.65mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F15323-xSL_0_1")
		(symbol "PIC16F15323-xSL_1_1"
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "~{MCLR}/VPP/RA3")
				(number "4")
				(alternate "IOCA3" input line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "13")
				(alternate "ANA0" input line)
				(alternate "C1IN0+" input line)
				(alternate "DAC1OUT" output line)
				(alternate "IOCA0" input line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "12")
				(alternate "ANA1" input line)
				(alternate "C1IN0-" input line)
				(alternate "C2IN0-" input line)
				(alternate "DAC1REF+" input line)
				(alternate "IOCA1" input line)
				(alternate "T0CKI" input line)
				(alternate "VREF+" input line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "RA2")
				(number "11")
				(alternate "ANA2" input line)
				(alternate "CWG1IN" input line)
				(alternate "INT" input line)
				(alternate "IOCA2" input line)
				(alternate "ZCD1" input line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RA4")
				(number "3")
				(alternate "ANA4" input line)
				(alternate "CLKOUT" output line)
				(alternate "IOCA4" input line)
				(alternate "OSC2" passive line)
				(alternate "T1G" input line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RA5")
				(number "2")
				(alternate "ANA5" input line)
				(alternate "CLCIN3" input line)
				(alternate "CLKIN" input line)
				(alternate "EIN" input line)
				(alternate "IOCA5" input line)
				(alternate "OSC1" passive line)
				(alternate "T1CKI" input line)
				(alternate "T2IN" input line)
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RC0")
				(number "10")
				(alternate "ANC0" input line)
				(alternate "C2IN0+" input line)
				(alternate "IOCC0" input line)
				(alternate "SCK1" bidirectional line)
				(alternate "SCL1" open_collector line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RC1")
				(number "9")
				(alternate "ANC1" input line)
				(alternate "C1IN1-" input line)
				(alternate "C2IN1-" input line)
				(alternate "CLCIN2" input line)
				(alternate "IOCC1" input line)
				(alternate "SDA1" open_collector line)
				(alternate "SDI1" input line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RC2")
				(number "8")
				(alternate "ANC2" input line)
				(alternate "C1IN2-" input line)
				(alternate "C2IN2-" input line)
				(alternate "IOCC2" input line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "RC3")
				(number "7")
				(alternate "ANC3" input line)
				(alternate "C1IN3-" input line)
				(alternate "C2IN3-" input line)
				(alternate "CCP2" bidirectional line)
				(alternate "CLCIN0" input line)
				(alternate "IOCC3" input line)
				(alternate "~{SS1}" input line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RC4")
				(number "6")
				(alternate "ANC4" input line)
				(alternate "CK1" bidirectional line)
				(alternate "CLCIN1" input line)
				(alternate "IOCC4" input line)
				(alternate "TX1" output line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RC5")
				(number "5")
				(alternate "ANC5" input line)
				(alternate "CCP1" bidirectional line)
				(alternate "DT1" bidirectional line)
				(alternate "IOCC5" input line)
				(alternate "RX1" input line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F15356-xML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 16.51 -24.13 0)
		)
		(property "Value" "PIC16F15356-xML"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at -1.27 11.43 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 22.86 2.54 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, QFN-28(6x6mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*6x6mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F15356-xML_0_0"
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "PAD")
				(number "29")
			)
		)
		(symbol "PIC16F15356-xML_0_1")
		(symbol "PIC16F15356-xML_1_1"
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "RE3/~{MCLR}/VPP")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "RC0")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "RC1")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "RC2")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "RC3")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "RC4")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "RC5")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "RC6")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "RC7")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "RA0")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "RA1")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "RA6")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "RA7")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "RB0")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "RB1")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "RB2")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "RB3")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "RB4")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "RB5")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "RB6/ICSPCLK")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "RB7/ICSPDAT")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F15356-xMV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 16.51 -24.13 0)
		)
		(property "Value" "PIC16F15356-xMV"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.4mm_EP2.3x2.3mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 22.86 2.54 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, QFN-28(4x4mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F15356-xMV_0_0"
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "PAD")
				(number "29")
			)
		)
		(symbol "PIC16F15356-xMV_0_1")
		(symbol "PIC16F15356-xMV_1_1"
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "RE3/~{MCLR}/VPP")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "RC0")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "RC1")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "RC2")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "RC3")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "RC4")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "RC5")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "RC6")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "RC7")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "RA0")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "RA1")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "RA6")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "RA7")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "RB0")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "RB1")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "RB2")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "RB3")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "RB4")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "RB5")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "RB6/ICSPCLK")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "RB7/ICSPDAT")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F15356-xSO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 17.78 -24.13 0)
		)
		(property "Value" "PIC16F15356-xSO"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at -21.59 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at -21.59 12.7 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*.5x17.9mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F15356-xSO_0_1")
		(symbol "PIC16F15356-xSO_1_1"
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "VPP/~{MCLR}/RE3")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RC0")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RC2")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RC3")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RC4")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RC5")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RC6")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RC7")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RA6")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RA7")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RB6/ICSPCLK")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RB7/ICSPDAT")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F15356-xSP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 17.78 -24.13 0)
		)
		(property "Value" "PIC16F15356-xSP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at -20.32 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at -20.32 12.7 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F15356-xSP_0_1")
		(symbol "PIC16F15356-xSP_1_1"
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "VPP/~{MCLR}/RE3")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RC0")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RC2")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RC3")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RC4")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RC5")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RC6")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RC7")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RA6")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RA7")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RB6/ICSPCLK")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RB7/ICSPDAT")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F15356-xSS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 17.78 -24.13 0)
		)
		(property "Value" "PIC16F15356-xSS"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at -21.59 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at -21.59 12.7 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F15356-xSS_0_1")
		(symbol "PIC16F15356-xSS_1_1"
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "VPP/~{MCLR}/RE3")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RC0")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RC2")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RC3")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RC4")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RC5")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RC6")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RC7")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RA6")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RA7")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RB6/ICSPCLK")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RB7/ICSPDAT")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F15375-xML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16F15375-xML"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 29.21 0)
		)
		(property "Description" "8KW FLASH, 1024B SRAM, QFN-44(8x8mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*8x8mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F15375-xML_0_0"
			(pin no_connect line
				(at -17.78 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "31")
			)
			(pin no_connect line
				(at -17.78 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at -17.78 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "29")
			)
			(pin no_connect line
				(at -17.78 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "PAD")
				(number "45")
			)
		)
		(symbol "PIC16F15375-xML_0_1")
		(symbol "PIC16F15375-xML_1_1"
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "VPP/MCLR/RE3")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "RE2")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "RE1")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "RE0")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RD0")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RD1")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RD2")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RD3")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "RD4")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "RD5")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "RD6")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "RD7")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "RA1")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "RA2")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "RA3")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "RA4")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA5")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA6")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA7")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RB0")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RB1")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RB2")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RB3")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RB4")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB5")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RB6/ICSPCLK")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RB7/ICSPDAT")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RC0")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RC3")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "RC7")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F15375-xMV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16F15375-xMV"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-40-1EP_5x5mm_P0.4mm_EP3.8x3.8mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 31.75 0)
		)
		(property "Description" "8KW FLASH, 1024B SRAM, QFN-40(5x5mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F15375-xMV_0_0"
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "PAD")
				(number "41")
			)
		)
		(symbol "PIC16F15375-xMV_0_1")
		(symbol "PIC16F15375-xMV_1_1"
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "VPP/MCLR/RE3")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "RE2")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "RE1")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "RE0")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RD0")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RD1")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RD2")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RD3")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "RD4")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "RD5")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "RD6")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "RD7")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "27")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "RA2")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "RA3")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "RA4")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA5")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA6")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA7")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RB0")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RB1")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RB2")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RB3")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RB4")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB5")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RB6/ICSPCLK")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RB7/ICSPDAT")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RC0")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RC1")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RC2")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RC3")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "RC4")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "RC5")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "RC6")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "RC7")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F15375-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16F15375-xP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 27.94 0)
		)
		(property "Description" "8KW FLASH, 1024B SRAM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*15.24mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F15375-xP_0_1")
		(symbol "PIC16F15375-xP_1_1"
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "VPP/MCLR/RE3")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "RE2")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "RE1")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "RE0")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RD0")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RD1")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RD2")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RD3")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "RD4")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "RD5")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "RD6")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "RD7")
				(number "30")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA6")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA7")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RB0")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RB1")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RB2")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RB3")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RB4")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB5")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RB6/ICSPCLK")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RB7/ICSPDAT")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "RC7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F15375-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16F15375-xPT"
			(at 0 0 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 30.48 0)
		)
		(property "Description" "8KW FLASH, 1024B SRAM, TQFP-44(10x10mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F15375-xPT_0_0"
			(pin no_connect line
				(at -17.78 7.62 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at -17.78 5.08 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -17.78 2.54 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at -17.78 0 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
		)
		(symbol "PIC16F15375-xPT_0_1")
		(symbol "PIC16F15375-xPT_1_1"
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "VPP/MCLR/RE3")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "RE2")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "RE1")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "RE0")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RD0")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RD1")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RD2")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RD3")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "RD4")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "RD5")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "RD6")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "RD7")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "RA1")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "RA2")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "RA3")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "RA4")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA5")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA6")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA7")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RB0")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RB1")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RB2")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RB3")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RB4")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB5")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RB6/ICSPCLK")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RB7/ICSPDAT")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RC0")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RC3")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "RC7")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F15386-xMV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16F15386-xMV"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.6x4.6mm"
			(at 50.8 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 38.1 6.35 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, QFN-48(6x6mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*6x6mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F15386-xMV_0_0"
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RD5")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RD6")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 2.54)
				(name "PAD")
				(number "49")
			)
		)
		(symbol "PIC16F15386-xMV_0_1")
		(symbol "PIC16F15386-xMV_1_1"
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "VPP/~{MCLR}/RE3")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "RE2")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "RE1")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "RE0")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RD0")
				(number "42")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RD1")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RD2")
				(number "44")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RD3")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD4")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RD7")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RF0")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RF1")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RF2")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RF3")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "RF4")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "RF5")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "RF6")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "RF7")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "RA0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "RA1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "RA2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "RA3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "RA4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA6")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA7")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RB0")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RB1")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RB2")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RB3")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RB4")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB5")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "ICSPCLK/RB6")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "ICSPDAT/RB7")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RC0")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RC2")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RC3")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "RC4")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "RC5")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "RC6")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "RC7")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F15386-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16F15386-xPT"
			(at 0 0 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 39.37 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 38.1 7.62 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, TQFP-48(7x7mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F15386-xPT_0_0"
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RD5")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RD6")
				(number "4")
			)
		)
		(symbol "PIC16F15386-xPT_0_1")
		(symbol "PIC16F15386-xPT_1_1"
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "VPP/~{MCLR}/RE3")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "RE2")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "RE1")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "RE0")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RD0")
				(number "42")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RD1")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RD2")
				(number "44")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RD3")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "RD4")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RD7")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RF0")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RF1")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RF2")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RF3")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "RF4")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "RF5")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "RF6")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "RF7")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "RA0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "RA1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "RA2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "RA3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "RA4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA6")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA7")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RB0")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RB1")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RB2")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RB3")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RB4")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB5")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "ICSPCLK/RB6")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "ICSPDAT/RB7")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RC0")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RC2")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RC3")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "RC4")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "RC5")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "RC6")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "RC7")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1619-xGZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 19.05 0)
		)
		(property "Value" "PIC16F1619-xGZ"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-20-1EP_4x4mm_P0.5mm_EP2.8x2.8mm"
			(at 3.81 -21.59 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001770D.pdf"
			(at 6.35 -13.97 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 14KB Flash, 1KB RAM, 1K High Endurance Flash (EEPROM), UQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F1619-xGZ_0_0"
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "EP")
				(number "21")
			)
		)
		(symbol "PIC16F1619-xGZ_0_1")
		(symbol "PIC16F1619-xGZ_1_1"
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "RB4")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RB5")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RB6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RB7")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RA2")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RA4")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RA5")
				(number "19")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "RC5")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1619-xML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 19.05 0)
		)
		(property "Value" "PIC16F1619-xML"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 3.81 -17.78 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001770D.pdf"
			(at 5.08 -13.97 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 14KB Flash, 1KB RAM, 1K High Endurance Flash (EEPROM), QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F1619-xML_0_0"
			(pin passive line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "EP")
				(number "21")
			)
		)
		(symbol "PIC16F1619-xML_0_1")
		(symbol "PIC16F1619-xML_1_1"
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "RB4")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RB5")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RB6")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RB7")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RA2")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RA4")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RA5")
				(number "19")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "RC5")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1619-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 19.05 0)
		)
		(property "Value" "PIC16F1619-xP"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 3.81 -17.78 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001770D.pdf"
			(at 5.08 -13.97 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 14KB Flash, 1KB RAM, 1K High Endurance Flash (EEPROM), PDIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F1619-xP_0_1")
		(symbol "PIC16F1619-xP_1_1"
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RB7")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RA2")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RA5")
				(number "2")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1619-xSO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 19.05 0)
		)
		(property "Value" "PIC16F1619-xSO"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 3.81 -17.78 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001770D.pdf"
			(at 5.08 -13.97 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 14KB Flash, 1KB RAM, 1K High Endurance Flash (EEPROM), SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F1619-xSO_0_1")
		(symbol "PIC16F1619-xSO_1_1"
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RB7")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RA2")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RA5")
				(number "2")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1619-xSS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 19.05 0)
		)
		(property "Value" "PIC16F1619-xSS"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 3.81 -17.78 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001770D.pdf"
			(at 5.08 -13.97 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 14KB Flash, 1KB RAM, 1K High Endurance Flash (EEPROM), SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F1619-xSS_0_1")
		(symbol "PIC16F1619-xSS_1_1"
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RB7")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RA2")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RA5")
				(number "2")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1786-xML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 27.94 0)
		)
		(property "Value" "PIC16F1786-xML"
			(at 2.54 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 -32.004 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001637C.pdf"
			(at 0 -34.0106 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 16KB Flash, 1KB RAM, 256B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F1786-xML_0_1")
		(symbol "PIC16F1786-xML_1_1"
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RE3/~{MCLR}/V_{PP}")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RC0")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RC1")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RC2")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RC3")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RC4")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RC5")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RC6")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RC7")
				(number "15")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "V_{DD}")
				(number "17")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "V_{SS}")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA0")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA1")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RA6")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RA7")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB0")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RB1")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RB2")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "RB3")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RB4")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RB5")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "ICSPCLK/RB6")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "ICSPDAT/RB7")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1786-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 40.64 0)
		)
		(property "Value" "PIC16F1786-xP"
			(at 2.54 38.1 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -43.434 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001637C.pdf"
			(at 0 -45.4406 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 16KB Flash, 1KB RAM, 256B EEPROM, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F1786-xP_0_1")
		(symbol "PIC16F1786-xP_1_1"
			(pin input line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "RE3/~{MCLR}/V_{PP}")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "RE2")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "RE1")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "RE0")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RD0")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RD1")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RD2")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RD3")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "RD4")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "RD5")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "RD6")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "RD7")
				(number "30")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "V_{DD}")
				(number "11")
			)
			(pin passive line
				(at 0 38.1 270)
				(length 2.54)
				(hide yes)
				(name "V_{DD}")
				(number "32")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 2.54)
				(name "V_{SS}")
				(number "12")
			)
			(pin passive line
				(at 0 -38.1 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA6")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA7")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RB0")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RB1")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RB2")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RB3")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RB4")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB5")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "ICSPCLK/RB6")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "ICSPDAT/RB7")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "RC7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1786-xSP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 27.94 0)
		)
		(property "Value" "PIC16F1786-xSP"
			(at 2.54 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 -32.004 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001637C.pdf"
			(at 0 -34.0106 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 16KB Flash, 1KB RAM, 256B EEPROM, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F1786-xSP_0_1")
		(symbol "PIC16F1786-xSP_1_1"
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RE3/~{MCLR}/V_{PP}")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RC0")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RC2")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RC3")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RC4")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RC5")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RC6")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RC7")
				(number "18")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "V_{DD}")
				(number "20")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "V_{SS}")
				(number "19")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "V_{SS}")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RA6")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RA7")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "ICSPCLK/RB6")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "ICSPDAT/RB7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1829-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 22.86 0)
		)
		(property "Value" "PIC16F1829-IML"
			(at -24.13 20.32 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41440C.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "Flash-Based, 8-Bit CMOS Microcontrollers, QFN"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F1829-IML_0_1")
		(symbol "PIC16F1829-IML_1_1"
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 3.81)
				(name "RA0/ICSPDAT")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "RA1/ICSPCLK")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "RA2")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "RA3/MCLR/VPP")
				(number "1")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RA4")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RA5")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB4")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB5")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "RB6")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "RB7")
				(number "7")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "RC7")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "RC6")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "RC5")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "RC4")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "RC3")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "RC2")
				(number "11")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "RC0")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1829-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 22.86 0)
		)
		(property "Value" "PIC16F1829-IP"
			(at -24.13 20.32 0)
		)
		(property "Footprint" ""
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41440C.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "Flash-Based, 8-Bit CMOS Microcontrollers, PDIP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F1829-IP_0_1")
		(symbol "PIC16F1829-IP_1_1"
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 3.81)
				(name "RA0/ICSPDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "RA1/ICSPCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "RA2")
				(number "17")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "RA3/MCLR/VPP")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RA5")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "RB7")
				(number "10")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "RC7")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "RC0")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1829LIN-ESS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 19.05 0)
		)
		(property "Value" "PIC16F1829LIN-ESS"
			(at -26.67 16.51 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41673A.pdf"
			(at 0 -46.99 0)
		)
		(property "Description" "Flash-Based, 8-Bit CMOS Microcontrollers with integrated voltage regulator and LIN transceiver"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS microcontroller regulator LIN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F1829LIN-ESS_0_1")
		(symbol "PIC16F1829LIN-ESS_1_1"
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "RA0/ICSPDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "RA1/ICSPCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "RA2")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RA3/MCLR")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RA5")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "/FAULT")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "LBUS")
				(number "9")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 2.54)
				(name "VBAT")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 2.54)
				(name "LINVSS")
				(number "8")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_out line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "VREG")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "RC0")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18324-xSL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 10.16 0)
		)
		(property "Value" "PIC16F18324-xSL"
			(at 1.27 10.16 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/40001800c.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "PIC16F18324, 4096W FLASH, 512B SRAM, 256B EEPROM, SOIC14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18324-xSL_1_1"
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "RA0")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "RA1")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "RA2")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "RA3/~{MCLR}")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "RA5")
				(number "2")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "RC0")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "RC2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "RC5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18325-ISL"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -58.42 15.24 0)
		)
		(property "Value" "PIC16F18325-ISL"
			(at -58.42 12.7 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/40001795b.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "PIC16F18325, 8192W FLASH, 1024B SRAM, SOIC14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18325-ISL_1_1"
			(pin bidirectional line
				(at -63.5 7.62 0)
				(length 3.81)
				(name "RA0/ANA0/C1IN0+/DAC1OUT/~{SS2}/ICSPDAT")
				(number "13")
			)
			(pin bidirectional line
				(at -63.5 5.08 0)
				(length 3.81)
				(name "RA1/ANA1/Vref+/C1IN0-/C2IN0-/DAC1Ref+/ICSPCLK")
				(number "12")
			)
			(pin bidirectional line
				(at -63.5 2.54 0)
				(length 3.81)
				(name "RA2/ANA2/Vref-/DAC1Ref-/T0CKI/CCP3/CWG1IN/CWG2IN")
				(number "11")
			)
			(pin bidirectional line
				(at -63.5 0 0)
				(length 3.81)
				(name "RA3/~{MCLR}/VPP")
				(number "4")
			)
			(pin bidirectional line
				(at -63.5 -2.54 0)
				(length 3.81)
				(name "RA4/ANA4/T1G/SOSCO/CLKOUT/OSC2")
				(number "3")
			)
			(pin bidirectional line
				(at -63.5 -5.08 0)
				(length 3.81)
				(name "RA5/ANA5/T1CKI/SOSCIN/SOSCI/CLCIN3/CLKIN/OSC1")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 63.5 7.62 180)
				(length 3.81)
				(name "SCL1/SCK/T5CKI/C2IN0+/ANC0/RC0")
				(number "10")
			)
			(pin bidirectional line
				(at 63.5 5.08 180)
				(length 3.81)
				(name "CLCIN2/SDA1/SDI/CCP4/C2IN1-/C1IN1-/ANC1/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 63.5 2.54 180)
				(length 3.81)
				(name "MDCIN1/C2IN2-/C1IN2-/ANC2/RC2")
				(number "8")
			)
			(pin bidirectional line
				(at 63.5 0 180)
				(length 3.81)
				(name "CLCIN0/~{SS1}/CCP2/T5G/MDMIN/C2IN3-/C1IN3-/ANC3/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 63.5 -2.54 180)
				(length 3.81)
				(name "CLCIN1/SCL2/SCK2/T3G/ANC4/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 63.5 -5.08 180)
				(length 3.81)
				(name "DT/RX/SDA2/SDI2/CCP1/T3CKI/MDCIN2/ANC5/RC5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18325-xGZ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "PIC16F18325-xGZ"
			(at 10.16 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-20-1EP_4x4mm_P0.5mm_EP2.8x2.8mm"
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001795E.pdf"
			(at 0 0 0)
		)
		(property "Description" "8192W FLASH, 1024B SRAM, 256B EEPROM, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18325-xGZ_1_1"
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RA2")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "RA4")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "RA5")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "RB4")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "RB5")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "RB6")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "RB7")
				(number "7")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "17")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "RC0")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "RC2")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "RC3")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "RC4")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "RC5")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "RC6")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "RC7")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18325-xJQ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 11.43 0)
		)
		(property "Value" "PIC16F18325-xJQ"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-16-1EP_4x4mm_P0.65mm_EP2.6x2.6mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001795E.pdf"
			(at 0 0 0)
		)
		(property "Description" "8192W FLASH, 1024B SRAM, 256B EEPROM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1EP*4x4mm*P0.65mm*EP2.6x2.6mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18325-xJQ_0_1")
		(symbol "PIC16F18325-xJQ_1_1"
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "RA2")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "RA3/~{MCLR}")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "RA4")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "RA5")
				(number "1")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 2.54)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -10.16 90)
				(length 2.54)
				(name "VSS")
				(number "13")
			)
			(pin no_connect line
				(at 5.08 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at 7.62 -7.62 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "RC0")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "RC1")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "RC2")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "RC3")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "RC4")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "RC5")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18344-GZ"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 16.51 0)
		)
		(property "Value" "PIC16F18344-GZ"
			(at 9.398 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-20-1EP_4x4mm_P0.5mm_EP2.8x2.8mm"
			(at 1.778 -20.574 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001839B.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "4096W FLASH, 512B RAM, 256B EEPROM, UQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*UQFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18344-GZ_0_1")
		(symbol "PIC16F18344-GZ_1_1"
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RA2")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RA4")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "RA5")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RB4")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RB5")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RB6")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RB7")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RC5")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18344-P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 16.51 0)
		)
		(property "Value" "PIC16F18344-P"
			(at 9.652 16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 -19.812 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/40001800a.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "4096W FLASH, 512B RAM, 256B EEPROM, PDIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18344-P_0_1")
		(symbol "PIC16F18344-P_1_1"
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RA2")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "RA5")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RB7")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18344-SO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 16.51 0)
		)
		(property "Value" "PIC16F18344-SO"
			(at 8.89 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -19.812 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/40001800a.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "4096W FLASH, 512B RAM, 256B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18344-SO_0_1")
		(symbol "PIC16F18344-SO_1_1"
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RA2")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "RA5")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RB7")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18344-SS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 16.51 0)
		)
		(property "Value" "PIC16F18344-SS"
			(at 9.652 16.51 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 -19.812 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/40001800a.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "4096W FLASH, 512B RAM, 256B EEPROM, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18344-SS_0_1")
		(symbol "PIC16F18344-SS_1_1"
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RA2")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "RA5")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RB7")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18346-GZ"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 16.51 0)
		)
		(property "Value" "PIC16F18346-GZ"
			(at 9.398 16.51 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-20-1EP_4x4mm_P0.5mm_EP2.8x2.8mm"
			(at 1.778 -20.574 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001839B.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "16384W FLASH, 2048B RAM, 256B EEPROM, UQFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*UQFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18346-GZ_0_1")
		(symbol "PIC16F18346-GZ_1_1"
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RA2")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RA4")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "RA5")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RB4")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RB5")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RB6")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RB7")
				(number "7")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RC5")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18346-P"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 16.51 0)
		)
		(property "Value" "PIC16F18346-P"
			(at 9.652 16.51 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 -19.812 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001839B.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "16384W FLASH, 2048B RAM, 256B EEPROM, PDIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18346-P_0_1")
		(symbol "PIC16F18346-P_1_1"
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RA2")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "RA5")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RB7")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18346-SO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 16.51 0)
		)
		(property "Value" "PIC16F18346-SO"
			(at 9.144 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at -0.254 -20.066 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001839B.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "16384W FLASH, 2048B RAM, 256B EEPROM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18346-SO_0_1")
		(symbol "PIC16F18346-SO_1_1"
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RA2")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "RA5")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RB7")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18346-SS_0"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 16.51 0)
		)
		(property "Value" "PIC16F18346-SS_0"
			(at 9.398 16.51 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 2.286 -19.304 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001839B.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "16384W FLASH, 2048B RAM, 256B EEPROM, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18346-SS_0_0_1")
		(symbol "PIC16F18346-SS_0_1_1"
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RA0/ICSPDAT")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RA1/ICSPCLK")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RA2")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RA3/~{MCLR}/VPP")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "RA5")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RB7")
				(number "10")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18854-xSO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 27.94 0)
		)
		(property "Value" "PIC16F18854-xSO"
			(at 10.16 25.4 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 1.27 -27.94 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF18855-75-Data-Sheet-40001802F.pdf"
			(at 15.24 -7.62 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 7KB Flash, 512B RAM 256B EEPROM, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power CRC DSM  ADC^2 CLC PLL 32MHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18854-xSO_0_0"
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "19")
			)
		)
		(symbol "PIC16F18854-xSO_0_1")
		(symbol "PIC16F18854-xSO_1_1"
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RE3/~{MCLR}/VPP")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RC0")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RC2")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RC3")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RC4")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RC5")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RC6")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RC7")
				(number "18")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RA6")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RA7")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RB6/ICSPCLK")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RB7/ICSPDAT")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F18855-xMV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 26.67 0)
		)
		(property "Value" "PIC16F18855-xMV"
			(at 10.16 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-28-1EP_4x4mm_P0.4mm_EP2.35x2.35mm"
			(at 1.27 -27.94 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF18855-75-Data-Sheet-40001802F.pdf"
			(at 15.24 -7.62 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 14KB Flash, 1KB RAM 256B EEPROM, UQFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power CRC DSM  ADC^2 CLC PLL 32MHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1EP*4x4mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F18855-xMV_0_0"
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "29")
			)
		)
		(symbol "PIC16F18855-xMV_0_1")
		(symbol "PIC16F18855-xMV_1_1"
			(pin input line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RE3/~{MCLR}/VPP")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RC0")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RC1")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RC2")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RC3")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RC4")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RC5")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RC6")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RC7")
				(number "15")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RA0")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RA1")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RA6")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RA7")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RB0")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RB1")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RB2")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "RB3")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RB4")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RB5")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RB6/ICSPCLK")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RB7/ICSPDAT")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F19195-x5LX"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16F19195-x5LX"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "8kW FLASH, 1kB RAM, 256B EEPROM, VQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F19195-x5LX_0_1")
		(symbol "PIC16F19195-x5LX_1_1"
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 2.54)
				(name "RA0/SEG33")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "RA1/SEG18")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "RA2/SEG34")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "RA3/SEG35")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "RA4/SEG14")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "RA5")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "RA6/SEG36")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "RA7/SEG37")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RB0/SEG30")
				(number "48")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "RB1/SEG8")
				(number "47")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "RB2/SEG9")
				(number "46")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RB3/SEG10")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RB4/SEG11")
				(number "44")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RB5/SEG29")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RB6/SEG38/ICSPCLK")
				(number "42")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RB7/SEG39/ICSPDAT")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RC0")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RC1")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RC2/SEG13")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RC3/SEG17")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RC4/SEG16")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RC5/SEG12")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RC6/SEG27")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RC7/SEG28")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "RD0/SEG0")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "RD1/SEG1")
				(number "55")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "RD2/SEG2")
				(number "54")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "RD3/SEG3")
				(number "53")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "RD4/SEG4")
				(number "52")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "RD5/SEG5")
				(number "51")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "RD6/SEG6")
				(number "50")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "RD7/SEG7")
				(number "49")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "41")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "65")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "VLCD1/RE0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "VLCD2/RE1")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "COM0/RE3")
				(number "63")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "COM1/RE4")
				(number "62")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "COM2/RE5")
				(number "61")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "COM3/RE6")
				(number "60")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "SEG31/RE7")
				(number "59")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "SEG41/RF0")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "SEG19/RF1")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "SEG20/RF2")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "SEG21/RF3")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "SEG22/RF4")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "SEG23/RF5")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "SEG24/RF6")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "SEG25/RF7")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "SEG42/RG0")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "SEG43/RG1")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "SEG44/RG2")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "SEG45/RG3")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "SEG26/RG4")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "VPP/~{MCLR}/RG5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "COM6/RG6")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "COM7/SEG15/RG7")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "COM4/RH0")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "COM5/RH1")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "CFLY1/SEG32/RH2")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "CFLY2/SEG40/RH3")
				(number "56")
			)
			(pin input line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "VLCD3")
				(number "64")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F19195-xMR"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16F19195-xMR"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "8kW FLASH, 1kB RAM, 256B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F19195-xMR_0_1")
		(symbol "PIC16F19195-xMR_1_1"
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 2.54)
				(name "RA0/SEG33")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "RA1/SEG18")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "RA2/SEG34")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "RA3/SEG35")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "RA4/SEG14")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "RA5")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "RA6/SEG36")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "RA7/SEG37")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RB0/SEG30")
				(number "48")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "RB1/SEG8")
				(number "47")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "RB2/SEG9")
				(number "46")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RB3/SEG10")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RB4/SEG11")
				(number "44")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RB5/SEG29")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RB6/SEG38/ICSPCLK")
				(number "42")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RB7/SEG39/ICSPDAT")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RC0")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RC1")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RC2/SEG13")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RC3/SEG17")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RC4/SEG16")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RC5/SEG12")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RC6/SEG27")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RC7/SEG28")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "RD0/SEG0")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "RD1/SEG1")
				(number "55")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "RD2/SEG2")
				(number "54")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "RD3/SEG3")
				(number "53")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "RD4/SEG4")
				(number "52")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "RD5/SEG5")
				(number "51")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "RD6/SEG6")
				(number "50")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "RD7/SEG7")
				(number "49")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "41")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "65")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "VLCD1/RE0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "VLCD2/RE1")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "COM0/RE3")
				(number "63")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "COM1/RE4")
				(number "62")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "COM2/RE5")
				(number "61")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "COM3/RE6")
				(number "60")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "SEG31/RE7")
				(number "59")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "SEG41/RF0")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "SEG19/RF1")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "SEG20/RF2")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "SEG21/RF3")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "SEG22/RF4")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "SEG23/RF5")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "SEG24/RF6")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "SEG25/RF7")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "SEG42/RG0")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "SEG43/RG1")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "SEG44/RG2")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "SEG45/RG3")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "SEG26/RG4")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "VPP/~{MCLR}/RG5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "COM6/RG6")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "COM7/SEG15/RG7")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "COM4/RH0")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "COM5/RH1")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "CFLY1/SEG32/RH2")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "CFLY2/SEG40/RH3")
				(number "56")
			)
			(pin input line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "VLCD3")
				(number "64")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F19195-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16F19195-xPT"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "8kW FLASH, 1kB RAM, 256B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC16F19195-xPT_0_1")
		(symbol "PIC16F19195-xPT_1_1"
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 2.54)
				(name "RA0/SEG33")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "RA1/SEG18")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "RA2/SEG34")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "RA3/SEG35")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "RA4/SEG14")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "RA5")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "RA6/SEG36")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "RA7/SEG37")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RB0/SEG30")
				(number "48")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "RB1/SEG8")
				(number "47")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "RB2/SEG9")
				(number "46")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RB3/SEG10")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RB4/SEG11")
				(number "44")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RB5/SEG29")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RB6/SEG38/ICSPCLK")
				(number "42")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RB7/SEG39/ICSPDAT")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RC0")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RC1")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "RC2/SEG13")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RC3/SEG17")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "RC4/SEG16")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RC5/SEG12")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "RC6/SEG27")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "RC7/SEG28")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "RD0/SEG0")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "RD1/SEG1")
				(number "55")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "RD2/SEG2")
				(number "54")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "RD3/SEG3")
				(number "53")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "RD4/SEG4")
				(number "52")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "RD5/SEG5")
				(number "51")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "RD6/SEG6")
				(number "50")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "RD7/SEG7")
				(number "49")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "41")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDD")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 2.54)
				(name "VLCD1/RE0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "VLCD2/RE1")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "COM0/RE3")
				(number "63")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "COM1/RE4")
				(number "62")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "COM2/RE5")
				(number "61")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "COM3/RE6")
				(number "60")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "SEG31/RE7")
				(number "59")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "SEG41/RF0")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "SEG19/RF1")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "SEG20/RF2")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "SEG21/RF3")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "SEG22/RF4")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "SEG23/RF5")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "SEG24/RF6")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "SEG25/RF7")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "SEG42/RG0")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "SEG43/RG1")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "SEG44/RG2")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "SEG45/RG3")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "SEG26/RG4")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "VPP/~{MCLR}/RG5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "COM6/RG6")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "COM7/SEG15/RG7")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "COM4/RH0")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "COM5/RH1")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "CFLY1/SEG32/RH2")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "CFLY2/SEG40/RH3")
				(number "56")
			)
			(pin input line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "VLCD3")
				(number "64")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1934-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -41.91 35.56 0)
		)
		(property "Value" "PIC16F1934-IML"
			(at -41.91 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41364E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F193XLF193X - Flash-Based, 8-Bit CMOS Microcontrollers, QFN-44"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*"
			(at 0 0 0)
		)
		(symbol "PIC16F1934-IML_0_1")
		(symbol "PIC16F1934-IML_1_1"
			(pin no_connect line
				(at -45.72 27.94 0)
				(length 3.81)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -45.72 25.4 0)
				(length 3.81)
				(name "NC")
				(number "29")
			)
			(pin bidirectional line
				(at -45.72 20.32 0)
				(length 3.81)
				(name "RA0/AN0/C12IN0-/C2OUT/SRNQ/SS/VCAP/SEG12")
				(number "19")
			)
			(pin bidirectional line
				(at -45.72 17.78 0)
				(length 3.81)
				(name "RA1/AN1/C12IN1-/SEG7")
				(number "20")
			)
			(pin bidirectional line
				(at -45.72 15.24 0)
				(length 3.81)
				(name "RA2/AN2/C2IN+/Vref-/DACOUT/COM2")
				(number "21")
			)
			(pin bidirectional line
				(at -45.72 12.7 0)
				(length 3.81)
				(name "RA3/AN3/C1IN+/Vref+/SEG15")
				(number "22")
			)
			(pin bidirectional line
				(at -45.72 10.16 0)
				(length 3.81)
				(name "RA4/C1OUT/CPS6/T0CKI/SRQ/SEG4")
				(number "23")
			)
			(pin bidirectional line
				(at -45.72 7.62 0)
				(length 3.81)
				(name "RA5/AN4/C2OUT/CPS7/SRNQ/SS/VCAP/SEG5")
				(number "24")
			)
			(pin bidirectional line
				(at -45.72 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT/VCAP/SEG1")
				(number "33")
			)
			(pin bidirectional line
				(at -45.72 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN/SEG2")
				(number "32")
			)
			(pin bidirectional line
				(at -45.72 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/CPS0/SRI/INT/SEG0")
				(number "9")
			)
			(pin bidirectional line
				(at -45.72 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/C12IN3-/CPS1/VLCD1")
				(number "10")
			)
			(pin bidirectional line
				(at -45.72 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/CPS2/VLCD2")
				(number "11")
			)
			(pin bidirectional line
				(at -45.72 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/C12IN2-/CPS3/CCP2/P2A/VLCD3")
				(number "12")
			)
			(pin bidirectional line
				(at -45.72 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/CPS4/COM0")
				(number "14")
			)
			(pin bidirectional line
				(at -45.72 -15.24 0)
				(length 3.81)
				(name "RB5/AN13/CPS5/CCP3/P3A/T1G/COM1")
				(number "15")
			)
			(pin bidirectional line
				(at -45.72 -17.78 0)
				(length 3.81)
				(name "RB6/ICSPCLK/ICDCLK/SEG14")
				(number "16")
			)
			(pin bidirectional line
				(at -45.72 -20.32 0)
				(length 3.81)
				(name "RB7/ICSPDAT/ICDDAT/SEG13")
				(number "17")
			)
			(pin bidirectional line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin bidirectional line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 45.72 27.94 180)
				(length 3.81)
				(name "P2B/T1CLKI/T1OSO/RC0")
				(number "34")
			)
			(pin bidirectional line
				(at 45.72 25.4 180)
				(length 3.81)
				(name "P2A/CCP2/T1OSI/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 45.72 22.86 180)
				(length 3.81)
				(name "SEG3/P1A/CCP1/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 45.72 20.32 180)
				(length 3.81)
				(name "SEG6/SCLK/SCL/RC3")
				(number "37")
			)
			(pin bidirectional line
				(at 45.72 17.78 180)
				(length 3.81)
				(name "SEG11/T1G/SDA/SDI/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 45.72 15.24 180)
				(length 3.81)
				(name "SEG10/SDO/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 45.72 12.7 180)
				(length 3.81)
				(name "SEG9/CK/TX/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 45.72 10.16 180)
				(length 3.81)
				(name "SEG8/DT/RX/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 45.72 5.08 180)
				(length 3.81)
				(name "COM3/CPS8/RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 45.72 2.54 180)
				(length 3.81)
				(name "CCP4/CPS9/RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 45.72 0 180)
				(length 3.81)
				(name "P2B/CPS10/RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 45.72 -2.54 180)
				(length 3.81)
				(name "SEG16/P2C/CPS11/RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 45.72 -5.08 180)
				(length 3.81)
				(name "SEG17/P2D/CPS12/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 45.72 -7.62 180)
				(length 3.81)
				(name "SEG18/P1B/CPS13/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 45.72 -10.16 180)
				(length 3.81)
				(name "SEG19/P1C/CPS14/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 45.72 -12.7 180)
				(length 3.81)
				(name "SEG20/P1D/CPS15/RD7")
				(number "5")
			)
			(pin bidirectional line
				(at 45.72 -17.78 180)
				(length 3.81)
				(name "SEG21/P3A/CCP3/AN5/RE0")
				(number "25")
			)
			(pin bidirectional line
				(at 45.72 -20.32 180)
				(length 3.81)
				(name "SEG22/P3B/AN6/RE1")
				(number "26")
			)
			(pin bidirectional line
				(at 45.72 -22.86 180)
				(length 3.81)
				(name "SEG23/CCP5/AN7/RE2")
				(number "27")
			)
			(pin bidirectional line
				(at 45.72 -25.4 180)
				(length 3.81)
				(name "RE3/MCLR/Vpp")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F1934-IPT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -41.91 35.56 0)
		)
		(property "Value" "PIC16F1934-IPT"
			(at -41.91 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41364E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F193XLF193X - Flash-Based, 8-Bit CMOS Microcontrollers, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*"
			(at 0 0 0)
		)
		(symbol "PIC16F1934-IPT_0_1")
		(symbol "PIC16F1934-IPT_1_1"
			(pin no_connect line
				(at -45.72 27.94 0)
				(length 3.81)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -45.72 25.4 0)
				(length 3.81)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -45.72 22.86 0)
				(length 3.81)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at -45.72 20.32 0)
				(length 3.81)
				(name "NC")
				(number "34")
			)
			(pin bidirectional line
				(at -45.72 15.24 0)
				(length 3.81)
				(name "RA0/AN0/C12IN0-/C2OUT/SRNQ/SS/VCAP/SEG12")
				(number "19")
			)
			(pin bidirectional line
				(at -45.72 12.7 0)
				(length 3.81)
				(name "RA1/AN1/C12IN1-/SEG7")
				(number "20")
			)
			(pin bidirectional line
				(at -45.72 10.16 0)
				(length 3.81)
				(name "RA2/AN2/C2IN+/Vref-/DACOUT/COM2")
				(number "21")
			)
			(pin bidirectional line
				(at -45.72 7.62 0)
				(length 3.81)
				(name "RA3/AN3/C1IN+/Vref+/SEG15")
				(number "22")
			)
			(pin bidirectional line
				(at -45.72 5.08 0)
				(length 3.81)
				(name "RA4/C1OUT/CPS6/T0CKI/SRQ/SEG4")
				(number "23")
			)
			(pin bidirectional line
				(at -45.72 2.54 0)
				(length 3.81)
				(name "RA5/AN4/C2OUT/CPS7/SRNQ/SS/VCAP/SEG5")
				(number "24")
			)
			(pin bidirectional line
				(at -45.72 0 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT/VCAP/SEG1")
				(number "31")
			)
			(pin bidirectional line
				(at -45.72 -2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN/SEG2")
				(number "30")
			)
			(pin bidirectional line
				(at -45.72 -7.62 0)
				(length 3.81)
				(name "RB0/AN12/CPS0/SRI/INT/SEG0")
				(number "8")
			)
			(pin bidirectional line
				(at -45.72 -10.16 0)
				(length 3.81)
				(name "RB1/AN10/C12IN3-/CPS1/VLCD1")
				(number "9")
			)
			(pin bidirectional line
				(at -45.72 -12.7 0)
				(length 3.81)
				(name "RB2/AN8/CPS2/VLCD2")
				(number "10")
			)
			(pin bidirectional line
				(at -45.72 -15.24 0)
				(length 3.81)
				(name "RB3/AN9/C12IN2-/CPS3/CCP2/P2A/VLCD3")
				(number "11")
			)
			(pin bidirectional line
				(at -45.72 -17.78 0)
				(length 3.81)
				(name "RB4/AN11/CPS4/COM0")
				(number "14")
			)
			(pin bidirectional line
				(at -45.72 -20.32 0)
				(length 3.81)
				(name "RB5/AN13/CPS5/CCP3/P3A/T1G/COM1")
				(number "15")
			)
			(pin bidirectional line
				(at -45.72 -22.86 0)
				(length 3.81)
				(name "RB6/ICSPCLK/ICDCLK/SEG14")
				(number "16")
			)
			(pin bidirectional line
				(at -45.72 -25.4 0)
				(length 3.81)
				(name "RB7/ICSPDAT/ICDDAT/SEG13")
				(number "17")
			)
			(pin bidirectional line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin bidirectional line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin bidirectional line
				(at 45.72 27.94 180)
				(length 3.81)
				(name "P2B/T1CKI/T1OSO/RC0")
				(number "32")
			)
			(pin bidirectional line
				(at 45.72 25.4 180)
				(length 3.81)
				(name "P2A/CCP2/T1OSI/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 45.72 22.86 180)
				(length 3.81)
				(name "SEG3/P1A/CCP1/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 45.72 20.32 180)
				(length 3.81)
				(name "SEG6/SCLK/SCL/RC3")
				(number "37")
			)
			(pin bidirectional line
				(at 45.72 17.78 180)
				(length 3.81)
				(name "SEG11/T1G/SDA/SDI/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 45.72 15.24 180)
				(length 3.81)
				(name "SEG10/SDO/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 45.72 12.7 180)
				(length 3.81)
				(name "SEG9/CK/TX/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 45.72 10.16 180)
				(length 3.81)
				(name "SEG8/DT/RX/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 45.72 5.08 180)
				(length 3.81)
				(name "COM3/CPS8/RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 45.72 2.54 180)
				(length 3.81)
				(name "CCP4/CPS9/RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 45.72 0 180)
				(length 3.81)
				(name "P2B/CPS10/RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 45.72 -2.54 180)
				(length 3.81)
				(name "SEG16/P2C/CPS11/RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 45.72 -5.08 180)
				(length 3.81)
				(name "SEG17/P2D/CPS12/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 45.72 -7.62 180)
				(length 3.81)
				(name "SEG18/P1B/CPS13/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 45.72 -10.16 180)
				(length 3.81)
				(name "SEG19/P1C/CPS14/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 45.72 -12.7 180)
				(length 3.81)
				(name "SEG20/P1D/CPS15/RD7")
				(number "5")
			)
			(pin bidirectional line
				(at 45.72 -17.78 180)
				(length 3.81)
				(name "SEG21/P3A/CCP3/AN5/RE0")
				(number "25")
			)
			(pin bidirectional line
				(at 45.72 -20.32 180)
				(length 3.81)
				(name "SEG22/P3B/AN6/RE1")
				(number "26")
			)
			(pin bidirectional line
				(at 45.72 -22.86 180)
				(length 3.81)
				(name "SEG23/CCP5/AN7/RE2")
				(number "27")
			)
			(pin bidirectional line
				(at 45.72 -25.4 180)
				(length 3.81)
				(name "RE3/MCLR/Vpp")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F505-IMG"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 12.7 0)
		)
		(property "Value" "PIC16F505-IMG"
			(at 2.54 10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F505, 1024W FLASH, 72B SRAM, QFN16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F505-IMG_0_1")
		(symbol "PIC16F505-IMG_1_1"
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "RC0")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "RC1")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "RC2")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "RC3")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "RC4")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "RC5/T0CKI")
				(number "4")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "ICSPDAT/RB0")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "ICSPCLK/RB1")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "RB2")
				(number "10")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RB3")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "CLKOUT/OSC2/RB4")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "CLKIN/OSC1/RB5")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F505-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 12.7 0)
		)
		(property "Value" "PIC16F505-IP"
			(at 5.08 10.16 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "1024W FLASH, 72B SRAM, DIP14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PDIP* DIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F505-IP_0_1")
		(symbol "PIC16F505-IP_1_1"
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "RC0")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "RC1")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "RC2")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "RC5/T0CKI")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "ICSPDAT/RB0")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "ICSPCLK/RB1")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "RB2")
				(number "11")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RB3")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "CLKOUT/OSC2/RB4")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "CLKIN/OSC1/RB5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F505-ISL"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 12.7 0)
		)
		(property "Value" "PIC16F505-ISL"
			(at 3.81 10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F505, 1024W FLASH, 72B SRAM, SO14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO* SOIC*"
			(at 0 0 0)
		)
		(symbol "PIC16F505-ISL_0_1")
		(symbol "PIC16F505-ISL_1_1"
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "RC0")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "RC1")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "RC2")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "RC5/T0CKI")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "ICSPDAT/RB0")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "ICSPCLK/RB1")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "RB2")
				(number "11")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RB3")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "CLKOUT/OSC2/RB4")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "CLKIN/OSC1/RB5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F505-IST"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 12.7 0)
		)
		(property "Value" "PIC16F505-IST"
			(at 3.81 10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F505, 1024W FLASH, 72B SRAM, TSSOP14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F505-IST_0_1")
		(symbol "PIC16F505-IST_1_1"
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "RC0")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "RC1")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "RC2")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "RC3")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "RC4")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "RC5/T0CKI")
				(number "5")
			)
			(pin power_in line
				(at 0 12.7 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "ICSPDAT/RB0")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "ICSPCLK/RB1")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "RB2")
				(number "11")
			)
			(pin input line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RB3")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "CLKOUT/OSC2/RB4")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "CLKIN/OSC1/RB5")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F54-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 22.86 0)
		)
		(property "Value" "PIC16F54-IP"
			(at 3.81 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41213D.pdf"
			(at 0 0 0)
		)
		(property "Description" "512W FLASH, 25B SRAM, DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F54-IP_0_1")
		(symbol "PIC16F54-IP_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "4")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "16")
			)
			(pin output line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "OSC2/CLKO")
				(number "15")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "T0CKI")
				(number "3")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "RB0")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "RB1")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RB2")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "RB3")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "RB4")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "ICSPCLK/RB6")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "ICSPDAT/RB7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F54-ISO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 22.86 0)
		)
		(property "Value" "PIC16F54-ISO"
			(at 2.54 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41213D.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F54, 512W FLASH, 25B SRAM, SO18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO* SOIC*"
			(at 0 0 0)
		)
		(symbol "PIC16F54-ISO_0_1")
		(symbol "PIC16F54-ISO_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "4")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "16")
			)
			(pin output line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "OSC2/CLKO")
				(number "15")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "T0CKI")
				(number "3")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "RB0")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "RB1")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RB2")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "RB3")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "RB4")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "ICSPCLK/RB6")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "ICSPDAT/RB7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F54-ISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 22.86 0)
		)
		(property "Value" "PIC16F54-ISS"
			(at 3.81 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41213D.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F54, 512W FLASH, 25B SRAM, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F54-ISS_0_1")
		(symbol "PIC16F54-ISS_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "4")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "18")
			)
			(pin output line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "17")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "T0CKI")
				(number "3")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -22.86 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "RA1")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "RB0")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "RB1")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RB2")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "RB3")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "RB4")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "ICSPCLK/RB6")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "ICSPDAT/RB7")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F610-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 15.24 0)
		)
		(property "Value" "PIC16F610-IML"
			(at -25.4 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41288F.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F610, 1024W FLASH, 64B SRAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F610-IML_0_1")
		(symbol "PIC16F610-IML_1_1"
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "RA0/C1IN+/ICSPDAT")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "RA1/C12IN0-/ICSPCLK")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RA2/T0CKI/INT/C1OUT")
				(number "10")
			)
			(pin input line
				(at -30.48 0 0)
				(length 3.81)
				(name "RA3/~{MCLR}/Vpp")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RA4/~{T1G}/OSC2/CLKOUT")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RA5/T1CKI/OSC1/CLKIN")
				(number "1")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "C2IN+/RC0")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "C12IN1-/RC1")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "C12IN2-/RC2")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "C12IN3-/RC3")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "C2OUT/RC4")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "RC5")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F610-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 15.24 0)
		)
		(property "Value" "PIC16F610-IP"
			(at -25.4 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41288F.pdf"
			(at 0 0 0)
		)
		(property "Description" "1024W FLASH, 64B SRAM, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F610-IP_0_1")
		(symbol "PIC16F610-IP_1_1"
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "RA0/C1IN+/ICSPDAT")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "RA1/C12IN0-/ICSPCLK")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RA2/T0CKI/INT/C1OUT")
				(number "11")
			)
			(pin input line
				(at -30.48 0 0)
				(length 3.81)
				(name "RA3/~{MCLR}/Vpp")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RA4/~{T1G}/OSC2/CLKOUT")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RA5/T1CKI/OSC1/CLKIN")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "C2IN+/RC0")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "C12IN1-/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "C12IN2-/RC2")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "C12IN3-/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "C2OUT/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "RC5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F616-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -45.72 15.24 0)
		)
		(property "Value" "PIC16F616-IML"
			(at -45.72 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41288F.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F616, 2048W FLASH, 128B SRAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F616-IML_0_1"
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 3.81)
				(name "RA5/T1CKI/OSC1/CLKIN")
				(number "1")
			)
		)
		(symbol "PIC16F616-IML_1_1"
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 3.81)
				(name "RA0/AN0/C1IN+/ICSPDAT")
				(number "12")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 3.81)
				(name "RA1/AN1/C12IN0-/Vref/ICSPCLK")
				(number "11")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 3.81)
				(name "RA2/AN2/T0CKI/INT/C1OUT")
				(number "10")
			)
			(pin input line
				(at -50.8 0 0)
				(length 3.81)
				(name "RA3/~{MCLR}/Vpp")
				(number "3")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 3.81)
				(name "RA4/AN3/~{T1G}/OSC2/CLKOUT")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "13")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 3.81)
				(name "C2IN+/AN4/RC0")
				(number "9")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 3.81)
				(name "C12IN1-/AN5/RC1")
				(number "8")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 3.81)
				(name "P1D/C12IN2-/AN6/RC2")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 3.81)
				(name "P1C/C12IN3-/AN7/RC3")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 3.81)
				(name "P1B/C2OUT/RC4")
				(number "5")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 3.81)
				(name "P1A/CCP1/RC5")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F616-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -45.72 15.24 0)
		)
		(property "Value" "PIC16F616-IP"
			(at -45.72 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41288F.pdf"
			(at 0 0 0)
		)
		(property "Description" "2048W FLASH, 128B SRAM, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F616-IP_0_1")
		(symbol "PIC16F616-IP_1_1"
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 3.81)
				(name "RA0/AN0/C1IN+/ICSPDAT")
				(number "13")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 3.81)
				(name "RA1/AN1/C12IN0-/Vref/ICSPCLK")
				(number "12")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 3.81)
				(name "RA2/AN2/T0CKI/INT/C1OUT")
				(number "11")
			)
			(pin input line
				(at -50.8 0 0)
				(length 3.81)
				(name "RA3/~{MCLR}/Vpp")
				(number "4")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 3.81)
				(name "RA4/AN3/~{T1G}/OSC2/CLKOUT")
				(number "3")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 3.81)
				(name "RA5/T1CKI/OSC1/CLKIN")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 3.81)
				(name "C2IN+/AN4/RC0")
				(number "10")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 3.81)
				(name "C12IN1-/AN5/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 3.81)
				(name "P1D/C12IN2-/AN6/RC2")
				(number "8")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 3.81)
				(name "P1C/C12IN3-/AN7/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 3.81)
				(name "P1B/C2OUT/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 3.81)
				(name "P1A/CCP1/RC5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F627-xxIP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 17.78 0)
		)
		(property "Value" "PIC16F627-xxIP"
			(at -24.13 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40300c.pdf"
			(at 0 0 0)
		)
		(property "Description" "1024W Flash, 224B SRAM, 128B EEPROM, DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F627-xxIP_0_1")
		(symbol "PIC16F627-xxIP_1_1"
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "RB0/INT")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "RB1/RX/DT")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "RB2/TX/CK")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RB3/CCP1")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RB4/PGM")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB6/T1OSC0/T1CKI/PGC")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB7/T1OSI/PGD")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "Vref/AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "CMP1/AN3/RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "TOCKI/CMP2/RA4")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "~{MCLR}/Vpp/RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "CLKOUT/OSC2/RA6")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "CLKIN/OSC1/RA7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F627-xxISO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 17.78 0)
		)
		(property "Value" "PIC16F627-xxISO"
			(at -24.13 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40300c.pdf"
			(at 0 0 0)
		)
		(property "Description" "1024W Flash, 224B SRAM, 128B EEPROM, SO18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F627-xxISO_0_1")
		(symbol "PIC16F627-xxISO_1_1"
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "RB0/INT")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "RB1/RX/DT")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "RB2/TX/CK")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RB3/CCP1")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RB4/PGM")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB6/T1OSC0/T1CKI/PGC")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB7/T1OSI/PGD")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "Vref/AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "CMP1/AN3/RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "TOCKI/CMP2/RA4")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "~{MCLR}/Vpp/RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "CLKOUT/OSC2/RA6")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "CLKIN/OSC1/RA7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F627-xxISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 17.78 0)
		)
		(property "Value" "PIC16F627-xxISS"
			(at 3.81 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40300c.pdf"
			(at 0 0 0)
		)
		(property "Description" "1024W Flash, 224B SRAM, 128B EEPROM, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F627-xxISS_0_1")
		(symbol "PIC16F627-xxISS_1_1"
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "RB0/INT")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "RB1/RX/DT")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "RB2/TX/CK")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RB3/CCP1")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RB4/PGM")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB6/T1OSC0/T1CKI/PGC")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB7/T1OSI/PGD")
				(number "14")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "Vref/AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "CMP1/AN3/RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "TOCKI/CMP2/RA4")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "~{MCLR}/Vpp/RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "CLKOUT/OSC2/RA6")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "CLKIN/OSC1/RA7")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F627A-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 17.78 0)
		)
		(property "Value" "PIC16F627A-IP"
			(at -24.13 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40300c.pdf"
			(at 0 0 0)
		)
		(property "Description" "1024W Flash, 224B SRAM, 128B EEPROM, DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F627A-IP_0_1")
		(symbol "PIC16F627A-IP_1_1"
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "RB0/INT")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "RB1/RX/DT")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "RB2/TX/CK")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RB3/CCP1")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RB4/PGM")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB6/T1OSC0/T1CKI/PGC")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB7/T1OSI/PGD")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "Vref/AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "CMP1/AN3/RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "TOCKI/CMP2/RA4")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "~{MCLR}/Vpp/RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "CLKOUT/OSC2/RA6")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "CLKIN/OSC1/RA7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F627A-ISO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -24.13 17.78 0)
		)
		(property "Value" "PIC16F627A-ISO"
			(at -24.13 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40300c.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F627A, 1024W Flash, 224B SRAM, 128B EEPROM, SO18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F627A-ISO_0_1")
		(symbol "PIC16F627A-ISO_1_1"
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "RB0/INT")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "RB1/RX/DT")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "RB2/TX/CK")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RB3/CCP1")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RB4/PGM")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB6/T1OSC0/T1CKI/PGC")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB7/T1OSI/PGD")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "Vref/AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "CMP1/AN3/RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "TOCKI/CMP2/RA4")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "~{MCLR}/Vpp/RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "CLKOUT/OSC2/RA6")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "CLKIN/OSC1/RA7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F627A-ISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 17.78 0)
		)
		(property "Value" "PIC16F627A-ISS"
			(at 5.08 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40044G.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F627A, 1024W Flash, 224B SRAM, 128B EEPROM, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F627A-ISS_0_1")
		(symbol "PIC16F627A-ISS_1_1"
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "RB0/INT")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "RB1/RX/DT")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "RB2/TX/CK")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RB3/CCP1")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RB4/PGM")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB6/T1OSC0/T1CKI/PGC")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB7/T1OSI/PGD")
				(number "14")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "Vref/AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "CMP1/AN3/RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "TOCKI/CMP2/RA4")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "~{MCLR}/Vpp/RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "CLKOUT/OSC2/RA6")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "CLKIN/OSC1/RA7")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F631-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 15.24 20.32 0)
		)
		(property "Value" "PIC16F631-IP"
			(at 15.24 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "1024W Flash, 64B SRAM, 128B EEPROM, DIP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F631-IP_0_1")
		(symbol "PIC16F631-IP_1_1"
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "RC0/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "RC1/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "RC2/C12IN2-")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "RC3/C12IN3-")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "RC6")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "RC7")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "T0CKI/INT/C1OUT/RA2")
				(number "17")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F631-ISO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 20.32 0)
		)
		(property "Value" "PIC16F631-ISO"
			(at 13.97 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F631, 1024W Flash, 64B SRAM, 128B EEPROM, SO20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F631-ISO_0_1")
		(symbol "PIC16F631-ISO_1_1"
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "RC0/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "RC1/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "RC2/C12IN2-")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "RC3/C12IN3-")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "RC6")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "RC7")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "T0CKI/INT/C1OUT/RA2")
				(number "17")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F631-ISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 20.32 0)
		)
		(property "Value" "PIC16F631-ISS"
			(at 13.97 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F631, 1024W Flash, 64B SRAM, 128B EEPROM, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F631-ISS_0_1")
		(symbol "PIC16F631-ISS_1_1"
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "RC0/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "RC1/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "RC2/C12IN2-")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "RC3/C12IN3-")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 3.81)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "RC6")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "RC7")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "T0CKI/INT/C1OUT/RA2")
				(number "17")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F677-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 20.32 0)
		)
		(property "Value" "PIC16F677-IP"
			(at 17.78 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "2048W Flash, 128B SRAM, 128B EEPROM, DIP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F677-IP_0_1")
		(symbol "PIC16F677-IP_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RC0/AN4/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RC1/AN5/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RC2/AN6/C12IN2-")
				(number "14")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RC3/AN7/C12IN3-")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT")
				(number "6")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "RC6/AN8/~{SS}")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RC7/AN9/SDO")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/Vref/AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "T0CKI/INT/C1OUT/AN2/RA2")
				(number "17")
			)
			(pin input line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/AN3/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "SDA/SDI/AN10/RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "AN11/RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "SCL/SCK/RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F677-ISO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 16.51 20.32 0)
		)
		(property "Value" "PIC16F677-ISO"
			(at 16.51 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F677, 2048W Flash, 128B SRAM, 128B EEPROM, SO20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F677-ISO_0_1")
		(symbol "PIC16F677-ISO_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RC0/AN4/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RC1/AN5/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RC2/AN6/C12IN2-")
				(number "14")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RC3/AN7/C12IN3-")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT")
				(number "6")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "RC6/AN8/~{SS}")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RC7/AN9/SDO")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/Vref/AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "T0CKI/INT/C1OUT/AN2/RA2")
				(number "17")
			)
			(pin input line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/AN3/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "SDA/SDI/AN10/RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "AN11/RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "SCL/SCK/RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F677-ISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 16.51 20.32 0)
		)
		(property "Value" "PIC16F677-ISS"
			(at 16.51 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F677, 2048W Flash, 128B SRAM, 128B EEPROM, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F677-ISS_0_1")
		(symbol "PIC16F677-ISS_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RC0/AN4/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RC1/AN5/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RC2/AN6/C12IN2-")
				(number "14")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RC3/AN7/C12IN3-")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT")
				(number "6")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "RC6/AN8/~{SS}")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RC7/AN9/SDO")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/Vref/AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "T0CKI/INT/C1OUT/AN2/RA2")
				(number "17")
			)
			(pin input line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/AN3/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "SDA/SDI/AN10/RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "AN11/RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "SCL/SCK/RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F684-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 15.24 0)
		)
		(property "Value" "PIC16F684-IML"
			(at -35.56 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41202F-print.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F684 , 2048W FLASH, 128B SRAM, 256B EEPROM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F684-IML_0_1")
		(symbol "PIC16F684-IML_1_1"
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 3.81)
				(name "RA0/AN0/C1IN+/ICSPDAT/ULPWU")
				(number "12")
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 3.81)
				(name "RA1/AN1/C1IN-/Vref/ICSPCLK")
				(number "11")
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 3.81)
				(name "RA2/AN2/T0CKI/INT/C1OUT")
				(number "10")
			)
			(pin input line
				(at -40.64 0 0)
				(length 3.81)
				(name "RA3/~{MCLR}/Vpp")
				(number "3")
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 3.81)
				(name "RA4/AN3/~{T1G}/OSC2/CLKOUT")
				(number "2")
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 3.81)
				(name "RA5/T1CKI/OSC1/CLKIN")
				(number "1")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "13")
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 3.81)
				(name "C2IN+/AN4/RC0")
				(number "9")
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 3.81)
				(name "C2IN-/AN5/RC1")
				(number "8")
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 3.81)
				(name "P1D/AN6/RC2")
				(number "7")
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 3.81)
				(name "P1C/AN7/RC3")
				(number "6")
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 3.81)
				(name "P1B/C2OUT/RC4")
				(number "5")
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 3.81)
				(name "P1A/CCP1/RC5")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F684-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -35.56 15.24 0)
		)
		(property "Value" "PIC16F684-IP"
			(at -35.56 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41202F-print.pdf"
			(at 0 0 0)
		)
		(property "Description" "2048W FLASH, 128B SRAM, 256B EEPROM, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F684-IP_0_1")
		(symbol "PIC16F684-IP_1_1"
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 3.81)
				(name "RA0/AN0/C1IN+/ICSPDAT/ULPWU")
				(number "13")
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 3.81)
				(name "RA1/AN1/C1IN-/Vref/ICSPCLK")
				(number "12")
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 3.81)
				(name "RA2/AN2/T0CKI/INT/C1OUT")
				(number "11")
			)
			(pin input line
				(at -40.64 0 0)
				(length 3.81)
				(name "RA3/~{MCLR}/Vpp")
				(number "4")
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 3.81)
				(name "RA4/AN3/~{T1G}/OSC2/CLKOUT")
				(number "3")
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 3.81)
				(name "RA5/T1CKI/OSC1/CLKIN")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "14")
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 3.81)
				(name "C2IN+/AN4/RC0")
				(number "10")
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 3.81)
				(name "C2IN-/AN5/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 3.81)
				(name "P1D/AN6/RC2")
				(number "8")
			)
			(pin bidirectional line
				(at 40.64 0 180)
				(length 3.81)
				(name "P1C/AN7/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 3.81)
				(name "P1B/C2OUT/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 3.81)
				(name "P1A/CCP1/RC5")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F685-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 20.32 0)
		)
		(property "Value" "PIC16F685-IP"
			(at 17.78 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "4096W Flash, 256B SRAM, 256B EEPROM, DIP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F685-IP_0_1")
		(symbol "PIC16F685-IP_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RC0/AN4/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RC1/AN5/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RC2/AN6/C12IN2-/P1D")
				(number "14")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RC3/AN7/C12IN3-/P1C")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT/P1B")
				(number "6")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "RC5/CCP1/P1A")
				(number "5")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "RC6/AN8")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RC7/AN9")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/Vref/AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "T0CKI/INT/C1OUT/AN2/RA2")
				(number "17")
			)
			(pin input line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/AN3/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "AN10/RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "AN11/RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F685-ISO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 16.51 20.32 0)
		)
		(property "Value" "PIC16F685-ISO"
			(at 16.51 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F685, 4096W Flash, 256B SRAM, 256B EEPROM, SO20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F685-ISO_0_1")
		(symbol "PIC16F685-ISO_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RC0/AN4/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RC1/AN5/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RC2/AN6/C12IN2-/P1D")
				(number "14")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RC3/AN7/C12IN3-/P1C")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT/P1B")
				(number "6")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "RC5/CCP1/P1A")
				(number "5")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "RC6/AN8")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RC7/AN9")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/Vref/AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "T0CKI/INT/C1OUT/AN2/RA2")
				(number "17")
			)
			(pin input line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/AN3/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "AN10/RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "AN11/RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F685-ISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 16.51 20.32 0)
		)
		(property "Value" "PIC16F685-ISS"
			(at 16.51 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F685, 4096W Flash, 256B SRAM, 256B EEPROM, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F685-ISS_0_1")
		(symbol "PIC16F685-ISS_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RC0/AN4/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RC1/AN5/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RC2/AN6/C12IN2-/P1D")
				(number "14")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RC3/AN7/C12IN3-/P1C")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT/P1B")
				(number "6")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "RC5/CCP1/P1A")
				(number "5")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "RC6/AN8")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RC7/AN9")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/Vref/AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "T0CKI/INT/C1OUT/AN2/RA2")
				(number "17")
			)
			(pin input line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/AN3/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "AN10/RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "AN11/RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F687-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 20.32 0)
		)
		(property "Value" "PIC16F687-IP"
			(at 17.78 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "2048W Flash, 128B SRAM, 256B EEPROM, DIP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F687-IP_0_1")
		(symbol "PIC16F687-IP_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RC0/AN4/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RC1/AN5/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RC2/AN6/C12IN2-")
				(number "14")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RC3/AN7/C12IN3-")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT")
				(number "6")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "RC6/AN8/~{SS}")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RC7/AN9/SDO")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/Vref/AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "T0CKI/INT/C1OUT/AN2/RA2")
				(number "17")
			)
			(pin input line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/AN3/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "SDI/SDA/AN10/RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "RX/DT/AN11/RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "SCK/SCL/RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "TX/CK/RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F687-ISO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 16.51 20.32 0)
		)
		(property "Value" "PIC16F687-ISO"
			(at 16.51 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F687, 2048W Flash, 128B SRAM, 256B EEPROM, SO20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F687-ISO_0_1")
		(symbol "PIC16F687-ISO_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RC0/AN4/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RC1/AN5/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RC2/AN6/C12IN2-")
				(number "14")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RC3/AN7/C12IN3-")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT")
				(number "6")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "RC6/AN8/~{SS}")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RC7/AN9/SDO")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/Vref/AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "T0CKI/INT/C1OUT/AN2/RA2")
				(number "17")
			)
			(pin input line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/AN3/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "SDI/SDA/AN10/RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "RX/DT/AN11/RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "SCK/SCL/RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "TX/CK/RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F687-ISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 16.51 20.32 0)
		)
		(property "Value" "PIC16F687-ISS"
			(at 16.51 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F687, 2048W Flash, 128B SRAM, 256B EEPROM, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F687-ISS_0_1")
		(symbol "PIC16F687-ISS_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RC0/AN4/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RC1/AN5/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RC2/AN6/C12IN2-")
				(number "14")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RC3/AN7/C12IN3-")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT")
				(number "6")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "RC5")
				(number "5")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "RC6/AN8/~{SS}")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RC7/AN9/SDO")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/Vref/AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "T0CKI/INT/C1OUT/AN2/RA2")
				(number "17")
			)
			(pin input line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/AN3/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "SDI/SDA/AN10/RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "RX/DT/AN11/RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "SCK/SCL/RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "TX/CK/RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F690-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 19.05 20.32 0)
		)
		(property "Value" "PIC16F690-IP"
			(at 19.05 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "4096W Flash, 256B SRAM, 256B EEPROM, DIP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F690-IP_0_1")
		(symbol "PIC16F690-IP_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RC0/AN4/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RC1/AN5/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RC2/AN6/C12IN2-/P1D")
				(number "14")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RC3/AN7/C12IN3-/P1C")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT/P1B")
				(number "6")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "RC5/CCP1/P1A")
				(number "5")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "RC6/AN8/~{SS}")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RC7/AN9/SDO")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/Vref/AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "C1OUT/T0CKI/INT/AN2/RA2")
				(number "17")
			)
			(pin input line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/AN3/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "SDI/SDA/AN10/RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "RX/DT/AN11/RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "SCK/SCL/RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "TX/CK/RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F690-ISO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 20.32 0)
		)
		(property "Value" "PIC16F690-ISO"
			(at 17.78 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F690, 4096W Flash, 256B SRAM, 256B EEPROM, SO20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F690-ISO_0_1")
		(symbol "PIC16F690-ISO_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RC0/AN4/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RC1/AN5/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RC2/AN6/C12IN2-/P1D")
				(number "14")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RC3/AN7/C12IN3-/P1C")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT/P1B")
				(number "6")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "RC5/CCP1/P1A")
				(number "5")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "RC6/AN8/~{SS}")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RC7/AN9/SDO")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/Vref/AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "C1OUT/T0CKI/INT/AN2/RA2")
				(number "17")
			)
			(pin input line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/AN3/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "SDI/SDA/AN10/RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "RX/DT/AN11/RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "SCK/SCL/RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "TX/CK/RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F690-ISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 20.32 0)
		)
		(property "Value" "PIC16F690-ISS"
			(at 17.78 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F690, 4096W Flash, 256B SRAM, 256B EEPROM, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F690-ISS_0_1")
		(symbol "PIC16F690-ISS_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RC0/AN4/C2IN+")
				(number "16")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RC1/AN5/C12IN1-")
				(number "15")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RC2/AN6/C12IN2-/P1D")
				(number "14")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RC3/AN7/C12IN3-/P1C")
				(number "7")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RC4/C2OUT/P1B")
				(number "6")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 3.81)
				(name "RC5/CCP1/P1A")
				(number "5")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 3.81)
				(name "RC6/AN8/~{SS}")
				(number "8")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RC7/AN9/SDO")
				(number "9")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "C1IN+/ICSPDAT/ULPWU/AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "C12IN0-/ICSPCLK/Vref/AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "C1OUT/T0CKI/INT/AN2/RA2")
				(number "17")
			)
			(pin input line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA3")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "~{T1G}/OSC2/CLKOUT/AN3/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T1CKI/OSC1/CLKIN/RA5")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "SDI/SDA/AN10/RB4")
				(number "13")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 3.81)
				(name "RX/DT/AN11/RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "SCK/SCL/RB6")
				(number "11")
			)
			(pin bidirectional line
				(at 38.1 -12.7 180)
				(length 3.81)
				(name "TX/CK/RB7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F716-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 22.86 0)
		)
		(property "Value" "PIC16F716-IP"
			(at 3.81 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41206B.pdf"
			(at 0 0 0)
		)
		(property "Description" "2048W Flash, 128B SRAM, DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F716-IP_0_1")
		(symbol "PIC16F716-IP_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "4")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "16")
			)
			(pin output line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "OSC2/CLKO")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "Vref/AN3/RA3")
				(number "2")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "INT/~{ECCPAS2}/RB0")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RB1")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "T1OSI/RB2")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "CCP1/P1A/RB3")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "~{ECCPAS0}/RB4")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "P1B/RB5")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "P1C/RB6")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "P1D/RB7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F716-ISO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 22.86 0)
		)
		(property "Value" "PIC16F716-ISO"
			(at 2.54 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41206B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F716, 2048W Flash, 128B SRAM, SO18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F716-ISO_0_1")
		(symbol "PIC16F716-ISO_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "4")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "16")
			)
			(pin output line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "OSC2/CLKO")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "Vref/AN3/RA3")
				(number "2")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "INT/~{ECCPAS2}/RB0")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RB1")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "T1OSI/RB2")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "CCP1/P1A/RB3")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "~{ECCPAS0}/RB4")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "P1B/RB5")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "P1C/RB6")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "P1D/RB7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F716-ISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 22.86 0)
		)
		(property "Value" "PIC16F716-ISS"
			(at 2.54 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41206B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F716, 2048W Flash, 128B SRAM, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F716-ISS_0_1")
		(symbol "PIC16F716-ISS_1_1"
			(pin input line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "4")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "18")
			)
			(pin output line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "OSC2/CLKO")
				(number "17")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "Vref/AN3/RA3")
				(number "2")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "INT/~{ECCPAS2}/RB0")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RB1")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "T1OSI/RB2")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "CCP1/P1A/RB3")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "~{ECCPAS0}/RB4")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "P1B/RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "P1C/RB6")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "P1D/RB7")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F73-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F73-IML"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30325b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F73, 4K Flash, 192B SRAM, ADC, PWM, MLF28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*"
			(at 0 0 0)
		)
		(symbol "PIC16F73-IML_0_1")
		(symbol "PIC16F73-IML_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "26")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "6")
			)
			(pin output line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "RC0/T10S0/T1CKI")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "RC1/CCP2/T1OSI")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "RC2/CCP1")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "RC3/SCK/SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "RC4/SDI/SDA")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "RC5/SDO")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "RC6/TX/CK")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "RC7/RX/DT")
				(number "15")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "Vref/AN3/RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "~{SS}/AN4/RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F73-ISO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F73-ISO"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30325b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F73, 4K Flash, 192B SRAM, ADC, PWM, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F73-ISO_0_1")
		(symbol "PIC16F73-ISO_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "1")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "9")
			)
			(pin output line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "RC0/T10S0/T1CKI")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "RC1/CCP2/T1OSI")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "RC2/CCP1")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "RC3/SCK/SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "RC4/SDI/SDA")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "RC5/SDO")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "RC6/TX/CK")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "RC7/RX/DT")
				(number "18")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "Vref/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "~{SS}/AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F73-ISP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F73-ISP"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30325b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F73, 4K Flash, 192B SRAM, ADC, PWM, SDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F73-ISP_0_1")
		(symbol "PIC16F73-ISP_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "1")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "9")
			)
			(pin output line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "RC0/T10S0/T1CKI")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "RC1/CCP2/T1OSI")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "RC2/CCP1")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "RC3/SCK/SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "RC4/SDI/SDA")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "RC5/SDO")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "RC6/TX/CK")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "RC7/RX/DT")
				(number "18")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "Vref/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "~{SS}/AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F73-ISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F73-ISS"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30325b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F73, 4K Flash, 192B SRAM, ADC, PWM, SSOP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F73-ISS_0_1")
		(symbol "PIC16F73-ISS_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "1")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "9")
			)
			(pin output line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "RC0/T10S0/T1CKI")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "RC1/CCP2/T1OSI")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "RC2/CCP1")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "RC3/SCK/SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "RC4/SDI/SDA")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "RC5/SDO")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "RC6/TX/CK")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "RC7/RX/DT")
				(number "18")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "Vref/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "~{SS}/AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F74-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 35.56 0)
		)
		(property "Value" "PIC16F74-IP"
			(at 6.35 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30325b.pdf"
			(at 0 0 0)
		)
		(property "Description" "4K Flash, 192B SRAM, ADC, PWM, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F74-IP_0_1")
		(symbol "PIC16F74-IP_1_1"
			(pin input line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "1")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "13")
			)
			(pin output line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "RD0/PSP0")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "RD1/PSP1")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "RD2/PSP2")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "RD3/PSP3")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "RD4/PSP4")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "RD5/PSP5")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "RD6/PSP6")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "RD7/PSP7")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "RE0/~{RD}/AN5")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "RE1/~{WR}/AN6")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "RE2/~{CS}/AN7")
				(number "10")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "CVref/Vref-/AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "T0CKI/C1OUT/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "~{SS}/C2OUT/AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "INT/RB0")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "RB1")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "RB2")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "RB4")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "RB5")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "T10S0/T1CKI/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "CCP2/T1OSI/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "SCK/SCL/RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "SDI/SDA/RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "SDO/RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F818-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 17.78 0)
		)
		(property "Value" "PIC16F818-IML"
			(at 5.08 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39598F.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F818, 1792B Flash, 128B SRAM, 128B EEPROM, ADC, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*"
			(at 0 0 0)
		)
		(symbol "PIC16F818-IML_0_1")
		(symbol "PIC16F818-IML_1_1"
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RB0/INT")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RB1/SDI/SDA")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RB2/SDO/CCP1")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RB3/CCP1/PGM")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "RB4/SCK/SCL")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB5/~{SS}")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB6/T1OSO/T1CKI/PGC")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB7/T1OSI/PGD")
				(number "16")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "3")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "T0CKL/AN4/RA4")
				(number "28")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA5")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "CLKO/OSC2/RA6")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "CLKI/OSC1/RA7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F818-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 3.81 17.78 0)
		)
		(property "Value" "PIC16F818-IP"
			(at 3.81 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39598F.pdf"
			(at 0 0 0)
		)
		(property "Description" "1792B Flash, 128B SRAM, 128B EEPROM, ADC, DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F818-IP_0_1")
		(symbol "PIC16F818-IP_1_1"
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RB0/INT")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RB1/SDI/SDA")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RB2/SDO/CCP1")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RB3/CCP1/PGM")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "RB4/SCK/SCL")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB5/~{SS}")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB6/T1OSO/T1CKI/PGC")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB7/T1OSI/PGD")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "T0CKL/AN4/RA4")
				(number "3")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "CLKO/OSC2/RA6")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "CLKI/OSC1/RA7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F818-ISO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 17.78 0)
		)
		(property "Value" "PIC16F818-ISO"
			(at 5.08 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39598F.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F818, 1792B Flash, 128B SRAM, 128B EEPROM, ADC, SOIC18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F818-ISO_0_1")
		(symbol "PIC16F818-ISO_1_1"
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RB0/INT")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RB1/SDI/SDA")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RB2/SDO/CCP1")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RB3/CCP1/PGM")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "RB4/SCK/SCL")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB5/~{SS}")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB6/T1OSO/T1CKI/PGC")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB7/T1OSI/PGD")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "T0CKL/AN4/RA4")
				(number "3")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "CLKO/OSC2/RA6")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "CLKI/OSC1/RA7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F818-ISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 17.78 0)
		)
		(property "Value" "PIC16F818-ISS"
			(at 6.35 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39598F.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F818, 1792B Flash, 128B SRAM, 128B EEPROM, ADC, SSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F818-ISS_0_1")
		(symbol "PIC16F818-ISS_1_1"
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RB0/INT")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RB1/SDI/SDA")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RB2/SDO/CCP1")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "RB3/CCP1/PGM")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "RB4/SCK/SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB5/~{SS}")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB6/T1OSO/T1CKI/PGC")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB7/T1OSI/PGD")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "T0CKL/AN4/RA4")
				(number "3")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "CLKO/OSC2/RA6")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "CLKI/OSC1/RA7")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F83-XXP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 22.86 0)
		)
		(property "Value" "PIC16F83-XXP"
			(at 2.54 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30430c.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F83, 512B Flash, 36B SRAM, 64B EEPROM, DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F83-XXP_0_1")
		(symbol "PIC16F83-XXP_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "4")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "16")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "TOCKI/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "RB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "RB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "RB7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F83-XXSO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 22.86 0)
		)
		(property "Value" "PIC16F83-XXSO"
			(at 2.54 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30430c.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F83, 512B Flash, 36B SRAM, 64B EEPROM, SOIC18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F83-XXSO_0_1")
		(symbol "PIC16F83-XXSO_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "4")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "16")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "TOCKI/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "RB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "RB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "RB7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F84A-XXP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 22.86 0)
		)
		(property "Value" "PIC16F84A-XXP"
			(at 2.54 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/35007b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F84A, 1K Flash, 68B SRAM, 64B EEPROM, DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F84A-XXP_0_1")
		(symbol "PIC16F84A-XXP_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "4")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "16")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "TOCKI/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "RB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "RB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "RB7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F84A-XXSO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 22.86 0)
		)
		(property "Value" "PIC16F84A-XXSO"
			(at 2.54 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/35007b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F84A, 1KB Flash, 68B SRAM, 64B EEPROM, SOIC18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F84A-XXSO_0_1")
		(symbol "PIC16F84A-XXSO_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "4")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "16")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "15")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "TOCKI/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "RB3")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "RB6")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "RB7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F84A-XXSS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 22.86 0)
		)
		(property "Value" "PIC16F84A-XXSS"
			(at 2.54 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/35007b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F84A, 1KB Flash, 68B SRAM, 64B EEPROM, SSOP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F84A-XXSS_0_1")
		(symbol "PIC16F84A-XXSS_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "4")
			)
			(pin input line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "18")
			)
			(pin output line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "17")
			)
			(pin power_in line
				(at -2.54 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "RA1")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "RB3")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "RB6")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "RB7")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F870-ISO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F870-ISO"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30569b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F870, 2K Flash, 128B SRAM, 64B EEPROM, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F870-ISO_0_1")
		(symbol "PIC16F870-ISO_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "~{MCLR}/Vpp/THV")
				(number "1")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "9")
			)
			(pin output line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "RC0/T10S0/T1CKI")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "RC1/T1OSI")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "RC2/CCP1")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "RC3")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "RC4")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "RC5")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "RC6/TX/CK")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "RC7/RX/DT")
				(number "18")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F870-ISP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F870-ISP"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30569b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F870, 2K Flash, 128B SRAM, 64B EEPROM, DIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F870-ISP_0_1")
		(symbol "PIC16F870-ISP_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "~{MCLR}/Vpp/THV")
				(number "1")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "9")
			)
			(pin output line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "RC0/T10S0/T1CKI")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "RC1/T1OSI")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "RC2/CCP1")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "RC3")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "RC4")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "RC5")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "RC6/TX/CK")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "RC7/RX/DT")
				(number "18")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F870-ISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F870-ISS"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30569b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F870, 2K Flash, 128B SRAM, 64B EEPROM, SSOP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
		(symbol "PIC16F870-ISS_0_1")
		(symbol "PIC16F870-ISS_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "~{MCLR}/Vpp/THV")
				(number "1")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "9")
			)
			(pin output line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "RC0/T10S0/T1CKI")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "RC1/T1OSI")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "RC2/CCP1")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "RC3")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "RC4")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "RC5")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "RC6/TX/CK")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "RC7/RX/DT")
				(number "18")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F871-IL"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 38.1 0)
		)
		(property "Value" "PIC16F871-IL"
			(at 5.08 35.56 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30569b.pdf"
			(at 0 0 0)
		)
		(property "Description" "2K Flash, 128B SRAM, 64B EEPROM, PLCC44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
		(symbol "PIC16F871-IL_0_1")
		(symbol "PIC16F871-IL_1_1"
			(pin input line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "~{MCLR}/Vpp/THV")
				(number "2")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "14")
			)
			(pin output line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "RD0/PSP0")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "RD1/PSP1")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "RD2/PSP2")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "RD3/PSP3")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "RD4/PSP4")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "RD5/PSP5")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "RD6/PSP6")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "RD7/PSP7")
				(number "33")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "RE0/~{RD}/AN5")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "RE1/~{WR}/AN6")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "RE2/~{CS}/AN7")
				(number "11")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "13")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 3.81)
				(name "VDD")
				(number "35")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "AN4/RA5")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "INT/RB0")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "RB1")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "RB2")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "RB4")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "RB5")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "43")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "T10S0/T1CKI/RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "T1OSI/RC1")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "RC3")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "RC4")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "RC5")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F871-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 38.1 0)
		)
		(property "Value" "PIC16F871-IP"
			(at 5.08 35.56 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30569b.pdf"
			(at 0 0 0)
		)
		(property "Description" "2K Flash, 128B SRAM, 64B EEPROM, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F871-IP_0_1")
		(symbol "PIC16F871-IP_1_1"
			(pin input line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "~{MCLR}/Vpp/THV")
				(number "1")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "13")
			)
			(pin output line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "RD0/PSP0")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "RD1/PSP1")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "RD2/PSP2")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "RD3/PSP3")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "RD4/PSP4")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "RD5/PSP5")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "RD6/PSP6")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "RD7/PSP7")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "RE0/~{RD}/AN5")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "RE1/~{WR}/AN6")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "RE2/~{CS}/AN7")
				(number "10")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "INT/RB0")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "RB1")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "RB2")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "RB4")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "RB5")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "T10S0/T1CKI/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "T1OSI/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F871-IPT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 38.1 0)
		)
		(property "Value" "PIC16F871-IPT"
			(at 5.08 35.56 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30569b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F871, 2K Flash, 128B SRAM, 64B EEPROM, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*"
			(at 0 0 0)
		)
		(symbol "PIC16F871-IPT_0_1")
		(symbol "PIC16F871-IPT_1_1"
			(pin input line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "~{MCLR}/Vpp/THV")
				(number "18")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "30")
			)
			(pin output line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "OSC2/CLKOUT")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "RD0/PSP0")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "RD1/PSP1")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "RD2/PSP2")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "RD3/PSP3")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "RD4/PSP4")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "RD5/PSP5")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "RD6/PSP6")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "RD7/PSP7")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "RE0/~{RD}/AN5")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "RE1/~{WR}/AN6")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "RE2/~{CS}/AN7")
				(number "27")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "AN4/RA5")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "INT/RB0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "RB1")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "RB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "RB4")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "RB5")
				(number "43")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "T10S0/T1CKI/RC0")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "T1OSI/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "RC3")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "RC4")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "RC5")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F873-XXISO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F873-XXISO"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30292C.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F873, 4K Flash, 192B SRAM, 128B EEPROM, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
		(symbol "PIC16F873-XXISO_0_1")
		(symbol "PIC16F873-XXISO_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "1")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "9")
			)
			(pin output line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "OSC2/CLKO")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "RC0/T1OSO/T1CKI")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "RC1/T1OSI/CCP2")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "RC2/CCP1")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "RC3/SCK/SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "RC4/SDI/SDA")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "RC5/SDO")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "RC6/CK/TX")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "RC7/DT/RX")
				(number "18")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "~{SS}/AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F873-XXISP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F873-XXISP"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30292C.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F873,  4K Flash, 192B SRAM, 128B EEPROM, SDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F873-XXISP_0_1")
		(symbol "PIC16F873-XXISP_1_1"
			(pin input line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "1")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "9")
			)
			(pin output line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "OSC2/CLKO")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "RC0/T1OSO/T1CKI")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "RC1/T1OSI/CCP2")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "RC2/CCP1")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "RC3/SCK/SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "RC4/SDI/SDA")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "RC5/SDO")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "RC6/CK/TX")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "RC7/DT/RX")
				(number "18")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "~{SS}/AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "INT/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F874-XXIP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 35.56 0)
		)
		(property "Value" "PIC16F874-XXIP"
			(at 5.08 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30292C.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F874, 4K Flash, 192B SRAM, 128B EEPROM, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F874-XXIP_0_1")
		(symbol "PIC16F874-XXIP_1_1"
			(pin input line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "1")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "13")
			)
			(pin output line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "OSC2/CLKO")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "RD0/PSP0")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "RD1/PSP1")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "RD2/PSP2")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "RD3/PSP3")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "RD4/PSP4")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "RD5/PSP5")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "RD6/PSP6")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "RD7/PSP7")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "RE0/~{RD}/AN5")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "RE1/~{WR}/AN6")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "RE2/~{CS}/AN7")
				(number "10")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "~{SS}/AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "INT/RB0")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "RB1")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "RB2")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "RB4")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RB5")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "T1OSI/CCP2/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "SCK/SCL/RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "SDI/SDA/RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "SDO/RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "CK/TX/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "DT/RX/RC7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F874A-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 35.56 0)
		)
		(property "Value" "PIC16F874A-IP"
			(at 5.08 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39582b.pdf"
			(at 0 0 0)
		)
		(property "Description" "4096W Flash, 192B SRAM, 128B EEPROM, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F874A-IP_0_1")
		(symbol "PIC16F874A-IP_1_1"
			(pin input line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "1")
			)
			(pin input line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "13")
			)
			(pin output line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "OSC2/CLKO")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "RD0/PSP0")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "RD1/PSP1")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "RD2/PSP2")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "RD3/PSP3")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "RD4/PSP4")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "RD5/PSP5")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "RD6/PSP6")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "RD7/PSP7")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "RE0/~{RD}/AN5")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "RE1/~{WR}/AN6")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "RE2/~{CS}/AN7")
				(number "10")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "CVref/Vref-/AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "C1OUT/T0CKI/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "~{SS}/C2OUT/AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "INT/RB0")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "RB1")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "RB2")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "RB4")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "RB5")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "T1OSI/CCP2/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "SCK/SCL/RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "SDI/SDA/RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "SDO/RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "CK/TX/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 3.81)
				(name "DT/RX/RC7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F874A-IPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 38.1 0)
		)
		(property "Value" "PIC16F874A-IPT"
			(at 5.08 38.1 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39582b.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "PIC16F874A, 4096W Flash, 192B SRAM, 128B EEPROM, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*"
			(at 0 0 0)
		)
		(symbol "PIC16F874A-IPT_0_1")
		(symbol "PIC16F874A-IPT_1_1"
			(pin input line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "18")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "30")
			)
			(pin output line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "OSC2/CLKO")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "RD0/PSP0")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "RD1/PSP1")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "RD2/PSP2")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "RD3/PSP3")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "RD4/PSP4")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "RD5/PSP5")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "RD6/PSP6")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "RD7/PSP7")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "RE0/~{RD}/AN5")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "RE1/~{WR}/AN6")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "RE2/~{CS}/AN7")
				(number "27")
			)
			(pin no_connect line
				(at -10.16 -40.64 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at -7.62 -40.64 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at -5.08 -40.64 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -2.54 -40.64 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin passive line
				(at 0 40.64 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 40.64 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin passive line
				(at 0 -40.64 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "CVref/Vref-/AN2/RA2")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "C1OUT/T0CKI/RA4")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "~{SS}/C2OUT/AN4/RA5")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "INT/RB0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "RB1")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "RB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "PGM/RB3")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "RB4")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "RB5")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "PGC/RB6")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "PGD/RB7")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "T1OSI/CCP2/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "SCK/SCL/RC3")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "SDI/SDA/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "SDO/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "CK/TX/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "DT/RX/RC7")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F88-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 17.78 0)
		)
		(property "Value" "PIC16F88-IML"
			(at -22.86 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30487D.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F88, 4096W Flash, 368B SRAM, 256B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F88-IML_0_1")
		(symbol "PIC16F88-IML_1_1"
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "RB0/INT/CCP1")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "RB1/SDI/SDA")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "RB2/SDO/RX/DT")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RB3/PGM/CCP1")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RB4/SCK/SCL")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RB5/~{SS}/TX/CK")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB6/AN5/PGC/T1CKI")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB7/AN6/PGD/T1OSI")
				(number "16")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "3")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "Vref-/CVref/AN2/RA2")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "C1OUT/Vref+/AN3/RA3")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "C2OUT/T0CKI/AN4/RA4")
				(number "28")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "~{MCLR}/Vpp/RA5")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "CLKOUT/OSC2/RA6")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "CLKIN/OSC1/RA7")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F88-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 17.78 0)
		)
		(property "Value" "PIC16F88-IP"
			(at -22.86 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30487D.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F88, 4096W Flash, 368B SRAM, 256B EEPROM, DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F88-IP_0_1")
		(symbol "PIC16F88-IP_1_1"
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "RB0/INT/CCP1")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "RB1/SDI/SDA")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "RB2/SDO/RX/DT")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RB3/PGM/CCP1")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RB4/SCK/SCL")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RB5/~{SS}/TX/CK")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB6/AN5/PGC/T1CKI")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB7/AN6/PGD/T1OSI")
				(number "13")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "AN0/RA0")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "AN1/RA1")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "Vref-/CVref/AN2/RA2")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "C1OUT/Vref+/AN3/RA3")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "C2OUT/T0CKI/AN4/RA4")
				(number "3")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "~{MCLR}/Vpp/RA5")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "CLKOUT/OSC2/RA6")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "CLKIN/OSC1/RA7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F882-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 27.94 0)
		)
		(property "Value" "PIC16F882-IP"
			(at 13.97 25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41291D.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "2K Flash, 128B SRAM, 128B EEPROM, XLP, DIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F882-IP_0_1")
		(symbol "PIC16F882-IP_1_1"
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 3.81)
				(name "RE3/~{MCLR}/Vpp")
				(number "1")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "RC0/T1OSO/T1CK1")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "RC1/T1OSI/CCP2")
				(number "12")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "RC2/P1A/CCP1")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "RC3/SCK/SCL")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "RC4/SDI/SDA")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "RC5/SDO")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "RC6/TX/CK")
				(number "17")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "RC7/RX/DT")
				(number "18")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "ULPWU/C12IN0-/AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "C12IN1-/AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "CVref/C2IN1+/Vref-/AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "C1IN+/Vref+/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "T0CKI/C1OUT/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "~{SS}/C2OUT/AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 3.81)
				(name "CLKOUT/OSC2/RA6")
				(number "10")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "CLKIN/OSC1/RA7")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "INT/AN12/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "P1C/AN10/RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "P1B/AN8/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "PGM/C12IN2-/AN8/RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "P1D/AN11/RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "~{T1G}/AN13/RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 3.81)
				(name "ICSPCLK/RB6")
				(number "27")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 3.81)
				(name "ICSPDAT/RB7")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16F884-IP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 38.1 0)
		)
		(property "Value" "PIC16F884-IP"
			(at 6.35 35.56 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41291D.pdf"
			(at 0 0 0)
		)
		(property "Description" "4K Flash, 256B SRAM, 256B EEPROM, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
		(symbol "PIC16F884-IP_0_1")
		(symbol "PIC16F884-IP_1_1"
			(pin input line
				(at -27.94 30.48 0)
				(length 3.81)
				(name "RE3/~{MCLR}/Vpp")
				(number "1")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 3.81)
				(name "RA7/OSC1/CLKIN")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 3.81)
				(name "RA6/OSC2/CLKOUT")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 3.81)
				(name "RD0")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "RD1")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "RD2")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "RD3")
				(number "22")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RD4")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RD5/P1B")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RD6/P1C")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RD7/P1D")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "RE0/AN5")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "RE1/AN6")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 3.81)
				(name "RE2/AN7")
				(number "10")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 3.81)
				(name "C12IN0-/ULPWU/AN0/RA0")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 3.81)
				(name "C12IN1-/AN1/RA1")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 3.81)
				(name "C2IN+/CVref/Vref-/AN2/RA2")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 3.81)
				(name "C1IN+/Vref+/AN3/RA3")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 3.81)
				(name "C1OUT/T0CKI/RA4")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "C2OUT/~{SS}/AN4/RA5")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 3.81)
				(name "INT/AN12/RB0")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "C12IN3-/AN10/RB1")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "AN8/RB2")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "C12IN2-/PGM/AN9/RB3")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "AN11/RB4")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "~{T1G}/AN13/RB5")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "ICSPCLK/RB6")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "ICSPDAT/RB7")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "T10S0/T1CKI/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "T1OSI/CCP2/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "P1A/CCP1/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 3.81)
				(name "SCL/SCK/RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 3.81)
				(name "SDA/SDI/RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 3.81)
				(name "SDO/RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16LF1904-IP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 33.02 0)
		)
		(property "Value" "PIC16LF1904-IP"
			(at 1.27 -33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/40001569D.pdf"
			(at 0 0 0)
		)
		(property "Description" "4096W FLASH, 256B SRAM, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*40*"
			(at 0 0 0)
		)
		(symbol "PIC16LF1904-IP_0_1")
		(symbol "PIC16LF1904-IP_1_1"
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 3.81)
				(name "RA0")
				(number "2")
				(alternate "AN0" bidirectional line)
				(alternate "SEG12" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 3.81)
				(name "RA1")
				(number "3")
				(alternate "AN1" bidirectional line)
				(alternate "SEG7" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 3.81)
				(name "RA2")
				(number "4")
				(alternate "AN2" bidirectional line)
				(alternate "COM2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 3.81)
				(name "RA3")
				(number "5")
				(alternate "AN3" bidirectional line)
				(alternate "SEG15" bidirectional line)
				(alternate "VREF+" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 3.81)
				(name "RA4")
				(number "6")
				(alternate "SEG4" bidirectional line)
				(alternate "T0CKI" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 3.81)
				(name "RA5")
				(number "7")
				(alternate "AN4" bidirectional line)
				(alternate "SEG5" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "RA6")
				(number "14")
				(alternate "CLKOUT" bidirectional line)
				(alternate "SEG1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 3.81)
				(name "RA7")
				(number "13")
				(alternate "CLKIN" bidirectional line)
				(alternate "SEG2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "RB0")
				(number "33")
				(alternate "AN12" bidirectional line)
				(alternate "INT" bidirectional line)
				(alternate "SEG0" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "RB1")
				(number "34")
				(alternate "AN10" bidirectional line)
				(alternate "SEG24" bidirectional line)
				(alternate "VLCD1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 3.81)
				(name "RB2")
				(number "35")
				(alternate "AN8" bidirectional line)
				(alternate "SEG25" bidirectional line)
				(alternate "VLCD2" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "RB3")
				(number "36")
				(alternate "AN9" bidirectional line)
				(alternate "SEG26" bidirectional line)
				(alternate "VLCD3" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "RB4")
				(number "37")
				(alternate "AN11" bidirectional line)
				(alternate "COM0" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 3.81)
				(name "RB5")
				(number "38")
				(alternate "AN13" bidirectional line)
				(alternate "COM1" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "RB6/ICSPCLK")
				(number "39")
				(alternate "ICDCLK" bidirectional line)
				(alternate "SEG14" bidirectional line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "RB7/ICSPDAT")
				(number "40")
				(alternate "ICDDAT" bidirectional line)
				(alternate "SEG13" bidirectional line)
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin passive line
				(at 0 35.56 270)
				(length 3.81)
				(hide yes)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 3.81)
				(name "RC0")
				(number "15")
				(alternate "T1CKI" bidirectional line)
				(alternate "T1OSO" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 3.81)
				(name "RC1")
				(number "16")
				(alternate "T1OSI" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 3.81)
				(name "RC2")
				(number "17")
				(alternate "SEG3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 3.81)
				(name "RC3")
				(number "18")
				(alternate "SEG6" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 3.81)
				(name "RC4")
				(number "23")
				(alternate "SEG11" bidirectional line)
				(alternate "T1G" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 3.81)
				(name "RC5")
				(number "24")
				(alternate "SEG10" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "RC6")
				(number "25")
				(alternate "CK" bidirectional line)
				(alternate "SEG9" bidirectional line)
				(alternate "TX" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "RC7")
				(number "26")
				(alternate "DT" bidirectional line)
				(alternate "RX" bidirectional line)
				(alternate "SEG8" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "RD0")
				(number "19")
				(alternate "COM3" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "RD1")
				(number "20")
				(alternate "SEG27" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "RD2")
				(number "21")
				(alternate "SEG28" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "RD3")
				(number "22")
				(alternate "SEG16" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "RD4")
				(number "27")
				(alternate "SEG17" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "RD5")
				(number "28")
				(alternate "SEG18" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "RD6")
				(number "29")
				(alternate "SEG19" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 3.81)
				(name "RD7")
				(number "30")
				(alternate "SEG20" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 3.81)
				(name "RE0")
				(number "8")
				(alternate "AN5" bidirectional line)
				(alternate "SEG21" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 3.81)
				(name "RE1")
				(number "9")
				(alternate "AN6" bidirectional line)
				(alternate "SEG22" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 3.81)
				(name "RE2")
				(number "10")
				(alternate "AN7" bidirectional line)
				(alternate "SEG23" bidirectional line)
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 3.81)
				(name "~{MCLR}/RE3")
				(number "1")
				(alternate "VPP" bidirectional line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC16C505-IP"
		(extends "PIC16F505-IP")
		(property "Reference" "U"
			(at 5.08 12.7 0)
		)
		(property "Value" "PIC16C505-IP"
			(at 5.08 10.16 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "1024W ROM, 72B SRAM, DIP14"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROM-Based 8bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PDIP* DIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16C505-ISL"
		(extends "PIC16F505-ISL")
		(property "Reference" "U"
			(at 3.81 12.7 0)
		)
		(property "Value" "PIC16C505-ISL"
			(at 3.81 10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16C505, 1024W ROM, 72B SRAM, SO14"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROM-Based 8bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO* SOIC*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16C505-IST"
		(extends "PIC16F505-IST")
		(property "Reference" "U"
			(at 3.81 12.7 0)
		)
		(property "Value" "PIC16C505-IST"
			(at 3.81 10.16 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41236E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16C505, 1024W ROM, 72B SRAM, TSSOP14"
			(at 0 0 0)
		)
		(property "ki_keywords" "ROM-Based 8bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1454-ISL"
		(extends "PIC16F1454-IP")
		(property "Reference" "U"
			(at -46.99 15.24 0)
		)
		(property "Value" "PIC16F1454-ISL"
			(at -46.99 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "8192W FLASH, 1024B SRAM, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1454-ISS"
		(extends "PIC16F1454-IP")
		(property "Reference" "U"
			(at -46.99 15.24 0)
		)
		(property "Value" "PIC16F1454-ISS"
			(at -46.99 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "8192W FLASH, 1024B SRAM, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1454-IST"
		(extends "PIC16F1454-IP")
		(property "Reference" "U"
			(at -46.99 15.24 0)
		)
		(property "Value" "PIC16F1454-IST"
			(at -46.99 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "8192W FLASH, 1024B SRAM, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1455-ISL"
		(extends "PIC16F1455-IP")
		(property "Reference" "U"
			(at -46.99 17.78 0)
		)
		(property "Value" "PIC16F1455-ISL"
			(at -46.99 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "PIC16F1454, 8192W FLASH, 1024B SRAM, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1455-ISS"
		(extends "PIC16F1455-IP")
		(property "Reference" "U"
			(at -46.99 17.78 0)
		)
		(property "Value" "PIC16F1455-ISS"
			(at -46.99 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "PIC16F1454, 8192W FLASH, 1024B SRAM, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1455-IST"
		(extends "PIC16F1455-IP")
		(property "Reference" "U"
			(at -46.99 17.78 0)
		)
		(property "Value" "PIC16F1455-IST"
			(at -46.99 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "PIC16F1454, 8192W FLASH, 1024B SRAM, PDIP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1459-ISO"
		(extends "PIC16F1459-IP")
		(property "Reference" "U"
			(at -46.99 17.78 0)
		)
		(property "Value" "PIC16F1459-ISO"
			(at -46.99 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "PIC16F1454, 8192W FLASH, 1024B SRAM, PDIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1459-ISS"
		(extends "PIC16F1459-IP")
		(property "Reference" "U"
			(at -46.99 17.78 0)
		)
		(property "Value" "PIC16F1459-ISS"
			(at -46.99 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "PIC16F1454, 8192W FLASH, 1024B SRAM, PDIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1459-IST"
		(extends "PIC16F1459-IP")
		(property "Reference" "U"
			(at -46.99 17.78 0)
		)
		(property "Value" "PIC16F1459-IST"
			(at -46.99 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "PIC16F1454, 8192W FLASH, 1024B SRAM, PDIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1503-ISL"
		(extends "PIC16F1503-IP")
		(property "Reference" "U"
			(at -46.99 15.24 0)
		)
		(property "Value" "PIC16F1503-ISL"
			(at -46.99 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41607A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1503, 2048W FLASH, 128B SRAM, SO-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1503-IST"
		(extends "PIC16F1503-IP")
		(property "Reference" "U"
			(at -46.99 15.24 0)
		)
		(property "Value" "PIC16F1503-IST"
			(at -46.99 12.7 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41607A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1503, 2048W FLASH, 128B SRAM, TSSOP-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1507-ISO"
		(extends "PIC16F1507-IP")
		(property "Reference" "U"
			(at -27.94 20.32 0)
		)
		(property "Value" "PIC16F1507-ISO"
			(at -29.21 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41586A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1507, 2048W FLASH, 128B SRAM, SO-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1507-ISS"
		(extends "PIC16F1507-IP")
		(property "Reference" "U"
			(at -27.94 20.32 0)
		)
		(property "Value" "PIC16F1507-ISS"
			(at -29.21 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41586A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1507, 2048W FLASH, 128B SRAM, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1508-ISO"
		(extends "PIC16F1508-IP")
		(property "Reference" "U"
			(at -52.07 20.32 0)
		)
		(property "Value" "PIC16F1508-ISO"
			(at -52.07 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41609A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1508, 4096W FLASH, 256B SRAM, SO-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1508-ISS"
		(extends "PIC16F1508-IP")
		(property "Reference" "U"
			(at -52.07 20.32 0)
		)
		(property "Value" "PIC16F1508-ISS"
			(at -52.07 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41609A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1508, 4096W FLASH, 256B SRAM, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1509-ISO"
		(extends "PIC16F1509-IP")
		(property "Reference" "U"
			(at -52.07 20.32 0)
		)
		(property "Value" "PIC16F1509-ISO"
			(at -52.07 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41609A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1509, 8192W FLASH, 512B SRAM, SO-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1509-ISS"
		(extends "PIC16F1509-IP")
		(property "Reference" "U"
			(at -52.07 20.32 0)
		)
		(property "Value" "PIC16F1509-ISS"
			(at -52.07 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41609A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1509, 8192W FLASH, 512B SRAM, SSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1512-ISO"
		(extends "PIC16F1512-ISP")
		(property "Reference" "U"
			(at 5.08 30.48 0)
		)
		(property "Value" "PIC16F1512-ISO"
			(at 5.08 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41624A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1512, 2048W FLASH, 128B SRAM, SO-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1512-ISS"
		(extends "PIC16F1512-ISP")
		(property "Reference" "U"
			(at 5.08 30.48 0)
		)
		(property "Value" "PIC16F1512-ISS"
			(at 5.08 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41624A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1512, 2048W FLASH, 128B SRAM, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1513-ISO"
		(extends "PIC16F1513-ISP")
		(property "Reference" "U"
			(at 5.08 30.48 0)
		)
		(property "Value" "PIC16F1513-ISO"
			(at 5.08 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41624A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1513, 4096W FLASH, 2568B SRAM, SO-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1513-ISS"
		(extends "PIC16F1513-ISP")
		(property "Reference" "U"
			(at 5.08 30.48 0)
		)
		(property "Value" "PIC16F1513-ISS"
			(at 5.08 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41624A.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1513, 4096W FLASH, 2568B SRAM, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1516-ISO"
		(extends "PIC16F1516-ISP")
		(property "Reference" "U"
			(at 5.08 30.48 0)
		)
		(property "Value" "PIC16F1516-ISO"
			(at 5.08 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1516, 8192W FLASH, 512B SRAM, SO-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1516-ISS"
		(extends "PIC16F1516-ISP")
		(property "Reference" "U"
			(at 5.08 30.48 0)
		)
		(property "Value" "PIC16F1516-ISS"
			(at 5.08 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1516, 8192W FLASH, 512B SRAM, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1518-ISO"
		(extends "PIC16F1518-ISP")
		(property "Reference" "U"
			(at 2.54 30.48 0)
		)
		(property "Value" "PIC16F1518-ISO"
			(at 2.54 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1518, 16384W FLASH, 1024B SRAM, SO-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1518-ISS"
		(extends "PIC16F1518-ISP")
		(property "Reference" "U"
			(at 2.54 30.48 0)
		)
		(property "Value" "PIC16F1518-ISS"
			(at 2.54 27.94 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41452B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1518, 16384W FLASH, 1024B SRAM, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP* SO* SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1526-IMR"
		(extends "PIC16F1526-IPT")
		(property "Reference" "U"
			(at 5.08 48.26 0)
		)
		(property "Value" "PIC16F1526-IMR"
			(at 5.08 45.72 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41458B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1526, 8192W FLASH, 768B SRAM, UQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP* QFN*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1527-IMR"
		(extends "PIC16F1527-IPT")
		(property "Reference" "U"
			(at 5.08 48.26 0)
		)
		(property "Value" "PIC16F1527-IMR"
			(at 5.08 45.72 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41458B.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F1527, 16384W FLASH, 1536B SRAM, UQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP* QFN*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F15376-xML"
		(extends "PIC16F15375-xML")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16F15376-xML"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 29.21 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, QFN-44(8x8mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*8x8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F15376-xMV"
		(extends "PIC16F15375-xMV")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16F15376-xMV"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-40-1EP_5x5mm_P0.4mm_EP3.8x3.8mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 31.75 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, QFN-40(5x5mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F15376-xP"
		(extends "PIC16F15375-xP")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16F15376-xP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 27.94 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F15376-xPT"
		(extends "PIC16F15375-xPT")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16F15376-xPT"
			(at 0 0 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 30.48 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, TQFP-44(10x10mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F15385-xMV"
		(extends "PIC16F15386-xMV")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16F15385-xMV"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.6x4.6mm"
			(at 50.8 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 38.1 6.35 0)
		)
		(property "Description" "8KW FLASH, 1024B SRAM, QFN-48(6x6mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*6x6mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F15385-xPT"
		(extends "PIC16F15386-xPT")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16F15385-xPT"
			(at 0 0 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 39.37 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 38.1 7.62 0)
		)
		(property "Description" "8KW FLASH, 1024B SRAM, TQFP-48(7x7mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1786-xSO"
		(extends "PIC16F1786-xSP")
		(property "Reference" "U"
			(at 2.54 27.94 0)
		)
		(property "Value" "PIC16F1786-xSO"
			(at 2.54 25.4 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 -32.004 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001637C.pdf"
			(at 0 -34.0106 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 16KB Flash, 1KB RAM, 256B EEPROM, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1786-xSS"
		(extends "PIC16F1786-xSP")
		(property "Reference" "U"
			(at 2.54 27.94 0)
		)
		(property "Value" "PIC16F1786-xSS"
			(at 2.54 25.4 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 -32.004 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001637C.pdf"
			(at 0 -34.0106 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 16KB Flash, 1KB RAM, 256B EEPROM, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1829-ISL"
		(extends "PIC16F1829-IP")
		(property "Reference" "U"
			(at -24.13 22.86 0)
		)
		(property "Value" "PIC16F1829-ISL"
			(at -24.13 20.32 0)
		)
		(property "Footprint" ""
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41440C.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "Flash-Based, 8-Bit CMOS Microcontrollers, SOIC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1829-ISO"
		(extends "PIC16F1829-IP")
		(property "Reference" "U"
			(at -24.13 22.86 0)
		)
		(property "Value" "PIC16F1829-ISO"
			(at -24.13 20.32 0)
		)
		(property "Footprint" ""
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41440C.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "Flash-Based, 8-Bit CMOS Microcontrollers, SOIC"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1829-ISS"
		(extends "PIC16F1829-IP")
		(property "Reference" "U"
			(at -24.13 22.86 0)
		)
		(property "Value" "PIC16F1829-ISS"
			(at -24.13 20.32 0)
		)
		(property "Footprint" ""
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41440C.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "Flash-Based, 8-Bit CMOS Microcontrollers, SSOP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1829-IST"
		(extends "PIC16F1829-IP")
		(property "Reference" "U"
			(at -24.13 22.86 0)
		)
		(property "Value" "PIC16F1829-IST"
			(at -24.13 20.32 0)
		)
		(property "Footprint" ""
			(at 0 -13.97 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41440C.pdf"
			(at 0 -13.97 0)
		)
		(property "Description" "Flash-Based, 8-Bit CMOS Microcontrollers, TSSOP"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* SOIC*3.9x8.7mm*P1.27mm* TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F18344-xSL"
		(extends "PIC16F18324-xSL")
		(property "Reference" "U"
			(at -13.97 10.16 0)
		)
		(property "Value" "PIC16F18344-xSL"
			(at 1.27 10.16 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -7.62 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/40001800c.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "PIC16F18324, 4096W FLASH, 512B SRAM, 256B EEPROM, SOIC14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F18855-xSO"
		(extends "PIC16F18854-xSO")
		(property "Reference" "U"
			(at 2.54 27.94 0)
		)
		(property "Value" "PIC16F18855-xSO"
			(at 10.16 25.4 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 1.27 -27.94 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001802G.pdf"
			(at 15.24 -7.62 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 14KB Flash, 1024B RAM 256B EEPROM, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power CRC DSM  ADC^2 CLC PLL 32MHz"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F19196-x5LX"
		(extends "PIC16F19195-x5LX")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16F19196-x5LX"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "16kW FLASH, 2kB RAM, 256B EEPROM, VQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F19196-xMR"
		(extends "PIC16F19195-xMR")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16F19196-xMR"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "16kW FLASH, 2kB RAM, 256B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F19196-xPT"
		(extends "PIC16F19195-xPT")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16F19196-xPT"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "16kW FLASH, 2kB RAM, 256B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F19197-x5LX"
		(extends "PIC16F19195-x5LX")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16F19197-x5LX"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "32kW FLASH, 4kB RAM, 256B EEPROM, VQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F19197-xMR"
		(extends "PIC16F19195-xMR")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16F19197-xMR"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "32kW FLASH, 4kB RAM, 256B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F19197-xPT"
		(extends "PIC16F19195-xPT")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16F19197-xPT"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "32kW FLASH, 4kB RAM, 256B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1937-IML"
		(extends "PIC16F1934-IML")
		(property "Reference" "U"
			(at -41.91 35.56 0)
		)
		(property "Value" "PIC16F1937-IML"
			(at -41.91 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41364E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F193XLF193X - Flash-Based, 8-Bit CMOS Microcontrollers, QFN-44"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1937-IPT"
		(extends "PIC16F1934-IPT")
		(property "Reference" "U"
			(at -41.91 35.56 0)
		)
		(property "Value" "PIC16F1937-IPT"
			(at -41.91 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41364E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F193XLF193X - Flash-Based, 8-Bit CMOS Microcontrollers, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1939-IML"
		(extends "PIC16F1934-IML")
		(property "Reference" "U"
			(at -41.91 35.56 0)
		)
		(property "Value" "PIC16F1939-IML"
			(at -41.91 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41364E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F193XLF193X - Flash-Based, 8-Bit CMOS Microcontrollers, QFN-44"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F1939-IPT"
		(extends "PIC16F1934-IPT")
		(property "Reference" "U"
			(at -41.91 35.56 0)
		)
		(property "Value" "PIC16F1939-IPT"
			(at -41.91 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41364E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F193XLF193X - Flash-Based, 8-Bit CMOS Microcontrollers, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F628-xxIP"
		(extends "PIC16F627-xxIP")
		(property "Reference" "U"
			(at -24.13 17.78 0)
		)
		(property "Value" "PIC16F628-xxIP"
			(at -24.13 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40300c.pdf"
			(at 0 0 0)
		)
		(property "Description" "2048W Flash, 224B SRAM, 128B EEPROM, DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F628-xxISO"
		(extends "PIC16F627-xxISO")
		(property "Reference" "U"
			(at -24.13 17.78 0)
		)
		(property "Value" "PIC16F628-xxISO"
			(at -24.13 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40300c.pdf"
			(at 0 0 0)
		)
		(property "Description" "2048W Flash, 224B SRAM, 128B EEPROM, SO18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F628-xxISS"
		(extends "PIC16F627-xxISS")
		(property "Reference" "U"
			(at 5.08 17.78 0)
		)
		(property "Value" "PIC16F628-xxISS"
			(at 3.81 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40300c.pdf"
			(at 0 0 0)
		)
		(property "Description" "2048W Flash, 224B SRAM, 128B EEPROM, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F628A-IP"
		(extends "PIC16F627A-IP")
		(property "Reference" "U"
			(at -24.13 17.78 0)
		)
		(property "Value" "PIC16F628A-IP"
			(at -24.13 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40300c.pdf"
			(at 0 0 0)
		)
		(property "Description" "2048W Flash, 224B SRAM, 128B EEPROM, DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F628A-ISO"
		(extends "PIC16F627A-ISO")
		(property "Reference" "U"
			(at -24.13 17.78 0)
		)
		(property "Value" "PIC16F628A-ISO"
			(at -24.13 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40300c.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F628A, 2048W Flash, 224B SRAM, 128B EEPROM, SO18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F628A-ISS"
		(extends "PIC16F627A-ISS")
		(property "Reference" "U"
			(at 5.08 17.78 0)
		)
		(property "Value" "PIC16F628A-ISS"
			(at 5.08 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40044G.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F628A, 2048W Flash, 224B SRAM, 128B EEPROM, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F648A-IP"
		(extends "PIC16F627A-IP")
		(property "Reference" "U"
			(at -24.13 17.78 0)
		)
		(property "Value" "PIC16F648A-IP"
			(at -24.13 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40300c.pdf"
			(at 0 0 0)
		)
		(property "Description" "4096W Flash, 256B SRAM, 256B EEPROM, DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F648A-ISO"
		(extends "PIC16F627A-ISO")
		(property "Reference" "U"
			(at -24.13 17.78 0)
		)
		(property "Value" "PIC16F648A-ISO"
			(at -24.13 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40300c.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F648A, 4096W Flash, 256B SRAM, 256B EEPROM, SO18"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F648A-ISS"
		(extends "PIC16F627A-ISS")
		(property "Reference" "U"
			(at 5.08 17.78 0)
		)
		(property "Value" "PIC16F648A-ISS"
			(at 5.08 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40044G.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F648A, 4096W Flash, 256B SRAM, 256B EEPROM, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F689-IP"
		(extends "PIC16F687-IP")
		(property "Reference" "U"
			(at 17.78 20.32 0)
		)
		(property "Value" "PIC16F689-IP"
			(at 17.78 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "4096W Flash, 256B SRAM, 256B EEPROM, DIP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F689-ISO"
		(extends "PIC16F687-ISO")
		(property "Reference" "U"
			(at 16.51 20.32 0)
		)
		(property "Value" "PIC16F689-ISO"
			(at 16.51 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F689, 4096W Flash, 256B SRAM, 256B EEPROM, SO20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F689-ISS"
		(extends "PIC16F687-ISS")
		(property "Reference" "U"
			(at 16.51 20.32 0)
		)
		(property "Value" "PIC16F689-ISS"
			(at 16.51 17.78 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41262E.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F689, 4096W Flash, 256B SRAM, 256B EEPROM, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F76-IML"
		(extends "PIC16F73-IML")
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F76-IML"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30325b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F76, 8K Flash, 368B SRAM, ADC, PWM, MLF28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MLF*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F76-ISO"
		(extends "PIC16F73-ISO")
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F76-ISO"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30325b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F76, 8K Flash, 368B SRAM, ADC, PWM, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F76-ISP"
		(extends "PIC16F73-ISP")
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F76-ISP"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30325b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F76, 8K Flash, 368B SRAM, ADC, PWM, SDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F76-ISS"
		(extends "PIC16F73-ISS")
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F76-ISS"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30325b.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F76, 8K Flash, 368B SRAM, ADC, PWM, SSOP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F77-IP"
		(extends "PIC16F74-IP")
		(property "Reference" "U"
			(at 6.35 35.56 0)
		)
		(property "Value" "PIC16F77-IP"
			(at 6.35 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30325b.pdf"
			(at 0 0 0)
		)
		(property "Description" "8K Flash, 368B SRAM, ADC, PWM, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F819-IML"
		(extends "PIC16F818-IML")
		(property "Reference" "U"
			(at 5.08 17.78 0)
		)
		(property "Value" "PIC16F819-IML"
			(at 5.08 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39598F.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F819, 3584B Flash, 256B SRAM, 256B EEPROM, ADC, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F819-IP"
		(extends "PIC16F818-IP")
		(property "Reference" "U"
			(at 3.81 17.78 0)
		)
		(property "Value" "PIC16F819-IP"
			(at 3.81 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39598F.pdf"
			(at 0 0 0)
		)
		(property "Description" "3584B Flash, 256B SRAM, 256B EEPROM, ADC, DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F819-ISO"
		(extends "PIC16F818-ISO")
		(property "Reference" "U"
			(at 5.08 17.78 0)
		)
		(property "Value" "PIC16F819-ISO"
			(at 5.08 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39598F.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F819, 3584B Flash, 256B SRAM, 256B EEPROM, ADC, SOIC18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F819-ISS"
		(extends "PIC16F818-ISS")
		(property "Reference" "U"
			(at 6.35 17.78 0)
		)
		(property "Value" "PIC16F819-ISS"
			(at 6.35 15.24 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39598F.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F819, 3584B Flash, 256B SRAM, 256B EEPROM, ADC, SSSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F84-XXP"
		(extends "PIC16F83-XXP")
		(property "Reference" "U"
			(at 2.54 22.86 0)
		)
		(property "Value" "PIC16F84-XXP"
			(at 2.54 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30430c.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F84, 1K Flash, 68B SRAM, 64B EEPROM, DIP18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F84-XXSO"
		(extends "PIC16F83-XXSO")
		(property "Reference" "U"
			(at 2.54 22.86 0)
		)
		(property "Value" "PIC16F84-XXSO"
			(at 2.54 20.32 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30430c.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F84, 1KB Flash, 68B SRAM, 64B EEPROM, SOIC18"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F876-XXISO"
		(extends "PIC16F873-XXISO")
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F876-XXISO"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30292C.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F876, 8K Flash, 386B SRAM, 256B EEPROM, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F876-XXISP"
		(extends "PIC16F873-XXISP")
		(property "Reference" "U"
			(at 2.54 25.4 0)
		)
		(property "Value" "PIC16F876-XXISP"
			(at 2.54 22.86 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30292C.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F876, 8K Flash, 386B SRAM, 256B EEPROM, SDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F877-XXIP"
		(extends "PIC16F874-XXIP")
		(property "Reference" "U"
			(at 5.08 35.56 0)
		)
		(property "Value" "PIC16F877-XXIP"
			(at 5.08 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30292C.pdf"
			(at 0 0 0)
		)
		(property "Description" "PIC16F877, 8K Flash, 386B SRAM, 256B EEPROM, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F877A-IP"
		(extends "PIC16F874A-IP")
		(property "Reference" "U"
			(at 5.08 35.56 0)
		)
		(property "Value" "PIC16F877A-IP"
			(at 5.08 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39582b.pdf"
			(at 0 0 0)
		)
		(property "Description" "8W Flash, 386B SRAM, 256B EEPROM, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F877A-IPT"
		(extends "PIC16F874A-IPT")
		(property "Reference" "U"
			(at 5.08 35.56 0)
		)
		(property "Value" "PIC16F877A-IPT"
			(at 5.08 33.02 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "PIC16F874A, 4W Flash, 192B SRAM, 128B EEPROM, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F883-IP"
		(extends "PIC16F882-IP")
		(property "Reference" "U"
			(at 13.97 27.94 0)
		)
		(property "Value" "PIC16F883-IP"
			(at 13.97 25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41291D.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "4K Flash, 256B SRAM, 256B EEPROM, XLP, DIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F886-IP"
		(extends "PIC16F882-IP")
		(property "Reference" "U"
			(at 13.97 27.94 0)
		)
		(property "Value" "PIC16F886-IP"
			(at 13.97 25.4 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41291D.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "8K Flash, 256B SRAM, 256B EEPROM, XLP, DIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16F887-IP"
		(extends "PIC16F884-IP")
		(property "Reference" "U"
			(at 6.35 38.1 0)
		)
		(property "Value" "PIC16F887-IP"
			(at 6.35 35.56 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41291D.pdf"
			(at 0 0 0)
		)
		(property "Description" "8K Flash, 368B SRAM, 256B EEPROM, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP* PDIP*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15356-xML"
		(extends "PIC16F15356-xML")
		(property "Reference" "U?"
			(at 16.51 -24.13 0)
		)
		(property "Value" "PIC16LF15356-xML"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at -1.27 11.43 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 22.86 2.54 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, QFN-28(6x6mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*6x6mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15356-xMV"
		(extends "PIC16F15356-xMV")
		(property "Reference" "U?"
			(at 16.51 -24.13 0)
		)
		(property "Value" "PIC16LF15356-xMV"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_4x4mm_P0.4mm_EP2.3x2.3mm"
			(at 0 8.89 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 22.86 2.54 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, QFN-28(4x4mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15356-xSO"
		(extends "PIC16F15356-xSO")
		(property "Reference" "U?"
			(at 17.78 -24.13 0)
		)
		(property "Value" "PIC16LF15356-xSO"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at -21.59 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at -21.59 12.7 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*.5x17.9mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15356-xSP"
		(extends "PIC16F15356-xSP")
		(property "Reference" "U?"
			(at 17.78 -24.13 0)
		)
		(property "Value" "PIC16LF15356-xSP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at -20.32 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at -20.32 12.7 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15356-xSS"
		(extends "PIC16F15356-xSS")
		(property "Reference" "U?"
			(at 17.78 -24.13 0)
		)
		(property "Value" "PIC16LF15356-xSS"
			(at 0 0 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at -21.59 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at -21.59 12.7 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15375-xML"
		(extends "PIC16F15375-xML")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16LF15375-xML"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 29.21 0)
		)
		(property "Description" "8KW FLASH, 1024B SRAM, QFN-44(8x8mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*8x8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15375-xMV"
		(extends "PIC16F15375-xMV")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16LF15375-xMV"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-40-1EP_5x5mm_P0.4mm_EP3.8x3.8mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 31.75 0)
		)
		(property "Description" "8KW FLASH, 1024B SRAM, QFN-40(5x5mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15375-xP"
		(extends "PIC16F15375-xP")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16LF15375-xP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 27.94 0)
		)
		(property "Description" "8KW FLASH, 1024B SRAM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15375-xPT"
		(extends "PIC16F15375-xPT")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16LF15375-xPT"
			(at 0 0 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 30.48 0)
		)
		(property "Description" "8KW FLASH, 1024B SRAM, TQFP-44(10x10mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15376-xML"
		(extends "PIC16F15375-xML")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16LF15376-xML"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 29.21 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, QFN-44(8x8mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*8x8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15376-xMV"
		(extends "PIC16F15375-xMV")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16LF15376-xMV"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-40-1EP_5x5mm_P0.4mm_EP3.8x3.8mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 31.75 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, QFN-40(5x5mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15376-xP"
		(extends "PIC16F15375-xP")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16LF15376-xP"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 27.94 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15376-xPT"
		(extends "PIC16F15375-xPT")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16LF15376-xPT"
			(at 0 0 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 35.56 30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 35.56 30.48 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, TQFP-44(10x10mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15385-xMV"
		(extends "PIC16F15386-xMV")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16LF15385-xMV"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.6x4.6mm"
			(at 50.8 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 38.1 6.35 0)
		)
		(property "Description" "8KW FLASH, 1024B SRAM, QFN-48(6x6mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*6x6mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15385-xPT"
		(extends "PIC16F15386-xPT")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16LF15385-xPT"
			(at 0 0 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 39.37 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 38.1 7.62 0)
		)
		(property "Description" "8KW FLASH, 1024B SRAM, TQFP-48(7x7mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15386-xMV"
		(extends "PIC16F15386-xMV")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16LF15386-xMV"
			(at 0 0 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_6x6mm_P0.4mm_EP4.6x4.6mm"
			(at 50.8 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 38.1 6.35 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, QFN-48(6x6mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*6x6mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF15386-xPT"
		(extends "PIC16F15386-xPT")
		(property "Reference" "U?"
			(at 16.51 -36.83 0)
		)
		(property "Value" "PIC16LF15386-xPT"
			(at 0 0 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 39.37 12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF15356-75-76-85-86-Data%20Sheet-40001866B.pdf"
			(at 38.1 7.62 0)
		)
		(property "Description" "16KW FLASH, 2048B SRAM, TQFP-48(7x7mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF1786-xML"
		(extends "PIC16F1786-xML")
		(property "Reference" "U"
			(at 2.54 27.94 0)
		)
		(property "Value" "PIC16LF1786-xML"
			(at 2.54 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 -32.004 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001637C.pdf"
			(at 0 -34.0106 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 16KB Flash, 1KB RAM, 256B EEPROM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF1786-xP"
		(extends "PIC16F1786-xP")
		(property "Reference" "U"
			(at 2.54 27.94 0)
		)
		(property "Value" "PIC16LF1786-xP"
			(at 2.54 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -38.354 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001637C.pdf"
			(at 0 -34.0106 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 16KB Flash, 1KB RAM, 256B EEPROM, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF1786-xSO"
		(extends "PIC16F1786-xSP")
		(property "Reference" "U"
			(at 2.54 27.94 0)
		)
		(property "Value" "PIC16LF1786-xSO"
			(at 2.54 25.4 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 -32.004 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001637C.pdf"
			(at 0 -34.0106 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 16KB Flash, 1KB RAM, 256B EEPROM, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF1786-xSP"
		(extends "PIC16F1786-xSP")
		(property "Reference" "U"
			(at 2.54 27.94 0)
		)
		(property "Value" "PIC16LF1786-xSP"
			(at 2.54 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 -32.004 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001637C.pdf"
			(at 0 -34.0106 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 16KB Flash, 1KB RAM, 256B EEPROM, SPDIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF1786-xSS"
		(extends "PIC16F1786-xSP")
		(property "Reference" "U"
			(at 2.54 27.94 0)
		)
		(property "Value" "PIC16LF1786-xSS"
			(at 2.54 25.4 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 -32.004 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001637C.pdf"
			(at 0 -34.0106 0)
		)
		(property "Description" "8-bit Flash MCU, 32MHz, 16KB Flash, 1KB RAM, 256B EEPROM, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF18325-ISL"
		(extends "PIC16F18325-ISL")
		(property "Reference" "U"
			(at -58.42 15.24 0)
		)
		(property "Value" "PIC16LF18325-ISL"
			(at -58.42 12.7 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -15.24 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/40001795b.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "PIC16LF18325, 8192W FLASH, 1024B SRAM, SOIC14"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF18325-xGZ"
		(extends "PIC16F18325-xGZ")
		(property "Reference" "U"
			(at -12.7 13.97 0)
		)
		(property "Value" "PIC16LF18325-xGZ"
			(at 10.16 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-20-1EP_4x4mm_P0.5mm_EP2.8x2.8mm"
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001795E.pdf"
			(at 0 0 0)
		)
		(property "Description" "8192W FLASH, 1024B SRAM, 256B EEPROM, QFN-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF18325-xJQ"
		(extends "PIC16F18325-xJQ")
		(property "Reference" "U"
			(at -13.97 11.43 0)
		)
		(property "Value" "PIC16LF18325-xJQ"
			(at 10.16 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:UQFN-16-1EP_4x4mm_P0.65mm_EP2.6x2.6mm"
			(at 0 -22.86 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001795E.pdf"
			(at 0 0 0)
		)
		(property "Description" "8192W FLASH, 1024B SRAM, 256B EEPROM,  QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UQFN*1EP*4x4mm*P0.65mm*EP2.6x2.6mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF1907-IP"
		(extends "PIC16LF1904-IP")
		(property "Reference" "U"
			(at -11.43 33.02 0)
		)
		(property "Value" "PIC16LF1907-IP"
			(at 1.27 -33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/40001569D.pdf"
			(at 0 0 0)
		)
		(property "Description" "8192W FLASH, 512B SRAM, PDIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*40*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF19195-x5LX"
		(extends "PIC16F19195-x5LX")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16LF19195-x5LX"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "8kW FLASH, 1kB RAM, 256B EEPROM, VQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF19195-xMR"
		(extends "PIC16F19195-xMR")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16LF19195-xMR"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "8kW FLASH, 1kB RAM, 256B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF19195-xPT"
		(extends "PIC16F19195-xPT")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16LF19195-xPT"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "8kW FLASH, 1kB RAM, 256B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF19196-x5LX"
		(extends "PIC16F19195-x5LX")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16LF19196-x5LX"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "16kW FLASH, 2kB RAM, 256B EEPROM, VQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF19196-xMR"
		(extends "PIC16F19195-xMR")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16LF19196-xMR"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "16kW FLASH, 2kB RAM, 256B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF19196-xPT"
		(extends "PIC16F19195-xPT")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16LF19196-xPT"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "16kW FLASH, 2kB RAM, 256B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF19197-x5LX"
		(extends "PIC16F19195-x5LX")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16LF19197-x5LX"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:VQFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "32kW FLASH, 4kB RAM, 256B EEPROM, VQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "VQFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF19197-xMR"
		(extends "PIC16F19195-xMR")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16LF19197-xMR"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP5.4x5.4mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "32kW FLASH, 4kB RAM, 256B EEPROM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC16LF19197-xPT"
		(extends "PIC16F19195-xPT")
		(property "Reference" "U"
			(at -16.51 46.99 0)
		)
		(property "Value" "PIC16LF19197-xPT"
			(at 11.43 -46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at -1.27 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC16LF19195-6-7-Data-Sheet-40001873D.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "32kW FLASH, 4kB RAM, 256B EEPROM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 8-Bit CMOS Microcontroller Low Power"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
