(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "PIC18F1220-SO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "PIC18F1220-SO"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39605F.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "18-Pin Flash Microcontroller 4K Flash 256byte RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "RAM ADC UART PWM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x11.6mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F1220-SO_0_1")
		(symbol "PIC18F1220-SO_1_1"
			(pin input line
				(at -33.02 10.16 0)
				(length 2.54)
				(name "~{MCLR}/Vpp/RA5")
				(number "4")
			)
			(pin input line
				(at -33.02 7.62 0)
				(length 2.54)
				(name "RA0/AN0")
				(number "1")
			)
			(pin input line
				(at -33.02 5.08 0)
				(length 2.54)
				(name "RA1/AN1/LVDIN")
				(number "2")
			)
			(pin input line
				(at -33.02 2.54 0)
				(length 2.54)
				(name "RA2/AN2/Vref-")
				(number "6")
			)
			(pin input line
				(at -33.02 0 0)
				(length 2.54)
				(name "RA3/AN3/Vref+")
				(number "7")
			)
			(pin input line
				(at -33.02 -2.54 0)
				(length 2.54)
				(name "RA4/TOCKI")
				(number "3")
			)
			(pin input line
				(at -33.02 -5.08 0)
				(length 2.54)
				(name "OSC1/CLKI/RA7")
				(number "16")
			)
			(pin input line
				(at -33.02 -7.62 0)
				(length 2.54)
				(name "OSC2/CLKO/RA6")
				(number "15")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "Vdd")
				(number "14")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "Vss")
				(number "5")
			)
			(pin input line
				(at 33.02 10.16 180)
				(length 2.54)
				(name "INT0/AN4/RB0")
				(number "8")
			)
			(pin input line
				(at 33.02 7.62 180)
				(length 2.54)
				(name "INT1/CK/TX/AN5/RB1")
				(number "9")
			)
			(pin input line
				(at 33.02 5.08 180)
				(length 2.54)
				(name "INT2/P1B/RB2")
				(number "17")
			)
			(pin input line
				(at 33.02 2.54 180)
				(length 2.54)
				(name "P1A/CCP1/RB3")
				(number "18")
			)
			(pin input line
				(at 33.02 0 180)
				(length 2.54)
				(name "KBI0/DT/RX/AN6/RB4")
				(number "10")
			)
			(pin input line
				(at 33.02 -2.54 180)
				(length 2.54)
				(name "KBI1/PGM/RB5")
				(number "11")
			)
			(pin input line
				(at 33.02 -5.08 180)
				(length 2.54)
				(name "KBI2/P1C/T13CKI/T1OSO/PGC/RB6")
				(number "12")
			)
			(pin input line
				(at 33.02 -7.62 180)
				(length 2.54)
				(name "KBI3/P1D/T1OSI/PGD/RB7")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F13K50-EP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "PIC18F13K50-EP"
			(at 24.13 -17.78 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/41350c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "8K Flash, 512 SRAM, 256 EEPROM, USB, nanoWatt XLP, DIP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F13K50-EP_0_1")
		(symbol "PIC18F13K50-EP_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RA0/IOCA0/D+/PGD")
				(number "19")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RA1/IOCA1/D-/PGC")
				(number "18")
			)
			(pin input line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RA3/IOCA3/~{MCLR}/Vpp")
				(number "4")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RA4/IOCA3/AN3/OSC2/CLKOUT")
				(number "3")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RA5/IOCA5/OSC1/CLKIN")
				(number "2")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RB4/IOCB4/AN10/SDI/SDA")
				(number "13")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 3.81)
				(name "RB5/IOCB5/AN11/RX/DT")
				(number "12")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 3.81)
				(name "RB6/IOCB6/SCK/SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 3.81)
				(name "RB7/IOCB7/TX/CK")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "INT0/C12IN+/VREF+/AN4/RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "INT1/C12IN1-/VREF-AN5/RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "INT2/CVREF/C12IN2-/P1D/AN6/RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "PGM/C12IN3-/P1C/AN7/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "SRQ/C12OUT/P1B/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T0CKI/CCP1/P1A/RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 3.81)
				(name "T1OSCI/T13CKI/SS/AN8/RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "T1OSCO/SDO/AN9/RC7")
				(number "9")
			)
			(pin passive line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "VUSB")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F13K50-ESO"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "PIC18F13K50-ESO"
			(at 22.86 -17.78 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/41350c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "8K Flash, 512 SRAM, 256 EEPROM, USB, nanoWatt XLP, SOIC20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F13K50-ESO_0_1")
		(symbol "PIC18F13K50-ESO_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RA0/IOCA0/D+/PGD")
				(number "19")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RA1/IOCA1/D-/PGC")
				(number "18")
			)
			(pin input line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RA3/IOCA3/~{MCLR}/Vpp")
				(number "4")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RA4/IOCA3/AN3/OSC2/CLKOUT")
				(number "3")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RA5/IOCA5/OSC1/CLKIN")
				(number "2")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RB4/IOCB4/AN10/SDI/SDA")
				(number "13")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 3.81)
				(name "RB5/IOCB5/AN11/RX/DT")
				(number "12")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 3.81)
				(name "RB6/IOCB6/SCK/SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 3.81)
				(name "RB7/IOCB7/TX/CK")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "INT0/C12IN+/VREF+/AN4/RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "INT1/C12IN1-/VREF-AN5/RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "INT2/CVREF/C12IN2-/P1D/AN6/RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "PGM/C12IN3-/P1C/AN7/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "SRQ/C12OUT/P1B/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T0CKI/CCP1/P1A/RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 3.81)
				(name "T1OSCI/T13CKI/SS/AN8/RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "T1OSCO/SDO/AN9/RC7")
				(number "9")
			)
			(pin passive line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "VUSB")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F13K50-ESS"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "PIC18F13K50-ESS"
			(at 22.86 -17.78 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/41350c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "8K Flash, 512 SRAM, 256 EEPROM, USB, nanoWatt XLP, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F13K50-ESS_0_1")
		(symbol "PIC18F13K50-ESS_1_1"
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 3.81)
				(name "RA0/IOCA0/D+/PGD")
				(number "19")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 3.81)
				(name "RA1/IOCA1/D-/PGC")
				(number "18")
			)
			(pin input line
				(at -38.1 7.62 0)
				(length 3.81)
				(name "RA3/IOCA3/~{MCLR}/Vpp")
				(number "4")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 3.81)
				(name "RA4/IOCA3/AN3/OSC2/CLKOUT")
				(number "3")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 3.81)
				(name "RA5/IOCA5/OSC1/CLKIN")
				(number "2")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 3.81)
				(name "RB4/IOCB4/AN10/SDI/SDA")
				(number "13")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 3.81)
				(name "RB5/IOCB5/AN11/RX/DT")
				(number "12")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 3.81)
				(name "RB6/IOCB6/SCK/SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 3.81)
				(name "RB7/IOCB7/TX/CK")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 3.81)
				(name "INT0/C12IN+/VREF+/AN4/RC0")
				(number "16")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 3.81)
				(name "INT1/C12IN1-/VREF-AN5/RC1")
				(number "15")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 3.81)
				(name "INT2/CVRef/C12IN2-/P1D/AN6/RC2")
				(number "14")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 3.81)
				(name "PGM/C12IN3-/P1C/AN7/RC3")
				(number "7")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 3.81)
				(name "SRQ/C12OUT/P1B/RC4")
				(number "6")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 3.81)
				(name "T0CKI/CCP1/P1A/RC5")
				(number "5")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 3.81)
				(name "T1OSCI/T13CKI/SS/AN8/RC6")
				(number "8")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 3.81)
				(name "T1OSCO/SDO/AN9/RC7")
				(number "9")
			)
			(pin passive line
				(at 38.1 -10.16 180)
				(length 3.81)
				(name "VUSB")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F2331-IML"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18F2331-IML"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "8K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F2331-IML_0_1")
		(symbol "PIC18F2331-IML_1_1"
			(pin input line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CAP1/INDX")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "RA3/AN3/Vref+/CAP2/QEA")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "RA4/AN4/CAP3/QEB")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKI")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RB0/PWM0")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RB1/PWM1")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RB2/PWM2")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RB3/PWM3")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RB4/KBI0/PWM5")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RB5/KBI1/PWM4/PGM")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "25")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 3.81)
				(name "AVDD")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "AVSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "~{FLTA}/T1OSI/CCP2/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "~{FLTB}/CCP1/RC2")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "INT0/T5CKI/T0CKI/RC3")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "INT1/SDI/SDA/RC4")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "INT2/SCK/SCL/RC5")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "TX/~{SS}/CK/RC6")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "RX/SDO/DT/RC7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F2331-ISO"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18F2331-ISO"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "8K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F2331-ISO_0_1")
		(symbol "PIC18F2331-ISO_1_1"
			(pin input line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CAP1/INDX")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "RA3/AN3/Vref+/CAP2/QEA")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "RA4/AN4/CAP3/QEB")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKI")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RB0/PWM0")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RB1/PWM1")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RB2/PWM2")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RB3/PWM3")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RB4/KBI0/PWM5")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RB5/KBI1/PWM4/PGM")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 3.81)
				(name "AVDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "AVSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "~{FLTA}/T1OSI/CCP2/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "~{FLTB}/CCP1/RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "INT0/T5CKI/T0CKI/RC3")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "INT1/SDI/SDA/RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "INT2/SCK/SCL/RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "TX/~{SS}/CK/RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "RX/SDO/DT/RC7")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F2331-ISP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18F2331-ISP"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "8K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F2331-ISP_0_1")
		(symbol "PIC18F2331-ISP_1_1"
			(pin input line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CAP1/INDX")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "RA3/AN3/Vref+/CAP2/QEA")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "RA4/AN4/CAP3/QEB")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKI")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RB0/PWM0")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RB1/PWM1")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RB2/PWM2")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RB3/PWM3")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RB4/KBI0/PWM5")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RB5/KBI1/PWM4/PGM")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 3.81)
				(name "AVDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "AVSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "~{FLTA}/T1OSI/CCP2/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "~{FLTB}/CCP1/RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "INT0/T5CKI/T0CKI/RC3")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "INT1/SDI/SDA/RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "INT2/SCK/SCL/RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "TX/~{SS}/CK/RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "RX/SDO/DT/RC7")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F23K20_ISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "PIC18F23K20_ISS"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at -12.7 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001303H.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "8K Flash, 512Byte RAM, 256Byte EEPROM, PIC18 Microcontroller ADC PWM SPI I2C USART in SSOP28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller PIC18F flash XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F23K20_ISS_0_1")
		(symbol "PIC18F23K20_ISS_1_1"
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "RA2/Vref-AN2")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RA3/Vref+AN3")
				(number "5")
			)
			(pin power_in line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RA5/AN4")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "~{MCLR}/RE3")
				(number "1")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RA6/OSC2/CLKOUT")
				(number "10")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "RA7/OSC1/CLKIN")
				(number "9")
			)
			(pin power_in line
				(at -5.08 -25.4 90)
				(length 2.54)
				(name "Vss")
				(number "8")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "Vdd")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "Vss")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "AN12/INT0/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "AN10/INT1/RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "AN8/INT2/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "AN9/RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "AN11/RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PGM/RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PGC/RB6")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PGD/RB7")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "CCP2/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "CCP1/RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "SCL/SCK/RC3")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "SDA/SDI/RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "SDO/RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "TX/RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RX/RC7")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F23K22-xSO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "PIC18F23K22-xSO"
			(at 12.7 25.4 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 5.08 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001412G.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "8K Flash, 512B SRAM, 256B EEPROM, nanoWatt XLP, 2.3V to 5.5V, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F23K22-xSO_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "~{MCLR}/VPP/RE3")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "RA5")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "RA6/OSC2_CLKOUT")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "RA7/OSC1_CLKIN")
				(number "9")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "19")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "RB6/PGC")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "RB7/PGD")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "RC0/SOSCO")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "RC1/SOSCI")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "RC3")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "RC7")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F23K22-xSP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "PIC18F23K22-xSP"
			(at 12.7 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 1.27 0.635 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001412G.pdf"
			(at 1.27 0.635 0)
		)
		(property "Description" "8K Flash, 512B SRAM, 256B EEPROM, nanoWatt XLP, 2.3V to 5.5V, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F23K22-xSP_1_1"
			(pin input line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "~{MCLR}/VPP/RE3")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "RA5")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "RA6/OSC2_CLKOUT")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "RA7/OSC1_CLKIN")
				(number "9")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "19")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "RB6/PGC")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "RB7/PGD")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "RC0/SOSCO")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "RC1/SOSCI")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "RC3")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "RC7")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F2420-xML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 26.67 0)
		)
		(property "Value" "PIC18F2420-xML"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39631E.pdf"
			(at -33.02 10.16 0)
		)
		(property "Description" "MCU 16k Flash, 768B SRAM, 256B EEPROM, ADC, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F2420-xML_0_1")
		(symbol "PIC18F2420-xML_1_1"
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "RE3/~{MCLR}")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RA5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RA6")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "RA7")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RB0")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RB3")
				(number "24")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "RB6")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "RB7")
				(number "28")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "19")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin passive line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "EP")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "RC3")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "RC7")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F2420-xSP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 26.67 0)
		)
		(property "Value" "PIC18F2420-xSP"
			(at 3.81 26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39631E.pdf"
			(at -29.21 33.02 0)
		)
		(property "Description" "MCU 16k Flash, 768B SRAM, 256B EEPROM, ADC, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F2420-xSP_0_1")
		(symbol "PIC18F2420-xSP_1_1"
			(pin input line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "RE3/~{MCLR}")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RA5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RA6")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "RA7")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RB0")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RB3")
				(number "24")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "RB6")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "RB7")
				(number "28")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "19")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "RC3")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "RC7")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F2450-IML"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 27.94 0)
		)
		(property "Value" "PIC18F2450-IML"
			(at 11.43 -27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "16K Flash, 8K SRAM, USB, nanoWatt XLP, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F2450-IML_0_1")
		(symbol "PIC18F2450-IML_1_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA2/AN2/Vref-")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA4/T0CKI/RCV")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA5/AN4/HLVDIN")
				(number "4")
			)
			(pin output line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "7")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/INT1")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/VPO")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/KBI0")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "25")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "~{UOE}/T1OSI/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "VUSB")
				(number "11")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F2450-ISO"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 27.94 0)
		)
		(property "Value" "PIC18F2450-ISO"
			(at 11.43 -27.94 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "16K Flash, 8K SRAM, USB, nanoWatt XLP, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F2450-ISO_0_1")
		(symbol "PIC18F2450-ISO_1_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA2/AN2/Vref-")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA4/T0CKI/RCV")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA5/AN4/HLVDIN")
				(number "7")
			)
			(pin output line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "10")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/INT1")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/VPO")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/KBI0")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "~{UOE}/T1OSI/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "VUSB")
				(number "14")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F2450-ISP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 27.94 0)
		)
		(property "Value" "PIC18F2450-ISP"
			(at 11.43 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "16K Flash, 8K SRAM, USB, nanoWatt XLP, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SPDIP*W7.62mm* DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F2450-ISP_0_1")
		(symbol "PIC18F2450-ISP_1_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA2/AN2/Vref-")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA4/T0CKI/RCV")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA5/AN4/HLVDIN")
				(number "7")
			)
			(pin output line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "10")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/INT1")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/VPO")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/KBI0")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "~{UOE}/T1OSI/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "VUSB")
				(number "14")
			)
			(pin input line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F2455-ISO"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 25.4 0)
		)
		(property "Value" "PIC18F2455-ISO"
			(at 16.51 -25.4 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm_P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F2455-ISO_0_1")
		(symbol "PIC18F2455-ISO_1_1"
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CVref")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "RA4/T0CKI/C1OUT/RCV")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "RA5/AN4/~{SS}/HLVDIN/C2OUT")
				(number "7")
			)
			(pin output line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "10")
			)
			(pin input line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0/FLT0/SDI/SDA")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/INT1/SCK/SCL")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/VPO")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/KBI0")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "T1OSO/T13CKI/RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "~{UOE}/CCP2/T1OSI/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "SDO/RX/DT/RC7")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "VUSB")
				(number "14")
			)
			(pin input line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F2455-ISP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18F2455-ISP"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SPDIP*28_W7.62mm* DIP*28_W7.62mm* PDIP*28_W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F2455-ISP_0_1")
		(symbol "PIC18F2455-ISP_1_1"
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CVref")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RA4/T0CKI/C1OUT/RCV")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "RA5/AN4/~{SS}/HLVDIN/C2OUT")
				(number "7")
			)
			(pin output line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "10")
			)
			(pin input line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0/FLT0/SDI/SDA")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RB1/AN10/INT1/SCK/SCL")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/VPO")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RB4/AN11/KBI0")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "T1OSO/T13CKI/RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "~{UOE}/CCP2/T1OSI/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "SDO/RX/DT/RC7")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "VUSB")
				(number "14")
			)
			(pin input line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F24K50-xML"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18F24K50-xML"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "16K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 2.3V to 5.5V, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F24K50-xML_0_1")
		(symbol "PIC18F24K50-xML_1_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA0")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA1")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA2")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA3")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA4")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA5")
				(number "4")
			)
			(pin output line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "7")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RA7/OSC1/CLKI")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RC0")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RC1")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RC2")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RC6")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RC7")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "RB7/PGD")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "RB6/PGC")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "RB5")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "RB4")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "RB3")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "RB2")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "RB1")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "RB0")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "VUSB3V3/VDDCORE")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "D-")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "D+")
				(number "13")
			)
			(pin input line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "RE3/Vpp/~{MCLR}")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F24K50-xSO"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18F24K50-xSO"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "16K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 2.3V to 5.5V, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F24K50-xSO_0_1")
		(symbol "PIC18F24K50-xSO_1_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA5")
				(number "7")
			)
			(pin output line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "10")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RA7/OSC1/CLKI")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RC0")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RC2")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RC6")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RC7")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "RB7/PGD")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "RB6/PGC")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "VUSB3V3/VDDCORE")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "D-")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "D+")
				(number "16")
			)
			(pin input line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "RE3/Vpp/~{MCLR}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F24K50-xSP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18F24K50-xSP"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "16K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 2.3V to 5.5V, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SPDIP*W7.62mm* DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F24K50-xSP_0_1")
		(symbol "PIC18F24K50-xSP_1_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA5")
				(number "7")
			)
			(pin output line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "10")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RA7/OSC1/CLKI")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RC0")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RC2")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RC6")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RC7")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "RB7/PGD")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "RB6/PGC")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "VUSB3V3/VDDCORE")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "D-")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "D+")
				(number "16")
			)
			(pin input line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "RE3/Vpp/~{MCLR}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F24K50-xSS"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18F24K50-xSS"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "16K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 2.3V to 5.5V, SSOP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F24K50-xSS_0_1")
		(symbol "PIC18F24K50-xSS_1_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA5")
				(number "7")
			)
			(pin output line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "10")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RA7/OSC1/CLKI")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RC0")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RC1")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RC2")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RC6")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RC7")
				(number "18")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "20")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 3.81)
				(name "VSS")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "RB7/PGD")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "RB6/PGC")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "VUSB3V3/VDDCORE")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "D-")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "D+")
				(number "16")
			)
			(pin input line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "RE3/Vpp/~{MCLR}")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F25K80_IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "PIC18F25K80_IML"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "32K Flash, 3.5K RAM, 1K EEPROM PIC18 Microcontroller ADC PWM CAN SPI I2C USART in QFN28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F25K80_IML_0_1")
		(symbol "PIC18F25K80_IML_1_1"
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RA0/AN0")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "RA1/AN1")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "RA2/Vref-/AN2")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RA3/Vref+/AN3")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RA5/AN4")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "~{MCLR}/RE3")
				(number "26")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "OSC2/CLKOUT")
				(number "7")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "OSC1/CLKIN")
				(number "6")
			)
			(pin power_in line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "Vdd")
				(number "17")
			)
			(pin power_in line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "Vcap")
				(number "3")
			)
			(pin power_in line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "Vss")
				(number "16")
			)
			(pin power_in line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "Vss")
				(number "5")
			)
			(pin power_in line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "PAD")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "AN10/INT0/RB0")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "AN8/INT1/RB1")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "CANTX/INT2/RB2")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "CANRX/INT3/RB3")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "AN9/ECCP1/RB4")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "CCP5/RB5")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PGC/TX2/RB6")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PGD/RX2/RB7")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "SOSCO/RC0")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "SOSCI/RC1")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "CCP2/RC2")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "SCL/SCK/RC3")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "SDA/SDI/RC4")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "SDO/RC5")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "CANTX/TX1/CCP3/RC6")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "CANRX/RX1/CCP4/RC7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F25K80_ISS"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "PIC18F25K80_ISS"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "32K Flash, 3.5K RAM, 1K EEPROM, PIC18 Microcontroller ADC PWM CAN SPI I2C USART in SSOP28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F25K80_ISS_0_1")
		(symbol "PIC18F25K80_ISS_1_1"
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "RA2/Vref-/AN2")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RA3/Vref+/AN3")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RA5/AN4")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "~{MCLR}/RE3")
				(number "1")
			)
			(pin input line
				(at -20.32 0 0)
				(length 2.54)
				(name "OSC2/CLKOUT")
				(number "10")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "OSC1/CLKIN")
				(number "9")
			)
			(pin power_in line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "Vdd")
				(number "20")
			)
			(pin power_in line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "Vcap")
				(number "6")
			)
			(pin power_in line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "Vss")
				(number "8")
			)
			(pin power_in line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "Vss")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "AN10/INT0/RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "AN8/INT1/RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "CANTX/INT2/RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "CANRX/INT3/RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "AN9/ECCP1/RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "CCP5/RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PGC/TX2/RB6")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PGD/RX2/RB7")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "SOSCO/RC0")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "SOSCI/RC1")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "CCP2/RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "SCL/SCK/RC3")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "SDA/SDI/RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "SDO/RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "CANTX/TX1/CCP3/RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "CANRX/RX1/CCP4/RC7")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F25K83-xSP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 26.67 0)
		)
		(property "Value" "PIC18F25K83-xSP"
			(at 11.43 26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001943A.pdf"
			(at 5.08 -2.54 0)
		)
		(property "Description" "32K Flash, 2K RAM, 1K EEPROM, 2.3-5.5V, PIC18, low-power microcontroller with CAN, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller Microchip DMA WWDT DIA DCI XLP CLC CWG CCP NCO DSM CRC UART LIN DMX DALI SPI CAN I2C PPS SMT ADC2 CVD DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F25K83-xSP_0_1")
		(symbol "PIC18F25K83-xSP_1_1"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "VPP/~{MCLR}/RE3")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RA5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "OSC2_CLKOUT/RA6")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "OSC1_CLKIN/RA7")
				(number "9")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin passive line
				(at 0 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "19")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "RB0")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "RB1")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "RB3")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "RB4")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "RB5")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "ICSPCLK/RB6")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "ICSPDAT/RB7")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "RC0/SOSCO")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RC1/SOSCI")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RC2")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "RC3")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "RC4")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "RC5")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RC6")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "RC7")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F27J53_ISS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 24.13 0)
		)
		(property "Value" "PIC18F27J53_ISS"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30009964C.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "128K Flash, 3.8K RAM, PIC18 Microcontroller ADC PWM I2C USART USB RTCC, SSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F27J53_ISS_0_1")
		(symbol "PIC18F27J53_ISS_1_1"
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "RA2/AN2")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RA3/AN3")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RA5/AN4")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "OSC2/CLKO/RA6")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "OSC1/CLKI/RA7")
				(number "9")
			)
			(pin input line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "~{MCLR}")
				(number "1")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VDDCORE/VCAP")
				(number "6")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "20")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "19")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "VUSB")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RB0/AN12")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RB1/AN10")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RB2/AN8")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RB3/AN9")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "RB4/SCL1")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RB5/SDA1")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RB6/PGC")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RB7/PGD")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RC0/T1OSO")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RC1/T1OSI")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RC2/AN11")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "RC4/D-")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RC5/D+")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RC6/TX1")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RC7/RX1")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4331-IML"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 30.48 0)
		)
		(property "Value" "PIC18F4331-IML"
			(at 21.59 -30.48 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "8K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F4331-IML_0_1")
		(symbol "PIC18F4331-IML_1_1"
			(pin input line
				(at -35.56 25.4 0)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "18")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "19")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "20")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CAP1/INDX")
				(number "21")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+/CAP2/QEA")
				(number "22")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 3.81)
				(name "RA4/AN4/CAP3/QEB")
				(number "23")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 3.81)
				(name "RA5/AN5/LVDIN")
				(number "24")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "33")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKI")
				(number "32")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 3.81)
				(name "RB0/PWM0")
				(number "9")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 3.81)
				(name "RB1/PWM1")
				(number "10")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 3.81)
				(name "RB2/PWM2")
				(number "11")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 3.81)
				(name "RB3/PWM3")
				(number "12")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 3.81)
				(name "RB4/KBI0/PWM5")
				(number "14")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 3.81)
				(name "RB5/KBI1/PWM4/PGM")
				(number "15")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "16")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "17")
			)
			(pin no_connect line
				(at -10.16 -29.21 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 3.81)
				(name "AVDD")
				(number "8")
			)
			(pin power_in line
				(at -5.08 -33.02 90)
				(length 3.81)
				(name "AVSS")
				(number "30")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 3.81)
				(name "AVDD")
				(number "29")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "34")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 3.81)
				(name "~{FLTA}/T1OSI/CCP2/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 3.81)
				(name "~{FLTB}/CCP1/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 3.81)
				(name "INT0/T5CKI/T0CKI/RC3")
				(number "37")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 3.81)
				(name "INT1/SDI/SDA/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 3.81)
				(name "INT2/SCK/SCL/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 3.81)
				(name "TX/~{SS}/CK/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 3.81)
				(name "RX/SDO/DT/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 3.81)
				(name "T5CKI/T0CKI/RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 3.81)
				(name "SDO/RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 3.81)
				(name "SDA/SDI/RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 3.81)
				(name "SCL/SCK/RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 3.81)
				(name "~{FLTA}/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 3.81)
				(name "PWM4/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 3.81)
				(name "PWM6/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 3.81)
				(name "PWM7/RD7")
				(number "5")
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 3.81)
				(name "AN6/RE0")
				(number "25")
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 3.81)
				(name "AN7/RE1")
				(number "26")
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 3.81)
				(name "AN8/RE2")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4331-IP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 30.48 0)
		)
		(property "Value" "PIC18F4331-IP"
			(at 19.05 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "8K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24* PDIP*W15.24*"
			(at 0 0 0)
		)
		(symbol "PIC18F4331-IP_0_1")
		(symbol "PIC18F4331-IP_1_1"
			(pin input line
				(at -33.02 25.4 0)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "1")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CAP1/INDX")
				(number "4")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+/CAP2/QEA")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 3.81)
				(name "RA4/AN4/CAP3/QEB")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 3.81)
				(name "RA5/AN5/LVDIN")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKI")
				(number "13")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 3.81)
				(name "RB0/PWM0")
				(number "33")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 3.81)
				(name "RB1/PWM1")
				(number "34")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 3.81)
				(name "RB2/PWM2")
				(number "35")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 3.81)
				(name "RB3/PWM3")
				(number "36")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 3.81)
				(name "RB4/KBI0/PWM5")
				(number "37")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 3.81)
				(name "RB5/KBI1/PWM4/PGM")
				(number "38")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "39")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "40")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 3.81)
				(name "AVDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 3.81)
				(name "AVSS")
				(number "12")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 3.81)
				(name "~{FLTA}/T1OSI/CCP2/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 3.81)
				(name "~{FLTB}/CCP1/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 3.81)
				(name "INT0/T5CKI/T0CKI/RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 3.81)
				(name "INT1/SDI/SDA/RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 3.81)
				(name "INT2/SCK/SCL/RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 3.81)
				(name "TX/~{SS}/CK/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 3.81)
				(name "RX/SDO/DT/RC7")
				(number "26")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 3.81)
				(name "T5CKI/T0CKI/RD0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 3.81)
				(name "SDO/RD1")
				(number "20")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 3.81)
				(name "SDA/SDI/RD2")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 3.81)
				(name "SCL/SCK/RD3")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 3.81)
				(name "~{FLTA}/RD4")
				(number "27")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 3.81)
				(name "PWM4/RD5")
				(number "28")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 3.81)
				(name "PWM6/RD6")
				(number "29")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 3.81)
				(name "PWM7/RD7")
				(number "30")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 3.81)
				(name "AN6/RE0")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 3.81)
				(name "AN7/RE1")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 3.81)
				(name "AN8/RE2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4331-IPT"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 30.48 0)
		)
		(property "Value" "PIC18F4331-IPT"
			(at 16.51 -30.48 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "8K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F4331-IPT_0_1")
		(symbol "PIC18F4331-IPT_1_1"
			(pin input line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CAP1/INDX")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+/CAP2/QEA")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "RA4/AN4/CAP3/QEB")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "RA5/AN5/LVDIN")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RA7/OSC1/CLKI")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RB0/PWM0")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RB1/PWM1")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RB2/PWM2")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RB3/PWM3")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RB4/KBI0/PWM5")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RB5/KBI1/PWM4/PGM")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "16")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "17")
			)
			(pin no_connect line
				(at -15.24 -29.21 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -12.7 -29.21 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -10.16 -29.21 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at -7.62 -29.21 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 3.81)
				(name "AVDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 3.81)
				(name "AVSS")
				(number "29")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "~{FLTA}/T1OSI/CCP2/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "~{FLTB}/CCP1/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "INT0/T5CKI/T0CKI/RC3")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "INT1/SDI/SDA/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "INT2/SCK/SCL/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "TX/~{SS}/CK/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "RX/SDO/DT/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "T5CKI/T0CKI/RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "SDO/RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "SDA/SDI/RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "SCL/SCK/RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "~{FLTA}/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "PWM4/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "PWM6/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "PWM7/RD7")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "AN6/RE0")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "AN7/RE1")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "AN8/RE2")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F442-IP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18F442-IP"
			(at 12.7 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39564c.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256 EEPROM, ADC, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F442-IP_0_1")
		(symbol "PIC18F442-IP_1_1"
			(pin input line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "~{MCLR}/VPP")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA2/AN2/Vref-")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA4/TOCKI")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA5/AN4/~{SS}/LVDIN")
				(number "7")
			)
			(pin output line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "14")
			)
			(pin input line
				(at -25.4 0 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB0/INT0")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB1/INT1")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB2/INT2")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB3/CCP2")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RB4")
				(number "37")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RB5/PGM")
				(number "38")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RB6/PGC")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "RB7/PGD")
				(number "40")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "T10S0/T1CKI/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "CCP2/T1OSI/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SCK/SCL/RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "SDI/SDA/RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "SDO/RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "PSP0/RD0")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "PSP1/RD1")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "PSP2/RD2")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "PSP3/RD3")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "PSP4/RD4")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "PSP5/RD5")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "PSP6/RD6")
				(number "29")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "PSP7/RD7")
				(number "30")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "~{RD}/AN5/RE0")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "~{WR}/AN6/RE1")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "~{CS}/AN7/RE2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F442-IPT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -21.59 30.48 0)
		)
		(property "Value" "PIC18F442-IPT"
			(at 5.08 -30.48 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39564c.pdf"
			(at 0 0 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256 EEPROM, ADC, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F442-IPT_0_1")
		(symbol "PIC18F442-IPT_1_1"
			(pin input line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "~{MCLR}/Vpp")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "RA2/AN2/Vref-")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "RA4/T0CKI")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "RA5/AN4/~{SS}/LVDin")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "31")
			)
			(pin input line
				(at -25.4 0 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "RB0/INT0")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "RB1/INT1")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "RB2/INT2")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "RB3/CCP2")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "RB4")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "RB5/PGM")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "RB6/PGC")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "RB7/PGD")
				(number "17")
			)
			(pin no_connect line
				(at -15.24 -29.21 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -12.7 -29.21 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -10.16 -29.21 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at -7.62 -29.21 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "T1OSI/CCP2/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "SCK/SCL/RC3")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "SDI/SDA/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "SDO/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "CK/TX/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "DT/RX/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "PSP0/RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 3.81)
				(name "PSP1/RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "PSP2/RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "PSP3/RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "PSP4/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "PSP5/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 3.81)
				(name "PSP6/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 3.81)
				(name "PSP7/RD7")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "~{RD}/AN5/RE0")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "~{WR}/AN6/RE1")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "~{CS}/AN7/RE2")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4420-xP"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 31.75 0)
		)
		(property "Value" "PIC18F4420-xP"
			(at 2.54 31.75 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39631E.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, ADC, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F4420-xP_0_1")
		(symbol "PIC18F4420-xP_1_1"
			(pin input line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "RE3/~{MCLR}")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "RE2")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "RE1")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "RE0")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "RA0")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "RA1")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RA2")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RA3")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RA4")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RA5")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "RA6")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "RA7")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "RB0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RB1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RB2")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "RB3")
				(number "36")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "RB4")
				(number "37")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "RB5")
				(number "38")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "RB6")
				(number "39")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "RB7")
				(number "40")
			)
			(pin passive line
				(at 0 33.02 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RC7")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "RD0")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "RD1")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "RD2")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RD3")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "RD4")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "RD5")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "RD6")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "RD7")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4450-IML"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18F4450-IML"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "16K Flash, 8K SRAM, USB, nanoWatt XLP, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F4450-IML_0_1")
		(symbol "PIC18F4450-IML_1_1"
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 3.81)
				(name "RA2/AN2/Vref-")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "22")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI/RCV")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 3.81)
				(name "RA5/AN4/HLVDIN")
				(number "24")
			)
			(pin output line
				(at -27.94 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "33")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "32")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RB1/AN10/INT1")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB3/AN9/VPO")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB4/AN11/KBI0")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "17")
			)
			(pin no_connect line
				(at -12.7 -31.75 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at -7.62 35.56 270)
				(length 3.81)
				(name "AVDD")
				(number "7")
			)
			(pin power_in line
				(at -7.62 -35.56 90)
				(length 3.81)
				(name "AVSS")
				(number "30")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 3.81)
				(name "AVDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 3.81)
				(name "~{UOE}/T1OSI/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "VUSB")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "RD7")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 3.81)
				(name "AN5/RE0")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 3.81)
				(name "AN6/RE1")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 3.81)
				(name "AN7/RE2")
				(number "27")
			)
			(pin input line
				(at 27.94 -27.94 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4450-IP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18F4450-IP"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "16K Flash, 8K SRAM, USB, nanoWatt XLP, PDIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F4450-IP_0_1")
		(symbol "PIC18F4450-IP_1_1"
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 3.81)
				(name "RA2/AN2/Vref-")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI/RCV")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 3.81)
				(name "RA5/AN4/HLVDIN")
				(number "7")
			)
			(pin output line
				(at -27.94 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "14")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RB1/AN10/INT1")
				(number "34")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB3/AN9/VPO")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB4/AN11/KBI0")
				(number "37")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "38")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "39")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "40")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 3.81)
				(name "~{UOE}/T1OSI/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "VUSB")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "RD0")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "RD1")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "RD2")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "RD3")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "RD4")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "RD5")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "RD6")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "RD7")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 3.81)
				(name "AN5/RE0")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 3.81)
				(name "AN6/RE1")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 3.81)
				(name "AN7/RE2")
				(number "10")
			)
			(pin input line
				(at 27.94 -27.94 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4450-IPT"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18F4450-IPT"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "16K Flash, 8K SRAM, USB, nanoWatt XLP, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F4450-IPT_0_1")
		(symbol "PIC18F4450-IPT_1_1"
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 3.81)
				(name "RA2/AN2/Vref-")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "22")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI/RCV")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 3.81)
				(name "RA5/AN4/HLVDIN")
				(number "24")
			)
			(pin output line
				(at -27.94 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "31")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RB1/AN10/INT1")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB3/AN9/VPO")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB4/AN11/KBI0")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "17")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 3.81)
				(name "(~{ICRST}/ICVpp)")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 3.81)
				(name "(ICCK/ICPGC)")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 3.81)
				(name "(ICDT/ICPGD)")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 3.81)
				(name "(ICPORTS)")
				(number "34")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 3.81)
				(name "~{UOE}/T1OSI/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "VUSB")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "RD7")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 3.81)
				(name "AN5/RE0")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 3.81)
				(name "AN6/RE1")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 3.81)
				(name "AN7/RE2")
				(number "27")
			)
			(pin input line
				(at 27.94 -27.94 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4455-IML"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18F4455-IML"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F4455-IML_0_1")
		(symbol "PIC18F4455-IML_1_1"
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CVref")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI/C1OUT/RCV")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RA5/AN4/~{SS}/HLVDIN/C2OUT")
				(number "24")
			)
			(pin output line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "33")
			)
			(pin input line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0/FLT0/SDI/SDA")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "RB1/AN10/INT1/SCK/SCL")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/VPO")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RB4/AN11/KBI0/CSSPP")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "16")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "17")
			)
			(pin power_in line
				(at -7.62 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin no_connect line
				(at -7.62 -31.75 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "29")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 3.81)
				(name "T1OSO/T13CKI/RC0")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "~{UOE}/CCP2/T1OSI/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "P1A/CCP1/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "SDO/RX/DT/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "VUSB")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "SPP0/RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "SPP1/RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "SPP2/RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "SPP3/RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "SPP4/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "P1B/SPP5/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "P1C/SPP6/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "P1D/SPP7/RD7")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "CK1SPP/AN5/RE0")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "CK2SPP/AN6/RE1")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "OESPP/AN7/RE2")
				(number "27")
			)
			(pin input line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4455-IP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18F4455-IP"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F4455-IP_0_1")
		(symbol "PIC18F4455-IP_1_1"
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CVref")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI/C1OUT/RCV")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 3.81)
				(name "RA5/AN4/~{SS}/HLVDIN/C2OUT")
				(number "7")
			)
			(pin output line
				(at -27.94 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "14")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0/FLT0/SDI/SDA")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RB1/AN10/INT1/SCK/SCL")
				(number "34")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/VPO")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB4/AN11/KBI0/CSSPP")
				(number "37")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "38")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "39")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "40")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 3.81)
				(name "T1OSO/T13CKI/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 3.81)
				(name "~{UOE}/CCP2/T1OSI/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 3.81)
				(name "P1A/CCP1/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 3.81)
				(name "SDO/RX/DT/RC7")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "VUSB")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "SPP0/RD0")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "SPP1/RD1")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "SPP2/RD2")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "SPP3/RD3")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "SPP4/RD4")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "P1B/SPP5/RD5")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "P1C/SPP6/RD6")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "P1D/SPP7/RD7")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 3.81)
				(name "CK1SPP/AN5/RE0")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 3.81)
				(name "CK2SPP/AN6/RE1")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 3.81)
				(name "OESPP/AN7/RE2")
				(number "10")
			)
			(pin input line
				(at 27.94 -27.94 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4455-IPT"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18F4455-IPT"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F4455-IPT_0_1")
		(symbol "PIC18F4455-IPT_1_1"
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CVref")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI/C1OUT/RCV")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RA5/AN4/~{SS}/HLVDIN/C2OUT")
				(number "24")
			)
			(pin output line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "31")
			)
			(pin input line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0/FLT0/SDI/SDA")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "RB1/AN10/INT1/SCK/SCL")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/VPO")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RB4/AN11/KBI0/CSSPP")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "16")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "(ICCK/ICPGC)")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "(ICDT/ICPGD)")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "(ICPORTS)")
				(number "34")
			)
			(pin input line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "(~{ICRST}/ICVpp)")
				(number "33")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 3.81)
				(name "T1OSO/T13CKI/RC0")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "~{UOE}/CCP2/T1OSI/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "P1A/CCP1/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "SDO/RX/DT/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "VUSB")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "SPP0/RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "SPP1/RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "SPP2/RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "SPP3/RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "SPP4/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "P1B/SPP5/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "P1C/SPP6/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "P1D/SPP7/RD7")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "CK1SPP/AN5/RE0")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "CK2SPP/AN6/RE1")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "OESPP/AN7/RE2")
				(number "27")
			)
			(pin input line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4458-IML"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18F4458-IML"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39887c.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, 12-Bit A/D, nanoWatt XLP, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F4458-IML_0_1")
		(symbol "PIC18F4458-IML_1_1"
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CVref")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI/C1OUT/RCV")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RA5/AN4/~{SS}/HLVDIN/C2OUT")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "33")
			)
			(pin input line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0/FLT0/SDI/SDA")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "RB1/AN10/INT1/SCK/SCL")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/VPO")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RB4/AN11/KBI0/CSSPP")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "16")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "17")
			)
			(pin no_connect line
				(at -26.67 -27.94 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at -7.62 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at -5.08 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "29")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 3.81)
				(name "PAD")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 3.81)
				(name "T1OSO/T13CKI/RC0")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "~{UOE}/CCP2/T1OSI/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "P1A/CCP1/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "SDO/RX/DT/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "VUSB")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "SPP0/RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "SPP1/RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "SPP2/RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "SPP3/RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "SPP4/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "P1B/SPP5/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "P1C/SPP6/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "P1D/SPP7/RD7")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "CK1SPP/AN5/RE0")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "CK2SPP/AN6/RE1")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "OESPP/AN7/RE2")
				(number "27")
			)
			(pin input line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4458-IP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18F4458-IP"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39887c.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, 12-Bit A/D, nanoWatt XLP, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F4458-IP_0_1")
		(symbol "PIC18F4458-IP_1_1"
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CVref")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI/C1OUT/RCV")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 3.81)
				(name "RA5/AN4/~{SS}/HLVDIN/C2OUT")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "14")
			)
			(pin input line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0/FLT0/SDI/SDA")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 3.81)
				(name "RB1/AN10/INT1/SCK/SCL")
				(number "34")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/VPO")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB4/AN11/KBI0/CSSPP")
				(number "37")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "38")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "39")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "40")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 3.81)
				(name "T1OSO/T13CKI/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 3.81)
				(name "~{UOE}/CCP2/T1OSI/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 3.81)
				(name "P1A/CCP1/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 3.81)
				(name "SDO/RX/DT/RC7")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "VUSB")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "SPP0/RD0")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "SPP1/RD1")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "SPP2/RD2")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "SPP3/RD3")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "SPP4/RD4")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "P1B/SPP5/RD5")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "P1C/SPP6/RD6")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "P1D/SPP7/RD7")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 3.81)
				(name "CK1SPP/AN5/RE0")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 3.81)
				(name "CK2SPP/AN6/RE1")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 3.81)
				(name "OESPP/AN7/RE2")
				(number "10")
			)
			(pin input line
				(at 27.94 -27.94 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4458-IPT"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18F4458-IPT"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39887c.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, 12-Bit A/D, nanoWatt XLP, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F4458-IPT_0_1")
		(symbol "PIC18F4458-IPT_1_1"
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CVref")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RA4/T0CKI/C1OUT/RCV")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RA5/AN4/~{SS}/HLVDIN/C2OUT")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "31")
			)
			(pin input line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RB0/AN12/INT0/FLT0/SDI/SDA")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "RB1/AN10/INT1/SCK/SCL")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RB2/AN8/INT2/VMO")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RB3/AN9/CCP2/VPO")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RB4/AN11/KBI0/CSSPP")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "16")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "(ICCK/ICPGC)")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "(ICDT/ICPGD)")
				(number "13")
			)
			(pin input line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "(ICPORTS)")
				(number "34")
			)
			(pin input line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "(~{ICRST}/ICVpp)")
				(number "33")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 3.81)
				(name "T1OSO/T13CKI/RC0")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "~{UOE}/CCP2/T1OSI/RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "P1A/CCP1/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "VM/D-/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "VP/D+/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "SDO/RX/DT/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "VUSB")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "SPP0/RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "SPP1/RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "SPP2/RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "SPP3/RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "SPP4/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "P1B/SPP5/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "P1C/SPP6/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "P1D/SPP7/RD7")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "CK1SPP/AN5/RE0")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "CK2SPP/AN6/RE1")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "OESPP/AN7/RE2")
				(number "27")
			)
			(pin input line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "Vpp/~{MCLR}/RE3")
				(number "18")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F448-IP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 30.48 0)
		)
		(property "Value" "PIC18F448-IP"
			(at 15.24 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41159e.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256 EEPROM, CAN, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller CAN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F448-IP_0_1")
		(symbol "PIC18F448-IP_1_1"
			(pin input line
				(at -27.94 25.4 0)
				(length 3.81)
				(name "~{MCLR}/VPP")
				(number "1")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 3.81)
				(name "RA0/AN0/CVref")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 3.81)
				(name "RA2/AN2/Vref-")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "RA4/TOCKI")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "RA5/AN4/~{SS}/LVDIN")
				(number "7")
			)
			(pin output line
				(at -27.94 5.08 0)
				(length 3.81)
				(name "RA6/OSC2/CLKO")
				(number "14")
			)
			(pin input line
				(at -27.94 0 0)
				(length 3.81)
				(name "OSC1/CLKIN")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB0/INT0")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB1/INT1")
				(number "34")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "RB2/INT2/CANTX")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "RB3/CANRX")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 3.81)
				(name "RB4")
				(number "37")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 3.81)
				(name "RB5/PGM")
				(number "38")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 3.81)
				(name "RB6/PGC")
				(number "39")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 3.81)
				(name "RB7/PGD")
				(number "40")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 3.81)
				(name "T10S0/T1CKI/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 3.81)
				(name "T1OSI/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "SCK/SCL/RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 3.81)
				(name "SDI/SDA/RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 3.81)
				(name "SDO/RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "C1IN+/PSP0/RD0")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "C1IN-/PSP1/RD1")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "C2IN+/PSP2/RD2")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "C2IN-/PSP3/RD3")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "P1A/ECCP1/PSP4/RD4")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "P1B/PSP5/RD5")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "P1C/PSP6/RD6")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "P1D/PSP7/RD7")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 3.81)
				(name "~{RD}/AN5/RE0")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 3.81)
				(name "C1OUT/~{WR}/AN6/RE1")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 3.81)
				(name "C2OUT/~{CS}/AN7/RE2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F44J10-IP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 30.48 0)
		)
		(property "Value" "PIC18F44J10-IP"
			(at 16.51 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39682E.pdf"
			(at -29.21 30.48 0)
		)
		(property "Description" "16K Flash, 1K SRAM, ADC, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F44J10-IP_0_0")
		(symbol "PIC18F44J10-IP_1_1"
			(pin input line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "1")
			)
			(pin tri_state line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "RA0/AN0")
				(number "2")
			)
			(pin tri_state line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin tri_state line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RA2/AN2/Vref-/CVref")
				(number "4")
			)
			(pin tri_state line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin tri_state line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "RA5/AN4/~{SS1}/C2OUT")
				(number "7")
			)
			(pin tri_state line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "RB0/INT0/FLT0/AN12")
				(number "33")
			)
			(pin tri_state line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RB1/INT1/AN10")
				(number "34")
			)
			(pin tri_state line
				(at -30.48 0 0)
				(length 3.81)
				(name "RB2/INT2/AN8")
				(number "35")
			)
			(pin tri_state line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RB3/CCP2/AN9")
				(number "36")
			)
			(pin tri_state line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RB4/KBI0/AN11")
				(number "37")
			)
			(pin tri_state line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RB5/KBI1/T0CKI/C1OUT")
				(number "38")
			)
			(pin tri_state line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "39")
			)
			(pin tri_state line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "40")
			)
			(pin input line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "13")
			)
			(pin output line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "OSC2/CLK0")
				(number "14")
			)
			(pin passive line
				(at -2.54 33.02 270)
				(length 3.81)
				(name "VDDCORE/VCAP")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin tri_state line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "T1OSO/T1CKI/RC0")
				(number "15")
			)
			(pin tri_state line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "T1OSI/CCP2/RC1")
				(number "16")
			)
			(pin tri_state line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "P1A/CCP1/RC2")
				(number "17")
			)
			(pin tri_state line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "SCK1/SCL1/RC3")
				(number "18")
			)
			(pin tri_state line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "SDI1/SDA1/RC4")
				(number "23")
			)
			(pin tri_state line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "SDO1/RC5")
				(number "24")
			)
			(pin tri_state line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "TX/CK/RC6")
				(number "25")
			)
			(pin tri_state line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "RX/DT/RC7")
				(number "26")
			)
			(pin tri_state line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "PSP0/SCK2/SCL2/RD0")
				(number "19")
			)
			(pin tri_state line
				(at 30.48 0 180)
				(length 3.81)
				(name "PSP1/SDI2/SDA2/RD1")
				(number "20")
			)
			(pin tri_state line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "PSP2/SDO2/RD2")
				(number "21")
			)
			(pin tri_state line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "PSP3/~{SS2}/RD3")
				(number "22")
			)
			(pin tri_state line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "PSP4/RD4")
				(number "27")
			)
			(pin tri_state line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "PSP5/P1B/RD5")
				(number "28")
			)
			(pin tri_state line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "PSP6/P1C/RD6")
				(number "29")
			)
			(pin tri_state line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "PSP7/P1D/RD7")
				(number "30")
			)
			(pin tri_state line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "~{RD}/AN5/RE0")
				(number "8")
			)
			(pin tri_state line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "~{WR}/AN6/RE1")
				(number "9")
			)
			(pin tri_state line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "~{CS}/AN7/RE2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F4580-IP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 30.48 0)
		)
		(property "Value" "PIC18F4580-IP"
			(at 15.24 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39637d.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "32K Flash, 1536B SRAM, 256 EEPROM, ECAN, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller CAN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F4580-IP_0_1")
		(symbol "PIC18F4580-IP_1_1"
			(pin input line
				(at -27.94 25.4 0)
				(length 3.81)
				(name "~{MCLR}/VPP/RE3")
				(number "1")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 3.81)
				(name "RA0/AN0/CVref")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 3.81)
				(name "RA1/AN1")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 3.81)
				(name "RA2/AN2/Vref-")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 3.81)
				(name "RA3/AN3/Vref+")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "RA4/TOCKI")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "RA5/ANA4/~{SS}/HLVDIN")
				(number "7")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "OSC1/CLKI/RA7")
				(number "13")
			)
			(pin output line
				(at -27.94 0 0)
				(length 3.81)
				(name "OSC2/CLKO/RA6")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "RB0/INT0/FLT0/AN10")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "RB1/INT1/AN8")
				(number "34")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "RB2/INT2/CANTX")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "RB3/CANRX")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 3.81)
				(name "RB4/KBI0/AN9")
				(number "37")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 3.81)
				(name "RB5/KBI1/PGM")
				(number "38")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 3.81)
				(name "RB6/KBI2/PGC")
				(number "39")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 3.81)
				(name "RB7/KBI3/PGD")
				(number "40")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 3.81)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 3.81)
				(name "T13CKI/T1OSO/RC0")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 3.81)
				(name "T1OSI/RC1")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 3.81)
				(name "CCP1/RC2")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "SCL/SCK/RC3")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 3.81)
				(name "SDA/SDI/RC4")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 3.81)
				(name "SDO/RC5")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "CK/TX/RC6")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "DT/RX/RC7")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "C1IN+/PSP0/RD0")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "C1IN-/PSP1/RD1")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 3.81)
				(name "C2IN+/PSP2/RD2")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "C2IN-/PSP3/RD3")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "P1A/ECCP1/PSP4/RD4")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "P1B/PSP5/RD5")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "P1C/PSP6/RD6")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "P1D/PSP7/RD7")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 3.81)
				(name "AN5/~{RD}/RE0")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 3.81)
				(name "C1OUT/AN6/~{WR}/RE1")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 3.81)
				(name "C2OUT/AN7/~{CS}/RE2")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F45K50_QFP"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -36.83 33.02 0)
		)
		(property "Value" "PIC18F45K50_QFP"
			(at 30.48 -35.56 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30000684B.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "32K Flash, 2K RAM, 256B EEPROM, Microchip PIC18F series enhanced flash microcontroller with USB in TQFP-44 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller Flash EEPROM SPI I2C USB UART USART ADC TQFP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F45K50_QFP_0_1")
		(symbol "PIC18F45K50_QFP_1_1"
			(pin bidirectional line
				(at -43.18 27.94 0)
				(length 3.81)
				(name "RE0/AN5")
				(number "25")
			)
			(pin bidirectional line
				(at -43.18 25.4 0)
				(length 3.81)
				(name "RE1/AN6")
				(number "26")
			)
			(pin bidirectional line
				(at -43.18 22.86 0)
				(length 3.81)
				(name "RE2/AN7")
				(number "27")
			)
			(pin bidirectional line
				(at -43.18 17.78 0)
				(length 3.81)
				(name "RD0/AN20")
				(number "38")
			)
			(pin bidirectional line
				(at -43.18 15.24 0)
				(length 3.81)
				(name "RD1/AN21")
				(number "39")
			)
			(pin bidirectional line
				(at -43.18 12.7 0)
				(length 3.81)
				(name "RD2/AN22")
				(number "40")
			)
			(pin bidirectional line
				(at -43.18 10.16 0)
				(length 3.81)
				(name "RD3/AN23")
				(number "41")
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 3.81)
				(name "RD4/AN24")
				(number "2")
			)
			(pin bidirectional line
				(at -43.18 5.08 0)
				(length 3.81)
				(name "RD5/P1B/AN25")
				(number "3")
			)
			(pin bidirectional line
				(at -43.18 2.54 0)
				(length 3.81)
				(name "RD6/P1C/AN26")
				(number "4")
			)
			(pin bidirectional line
				(at -43.18 0 0)
				(length 3.81)
				(name "RD7/P1D/AN27")
				(number "5")
			)
			(pin bidirectional line
				(at -43.18 -5.08 0)
				(length 3.81)
				(name "RC0/SOSCO/T1CKI/T3CKI/T3G/IOCC0")
				(number "32")
			)
			(pin bidirectional line
				(at -43.18 -7.62 0)
				(length 3.81)
				(name "RC1/SOSCI/CCP2/IOCC1")
				(number "35")
			)
			(pin bidirectional line
				(at -43.18 -10.16 0)
				(length 3.81)
				(name "RC2/AN14/CTPLS/CCP1/P1A/IOCC2")
				(number "36")
			)
			(pin bidirectional line
				(at -43.18 -12.7 0)
				(length 3.81)
				(name "RC6/AN18/TX/CK/IOCC6")
				(number "44")
			)
			(pin bidirectional line
				(at -43.18 -15.24 0)
				(length 3.81)
				(name "RC7/AN19/RX/DT/IOCC7")
				(number "1")
			)
			(pin power_in line
				(at -43.18 -20.32 0)
				(length 3.81)
				(name "VUSB3V3/VDDCORE")
				(number "37")
			)
			(pin bidirectional line
				(at -43.18 -22.86 0)
				(length 3.81)
				(name "D-/IOCC4")
				(number "42")
			)
			(pin bidirectional line
				(at -43.18 -25.4 0)
				(length 3.81)
				(name "D+/IOCC5")
				(number "43")
			)
			(pin no_connect line
				(at -17.78 -34.29 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin input line
				(at 43.18 27.94 180)
				(length 3.81)
				(name "~{MCLR}/VPP/RE3")
				(number "18")
			)
			(pin bidirectional line
				(at 43.18 22.86 180)
				(length 3.81)
				(name "OSC2/CLKO/RA6")
				(number "31")
			)
			(pin bidirectional line
				(at 43.18 20.32 180)
				(length 3.81)
				(name "OSC1/CLKI/RA7")
				(number "30")
			)
			(pin bidirectional line
				(at 43.18 15.24 180)
				(length 3.81)
				(name "AN0/C12IN0-/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 43.18 12.7 180)
				(length 3.81)
				(name "AN1/C12IN1-/CTCMP/RA1")
				(number "20")
			)
			(pin bidirectional line
				(at 43.18 10.16 180)
				(length 3.81)
				(name "VREF-/DACOUT/AN2/C2IN+/RA2")
				(number "21")
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 3.81)
				(name "VREF+/AN3/C1IN+/RA3")
				(number "22")
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 3.81)
				(name "C1OUT/SRQ/T0CKI/RA4")
				(number "23")
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 3.81)
				(name "AN4/HLVDIN/SRNQ/C2OUT/~{SS}/RA5")
				(number "24")
			)
			(pin bidirectional line
				(at 43.18 -2.54 180)
				(length 3.81)
				(name "AN12/SRI/~{FLT0}/SDI/SDA/INT0/RB0")
				(number "8")
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 3.81)
				(name "AN10/C12IN3-/SCK/SCL/INT1/RB1")
				(number "9")
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 3.81)
				(name "AN8/CTED1/INT2/RB2")
				(number "10")
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 3.81)
				(name "AN9/C12IN2-/CTED2/CCP2/SDO/RB3")
				(number "11")
			)
			(pin bidirectional line
				(at 43.18 -12.7 180)
				(length 3.81)
				(name "AN11/IOCB4/RB4")
				(number "14")
			)
			(pin bidirectional line
				(at 43.18 -15.24 180)
				(length 3.81)
				(name "AN13/T1G/T3CKI/IOCB5/RB5")
				(number "15")
			)
			(pin bidirectional line
				(at 43.18 -17.78 180)
				(length 3.81)
				(name "PGC/IOCB6/RB6")
				(number "16")
			)
			(pin bidirectional line
				(at 43.18 -20.32 180)
				(length 3.81)
				(name "PGD/IOCB7/RB7")
				(number "17")
			)
			(pin bidirectional line
				(at 43.18 -25.4 180)
				(length 3.81)
				(name "ICPGC/ICCK/NC")
				(number "12")
			)
			(pin bidirectional line
				(at 43.18 -27.94 180)
				(length 3.81)
				(name "ICPGD/ICDT/NC")
				(number "13")
			)
			(pin bidirectional line
				(at 43.18 -30.48 180)
				(length 3.81)
				(name "ICVPP/ICRST/NC")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F45K80-IML"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "PIC18F45K80-IML"
			(at -22.86 -26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC18F66K80%20FAMILY%20Enhanced%20Flash%20MCU%20with%20ECAN%20XLP%20Technology%2030009977G.pdf"
			(at -16.51 -2.54 0)
		)
		(property "Description" "32K Flash, 3.5K RAM, 1K EEPROM, Microchip PIC18F series enhanced flash microcontroller with ECAN and nanoWatt XLP Technology in QFN-44 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller Flash EEPROM SPI I2C CAN UART USART ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F45K80-IML_0_1")
		(symbol "PIC18F45K80-IML_1_1"
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "RA0/CVref/AN0")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "RA1/AN1")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "RA2/Vref-/AN2")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "RA3/Vref+/AN3")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "RA5/AN4")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "RB0/AN10/INT0")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "RB1/AN8/INT1")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 2.54)
				(name "RB2/CANTX/INT2")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "RB3/CANRX/INT3")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 2.54)
				(name "RB4/AN9")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "RB5/CCP5")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "RB6/PGC")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "RB7/PGD")
				(number "17")
			)
			(pin input line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "OSC1/CLKIN/RA7")
				(number "30")
			)
			(pin input line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "OSC2/CLKOUT/RA6")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "~{MLCR}/RE3")
				(number "18")
			)
			(pin power_in line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "Vddcore/Vcap")
				(number "23")
			)
			(pin no_connect line
				(at -10.16 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -7.62 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -5.08 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "Vdd")
				(number "28")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "Vss")
				(number "6")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "Vdd")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 2.54)
				(name "Vss")
				(number "29")
			)
			(pin power_in line
				(at 7.62 -30.48 90)
				(length 2.54)
				(name "PAD")
				(number "45")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "RC0")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 2.54)
				(name "CCP2/RC2")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "SCL/SCK/RC3")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "SDA/SDI/RC4")
				(number "42")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "SDO/RC5")
				(number "43")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "CANTX/TX1/CCP3/RC6")
				(number "44")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 2.54)
				(name "CANRX/RX1/CCP4/RC7")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "C1INA/PSP0/RD0")
				(number "38")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 2.54)
				(name "C1INB/PSP1/RD1")
				(number "39")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "C2INA/PSP2/RD2")
				(number "40")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "C2INB/PSP3/RD3")
				(number "41")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 2.54)
				(name "ECCP1/PSP4/RD4")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "PSP5/RD5")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "TX2/PSP6/RD6")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 2.54)
				(name "RX2/PSP7/RD7")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "RE2/AN7")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 2.54)
				(name "RE1/AN6")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "RE0/AN5")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F45K80-IPT"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 33.02 0)
		)
		(property "Value" "PIC18F45K80-IPT"
			(at 20.32 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "32K Flash, 3.5K RAM, 1K EEPROM, Microchip PIC18F series enhanced flash microcontroller with ECAN and nanoWatt XLP Technology in TQFP-44 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller Flash EEPROM SPI I2C CAN UART USART ADC TQFP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F45K80-IPT_0_1")
		(symbol "PIC18F45K80-IPT_1_1"
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 3.81)
				(name "RE0/AN5/~{RD}")
				(number "25")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 3.81)
				(name "RE1/AN6/C1OUT/~{WR}")
				(number "26")
			)
			(pin power_in line
				(at -35.56 22.86 0)
				(length 3.81)
				(name "RE2/AN7/C2OUT/~{CS}")
				(number "27")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 3.81)
				(name "RD0/C1INA/PSP0")
				(number "38")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 3.81)
				(name "RD1/C1INB/PSP1")
				(number "39")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 3.81)
				(name "RD2/C2INA/PSP2")
				(number "40")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 3.81)
				(name "RD3/C2INB/CTMUI/PSP3")
				(number "41")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 3.81)
				(name "RD4/ECCP1/P1A/PSP4")
				(number "2")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 3.81)
				(name "RD5/P1B/PSP5")
				(number "3")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 3.81)
				(name "RD6/TX2/CK2/P1C/PSP6")
				(number "4")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 3.81)
				(name "RD7/RX2/DT2/P1D/PSP7")
				(number "5")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 3.81)
				(name "RC0/SOSCO/SCLKI")
				(number "32")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 3.81)
				(name "RC1/SOSCI")
				(number "35")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 3.81)
				(name "RC2/T1G/CCP2")
				(number "36")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 3.81)
				(name "RC3/REFO/SCL/SCK")
				(number "37")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 3.81)
				(name "RC4/SDA/SDI")
				(number "42")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 3.81)
				(name "RC5/SDO")
				(number "43")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 3.81)
				(name "RC6/CANTX/TX1/CK1/CCP3")
				(number "44")
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 3.81)
				(name "RC7/CANRX/RX1/DT1/CCP4")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -35.56 90)
				(length 3.81)
				(name "N/C")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 -35.56 90)
				(length 3.81)
				(name "N/C")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -35.56 90)
				(length 3.81)
				(name "N/C")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 -35.56 90)
				(length 3.81)
				(name "N/C")
				(number "34")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 3.81)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin input line
				(at 35.56 27.94 180)
				(length 3.81)
				(name "~{MCLR}/RE3")
				(number "18")
			)
			(pin input line
				(at 35.56 22.86 180)
				(length 3.81)
				(name "OSC1/CLKIN/RA7")
				(number "30")
			)
			(pin output line
				(at 35.56 20.32 180)
				(length 3.81)
				(name "OSC2/CLKOUT/RA6")
				(number "31")
			)
			(pin passive line
				(at 35.56 15.24 180)
				(length 3.81)
				(name "VDDCORE/VCAP")
				(number "23")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 3.81)
				(name "CVref/AN0/ULPWU/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 3.81)
				(name "AN1/C1INC/RA1")
				(number "20")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 3.81)
				(name "VREF-/AN2/C2INC/RA2")
				(number "21")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "22")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 3.81)
				(name "AN4/HLVDIN/T1CKI/~{SS}/RA5")
				(number "24")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 3.81)
				(name "AN10/FLT0/INT0/RB0")
				(number "8")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 3.81)
				(name "AN8/CTDIN/INT1/RB1")
				(number "9")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 3.81)
				(name "CANTX/CTED1/INT2/RB2")
				(number "10")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 3.81)
				(name "CANRX/CTED2/INT3/RB3")
				(number "11")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 3.81)
				(name "AN9/CTPLS/KBI0/RB4")
				(number "14")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 3.81)
				(name "T0CKI/T3CKI/CCP5/KBI1/RB5")
				(number "15")
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 3.81)
				(name "PGC/KBI2/RB6")
				(number "16")
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 3.81)
				(name "PGD/T3G/KBI3/RB7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F46K22-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -29.21 29.21 0)
		)
		(property "Value" "PIC18F46K22-xPT"
			(at 21.59 -29.21 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at -3.81 -5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001412G.pdf"
			(at -1.27 -10.16 0)
		)
		(property "Description" "64K Flash, 3.5K RAM, 1K EEPROM PIC18 Microcontroller ADC PWM SPI I2C USART in TQFP44 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microchip microcontroller PIC18 flash XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F46K22-xPT_0_1")
		(symbol "PIC18F46K22-xPT_1_1"
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 2.54)
				(name "RE0/P3A/AN5")
				(number "25")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 2.54)
				(name "RE1/P3B/AN6")
				(number "26")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 2.54)
				(name "RE2/CCP5/AN7")
				(number "27")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 2.54)
				(name "RD0/SCL2/SCK2/AN20")
				(number "38")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 2.54)
				(name "RD1/SDI1/SDA2/AN21")
				(number "39")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 2.54)
				(name "RD2/P2B/AN22")
				(number "40")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 2.54)
				(name "RD3/P2C/~{SS2}/AN23")
				(number "41")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 2.54)
				(name "RD4/P2D/SDO2/AN24")
				(number "2")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 2.54)
				(name "RD5/P1B/AN25")
				(number "3")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 2.54)
				(name "RD6/TX2/CK2/P1C/AN26")
				(number "4")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 2.54)
				(name "RD7/RX2/DT2/P1D/AN27")
				(number "5")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 2.54)
				(name "RC0/P2B/SOSCO/SCLKI")
				(number "32")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 2.54)
				(name "RC1/SOSCI/P2A")
				(number "35")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 2.54)
				(name "RC2/T1G/CCP2/AN14")
				(number "36")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 2.54)
				(name "RC3/REFO/SCL1/SCK1/AN15")
				(number "37")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 2.54)
				(name "RC4/SDA1/SDI1/AN16")
				(number "42")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 2.54)
				(name "RC5/SDO1/AN17")
				(number "43")
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 2.54)
				(name "RC6/TX1/CK1/AN18")
				(number "44")
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 2.54)
				(name "RC7/RX1/DT1/AN19")
				(number "1")
			)
			(pin no_connect line
				(at -10.16 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -7.62 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -5.08 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at -2.54 -27.94 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin passive line
				(at 0 30.48 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at 0 30.48 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "VSS")
				(number "6")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 2.54)
				(name "~{MCLR}/VPP/RE3")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 2.54)
				(name "OSC1/CLKIN/RA7")
				(number "30")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 2.54)
				(name "OSC2/CLKOUT/RA6")
				(number "31")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 2.54)
				(name "AN0/C12IN0-/RA0")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 2.54)
				(name "AN1/C12INC1-/RA1")
				(number "20")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 2.54)
				(name "VREF-/AN2/C2IN+/RA2")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 2.54)
				(name "VREF+/AN3/C1IN+/RA3")
				(number "22")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 2.54)
				(name "C1OUT/SRQ/T0CKI/RA4")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 2.54)
				(name "AN4/C2OUT/SRQN/~{SS1}/RA5")
				(number "24")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 2.54)
				(name "AN12/FLT0/INT0/RB0")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 2.54)
				(name "AN10/C12IN3-/CTDIN/INT1/RB1")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 2.54)
				(name "AN8/CTED1/INT2/RB2")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 2.54)
				(name "AN9/C12IN2-/CTED2/RB3")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 2.54)
				(name "AN11/T5G/IOC/RB4")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 2.54)
				(name "AN13/CCP3/IOC/RB5")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 2.54)
				(name "PGC/IOC/RB6")
				(number "16")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 2.54)
				(name "PGD/IOC/RB7")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F66J60-IPT"
		(pin_names
			(offset 1.27)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.26 0)
		)
		(property "Value" "PIC18F66J60-IPT"
			(at 17.78 -48.26 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39762f.pdf"
			(at 0 6.35 0)
		)
		(property "Description" "64K Flash, 3.7K SRAM, Ethernet Controller with PHY, 8K Buffer, TQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash Based 8-Bit Microcontroller Ethernet Controller PHY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F66J60-IPT_0_1")
		(symbol "PIC18F66J60-IPT_1_1"
			(pin input line
				(at -30.48 43.18 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "7")
			)
			(pin input line
				(at -30.48 35.56 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "39")
			)
			(pin output line
				(at -30.48 33.02 0)
				(length 3.81)
				(name "OSC2/CLK2")
				(number "40")
			)
			(pin passive line
				(at -30.48 27.94 0)
				(length 3.81)
				(name "ENVREG")
				(number "18")
			)
			(pin passive line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "VDDCORE/VCAP")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RD0/P1B")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RD1/ECCP3/P3A")
				(number "59")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RD2/CCP4/P3D")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "RE0/P2D")
				(number "2")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "RE1/P2C")
				(number "1")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RE2/P2B")
				(number "64")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "RE3/P3C")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RE4/P3B")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RE5/P1C")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RF1/AN6/C2OUT")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RF2/AN7/C1OUT")
				(number "16")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RF3/AN8")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "RF4/AN9")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "RF5/AN10/CVref")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 3.81)
				(name "RF6/AN11")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "RF7/~{SS1}")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "RG4/CCP5/P1D")
				(number "8")
			)
			(pin power_in line
				(at -10.16 -50.8 90)
				(length 3.81)
				(name "AVSS")
				(number "20")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 3.81)
				(name "AVDD")
				(number "19")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "25")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "41")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "57")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "VSS")
				(number "56")
			)
			(pin power_in line
				(at 7.62 50.8 270)
				(length 3.81)
				(name "VDDPLL")
				(number "54")
			)
			(pin power_in line
				(at 7.62 -50.8 90)
				(length 3.81)
				(name "VSSPLL")
				(number "55")
			)
			(pin power_in line
				(at 30.48 45.72 180)
				(length 3.81)
				(name "VDDRX")
				(number "48")
			)
			(pin passive line
				(at 30.48 43.18 180)
				(length 3.81)
				(name "TPIN+")
				(number "47")
			)
			(pin passive line
				(at 30.48 40.64 180)
				(length 3.81)
				(name "TPIN-")
				(number "46")
			)
			(pin power_in line
				(at 30.48 38.1 180)
				(length 3.81)
				(name "VSSRX")
				(number "45")
			)
			(pin power_in line
				(at 30.48 33.02 180)
				(length 3.81)
				(name "VDDTX")
				(number "49")
			)
			(pin passive line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "TPOUT+")
				(number "51")
			)
			(pin passive line
				(at 30.48 27.94 180)
				(length 3.81)
				(name "TPOUT-")
				(number "50")
			)
			(pin power_in line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "VSSTX")
				(number "52")
			)
			(pin passive line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "RBIAS")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "LEDA/AN0/RA0")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "LEDB/AN1/RA1")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "T0CKI/RA4")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "AN4/RA5")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "INT0/FLT0/RB0")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "INT1/RB1")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "INT2/RB2")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "INT3/RB3")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "KBI0/RB4")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "KBI1/RB5")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 3.81)
				(name "PGC/KBI2/RB6")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "PGD/KBI3/RB7")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "T13CKI/T1OSO/RC0")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "T1OSI/ECCP2/P2A/RC1")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 3.81)
				(name "ECCP1/P1A/RC2")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 3.81)
				(name "SCK1/SCL1/RC3")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 3.81)
				(name "SDI1/SDA1/RC4")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 3.81)
				(name "SDO1/RC5")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 3.81)
				(name "TX1/CK1/RC6")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 3.81)
				(name "RX1/DT1/RC7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F87K22-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 67.31 0)
		)
		(property "Value" "PIC18F87K22-xPT"
			(at -11.43 -67.31 0)
		)
		(property "Footprint" "Package_QFP:TQFP-80_12x12mm_P0.5mm"
			(at 27.94 -67.31 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39960d.pdf"
			(at -16.51 -12.7 0)
		)
		(property "Description" "PIC18F nanoWatt XLP Technology MCU, 64MHz, 128KB Flash, 4KB RAM, 1KB EEPROM, 1.8-5.5V, 69 GPIO, TQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F87K22-xPT_0_1")
		(symbol "PIC18F87K22-xPT_1_1"
			(pin bidirectional line
				(at -15.24 58.42 0)
				(length 2.54)
				(name "RA0/AN0")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 55.88 0)
				(length 2.54)
				(name "RA1/AN1")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 53.34 0)
				(length 2.54)
				(name "RA2/AN2/Vref-")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 50.8 0)
				(length 2.54)
				(name "RA3/AN3/Vref+")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 48.26 0)
				(length 2.54)
				(name "RA4")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 45.72 0)
				(length 2.54)
				(name "RA5/AN4")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 43.18 0)
				(length 2.54)
				(name "RA6/OSC2")
				(number "50")
			)
			(pin bidirectional line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "RA7/OSC1")
				(number "49")
			)
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "RF1/AN6")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "RF2/AN7")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "RF3/AN8")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "RF4/AN9")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "RF5/AN10")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "RF6/AN11")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "RF7/AN5")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "RG0")
				(number "5")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "RG1/AN19")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "RG2/AN18")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RG3/AN17")
				(number "8")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RG4/AN16")
				(number "10")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "RG5/~{MCLR}")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "RH0/AN23")
				(number "79")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "RH1/AN22")
				(number "80")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "RH2/AN21")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "RH3/AN20")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "RH4/AN12")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "RH5/AN13")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "RH6/AN14")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "RH7/AN15")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "RJ0")
				(number "62")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "RJ1")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "RJ2")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "RJ3")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 -43.18 0)
				(length 2.54)
				(name "RJ4")
				(number "39")
			)
			(pin bidirectional line
				(at -15.24 -45.72 0)
				(length 2.54)
				(name "RJ5")
				(number "40")
			)
			(pin bidirectional line
				(at -15.24 -48.26 0)
				(length 2.54)
				(name "RJ6")
				(number "41")
			)
			(pin bidirectional line
				(at -15.24 -50.8 0)
				(length 2.54)
				(name "RJ7")
				(number "42")
			)
			(pin passive line
				(at -15.24 -55.88 0)
				(length 2.54)
				(name "VDDCORE/VCAP")
				(number "12")
			)
			(pin power_in line
				(at -2.54 68.58 270)
				(length 2.54)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at 0 68.58 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 2.54)
				(name "VSS")
				(number "11")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "51")
			)
			(pin passive line
				(at 0 -68.58 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "70")
			)
			(pin power_in line
				(at 2.54 68.58 270)
				(length 2.54)
				(name "VDD")
				(number "71")
			)
			(pin power_in line
				(at 5.08 -68.58 90)
				(length 2.54)
				(name "AVSS")
				(number "26")
			)
			(pin power_in line
				(at 7.62 68.58 270)
				(length 2.54)
				(name "AVDD")
				(number "25")
			)
			(pin input line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "ENVREG")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "RB0")
				(number "58")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "RB1")
				(number "57")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "RB2")
				(number "56")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "RB3")
				(number "55")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "RB4")
				(number "54")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "RB5")
				(number "53")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "RB6")
				(number "52")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "RB7")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "RC0")
				(number "36")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "RC1")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RC2")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RC3")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RC4")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "RC5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RC6")
				(number "37")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RC7")
				(number "38")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "RD0")
				(number "72")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "RD1")
				(number "69")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RD2")
				(number "68")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "RD3")
				(number "67")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "RD4")
				(number "66")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "RD5")
				(number "65")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "RD6")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "RD7")
				(number "63")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "RE0")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "RE1")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "RE2")
				(number "78")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "RE3")
				(number "77")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "RE4")
				(number "76")
			)
			(pin bidirectional line
				(at 15.24 -45.72 180)
				(length 2.54)
				(name "RE5")
				(number "75")
			)
			(pin bidirectional line
				(at 15.24 -48.26 180)
				(length 2.54)
				(name "RE6")
				(number "74")
			)
			(pin bidirectional line
				(at 15.24 -50.8 180)
				(length 2.54)
				(name "RE7")
				(number "73")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F96J60-IPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -34.29 71.12 0)
		)
		(property "Value" "PIC18F96J60-IPT"
			(at 27.94 -71.12 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_12x12mm_P0.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39762f.pdf"
			(at -16.51 -12.7 0)
		)
		(property "Description" "64K Flash, 3.7K SRAM, Ethernet Controller with PHY, 8K Buffer, TQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash Based 8-Bit Microcontroller Ethernet Controller PHY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm* TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC18F96J60-IPT_0_1")
		(symbol "PIC18F96J60-IPT_1_1"
			(pin input line
				(at -40.64 66.04 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "13")
			)
			(pin input line
				(at -40.64 58.42 0)
				(length 3.81)
				(name "OSC1/CLKI")
				(number "63")
			)
			(pin output line
				(at -40.64 53.34 0)
				(length 3.81)
				(name "OSC2/CLK0")
				(number "64")
			)
			(pin passive line
				(at -40.64 48.26 0)
				(length 3.81)
				(name "ENVREG")
				(number "29")
			)
			(pin passive line
				(at -40.64 43.18 0)
				(length 3.81)
				(name "VDDCORE/VCAP")
				(number "16")
			)
			(pin bidirectional line
				(at -40.64 38.1 0)
				(length 3.81)
				(name "RF0/AN5")
				(number "12")
			)
			(pin bidirectional line
				(at -40.64 35.56 0)
				(length 3.81)
				(name "RF1/AN6/C2OUT")
				(number "28")
			)
			(pin bidirectional line
				(at -40.64 33.02 0)
				(length 3.81)
				(name "RF2/AN7/C1OUT")
				(number "23")
			)
			(pin bidirectional line
				(at -40.64 30.48 0)
				(length 3.81)
				(name "RF3/AN8")
				(number "22")
			)
			(pin bidirectional line
				(at -40.64 27.94 0)
				(length 3.81)
				(name "RF4/AN9")
				(number "21")
			)
			(pin bidirectional line
				(at -40.64 25.4 0)
				(length 3.81)
				(name "RF5/AN10/CVref")
				(number "20")
			)
			(pin bidirectional line
				(at -40.64 22.86 0)
				(length 3.81)
				(name "RF6/AN11")
				(number "19")
			)
			(pin bidirectional line
				(at -40.64 20.32 0)
				(length 3.81)
				(name "RF7/~{SS1}")
				(number "18")
			)
			(pin bidirectional line
				(at -40.64 15.24 0)
				(length 3.81)
				(name "RG0/ECCP3/P3A")
				(number "71")
			)
			(pin bidirectional line
				(at -40.64 12.7 0)
				(length 3.81)
				(name "RG1/TX2/CK2")
				(number "70")
			)
			(pin bidirectional line
				(at -40.64 10.16 0)
				(length 3.81)
				(name "RG2/RX2/DT2")
				(number "52")
			)
			(pin bidirectional line
				(at -40.64 7.62 0)
				(length 3.81)
				(name "RG3/CCP4/P3D")
				(number "51")
			)
			(pin bidirectional line
				(at -40.64 5.08 0)
				(length 3.81)
				(name "RG4/CCP5/P1D")
				(number "14")
			)
			(pin bidirectional line
				(at -40.64 2.54 0)
				(length 3.81)
				(name "RG5")
				(number "11")
			)
			(pin bidirectional line
				(at -40.64 0 0)
				(length 3.81)
				(name "RG6")
				(number "10")
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 3.81)
				(name "RG7")
				(number "38")
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 3.81)
				(name "RH0/A16")
				(number "99")
			)
			(pin bidirectional line
				(at -40.64 -10.16 0)
				(length 3.81)
				(name "RH1/A17")
				(number "100")
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 3.81)
				(name "RH2/A18")
				(number "1")
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 3.81)
				(name "RH3/A19")
				(number "2")
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 3.81)
				(name "RH4/AN12/P3C")
				(number "27")
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 3.81)
				(name "RH5/AN13/P3B")
				(number "26")
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 3.81)
				(name "RH6/AN14/P1C")
				(number "25")
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 3.81)
				(name "RH7/AN15/P1B")
				(number "24")
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 3.81)
				(name "RJ0/ALE")
				(number "49")
			)
			(pin bidirectional line
				(at -40.64 -33.02 0)
				(length 3.81)
				(name "RJ1/~{OE}")
				(number "50")
			)
			(pin bidirectional line
				(at -40.64 -35.56 0)
				(length 3.81)
				(name "RJ2/~{WRL}")
				(number "66")
			)
			(pin bidirectional line
				(at -40.64 -38.1 0)
				(length 3.81)
				(name "RJ3/~{WRH}")
				(number "61")
			)
			(pin bidirectional line
				(at -40.64 -40.64 0)
				(length 3.81)
				(name "RJ4/BA0")
				(number "47")
			)
			(pin bidirectional line
				(at -40.64 -43.18 0)
				(length 3.81)
				(name "RJ5/~{CE}")
				(number "48")
			)
			(pin bidirectional line
				(at -40.64 -45.72 0)
				(length 3.81)
				(name "RJ6/~{LB}")
				(number "58")
			)
			(pin bidirectional line
				(at -40.64 -48.26 0)
				(length 3.81)
				(name "RJ7/~{UB}")
				(number "39")
			)
			(pin no_connect line
				(at -20.32 -69.85 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin power_in line
				(at -15.24 -73.66 90)
				(length 3.81)
				(name "AVSS")
				(number "31")
			)
			(pin power_in line
				(at -12.7 73.66 270)
				(length 3.81)
				(name "AVDD")
				(number "30")
			)
			(pin power_in line
				(at -7.62 -73.66 90)
				(length 3.81)
				(name "VSS")
				(number "15")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -5.08 -73.66 90)
				(length 3.81)
				(name "VSS")
				(number "36")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "37")
			)
			(pin power_in line
				(at -2.54 -73.66 90)
				(length 3.81)
				(name "VSS")
				(number "40")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "59")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 3.81)
				(name "VSS")
				(number "60")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 2.54 -73.66 90)
				(length 3.81)
				(name "VSS")
				(number "65")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "86")
			)
			(pin power_in line
				(at 5.08 -73.66 90)
				(length 3.81)
				(name "VSS")
				(number "85")
			)
			(pin power_in line
				(at 10.16 -73.66 90)
				(length 3.81)
				(name "VSSPLL")
				(number "82")
			)
			(pin power_in line
				(at 12.7 73.66 270)
				(length 3.81)
				(name "VDDPLL")
				(number "81")
			)
			(pin power_in line
				(at 40.64 66.04 180)
				(length 3.81)
				(name "VDDRX")
				(number "75")
			)
			(pin passive line
				(at 40.64 63.5 180)
				(length 3.81)
				(name "TPIN+")
				(number "74")
			)
			(pin passive line
				(at 40.64 60.96 180)
				(length 3.81)
				(name "TPIN-")
				(number "73")
			)
			(pin power_in line
				(at 40.64 58.42 180)
				(length 3.81)
				(name "VSSRX")
				(number "72")
			)
			(pin power_in line
				(at 40.64 53.34 180)
				(length 3.81)
				(name "VDDTX")
				(number "76")
			)
			(pin passive line
				(at 40.64 50.8 180)
				(length 3.81)
				(name "TP0UT+")
				(number "78")
			)
			(pin passive line
				(at 40.64 48.26 180)
				(length 3.81)
				(name "TPOUT-")
				(number "77")
			)
			(pin power_in line
				(at 40.64 45.72 180)
				(length 3.81)
				(name "VSSTX")
				(number "79")
			)
			(pin passive line
				(at 40.64 40.64 180)
				(length 3.81)
				(name "RBIAS")
				(number "80")
			)
			(pin bidirectional line
				(at 40.64 35.56 180)
				(length 3.81)
				(name "LEDA/AN0/RA0")
				(number "35")
			)
			(pin bidirectional line
				(at 40.64 33.02 180)
				(length 3.81)
				(name "LEDB/AN1/RA1")
				(number "34")
			)
			(pin bidirectional line
				(at 40.64 30.48 180)
				(length 3.81)
				(name "Vref-/AN2/RA2")
				(number "33")
			)
			(pin bidirectional line
				(at 40.64 27.94 180)
				(length 3.81)
				(name "Vref+/AN3/RA3")
				(number "32")
			)
			(pin bidirectional line
				(at 40.64 25.4 180)
				(length 3.81)
				(name "TOCKI/RA4")
				(number "42")
			)
			(pin bidirectional line
				(at 40.64 22.86 180)
				(length 3.81)
				(name "AN4/RA5")
				(number "41")
			)
			(pin bidirectional line
				(at 40.64 20.32 180)
				(length 3.81)
				(name "INT0/FLT0/RB0")
				(number "5")
			)
			(pin bidirectional line
				(at 40.64 17.78 180)
				(length 3.81)
				(name "INT1/RB1")
				(number "6")
			)
			(pin bidirectional line
				(at 40.64 15.24 180)
				(length 3.81)
				(name "INT2/RB2")
				(number "7")
			)
			(pin bidirectional line
				(at 40.64 12.7 180)
				(length 3.81)
				(name "INT3/ECCP2/P2A/RB3")
				(number "8")
			)
			(pin bidirectional line
				(at 40.64 10.16 180)
				(length 3.81)
				(name "KBI0/RB4")
				(number "69")
			)
			(pin bidirectional line
				(at 40.64 7.62 180)
				(length 3.81)
				(name "KBI1/RB5")
				(number "68")
			)
			(pin bidirectional line
				(at 40.64 5.08 180)
				(length 3.81)
				(name "PGC/KBI2/RB6")
				(number "67")
			)
			(pin bidirectional line
				(at 40.64 2.54 180)
				(length 3.81)
				(name "PGD/KBI3/RB7")
				(number "57")
			)
			(pin bidirectional line
				(at 40.64 -2.54 180)
				(length 3.81)
				(name "T13CKI/T1OSO/RC0")
				(number "44")
			)
			(pin bidirectional line
				(at 40.64 -5.08 180)
				(length 3.81)
				(name "T1OSI/ECCP2/P2A/RC1")
				(number "43")
			)
			(pin bidirectional line
				(at 40.64 -7.62 180)
				(length 3.81)
				(name "ECCP1/P1A/RC2")
				(number "53")
			)
			(pin bidirectional line
				(at 40.64 -10.16 180)
				(length 3.81)
				(name "SCK1/SCL1/RC3")
				(number "54")
			)
			(pin bidirectional line
				(at 40.64 -12.7 180)
				(length 3.81)
				(name "SDI1/SDA1/RC4")
				(number "55")
			)
			(pin bidirectional line
				(at 40.64 -15.24 180)
				(length 3.81)
				(name "SDO1/RC5")
				(number "56")
			)
			(pin bidirectional line
				(at 40.64 -17.78 180)
				(length 3.81)
				(name "TX1/CK1/RC6")
				(number "45")
			)
			(pin bidirectional line
				(at 40.64 -20.32 180)
				(length 3.81)
				(name "RX1/DT1/RC7")
				(number "46")
			)
			(pin bidirectional line
				(at 40.64 -25.4 180)
				(length 3.81)
				(name "AD0/PSP0/RD0")
				(number "92")
			)
			(pin bidirectional line
				(at 40.64 -27.94 180)
				(length 3.81)
				(name "AD1/PSP1/RD1")
				(number "91")
			)
			(pin bidirectional line
				(at 40.64 -30.48 180)
				(length 3.81)
				(name "AD2/PSP2/RD2")
				(number "90")
			)
			(pin bidirectional line
				(at 40.64 -33.02 180)
				(length 3.81)
				(name "AD3/PSP3/RD3")
				(number "89")
			)
			(pin bidirectional line
				(at 40.64 -35.56 180)
				(length 3.81)
				(name "SD02/AD4/PSP4/RD4")
				(number "88")
			)
			(pin bidirectional line
				(at 40.64 -38.1 180)
				(length 3.81)
				(name "AD5/PSP5/SDI2/SDA2/RD5")
				(number "87")
			)
			(pin bidirectional line
				(at 40.64 -40.64 180)
				(length 3.81)
				(name "AD6/PSP6/SCK2/SCL2/RD6")
				(number "84")
			)
			(pin bidirectional line
				(at 40.64 -43.18 180)
				(length 3.81)
				(name "AD7/PSP7/~{SS2}/RD7")
				(number "83")
			)
			(pin bidirectional line
				(at 40.64 -48.26 180)
				(length 3.81)
				(name "~{RD}/AD8/P2D/RE0")
				(number "4")
			)
			(pin bidirectional line
				(at 40.64 -50.8 180)
				(length 3.81)
				(name "~{WR}/AD9/P2C/RE1")
				(number "3")
			)
			(pin bidirectional line
				(at 40.64 -53.34 180)
				(length 3.81)
				(name "~{CS}/AD10/P2B/RE2")
				(number "98")
			)
			(pin bidirectional line
				(at 40.64 -55.88 180)
				(length 3.81)
				(name "AD11/P3C/RE3")
				(number "97")
			)
			(pin bidirectional line
				(at 40.64 -58.42 180)
				(length 3.81)
				(name "AD12/P3B/RE4")
				(number "96")
			)
			(pin bidirectional line
				(at 40.64 -60.96 180)
				(length 3.81)
				(name "AD13/P1C/RE5")
				(number "95")
			)
			(pin bidirectional line
				(at 40.64 -63.5 180)
				(length 3.81)
				(name "AD14/P1B/RE6")
				(number "94")
			)
			(pin bidirectional line
				(at 40.64 -66.04 180)
				(length 3.81)
				(name "ECCP2/AD15/P2A/RE7")
				(number "93")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC18F1320-SO"
		(extends "PIC18F1220-SO")
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "PIC18F1320-SO"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39605F.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "18-Pin Flash Microcontroller 8K Flash 256byte RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "RAM ADC UART PWM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x11.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F14K50-EP"
		(extends "PIC18F13K50-EP")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "PIC18F14K50-EP"
			(at 24.13 -17.78 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/41350c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "16K Flash, 768 SRAM, 256 EEPROM, USB, nanoWatt XLP, DIP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F14K50-ESO"
		(extends "PIC18F13K50-ESO")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "PIC18F14K50-ESO"
			(at 22.86 -17.78 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/41350c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "16K Flash, 768 SRAM, 256 EEPROM, USB, nanoWatt XLP, SOIC20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F14K50-ESS"
		(extends "PIC18F13K50-ESS")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "PIC18F14K50-ESS"
			(at 22.86 -17.78 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/41350c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "16K Flash, 768 SRAM, 256 EEPROM, USB, nanoWatt XLP, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F2431-IML"
		(extends "PIC18F2331-IML")
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18F2431-IML"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F2431-ISO"
		(extends "PIC18F2331-ISO")
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18F2431-ISO"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F2431-ISP"
		(extends "PIC18F2331-ISP")
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18F2431-ISP"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F24K20_ISS"
		(extends "PIC18F23K20_ISS")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "PIC18F24K20_ISS"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at -12.7 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001303H.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "16K Flash, 768Byte RAM, 256Byte EEPROM, PIC18 Microcontroller ADC PWM SPI I2C USART in SSOP28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller PIC18F flash XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F24K22-xSO"
		(extends "PIC18F23K22-xSO")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "PIC18F24K22-xSO"
			(at 12.7 25.4 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 5.08 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001412G.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, 2.3V to 5.5V, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F24K22-xSP"
		(extends "PIC18F23K22-xSP")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "PIC18F24K22-xSP"
			(at 12.7 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 1.27 0.635 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001412G.pdf"
			(at 1.27 0.635 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, 2.3V to 5.5V, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F2520-xML"
		(extends "PIC18F2420-xML")
		(property "Reference" "U"
			(at -11.43 26.67 0)
		)
		(property "Value" "PIC18F2520-xML"
			(at 2.54 26.67 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39631E.pdf"
			(at -33.02 10.16 0)
		)
		(property "Description" "MCU 32k Flash, 1536B SRAM, 256B EEPROM, ADC, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F2520-xSP"
		(extends "PIC18F2420-xSP")
		(property "Reference" "U"
			(at -11.43 26.67 0)
		)
		(property "Value" "PIC18F2520-xSP"
			(at 3.81 26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 0 -30.48 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39631E.pdf"
			(at -29.21 33.02 0)
		)
		(property "Description" "MCU 32k Flash, 1536B SRAM, 256B EEPROM, ADC, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F2550-ISO"
		(extends "PIC18F2455-ISO")
		(property "Reference" "U"
			(at -25.4 25.4 0)
		)
		(property "Value" "PIC18F2550-ISO"
			(at 16.51 -25.4 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm_P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F2550-ISP"
		(extends "PIC18F2455-ISP")
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18F2550-ISP"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SPDIP*28_W7.62mm* DIP*28_W7.62mm* PDIP*28_W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F25K20_ISS"
		(extends "PIC18F23K20_ISS")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "PIC18F25K20_ISS"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at -12.7 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001303H.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "32K Flash, 1536Byte RAM, 256Byte EEPROM, PIC18 Microcontroller ADC PWM SPI I2C USART in SSOP28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller PIC18F flash XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F25K22-xSO"
		(extends "PIC18F23K22-xSO")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "PIC18F25K22-xSO"
			(at 12.7 25.4 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 5.08 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001412G.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "32K Flash, 1536B SRAM, 256B EEPROM, nanoWatt XLP, 2.3V to 5.5V, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F25K22-xSP"
		(extends "PIC18F23K22-xSP")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "PIC18F25K22-xSP"
			(at 12.7 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 1.27 0.635 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001412G.pdf"
			(at 1.27 0.635 0)
		)
		(property "Description" "32K Flash, 1536B SRAM, 256B EEPROM, nanoWatt XLP, 2.3V to 5.5V, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F25K50-xML"
		(extends "PIC18F24K50-xML")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18F25K50-xML"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 2.3V to 5.5V, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F25K50-xSO"
		(extends "PIC18F24K50-xSO")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18F25K50-xSO"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 2.3V to 5.5V, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F25K50-xSP"
		(extends "PIC18F24K50-xSP")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18F25K50-xSP"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 2.3V to 5.5V, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SPDIP*W7.62mm* DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F25K50-xSS"
		(extends "PIC18F24K50-xSS")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18F25K50-xSS"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 2.3V to 5.5V, SSOP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F26K20_ISS"
		(extends "PIC18F23K20_ISS")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "PIC18F26K20_ISS"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at -12.7 -12.7 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001303H.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "64K Flash, 3936Byte RAM, 1KByte EEPROM, PIC18 Microcontroller ADC PWM SPI I2C USART in SSOP28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller PIC18F flash XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F26K22-xSO"
		(extends "PIC18F23K22-xSO")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "PIC18F26K22-xSO"
			(at 12.7 25.4 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 5.08 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001412G.pdf"
			(at 5.08 0 0)
		)
		(property "Description" "64K Flash, 3896B SRAM, 1024B EEPROM, nanoWatt XLP, 2.3V to 5.5V, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F26K22-xSP"
		(extends "PIC18F23K22-xSP")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "PIC18F26K22-xSP"
			(at 12.7 25.4 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 1.27 0.635 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001412G.pdf"
			(at 1.27 0.635 0)
		)
		(property "Description" "64K Flash, 3896B SRAM, 1024B EEPROM, nanoWatt XLP, 2.3V to 5.5V, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F26K80_IML"
		(extends "PIC18F25K80_IML")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "PIC18F26K80_IML"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "64K Flash, 3.5K RAM, 1K EEPROM PIC18 Microcontroller ADC PWM CAN SPI I2C USART in QFN28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F26K80_ISS"
		(extends "PIC18F25K80_ISS")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "PIC18F26K80_ISS"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "64K Flash, 3.5K RAM, 1K EEPROM PIC18 Microcontroller ADC PWM CAN SPI I2C USART in SSOP28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F26K83-xSP"
		(extends "PIC18F25K83-xSP")
		(property "Reference" "U"
			(at -11.43 26.67 0)
		)
		(property "Value" "PIC18F26K83-xSP"
			(at 11.43 26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001943A.pdf"
			(at 5.08 -2.54 0)
		)
		(property "Description" "64K Flash, 4K RAM, 1K EEPROM, 2.3-5.5V, PIC18, low-power microcontroller with CAN, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller Microchip DMA WWDT DIA DCI XLP CLC CWG CCP NCO DSM CRC UART LIN DMX DALI SPI CAN I2C PPS SMT ADC2 CVD DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F4431-IML"
		(extends "PIC18F4331-IML")
		(property "Reference" "U"
			(at -30.48 30.48 0)
		)
		(property "Value" "PIC18F4431-IML"
			(at 21.59 -30.48 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F4431-IP"
		(extends "PIC18F4331-IP")
		(property "Reference" "U"
			(at -27.94 30.48 0)
		)
		(property "Value" "PIC18F4431-IP"
			(at 19.05 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24* PDIP*W15.24*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F4431-IPT"
		(extends "PIC18F4331-IPT")
		(property "Reference" "U"
			(at -25.4 30.48 0)
		)
		(property "Value" "PIC18F4431-IPT"
			(at 16.51 -30.48 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F4480-IP"
		(extends "PIC18F4580-IP")
		(property "Reference" "U"
			(at -22.86 30.48 0)
		)
		(property "Value" "PIC18F4480-IP"
			(at 15.24 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39637d.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "32K Flash, 768B SRAM, 256 EEPROM, ECAN, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller CAN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F452-IP"
		(extends "PIC18F442-IP")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18F452-IP"
			(at 12.7 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39564c.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "32K Flash, 1536B SRAM, 256 EEPROM, ADC, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F452-IPT"
		(extends "PIC18F442-IPT")
		(property "Reference" "U"
			(at -21.59 30.48 0)
		)
		(property "Value" "PIC18F452-IPT"
			(at 5.08 -30.48 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39564c.pdf"
			(at 0 0 0)
		)
		(property "Description" "32K Flash, 1536B SRAM, 256 EEPROM, ADC, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F4520-xP"
		(extends "PIC18F4420-xP")
		(property "Reference" "U"
			(at -13.97 31.75 0)
		)
		(property "Value" "PIC18F4520-xP"
			(at 2.54 31.75 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 -35.56 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39631E.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "32K Flash, 1536b SRAM, 256b EEPROM, ADC, DIP-40"
			(at 0 0 0)
		)
		(property "ki_keywords" "32K Flash, 1536b SRAM, 256b EEPROM, ADC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F4550-IML"
		(extends "PIC18F4455-IML")
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18F4550-IML"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F4550-IP"
		(extends "PIC18F4455-IP")
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18F4550-IP"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F4550-IPT"
		(extends "PIC18F4455-IPT")
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18F4550-IPT"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F4553-IML"
		(extends "PIC18F4458-IML")
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18F4553-IML"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39887c.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, 12-Bit A/D, nanoWatt XLP, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F4553-IP"
		(extends "PIC18F4458-IP")
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18F4553-IP"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39887c.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, 12-Bit A/D, nanoWatt XLP, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F4553-IPT"
		(extends "PIC18F4458-IPT")
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18F4553-IPT"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39887c.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, 12-Bit A/D, nanoWatt XLP, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F458-IP"
		(extends "PIC18F448-IP")
		(property "Reference" "U"
			(at -22.86 30.48 0)
		)
		(property "Value" "PIC18F458-IP"
			(at 15.24 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41159e.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "32K Flash, 1536B SRAM, 256 EEPROM, CAN, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller CAN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F45J10-IP"
		(extends "PIC18F44J10-IP")
		(property "Reference" "U"
			(at -25.4 30.48 0)
		)
		(property "Value" "PIC18F45J10-IP"
			(at 16.51 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39682E.pdf"
			(at -29.21 30.48 0)
		)
		(property "Description" "32K Flash, 1K SRAM, ADC, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F46K80-IML"
		(extends "PIC18F45K80-IML")
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "PIC18F46K80-IML"
			(at -22.86 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at -16.51 -2.54 0)
		)
		(property "Description" "64K Flash, 3.5K RAM, 1K EEPROM PIC18 Microcontroller ADC PWM CAN SPI I2C USART in QFN44 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F46K80-IPT"
		(extends "PIC18F45K80-IPT")
		(property "Reference" "U"
			(at -30.48 33.02 0)
		)
		(property "Value" "PIC18F46K80-IPT"
			(at 20.32 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "64K Flash, 3.5K RAM, 1K EEPROM PIC18 Microcontroller ADC PWM CAN SPI I2C USART in TQFP44 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microchip microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F66J65-IPT"
		(extends "PIC18F66J60-IPT")
		(property "Reference" "U"
			(at -25.4 48.26 0)
		)
		(property "Value" "PIC18F66J65-IPT"
			(at 17.78 -48.26 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39762f.pdf"
			(at 0 6.35 0)
		)
		(property "Description" "96K Flash, 3.7K SRAM, Ethernet Controller with PHY, 8K Buffer, TQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash Based 8-Bit Microcontroller Ethernet Controller PHY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F67J60-IPT"
		(extends "PIC18F66J60-IPT")
		(property "Reference" "U"
			(at -25.4 48.26 0)
		)
		(property "Value" "PIC18F67J60-IPT"
			(at 17.78 -48.26 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39762f.pdf"
			(at 0 6.35 0)
		)
		(property "Description" "128K Flash, 3.7K SRAM, Ethernet Controller with PHY, 8K Buffer, TQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash Based 8-Bit Microcontroller Ethernet Controller PHY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F96J60-IPF"
		(extends "PIC18F96J60-IPT")
		(property "Reference" "U"
			(at -34.29 71.12 0)
		)
		(property "Value" "PIC18F96J60-IPF"
			(at 27.94 -71.12 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_12x12mm_P0.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39762f.pdf"
			(at -16.51 -12.7 0)
		)
		(property "Description" "64K Flash, 3.7K SRAM, Ethernet Controller with PHY, 8K Buffer, TQFP100 (14x14mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash Based 8-Bit Microcontroller Ethernet Controller PHY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm* TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F96J65-IPF"
		(extends "PIC18F96J60-IPT")
		(property "Reference" "U"
			(at -34.29 71.12 0)
		)
		(property "Value" "PIC18F96J65-IPF"
			(at 27.94 -71.12 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_12x12mm_P0.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39762f.pdf"
			(at -16.51 -12.7 0)
		)
		(property "Description" "96K Flash, 3.7K SRAM, Ethernet Controller with PHY, 8K Buffer, TQFP100 (14x14mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash Based 8-Bit Microcontroller Ethernet Controller PHY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm* TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F96J65-IPT"
		(extends "PIC18F96J60-IPT")
		(property "Reference" "U"
			(at -34.29 71.12 0)
		)
		(property "Value" "PIC18F96J65-IPT"
			(at 27.94 -71.12 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_12x12mm_P0.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39762f.pdf"
			(at -16.51 -12.7 0)
		)
		(property "Description" "96K Flash, 3.7K SRAM, Ethernet Controller with PHY, 8K Buffer, TQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash Based 8-Bit Microcontroller Ethernet Controller PHY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm* TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F97J60-IPF"
		(extends "PIC18F96J60-IPT")
		(property "Reference" "U"
			(at -34.29 71.12 0)
		)
		(property "Value" "PIC18F97J60-IPF"
			(at 27.94 -71.12 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_12x12mm_P0.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39762f.pdf"
			(at -16.51 -12.7 0)
		)
		(property "Description" "128K Flash, 3.7K SRAM, Ethernet Controller with PHY, 8K Buffer, TQFP100 (14x14mm)"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash Based 8-Bit Microcontroller Ethernet Controller PHY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm* TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18F97J60-IPT"
		(extends "PIC18F96J60-IPT")
		(property "Reference" "U"
			(at -34.29 71.12 0)
		)
		(property "Value" "PIC18F97J60-IPT"
			(at 27.94 -71.12 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_12x12mm_P0.4mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39762f.pdf"
			(at -16.51 -12.7 0)
		)
		(property "Description" "128K Flash, 3.7K SRAM, Ethernet Controller with PHY, 8K Buffer, TQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash Based 8-Bit Microcontroller Ethernet Controller PHY"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm* TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF1220-SO"
		(extends "PIC18F1220-SO")
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "PIC18LF1220-SO"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39605F.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "18-Pin Flash Microcontroller 4K Flash 256byte RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "RAM ADC UART PWM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x11.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF1320-SO"
		(extends "PIC18F1220-SO")
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "PIC18LF1320-SO"
			(at 2.54 13.97 0)
		)
		(property "Footprint" "Package_SO:SOIC-18W_7.5x11.6mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39605F.pdf"
			(at -3.81 13.97 0)
		)
		(property "Description" "18-Pin Flash Microcontroller 8K Flash 256byte RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "RAM ADC UART PWM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x11.6mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF13K50-EP"
		(extends "PIC18F13K50-EP")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "PIC18LF13K50-EP"
			(at 24.13 -17.78 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/41350c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "8K Flash, 512 SRAM, 256 EEPROM, USB, nanoWatt XLP, DIP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF13K50-ESO"
		(extends "PIC18F13K50-ESO")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "PIC18LF13K50-ESO"
			(at 22.86 -17.78 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/41350c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "8K Flash, 512 SRAM, 256 EEPROM, USB, nanoWatt XLP, SOIC20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF13K50-ESS"
		(extends "PIC18F13K50-ESS")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "PIC18LF13K50-ESS"
			(at 22.86 -17.78 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/41350c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "8K Flash, 512 SRAM, 256 EEPROM, USB, nanoWatt XLP, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF14K50-EP"
		(extends "PIC18F13K50-EP")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "PIC18LF14K50-EP"
			(at 24.13 -17.78 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/41350c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "16K Flash, 768 SRAM, 256 EEPROM, USB, nanoWatt XLP, DIP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF14K50-ESO"
		(extends "PIC18F13K50-ESO")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "PIC18LF14K50-ESO"
			(at 22.86 -17.78 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/41350c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "16K Flash, 768 SRAM, 256 EEPROM, USB, nanoWatt XLP, SOIC20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF14K50-ESS"
		(extends "PIC18F13K50-ESS")
		(property "Reference" "U"
			(at -33.02 17.78 0)
		)
		(property "Value" "PIC18LF14K50-ESS"
			(at 22.86 -17.78 0)
		)
		(property "Footprint" "Package_SO:SSOP-20_5.3x7.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/41350c.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "16K Flash, 768 SRAM, 256 EEPROM, USB, nanoWatt XLP, SSOP20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8bit CMOS Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x7.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF2331-IML"
		(extends "PIC18F2331-IML")
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18LF2331-IML"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "8K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF2331-ISO"
		(extends "PIC18F2331-ISO")
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18LF2331-ISO"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "8K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF2331-ISP"
		(extends "PIC18F2331-ISP")
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18LF2331-ISP"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "8K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF2431-IML"
		(extends "PIC18F2331-IML")
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18LF2431-IML"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF2431-ISO"
		(extends "PIC18F2331-ISO")
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18LF2431-ISO"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF2431-ISP"
		(extends "PIC18F2331-ISP")
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18LF2431-ISP"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF2450-IML"
		(extends "PIC18F2450-IML")
		(property "Reference" "U"
			(at -20.32 27.94 0)
		)
		(property "Value" "PIC18LF2450-IML"
			(at 11.43 -27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "16K Flash, 8K SRAM, USB, nanoWatt XLP, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF2450-ISO"
		(extends "PIC18F2450-ISO")
		(property "Reference" "U"
			(at -20.32 27.94 0)
		)
		(property "Value" "PIC18LF2450-ISO"
			(at 11.43 -27.94 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "16K Flash, 8K SRAM, USB, nanoWatt XLP, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*W*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF2450-ISP"
		(extends "PIC18F2450-ISP")
		(property "Reference" "U"
			(at -20.32 27.94 0)
		)
		(property "Value" "PIC18LF2450-ISP"
			(at 11.43 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "16K Flash, 8K SRAM, USB, nanoWatt XLP, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SPDIP*W7.62mm* DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF2455-ISO"
		(extends "PIC18F2455-ISO")
		(property "Reference" "U"
			(at -25.4 25.4 0)
		)
		(property "Value" "PIC18LF2455-ISO"
			(at 16.51 -25.4 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm_P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF2455-ISP"
		(extends "PIC18F2455-ISP")
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18LF2455-ISP"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SPDIP*28_W7.62mm* DIP*28_W7.62mm* PDIP*28_W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF24K50-xML"
		(extends "PIC18F24K50-xML")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18LF24K50-xML"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "16K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 1.8V to 3.6V, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF24K50-xSO"
		(extends "PIC18F24K50-xSO")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18LF24K50-xSO"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "16K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 1.8V to 3.6V, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF24K50-xSP"
		(extends "PIC18F24K50-xSP")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18LF24K50-xSP"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "16K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 1.8V to 3.6V, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SPDIP*W7.62mm* DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF24K50-xSS"
		(extends "PIC18F24K50-xSS")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18LF24K50-xSS"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "16K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 1.8V to 3.6V, SSOP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF2550-ISO"
		(extends "PIC18F2455-ISO")
		(property "Reference" "U"
			(at -25.4 25.4 0)
		)
		(property "Value" "PIC18LF2550-ISO"
			(at 16.51 -25.4 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm_P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF2550-ISP"
		(extends "PIC18F2455-ISP")
		(property "Reference" "U"
			(at -25.4 27.94 0)
		)
		(property "Value" "PIC18LF2550-ISP"
			(at 16.51 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/39632c.pdf"
			(at 0 -11.43 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SPDIP*28_W7.62mm* DIP*28_W7.62mm* PDIP*28_W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF25K50-xML"
		(extends "PIC18F24K50-xML")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18LF25K50-xML"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 1.8V to 3.6V, QFN28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF25K50-xSO"
		(extends "PIC18F24K50-xSO")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18LF25K50-xSO"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 1.8V to 3.6V, SOIC28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SO*W*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF25K50-xSP"
		(extends "PIC18F24K50-xSP")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18LF25K50-xSP"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 1.8V to 3.6V, SPDIP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SPDIP*W7.62mm* DIP*W7.62mm* PDIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF25K50-xSS"
		(extends "PIC18F24K50-xSS")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18LF25K50-xSS"
			(at 12.7 -27.94 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/devicedoc/30000684B.pdf"
			(at -73.66 -34.29 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, 1.8V to 3.6V, SSOP28"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF25K80_IML"
		(extends "PIC18F25K80_IML")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "PIC18LF25K80_IML"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "32K Flash, 3.5K RAM, 1K EEPROM 28-Pin QFN Flash Microcontroller with ECAN and nanoWatt XLP Technology"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller microchip CAN USB UART QFN SPI I2C FLASH EEPROM"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF25K80_ISS"
		(extends "PIC18F25K80_ISS")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "PIC18LF25K80_ISS"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "32K Flash, 3.5K RAM, 1K EEPROM PIC18 Microcontroller ADC PWM CAN SPI I2C USART in SSOP28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microchip microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF25K83-xSP"
		(extends "PIC18F25K83-xSP")
		(property "Reference" "U"
			(at -11.43 26.67 0)
		)
		(property "Value" "PIC18LF25K83-xSP"
			(at 11.43 26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001943A.pdf"
			(at 5.08 -2.54 0)
		)
		(property "Description" "32K Flash, 2K RAM, 1K EEPROM, 1.8-3.6V, PIC18, low-power microcontroller with CAN, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller Microchip DMA WWDT DIA DCI XLP CLC CWG CCP NCO DSM CRC UART LIN DMX DALI SPI CAN I2C PPS SMT ADC2 CVD DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF26K80_IML"
		(extends "PIC18F25K80_IML")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "PIC18LF26K80_IML"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "64K Flash, 3.5K RAM, 1K EEPROM PIC18 Microcontroller ADC PWM CAN SPI I2C USART in QFN28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microchip microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF26K80_ISS"
		(extends "PIC18F25K80_ISS")
		(property "Reference" "U"
			(at -17.78 24.13 0)
		)
		(property "Value" "PIC18LF26K80_ISS"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_SO:SSOP-28_5.3x10.2mm_P0.65mm"
			(at 0 -6.35 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at 0 -1.27 0)
		)
		(property "Description" "64K Flash, 3.5K RAM, 1K EEPROM PIC18 Microcontroller ADC PWM CAN SPI I2C USART in SSOP28 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microchip microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SSOP*5.3x10.2mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF26K83-xSP"
		(extends "PIC18F25K83-xSP")
		(property "Reference" "U"
			(at -11.43 26.67 0)
		)
		(property "Value" "PIC18LF26K83-xSP"
			(at 11.43 26.67 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W7.62mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/40001943A.pdf"
			(at 5.08 -2.54 0)
		)
		(property "Description" "64K Flash, 4K RAM, 1K EEPROM, 1.8-3.6V, PIC18, low-power microcontroller with CAN, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller Microchip DMA WWDT DIA DCI XLP CLC CWG CCP NCO DSM CRC UART LIN DMX DALI SPI CAN I2C PPS SMT ADC2 CVD DAC"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4331-IML"
		(extends "PIC18F4331-IML")
		(property "Reference" "U"
			(at -30.48 30.48 0)
		)
		(property "Value" "PIC18LF4331-IML"
			(at 21.59 -30.48 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "8K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4331-IP"
		(extends "PIC18F4331-IP")
		(property "Reference" "U"
			(at -27.94 30.48 0)
		)
		(property "Value" "PIC18LF4331-IP"
			(at 19.05 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "8K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24* PDIP*W15.24*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4331-IPT"
		(extends "PIC18F4331-IPT")
		(property "Reference" "U"
			(at -25.4 30.48 0)
		)
		(property "Value" "PIC18LF4331-IPT"
			(at 16.51 -30.48 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "8K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF442-IP"
		(extends "PIC18F442-IP")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18LF442-IP"
			(at 12.7 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39564c.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256 EEPROM, ADC, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF442-IPT"
		(extends "PIC18F442-IPT")
		(property "Reference" "U"
			(at -21.59 30.48 0)
		)
		(property "Value" "PIC18LF442-IPT"
			(at 5.08 -30.48 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39564c.pdf"
			(at 0 0 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256 EEPROM, ADC, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4431-IML"
		(extends "PIC18F4331-IML")
		(property "Reference" "U"
			(at -30.48 30.48 0)
		)
		(property "Value" "PIC18LF4431-IML"
			(at 21.59 -30.48 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4431-IP"
		(extends "PIC18F4331-IP")
		(property "Reference" "U"
			(at -27.94 30.48 0)
		)
		(property "Value" "PIC18LF4431-IP"
			(at 19.05 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24* PDIP*W15.24*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4431-IPT"
		(extends "PIC18F4331-IPT")
		(property "Reference" "U"
			(at -25.4 30.48 0)
		)
		(property "Value" "PIC18LF4431-IPT"
			(at 16.51 -30.48 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39616d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256B EEPROM, nanoWatt XLP, ADC, PWM, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4450-IML"
		(extends "PIC18F4450-IML")
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18LF4450-IML"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "16K Flash, 8K SRAM, USB, nanoWatt XLP, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4450-IP"
		(extends "PIC18F4450-IP")
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18LF4450-IP"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "16K Flash, 8K SRAM, USB, nanoWatt XLP, PDIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4450-IPT"
		(extends "PIC18F4450-IPT")
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18LF4450-IPT"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "16K Flash, 8K SRAM, USB, nanoWatt XLP, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4455-IML"
		(extends "PIC18F4455-IML")
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18LF4455-IML"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4455-IP"
		(extends "PIC18F4455-IP")
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18LF4455-IP"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4455-IPT"
		(extends "PIC18F4455-IPT")
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18LF4455-IPT"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4458-IML"
		(extends "PIC18F4458-IML")
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18LF4458-IML"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39887c.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, 12-Bit A/D, nanoWatt XLP, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4458-IP"
		(extends "PIC18F4458-IP")
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18LF4458-IP"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39887c.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, 12-Bit A/D, nanoWatt XLP, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4458-IPT"
		(extends "PIC18F4458-IPT")
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18LF4458-IPT"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39887c.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "24K Flash, 2K SRAM, 256 EEPROM, USB, 12-Bit A/D, nanoWatt XLP, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF448-IP"
		(extends "PIC18F448-IP")
		(property "Reference" "U"
			(at -22.86 30.48 0)
		)
		(property "Value" "PIC18LF448-IP"
			(at 15.24 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41159e.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "16K Flash, 768B SRAM, 256 EEPROM, CAN, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller CAN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4480-IP"
		(extends "PIC18F4580-IP")
		(property "Reference" "U"
			(at -22.86 30.48 0)
		)
		(property "Value" "PIC18LF4480-IP"
			(at 15.24 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39637d.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "32K Flash, 768B SRAM, 256 EEPROM, ECAN, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller CAN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF44J10-IP"
		(extends "PIC18F44J10-IP")
		(property "Reference" "U"
			(at -25.4 30.48 0)
		)
		(property "Value" "PIC18LF44J10-IP"
			(at 16.51 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39682E.pdf"
			(at -29.21 30.48 0)
		)
		(property "Description" "16K Flash, 1K SRAM, ADC, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF452-IP"
		(extends "PIC18F442-IP")
		(property "Reference" "U"
			(at -20.32 30.48 0)
		)
		(property "Value" "PIC18LF452-IP"
			(at 12.7 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39564c.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "32K Flash, 1536B SRAM, 256 EEPROM, ADC, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF452-IPT"
		(extends "PIC18F442-IPT")
		(property "Reference" "U"
			(at -21.59 30.48 0)
		)
		(property "Value" "PIC18LF452-IPT"
			(at 5.08 -30.48 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39564c.pdf"
			(at 0 0 0)
		)
		(property "Description" "32K Flash, 1536B SRAM, 256 EEPROM, ADC, TQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4550-IML"
		(extends "PIC18F4455-IML")
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18LF4550-IML"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4550-IP"
		(extends "PIC18F4455-IP")
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18LF4550-IP"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4550-IPT"
		(extends "PIC18F4455-IPT")
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18LF4550-IPT"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39760d.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, nanoWatt XLP, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4553-IML"
		(extends "PIC18F4458-IML")
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18LF4553-IML"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39887c.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, 12-Bit A/D, nanoWatt XLP, QFN44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4553-IP"
		(extends "PIC18F4458-IP")
		(property "Reference" "U"
			(at -22.86 33.02 0)
		)
		(property "Value" "PIC18LF4553-IP"
			(at 13.97 -33.02 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39887c.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, 12-Bit A/D, nanoWatt XLP, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4553-IPT"
		(extends "PIC18F4458-IPT")
		(property "Reference" "U"
			(at -25.4 33.02 0)
		)
		(property "Value" "PIC18LF4553-IPT"
			(at 16.51 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 5.08 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39887c.pdf"
			(at 0 -6.35 0)
		)
		(property "Description" "32K Flash, 2K SRAM, 256 EEPROM, USB, 12-Bit A/D, nanoWatt XLP, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller XLP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF458-IP"
		(extends "PIC18F448-IP")
		(property "Reference" "U"
			(at -22.86 30.48 0)
		)
		(property "Value" "PIC18LF458-IP"
			(at 15.24 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/41159e.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "32K Flash, 1536B SRAM, 256 EEPROM, CAN, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller CAN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF4580-IP"
		(extends "PIC18F4580-IP")
		(property "Reference" "U"
			(at -22.86 30.48 0)
		)
		(property "Value" "PIC18LF4580-IP"
			(at 15.24 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39637d.pdf"
			(at 0 -8.89 0)
		)
		(property "Description" "32K Flash, 1536B SRAM, 256 EEPROM, ECAN, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller CAN"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF45J10-IP"
		(extends "PIC18F44J10-IP")
		(property "Reference" "U"
			(at -25.4 30.48 0)
		)
		(property "Value" "PIC18LF45J10-IP"
			(at 16.51 -30.48 0)
		)
		(property "Footprint" "Package_DIP:DIP-40_W15.24mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39682E.pdf"
			(at -29.21 30.48 0)
		)
		(property "Description" "32K Flash, 1K SRAM, ADC, DIP40"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 8-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*W15.24mm* PDIP*W15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF45K50_QFP"
		(extends "PIC18F45K50_QFP")
		(property "Reference" "U"
			(at -36.83 33.02 0)
		)
		(property "Value" "PIC18LF45K50_QFP"
			(at 30.48 -35.56 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/30000684B.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "32K Flash, 2K RAM, 256B EEPROM, Microchip PIC18F series enhanced flash microcontroller with USB and nanoWatt XLP Technology in TQFP-44 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microcontroller Flash EEPROM SPI I2C USB UART USART ADC TQFP"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF45K80-IML"
		(extends "PIC18F45K80-IML")
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "PIC18LF45K80-IML"
			(at -22.86 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at -16.51 -2.54 0)
		)
		(property "Description" "32K Flash, 3.5K RAM, 1K EEPROM PIC18 Microcontroller ADC PWM CAN SPI I2C USART in QFN44 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microchip microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF45K80-IPT"
		(extends "PIC18F45K80-IPT")
		(property "Reference" "U"
			(at -30.48 33.02 0)
		)
		(property "Value" "PIC18LF45K80-IPT"
			(at 20.32 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "32K Flash, 3.5K RAM, 1K EEPROM PIC18 Microcontroller ADC PWM CAN SPI I2C USART in TQFP44 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microchip microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF46K80-IML"
		(extends "PIC18F45K80-IML")
		(property "Reference" "U"
			(at -22.86 29.21 0)
		)
		(property "Value" "PIC18LF46K80-IML"
			(at -22.86 -29.21 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-44-1EP_8x8mm_P0.65mm_EP6.45x6.45mm"
			(at 0 -20.32 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at -16.51 -2.54 0)
		)
		(property "Description" "64K Flash, 3.5K RAM, 1K EEPROM PIC18 Microcontroller ADC PWM CAN SPI I2C USART in QFN44 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microchip microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC18LF46K80-IPT"
		(extends "PIC18F45K80-IPT")
		(property "Reference" "U"
			(at -30.48 33.02 0)
		)
		(property "Value" "PIC18LF46K80-IPT"
			(at 20.32 -33.02 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39977f.pdf"
			(at 0 -7.62 0)
		)
		(property "Description" "64K Flash, 3.5K RAM, 1K EEPROM PIC18 Microcontroller ADC PWM CAN SPI I2C USART in TQFP44 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "microchip microcontroller PIC18 flash ECAN XLP nanoWatt"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
)
