(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "PIC24FJ256DA210-xBG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 71.12 0)
		)
		(property "Value" "PIC24FJ256DA210-xBG"
			(at 8.89 71.12 0)
		)
		(property "Footprint" "Package_BGA:XBGA-121_10x10mm_Layout11x11_P0.8mm"
			(at 0 -83.82 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39969b.pdf"
			(at 105.41 21.59 0)
		)
		(property "Description" "256K Flash, 96KB SRAM, Graphic controller, USB, BGA-121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 16-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XBGA*10x10mm*Layout11x11*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "PIC24FJ256DA210-xBG_1_1"
			(pin input line
				(at -22.86 58.42 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "F1")
			)
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 3.81)
				(name "RA0")
				(number "G3")
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 3.81)
				(name "RA1")
				(number "J6")
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 3.81)
				(name "RA2")
				(number "H11")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 3.81)
				(name "RA3")
				(number "G10")
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 3.81)
				(name "RA4")
				(number "G11")
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 3.81)
				(name "RA5")
				(number "G9")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 3.81)
				(name "RA6")
				(number "C5")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 3.81)
				(name "RA7")
				(number "B5")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 3.81)
				(name "RA9")
				(number "L2")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "RA10")
				(number "K3")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "RA14")
				(number "E11")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "RA15")
				(number "E8")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "RB0/PGED1")
				(number "K2")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "RB1/PGEC1")
				(number "K1")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "RB2")
				(number "J2")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "RB3")
				(number "J1")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "RB4/PGED3")
				(number "H2")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "RB5/PGEC3")
				(number "H1")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "RB6/PGEC2")
				(number "L1")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "RB7/PGED2")
				(number "J3")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "RB8")
				(number "K4")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "RB9")
				(number "L4")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "RB10")
				(number "L5")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "RB11")
				(number "J5")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "RB12")
				(number "J7")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "RB13")
				(number "L7")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "RB14")
				(number "K7")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "RB15")
				(number "L8")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "RC1")
				(number "D1")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 3.81)
				(name "RC2")
				(number "E4")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "RC3")
				(number "E2")
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 3.81)
				(name "RC4")
				(number "E1")
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 3.81)
				(name "RC12/OSCI")
				(number "F9")
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 3.81)
				(name "RC13")
				(number "C10")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 3.81)
				(name "RC14")
				(number "B11")
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 3.81)
				(name "RC15/OSCO")
				(number "F11")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 3.81)
				(name "RE0")
				(number "A4")
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 3.81)
				(name "RE1")
				(number "B4")
			)
			(pin bidirectional line
				(at -22.86 -50.8 0)
				(length 3.81)
				(name "RE2")
				(number "B3")
			)
			(pin bidirectional line
				(at -22.86 -53.34 0)
				(length 3.81)
				(name "RE3")
				(number "A2")
			)
			(pin bidirectional line
				(at -22.86 -55.88 0)
				(length 3.81)
				(name "RE4")
				(number "A1")
			)
			(pin bidirectional line
				(at -22.86 -58.42 0)
				(length 3.81)
				(name "RE5")
				(number "D3")
			)
			(pin bidirectional line
				(at -22.86 -60.96 0)
				(length 3.81)
				(name "RE6")
				(number "C1")
			)
			(pin bidirectional line
				(at -22.86 -63.5 0)
				(length 3.81)
				(name "RE7")
				(number "D2")
			)
			(pin bidirectional line
				(at -22.86 -66.04 0)
				(length 3.81)
				(name "RE8")
				(number "G1")
			)
			(pin bidirectional line
				(at -22.86 -68.58 0)
				(length 3.81)
				(name "RE9")
				(number "G2")
			)
			(pin power_in line
				(at -15.24 73.66 270)
				(length 3.81)
				(name "AVDD")
				(number "J4")
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "C2")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "C9")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "E5")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "F8")
			)
			(pin power_in line
				(at -2.54 -73.66 90)
				(length 3.81)
				(name "AVSS")
				(number "L3")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "G5")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "B10")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "D4")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "D5")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 3.81)
				(name "VSS")
				(number "F10")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "F5")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "G6")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "H3")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "H4")
			)
			(pin no_connect line
				(at 2.54 -25.4 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "A8")
			)
			(pin no_connect line
				(at 2.54 -27.94 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "B1")
			)
			(pin no_connect line
				(at 2.54 -30.48 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "C6")
			)
			(pin no_connect line
				(at 2.54 -33.02 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "D6")
			)
			(pin no_connect line
				(at 2.54 -35.56 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "D10")
			)
			(pin no_connect line
				(at 2.54 -38.1 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "E7")
			)
			(pin no_connect line
				(at 2.54 -40.64 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "F6")
			)
			(pin no_connect line
				(at 2.54 -43.18 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "F7")
			)
			(pin no_connect line
				(at 2.54 -45.72 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "G4")
			)
			(pin no_connect line
				(at 2.54 -48.26 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "G8")
			)
			(pin no_connect line
				(at 2.54 -50.8 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "H5")
			)
			(pin no_connect line
				(at 2.54 -53.34 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "H7")
			)
			(pin no_connect line
				(at 2.54 -55.88 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "J8")
			)
			(pin no_connect line
				(at 2.54 -58.42 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "J9")
			)
			(pin no_connect line
				(at 2.54 -60.96 180)
				(length 3.81)
				(hide yes)
				(name "N/C")
				(number "K5")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "H6")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "K8")
			)
			(pin passive line
				(at 22.86 63.5 180)
				(length 3.81)
				(name "VCAP")
				(number "B7")
			)
			(pin input line
				(at 22.86 60.96 180)
				(length 3.81)
				(name "ENVREG")
				(number "A7")
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 3.81)
				(name "VUSB")
				(number "H9")
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 3.81)
				(name "RF0")
				(number "B6")
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 3.81)
				(name "RF1")
				(number "A6")
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 3.81)
				(name "RF2")
				(number "K11")
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 3.81)
				(name "RF3")
				(number "K10")
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 3.81)
				(name "RF4")
				(number "L10")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 3.81)
				(name "RF5")
				(number "L11")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 3.81)
				(name "RF7")
				(number "H8")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 3.81)
				(name "RF8")
				(number "J10")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 3.81)
				(name "RF12")
				(number "K6")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "RF13")
				(number "L6")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "RD0")
				(number "D9")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "RD1")
				(number "A11")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "RD2")
				(number "A10")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "RD3")
				(number "B9")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "RD4")
				(number "C8")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "RD5")
				(number "B8")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "RD6")
				(number "D7")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "RD7")
				(number "C7")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "RD8")
				(number "E9")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "RD9")
				(number "E10")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "RD10")
				(number "D11")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "RD11")
				(number "C11")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "RD12")
				(number "A9")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "RD13")
				(number "D8")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "RD14")
				(number "L9")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "RD15")
				(number "K9")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "RG0")
				(number "A5")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "RG1")
				(number "E6")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "D+/RG2")
				(number "H10")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 3.81)
				(name "D-/RG3")
				(number "J11")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 3.81)
				(name "RG6")
				(number "E3")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 3.81)
				(name "RG7")
				(number "F4")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 3.81)
				(name "RG8")
				(number "F2")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 3.81)
				(name "RG9")
				(number "F3")
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 3.81)
				(name "RG12")
				(number "C3")
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 3.81)
				(name "RG13")
				(number "A3")
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 3.81)
				(name "RG14")
				(number "C4")
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 3.81)
				(name "RG15")
				(number "B2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC24FJ256DA210-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 71.12 0)
		)
		(property "Value" "PIC24FJ256DA210-xPT"
			(at 8.89 71.12 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_12x12mm_P0.4mm"
			(at -2.54 -83.82 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39969b.pdf"
			(at 105.41 21.59 0)
		)
		(property "Description" "256K Flash, 96KB SRAM, Graphic controller, USB, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 16-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "PIC24FJ256DA210-xPT_1_1"
			(pin input line
				(at -20.32 63.5 0)
				(length 3.81)
				(name "~{MCLR}")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 58.42 0)
				(length 3.81)
				(name "RA0")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 55.88 0)
				(length 3.81)
				(name "RA1")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 53.34 0)
				(length 3.81)
				(name "RA2")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 3.81)
				(name "RA3")
				(number "59")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 3.81)
				(name "RA4")
				(number "60")
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 3.81)
				(name "RA5")
				(number "61")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 3.81)
				(name "RA6")
				(number "91")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "RA7")
				(number "92")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "RA9")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "RA10")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 3.81)
				(name "RA14")
				(number "66")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "RA15")
				(number "67")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "RB0/PGED1")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "RB1/PGEC1")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "RB3")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "RB4/PGED3/USBOEN")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "RB5/PGEC3")
				(number "20")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "RB6/PGEC2")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "RB7/PGED2")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "RB8")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "RB9")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "RB10")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "RB11")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "RB12")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "RB13")
				(number "42")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "RB14")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "RB15")
				(number "44")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "RC1")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "RC2")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "RC3")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "RC4")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "RC12/OSCI")
				(number "63")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "RC13")
				(number "73")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "RC14")
				(number "74")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 3.81)
				(name "RC15/OSCO")
				(number "64")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "RE0")
				(number "93")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "RE1")
				(number "94")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "RE2")
				(number "98")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "RE3")
				(number "99")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "RE4")
				(number "100")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "RE5")
				(number "3")
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "RE6")
				(number "4")
			)
			(pin bidirectional line
				(at -20.32 -58.42 0)
				(length 3.81)
				(name "RE7")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -60.96 0)
				(length 3.81)
				(name "RE8")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 -63.5 0)
				(length 3.81)
				(name "RE9")
				(number "19")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 3.81)
				(name "AVDD")
				(number "30")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -73.66 90)
				(length 3.81)
				(name "AVSS")
				(number "31")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "37")
			)
			(pin power_in line
				(at 2.54 -73.66 90)
				(length 3.81)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at 2.54 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "36")
			)
			(pin passive line
				(at 2.54 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "45")
			)
			(pin passive line
				(at 2.54 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "65")
			)
			(pin passive line
				(at 2.54 -73.66 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "75")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "46")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "62")
			)
			(pin passive line
				(at 20.32 63.5 180)
				(length 3.81)
				(name "VCAP")
				(number "85")
			)
			(pin input line
				(at 20.32 60.96 180)
				(length 3.81)
				(name "ENVREG")
				(number "86")
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "VUSB")
				(number "55")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "RD0")
				(number "72")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "RD1")
				(number "76")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "RD2")
				(number "77")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "RD3")
				(number "78")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "RD4")
				(number "81")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "RD5")
				(number "82")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "RD6")
				(number "83")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "RD7")
				(number "84")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "RD8")
				(number "68")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "RD9")
				(number "69")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "RD10")
				(number "70")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "RD11")
				(number "71")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "RD12")
				(number "79")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "RD13")
				(number "80")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "RD14")
				(number "47")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "RD15")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "RF0")
				(number "87")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "RF1")
				(number "88")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "RF2")
				(number "52")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "USBID/RF3")
				(number "51")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "RF4")
				(number "49")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "RF5")
				(number "50")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "RF7")
				(number "54")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "RF8")
				(number "53")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "RF12")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "RF31")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "RG0")
				(number "90")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "RG1")
				(number "89")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "D+/RG2")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "D-/RG3")
				(number "56")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "RG6")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "RG7")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 3.81)
				(name "RG8")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 3.81)
				(name "RG9")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 3.81)
				(name "RG12")
				(number "96")
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 3.81)
				(name "RG13")
				(number "97")
			)
			(pin bidirectional line
				(at 20.32 -63.5 180)
				(length 3.81)
				(name "RG14")
				(number "95")
			)
			(pin bidirectional line
				(at 20.32 -66.04 180)
				(length 3.81)
				(name "RG15")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC24FJ64GA306-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 44.45 0)
		)
		(property "Value" "PIC24FJ64GA306-xPT"
			(at 1.27 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at -1.27 -5.08 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/30009996g.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "64K Flash, 8KB SRAM, LCD controller, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 16-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC24FJ64GA306-xPT_1_1"
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 2.54)
				(name "RB0/PGED1")
				(number "16")
				(alternate "AN0" bidirectional line)
				(alternate "CN2" bidirectional line)
				(alternate "CVREF+" bidirectional line)
				(alternate "PMA6" bidirectional line)
				(alternate "RP0" bidirectional line)
				(alternate "SEG7" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "RB1/PGEC1")
				(number "15")
				(alternate "AN1" bidirectional line)
				(alternate "CN3" bidirectional line)
				(alternate "CTED12" bidirectional line)
				(alternate "CVREF-" bidirectional line)
				(alternate "RP1" bidirectional line)
				(alternate "SEG6" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "RB2")
				(number "14")
				(alternate "AN2" bidirectional line)
				(alternate "C2INB" bidirectional line)
				(alternate "CN4" bidirectional line)
				(alternate "CTCMP" bidirectional line)
				(alternate "CTED13" bidirectional line)
				(alternate "RP13" bidirectional line)
				(alternate "SEG5" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "RB3")
				(number "13")
				(alternate "AN3" bidirectional line)
				(alternate "C2INA" bidirectional line)
				(alternate "CN5" bidirectional line)
				(alternate "SEG4" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 2.54)
				(name "RB4/PGED3")
				(number "12")
				(alternate "AN4" bidirectional line)
				(alternate "C1INB" bidirectional line)
				(alternate "CN6" bidirectional line)
				(alternate "RP28" bidirectional line)
				(alternate "SEG3" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "RB5/PGEC3")
				(number "11")
				(alternate "AN5" bidirectional line)
				(alternate "C1INA" bidirectional line)
				(alternate "CN7" bidirectional line)
				(alternate "RP18" bidirectional line)
				(alternate "SEG2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "RB6/PGEC2")
				(number "17")
				(alternate "AN6" bidirectional line)
				(alternate "CN24" bidirectional line)
				(alternate "LCDBIAS3" bidirectional line)
				(alternate "RP6" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 2.54)
				(name "RB7/PGED2")
				(number "18")
				(alternate "AN7" bidirectional line)
				(alternate "CN25" bidirectional line)
				(alternate "RP7" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "RB8")
				(number "21")
				(alternate "AN8" bidirectional line)
				(alternate "CN26" bidirectional line)
				(alternate "COM7" bidirectional line)
				(alternate "RP8" bidirectional line)
				(alternate "SEG31" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "RB9")
				(number "22")
				(alternate "AN9" bidirectional line)
				(alternate "CN27" bidirectional line)
				(alternate "COM6" bidirectional line)
				(alternate "PMA7" bidirectional line)
				(alternate "RP9" bidirectional line)
				(alternate "SEG30" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "RB10")
				(number "23")
				(alternate "AN10" bidirectional line)
				(alternate "CN28" bidirectional line)
				(alternate "COM5" bidirectional line)
				(alternate "CVREF" bidirectional line)
				(alternate "PMA13" bidirectional line)
				(alternate "SEG29" bidirectional line)
				(alternate "TMS" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 2.54)
				(name "RB11")
				(number "24")
				(alternate "AN11" bidirectional line)
				(alternate "CN29" bidirectional line)
				(alternate "PMA12" bidirectional line)
				(alternate "TDO" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RB12")
				(number "27")
				(alternate "AN12" bidirectional line)
				(alternate "CN30" bidirectional line)
				(alternate "CTED2" bidirectional line)
				(alternate "PMA11" bidirectional line)
				(alternate "SEG18" bidirectional line)
				(alternate "TCK" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "RB13")
				(number "28")
				(alternate "AN13" bidirectional line)
				(alternate "CN31" bidirectional line)
				(alternate "CTED1" bidirectional line)
				(alternate "PMA10" bidirectional line)
				(alternate "SEG19" bidirectional line)
				(alternate "TDI" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "RB14")
				(number "29")
				(alternate "AN14" bidirectional line)
				(alternate "CN32" bidirectional line)
				(alternate "CTED5" bidirectional line)
				(alternate "CTPLS" bidirectional line)
				(alternate "PMA1" bidirectional line)
				(alternate "RP14" bidirectional line)
				(alternate "SEG8" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "RB15")
				(number "30")
				(alternate "AN15" bidirectional line)
				(alternate "CN12" bidirectional line)
				(alternate "CTED6" bidirectional line)
				(alternate "PMA0" bidirectional line)
				(alternate "REFO" bidirectional line)
				(alternate "RP29" bidirectional line)
				(alternate "SEG9" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "RC13/SOSCI")
				(number "47")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "RC14/SCKLI/SOSCO")
				(number "48")
				(alternate "RPI37" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "RC12/CLKI/OSCI")
				(number "39")
				(alternate "CN23" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "RC15/CLKO/OSCO")
				(number "40")
				(alternate "CN22" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "RG2")
				(number "37")
				(alternate "CN72" bidirectional line)
				(alternate "SCL1" bidirectional line)
				(alternate "SEG28" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "RG3")
				(number "36")
				(alternate "CN73" bidirectional line)
				(alternate "SDA1" bidirectional line)
				(alternate "SEG47" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "RG6")
				(number "4")
				(alternate "C1IND" bidirectional line)
				(alternate "CN8" bidirectional line)
				(alternate "PMA5" bidirectional line)
				(alternate "RP21" bidirectional line)
				(alternate "SEG0" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "RG7")
				(number "5")
				(alternate "C1INC" bidirectional line)
				(alternate "CN9" bidirectional line)
				(alternate "PMA4" bidirectional line)
				(alternate "RP26" bidirectional line)
				(alternate "VLCAP1" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "RG8")
				(number "6")
				(alternate "C2IND" bidirectional line)
				(alternate "CN10" bidirectional line)
				(alternate "PMA3" bidirectional line)
				(alternate "RP19" bidirectional line)
				(alternate "VLCAP2" bidirectional line)
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "RG9")
				(number "8")
				(alternate "C2INC" bidirectional line)
				(alternate "CN11" bidirectional line)
				(alternate "PMA2" bidirectional line)
				(alternate "RP27" bidirectional line)
				(alternate "SEG1" bidirectional line)
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "AVDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "AVSS")
				(number "20")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "26")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDD")
				(number "38")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "25")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "41")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VBAT")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 2.54)
				(name "RD0")
				(number "46")
				(alternate "CN49" bidirectional line)
				(alternate "RP11" bidirectional line)
				(alternate "SEG17" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "RD1")
				(number "49")
				(alternate "CN50" bidirectional line)
				(alternate "RP24" bidirectional line)
				(alternate "SEG20" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "RD2")
				(number "50")
				(alternate "CN51" bidirectional line)
				(alternate "PMACK1" bidirectional line)
				(alternate "RP23" bidirectional line)
				(alternate "SEG21" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 2.54)
				(name "RD3")
				(number "51")
				(alternate "CN52" bidirectional line)
				(alternate "PMBE0" bidirectional line)
				(alternate "RP22" bidirectional line)
				(alternate "SEG22" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "RD4")
				(number "52")
				(alternate "CN13" bidirectional line)
				(alternate "PMWR" bidirectional line)
				(alternate "RP25" bidirectional line)
				(alternate "SEG23" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "RD5")
				(number "53")
				(alternate "CN14" bidirectional line)
				(alternate "PMRD" bidirectional line)
				(alternate "RP20" bidirectional line)
				(alternate "SEG24" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 2.54)
				(name "RD6")
				(number "54")
				(alternate "C3INB" bidirectional line)
				(alternate "CN15" bidirectional line)
				(alternate "SEG25" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "RD7")
				(number "55")
				(alternate "C3INA" bidirectional line)
				(alternate "CN16" bidirectional line)
				(alternate "SEG26" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "RD8")
				(number "42")
				(alternate "CN53" bidirectional line)
				(alternate "RP2" bidirectional line)
				(alternate "RTCC" bidirectional line)
				(alternate "SEG13" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 2.54)
				(name "RD9")
				(number "43")
				(alternate "CN54" bidirectional line)
				(alternate "PMACK2" bidirectional line)
				(alternate "RP4" bidirectional line)
				(alternate "SEG14" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "RD10")
				(number "44")
				(alternate "C3IND" bidirectional line)
				(alternate "CN55" bidirectional line)
				(alternate "CS2" bidirectional line)
				(alternate "PMA15" bidirectional line)
				(alternate "RP3" bidirectional line)
				(alternate "SEG15" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "RD11")
				(number "45")
				(alternate "C3INC" bidirectional line)
				(alternate "CN56" bidirectional line)
				(alternate "CS1" bidirectional line)
				(alternate "PMA14" bidirectional line)
				(alternate "RP12" bidirectional line)
				(alternate "SEG16" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "RE0")
				(number "60")
				(alternate "CN58" bidirectional line)
				(alternate "COM3" bidirectional line)
				(alternate "PMD0" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "RE1")
				(number "61")
				(alternate "CN59" bidirectional line)
				(alternate "COM2" bidirectional line)
				(alternate "PMD1" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "RE2")
				(number "62")
				(alternate "CN60" bidirectional line)
				(alternate "COM1" bidirectional line)
				(alternate "PMD2" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 2.54)
				(name "RE3")
				(number "63")
				(alternate "CN61" bidirectional line)
				(alternate "COM0" bidirectional line)
				(alternate "CTED9" bidirectional line)
				(alternate "PMD3" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "RE4")
				(number "64")
				(alternate "CN62" bidirectional line)
				(alternate "CTED8" bidirectional line)
				(alternate "HLVDIN" bidirectional line)
				(alternate "PMD4" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "RE5")
				(number "1")
				(alternate "CN63" bidirectional line)
				(alternate "CTED4" bidirectional line)
				(alternate "LCDBIAS2" bidirectional line)
				(alternate "PMD5" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 2.54)
				(name "RE6")
				(number "2")
				(alternate "CN64" bidirectional line)
				(alternate "LCDBIAS1" bidirectional line)
				(alternate "PMD6" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "RE7")
				(number "3")
				(alternate "CN65" bidirectional line)
				(alternate "LCDBIAS0" bidirectional line)
				(alternate "PMD7" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "RF0")
				(number "58")
				(alternate "CN68" bidirectional line)
				(alternate "SEG27" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "RF1")
				(number "59")
				(alternate "CN69" bidirectional line)
				(alternate "COM4" bidirectional line)
				(alternate "SEG48" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "RF2")
				(number "34")
				(alternate "CN70" bidirectional line)
				(alternate "RP30" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "RF3")
				(number "33")
				(alternate "CN71" bidirectional line)
				(alternate "RP16" bidirectional line)
				(alternate "SEG12" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "RF4")
				(number "31")
				(alternate "CN17" bidirectional line)
				(alternate "PMA9" bidirectional line)
				(alternate "RP10" bidirectional line)
				(alternate "SDA2" bidirectional line)
				(alternate "SEG10" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "RF5")
				(number "32")
				(alternate "CN18" bidirectional line)
				(alternate "PMA8" bidirectional line)
				(alternate "RP17" bidirectional line)
				(alternate "SCL2" bidirectional line)
				(alternate "SEG11" bidirectional line)
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "RF6")
				(number "35")
				(alternate "CN84" bidirectional line)
				(alternate "INT0" bidirectional line)
			)
			(pin passive line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "VCAP/VDDCORE")
				(number "56")
			)
			(pin input line
				(at 20.32 -40.64 180)
				(length 2.54)
				(name "~{MCLR}")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC24FV32KA304-IPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -43.18 54.61 0)
		)
		(property "Value" "PIC24FV32KA304-IPT"
			(at -43.18 52.07 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 0 2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/39995d.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "32K Flash, 2048B SRAM, 512B EEPROM, nanoWatt XLP, 12-bit ADC, PWM, RTCC, TQFP44"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 16-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "PIC24FV32KA304-IPT_1_0")
		(symbol "PIC24FV32KA304-IPT_1_1"
			(pin bidirectional line
				(at -48.26 38.1 0)
				(length 5.08)
				(name "RA0/VREF+/CVREF+/AN0/C3INC/CN2")
				(number "19")
			)
			(pin bidirectional line
				(at -48.26 35.56 0)
				(length 5.08)
				(name "RA1/CVREF-/VREF-/AN1/CN3")
				(number "20")
			)
			(pin bidirectional line
				(at -48.26 33.02 0)
				(length 5.08)
				(name "RA2/OSCI/AN13/CLKI/CN30")
				(number "30")
			)
			(pin bidirectional line
				(at -48.26 30.48 0)
				(length 5.08)
				(name "RA3/OSCO/AN14/CLKO/CN29")
				(number "31")
			)
			(pin bidirectional line
				(at -48.26 27.94 0)
				(length 5.08)
				(name "RA4/SOSCO/SCLKI/U2CTS/CN0")
				(number "34")
			)
			(pin bidirectional line
				(at -48.26 25.4 0)
				(length 5.08)
				(name "RA5/~{MCLR}/Vpp")
				(number "18")
			)
			(pin bidirectional line
				(at -48.26 22.86 0)
				(length 5.08)
				(name "RA6/C2OUT/OC1/CTED1/INT2/CN8")
				(number "7")
			)
			(pin bidirectional line
				(at -48.26 20.32 0)
				(length 5.08)
				(name "RA7/IC1/CTED3/CN9")
				(number "6")
			)
			(pin bidirectional line
				(at -48.26 17.78 0)
				(length 5.08)
				(name "RA8/OCFB/CN33")
				(number "32")
			)
			(pin bidirectional line
				(at -48.26 15.24 0)
				(length 5.08)
				(name "RA9/~{SS2}/CN34")
				(number "35")
			)
			(pin bidirectional line
				(at -48.26 12.7 0)
				(length 5.08)
				(name "RA10/OC3/CN35")
				(number "12")
			)
			(pin bidirectional line
				(at -48.26 10.16 0)
				(length 5.08)
				(name "RA11/IC3/CTED8/CN36")
				(number "13")
			)
			(pin bidirectional line
				(at -48.26 0 0)
				(length 5.08)
				(name "RB0/PGED1/AN2/ULPWU/CTCMP/C1IND/C2INB/C3IND/U2TX/CN4")
				(number "21")
			)
			(pin bidirectional line
				(at -48.26 -2.54 0)
				(length 5.08)
				(name "RB1/PGEC1/AN3/C1INC/C2INA/U2RX/CTED12/CN5")
				(number "22")
			)
			(pin bidirectional line
				(at -48.26 -5.08 0)
				(length 5.08)
				(name "RB2/AN4/C1INB/C2IND/SDA2/T5CK/T4CK/CTED13/CN6")
				(number "23")
			)
			(pin bidirectional line
				(at -48.26 -7.62 0)
				(length 5.08)
				(name "RB3/AN5/C1INA/C2INC/SCL2/CN7")
				(number "24")
			)
			(pin bidirectional line
				(at -48.26 -10.16 0)
				(length 5.08)
				(name "RB4/SOSCI/AN15/~{U2RTS}/CN1")
				(number "33")
			)
			(pin bidirectional line
				(at -48.26 -12.7 0)
				(length 5.08)
				(name "RB5/PGED3/ASDA1*/CN27")
				(number "41")
			)
			(pin bidirectional line
				(at -48.26 -15.24 0)
				(length 5.08)
				(name "RB6/PGEC3/ASCL1*/CN24")
				(number "42")
			)
			(pin bidirectional line
				(at -48.26 -17.78 0)
				(length 5.08)
				(name "RB7/INT0/CN23")
				(number "43")
			)
			(pin bidirectional line
				(at -48.26 -20.32 0)
				(length 5.08)
				(name "RB8/SCL1/U1CTS/C3OUT/CTED10")
				(number "44")
			)
			(pin bidirectional line
				(at -48.26 -22.86 0)
				(length 5.08)
				(name "RB9/DA1/T1CK/~{U1RTS}/CTED4/CN21")
				(number "1")
			)
			(pin bidirectional line
				(at -48.26 -25.4 0)
				(length 5.08)
				(name "RB10/PGED2/SDI1/CTED11/CN16")
				(number "8")
			)
			(pin bidirectional line
				(at -48.26 -27.94 0)
				(length 5.08)
				(name "RB11/PGEC2/SCK1/CTED9/CN15")
				(number "9")
			)
			(pin bidirectional line
				(at -48.26 -30.48 0)
				(length 5.08)
				(name "RB12/N12/HLVDIN/CTED2/CN14")
				(number "10")
			)
			(pin bidirectional line
				(at -48.26 -33.02 0)
				(length 5.08)
				(name "RB13/AN11/SDO1/CTPLS/CN13")
				(number "11")
			)
			(pin bidirectional line
				(at -48.26 -35.56 0)
				(length 5.08)
				(name "RB14/CVREF/AN10/C3INB/RTCC/C1OUT/OCFA/CTED5/INT1/CN12")
				(number "14")
			)
			(pin bidirectional line
				(at -48.26 -38.1 0)
				(length 5.08)
				(name "RB15/AN9/C3INA/T3CK/T2CK/REFO/SS1/CTED6/CN11")
				(number "15")
			)
			(pin power_in line
				(at -5.08 55.88 270)
				(length 5.08)
				(name "Vdd")
				(number "28")
			)
			(pin power_in line
				(at -5.08 -55.88 90)
				(length 5.08)
				(name "Vss")
				(number "29")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "Vdd")
				(number "40")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "Vss")
				(number "39")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "AVdd/Vdd")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 5.08)
				(name "Vss/AVss")
				(number "16")
			)
			(pin bidirectional line
				(at 48.26 38.1 180)
				(length 5.08)
				(name "IC2/CTED7/CN19/RC9")
				(number "5")
			)
			(pin bidirectional line
				(at 48.26 35.56 180)
				(length 5.08)
				(name "OC2/CN20/RC8")
				(number "4")
			)
			(pin bidirectional line
				(at 48.26 33.02 180)
				(length 5.08)
				(name "U1TX/CN17/RC7")
				(number "3")
			)
			(pin bidirectional line
				(at 48.26 30.48 180)
				(length 5.08)
				(name "U1RX/CN18/RC6")
				(number "2")
			)
			(pin bidirectional line
				(at 48.26 27.94 180)
				(length 5.08)
				(name "SCK2/CN26/RC5")
				(number "38")
			)
			(pin bidirectional line
				(at 48.26 25.4 180)
				(length 5.08)
				(name "SDO2/CN25/RC4")
				(number "37")
			)
			(pin bidirectional line
				(at 48.26 22.86 180)
				(length 5.08)
				(name "SDI2/CN28/RC3")
				(number "36")
			)
			(pin bidirectional line
				(at 48.26 20.32 180)
				(length 5.08)
				(name "AN8/CN10/RC2")
				(number "27")
			)
			(pin bidirectional line
				(at 48.26 17.78 180)
				(length 5.08)
				(name "AN7/CN31/RC1")
				(number "26")
			)
			(pin bidirectional line
				(at 48.26 15.24 180)
				(length 5.08)
				(name "AN6/CN32/RC0")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC24FJ128GA306-xMR"
		(extends "PIC24FJ64GA306-xPT")
		(property "Reference" "U"
			(at -17.78 44.45 0)
		)
		(property "Value" "PIC24FJ128GA306-xMR"
			(at 1.27 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at -1.27 -5.08 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/30009996g.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "128K Flash, 8KB SRAM, LCD controller, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 16-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*EP7.15x7.15mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC24FJ128GA306-xPT"
		(extends "PIC24FJ64GA306-xPT")
		(property "Reference" "U"
			(at -17.78 44.45 0)
		)
		(property "Value" "PIC24FJ128GA306-xPT"
			(at 1.27 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at -1.27 -5.08 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/30009996g.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "128K Flash, 8KB SRAM, LCD controller, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 16-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC24FJ64GA306-xMR"
		(extends "PIC24FJ64GA306-xPT")
		(property "Reference" "U"
			(at -17.78 44.45 0)
		)
		(property "Value" "PIC24FJ64GA306-xMR"
			(at 1.27 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP7.15x7.15mm"
			(at -1.27 -5.08 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/OTH/ProductDocuments/DataSheets/30009996g.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "64K Flash, 8KB SRAM, LCD controller, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Flash-Based 16-Bit Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*EP7.15x7.15mm*"
			(at 0 0 0)
		)
	)
)
