(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "PIC32MK1024GPD100-xPT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 64.77 0)
		)
		(property "Value" "PIC32MK1024GPD100-xPT"
			(at 6.35 -67.31 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_12x12mm_P0.4mm"
			(at 0 -80.01 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC32MK_GP_MC_Familly_Datasheet_60001402G.pdf"
			(at 0 -76.2 0)
		)
		(property "Description" "MIPS MCU, 120MHz, 1MB Flash, 256KB RAM, 2.3-3.6V, USB, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit MIPS MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "PIC32MK1024GPD100-xPT_0_1")
		(symbol "PIC32MK1024GPD100-xPT_1_1"
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 3.81)
				(name "RA0")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 3.81)
				(name "RA1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 3.81)
				(name "RA4")
				(number "51")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 3.81)
				(name "RA7/TCK")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 3.81)
				(name "RA8/TDI")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 3.81)
				(name "RA10/TDO")
				(number "100")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 3.81)
				(name "RA11")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 3.81)
				(name "RA12")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 3.81)
				(name "RA14")
				(number "66")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 3.81)
				(name "RA15")
				(number "67")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 3.81)
				(name "RC0")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 3.81)
				(name "RC1")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "RC2")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "RC6")
				(number "77")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "RC7")
				(number "78")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RC8")
				(number "81")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RC9")
				(number "84")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RC10")
				(number "71")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "RC11")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "RC12/OSCI/CLKI")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 3.81)
				(name "RC13/SOSCI")
				(number "73")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RC15/OSCO/CLKO")
				(number "64")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RE0")
				(number "52")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RE1")
				(number "53")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RE8")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RE9")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RE12")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RE13")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "RE14")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "RE15")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "RG0")
				(number "90")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "RG1")
				(number "89")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "RG6/VBUSON2")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 3.81)
				(name "RG7")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 3.81)
				(name "RG8")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 3.81)
				(name "RG9")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 3.81)
				(name "RG10")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 3.81)
				(name "RG11")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 3.81)
				(name "RG12")
				(number "96")
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 3.81)
				(name "RG13/TRD0")
				(number "97")
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 3.81)
				(name "RG14/TRD2")
				(number "95")
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 3.81)
				(name "RG15")
				(number "1")
			)
			(pin input line
				(at -30.48 -58.42 0)
				(length 3.81)
				(name "VBUS1")
				(number "54")
			)
			(pin input line
				(at -30.48 -60.96 0)
				(length 3.81)
				(name "VBUS2")
				(number "58")
			)
			(pin power_in line
				(at -12.7 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -10.16 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -7.62 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "37")
			)
			(pin power_in line
				(at -5.08 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "46")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 -68.58 90)
				(length 3.81)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "36")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "45")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "65")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "75")
			)
			(pin passive line
				(at -2.54 -68.58 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "85")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "86")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 3.81)
				(name "VUSB3V3")
				(number "55")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 3.81)
				(name "AVSS")
				(number "31")
			)
			(pin power_in line
				(at 5.08 66.04 270)
				(length 3.81)
				(name "AVDD")
				(number "30")
			)
			(pin power_in line
				(at 10.16 66.04 270)
				(length 3.81)
				(name "VBAT")
				(number "68")
			)
			(pin input line
				(at 30.48 55.88 180)
				(length 3.81)
				(name "~{MCLR}")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 3.81)
				(name "PGD3/RB0")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 3.81)
				(name "PGC3/RB1")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 3.81)
				(name "PGC1/RB2")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 3.81)
				(name "PGD1/RB3")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 3.81)
				(name "RB4")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 3.81)
				(name "PGD2/RB5")
				(number "69")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 3.81)
				(name "PGC2/RB6")
				(number "70")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 3.81)
				(name "RB7")
				(number "72")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "SOSCO/RB8")
				(number "74")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 3.81)
				(name "TMS/RB9")
				(number "76")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "RB10")
				(number "93")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "RB11")
				(number "94")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "RB12")
				(number "98")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "RB13")
				(number "99")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "RB14/VBUSON1")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "RB15")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "RD1")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "RD2")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "RD3")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "RD4")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "RD5")
				(number "82")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "RD6")
				(number "83")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "RD12")
				(number "79")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "RD13")
				(number "80")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "RD14")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "RD15")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "RF0")
				(number "87")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "RF1")
				(number "88")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "RF5")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "TRCLK/RF6")
				(number "91")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 3.81)
				(name "TRD3/RF7")
				(number "92")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 3.81)
				(name "RF9")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 3.81)
				(name "RF10")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 3.81)
				(name "RF12")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 3.81)
				(name "RF13")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 3.81)
				(name "D1-")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 3.81)
				(name "D1+")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 3.81)
				(name "D2-")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 3.81)
				(name "D2+")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC32MM0064GPL028x-ML"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 26.67 0)
		)
		(property "Value" "PIC32MM0064GPL028x-ML"
			(at 16.51 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-28-1EP_6x6mm_P0.65mm_EP4.25x4.25mm"
			(at 2.54 -27.94 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC32MM0064GPL036-Family-Data-Sheet-DS60001324C.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "32-Bit Flash MCU, 25MHz, 64KB Flash, 8KB RAM, QFN-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "FLASH-Based 32-Bit CMOS Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*6x6mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "PIC32MM0064GPL028x-ML_0_0"
			(pin input line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "~{MCLR}")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "RA0")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "RA1")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "RA2")
				(number "6")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "RA3")
				(number "7")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "RA4")
				(number "9")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "RC9")
				(number "16")
			)
			(pin power_out line
				(at -5.08 22.86 270)
				(length 2.54)
				(name "VCAP")
				(number "17")
			)
			(pin passive line
				(at -2.54 -25.4 90)
				(length 2.54)
				(name "EP")
				(number "29")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 2.54)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "AVDD")
				(number "25")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "AVSS")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "RBO")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "RB1")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "RB2")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "RB3")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "RB4")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "RB6")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "RB7")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "RB8")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "RB9")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "RB10")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "RB11")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "RB12")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "RB13")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "RB14")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "RB15")
				(number "23")
			)
		)
		(symbol "PIC32MM0064GPL028x-ML_0_1")
		(embedded_fonts no)
	)
	(symbol "PIC32MX110F016D-IPT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 34.29 0)
		)
		(property "Value" "PIC32MX110F016D-IPT"
			(at 26.67 31.75 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 3.81 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001168F.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "32-bit Microcontrollers (16KB Flash and 4KB SRAM TQFP-44) with Audio and Graphics Interfaces, USB, and Advanced Analog"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip PIC32 Microcontroller MIPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "PIC32MX110F016D-IPT_0_1")
		(symbol "PIC32MX110F016D-IPT_1_1"
			(pin input line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "RB0")
				(number "21")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "RB1")
				(number "22")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "RB2")
				(number "23")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "RB3")
				(number "24")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "RB4")
				(number "33")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "RB5")
				(number "41")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "RB6")
				(number "42")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "RB7")
				(number "43")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "RB8")
				(number "44")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "RB9")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "RB10")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "RB11")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "RB12")
				(number "10")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "RB13")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "RB14")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "RB15")
				(number "15")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "~{MCLR}")
				(number "18")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 5.08)
				(name "VCAP")
				(number "7")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "40")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "29")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 5.08)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 5.08)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 5.08)
				(name "AVSS")
				(number "16")
			)
			(pin input line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "RA0")
				(number "19")
			)
			(pin input line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "RA1")
				(number "20")
			)
			(pin input line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "RA2")
				(number "30")
			)
			(pin input line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "RA3")
				(number "31")
			)
			(pin input line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "RA4")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "RA7")
				(number "13")
			)
			(pin input line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "RA8")
				(number "32")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "RA9")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "RA10")
				(number "12")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "RC0")
				(number "25")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "RC1")
				(number "26")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "RC2")
				(number "27")
			)
			(pin input line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "RC3")
				(number "36")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "RC4")
				(number "37")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "RC5")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "RC6")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "RC7")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "RC8")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "RC9")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC32MX210F016D-IPT"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 34.29 0)
		)
		(property "Value" "PIC32MX210F016D-IPT"
			(at 26.67 31.75 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 3.81 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001168F.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "32-bit Microcontrollers (16KB Flash and 4KB SRAM TQFP-44) with Audio and Graphics Interfaces, USB, and Advanced Analog"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip PIC32 Microcontroller MIPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "PIC32MX210F016D-IPT_0_1")
		(symbol "PIC32MX210F016D-IPT_1_1"
			(pin input line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "RB0")
				(number "21")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "RB1")
				(number "22")
			)
			(pin input line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "RB2")
				(number "23")
			)
			(pin input line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "RB3")
				(number "24")
			)
			(pin input line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "RB4")
				(number "33")
			)
			(pin input line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "RB5")
				(number "41")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "RB7")
				(number "43")
			)
			(pin input line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "RB8")
				(number "44")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "RB9")
				(number "1")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "RB10")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "RB11")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "RB13")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 5.08)
				(name "RB14")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 5.08)
				(name "RB15")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "VUSB3V3")
				(number "10")
			)
			(pin input line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "~{MCLR}")
				(number "18")
			)
			(pin input line
				(at -20.32 -22.86 0)
				(length 5.08)
				(name "VBUS")
				(number "42")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 5.08)
				(name "VCAP")
				(number "7")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 5.08)
				(name "VDD")
				(number "28")
			)
			(pin passive line
				(at -2.54 35.56 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "40")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "29")
			)
			(pin passive line
				(at -2.54 -35.56 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 5.08)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 5.08)
				(name "AVDD")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 5.08)
				(name "AVSS")
				(number "16")
			)
			(pin input line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "RA0")
				(number "19")
			)
			(pin input line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "RA1")
				(number "20")
			)
			(pin input line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "RA2")
				(number "30")
			)
			(pin input line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "RA3")
				(number "31")
			)
			(pin input line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "RA4")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "RA7")
				(number "13")
			)
			(pin input line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "RA8")
				(number "32")
			)
			(pin input line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "RA9")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "RA10")
				(number "12")
			)
			(pin input line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "RC0")
				(number "25")
			)
			(pin input line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "RC1")
				(number "26")
			)
			(pin input line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "RC2")
				(number "27")
			)
			(pin input line
				(at 20.32 -10.16 180)
				(length 5.08)
				(name "RC3")
				(number "36")
			)
			(pin input line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "RC4")
				(number "37")
			)
			(pin input line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "RC5")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "RC6")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "RC7")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "RC8")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 5.08)
				(name "RC9")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC32MX575F256H"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 6.35 50.8 0)
		)
		(property "Value" "PIC32MX575F256H"
			(at 21.59 48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/61156G.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit Microcontrollers (64KB Flash and 16KB SRAM TQFP-64 QFN-64) USB, CAN and Ethernet"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip PIC32 Microcontroller MIPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Package*QFP:QFP*10x10mm*P0.5mm* Package*DFN*QFN:QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC32MX575F256H_0_1")
		(symbol "PIC32MX575F256H_1_1"
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 5.08)
				(name "RB0")
				(number "16")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 5.08)
				(name "RB1")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 5.08)
				(name "RB2")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 5.08)
				(name "RB3")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 5.08)
				(name "RB4")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 5.08)
				(name "RB5")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 5.08)
				(name "RB6")
				(number "17")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 5.08)
				(name "RB7")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 5.08)
				(name "RB8")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 5.08)
				(name "RB9")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 5.08)
				(name "RB10")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 5.08)
				(name "RB11")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 5.08)
				(name "RB12")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "RB13")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "RB14")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "RB15")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "RC12")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "RC13")
				(number "47")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "RC14")
				(number "48")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "RC15")
				(number "40")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 5.08)
				(name "~{MCLR}")
				(number "7")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 5.08)
				(name "VBUS")
				(number "34")
			)
			(pin power_in line
				(at -20.32 -20.32 0)
				(length 5.08)
				(name "VUSB")
				(number "35")
			)
			(pin power_out line
				(at -5.08 50.8 270)
				(length 5.08)
				(name "VCAP")
				(number "56")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 5.08)
				(name "AVDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 5.08)
				(name "AVSS")
				(number "20")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 5.08)
				(name "VDD")
				(number "10")
			)
			(pin passive line
				(at 2.54 50.8 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "26")
			)
			(pin passive line
				(at 2.54 50.8 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "38")
			)
			(pin passive line
				(at 2.54 50.8 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "57")
			)
			(pin passive line
				(at 2.54 -50.8 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "25")
			)
			(pin passive line
				(at 2.54 -50.8 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "41")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 5.08)
				(name "VSS")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 5.08)
				(name "RD0")
				(number "46")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 5.08)
				(name "RD1")
				(number "49")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 5.08)
				(name "RD2")
				(number "50")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 5.08)
				(name "RD3")
				(number "51")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 5.08)
				(name "RD4")
				(number "52")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 5.08)
				(name "RD5")
				(number "53")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 5.08)
				(name "RD6")
				(number "54")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 5.08)
				(name "RD7")
				(number "55")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 5.08)
				(name "RD8")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 5.08)
				(name "RD9")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 5.08)
				(name "RD10")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 5.08)
				(name "RD11")
				(number "45")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "RE0")
				(number "60")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "RE1")
				(number "61")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "RE2")
				(number "62")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "RE3")
				(number "63")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "RE4")
				(number "64")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "RE5")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "RE6")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "RE7")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 5.08)
				(name "RF0")
				(number "58")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 5.08)
				(name "RF1")
				(number "59")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 5.08)
				(name "RF3")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 5.08)
				(name "RF4")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 5.08)
				(name "RF5")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 5.08)
				(name "RG2")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 5.08)
				(name "RG3")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 5.08)
				(name "RG6")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 5.08)
				(name "RG7")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 5.08)
				(name "RG8")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 5.08)
				(name "RG9")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC32MX795F512L-80x-PF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 64.77 0)
		)
		(property "Value" "PIC32MX795F512L-80x-PF"
			(at 6.35 -64.77 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 -76.2 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001156J.pdf"
			(at 0 -76.2 0)
		)
		(property "Description" "MIPS MCU, 80MHz, 512KB Flash, 12KB Boot Flash, 128KB RAM, 2.3-3.6V, USB, CAN, Ethernet, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit MIPS MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "PIC32MX795F512L-80x-PF_0_1")
		(symbol "PIC32MX795F512L-80x-PF_1_1"
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 3.81)
				(name "RA0/TMS")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 3.81)
				(name "RA1/TCK")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 3.81)
				(name "RA2")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 3.81)
				(name "RA3")
				(number "59")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 3.81)
				(name "RA4/TDI")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 3.81)
				(name "RA5/TDO")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 3.81)
				(name "RA6/TRCLK")
				(number "91")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 3.81)
				(name "RA7/TRD3")
				(number "92")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 3.81)
				(name "RA9")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 3.81)
				(name "RA10")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 3.81)
				(name "RA14")
				(number "66")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 3.81)
				(name "RA15")
				(number "67")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "RC1")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "RC2")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "RC3")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RC4")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RC12/OSC1/CLK")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RC13/SOSCI")
				(number "73")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "RC14/SOSCO")
				(number "74")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "RC15/OSC2/CLKO")
				(number "64")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RE0")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "RE1")
				(number "94")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RE2")
				(number "98")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RE3")
				(number "99")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RE4")
				(number "100")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RE5")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RE6")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RE7")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "RE8")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "RE9")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "RG0")
				(number "90")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "RG1")
				(number "89")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "RG2/D+")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 3.81)
				(name "RG3/D-")
				(number "56")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 3.81)
				(name "RG6")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 3.81)
				(name "RG7")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 3.81)
				(name "RG8")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 3.81)
				(name "RG9")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 3.81)
				(name "RG12/TRD1")
				(number "96")
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 3.81)
				(name "RG13/TRD0")
				(number "97")
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 3.81)
				(name "RG14/TRD2")
				(number "95")
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 3.81)
				(name "RG15")
				(number "1")
			)
			(pin input line
				(at -30.48 -58.42 0)
				(length 3.81)
				(name "VBUS")
				(number "54")
			)
			(pin power_in line
				(at -12.7 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -10.16 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -7.62 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "37")
			)
			(pin power_in line
				(at -5.08 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "46")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 3.81)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "36")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "45")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "65")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "75")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "86")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 3.81)
				(name "VUSB3V3")
				(number "55")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 3.81)
				(name "AVSS")
				(number "31")
			)
			(pin power_in line
				(at 5.08 66.04 270)
				(length 3.81)
				(name "AVDD")
				(number "30")
			)
			(pin power_out line
				(at 10.16 66.04 270)
				(length 3.81)
				(name "VCAP/VDDCORE")
				(number "85")
			)
			(pin input line
				(at 30.48 55.88 180)
				(length 3.81)
				(name "~{MCLR}")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 3.81)
				(name "PGED1/RB0")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 3.81)
				(name "PGEC1/RB1")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 3.81)
				(name "RB3")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 3.81)
				(name "RB4")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 3.81)
				(name "RB5")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 3.81)
				(name "PGEC2/RB6")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 3.81)
				(name "PGED2/RB7")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "RB8")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 3.81)
				(name "RB9")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "RB10")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "RB11")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "RB12")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "RB13")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "RB14")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "RB15")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "RD0")
				(number "72")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "RD1")
				(number "76")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "RD2")
				(number "77")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "RD3")
				(number "78")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "RD4")
				(number "81")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "RD5")
				(number "82")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "RD6")
				(number "83")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "RD7")
				(number "84")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "RD8")
				(number "68")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "RD9")
				(number "69")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 3.81)
				(name "RD10")
				(number "70")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "RD11")
				(number "71")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "RD12")
				(number "79")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "RD13")
				(number "80")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "RD14")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 3.81)
				(name "RD15")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 3.81)
				(name "RF0")
				(number "87")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 3.81)
				(name "RF1")
				(number "88")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 3.81)
				(name "RF2")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 3.81)
				(name "RF3")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 3.81)
				(name "RF4")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 3.81)
				(name "RF5")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 3.81)
				(name "RF8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 3.81)
				(name "RF12")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 3.81)
				(name "RF13")
				(number "39")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC32MX795F512L-80x-PT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 64.77 0)
		)
		(property "Value" "PIC32MX795F512L-80x-PT"
			(at 5.08 -63.5 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_12x12mm_P0.4mm"
			(at 0 -76.2 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001156J.pdf"
			(at 214.63 -71.12 0)
		)
		(property "Description" "MIPS MCU, 80MHz, 512KB Flash, 12KB Boot Flash, 128KB RAM, 2.3-3.6V, USB, CAN, Ethernet, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit MIPS MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "PIC32MX795F512L-80x-PT_1_1"
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 3.81)
				(name "RA0/TMS")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 3.81)
				(name "RA1//TCK")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 3.81)
				(name "RA2")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 3.81)
				(name "RA3")
				(number "59")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 3.81)
				(name "RA4/TDI")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 3.81)
				(name "RA5/TDO")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 3.81)
				(name "RA6/TRCLK")
				(number "91")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 3.81)
				(name "RA7/TRD3")
				(number "92")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 3.81)
				(name "RA9")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 3.81)
				(name "RA10")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 3.81)
				(name "RA14")
				(number "66")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 3.81)
				(name "RA15")
				(number "67")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 3.81)
				(name "RC1")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 3.81)
				(name "RC2")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 3.81)
				(name "RC3")
				(number "8")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 3.81)
				(name "RC4")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 3.81)
				(name "RC12/OSC1/CLK")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 3.81)
				(name "RC13/SOSCI")
				(number "73")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 3.81)
				(name "RC14/SOSCO")
				(number "74")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 3.81)
				(name "RC15/OSC2/CLKO")
				(number "64")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 3.81)
				(name "RE0")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 3.81)
				(name "RE1")
				(number "94")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 3.81)
				(name "RE2")
				(number "98")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 3.81)
				(name "RE3")
				(number "99")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 3.81)
				(name "RE4")
				(number "100")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 3.81)
				(name "RE5")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 3.81)
				(name "RE6")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 3.81)
				(name "RE7")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 3.81)
				(name "RE8")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 3.81)
				(name "RE9")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 3.81)
				(name "RG0")
				(number "90")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 3.81)
				(name "RG1")
				(number "89")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 3.81)
				(name "RG2/D+")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 3.81)
				(name "RG3/D-")
				(number "56")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 3.81)
				(name "RG6")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 3.81)
				(name "RG7")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 3.81)
				(name "RG8")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 3.81)
				(name "RG9")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 3.81)
				(name "RG12/TRD1")
				(number "96")
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 3.81)
				(name "RG13/TRD0")
				(number "97")
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 3.81)
				(name "RG14/TRD2")
				(number "95")
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 3.81)
				(name "RG15")
				(number "1")
			)
			(pin input line
				(at -30.48 -58.42 0)
				(length 3.81)
				(name "VBUS")
				(number "54")
			)
			(pin power_in line
				(at -12.7 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -10.16 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -7.62 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "37")
			)
			(pin power_in line
				(at -5.08 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "46")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 3.81)
				(name "VSS")
				(number "15")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "36")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "45")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "65")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 3.81)
				(hide yes)
				(name "VSS")
				(number "75")
			)
			(pin power_in line
				(at 0 66.04 270)
				(length 3.81)
				(name "VDD")
				(number "86")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 3.81)
				(name "VUSB3V3")
				(number "55")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 3.81)
				(name "AVSS")
				(number "31")
			)
			(pin power_in line
				(at 5.08 66.04 270)
				(length 3.81)
				(name "AVDD")
				(number "30")
			)
			(pin power_out line
				(at 10.16 66.04 270)
				(length 3.81)
				(name "VCAP/VDDCORE")
				(number "85")
			)
			(pin input line
				(at 30.48 55.88 180)
				(length 3.81)
				(name "~{MCLR}")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 3.81)
				(name "PGED1/RB0")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 3.81)
				(name "PGEC1/RB1")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 3.81)
				(name "RB2")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 3.81)
				(name "RB3")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 3.81)
				(name "RB4")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 3.81)
				(name "RB5")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 3.81)
				(name "PGEC2/RB6")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 3.81)
				(name "PGED2/RB7")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 3.81)
				(name "RB8")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 3.81)
				(name "RB9")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 3.81)
				(name "RB10")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 3.81)
				(name "RB11")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 3.81)
				(name "RB12")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 3.81)
				(name "RB13")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 3.81)
				(name "RB14")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 3.81)
				(name "RB15")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 3.81)
				(name "RD0")
				(number "72")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 3.81)
				(name "RD1")
				(number "76")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 3.81)
				(name "RD2")
				(number "77")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 3.81)
				(name "RD3")
				(number "78")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 3.81)
				(name "RD4")
				(number "81")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 3.81)
				(name "RD5")
				(number "82")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 3.81)
				(name "RD6")
				(number "83")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 3.81)
				(name "RD7")
				(number "84")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 3.81)
				(name "RD8")
				(number "68")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 3.81)
				(name "RD9")
				(number "69")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 3.81)
				(name "RD10")
				(number "70")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 3.81)
				(name "RD11")
				(number "71")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 3.81)
				(name "RD12")
				(number "79")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 3.81)
				(name "RD13")
				(number "80")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 3.81)
				(name "RD14")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 3.81)
				(name "RD15")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 3.81)
				(name "RF0")
				(number "87")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 3.81)
				(name "RF1")
				(number "88")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 3.81)
				(name "RF2")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 3.81)
				(name "RF3")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 3.81)
				(name "RF4")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 3.81)
				(name "RF5")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 3.81)
				(name "RF8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 3.81)
				(name "RF12")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 3.81)
				(name "RF13")
				(number "39")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PIC32MK1024GPE100-xPT"
		(extends "PIC32MK1024GPD100-xPT")
		(property "Reference" "U"
			(at -19.05 64.77 0)
		)
		(property "Value" "PIC32MK1024GPE100-xPT"
			(at 6.35 -67.31 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_12x12mm_P0.4mm"
			(at 0 -80.01 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/PIC32MK_GP_MC_Familly_Datasheet_60001402G.pdf"
			(at 0 -76.2 0)
		)
		(property "Description" "MIPS MCU, 120MHz, 1MB Flash, 256KB RAM, 2.3-3.6V, USB, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit MIPS MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*12x12mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC32MX120F032D-IPT"
		(extends "PIC32MX110F016D-IPT")
		(property "Reference" "U"
			(at 6.35 34.29 0)
		)
		(property "Value" "PIC32MX120F032D-IPT"
			(at 26.67 31.75 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 3.81 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001168F.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "32-bit Microcontrollers (32KB Flash and 8KB SRAM TQFP-44) with Audio and Graphics Interfaces, USB, and Advanced Analog"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip PIC32 Microcontroller MIPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC32MX130F064D-IPT"
		(extends "PIC32MX110F016D-IPT")
		(property "Reference" "U"
			(at 6.35 34.29 0)
		)
		(property "Value" "PIC32MX130F064D-IPT"
			(at 26.67 31.75 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 3.81 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001168F.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "32-bit Microcontrollers (64KB Flash and 16KB SRAM TQFP-44) with Audio and Graphics Interfaces, USB, and Advanced Analog"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip PIC32 Microcontroller MIPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC32MX150F128D-IPT"
		(extends "PIC32MX110F016D-IPT")
		(property "Reference" "U"
			(at 6.35 34.29 0)
		)
		(property "Value" "PIC32MX150F128D-IPT"
			(at 26.67 31.75 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 3.81 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001168F.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "32-bit Microcontrollers (128KB Flash and 32KB SRAM TQFP-44) with Audio and Graphics Interfaces, USB, and Advanced Analog"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip PIC32 Microcontroller MIPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC32MX170F256D-IPT"
		(extends "PIC32MX110F016D-IPT")
		(property "Reference" "U"
			(at 6.35 34.29 0)
		)
		(property "Value" "PIC32MX170F256D-IPT"
			(at 26.67 31.75 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 3.81 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001168F.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "32-bit Microcontrollers (256KB Flash and 64KB SRAM TQFP-44) with Audio and Graphics Interfaces, USB, and Advanced Analog"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip PIC32 Microcontroller MIPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC32MX220F032D-IPT"
		(extends "PIC32MX210F016D-IPT")
		(property "Reference" "U"
			(at 6.35 34.29 0)
		)
		(property "Value" "PIC32MX220F032D-IPT"
			(at 26.67 31.75 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 3.81 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001168F.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "32-bit Microcontrollers (32KB Flash and 8KB SRAM TQFP-44) with Audio and Graphics Interfaces, USB, and Advanced Analog"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip PIC32 Microcontroller MIPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC32MX230F064D-IPT"
		(extends "PIC32MX210F016D-IPT")
		(property "Reference" "U"
			(at 6.35 34.29 0)
		)
		(property "Value" "PIC32MX230F064D-IPT"
			(at 26.67 31.75 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 3.81 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001168F.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "32-bit Microcontrollers (64KB Flash and 16KB SRAM TQFP-44) with Audio and Graphics Interfaces, USB, and Advanced Analog"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip PIC32 Microcontroller MIPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC32MX250F128D-IPT"
		(extends "PIC32MX210F016D-IPT")
		(property "Reference" "U"
			(at 6.35 34.29 0)
		)
		(property "Value" "PIC32MX250F128D-IPT"
			(at 26.67 31.75 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 3.81 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001168F.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "32-bit Microcontrollers (128KB Flash and 32KB SRAM TQFP-44) with Audio and Graphics Interfaces, USB, and Advanced Analog"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip PIC32 Microcontroller MIPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC32MX270F256D-IPT"
		(extends "PIC32MX210F016D-IPT")
		(property "Reference" "U"
			(at 6.35 34.29 0)
		)
		(property "Value" "PIC32MX270F256D-IPT"
			(at 26.67 31.75 0)
		)
		(property "Footprint" "Package_QFP:TQFP-44_10x10mm_P0.8mm"
			(at 3.81 36.83 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001168F.pdf"
			(at 0 -5.08 0)
		)
		(property "Description" "32-bit Microcontrollers (256KB Flash and 64KB SRAM TQFP-44) with Audio and Graphics Interfaces, USB, and Advanced Analog"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip PIC32 Microcontroller MIPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "PIC32MX575F512H"
		(extends "PIC32MX575F256H")
		(property "Reference" "U"
			(at 6.35 50.8 0)
		)
		(property "Value" "PIC32MX575F512H"
			(at 21.59 48.26 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/61156G.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit Microcontrollers (64KB Flash and 16KB SRAM TQFP-64 QFN-64) USB, CAN and Ethernet"
			(at 0 0 0)
		)
		(property "ki_keywords" "Microchip PIC32 Microcontroller MIPS"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Package*QFP:QFP*10x10mm*P0.5mm* Package*DFN*QFN:QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
