(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ATSAMA5D21"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 63.5 0)
		)
		(property "Value" "ATSAMA5D21"
			(at 0 60.96 0)
		)
		(property "Footprint" "Package_BGA:Microchip_TFBGA-196_11x11mm_Layout14x14_P0.75mm_SMD"
			(at 0 -2.54 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAMA5D2-Series-Data-Sheet-DS60001476C.pdf"
			(at -11.43 22.86 0)
		)
		(property "Description" "ARM Cortex-A5 MPU, 500 MHz max, 1x SDIO/SD-CARD/eMMC/QSPI memory, 128 kB SRAM, 16-bit bus DDR2/DDR3 RAM, 1.1-1.32 V, 72 GPIO, TFBGA-196"
			(at 0 0 0)
		)
		(property "ki_locked" ""
			(at 0 0 0)
		)
		(property "ki_keywords" "MPU Cortex-A5 Cortex A5 Linux DDR DRAM BGA"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Microchip*TFBGA*11x11mm*P0.75mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMA5D21_1_1"
			(pin bidirectional line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "PA18")
				(number "L9")
			)
			(pin bidirectional line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "PA19")
				(number "N9")
			)
			(pin bidirectional line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "PA20")
				(number "M9")
			)
			(pin bidirectional line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "PA21")
				(number "M10")
			)
			(pin bidirectional line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "PA22")
				(number "P9")
			)
			(pin bidirectional line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "PA23")
				(number "P10")
			)
			(pin bidirectional line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "PA24")
				(number "N10")
			)
			(pin bidirectional line
				(at 5.08 0 180)
				(length 3.81)
				(name "PA25")
				(number "L10")
			)
			(pin bidirectional line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "PA26")
				(number "P11")
			)
			(pin bidirectional line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "PA27")
				(number "P12")
			)
			(pin bidirectional line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "PA28")
				(number "M11")
			)
			(pin bidirectional line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "PA29")
				(number "N11")
			)
			(pin bidirectional line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "PA30")
				(number "N12")
			)
			(pin bidirectional line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "PA31")
				(number "M12")
			)
		)
		(symbol "ATSAMA5D21_2_1"
			(pin bidirectional line
				(at 5.08 40.64 180)
				(length 3.81)
				(name "PB0")
				(number "A6")
			)
			(pin bidirectional line
				(at 5.08 38.1 180)
				(length 3.81)
				(name "PB1")
				(number "A5")
			)
			(pin bidirectional line
				(at 5.08 35.56 180)
				(length 3.81)
				(name "PB2")
				(number "B6")
			)
			(pin bidirectional line
				(at 5.08 33.02 180)
				(length 3.81)
				(name "PB3")
				(number "B5")
			)
			(pin bidirectional line
				(at 5.08 30.48 180)
				(length 3.81)
				(name "PB4")
				(number "A4")
			)
			(pin bidirectional line
				(at 5.08 27.94 180)
				(length 3.81)
				(name "PB5")
				(number "D6")
			)
			(pin bidirectional line
				(at 5.08 25.4 180)
				(length 3.81)
				(name "PB6")
				(number "A3")
			)
			(pin bidirectional line
				(at 5.08 22.86 180)
				(length 3.81)
				(name "PB7")
				(number "B4")
			)
			(pin bidirectional line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "PB8")
				(number "A2")
			)
			(pin bidirectional line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "PB9")
				(number "B3")
			)
			(pin bidirectional line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "PB10")
				(number "A1")
			)
			(pin bidirectional line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "PB11")
				(number "B1")
			)
			(pin bidirectional line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "PB12")
				(number "B2")
			)
			(pin bidirectional line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "PB13")
				(number "C1")
			)
			(pin bidirectional line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "PB14")
				(number "D5")
			)
			(pin bidirectional line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "PB15")
				(number "E5")
			)
			(pin bidirectional line
				(at 5.08 0 180)
				(length 3.81)
				(name "PB16")
				(number "C5")
			)
			(pin bidirectional line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "PB17")
				(number "C2")
			)
			(pin bidirectional line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "PB18")
				(number "D4")
			)
			(pin bidirectional line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "PB19")
				(number "C4")
			)
			(pin bidirectional line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "PB20")
				(number "C3")
			)
			(pin bidirectional line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "PB21")
				(number "D1")
			)
			(pin bidirectional line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "PB22")
				(number "D2")
			)
			(pin bidirectional line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "PB23")
				(number "E1")
			)
			(pin bidirectional line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "PB24")
				(number "D3")
			)
			(pin bidirectional line
				(at 5.08 -22.86 180)
				(length 3.81)
				(name "PB25")
				(number "E3")
			)
			(pin bidirectional line
				(at 5.08 -25.4 180)
				(length 3.81)
				(name "PB26")
				(number "E2")
			)
			(pin bidirectional line
				(at 5.08 -27.94 180)
				(length 3.81)
				(name "PB27")
				(number "E6")
			)
			(pin bidirectional line
				(at 5.08 -30.48 180)
				(length 3.81)
				(name "PB28")
				(number "F1")
			)
			(pin bidirectional line
				(at 5.08 -33.02 180)
				(length 3.81)
				(name "PB29")
				(number "F6")
			)
			(pin bidirectional line
				(at 5.08 -35.56 180)
				(length 3.81)
				(name "PB30")
				(number "F2")
			)
			(pin bidirectional line
				(at 5.08 -38.1 180)
				(length 3.81)
				(name "PB31")
				(number "F7")
			)
		)
		(symbol "ATSAMA5D21_3_1"
			(pin bidirectional line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "PC0")
				(number "M13")
			)
			(pin bidirectional line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "PC1")
				(number "P13")
			)
			(pin bidirectional line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "PC2")
				(number "N13")
			)
			(pin bidirectional line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "PC3")
				(number "K10")
			)
			(pin bidirectional line
				(at 5.08 0 180)
				(length 3.81)
				(name "PC4")
				(number "P14")
			)
			(pin bidirectional line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "PC5")
				(number "J8")
			)
			(pin bidirectional line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "PC6")
				(number "N14")
			)
			(pin bidirectional line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "PC7")
				(number "M14")
			)
			(pin bidirectional line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "PC8")
				(number "J9")
			)
		)
		(symbol "ATSAMA5D21_4_1"
			(pin bidirectional line
				(at 5.08 20.32 180)
				(length 3.81)
				(name "PD7")
				(number "F5")
			)
			(pin bidirectional line
				(at 5.08 17.78 180)
				(length 3.81)
				(name "PD8")
				(number "F3")
			)
			(pin bidirectional line
				(at 5.08 15.24 180)
				(length 3.81)
				(name "PD9")
				(number "G5")
			)
			(pin bidirectional line
				(at 5.08 12.7 180)
				(length 3.81)
				(name "PD10")
				(number "G4")
			)
			(pin bidirectional line
				(at 5.08 10.16 180)
				(length 3.81)
				(name "PD11")
				(number "H1")
			)
			(pin bidirectional line
				(at 5.08 7.62 180)
				(length 3.81)
				(name "PD12")
				(number "H6")
			)
			(pin bidirectional line
				(at 5.08 5.08 180)
				(length 3.81)
				(name "PD13")
				(number "H3")
			)
			(pin bidirectional line
				(at 5.08 2.54 180)
				(length 3.81)
				(name "PD14")
				(number "G6")
			)
			(pin bidirectional line
				(at 5.08 0 180)
				(length 3.81)
				(name "PD15")
				(number "H5")
			)
			(pin bidirectional line
				(at 5.08 -2.54 180)
				(length 3.81)
				(name "PD16")
				(number "G1")
			)
			(pin bidirectional line
				(at 5.08 -5.08 180)
				(length 3.81)
				(name "PD17")
				(number "G2")
			)
			(pin bidirectional line
				(at 5.08 -7.62 180)
				(length 3.81)
				(name "PD18")
				(number "G3")
			)
			(pin bidirectional line
				(at 5.08 -10.16 180)
				(length 3.81)
				(name "PD19")
				(number "H4")
			)
			(pin bidirectional line
				(at 5.08 -12.7 180)
				(length 3.81)
				(name "PD20")
				(number "J1")
			)
			(pin bidirectional line
				(at 5.08 -15.24 180)
				(length 3.81)
				(name "PD21")
				(number "K1")
			)
			(pin bidirectional line
				(at 5.08 -17.78 180)
				(length 3.81)
				(name "PD22")
				(number "J3")
			)
			(pin bidirectional line
				(at 5.08 -20.32 180)
				(length 3.81)
				(name "PD23")
				(number "K2")
			)
		)
		(symbol "ATSAMA5D21_5_1"
			(pin power_in line
				(at -10.16 15.24 270)
				(length 3.81)
				(name "VDDCORE")
				(number "E8")
			)
			(pin passive line
				(at -10.16 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDDCORE")
				(number "G8")
			)
			(pin passive line
				(at -10.16 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDDCORE")
				(number "H8")
			)
			(pin passive line
				(at -10.16 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDDCORE")
				(number "H9")
			)
			(pin passive line
				(at -10.16 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDDCORE")
				(number "J5")
			)
			(pin power_in line
				(at -10.16 -12.7 90)
				(length 3.81)
				(name "GNDCORE")
				(number "F8")
			)
			(pin passive line
				(at -10.16 -12.7 90)
				(length 3.81)
				(hide yes)
				(name "GNDCORE")
				(number "G7")
			)
			(pin passive line
				(at -10.16 -12.7 90)
				(length 3.81)
				(hide yes)
				(name "GNDCORE")
				(number "G9")
			)
			(pin passive line
				(at -10.16 -12.7 90)
				(length 3.81)
				(hide yes)
				(name "GNDCORE")
				(number "H7")
			)
			(pin passive line
				(at -10.16 -12.7 90)
				(length 3.81)
				(hide yes)
				(name "GNDCORE")
				(number "J4")
			)
			(pin power_in line
				(at -7.62 15.24 270)
				(length 3.81)
				(name "VDDIOP0")
				(number "D7")
			)
			(pin passive line
				(at -7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDDIOP0")
				(number "F4")
			)
			(pin power_in line
				(at -7.62 -12.7 90)
				(length 3.81)
				(name "GNDIOP0")
				(number "E4")
			)
			(pin passive line
				(at -7.62 -12.7 90)
				(length 3.81)
				(hide yes)
				(name "GNDIOP0")
				(number "E7")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 3.81)
				(name "VDDIOP1")
				(number "K8")
			)
			(pin passive line
				(at -5.08 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDDIOP1")
				(number "L11")
			)
			(pin power_in line
				(at -5.08 -12.7 90)
				(length 3.81)
				(name "GNDIOP1")
				(number "K9")
			)
			(pin passive line
				(at -5.08 -12.7 90)
				(length 3.81)
				(hide yes)
				(name "GNDIOP1")
				(number "L12")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDDPLLA")
				(number "P3")
			)
			(pin power_in line
				(at 0 -12.7 90)
				(length 3.81)
				(name "GNDPLLA")
				(number "P4")
			)
			(pin power_in line
				(at 2.54 -12.7 90)
				(length 3.81)
				(name "GNDDPLL")
				(number "L6")
			)
			(pin power_in line
				(at 5.08 15.24 270)
				(length 3.81)
				(name "ADVREF")
				(number "L2")
			)
			(pin passive line
				(at 7.62 15.24 270)
				(length 3.81)
				(hide yes)
				(name "VDDANA")
				(number "H2")
			)
			(pin power_in line
				(at 7.62 15.24 270)
				(length 3.81)
				(name "VDDANA")
				(number "K3")
			)
			(pin passive line
				(at 7.62 -12.7 90)
				(length 3.81)
				(hide yes)
				(name "GNDANA")
				(number "J2")
			)
			(pin power_in line
				(at 7.62 -12.7 90)
				(length 3.81)
				(name "GNDANA")
				(number "K4")
			)
		)
		(symbol "ATSAMA5D21_6_1"
			(pin input line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "DDR_CAL")
				(number "F10")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "DDR_D0")
				(number "B7")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 3.81)
				(name "DDR_D1")
				(number "A7")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "DDR_D2")
				(number "C8")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "DDR_D3")
				(number "B9")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "DDR_D4")
				(number "A9")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "DDR_D5")
				(number "C9")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "DDR_D6")
				(number "A10")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "DDR_D7")
				(number "B10")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "DDR_D8")
				(number "H13")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "DDR_D9")
				(number "H14")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "DDR_D10")
				(number "J13")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "DDR_D11")
				(number "J14")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "DDR_D12")
				(number "L13")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "DDR_D13")
				(number "L14")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "DDR_D14")
				(number "J12")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "DDR_D15")
				(number "K12")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 3.81)
				(name "VDDIODDR")
				(number "C6")
			)
			(pin passive line
				(at -5.08 48.26 270)
				(length 3.81)
				(hide yes)
				(name "VDDIODDR")
				(number "E10")
			)
			(pin passive line
				(at -5.08 48.26 270)
				(length 3.81)
				(hide yes)
				(name "VDDIODDR")
				(number "E12")
			)
			(pin passive line
				(at -5.08 48.26 270)
				(length 3.81)
				(hide yes)
				(name "VDDIODDR")
				(number "G10")
			)
			(pin passive line
				(at -5.08 48.26 270)
				(length 3.81)
				(hide yes)
				(name "VDDIODDR")
				(number "G12")
			)
			(pin passive line
				(at -5.08 48.26 270)
				(length 3.81)
				(hide yes)
				(name "VDDIODDR")
				(number "H11")
			)
			(pin passive line
				(at -5.08 48.26 270)
				(length 3.81)
				(hide yes)
				(name "VDDIODDR")
				(number "J10")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "GNDIODDR")
				(number "C7")
			)
			(pin passive line
				(at -5.08 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GNDIODDR")
				(number "D12")
			)
			(pin passive line
				(at -5.08 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GNDIODDR")
				(number "E9")
			)
			(pin passive line
				(at -5.08 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GNDIODDR")
				(number "F12")
			)
			(pin passive line
				(at -5.08 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GNDIODDR")
				(number "G11")
			)
			(pin passive line
				(at -5.08 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GNDIODDR")
				(number "H10")
			)
			(pin passive line
				(at -5.08 -50.8 90)
				(length 3.81)
				(hide yes)
				(name "GNDIODDR")
				(number "J11")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 3.81)
				(name "DDR_VREF")
				(number "C12")
			)
			(pin passive line
				(at 0 48.26 270)
				(length 3.81)
				(hide yes)
				(name "DDR_VREF")
				(number "H12")
			)
			(pin output line
				(at 17.78 40.64 180)
				(length 3.81)
				(name "~{DDR_RESET}")
				(number "D13")
			)
			(pin output line
				(at 17.78 35.56 180)
				(length 3.81)
				(name "DDR_A0")
				(number "E11")
			)
			(pin output line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "DDR_A1")
				(number "C11")
			)
			(pin output line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "DDR_A2")
				(number "B12")
			)
			(pin output line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "DDR_A3")
				(number "A12")
			)
			(pin output line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "DDR_A4")
				(number "D11")
			)
			(pin output line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "DDR_A5")
				(number "D14")
			)
			(pin output line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "DDR_A6")
				(number "B14")
			)
			(pin output line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "DDR_A7")
				(number "D9")
			)
			(pin output line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "DDR_A8")
				(number "C10")
			)
			(pin output line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "DDR_A9")
				(number "D10")
			)
			(pin output line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "DDR_A10")
				(number "F9")
			)
			(pin output line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "DDR_A11")
				(number "A11")
			)
			(pin output line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "DDR_A12")
				(number "B11")
			)
			(pin output line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "DDR_A13")
				(number "E13")
			)
			(pin output line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "DDR_CLK")
				(number "A13")
			)
			(pin output line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "DDR_CLKN")
				(number "B13")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "DDR_CKE")
				(number "E14")
			)
			(pin output line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "DDR_CS")
				(number "F11")
			)
			(pin output line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "DDR_WE")
				(number "A14")
			)
			(pin output line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "DDR_RAS")
				(number "C14")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "DDR_CAS")
				(number "C13")
			)
			(pin output line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "DDR_DQM0")
				(number "D8")
			)
			(pin output line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "DDR_DQM1")
				(number "G14")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "DDR_DQS0")
				(number "B8")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "DDR_DQS1")
				(number "K14")
			)
			(pin output line
				(at 17.78 -33.02 180)
				(length 3.81)
				(name "DDR_DQSN0")
				(number "A8")
			)
			(pin output line
				(at 17.78 -35.56 180)
				(length 3.81)
				(name "DDR_DQSN1")
				(number "K13")
			)
			(pin output line
				(at 17.78 -38.1 180)
				(length 3.81)
				(name "DDR_BA0")
				(number "F13")
			)
			(pin output line
				(at 17.78 -40.64 180)
				(length 3.81)
				(name "DDR_BA1")
				(number "G13")
			)
			(pin output line
				(at 17.78 -43.18 180)
				(length 3.81)
				(name "DDR_BA2")
				(number "F14")
			)
		)
		(symbol "ATSAMA5D21_7_1"
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "HHSDPA")
				(number "N7")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "HHSDMA")
				(number "P7")
			)
			(pin power_in line
				(at -5.08 15.24 270)
				(length 3.81)
				(name "VDDFUSE")
				(number "K11")
			)
			(pin power_in line
				(at -2.54 15.24 270)
				(length 3.81)
				(name "VDDUTMIC")
				(number "M7")
			)
			(pin power_in line
				(at -2.54 -15.24 90)
				(length 3.81)
				(name "GNDUTMIC")
				(number "M8")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDDUTMII")
				(number "K7")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "GNDUTMII")
				(number "L8")
			)
			(pin power_in line
				(at 2.54 15.24 270)
				(length 3.81)
				(name "VBG")
				(number "L7")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "HHSDPB")
				(number "N8")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "HHSDMB")
				(number "P8")
			)
		)
		(symbol "ATSAMA5D21_8_1"
			(pin input line
				(at -15.24 12.7 0)
				(length 3.81)
				(name "XIN32")
				(number "M1")
			)
			(pin output line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "XOUT32")
				(number "L1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "~{RST}")
				(number "N3")
			)
			(pin input line
				(at -15.24 0 0)
				(length 3.81)
				(name "TST")
				(number "M2")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "JTAGSEL")
				(number "L4")
			)
			(pin input line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "WKUP")
				(number "P1")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "COMPP")
				(number "N2")
			)
			(pin input line
				(at -15.24 -12.7 0)
				(length 3.81)
				(name "COMPN")
				(number "P2")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "VDDBU")
				(number "M4")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 3.81)
				(name "GNDBU")
				(number "M5")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 3.81)
				(name "PIOBU0")
				(number "K5")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "PIOBU1")
				(number "L3")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "PIOBU2")
				(number "M3")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "PIOBU3")
				(number "N4")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "PIOBU4")
				(number "L5")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "PIOBU5")
				(number "M6")
			)
			(pin output line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "SHDN")
				(number "N1")
			)
		)
		(symbol "ATSAMA5D21_9_1"
			(pin power_in line
				(at -2.54 20.32 270)
				(length 3.81)
				(name "VDDAUDIOPLL")
				(number "K6")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "GNDAUDIOPLL")
				(number "J6")
			)
			(pin output line
				(at 7.62 0 180)
				(length 3.81)
				(name "CLK_AUDIO")
				(number "J7")
			)
		)
		(symbol "ATSAMA5D21_10_1"
			(pin power_in line
				(at -2.54 -10.16 90)
				(length 3.81)
				(name "GNDOSC")
				(number "N6")
			)
			(pin power_in line
				(at 0 10.16 270)
				(length 3.81)
				(name "VDDOSC")
				(number "N5")
			)
			(pin input line
				(at 10.16 2.54 180)
				(length 3.81)
				(name "XIN")
				(number "P5")
			)
			(pin output line
				(at 10.16 -2.54 180)
				(length 3.81)
				(name "XOUT")
				(number "P6")
			)
		)
		(embedded_fonts no)
	)
)
