(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ATSAMD09C13A-SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "ATSAMD09C13A-SS"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -26.67 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42414-SAM-D09_Datasheet.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 48MHz, 8KB Flash, 4KB RAM, 2.4-3.6V, 12 GPIO, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD09C13A-SS_0_1")
		(symbol "ATSAMD09C13A-SS_1_1"
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PA28/~{RST}")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PA30/SWCLK")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PA31/SWDIO")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PA08/XIN")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "PA09/XOUT")
				(number "3")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA02")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA04")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA05")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA14")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA24")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA25")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD09D14A-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "ATSAMD09D14A-M"
			(at 1.27 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42414-SAM-D09_Datasheet.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 48MHz, 16KB Flash, 4KB RAM, 2.4-3.6V, 22 GPIO, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD09D14A-M_0_1")
		(symbol "ATSAMD09D14A-M_1_1"
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "PA28/~{RST}")
				(number "18")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PA30/SWCLK")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "PA31/SWDIO")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PA08/XIN")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "PA09/XOUT")
				(number "8")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 2.54)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "PA02")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "PA03")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA04")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA05")
				(number "4")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA06")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA07")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA10")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA11")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA14")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA16")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA17")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA22")
				(number "15")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA23")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA24")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "PA25")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "PA27")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD10D13A-SS"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "ATSAMD10D13A-SS"
			(at 1.27 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42242-SAM-D10_Datasheet.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 48MHz, 8KB Flash, 4KB RAM, 1.6-3.6V, 18 GPIO, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD10D13A-SS_0_1")
		(symbol "ATSAMD10D13A-SS_1_1"
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PA28/~{RST}")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PA30/SWCLK")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PA31/SWDIO")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PA08/XIN")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PA09/XOUT")
				(number "5")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA02")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA03")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA04")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA05")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA06")
				(number "2")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA07")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA14")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA16")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA22")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA23")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA24")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA25")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD10D14A-U"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "ATSAMD10D14A-U"
			(at 1.27 19.05 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-20_1.934x2.434mm_Layout4x5_P0.4mm"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42242-SAM-D10_Datasheet.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 48MHz, 16KB Flash, 4KB RAM, 1.6-3.6V, 18 GPIO, WLCSP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*1.934x2.434mm*Layout4x5*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD10D14A-U_0_1")
		(symbol "ATSAMD10D14A-U_1_1"
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "PA28/~{RST}")
				(number "E2")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "PA30/SWCLK")
				(number "D2")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "PA31/SWDIO")
				(number "E1")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "PA08/XIN")
				(number "B4")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "PA09/XOUT")
				(number "C4")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "VDD")
				(number "B1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "C2")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "PA02")
				(number "A1")
			)
			(pin bidirectional line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "PA03")
				(number "A2")
			)
			(pin bidirectional line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "PA04")
				(number "A3")
			)
			(pin bidirectional line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "PA05")
				(number "B2")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "PA06")
				(number "A4")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "PA07")
				(number "B3")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "PA14")
				(number "D4")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "PA15")
				(number "E4")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "PA16")
				(number "C3")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "PA22")
				(number "E3")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "PA23")
				(number "D3")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "PA24")
				(number "D1")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "PA25")
				(number "C1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD21E15A-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "ATSAMD21E15A-A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash, 4K SRAM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD21E15A-A_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA04")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA05")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA06")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA07")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA08")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA09")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA10")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA11")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA14")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA15")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA16")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA17")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA18")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA19")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA22")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA23")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA24")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA25")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA27")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA28")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PA30")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PA31")
				(number "32")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "26")
			)
			(pin power_out line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDDCORE")
				(number "29")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDDIN")
				(number "30")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDANA")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD21E15A-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "ATSAMD21E15A-M"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash, 4K SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD21E15A-M_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA04")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA05")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA06")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA07")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA08")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA09")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA10")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA11")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA14")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA15")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA16")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA17")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA18")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA19")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA22")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA23")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA24")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA25")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA27")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA28")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PA30")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PA31")
				(number "32")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "26")
			)
			(pin power_out line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDDCORE")
				(number "29")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDDIN")
				(number "30")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "EP")
				(number "33")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDANA")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD21E15L-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "ATSAMD21E15L-A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, Pinout Optimized for Analog & PWM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD21E15L-A_1_1"
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA02")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA03")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA04")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA05")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA06")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA07")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA08")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA09")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA10")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA11")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA14")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA15")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA16")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA17")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA18")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA19")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA22")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA23")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA24")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA25")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PA30")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PA31")
				(number "30")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "25")
			)
			(pin power_out line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDDCORE")
				(number "27")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "28")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO/VDDANA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PB02")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB03")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB04")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB05")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD21E15L-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "ATSAMD21E15L-M"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, Pinout Optimized for Analog & PWM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD21E15L-M_1_1"
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA02")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA03")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA04")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA05")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA06")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA07")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA08")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA09")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA10")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA11")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA14")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA15")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA16")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA17")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA18")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA19")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA22")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA23")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA24")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA25")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PA30")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PA31")
				(number "30")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "25")
			)
			(pin power_out line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDDCORE")
				(number "27")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "EP")
				(number "33")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "28")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDIO/VDDANA")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PB02")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB03")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB04")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB05")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD21G15A-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "ATSAMD21G15A-A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash, 4K SRAM, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD21G15A-A_0_1")
		(symbol "ATSAMD21G15A-A_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA04")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA05")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA06")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA07")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA08")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA09")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA10")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA11")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA12")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA13")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA14")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA15")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA16")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA17")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA18")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA19")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA20")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA21")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA22")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA23")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA24")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA25")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA27")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA28")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PA30")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PA31")
				(number "46")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "40")
			)
			(pin power_out line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDDCORE")
				(number "43")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDDIN")
				(number "44")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "36")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "GNDANA")
				(number "5")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDANA")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PB02")
				(number "47")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB03")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB08")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB09")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB10")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB11")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB22")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB23")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD21G15A-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "ATSAMD21G15A-M"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash, 4K SRAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD21G15A-M_0_1")
		(symbol "ATSAMD21G15A-M_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA04")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA05")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA06")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA07")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA08")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA09")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA10")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA11")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA12")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA13")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA14")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA15")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA16")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA17")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA18")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA19")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA20")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA21")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA22")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA23")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA24")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA25")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA27")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA28")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PA30")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PA31")
				(number "46")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "40")
			)
			(pin power_out line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDDCORE")
				(number "43")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDDIN")
				(number "44")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "EP")
				(number "49")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "36")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "GNDANA")
				(number "5")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDANA")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PB02")
				(number "47")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB03")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB08")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB09")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB10")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB11")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB22")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB23")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD21G16L-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "ATSAMD21G16L-M"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, Pinout Optimized for Analog & PWM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD21G16L-M_0_1")
		(symbol "ATSAMD21G16L-M_1_1"
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA02")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA03")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA04")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA05")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA06")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA07")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA08")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA09")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA10")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA11")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA12")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA13")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA14")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA15")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA16")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA17")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA18")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA19")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA20")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA21")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA22")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA23")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA24")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA25")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA27")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA28")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PA30")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PA31")
				(number "44")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "38")
			)
			(pin power_out line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDDCORE")
				(number "41")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDDIN")
				(number "42")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "EP")
				(number "49")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "36")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "GNDANA")
				(number "5")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDANA")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PB00")
				(number "45")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PB01")
				(number "46")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PB02")
				(number "47")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB03")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB04")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB05")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB08")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB09")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB10")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB11")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD21J15A-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "ATSAMD21J15A-A"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash, 4K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD21J15A-A_0_1")
		(symbol "ATSAMD21J15A-A_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA04")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA05")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA06")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA07")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA08")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA09")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA10")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA11")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA12")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA13")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA14")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA15")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA16")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA17")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA18")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA19")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA20")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA21")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA22")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA23")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA24")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA25")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA27")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA28")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PA30")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PA31")
				(number "58")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "52")
			)
			(pin power_out line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDDCORE")
				(number "55")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDDIN")
				(number "56")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "34")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "GNDANA")
				(number "7")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "21")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDANA")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PB00")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PB01")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PB02")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB03")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB04")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB05")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PB06")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PB07")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB08")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB09")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB10")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB11")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB12")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB13")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB14")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB15")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB16")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB17")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB22")
				(number "49")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB23")
				(number "50")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB30")
				(number "59")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB31")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD21J15A-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "ATSAMD21J15A-M"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash, 4K SRAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD21J15A-M_0_1")
		(symbol "ATSAMD21J15A-M_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA04")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA05")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA06")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA07")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA08")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA09")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA10")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA11")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA12")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA13")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA14")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA15")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA16")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA17")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA18")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA19")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA20")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA21")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA22")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA23")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA24")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA25")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA27")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA28")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PA30")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PA31")
				(number "58")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "52")
			)
			(pin power_out line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDDCORE")
				(number "55")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDDIN")
				(number "56")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 2.54)
				(name "EP")
				(number "65")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "48")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "34")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "GNDANA")
				(number "7")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "21")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDANA")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PB00")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PB01")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PB02")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB03")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB04")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB05")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PB06")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PB07")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB08")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB09")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB10")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB11")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB12")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB13")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB14")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB15")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB16")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB17")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB22")
				(number "49")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB23")
				(number "50")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB30")
				(number "59")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB31")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD21J15B-C"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "ATSAMD21J15B-C"
			(at 0 -2.54 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, UFBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD21J15B-C_0_1")
		(symbol "ATSAMD21J15B-C_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PA00")
				(number "B1")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA01")
				(number "C1")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA02")
				(number "C3")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA03")
				(number "D3")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA04")
				(number "F1")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA05")
				(number "F2")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA06")
				(number "G2")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA07")
				(number "G1")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA08")
				(number "H1")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA09")
				(number "H2")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA10")
				(number "F3")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA11")
				(number "G3")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA12")
				(number "F6")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA13")
				(number "G6")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA14")
				(number "H6")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA15")
				(number "H7")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA16")
				(number "G7")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA17")
				(number "F8")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA18")
				(number "F7")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA19")
				(number "E7")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA20")
				(number "D6")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA21")
				(number "C5")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA22")
				(number "C6")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA23")
				(number "C7")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA24")
				(number "E8")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA25")
				(number "D8")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA27")
				(number "B7")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA28")
				(number "A6")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PA30")
				(number "B5")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PA31")
				(number "B4")
			)
			(pin input line
				(at -17.78 -43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "B6")
			)
			(pin power_out line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDDCORE")
				(number "A4")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDDIN")
				(number "A3")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "B8")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "A5")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "C8")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "H4")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "G8")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "GNDANA")
				(number "D1")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "H3")
			)
			(pin power_in line
				(at 7.62 48.26 270)
				(length 2.54)
				(name "VDDANA")
				(number "E1")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PB00")
				(number "B2")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PB01")
				(number "A2")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PB02")
				(number "A1")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB03")
				(number "C2")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB04")
				(number "D2")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB05")
				(number "D4")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PB06")
				(number "E4")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PB07")
				(number "E3")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB08")
				(number "E2")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB09")
				(number "F4")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB10")
				(number "G4")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB11")
				(number "E5")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB12")
				(number "F5")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB13")
				(number "G5")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB14")
				(number "H5")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB15")
				(number "E6")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB16")
				(number "D7")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB17")
				(number "D5")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB22")
				(number "A8")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB23")
				(number "A7")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "PB30")
				(number "C4")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "PB31")
				(number "B3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD51J18A-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 -44.45 0)
		)
		(property "Value" "ATSAMD51J18A-A"
			(at 5.08 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001507E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D51 Microchip SMART ARM Cortex-M4F-based MCU, 256K Flash, 128K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4F MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD51J18A-A_0_1")
		(symbol "ATSAMD51J18A-A_1_0"
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PB03")
				(number "64")
			)
		)
		(symbol "ATSAMD51J18A-A_1_1"
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA04")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA05")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA06")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA07")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA08")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA09")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA10")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA11")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA12")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA13")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA14")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA15")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA16")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA17")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA18")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA19")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA20")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA21")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA22")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA23")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PA24")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA25")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA27")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PA30")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PA31")
				(number "58")
			)
			(pin input line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "~{RESET}")
				(number "52")
			)
			(pin power_in line
				(at -10.16 45.72 270)
				(length 2.54)
				(name "VSW")
				(number "55")
			)
			(pin power_out line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDDCORE")
				(number "53")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDDIOB")
				(number "21")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "34")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "GNDANA")
				(number "7")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "56")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 2.54)
				(name "VDDANA")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB00")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB01")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB02")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PB04")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB05")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB06")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB07")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB08")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB09")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB10")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB11")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB12")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB13")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB14")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB15")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB16")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB17")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB22")
				(number "49")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB23")
				(number "50")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB30")
				(number "59")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB31")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD51J18A-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 -44.45 0)
		)
		(property "Value" "ATSAMD51J18A-M"
			(at 5.08 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001507E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D51 Microchip SMART ARM Cortex-M4F-based MCU, 256K Flash, 128K SRAM, VQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4F MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAMD51J18A-M_0_1")
		(symbol "ATSAMD51J18A-M_1_0"
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PB03")
				(number "64")
			)
		)
		(symbol "ATSAMD51J18A-M_1_1"
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA04")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA05")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA06")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA07")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA08")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA09")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA10")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA11")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA12")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA13")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA14")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA15")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA16")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA17")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA18")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA19")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA20")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA21")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA22")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA23")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PA24")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA25")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA27")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PA30")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PA31")
				(number "58")
			)
			(pin input line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "~{RESET}")
				(number "52")
			)
			(pin power_in line
				(at -10.16 45.72 270)
				(length 2.54)
				(name "VSW")
				(number "55")
			)
			(pin power_out line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDDCORE")
				(number "53")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDDIOB")
				(number "21")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "34")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "GNDANA")
				(number "7")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "56")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 2.54)
				(name "VDDANA")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB00")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB01")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB02")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PB04")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB05")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB06")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB07")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB08")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB09")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB10")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB11")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB12")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB13")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB14")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB15")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PB16")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PB17")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PB22")
				(number "49")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PB23")
				(number "50")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB30")
				(number "59")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB31")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAMD10C13A-SS"
		(extends "ATSAMD09C13A-SS")
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "ATSAMD10C13A-SS"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -26.67 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42242-SAM-D10_Datasheet.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 48MHz, 8KB Flash, 4KB RAM, 1.6-3.6V, 12 GPIO, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD10C14A-SS"
		(extends "ATSAMD09C13A-SS")
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "ATSAMD10C14A-SS"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -26.67 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42242-SAM-D10_Datasheet.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 48MHz, 16KB Flash, 4KB RAM, 1.6-3.6V, 12 GPIO, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD10D13A-M"
		(extends "ATSAMD09D14A-M")
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "ATSAMD10D13A-M"
			(at 1.27 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42242-SAM-D10_Datasheet.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 48MHz, 8KB Flash, 4KB RAM, 1.6-3.6V, 22 GPIO, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD10D14A-M"
		(extends "ATSAMD09D14A-M")
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "ATSAMD10D14A-M"
			(at 1.27 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42242-SAM-D10_Datasheet.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 48MHz, 16KB Flash, 4KB RAM, 1.6-3.6V, 22 GPIO, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD10D14A-SS"
		(extends "ATSAMD10D13A-SS")
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "ATSAMD10D14A-SS"
			(at 1.27 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42242-SAM-D10_Datasheet.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 48MHz, 16KB Flash, 4KB RAM, 1.6-3.6V, 18 GPIO, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD11C14A-SS"
		(extends "ATSAMD09C13A-SS")
		(property "Reference" "U"
			(at -10.16 16.51 0)
		)
		(property "Value" "ATSAMD11C14A-SS"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 -26.67 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42363-SAM-D11_Datasheet.pdf"
			(at 0 -17.78 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 48MHz, 16KB Flash, 4KB RAM, 1.6-3.6V, 18 GPIO, SOIC-14"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x8.7mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD11D14A-M"
		(extends "ATSAMD09D14A-M")
		(property "Reference" "U"
			(at -10.16 24.13 0)
		)
		(property "Value" "ATSAMD11D14A-M"
			(at 1.27 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 0 -34.29 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42363-SAM-D11_Datasheet.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 48MHz, 16KB Flash, 4KB RAM, 1.6-3.6V, 22 GPIO, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD11D14A-SS"
		(extends "ATSAMD10D13A-SS")
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "ATSAMD11D14A-SS"
			(at 1.27 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 0 -29.21 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42363-SAM-D11_Datasheet.pdf"
			(at 0 -22.86 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 48MHz, 16KB Flash, 4KB RAM, 1.6-3.6V, 18 GPIO, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD11D14A-U"
		(extends "ATSAMD10D14A-U")
		(property "Reference" "U"
			(at -10.16 19.05 0)
		)
		(property "Value" "ATSAMD11D14A-U"
			(at 1.27 19.05 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-20_1.934x2.434mm_Layout4x5_P0.4mm"
			(at 0 -27.94 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/Atmel-42363-SAM-D11_Datasheet.pdf"
			(at 0 -25.4 0)
		)
		(property "Description" "ARM Cortex-M0+ MCU, 48MHz, 16KB Flash, 4KB RAM, 1.6-3.6V, 18 GPIO, WLCSP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*1.934x2.434mm*Layout4x5*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E15B-A"
		(extends "ATSAMD21E15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E15B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E15B-M"
		(extends "ATSAMD21E15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E15B-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E16A-A"
		(extends "ATSAMD21E15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E16A-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E16A-M"
		(extends "ATSAMD21E15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E16A-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E16B-A"
		(extends "ATSAMD21E15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E16B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E16B-M"
		(extends "ATSAMD21E15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E16B-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E16L-A"
		(extends "ATSAMD21E15L-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E16L-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, Pinout Optimized for Analog & PWM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E16L-M"
		(extends "ATSAMD21E15L-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E16L-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, Pinout Optimized for Analog & PWM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E17A-A"
		(extends "ATSAMD21E15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E17A-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash, 16K SRAM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E17A-M"
		(extends "ATSAMD21E15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E17A-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash, 16K SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E17D-A"
		(extends "ATSAMD21E15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E17D-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash w/ 4K RWW, 16K SRAM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E17D-M"
		(extends "ATSAMD21E15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E17D-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash w/ 4K RWW, 16K SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E17L-A"
		(extends "ATSAMD21E15L-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E17L-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash w/ 4K RWW, 16K SRAM, Pinout Optimized for Analog & PWM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E17L-M"
		(extends "ATSAMD21E15L-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E17L-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash w/ 4K RWW, 16K SRAM, Pinout Optimized for Analog & PWM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E18A-A"
		(extends "ATSAMD21E15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E18A-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 256K Flash, 32K SRAM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21E18A-M"
		(extends "ATSAMD21E15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21E18A-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 256K Flash, 32K SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21G15B-A"
		(extends "ATSAMD21G15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21G15B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21G15B-M"
		(extends "ATSAMD21G15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21G15B-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 35.56 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21G16A-A"
		(extends "ATSAMD21G15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21G16A-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21G16A-M"
		(extends "ATSAMD21G15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21G16A-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 35.56 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21G16B-A"
		(extends "ATSAMD21G15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21G16B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21G16B-M"
		(extends "ATSAMD21G15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21G16B-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 35.56 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21G17A-A"
		(extends "ATSAMD21G15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21G17A-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash, 16K SRAM, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21G17A-M"
		(extends "ATSAMD21G15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21G17A-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 35.56 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash, 16K SRAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21G17D-A"
		(extends "ATSAMD21G15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21G17D-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash w/ 4K RWW, 16K SRAM, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21G17D-M"
		(extends "ATSAMD21G15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21G17D-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 35.56 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash w/ 4K RWW, 16K SRAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21G17L-M"
		(extends "ATSAMD21G16L-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21G17L-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 35.56 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash w/ 4K RWW, 16K SRAM, Pinout Optimized for Analog & PWM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21G18A-A"
		(extends "ATSAMD21G15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21G18A-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 256K Flash, 32K SRAM, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21G18A-M"
		(extends "ATSAMD21G15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21G18A-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 35.56 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 256K Flash, 32K SRAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J15B-A"
		(extends "ATSAMD21J15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J15B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 24.13 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J15B-M"
		(extends "ATSAMD21J15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J15B-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J16A-A"
		(extends "ATSAMD21J15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J16A-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 24.13 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J16A-M"
		(extends "ATSAMD21J15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J16A-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J16B-A"
		(extends "ATSAMD21J15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J16B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 24.13 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J16B-C"
		(extends "ATSAMD21J15B-C")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J16B-C"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at 29.21 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, UFBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J16B-M"
		(extends "ATSAMD21J15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J16B-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J17A-A"
		(extends "ATSAMD21J15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J17A-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 24.13 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash, 16K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J17A-M"
		(extends "ATSAMD21J15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J17A-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash, 16K SRAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J17D-A"
		(extends "ATSAMD21J15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J17D-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 24.13 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash w/ 4K RWW, 16K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J17D-C"
		(extends "ATSAMD21J15B-C")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J17D-C"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_BGA:UFBGA-64_5x5mm_Layout8x8_P0.5mm"
			(at 29.21 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash w/ 4K RWW, 16K SRAM, UFBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "UFBGA*5x5mm*Layout8x8*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J17D-M"
		(extends "ATSAMD21J15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J17D-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash w/ 4K RWW, 16K SRAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J18A-A"
		(extends "ATSAMD21J15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J18A-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 24.13 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 256K Flash, 32K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD21J18A-M"
		(extends "ATSAMD21J15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMD21J18A-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM D21 Microchip SMART ARM-based Flash MCU, 48Mhz, 256K Flash, 32K SRAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD51J19A-A"
		(extends "ATSAMD51J18A-A")
		(property "Reference" "U"
			(at -15.24 -44.45 0)
		)
		(property "Value" "ATSAMD51J19A-A"
			(at 5.08 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001507E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D51 Microchip SMART ARM Cortex-M4F-based MCU, 512K Flash, 192K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4F MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD51J19A-M"
		(extends "ATSAMD51J18A-M")
		(property "Reference" "U"
			(at -15.24 -44.45 0)
		)
		(property "Value" "ATSAMD51J19A-M"
			(at 5.08 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001507E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D51 Microchip SMART ARM Cortex-M4F-based MCU, 512K Flash, 192K SRAM, VQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4F MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD51J20A-A"
		(extends "ATSAMD51J18A-A")
		(property "Reference" "U"
			(at -15.24 -44.45 0)
		)
		(property "Value" "ATSAMD51J20A-A"
			(at 5.08 -44.45 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001507E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D51 Microchip SMART ARM Cortex-M4F-based MCU, 1024K Flash, 256K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4F MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMD51J20A-M"
		(extends "ATSAMD51J18A-M")
		(property "Reference" "U"
			(at -15.24 -44.45 0)
		)
		(property "Value" "ATSAMD51J20A-M"
			(at 5.08 -44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 0 0 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001507E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM D51 Microchip SMART ARM Cortex-M4F-based MCU, 1024K Flash, 256K SRAM, VQFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4F MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1E14B-A"
		(extends "ATSAMD21E15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1E14B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 16K Flash w/ 0.5K RWW, 4K SRAM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1E14B-M"
		(extends "ATSAMD21E15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1E14B-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 16K Flash w/ 0.5K RWW, 4K SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1E15B-A"
		(extends "ATSAMD21E15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1E15B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1E15B-M"
		(extends "ATSAMD21E15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1E15B-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1E16B-A"
		(extends "ATSAMD21E15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1E16B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, TQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1E16B-M"
		(extends "ATSAMD21E15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1E16B-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.6x3.6mm"
			(at 34.29 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1G14B-A"
		(extends "ATSAMD21G15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1G14B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 16K Flash w/ 0.5K RWW, 4K SRAM, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1G14B-M"
		(extends "ATSAMD21G15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1G14B-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 35.56 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 16K Flash w/ 0.5K RWW, 4K SRAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1G15B-A"
		(extends "ATSAMD21G15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1G15B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1G15B-M"
		(extends "ATSAMD21G15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1G15B-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 35.56 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1G16B-A"
		(extends "ATSAMD21G15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1G16B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 22.86 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, TQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1G16B-M"
		(extends "ATSAMD21G15A-M")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1G16B-M"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 35.56 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1J14B-A"
		(extends "ATSAMD21J15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1J14B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 24.13 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 16K Flash w/ 0.5K RWW, 4K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1J15B-A"
		(extends "ATSAMD21J15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1J15B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 24.13 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash w/ 1K RWW, 4K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAMDA1J16B-A"
		(extends "ATSAMD21J15A-A")
		(property "Reference" "U"
			(at -13.97 46.99 0)
		)
		(property "Value" "ATSAMDA1J16B-A"
			(at 16.51 46.99 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 24.13 -46.99 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM_D21_DA1_Family_Data%20Sheet_DS40001882E.pdf"
			(at 0 25.4 0)
		)
		(property "Description" "SAM DA1 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash w/ 2K RWW, 8K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
