(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ATSAME51J18A-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 48.26 0)
		)
		(property "Value" "ATSAME51J18A-A"
			(at -12.7 -48.26 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 33.02 48.26 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001507E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM E51 Microchip SMART ARM Cortex-M4F-based MCU, 256K Flash, 128K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4F MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAME51J18A-A_0_1")
		(symbol "ATSAME51J18A-A_1_0"
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PB03")
				(number "64")
			)
		)
		(symbol "ATSAME51J18A-A_1_1"
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "PA04")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "PA05")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "PA06")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 2.54)
				(name "PA07")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 2.54)
				(name "PA08")
				(number "17")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 2.54)
				(name "PA09")
				(number "18")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 2.54)
				(name "PA10")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 2.54)
				(name "PA11")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "PA12")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "PA13")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 2.54)
				(name "PA14")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 2.54)
				(name "PA15")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PA16")
				(number "35")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 2.54)
				(name "PA17")
				(number "36")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "PA18")
				(number "37")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 2.54)
				(name "PA19")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "PA20")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 2.54)
				(name "PA21")
				(number "42")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 2.54)
				(name "PA22")
				(number "43")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "PA23")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "PA24")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 2.54)
				(name "PA25")
				(number "46")
			)
			(pin bidirectional line
				(at -22.86 -30.48 0)
				(length 2.54)
				(name "PA27")
				(number "51")
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 2.54)
				(name "PA30")
				(number "57")
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 2.54)
				(name "PA31")
				(number "58")
			)
			(pin input line
				(at -22.86 -40.64 0)
				(length 2.54)
				(name "~{RESET}")
				(number "52")
			)
			(pin power_in line
				(at -10.16 48.26 270)
				(length 2.54)
				(name "VSW")
				(number "55")
			)
			(pin power_out line
				(at -7.62 48.26 270)
				(length 2.54)
				(name "VDDCORE")
				(number "53")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "VDDIOB")
				(number "21")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "34")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "48")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 2.54)
				(name "GNDANA")
				(number "7")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 2.54)
				(name "VDDIO")
				(number "56")
			)
			(pin power_in line
				(at 10.16 48.26 270)
				(length 2.54)
				(name "VDDANA")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PB00")
				(number "61")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PB01")
				(number "62")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PB02")
				(number "63")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PB04")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PB05")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PB06")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PB07")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PB08")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PB09")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 2.54)
				(name "PB10")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PB11")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PB12")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PB13")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PB14")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PB15")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PB16")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PB17")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 2.54)
				(name "PB22")
				(number "49")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PB23")
				(number "50")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PB30")
				(number "59")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PB31")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAME53J18A-M"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 44.45 0)
		)
		(property "Value" "ATSAME53J18A-M"
			(at 16.51 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 15.24 25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001507E.pdf"
			(at 15.24 25.4 0)
		)
		(property "Description" "SAM E53 Microchip SMART ARM Cortex-M4F based MCU, 256K Flash, 128K SRAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4F MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAME53J18A-M_0_1")
		(symbol "ATSAME53J18A-M_1_1"
			(pin bidirectional line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PA04")
				(number "13")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PA05")
				(number "14")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PA06")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PA07")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PA08")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PA09")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PA10")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PA11")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PA12")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PA13")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PA14")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PA15")
				(number "32")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PA16")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PA17")
				(number "36")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PA18")
				(number "37")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PA19")
				(number "38")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PA20")
				(number "41")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PA21")
				(number "42")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PA22")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PA23")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PA24")
				(number "45")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PA25")
				(number "46")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PA27")
				(number "51")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "PA30")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "PA31")
				(number "58")
			)
			(pin input line
				(at -15.24 -40.64 0)
				(length 2.54)
				(name "~{RESET}")
				(number "52")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VSW")
				(number "55")
			)
			(pin power_out line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDDCORE")
				(number "53")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDDANA")
				(number "8")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDDIOB")
				(number "21")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "56")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "GNDANA")
				(number "7")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "48")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "PB00")
				(number "61")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PB01")
				(number "62")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PB02")
				(number "63")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PB03")
				(number "64")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PB04")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PB05")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PB06")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PB07")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PB08")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PB09")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PB10")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PB11")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PB12")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PB13")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PB14")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PB15")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PB16")
				(number "39")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PB17")
				(number "40")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PB22")
				(number "49")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PB23")
				(number "50")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PB30")
				(number "59")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "PB31")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAME54N19A-A"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 76.2 0)
		)
		(property "Value" "ATSAME54N19A-A"
			(at 30.48 76.2 0)
		)
		(property "Footprint" "Package_QFP:TQFP-100_14x14mm_P0.5mm"
			(at 0 0 90)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001507E.pdf"
			(at -40.64 53.34 0)
		)
		(property "Description" "SAM E54 Microchip SMART ARM Cortex-M4F based MCU, 512K Flash, 192K SRAM, TQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4F MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAME54N19A-A_1_1"
			(pin bidirectional line
				(at -17.78 63.5 0)
				(length 3.81)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 60.96 0)
				(length 3.81)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 58.42 0)
				(length 3.81)
				(name "PA02")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 55.88 0)
				(length 3.81)
				(name "PA03")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 53.34 0)
				(length 3.81)
				(name "PA04")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 50.8 0)
				(length 3.81)
				(name "PA05")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 48.26 0)
				(length 3.81)
				(name "PA06")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 45.72 0)
				(length 3.81)
				(name "PA07")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 43.18 0)
				(length 3.81)
				(name "PA08")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 3.81)
				(name "PA09")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 3.81)
				(name "PA10")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 3.81)
				(name "PA11")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "PA12")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 3.81)
				(name "PA13")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "PA14")
				(number "48")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 3.81)
				(name "PA15")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "PA16")
				(number "52")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "PA17")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "PA18")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "PA19")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "PA20")
				(number "70")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "PA21")
				(number "71")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PA22")
				(number "72")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "PA23")
				(number "73")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "PA24")
				(number "74")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "PA25")
				(number "75")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "PA27")
				(number "87")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "PA30")
				(number "93")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "PA31")
				(number "94")
			)
			(pin input line
				(at -17.78 -68.58 0)
				(length 3.81)
				(name "~{RESET}")
				(number "88")
			)
			(pin power_in line
				(at -10.16 78.74 270)
				(length 3.81)
				(name "VSW")
				(number "91")
			)
			(pin power_out line
				(at -7.62 78.74 270)
				(length 3.81)
				(name "VDDCORE")
				(number "89")
			)
			(pin power_in line
				(at -5.08 78.74 270)
				(length 3.81)
				(name "VDDANA")
				(number "12")
			)
			(pin power_in line
				(at -2.54 78.74 270)
				(length 3.81)
				(name "VDDIOB")
				(number "25")
			)
			(pin power_in line
				(at -2.54 -78.74 90)
				(length 3.81)
				(name "GNDANA")
				(number "11")
			)
			(pin power_in line
				(at 0 78.74 270)
				(length 3.81)
				(name "VDDIOB")
				(number "30")
			)
			(pin passive line
				(at 0 -78.74 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -78.74 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -78.74 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -78.74 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -78.74 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at 0 -78.74 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "76")
			)
			(pin power_in line
				(at 0 -78.74 90)
				(length 3.81)
				(name "GND")
				(number "90")
			)
			(pin power_in line
				(at 2.54 78.74 270)
				(length 3.81)
				(name "VDDIO")
				(number "39")
			)
			(pin power_in line
				(at 5.08 78.74 270)
				(length 3.81)
				(name "VDDIO")
				(number "51")
			)
			(pin power_in line
				(at 7.62 78.74 270)
				(length 3.81)
				(name "VDDIO")
				(number "77")
			)
			(pin power_in line
				(at 10.16 78.74 270)
				(length 3.81)
				(name "VDDIO")
				(number "63")
			)
			(pin power_in line
				(at 12.7 78.74 270)
				(length 3.81)
				(name "VDDIO")
				(number "92")
			)
			(pin bidirectional line
				(at 17.78 63.5 180)
				(length 3.81)
				(name "PB00")
				(number "97")
			)
			(pin bidirectional line
				(at 17.78 60.96 180)
				(length 3.81)
				(name "PB01")
				(number "98")
			)
			(pin bidirectional line
				(at 17.78 58.42 180)
				(length 3.81)
				(name "PB02")
				(number "99")
			)
			(pin bidirectional line
				(at 17.78 55.88 180)
				(length 3.81)
				(name "PB03")
				(number "100")
			)
			(pin bidirectional line
				(at 17.78 53.34 180)
				(length 3.81)
				(name "PB04")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 50.8 180)
				(length 3.81)
				(name "PB05")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 48.26 180)
				(length 3.81)
				(name "PB06")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 45.72 180)
				(length 3.81)
				(name "PB07")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 43.18 180)
				(length 3.81)
				(name "PB08")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 3.81)
				(name "PB09")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 3.81)
				(name "PB10")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 3.81)
				(name "PB11")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "PB12")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "PB13")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "PB14")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "PB15")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "PB16")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "PB17")
				(number "65")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "PB18")
				(number "66")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "PB19")
				(number "67")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "PB20")
				(number "68")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PB21")
				(number "69")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PB22")
				(number "78")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PB23")
				(number "79")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PB24")
				(number "80")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "PB25")
				(number "81")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PB30")
				(number "95")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PB31")
				(number "96")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "PC00")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "PC01")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "PC02")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "PC03")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "PC05")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 3.81)
				(name "PC06")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "PC07")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "PC10")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "PC11")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 3.81)
				(name "PC12")
				(number "42")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 3.81)
				(name "PC13")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 -38.1 180)
				(length 3.81)
				(name "PC14")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 -40.64 180)
				(length 3.81)
				(name "PC15")
				(number "45")
			)
			(pin bidirectional line
				(at 17.78 -43.18 180)
				(length 3.81)
				(name "PC16")
				(number "56")
			)
			(pin bidirectional line
				(at 17.78 -45.72 180)
				(length 3.81)
				(name "PC17")
				(number "57")
			)
			(pin bidirectional line
				(at 17.78 -48.26 180)
				(length 3.81)
				(name "PC18")
				(number "58")
			)
			(pin bidirectional line
				(at 17.78 -50.8 180)
				(length 3.81)
				(name "PC19")
				(number "59")
			)
			(pin bidirectional line
				(at 17.78 -53.34 180)
				(length 3.81)
				(name "PC20")
				(number "60")
			)
			(pin bidirectional line
				(at 17.78 -55.88 180)
				(length 3.81)
				(name "PC21")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 -58.42 180)
				(length 3.81)
				(name "PC24")
				(number "82")
			)
			(pin bidirectional line
				(at 17.78 -60.96 180)
				(length 3.81)
				(name "PC25")
				(number "83")
			)
			(pin bidirectional line
				(at 17.78 -63.5 180)
				(length 3.81)
				(name "PC26")
				(number "84")
			)
			(pin bidirectional line
				(at 17.78 -66.04 180)
				(length 3.81)
				(name "PC27")
				(number "85")
			)
			(pin bidirectional line
				(at 17.78 -68.58 180)
				(length 3.81)
				(name "PC28")
				(number "86")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAME70J21A-AN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 53.34 0)
		)
		(property "Value" "ATSAME70J21A-AN"
			(at -12.7 -53.34 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 33.02 53.34 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM-E70-S70-V70-V71-Family-Data-Sheet-DS60001527D.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM E70 Microchip SMART ARM Cortex-M7-based MCU, 2048K Flash, 384K SRAM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M7 MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAME70J21A-AN_0_1")
		(symbol "ATSAME70J21A-AN_1_0"
			(pin power_in line
				(at 10.16 55.88 270)
				(length 5.08)
				(name "VDDPLLUSB")
				(number "64")
			)
		)
		(symbol "ATSAME70J21A-AN_1_1"
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 5.08)
				(name "PA3")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 5.08)
				(name "PA4")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 5.08)
				(name "PA5")
				(number "32")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 5.08)
				(name "PA7")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 5.08)
				(name "PA8")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 5.08)
				(name "PA9")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 5.08)
				(name "PA10")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 5.08)
				(name "PA11")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 5.08)
				(name "PA12")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PA13")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PA14")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PA21")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PA22")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PA24")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PA27")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PB0")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PB1")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PB2")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PB3")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PB4")
				(number "46")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PB5")
				(number "47")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PB6")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PB7")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PB8")
				(number "62")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PB9")
				(number "63")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PB12")
				(number "38")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "DP")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 5.08)
				(name "DM")
				(number "59")
			)
			(pin input line
				(at -25.4 -33.02 0)
				(length 5.08)
				(name "TST")
				(number "37")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 5.08)
				(name "NRST")
				(number "36")
			)
			(pin input line
				(at -25.4 -40.64 0)
				(length 5.08)
				(name "JTAGSEL")
				(number "45")
			)
			(pin input line
				(at -25.4 -45.72 0)
				(length 5.08)
				(name "VREFP")
				(number "5")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 5.08)
				(name "VDDIO")
				(number "10")
			)
			(pin passive line
				(at -7.62 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDDIO")
				(number "42")
			)
			(pin passive line
				(at -7.62 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDDIO")
				(number "58")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "VDDCORE")
				(number "13")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDDCORE")
				(number "24")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDDCORE")
				(number "61")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin power_in line
				(at 0 -55.88 90)
				(length 5.08)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VDDOUT")
				(number "3")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 5.08)
				(name "VDDIN")
				(number "4")
			)
			(pin power_in line
				(at 7.62 55.88 270)
				(length 5.08)
				(name "VDDPLL")
				(number "52")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "PD0")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PD1")
				(number "57")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PD2")
				(number "56")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PD3")
				(number "55")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PD4")
				(number "54")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PD5")
				(number "53")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PD6")
				(number "51")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PD7")
				(number "50")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PD8")
				(number "49")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PD9")
				(number "48")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PD10")
				(number "44")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PD11")
				(number "43")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PD12")
				(number "41")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PD21")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PD22")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PD24")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PD25")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "PD26")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "PD31")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAME70N21A-AN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 76.2 0)
		)
		(property "Value" "ATSAME70N21A-AN"
			(at -15.24 -76.2 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 35.56 76.2 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM-E70-S70-V70-V71-Family-Data-Sheet-DS60001527D.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM E70 Microchip SMART ARM Cortex-M7-based MCU, 2048K Flash, 384K SRAM, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M7 MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAME70N21A-AN_0_1")
		(symbol "ATSAME70N21A-AN_1_1"
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "PA0")
				(number "72")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PA1")
				(number "70")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PA2")
				(number "66")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PA3")
				(number "64")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PA4")
				(number "55")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PA5")
				(number "52")
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PA7")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PA8")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PA9")
				(number "54")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PA10")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PA11")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PA12")
				(number "48")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PA13")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PA14")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PA15")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PA16")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PA17")
				(number "16")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PA18")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PA19")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PA20")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PA21")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PA22")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PA23")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PA24")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PA25")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PA26")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PA27")
				(number "50")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PA28")
				(number "79")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PA30")
				(number "82")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PA31")
				(number "83")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PB0")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PB1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PB2")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PB3")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PB4")
				(number "74")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PB5")
				(number "77")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PB6")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PB7")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PB8")
				(number "98")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PB9")
				(number "99")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PB12")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PB13")
				(number "100")
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "HSDP")
				(number "95")
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "HSDM")
				(number "94")
			)
			(pin input line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "VBG")
				(number "97")
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "NRST")
				(number "58")
			)
			(pin input line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "TST")
				(number "60")
			)
			(pin input line
				(at -30.48 -60.96 0)
				(length 5.08)
				(name "JTAGSEL")
				(number "73")
			)
			(pin input line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "VREFP")
				(number "9")
			)
			(pin input line
				(at -30.48 -68.58 0)
				(length 5.08)
				(name "VREFN")
				(number "6")
			)
			(pin power_in line
				(at -10.16 78.74 270)
				(length 5.08)
				(name "VDDCORE")
				(number "18")
			)
			(pin passive line
				(at -10.16 78.74 270)
				(length 5.08)
				(hide yes)
				(name "VDDCORE")
				(number "22")
			)
			(pin passive line
				(at -10.16 78.74 270)
				(length 5.08)
				(hide yes)
				(name "VDDCORE")
				(number "39")
			)
			(pin passive line
				(at -10.16 78.74 270)
				(length 5.08)
				(hide yes)
				(name "VDDCORE")
				(number "76")
			)
			(pin power_in line
				(at -5.08 78.74 270)
				(length 5.08)
				(name "VDDIO")
				(number "19")
			)
			(pin passive line
				(at -5.08 78.74 270)
				(length 5.08)
				(hide yes)
				(name "VDDIO")
				(number "28")
			)
			(pin passive line
				(at -5.08 78.74 270)
				(length 5.08)
				(hide yes)
				(name "VDDIO")
				(number "68")
			)
			(pin passive line
				(at -5.08 78.74 270)
				(length 5.08)
				(hide yes)
				(name "VDDIO")
				(number "81")
			)
			(pin power_out line
				(at 0 78.74 270)
				(length 5.08)
				(name "VDDOUT")
				(number "4")
			)
			(pin passive line
				(at 0 -78.74 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -78.74 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -78.74 90)
				(length 5.08)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -78.74 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "67")
			)
			(pin passive line
				(at 0 -78.74 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -78.74 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at 2.54 78.74 270)
				(length 5.08)
				(name "VDDIN")
				(number "5")
			)
			(pin power_in line
				(at 5.08 78.74 270)
				(length 5.08)
				(name "VDDPLL")
				(number "86")
			)
			(pin power_in line
				(at 7.62 78.74 270)
				(length 5.08)
				(name "VDDUTMIC")
				(number "96")
			)
			(pin power_in line
				(at 10.16 78.74 270)
				(length 5.08)
				(name "VDDUTMII")
				(number "93")
			)
			(pin power_in line
				(at 12.7 78.74 270)
				(length 5.08)
				(name "VDDPLLUSB")
				(number "90")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PD0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PD1")
				(number "92")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PD2")
				(number "91")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PD3")
				(number "89")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PD4")
				(number "88")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PD5")
				(number "87")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PD6")
				(number "85")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PD7")
				(number "84")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PD8")
				(number "80")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PD9")
				(number "78")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PD10")
				(number "71")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PD11")
				(number "69")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PD12")
				(number "65")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PD13")
				(number "62")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PD14")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PD15")
				(number "75")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PD16")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PD17")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PD18")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PD19")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PD20")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PD21")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PD22")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PD24")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PD25")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PD26")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PD27")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PD28")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PD30")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PD31")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAME70Q21A-AN"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 88.9 0)
		)
		(property "Value" "ATSAME70Q21A-AN"
			(at -12.7 -88.9 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at 35.56 88.9 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM-E70-S70-V70-V71-Family-Data-Sheet-DS60001527D.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM E70 Microchip SMART ARM Cortex-M7-based MCU, 2048K Flash, 384K SRAM, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M7 MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAME70Q21A-AN_0_1")
		(symbol "ATSAME70Q21A-AN_1_1"
			(pin bidirectional line
				(at -30.48 81.28 0)
				(length 5.08)
				(name "PA0")
				(number "102")
			)
			(pin bidirectional line
				(at -30.48 78.74 0)
				(length 5.08)
				(name "PA1")
				(number "99")
			)
			(pin bidirectional line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "PA2")
				(number "93")
			)
			(pin bidirectional line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "PA3")
				(number "91")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "PA4")
				(number "77")
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "PA5")
				(number "73")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PA6")
				(number "114")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PA7")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PA8")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PA9")
				(number "75")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PA10")
				(number "66")
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PA11")
				(number "64")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PA12")
				(number "68")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PA13")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PA14")
				(number "51")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PA15")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PA16")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PA17")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PA18")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PA19")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PA20")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PA21")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PA22")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PA23")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PA24")
				(number "56")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PA25")
				(number "59")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PA26")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PA27")
				(number "70")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PA28")
				(number "112")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PA29")
				(number "129")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PA30")
				(number "116")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PA31")
				(number "118")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PB0")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PB1")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PB2")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PB3")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PB4")
				(number "105")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PB5")
				(number "109")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PB6")
				(number "79")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PB7")
				(number "89")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PB8")
				(number "141")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PB9")
				(number "142")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PB12")
				(number "87")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PB13")
				(number "144")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PE0")
				(number "4")
			)
			(pin bidirectional line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "PE1")
				(number "6")
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PE2")
				(number "7")
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PE3")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "PE4")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 -48.26 0)
				(length 5.08)
				(name "PE5")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "HSDP")
				(number "137")
			)
			(pin bidirectional line
				(at -30.48 -55.88 0)
				(length 5.08)
				(name "HSDM")
				(number "136")
			)
			(pin input line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "VBG")
				(number "140")
			)
			(pin bidirectional line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "NRST")
				(number "83")
			)
			(pin input line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "TST")
				(number "85")
			)
			(pin input line
				(at -30.48 -71.12 0)
				(length 5.08)
				(name "JTAGSEL")
				(number "104")
			)
			(pin input line
				(at -30.48 -76.2 0)
				(length 5.08)
				(name "VREFP")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -78.74 0)
				(length 5.08)
				(name "VREFN")
				(number "8")
			)
			(pin passive line
				(at -10.16 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDDCORE")
				(number "107")
			)
			(pin power_in line
				(at -10.16 91.44 270)
				(length 5.08)
				(name "VDDCORE")
				(number "29")
			)
			(pin passive line
				(at -10.16 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDDCORE")
				(number "33")
			)
			(pin passive line
				(at -10.16 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDDCORE")
				(number "50")
			)
			(pin passive line
				(at -10.16 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDDCORE")
				(number "81")
			)
			(pin power_in line
				(at -5.08 91.44 270)
				(length 5.08)
				(name "VDDIO")
				(number "30")
			)
			(pin passive line
				(at -5.08 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDDIO")
				(number "43")
			)
			(pin passive line
				(at -5.08 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDDIO")
				(number "72")
			)
			(pin passive line
				(at -5.08 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDDIO")
				(number "80")
			)
			(pin passive line
				(at -5.08 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDDIO")
				(number "96")
			)
			(pin power_out line
				(at 0 91.44 270)
				(length 5.08)
				(name "VDDOUT")
				(number "3")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "115")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "135")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "138")
			)
			(pin power_in line
				(at 0 -91.44 90)
				(length 5.08)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 0 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "GND")
				(number "95")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDDIN")
				(number "5")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VDDPLL")
				(number "123")
			)
			(pin power_in line
				(at 7.62 91.44 270)
				(length 5.08)
				(name "VDDUTMIC")
				(number "139")
			)
			(pin power_in line
				(at 10.16 91.44 270)
				(length 5.08)
				(name "VDDUTMII")
				(number "134")
			)
			(pin power_in line
				(at 12.7 91.44 270)
				(length 5.08)
				(name "VDDPLLUSB")
				(number "143")
			)
			(pin bidirectional line
				(at 30.48 81.28 180)
				(length 5.08)
				(name "PC0")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 78.74 180)
				(length 5.08)
				(name "PC1")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PC2")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PC3")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PC4")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PC5")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PC6")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PC7")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PC8")
				(number "82")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PC9")
				(number "86")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PC10")
				(number "90")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PC11")
				(number "94")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PC12")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PC13")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PC14")
				(number "97")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PC15")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PC16")
				(number "100")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PC17")
				(number "103")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PC18")
				(number "111")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PC19")
				(number "117")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PC20")
				(number "120")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PC21")
				(number "122")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PC22")
				(number "124")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PC23")
				(number "127")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PC24")
				(number "130")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PC25")
				(number "133")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PC26")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PC27")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PC28")
				(number "76")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PC29")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PC30")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PC31")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PD0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PD1")
				(number "132")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PD2")
				(number "131")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PD3")
				(number "128")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PD4")
				(number "126")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PD5")
				(number "125")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PD6")
				(number "121")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PD7")
				(number "119")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PD8")
				(number "113")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PD9")
				(number "110")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PD10")
				(number "101")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PD11")
				(number "98")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PD12")
				(number "92")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PD13")
				(number "88")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PD14")
				(number "84")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PD15")
				(number "106")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PD16")
				(number "78")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PD17")
				(number "74")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PD18")
				(number "69")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PD19")
				(number "67")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PD20")
				(number "65")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PD21")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PD22")
				(number "60")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PD23")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PD24")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PD25")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PD26")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PD27")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PD28")
				(number "71")
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PD29")
				(number "108")
			)
			(pin bidirectional line
				(at 30.48 -78.74 180)
				(length 5.08)
				(name "PD30")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 -81.28 180)
				(length 5.08)
				(name "PD31")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAME51J19A-A"
		(extends "ATSAME51J18A-A")
		(property "Reference" "U"
			(at -17.78 48.26 0)
		)
		(property "Value" "ATSAME51J19A-A"
			(at -12.7 -48.26 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 33.02 48.26 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001507E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM E51 Microchip SMART ARM Cortex-M4F-based MCU, 512K Flash, 192K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4F MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAME51J20A-A"
		(extends "ATSAME51J18A-A")
		(property "Reference" "U"
			(at -17.78 48.26 0)
		)
		(property "Value" "ATSAME51J20A-A"
			(at -12.7 -48.26 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 33.02 48.26 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001507E.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM E51 Microchip SMART ARM Cortex-M4F-based MCU, 1024K Flash, 256K SRAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4F MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAME53J19A-M"
		(extends "ATSAME53J18A-M")
		(property "Reference" "U"
			(at -11.43 44.45 0)
		)
		(property "Value" "ATSAME53J19A-M"
			(at 16.51 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 15.24 25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001507E.pdf"
			(at 15.24 25.4 0)
		)
		(property "Description" "SAM E53 Microchip SMART ARM Cortex-M4F based MCU, 512K Flash, 128K SRAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4F MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAME53J20A-M"
		(extends "ATSAME53J18A-M")
		(property "Reference" "U"
			(at -11.43 44.45 0)
		)
		(property "Value" "ATSAME53J20A-M"
			(at 16.51 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 15.24 25.4 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/60001507E.pdf"
			(at 15.24 25.4 0)
		)
		(property "Description" "SAM E53 Microchip SMART ARM Cortex-M4F based MCU, 1024K Flash, 128K SRAM, QFN-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M4F MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAME70J19A-AN"
		(extends "ATSAME70J21A-AN")
		(property "Reference" "U"
			(at -17.78 53.34 0)
		)
		(property "Value" "ATSAME70J19A-AN"
			(at -12.7 -53.34 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 33.02 53.34 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM-E70-S70-V70-V71-Family-Data-Sheet-DS60001527D.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM E70 Microchip SMART ARM Cortex-M7-based MCU, 2048K Flash, 384K SRAM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M7 MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAME70J20A-AN"
		(extends "ATSAME70J21A-AN")
		(property "Reference" "U"
			(at -17.78 53.34 0)
		)
		(property "Value" "ATSAME70J20A-AN"
			(at -12.7 -53.34 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 33.02 53.34 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM-E70-S70-V70-V71-Family-Data-Sheet-DS60001527D.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM E70 Microchip SMART ARM Cortex-M7-based MCU, 512K Flash, 384K SRAM, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M7 MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAME70N19A-AN"
		(extends "ATSAME70N21A-AN")
		(property "Reference" "U"
			(at -22.86 76.2 0)
		)
		(property "Value" "ATSAME70N19A-AN"
			(at -15.24 -76.2 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 35.56 76.2 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM-E70-S70-V70-V71-Family-Data-Sheet-DS60001527D.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM E70 Microchip SMART ARM Cortex-M7-based MCU, 512K Flash, 256K SRAM, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M7 MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAME70N20A-AN"
		(extends "ATSAME70N21A-AN")
		(property "Reference" "U"
			(at -22.86 76.2 0)
		)
		(property "Value" "ATSAME70N20A-AN"
			(at -15.24 -76.2 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 35.56 76.2 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM-E70-S70-V70-V71-Family-Data-Sheet-DS60001527D.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM E70 Microchip SMART ARM Cortex-M7-based MCU, 1024K Flash, 384K SRAM, LQFP100"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M7 MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAME70Q19A-AN"
		(extends "ATSAME70Q21A-AN")
		(property "Reference" "U"
			(at -22.86 88.9 0)
		)
		(property "Value" "ATSAME70Q19A-AN"
			(at -12.7 -88.9 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at 35.56 88.9 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM-E70-S70-V70-V71-Family-Data-Sheet-DS60001527D.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM E70 Microchip SMART ARM Cortex-M7-based MCU, 512K Flash, 256K SRAM, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M7 MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAME70Q20A-AN"
		(extends "ATSAME70Q21A-AN")
		(property "Reference" "U"
			(at -22.86 88.9 0)
		)
		(property "Value" "ATSAME70Q20A-AN"
			(at -12.7 -88.9 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at 35.56 88.9 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/SAM-E70-S70-V70-V71-Family-Data-Sheet-DS60001527D.pdf"
			(at 0 0 0)
		)
		(property "Description" "SAM E70 Microchip SMART ARM Cortex-M7-based MCU, 1024K Flash, 384K SRAM, LQFP144"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M7 MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
