(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "ATSAML21E15B-AUT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 22.86 0)
		)
		(property "Value" "ATSAML21E15B-AUT"
			(at -12.7 -22.86 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 2.54 -22.86 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 2.54 -25.4 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash, 4K SRAM, TQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "ATSAML21E15B-AUT_0_1")
		(symbol "ATSAML21E15B-AUT_1_1"
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA04")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA05")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA06")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA07")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA08")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA09")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA10")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA11")
				(number "14")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "26")
			)
			(pin power_in line
				(at -7.62 22.86 270)
				(length 2.54)
				(name "VDDANA")
				(number "9")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDCORE")
				(number "27")
			)
			(pin power_out line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VSW")
				(number "29")
			)
			(pin power_in line
				(at 7.62 22.86 270)
				(length 2.54)
				(name "VDDIN")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA16")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA17")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA18")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA19")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA22")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA23")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA24")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA25")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA27")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA30")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PA31")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAML21E15B-MUT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 22.86 0)
		)
		(property "Value" "ATSAML21E15B-MUT"
			(at -12.7 -22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 2.54 -22.86 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 2.54 -25.4 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 32K Flash, 4K SRAM, QFN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAML21E15B-MUT_0_1")
		(symbol "ATSAML21E15B-MUT_1_1"
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA04")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA05")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA06")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA07")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA08")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA09")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA10")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA11")
				(number "14")
			)
			(pin input line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "~{RESET}")
				(number "26")
			)
			(pin power_in line
				(at -7.62 22.86 270)
				(length 2.54)
				(name "VDDANA")
				(number "9")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -22.86 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at 2.54 22.86 270)
				(length 2.54)
				(name "VDDCORE")
				(number "27")
			)
			(pin power_out line
				(at 5.08 22.86 270)
				(length 2.54)
				(name "VSW")
				(number "29")
			)
			(pin power_in line
				(at 7.62 22.86 270)
				(length 2.54)
				(name "VDDIN")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PA14")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PA15")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PA16")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PA17")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PA18")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PA19")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PA22")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PA23")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PA24")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PA25")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PA27")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PA30")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PA31")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAML21G16B-AUT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 45.72 0)
		)
		(property "Value" "ATSAML21G16B-AUT"
			(at -15.24 -45.72 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 5.08 -45.72 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 5.08 -48.26 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, TQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAML21G16B-AUT_0_1")
		(symbol "ATSAML21G16B-AUT_1_1"
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA04")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA05")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA06")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA07")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA08")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA09")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA10")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA11")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA12")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA13")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA14")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA15")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA16")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA17")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA18")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA19")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA20")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA21")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA22")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA23")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA24")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PA25")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA27")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA30")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PA31")
				(number "46")
			)
			(pin input line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "~{RESET}")
				(number "40")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDDANA")
				(number "6")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "17")
			)
			(pin passive line
				(at -2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDDIO")
				(number "36")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "GNDANA")
				(number "5")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDCORE")
				(number "41")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin power_out line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VSW")
				(number "43")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDIN")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB02")
				(number "47")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB03")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB08")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB09")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB10")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB11")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB22")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB23")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAML21G16B-MUT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 45.72 0)
		)
		(property "Value" "ATSAML21G16B-MUT"
			(at -15.24 -45.72 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 5.08 -45.72 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 5.08 -48.26 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, QFN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAML21G16B-MUT_0_1")
		(symbol "ATSAML21G16B-MUT_1_1"
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA04")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA05")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA06")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA07")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA08")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA09")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA10")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA11")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA12")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA13")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA14")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA15")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA16")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA17")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA18")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA19")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA20")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA21")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA22")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA23")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA24")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PA25")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA27")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA30")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PA31")
				(number "46")
			)
			(pin input line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "~{RESET}")
				(number "40")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDDANA")
				(number "6")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "17")
			)
			(pin passive line
				(at -2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDDIO")
				(number "36")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "GNDANA")
				(number "5")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDCORE")
				(number "41")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin power_out line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VSW")
				(number "43")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDIN")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB02")
				(number "47")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB03")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB08")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB09")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB10")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB11")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB22")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB23")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAML21J16B-AUT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 45.72 0)
		)
		(property "Value" "ATSAML21J16B-AUT"
			(at -15.24 -45.72 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 5.08 -45.72 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 5.08 -48.26 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, TQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*64*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAML21J16B-AUT_0_1")
		(symbol "ATSAML21J16B-AUT_1_1"
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA04")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA05")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA06")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA07")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA08")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA09")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA10")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA11")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA12")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA13")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA14")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA15")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA16")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA17")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA18")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA19")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA20")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA21")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA22")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA23")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA24")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PA25")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA27")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA30")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PA31")
				(number "58")
			)
			(pin input line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "~{RESET}")
				(number "52")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDDANA")
				(number "8")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "21")
			)
			(pin passive line
				(at -2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDDIO")
				(number "34")
			)
			(pin passive line
				(at -2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDDIO")
				(number "48")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "GNDANA")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDCORE")
				(number "53")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin power_out line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VSW")
				(number "55")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDIN")
				(number "56")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PB00")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PB01")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB02")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB03")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB04")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PB05")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PB06")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB07")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB08")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB09")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB10")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB11")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB12")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB13")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB14")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB15")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB16")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB17")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB22")
				(number "49")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB23")
				(number "50")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB30")
				(number "59")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB31")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAML21J16B-MUT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 45.72 0)
		)
		(property "Value" "ATSAML21J16B-MUT"
			(at -15.24 -45.72 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 5.08 -45.72 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 5.08 -48.26 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, QFN64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "ATSAML21J16B-MUT_0_1")
		(symbol "ATSAML21J16B-MUT_1_1"
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PA00")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PA01")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PA02")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PA03")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PA04")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PA05")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PA06")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PA07")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PA08")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PA09")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PA10")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PA11")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PA12")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PA13")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PA14")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PA15")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PA16")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PA17")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PA18")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PA19")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PA20")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PA21")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PA22")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PA23")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PA24")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PA25")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PA27")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PA30")
				(number "57")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PA31")
				(number "58")
			)
			(pin input line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "~{RESET}")
				(number "52")
			)
			(pin power_in line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDDANA")
				(number "8")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "21")
			)
			(pin passive line
				(at -2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDDIO")
				(number "34")
			)
			(pin passive line
				(at -2.54 45.72 270)
				(length 2.54)
				(hide yes)
				(name "VDDIO")
				(number "48")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "GNDANA")
				(number "7")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDCORE")
				(number "53")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "54")
			)
			(pin passive line
				(at 2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "65")
			)
			(pin power_out line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VSW")
				(number "55")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDDIN")
				(number "56")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PB00")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PB01")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PB02")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PB03")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PB04")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PB05")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PB06")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PB07")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PB08")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PB09")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PB10")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PB11")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PB12")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PB13")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PB14")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PB15")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PB16")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PB17")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PB22")
				(number "49")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "PB23")
				(number "50")
			)
			(pin bidirectional line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "PB30")
				(number "59")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 2.54)
				(name "PB31")
				(number "60")
			)
		)
		(embedded_fonts no)
	)
	(symbol "ATSAML21E16B-AUT"
		(extends "ATSAML21E15B-AUT")
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "ATSAML21E16B-AUT"
			(at -12.7 -22.86 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 2.54 -22.86 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 2.54 -25.4 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, TQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAML21E16B-MUT"
		(extends "ATSAML21E15B-MUT")
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "ATSAML21E16B-MUT"
			(at -12.7 -22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 2.54 -22.86 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 2.54 -25.4 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, QFN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAML21E17B-AUT"
		(extends "ATSAML21E15B-AUT")
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "ATSAML21E17B-AUT"
			(at -12.7 -22.86 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 2.54 -22.86 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 2.54 -25.4 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash, 16K SRAM, TQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAML21E17B-MUT"
		(extends "ATSAML21E15B-MUT")
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "ATSAML21E17B-MUT"
			(at -12.7 -22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 2.54 -22.86 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 2.54 -25.4 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash, 16K SRAM, QFN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAML21E18B-AUT"
		(extends "ATSAML21E15B-AUT")
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "ATSAML21E18B-AUT"
			(at -12.7 -22.86 0)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 2.54 -22.86 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 2.54 -25.4 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 256K Flash, 32K SRAM, TQFP32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAML21E18B-MUT"
		(extends "ATSAML21E15B-MUT")
		(property "Reference" "U"
			(at -17.78 22.86 0)
		)
		(property "Value" "ATSAML21E18B-MUT"
			(at -12.7 -22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 2.54 -22.86 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 2.54 -25.4 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 256K Flash, 32K SRAM, QFN32"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAML21G17B-AUT"
		(extends "ATSAML21G16B-AUT")
		(property "Reference" "U"
			(at -17.78 45.72 0)
		)
		(property "Value" "ATSAML21G17B-AUT"
			(at -15.24 -45.72 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 5.08 -45.72 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 5.08 -48.26 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash, 16K SRAM, TQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAML21G17B-MUT"
		(extends "ATSAML21G16B-MUT")
		(property "Reference" "U"
			(at -17.78 45.72 0)
		)
		(property "Value" "ATSAML21G17B-MUT"
			(at -15.24 -45.72 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 5.08 -45.72 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 5.08 -48.26 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash, 16K SRAM, QFN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAML21G18B-AUT"
		(extends "ATSAML21G16B-AUT")
		(property "Reference" "U"
			(at -17.78 45.72 0)
		)
		(property "Value" "ATSAML21G18B-AUT"
			(at -15.24 -45.72 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48_7x7mm_P0.5mm"
			(at 5.08 -45.72 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 5.08 -48.26 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 256K Flash, 32K SRAM, TQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAML21G18B-MUT"
		(extends "ATSAML21G16B-MUT")
		(property "Reference" "U"
			(at -17.78 45.72 0)
		)
		(property "Value" "ATSAML21G18B-MUT"
			(at -15.24 -45.72 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 5.08 -45.72 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 5.08 -48.26 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 256K Flash, 32K SRAM, QFN48"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAML21J17B-AUT"
		(extends "ATSAML21J16B-AUT")
		(property "Reference" "U"
			(at -17.78 45.72 0)
		)
		(property "Value" "ATSAML21J17B-AUT"
			(at -15.24 -45.72 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 5.08 -45.72 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 5.08 -48.26 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 128K Flash, 16K SRAM, TQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*64*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAML21J17B-MUT"
		(extends "ATSAML21J16B-MUT")
		(property "Reference" "U"
			(at -17.78 45.72 0)
		)
		(property "Value" "ATSAML21J17B-MUT"
			(at -15.24 -45.72 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 5.08 -45.72 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 5.08 -48.26 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, QFN64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAML21J18B-AUT"
		(extends "ATSAML21J16B-AUT")
		(property "Reference" "U"
			(at -17.78 45.72 0)
		)
		(property "Value" "ATSAML21J18B-AUT"
			(at -15.24 -45.72 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 5.08 -45.72 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 5.08 -48.26 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 256K Flash, 32K SRAM, TQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*64*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "ATSAML21J18B-MUT"
		(extends "ATSAML21J16B-MUT")
		(property "Reference" "U"
			(at -17.78 45.72 0)
		)
		(property "Value" "ATSAML21J18B-MUT"
			(at -15.24 -45.72 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-64-1EP_9x9mm_P0.5mm_EP4.7x4.7mm"
			(at 5.08 -45.72 0)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/aemDocuments/documents/MCU32/ProductDocuments/DataSheets/SAM-L21-Family-Data-Sheet-DS60001477.pdf"
			(at 5.08 -48.26 0)
		)
		(property "Description" "SAM L21 Microchip SMART ARM-based Flash MCU, 48Mhz, 64K Flash, 8K SRAM, QFN64"
			(at 0 0 0)
		)
		(property "ki_keywords" "32-bit ARM Cortex-M0+ MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*9x9mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
