(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "Adafruit_Feather_32u4_BluefruitLE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -10.16 28.575 0)
		)
		(property "Value" "Adafruit_Feather_32u4_BluefruitLE"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Module:Adafruit_Feather"
			(at 2.54 -34.29 0)
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-feather-32u4-bluefruit-le.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Microcontroller module with ATmega32u4 MCU and bluetooth"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adafruit feather microcontroller module USB AVR ATmega32U4  Bluetooth BLE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Adafruit*Feather*"
			(at 0 0 0)
		)
		(symbol "Adafruit_Feather_32u4_BluefruitLE_0_1")
		(symbol "Adafruit_Feather_32u4_BluefruitLE_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D5")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D6")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D9")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D10")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D11")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D12")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D13")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCK/D15")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MOSI/D16")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "MISO/D14")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RX/D0")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "TX/D1")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "SDA/D2")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "SCL/D3")
				(number "18")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VBAT")
				(number "28")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "3V3")
				(number "2")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "USB")
				(number "26")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "~{DFU}")
				(number "16")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "EN")
				(number "27")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "AREF")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "A2")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A3")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A4")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A5")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Adafruit_Feather_Generic"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -10.16 29.21 0)
		)
		(property "Value" "Adafruit_Feather_Generic"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Module:Adafruit_Feather"
			(at 2.54 -34.29 0)
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-feather.pdf"
			(at 0 -20.32 0)
		)
		(property "Description" "Microcontroller module in various flavor, generic symbol"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adafruit feather microcontroller module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Adafruit*Feather*"
			(at 0 0 0)
		)
		(symbol "Adafruit_Feather_Generic_0_1")
		(symbol "Adafruit_Feather_Generic_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D0")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D1")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D2")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D3")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D4")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D5")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D6")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "SPARE")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCK")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MOSI")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "MISO")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RX")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "TX")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "SDA")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "SCL")
				(number "18")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VBAT")
				(number "28")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "3V3")
				(number "2")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "USB")
				(number "26")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "EN")
				(number "27")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "AREF")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "A0")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "A2")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A3")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A4")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A5")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Adafruit_Feather_HUZZAH32_ESP32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -10.16 29.21 0)
		)
		(property "Value" "Adafruit_Feather_HUZZAH32_ESP32"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Module:Adafruit_Feather"
			(at 2.54 -34.29 0)
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-huzzah32-esp32-feather.pdf"
			(at 0 -30.48 0)
		)
		(property "Description" "Microcontroller module with ESP32 MCU"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adafruit feather microcontroller module USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Adafruit*Feather*"
			(at 0 0 0)
		)
		(symbol "Adafruit_Feather_HUZZAH32_ESP32_0_1")
		(symbol "Adafruit_Feather_HUZZAH32_ESP32_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "A6/IO14")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "A7/IO32")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A8/IO15")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "A9/IO33")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A10/IO27")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "A11/IO12")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "A12/IO13")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "IO21")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCK/IO5")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MOSI/IO18")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "MISO/IO19")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RX/IO16")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "TX/IO17")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "SDA/IO23")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "SCL/IO22")
				(number "18")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VBAT")
				(number "28")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "3V3")
				(number "2")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "USB")
				(number "26")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "EN")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DAC2/A0")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "DAC1/A1")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "I34/A2")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "I39/A3")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "IO36/A4")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "IO4/A5")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Adafruit_Feather_HUZZAH_ESP8266"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -10.16 29.21 0)
		)
		(property "Value" "Adafruit_Feather_HUZZAH_ESP8266"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Module:Adafruit_Feather"
			(at 2.54 -34.29 0)
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-feather-huzzah-esp8266.pdf"
			(at 0 -30.48 0)
		)
		(property "Description" "Microcontroller module with ESP8266 MCU"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adafruit feather microcontroller module USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Adafruit*Feather*"
			(at 0 0 0)
		)
		(symbol "Adafruit_Feather_HUZZAH_ESP8266_0_1")
		(symbol "Adafruit_Feather_HUZZAH_ESP8266_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "IO2")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "IO16")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "IO0")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "IO15")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "IO13/MOSI")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "IO12/MISO")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "IO14/SCK")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCK/IO14")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MOSI/IO13")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "MISO/IO12")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RX/IO3")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "TX/IO1")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "SDA/IO4")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "SCL/IO5")
				(number "18")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VBAT")
				(number "28")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "3V3")
				(number "2")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "USB")
				(number "26")
			)
			(pin no_connect line
				(at 10.16 10.16 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "3")
			)
			(pin no_connect line
				(at 10.16 2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 10.16 0 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "7")
			)
			(pin no_connect line
				(at 10.16 -2.54 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 10.16 -5.08 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at 10.16 -7.62 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "CH_PD")
				(number "16")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "EN")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "ADC")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Adafruit_Feather_M0_Basic_Proto"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -10.16 29.21 0)
		)
		(property "Value" "Adafruit_Feather_M0_Basic_Proto"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Module:Adafruit_Feather"
			(at 2.54 -34.29 0)
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-feather-m0-basic-proto.pdf"
			(at 0 -30.48 0)
		)
		(property "Description" "Microcontroller module with SAMD21 Cortex-M0 MCU"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adafruit feather microcontroller module USB M0 SAMD21"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Adafruit*Feather*"
			(at 0 0 0)
		)
		(symbol "Adafruit_Feather_M0_Basic_Proto_0_1")
		(symbol "Adafruit_Feather_M0_Basic_Proto_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D5")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D6")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D9")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D10")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D11")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D12")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D13")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCK/D24")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MOSI/D23")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "MISO/D22")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RX/D0")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "TX/D1")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "SDA/D20")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "SCL/D21")
				(number "18")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VBAT")
				(number "28")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "3V3")
				(number "2")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "USB")
				(number "26")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "EN")
				(number "27")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "AREF")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DAC0/A0")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "A2")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A3")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A4")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A5")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Adafruit_Feather_M0_BluefruitLE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -10.16 28.575 0)
		)
		(property "Value" "Adafruit_Feather_M0_BluefruitLE"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Module:Adafruit_Feather"
			(at 2.54 -34.29 0)
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-feather-m0-bluefruit-le.pdf"
			(at 0 5.08 0)
		)
		(property "Description" "Microcontroller module with SAMD21 Cortex-M0 MCU and bluetooth"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adafruit feather microcontroller module USB M0 SAMD21 Bluetooth BLE"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Adafruit*Feather*"
			(at 0 0 0)
		)
		(symbol "Adafruit_Feather_M0_BluefruitLE_0_1")
		(symbol "Adafruit_Feather_M0_BluefruitLE_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D5")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D6")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D9")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D10")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D11")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D12")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D13")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCK/D24")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MOSI/D23")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "MISO/D22")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RX/D0")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "TX/D1")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "SDA/D20")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "SCL/D21")
				(number "18")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VBAT")
				(number "28")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "3V3")
				(number "2")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "USB")
				(number "26")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "~{DFU}")
				(number "16")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "EN")
				(number "27")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "AREF")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DAC0/A0")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "A2")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A3")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A4")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A5")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Adafruit_Feather_M0_RFM69HCW_Packet_Radio"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -10.16 29.21 0)
		)
		(property "Value" "Adafruit_Feather_M0_RFM69HCW_Packet_Radio"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Module:Adafruit_Feather_M0_RFM"
			(at 2.54 -34.29 0)
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-feather-m0-radio-with-rfm69-packet-radio.pdf"
			(at 0 -20.32 0)
		)
		(property "Description" "Microcontroller module with SAMD21 Cortex-M0 MCU and RFM69HCW Radio"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adafruit feather microcontroller module USB M0 SAMD21 Radio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Adafruit*Feather*"
			(at 0 0 0)
		)
		(symbol "Adafruit_Feather_M0_RFM69HCW_Packet_Radio_0_1")
		(symbol "Adafruit_Feather_M0_RFM69HCW_Packet_Radio_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D5")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D6")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D9")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D10")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D11")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D12")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D13")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCK/D24")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MOSI/D23")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "MISO/D22")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RX/D0")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "TX/D1")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "SDA/D20")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "SCL/D21")
				(number "18")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VBAT")
				(number "28")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "3V3")
				(number "2")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "USB")
				(number "26")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "EN")
				(number "27")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "AREF")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DAC0/A0")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "A2")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A3")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A4")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A5")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "DIO1")
				(number "16")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "DIO2")
				(number "32")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "DIO3")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "DIO5")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 -22.86 180)
				(length 2.54)
				(name "ANT")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Adafruit_Feather_M0_Wifi"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -10.16 29.21 0)
		)
		(property "Value" "Adafruit_Feather_M0_Wifi"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Module:Adafruit_Feather_M0_Wifi"
			(at 2.54 -34.29 0)
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-feather-m0-wifi-atwinc1500.pdf"
			(at 0 -20.32 0)
		)
		(property "Description" "Microcontroller module with SAMD21 Cortex-M0 MCU and ATWINC1500 Wifi"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adafruit feather microcontroller module USB M0 SAMD21 Wifi ATWINC1500"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Adafruit*Feather*"
			(at 0 0 0)
		)
		(symbol "Adafruit_Feather_M0_Wifi_0_1")
		(symbol "Adafruit_Feather_M0_Wifi_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "D5")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "D6")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D9")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D10")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D11")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D12")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D13")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCK/D24")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MOSI/D23")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "MISO/D22")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RX/D0")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "TX/D1")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "SDA/D20")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "SCL/D21")
				(number "18")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VBAT")
				(number "28")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "3V3")
				(number "2")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "USB")
				(number "26")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin input line
				(at 12.7 17.78 180)
				(length 2.54)
				(name "WAKE")
				(number "16")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "EN")
				(number "27")
			)
			(pin input line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "AREF")
				(number "3")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "DAC0/A0")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "A1")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "A2")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A3")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A4")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A5")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Adafruit_Feather_WICED_Wifi"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -8.89 31.75 0)
		)
		(property "Value" "Adafruit_Feather_WICED_Wifi"
			(at -8.89 29.21 0)
		)
		(property "Footprint" "Module:Adafruit_Feather_WICED"
			(at 1.27 -31.75 0)
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/introducing-the-adafruit-wiced-feather-wifi.pdf"
			(at 0 -20.32 0)
		)
		(property "Description" "Microcontroller module with STM32F205 Cortex-M3 MCU and BCM43362 Wifi"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adafruit feather microcontroller module USB M3 STM32F205 Wifi"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Adafruit*Feather*"
			(at 0 0 0)
		)
		(symbol "Adafruit_Feather_WICED_Wifi_0_1")
		(symbol "Adafruit_Feather_WICED_Wifi_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "C5")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "C7")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "A15")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "B4/MISO3")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "A4/CS")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "B5/MOSI3")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "SCK/A5")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "MOSI/A7")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "MISO/A6")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "RX/A10")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "TX/A9")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -20.32 0)
				(length 2.54)
				(name "SDA/B7")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -22.86 0)
				(length 2.54)
				(name "SCL/B6")
				(number "18")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 2.54)
				(name "VRTC")
				(number "3")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "VBAT")
				(number "28")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "3V3")
				(number "2")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 2.54)
				(name "USB")
				(number "26")
			)
			(pin input line
				(at 12.7 20.32 180)
				(length 2.54)
				(name "~{RESET}")
				(number "1")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "EN")
				(number "27")
			)
			(pin bidirectional line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "WAKE/A0")
				(number "5")
			)
			(pin bidirectional line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "C3")
				(number "6")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "C2")
				(number "7")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A3")
				(number "8")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A2")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A1")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SWCLK")
				(number "29")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "SWDIO")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "SCK3/DFU")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Adafruit_HUZZAH_ESP8266_breakout"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at 7.62 19.05 0)
		)
		(property "Value" "Adafruit_HUZZAH_ESP8266_breakout"
			(at 3.81 -19.05 0)
		)
		(property "Footprint" ""
			(at 5.08 15.24 0)
		)
		(property "Datasheet" "https://www.adafruit.com/product/2471"
			(at 7.62 17.78 0)
		)
		(property "Description" "32-bit microcontroller module with WiFi"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESP8266 WiFi microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Adafruit*HUZZAH*ESP8266*breakout* Adafruit*HUZZAH*ESP8266*breakout*WithMountingHoles*"
			(at 0 0 0)
		)
		(symbol "Adafruit_HUZZAH_ESP8266_breakout_0_1")
		(symbol "Adafruit_HUZZAH_ESP8266_breakout_1_1"
			(pin input line
				(at -15.24 7.62 0)
				(length 3.81)
				(name "LDO")
				(number "12")
			)
			(pin input line
				(at -15.24 5.08 0)
				(length 3.81)
				(name "~{RST}")
				(number "1")
			)
			(pin input line
				(at -15.24 2.54 0)
				(length 3.81)
				(name "EN")
				(number "3")
			)
			(pin input line
				(at -15.24 -2.54 0)
				(length 3.81)
				(name "RX")
				(number "19")
			)
			(pin output line
				(at -15.24 -5.08 0)
				(length 3.81)
				(name "TX")
				(number "20")
			)
			(pin input line
				(at -15.24 -10.16 0)
				(length 3.81)
				(name "A")
				(number "2")
			)
			(pin power_in line
				(at -5.08 20.32 270)
				(length 3.81)
				(name "VBat")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 3.81)
				(name "V+")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 3.81)
				(name "GND")
				(number "11")
			)
			(pin power_out line
				(at 5.08 20.32 270)
				(length 3.81)
				(name "3V")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 3.81)
				(name "0")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 3.81)
				(name "2")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 3.81)
				(name "4")
				(number "17")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 3.81)
				(name "5")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 3.81)
				(name "12")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 3.81)
				(name "13")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 3.81)
				(name "14")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 3.81)
				(name "15")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 3.81)
				(name "16")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Arduino_Leonardo"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -10.16 23.495 0)
		)
		(property "Value" "Arduino_Leonardo"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Module:Arduino_UNO_R3"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.arduino.cc/en/Main/ArduinoBoardLeonardo"
			(at 0 0 0)
		)
		(property "Description" "Arduino LEONARDO Microcontroller Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arduino LEONARDO Microcontroller Module Atmel AVR USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Arduino*UNO*R3*"
			(at 0 0 0)
		)
		(symbol "Arduino_Leonardo_0_1")
		(symbol "Arduino_Leonardo_1_1"
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D0/RX")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D1/TX")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D2/SDA")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D3/SCL")
				(number "18")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D4")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "D5")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "D6")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "D7")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "D8")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "D9")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "D10")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "D11")
				(number "26")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "D12")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "D13")
				(number "28")
			)
			(pin no_connect line
				(at -10.16 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "3V3")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "+5V")
				(number "5")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IOREF")
				(number "2")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "AREF")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "A0")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A1")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A2")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A3")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "A4")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "A5")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "SDA/D2")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "SCL/D3")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Arduino_Nano_ESP32"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -14.986 23.622 0)
		)
		(property "Value" "Arduino_Nano_ESP32"
			(at 3.81 -25.654 0)
		)
		(property "Footprint" "Module:Arduino_Nano"
			(at 13.716 -34.036 0)
		)
		(property "Datasheet" "https://docs.arduino.cc/resources/datasheets/ABX00083-datasheet.pdf"
			(at 39.116 -31.496 0)
		)
		(property "Description" "Arduino Nano board based on the ESP32-S3 with a dual-core 240 MHz processor, 384 kB ROM, 512 kB SRAM. Operates at 3.3V, with 5V USB-C® input and 6-21V VIN. Features Wi-Fi®, Bluetooth® LE, digital and analog pins, and supports SPI, I2C, UART, I2S, and CAN."
			(at 138.43 -28.956 0)
		)
		(property "ki_keywords" "Arduino Nano ESP32"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Arduino*Nano*"
			(at 0 0 0)
		)
		(symbol "Arduino_Nano_ESP32_0_1")
		(symbol "Arduino_Nano_ESP32_1_1"
			(pin power_in line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "VIN")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "D0/RX")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "D1/TX")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "D2")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "D3")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "D4")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "D5")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "D6")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "D7")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "D8")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "D9")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "D10/CS")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "D11/COPI")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "D12/CIPO")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "D13/SCK")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "3V3")
				(number "17")
			)
			(pin power_out line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "VUSB/5V")
				(number "27")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "B0")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "B1")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "A0")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "A1")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "A2")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "A3")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "SDA/A4")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "SCL/A5")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "A6")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "A7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Arduino_Nano_Every"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -10.16 23.495 0)
		)
		(property "Value" "Arduino_Nano_Every"
			(at 5.08 -24.13 0)
		)
		(property "Footprint" "Module:Arduino_Nano"
			(at 0 0 0)
		)
		(property "Datasheet" "https://content.arduino.cc/assets/NANOEveryV3.0_sch.pdf"
			(at 0 0 0)
		)
		(property "Description" "Arduino Nano Every"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arduino nano microcontroller module USB UPDI AATMega4809 AVR"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Arduino*Nano*"
			(at 0 0 0)
		)
		(symbol "Arduino_Nano_Every_0_1")
		(symbol "Arduino_Nano_Every_1_1"
			(pin bidirectional line
				(at -12.7 20.32 0)
				(length 2.54)
				(name "TX1")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 17.78 0)
				(length 2.54)
				(name "RX1")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D2")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D3")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D4")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D5")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "D6")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "D7")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "D8")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "D9")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "D10")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "MOSI")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "MISO")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "SCK")
				(number "16")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VIN")
				(number "30")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "3V3")
				(number "17")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "+5V")
				(number "27")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{RESET}")
				(number "28")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "AREF")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "A0")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A1")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A2")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A3")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SDA/A4")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SCL/A5")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "A6")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "A7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Arduino_Nano_RP2040_Connect"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -14.986 23.622 0)
		)
		(property "Value" "Arduino_Nano_RP2040_Connect"
			(at 3.81 -25.654 0)
		)
		(property "Footprint" "Module:Arduino_Nano"
			(at 13.716 -34.036 0)
		)
		(property "Datasheet" "https://docs.arduino.cc/resources/datasheets/ABX00053-datasheet.pdf"
			(at 39.116 -31.496 0)
		)
		(property "Description" "Arduino Nano board based on the RP2040 microcontroller with a dual-core 133 MHz ARM Cortex-M0+ processor, 264 kB SRAM, and up to 16 MB flash memory. Operates at 3.3V, with 5V Micro USB input and 4-20V VIN. Features Wi-Fi®, Bluetooth® LE, digital and analog pins, and supports SPI, I2C, UART, and PIO. Includes a 6-axis IMU, RGB LED, microphone, and cryptographic chip for secure communication."
			(at 209.042 -28.956 0)
		)
		(property "ki_keywords" "Raspberry Pi MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Arduino*Nano*"
			(at 0 0 0)
		)
		(symbol "Arduino_Nano_RP2040_Connect_0_1")
		(symbol "Arduino_Nano_RP2040_Connect_1_1"
			(pin power_in line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "VIN")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "D0/RX")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "D1/TX")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "D2")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "D3")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "D4")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "D5")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "D6")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "D7")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "D8")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "D9")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "D10/CS")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "D11/COPI")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "D12/CIPO")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "D13/SCK")
				(number "16")
			)
			(pin passive line
				(at 0 -25.4 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "3V3")
				(number "17")
			)
			(pin power_out line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "VUSB/5V")
				(number "27")
			)
			(pin input line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "REF")
				(number "18")
			)
			(pin input line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "REC")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "A0")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "A1")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "A2")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "A3")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "SDA/A4")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "SCL/A5")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "A6")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "A7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Arduino_Nano_v2.x"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -10.16 23.495 0)
		)
		(property "Value" "Arduino_Nano_v2.x"
			(at 5.08 -24.13 0)
		)
		(property "Footprint" "Module:Arduino_Nano"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.arduino.cc/en/uploads/Main/ArduinoNanoManual23.pdf"
			(at 0 0 0)
		)
		(property "Description" "Arduino Nano v2.x"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arduino nano microcontroller module USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Arduino*Nano*"
			(at 0 0 0)
		)
		(symbol "Arduino_Nano_v2.x_0_1")
		(symbol "Arduino_Nano_v2.x_1_1"
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D0/RX")
				(number "2")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D1/TX")
				(number "1")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D2")
				(number "5")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D3")
				(number "6")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D4")
				(number "7")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "D5")
				(number "8")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "D6")
				(number "9")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "D7")
				(number "10")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "D8")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "D9")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "D10")
				(number "13")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "D11")
				(number "14")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "D12")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "D13")
				(number "16")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VIN")
				(number "30")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "4")
			)
			(pin power_out line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "3V3")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -25.4 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "+5V")
				(number "27")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{RESET}")
				(number "28")
			)
			(pin input line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "AREF")
				(number "18")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "A0")
				(number "19")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A1")
				(number "20")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A2")
				(number "21")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A3")
				(number "22")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "A4")
				(number "23")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "A5")
				(number "24")
			)
			(pin bidirectional line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "A6")
				(number "25")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "A7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Arduino_UNO_R2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -10.16 23.495 0)
		)
		(property "Value" "Arduino_UNO_R2"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Module:Arduino_UNO_R2"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.arduino.cc/en/Main/arduinoBoardUno"
			(at 0 0 0)
		)
		(property "Description" "Arduino UNO Microcontroller Module, release 2"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arduino UNO R3 Microcontroller Module Atmel AVR USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Arduino*UNO*R2*"
			(at 0 0 0)
		)
		(symbol "Arduino_UNO_R2_0_1")
		(symbol "Arduino_UNO_R2_1_1"
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D0/RX")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D1/TX")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D2")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D3")
				(number "18")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D4")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "D5")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "D6")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "D7")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "D8")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "D9")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "D10")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "D11")
				(number "26")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "D12")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "D13")
				(number "28")
			)
			(pin no_connect line
				(at -10.16 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "3V3")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "+5V")
				(number "5")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IOREF")
				(number "2")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "AREF")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "A0")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A1")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A2")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A3")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SDA/A4")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SCL/A5")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Arduino_UNO_R3"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -10.16 23.495 0)
		)
		(property "Value" "Arduino_UNO_R3"
			(at 5.08 -26.67 0)
		)
		(property "Footprint" "Module:Arduino_UNO_R3"
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.arduino.cc/en/Main/arduinoBoardUno"
			(at 0 0 0)
		)
		(property "Description" "Arduino UNO Microcontroller Module, release 3"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arduino UNO R3 Microcontroller Module Atmel AVR USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Arduino*UNO*R3*"
			(at 0 0 0)
		)
		(symbol "Arduino_UNO_R3_0_1")
		(symbol "Arduino_UNO_R3_1_1"
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "D0/RX")
				(number "15")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "D1/TX")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "D2")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "D3")
				(number "18")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "D4")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "D5")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 0 0)
				(length 2.54)
				(name "D6")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "D7")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "D8")
				(number "23")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "D9")
				(number "24")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "D10")
				(number "25")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "D11")
				(number "26")
			)
			(pin bidirectional line
				(at -12.7 -15.24 0)
				(length 2.54)
				(name "D12")
				(number "27")
			)
			(pin bidirectional line
				(at -12.7 -17.78 0)
				(length 2.54)
				(name "D13")
				(number "28")
			)
			(pin no_connect line
				(at -10.16 -20.32 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "1")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 2.54)
				(name "VIN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "29")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "6")
			)
			(pin power_out line
				(at 2.54 25.4 270)
				(length 2.54)
				(name "3V3")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 5.08 25.4 270)
				(length 2.54)
				(name "+5V")
				(number "5")
			)
			(pin input line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "~{RESET}")
				(number "3")
			)
			(pin output line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "IOREF")
				(number "2")
			)
			(pin input line
				(at 12.7 5.08 180)
				(length 2.54)
				(name "AREF")
				(number "30")
			)
			(pin bidirectional line
				(at 12.7 0 180)
				(length 2.54)
				(name "A0")
				(number "9")
			)
			(pin bidirectional line
				(at 12.7 -2.54 180)
				(length 2.54)
				(name "A1")
				(number "10")
			)
			(pin bidirectional line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "A2")
				(number "11")
			)
			(pin bidirectional line
				(at 12.7 -7.62 180)
				(length 2.54)
				(name "A3")
				(number "12")
			)
			(pin bidirectional line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "SDA/A4")
				(number "13")
			)
			(pin bidirectional line
				(at 12.7 -12.7 180)
				(length 2.54)
				(name "SCL/A5")
				(number "14")
			)
			(pin bidirectional line
				(at 12.7 -17.78 180)
				(length 2.54)
				(name "SDA/A4")
				(number "31")
			)
			(pin bidirectional line
				(at 12.7 -20.32 180)
				(length 2.54)
				(name "SCL/A5")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CHIP"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 49.53 0)
		)
		(property "Value" "CHIP"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Module:MODULE_NEXTTHINGCO_CHIP"
			(at 30.48 -58.42 0)
		)
		(property "Datasheet" "https://github.com/NextThingCo/CHIP-Hardware/tree/master/CHIP%5Bv1_0%5D"
			(at -81.28 -10.16 0)
		)
		(property "Description" "NextThingCo C.H.I.P. Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "nextthingco chip module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MODULE*NEXTTHINGCO*CHIP*"
			(at 0 0 0)
		)
		(symbol "CHIP_0_1")
		(symbol "CHIP_1_1"
			(pin input line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "X1")
				(number "13")
			)
			(pin input line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "X2")
				(number "14")
			)
			(pin input line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "Y1")
				(number "15")
			)
			(pin input line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "Y2")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PD2/LCD-D2")
				(number "17")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PD3/LCD-D3")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PD4/LCD-D4")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PD5/LCD-D5")
				(number "22")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PD6/LCD-D6")
				(number "21")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PD7/LCD-D7")
				(number "24")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PD10/LCD-D10")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PD11/LCD-D11")
				(number "26")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PD12/LCD-D12")
				(number "25")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PD13/LCD-D13")
				(number "28")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PD14/LCD-D14")
				(number "27")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PD15/LCD-D15")
				(number "30")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PD18/LCD-D18")
				(number "29")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PD19/LCD-D19")
				(number "32")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PD20/LCD-D20")
				(number "31")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PD21/LCD-D21")
				(number "34")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PD22/LCD-D22")
				(number "33")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PD23/LCD-D23")
				(number "36")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PD24/LCD-CLK")
				(number "35")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PD25/LCD-DE")
				(number "40")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PD26/LCD-HSYNC")
				(number "38")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PD27/LCD-VSYNC")
				(number "37")
			)
			(pin output line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "HPL")
				(number "44")
			)
			(pin output line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "HPCOM")
				(number "46")
			)
			(pin output line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "HPR")
				(number "48")
			)
			(pin power_out line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "MICM")
				(number "50")
			)
			(pin power_out line
				(at -33.02 -43.18 0)
				(length 5.08)
				(name "LRADC")
				(number "51")
			)
			(pin input line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "MICIN1")
				(number "52")
			)
			(pin input line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "~{POWER-ON}")
				(number "10")
			)
			(pin power_in line
				(at -17.78 53.34 270)
				(length 5.08)
				(name "CHG-IN")
				(number "2")
			)
			(pin power_in line
				(at -10.16 53.34 270)
				(length 5.08)
				(name "BAT")
				(number "8")
			)
			(pin power_in line
				(at -10.16 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin input line
				(at -7.62 53.34 270)
				(length 5.08)
				(name "TS")
				(number "6")
			)
			(pin power_in line
				(at -7.62 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "12")
			)
			(pin power_in line
				(at -2.54 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "39")
			)
			(pin power_in line
				(at 0 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "41")
			)
			(pin power_out line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "+5V")
				(number "3")
			)
			(pin power_in line
				(at 2.54 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "61")
			)
			(pin power_out line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "+5V")
				(number "42")
			)
			(pin power_in line
				(at 5.08 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "62")
			)
			(pin power_in line
				(at 7.62 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "79")
			)
			(pin power_out line
				(at 10.16 53.34 270)
				(length 5.08)
				(name "+3.3V")
				(number "5")
			)
			(pin power_in line
				(at 10.16 -60.96 90)
				(length 5.08)
				(name "GND")
				(number "80")
			)
			(pin power_out line
				(at 12.7 53.34 270)
				(length 5.08)
				(name "+3.3V")
				(number "49")
			)
			(pin power_out line
				(at 17.78 53.34 270)
				(length 5.08)
				(name "+1.8V")
				(number "7")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PG3/UART1-TX")
				(number "43")
			)
			(pin input line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PG4/UART1-RX")
				(number "45")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB16/TWI1-SDA")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB15/TWI1-SCK")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PB18/TWI2-SDA")
				(number "65")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB17/TWI2-SCK")
				(number "66")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB2/PWM0")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PG1/AP-EINT1")
				(number "63")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB3/AP-EINT3")
				(number "64")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PE0/CSI-PCLK/SPI2-CS0")
				(number "67")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PE1/CSI-MCLK/SPI2-CLK")
				(number "68")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "PE2/CSI-HSYNC/SPI2-MOSI")
				(number "69")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PE3/CSI-VSYNC/SPI2-MISO")
				(number "70")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PE4/CSI-D0")
				(number "71")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PE5/CSI-D1")
				(number "72")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PE6/CSI-D2")
				(number "73")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PE7/CSI-D3")
				(number "74")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PE8/CSI-D4")
				(number "75")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PE9/CSI-D5")
				(number "76")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PE10/CSI-D6")
				(number "77")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PE11/CSI-D7")
				(number "78")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "XIO-P0")
				(number "53")
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "XIO-P1")
				(number "54")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "XIO-P2")
				(number "55")
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "XIO-P3")
				(number "56")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "XIO-P4")
				(number "57")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "XIO-P5")
				(number "58")
			)
			(pin bidirectional line
				(at 33.02 -43.18 180)
				(length 5.08)
				(name "XIO-P6")
				(number "59")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "XIO-P7")
				(number "60")
			)
			(pin input line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "~{FEL}")
				(number "47")
			)
		)
		(embedded_fonts no)
	)
	(symbol "CHIP-PRO"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -26.67 39.37 0)
		)
		(property "Value" "CHIP-PRO"
			(at 17.78 39.37 0)
		)
		(property "Footprint" "Module:MODULE_NEXTTHINGCO_CHIPPRO"
			(at 30.48 -43.18 0)
		)
		(property "Datasheet" "https://github.com/NextThingCo/CHIP_Pro-Hardware/blob/master/Datasheets/CHIP_PRO_Datasheet_v1.0.pdf"
			(at -81.28 -20.32 0)
		)
		(property "Description" "NextThingCo C.H.I.P. Pro Module"
			(at 0 0 0)
		)
		(property "ki_keywords" "nextthingco chip pro module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "MODULE*NEXTTHINGCO*CHIPPRO*"
			(at 0 0 0)
		)
		(symbol "CHIP-PRO_0_1")
		(symbol "CHIP-PRO_1_1"
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "USB0-D+")
				(number "51")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "USB0-D-")
				(number "52")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "USB1-D+")
				(number "47")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "USB1-D-")
				(number "48")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PB5/I2S-MCLK")
				(number "21")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PB6/I2S-BCLK")
				(number "22")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PB7/I2S-LCLK")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PB8/I2S-DO")
				(number "24")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PB9/I2S-DI")
				(number "25")
			)
			(pin output line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "HPL")
				(number "18")
			)
			(pin output line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "HPCOM")
				(number "19")
			)
			(pin output line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "HPR")
				(number "20")
			)
			(pin unspecified line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "VMIC")
				(number "29")
			)
			(pin input line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "MICIN1")
				(number "27")
			)
			(pin input line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "MICIN2")
				(number "28")
			)
			(pin power_out line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "LRADC0")
				(number "42")
			)
			(pin input line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "~{POWER-ON}")
				(number "5")
			)
			(pin power_in line
				(at -10.16 43.18 270)
				(length 5.08)
				(name "VBUS")
				(number "50")
			)
			(pin power_in line
				(at -10.16 -45.72 90)
				(length 5.08)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at -7.62 43.18 270)
				(length 5.08)
				(name "CHG-IN")
				(number "4")
			)
			(pin power_in line
				(at -7.62 -45.72 90)
				(length 5.08)
				(name "GND")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -45.72 90)
				(length 5.08)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 5.08)
				(name "BAT")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 5.08)
				(name "GND")
				(number "45")
			)
			(pin input line
				(at 0 43.18 270)
				(length 5.08)
				(name "TS")
				(number "7")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 5.08)
				(name "AGND")
				(number "26")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 5.08)
				(name "GND")
				(number "46")
			)
			(pin power_out line
				(at 5.08 43.18 270)
				(length 5.08)
				(name "IPSOUT")
				(number "3")
			)
			(pin power_in line
				(at 5.08 -45.72 90)
				(length 5.08)
				(name "GND")
				(number "49")
			)
			(pin power_out line
				(at 7.62 43.18 270)
				(length 5.08)
				(name "+3.3V")
				(number "2")
			)
			(pin power_in line
				(at 7.62 -45.72 90)
				(length 5.08)
				(name "GND")
				(number "53")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PG3/UART1-TX")
				(number "44")
			)
			(pin input line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PG4/UART1-RX")
				(number "43")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "PD2/UART2-TX")
				(number "13")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PD3/UART2-RX")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PD4/UART2-CTS")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PD5/UART2-RTS")
				(number "16")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB16/TWI1-SDA")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PB15/TWI1-SCK")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB2/SPDIF-DO/PWM0")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "PG13/EINT13/PWM1")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PE0/CSI-PCLK/SPI2-CS0")
				(number "41")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PE1/CSI-MCLK/SPI2-CLK")
				(number "40")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PE2/CSI-HSYNC/SPI2-MOSI")
				(number "39")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PE3/CSI-VSYNC/SPI2-MISO")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PE4/CSI-D0")
				(number "37")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PE5/CSI-D1")
				(number "36")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PE6/CSI-D2")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PE7/CSI-D3")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PE8/CSI-D4")
				(number "33")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PE9/CSI-D5")
				(number "32")
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PE10/CSI-D6")
				(number "31")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PE11/CSI-D7")
				(number "30")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Carambola2"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 31.75 0)
		)
		(property "Value" "Carambola2"
			(at 17.78 31.75 0)
		)
		(property "Footprint" "Module:Carambola2"
			(at 17.78 27.94 0)
		)
		(property "Datasheet" "https://www.8devices.com/media/products/carambola2/downloads/carambola2-datasheet.pdf"
			(at -27.94 31.75 0)
		)
		(property "Description" "Qualcomm AR9331, 16MB Flash, 64MB RAM, USB, Serial, Ethernet, GPIO, OpenWRT, industrial SoM computer"
			(at 0 0 0)
		)
		(property "ki_keywords" "carambola, 8devices, openwrt, board, wlan"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Carambola2*"
			(at 0 0 0)
		)
		(symbol "Carambola2_0_1")
		(symbol "Carambola2_1_1"
			(pin input line
				(at -33.02 25.4 0)
				(length 2.54)
				(name "ETH1_RXP")
				(number "8")
			)
			(pin input line
				(at -33.02 22.86 0)
				(length 2.54)
				(name "ETH1_RXM")
				(number "9")
			)
			(pin output line
				(at -33.02 20.32 0)
				(length 2.54)
				(name "ETH1_TXP")
				(number "10")
			)
			(pin output line
				(at -33.02 17.78 0)
				(length 2.54)
				(name "ETH1_TXM")
				(number "11")
			)
			(pin input line
				(at -33.02 12.7 0)
				(length 2.54)
				(name "ETH0_RXP")
				(number "12")
			)
			(pin input line
				(at -33.02 10.16 0)
				(length 2.54)
				(name "ETH0_RXM")
				(number "13")
			)
			(pin output line
				(at -33.02 7.62 0)
				(length 2.54)
				(name "ETH0_TXP")
				(number "14")
			)
			(pin output line
				(at -33.02 5.08 0)
				(length 2.54)
				(name "ETH0_TXM")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 2.54)
				(name "SPI_MOSI/GPIO_4")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 2.54)
				(name "SPI_CLK/GPIO_3")
				(number "17")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 2.54)
				(name "SPI_MISO/GPIO_5")
				(number "18")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 2.54)
				(name "SPI_CS0/GPIO_2")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 2.54)
				(name "GPIO_9/UART_RX/SPI_CS_1")
				(number "43")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 2.54)
				(name "GPIO_10/UART_TX/SPI_CS_2")
				(number "44")
			)
			(pin input line
				(at -33.02 -17.78 0)
				(length 2.54)
				(name "GPIO_12/UART_CTS/I2S_MCIN")
				(number "24")
			)
			(pin output line
				(at -33.02 -20.32 0)
				(length 2.54)
				(name "GPIO_11/UART_RTS/I2S_MCK/JS/~{SOFT_RESET}")
				(number "23")
			)
			(pin input line
				(at -33.02 -25.4 0)
				(length 2.54)
				(name "~{RESET}")
				(number "33")
			)
			(pin power_in line
				(at -7.62 33.02 270)
				(length 2.54)
				(name "+3VD")
				(number "51")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 2.54)
				(name "+3VD")
				(number "50")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "48")
			)
			(pin passive line
				(at 0 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "GND")
				(number "7")
			)
			(pin power_out line
				(at 5.08 33.02 270)
				(length 2.54)
				(name "+2VD")
				(number "52")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 2.54)
				(name "SPDIF_OUT/GPIO_23")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 2.54)
				(name "I2S_MICIN/SLIC_DATA_IN/GPIO_22")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 2.54)
				(name "I2S_MCK/SLIC_DATA_OUT/GPIO_21")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 2.54)
				(name "I2S_WS/SLIC_FS_IN/GPIO_20")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 2.54)
				(name "I2S_WS/SLIC_FS_OUT/GPIO_19")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 2.54)
				(name "I2S_CK/SLIK_CLK/GPIO_18")
				(number "6")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 2.54)
				(name "LED0/WLAN_LED/GPIO_0")
				(number "41")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 2.54)
				(name "LED1/GPIO_1")
				(number "40")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 2.54)
				(name "LED2/ETH1_LED/GPIO_13")
				(number "39")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 2.54)
				(name "LED3/ETH0_LED/GPIO_14")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 2.54)
				(name "LED4/GPIO_15")
				(number "37")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 2.54)
				(name "LED5/GPIO_16")
				(number "36")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 2.54)
				(name "LED6/GPIO_17")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 2.54)
				(name "USB_D-")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 2.54)
				(name "USB_D+")
				(number "20")
			)
			(pin passive line
				(at 33.02 -25.4 180)
				(length 2.54)
				(name "ANTENNA")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Electrosmith_Daisy_Seed_Rev4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -20.32 34.29 0)
		)
		(property "Value" "Electrosmith_Daisy_Seed_Rev4"
			(at 33.02 34.29 0)
		)
		(property "Footprint" "Module:Electrosmith_Daisy_Seed"
			(at 19.05 -35.56 0)
		)
		(property "Datasheet" "https://static1.squarespace.com/static/58d03fdc1b10e3bf442567b8/t/6227e6236f02fb68d1577146/1646781988478/Daisy_Seed_datasheet_v1.0.3.pdf"
			(at 77.47 -38.1 0)
		)
		(property "Description" "Daisy is an embedded platform for music."
			(at 0 0 0)
		)
		(property "ki_keywords" "Electrosmith Daisy Seed Microcontroller Module ARM Cortex-M7"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Electrosmith*Daisy*Seed*"
			(at 0 0 0)
		)
		(symbol "Electrosmith_Daisy_Seed_Rev4_0_0"
			(text "GPIO15"
				(at -1.27 10.16 0)
			)
			(text "GPIO16"
				(at -1.27 7.62 0)
			)
			(text "GPIO17"
				(at -1.27 5.08 0)
			)
			(text "GPIO18"
				(at -1.27 2.54 0)
			)
			(text "GPIO19"
				(at -1.27 0 0)
			)
			(text "GPIO20"
				(at -1.27 -2.54 0)
			)
			(text "GPIO21"
				(at -1.27 -5.08 0)
			)
			(text "GPIO22"
				(at -1.27 -7.62 0)
			)
			(text "GPIO23"
				(at -1.27 -10.16 0)
			)
			(text "GPIO24"
				(at -1.27 -15.24 0)
			)
			(text "GPIO25"
				(at -1.27 -17.78 0)
			)
			(text "GPIO26"
				(at -1.27 -20.32 0)
			)
			(text "GPIO27"
				(at -1.27 -22.86 0)
			)
			(text "GPIO28"
				(at -1.27 -25.4 0)
			)
			(text "GPIO0"
				(at 1.27 25.4 0)
			)
			(text "GPIO29"
				(at 1.27 22.86 0)
			)
			(text "GPIO30"
				(at 1.27 20.32 0)
			)
			(text "GPIO13"
				(at 1.27 15.24 0)
			)
			(text "GPIO14"
				(at 1.27 12.7 0)
			)
			(text "GPIO11"
				(at 1.27 7.62 0)
			)
			(text "GPIO12"
				(at 1.27 5.08 0)
			)
			(text "GPIO7"
				(at 1.27 0 0)
			)
			(text "GPIO8"
				(at 1.27 -2.54 0)
			)
			(text "GPIO9"
				(at 1.27 -5.08 0)
			)
			(text "GPIO10"
				(at 1.27 -7.62 0)
			)
			(text "GPIO4"
				(at 1.27 -12.7 0)
			)
			(text "GPIO3"
				(at 1.27 -15.24 0)
			)
			(text "GPIO2"
				(at 1.27 -17.78 0)
			)
			(text "GPIO1"
				(at 1.27 -20.32 0)
			)
			(text "GPIO5"
				(at 1.27 -22.86 0)
			)
			(text "GPIO6"
				(at 1.27 -25.4 0)
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "AUDIO_IN_1")
				(number "16")
			)
			(pin input line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "AUDIO_IN_2")
				(number "17")
			)
			(pin output line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "AUDIO_OUT_1")
				(number "18")
			)
			(pin output line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "AUDIO_OUT_2")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "ADC_0")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "ADC_1")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "ADC_2")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "ADC_3")
				(number "25")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "ADC_4")
				(number "26")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "ADC_5")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "ADC_6")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "DAC_OUT2")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "DAC_OUT1")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "SAI2_MCLK")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "SAI2_SD_B")
				(number "32")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "SAI2_SD_A")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 5.08)
				(name "SAI2_FS")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 5.08)
				(name "SAI2_SCK")
				(number "35")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 5.08)
				(name "VIN")
				(number "39")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 5.08)
				(name "DGND")
				(number "40")
			)
			(pin power_out line
				(at 0 38.1 270)
				(length 5.08)
				(name "3V3_D")
				(number "38")
			)
			(pin power_out line
				(at 2.54 38.1 270)
				(length 5.08)
				(name "3V3_A")
				(number "21")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 5.08)
				(name "AGND")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 5.08)
				(name "USB_ID")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "USB_D_-")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "USB_D_+")
				(number "37")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "USART1_TX")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "USART1_RX")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "I2C1_SCL")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "I2C1_SDA")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "SPI1_CS")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "SPI1_SCK")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "SPI1_POCI")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "SPI1_PICO")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "SD_DATA_0")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "SD_DATA_1")
				(number "4")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "SD_DATA_2")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "SD_DATA_3")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 -22.86 180)
				(length 5.08)
				(name "SD_CMD")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 5.08)
				(name "SD_CLK")
				(number "7")
			)
		)
		(symbol "Electrosmith_Daisy_Seed_Rev4_0_1")
		(embedded_fonts no)
	)
	(symbol "Google_Coral"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 17.78 0)
		)
		(property "Value" "Google_Coral"
			(at -11.43 -17.78 0)
		)
		(property "Footprint" "Module:Google_Coral_SMT_TPU_Module"
			(at -10.16 -30.48 0)
		)
		(property "Datasheet" "https://coral.ai/static/files/Coral-Accelerator-Module-datasheet.pdf"
			(at -33.02 -33.02 0)
		)
		(property "Description" "Edge TPU, 4 TOPS, 2W, 120-LGA"
			(at 0 0 0)
		)
		(property "ki_keywords" "TPU Coral"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Google*Coral*SMT*TPU*Module*"
			(at 0 0 0)
		)
		(symbol "Google_Coral_0_0"
			(pin input line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "RST_L")
				(number "76")
			)
			(pin input line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "PMIC_EN")
				(number "53")
			)
			(pin output line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "PGOOD4")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "CLKREQ_L")
				(number "78")
			)
			(pin output line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "SD_ALARM")
				(number "82")
			)
			(pin output line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "INTR")
				(number "77")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "USB_SEL")
				(number "83")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 2.54)
				(name "VIN")
				(number "56")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 2.54)
				(name "AON")
				(number "54")
			)
			(pin input clock
				(at 20.32 0 180)
				(length 2.54)
				(name "PCIE_REFCLK_N")
				(number "10")
			)
			(pin input clock
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "PCIE_REFCLK_P")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "USB2_D_N")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "USB2_D_P")
				(number "13")
			)
		)
		(symbol "Google_Coral_1_0"
			(pin no_connect line
				(at -7.62 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "52")
			)
			(pin no_connect line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "49")
			)
			(pin no_connect line
				(at -2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "50")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "57")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "58")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "59")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "60")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "61")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "62")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "63")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "64")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "65")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "66")
			)
			(pin passive line
				(at 0 17.78 270)
				(length 2.54)
				(hide yes)
				(name "VIN")
				(number "67")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "100")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "101")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "102")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "104")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "105")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "106")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "107")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "108")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "109")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "110")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "111")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "112")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "113")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "114")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "115")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "116")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "117")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "118")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "119")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "12")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "120")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "21")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "27")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "3")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "30")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "33")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "34")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "39")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "42")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "48")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "6")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "68")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "69")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "70")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "71")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "74")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "75")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "80")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "86")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "87")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "88")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "89")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "9")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "90")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "91")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "92")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "93")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "94")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "95")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "96")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "97")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "98")
			)
			(pin passive line
				(at 0 -17.78 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "99")
			)
			(pin no_connect line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "84")
			)
			(pin no_connect line
				(at 2.54 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "RESERVED")
				(number "85")
			)
			(pin input line
				(at 20.32 10.16 180)
				(length 2.54)
				(name "PCIE_RX_P")
				(number "7")
			)
			(pin input line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "PCIE_RX_N")
				(number "8")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "PCIE_TX_P")
				(number "5")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "PCIE_TX_N")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Maple_Mini"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -16.51 25.4 0)
		)
		(property "Value" "Maple_Mini"
			(at 16.51 25.4 0)
		)
		(property "Footprint" "Module:Maple_Mini"
			(at 1.27 -26.67 0)
		)
		(property "Datasheet" "http://docs.leaflabs.com/static.leaflabs.com/pub/leaflabs/maple-docs/0.0.12/hardware/maple-mini.html"
			(at 1.27 -50.8 0)
		)
		(property "Description" "Maple Mini Microcontroller Module by LeafLabs"
			(at 0 0 0)
		)
		(property "ki_keywords" "Maple Mini Microcontroller Module LeafLabs STM32 STM32F103"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Maple*Mini*"
			(at 0 0 0)
		)
		(symbol "Maple_Mini_0_1")
		(symbol "Maple_Mini_1_1"
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "D0/SDA2")
				(number "22")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 3.81)
				(name "D1/SCL2")
				(number "23")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "D2")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "D3")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "D4/MOSI1")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "D5/MISO1")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "D6/SCK1")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "D7/SS1")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "D8/RX2")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "D9/TX2")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "D10")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "D11")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "D12")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "D13")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "D14")
				(number "37")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "~{RESET}")
				(number "34")
			)
			(pin output line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "AV+")
				(number "40")
			)
			(pin output line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "AV-")
				(number "39")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 3.81)
				(name "VIN")
				(number "21")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "GND")
				(number "2")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "VBAT")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "SCL1/D15")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "SDA1/D16")
				(number "5")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "D17")
				(number "6")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "D18")
				(number "7")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "D19")
				(number "8")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "D20")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "D21")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "D22")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "D23")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "D24")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "RX1/D25")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "TX1/D26")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "D27")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "MOSI2/D28")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "MISO2/D29")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "SCK2/D30")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "SS2/D31")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "BUT/D32")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NUCLEO144-F429ZI"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 94.615 0)
		)
		(property "Value" "NUCLEO144-F429ZI"
			(at -22.86 92.71 0)
		)
		(property "Footprint" "Module:ST_Morpho_Connector_144_STLink"
			(at 21.59 -92.71 0)
		)
		(property "Datasheet" "http://www.st.com/content/ccc/resource/technical/document/data_brief/group0/7b/df/1d/e9/64/55/43/8d/DM00247910/files/DM00247910.pdf/jcr:content/translations/en.DM00247910.pdf"
			(at -22.86 7.62 0)
		)
		(property "Description" "Nucleo 144 Development Board with STM32F429ZIT6 MCU, 256kB RAM, 1Mb FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM32 Nucleo ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*Morpho*Connector*144*STLink*"
			(at 0 0 0)
		)
		(symbol "NUCLEO144-F429ZI_0_1")
		(symbol "NUCLEO144-F429ZI_1_1"
			(pin input line
				(at -33.02 83.82 0)
				(length 5.08)
				(name "~{BOOT0}")
				(number "7")
			)
			(pin input line
				(at -33.02 81.28 0)
				(length 5.08)
				(name "~{RST}")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 48.26 0)
				(length 5.08)
				(name "PH0")
				(number "29")
			)
			(pin bidirectional line
				(at -33.02 45.72 0)
				(length 5.08)
				(name "PH1")
				(number "31")
			)
			(pin bidirectional line
				(at -33.02 40.64 0)
				(length 5.08)
				(name "PG0")
				(number "59")
			)
			(pin bidirectional line
				(at -33.02 38.1 0)
				(length 5.08)
				(name "PG1")
				(number "58")
			)
			(pin bidirectional line
				(at -33.02 35.56 0)
				(length 5.08)
				(name "PG2")
				(number "42")
			)
			(pin bidirectional line
				(at -33.02 33.02 0)
				(length 5.08)
				(name "PG3")
				(number "44")
			)
			(pin bidirectional line
				(at -33.02 30.48 0)
				(length 5.08)
				(name "PG4")
				(number "141")
			)
			(pin bidirectional line
				(at -33.02 27.94 0)
				(length 5.08)
				(name "PG5")
				(number "140")
			)
			(pin bidirectional line
				(at -33.02 25.4 0)
				(length 5.08)
				(name "PG6/USB_GPIO_OUT")
				(number "142")
			)
			(pin bidirectional line
				(at -33.02 22.86 0)
				(length 5.08)
				(name "PG7/USB_GPIO_IN")
				(number "139")
			)
			(pin bidirectional line
				(at -33.02 20.32 0)
				(length 5.08)
				(name "PG8")
				(number "138")
			)
			(pin bidirectional line
				(at -33.02 17.78 0)
				(length 5.08)
				(name "PG9")
				(number "63")
			)
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PG10")
				(number "66")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PG11/ETH_TX_EN")
				(number "70")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PG12")
				(number "65")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PG13/ETH_TXD0")
				(number "68")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PG14")
				(number "133")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PG15")
				(number "64")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PF0")
				(number "53")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PF1")
				(number "51")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PF2")
				(number "52")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PF3")
				(number "130")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PF4")
				(number "110")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PF5")
				(number "108")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PF6")
				(number "9")
			)
			(pin bidirectional line
				(at -33.02 -20.32 0)
				(length 5.08)
				(name "PF7")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 -22.86 0)
				(length 5.08)
				(name "PF8")
				(number "54")
			)
			(pin bidirectional line
				(at -33.02 -25.4 0)
				(length 5.08)
				(name "PF9")
				(number "56")
			)
			(pin bidirectional line
				(at -33.02 -27.94 0)
				(length 5.08)
				(name "PF10")
				(number "114")
			)
			(pin bidirectional line
				(at -33.02 -30.48 0)
				(length 5.08)
				(name "PF11")
				(number "134")
			)
			(pin bidirectional line
				(at -33.02 -33.02 0)
				(length 5.08)
				(name "PF12")
				(number "131")
			)
			(pin bidirectional line
				(at -33.02 -35.56 0)
				(length 5.08)
				(name "PF13")
				(number "129")
			)
			(pin bidirectional line
				(at -33.02 -38.1 0)
				(length 5.08)
				(name "PF14")
				(number "122")
			)
			(pin bidirectional line
				(at -33.02 -40.64 0)
				(length 5.08)
				(name "PF15")
				(number "132")
			)
			(pin bidirectional line
				(at -33.02 -45.72 0)
				(length 5.08)
				(name "PE0")
				(number "136")
			)
			(pin bidirectional line
				(at -33.02 -48.26 0)
				(length 5.08)
				(name "PE1")
				(number "61")
			)
			(pin bidirectional line
				(at -33.02 -50.8 0)
				(length 5.08)
				(name "PE2")
				(number "46")
			)
			(pin bidirectional line
				(at -33.02 -53.34 0)
				(length 5.08)
				(name "PE3")
				(number "47")
			)
			(pin bidirectional line
				(at -33.02 -55.88 0)
				(length 5.08)
				(name "PE4")
				(number "48")
			)
			(pin bidirectional line
				(at -33.02 -58.42 0)
				(length 5.08)
				(name "PE5")
				(number "50")
			)
			(pin bidirectional line
				(at -33.02 -60.96 0)
				(length 5.08)
				(name "PE6")
				(number "62")
			)
			(pin bidirectional line
				(at -33.02 -63.5 0)
				(length 5.08)
				(name "PE7")
				(number "116")
			)
			(pin bidirectional line
				(at -33.02 -66.04 0)
				(length 5.08)
				(name "PE8")
				(number "112")
			)
			(pin bidirectional line
				(at -33.02 -68.58 0)
				(length 5.08)
				(name "PE9")
				(number "124")
			)
			(pin bidirectional line
				(at -33.02 -71.12 0)
				(length 5.08)
				(name "PE10")
				(number "119")
			)
			(pin bidirectional line
				(at -33.02 -73.66 0)
				(length 5.08)
				(name "PE11")
				(number "128")
			)
			(pin bidirectional line
				(at -33.02 -76.2 0)
				(length 5.08)
				(name "PE12")
				(number "121")
			)
			(pin bidirectional line
				(at -33.02 -78.74 0)
				(length 5.08)
				(name "PE13")
				(number "127")
			)
			(pin bidirectional line
				(at -33.02 -81.28 0)
				(length 5.08)
				(name "PE14")
				(number "123")
			)
			(pin bidirectional line
				(at -33.02 -83.82 0)
				(length 5.08)
				(name "PE15")
				(number "125")
			)
			(pin no_connect line
				(at -27.94 58.42 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin no_connect line
				(at -27.94 55.88 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -27.94 53.34 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "67")
			)
			(pin power_in line
				(at -20.32 96.52 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -20.32 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at -17.78 96.52 270)
				(length 5.08)
				(name "E5V")
				(number "6")
			)
			(pin power_in line
				(at -17.78 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at -15.24 96.52 270)
				(length 5.08)
				(name "IOREF")
				(number "12")
			)
			(pin power_in line
				(at -15.24 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at -12.7 96.52 270)
				(length 5.08)
				(name "+3V3")
				(number "16")
			)
			(pin power_in line
				(at -12.7 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "49")
			)
			(pin power_in line
				(at -10.16 96.52 270)
				(length 5.08)
				(name "+5V")
				(number "18")
			)
			(pin power_in line
				(at -10.16 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "22")
			)
			(pin power_in line
				(at -7.62 96.52 270)
				(length 5.08)
				(name "VIN")
				(number "24")
			)
			(pin power_in line
				(at -7.62 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "60")
			)
			(pin power_in line
				(at -5.08 96.52 270)
				(length 5.08)
				(name "VBAT")
				(number "33")
			)
			(pin power_in line
				(at -5.08 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "71")
			)
			(pin power_in line
				(at -2.54 96.52 270)
				(length 5.08)
				(name "U5V")
				(number "80")
			)
			(pin power_in line
				(at -2.54 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "72")
			)
			(pin power_in line
				(at 0 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "81")
			)
			(pin power_in line
				(at 2.54 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "92")
			)
			(pin power_in line
				(at 5.08 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "111")
			)
			(pin power_in line
				(at 7.62 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "126")
			)
			(pin power_in line
				(at 10.16 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "135")
			)
			(pin power_in line
				(at 12.7 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "143")
			)
			(pin power_in line
				(at 15.24 -96.52 90)
				(length 5.08)
				(name "GND")
				(number "144")
			)
			(pin power_in line
				(at 20.32 96.52 270)
				(length 5.08)
				(name "AVDD")
				(number "79")
			)
			(pin power_in line
				(at 20.32 -96.52 90)
				(length 5.08)
				(name "AGND")
				(number "104")
			)
			(pin bidirectional line
				(at 33.02 83.82 180)
				(length 5.08)
				(name "PA0")
				(number "28")
			)
			(pin bidirectional line
				(at 33.02 81.28 180)
				(length 5.08)
				(name "ETH_REF_CLK/PA1")
				(number "30")
			)
			(pin bidirectional line
				(at 33.02 78.74 180)
				(length 5.08)
				(name "ETH_MDIO/PA2")
				(number "107")
			)
			(pin bidirectional line
				(at 33.02 76.2 180)
				(length 5.08)
				(name "PA3")
				(number "109")
			)
			(pin bidirectional line
				(at 33.02 73.66 180)
				(length 5.08)
				(name "PA4")
				(number "32")
			)
			(pin bidirectional line
				(at 33.02 71.12 180)
				(length 5.08)
				(name "PA5")
				(number "83")
			)
			(pin bidirectional line
				(at 33.02 68.58 180)
				(length 5.08)
				(name "PA6")
				(number "85")
			)
			(pin bidirectional line
				(at 33.02 66.04 180)
				(length 5.08)
				(name "ETH_CRS_DV/PA7")
				(number "87")
			)
			(pin bidirectional line
				(at 33.02 63.5 180)
				(length 5.08)
				(name "USB_SOF/PA8")
				(number "95")
			)
			(pin bidirectional line
				(at 33.02 60.96 180)
				(length 5.08)
				(name "USB_VBUS/PA9")
				(number "93")
			)
			(pin bidirectional line
				(at 33.02 58.42 180)
				(length 5.08)
				(name "USB_ID/PA10")
				(number "105")
			)
			(pin bidirectional line
				(at 33.02 55.88 180)
				(length 5.08)
				(name "USB_DM/PA11")
				(number "86")
			)
			(pin bidirectional line
				(at 33.02 53.34 180)
				(length 5.08)
				(name "USB_DP/PA12")
				(number "84")
			)
			(pin bidirectional line
				(at 33.02 50.8 180)
				(length 5.08)
				(name "TMS/PA13")
				(number "13")
			)
			(pin bidirectional line
				(at 33.02 48.26 180)
				(length 5.08)
				(name "TCK/PA14")
				(number "15")
			)
			(pin bidirectional line
				(at 33.02 45.72 180)
				(length 5.08)
				(name "PA15")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 40.64 180)
				(length 5.08)
				(name "PB0")
				(number "34")
			)
			(pin bidirectional line
				(at 33.02 38.1 180)
				(length 5.08)
				(name "PB1")
				(number "96")
			)
			(pin bidirectional line
				(at 33.02 35.56 180)
				(length 5.08)
				(name "PB2")
				(number "94")
			)
			(pin bidirectional line
				(at 33.02 33.02 180)
				(length 5.08)
				(name "SWO/PB3")
				(number "103")
			)
			(pin bidirectional line
				(at 33.02 30.48 180)
				(length 5.08)
				(name "PB4")
				(number "99")
			)
			(pin bidirectional line
				(at 33.02 27.94 180)
				(length 5.08)
				(name "PB5")
				(number "101")
			)
			(pin bidirectional line
				(at 33.02 25.4 180)
				(length 5.08)
				(name "PB6")
				(number "89")
			)
			(pin bidirectional line
				(at 33.02 22.86 180)
				(length 5.08)
				(name "LD2/PB7")
				(number "21")
			)
			(pin bidirectional line
				(at 33.02 20.32 180)
				(length 5.08)
				(name "PB8")
				(number "75")
			)
			(pin bidirectional line
				(at 33.02 17.78 180)
				(length 5.08)
				(name "PB9")
				(number "77")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PB10")
				(number "97")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PB11")
				(number "90")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PB12")
				(number "88")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "ETH_TXD1/PB13")
				(number "102")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "LD3/PB14")
				(number "100")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PB15")
				(number "98")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PC0")
				(number "38")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "ETH_MDC/PC1")
				(number "36")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PC2")
				(number "35")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PC3")
				(number "37")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "ETH_RXD0/PC4")
				(number "106")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "ETH_RXD1/PC5")
				(number "78")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PC6")
				(number "76")
			)
			(pin bidirectional line
				(at 33.02 -20.32 180)
				(length 5.08)
				(name "PC7")
				(number "91")
			)
			(pin bidirectional line
				(at 33.02 -22.86 180)
				(length 5.08)
				(name "PC8")
				(number "74")
			)
			(pin bidirectional line
				(at 33.02 -25.4 180)
				(length 5.08)
				(name "PC9")
				(number "73")
			)
			(pin bidirectional line
				(at 33.02 -27.94 180)
				(length 5.08)
				(name "PC10")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 -30.48 180)
				(length 5.08)
				(name "PC11")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -33.02 180)
				(length 5.08)
				(name "PC12")
				(number "3")
			)
			(pin bidirectional line
				(at 33.02 -35.56 180)
				(length 5.08)
				(name "BT/PC13")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 -38.1 180)
				(length 5.08)
				(name "RTC_CRYSTAL/PC14")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 -40.64 180)
				(length 5.08)
				(name "RTC_CRYSTAL/PC15")
				(number "27")
			)
			(pin bidirectional line
				(at 33.02 -45.72 180)
				(length 5.08)
				(name "PD0")
				(number "57")
			)
			(pin bidirectional line
				(at 33.02 -48.26 180)
				(length 5.08)
				(name "PD1")
				(number "55")
			)
			(pin bidirectional line
				(at 33.02 -50.8 180)
				(length 5.08)
				(name "PD2")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 -53.34 180)
				(length 5.08)
				(name "PD3")
				(number "40")
			)
			(pin bidirectional line
				(at 33.02 -55.88 180)
				(length 5.08)
				(name "PD4")
				(number "39")
			)
			(pin bidirectional line
				(at 33.02 -58.42 180)
				(length 5.08)
				(name "PD5")
				(number "41")
			)
			(pin bidirectional line
				(at 33.02 -60.96 180)
				(length 5.08)
				(name "PD6")
				(number "43")
			)
			(pin bidirectional line
				(at 33.02 -63.5 180)
				(length 5.08)
				(name "PD7")
				(number "45")
			)
			(pin bidirectional line
				(at 33.02 -66.04 180)
				(length 5.08)
				(name "STLINK_TX/PD8")
				(number "82")
			)
			(pin bidirectional line
				(at 33.02 -68.58 180)
				(length 5.08)
				(name "STLINK_RX/PD9")
				(number "69")
			)
			(pin bidirectional line
				(at 33.02 -71.12 180)
				(length 5.08)
				(name "PD10")
				(number "137")
			)
			(pin bidirectional line
				(at 33.02 -73.66 180)
				(length 5.08)
				(name "PD11")
				(number "117")
			)
			(pin bidirectional line
				(at 33.02 -76.2 180)
				(length 5.08)
				(name "PD12")
				(number "115")
			)
			(pin bidirectional line
				(at 33.02 -78.74 180)
				(length 5.08)
				(name "PD13")
				(number "113")
			)
			(pin bidirectional line
				(at 33.02 -81.28 180)
				(length 5.08)
				(name "PD14")
				(number "118")
			)
			(pin bidirectional line
				(at 33.02 -83.82 180)
				(length 5.08)
				(name "PD15")
				(number "120")
			)
		)
		(embedded_fonts no)
	)
	(symbol "NUCLEO64-F411RE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 50.165 0)
		)
		(property "Value" "NUCLEO64-F411RE"
			(at -17.78 48.26 0)
		)
		(property "Footprint" "Module:ST_Morpho_Connector_144_STLink"
			(at 13.97 -48.26 0)
		)
		(property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/data_brief/DM00105918.pdf"
			(at -22.86 -35.56 0)
		)
		(property "Description" "Nucleo 64 Development Board with STM32F411RET6 MCU, 128kB RAM, 512KB FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM32 Nucleo ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*Morpho*Connector*144*STLink*"
			(at 0 0 0)
		)
		(symbol "NUCLEO64-F411RE_0_1")
		(symbol "NUCLEO64-F411RE_1_1"
			(pin input line
				(at -27.94 38.1 0)
				(length 3.81)
				(name "~{BOOT0}")
				(number "7")
			)
			(pin input line
				(at -27.94 35.56 0)
				(length 3.81)
				(name "~{RESET}")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 3.81)
				(name "PH0")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 3.81)
				(name "PH1")
				(number "31")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 3.81)
				(name "PD2")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 3.81)
				(name "PC0")
				(number "38")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 3.81)
				(name "PC1")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 3.81)
				(name "PC2")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 3.81)
				(name "PC3")
				(number "37")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 3.81)
				(name "PC4")
				(number "72")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 3.81)
				(name "PC5")
				(number "44")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 3.81)
				(name "PC6")
				(number "42")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 3.81)
				(name "PC7")
				(number "57")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 3.81)
				(name "PC8")
				(number "40")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 3.81)
				(name "PC9")
				(number "39")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 3.81)
				(name "PC10")
				(number "1")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 3.81)
				(name "PC11")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 3.81)
				(name "PC12")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 3.81)
				(name "PC13")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 3.81)
				(name "PC14")
				(number "25")
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 3.81)
				(name "PC15")
				(number "27")
			)
			(pin no_connect line
				(at -24.13 33.02 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "56")
			)
			(pin no_connect line
				(at -24.13 30.48 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "74")
			)
			(pin no_connect line
				(at -24.13 27.94 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "76")
			)
			(pin no_connect line
				(at -24.13 25.4 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "48")
			)
			(pin no_connect line
				(at -24.13 22.86 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "26")
			)
			(pin no_connect line
				(at -24.13 20.32 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -24.13 17.78 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "9")
			)
			(pin no_connect line
				(at -24.13 15.24 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "11")
			)
			(pin power_in line
				(at -15.24 50.8 270)
				(length 3.81)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -15.24 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "8")
			)
			(pin power_in line
				(at -12.7 50.8 270)
				(length 3.81)
				(name "E5V")
				(number "6")
			)
			(pin power_in line
				(at -12.7 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "19")
			)
			(pin power_in line
				(at -10.16 50.8 270)
				(length 3.81)
				(name "IOREF")
				(number "12")
			)
			(pin power_in line
				(at -10.16 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "20")
			)
			(pin power_in line
				(at -7.62 50.8 270)
				(length 3.81)
				(name "+3V3")
				(number "16")
			)
			(pin power_in line
				(at -7.62 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "22")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 3.81)
				(name "+5V")
				(number "18")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "47")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 3.81)
				(name "VIN")
				(number "24")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "58")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 3.81)
				(name "VBAT")
				(number "33")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "77")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 3.81)
				(name "U5V")
				(number "46")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "78")
			)
			(pin power_in line
				(at 5.08 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "79")
			)
			(pin power_in line
				(at 7.62 -50.8 90)
				(length 3.81)
				(name "GND")
				(number "80")
			)
			(pin power_in line
				(at 12.7 50.8 270)
				(length 3.81)
				(name "AVDD")
				(number "45")
			)
			(pin power_in line
				(at 12.7 -50.8 90)
				(length 3.81)
				(name "AGND")
				(number "70")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 3.81)
				(name "PA0")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 3.81)
				(name "PA1")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 3.81)
				(name "STLINK_UART_TX/PA2")
				(number "73")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 3.81)
				(name "STLINK_UART_RX/PA3")
				(number "75")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 3.81)
				(name "PA4")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 3.81)
				(name "PA5")
				(number "49")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 3.81)
				(name "PA6")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 3.81)
				(name "PA7")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 3.81)
				(name "PA8")
				(number "61")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 3.81)
				(name "PA9")
				(number "59")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 3.81)
				(name "PA10")
				(number "71")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 3.81)
				(name "PA11")
				(number "52")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 3.81)
				(name "PA12")
				(number "50")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 3.81)
				(name "STLINK_TMS/PA13")
				(number "13")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 3.81)
				(name "STLINK_TCK/PA14")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 3.81)
				(name "PA15")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 3.81)
				(name "PB0")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 3.81)
				(name "PB1")
				(number "62")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 3.81)
				(name "PB2")
				(number "60")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 3.81)
				(name "STLINK_SWO/PB3")
				(number "69")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 3.81)
				(name "PB4")
				(number "65")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 3.81)
				(name "PB5")
				(number "67")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 3.81)
				(name "PB6")
				(number "55")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 3.81)
				(name "PB7")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 3.81)
				(name "PB8")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 3.81)
				(name "PB9")
				(number "43")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 3.81)
				(name "PB10")
				(number "63")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 3.81)
				(name "PB12")
				(number "54")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 3.81)
				(name "PB13")
				(number "68")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 3.81)
				(name "PB14")
				(number "66")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 3.81)
				(name "PB15")
				(number "64")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPOS6UL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -19.05 86.36 0)
		)
		(property "Value" "OPOS6UL"
			(at 15.24 -86.36 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.opossom.com/_downloads/opos6ul/documentation/datasheet_opos6ul.pdf"
			(at 0 0 0)
		)
		(property "Description" "Armadeus Systems i.MX6UL based single board computer, SODIMM"
			(at 0 0 0)
		)
		(property "ki_keywords" "armadeus systems opos6ul sbc som compute module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SODIMM*"
			(at 0 0 0)
		)
		(symbol "OPOS6UL_1_1"
			(pin bidirectional line
				(at -22.86 81.28 0)
				(length 3.81)
				(name "ENET_MDIO")
				(number "69")
			)
			(pin bidirectional line
				(at -22.86 78.74 0)
				(length 3.81)
				(name "ENET_MDC")
				(number "71")
			)
			(pin bidirectional line
				(at -22.86 76.2 0)
				(length 3.81)
				(name "ENET2_TX_CLK")
				(number "73")
			)
			(pin bidirectional line
				(at -22.86 73.66 0)
				(length 3.81)
				(name "ENET2_RX_ER")
				(number "77")
			)
			(pin bidirectional line
				(at -22.86 71.12 0)
				(length 3.81)
				(name "ENET2_RXDATA0")
				(number "79")
			)
			(pin bidirectional line
				(at -22.86 68.58 0)
				(length 3.81)
				(name "ENET2_RXDATA1")
				(number "81")
			)
			(pin bidirectional line
				(at -22.86 66.04 0)
				(length 3.81)
				(name "ENET2_RX_EN")
				(number "83")
			)
			(pin bidirectional line
				(at -22.86 63.5 0)
				(length 3.81)
				(name "ENET2_TX_EN")
				(number "85")
			)
			(pin bidirectional line
				(at -22.86 60.96 0)
				(length 3.81)
				(name "ENET2_TXDATA0")
				(number "87")
			)
			(pin bidirectional line
				(at -22.86 58.42 0)
				(length 3.81)
				(name "ENET2_TXDATA1")
				(number "89")
			)
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 3.81)
				(name "JTAG_TMS")
				(number "26")
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 3.81)
				(name "JTAG_TDO")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 3.81)
				(name "JTAG_TDI")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 3.81)
				(name "JTAG_TRST")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 3.81)
				(name "JTAG_TCK")
				(number "34")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 3.81)
				(name "UART1_CTS_B")
				(number "50")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 3.81)
				(name "UART1_RTS_B")
				(number "48")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 3.81)
				(name "UART1_TX")
				(number "52")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "UART1_RX")
				(number "54")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "UART2_CTS_B")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "UART2_RTS_B")
				(number "41")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "UART2_TX")
				(number "43")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "UART2_RX")
				(number "45")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "UART3_CTS_B")
				(number "49")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "UART3_RTS_B")
				(number "51")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "UART3_TX")
				(number "55")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "UART3_RX")
				(number "53")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "UART4_TX")
				(number "59")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "UART4_RX")
				(number "61")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "UART5_TX")
				(number "63")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "UART5_RX")
				(number "65")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "TAMPER9")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "TAMPER8")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "TAMPER7")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "TAMPER6")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "TAMPER5")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "TAMPER4")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "TAMPER3")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "TAMPER2")
				(number "18")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 3.81)
				(name "TAMPER1")
				(number "20")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "TAMPER0")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 -33.02 0)
				(length 3.81)
				(name "CSI_D7")
				(number "131")
			)
			(pin bidirectional line
				(at -22.86 -35.56 0)
				(length 3.81)
				(name "CSI_D6")
				(number "133")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 3.81)
				(name "CSI_D5")
				(number "135")
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 3.81)
				(name "CSI_D4")
				(number "137")
			)
			(pin bidirectional line
				(at -22.86 -43.18 0)
				(length 3.81)
				(name "CSI_D3")
				(number "139")
			)
			(pin bidirectional line
				(at -22.86 -45.72 0)
				(length 3.81)
				(name "CSI_D2")
				(number "141")
			)
			(pin bidirectional line
				(at -22.86 -48.26 0)
				(length 3.81)
				(name "CSI_D1")
				(number "143")
			)
			(pin bidirectional line
				(at -22.86 -50.8 0)
				(length 3.81)
				(name "CSI_D0")
				(number "145")
			)
			(pin bidirectional line
				(at -22.86 -53.34 0)
				(length 3.81)
				(name "CSI_VSYNC")
				(number "147")
			)
			(pin bidirectional line
				(at -22.86 -55.88 0)
				(length 3.81)
				(name "CSI_HSYNC")
				(number "149")
			)
			(pin bidirectional line
				(at -22.86 -58.42 0)
				(length 3.81)
				(name "CSI_PIXCLK")
				(number "153")
			)
			(pin bidirectional line
				(at -22.86 -60.96 0)
				(length 3.81)
				(name "CSI_MCLK")
				(number "157")
			)
			(pin input line
				(at -22.86 -66.04 0)
				(length 3.81)
				(name "ON/OFF")
				(number "199")
			)
			(pin input line
				(at -22.86 -68.58 0)
				(length 3.81)
				(name "POR_B")
				(number "197")
			)
			(pin input line
				(at -22.86 -71.12 0)
				(length 3.81)
				(name "BOOT_MODE1")
				(number "200")
			)
			(pin input line
				(at -22.86 -73.66 0)
				(length 3.81)
				(name "BOOT_MODE0")
				(number "198")
			)
			(pin power_in line
				(at 0 88.9 270)
				(length 3.81)
				(name "+3V3")
				(number "201")
			)
			(pin passive line
				(at 0 88.9 270)
				(length 3.81)
				(hide yes)
				(name "+3V3")
				(number "202")
			)
			(pin passive line
				(at 0 88.9 270)
				(length 3.81)
				(hide yes)
				(name "+3V3")
				(number "203")
			)
			(pin passive line
				(at 0 88.9 270)
				(length 3.81)
				(hide yes)
				(name "+3V3")
				(number "204")
			)
			(pin no_connect line
				(at 0 68.58 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "161")
			)
			(pin no_connect line
				(at 0 66.04 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "163")
			)
			(pin no_connect line
				(at 0 63.5 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "165")
			)
			(pin no_connect line
				(at 0 60.96 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "167")
			)
			(pin no_connect line
				(at 0 58.42 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "169")
			)
			(pin no_connect line
				(at 0 55.88 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "171")
			)
			(pin no_connect line
				(at 0 53.34 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "173")
			)
			(pin no_connect line
				(at 0 50.8 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "175")
			)
			(pin no_connect line
				(at 0 48.26 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "177")
			)
			(pin no_connect line
				(at 0 45.72 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "179")
			)
			(pin no_connect line
				(at 0 43.18 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "181")
			)
			(pin no_connect line
				(at 0 40.64 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "183")
			)
			(pin no_connect line
				(at 0 38.1 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "185")
			)
			(pin no_connect line
				(at 0 35.56 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "187")
			)
			(pin no_connect line
				(at 0 33.02 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "189")
			)
			(pin no_connect line
				(at 0 30.48 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "191")
			)
			(pin no_connect line
				(at 0 27.94 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "193")
			)
			(pin no_connect line
				(at 0 25.4 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "195")
			)
			(pin no_connect line
				(at 0 22.86 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "58")
			)
			(pin no_connect line
				(at 0 20.32 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "60")
			)
			(pin no_connect line
				(at 0 17.78 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "130")
			)
			(pin no_connect line
				(at 0 15.24 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "132")
			)
			(pin no_connect line
				(at 0 12.7 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "134")
			)
			(pin no_connect line
				(at 0 10.16 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "136")
			)
			(pin no_connect line
				(at 0 7.62 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "138")
			)
			(pin no_connect line
				(at 0 5.08 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "140")
			)
			(pin no_connect line
				(at 0 2.54 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "142")
			)
			(pin no_connect line
				(at 0 0 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "144")
			)
			(pin no_connect line
				(at 0 -2.54 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "146")
			)
			(pin no_connect line
				(at 0 -5.08 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "148")
			)
			(pin no_connect line
				(at 0 -7.62 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "150")
			)
			(pin no_connect line
				(at 0 -10.16 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "152")
			)
			(pin no_connect line
				(at 0 -12.7 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "154")
			)
			(pin no_connect line
				(at 0 -15.24 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "156")
			)
			(pin no_connect line
				(at 0 -17.78 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "158")
			)
			(pin no_connect line
				(at 0 -20.32 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "160")
			)
			(pin no_connect line
				(at 0 -22.86 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "162")
			)
			(pin no_connect line
				(at 0 -25.4 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "164")
			)
			(pin no_connect line
				(at 0 -27.94 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "166")
			)
			(pin no_connect line
				(at 0 -30.48 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "168")
			)
			(pin no_connect line
				(at 0 -33.02 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "170")
			)
			(pin no_connect line
				(at 0 -35.56 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "172")
			)
			(pin no_connect line
				(at 0 -38.1 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "174")
			)
			(pin no_connect line
				(at 0 -40.64 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "176")
			)
			(pin no_connect line
				(at 0 -43.18 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "178")
			)
			(pin no_connect line
				(at 0 -45.72 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "180")
			)
			(pin no_connect line
				(at 0 -48.26 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "182")
			)
			(pin no_connect line
				(at 0 -50.8 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "184")
			)
			(pin no_connect line
				(at 0 -53.34 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "186")
			)
			(pin no_connect line
				(at 0 -55.88 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "188")
			)
			(pin no_connect line
				(at 0 -58.42 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "190")
			)
			(pin no_connect line
				(at 0 -60.96 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "192")
			)
			(pin no_connect line
				(at 0 -63.5 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "194")
			)
			(pin no_connect line
				(at 0 -66.04 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "196")
			)
			(pin power_in line
				(at 0 -88.9 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "102")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "107")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "114")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "122")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "126")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "129")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "151")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "155")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "159")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "24")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "36")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "46")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "47")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "56")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "67")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "75")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "82")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "91")
			)
			(pin passive line
				(at 0 -88.9 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "92")
			)
			(pin power_in line
				(at 22.86 81.28 180)
				(length 3.81)
				(name "USB_OTG2_VBUS")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 78.74 180)
				(length 3.81)
				(name "USB_OTG2_DN")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 76.2 180)
				(length 3.81)
				(name "USB_OTG2_DP")
				(number "5")
			)
			(pin power_in line
				(at 22.86 71.12 180)
				(length 3.81)
				(name "USB_OTG1_VBUS")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 68.58 180)
				(length 3.81)
				(name "USB_OTG1_DN")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 66.04 180)
				(length 3.81)
				(name "USB_OTG1_DP")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 60.96 180)
				(length 3.81)
				(name "ETH_TXP")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 58.42 180)
				(length 3.81)
				(name "ETH_TXN")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 3.81)
				(name "ETH_RXP")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 3.81)
				(name "ETH_RXN")
				(number "29")
			)
			(pin output line
				(at 22.86 50.8 180)
				(length 3.81)
				(name "ETH_LED1")
				(number "33")
			)
			(pin output line
				(at 22.86 48.26 180)
				(length 3.81)
				(name "ETH_LED2")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 3.81)
				(name "LCD_D23")
				(number "93")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 3.81)
				(name "LCD_D22")
				(number "95")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 3.81)
				(name "LCD_D21")
				(number "97")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 3.81)
				(name "LCD_D20")
				(number "99")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 3.81)
				(name "LCD_D19")
				(number "101")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "LCD_D18")
				(number "103")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "LCD_D17")
				(number "105")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "LCD_D16")
				(number "74")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "LCD_D15")
				(number "76")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "LCD_D14")
				(number "78")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "LCD_D13")
				(number "80")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "LCD_D12")
				(number "84")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "LCD_D11")
				(number "86")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "LCD_D10")
				(number "88")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "LCD_D9")
				(number "90")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "LCD_D8")
				(number "94")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "LCD_D7")
				(number "96")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "LCD_D6")
				(number "98")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "LCD_D5")
				(number "100")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 3.81)
				(name "LCD_D4")
				(number "104")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "LCD_D3")
				(number "106")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "LCD_D2")
				(number "108")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "LCD_D1")
				(number "110")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "LCD_D0")
				(number "112")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "LCD_HSYNC")
				(number "116")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "LCD_RESET")
				(number "118")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "LCD_VSYNC")
				(number "120")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "LCD_DOTCLK")
				(number "124")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "LCD_ENABLE")
				(number "128")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 3.81)
				(name "AIN1/YNLR")
				(number "64")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 3.81)
				(name "AIN2/YPLL")
				(number "66")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 3.81)
				(name "AIN3/XNUR")
				(number "68")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 3.81)
				(name "AIN4/XPUL")
				(number "70")
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 3.81)
				(name "NAND_ALE")
				(number "127")
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 3.81)
				(name "NAND_WE_B")
				(number "109")
			)
			(pin bidirectional line
				(at 22.86 -50.8 180)
				(length 3.81)
				(name "NAND_RE_B")
				(number "111")
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 3.81)
				(name "NAND_DATA01")
				(number "113")
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 3.81)
				(name "NAND_DATA_02")
				(number "115")
			)
			(pin bidirectional line
				(at 22.86 -58.42 180)
				(length 3.81)
				(name "NAND_DATA03")
				(number "117")
			)
			(pin bidirectional line
				(at 22.86 -60.96 180)
				(length 3.81)
				(name "NAND_DATA04")
				(number "119")
			)
			(pin bidirectional line
				(at 22.86 -63.5 180)
				(length 3.81)
				(name "NAND_DATA05")
				(number "121")
			)
			(pin bidirectional line
				(at 22.86 -66.04 180)
				(length 3.81)
				(name "NAND_DATA06")
				(number "123")
			)
			(pin bidirectional line
				(at 22.86 -68.58 180)
				(length 3.81)
				(name "NAND_DATA07")
				(number "125")
			)
			(pin bidirectional line
				(at 22.86 -73.66 180)
				(length 3.81)
				(name "GPIO0")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 -76.2 180)
				(length 3.81)
				(name "GPIO5")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 -78.74 180)
				(length 3.81)
				(name "GPIO8")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 -81.28 180)
				(length 3.81)
				(name "GPIO9")
				(number "44")
			)
		)
		(embedded_fonts no)
	)
	(symbol "OPOS6UL_NANO"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 46.99 0)
		)
		(property "Value" "OPOS6UL_NANO"
			(at 2.54 -46.99 0)
		)
		(property "Footprint" ""
			(at -1.27 -36.83 0)
		)
		(property "Datasheet" "http://www.opossom.com/_downloads/opos6ul_nano/datasheet_opos6ul_nano.pdf"
			(at 0 0 0)
		)
		(property "Description" "NXP i.MX6ULL/i.MX6UL, 256 or 512 MB RAM, industrial SoM computer, M.2M (NGFF)"
			(at 0 0 0)
		)
		(property "ki_keywords" "opos6ul compute module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*M.2*"
			(at 0 0 0)
		)
		(symbol "OPOS6UL_NANO_0_1")
		(symbol "OPOS6UL_NANO_1_1"
			(pin input line
				(at -20.32 43.18 0)
				(length 2.54)
				(name "~{POR_B}")
				(number "4")
			)
			(pin power_in line
				(at -20.32 38.1 0)
				(length 2.54)
				(name "USB_OTG1_VBUS")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 2.54)
				(name "USB_OTG1_DN")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 2.54)
				(name "USB_OTG1_DP")
				(number "9")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 2.54)
				(name "USB_OTG2_DN")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 2.54)
				(name "USB_OTG2_DP")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 20.32 0)
				(length 2.54)
				(name "GPIO3")
				(number "15")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 2.54)
				(name "GPIO8")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 2.54)
				(name "GPIO9")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 2.54)
				(name "LCD_D0")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 2.54)
				(name "LCD_D1")
				(number "24")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 2.54)
				(name "LCD_D2")
				(number "29")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 2.54)
				(name "LCD_D3")
				(number "26")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 2.54)
				(name "LCD_D4")
				(number "31")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 2.54)
				(name "LCD_D5")
				(number "28")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 2.54)
				(name "LCD_D6")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 2.54)
				(name "LCD_D7")
				(number "30")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 2.54)
				(name "LCD_D8")
				(number "35")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 2.54)
				(name "LCD_D9")
				(number "32")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 2.54)
				(name "LCD_D10")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 2.54)
				(name "LCD_D11")
				(number "34")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 2.54)
				(name "LCD_D12")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 2.54)
				(name "LCD_D13")
				(number "36")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 2.54)
				(name "LCD_D14")
				(number "41")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 2.54)
				(name "LCD_D15")
				(number "38")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 2.54)
				(name "LCD_D16")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 2.54)
				(name "LCD_D17")
				(number "40")
			)
			(pin bidirectional line
				(at -20.32 -35.56 0)
				(length 2.54)
				(name "LCD_HSYNC")
				(number "42")
			)
			(pin bidirectional line
				(at -20.32 -38.1 0)
				(length 2.54)
				(name "LCD_VSYNC")
				(number "44")
			)
			(pin bidirectional line
				(at -20.32 -40.64 0)
				(length 2.54)
				(name "LCD_ENABLE")
				(number "46")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 2.54)
				(name "LCD_DOTCLK")
				(number "47")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 2.54)
				(name "+3V3")
				(number "1")
			)
			(pin passive line
				(at -2.54 48.26 270)
				(length 2.54)
				(hide yes)
				(name "+3V3")
				(number "2")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 2.54)
				(name "GND")
				(number "10")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "11")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "45")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin passive line
				(at 0 -48.26 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "71")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 2.54)
				(name "VSNVS")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 2.54)
				(name "UART1_RX")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 2.54)
				(name "UART1_TX")
				(number "19")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 2.54)
				(name "UART2_RX")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 2.54)
				(name "UART2_TX")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 2.54)
				(name "UART4_RX")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 2.54)
				(name "UART4_TX")
				(number "16")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 2.54)
				(name "UART5_RX")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 2.54)
				(name "UART5_TX")
				(number "20")
			)
			(pin output line
				(at 20.32 7.62 180)
				(length 2.54)
				(name "ETH_TXP")
				(number "73")
			)
			(pin output line
				(at 20.32 5.08 180)
				(length 2.54)
				(name "ETH_TXN")
				(number "75")
			)
			(pin input line
				(at 20.32 2.54 180)
				(length 2.54)
				(name "ETH_RXP")
				(number "72")
			)
			(pin input line
				(at 20.32 0 180)
				(length 2.54)
				(name "ETH_RXN")
				(number "74")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 2.54)
				(name "ETH_LED1")
				(number "68")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 2.54)
				(name "ETH_LED2")
				(number "70")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 2.54)
				(name "CSI_D0")
				(number "55")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 2.54)
				(name "CSI_D1")
				(number "52")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 2.54)
				(name "CSI_D2")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 2.54)
				(name "CSI_D3")
				(number "54")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 2.54)
				(name "CSI_D4")
				(number "67")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 2.54)
				(name "CSI_D5")
				(number "56")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 2.54)
				(name "CSI_D6")
				(number "69")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 2.54)
				(name "CSI_D7")
				(number "58")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 2.54)
				(name "CSI_HSYNC")
				(number "48")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 2.54)
				(name "CSI_VSYNC")
				(number "50")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 2.54)
				(name "CSI_PIXCLK")
				(number "51")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 2.54)
				(name "CSI_MCLK")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Olimex_MOD-WIFI-ESP8266-DEV"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 21.59 0)
		)
		(property "Value" "Olimex_MOD-WIFI-ESP8266-DEV"
			(at 1.27 19.05 0)
		)
		(property "Footprint" "Module:Olimex_MOD-WIFI-ESP8266-DEV"
			(at 0 -33.02 0)
		)
		(property "Datasheet" "https://raw.githubusercontent.com/OLIMEX/ESP8266/master/HARDWARE/MOD-WIFI-ESP8266-DEV/MOD-WiFi-ESP8266-DEV%20revision%20B2/MOD-WiFi-ESP8266-DEV_Rev_B2.pdf"
			(at 0 -30.48 0)
		)
		(property "Description" "ESP8266 development board"
			(at 0 0 0)
		)
		(property "ki_keywords" "ESP8266"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*MOD?WIFI?ESP8266?DEV*"
			(at 0 0 0)
		)
		(symbol "Olimex_MOD-WIFI-ESP8266-DEV_0_1")
		(symbol "Olimex_MOD-WIFI-ESP8266-DEV_1_1"
			(pin bidirectional line
				(at -12.7 15.24 0)
				(length 2.54)
				(name "GPIO-0")
				(number "21")
			)
			(pin bidirectional line
				(at -12.7 12.7 0)
				(length 2.54)
				(name "GPIO1")
				(number "3")
			)
			(pin bidirectional line
				(at -12.7 10.16 0)
				(length 2.54)
				(name "GPIO-2")
				(number "20")
			)
			(pin bidirectional line
				(at -12.7 7.62 0)
				(length 2.54)
				(name "GPIO3")
				(number "4")
			)
			(pin bidirectional line
				(at -12.7 5.08 0)
				(length 2.54)
				(name "GPIO4")
				(number "22")
			)
			(pin bidirectional line
				(at -12.7 2.54 0)
				(length 2.54)
				(name "GPIO5")
				(number "11")
			)
			(pin bidirectional line
				(at -12.7 -2.54 0)
				(length 2.54)
				(name "GPIO12")
				(number "16")
			)
			(pin bidirectional line
				(at -12.7 -5.08 0)
				(length 2.54)
				(name "GPIO13")
				(number "18")
			)
			(pin bidirectional line
				(at -12.7 -7.62 0)
				(length 2.54)
				(name "GPIO14")
				(number "17")
			)
			(pin bidirectional line
				(at -12.7 -10.16 0)
				(length 2.54)
				(name "GPIO15")
				(number "19")
			)
			(pin bidirectional line
				(at -12.7 -12.7 0)
				(length 2.54)
				(name "GPIO16")
				(number "15")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 2.54)
				(name "3.3V")
				(number "1")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 2.54)
				(name "GND")
				(number "2")
			)
			(pin unspecified line
				(at 12.7 15.24 180)
				(length 2.54)
				(name "SD_D0")
				(number "9")
			)
			(pin unspecified line
				(at 12.7 12.7 180)
				(length 2.54)
				(name "SD_D1")
				(number "7")
			)
			(pin unspecified line
				(at 12.7 10.16 180)
				(length 2.54)
				(name "SD_D2")
				(number "6")
			)
			(pin unspecified line
				(at 12.7 7.62 180)
				(length 2.54)
				(name "SD_D3")
				(number "10")
			)
			(pin unspecified line
				(at 12.7 2.54 180)
				(length 2.54)
				(name "SD_CLK")
				(number "5")
			)
			(pin unspecified line
				(at 12.7 0 180)
				(length 2.54)
				(name "SD_CMD")
				(number "8")
			)
			(pin unspecified line
				(at 12.7 -5.08 180)
				(length 2.54)
				(name "ADC")
				(number "12")
			)
			(pin input line
				(at 12.7 -10.16 180)
				(length 2.54)
				(name "RSTB")
				(number "13")
			)
			(pin unspecified line
				(at 12.7 -15.24 180)
				(length 2.54)
				(name "CHIP_E")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Omega2+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 29.21 0)
		)
		(property "Value" "Omega2+"
			(at 6.35 29.21 0)
		)
		(property "Footprint" "Module:Onion_Omega2+"
			(at 0 -38.1 0)
		)
		(property "Datasheet" "https://docs.onion.io/omega2-docs/omega2p.html"
			(at -81.28 -29.21 0)
		)
		(property "Description" "Iot Computer Module by Onion"
			(at 0 0 0)
		)
		(property "ki_keywords" "onion omega module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Onion*Omega2+*"
			(at 0 0 0)
		)
		(symbol "Omega2+_0_1")
		(symbol "Omega2+_1_1"
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "11")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "17")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "16")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "15")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "19")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "18")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "9/SPI_MISO")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "8/SPI_MOSI")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "7/SPI_CLK")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "6/SPI_CS1")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "3/I2S_CLK")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "2/I2S_WS")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "1/I2S_SDO")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "0/I2S_SDI")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "USB_D-")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "USB_D+")
				(number "30")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 2.54)
				(name "3.3V_VIN")
				(number "31")
			)
			(pin power_in line
				(at 0 -30.48 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -30.48 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin power_out line
				(at 2.54 30.48 270)
				(length 2.54)
				(name "3.3V_VOUT")
				(number "25")
			)
			(pin input line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "~{RST}")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "FW_RST/38")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "SER0_RX/13")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "SER0_TX/12")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "SER1_TX/45")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "SER1_RX/46")
				(number "8")
			)
			(pin output line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "ETH_TX-")
				(number "24")
			)
			(pin output line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "ETH_TX+")
				(number "23")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "ETH_RX-")
				(number "22")
			)
			(pin input line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "ETH_RX+")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -20.32 180)
				(length 2.54)
				(name "I2C_SCL/4")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "I2C_SDA/5")
				(number "17")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Omega2S"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 52.07 0)
		)
		(property "Value" "Omega2S"
			(at 17.78 52.07 0)
		)
		(property "Footprint" "Module:Onion_Omega2S"
			(at 0 -68.58 0)
		)
		(property "Datasheet" "https://github.com/OnionIoT/Omega2/raw/master/Documents/Omega2S%20Datasheet.pdf"
			(at 19.05 -26.67 0)
		)
		(property "Description" "Iot Computer Module by Onion, 64MB RAM, 16MB FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "onion omega module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Onion*Omega2S*"
			(at 0 0 0)
		)
		(symbol "Omega2S_0_1")
		(symbol "Omega2S_1_1"
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 2.54)
				(name "GPIO_11")
				(number "38")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 2.54)
				(name "GPIO_14")
				(number "45")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 2.54)
				(name "GPIO_15")
				(number "46")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 2.54)
				(name "GPIO_16")
				(number "47")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 2.54)
				(name "GPIO_17")
				(number "48")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 2.54)
				(name "GPIO_18/PWM_CH0")
				(number "49")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 2.54)
				(name "GPIO_19/PWM_CH1")
				(number "50")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 2.54)
				(name "GPIO_39/LINK4")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 2.54)
				(name "GPIO_40/LINK3")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 2.54)
				(name "GPIO_41")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 2.54)
				(name "GPIO_42")
				(number "17")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 2.54)
				(name "GPIO_43")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 2.54)
				(name "GPIO_44/~{WLED}")
				(number "19")
			)
			(pin output line
				(at -27.94 7.62 0)
				(length 2.54)
				(name "PCIE_TXN0")
				(number "10")
			)
			(pin output line
				(at -27.94 5.08 0)
				(length 2.54)
				(name "PCIE_TXP0")
				(number "11")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 2.54)
				(name "PCIE_RXN0")
				(number "13")
			)
			(pin input line
				(at -27.94 0 0)
				(length 2.54)
				(name "PCIE_RXP0")
				(number "12")
			)
			(pin output line
				(at -27.94 -2.54 0)
				(length 2.54)
				(name "PCIE_CKN0")
				(number "14")
			)
			(pin output line
				(at -27.94 -5.08 0)
				(length 2.54)
				(name "PCIE_CKP0")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 2.54)
				(name "GPIO_37/REFCLK")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 2.54)
				(name "GPIO_36/~{PERST}")
				(number "2")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 2.54)
				(name "SPI_MISO")
				(number "35")
			)
			(pin output line
				(at -27.94 -17.78 0)
				(length 2.54)
				(name "SPI_MOSI")
				(number "36")
			)
			(pin output line
				(at -27.94 -20.32 0)
				(length 2.54)
				(name "SPI_CLK")
				(number "34")
			)
			(pin output line
				(at -27.94 -22.86 0)
				(length 2.54)
				(name "SPI_CS0")
				(number "37")
			)
			(pin output line
				(at -27.94 -25.4 0)
				(length 2.54)
				(name "SPI_CS1")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 2.54)
				(name "GPIO_3/I2S_CLK")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 2.54)
				(name "GPIO_2/I2S_WS")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 2.54)
				(name "GPIO_1/I2S_SD0")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 2.54)
				(name "GPIO_0/I2S_SDI")
				(number "26")
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 2.54)
				(name "USB_DM")
				(number "62")
			)
			(pin bidirectional line
				(at -27.94 -45.72 0)
				(length 2.54)
				(name "USB_DP")
				(number "61")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 2.54)
				(name "3.3V")
				(number "8")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 2.54)
				(name "3.3V")
				(number "9")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 2.54)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "63")
			)
			(pin passive line
				(at 0 -53.34 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "64")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 2.54)
				(name "VDD_FLASH")
				(number "32")
			)
			(pin input line
				(at 27.94 43.18 180)
				(length 2.54)
				(name "~{HW_RST}")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 2.54)
				(name "SW_RST/GPIO_38")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 2.54)
				(name "UART_TXD0/GPIO_12")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 2.54)
				(name "UART_RXD0/GPIO_13")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 2.54)
				(name "UART_TXD1/GPIO_45")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 2.54)
				(name "UART_RXD1/GPIO_46")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 2.54)
				(name "UART_TXD2/PWM_CH2/GPIO_20")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 2.54)
				(name "UART_RXD2/PWM_CH3/GPIO_21")
				(number "52")
			)
			(pin passive line
				(at 27.94 2.54 180)
				(length 2.54)
				(name "WIFI_RF")
				(number "24")
			)
			(pin output line
				(at 27.94 -7.62 180)
				(length 2.54)
				(name "TX0_N0")
				(number "44")
			)
			(pin output line
				(at 27.94 -10.16 180)
				(length 2.54)
				(name "TXO_P0")
				(number "43")
			)
			(pin input line
				(at 27.94 -12.7 180)
				(length 2.54)
				(name "RXI_N0")
				(number "42")
			)
			(pin input line
				(at 27.94 -15.24 180)
				(length 2.54)
				(name "RXI_P0")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 2.54)
				(name "SD_D0/GPIO_25")
				(number "56")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 2.54)
				(name "SD_D1/GPIO_24")
				(number "55")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 2.54)
				(name "SD_D2/GPIO_29")
				(number "60")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 2.54)
				(name "SD_D3/GPIO_28")
				(number "59")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 2.54)
				(name "SD_CMD/GPIO_27")
				(number "58")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 2.54)
				(name "SD_CLK/GPIO_26")
				(number "57")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 2.54)
				(name "SD_CD/GPIO_23")
				(number "54")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 2.54)
				(name "SD_WP/GPIO_22")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 2.54)
				(name "I2C_SCLK/GPIO_4")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 2.54)
				(name "I2C_SDA/GPIO_5")
				(number "31")
			)
		)
		(embedded_fonts no)
	)
	(symbol "PocketBeagle"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -22.86 -54.61 0)
		)
		(property "Value" "PocketBeagle"
			(at 22.86 -54.61 0)
		)
		(property "Footprint" "Module:BeagleBoard_PocketBeagle"
			(at 0 0 0)
		)
		(property "Datasheet" "https://github.com/beagleboard/pocketbeagle/wiki/System-Reference-Manual"
			(at 43.18 -33.02 0)
		)
		(property "Description" "Singleboard computer with ARM Cortex-A8 1GHz, 512MB RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "beagleboard pocketbeagle"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BeagleBoard*PocketBeagle*"
			(at 0 0 0)
		)
		(symbol "PocketBeagle_0_1")
		(symbol "PocketBeagle_1_1"
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 2.54)
				(name "GPIO20")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 2.54)
				(name "GPIO23")
				(number "39")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 2.54)
				(name "GPIO26")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 2.54)
				(name "GPIO27")
				(number "55")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 2.54)
				(name "GPIO45")
				(number "69")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 2.54)
				(name "GPIO46")
				(number "58")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 2.54)
				(name "GPIO47")
				(number "54")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 2.54)
				(name "GPIO48")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 2.54)
				(name "GPIO52")
				(number "46")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 2.54)
				(name "GPIO57")
				(number "42")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 2.54)
				(name "GPIO58")
				(number "40")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 2.54)
				(name "GPIO59")
				(number "38")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 2.54)
				(name "GPIO60")
				(number "44")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 2.54)
				(name "GPIO64")
				(number "56")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 2.54)
				(name "GPIO65")
				(number "53")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 2.54)
				(name "GPIO89")
				(number "4")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 2.54)
				(name "AIN0(1.8V)")
				(number "19")
			)
			(pin input line
				(at -25.4 0 0)
				(length 2.54)
				(name "AIN1(1.8V)")
				(number "21")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 2.54)
				(name "AIN2(1.8V)")
				(number "23")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 2.54)
				(name "AIN3(1.8V)")
				(number "25")
			)
			(pin input line
				(at -25.4 -7.62 0)
				(length 2.54)
				(name "AIN4(1.8V)")
				(number "27")
			)
			(pin input line
				(at -25.4 -10.16 0)
				(length 2.54)
				(name "AIN5(3.3V)")
				(number "71")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 2.54)
				(name "AIN6/GPIO87")
				(number "2")
			)
			(pin input line
				(at -25.4 -15.24 0)
				(length 2.54)
				(name "AIN7(1.8V)")
				(number "72")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 2.54)
				(name "PRU0.1")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 2.54)
				(name "PRU0.2")
				(number "68")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 2.54)
				(name "PRU0.3")
				(number "66")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 2.54)
				(name "PRU0.4")
				(number "31")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 2.54)
				(name "PRU0.5")
				(number "70")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 2.54)
				(name "PRU0.6")
				(number "64")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 2.54)
				(name "PRU0.7")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 2.54)
				(name "PRU1.10")
				(number "35")
			)
			(pin input line
				(at -25.4 -43.18 0)
				(length 2.54)
				(name "~{RESET}")
				(number "62")
			)
			(pin input line
				(at -25.4 -48.26 0)
				(length 2.54)
				(name "PWR.BTN")
				(number "48")
			)
			(pin power_in line
				(at -15.24 55.88 270)
				(length 2.54)
				(name "VIN")
				(number "1")
			)
			(pin power_in line
				(at -10.16 55.88 270)
				(length 2.54)
				(name "USB1.VIN")
				(number "7")
			)
			(pin power_in line
				(at -5.08 55.88 270)
				(length 2.54)
				(name "BAT.VIN")
				(number "50")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 2.54)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "16")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "57")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 2.54)
				(name "AIN.VREF+")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 2.54)
				(name "AIN.VREF-")
				(number "17")
			)
			(pin power_out line
				(at 5.08 55.88 270)
				(length 2.54)
				(name "3.3V")
				(number "14")
			)
			(pin power_out line
				(at 7.62 55.88 270)
				(length 2.54)
				(name "3.3V")
				(number "59")
			)
			(pin power_out line
				(at 12.7 55.88 270)
				(length 2.54)
				(name "VOUT")
				(number "24")
			)
			(pin power_out line
				(at 15.24 55.88 270)
				(length 2.54)
				(name "VOUT")
				(number "49")
			)
			(pin output line
				(at 25.4 45.72 180)
				(length 2.54)
				(name "USB1.DRVVBUS")
				(number "3")
			)
			(pin input line
				(at 25.4 43.18 180)
				(length 2.54)
				(name "USB1.VBUS")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 40.64 180)
				(length 2.54)
				(name "USB1.D-")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 38.1 180)
				(length 2.54)
				(name "USB1.D+")
				(number "11")
			)
			(pin input line
				(at 25.4 35.56 180)
				(length 2.54)
				(name "USB1.ID")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 30.48 180)
				(length 2.54)
				(name "SPI0.CS")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 27.94 180)
				(length 2.54)
				(name "SPI0.CLK")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 25.4 180)
				(length 2.54)
				(name "SPI0.MISO")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 2.54)
				(name "SPI0.MOSI")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 2.54)
				(name "SPI1.CS")
				(number "67")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 2.54)
				(name "SPI1.CLK")
				(number "65")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 2.54)
				(name "SPI1.MISO")
				(number "63")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 2.54)
				(name "SPI1.MOSI")
				(number "61")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 2.54)
				(name "I2C1.SCL")
				(number "45")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 2.54)
				(name "I2C1.SDA")
				(number "47")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 2.54)
				(name "I2C2.SCL")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 2.54)
				(name "I2C2.SDA")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 2.54)
				(name "UART0.TX")
				(number "30")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 2.54)
				(name "UART0.RX")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 2.54)
				(name "UART4.TX")
				(number "43")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 2.54)
				(name "UART4.RX")
				(number "41")
			)
			(pin bidirectional line
				(at 25.4 -25.4 180)
				(length 2.54)
				(name "PWM0A")
				(number "36")
			)
			(pin bidirectional line
				(at 25.4 -27.94 180)
				(length 2.54)
				(name "PWM1A")
				(number "37")
			)
			(pin passive line
				(at 25.4 -33.02 180)
				(length 2.54)
				(name "BAT.TEMP")
				(number "52")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RaspberryPi-CM1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 81.28 0)
		)
		(property "Value" "RaspberryPi-CM1"
			(at 20.32 81.28 0)
		)
		(property "Footprint" ""
			(at -15.24 86.36 0)
		)
		(property "Datasheet" "https://www.raspberrypi.org/documentation/hardware/computemodule/datasheets/rpi_DATA_CM_1p0.pdf"
			(at -15.24 86.36 0)
		)
		(property "Description" "BCM2835 Broadcom 700 MZ single core, 512 MB RAM 4 GB eMMC, industrial SoM computer"
			(at 0 0 0)
		)
		(property "ki_keywords" "raspberry pi compute module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SODIMM*"
			(at 0 0 0)
		)
		(symbol "RaspberryPi-CM1_0_1")
		(symbol "RaspberryPi-CM1_1_1"
			(pin input line
				(at -25.4 76.2 0)
				(length 3.81)
				(name "RUN")
				(number "177")
			)
			(pin input line
				(at -25.4 73.66 0)
				(length 3.81)
				(name "~{EMMC_DISABLE}")
				(number "2")
			)
			(pin passive line
				(at -25.4 53.34 0)
				(length 3.81)
				(name "USB_OTGID")
				(number "168")
			)
			(pin bidirectional line
				(at -25.4 50.8 0)
				(length 3.81)
				(name "USB_DP")
				(number "165")
			)
			(pin bidirectional line
				(at -25.4 48.26 0)
				(length 3.81)
				(name "USB_DM")
				(number "167")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 3.81)
				(name "GPIO0")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 3.81)
				(name "GPIO1")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 3.81)
				(name "GPIO2")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "GPIO3")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "GPIO4")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "GPIO5")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "GPIO6")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "GPIO7")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "GPIO8")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "GPIO9")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "GPIO10")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "GPIO11")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "GPIO12")
				(number "45")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "GPIO13")
				(number "47")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "GPIO14")
				(number "51")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "GPIO15")
				(number "53")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "GPIO16")
				(number "57")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "GPIO17")
				(number "59")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "GPIO18")
				(number "63")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "GPIO19")
				(number "65")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "GPIO20")
				(number "69")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "GPIO21")
				(number "71")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "GPIO22")
				(number "75")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "GPIO23")
				(number "77")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "GPIO24")
				(number "81")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "GPIO25")
				(number "83")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "GPIO26")
				(number "87")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "GPIO27")
				(number "89")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "GPIO28")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "GPIO29")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 3.81)
				(name "GPIO30")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 3.81)
				(name "GPIO31")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 3.81)
				(name "GPIO32")
				(number "46")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 3.81)
				(name "GPIO33")
				(number "48")
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 3.81)
				(name "GPIO34")
				(number "52")
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 3.81)
				(name "GPIO35")
				(number "54")
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 3.81)
				(name "GPIO36")
				(number "58")
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 3.81)
				(name "GPIO37")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 3.81)
				(name "GPIO38")
				(number "64")
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 3.81)
				(name "GPIO39")
				(number "66")
			)
			(pin bidirectional line
				(at -25.4 -58.42 0)
				(length 3.81)
				(name "GPIO40")
				(number "70")
			)
			(pin bidirectional line
				(at -25.4 -60.96 0)
				(length 3.81)
				(name "GPIO41")
				(number "72")
			)
			(pin bidirectional line
				(at -25.4 -63.5 0)
				(length 3.81)
				(name "GPIO42")
				(number "76")
			)
			(pin bidirectional line
				(at -25.4 -66.04 0)
				(length 3.81)
				(name "GPIO43")
				(number "78")
			)
			(pin bidirectional line
				(at -25.4 -68.58 0)
				(length 3.81)
				(name "GPIO44")
				(number "82")
			)
			(pin bidirectional line
				(at -25.4 -71.12 0)
				(length 3.81)
				(name "GPIO45")
				(number "84")
			)
			(pin bidirectional line
				(at -25.4 -73.66 0)
				(length 3.81)
				(name "GPIO46_1V8")
				(number "88")
			)
			(pin bidirectional line
				(at -25.4 -76.2 0)
				(length 3.81)
				(name "GPIO47_1V8")
				(number "90")
			)
			(pin no_connect line
				(at -20.32 71.12 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -20.32 68.58 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -20.32 66.04 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -20.32 63.5 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -20.32 60.96 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at -20.32 58.42 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "1V8")
				(number "183")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "1V8")
				(number "184")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "1V8")
				(number "185")
			)
			(pin power_in line
				(at -7.62 83.82 270)
				(length 3.81)
				(name "1V8")
				(number "186")
			)
			(pin passive line
				(at -5.08 83.82 270)
				(length 3.81)
				(hide yes)
				(name "3V3")
				(number "191")
			)
			(pin passive line
				(at -5.08 83.82 270)
				(length 3.81)
				(hide yes)
				(name "3V3")
				(number "192")
			)
			(pin passive line
				(at -5.08 83.82 270)
				(length 3.81)
				(hide yes)
				(name "3V3")
				(number "193")
			)
			(pin power_in line
				(at -5.08 83.82 270)
				(length 3.81)
				(name "3V3")
				(number "194")
			)
			(pin passive line
				(at -2.54 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VBAT")
				(number "197")
			)
			(pin passive line
				(at -2.54 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VBAT")
				(number "198")
			)
			(pin passive line
				(at -2.54 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VBAT")
				(number "199")
			)
			(pin power_in line
				(at -2.54 83.82 270)
				(length 3.81)
				(name "VBAT")
				(number "200")
			)
			(pin no_connect line
				(at 0 78.74 270)
				(length 2.54)
				(hide yes)
				(name "VDD_CORE_(DO_NOT_CONNECT)")
				(number "179")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "104")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "109")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "110")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "115")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "116")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "121")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "122")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "127")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "133")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "134")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "139")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "140")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "145")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "146")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "151")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "152")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "157")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "163")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "164")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "169")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "170")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "181")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "182")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "187")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "188")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "195")
			)
			(pin power_out line
				(at 0 -83.82 90)
				(length 3.81)
				(name "GND")
				(number "196")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "56")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "67")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "68")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "74")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "80")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "85")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "86")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "91")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "92")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "97")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "98")
			)
			(pin passive line
				(at 2.54 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VDAC")
				(number "189")
			)
			(pin power_in line
				(at 2.54 83.82 270)
				(length 3.81)
				(name "VDAC")
				(number "190")
			)
			(pin no_connect line
				(at 2.54 -78.74 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "8")
			)
			(pin no_connect line
				(at 5.08 78.74 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin no_connect line
				(at 5.08 -78.74 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin passive line
				(at 7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "GPIO0-27_VDD")
				(number "39")
			)
			(pin power_in line
				(at 7.62 83.82 270)
				(length 3.81)
				(name "GPIO0-27_VDD")
				(number "40")
			)
			(pin no_connect line
				(at 7.62 -78.74 90)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin passive line
				(at 10.16 83.82 270)
				(length 3.81)
				(hide yes)
				(name "GPIO28-45_VDD")
				(number "41")
			)
			(pin power_in line
				(at 10.16 83.82 270)
				(length 3.81)
				(name "GPIO28-45_VDD")
				(number "42")
			)
			(pin no_connect line
				(at 12.7 78.74 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 20.32 76.2 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "124")
			)
			(pin no_connect line
				(at 20.32 73.66 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "126")
			)
			(pin no_connect line
				(at 20.32 71.12 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "128")
			)
			(pin no_connect line
				(at 20.32 66.04 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "130")
			)
			(pin no_connect line
				(at 20.32 48.26 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "132")
			)
			(pin no_connect line
				(at 20.32 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "158")
			)
			(pin no_connect line
				(at 20.32 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "156")
			)
			(pin no_connect line
				(at 20.32 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "154")
			)
			(pin no_connect line
				(at 20.32 -60.96 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "160")
			)
			(pin no_connect line
				(at 20.32 -63.5 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "162")
			)
			(pin output line
				(at 25.4 68.58 180)
				(length 3.81)
				(name "TVDAC")
				(number "166")
			)
			(pin output line
				(at 25.4 63.5 180)
				(length 3.81)
				(name "DSI0_CP")
				(number "107")
			)
			(pin output line
				(at 25.4 60.96 180)
				(length 3.81)
				(name "DSI0_CN")
				(number "105")
			)
			(pin output line
				(at 25.4 58.42 180)
				(length 3.81)
				(name "DSI0_DP0")
				(number "101")
			)
			(pin output line
				(at 25.4 55.88 180)
				(length 3.81)
				(name "DSI0_DN0")
				(number "99")
			)
			(pin output line
				(at 25.4 53.34 180)
				(length 3.81)
				(name "DSI0_DP1")
				(number "95")
			)
			(pin output line
				(at 25.4 50.8 180)
				(length 3.81)
				(name "DSI0_DN1")
				(number "93")
			)
			(pin output line
				(at 25.4 45.72 180)
				(length 3.81)
				(name "DSI1_CP")
				(number "100")
			)
			(pin output line
				(at 25.4 43.18 180)
				(length 3.81)
				(name "DSI1_CN")
				(number "102")
			)
			(pin output line
				(at 25.4 40.64 180)
				(length 3.81)
				(name "DSI1_DP0")
				(number "94")
			)
			(pin output line
				(at 25.4 38.1 180)
				(length 3.81)
				(name "DSI1_DN0")
				(number "96")
			)
			(pin output line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "DSI1_DP1")
				(number "118")
			)
			(pin output line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "DSI1_DN1")
				(number "120")
			)
			(pin output line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "DSI1_DP2")
				(number "112")
			)
			(pin output line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "DSI1_DN2")
				(number "114")
			)
			(pin output line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "DSI1_DP3")
				(number "106")
			)
			(pin output line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "DSI1_DN3")
				(number "108")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "HDMI_CEC")
				(number "171")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "HDMI_SDA")
				(number "173")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "HDMI_SCL")
				(number "175")
			)
			(pin output line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "HDMI_CLK_P")
				(number "113")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "HDMI_CLK_N")
				(number "111")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "HDMI_D0_P")
				(number "119")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "HDMI_D0_N")
				(number "117")
			)
			(pin output line
				(at 25.4 0 180)
				(length 3.81)
				(name "HDMI_D1_P")
				(number "125")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "HDMI_D1_N")
				(number "123")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "HDMI_D2_P")
				(number "131")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "HDMI_D2_N")
				(number "129")
			)
			(pin input line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "CAM0_CP")
				(number "142")
			)
			(pin input line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "CAM0_CN")
				(number "144")
			)
			(pin input line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "CAM0_DP0")
				(number "136")
			)
			(pin input line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "CAM0_DN0")
				(number "138")
			)
			(pin input line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "CAM0_DP1")
				(number "148")
			)
			(pin input line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "CAM0_DN1")
				(number "150")
			)
			(pin input line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "CAM1_CP")
				(number "147")
			)
			(pin input line
				(at 25.4 -38.1 180)
				(length 3.81)
				(name "CAM1_CN")
				(number "149")
			)
			(pin input line
				(at 25.4 -40.64 180)
				(length 3.81)
				(name "CAM1_DP0")
				(number "159")
			)
			(pin input line
				(at 25.4 -43.18 180)
				(length 3.81)
				(name "CAM1_DN0")
				(number "161")
			)
			(pin input line
				(at 25.4 -45.72 180)
				(length 3.81)
				(name "CAM1_DP1")
				(number "153")
			)
			(pin input line
				(at 25.4 -48.26 180)
				(length 3.81)
				(name "CAM1_DN1")
				(number "155")
			)
			(pin input line
				(at 25.4 -50.8 180)
				(length 3.81)
				(name "CAM1_DP2")
				(number "141")
			)
			(pin input line
				(at 25.4 -53.34 180)
				(length 3.81)
				(name "CAM1_DN2")
				(number "143")
			)
			(pin input line
				(at 25.4 -55.88 180)
				(length 3.81)
				(name "CAM1_DP3")
				(number "135")
			)
			(pin input line
				(at 25.4 -58.42 180)
				(length 3.81)
				(name "CAM1_DN3")
				(number "137")
			)
			(pin input line
				(at 25.4 -66.04 180)
				(length 3.81)
				(name "VC_TMS")
				(number "176")
			)
			(pin input line
				(at 25.4 -68.58 180)
				(length 3.81)
				(name "~{VC_TRST}")
				(number "172")
			)
			(pin input line
				(at 25.4 -71.12 180)
				(length 3.81)
				(name "VC_TCK")
				(number "180")
			)
			(pin input line
				(at 25.4 -73.66 180)
				(length 3.81)
				(name "VC_TDI")
				(number "174")
			)
			(pin output line
				(at 25.4 -76.2 180)
				(length 3.81)
				(name "VC_TDO")
				(number "178")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RaspberryPi-CM3+"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 81.28 0)
		)
		(property "Value" "RaspberryPi-CM3+"
			(at 20.32 81.28 0)
		)
		(property "Footprint" ""
			(at -15.24 86.36 0)
		)
		(property "Datasheet" "https://www.raspberrypi.org/documentation/hardware/computemodule/datasheets/rpi_DATA_CM3plus_1p0.pdf"
			(at -15.24 86.36 0)
		)
		(property "Description" "BCM2837B0 Broadcom 1.2 GHZ quad core, 1 GB RAM 8/16/32 GB eMMC, industrial SoM computer"
			(at 0 0 0)
		)
		(property "ki_keywords" "raspberry pi compute module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SODIMM*"
			(at 0 0 0)
		)
		(symbol "RaspberryPi-CM3+_0_1")
		(symbol "RaspberryPi-CM3+_1_1"
			(pin input line
				(at -25.4 76.2 0)
				(length 3.81)
				(name "RUN")
				(number "177")
			)
			(pin input line
				(at -25.4 73.66 0)
				(length 3.81)
				(name "~{EMMC_DISABLE}")
				(number "2")
			)
			(pin output line
				(at -25.4 71.12 0)
				(length 3.81)
				(name "EMMC_EN_N_1V8")
				(number "90")
			)
			(pin passive line
				(at -25.4 48.26 0)
				(length 3.81)
				(name "USB_OTGID")
				(number "168")
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 3.81)
				(name "USB_DP")
				(number "165")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 3.81)
				(name "USB_DM")
				(number "167")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 3.81)
				(name "GPIO0")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "GPIO1")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "GPIO2")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "GPIO3")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "GPIO4")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "GPIO5")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "GPIO6")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "GPIO7")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "GPIO8")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "GPIO9")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "GPIO10")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "GPIO11")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "GPIO12")
				(number "45")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "GPIO13")
				(number "47")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "GPIO14")
				(number "51")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "GPIO15")
				(number "53")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "GPIO16")
				(number "57")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "GPIO17")
				(number "59")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "GPIO18")
				(number "63")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "GPIO19")
				(number "65")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "GPIO20")
				(number "69")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "GPIO21")
				(number "71")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "GPIO22")
				(number "75")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "GPIO23")
				(number "77")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "GPIO24")
				(number "81")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "GPIO25")
				(number "83")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "GPIO26")
				(number "87")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "GPIO27")
				(number "89")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 3.81)
				(name "GPIO28")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 3.81)
				(name "GPIO29")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 3.81)
				(name "GPIO30")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 3.81)
				(name "GPIO31")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 3.81)
				(name "GPIO32")
				(number "46")
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 3.81)
				(name "GPIO33")
				(number "48")
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 3.81)
				(name "GPIO34")
				(number "52")
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 3.81)
				(name "GPIO35")
				(number "54")
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 3.81)
				(name "GPIO36")
				(number "58")
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 3.81)
				(name "GPIO37")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 -58.42 0)
				(length 3.81)
				(name "GPIO38")
				(number "64")
			)
			(pin bidirectional line
				(at -25.4 -60.96 0)
				(length 3.81)
				(name "GPIO39")
				(number "66")
			)
			(pin bidirectional line
				(at -25.4 -63.5 0)
				(length 3.81)
				(name "GPIO40")
				(number "70")
			)
			(pin bidirectional line
				(at -25.4 -66.04 0)
				(length 3.81)
				(name "GPIO41")
				(number "72")
			)
			(pin bidirectional line
				(at -25.4 -68.58 0)
				(length 3.81)
				(name "GPIO42")
				(number "76")
			)
			(pin bidirectional line
				(at -25.4 -71.12 0)
				(length 3.81)
				(name "GPIO43")
				(number "78")
			)
			(pin bidirectional line
				(at -25.4 -73.66 0)
				(length 3.81)
				(name "GPIO44")
				(number "82")
			)
			(pin bidirectional line
				(at -25.4 -76.2 0)
				(length 3.81)
				(name "GPIO45")
				(number "84")
			)
			(pin no_connect line
				(at -20.32 66.04 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "10")
			)
			(pin no_connect line
				(at -20.32 63.5 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -20.32 60.96 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -20.32 58.42 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -20.32 55.88 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "22")
			)
			(pin no_connect line
				(at -20.32 53.34 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "1V8")
				(number "183")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "1V8")
				(number "184")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "1V8")
				(number "185")
			)
			(pin power_in line
				(at -7.62 83.82 270)
				(length 3.81)
				(name "1V8")
				(number "186")
			)
			(pin passive line
				(at -5.08 83.82 270)
				(length 3.81)
				(hide yes)
				(name "3V3")
				(number "191")
			)
			(pin passive line
				(at -5.08 83.82 270)
				(length 3.81)
				(hide yes)
				(name "3V3")
				(number "192")
			)
			(pin passive line
				(at -5.08 83.82 270)
				(length 3.81)
				(hide yes)
				(name "3V3")
				(number "193")
			)
			(pin power_in line
				(at -5.08 83.82 270)
				(length 3.81)
				(name "3V3")
				(number "194")
			)
			(pin passive line
				(at -2.54 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VBAT")
				(number "197")
			)
			(pin passive line
				(at -2.54 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VBAT")
				(number "198")
			)
			(pin passive line
				(at -2.54 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VBAT")
				(number "199")
			)
			(pin power_in line
				(at -2.54 83.82 270)
				(length 3.81)
				(name "VBAT")
				(number "200")
			)
			(pin no_connect line
				(at 0 78.74 270)
				(length 2.54)
				(hide yes)
				(name "VDD_CORE_(DO_NOT_CONNECT)")
				(number "179")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "104")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "109")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "110")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "115")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "116")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "121")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "122")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "127")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "133")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "134")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "139")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "140")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "145")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "146")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "151")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "152")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "157")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "163")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "164")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "169")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "170")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "181")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "182")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "187")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "188")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "195")
			)
			(pin power_out line
				(at 0 -83.82 90)
				(length 3.81)
				(name "GND")
				(number "196")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "56")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "67")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "68")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "74")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "80")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "85")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "86")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "91")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "92")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "97")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "98")
			)
			(pin passive line
				(at 2.54 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VDAC")
				(number "189")
			)
			(pin power_in line
				(at 2.54 83.82 270)
				(length 3.81)
				(name "VDAC")
				(number "190")
			)
			(pin no_connect line
				(at 5.08 78.74 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "4")
			)
			(pin passive line
				(at 7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "GPIO0-27_VDD")
				(number "39")
			)
			(pin power_in line
				(at 7.62 83.82 270)
				(length 3.81)
				(name "GPIO0-27_VDD")
				(number "40")
			)
			(pin passive line
				(at 10.16 83.82 270)
				(length 3.81)
				(hide yes)
				(name "GPIO28-45_VDD")
				(number "41")
			)
			(pin power_in line
				(at 10.16 83.82 270)
				(length 3.81)
				(name "GPIO28-45_VDD")
				(number "42")
			)
			(pin no_connect line
				(at 12.7 78.74 270)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "6")
			)
			(pin no_connect line
				(at 20.32 76.2 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "124")
			)
			(pin no_connect line
				(at 20.32 73.66 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "126")
			)
			(pin no_connect line
				(at 20.32 71.12 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "128")
			)
			(pin no_connect line
				(at 20.32 66.04 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "130")
			)
			(pin no_connect line
				(at 20.32 48.26 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "132")
			)
			(pin no_connect line
				(at 20.32 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "158")
			)
			(pin no_connect line
				(at 20.32 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "156")
			)
			(pin no_connect line
				(at 20.32 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "154")
			)
			(pin no_connect line
				(at 20.32 -60.96 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "160")
			)
			(pin no_connect line
				(at 20.32 -63.5 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "162")
			)
			(pin output line
				(at 25.4 68.58 180)
				(length 3.81)
				(name "TVDAC")
				(number "166")
			)
			(pin output line
				(at 25.4 63.5 180)
				(length 3.81)
				(name "DSI0_CP")
				(number "107")
			)
			(pin output line
				(at 25.4 60.96 180)
				(length 3.81)
				(name "DSI0_CN")
				(number "105")
			)
			(pin output line
				(at 25.4 58.42 180)
				(length 3.81)
				(name "DSI0_DP0")
				(number "101")
			)
			(pin output line
				(at 25.4 55.88 180)
				(length 3.81)
				(name "DSI0_DN0")
				(number "99")
			)
			(pin output line
				(at 25.4 53.34 180)
				(length 3.81)
				(name "DSI0_DP1")
				(number "95")
			)
			(pin output line
				(at 25.4 50.8 180)
				(length 3.81)
				(name "DSI0_DN1")
				(number "93")
			)
			(pin output line
				(at 25.4 45.72 180)
				(length 3.81)
				(name "DSI1_CP")
				(number "100")
			)
			(pin output line
				(at 25.4 43.18 180)
				(length 3.81)
				(name "DSI1_CN")
				(number "102")
			)
			(pin output line
				(at 25.4 40.64 180)
				(length 3.81)
				(name "DSI1_DP0")
				(number "94")
			)
			(pin output line
				(at 25.4 38.1 180)
				(length 3.81)
				(name "DSI1_DN0")
				(number "96")
			)
			(pin output line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "DSI1_DP1")
				(number "118")
			)
			(pin output line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "DSI1_DN1")
				(number "120")
			)
			(pin output line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "DSI1_DP2")
				(number "112")
			)
			(pin output line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "DSI1_DN2")
				(number "114")
			)
			(pin output line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "DSI1_DP3")
				(number "106")
			)
			(pin output line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "DSI1_DN3")
				(number "108")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "HDMI_CEC")
				(number "171")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "HDMI_SDA")
				(number "173")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "HDMI_SCL")
				(number "175")
			)
			(pin output line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "HDMI_CLK_P")
				(number "113")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "HDMI_CLK_N")
				(number "111")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "HDMI_D0_P")
				(number "119")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "HDMI_D0_N")
				(number "117")
			)
			(pin output line
				(at 25.4 0 180)
				(length 3.81)
				(name "HDMI_D1_P")
				(number "125")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "HDMI_D1_N")
				(number "123")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "HDMI_D2_P")
				(number "131")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "HDMI_D2_N")
				(number "129")
			)
			(pin input line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "HDMI_HPD_N_1V8")
				(number "88")
			)
			(pin input line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "CAM0_CP")
				(number "142")
			)
			(pin input line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "CAM0_CN")
				(number "144")
			)
			(pin input line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "CAM0_DP0")
				(number "136")
			)
			(pin input line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "CAM0_DN0")
				(number "138")
			)
			(pin input line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "CAM0_DP1")
				(number "148")
			)
			(pin input line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "CAM0_DN1")
				(number "150")
			)
			(pin input line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "CAM1_CP")
				(number "147")
			)
			(pin input line
				(at 25.4 -38.1 180)
				(length 3.81)
				(name "CAM1_CN")
				(number "149")
			)
			(pin input line
				(at 25.4 -40.64 180)
				(length 3.81)
				(name "CAM1_DP0")
				(number "159")
			)
			(pin input line
				(at 25.4 -43.18 180)
				(length 3.81)
				(name "CAM1_DN0")
				(number "161")
			)
			(pin input line
				(at 25.4 -45.72 180)
				(length 3.81)
				(name "CAM1_DP1")
				(number "153")
			)
			(pin input line
				(at 25.4 -48.26 180)
				(length 3.81)
				(name "CAM1_DN1")
				(number "155")
			)
			(pin input line
				(at 25.4 -50.8 180)
				(length 3.81)
				(name "CAM1_DP2")
				(number "141")
			)
			(pin input line
				(at 25.4 -53.34 180)
				(length 3.81)
				(name "CAM1_DN2")
				(number "143")
			)
			(pin input line
				(at 25.4 -55.88 180)
				(length 3.81)
				(name "CAM1_DP3")
				(number "135")
			)
			(pin input line
				(at 25.4 -58.42 180)
				(length 3.81)
				(name "CAM1_DN3")
				(number "137")
			)
			(pin input line
				(at 25.4 -66.04 180)
				(length 3.81)
				(name "VC_TMS")
				(number "176")
			)
			(pin input line
				(at 25.4 -68.58 180)
				(length 3.81)
				(name "~{VC_TRST}")
				(number "172")
			)
			(pin input line
				(at 25.4 -71.12 180)
				(length 3.81)
				(name "VC_TCK")
				(number "180")
			)
			(pin input line
				(at 25.4 -73.66 180)
				(length 3.81)
				(name "VC_TDI")
				(number "174")
			)
			(pin output line
				(at 25.4 -76.2 180)
				(length 3.81)
				(name "VC_TDO")
				(number "178")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RaspberryPi-CM3+L"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 81.28 0)
		)
		(property "Value" "RaspberryPi-CM3+L"
			(at 20.32 81.28 0)
		)
		(property "Footprint" ""
			(at -15.24 86.36 0)
		)
		(property "Datasheet" "https://www.raspberrypi.org/documentation/hardware/computemodule/datasheets/rpi_DATA_CM3plus_1p0.pdf"
			(at -15.24 86.36 0)
		)
		(property "Description" "BCM2837B0 Broadcom 1.2 GHZ quad core, 1 GB RAM, industrial SoM computer"
			(at 0 0 0)
		)
		(property "ki_keywords" "raspberry pi compute module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SODIMM*"
			(at 0 0 0)
		)
		(symbol "RaspberryPi-CM3+L_0_1")
		(symbol "RaspberryPi-CM3+L_1_1"
			(pin input line
				(at -25.4 76.2 0)
				(length 3.81)
				(name "RUN")
				(number "177")
			)
			(pin input line
				(at -25.4 73.66 0)
				(length 3.81)
				(name "~{EMMC_DISABLE}")
				(number "2")
			)
			(pin output line
				(at -25.4 71.12 0)
				(length 3.81)
				(name "EMMC_EN_N_1V8")
				(number "90")
			)
			(pin output line
				(at -25.4 66.04 0)
				(length 3.81)
				(name "SDX_CLK")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 63.5 0)
				(length 3.81)
				(name "SDX_CMD")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 60.96 0)
				(length 3.81)
				(name "SDX_D0")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 58.42 0)
				(length 3.81)
				(name "SDX_D1")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 55.88 0)
				(length 3.81)
				(name "SDX_D2")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 53.34 0)
				(length 3.81)
				(name "SDX_D3")
				(number "24")
			)
			(pin passive line
				(at -25.4 48.26 0)
				(length 3.81)
				(name "USB_OTGID")
				(number "168")
			)
			(pin bidirectional line
				(at -25.4 45.72 0)
				(length 3.81)
				(name "USB_DP")
				(number "165")
			)
			(pin bidirectional line
				(at -25.4 43.18 0)
				(length 3.81)
				(name "USB_DM")
				(number "167")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 3.81)
				(name "GPIO0")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 3.81)
				(name "GPIO1")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 33.02 0)
				(length 3.81)
				(name "GPIO2")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 3.81)
				(name "GPIO3")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 3.81)
				(name "GPIO4")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 25.4 0)
				(length 3.81)
				(name "GPIO5")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 3.81)
				(name "GPIO6")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 3.81)
				(name "GPIO7")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 3.81)
				(name "GPIO8")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 3.81)
				(name "GPIO9")
				(number "29")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 3.81)
				(name "GPIO10")
				(number "33")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 3.81)
				(name "GPIO11")
				(number "35")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 3.81)
				(name "GPIO12")
				(number "45")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 3.81)
				(name "GPIO13")
				(number "47")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 3.81)
				(name "GPIO14")
				(number "51")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 3.81)
				(name "GPIO15")
				(number "53")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 3.81)
				(name "GPIO16")
				(number "57")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 3.81)
				(name "GPIO17")
				(number "59")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 3.81)
				(name "GPIO18")
				(number "63")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 3.81)
				(name "GPIO19")
				(number "65")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 3.81)
				(name "GPIO20")
				(number "69")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 3.81)
				(name "GPIO21")
				(number "71")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 3.81)
				(name "GPIO22")
				(number "75")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 3.81)
				(name "GPIO23")
				(number "77")
			)
			(pin bidirectional line
				(at -25.4 -22.86 0)
				(length 3.81)
				(name "GPIO24")
				(number "81")
			)
			(pin bidirectional line
				(at -25.4 -25.4 0)
				(length 3.81)
				(name "GPIO25")
				(number "83")
			)
			(pin bidirectional line
				(at -25.4 -27.94 0)
				(length 3.81)
				(name "GPIO26")
				(number "87")
			)
			(pin bidirectional line
				(at -25.4 -30.48 0)
				(length 3.81)
				(name "GPIO27")
				(number "89")
			)
			(pin bidirectional line
				(at -25.4 -33.02 0)
				(length 3.81)
				(name "GPIO28")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 -35.56 0)
				(length 3.81)
				(name "GPIO29")
				(number "30")
			)
			(pin bidirectional line
				(at -25.4 -38.1 0)
				(length 3.81)
				(name "GPIO30")
				(number "34")
			)
			(pin bidirectional line
				(at -25.4 -40.64 0)
				(length 3.81)
				(name "GPIO31")
				(number "36")
			)
			(pin bidirectional line
				(at -25.4 -43.18 0)
				(length 3.81)
				(name "GPIO32")
				(number "46")
			)
			(pin bidirectional line
				(at -25.4 -45.72 0)
				(length 3.81)
				(name "GPIO33")
				(number "48")
			)
			(pin bidirectional line
				(at -25.4 -48.26 0)
				(length 3.81)
				(name "GPIO34")
				(number "52")
			)
			(pin bidirectional line
				(at -25.4 -50.8 0)
				(length 3.81)
				(name "GPIO35")
				(number "54")
			)
			(pin bidirectional line
				(at -25.4 -53.34 0)
				(length 3.81)
				(name "GPIO36")
				(number "58")
			)
			(pin bidirectional line
				(at -25.4 -55.88 0)
				(length 3.81)
				(name "GPIO37")
				(number "60")
			)
			(pin bidirectional line
				(at -25.4 -58.42 0)
				(length 3.81)
				(name "GPIO38")
				(number "64")
			)
			(pin bidirectional line
				(at -25.4 -60.96 0)
				(length 3.81)
				(name "GPIO39")
				(number "66")
			)
			(pin bidirectional line
				(at -25.4 -63.5 0)
				(length 3.81)
				(name "GPIO40")
				(number "70")
			)
			(pin bidirectional line
				(at -25.4 -66.04 0)
				(length 3.81)
				(name "GPIO41")
				(number "72")
			)
			(pin bidirectional line
				(at -25.4 -68.58 0)
				(length 3.81)
				(name "GPIO42")
				(number "76")
			)
			(pin bidirectional line
				(at -25.4 -71.12 0)
				(length 3.81)
				(name "GPIO43")
				(number "78")
			)
			(pin bidirectional line
				(at -25.4 -73.66 0)
				(length 3.81)
				(name "GPIO44")
				(number "82")
			)
			(pin bidirectional line
				(at -25.4 -76.2 0)
				(length 3.81)
				(name "GPIO45")
				(number "84")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "1V8")
				(number "183")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "1V8")
				(number "184")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "1V8")
				(number "185")
			)
			(pin power_in line
				(at -7.62 83.82 270)
				(length 3.81)
				(name "1V8")
				(number "186")
			)
			(pin passive line
				(at -5.08 83.82 270)
				(length 3.81)
				(hide yes)
				(name "3V3")
				(number "191")
			)
			(pin passive line
				(at -5.08 83.82 270)
				(length 3.81)
				(hide yes)
				(name "3V3")
				(number "192")
			)
			(pin passive line
				(at -5.08 83.82 270)
				(length 3.81)
				(hide yes)
				(name "3V3")
				(number "193")
			)
			(pin power_in line
				(at -5.08 83.82 270)
				(length 3.81)
				(name "3V3")
				(number "194")
			)
			(pin passive line
				(at -2.54 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VBAT")
				(number "197")
			)
			(pin passive line
				(at -2.54 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VBAT")
				(number "198")
			)
			(pin passive line
				(at -2.54 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VBAT")
				(number "199")
			)
			(pin power_in line
				(at -2.54 83.82 270)
				(length 3.81)
				(name "VBAT")
				(number "200")
			)
			(pin no_connect line
				(at 0 78.74 270)
				(length 2.54)
				(hide yes)
				(name "VDD_CORE_(DO_NOT_CONNECT)")
				(number "179")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "104")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "109")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "110")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "115")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "116")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "121")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "122")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "127")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "133")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "134")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "139")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "14")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "140")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "145")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "146")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "151")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "152")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "157")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "163")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "164")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "169")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "170")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "181")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "182")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "187")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "188")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "19")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "195")
			)
			(pin power_out line
				(at 0 -83.82 90)
				(length 3.81)
				(name "GND")
				(number "196")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "25")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "31")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "32")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "37")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "43")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "44")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "49")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "55")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "56")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "61")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "62")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "67")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "68")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "7")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "73")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "74")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "79")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "80")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "85")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "86")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "91")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "92")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "97")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "98")
			)
			(pin passive line
				(at 2.54 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VDAC")
				(number "189")
			)
			(pin power_in line
				(at 2.54 83.82 270)
				(length 3.81)
				(name "VDAC")
				(number "190")
			)
			(pin passive line
				(at 5.08 83.82 270)
				(length 3.81)
				(hide yes)
				(name "SDX_VDD")
				(number "4")
			)
			(pin power_in line
				(at 5.08 83.82 270)
				(length 3.81)
				(name "SDX_VDD")
				(number "6")
			)
			(pin passive line
				(at 7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "GPIO0-27_VDD")
				(number "39")
			)
			(pin power_in line
				(at 7.62 83.82 270)
				(length 3.81)
				(name "GPIO0-27_VDD")
				(number "40")
			)
			(pin passive line
				(at 10.16 83.82 270)
				(length 3.81)
				(hide yes)
				(name "GPIO28-45_VDD")
				(number "41")
			)
			(pin power_in line
				(at 10.16 83.82 270)
				(length 3.81)
				(name "GPIO28-45_VDD")
				(number "42")
			)
			(pin no_connect line
				(at 20.32 76.2 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "124")
			)
			(pin no_connect line
				(at 20.32 73.66 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "126")
			)
			(pin no_connect line
				(at 20.32 71.12 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "128")
			)
			(pin no_connect line
				(at 20.32 66.04 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "130")
			)
			(pin no_connect line
				(at 20.32 48.26 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "132")
			)
			(pin no_connect line
				(at 20.32 20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "158")
			)
			(pin no_connect line
				(at 20.32 -12.7 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "156")
			)
			(pin no_connect line
				(at 20.32 -15.24 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "154")
			)
			(pin no_connect line
				(at 20.32 -60.96 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "160")
			)
			(pin no_connect line
				(at 20.32 -63.5 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "162")
			)
			(pin output line
				(at 25.4 68.58 180)
				(length 3.81)
				(name "TVDAC")
				(number "166")
			)
			(pin output line
				(at 25.4 63.5 180)
				(length 3.81)
				(name "DSI0_CP")
				(number "107")
			)
			(pin output line
				(at 25.4 60.96 180)
				(length 3.81)
				(name "DSI0_CN")
				(number "105")
			)
			(pin output line
				(at 25.4 58.42 180)
				(length 3.81)
				(name "DSI0_DP0")
				(number "101")
			)
			(pin output line
				(at 25.4 55.88 180)
				(length 3.81)
				(name "DSI0_DN0")
				(number "99")
			)
			(pin output line
				(at 25.4 53.34 180)
				(length 3.81)
				(name "DSI0_DP1")
				(number "95")
			)
			(pin output line
				(at 25.4 50.8 180)
				(length 3.81)
				(name "DSI0_DN1")
				(number "93")
			)
			(pin output line
				(at 25.4 45.72 180)
				(length 3.81)
				(name "DSI1_CP")
				(number "100")
			)
			(pin output line
				(at 25.4 43.18 180)
				(length 3.81)
				(name "DSI1_CN")
				(number "102")
			)
			(pin output line
				(at 25.4 40.64 180)
				(length 3.81)
				(name "DSI1_DP0")
				(number "94")
			)
			(pin output line
				(at 25.4 38.1 180)
				(length 3.81)
				(name "DSI1_DN0")
				(number "96")
			)
			(pin output line
				(at 25.4 35.56 180)
				(length 3.81)
				(name "DSI1_DP1")
				(number "118")
			)
			(pin output line
				(at 25.4 33.02 180)
				(length 3.81)
				(name "DSI1_DN1")
				(number "120")
			)
			(pin output line
				(at 25.4 30.48 180)
				(length 3.81)
				(name "DSI1_DP2")
				(number "112")
			)
			(pin output line
				(at 25.4 27.94 180)
				(length 3.81)
				(name "DSI1_DN2")
				(number "114")
			)
			(pin output line
				(at 25.4 25.4 180)
				(length 3.81)
				(name "DSI1_DP3")
				(number "106")
			)
			(pin output line
				(at 25.4 22.86 180)
				(length 3.81)
				(name "DSI1_DN3")
				(number "108")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 3.81)
				(name "HDMI_CEC")
				(number "171")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 3.81)
				(name "HDMI_SDA")
				(number "173")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 3.81)
				(name "HDMI_SCL")
				(number "175")
			)
			(pin output line
				(at 25.4 10.16 180)
				(length 3.81)
				(name "HDMI_CLK_P")
				(number "113")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 3.81)
				(name "HDMI_CLK_N")
				(number "111")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 3.81)
				(name "HDMI_D0_P")
				(number "119")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 3.81)
				(name "HDMI_D0_N")
				(number "117")
			)
			(pin output line
				(at 25.4 0 180)
				(length 3.81)
				(name "HDMI_D1_P")
				(number "125")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 3.81)
				(name "HDMI_D1_N")
				(number "123")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 3.81)
				(name "HDMI_D2_P")
				(number "131")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 3.81)
				(name "HDMI_D2_N")
				(number "129")
			)
			(pin input line
				(at 25.4 -10.16 180)
				(length 3.81)
				(name "HDMI_HPD_N_1V8")
				(number "88")
			)
			(pin input line
				(at 25.4 -17.78 180)
				(length 3.81)
				(name "CAM0_CP")
				(number "142")
			)
			(pin input line
				(at 25.4 -20.32 180)
				(length 3.81)
				(name "CAM0_CN")
				(number "144")
			)
			(pin input line
				(at 25.4 -22.86 180)
				(length 3.81)
				(name "CAM0_DP0")
				(number "136")
			)
			(pin input line
				(at 25.4 -25.4 180)
				(length 3.81)
				(name "CAM0_DN0")
				(number "138")
			)
			(pin input line
				(at 25.4 -27.94 180)
				(length 3.81)
				(name "CAM0_DP1")
				(number "148")
			)
			(pin input line
				(at 25.4 -30.48 180)
				(length 3.81)
				(name "CAM0_DN1")
				(number "150")
			)
			(pin input line
				(at 25.4 -35.56 180)
				(length 3.81)
				(name "CAM1_CP")
				(number "147")
			)
			(pin input line
				(at 25.4 -38.1 180)
				(length 3.81)
				(name "CAM1_CN")
				(number "149")
			)
			(pin input line
				(at 25.4 -40.64 180)
				(length 3.81)
				(name "CAM1_DP0")
				(number "159")
			)
			(pin input line
				(at 25.4 -43.18 180)
				(length 3.81)
				(name "CAM1_DN0")
				(number "161")
			)
			(pin input line
				(at 25.4 -45.72 180)
				(length 3.81)
				(name "CAM1_DP1")
				(number "153")
			)
			(pin input line
				(at 25.4 -48.26 180)
				(length 3.81)
				(name "CAM1_DN1")
				(number "155")
			)
			(pin input line
				(at 25.4 -50.8 180)
				(length 3.81)
				(name "CAM1_DP2")
				(number "141")
			)
			(pin input line
				(at 25.4 -53.34 180)
				(length 3.81)
				(name "CAM1_DN2")
				(number "143")
			)
			(pin input line
				(at 25.4 -55.88 180)
				(length 3.81)
				(name "CAM1_DP3")
				(number "135")
			)
			(pin input line
				(at 25.4 -58.42 180)
				(length 3.81)
				(name "CAM1_DN3")
				(number "137")
			)
			(pin input line
				(at 25.4 -66.04 180)
				(length 3.81)
				(name "VC_TMS")
				(number "176")
			)
			(pin input line
				(at 25.4 -68.58 180)
				(length 3.81)
				(name "~{VC_TRST}")
				(number "172")
			)
			(pin input line
				(at 25.4 -71.12 180)
				(length 3.81)
				(name "VC_TCK")
				(number "180")
			)
			(pin input line
				(at 25.4 -73.66 180)
				(length 3.81)
				(name "VC_TDI")
				(number "174")
			)
			(pin output line
				(at 25.4 -76.2 180)
				(length 3.81)
				(name "VC_TDO")
				(number "178")
			)
		)
		(embedded_fonts no)
	)
	(symbol "RaspberryPi_Pico"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -19.05 35.56 0)
		)
		(property "Value" "RaspberryPi_Pico"
			(at 7.62 35.56 0)
		)
		(property "Footprint" "Module:RaspberryPi_Pico_Common_Unspecified"
			(at 0 -46.99 0)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 0 -49.53 0)
		)
		(property "Description" "Versatile and inexpensive microcontroller module powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash; also supports Raspberry Pi Pico 2"
			(at 0 -52.07 0)
		)
		(property "ki_keywords" "RP2350A M33 RISC-V Hazard3 usb"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?Common* RaspberryPi?Pico?SMD*"
			(at 0 0 0)
		)
		(symbol "RaspberryPi_Pico_0_1")
		(symbol "RaspberryPi_Pico_1_1"
			(pin passive line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "RUN")
				(number "30")
				(alternate "~{RESET}" passive line)
			)
			(pin passive line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "3V3_EN")
				(number "37")
				(alternate "~{3V3_DISABLE}" passive line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "GPIO0")
				(number "1")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "GPIO1")
				(number "2")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" passive line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "GPIO2")
				(number "4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "GPIO3")
				(number "5")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "GPIO4")
				(number "6")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "GPIO5")
				(number "7")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "GPIO6")
				(number "9")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "GPIO7")
				(number "10")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM3_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "GPIO8")
				(number "11")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM4_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "GPIO9")
				(number "12")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM4_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "GPIO10")
				(number "14")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "GPIO11")
				(number "15")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "GPIO12")
				(number "16")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "GPIO13")
				(number "17")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM6_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "GPIO14")
				(number "19")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM7_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "GPIO15")
				(number "20")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM7_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 3.81)
				(name "VSYS")
				(number "39")
				(alternate "VSYS_OUT" power_out line)
			)
			(pin power_out line
				(at 0 38.1 270)
				(length 3.81)
				(name "VBUS")
				(number "40")
				(alternate "VBUS_IN" power_in line)
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin power_out line
				(at 0 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "3")
				(alternate "GND_IN" power_in line)
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin power_out line
				(at 5.08 38.1 270)
				(length 3.81)
				(name "3V3")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "GPIO16")
				(number "21")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "GPIO17")
				(number "22")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "GPIO18")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "GPIO19")
				(number "25")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "GPIO20")
				(number "26")
				(alternate "CLOCK_GPIN0" input clock)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "GPIO21")
				(number "27")
				(alternate "CLOCK_GPOUT0" output clock)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "GPIO22")
				(number "29")
				(alternate "CLOCK_GPIN1" input clock)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_in line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "ADC_VREF")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "GPIO26_ADC0")
				(number "31")
				(alternate "ADC0" input line)
				(alternate "GPIO26" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "GPIO27_ADC1")
				(number "32")
				(alternate "ADC1" input line)
				(alternate "GPIO27" bidirectional line)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "GPIO28_ADC2")
				(number "34")
				(alternate "ADC2" input line)
				(alternate "GPIO28" bidirectional line)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_out line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "AGND")
				(number "33")
				(alternate "GND" passive line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "RaspberryPi_Pico_Debug"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -19.05 35.56 0)
		)
		(property "Value" "RaspberryPi_Pico"
			(at 7.62 35.56 0)
		)
		(property "Footprint" "Module:RaspberryPi_Pico_SMD_HandSolder"
			(at 0 -46.99 0)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 0 -49.53 0)
		)
		(property "Description" "Versatile and inexpensive microcontroller module (with debug pins) powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash; also supports Raspberry Pi Pico 2"
			(at 0 -52.07 0)
		)
		(property "ki_keywords" "RP2350A M33 RISC-V Hazard3 usb swd"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?SMD*"
			(at 0 0 0)
		)
		(symbol "RaspberryPi_Pico_Debug_0_1")
		(symbol "RaspberryPi_Pico_Debug_1_1"
			(pin input line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "SWCLK")
				(number "D1")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "SWDIO")
				(number "D3")
			)
			(pin passive line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "RUN")
				(number "30")
				(alternate "~{RESET}" passive line)
			)
			(pin passive line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "3V3_EN")
				(number "37")
				(alternate "~{3V3_DISABLE}" passive line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "GPIO0")
				(number "1")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "GPIO1")
				(number "2")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" passive line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "GPIO2")
				(number "4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "GPIO3")
				(number "5")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "GPIO4")
				(number "6")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "GPIO5")
				(number "7")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "GPIO6")
				(number "9")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "GPIO7")
				(number "10")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM3_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "GPIO8")
				(number "11")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM4_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "GPIO9")
				(number "12")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM4_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "GPIO10")
				(number "14")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "GPIO11")
				(number "15")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "GPIO12")
				(number "16")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "GPIO13")
				(number "17")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM6_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "GPIO14")
				(number "19")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM7_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "GPIO15")
				(number "20")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM7_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 3.81)
				(name "VSYS")
				(number "39")
				(alternate "VSYS_OUT" power_out line)
			)
			(pin power_out line
				(at 0 38.1 270)
				(length 3.81)
				(name "VBUS")
				(number "40")
				(alternate "VBUS_IN" power_in line)
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin power_out line
				(at 0 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "3")
				(alternate "GND_IN" power_in line)
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin power_out line
				(at 5.08 38.1 270)
				(length 3.81)
				(name "3V3")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "GPIO16")
				(number "21")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "GPIO17")
				(number "22")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "GPIO18")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "GPIO19")
				(number "25")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "GPIO20")
				(number "26")
				(alternate "CLOCK_GPIN0" input clock)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "GPIO21")
				(number "27")
				(alternate "CLOCK_GPOUT0" output clock)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "GPIO22")
				(number "29")
				(alternate "CLOCK_GPIN1" input clock)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_in line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "ADC_VREF")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "GPIO26_ADC0")
				(number "31")
				(alternate "ADC0" input line)
				(alternate "GPIO26" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "GPIO27_ADC1")
				(number "32")
				(alternate "ADC1" input line)
				(alternate "GPIO27" bidirectional line)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "GPIO28_ADC2")
				(number "34")
				(alternate "ADC2" input line)
				(alternate "GPIO28" bidirectional line)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_out line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "AGND")
				(number "33")
				(alternate "GND" passive line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "RaspberryPi_Pico_Extensive"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "A"
			(at -19.05 35.56 0)
		)
		(property "Value" "RaspberryPi_Pico"
			(at 7.62 35.56 0)
		)
		(property "Footprint" "Module:RaspberryPi_Pico_SMD"
			(at 0 -46.99 0)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/pico/pico-datasheet.pdf"
			(at 0 -49.53 0)
		)
		(property "Description" "Versatile and inexpensive microcontroller module (with full pinout for test point and debug connections) powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash; also supports Raspberry Pi Pico 2"
			(at 0 -52.07 0)
		)
		(property "ki_keywords" "RP2350A M33 RISC-V Hazard3 usb swd"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?SMD"
			(at 0 0 0)
		)
		(symbol "RaspberryPi_Pico_Extensive_0_1")
		(symbol "RaspberryPi_Pico_Extensive_1_1"
			(pin input line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "SWCLK")
				(number "D1")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "SWDIO")
				(number "D3")
			)
			(pin passive line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "RUN")
				(number "30")
				(alternate "~{RESET}" passive line)
			)
			(pin passive line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "3V3_EN")
				(number "37")
				(alternate "~{3V3_DISABLE}" passive line)
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "GPIO0")
				(number "1")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "GPIO1")
				(number "2")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" passive line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "GPIO2")
				(number "4")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "GPIO3")
				(number "5")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "GPIO4")
				(number "6")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "GPIO5")
				(number "7")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "GPIO6")
				(number "9")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "GPIO7")
				(number "10")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM3_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "GPIO8")
				(number "11")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM4_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "GPIO9")
				(number "12")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM4_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "GPIO10")
				(number "14")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "GPIO11")
				(number "15")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 3.81)
				(name "GPIO12")
				(number "16")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "GPIO13")
				(number "17")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM6_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_DET" input line)
				(alternate "~{SPI1_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "GPIO14")
				(number "19")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM7_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "GPIO15")
				(number "20")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM7_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "~{BOOTSEL}")
				(number "TP6")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 3.81)
				(name "VSYS")
				(number "39")
				(alternate "VSYS_OUT" power_out line)
			)
			(pin power_out line
				(at 0 38.1 270)
				(length 3.81)
				(name "VBUS")
				(number "40")
				(alternate "VBUS_IN" power_in line)
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "13")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "18")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin power_out line
				(at 0 -35.56 90)
				(length 3.81)
				(name "GND")
				(number "3")
				(alternate "GND_IN" power_in line)
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "8")
			)
			(pin passive line
				(at 0 -35.56 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "D2")
			)
			(pin power_out line
				(at 5.08 38.1 270)
				(length 3.81)
				(name "3V3")
				(number "36")
			)
			(pin power_out line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "USB_GND")
				(number "TP1")
				(alternate "USB_GND_IN" power_in line)
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "USB_DM")
				(number "TP2")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "USB_DP")
				(number "TP3")
			)
			(pin no_connect line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "~{SMPS_PS}")
				(number "TP4")
				(alternate "GPIO23_UNSAFE" output line)
				(alternate "~{SMPS_PS_UNSAFE}" output line)
			)
			(pin output line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "LED_OUT")
				(number "TP5")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "GPIO16")
				(number "21")
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM0_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "GPIO17")
				(number "22")
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM0_B" bidirectional line)
				(alternate "UART0_RX" input line)
				(alternate "USB_VBUS_EN" output line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "GPIO18")
				(number "24")
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM1_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART0_CTS" input line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "GPIO19")
				(number "25")
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM1_B" bidirectional line)
				(alternate "SPI0_TX" output line)
				(alternate "UART0_RTS" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "GPIO20")
				(number "26")
				(alternate "CLOCK_GPIN0" input clock)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM2_A" output line)
				(alternate "SPI0_RX" input line)
				(alternate "UART1_TX" output line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "GPIO21")
				(number "27")
				(alternate "CLOCK_GPOUT0" output clock)
				(alternate "I2C0_SCL" bidirectional clock)
				(alternate "PWM2_B" bidirectional line)
				(alternate "UART1_RX" input line)
				(alternate "USB_OVCUR_DET" input line)
				(alternate "~{SPI0_CSn}" bidirectional line)
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "GPIO22")
				(number "29")
				(alternate "CLOCK_GPIN1" input clock)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM3_A" output line)
				(alternate "SPI0_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_in line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "ADC_VREF")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "GPIO26_ADC0")
				(number "31")
				(alternate "ADC0" input line)
				(alternate "GPIO26" bidirectional line)
				(alternate "I2C1_SDA" bidirectional line)
				(alternate "PWM5_A" output line)
				(alternate "SPI1_SCK" bidirectional clock)
				(alternate "UART1_CTS" input line)
				(alternate "USB_VBUS_EN" output line)
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "GPIO27_ADC1")
				(number "32")
				(alternate "ADC1" input line)
				(alternate "GPIO27" bidirectional line)
				(alternate "I2C1_SCL" bidirectional clock)
				(alternate "PWM5_B" bidirectional line)
				(alternate "SPI1_TX" output line)
				(alternate "UART1_RTS" output line)
				(alternate "USB_OVCUR_DET" input line)
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "GPIO28_ADC2")
				(number "34")
				(alternate "ADC2" input line)
				(alternate "GPIO28" bidirectional line)
				(alternate "I2C0_SDA" bidirectional line)
				(alternate "PWM6_A" output line)
				(alternate "SPI1_RX" input line)
				(alternate "UART0_TX" output line)
				(alternate "USB_VBUS_DET" input line)
			)
			(pin power_out line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "AGND")
				(number "33")
				(alternate "GND" passive line)
			)
		)
		(embedded_fonts no)
	)
	(symbol "Sipeed-M1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.716 51.308 0)
		)
		(property "Value" "Sipeed-M1"
			(at -11.938 49.53 0)
		)
		(property "Footprint" "Module:Sipeed-M1"
			(at -0.762 -1.524 0)
		)
		(property "Datasheet" "https://dl.sipeed.com/MAIX/HDK/Sipeed-M1&M1W/Specifications"
			(at -7.62 6.35 0)
		)
		(property "Description" "AI accelerated RISC-V microcontroller"
			(at 0 0 0)
		)
		(property "ki_keywords" "AI Kendryte K210 RISC-V"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sipeed?*M1*"
			(at 0 0 0)
		)
		(symbol "Sipeed-M1_0_1")
		(symbol "Sipeed-M1_1_1"
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "RST")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "LCD_D0")
				(number "63")
			)
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "LCD_D1")
				(number "62")
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "LCD_D2")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "LCD_D3")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "LCD_D4")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "LCD_D5")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "LCD_D6")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "LCD_D7")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "DVP_D0")
				(number "71")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DVP_D1")
				(number "70")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DVP_D2")
				(number "69")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DVP_D3")
				(number "68")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DVP_D4")
				(number "67")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "DVP_D5")
				(number "66")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DVP_D6")
				(number "65")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DVP_D7")
				(number "64")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "IO36")
				(number "37")
				(alternate "LCD_CS" output line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "IO37")
				(number "38")
				(alternate "LCD_RST" output line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "IO38")
				(number "39")
				(alternate "LCD_DC" output line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "IO39")
				(number "40")
				(alternate "LCD_WR" output line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "IO40")
				(number "41")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "IO41")
				(number "42")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "IO42")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "IO43")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "IO44")
				(number "45")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "IO45")
				(number "46")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "IO46")
				(number "47")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "IO47")
				(number "48")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "5V")
				(number "51")
			)
			(pin passive line
				(at -2.54 50.8 270)
				(length 2.54)
				(hide yes)
				(name "5V")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "49")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin power_out line
				(at 5.08 50.8 270)
				(length 2.54)
				(name "3V3")
				(number "54")
			)
			(pin power_out line
				(at 7.62 50.8 270)
				(length 2.54)
				(name "1V8")
				(number "53")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "IO0/JTAG_TCK")
				(number "1")
				(alternate "JTAG_TCK" input line)
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "IO1/JTAG_TDI")
				(number "2")
				(alternate "JTAG_TDI" input line)
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "IO2/JTAG_TMS")
				(number "3")
				(alternate "JTAG_TMS" input line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "IO3/JTAG_TDO")
				(number "4")
				(alternate "JTAG_TDO" output line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "IO4/ISP_Rx")
				(number "5")
				(alternate "ISP_RX" input line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "IO5/ISP_Tx")
				(number "6")
				(alternate "ISP_Tx" output line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "IO6")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "IO7")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "IO8")
				(number "9")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "IO9")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "IO10")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IO11")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "IO12")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "IO13")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "IO14")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "IO15")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "IO16/BOOT")
				(number "17")
				(alternate "BOOT" input line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "IO17")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "IO18")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "IO19")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IO20")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "IO21")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "IO22")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "IO23")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "IO24")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "IO25")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "IO26")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "IO27")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "IO28")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "IO29")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "IO30")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "IO31")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "IO32")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "IO33")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "IO34")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -45.72 180)
				(length 2.54)
				(name "IO35")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Sipeed-M1W"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.462 51.816 0)
		)
		(property "Value" "Sipeed-M1W"
			(at -12.7 49.53 0)
		)
		(property "Footprint" "Module:Sipeed-M1W"
			(at 2.54 2.54 0)
		)
		(property "Datasheet" "https://dl.sipeed.com/MAIX/HDK/Sipeed-M1&M1W/Specifications"
			(at 2.54 2.54 0)
		)
		(property "Description" "AI Accelerated RISC-V MCU with WiFi"
			(at 2.54 2.54 0)
		)
		(property "ki_keywords" "WiFi K210 Kendryte"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Sipeed?*M1W*"
			(at 0 0 0)
		)
		(symbol "Sipeed-M1W_0_1")
		(symbol "Sipeed-M1W_1_1"
			(pin input line
				(at -15.24 40.64 0)
				(length 2.54)
				(name "RST")
				(number "55")
			)
			(pin bidirectional line
				(at -15.24 35.56 0)
				(length 2.54)
				(name "LCD_D0")
				(number "63")
			)
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "LCD_D1")
				(number "62")
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "LCD_D2")
				(number "61")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "LCD_D3")
				(number "60")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "LCD_D4")
				(number "59")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "LCD_D5")
				(number "58")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "LCD_D6")
				(number "57")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "LCD_D7")
				(number "56")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "DVP_D0")
				(number "71")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "DVP_D1")
				(number "70")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "DVP_D2")
				(number "69")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "DVP_D3")
				(number "68")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "DVP_D4")
				(number "67")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "DVP_D5")
				(number "66")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "DVP_D6")
				(number "65")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "DVP_D7")
				(number "64")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "IO36")
				(number "37")
				(alternate "LCD_CS" output line)
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "IO37")
				(number "38")
				(alternate "LCD_RST" output line)
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "IO38")
				(number "39")
				(alternate "LCD_DC" output line)
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "IO39")
				(number "40")
				(alternate "LCD_WR" output line)
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "IO40")
				(number "41")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "IO41")
				(number "42")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "IO42")
				(number "43")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "IO43")
				(number "44")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "IO44")
				(number "45")
			)
			(pin bidirectional line
				(at -15.24 -33.02 0)
				(length 2.54)
				(name "IO45")
				(number "46")
			)
			(pin bidirectional line
				(at -15.24 -35.56 0)
				(length 2.54)
				(name "IO46")
				(number "47")
			)
			(pin bidirectional line
				(at -15.24 -38.1 0)
				(length 2.54)
				(name "IO47")
				(number "48")
			)
			(pin power_in line
				(at -2.54 50.8 270)
				(length 2.54)
				(name "5V")
				(number "51")
			)
			(pin passive line
				(at -2.54 50.8 270)
				(length 2.54)
				(hide yes)
				(name "5V")
				(number "52")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 2.54)
				(name "GND")
				(number "49")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -50.8 90)
				(length 2.54)
				(hide yes)
				(name "GND")
				(number "72")
			)
			(pin power_out line
				(at 5.08 50.8 270)
				(length 2.54)
				(name "3V3")
				(number "54")
			)
			(pin power_out line
				(at 7.62 50.8 270)
				(length 2.54)
				(name "1V8")
				(number "53")
			)
			(pin bidirectional line
				(at 15.24 43.18 180)
				(length 2.54)
				(name "IO0/JTAG_TCK")
				(number "1")
				(alternate "JTAG_TCK" input line)
				(alternate "WIFI_SPI_CS" output line)
			)
			(pin bidirectional line
				(at 15.24 40.64 180)
				(length 2.54)
				(name "IO1/JTAG_TDI")
				(number "2")
				(alternate "JTAG_TDI" input line)
				(alternate "WIFI_SPI_CLK" output line)
			)
			(pin bidirectional line
				(at 15.24 38.1 180)
				(length 2.54)
				(name "IO2/JTAG_TMS")
				(number "3")
				(alternate "JTAG_TMS" input line)
				(alternate "WIFI_SPI_MISO" input line)
			)
			(pin bidirectional line
				(at 15.24 35.56 180)
				(length 2.54)
				(name "IO3/JTAG_TDO")
				(number "4")
				(alternate "JTAG_TDO" output line)
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "IO4/ISP_RX")
				(number "5")
				(alternate "ISP_RX" input line)
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "IO5/ISP_TX")
				(number "6")
				(alternate "ISP_TX" input line)
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "IO6")
				(number "7")
				(alternate "MCU_RX" input line)
				(alternate "WIFI_TX" output line)
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "IO7")
				(number "8")
				(alternate "MCU_TX" output line)
				(alternate "WIFI_RX" input line)
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "IO8")
				(number "9")
				(alternate "WIFI_EN" input line)
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "IO9")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "IO10")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "IO11")
				(number "12")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "IO12")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "IO13")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "IO14")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "IO15")
				(number "16")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "IO16/BOOT")
				(number "17")
				(alternate "BOOT" input line)
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "IO17")
				(number "18")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "IO18")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "IO19")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "IO20")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "IO21")
				(number "22")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "IO22")
				(number "23")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "IO23")
				(number "24")
			)
			(pin bidirectional line
				(at 15.24 -17.78 180)
				(length 2.54)
				(name "IO24")
				(number "25")
			)
			(pin bidirectional line
				(at 15.24 -20.32 180)
				(length 2.54)
				(name "IO25")
				(number "26")
			)
			(pin bidirectional line
				(at 15.24 -22.86 180)
				(length 2.54)
				(name "IO26")
				(number "27")
			)
			(pin bidirectional line
				(at 15.24 -25.4 180)
				(length 2.54)
				(name "IO27")
				(number "28")
			)
			(pin bidirectional line
				(at 15.24 -27.94 180)
				(length 2.54)
				(name "IO28")
				(number "29")
			)
			(pin bidirectional line
				(at 15.24 -30.48 180)
				(length 2.54)
				(name "IO29")
				(number "30")
			)
			(pin bidirectional line
				(at 15.24 -33.02 180)
				(length 2.54)
				(name "IO30")
				(number "31")
			)
			(pin bidirectional line
				(at 15.24 -35.56 180)
				(length 2.54)
				(name "IO31")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 -38.1 180)
				(length 2.54)
				(name "IO32")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 -40.64 180)
				(length 2.54)
				(name "IO33")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 -43.18 180)
				(length 2.54)
				(name "IO34")
				(number "35")
			)
			(pin bidirectional line
				(at 15.24 -45.72 180)
				(length 2.54)
				(name "IO35")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VisionSOM-6UL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 101.6 0)
		)
		(property "Value" "VisionSOM-6UL"
			(at 16.51 101.6 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://wiki.somlabs.com/extensions/JZPDFGen/pdf/VisionSOM-6UL%20Datasheet%20and%20Pinout-41.pdf"
			(at 1.27 104.14 0)
		)
		(property "Description" "i.MX6-UL NXP ARM Cortex-A7 696MHz single core industrial SoM computer"
			(at 0 0 0)
		)
		(property "ki_keywords" "somlabs module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SODIMM*"
			(at 0 0 0)
		)
		(symbol "VisionSOM-6UL_0_1")
		(symbol "VisionSOM-6UL_1_1"
			(pin bidirectional line
				(at -20.32 81.28 0)
				(length 3.81)
				(name "GPIO-0")
				(number "64")
			)
			(pin bidirectional line
				(at -20.32 78.74 0)
				(length 3.81)
				(name "GPIO-1")
				(number "62")
			)
			(pin bidirectional line
				(at -20.32 76.2 0)
				(length 3.81)
				(name "GPIO-2")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 73.66 0)
				(length 3.81)
				(name "GPIO-3")
				(number "55")
			)
			(pin bidirectional line
				(at -20.32 71.12 0)
				(length 3.81)
				(name "GPIO-4")
				(number "47")
			)
			(pin bidirectional line
				(at -20.32 68.58 0)
				(length 3.81)
				(name "GPIO-5")
				(number "49")
			)
			(pin bidirectional line
				(at -20.32 66.04 0)
				(length 3.81)
				(name "GPIO-6")
				(number "61")
			)
			(pin bidirectional line
				(at -20.32 63.5 0)
				(length 3.81)
				(name "GPIO-7")
				(number "53")
			)
			(pin bidirectional line
				(at -20.32 60.96 0)
				(length 3.81)
				(name "GPIO-8")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 58.42 0)
				(length 3.81)
				(name "GPIO-9")
				(number "56")
			)
			(pin passive line
				(at -20.32 53.34 0)
				(length 3.81)
				(name "CSI-VREF")
				(number "196")
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 3.81)
				(name "CSI-DATA0")
				(number "195")
			)
			(pin bidirectional line
				(at -20.32 48.26 0)
				(length 3.81)
				(name "CSI-DATA1")
				(number "193")
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 3.81)
				(name "CSI-DATA2")
				(number "194")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 3.81)
				(name "CSI-DATA3")
				(number "192")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "CSI-DATA4")
				(number "191")
			)
			(pin bidirectional line
				(at -20.32 38.1 0)
				(length 3.81)
				(name "CSI-DATA5")
				(number "190")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "CSI-DATA6")
				(number "186")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 3.81)
				(name "CSI-DATA7")
				(number "188")
			)
			(pin bidirectional line
				(at -20.32 30.48 0)
				(length 3.81)
				(name "CSI-HSYNC")
				(number "197")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "CSI-VSYNC")
				(number "198")
			)
			(pin bidirectional line
				(at -20.32 25.4 0)
				(length 3.81)
				(name "CSI-MCLK")
				(number "187")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "CSI-PIXCLK")
				(number "183")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "ENET1-RXD0")
				(number "97")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "ENET1-RXD1")
				(number "99")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "ENET1-CRS-DV")
				(number "101")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "ENET1-RXER")
				(number "126")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "ENET1-TXD0")
				(number "122")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "ENET1-TXD1")
				(number "124")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "ENET1-TXEN")
				(number "114")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "ENET1-TX-CLK")
				(number "118")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "ENET2-RXD0")
				(number "111")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "ENET2-RXD1")
				(number "113")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "ENET2-CRS-DV")
				(number "117")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "ENET2-RXER")
				(number "109")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "ENET2-TXD0")
				(number "123")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "ENET2-TXD1")
				(number "119")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "ENET2-TXEN")
				(number "121")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "ENET2-TX-CLK")
				(number "105")
			)
			(pin input line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "USB-OTG1-VBUS")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "USB-OTG1-DN")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "USB-OTG1-DP")
				(number "25")
			)
			(pin open_collector line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "~{USB-OTG1-CHD}")
				(number "31")
			)
			(pin input line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "USB-OTG2-VBUS")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "USB-OTG2-DN")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "USB-OTG2-DP")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "CLK1-N")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "CLK1-P")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 -60.96 0)
				(length 3.81)
				(name "JTAG-TDI")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 -63.5 0)
				(length 3.81)
				(name "JTAG-TDO")
				(number "52")
			)
			(pin bidirectional line
				(at -20.32 -66.04 0)
				(length 3.81)
				(name "JTAG-TMS")
				(number "46")
			)
			(pin bidirectional line
				(at -20.32 -68.58 0)
				(length 3.81)
				(name "JTAG-TCK")
				(number "54")
			)
			(pin bidirectional line
				(at -20.32 -71.12 0)
				(length 3.81)
				(name "JTAG-MOD")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 -73.66 0)
				(length 3.81)
				(name "~{JTAG-TRST}")
				(number "48")
			)
			(pin output line
				(at -20.32 -78.74 0)
				(length 3.81)
				(name "PMIC-ON-REQ")
				(number "5")
			)
			(pin output line
				(at -20.32 -81.28 0)
				(length 3.81)
				(name "PMIC-STBY-REQ")
				(number "3")
			)
			(pin input line
				(at -20.32 -86.36 0)
				(length 3.81)
				(name "~{POR-B}")
				(number "16")
			)
			(pin input line
				(at -20.32 -88.9 0)
				(length 3.81)
				(name "~{MX6-POR-B}")
				(number "4")
			)
			(pin input line
				(at -20.32 -93.98 0)
				(length 3.81)
				(name "BOOT-MODE1")
				(number "7")
			)
			(pin input line
				(at -20.32 -96.52 0)
				(length 3.81)
				(name "BOOT-MODE0")
				(number "9")
			)
			(pin no_connect line
				(at -15.24 -76.2 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "86")
			)
			(pin no_connect line
				(at -15.24 -83.82 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "94")
			)
			(pin no_connect line
				(at -15.24 -91.44 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "95")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "100")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "102")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "104")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "106")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "108")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "110")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "112")
			)
			(pin power_in line
				(at -7.62 104.14 270)
				(length 3.81)
				(name "+5VIN")
				(number "96")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "98")
			)
			(pin power_in line
				(at -2.54 104.14 270)
				(length 3.81)
				(name "VDD-COIN-3V")
				(number "8")
			)
			(pin power_in line
				(at 0 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "107")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "115")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "116")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "120")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "125")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "127")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "128")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "130")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "132")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "135")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "136")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "146")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "147")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "156")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "159")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "165")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "168")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "170")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "172")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "174")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "176")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "177")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "178")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "180")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "181")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "182")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "184")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "185")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "189")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "199")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "200")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "70")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "71")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "82")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "84")
			)
			(pin power_in line
				(at 2.54 104.14 270)
				(length 3.81)
				(name "VDD-SNVS-3V3")
				(number "6")
			)
			(pin power_out line
				(at 7.62 104.14 270)
				(length 3.81)
				(name "+3.3VOUT")
				(number "85")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "87")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "88")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "89")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "90")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "91")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "92")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "93")
			)
			(pin no_connect line
				(at 15.24 -93.98 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "83")
			)
			(pin bidirectional line
				(at 20.32 81.28 180)
				(length 3.81)
				(name "SNVS-TAMPER0")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 78.74 180)
				(length 3.81)
				(name "SNVS-TAMPER1")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 76.2 180)
				(length 3.81)
				(name "SNVS-TAMPER2")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 73.66 180)
				(length 3.81)
				(name "SNVS-TAMPER3")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 71.12 180)
				(length 3.81)
				(name "SNVS-TAMPER4")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 68.58 180)
				(length 3.81)
				(name "SNVS-TAMPER5")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 66.04 180)
				(length 3.81)
				(name "SNVS-TAMPER6")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 3.81)
				(name "SNVS-TAMPER7")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 3.81)
				(name "SNVS-TAMPER8")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "SNVS-TAMPER9")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "UART1-TXD")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "UART1-RXD")
				(number "63")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "UART1-RTS")
				(number "74")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "UART1-CTS")
				(number "66")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "UART2-TXD")
				(number "65")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "UART2-RXD")
				(number "67")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "UART2-RTS")
				(number "78")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "UART2-CTS")
				(number "72")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "UART3-TXD")
				(number "69")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "UART3-RXD")
				(number "73")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "UART3-RTS")
				(number "80")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "UART3-CTS")
				(number "76")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "UART4-TXD")
				(number "75")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "UART4-RXD")
				(number "77")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "UART5-RXD")
				(number "68")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "UART5-TXD")
				(number "79")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "SDIO1-D0")
				(number "167")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "SDIO1-D1")
				(number "171")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "SDIO1-D2")
				(number "175")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "SDIO1-D3")
				(number "169")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "SDIO1-CMD")
				(number "173")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "SDIO1-CLK")
				(number "179")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "LCD-DATA0")
				(number "153")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "LCD-DATA1")
				(number "155")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "LCD-DATA2")
				(number "164")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "LCD-DATA3")
				(number "154")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "LCD-DATA4")
				(number "158")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "LCD-DATA5")
				(number "149")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "LCD-DATA6")
				(number "151")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "LCD-DATA7")
				(number "166")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "LCD-DATA8")
				(number "143")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "LCD-DATA9")
				(number "145")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "LCD-DATA10")
				(number "152")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "LCD-DATA11")
				(number "148")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "LCD-DATA12")
				(number "150")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "LCD-DATA13")
				(number "139")
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 3.81)
				(name "LCD-DATA14")
				(number "141")
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 3.81)
				(name "LCD-DATA15")
				(number "142")
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 3.81)
				(name "LCD-DATA16")
				(number "144")
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 3.81)
				(name "LCD-DATA17")
				(number "133")
			)
			(pin bidirectional line
				(at 20.32 -63.5 180)
				(length 3.81)
				(name "LCD-DATA18")
				(number "137")
			)
			(pin bidirectional line
				(at 20.32 -66.04 180)
				(length 3.81)
				(name "LCD-DATA19")
				(number "138")
			)
			(pin bidirectional line
				(at 20.32 -68.58 180)
				(length 3.81)
				(name "LCD-DATA20")
				(number "140")
			)
			(pin bidirectional line
				(at 20.32 -71.12 180)
				(length 3.81)
				(name "LCD-DATA21")
				(number "129")
			)
			(pin bidirectional line
				(at 20.32 -73.66 180)
				(length 3.81)
				(name "LCD-DATA22")
				(number "131")
			)
			(pin bidirectional line
				(at 20.32 -76.2 180)
				(length 3.81)
				(name "LCD-DATA23")
				(number "134")
			)
			(pin bidirectional line
				(at 20.32 -78.74 180)
				(length 3.81)
				(name "LCD-ENABLE")
				(number "163")
			)
			(pin bidirectional line
				(at 20.32 -81.28 180)
				(length 3.81)
				(name "LCD-HSYNC")
				(number "160")
			)
			(pin bidirectional line
				(at 20.32 -83.82 180)
				(length 3.81)
				(name "LCD-VSYNC")
				(number "162")
			)
			(pin bidirectional line
				(at 20.32 -86.36 180)
				(length 3.81)
				(name "LCD-CLK")
				(number "161")
			)
			(pin bidirectional line
				(at 20.32 -88.9 180)
				(length 3.81)
				(name "LCD-RESET")
				(number "157")
			)
			(pin input line
				(at 20.32 -96.52 180)
				(length 3.81)
				(name "ONOFF")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VisionSOM-RT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 101.6 0)
		)
		(property "Value" "VisionSOM-RT"
			(at 16.51 101.6 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://wiki.somlabs.com/index.php/VisionSOM-RT_Datasheet_and_Pinout"
			(at 1.27 104.14 0)
		)
		(property "Description" "i.MX-RT NXP ARM Cortex-M7 528MHz single core industrial SoM computer"
			(at 0 0 0)
		)
		(property "ki_keywords" "somlabs module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SODIMM*"
			(at 0 0 0)
		)
		(symbol "VisionSOM-RT_0_1")
		(symbol "VisionSOM-RT_1_1"
			(pin bidirectional line
				(at -20.32 81.28 0)
				(length 3.81)
				(name "GPIO-0")
				(number "64")
			)
			(pin bidirectional line
				(at -20.32 78.74 0)
				(length 3.81)
				(name "GPIO-1")
				(number "62")
			)
			(pin bidirectional line
				(at -20.32 76.2 0)
				(length 3.81)
				(name "GPIO-2")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 73.66 0)
				(length 3.81)
				(name "GPIO-3")
				(number "55")
			)
			(pin bidirectional line
				(at -20.32 71.12 0)
				(length 3.81)
				(name "GPIO-4")
				(number "47")
			)
			(pin bidirectional line
				(at -20.32 68.58 0)
				(length 3.81)
				(name "GPIO-5")
				(number "49")
			)
			(pin bidirectional line
				(at -20.32 66.04 0)
				(length 3.81)
				(name "GPIO-6")
				(number "61")
			)
			(pin bidirectional line
				(at -20.32 63.5 0)
				(length 3.81)
				(name "GPIO-7")
				(number "53")
			)
			(pin bidirectional line
				(at -20.32 60.96 0)
				(length 3.81)
				(name "GPIO-8")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 58.42 0)
				(length 3.81)
				(name "GPIO-9")
				(number "56")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "ENET1-RXD0")
				(number "97")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "ENET1-RXD1")
				(number "99")
			)
			(pin bidirectional line
				(at -20.32 12.7 0)
				(length 3.81)
				(name "ENET1-CRS-DV")
				(number "101")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "ENET1-RXER")
				(number "126")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "ENET1-TXD0")
				(number "122")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "ENET1-TXD1")
				(number "124")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "ENET1-TXEN")
				(number "114")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "ENET1-TX-CLK")
				(number "118")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "ENET2-RXD0")
				(number "111")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "ENET2-RXD1")
				(number "113")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "ENET2-CRS-DV")
				(number "117")
			)
			(pin bidirectional line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "ENET2-RXER")
				(number "109")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "ENET2-TXD0")
				(number "123")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "ENET2-TXD1")
				(number "119")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "ENET2-TXEN")
				(number "121")
			)
			(pin bidirectional line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "ENET2-TX-CLK")
				(number "105")
			)
			(pin input line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "USB-OTG1-VBUS")
				(number "13")
			)
			(pin bidirectional line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "USB-OTG1-DN")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "USB-OTG1-DP")
				(number "25")
			)
			(pin open_collector line
				(at -20.32 -38.1 0)
				(length 3.81)
				(name "~{USB-OTG1-CHD}")
				(number "31")
			)
			(pin input line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "USB-OTG2-VBUS")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "USB-OTG2-DN")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "USB-OTG2-DP")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "CLK1-N")
				(number "37")
			)
			(pin bidirectional line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "CLK1-P")
				(number "39")
			)
			(pin bidirectional line
				(at -20.32 -60.96 0)
				(length 3.81)
				(name "JTAG-TDI")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 -63.5 0)
				(length 3.81)
				(name "JTAG-TDO")
				(number "52")
			)
			(pin bidirectional line
				(at -20.32 -66.04 0)
				(length 3.81)
				(name "JTAG-TMS")
				(number "46")
			)
			(pin bidirectional line
				(at -20.32 -68.58 0)
				(length 3.81)
				(name "JTAG-TCK")
				(number "54")
			)
			(pin bidirectional line
				(at -20.32 -71.12 0)
				(length 3.81)
				(name "JTAG-MOD")
				(number "33")
			)
			(pin bidirectional line
				(at -20.32 -73.66 0)
				(length 3.81)
				(name "~{JTAG-TRST}")
				(number "48")
			)
			(pin output line
				(at -20.32 -78.74 0)
				(length 3.81)
				(name "PMIC-ON-REQ")
				(number "5")
			)
			(pin output line
				(at -20.32 -81.28 0)
				(length 3.81)
				(name "PMIC-STBY-REQ")
				(number "3")
			)
			(pin input line
				(at -20.32 -86.36 0)
				(length 3.81)
				(name "~{POR-B}")
				(number "16")
			)
			(pin input line
				(at -20.32 -88.9 0)
				(length 3.81)
				(name "~{MX6-POR-B}")
				(number "4")
			)
			(pin input line
				(at -20.32 -93.98 0)
				(length 3.81)
				(name "BOOT-MODE1")
				(number "7")
			)
			(pin input line
				(at -20.32 -96.52 0)
				(length 3.81)
				(name "BOOT-MODE0")
				(number "9")
			)
			(pin no_connect line
				(at -15.24 53.34 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "196")
			)
			(pin no_connect line
				(at -15.24 50.8 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "195")
			)
			(pin no_connect line
				(at -15.24 48.26 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "193")
			)
			(pin no_connect line
				(at -15.24 45.72 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "194")
			)
			(pin no_connect line
				(at -15.24 43.18 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "192")
			)
			(pin no_connect line
				(at -15.24 40.64 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "191")
			)
			(pin no_connect line
				(at -15.24 38.1 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "190")
			)
			(pin no_connect line
				(at -15.24 35.56 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "186")
			)
			(pin no_connect line
				(at -15.24 33.02 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "188")
			)
			(pin no_connect line
				(at -15.24 30.48 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "197")
			)
			(pin no_connect line
				(at -15.24 27.94 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "198")
			)
			(pin no_connect line
				(at -15.24 25.4 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "187")
			)
			(pin no_connect line
				(at -15.24 22.86 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "183")
			)
			(pin no_connect line
				(at -15.24 -76.2 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "86")
			)
			(pin no_connect line
				(at -15.24 -83.82 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "94")
			)
			(pin no_connect line
				(at -15.24 -91.44 0)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "95")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "100")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "102")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "104")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "106")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "108")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "110")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "112")
			)
			(pin power_in line
				(at -7.62 104.14 270)
				(length 3.81)
				(name "+5VIN")
				(number "96")
			)
			(pin passive line
				(at -7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+5VIN")
				(number "98")
			)
			(pin no_connect line
				(at -5.08 -99.06 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "176")
			)
			(pin power_in line
				(at -2.54 104.14 270)
				(length 3.81)
				(name "VDD-COIN-3V")
				(number "8")
			)
			(pin no_connect line
				(at -2.54 -99.06 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "178")
			)
			(pin power_in line
				(at 0 -104.14 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "107")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "115")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "116")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "120")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "125")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "127")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "128")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "130")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "132")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "135")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "136")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "146")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "147")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "156")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "159")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "165")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "168")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "170")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "172")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "174")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "177")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "181")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "184")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "185")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "189")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "199")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "200")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "70")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "71")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "82")
			)
			(pin passive line
				(at 0 -104.14 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "84")
			)
			(pin power_in line
				(at 2.54 104.14 270)
				(length 3.81)
				(name "VDD-SNVS-3V3")
				(number "6")
			)
			(pin no_connect line
				(at 2.54 -99.06 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "180")
			)
			(pin no_connect line
				(at 5.08 -99.06 90)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "182")
			)
			(pin power_out line
				(at 7.62 104.14 270)
				(length 3.81)
				(name "+3.3VOUT")
				(number "85")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "87")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "88")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "89")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "90")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "91")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "92")
			)
			(pin passive line
				(at 7.62 104.14 270)
				(length 3.81)
				(hide yes)
				(name "+3.3VOUT")
				(number "93")
			)
			(pin no_connect line
				(at 15.24 -93.98 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "83")
			)
			(pin bidirectional line
				(at 20.32 81.28 180)
				(length 3.81)
				(name "SNVS-TAMPER0")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 78.74 180)
				(length 3.81)
				(name "SNVS-TAMPER1")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 76.2 180)
				(length 3.81)
				(name "SNVS-TAMPER2")
				(number "44")
			)
			(pin bidirectional line
				(at 20.32 73.66 180)
				(length 3.81)
				(name "SNVS-TAMPER3")
				(number "34")
			)
			(pin bidirectional line
				(at 20.32 71.12 180)
				(length 3.81)
				(name "SNVS-TAMPER4")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 68.58 180)
				(length 3.81)
				(name "SNVS-TAMPER5")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 66.04 180)
				(length 3.81)
				(name "SNVS-TAMPER6")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 3.81)
				(name "SNVS-TAMPER7")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 3.81)
				(name "SNVS-TAMPER8")
				(number "18")
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "SNVS-TAMPER9")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "UART1-TXD")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "UART1-RXD")
				(number "63")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "UART1-RTS")
				(number "74")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "UART1-CTS")
				(number "66")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "UART2-TXD")
				(number "65")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "UART2-RXD")
				(number "67")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "UART2-RTS")
				(number "78")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "UART2-CTS")
				(number "72")
			)
			(pin bidirectional line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "UART3-TXD")
				(number "69")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "UART3-RXD")
				(number "73")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "UART3-RTS")
				(number "80")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "UART3-CTS")
				(number "76")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "UART4-TXD")
				(number "75")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "UART4-RXD")
				(number "77")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "UART5-RXD")
				(number "68")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "UART5-TXD")
				(number "79")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "SDIO1-D0")
				(number "167")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "SDIO1-D1")
				(number "171")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "SDIO1-D2")
				(number "175")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "SDIO1-D3")
				(number "169")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "SDIO1-CMD")
				(number "173")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "SDIO1-CLK")
				(number "179")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "LCD-DATA0")
				(number "153")
			)
			(pin bidirectional line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "LCD-DATA1")
				(number "155")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "LCD-DATA2")
				(number "164")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "LCD-DATA3")
				(number "154")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "LCD-DATA4")
				(number "158")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "LCD-DATA5")
				(number "149")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "LCD-DATA6")
				(number "151")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "LCD-DATA7")
				(number "166")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "LCD-DATA8")
				(number "143")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "LCD-DATA9")
				(number "145")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "LCD-DATA10")
				(number "152")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "LCD-DATA11")
				(number "148")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "LCD-DATA12")
				(number "150")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "LCD-DATA13")
				(number "139")
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 3.81)
				(name "LCD-DATA14")
				(number "141")
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 3.81)
				(name "LCD-DATA15")
				(number "142")
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 3.81)
				(name "LCD-DATA16")
				(number "144")
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 3.81)
				(name "LCD-DATA17")
				(number "133")
			)
			(pin bidirectional line
				(at 20.32 -63.5 180)
				(length 3.81)
				(name "LCD-DATA18")
				(number "137")
			)
			(pin bidirectional line
				(at 20.32 -66.04 180)
				(length 3.81)
				(name "LCD-DATA19")
				(number "138")
			)
			(pin bidirectional line
				(at 20.32 -68.58 180)
				(length 3.81)
				(name "LCD-DATA20")
				(number "140")
			)
			(pin bidirectional line
				(at 20.32 -71.12 180)
				(length 3.81)
				(name "LCD-DATA21")
				(number "129")
			)
			(pin bidirectional line
				(at 20.32 -73.66 180)
				(length 3.81)
				(name "LCD-DATA22")
				(number "131")
			)
			(pin bidirectional line
				(at 20.32 -76.2 180)
				(length 3.81)
				(name "LCD-DATA23")
				(number "134")
			)
			(pin bidirectional line
				(at 20.32 -78.74 180)
				(length 3.81)
				(name "LCD-ENABLE")
				(number "163")
			)
			(pin bidirectional line
				(at 20.32 -81.28 180)
				(length 3.81)
				(name "LCD-HSYNC")
				(number "160")
			)
			(pin bidirectional line
				(at 20.32 -83.82 180)
				(length 3.81)
				(name "LCD-VSYNC")
				(number "162")
			)
			(pin bidirectional line
				(at 20.32 -86.36 180)
				(length 3.81)
				(name "LCD-CLK")
				(number "161")
			)
			(pin bidirectional line
				(at 20.32 -88.9 180)
				(length 3.81)
				(name "LCD-RESET")
				(number "157")
			)
			(pin input line
				(at 20.32 -96.52 180)
				(length 3.81)
				(name "ONOFF")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "VisionSOM-STM32MP1"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 81.28 0)
		)
		(property "Value" "VisionSOM-STM32MP1"
			(at 19.05 81.28 0)
		)
		(property "Footprint" ""
			(at 0 17.78 0)
		)
		(property "Datasheet" "https://wiki.somlabs.com/index.php/VisionSOM-STM32MP1_Datasheet_and_Pinout"
			(at 1.27 83.82 0)
		)
		(property "Description" "STM32MP1 STMicroelectronics ARM Cortex-A7 800MHz single/dual core + ARM Cortex-M4 209MHz single core industrial SoM computer"
			(at 0 0 0)
		)
		(property "ki_keywords" "somlabs module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SODIMM*"
			(at 0 0 0)
		)
		(symbol "VisionSOM-STM32MP1_0_1")
		(symbol "VisionSOM-STM32MP1_1_1"
			(pin bidirectional line
				(at -20.32 66.04 0)
				(length 3.81)
				(name "GPIO-PA0")
				(number "62")
			)
			(pin bidirectional line
				(at -20.32 63.5 0)
				(length 3.81)
				(name "GPIO-PA1")
				(number "157")
			)
			(pin bidirectional line
				(at -20.32 60.96 0)
				(length 3.81)
				(name "GPIO-PA13")
				(number "113")
			)
			(pin bidirectional line
				(at -20.32 58.42 0)
				(length 3.81)
				(name "GPIO-PA14")
				(number "117")
			)
			(pin bidirectional line
				(at -20.32 53.34 0)
				(length 3.81)
				(name "GPIO-PB1")
				(number "58")
			)
			(pin bidirectional line
				(at -20.32 50.8 0)
				(length 3.81)
				(name "GPIO-PB7")
				(number "56")
			)
			(pin bidirectional line
				(at -20.32 45.72 0)
				(length 3.81)
				(name "GPIO-PC0")
				(number "55")
			)
			(pin bidirectional line
				(at -20.32 43.18 0)
				(length 3.81)
				(name "GPIO-PC2")
				(number "119")
			)
			(pin bidirectional line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "GPIO-PC3")
				(number "47")
			)
			(pin bidirectional line
				(at -20.32 35.56 0)
				(length 3.81)
				(name "GPIO-PD13")
				(number "49")
			)
			(pin bidirectional line
				(at -20.32 33.02 0)
				(length 3.81)
				(name "GPIO-PD15")
				(number "111")
			)
			(pin bidirectional line
				(at -20.32 27.94 0)
				(length 3.81)
				(name "GPIO-PE2")
				(number "121")
			)
			(pin bidirectional line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "GPIO-PF10")
				(number "64")
			)
			(pin bidirectional line
				(at -20.32 17.78 0)
				(length 3.81)
				(name "GPIO-PG10")
				(number "45")
			)
			(pin bidirectional line
				(at -20.32 15.24 0)
				(length 3.81)
				(name "GPIO-PG12")
				(number "109")
			)
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "ENET1-MDIO")
				(number "61")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 3.81)
				(name "ENET1-MDC")
				(number "53")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 3.81)
				(name "ENET1-RXD0")
				(number "97")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "ENET1-RXD1")
				(number "99")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 3.81)
				(name "ENET1-CRS-DV")
				(number "101")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "ENET1-TXD0")
				(number "122")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "ENET1-TXD1")
				(number "124")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 3.81)
				(name "ENET1-TXD-EN")
				(number "114")
			)
			(pin bidirectional line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "ENET1-CLK")
				(number "118")
			)
			(pin input line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "USB-OTG1-VBUS")
				(number "11")
			)
			(pin bidirectional line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "USB-OTG1-DN")
				(number "21")
			)
			(pin bidirectional line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "USB-OTG1-DP")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "USB-OTG2-DN")
				(number "27")
			)
			(pin bidirectional line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "USB-OTG2-DP")
				(number "25")
			)
			(pin bidirectional line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "JTAG-TDI")
				(number "43")
			)
			(pin bidirectional line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "JTAG-TDO")
				(number "52")
			)
			(pin bidirectional line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "JTAG-TMS")
				(number "46")
			)
			(pin bidirectional line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "JTAG-TCK")
				(number "54")
			)
			(pin bidirectional line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "~{JTAG-RST}")
				(number "48")
			)
			(pin output line
				(at -20.32 -58.42 0)
				(length 3.81)
				(name "PWR-ON")
				(number "5")
			)
			(pin output line
				(at -20.32 -60.96 0)
				(length 3.81)
				(name "PWR-LP")
				(number "3")
			)
			(pin input line
				(at -20.32 -66.04 0)
				(length 3.81)
				(name "~{STM32-NRST}")
				(number "4")
			)
			(pin input line
				(at -20.32 -71.12 0)
				(length 3.81)
				(name "BOOT2")
				(number "10")
			)
			(pin input line
				(at -20.32 -73.66 0)
				(length 3.81)
				(name "BOOT1")
				(number "7")
			)
			(pin input line
				(at -20.32 -76.2 0)
				(length 3.81)
				(name "BOOT0")
				(number "9")
			)
			(pin no_connect line
				(at -15.24 73.66 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "12")
			)
			(pin no_connect line
				(at -15.24 71.12 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin no_connect line
				(at -15.24 68.58 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "14")
			)
			(pin no_connect line
				(at -15.24 55.88 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "16")
			)
			(pin no_connect line
				(at -15.24 48.26 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "18")
			)
			(pin no_connect line
				(at -15.24 38.1 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "24")
			)
			(pin no_connect line
				(at -15.24 30.48 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "30")
			)
			(pin no_connect line
				(at -15.24 25.4 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "31")
			)
			(pin no_connect line
				(at -15.24 20.32 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "32")
			)
			(pin no_connect line
				(at -15.24 12.7 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "33")
			)
			(pin no_connect line
				(at -15.24 -12.7 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "34")
			)
			(pin no_connect line
				(at -15.24 -22.86 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "36")
			)
			(pin no_connect line
				(at -15.24 -30.48 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "37")
			)
			(pin no_connect line
				(at -15.24 -33.02 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "39")
			)
			(pin no_connect line
				(at -15.24 -35.56 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "42")
			)
			(pin no_connect line
				(at -15.24 -38.1 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "44")
			)
			(pin no_connect line
				(at -15.24 -40.64 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "83")
			)
			(pin no_connect line
				(at -15.24 -55.88 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "86")
			)
			(pin no_connect line
				(at -15.24 -63.5 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "94")
			)
			(pin no_connect line
				(at -15.24 -68.58 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "95")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VDD-5V")
				(number "100")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VDD-5V")
				(number "102")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VDD-5V")
				(number "104")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VDD-5V")
				(number "106")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VDD-5V")
				(number "108")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VDD-5V")
				(number "110")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VDD-5V")
				(number "112")
			)
			(pin power_in line
				(at -7.62 83.82 270)
				(length 3.81)
				(name "VDD-5V")
				(number "96")
			)
			(pin passive line
				(at -7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VDD-5V")
				(number "98")
			)
			(pin power_in line
				(at -2.54 83.82 270)
				(length 3.81)
				(name "VDD-COIN-3V")
				(number "8")
			)
			(pin power_in line
				(at 0 -83.82 90)
				(length 3.81)
				(name "GND")
				(number "1")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "103")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "107")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "115")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "116")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "120")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "125")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "127")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "128")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "130")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "132")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "133")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "135")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "136")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "143")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "144")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "145")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "146")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "147")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "15")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "153")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "155")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "156")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "159")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "165")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "168")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "17")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "170")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "172")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "174")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "176")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "177")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "178")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "180")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "181")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "182")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "184")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "185")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "189")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "199")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "2")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "20")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "200")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "22")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "23")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "26")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "28")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "29")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "35")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "38")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "40")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "41")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "50")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "51")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "59")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "60")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "70")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "71")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "81")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "82")
			)
			(pin passive line
				(at 0 -83.82 90)
				(length 3.81)
				(hide yes)
				(name "GND")
				(number "84")
			)
			(pin power_in line
				(at 2.54 83.82 270)
				(length 3.81)
				(name "VDD-3V3")
				(number "6")
			)
			(pin power_out line
				(at 7.62 83.82 270)
				(length 3.81)
				(name "VOUT-3V3")
				(number "85")
			)
			(pin passive line
				(at 7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VOUT-3V3")
				(number "87")
			)
			(pin passive line
				(at 7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VOUT-3V3")
				(number "88")
			)
			(pin passive line
				(at 7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VOUT-3V3")
				(number "89")
			)
			(pin passive line
				(at 7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VOUT-3V3")
				(number "90")
			)
			(pin passive line
				(at 7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VOUT-3V3")
				(number "91")
			)
			(pin passive line
				(at 7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VOUT-3V3")
				(number "92")
			)
			(pin passive line
				(at 7.62 83.82 270)
				(length 3.81)
				(hide yes)
				(name "VOUT-3V3")
				(number "93")
			)
			(pin no_connect line
				(at 15.24 73.66 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "105")
			)
			(pin no_connect line
				(at 15.24 71.12 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "123")
			)
			(pin no_connect line
				(at 15.24 68.58 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "126")
			)
			(pin no_connect line
				(at 15.24 55.88 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "183")
			)
			(pin no_connect line
				(at 15.24 43.18 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "187")
			)
			(pin no_connect line
				(at 15.24 35.56 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "190")
			)
			(pin no_connect line
				(at 15.24 27.94 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "191")
			)
			(pin no_connect line
				(at 15.24 15.24 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "196")
			)
			(pin no_connect line
				(at 15.24 -2.54 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "197")
			)
			(pin no_connect line
				(at 15.24 -20.32 180)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "198")
			)
			(pin bidirectional line
				(at 20.32 66.04 180)
				(length 3.81)
				(name "USART1-TXD")
				(number "73")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 3.81)
				(name "USART1-RXD")
				(number "69")
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 3.81)
				(name "USART1-RTS")
				(number "80")
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "USART1-CTS")
				(number "76")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "USART3-TXD")
				(number "65")
			)
			(pin bidirectional line
				(at 20.32 50.8 180)
				(length 3.81)
				(name "USART3-RXD")
				(number "67")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "USART3-RTS")
				(number "78")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "USART3-CTS")
				(number "72")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "UART4-TXD")
				(number "75")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "UART4-RXD")
				(number "77")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "USART6-TXD")
				(number "79")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "USART6-RXD")
				(number "68")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "UART8-TXD")
				(number "57")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "UART8-RXD")
				(number "63")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "UART8-RTS")
				(number "74")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "UART8-CTS")
				(number "66")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "SD2-DATA0")
				(number "167")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "SD2-DATA1")
				(number "171")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "SD2-DATA2")
				(number "175")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "SD2-DATA3")
				(number "169")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "SD2-CMD")
				(number "173")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "SD2-CLK")
				(number "179")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "DSI-D0P")
				(number "188")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "DSI-D0N")
				(number "186")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "DSI-D1P")
				(number "194")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "DSI-D1N")
				(number "192")
			)
			(pin bidirectional line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "DSI-CK-P")
				(number "195")
			)
			(pin bidirectional line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "DSI-CK-N")
				(number "193")
			)
			(pin bidirectional line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "LCD-R2")
				(number "137")
			)
			(pin bidirectional line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "LCD-R3")
				(number "138")
			)
			(pin bidirectional line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "LCD-R4")
				(number "140")
			)
			(pin bidirectional line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "LCD-R5")
				(number "129")
			)
			(pin bidirectional line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "LCD-R6")
				(number "131")
			)
			(pin bidirectional line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "LCD-R7")
				(number "134")
			)
			(pin bidirectional line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "LCD-G2")
				(number "152")
			)
			(pin bidirectional line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "LCD-G3")
				(number "148")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "LCD-G4")
				(number "150")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "LCD-G5")
				(number "139")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "LCD-G6")
				(number "141")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "LCD-G7")
				(number "142")
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 3.81)
				(name "LCD-B2")
				(number "164")
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 3.81)
				(name "LCD-B3")
				(number "154")
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 3.81)
				(name "LCD-B4")
				(number "158")
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 3.81)
				(name "LCD-B5")
				(number "149")
			)
			(pin bidirectional line
				(at 20.32 -63.5 180)
				(length 3.81)
				(name "LCD-B6")
				(number "151")
			)
			(pin bidirectional line
				(at 20.32 -66.04 180)
				(length 3.81)
				(name "LCD-B7")
				(number "166")
			)
			(pin bidirectional line
				(at 20.32 -68.58 180)
				(length 3.81)
				(name "LCD-DE")
				(number "163")
			)
			(pin bidirectional line
				(at 20.32 -71.12 180)
				(length 3.81)
				(name "LCD-HSYNC")
				(number "160")
			)
			(pin bidirectional line
				(at 20.32 -73.66 180)
				(length 3.81)
				(name "LCD-VSYNC")
				(number "162")
			)
			(pin bidirectional line
				(at 20.32 -76.2 180)
				(length 3.81)
				(name "LCD-CLK")
				(number "161")
			)
		)
		(embedded_fonts no)
	)
	(symbol "Adafruit_Feather_M0_Adalogger"
		(extends "Adafruit_Feather_M0_Basic_Proto")
		(property "Reference" "A"
			(at -10.16 29.21 0)
		)
		(property "Value" "Adafruit_Feather_M0_Adalogger"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Module:Adafruit_Feather"
			(at 2.54 -34.29 0)
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-feather-m0-adalogger.pdf"
			(at 0 -30.48 0)
		)
		(property "Description" "Microcontroller module with SAMD21 Cortex-M0 MCU and SD card reader"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adafruit feather microcontroller module USB SD"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Adafruit*Feather*"
			(at 0 0 0)
		)
	)
	(symbol "Adafruit_Feather_M0_Express"
		(extends "Adafruit_Feather_M0_Basic_Proto")
		(property "Reference" "A"
			(at -10.16 29.21 0)
		)
		(property "Value" "Adafruit_Feather_M0_Express"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Module:Adafruit_Feather"
			(at 2.54 -34.29 0)
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-feather-m0-express-designed-for-circuit-python-circuitpython.pdf"
			(at 0 -30.48 0)
		)
		(property "Description" "Microcontroller module with SAMD21 Cortex-M0 MCU and SPI Flash"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adafruit feather microcontroller module USB SPI Flash CircuitPython"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Adafruit*Feather*"
			(at 0 0 0)
		)
	)
	(symbol "Adafruit_Feather_M0_RFM9x_LoRa_Radio"
		(extends "Adafruit_Feather_M0_RFM69HCW_Packet_Radio")
		(property "Reference" "A"
			(at -10.16 29.21 0)
		)
		(property "Value" "Adafruit_Feather_M0_RFM9x_LoRa_Radio"
			(at 2.54 -31.75 0)
		)
		(property "Footprint" "Module:Adafruit_Feather_M0_RFM"
			(at 2.54 -34.29 0)
		)
		(property "Datasheet" "https://cdn-learn.adafruit.com/downloads/pdf/adafruit-feather-m0-radio-with-lora-radio-module.pdf"
			(at 0 -20.32 0)
		)
		(property "Description" "Microcontroller module with SAMD21 Cortex-M0 MCU and RFM9x Radio"
			(at 0 0 0)
		)
		(property "ki_keywords" "Adafruit feather microcontroller module USB M0 SAMD21 LoRa Radio"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Adafruit*Feather*"
			(at 0 0 0)
		)
	)
	(symbol "Arduino_Nano_v3.x"
		(extends "Arduino_Nano_v2.x")
		(property "Reference" "A"
			(at -10.16 23.495 0)
		)
		(property "Value" "Arduino_Nano_v3.x"
			(at 5.08 -24.13 0)
		)
		(property "Footprint" "Module:Arduino_Nano"
			(at 0 0 0)
		)
		(property "Datasheet" "http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf"
			(at 0 0 0)
		)
		(property "Description" "Arduino Nano v3.x"
			(at 0 0 0)
		)
		(property "ki_keywords" "Arduino nano microcontroller module USB"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Arduino*Nano*"
			(at 0 0 0)
		)
	)
	(symbol "NUCLEO144-F207ZG"
		(extends "NUCLEO144-F429ZI")
		(property "Reference" "U"
			(at -22.86 94.615 0)
		)
		(property "Value" "NUCLEO144-F207ZG"
			(at -22.86 92.71 0)
		)
		(property "Footprint" "Module:ST_Morpho_Connector_144_STLink"
			(at 21.59 -92.71 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/user_manual/dm00244518-stm32-nucleo144-boards-stmicroelectronics.pdf"
			(at -22.86 7.62 0)
		)
		(property "Description" "Nucleo 144 Development Board with STM32F207ZGT6 MCU, 128+4Kb RAM, 1Mb FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM32 Nucleo ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*Morpho*Connector*144*STLink*"
			(at 0 0 0)
		)
	)
	(symbol "NUCLEO144-F412ZG"
		(extends "NUCLEO144-F429ZI")
		(property "Reference" "U"
			(at -22.86 94.615 0)
		)
		(property "Value" "NUCLEO144-F412ZG"
			(at -22.86 92.71 0)
		)
		(property "Footprint" "Module:ST_Morpho_Connector_144_STLink"
			(at 21.59 -92.71 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/user_manual/dm00244518-stm32-nucleo144-boards-stmicroelectronics.pdf"
			(at -22.86 7.62 0)
		)
		(property "Description" "Nucleo 144 Development Board with STM32F412ZGT6 MCU, 256kB RAM, 1Mb FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM32 Nucleo ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*Morpho*Connector*144*STLink*"
			(at 0 0 0)
		)
	)
	(symbol "NUCLEO144-F413ZH"
		(extends "NUCLEO144-F429ZI")
		(property "Reference" "U"
			(at -22.86 94.615 0)
		)
		(property "Value" "NUCLEO144-F413ZH"
			(at -22.86 92.71 0)
		)
		(property "Footprint" "Module:ST_Morpho_Connector_144_STLink"
			(at 21.59 -92.71 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/user_manual/dm00244518-stm32-nucleo144-boards-stmicroelectronics.pdf"
			(at -22.86 7.62 0)
		)
		(property "Description" "Nucleo 144 Development Board with STM32F413ZHT6 MCU, 320kB RAM, 1.5Mb FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM32 Nucleo ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*Morpho*Connector*144*STLink*"
			(at 0 0 0)
		)
	)
	(symbol "NUCLEO144-F439ZI"
		(extends "NUCLEO144-F429ZI")
		(property "Reference" "U"
			(at -22.86 94.615 0)
		)
		(property "Value" "NUCLEO144-F439ZI"
			(at -22.86 92.71 0)
		)
		(property "Footprint" "Module:ST_Morpho_Connector_144_STLink"
			(at 21.59 -92.71 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/user_manual/dm00244518-stm32-nucleo144-boards-stmicroelectronics.pdf"
			(at -22.86 7.62 0)
		)
		(property "Description" "Nucleo 144 Development Board with STM32F439ZIT6 MCU, 256kB RAM, 2Mb FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM32 Nucleo ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*Morpho*Connector*144*STLink*"
			(at 0 0 0)
		)
	)
	(symbol "NUCLEO144-F446ZE"
		(extends "NUCLEO144-F429ZI")
		(property "Reference" "U"
			(at -22.86 94.615 0)
		)
		(property "Value" "NUCLEO144-F446ZE"
			(at -22.86 92.71 0)
		)
		(property "Footprint" "Module:ST_Morpho_Connector_144_STLink"
			(at 21.59 -92.71 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/user_manual/dm00244518-stm32-nucleo144-boards-stmicroelectronics.pdf"
			(at -22.86 7.62 0)
		)
		(property "Description" "Nucleo 144 Development Board with STM32F446ZET6 MCU, 128kB RAM, 512Kb FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM32 Nucleo ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*Morpho*Connector*144*STLink*"
			(at 0 0 0)
		)
	)
	(symbol "NUCLEO144-F722ZE"
		(extends "NUCLEO144-F429ZI")
		(property "Reference" "U"
			(at -22.86 94.615 0)
		)
		(property "Value" "NUCLEO144-F722ZE"
			(at -22.86 92.71 0)
		)
		(property "Footprint" "Module:ST_Morpho_Connector_144_STLink"
			(at 21.59 -92.71 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/user_manual/dm00244518-stm32-nucleo144-boards-stmicroelectronics.pdf"
			(at -22.86 7.62 0)
		)
		(property "Description" "Nucleo 144 Development Board with STM32F722ZET6 MCU, 256kB RAM, 512Kb FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM32 Nucleo ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*Morpho*Connector*144*STLink*"
			(at 0 0 0)
		)
	)
	(symbol "NUCLEO144-F746ZG"
		(extends "NUCLEO144-F429ZI")
		(property "Reference" "U"
			(at -22.86 94.615 0)
		)
		(property "Value" "NUCLEO144-F746ZG"
			(at -22.86 92.71 0)
		)
		(property "Footprint" "Module:ST_Morpho_Connector_144_STLink"
			(at 21.59 -92.71 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/user_manual/dm00244518-stm32-nucleo144-boards-stmicroelectronics.pdf"
			(at -22.86 7.62 0)
		)
		(property "Description" "Nucleo 144 Development Board with STM32F746ZG MCU, 256kB RAM, 1Mb FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM32 Nucleo ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*Morpho*Connector*144*STLink*"
			(at 0 0 0)
		)
	)
	(symbol "NUCLEO144-F756ZG"
		(extends "NUCLEO144-F429ZI")
		(property "Reference" "U"
			(at -22.86 94.615 0)
		)
		(property "Value" "NUCLEO144-F756ZG"
			(at -22.86 92.71 0)
		)
		(property "Footprint" "Module:ST_Morpho_Connector_144_STLink"
			(at 21.59 -92.71 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/user_manual/dm00244518-stm32-nucleo144-boards-stmicroelectronics.pdf"
			(at -22.86 7.62 0)
		)
		(property "Description" "Nucleo 144 Development Board with STM32F756ZGT6 MCU, 320kB RAM, 1Mb FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM32 Nucleo ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*Morpho*Connector*144*STLink*"
			(at 0 0 0)
		)
	)
	(symbol "NUCLEO144-F767ZI"
		(extends "NUCLEO144-F429ZI")
		(property "Reference" "U"
			(at -22.86 94.615 0)
		)
		(property "Value" "NUCLEO144-F767ZI"
			(at -22.86 92.71 0)
		)
		(property "Footprint" "Module:ST_Morpho_Connector_144_STLink"
			(at 21.59 -92.71 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/user_manual/dm00244518-stm32-nucleo144-boards-stmicroelectronics.pdf"
			(at -22.86 7.62 0)
		)
		(property "Description" "Nucleo 144 Development Board with STM32F767ZIT6 MCU, 512kB RAM, 2Mb FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM32 Nucleo ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*Morpho*Connector*144*STLink*"
			(at 0 0 0)
		)
	)
	(symbol "NUCLEO144-H743ZI"
		(extends "NUCLEO144-F429ZI")
		(property "Reference" "U"
			(at -22.86 94.615 0)
		)
		(property "Value" "NUCLEO144-H743ZI"
			(at -22.86 92.71 0)
		)
		(property "Footprint" "Module:ST_Morpho_Connector_144_STLink"
			(at 21.59 -92.71 0)
		)
		(property "Datasheet" "https://www.st.com/resource/en/user_manual/dm00244518-stm32-nucleo144-boards-stmicroelectronics.pdf"
			(at -22.86 7.62 0)
		)
		(property "Description" "Nucleo 144 Development Board with STM32H743ZIT6 MCU, 1024kB RAM, 2Mb FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "STM32 Nucleo ST"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "ST*Morpho*Connector*144*STLink*"
			(at 0 0 0)
		)
	)
	(symbol "Omega2S+"
		(extends "Omega2S")
		(property "Reference" "U"
			(at -20.32 52.07 0)
		)
		(property "Value" "Omega2S+"
			(at 17.78 52.07 0)
		)
		(property "Footprint" "Module:Onion_Omega2S"
			(at 0 -68.58 0)
		)
		(property "Datasheet" "https://github.com/OnionIoT/Omega2/raw/master/Documents/Omega2S%20Datasheet.pdf"
			(at 19.05 -26.67 0)
		)
		(property "Description" "Iot Computer Module by Onion, 128MB RAM, 32MB FLASH"
			(at 0 0 0)
		)
		(property "ki_keywords" "onion omega module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "Onion*Omega2S*"
			(at 0 0 0)
		)
	)
	(symbol "RaspberryPi-CM3"
		(extends "RaspberryPi-CM3+")
		(property "Reference" "U"
			(at -20.32 81.28 0)
		)
		(property "Value" "RaspberryPi-CM3"
			(at 20.32 81.28 0)
		)
		(property "Footprint" ""
			(at -15.24 86.36 0)
		)
		(property "Datasheet" "https://www.raspberrypi.org/documentation/hardware/computemodule/datasheets/rpi_DATA_CM_1p0.pdf"
			(at -15.24 86.36 0)
		)
		(property "Description" "BCM2837 Broadcom 1.2 GHZ quad core, 1 GB RAM 4 GB eMMC,  industrial SoM computer"
			(at 0 0 0)
		)
		(property "ki_keywords" "raspberry pi compute module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SODIMM*"
			(at 0 0 0)
		)
	)
	(symbol "RaspberryPi-CM3-L"
		(extends "RaspberryPi-CM3+L")
		(property "Reference" "U"
			(at -20.32 81.28 0)
		)
		(property "Value" "RaspberryPi-CM3-L"
			(at 20.32 81.28 0)
		)
		(property "Footprint" ""
			(at -15.24 86.36 0)
		)
		(property "Datasheet" "https://www.raspberrypi.org/documentation/hardware/computemodule/datasheets/rpi_DATA_CM_1p0.pdf"
			(at -15.24 86.36 0)
		)
		(property "Description" "BCM2837 Broadcom 1.2 GHZ quad core, 1 GB RAM, industrial SoM computer"
			(at 0 0 0)
		)
		(property "ki_keywords" "raspberry pi compute module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SODIMM*"
			(at 0 0 0)
		)
	)
	(symbol "RaspberryPi_Pico_W"
		(extends "RaspberryPi_Pico")
		(property "Reference" "A"
			(at -19.05 35.56 0)
		)
		(property "Value" "RaspberryPi_Pico_W"
			(at 7.62 35.56 0)
		)
		(property "Footprint" "Module:RaspberryPi_Pico_W_SMD_HandSolder"
			(at 0 -46.99 0)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf"
			(at 0 -49.53 0)
		)
		(property "Description" "Versatile and inexpensive wireless microcontroller module powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash, Infineon CYW43439 2.4GHz 802.11n wireless LAN; also supports Raspberry Pi Pico 2 W"
			(at 0 -52.07 0)
		)
		(property "ki_keywords" "RP2350A M33 RISC-V Hazard3 usb wifi bluetooth"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?Common* RaspberryPi?Pico?W?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "RaspberryPi_Pico_W_Debug"
		(extends "RaspberryPi_Pico_Debug")
		(property "Reference" "A"
			(at -19.05 35.56 0)
		)
		(property "Value" "RaspberryPi_Pico_W"
			(at 7.62 35.56 0)
		)
		(property "Footprint" "Module:RaspberryPi_Pico_W_SMD_HandSolder"
			(at 0 -46.99 0)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf"
			(at 0 -49.53 0)
		)
		(property "Description" "Versatile and inexpensive wireless microcontroller module (with debug pins) powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash, Infineon CYW43439 2.4GHz 802.11n wireless LAN; also supports Raspberry Pi Pico 2 W"
			(at 0 -52.07 0)
		)
		(property "ki_keywords" "RP2350A M33 RISC-V Hazard3 usb swd wifi bluetooth"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?W?SMD*"
			(at 0 0 0)
		)
	)
	(symbol "RaspberryPi_Pico_W_Extensive"
		(extends "RaspberryPi_Pico_Extensive")
		(property "Reference" "A"
			(at -19.05 35.56 0)
		)
		(property "Value" "RaspberryPi_Pico_W"
			(at 7.62 35.56 0)
		)
		(property "Footprint" "Module:RaspberryPi_Pico_W_SMD"
			(at 0 -46.99 0)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/picow/pico-w-datasheet.pdf"
			(at 0 -49.53 0)
		)
		(property "Description" "Versatile and inexpensive wireless microcontroller module (with full pinout for test point and debug connections) powered by RP2040 dual-core Arm Cortex-M0+ processor up to 133 MHz, 264kB SRAM, 2MB QSPI flash, Infineon CYW43439 2.4GHz 802.11n wireless LAN; also supports Raspberry Pi Pico 2 W"
			(at 0 -52.07 0)
		)
		(property "ki_keywords" "RP2350A M33 RISC-V Hazard3 usb swd wifi bluetooth"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "RaspberryPi?Pico?W?SMD"
			(at 0 0 0)
		)
	)
	(symbol "VisionSOM-6ULL"
		(extends "VisionSOM-6UL")
		(property "Reference" "U"
			(at -13.97 101.6 0)
		)
		(property "Value" "VisionSOM-6ULL"
			(at 16.51 101.6 0)
		)
		(property "Footprint" ""
			(at 0 -2.54 0)
		)
		(property "Datasheet" "https://wiki.somlabs.com/extensions/JZPDFGen/pdf/VisionSOM-6ULL%20Datasheet%20and%20Pinout-21.pdf"
			(at 1.27 104.14 0)
		)
		(property "Description" "i.MX6-ULL NXP ARM Cortex-A7 900MHz single core industrial SoM computer"
			(at 0 0 0)
		)
		(property "ki_keywords" "somlabs module"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SODIMM*"
			(at 0 0 0)
		)
	)
)
