(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "MCF5212CAE66"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 19.05 50.8 0)
		)
		(property "Value" "MCF5212CAE66"
			(at 16.51 -48.26 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MCF5213EC.pdf"
			(at 1.27 1.27 0)
		)
		(property "Description" "ColdFire Microcontroller, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MCF5212CAE66_0_1")
		(symbol "MCF5212CAE66_1_1"
			(pin passive line
				(at -40.64 45.72 0)
				(length 7.62)
				(name "VCCPLL")
				(number "48")
			)
			(pin passive line
				(at -40.64 43.18 0)
				(length 7.62)
				(name "GNDPLL")
				(number "45")
			)
			(pin input line
				(at -40.64 38.1 0)
				(length 7.62)
				(name "CLKIN/EXTAL")
				(number "47")
			)
			(pin output line
				(at -40.64 35.56 0)
				(length 7.62)
				(name "XTAL")
				(number "46")
			)
			(pin input input_low
				(at -40.64 30.48 0)
				(length 7.62)
				(name "RSTI")
				(number "59")
			)
			(pin output output_low
				(at -40.64 27.94 0)
				(length 7.62)
				(name "RSTO")
				(number "60")
			)
			(pin input line
				(at -40.64 25.4 0)
				(length 7.62)
				(name "CLKMOD0")
				(number "24")
			)
			(pin input line
				(at -40.64 22.86 0)
				(length 7.62)
				(name "RCON/EZPCS")
				(number "16")
			)
			(pin input line
				(at -40.64 20.32 0)
				(length 7.62)
				(name "TEST")
				(number "3")
			)
			(pin input line
				(at -40.64 17.78 0)
				(length 7.62)
				(name "JTAG_EN")
				(number "17")
			)
			(pin input line
				(at -40.64 15.24 0)
				(length 7.62)
				(name "DSCLK/~{TRST}")
				(number "54")
			)
			(pin input line
				(at -40.64 12.7 0)
				(length 7.62)
				(name "DSI/TDI")
				(number "50")
			)
			(pin output line
				(at -40.64 10.16 0)
				(length 7.62)
				(name "DSO/TDO")
				(number "51")
			)
			(pin input line
				(at -40.64 7.62 0)
				(length 7.62)
				(name "TCLK/PSTCLK/CLKOUT")
				(number "44")
			)
			(pin input line
				(at -40.64 5.08 0)
				(length 7.62)
				(name "~{BKPT}/TMS")
				(number "49")
			)
			(pin output line
				(at -40.64 2.54 0)
				(length 7.62)
				(name "ALLPST")
				(number "55")
			)
			(pin bidirectional line
				(at -40.64 -2.54 0)
				(length 7.62)
				(name "~{IRQ1}/PNQ1/SYNCA/PWM1")
				(number "56")
			)
			(pin bidirectional line
				(at -40.64 -5.08 0)
				(length 7.62)
				(name "IRQ4*/PNQ4")
				(number "57")
			)
			(pin bidirectional line
				(at -40.64 -7.62 0)
				(length 7.62)
				(name "IRQ7*/PNQ7")
				(number "58")
			)
			(pin bidirectional line
				(at -40.64 -12.7 0)
				(length 7.62)
				(name "AN0/PAN0")
				(number "25")
			)
			(pin bidirectional line
				(at -40.64 -15.24 0)
				(length 7.62)
				(name "AN1/PAN1")
				(number "26")
			)
			(pin bidirectional line
				(at -40.64 -17.78 0)
				(length 7.62)
				(name "AN2/PAN2")
				(number "27")
			)
			(pin bidirectional line
				(at -40.64 -20.32 0)
				(length 7.62)
				(name "AN3/PAN3")
				(number "28")
			)
			(pin bidirectional line
				(at -40.64 -22.86 0)
				(length 7.62)
				(name "AN4/PAN4")
				(number "36")
			)
			(pin bidirectional line
				(at -40.64 -25.4 0)
				(length 7.62)
				(name "AN5/PAN5")
				(number "35")
			)
			(pin bidirectional line
				(at -40.64 -27.94 0)
				(length 7.62)
				(name "AN6/PAN6")
				(number "34")
			)
			(pin bidirectional line
				(at -40.64 -30.48 0)
				(length 7.62)
				(name "AN7/PAN7")
				(number "33")
			)
			(pin input line
				(at -40.64 -35.56 0)
				(length 7.62)
				(name "VRH")
				(number "31")
			)
			(pin input line
				(at -40.64 -38.1 0)
				(length 7.62)
				(name "VRL")
				(number "30")
			)
			(pin input line
				(at -40.64 -43.18 0)
				(length 7.62)
				(name "VCCA")
				(number "32")
			)
			(pin input line
				(at -40.64 -45.72 0)
				(length 7.62)
				(name "VSSA")
				(number "29")
			)
			(pin power_in line
				(at -5.08 55.88 270)
				(length 6.35)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -5.08 -53.34 90)
				(length 6.35)
				(name "GND")
				(number "11")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 6.35)
				(name "VCC")
				(number "10")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 6.35)
				(name "GND")
				(number "21")
			)
			(pin power_in line
				(at 0 55.88 270)
				(length 6.35)
				(name "VCC")
				(number "20")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 6.35)
				(name "GND")
				(number "38")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 6.35)
				(name "VCC")
				(number "39")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 6.35)
				(name "GND")
				(number "53")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 6.35)
				(name "VCC")
				(number "52")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 6.35)
				(name "GND")
				(number "64")
			)
			(pin power_in line
				(at 10.16 55.88 270)
				(length 6.35)
				(name "VSTBY")
				(number "37")
			)
			(pin bidirectional line
				(at 43.18 40.64 180)
				(length 7.62)
				(name "GPT0/PWM1/PTA0")
				(number "40")
			)
			(pin bidirectional line
				(at 43.18 38.1 180)
				(length 7.62)
				(name "GPT1/PWM3/PTA1")
				(number "41")
			)
			(pin bidirectional line
				(at 43.18 35.56 180)
				(length 7.62)
				(name "GPT2PWM5//PTA2")
				(number "42")
			)
			(pin bidirectional line
				(at 43.18 33.02 180)
				(length 7.62)
				(name "GPT3/PWM7/PTA3")
				(number "43")
			)
			(pin bidirectional line
				(at 43.18 27.94 180)
				(length 7.62)
				(name "DTIN0/DTOUT0/PWM0/PTC0")
				(number "22")
			)
			(pin bidirectional line
				(at 43.18 25.4 180)
				(length 7.62)
				(name "DTIN1/DTOUT1/PWM2/PTC1")
				(number "23")
			)
			(pin bidirectional line
				(at 43.18 22.86 180)
				(length 7.62)
				(name "DTIN2/DTOUT2/PWM4/PTC2")
				(number "18")
			)
			(pin bidirectional line
				(at 43.18 20.32 180)
				(length 7.62)
				(name "DTIN3/DTOUT3/PWM6/PTC3")
				(number "19")
			)
			(pin bidirectional line
				(at 43.18 15.24 180)
				(length 7.62)
				(name "SCL/PAS0/UTxD2")
				(number "8")
			)
			(pin bidirectional line
				(at 43.18 12.7 180)
				(length 7.62)
				(name "SDA/PAS1/URxD2")
				(number "9")
			)
			(pin bidirectional line
				(at 43.18 7.62 180)
				(length 7.62)
				(name "UTXD0/PUA0")
				(number "6")
			)
			(pin bidirectional line
				(at 43.18 5.08 180)
				(length 7.62)
				(name "URXD0/PUA1")
				(number "5")
			)
			(pin bidirectional line
				(at 43.18 2.54 180)
				(length 7.62)
				(name "UTXD1/PUB0")
				(number "62")
			)
			(pin bidirectional line
				(at 43.18 0 180)
				(length 7.62)
				(name "URXD1/PUB1")
				(number "63")
			)
			(pin bidirectional line
				(at 43.18 -5.08 180)
				(length 7.62)
				(name "~{URTS0}/CANTX/PUA2")
				(number "7")
			)
			(pin bidirectional line
				(at 43.18 -7.62 180)
				(length 7.62)
				(name "~{UCTS0}/CANRTX/PUA3")
				(number "4")
			)
			(pin bidirectional line
				(at 43.18 -10.16 180)
				(length 7.62)
				(name "~{URTS1}/SYNCB/UTXD2/PUB2")
				(number "2")
			)
			(pin bidirectional line
				(at 43.18 -12.7 180)
				(length 7.62)
				(name "~{UCTS1}/SYNCA/URXD2/PUB3")
				(number "61")
			)
			(pin bidirectional line
				(at 43.18 -17.78 180)
				(length 7.62)
				(name "QSPI_DOUT/EZPQ/CANTX/RXD0/PQS0")
				(number "13")
			)
			(pin bidirectional line
				(at 43.18 -20.32 180)
				(length 7.62)
				(name "QSPI_DIN/EZPD/CANRX/RXD1/PQS1")
				(number "12")
			)
			(pin bidirectional line
				(at 43.18 -22.86 180)
				(length 7.62)
				(name "QSPI_CLK/EZPCK/SCL/RTS1/PQS2")
				(number "14")
			)
			(pin bidirectional line
				(at 43.18 -25.4 180)
				(length 7.62)
				(name "QSPI_CS0/SDA/CTS1/PQS3")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCF5213-LQFP100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 29.21 68.58 0)
		)
		(property "Value" "MCF5213-LQFP100"
			(at 15.24 -67.31 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Coldfire with SRAM and Flash Eprom - LQFP100 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "COLDFIRE"
			(at 0 0 0)
		)
		(symbol "MCF5213-LQFP100_0_1")
		(symbol "MCF5213-LQFP100_1_1"
			(pin passive line
				(at -50.8 63.5 0)
				(length 7.62)
				(name "VCCPLL")
				(number "74")
			)
			(pin passive line
				(at -50.8 60.96 0)
				(length 7.62)
				(name "GNDPLL")
				(number "71")
			)
			(pin input line
				(at -50.8 58.42 0)
				(length 7.62)
				(name "CLKIN/EXTAL")
				(number "73")
			)
			(pin output line
				(at -50.8 55.88 0)
				(length 7.62)
				(name "XTAL")
				(number "72")
			)
			(pin input input_low
				(at -50.8 50.8 0)
				(length 7.62)
				(name "RSTI")
				(number "96")
			)
			(pin output output_low
				(at -50.8 48.26 0)
				(length 7.62)
				(name "RSTO")
				(number "97")
			)
			(pin input line
				(at -50.8 45.72 0)
				(length 7.62)
				(name "CLKMOD0")
				(number "40")
			)
			(pin input line
				(at -50.8 43.18 0)
				(length 7.62)
				(name "CLKMOD1")
				(number "39")
			)
			(pin input input_low
				(at -50.8 40.64 0)
				(length 7.62)
				(name "RCON/EZPCS")
				(number "21")
			)
			(pin input line
				(at -50.8 38.1 0)
				(length 7.62)
				(name "TEST")
				(number "5")
			)
			(pin input line
				(at -50.8 33.02 0)
				(length 7.62)
				(name "JTAG_EN")
				(number "26")
			)
			(pin input line
				(at -50.8 30.48 0)
				(length 7.62)
				(name "DSCLK/~{TRST}")
				(number "85")
			)
			(pin input line
				(at -50.8 27.94 0)
				(length 7.62)
				(name "DSI/TDI")
				(number "79")
			)
			(pin output line
				(at -50.8 25.4 0)
				(length 7.62)
				(name "DSO/TDO")
				(number "80")
			)
			(pin input line
				(at -50.8 22.86 0)
				(length 7.62)
				(name "TCLK/PSTCLK/CLKOUT")
				(number "64")
			)
			(pin input line
				(at -50.8 20.32 0)
				(length 7.62)
				(name "~{BKPT}/TMS")
				(number "76")
			)
			(pin output line
				(at -50.8 15.24 0)
				(length 7.62)
				(name "ALLPST")
				(number "86")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 7.62)
				(name "PST0/PDD0")
				(number "65")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 7.62)
				(name "PST1/PDD1")
				(number "66")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 7.62)
				(name "PST2/PDD2")
				(number "69")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 7.62)
				(name "PST3/PDD3")
				(number "70")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 7.62)
				(name "DDATA0/PDD4")
				(number "77")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 7.62)
				(name "DDATA1/PDD5")
				(number "78")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 7.62)
				(name "DDATA2/PDD6")
				(number "83")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 7.62)
				(name "DDATA3/PDD7")
				(number "84")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 7.62)
				(name "~{IRQ1}/PNQ1/SYNCA/PWM1")
				(number "87")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 7.62)
				(name "~{IRQ2}/PNQ2")
				(number "88")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 7.62)
				(name "~{IRQ3}/PNQ3")
				(number "89")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 7.62)
				(name "~{IRQ4}/PNQ4")
				(number "90")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 7.62)
				(name "~{IRQ5}/PNQ5")
				(number "91")
			)
			(pin bidirectional line
				(at -50.8 -22.86 0)
				(length 7.62)
				(name "~{IRQ6}/PNQ6")
				(number "94")
			)
			(pin bidirectional line
				(at -50.8 -25.4 0)
				(length 7.62)
				(name "~{IRQ7}/PNQ7")
				(number "95")
			)
			(pin bidirectional line
				(at -50.8 -30.48 0)
				(length 7.62)
				(name "AN0/PAN0")
				(number "43")
			)
			(pin bidirectional line
				(at -50.8 -33.02 0)
				(length 7.62)
				(name "AN1/PAN1")
				(number "44")
			)
			(pin bidirectional line
				(at -50.8 -35.56 0)
				(length 7.62)
				(name "AN2/PAN2")
				(number "45")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 7.62)
				(name "AN3/PAN3")
				(number "46")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 7.62)
				(name "AN4/PAN4")
				(number "54")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 7.62)
				(name "AN5/PAN5")
				(number "53")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 7.62)
				(name "AN6/PAN6")
				(number "52")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 7.62)
				(name "AN7/PAN7")
				(number "51")
			)
			(pin input line
				(at -50.8 -53.34 0)
				(length 7.62)
				(name "VRH")
				(number "49")
			)
			(pin input line
				(at -50.8 -55.88 0)
				(length 7.62)
				(name "VRL")
				(number "48")
			)
			(pin input line
				(at -50.8 -60.96 0)
				(length 7.62)
				(name "VCCA")
				(number "50")
			)
			(pin input line
				(at -50.8 -63.5 0)
				(length 7.62)
				(name "VSSA")
				(number "47")
			)
			(pin power_in line
				(at -17.78 73.66 270)
				(length 6.35)
				(name "VCC")
				(number "1")
			)
			(pin power_in line
				(at -15.24 73.66 270)
				(length 6.35)
				(name "VCC")
				(number "14")
			)
			(pin power_in line
				(at -12.7 73.66 270)
				(length 6.35)
				(name "VCC")
				(number "2")
			)
			(pin power_in line
				(at -12.7 -73.66 90)
				(length 6.35)
				(name "GND")
				(number "3")
			)
			(pin power_in line
				(at -10.16 73.66 270)
				(length 6.35)
				(name "VCC")
				(number "22")
			)
			(pin power_in line
				(at -10.16 -73.66 90)
				(length 6.35)
				(name "GND")
				(number "15")
			)
			(pin power_in line
				(at -7.62 73.66 270)
				(length 6.35)
				(name "VCC")
				(number "23")
			)
			(pin power_in line
				(at -7.62 -73.66 90)
				(length 6.35)
				(name "GND")
				(number "24")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 6.35)
				(name "VCC")
				(number "34")
			)
			(pin power_in line
				(at -5.08 -73.66 90)
				(length 6.35)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 6.35)
				(name "VCC")
				(number "41")
			)
			(pin power_in line
				(at -2.54 -73.66 90)
				(length 6.35)
				(name "GND")
				(number "35")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 6.35)
				(name "VCC")
				(number "57")
			)
			(pin power_in line
				(at 0 -73.66 90)
				(length 6.35)
				(name "GND")
				(number "42")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 6.35)
				(name "VCC")
				(number "68")
			)
			(pin power_in line
				(at 2.54 -73.66 90)
				(length 6.35)
				(name "GND")
				(number "67")
			)
			(pin power_in line
				(at 5.08 73.66 270)
				(length 6.35)
				(name "VCC")
				(number "93")
			)
			(pin power_in line
				(at 5.08 -73.66 90)
				(length 6.35)
				(name "GND")
				(number "56")
			)
			(pin power_in line
				(at 7.62 73.66 270)
				(length 6.35)
				(name "VSTBY")
				(number "55")
			)
			(pin power_in line
				(at 7.62 -73.66 90)
				(length 6.35)
				(name "GND")
				(number "75")
			)
			(pin power_in line
				(at 10.16 73.66 270)
				(length 6.35)
				(name "VCC")
				(number "81")
			)
			(pin power_in line
				(at 10.16 -73.66 90)
				(length 6.35)
				(name "GND")
				(number "82")
			)
			(pin power_in line
				(at 12.7 -73.66 90)
				(length 6.35)
				(name "GND")
				(number "92")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 7.62)
				(name "PWM1/PTD0")
				(number "38")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 7.62)
				(name "PWM3/PTD1")
				(number "33")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 7.62)
				(name "PWM5/PTD2")
				(number "60")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 7.62)
				(name "PWM7/PTD3")
				(number "63")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 7.62)
				(name "GPT0/PWM1/PTA0")
				(number "58")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 7.62)
				(name "GPT1/PWM3/PTA1")
				(number "59")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 7.62)
				(name "GPT2PWM5//PTA2")
				(number "61")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 7.62)
				(name "GPT3/PWM7/PTA3")
				(number "62")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 7.62)
				(name "DTIN0/DTOUT0/PWM0/PTC0")
				(number "36")
			)
			(pin bidirectional line
				(at 50.8 38.1 180)
				(length 7.62)
				(name "DTIN1/DTOUT1/PWM2/PTC1")
				(number "37")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 7.62)
				(name "DTIN2/DTOUT2/PWM4/PTC2")
				(number "31")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 7.62)
				(name "DTIN3/DTOUT3/PWM6/PTC3")
				(number "32")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 7.62)
				(name "SCL/CANTX/PAS0/UTXD2")
				(number "10")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 7.62)
				(name "SDA/CANRX/PAS1/URXD2")
				(number "11")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 7.62)
				(name "UTXD0/PUA0")
				(number "8")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 7.62)
				(name "URXD0/PUA1")
				(number "7")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 7.62)
				(name "UTXD1/PUB0")
				(number "99")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 7.62)
				(name "URXD1/PUB1")
				(number "100")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 7.62)
				(name "UTXD2/PUC0")
				(number "29")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 7.62)
				(name "URXD2/PUC1")
				(number "28")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 7.62)
				(name "~{URTS0}/CANTX/PUA2")
				(number "9")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 7.62)
				(name "~{UCTS0}/CANRX/PUA3")
				(number "6")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 7.62)
				(name "~{URTS1}/SYNCB/UTXD2/PUB2")
				(number "4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 7.62)
				(name "~{UCTS1}/SYNCA/URXD2/PUB3")
				(number "98")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 7.62)
				(name "~{URTS2}/PUC2")
				(number "30")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 7.62)
				(name "~{UCTS2}/PUC3")
				(number "27")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 7.62)
				(name "QSPI_DOUT/EZPQ/CANTX/RXD0/PQS0")
				(number "17")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 7.62)
				(name "QSPI_DIN/EZPD/CANRX/RXD1/PQS1")
				(number "16")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 7.62)
				(name "QSPI_CLK/EZPCK/SCL/RTS1/PQS2")
				(number "18")
			)
			(pin bidirectional line
				(at 50.8 -35.56 180)
				(length 7.62)
				(name "QSPI_CS0/SDA/CTS1/PQS3")
				(number "20")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 7.62)
				(name "QSPI_CS1/PQS4")
				(number "19")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 7.62)
				(name "QSPI_CS2/PQS5")
				(number "13")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 7.62)
				(name "QSPI_CS3/SYNCA/SYNCB/PQS6")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCF5282"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 40.64 125.73 0)
		)
		(property "Value" "MCF5282"
			(at 30.48 -129.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Coldfire with SRAM and Flash Eprom"
			(at 0 0 0)
		)
		(property "ki_keywords" "COLDFIRE"
			(at 0 0 0)
		)
		(symbol "MCF5282_0_1")
		(symbol "MCF5282_1_1"
			(pin passive line
				(at -50.8 119.38 0)
				(length 7.62)
				(name "VCCPLL")
				(number "N8")
			)
			(pin passive line
				(at -50.8 116.84 0)
				(length 7.62)
				(name "GNDPLL")
				(number "P8")
			)
			(pin input line
				(at -50.8 114.3 0)
				(length 7.62)
				(name "CLKIN/EXTAL")
				(number "T8")
			)
			(pin output line
				(at -50.8 111.76 0)
				(length 7.62)
				(name "XTAL")
				(number "R8")
			)
			(pin output line
				(at -50.8 109.22 0)
				(length 7.62)
				(name "CLKOUT")
				(number "N7")
			)
			(pin input input_low
				(at -50.8 104.14 0)
				(length 7.62)
				(name "RSTI")
				(number "R11")
			)
			(pin output output_low
				(at -50.8 101.6 0)
				(length 7.62)
				(name "RSTO")
				(number "P11")
			)
			(pin input line
				(at -50.8 99.06 0)
				(length 7.62)
				(name "CLKMOD0")
				(number "R14")
			)
			(pin input line
				(at -50.8 96.52 0)
				(length 7.62)
				(name "CLKMOD1")
				(number "T14")
			)
			(pin input input_low
				(at -50.8 93.98 0)
				(length 7.62)
				(name "RCON")
				(number "T11")
			)
			(pin input line
				(at -50.8 91.44 0)
				(length 7.62)
				(name "TEST")
				(number "N10")
			)
			(pin bidirectional line
				(at -50.8 86.36 0)
				(length 7.62)
				(name "~{IRQ1}/PNQ1")
				(number "D15")
			)
			(pin bidirectional line
				(at -50.8 83.82 0)
				(length 7.62)
				(name "~{IRQ2}/PNQ2")
				(number "D14")
			)
			(pin bidirectional line
				(at -50.8 81.28 0)
				(length 7.62)
				(name "~{IRQ3}/PNQ3")
				(number "C16")
			)
			(pin bidirectional line
				(at -50.8 78.74 0)
				(length 7.62)
				(name "~{IRQ4}/PNQ4")
				(number "C15")
			)
			(pin bidirectional line
				(at -50.8 76.2 0)
				(length 7.62)
				(name "~{IRQ5}/PNQ5")
				(number "C14")
			)
			(pin bidirectional line
				(at -50.8 73.66 0)
				(length 7.62)
				(name "~{IRQ6}/PNQ6")
				(number "B16")
			)
			(pin bidirectional line
				(at -50.8 71.12 0)
				(length 7.62)
				(name "~{IRQ7}/PNQ7")
				(number "B15")
			)
			(pin bidirectional line
				(at -50.8 68.58 0)
				(length 7.62)
				(name "SCL/PAS0/UTxD2")
				(number "E15")
			)
			(pin bidirectional line
				(at -50.8 66.04 0)
				(length 7.62)
				(name "SDA/PAS1/URxD2")
				(number "E14")
			)
			(pin bidirectional line
				(at -50.8 63.5 0)
				(length 7.62)
				(name "CANTX/PAS2/UTxD2")
				(number "E13")
			)
			(pin bidirectional line
				(at -50.8 60.96 0)
				(length 7.62)
				(name "CANRX/PAS3/URxD2")
				(number "D16")
			)
			(pin bidirectional line
				(at -50.8 55.88 0)
				(length 7.62)
				(name "UTXD0/PUA0")
				(number "T7")
			)
			(pin bidirectional line
				(at -50.8 53.34 0)
				(length 7.62)
				(name "URXD0/PUA1")
				(number "N6")
			)
			(pin bidirectional line
				(at -50.8 50.8 0)
				(length 7.62)
				(name "UTXD1/PUA2")
				(number "P7")
			)
			(pin bidirectional line
				(at -50.8 48.26 0)
				(length 7.62)
				(name "URXD1/PUA3")
				(number "R7")
			)
			(pin bidirectional line
				(at -50.8 45.72 0)
				(length 7.62)
				(name "EMDIO/PAS5/URXD2")
				(number "C10")
			)
			(pin input line
				(at -50.8 43.18 0)
				(length 7.62)
				(name "EMDC/PAS4/UTXD2")
				(number "B10")
			)
			(pin bidirectional line
				(at -50.8 38.1 0)
				(length 7.62)
				(name "DTIN3/PTC3/~{URTS1}/~{URTS0}")
				(number "K16")
			)
			(pin bidirectional line
				(at -50.8 35.56 0)
				(length 7.62)
				(name "DTOUT3/PTC2/~{URTS1}/~{URTS0}")
				(number "K15")
			)
			(pin bidirectional line
				(at -50.8 33.02 0)
				(length 7.62)
				(name "DTIN2/PTC1/~{UCTS1}/~{UCTS0}")
				(number "K14")
			)
			(pin bidirectional line
				(at -50.8 30.48 0)
				(length 7.62)
				(name "DTOUT2/PTC0/~{UCTS1}/~{UCTS0}")
				(number "K13")
			)
			(pin bidirectional line
				(at -50.8 27.94 0)
				(length 7.62)
				(name "DTIN1/PTD3/~{URTS1}/~{URTS0}")
				(number "J16")
			)
			(pin bidirectional line
				(at -50.8 25.4 0)
				(length 7.62)
				(name "DTOUT1/PTD2/~{URTS1}/~{URTS0}")
				(number "J15")
			)
			(pin bidirectional line
				(at -50.8 22.86 0)
				(length 7.62)
				(name "DTIN0/PTD1/~{UCTS1}/~{UCTS0}")
				(number "J14")
			)
			(pin input line
				(at -50.8 20.32 0)
				(length 7.62)
				(name "DTOUT0/PTD0/~{UCTS1}/~{UCTS0}")
				(number "J13")
			)
			(pin bidirectional line
				(at -50.8 15.24 0)
				(length 7.62)
				(name "QSPI_DOUT/PQS0")
				(number "F13")
			)
			(pin bidirectional line
				(at -50.8 12.7 0)
				(length 7.62)
				(name "QSPI_DIN/PQS1")
				(number "E16")
			)
			(pin bidirectional line
				(at -50.8 10.16 0)
				(length 7.62)
				(name "QSPI_CLK/PQS2")
				(number "F14")
			)
			(pin bidirectional line
				(at -50.8 7.62 0)
				(length 7.62)
				(name "QSPI_CS0/PQS3")
				(number "F15")
			)
			(pin bidirectional line
				(at -50.8 5.08 0)
				(length 7.62)
				(name "QSPI_CS1/PQS4")
				(number "F16")
			)
			(pin bidirectional line
				(at -50.8 2.54 0)
				(length 7.62)
				(name "QSPI_CS2/PQS5")
				(number "G13")
			)
			(pin bidirectional line
				(at -50.8 0 0)
				(length 7.62)
				(name "QSPI_CS3/PQS6")
				(number "G14")
			)
			(pin bidirectional line
				(at -50.8 -2.54 0)
				(length 7.62)
				(name "AN0/PQB0/ANW")
				(number "T3")
			)
			(pin bidirectional line
				(at -50.8 -5.08 0)
				(length 7.62)
				(name "AN1/PQB1/ANX")
				(number "R2")
			)
			(pin bidirectional line
				(at -50.8 -7.62 0)
				(length 7.62)
				(name "AN2/PQB2/ANY")
				(number "T2")
			)
			(pin bidirectional line
				(at -50.8 -10.16 0)
				(length 7.62)
				(name "AN3/PQB3/ANZ")
				(number "R1")
			)
			(pin bidirectional line
				(at -50.8 -12.7 0)
				(length 7.62)
				(name "AN52/PQA0/MA0")
				(number "R4")
			)
			(pin bidirectional line
				(at -50.8 -15.24 0)
				(length 7.62)
				(name "AN53/PQA1/MA1")
				(number "T4")
			)
			(pin bidirectional line
				(at -50.8 -17.78 0)
				(length 7.62)
				(name "AN55/PQA3/ETRIG1")
				(number "P3")
			)
			(pin bidirectional line
				(at -50.8 -20.32 0)
				(length 7.62)
				(name "AN56/PQA4/ETRIG2")
				(number "R3")
			)
			(pin input line
				(at -50.8 -25.4 0)
				(length 7.62)
				(name "VRH")
				(number "P4")
			)
			(pin input line
				(at -50.8 -27.94 0)
				(length 7.62)
				(name "VRL")
				(number "T5")
			)
			(pin input line
				(at -50.8 -30.48 0)
				(length 7.62)
				(name "VCCA")
				(number "R5")
			)
			(pin input line
				(at -50.8 -33.02 0)
				(length 7.62)
				(name "VSSA")
				(number "P5")
			)
			(pin input line
				(at -50.8 -35.56 0)
				(length 7.62)
				(name "VSSA")
				(number "T1")
			)
			(pin bidirectional line
				(at -50.8 -38.1 0)
				(length 7.62)
				(name "ETXCLK/PEH7")
				(number "A8")
			)
			(pin bidirectional line
				(at -50.8 -40.64 0)
				(length 7.62)
				(name "ETXEN/PEH6")
				(number "D6")
			)
			(pin bidirectional line
				(at -50.8 -43.18 0)
				(length 7.62)
				(name "ETXD0/PEH5")
				(number "D7")
			)
			(pin bidirectional line
				(at -50.8 -45.72 0)
				(length 7.62)
				(name "ECOL/PEH4")
				(number "B11")
			)
			(pin bidirectional line
				(at -50.8 -48.26 0)
				(length 7.62)
				(name "ERXCLK/PEH3")
				(number "A10")
			)
			(pin bidirectional line
				(at -50.8 -50.8 0)
				(length 7.62)
				(name "ERXDV/PEH2")
				(number "C8")
			)
			(pin bidirectional line
				(at -50.8 -53.34 0)
				(length 7.62)
				(name "ERXDO/PEH1")
				(number "D9")
			)
			(pin bidirectional line
				(at -50.8 -55.88 0)
				(length 7.62)
				(name "ECRS/PEH0")
				(number "A11")
			)
			(pin bidirectional line
				(at -50.8 -60.96 0)
				(length 7.62)
				(name "ERXER/PEL0")
				(number "B8")
			)
			(pin bidirectional line
				(at -50.8 -63.5 0)
				(length 7.62)
				(name "ERXD1/PEL1")
				(number "C9")
			)
			(pin bidirectional line
				(at -50.8 -66.04 0)
				(length 7.62)
				(name "ERXD2/PEL2")
				(number "B9")
			)
			(pin bidirectional line
				(at -50.8 -68.58 0)
				(length 7.62)
				(name "ERXD3/PEL3")
				(number "A9")
			)
			(pin bidirectional line
				(at -50.8 -71.12 0)
				(length 7.62)
				(name "ETXER/PEL4")
				(number "D10")
			)
			(pin bidirectional line
				(at -50.8 -73.66 0)
				(length 7.62)
				(name "ETXD1/PEL5")
				(number "C7")
			)
			(pin bidirectional line
				(at -50.8 -76.2 0)
				(length 7.62)
				(name "ETXD2/PEL6")
				(number "B7")
			)
			(pin bidirectional line
				(at -50.8 -78.74 0)
				(length 7.62)
				(name "ETXD3/PEL7")
				(number "A7")
			)
			(pin input line
				(at -50.8 -83.82 0)
				(length 7.62)
				(name "JTAG_EN")
				(number "R9")
			)
			(pin input line
				(at -50.8 -86.36 0)
				(length 7.62)
				(name "DSCLK/~{TRST}")
				(number "P9")
			)
			(pin input line
				(at -50.8 -88.9 0)
				(length 7.62)
				(name "DSI/TDI")
				(number "R10")
			)
			(pin output line
				(at -50.8 -91.44 0)
				(length 7.62)
				(name "DSO/TDO")
				(number "T10")
			)
			(pin input line
				(at -50.8 -93.98 0)
				(length 7.62)
				(name "TCLK")
				(number "T9")
			)
			(pin input line
				(at -50.8 -96.52 0)
				(length 7.62)
				(name "~{BKPT}/TMS")
				(number "P10")
			)
			(pin output line
				(at -50.8 -99.06 0)
				(length 7.62)
				(name "PST0/PDD0")
				(number "A15")
			)
			(pin output line
				(at -50.8 -101.6 0)
				(length 7.62)
				(name "PST1/PDD1")
				(number "B14")
			)
			(pin output line
				(at -50.8 -104.14 0)
				(length 7.62)
				(name "PST2/PDD2")
				(number "A14")
			)
			(pin output line
				(at -50.8 -106.68 0)
				(length 7.62)
				(name "PST3/PDD3")
				(number "C13")
			)
			(pin output line
				(at -50.8 -109.22 0)
				(length 7.62)
				(name "DDATA0/PDD4")
				(number "B13")
			)
			(pin output line
				(at -50.8 -111.76 0)
				(length 7.62)
				(name "DDATA1/PDD5")
				(number "A13")
			)
			(pin output line
				(at -50.8 -114.3 0)
				(length 7.62)
				(name "DDATA2/PDD6")
				(number "D12")
			)
			(pin output line
				(at -50.8 -116.84 0)
				(length 7.62)
				(name "DDATA3/PDD7")
				(number "C12")
			)
			(pin power_in line
				(at -31.75 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "E6")
			)
			(pin power_in line
				(at -30.48 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "E7")
			)
			(pin power_in line
				(at -29.21 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "E8")
			)
			(pin power_in line
				(at -27.94 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "E9")
			)
			(pin power_in line
				(at -26.67 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "E10")
			)
			(pin power_in line
				(at -25.4 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "E11")
			)
			(pin power_in line
				(at -24.13 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "F5")
			)
			(pin power_in line
				(at -22.86 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "F7")
			)
			(pin power_in line
				(at -21.59 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "F8")
			)
			(pin power_in line
				(at -20.32 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "F9")
			)
			(pin power_in line
				(at -19.05 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "F10")
			)
			(pin power_in line
				(at -17.78 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "F12")
			)
			(pin power_in line
				(at -16.51 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "G5")
			)
			(pin power_in line
				(at -16.51 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "F11")
			)
			(pin power_in line
				(at -15.24 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "G6")
			)
			(pin power_in line
				(at -15.24 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "E12")
			)
			(pin power_in line
				(at -13.97 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "G11")
			)
			(pin power_in line
				(at -13.97 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "F6")
			)
			(pin power_in line
				(at -12.7 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "G12")
			)
			(pin power_in line
				(at -12.7 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "A1")
			)
			(pin power_in line
				(at -11.43 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "H5")
			)
			(pin power_in line
				(at -11.43 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "A16")
			)
			(pin power_in line
				(at -10.16 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "H6")
			)
			(pin power_in line
				(at -10.16 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "E5")
			)
			(pin power_in line
				(at -8.89 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "H11")
			)
			(pin power_in line
				(at -8.89 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "G7")
			)
			(pin power_in line
				(at -7.62 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "H12")
			)
			(pin power_in line
				(at -7.62 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "G8")
			)
			(pin power_in line
				(at -6.35 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "J5")
			)
			(pin power_in line
				(at -6.35 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "G9")
			)
			(pin power_in line
				(at -5.08 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "J6")
			)
			(pin power_in line
				(at -5.08 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "G10")
			)
			(pin power_in line
				(at -3.81 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "J11")
			)
			(pin power_in line
				(at -3.81 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "H7")
			)
			(pin power_in line
				(at -2.54 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "J12")
			)
			(pin power_in line
				(at -2.54 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "H8")
			)
			(pin power_in line
				(at -1.27 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "K5")
			)
			(pin power_in line
				(at -1.27 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "H9")
			)
			(pin power_in line
				(at 0 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "K6")
			)
			(pin power_in line
				(at 0 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "H10")
			)
			(pin power_in line
				(at 1.27 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "K11")
			)
			(pin power_in line
				(at 1.27 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "J7")
			)
			(pin power_in line
				(at 2.54 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "K12")
			)
			(pin power_in line
				(at 2.54 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "J8")
			)
			(pin power_in line
				(at 3.81 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "L5")
			)
			(pin power_in line
				(at 3.81 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "J9")
			)
			(pin power_in line
				(at 5.08 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "L7")
			)
			(pin power_in line
				(at 5.08 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "J10")
			)
			(pin power_in line
				(at 6.35 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "L8")
			)
			(pin power_in line
				(at 6.35 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "K7")
			)
			(pin power_in line
				(at 7.62 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "L9")
			)
			(pin power_in line
				(at 7.62 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "K8")
			)
			(pin power_in line
				(at 8.89 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "L10")
			)
			(pin power_in line
				(at 8.89 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "K9")
			)
			(pin power_in line
				(at 10.16 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "L12")
			)
			(pin power_in line
				(at 10.16 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "K10")
			)
			(pin power_in line
				(at 11.43 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "M6")
			)
			(pin power_in line
				(at 11.43 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "L6")
			)
			(pin power_in line
				(at 12.7 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "M7")
			)
			(pin power_in line
				(at 12.7 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "L11")
			)
			(pin power_in line
				(at 13.97 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "M8")
			)
			(pin power_in line
				(at 13.97 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "M5")
			)
			(pin power_in line
				(at 15.24 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "M9")
			)
			(pin power_in line
				(at 15.24 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "M12")
			)
			(pin power_in line
				(at 16.51 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "M10")
			)
			(pin power_in line
				(at 16.51 -128.27 90)
				(length 6.35)
				(name "GND")
				(number "T16")
			)
			(pin power_in line
				(at 17.78 128.27 270)
				(length 6.35)
				(name "VCC")
				(number "M11")
			)
			(pin passive line
				(at 19.05 -128.27 90)
				(length 6.35)
				(name "GNDF")
				(number "B5")
			)
			(pin power_in line
				(at 20.32 -128.27 90)
				(length 6.35)
				(name "GNDF")
				(number "B12")
			)
			(pin power_in line
				(at 21.59 128.27 270)
				(length 6.35)
				(name "VDDF")
				(number "A12")
			)
			(pin power_in line
				(at 22.86 128.27 270)
				(length 6.35)
				(name "VDDF")
				(number "C5")
			)
			(pin power_in line
				(at 24.13 128.27 270)
				(length 6.35)
				(name "VDDF")
				(number "D5")
			)
			(pin power_in line
				(at 25.4 128.27 270)
				(length 6.35)
				(name "VDDF")
				(number "D11")
			)
			(pin power_in line
				(at 27.94 128.27 270)
				(length 6.35)
				(name "VPP")
				(number "A6")
			)
			(pin power_in line
				(at 29.21 128.27 270)
				(length 6.35)
				(name "VDDH")
				(number "P2")
			)
			(pin power_in line
				(at 30.48 128.27 270)
				(length 6.35)
				(name "VSTBY")
				(number "N11")
			)
			(pin bidirectional line
				(at 50.8 119.38 180)
				(length 7.62)
				(name "D0/PD0")
				(number "P6")
			)
			(pin bidirectional line
				(at 50.8 116.84 180)
				(length 7.62)
				(name "D1/PD1")
				(number "R6")
			)
			(pin bidirectional line
				(at 50.8 114.3 180)
				(length 7.62)
				(name "D2/PD2")
				(number "T6")
			)
			(pin bidirectional line
				(at 50.8 111.76 180)
				(length 7.62)
				(name "D3/PD3")
				(number "N5")
			)
			(pin bidirectional line
				(at 50.8 109.22 180)
				(length 7.62)
				(name "D4/PD4")
				(number "P1")
			)
			(pin bidirectional line
				(at 50.8 106.68 180)
				(length 7.62)
				(name "D5/PD5")
				(number "N3")
			)
			(pin bidirectional line
				(at 50.8 104.14 180)
				(length 7.62)
				(name "D6/PD6")
				(number "N2")
			)
			(pin bidirectional line
				(at 50.8 101.6 180)
				(length 7.62)
				(name "D7/PD7")
				(number "N1")
			)
			(pin bidirectional line
				(at 50.8 99.06 180)
				(length 7.62)
				(name "D8/PC0")
				(number "M4")
			)
			(pin bidirectional line
				(at 50.8 96.52 180)
				(length 7.62)
				(name "D9/PC1")
				(number "M3")
			)
			(pin bidirectional line
				(at 50.8 93.98 180)
				(length 7.62)
				(name "D10/PC2")
				(number "M2")
			)
			(pin bidirectional line
				(at 50.8 91.44 180)
				(length 7.62)
				(name "D11/PC3")
				(number "M1")
			)
			(pin bidirectional line
				(at 50.8 88.9 180)
				(length 7.62)
				(name "D12/PC4")
				(number "L4")
			)
			(pin bidirectional line
				(at 50.8 86.36 180)
				(length 7.62)
				(name "D13/PC5")
				(number "L3")
			)
			(pin bidirectional line
				(at 50.8 83.82 180)
				(length 7.62)
				(name "D14/PC6")
				(number "L2")
			)
			(pin bidirectional line
				(at 50.8 81.28 180)
				(length 7.62)
				(name "D15/PC7")
				(number "L1")
			)
			(pin bidirectional line
				(at 50.8 78.74 180)
				(length 7.62)
				(name "D16/PB0")
				(number "K3")
			)
			(pin bidirectional line
				(at 50.8 76.2 180)
				(length 7.62)
				(name "D17/PB1")
				(number "K2")
			)
			(pin bidirectional line
				(at 50.8 73.66 180)
				(length 7.62)
				(name "D18/PB2")
				(number "K1")
			)
			(pin bidirectional line
				(at 50.8 71.12 180)
				(length 7.62)
				(name "D19/PB3")
				(number "J4")
			)
			(pin bidirectional line
				(at 50.8 68.58 180)
				(length 7.62)
				(name "D20/PB4")
				(number "J3")
			)
			(pin bidirectional line
				(at 50.8 66.04 180)
				(length 7.62)
				(name "D21/PB5")
				(number "J2")
			)
			(pin bidirectional line
				(at 50.8 63.5 180)
				(length 7.62)
				(name "D22/PB6")
				(number "J1")
			)
			(pin bidirectional line
				(at 50.8 60.96 180)
				(length 7.62)
				(name "D23/PB7")
				(number "H4")
			)
			(pin bidirectional line
				(at 50.8 58.42 180)
				(length 7.62)
				(name "D24/PA0")
				(number "H3")
			)
			(pin bidirectional line
				(at 50.8 55.88 180)
				(length 7.62)
				(name "D25/PA1")
				(number "H2")
			)
			(pin bidirectional line
				(at 50.8 53.34 180)
				(length 7.62)
				(name "D26/PA2")
				(number "H1")
			)
			(pin bidirectional line
				(at 50.8 50.8 180)
				(length 7.62)
				(name "D27/PA3")
				(number "G4")
			)
			(pin bidirectional line
				(at 50.8 48.26 180)
				(length 7.62)
				(name "D28/PA4")
				(number "G3")
			)
			(pin bidirectional line
				(at 50.8 45.72 180)
				(length 7.62)
				(name "D29/PA5")
				(number "G2")
			)
			(pin bidirectional line
				(at 50.8 43.18 180)
				(length 7.62)
				(name "D30/PA6")
				(number "G1")
			)
			(pin bidirectional line
				(at 50.8 40.64 180)
				(length 7.62)
				(name "D31/PA7")
				(number "F3")
			)
			(pin bidirectional line
				(at 50.8 35.56 180)
				(length 7.62)
				(name "A0/PH0")
				(number "F2")
			)
			(pin bidirectional line
				(at 50.8 33.02 180)
				(length 7.62)
				(name "A1/PH1")
				(number "F1")
			)
			(pin bidirectional line
				(at 50.8 30.48 180)
				(length 7.62)
				(name "A2/PH2")
				(number "E4")
			)
			(pin bidirectional line
				(at 50.8 27.94 180)
				(length 7.62)
				(name "A3/PH3")
				(number "E3")
			)
			(pin bidirectional line
				(at 50.8 25.4 180)
				(length 7.62)
				(name "A4/PH4")
				(number "E2")
			)
			(pin bidirectional line
				(at 50.8 22.86 180)
				(length 7.62)
				(name "A5/PH5")
				(number "E1")
			)
			(pin bidirectional line
				(at 50.8 20.32 180)
				(length 7.62)
				(name "A6/PH6")
				(number "D4")
			)
			(pin bidirectional line
				(at 50.8 17.78 180)
				(length 7.62)
				(name "A7/PH7")
				(number "D3")
			)
			(pin bidirectional line
				(at 50.8 15.24 180)
				(length 7.62)
				(name "A8/PG0")
				(number "D2")
			)
			(pin bidirectional line
				(at 50.8 12.7 180)
				(length 7.62)
				(name "A9/PG1")
				(number "D1")
			)
			(pin bidirectional line
				(at 50.8 10.16 180)
				(length 7.62)
				(name "A10/PG2")
				(number "C3")
			)
			(pin bidirectional line
				(at 50.8 7.62 180)
				(length 7.62)
				(name "A11/PG3")
				(number "C2")
			)
			(pin bidirectional line
				(at 50.8 5.08 180)
				(length 7.62)
				(name "A12/PG4")
				(number "C1")
			)
			(pin bidirectional line
				(at 50.8 2.54 180)
				(length 7.62)
				(name "A13/PG5")
				(number "B2")
			)
			(pin bidirectional line
				(at 50.8 0 180)
				(length 7.62)
				(name "A14/PG6")
				(number "B1")
			)
			(pin bidirectional line
				(at 50.8 -2.54 180)
				(length 7.62)
				(name "A15/PG7")
				(number "A2")
			)
			(pin bidirectional line
				(at 50.8 -5.08 180)
				(length 7.62)
				(name "A16/PF0")
				(number "A3")
			)
			(pin bidirectional line
				(at 50.8 -7.62 180)
				(length 7.62)
				(name "A17/PF1")
				(number "B3")
			)
			(pin bidirectional line
				(at 50.8 -10.16 180)
				(length 7.62)
				(name "A18/PF2")
				(number "A4")
			)
			(pin bidirectional line
				(at 50.8 -12.7 180)
				(length 7.62)
				(name "A19/PF3")
				(number "B4")
			)
			(pin bidirectional line
				(at 50.8 -15.24 180)
				(length 7.62)
				(name "A20/PF4")
				(number "C4")
			)
			(pin bidirectional line
				(at 50.8 -17.78 180)
				(length 7.62)
				(name "A21/PF5/~{CS4}")
				(number "A5")
			)
			(pin bidirectional line
				(at 50.8 -20.32 180)
				(length 7.62)
				(name "A22/PF6/~{CS5}")
				(number "B6")
			)
			(pin bidirectional line
				(at 50.8 -22.86 180)
				(length 7.62)
				(name "A23/PF7/~{CS6}")
				(number "C6")
			)
			(pin bidirectional line
				(at 50.8 -25.4 180)
				(length 7.62)
				(name "~{CS0}/PJ0")
				(number "L13")
			)
			(pin bidirectional line
				(at 50.8 -27.94 180)
				(length 7.62)
				(name "~{CS1}/PJ1")
				(number "L14")
			)
			(pin bidirectional line
				(at 50.8 -30.48 180)
				(length 7.62)
				(name "~{CS2}/PJ2")
				(number "L15")
			)
			(pin bidirectional line
				(at 50.8 -33.02 180)
				(length 7.62)
				(name "~{CS3}/PJ3")
				(number "L16")
			)
			(pin bidirectional line
				(at 50.8 -38.1 180)
				(length 7.62)
				(name "~{TIP}/PE0/SYNCB")
				(number "M14")
			)
			(pin bidirectional line
				(at 50.8 -40.64 180)
				(length 7.62)
				(name "~{TS}/PE1/SYNCA")
				(number "M15")
			)
			(pin bidirectional line
				(at 50.8 -43.18 180)
				(length 7.62)
				(name "SIZ0/PE2/SYNCB")
				(number "M16")
			)
			(pin bidirectional line
				(at 50.8 -45.72 180)
				(length 7.62)
				(name "SIZ1/PE3/SYNCA")
				(number "N14")
			)
			(pin bidirectional line
				(at 50.8 -48.26 180)
				(length 7.62)
				(name "R/W/PE4")
				(number "N15")
			)
			(pin bidirectional line
				(at 50.8 -50.8 180)
				(length 7.62)
				(name "~{TEA}/PE5")
				(number "P15")
			)
			(pin bidirectional line
				(at 50.8 -53.34 180)
				(length 7.62)
				(name "~{TA}/PE6")
				(number "P16")
			)
			(pin bidirectional line
				(at 50.8 -55.88 180)
				(length 7.62)
				(name "~{OE}/PE7")
				(number "N16")
			)
			(pin bidirectional line
				(at 50.8 -60.96 180)
				(length 7.62)
				(name "~{BS0}/PJ4")
				(number "R16")
			)
			(pin bidirectional line
				(at 50.8 -63.5 180)
				(length 7.62)
				(name "~{BS1}/PJ5")
				(number "R15")
			)
			(pin bidirectional line
				(at 50.8 -66.04 180)
				(length 7.62)
				(name "~{BS2}/PJ6")
				(number "T15")
			)
			(pin bidirectional line
				(at 50.8 -68.58 180)
				(length 7.62)
				(name "~{BS3}/PJ7")
				(number "P14")
			)
			(pin bidirectional line
				(at 50.8 -73.66 180)
				(length 7.62)
				(name "~{SDRAM_CS0}/PSD1")
				(number "G16")
			)
			(pin output line
				(at 50.8 -76.2 180)
				(length 7.62)
				(name "~{SDRAM_CS1}/PSD2")
				(number "H13")
			)
			(pin bidirectional line
				(at 50.8 -78.74 180)
				(length 7.62)
				(name "~{DRAMW}/PSD3")
				(number "G15")
			)
			(pin bidirectional line
				(at 50.8 -81.28 180)
				(length 7.62)
				(name "~{SRAS}/PSD5")
				(number "H15")
			)
			(pin bidirectional line
				(at 50.8 -83.82 180)
				(length 7.62)
				(name "~{SCAS}/PSD4")
				(number "H16")
			)
			(pin bidirectional line
				(at 50.8 -86.36 180)
				(length 7.62)
				(name "SCKE/PSD0")
				(number "H14")
			)
			(pin bidirectional line
				(at 50.8 -91.44 180)
				(length 7.62)
				(name "GPTA0/PTA0")
				(number "N13")
			)
			(pin bidirectional line
				(at 50.8 -93.98 180)
				(length 7.62)
				(name "GPTA1/PTA1")
				(number "P13")
			)
			(pin bidirectional line
				(at 50.8 -96.52 180)
				(length 7.62)
				(name "GPTA2/PTA2")
				(number "R13")
			)
			(pin bidirectional line
				(at 50.8 -99.06 180)
				(length 7.62)
				(name "GPTA3/PTA3")
				(number "T13")
			)
			(pin bidirectional line
				(at 50.8 -101.6 180)
				(length 7.62)
				(name "GPTB0/PTB0")
				(number "N12")
			)
			(pin bidirectional line
				(at 50.8 -104.14 180)
				(length 7.62)
				(name "GPTB1/PTB1")
				(number "P12")
			)
			(pin bidirectional line
				(at 50.8 -106.68 180)
				(length 7.62)
				(name "GPTB2/PTB2")
				(number "R12")
			)
			(pin bidirectional line
				(at 50.8 -109.22 180)
				(length 7.62)
				(name "GPTB3/PTB3")
				(number "T12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCF5328-BGA256"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 3.81 0)
		)
		(property "Value" "MCF5328-BGA256"
			(at 2.54 0 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" ""
			(at 0 0 0)
		)
		(symbol "MCF5328-BGA256_0_1")
		(symbol "MCF5328-BGA256_1_1"
			(pin input line
				(at -60.96 139.7 0)
				(length 7.62)
				(name "/RESET")
				(number "N15")
			)
			(pin output line
				(at -60.96 137.16 0)
				(length 7.62)
				(name "/RSTOUT")
				(number "P14")
			)
			(pin input line
				(at -60.96 132.08 0)
				(length 7.62)
				(name "EXTAL")
				(number "P16")
			)
			(pin output line
				(at -60.96 129.54 0)
				(length 7.62)
				(name "XTAL")
				(number "N16")
			)
			(pin input line
				(at -60.96 127 0)
				(length 7.62)
				(name "EXTAL32K")
				(number "P13")
			)
			(pin output line
				(at -60.96 124.46 0)
				(length 7.62)
				(name "XTAL32K")
				(number "R13")
			)
			(pin input line
				(at -60.96 121.92 0)
				(length 7.62)
				(name "/RCON")
				(number "M8")
			)
			(pin input line
				(at -60.96 119.38 0)
				(length 7.62)
				(name "DRAMSEL")
				(number "H12")
			)
			(pin input line
				(at -60.96 114.3 0)
				(length 7.62)
				(name "/IRQ7")
				(number "J13")
			)
			(pin input line
				(at -60.96 111.76 0)
				(length 7.62)
				(name "/IRQ6/VBUS_EN")
				(number "J14")
			)
			(pin input line
				(at -60.96 109.22 0)
				(length 7.62)
				(name "/IRQ5/VBUS_OC")
				(number "J15")
			)
			(pin input line
				(at -60.96 106.68 0)
				(length 7.62)
				(name "/IRQ4/SSI_MCLK")
				(number "J16")
			)
			(pin input line
				(at -60.96 104.14 0)
				(length 7.62)
				(name "/IRQ3")
				(number "K14")
			)
			(pin input line
				(at -60.96 101.6 0)
				(length 7.62)
				(name "/IRQ2/USB_CLKIN")
				(number "K15")
			)
			(pin input line
				(at -60.96 99.06 0)
				(length 7.62)
				(name "/IRQ1/DREQ1")
				(number "K16")
			)
			(pin bidirectional line
				(at -60.96 96.52 0)
				(length 7.62)
				(name "USBOTG_M")
				(number "L15")
			)
			(pin bidirectional line
				(at -60.96 93.98 0)
				(length 7.62)
				(name "USBOTG_P")
				(number "L16")
			)
			(pin bidirectional line
				(at -60.96 91.44 0)
				(length 7.62)
				(name "USBHOST_M")
				(number "M15")
			)
			(pin bidirectional line
				(at -60.96 88.9 0)
				(length 7.62)
				(name "USBHOST_P")
				(number "M16")
			)
			(pin output line
				(at -60.96 83.82 0)
				(length 7.62)
				(name "QSPI_CS2/U2RTS")
				(number "T12")
			)
			(pin output line
				(at -60.96 81.28 0)
				(length 7.62)
				(name "QSPI_CS1/PWM7")
				(number "T13")
			)
			(pin output line
				(at -60.96 78.74 0)
				(length 7.62)
				(name "QSPI_CSO/PWM5")
				(number "P11")
			)
			(pin output line
				(at -60.96 76.2 0)
				(length 7.62)
				(name "QSPI_CLK/I2C_SCL")
				(number "R12")
			)
			(pin input line
				(at -60.96 73.66 0)
				(length 7.62)
				(name "QSPI_DIN/U2CTS")
				(number "N12")
			)
			(pin output line
				(at -60.96 71.12 0)
				(length 7.62)
				(name "QSPI_DOUT/I2C_SDA")
				(number "P12")
			)
			(pin bidirectional line
				(at -60.96 68.58 0)
				(length 7.62)
				(name "PWM7")
				(number "H13")
			)
			(pin bidirectional line
				(at -60.96 66.04 0)
				(length 7.62)
				(name "PWM5")
				(number "H14")
			)
			(pin bidirectional line
				(at -60.96 63.5 0)
				(length 7.62)
				(name "PWM3/DT3OUT")
				(number "H15")
			)
			(pin bidirectional line
				(at -60.96 60.96 0)
				(length 7.62)
				(name "PWM1/DT2OUT")
				(number "H16")
			)
			(pin bidirectional line
				(at -60.96 58.42 0)
				(length 7.62)
				(name "I2C_SCL")
				(number "F3")
			)
			(pin bidirectional line
				(at -60.96 55.88 0)
				(length 7.62)
				(name "I2C_SDA")
				(number "F2")
			)
			(pin bidirectional line
				(at -60.96 50.8 0)
				(length 7.62)
				(name "SSI_MCLK")
				(number "G4")
			)
			(pin bidirectional line
				(at -60.96 48.26 0)
				(length 7.62)
				(name "SSI_BCLK/U2CTS")
				(number "F4")
			)
			(pin bidirectional line
				(at -60.96 45.72 0)
				(length 7.62)
				(name "SSI_FS/U2RTS")
				(number "G3")
			)
			(pin input line
				(at -60.96 43.18 0)
				(length 7.62)
				(name "SSI_RXD/U2RXD")
				(number "G2")
			)
			(pin output line
				(at -60.96 40.64 0)
				(length 7.62)
				(name "SSI_TXD/U2TXD")
				(number "G1")
			)
			(pin input line
				(at -60.96 35.56 0)
				(length 7.62)
				(name "DT3IN/DT3OUT")
				(number "F1")
			)
			(pin input line
				(at -60.96 33.02 0)
				(length 7.62)
				(name "DT2IN/DT2OUT")
				(number "E1")
			)
			(pin input line
				(at -60.96 30.48 0)
				(length 7.62)
				(name "DT1IN/DT1OUT")
				(number "E2")
			)
			(pin input line
				(at -60.96 27.94 0)
				(length 7.62)
				(name "DT0IN/TD0OUT")
				(number "E3")
			)
			(pin input line
				(at -60.96 22.86 0)
				(length 7.62)
				(name "/U1CTS/SSI_BCLK")
				(number "D11")
			)
			(pin output line
				(at -60.96 20.32 0)
				(length 7.62)
				(name "/U1RTS/SSI_FS")
				(number "E10")
			)
			(pin output line
				(at -60.96 17.78 0)
				(length 7.62)
				(name "U1TXD/SSI_TXD")
				(number "E11")
			)
			(pin input line
				(at -60.96 15.24 0)
				(length 7.62)
				(name "U1RXD/SSI_RXD")
				(number "E12")
			)
			(pin input line
				(at -60.96 12.7 0)
				(length 7.62)
				(name "/U0CTS")
				(number "R15")
			)
			(pin output line
				(at -60.96 10.16 0)
				(length 7.62)
				(name "/U0RTS")
				(number "T15")
			)
			(pin output line
				(at -60.96 7.62 0)
				(length 7.62)
				(name "U0TXD")
				(number "T14")
			)
			(pin input line
				(at -60.96 5.08 0)
				(length 7.62)
				(name "U0RXD")
				(number "R14")
			)
			(pin input line
				(at -60.96 2.54 0)
				(length 7.62)
				(name "JTAG_EN")
				(number "M13")
			)
			(pin input line
				(at -60.96 0 0)
				(length 7.62)
				(name "DSCLK/TRST")
				(number "P15")
			)
			(pin output line
				(at -60.96 -2.54 0)
				(length 7.62)
				(name "PSTCLK/TCLK")
				(number "T9")
			)
			(pin input line
				(at -60.96 -5.08 0)
				(length 7.62)
				(name "BKPT/TMS")
				(number "R16")
			)
			(pin input line
				(at -60.96 -7.62 0)
				(length 7.62)
				(name "DSI/TDI")
				(number "N14")
			)
			(pin output line
				(at -60.96 -10.16 0)
				(length 7.62)
				(name "DSO/TDO")
				(number "N11")
			)
			(pin output line
				(at -60.96 -12.7 0)
				(length 7.62)
				(name "DDATA3")
				(number "N9")
			)
			(pin output line
				(at -60.96 -15.24 0)
				(length 7.62)
				(name "DDATA2")
				(number "P9")
			)
			(pin output line
				(at -60.96 -17.78 0)
				(length 7.62)
				(name "DDATA1")
				(number "N10")
			)
			(pin output line
				(at -60.96 -20.32 0)
				(length 7.62)
				(name "DDATA0")
				(number "P10")
			)
			(pin output line
				(at -60.96 -22.86 0)
				(length 7.62)
				(name "PST3")
				(number "R10")
			)
			(pin output line
				(at -60.96 -25.4 0)
				(length 7.62)
				(name "PST2")
				(number "T10")
			)
			(pin output line
				(at -60.96 -27.94 0)
				(length 7.62)
				(name "PST1")
				(number "R11")
			)
			(pin output line
				(at -60.96 -30.48 0)
				(length 7.62)
				(name "PST0")
				(number "T11")
			)
			(pin input line
				(at -60.96 -33.02 0)
				(length 7.62)
				(name "TEST")
				(number "A16")
			)
			(pin input line
				(at -60.96 -35.56 0)
				(length 7.62)
				(name "PLL_TEST")
				(number "N13")
			)
			(pin output line
				(at -60.96 -40.64 0)
				(length 7.62)
				(name "FEC_MDC/I2C_SCL")
				(number "C1")
			)
			(pin bidirectional line
				(at -60.96 -43.18 0)
				(length 7.62)
				(name "FEC_MDIO/I2C_SDA")
				(number "C2")
			)
			(pin input line
				(at -60.96 -45.72 0)
				(length 7.62)
				(name "FEC_TXCLK")
				(number "A2")
			)
			(pin output line
				(at -60.96 -48.26 0)
				(length 7.62)
				(name "FEC_TXEN")
				(number "B2")
			)
			(pin output line
				(at -60.96 -50.8 0)
				(length 7.62)
				(name "FEC_TXD0/ULPI_DATA0")
				(number "E4")
			)
			(pin input line
				(at -60.96 -53.34 0)
				(length 7.62)
				(name "FEC_COL/ULPI_CLK")
				(number "A8")
			)
			(pin input line
				(at -60.96 -55.88 0)
				(length 7.62)
				(name "FEC_RXCLK/ULPI_NXT")
				(number "C8")
			)
			(pin input line
				(at -60.96 -58.42 0)
				(length 7.62)
				(name "FEC_RXDV/ULPI_STP")
				(number "D8")
			)
			(pin input line
				(at -60.96 -60.96 0)
				(length 7.62)
				(name "FEC_RXD0/ULPI_DATA4")
				(number "C6")
			)
			(pin input line
				(at -60.96 -63.5 0)
				(length 7.62)
				(name "FEC_CRS/ULPI_DIR")
				(number "B8")
			)
			(pin output line
				(at -60.96 -66.04 0)
				(length 7.62)
				(name "FEC_TDX3/ULPI_DATA3")
				(number "D3")
			)
			(pin output line
				(at -60.96 -68.58 0)
				(length 7.62)
				(name "FEC_TXD2/ULPI_DATA2")
				(number "D2")
			)
			(pin output line
				(at -60.96 -71.12 0)
				(length 7.62)
				(name "FEC_TXD1/ULPI_DATA1")
				(number "D1")
			)
			(pin output line
				(at -60.96 -73.66 0)
				(length 7.62)
				(name "FEC_TXER")
				(number "B1")
			)
			(pin input line
				(at -60.96 -76.2 0)
				(length 7.62)
				(name "FEC_RXD3/ULPI_DATA7")
				(number "E7")
			)
			(pin input line
				(at -60.96 -78.74 0)
				(length 7.62)
				(name "FEC_RXD2/ULPI_DATA6")
				(number "A6")
			)
			(pin input line
				(at -60.96 -81.28 0)
				(length 7.62)
				(name "FEC_RXD1/ULPI_DATA5")
				(number "B6")
			)
			(pin input line
				(at -60.96 -83.82 0)
				(length 7.62)
				(name "FEC_RXER")
				(number "D4")
			)
			(pin power_in line
				(at -60.96 -88.9 0)
				(length 7.62)
				(name "PLL_VDD")
				(number "J12")
			)
			(pin power_in line
				(at -60.96 -91.44 0)
				(length 7.62)
				(name "PLL_VSS")
				(number "K13")
			)
			(pin power_in line
				(at -60.96 -96.52 0)
				(length 7.62)
				(name "USBOTG_VDD")
				(number "L14")
			)
			(pin power_in line
				(at -60.96 -99.06 0)
				(length 7.62)
				(name "USBHOST_VSS")
				(number "M14")
			)
			(pin power_in line
				(at -48.26 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "E8")
			)
			(pin power_in line
				(at -45.72 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "F5")
			)
			(pin power_in line
				(at -43.18 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "F6")
			)
			(pin power_in line
				(at -40.64 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "F7")
			)
			(pin power_in line
				(at -38.1 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "F8")
			)
			(pin power_in line
				(at -35.56 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "G5")
			)
			(pin power_in line
				(at -33.02 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "G6")
			)
			(pin power_in line
				(at -30.48 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "H5")
			)
			(pin power_in line
				(at -27.94 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "H6")
			)
			(pin power_in line
				(at -25.4 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "J11")
			)
			(pin power_in line
				(at -22.86 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "K11")
			)
			(pin power_in line
				(at -22.86 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "G7")
			)
			(pin power_in line
				(at -20.32 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "K12")
			)
			(pin power_in line
				(at -20.32 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "G8")
			)
			(pin power_in line
				(at -17.78 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "L9")
			)
			(pin power_in line
				(at -17.78 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "G9")
			)
			(pin power_in line
				(at -15.24 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "L10")
			)
			(pin power_in line
				(at -15.24 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "G10")
			)
			(pin power_in line
				(at -12.7 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "L11")
			)
			(pin power_in line
				(at -12.7 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "H7")
			)
			(pin power_in line
				(at -10.16 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "M9")
			)
			(pin power_in line
				(at -10.16 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "H8")
			)
			(pin power_in line
				(at -7.62 157.48 270)
				(length 7.62)
				(name "EVDD")
				(number "M10")
			)
			(pin power_in line
				(at -7.62 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "H9")
			)
			(pin power_in line
				(at -5.08 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "E9")
			)
			(pin power_in line
				(at -5.08 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "H10")
			)
			(pin power_in line
				(at -2.54 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "F9")
			)
			(pin power_in line
				(at -2.54 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "J7")
			)
			(pin power_in line
				(at 0 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "F10")
			)
			(pin power_in line
				(at 0 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "J8")
			)
			(pin power_in line
				(at 2.54 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "F11")
			)
			(pin power_in line
				(at 2.54 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "J9")
			)
			(pin power_in line
				(at 5.08 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "G11")
			)
			(pin power_in line
				(at 5.08 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "J10")
			)
			(pin power_in line
				(at 7.62 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "H11")
			)
			(pin power_in line
				(at 7.62 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "K7")
			)
			(pin power_in line
				(at 10.16 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "J5")
			)
			(pin power_in line
				(at 10.16 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "K8")
			)
			(pin power_in line
				(at 12.7 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "J6")
			)
			(pin power_in line
				(at 12.7 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "K9")
			)
			(pin power_in line
				(at 15.24 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "K5")
			)
			(pin power_in line
				(at 15.24 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "K10")
			)
			(pin power_in line
				(at 17.78 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "K6")
			)
			(pin power_in line
				(at 17.78 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "L12")
			)
			(pin power_in line
				(at 20.32 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "L5")
			)
			(pin power_in line
				(at 20.32 -157.48 90)
				(length 7.62)
				(name "VSS")
				(number "L13")
			)
			(pin power_in line
				(at 22.86 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "L6")
			)
			(pin power_in line
				(at 25.4 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "L7")
			)
			(pin power_in line
				(at 27.94 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "L8")
			)
			(pin power_in line
				(at 30.48 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "M6")
			)
			(pin power_in line
				(at 33.02 157.48 270)
				(length 7.62)
				(name "SD_VDD")
				(number "M7")
			)
			(pin power_in line
				(at 38.1 157.48 270)
				(length 7.62)
				(name "IVDD")
				(number "E5")
			)
			(pin power_in line
				(at 40.64 157.48 270)
				(length 7.62)
				(name "IVDD")
				(number "G12")
			)
			(pin power_in line
				(at 43.18 157.48 270)
				(length 7.62)
				(name "IVDD")
				(number "M5")
			)
			(pin power_in line
				(at 45.72 157.48 270)
				(length 7.62)
				(name "IVDD")
				(number "M11")
			)
			(pin power_in line
				(at 48.26 157.48 270)
				(length 7.62)
				(name "IVDD")
				(number "M12")
			)
			(pin output line
				(at 60.96 139.7 180)
				(length 7.62)
				(name "FB_CLK")
				(number "T2")
			)
			(pin output line
				(at 60.96 137.16 180)
				(length 7.62)
				(name "FB_CS5")
				(number "B13")
			)
			(pin output line
				(at 60.96 134.62 180)
				(length 7.62)
				(name "FB_CS4")
				(number "A13")
			)
			(pin output line
				(at 60.96 132.08 180)
				(length 7.62)
				(name "FB_CS3")
				(number "A12")
			)
			(pin output line
				(at 60.96 129.54 180)
				(length 7.62)
				(name "FB_CS2")
				(number "B12")
			)
			(pin output line
				(at 60.96 127 180)
				(length 7.62)
				(name "FB_CS1")
				(number "C12")
			)
			(pin output line
				(at 60.96 124.46 180)
				(length 7.62)
				(name "FB_CS0")
				(number "D12")
			)
			(pin output line
				(at 60.96 119.38 180)
				(length 7.62)
				(name "A23/FB_CS5")
				(number "C13")
			)
			(pin output line
				(at 60.96 116.84 180)
				(length 7.62)
				(name "A22/FB_CS4")
				(number "D13")
			)
			(pin output line
				(at 60.96 114.3 180)
				(length 7.62)
				(name "A21")
				(number "E13")
			)
			(pin output line
				(at 60.96 111.76 180)
				(length 7.62)
				(name "A20")
				(number "A14")
			)
			(pin output line
				(at 60.96 109.22 180)
				(length 7.62)
				(name "A19")
				(number "B14")
			)
			(pin output line
				(at 60.96 106.68 180)
				(length 7.62)
				(name "A18")
				(number "C14")
			)
			(pin output line
				(at 60.96 104.14 180)
				(length 7.62)
				(name "A17")
				(number "A15")
			)
			(pin output line
				(at 60.96 101.6 180)
				(length 7.62)
				(name "A16")
				(number "B15")
			)
			(pin output line
				(at 60.96 99.06 180)
				(length 7.62)
				(name "A15/SD_BA1")
				(number "D14")
			)
			(pin output line
				(at 60.96 96.52 180)
				(length 7.62)
				(name "A14/SD_BA0")
				(number "B16")
			)
			(pin output line
				(at 60.96 93.98 180)
				(length 7.62)
				(name "A13/SD_A13")
				(number "C15")
			)
			(pin output line
				(at 60.96 91.44 180)
				(length 7.62)
				(name "A12/SD_A12")
				(number "C16")
			)
			(pin output line
				(at 60.96 88.9 180)
				(length 7.62)
				(name "A11/SD-A11")
				(number "D15")
			)
			(pin output line
				(at 60.96 86.36 180)
				(length 7.62)
				(name "A10")
				(number "D16")
			)
			(pin output line
				(at 60.96 83.82 180)
				(length 7.62)
				(name "A9/SD_A9")
				(number "E14")
			)
			(pin output line
				(at 60.96 81.28 180)
				(length 7.62)
				(name "A8/SD_A8")
				(number "E15")
			)
			(pin output line
				(at 60.96 78.74 180)
				(length 7.62)
				(name "A7/SD_A7")
				(number "E16")
			)
			(pin output line
				(at 60.96 76.2 180)
				(length 7.62)
				(name "A6/SD_A6")
				(number "F13")
			)
			(pin output line
				(at 60.96 73.66 180)
				(length 7.62)
				(name "A5/SD_A5")
				(number "F14")
			)
			(pin output line
				(at 60.96 71.12 180)
				(length 7.62)
				(name "A4/SD_A4")
				(number "F15")
			)
			(pin output line
				(at 60.96 68.58 180)
				(length 7.62)
				(name "A3/SD_A3")
				(number "F16")
			)
			(pin output line
				(at 60.96 66.04 180)
				(length 7.62)
				(name "A2/SD_A2")
				(number "G16")
			)
			(pin output line
				(at 60.96 63.5 180)
				(length 7.62)
				(name "A1/SD_A1")
				(number "G15")
			)
			(pin output line
				(at 60.96 60.96 180)
				(length 7.62)
				(name "A0/SD_A0")
				(number "G14")
			)
			(pin output line
				(at 60.96 55.88 180)
				(length 7.62)
				(name "D31/SD_D31")
				(number "M1")
			)
			(pin output line
				(at 60.96 53.34 180)
				(length 7.62)
				(name "D30/SD_D30")
				(number "M2")
			)
			(pin output line
				(at 60.96 50.8 180)
				(length 7.62)
				(name "D29/SD_D29")
				(number "M3")
			)
			(pin output line
				(at 60.96 48.26 180)
				(length 7.62)
				(name "D28/SD_D28")
				(number "M4")
			)
			(pin output line
				(at 60.96 45.72 180)
				(length 7.62)
				(name "D27/SD_D27")
				(number "N1")
			)
			(pin output line
				(at 60.96 43.18 180)
				(length 7.62)
				(name "D26/SD_D26")
				(number "N2")
			)
			(pin output line
				(at 60.96 40.64 180)
				(length 7.62)
				(name "D25/SD_D25")
				(number "N3")
			)
			(pin output line
				(at 60.96 38.1 180)
				(length 7.62)
				(name "D24/SD_D24")
				(number "N4")
			)
			(pin output line
				(at 60.96 35.56 180)
				(length 7.62)
				(name "D23/SD_D23")
				(number "T3")
			)
			(pin output line
				(at 60.96 33.02 180)
				(length 7.62)
				(name "D22/SD_D22")
				(number "P4")
			)
			(pin output line
				(at 60.96 30.48 180)
				(length 7.62)
				(name "D21/SD_D21")
				(number "R4")
			)
			(pin output line
				(at 60.96 27.94 180)
				(length 7.62)
				(name "D20/SD_D20")
				(number "T4")
			)
			(pin output line
				(at 60.96 25.4 180)
				(length 7.62)
				(name "D19/SD_D19")
				(number "N5")
			)
			(pin output line
				(at 60.96 22.86 180)
				(length 7.62)
				(name "D18/SD_D18")
				(number "P5")
			)
			(pin output line
				(at 60.96 20.32 180)
				(length 7.62)
				(name "D17/SD_D17")
				(number "R5")
			)
			(pin output line
				(at 60.96 17.78 180)
				(length 7.62)
				(name "D16/SD_D16")
				(number "T5")
			)
			(pin output line
				(at 60.96 15.24 180)
				(length 7.62)
				(name "D15/FB_D31")
				(number "J3")
			)
			(pin output line
				(at 60.96 12.7 180)
				(length 7.62)
				(name "D14/FB_D30")
				(number "J2")
			)
			(pin output line
				(at 60.96 10.16 180)
				(length 7.62)
				(name "D13/FB_D29")
				(number "J1")
			)
			(pin output line
				(at 60.96 7.62 180)
				(length 7.62)
				(name "D12/FB_D28")
				(number "K4")
			)
			(pin output line
				(at 60.96 5.08 180)
				(length 7.62)
				(name "D11/FB_D27")
				(number "K3")
			)
			(pin output line
				(at 60.96 2.54 180)
				(length 7.62)
				(name "D10/FB_D26")
				(number "K2")
			)
			(pin output line
				(at 60.96 0 180)
				(length 7.62)
				(name "D9/FB_D25")
				(number "K1")
			)
			(pin output line
				(at 60.96 -2.54 180)
				(length 7.62)
				(name "D8/FB_D24")
				(number "L2")
			)
			(pin output line
				(at 60.96 -5.08 180)
				(length 7.62)
				(name "D7/FB_D23")
				(number "R6")
			)
			(pin output line
				(at 60.96 -7.62 180)
				(length 7.62)
				(name "D6/FB_D22")
				(number "N7")
			)
			(pin output line
				(at 60.96 -10.16 180)
				(length 7.62)
				(name "D5/FB_D21")
				(number "P7")
			)
			(pin output line
				(at 60.96 -12.7 180)
				(length 7.62)
				(name "D4/FB_D20")
				(number "R7")
			)
			(pin output line
				(at 60.96 -15.24 180)
				(length 7.62)
				(name "D3/FB_D19")
				(number "T7")
			)
			(pin output line
				(at 60.96 -17.78 180)
				(length 7.62)
				(name "D2/FB_D18")
				(number "P8")
			)
			(pin output line
				(at 60.96 -20.32 180)
				(length 7.62)
				(name "D1/FB_D17")
				(number "R8")
			)
			(pin output line
				(at 60.96 -22.86 180)
				(length 7.62)
				(name "D0/FB_D16")
				(number "T8")
			)
			(pin output line
				(at 60.96 -27.94 180)
				(length 7.62)
				(name "BE/BWE3/SD_DQM3")
				(number "L4")
			)
			(pin output line
				(at 60.96 -30.48 180)
				(length 7.62)
				(name "BE/BWE2/SD_DQM2")
				(number "P6")
			)
			(pin output line
				(at 60.96 -33.02 180)
				(length 7.62)
				(name "BE/BWE1/SD_DQM1")
				(number "L3")
			)
			(pin output line
				(at 60.96 -35.56 180)
				(length 7.62)
				(name "BE/BWE0/SD_DQM0")
				(number "N6")
			)
			(pin output line
				(at 60.96 -40.64 180)
				(length 7.62)
				(name "OE")
				(number "R9")
			)
			(pin input line
				(at 60.96 -43.18 180)
				(length 7.62)
				(name "TA")
				(number "G13")
			)
			(pin output line
				(at 60.96 -45.72 180)
				(length 7.62)
				(name "R/W")
				(number "N8")
			)
			(pin output line
				(at 60.96 -48.26 180)
				(length 7.62)
				(name "TS/DACK0")
				(number "H4")
			)
			(pin output line
				(at 60.96 -50.8 180)
				(length 7.62)
				(name "SD_A10")
				(number "P2")
			)
			(pin output line
				(at 60.96 -53.34 180)
				(length 7.62)
				(name "SD_CKE")
				(number "H2")
			)
			(pin output line
				(at 60.96 -55.88 180)
				(length 7.62)
				(name "SD_CLK")
				(number "R1")
			)
			(pin output line
				(at 60.96 -58.42 180)
				(length 7.62)
				(name "/SD_CLK")
				(number "R2")
			)
			(pin output line
				(at 60.96 -60.96 180)
				(length 7.62)
				(name "/SD_CS1")
				(number "J4")
			)
			(pin output line
				(at 60.96 -63.5 180)
				(length 7.62)
				(name "/SD_CS0")
				(number "H1")
			)
			(pin input line
				(at 60.96 -66.04 180)
				(length 7.62)
				(name "SD_DQS3")
				(number "L1")
			)
			(pin input line
				(at 60.96 -68.58 180)
				(length 7.62)
				(name "SD_DQS2")
				(number "T6")
			)
			(pin output line
				(at 60.96 -71.12 180)
				(length 7.62)
				(name "/SD_SCAS")
				(number "P3")
			)
			(pin output line
				(at 60.96 -73.66 180)
				(length 7.62)
				(name "/SD_SRAS")
				(number "R3")
			)
			(pin output line
				(at 60.96 -76.2 180)
				(length 7.62)
				(name "SD_SDR_DQS")
				(number "P1")
			)
			(pin output line
				(at 60.96 -78.74 180)
				(length 7.62)
				(name "/SD_WE")
				(number "H3")
			)
			(pin output line
				(at 60.96 -81.28 180)
				(length 7.62)
				(name "LCD_D17")
				(number "C9")
			)
			(pin output line
				(at 60.96 -83.82 180)
				(length 7.62)
				(name "LCD_D16")
				(number "D9")
			)
			(pin output line
				(at 60.96 -86.36 180)
				(length 7.62)
				(name "LCD_D15/FEC_COL")
				(number "A7")
			)
			(pin output line
				(at 60.96 -88.9 180)
				(length 7.62)
				(name "LCD_D14/FEC_CRS")
				(number "B7")
			)
			(pin output line
				(at 60.96 -91.44 180)
				(length 7.62)
				(name "LCD_D13/FEC_RXCLK")
				(number "C7")
			)
			(pin output line
				(at 60.96 -93.98 180)
				(length 7.62)
				(name "LCD_D12/FEC_RXDV")
				(number "D7")
			)
			(pin output line
				(at 60.96 -96.52 180)
				(length 7.62)
				(name "LCD_D11/FEC_RXD3")
				(number "D6")
			)
			(pin output line
				(at 60.96 -99.06 180)
				(length 7.62)
				(name "LCD_D10/FEC_RXD2")
				(number "E6")
			)
			(pin output line
				(at 60.96 -101.6 180)
				(length 7.62)
				(name "LCD_D9/FEC_RXD1")
				(number "A5")
			)
			(pin output line
				(at 60.96 -104.14 180)
				(length 7.62)
				(name "LCD_D8/FEC_RXD0")
				(number "B5")
			)
			(pin output line
				(at 60.96 -106.68 180)
				(length 7.62)
				(name "LCD_D7/FEC_RXER")
				(number "C5")
			)
			(pin output line
				(at 60.96 -109.22 180)
				(length 7.62)
				(name "LCD_D6/FEC_TXCLK")
				(number "D5")
			)
			(pin output line
				(at 60.96 -111.76 180)
				(length 7.62)
				(name "LCD_D5/FEC_TXEN")
				(number "A4")
			)
			(pin output line
				(at 60.96 -114.3 180)
				(length 7.62)
				(name "LCD_D4/FEC_TXER")
				(number "A3")
			)
			(pin output line
				(at 60.96 -116.84 180)
				(length 7.62)
				(name "LCD_D3/FEC_TXD3")
				(number "B4")
			)
			(pin output line
				(at 60.96 -119.38 180)
				(length 7.62)
				(name "LCD_D2/FEC_TXD2")
				(number "C4")
			)
			(pin output line
				(at 60.96 -121.92 180)
				(length 7.62)
				(name "LCD_D1/FEC_TXD1")
				(number "B3")
			)
			(pin output line
				(at 60.96 -124.46 180)
				(length 7.62)
				(name "LCD_D0/FEC_TXD0")
				(number "C3")
			)
			(pin output line
				(at 60.96 -127 180)
				(length 7.62)
				(name "LCD_ACD/LCD_OE")
				(number "B9")
			)
			(pin output line
				(at 60.96 -129.54 180)
				(length 7.62)
				(name "LCD_CLS")
				(number "A9")
			)
			(pin output line
				(at 60.96 -132.08 180)
				(length 7.62)
				(name "LCD_CONTRAST")
				(number "D10")
			)
			(pin output line
				(at 60.96 -134.62 180)
				(length 7.62)
				(name "LCD_FLM/LCD_VSYNC")
				(number "C10")
			)
			(pin output line
				(at 60.96 -137.16 180)
				(length 7.62)
				(name "LCD_LP/LCD_HSYNC")
				(number "B10")
			)
			(pin output line
				(at 60.96 -139.7 180)
				(length 7.62)
				(name "LCD_LSCLK")
				(number "A10")
			)
			(pin output line
				(at 60.96 -142.24 180)
				(length 7.62)
				(name "LCD_PS")
				(number "A11")
			)
			(pin output line
				(at 60.96 -144.78 180)
				(length 7.62)
				(name "LCD_REV")
				(number "B11")
			)
			(pin output line
				(at 60.96 -147.32 180)
				(length 7.62)
				(name "LCD_SPL_SPR")
				(number "C11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCF5407"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 6.35 0)
		)
		(property "Value" "MCF5407"
			(at 0 11.43 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "Coldfire CPU"
			(at 0 0 0)
		)
		(property "ki_keywords" "COLDFIRE"
			(at 0 0 0)
		)
		(symbol "MCF5407_0_1")
		(symbol "MCF5407_1_1"
			(pin output line
				(at -53.34 104.14 0)
				(length 7.62)
				(name "/RAS0")
				(number "83")
			)
			(pin output line
				(at -53.34 101.6 0)
				(length 7.62)
				(name "/RAS1")
				(number "84")
			)
			(pin output line
				(at -53.34 99.06 0)
				(length 7.62)
				(name "/CAS0")
				(number "86")
			)
			(pin output line
				(at -53.34 96.52 0)
				(length 7.62)
				(name "/CAS1")
				(number "87")
			)
			(pin output line
				(at -53.34 93.98 0)
				(length 7.62)
				(name "/CAS2")
				(number "88")
			)
			(pin output line
				(at -53.34 91.44 0)
				(length 7.62)
				(name "/CAS3")
				(number "90")
			)
			(pin output line
				(at -53.34 88.9 0)
				(length 7.62)
				(name "/DRAMW")
				(number "91")
			)
			(pin output line
				(at -53.34 86.36 0)
				(length 7.62)
				(name "/SRAS")
				(number "92")
			)
			(pin output line
				(at -53.34 83.82 0)
				(length 7.62)
				(name "/SCAS")
				(number "94")
			)
			(pin output line
				(at -53.34 81.28 0)
				(length 7.62)
				(name "SCKE")
				(number "95")
			)
			(pin input line
				(at -53.34 78.74 0)
				(length 7.62)
				(name "EDGESEL")
				(number "168")
			)
			(pin input line
				(at -53.34 73.66 0)
				(length 7.62)
				(name "/IRQ7")
				(number "68")
			)
			(pin input line
				(at -53.34 71.12 0)
				(length 7.62)
				(name "/IRQ5")
				(number "70")
			)
			(pin input line
				(at -53.34 68.58 0)
				(length 7.62)
				(name "/IRQ3")
				(number "71")
			)
			(pin input line
				(at -53.34 66.04 0)
				(length 7.62)
				(name "/IRQ1")
				(number "72")
			)
			(pin output line
				(at -53.34 60.96 0)
				(length 7.62)
				(name "TXD0")
				(number "166")
			)
			(pin input line
				(at -53.34 58.42 0)
				(length 7.62)
				(name "RXD0")
				(number "165")
			)
			(pin output line
				(at -53.34 55.88 0)
				(length 7.62)
				(name "/RTS0")
				(number "164")
			)
			(pin input line
				(at -53.34 53.34 0)
				(length 7.62)
				(name "/CTS0")
				(number "163")
			)
			(pin output line
				(at -53.34 50.8 0)
				(length 7.62)
				(name "TXD1")
				(number "161")
			)
			(pin input line
				(at -53.34 48.26 0)
				(length 7.62)
				(name "RXD1")
				(number "160")
			)
			(pin output line
				(at -53.34 45.72 0)
				(length 7.62)
				(name "/RTS1")
				(number "159")
			)
			(pin input line
				(at -53.34 43.18 0)
				(length 7.62)
				(name "/CTS1")
				(number "158")
			)
			(pin input line
				(at -53.34 38.1 0)
				(length 7.62)
				(name "TIN0")
				(number "80")
			)
			(pin output line
				(at -53.34 35.56 0)
				(length 7.62)
				(name "TOUT0")
				(number "79")
			)
			(pin input line
				(at -53.34 33.02 0)
				(length 7.62)
				(name "TIN1")
				(number "82")
			)
			(pin output line
				(at -53.34 30.48 0)
				(length 7.62)
				(name "TOUT1")
				(number "78")
			)
			(pin bidirectional line
				(at -53.34 25.4 0)
				(length 7.62)
				(name "SDA")
				(number "103")
			)
			(pin bidirectional line
				(at -53.34 22.86 0)
				(length 7.62)
				(name "SCL")
				(number "102")
			)
			(pin passive line
				(at -53.34 16.51 0)
				(length 7.62)
				(name "PVCC")
				(number "180")
			)
			(pin passive line
				(at -53.34 12.7 0)
				(length 7.62)
				(name "PGND")
				(number "178")
			)
			(pin output line
				(at -53.34 7.62 0)
				(length 7.62)
				(name "CLKIN")
				(number "174")
			)
			(pin output line
				(at -53.34 5.08 0)
				(length 7.62)
				(name "BCLKO")
				(number "170")
			)
			(pin bidirectional line
				(at -53.34 0 0)
				(length 7.62)
				(name "PP0/TT0")
				(number "207")
			)
			(pin bidirectional line
				(at -53.34 -2.54 0)
				(length 7.62)
				(name "PP1/TT1")
				(number "206")
			)
			(pin bidirectional line
				(at -53.34 -5.08 0)
				(length 7.62)
				(name "PP2/TM0")
				(number "204")
			)
			(pin bidirectional line
				(at -53.34 -7.62 0)
				(length 7.62)
				(name "PP3/TM1")
				(number "203")
			)
			(pin bidirectional line
				(at -53.34 -10.16 0)
				(length 7.62)
				(name "PP4/TM2")
				(number "202")
			)
			(pin bidirectional line
				(at -53.34 -12.7 0)
				(length 7.62)
				(name "PP6/DREQ0")
				(number "199")
			)
			(pin bidirectional line
				(at -53.34 -15.24 0)
				(length 7.62)
				(name "PP5/DREQ1")
				(number "200")
			)
			(pin bidirectional line
				(at -53.34 -17.78 0)
				(length 7.62)
				(name "PP7/TIP")
				(number "198")
			)
			(pin input line
				(at -53.34 -22.86 0)
				(length 7.62)
				(name "/RSTI")
				(number "67")
			)
			(pin output line
				(at -53.34 -25.4 0)
				(length 7.62)
				(name "/RSTO")
				(number "172")
			)
			(pin input line
				(at -53.34 -30.48 0)
				(length 7.62)
				(name "/BG")
				(number "76")
			)
			(pin output line
				(at -53.34 -33.02 0)
				(length 7.62)
				(name "/BD")
				(number "75")
			)
			(pin output line
				(at -53.34 -35.56 0)
				(length 7.62)
				(name "/BR")
				(number "74")
			)
			(pin bidirectional line
				(at -53.34 -40.64 0)
				(length 7.62)
				(name "SIZ0")
				(number "46")
			)
			(pin bidirectional line
				(at -53.34 -43.18 0)
				(length 7.62)
				(name "SIZ1")
				(number "47")
			)
			(pin bidirectional line
				(at -53.34 -48.26 0)
				(length 7.62)
				(name "/AS")
				(number "62")
			)
			(pin bidirectional line
				(at -53.34 -50.8 0)
				(length 7.62)
				(name "R/W")
				(number "63")
			)
			(pin bidirectional line
				(at -53.34 -53.34 0)
				(length 7.62)
				(name "/TA")
				(number "64")
			)
			(pin bidirectional line
				(at -53.34 -55.88 0)
				(length 7.62)
				(name "/TS")
				(number "66")
			)
			(pin input line
				(at -53.34 -60.96 0)
				(length 7.62)
				(name "DSCLK")
				(number "149")
			)
			(pin input line
				(at -53.34 -63.5 0)
				(length 7.62)
				(name "DSI")
				(number "153")
			)
			(pin output line
				(at -53.34 -66.04 0)
				(length 7.62)
				(name "DSO")
				(number "151")
			)
			(pin input line
				(at -53.34 -68.58 0)
				(length 7.62)
				(name "TCK")
				(number "150")
			)
			(pin input line
				(at -53.34 -71.12 0)
				(length 7.62)
				(name "/BKPT")
				(number "154")
			)
			(pin input line
				(at -53.34 -73.66 0)
				(length 7.62)
				(name "/HIZ")
				(number "155")
			)
			(pin output line
				(at -53.34 -76.2 0)
				(length 7.62)
				(name "PSTCLK")
				(number "184")
			)
			(pin output line
				(at -53.34 -78.74 0)
				(length 7.62)
				(name "PSTDDATA0")
				(number "186")
			)
			(pin output line
				(at -53.34 -81.28 0)
				(length 7.62)
				(name "PSTDDATA1")
				(number "187")
			)
			(pin output line
				(at -53.34 -83.82 0)
				(length 7.62)
				(name "PSTDDATA2")
				(number "189")
			)
			(pin output line
				(at -53.34 -86.36 0)
				(length 7.62)
				(name "PSTDDATA3")
				(number "190")
			)
			(pin output line
				(at -53.34 -88.9 0)
				(length 7.62)
				(name "PSTDDATA4")
				(number "192")
			)
			(pin output line
				(at -53.34 -91.44 0)
				(length 7.62)
				(name "PSTDDATA5")
				(number "193")
			)
			(pin output line
				(at -53.34 -93.98 0)
				(length 7.62)
				(name "PSTDDATA6")
				(number "195")
			)
			(pin output line
				(at -53.34 -96.52 0)
				(length 7.62)
				(name "PSTDDATA7")
				(number "196")
			)
			(pin input line
				(at -53.34 -101.6 0)
				(length 7.62)
				(name "MTMOD0")
				(number "176")
			)
			(pin input line
				(at -53.34 -104.14 0)
				(length 7.62)
				(name "MTMOD1")
				(number "177")
			)
			(pin input line
				(at -53.34 -106.68 0)
				(length 7.62)
				(name "MTMOD2")
				(number "181")
			)
			(pin input line
				(at -53.34 -109.22 0)
				(length 7.62)
				(name "MTMOD3")
				(number "182")
			)
			(pin power_in line
				(at -35.56 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "7")
			)
			(pin power_in line
				(at -33.02 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "13")
			)
			(pin power_in line
				(at -33.02 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "4")
			)
			(pin power_in line
				(at -30.48 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "21")
			)
			(pin power_in line
				(at -30.48 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "10")
			)
			(pin power_in line
				(at -27.94 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "29")
			)
			(pin power_in line
				(at -27.94 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "17")
			)
			(pin power_in line
				(at -25.4 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "37")
			)
			(pin power_in line
				(at -25.4 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "25")
			)
			(pin power_in line
				(at -22.86 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "45")
			)
			(pin power_in line
				(at -22.86 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "33")
			)
			(pin power_in line
				(at -20.32 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "52")
			)
			(pin power_in line
				(at -20.32 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "41")
			)
			(pin power_in line
				(at -17.78 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "65")
			)
			(pin power_in line
				(at -17.78 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "48")
			)
			(pin power_in line
				(at -15.24 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "81")
			)
			(pin power_in line
				(at -15.24 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "53")
			)
			(pin power_in line
				(at -12.7 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "89")
			)
			(pin power_in line
				(at -12.7 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "61")
			)
			(pin power_in line
				(at -10.16 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "97")
			)
			(pin power_in line
				(at -10.16 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "69")
			)
			(pin power_in line
				(at -7.62 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "113")
			)
			(pin power_in line
				(at -7.62 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "77")
			)
			(pin power_in line
				(at -5.08 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "121")
			)
			(pin power_in line
				(at -5.08 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "85")
			)
			(pin power_in line
				(at -2.54 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "129")
			)
			(pin power_in line
				(at -2.54 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "93")
			)
			(pin power_in line
				(at 0 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "137")
			)
			(pin power_in line
				(at 0 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "101")
			)
			(pin power_in line
				(at 2.54 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "145")
			)
			(pin power_in line
				(at 2.54 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "104")
			)
			(pin power_in line
				(at 5.08 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "167")
			)
			(pin power_in line
				(at 5.08 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "109")
			)
			(pin power_in line
				(at 7.62 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "191")
			)
			(pin power_in line
				(at 7.62 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "117")
			)
			(pin power_in line
				(at 10.16 121.92 270)
				(length 6.35)
				(name "EVCC")
				(number "205")
			)
			(pin power_in line
				(at 10.16 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "125")
			)
			(pin power_in line
				(at 12.7 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "133")
			)
			(pin power_in line
				(at 15.24 121.92 270)
				(length 6.35)
				(name "IVCC")
				(number "1")
			)
			(pin power_in line
				(at 15.24 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "141")
			)
			(pin power_in line
				(at 17.78 121.92 270)
				(length 6.35)
				(name "IVCC")
				(number "57")
			)
			(pin power_in line
				(at 17.78 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "148")
			)
			(pin power_in line
				(at 20.32 121.92 270)
				(length 6.35)
				(name "IVCC")
				(number "73")
			)
			(pin power_in line
				(at 20.32 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "156")
			)
			(pin power_in line
				(at 22.86 121.92 270)
				(length 6.35)
				(name "IVCC")
				(number "105")
			)
			(pin power_in line
				(at 22.86 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "162")
			)
			(pin power_in line
				(at 25.4 121.92 270)
				(length 6.35)
				(name "IVCC")
				(number "152")
			)
			(pin power_in line
				(at 25.4 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "169")
			)
			(pin power_in line
				(at 27.94 121.92 270)
				(length 6.35)
				(name "IVCC")
				(number "157")
			)
			(pin power_in line
				(at 27.94 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "173")
			)
			(pin power_in line
				(at 30.48 121.92 270)
				(length 6.35)
				(name "IVCC")
				(number "171")
			)
			(pin power_in line
				(at 30.48 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "183")
			)
			(pin power_in line
				(at 33.02 121.92 270)
				(length 6.35)
				(name "IVCC")
				(number "175")
			)
			(pin power_in line
				(at 33.02 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "188")
			)
			(pin power_in line
				(at 35.56 121.92 270)
				(length 6.35)
				(name "IVCC")
				(number "185")
			)
			(pin power_in line
				(at 35.56 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "194")
			)
			(pin power_in line
				(at 38.1 121.92 270)
				(length 6.35)
				(name "IVCC")
				(number "197")
			)
			(pin power_in line
				(at 38.1 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "201")
			)
			(pin power_in line
				(at 40.64 -121.92 90)
				(length 6.35)
				(name "GND")
				(number "208")
			)
			(pin bidirectional line
				(at 53.34 104.14 180)
				(length 7.62)
				(name "D0")
				(number "147")
			)
			(pin bidirectional line
				(at 53.34 101.6 180)
				(length 7.62)
				(name "D1")
				(number "146")
			)
			(pin bidirectional line
				(at 53.34 99.06 180)
				(length 7.62)
				(name "D2")
				(number "144")
			)
			(pin bidirectional line
				(at 53.34 96.52 180)
				(length 7.62)
				(name "D3")
				(number "143")
			)
			(pin bidirectional line
				(at 53.34 93.98 180)
				(length 7.62)
				(name "D4")
				(number "142")
			)
			(pin bidirectional line
				(at 53.34 91.44 180)
				(length 7.62)
				(name "D5")
				(number "140")
			)
			(pin bidirectional line
				(at 53.34 88.9 180)
				(length 7.62)
				(name "D6")
				(number "139")
			)
			(pin bidirectional line
				(at 53.34 86.36 180)
				(length 7.62)
				(name "D7")
				(number "138")
			)
			(pin bidirectional line
				(at 53.34 83.82 180)
				(length 7.62)
				(name "D8")
				(number "136")
			)
			(pin bidirectional line
				(at 53.34 81.28 180)
				(length 7.62)
				(name "D9")
				(number "135")
			)
			(pin bidirectional line
				(at 53.34 78.74 180)
				(length 7.62)
				(name "D10")
				(number "134")
			)
			(pin bidirectional line
				(at 53.34 76.2 180)
				(length 7.62)
				(name "D11")
				(number "132")
			)
			(pin bidirectional line
				(at 53.34 73.66 180)
				(length 7.62)
				(name "D12")
				(number "131")
			)
			(pin bidirectional line
				(at 53.34 71.12 180)
				(length 7.62)
				(name "D13")
				(number "130")
			)
			(pin bidirectional line
				(at 53.34 68.58 180)
				(length 7.62)
				(name "D14")
				(number "128")
			)
			(pin bidirectional line
				(at 53.34 66.04 180)
				(length 7.62)
				(name "D15")
				(number "127")
			)
			(pin bidirectional line
				(at 53.34 63.5 180)
				(length 7.62)
				(name "D16")
				(number "126")
			)
			(pin bidirectional line
				(at 53.34 60.96 180)
				(length 7.62)
				(name "D17")
				(number "124")
			)
			(pin bidirectional line
				(at 53.34 58.42 180)
				(length 7.62)
				(name "D18")
				(number "123")
			)
			(pin bidirectional line
				(at 53.34 55.88 180)
				(length 7.62)
				(name "D19")
				(number "122")
			)
			(pin bidirectional line
				(at 53.34 53.34 180)
				(length 7.62)
				(name "D20")
				(number "120")
			)
			(pin bidirectional line
				(at 53.34 50.8 180)
				(length 7.62)
				(name "D21")
				(number "119")
			)
			(pin bidirectional line
				(at 53.34 48.26 180)
				(length 7.62)
				(name "D22")
				(number "118")
			)
			(pin bidirectional line
				(at 53.34 45.72 180)
				(length 7.62)
				(name "D23")
				(number "116")
			)
			(pin bidirectional line
				(at 53.34 43.18 180)
				(length 7.62)
				(name "D24")
				(number "115")
			)
			(pin bidirectional line
				(at 53.34 40.64 180)
				(length 7.62)
				(name "D25")
				(number "114")
			)
			(pin bidirectional line
				(at 53.34 38.1 180)
				(length 7.62)
				(name "D26")
				(number "112")
			)
			(pin bidirectional line
				(at 53.34 35.56 180)
				(length 7.62)
				(name "D27")
				(number "111")
			)
			(pin bidirectional line
				(at 53.34 33.02 180)
				(length 7.62)
				(name "D28")
				(number "110")
			)
			(pin bidirectional line
				(at 53.34 30.48 180)
				(length 7.62)
				(name "D29")
				(number "108")
			)
			(pin bidirectional line
				(at 53.34 27.94 180)
				(length 7.62)
				(name "D30")
				(number "107")
			)
			(pin bidirectional line
				(at 53.34 25.4 180)
				(length 7.62)
				(name "D31")
				(number "106")
			)
			(pin bidirectional line
				(at 53.34 20.32 180)
				(length 7.62)
				(name "A0")
				(number "2")
			)
			(pin bidirectional line
				(at 53.34 17.78 180)
				(length 7.62)
				(name "A1")
				(number "3")
			)
			(pin bidirectional line
				(at 53.34 15.24 180)
				(length 7.62)
				(name "A2")
				(number "5")
			)
			(pin bidirectional line
				(at 53.34 12.7 180)
				(length 7.62)
				(name "A3")
				(number "6")
			)
			(pin bidirectional line
				(at 53.34 10.16 180)
				(length 7.62)
				(name "A4")
				(number "8")
			)
			(pin bidirectional line
				(at 53.34 7.62 180)
				(length 7.62)
				(name "A5")
				(number "9")
			)
			(pin bidirectional line
				(at 53.34 5.08 180)
				(length 7.62)
				(name "A6")
				(number "11")
			)
			(pin bidirectional line
				(at 53.34 2.54 180)
				(length 7.62)
				(name "A7")
				(number "12")
			)
			(pin bidirectional line
				(at 53.34 0 180)
				(length 7.62)
				(name "A8")
				(number "14")
			)
			(pin bidirectional line
				(at 53.34 -2.54 180)
				(length 7.62)
				(name "A9")
				(number "15")
			)
			(pin bidirectional line
				(at 53.34 -5.08 180)
				(length 7.62)
				(name "A10")
				(number "16")
			)
			(pin bidirectional line
				(at 53.34 -7.62 180)
				(length 7.62)
				(name "A11")
				(number "18")
			)
			(pin bidirectional line
				(at 53.34 -10.16 180)
				(length 7.62)
				(name "A12")
				(number "19")
			)
			(pin bidirectional line
				(at 53.34 -12.7 180)
				(length 7.62)
				(name "A13")
				(number "20")
			)
			(pin bidirectional line
				(at 53.34 -15.24 180)
				(length 7.62)
				(name "A14")
				(number "22")
			)
			(pin bidirectional line
				(at 53.34 -17.78 180)
				(length 7.62)
				(name "A15")
				(number "23")
			)
			(pin bidirectional line
				(at 53.34 -20.32 180)
				(length 7.62)
				(name "A16")
				(number "24")
			)
			(pin bidirectional line
				(at 53.34 -22.86 180)
				(length 7.62)
				(name "A17")
				(number "26")
			)
			(pin bidirectional line
				(at 53.34 -25.4 180)
				(length 7.62)
				(name "A18")
				(number "27")
			)
			(pin bidirectional line
				(at 53.34 -27.94 180)
				(length 7.62)
				(name "A19")
				(number "28")
			)
			(pin bidirectional line
				(at 53.34 -30.48 180)
				(length 7.62)
				(name "A20")
				(number "30")
			)
			(pin bidirectional line
				(at 53.34 -33.02 180)
				(length 7.62)
				(name "A21")
				(number "31")
			)
			(pin bidirectional line
				(at 53.34 -35.56 180)
				(length 7.62)
				(name "A22")
				(number "32")
			)
			(pin bidirectional line
				(at 53.34 -38.1 180)
				(length 7.62)
				(name "A23")
				(number "34")
			)
			(pin bidirectional line
				(at 53.34 -40.64 180)
				(length 7.62)
				(name "PP8/A24")
				(number "35")
			)
			(pin bidirectional line
				(at 53.34 -43.18 180)
				(length 7.62)
				(name "PP9/A25")
				(number "36")
			)
			(pin bidirectional line
				(at 53.34 -45.72 180)
				(length 7.62)
				(name "PP10/A26")
				(number "38")
			)
			(pin bidirectional line
				(at 53.34 -48.26 180)
				(length 7.62)
				(name "PP11/A27")
				(number "39")
			)
			(pin bidirectional line
				(at 53.34 -50.8 180)
				(length 7.62)
				(name "PP12/A28")
				(number "40")
			)
			(pin bidirectional line
				(at 53.34 -53.34 180)
				(length 7.62)
				(name "PP13/A29")
				(number "42")
			)
			(pin bidirectional line
				(at 53.34 -55.88 180)
				(length 7.62)
				(name "PP14/A30")
				(number "43")
			)
			(pin bidirectional line
				(at 53.34 -58.42 180)
				(length 7.62)
				(name "PP15/A31")
				(number "44")
			)
			(pin output line
				(at 53.34 -63.5 180)
				(length 7.62)
				(name "/CS0")
				(number "50")
			)
			(pin output line
				(at 53.34 -66.04 180)
				(length 7.62)
				(name "/CS1")
				(number "51")
			)
			(pin output line
				(at 53.34 -68.58 180)
				(length 7.62)
				(name "/CS2")
				(number "54")
			)
			(pin output line
				(at 53.34 -71.12 180)
				(length 7.62)
				(name "/CS3")
				(number "55")
			)
			(pin output line
				(at 53.34 -73.66 180)
				(length 7.62)
				(name "/CS4")
				(number "56")
			)
			(pin output line
				(at 53.34 -76.2 180)
				(length 7.62)
				(name "/CS5")
				(number "58")
			)
			(pin output line
				(at 53.34 -78.74 180)
				(length 7.62)
				(name "/CS6")
				(number "59")
			)
			(pin output line
				(at 53.34 -81.28 180)
				(length 7.62)
				(name "/CS7")
				(number "60")
			)
			(pin output line
				(at 53.34 -86.36 180)
				(length 7.62)
				(name "/OE")
				(number "49")
			)
			(pin bidirectional line
				(at 53.34 -91.44 180)
				(length 7.62)
				(name "/BE0")
				(number "96")
			)
			(pin bidirectional line
				(at 53.34 -93.98 180)
				(length 7.62)
				(name "/BE1")
				(number "98")
			)
			(pin bidirectional line
				(at 53.34 -96.52 180)
				(length 7.62)
				(name "/BE2")
				(number "99")
			)
			(pin bidirectional line
				(at 53.34 -99.06 180)
				(length 7.62)
				(name "/BE3")
				(number "100")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MCF5211CAE66"
		(extends "MCF5212CAE66")
		(property "Reference" "U"
			(at 19.05 50.8 0)
		)
		(property "Value" "MCF5211CAE66"
			(at 16.51 -48.26 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 1.27 1.27 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MCF5213EC.pdf"
			(at 1.27 1.27 0)
		)
		(property "Description" "ColdFire Microcontroller, LQFP64"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
