(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "68HC11"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 45.72 0)
		)
		(property "Value" "68HC11"
			(at 8.89 -45.72 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "HC11 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU Microcontroller HC11"
			(at 0 0 0)
		)
		(symbol "68HC11_0_1")
		(symbol "68HC11_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 7.62)
				(name "PD0/RX")
				(number "42")
			)
			(pin input line
				(at -25.4 38.1 0)
				(length 7.62)
				(name "PD1/TX")
				(number "43")
			)
			(pin input line
				(at -25.4 35.56 0)
				(length 7.62)
				(name "PD2/MISO")
				(number "44")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 7.62)
				(name "PD3/MOSI")
				(number "45")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 7.62)
				(name "PD4/SCLK")
				(number "46")
			)
			(pin input line
				(at -25.4 27.94 0)
				(length 7.62)
				(name "PD5/SS-")
				(number "47")
			)
			(pin input line
				(at -25.4 20.32 0)
				(length 7.62)
				(name "PE0")
				(number "17")
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 7.62)
				(name "PE1")
				(number "18")
			)
			(pin input line
				(at -25.4 15.24 0)
				(length 7.62)
				(name "PE2")
				(number "19")
			)
			(pin input line
				(at -25.4 12.7 0)
				(length 7.62)
				(name "PE3")
				(number "20")
			)
			(pin input input_low
				(at -25.4 5.08 0)
				(length 7.62)
				(name "IRQ")
				(number "41")
			)
			(pin input input_low
				(at -25.4 2.54 0)
				(length 7.62)
				(name "XIRQ")
				(number "40")
			)
			(pin input input_low
				(at -25.4 0 0)
				(length 7.62)
				(name "RESET")
				(number "39")
			)
			(pin output line
				(at -25.4 -7.62 0)
				(length 7.62)
				(name "XTAL")
				(number "30")
			)
			(pin input line
				(at -25.4 -15.24 0)
				(length 7.62)
				(name "EXTAL")
				(number "29")
			)
			(pin output line
				(at -25.4 -22.86 0)
				(length 7.62)
				(name "R/W")
				(number "28")
			)
			(pin output line
				(at -25.4 -25.4 0)
				(length 7.62)
				(name "E")
				(number "27")
			)
			(pin output line
				(at -25.4 -27.94 0)
				(length 7.62)
				(name "AS")
				(number "26")
			)
			(pin input line
				(at -25.4 -33.02 0)
				(length 7.62)
				(name "MODA")
				(number "25")
			)
			(pin input line
				(at -25.4 -35.56 0)
				(length 7.62)
				(name "MODB")
				(number "24")
			)
			(pin passive line
				(at -25.4 -38.1 0)
				(length 7.62)
				(name "VRH")
				(number "22")
			)
			(pin passive line
				(at -25.4 -40.64 0)
				(length 7.62)
				(name "VRL")
				(number "21")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 7.62)
				(name "VCC")
				(number "48")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 7.62)
				(name "GND")
				(number "23")
			)
			(pin input line
				(at 25.4 38.1 180)
				(length 7.62)
				(name "IC3/PA0")
				(number "8")
			)
			(pin input line
				(at 25.4 35.56 180)
				(length 7.62)
				(name "IC2/PA1")
				(number "7")
			)
			(pin input line
				(at 25.4 33.02 180)
				(length 7.62)
				(name "IC1/PA2")
				(number "6")
			)
			(pin output line
				(at 25.4 30.48 180)
				(length 7.62)
				(name "OC5/PA3")
				(number "5")
			)
			(pin output line
				(at 25.4 27.94 180)
				(length 7.62)
				(name "OC4/PA4")
				(number "4")
			)
			(pin output line
				(at 25.4 25.4 180)
				(length 7.62)
				(name "OC3/PA5")
				(number "3")
			)
			(pin output line
				(at 25.4 22.86 180)
				(length 7.62)
				(name "OC2/PA6")
				(number "2")
			)
			(pin input line
				(at 25.4 20.32 180)
				(length 7.62)
				(name "PAI/PA7")
				(number "1")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 7.62)
				(name "A8/PB0")
				(number "16")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 7.62)
				(name "PB1")
				(number "15")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 7.62)
				(name "PB2")
				(number "14")
			)
			(pin output line
				(at 25.4 0 180)
				(length 7.62)
				(name "PB3")
				(number "13")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 7.62)
				(name "PB4")
				(number "12")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 7.62)
				(name "PB5")
				(number "11")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 7.62)
				(name "PB6")
				(number "10")
			)
			(pin output line
				(at 25.4 -10.16 180)
				(length 7.62)
				(name "A15/PB7")
				(number "9")
			)
			(pin tri_state line
				(at 25.4 -20.32 180)
				(length 7.62)
				(name "AD0/PC0")
				(number "31")
			)
			(pin tri_state line
				(at 25.4 -22.86 180)
				(length 7.62)
				(name "PC1")
				(number "32")
			)
			(pin tri_state line
				(at 25.4 -25.4 180)
				(length 7.62)
				(name "PC2")
				(number "33")
			)
			(pin tri_state line
				(at 25.4 -27.94 180)
				(length 7.62)
				(name "PC3")
				(number "34")
			)
			(pin tri_state line
				(at 25.4 -30.48 180)
				(length 7.62)
				(name "PC4")
				(number "35")
			)
			(pin tri_state line
				(at 25.4 -33.02 180)
				(length 7.62)
				(name "PC5")
				(number "36")
			)
			(pin tri_state line
				(at 25.4 -35.56 180)
				(length 7.62)
				(name "PC6")
				(number "37")
			)
			(pin tri_state line
				(at 25.4 -38.1 180)
				(length 7.62)
				(name "AD7/PC7")
				(number "38")
			)
		)
		(embedded_fonts no)
	)
	(symbol "68HC11F1"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 0 2.54 0)
		)
		(property "Value" "68HC11F1"
			(at 0 -2.54 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC68HC11FTS.pdf"
			(at 0 0 0)
		)
		(property "Description" "HC11 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU Microcontroller HC11"
			(at 0 0 0)
		)
		(symbol "68HC11F1_0_1")
		(symbol "68HC11F1_1_1"
			(pin bidirectional line
				(at -27.94 66.04 0)
				(length 7.62)
				(name "PD0/RX")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 7.62)
				(name "PD1/TX")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 7.62)
				(name "PD2/MISO")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 7.62)
				(name "PD3/MOSI")
				(number "31")
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 7.62)
				(name "PD4/SCLK")
				(number "32")
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 7.62)
				(name "PD5/SS-")
				(number "33")
			)
			(pin input line
				(at -27.94 48.26 0)
				(length 7.62)
				(name "PE0")
				(number "59")
			)
			(pin input line
				(at -27.94 45.72 0)
				(length 7.62)
				(name "PE1")
				(number "61")
			)
			(pin input line
				(at -27.94 43.18 0)
				(length 7.62)
				(name "PE2")
				(number "63")
			)
			(pin input line
				(at -27.94 40.64 0)
				(length 7.62)
				(name "PE3")
				(number "65")
			)
			(pin input line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "PE4")
				(number "60")
			)
			(pin input line
				(at -27.94 35.56 0)
				(length 7.62)
				(name "PE5")
				(number "62")
			)
			(pin input line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "PE6")
				(number "64")
			)
			(pin input line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "PE7")
				(number "66")
			)
			(pin input inverted
				(at -27.94 25.4 0)
				(length 7.62)
				(name "IRQ")
				(number "19")
			)
			(pin input inverted
				(at -27.94 22.86 0)
				(length 7.62)
				(name "XIRQ")
				(number "18")
			)
			(pin input inverted
				(at -27.94 20.32 0)
				(length 7.62)
				(name "RESET")
				(number "17")
			)
			(pin output line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "XTAL")
				(number "7")
			)
			(pin input line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "EXTAL")
				(number "6")
			)
			(pin output line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "R/W")
				(number "5")
			)
			(pin output line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "E")
				(number "4")
			)
			(pin input line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "MODA/LR")
				(number "3")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "MODB/STBY")
				(number "2")
			)
			(pin passive line
				(at -27.94 -22.86 0)
				(length 7.62)
				(name "VRH")
				(number "68")
			)
			(pin passive line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "VRL")
				(number "67")
			)
			(pin output line
				(at -27.94 -35.56 0)
				(length 7.62)
				(name "4XOUT")
				(number "8")
			)
			(pin power_in line
				(at -2.54 76.2 270)
				(length 7.62)
				(name "VDD")
				(number "34")
			)
			(pin power_in line
				(at -2.54 -76.2 90)
				(length 7.62)
				(name "VSS")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 7.62)
				(name "IC3/PA0")
				(number "42")
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 7.62)
				(name "IC2/PA1")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 7.62)
				(name "IC1/PA2")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 7.62)
				(name "OC5/PA3")
				(number "39")
			)
			(pin output line
				(at 27.94 53.34 180)
				(length 7.62)
				(name "OC4/PA4")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 7.62)
				(name "OC3/PA5")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "OC2/PA6")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "PA1/PA7")
				(number "35")
			)
			(pin tri_state line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "A8/PB0")
				(number "50")
			)
			(pin tri_state line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "PB1")
				(number "49")
			)
			(pin output line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "PB2")
				(number "48")
			)
			(pin output line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "PB3")
				(number "47")
			)
			(pin output line
				(at 27.94 22.86 180)
				(length 7.62)
				(name "PB4")
				(number "46")
			)
			(pin output line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "PB5")
				(number "45")
			)
			(pin output line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "PB6")
				(number "44")
			)
			(pin output line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "A15/PB7")
				(number "43")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "D0/PC0")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "PC1")
				(number "10")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 7.62)
				(name "PC2")
				(number "11")
			)
			(pin input line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "PC3")
				(number "12")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "PC4")
				(number "13")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "PC5")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "PC6")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 7.62)
				(name "D7/PC7")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "A0/PF0")
				(number "58")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "PF1")
				(number "57")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 7.62)
				(name "PF2")
				(number "56")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 7.62)
				(name "PF3")
				(number "55")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 7.62)
				(name "PF4")
				(number "54")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "PF5")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "PF6")
				(number "52")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "A7/PF7")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 7.62)
				(name "PG0")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "PG1")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "PG2")
				(number "25")
			)
			(pin input line
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "PG3")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 7.62)
				(name "CSIO2/PG4")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 7.62)
				(name "CSIO1/PG5")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 7.62)
				(name "CSGEN/PG6")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 7.62)
				(name "CSPROG/PG7")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "68HC11_PLCC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 7.62 45.72 0)
		)
		(property "Value" "68HC11_PLCC"
			(at 12.7 -46.99 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "HC11 Microcontroller, PLCC-52"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU Microcontroller HC11"
			(at 0 0 0)
		)
		(symbol "68HC11_PLCC_0_1")
		(symbol "68HC11_PLCC_1_1"
			(pin bidirectional line
				(at -25.4 40.64 0)
				(length 7.62)
				(name "PD0/RX")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 38.1 0)
				(length 7.62)
				(name "PD1/TX")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 35.56 0)
				(length 7.62)
				(name "PD2")
				(number "22")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 7.62)
				(name "PD3")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 30.48 0)
				(length 7.62)
				(name "PD4")
				(number "24")
			)
			(pin bidirectional line
				(at -25.4 27.94 0)
				(length 7.62)
				(name "PD5")
				(number "25")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 7.62)
				(name "PE0")
				(number "43")
			)
			(pin input line
				(at -25.4 22.86 0)
				(length 7.62)
				(name "PE1")
				(number "45")
			)
			(pin input line
				(at -25.4 20.32 0)
				(length 7.62)
				(name "PE2")
				(number "47")
			)
			(pin input line
				(at -25.4 17.78 0)
				(length 7.62)
				(name "PE3")
				(number "49")
			)
			(pin input line
				(at -25.4 15.24 0)
				(length 7.62)
				(name "PE4")
				(number "44")
			)
			(pin input line
				(at -25.4 12.7 0)
				(length 7.62)
				(name "PE5")
				(number "46")
			)
			(pin input line
				(at -25.4 10.16 0)
				(length 7.62)
				(name "PE6")
				(number "48")
			)
			(pin input line
				(at -25.4 7.62 0)
				(length 7.62)
				(name "PE7")
				(number "50")
			)
			(pin input line
				(at -25.4 5.08 0)
				(length 7.62)
				(name "IRQ")
				(number "19")
			)
			(pin input line
				(at -25.4 2.54 0)
				(length 7.62)
				(name "XIRQ")
				(number "18")
			)
			(pin input input_low
				(at -25.4 0 0)
				(length 7.62)
				(name "RESET")
				(number "17")
			)
			(pin output line
				(at -25.4 -7.62 0)
				(length 7.62)
				(name "XTAL")
				(number "8")
			)
			(pin input line
				(at -25.4 -15.24 0)
				(length 7.62)
				(name "EXTAL")
				(number "7")
			)
			(pin output line
				(at -25.4 -22.86 0)
				(length 7.62)
				(name "R/W")
				(number "6")
			)
			(pin output line
				(at -25.4 -25.4 0)
				(length 7.62)
				(name "E")
				(number "5")
			)
			(pin output line
				(at -25.4 -27.94 0)
				(length 7.62)
				(name "AS")
				(number "4")
			)
			(pin input line
				(at -25.4 -33.02 0)
				(length 7.62)
				(name "MODA")
				(number "3")
			)
			(pin input line
				(at -25.4 -35.56 0)
				(length 7.62)
				(name "MODB")
				(number "2")
			)
			(pin passive line
				(at -25.4 -38.1 0)
				(length 7.62)
				(name "VRH")
				(number "52")
			)
			(pin passive line
				(at -25.4 -40.64 0)
				(length 7.62)
				(name "VRL")
				(number "51")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 7.62)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 7.62)
				(name "VSS")
				(number "1")
			)
			(pin input line
				(at 25.4 38.1 180)
				(length 7.62)
				(name "IC3/PA0")
				(number "34")
			)
			(pin input line
				(at 25.4 35.56 180)
				(length 7.62)
				(name "IC2/PA1")
				(number "33")
			)
			(pin input line
				(at 25.4 33.02 180)
				(length 7.62)
				(name "IC1/PA2")
				(number "32")
			)
			(pin output line
				(at 25.4 30.48 180)
				(length 7.62)
				(name "OC5/PA3")
				(number "31")
			)
			(pin output line
				(at 25.4 27.94 180)
				(length 7.62)
				(name "OC4/PA4")
				(number "30")
			)
			(pin output line
				(at 25.4 25.4 180)
				(length 7.62)
				(name "OC3/PA5")
				(number "29")
			)
			(pin output line
				(at 25.4 22.86 180)
				(length 7.62)
				(name "OC2/PA6")
				(number "28")
			)
			(pin input line
				(at 25.4 20.32 180)
				(length 7.62)
				(name "PA1/PA7")
				(number "27")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 7.62)
				(name "A8/PB0")
				(number "42")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 7.62)
				(name "PB1")
				(number "41")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 7.62)
				(name "PB2")
				(number "40")
			)
			(pin output line
				(at 25.4 0 180)
				(length 7.62)
				(name "PB3")
				(number "39")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 7.62)
				(name "PB4")
				(number "38")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 7.62)
				(name "PB5")
				(number "37")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 7.62)
				(name "PB6")
				(number "36")
			)
			(pin output line
				(at 25.4 -10.16 180)
				(length 7.62)
				(name "A15/PB7")
				(number "35")
			)
			(pin tri_state line
				(at 25.4 -20.32 180)
				(length 7.62)
				(name "AD0/PC0")
				(number "9")
			)
			(pin tri_state line
				(at 25.4 -22.86 180)
				(length 7.62)
				(name "AD1/PC1")
				(number "10")
			)
			(pin tri_state line
				(at 25.4 -25.4 180)
				(length 7.62)
				(name "AD2/PC2")
				(number "11")
			)
			(pin tri_state line
				(at 25.4 -27.94 180)
				(length 7.62)
				(name "AD3/PC3")
				(number "12")
			)
			(pin tri_state line
				(at 25.4 -30.48 180)
				(length 7.62)
				(name "AD4/PC4")
				(number "13")
			)
			(pin tri_state line
				(at 25.4 -33.02 180)
				(length 7.62)
				(name "AD5/PC5")
				(number "14")
			)
			(pin tri_state line
				(at 25.4 -35.56 180)
				(length 7.62)
				(name "AD6/PC6")
				(number "15")
			)
			(pin tri_state line
				(at 25.4 -38.1 180)
				(length 7.62)
				(name "AD7/PC7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "68HC711_PLCC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 5.08 45.72 0)
		)
		(property "Value" "68HC711_PLCC"
			(at 5.08 -45.72 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "HC11 Microcontroller, PLCC-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU Microcontroller HC11"
			(at 0 0 0)
		)
		(symbol "68HC711_PLCC_0_1")
		(symbol "68HC711_PLCC_1_1"
			(pin input line
				(at -25.4 40.64 0)
				(length 7.62)
				(name "PD0/RX")
				(number "16")
			)
			(pin input line
				(at -25.4 38.1 0)
				(length 7.62)
				(name "PD1/TX")
				(number "17")
			)
			(pin input line
				(at -25.4 35.56 0)
				(length 7.62)
				(name "PD2")
				(number "18")
			)
			(pin input line
				(at -25.4 33.02 0)
				(length 7.62)
				(name "PD3")
				(number "19")
			)
			(pin input line
				(at -25.4 30.48 0)
				(length 7.62)
				(name "PD4")
				(number "20")
			)
			(pin input line
				(at -25.4 27.94 0)
				(length 7.62)
				(name "PD5")
				(number "21")
			)
			(pin input line
				(at -25.4 25.4 0)
				(length 7.62)
				(name "PD6-AS")
				(number "13")
			)
			(pin output line
				(at -25.4 22.86 0)
				(length 7.62)
				(name "PD7-R/W")
				(number "12")
			)
			(pin input inverted
				(at -25.4 5.08 0)
				(length 7.62)
				(name "IRQ/CE")
				(number "15")
			)
			(pin input inverted
				(at -25.4 2.54 0)
				(length 7.62)
				(name "XIRQ/VPP")
				(number "11")
			)
			(pin input inverted
				(at -25.4 0 0)
				(length 7.62)
				(name "RESET")
				(number "14")
			)
			(pin output line
				(at -25.4 -7.62 0)
				(length 7.62)
				(name "XTAL")
				(number "44")
			)
			(pin input line
				(at -25.4 -15.24 0)
				(length 7.62)
				(name "EXTAL")
				(number "43")
			)
			(pin output line
				(at -25.4 -25.4 0)
				(length 7.62)
				(name "E")
				(number "42")
			)
			(pin input line
				(at -25.4 -33.02 0)
				(length 7.62)
				(name "MODA")
				(number "41")
			)
			(pin input line
				(at -25.4 -35.56 0)
				(length 7.62)
				(name "MODB")
				(number "40")
			)
			(pin power_in line
				(at 0 50.8 270)
				(length 7.62)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -50.8 90)
				(length 7.62)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 7.62)
				(name "EVSS")
				(number "1")
			)
			(pin input line
				(at 25.4 38.1 180)
				(length 7.62)
				(name "IC3/PA0")
				(number "30")
			)
			(pin input line
				(at 25.4 35.56 180)
				(length 7.62)
				(name "IC2/PA1")
				(number "29")
			)
			(pin input line
				(at 25.4 33.02 180)
				(length 7.62)
				(name "IC1/PA2")
				(number "28")
			)
			(pin output line
				(at 25.4 30.48 180)
				(length 7.62)
				(name "OC5/PA3")
				(number "27")
			)
			(pin output line
				(at 25.4 27.94 180)
				(length 7.62)
				(name "OC4/PA4")
				(number "26")
			)
			(pin output line
				(at 25.4 25.4 180)
				(length 7.62)
				(name "OC3/PA5")
				(number "25")
			)
			(pin output line
				(at 25.4 22.86 180)
				(length 7.62)
				(name "OC2/PA6")
				(number "24")
			)
			(pin input line
				(at 25.4 20.32 180)
				(length 7.62)
				(name "PA1/PA7")
				(number "23")
			)
			(pin output line
				(at 25.4 7.62 180)
				(length 7.62)
				(name "PB0")
				(number "39")
			)
			(pin output line
				(at 25.4 5.08 180)
				(length 7.62)
				(name "PB1")
				(number "38")
			)
			(pin output line
				(at 25.4 2.54 180)
				(length 7.62)
				(name "PB2")
				(number "37")
			)
			(pin output line
				(at 25.4 0 180)
				(length 7.62)
				(name "PB3")
				(number "36")
			)
			(pin output line
				(at 25.4 -2.54 180)
				(length 7.62)
				(name "PB4")
				(number "35")
			)
			(pin output line
				(at 25.4 -5.08 180)
				(length 7.62)
				(name "PB5")
				(number "34")
			)
			(pin output line
				(at 25.4 -7.62 180)
				(length 7.62)
				(name "PB6")
				(number "33")
			)
			(pin output line
				(at 25.4 -10.16 180)
				(length 7.62)
				(name "PB7/OE")
				(number "32")
			)
			(pin input line
				(at 25.4 -20.32 180)
				(length 7.62)
				(name "PC0")
				(number "3")
			)
			(pin input line
				(at 25.4 -22.86 180)
				(length 7.62)
				(name "PC1")
				(number "4")
			)
			(pin input line
				(at 25.4 -25.4 180)
				(length 7.62)
				(name "PC2")
				(number "5")
			)
			(pin input line
				(at 25.4 -27.94 180)
				(length 7.62)
				(name "PC3")
				(number "6")
			)
			(pin input line
				(at 25.4 -30.48 180)
				(length 7.62)
				(name "PC4")
				(number "7")
			)
			(pin input line
				(at 25.4 -33.02 180)
				(length 7.62)
				(name "PC5")
				(number "8")
			)
			(pin input line
				(at 25.4 -35.56 180)
				(length 7.62)
				(name "PC6")
				(number "9")
			)
			(pin input line
				(at 25.4 -38.1 180)
				(length 7.62)
				(name "PC7")
				(number "10")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC68HC11A8CC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 50.8 0)
		)
		(property "Value" "MC68HC11A8CC"
			(at 1.27 50.8 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" ""
			(at 0 -5.08 0)
		)
		(property "Description" "8K ROM, 256B RAM, 512B EEPROM"
			(at 0 0 0)
		)
		(property "ki_keywords" "HC11 MCU Microcotroller"
			(at 0 0 0)
		)
		(symbol "MC68HC11A8CC_0_1")
		(symbol "MC68HC11A8CC_1_1"
			(pin input line
				(at -20.32 45.72 0)
				(length 3.81)
				(name "EXTAL")
				(number "7")
			)
			(pin output line
				(at -20.32 40.64 0)
				(length 3.81)
				(name "XTAL")
				(number "8")
			)
			(pin input line
				(at -20.32 10.16 0)
				(length 3.81)
				(name "~{RESET}")
				(number "17")
			)
			(pin input line
				(at -20.32 2.54 0)
				(length 3.81)
				(name "~{IRQ}")
				(number "19")
			)
			(pin input line
				(at -20.32 0 0)
				(length 3.81)
				(name "~{XIRQ}")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 3.81)
				(name "MODA")
				(number "3")
			)
			(pin input line
				(at -20.32 -5.08 0)
				(length 3.81)
				(name "MODB")
				(number "2")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "PE0")
				(number "43")
			)
			(pin input line
				(at -20.32 -20.32 0)
				(length 3.81)
				(name "PE1")
				(number "45")
			)
			(pin input line
				(at -20.32 -22.86 0)
				(length 3.81)
				(name "PE2")
				(number "47")
			)
			(pin input line
				(at -20.32 -25.4 0)
				(length 3.81)
				(name "PE3")
				(number "49")
			)
			(pin input line
				(at -20.32 -27.94 0)
				(length 3.81)
				(name "PE4")
				(number "44")
			)
			(pin input line
				(at -20.32 -30.48 0)
				(length 3.81)
				(name "PE5")
				(number "46")
			)
			(pin input line
				(at -20.32 -33.02 0)
				(length 3.81)
				(name "PE6")
				(number "48")
			)
			(pin input line
				(at -20.32 -35.56 0)
				(length 3.81)
				(name "PE7")
				(number "50")
			)
			(pin input line
				(at -20.32 -40.64 0)
				(length 3.81)
				(name "VRH")
				(number "52")
			)
			(pin input line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "VRL")
				(number "51")
			)
			(pin power_in line
				(at 0 53.34 270)
				(length 3.81)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 3.81)
				(name "VSS")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "RXD/PD0")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "TXD/PD1")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "MIS/PD2")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "MOS/PD3")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "SCK/PD4")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "SS/PD5")
				(number "25")
			)
			(pin input line
				(at 20.32 27.94 180)
				(length 3.81)
				(name "PA0")
				(number "34")
			)
			(pin input line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "PA1")
				(number "33")
			)
			(pin input line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "PA2")
				(number "32")
			)
			(pin output line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "PA3")
				(number "31")
			)
			(pin output line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "PA4")
				(number "30")
			)
			(pin output line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "PA5")
				(number "29")
			)
			(pin output line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "PA6")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "PA7")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 3.81)
				(name "AD0/PC0")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "AD1/PC1")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 3.81)
				(name "AD2/PC2")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "AD3/PC3")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "AD4/PC4")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "AD5/PC5")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "AD6/PC6")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "AD7/PC7")
				(number "16")
			)
			(pin output line
				(at 20.32 -17.78 180)
				(length 3.81)
				(name "A8/PB0")
				(number "42")
			)
			(pin output line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "A9/PB1")
				(number "41")
			)
			(pin output line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "A10/PB2")
				(number "40")
			)
			(pin output line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "A11/PB3")
				(number "39")
			)
			(pin output line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "A12/PB4")
				(number "38")
			)
			(pin output line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "A13/PB5")
				(number "37")
			)
			(pin output line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "A14/PB6")
				(number "36")
			)
			(pin output line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "A15/PB7")
				(number "35")
			)
			(pin output line
				(at 20.32 -40.64 180)
				(length 3.81)
				(name "R/W")
				(number "6")
			)
			(pin output line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "E")
				(number "5")
			)
			(pin output line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "AS")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC68HC11F1CC"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -16.51 71.12 0)
		)
		(property "Value" "MC68HC11F1CC"
			(at 1.27 71.12 0)
		)
		(property "Footprint" "Package_LCC:PLCC-68"
			(at 15.24 -77.47 0)
		)
		(property "Datasheet" "http://cache.freescale.com/files/microcontrollers/doc/data_sheet/MC68HC11F1.pdf"
			(at 0 0 0)
		)
		(property "Description" "ROMless, 1K RAM, 512B EEPROM, PLCC-68"
			(at 0 0 0)
		)
		(property "ki_keywords" "HC11 MCU Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "PLCC*"
			(at 0 0 0)
		)
		(symbol "MC68HC11F1CC_0_1")
		(symbol "MC68HC11F1CC_1_1"
			(pin output line
				(at -20.32 60.96 0)
				(length 3.81)
				(name "EXTAL")
				(number "6")
			)
			(pin input line
				(at -20.32 55.88 0)
				(length 3.81)
				(name "XTAL")
				(number "7")
			)
			(pin input line
				(at -20.32 22.86 0)
				(length 3.81)
				(name "~{RESET}")
				(number "17")
			)
			(pin input line
				(at -20.32 -10.16 0)
				(length 3.81)
				(name "~{IRQ}")
				(number "19")
			)
			(pin input line
				(at -20.32 -12.7 0)
				(length 3.81)
				(name "~{XIRQ}")
				(number "18")
			)
			(pin bidirectional line
				(at -20.32 -15.24 0)
				(length 3.81)
				(name "MODA")
				(number "3")
			)
			(pin input line
				(at -20.32 -17.78 0)
				(length 3.81)
				(name "MODB")
				(number "2")
			)
			(pin input line
				(at -20.32 -43.18 0)
				(length 3.81)
				(name "PE0")
				(number "59")
			)
			(pin input line
				(at -20.32 -45.72 0)
				(length 3.81)
				(name "PE1")
				(number "61")
			)
			(pin input line
				(at -20.32 -48.26 0)
				(length 3.81)
				(name "PE2")
				(number "63")
			)
			(pin input line
				(at -20.32 -50.8 0)
				(length 3.81)
				(name "PE3")
				(number "65")
			)
			(pin input line
				(at -20.32 -53.34 0)
				(length 3.81)
				(name "PE4")
				(number "60")
			)
			(pin input line
				(at -20.32 -55.88 0)
				(length 3.81)
				(name "PE5")
				(number "62")
			)
			(pin input line
				(at -20.32 -58.42 0)
				(length 3.81)
				(name "PE6")
				(number "64")
			)
			(pin input line
				(at -20.32 -60.96 0)
				(length 3.81)
				(name "PE7")
				(number "66")
			)
			(pin input line
				(at -20.32 -66.04 0)
				(length 3.81)
				(name "VRH")
				(number "68")
			)
			(pin input line
				(at -20.32 -71.12 0)
				(length 3.81)
				(name "VRL")
				(number "67")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 3.81)
				(name "VDD")
				(number "34")
			)
			(pin power_in line
				(at 0 -78.74 90)
				(length 3.81)
				(name "VSS")
				(number "1")
			)
			(pin bidirectional line
				(at 20.32 66.04 180)
				(length 3.81)
				(name "RXD/PD0")
				(number "28")
			)
			(pin bidirectional line
				(at 20.32 63.5 180)
				(length 3.81)
				(name "TXD/PD1")
				(number "29")
			)
			(pin bidirectional line
				(at 20.32 60.96 180)
				(length 3.81)
				(name "MIS/PD2")
				(number "30")
			)
			(pin bidirectional line
				(at 20.32 58.42 180)
				(length 3.81)
				(name "MOS/PD3")
				(number "31")
			)
			(pin bidirectional line
				(at 20.32 55.88 180)
				(length 3.81)
				(name "SCK/PD4")
				(number "32")
			)
			(pin bidirectional line
				(at 20.32 53.34 180)
				(length 3.81)
				(name "SS/PD5")
				(number "33")
			)
			(pin bidirectional line
				(at 20.32 48.26 180)
				(length 3.81)
				(name "PA0")
				(number "42")
			)
			(pin bidirectional line
				(at 20.32 45.72 180)
				(length 3.81)
				(name "PA1")
				(number "41")
			)
			(pin bidirectional line
				(at 20.32 43.18 180)
				(length 3.81)
				(name "PA2")
				(number "40")
			)
			(pin bidirectional line
				(at 20.32 40.64 180)
				(length 3.81)
				(name "PA3")
				(number "39")
			)
			(pin bidirectional line
				(at 20.32 38.1 180)
				(length 3.81)
				(name "PA4")
				(number "38")
			)
			(pin bidirectional line
				(at 20.32 35.56 180)
				(length 3.81)
				(name "PA5")
				(number "37")
			)
			(pin bidirectional line
				(at 20.32 33.02 180)
				(length 3.81)
				(name "PA6")
				(number "36")
			)
			(pin bidirectional line
				(at 20.32 30.48 180)
				(length 3.81)
				(name "PA7")
				(number "35")
			)
			(pin bidirectional line
				(at 20.32 25.4 180)
				(length 3.81)
				(name "D0/PC0")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 22.86 180)
				(length 3.81)
				(name "D1/PC1")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 20.32 180)
				(length 3.81)
				(name "D2/PC2")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 17.78 180)
				(length 3.81)
				(name "D3/PC3")
				(number "12")
			)
			(pin bidirectional line
				(at 20.32 15.24 180)
				(length 3.81)
				(name "D4/PC4")
				(number "13")
			)
			(pin bidirectional line
				(at 20.32 12.7 180)
				(length 3.81)
				(name "D5/PC5")
				(number "14")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 3.81)
				(name "D6/PC6")
				(number "15")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 3.81)
				(name "D7/PC7")
				(number "16")
			)
			(pin output line
				(at 20.32 2.54 180)
				(length 3.81)
				(name "A0/PF0")
				(number "58")
			)
			(pin output line
				(at 20.32 0 180)
				(length 3.81)
				(name "A1/PF1")
				(number "57")
			)
			(pin output line
				(at 20.32 -2.54 180)
				(length 3.81)
				(name "A2/PF2")
				(number "56")
			)
			(pin output line
				(at 20.32 -5.08 180)
				(length 3.81)
				(name "A3/PF3")
				(number "55")
			)
			(pin output line
				(at 20.32 -7.62 180)
				(length 3.81)
				(name "A4/PF4")
				(number "54")
			)
			(pin output line
				(at 20.32 -10.16 180)
				(length 3.81)
				(name "A5/PF5")
				(number "53")
			)
			(pin output line
				(at 20.32 -12.7 180)
				(length 3.81)
				(name "A6/PF6")
				(number "52")
			)
			(pin output line
				(at 20.32 -15.24 180)
				(length 3.81)
				(name "A7/PF7")
				(number "51")
			)
			(pin output line
				(at 20.32 -20.32 180)
				(length 3.81)
				(name "A8/PB0")
				(number "50")
			)
			(pin output line
				(at 20.32 -22.86 180)
				(length 3.81)
				(name "A9/PB1")
				(number "49")
			)
			(pin output line
				(at 20.32 -25.4 180)
				(length 3.81)
				(name "A10/PB2")
				(number "48")
			)
			(pin output line
				(at 20.32 -27.94 180)
				(length 3.81)
				(name "A11/PB3")
				(number "47")
			)
			(pin output line
				(at 20.32 -30.48 180)
				(length 3.81)
				(name "A12/PB4")
				(number "46")
			)
			(pin output line
				(at 20.32 -33.02 180)
				(length 3.81)
				(name "A13/PB5")
				(number "45")
			)
			(pin output line
				(at 20.32 -35.56 180)
				(length 3.81)
				(name "A14/PB6")
				(number "44")
			)
			(pin output line
				(at 20.32 -38.1 180)
				(length 3.81)
				(name "A15/PB7")
				(number "43")
			)
			(pin bidirectional line
				(at 20.32 -43.18 180)
				(length 3.81)
				(name "PG0")
				(number "27")
			)
			(pin bidirectional line
				(at 20.32 -45.72 180)
				(length 3.81)
				(name "PG1")
				(number "26")
			)
			(pin bidirectional line
				(at 20.32 -48.26 180)
				(length 3.81)
				(name "PG2")
				(number "25")
			)
			(pin bidirectional line
				(at 20.32 -50.8 180)
				(length 3.81)
				(name "PG3")
				(number "24")
			)
			(pin bidirectional line
				(at 20.32 -53.34 180)
				(length 3.81)
				(name "CSIO2/PG4")
				(number "23")
			)
			(pin bidirectional line
				(at 20.32 -55.88 180)
				(length 3.81)
				(name "CSIO1/PG5")
				(number "22")
			)
			(pin bidirectional line
				(at 20.32 -58.42 180)
				(length 3.81)
				(name "CSGEN/PG6")
				(number "21")
			)
			(pin bidirectional line
				(at 20.32 -60.96 180)
				(length 3.81)
				(name "CSPROG/PG7")
				(number "20")
			)
			(pin output line
				(at 20.32 -66.04 180)
				(length 3.81)
				(name "R/W")
				(number "5")
			)
			(pin output line
				(at 20.32 -68.58 180)
				(length 3.81)
				(name "E")
				(number "4")
			)
			(pin output line
				(at 20.32 -71.12 180)
				(length 3.81)
				(name "4XOUT")
				(number "8")
			)
		)
		(embedded_fonts no)
	)
	(symbol "68HC11A8"
		(extends "68HC11")
		(property "Reference" "U"
			(at 5.08 45.72 0)
		)
		(property "Value" "68HC11A8"
			(at 8.89 -45.72 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "HC11 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_keywords" "MCU Microcontroller HC11"
			(at 0 0 0)
		)
	)
	(symbol "MC68HC11A0CC"
		(extends "MC68HC11A8CC")
		(property "Reference" "U"
			(at -16.51 50.8 0)
		)
		(property "Value" "MC68HC11A0CC"
			(at 1.27 50.8 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" ""
			(at 0 -5.08 0)
		)
		(property "Description" "ROMless, 256B RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "HC11 MCU Microcotroller"
			(at 0 0 0)
		)
	)
	(symbol "MC68HC11A1CC"
		(extends "MC68HC11A8CC")
		(property "Reference" "U"
			(at -16.51 50.8 0)
		)
		(property "Value" "MC68HC11A1CC"
			(at 1.27 50.8 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" ""
			(at 0 -5.08 0)
		)
		(property "Description" "ROMLess, 256B RAM, 512B EEPROM"
			(at 0 0 0)
		)
		(property "ki_keywords" "HC11 MCU Microcotroller"
			(at 0 0 0)
		)
	)
	(symbol "MC68HC11A7CC"
		(extends "MC68HC11A8CC")
		(property "Reference" "U"
			(at -16.51 50.8 0)
		)
		(property "Value" "MC68HC11A7CC"
			(at 1.27 50.8 0)
		)
		(property "Footprint" ""
			(at 0 -5.08 0)
		)
		(property "Datasheet" ""
			(at 0 -5.08 0)
		)
		(property "Description" "8K ROM, 256B RAM, 512B EEPROM"
			(at 0 0 0)
		)
		(property "ki_keywords" "HC11 MCU Microcotroller"
			(at 0 0 0)
		)
	)
)
