(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "MC68HC812A4"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 16.51 86.36 0)
		)
		(property "Value" "MC68HC812A4"
			(at 19.05 -73.66 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" ""
			(at 0 0 0)
		)
		(property "Description" "HC12 Microcontroller 112 pins"
			(at 0 0 0)
		)
		(property "ki_keywords" "68HC12 Microcontroller"
			(at 0 0 0)
		)
		(symbol "MC68HC812A4_0_1")
		(symbol "MC68HC812A4_1_1"
			(pin bidirectional line
				(at -35.56 81.28 0)
				(length 7.62)
				(name "PD0/D0/KWUD0")
				(number "20")
			)
			(pin bidirectional line
				(at -35.56 78.74 0)
				(length 7.62)
				(name "PD1/D1/KWUD1")
				(number "21")
			)
			(pin bidirectional line
				(at -35.56 76.2 0)
				(length 7.62)
				(name "PD2/D2/KWUD2")
				(number "22")
			)
			(pin bidirectional line
				(at -35.56 73.66 0)
				(length 7.62)
				(name "PD3/D3/KWUD3")
				(number "23")
			)
			(pin bidirectional line
				(at -35.56 71.12 0)
				(length 7.62)
				(name "PD4/D4/KWUD4")
				(number "24")
			)
			(pin bidirectional line
				(at -35.56 68.58 0)
				(length 7.62)
				(name "PD5/D5/KWUD5")
				(number "25")
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 7.62)
				(name "PD6/D6/KWUD6")
				(number "26")
			)
			(pin bidirectional line
				(at -35.56 63.5 0)
				(length 7.62)
				(name "PD7/D7/KWUD7")
				(number "27")
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 7.62)
				(name "PC0/D8/D0")
				(number "28")
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 7.62)
				(name "PC1/D9/D1")
				(number "29")
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 7.62)
				(name "PC2/D10/D2")
				(number "30")
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 7.62)
				(name "PC3/D11/D3")
				(number "31")
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 7.62)
				(name "PC4/D12/D4")
				(number "32")
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 7.62)
				(name "PC5/D13/D5")
				(number "33")
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 7.62)
				(name "PC6/D14/D6")
				(number "34")
			)
			(pin bidirectional line
				(at -35.56 40.64 0)
				(length 7.62)
				(name "PC7/D15/D7")
				(number "35")
			)
			(pin input line
				(at -35.56 35.56 0)
				(length 7.62)
				(name "PE0/XIRQ")
				(number "36")
			)
			(pin input line
				(at -35.56 33.02 0)
				(length 7.62)
				(name "PE1/IRQ")
				(number "37")
			)
			(pin bidirectional line
				(at -35.56 30.48 0)
				(length 7.62)
				(name "PE2/RW")
				(number "38")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 7.62)
				(name "PE3/LSTRB/TAGL0")
				(number "39")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 7.62)
				(name "PE4/ECLK")
				(number "48")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 7.62)
				(name "PE5/MODA/IPIPE0")
				(number "49")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 7.62)
				(name "PE6/MODB/IPIPE1")
				(number "50")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 7.62)
				(name "PE7/ARST")
				(number "51")
			)
			(pin input line
				(at -35.56 12.7 0)
				(length 7.62)
				(name "EXTAL")
				(number "46")
			)
			(pin output line
				(at -35.56 10.16 0)
				(length 7.62)
				(name "XTAL")
				(number "47")
			)
			(pin bidirectional inverted
				(at -35.56 5.08 0)
				(length 7.62)
				(name "RESET")
				(number "40")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 7.62)
				(name "BKGD/TAGHI")
				(number "19")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 7.62)
				(name "PS0/RXD0")
				(number "97")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 7.62)
				(name "PS1/TXD0")
				(number "98")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 7.62)
				(name "PS2/RXD1")
				(number "99")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 7.62)
				(name "PS3/TXD1")
				(number "100")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 7.62)
				(name "PS4/SDI/MISO")
				(number "101")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 7.62)
				(name "PS5/SDO/MOSI")
				(number "102")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 7.62)
				(name "PS6/SCK")
				(number "103")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 7.62)
				(name "PS7/SS")
				(number "104")
			)
			(pin bidirectional line
				(at -35.56 -25.4 0)
				(length 7.62)
				(name "PT0/IOC0")
				(number "105")
			)
			(pin bidirectional line
				(at -35.56 -27.94 0)
				(length 7.62)
				(name "PT1/IOC1")
				(number "106")
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 7.62)
				(name "PT2/IOC2")
				(number "107")
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 7.62)
				(name "PT3/IOC3")
				(number "108")
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 7.62)
				(name "PT4/IOC4")
				(number "109")
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 7.62)
				(name "PT5/IOC5")
				(number "110")
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 7.62)
				(name "PT6/IOC6")
				(number "111")
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 7.62)
				(name "PT7/IOC7/PAI")
				(number "112")
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 7.62)
				(name "PF0/CS0")
				(number "68")
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 7.62)
				(name "PF1/CS1")
				(number "69")
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 7.62)
				(name "PF2/CS2")
				(number "70")
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 7.62)
				(name "PF3/CS3")
				(number "71")
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 7.62)
				(name "PF4/CSD")
				(number "72")
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 7.62)
				(name "PF5/CSP0")
				(number "73")
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 7.62)
				(name "PF6/CSP1")
				(number "74")
			)
			(pin power_in line
				(at -5.08 91.44 270)
				(length 7.62)
				(name "VDDX")
				(number "2")
			)
			(pin power_in line
				(at -5.08 -78.74 90)
				(length 7.62)
				(name "VSSX")
				(number "80")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 7.62)
				(name "VDDX")
				(number "42")
			)
			(pin power_in line
				(at -2.54 -78.74 90)
				(length 7.62)
				(name "VSSX")
				(number "1")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 7.62)
				(name "VDDX")
				(number "79")
			)
			(pin power_in line
				(at 0 -78.74 90)
				(length 7.62)
				(name "VSSX")
				(number "41")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 7.62)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -78.74 90)
				(length 7.62)
				(name "VSS")
				(number "15")
			)
			(pin bidirectional line
				(at 35.56 81.28 180)
				(length 7.62)
				(name "PB0/A0")
				(number "52")
			)
			(pin bidirectional line
				(at 35.56 78.74 180)
				(length 7.62)
				(name "PB1/A1")
				(number "53")
			)
			(pin bidirectional line
				(at 35.56 76.2 180)
				(length 7.62)
				(name "PB2/A2")
				(number "54")
			)
			(pin bidirectional line
				(at 35.56 73.66 180)
				(length 7.62)
				(name "PB3/A3")
				(number "55")
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 7.62)
				(name "PB4/A4")
				(number "56")
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 7.62)
				(name "PB5/A5")
				(number "57")
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 7.62)
				(name "PB6/A6")
				(number "58")
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 7.62)
				(name "PB7/A7")
				(number "59")
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 7.62)
				(name "PA0/A8")
				(number "60")
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 7.62)
				(name "PA1/A9")
				(number "61")
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 7.62)
				(name "PA2/A10")
				(number "62")
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 7.62)
				(name "PA3/A11")
				(number "63")
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 7.62)
				(name "PA4/A12")
				(number "64")
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 7.62)
				(name "PA5/A13")
				(number "65")
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 7.62)
				(name "PA6/A14")
				(number "66")
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 7.62)
				(name "PA7/A15")
				(number "67")
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 7.62)
				(name "PG0/A16")
				(number "11")
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 7.62)
				(name "PG1/A17")
				(number "12")
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 7.62)
				(name "PG2/A18")
				(number "13")
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 7.62)
				(name "PG3/A19")
				(number "16")
			)
			(pin bidirectional line
				(at 35.56 30.48 180)
				(length 7.62)
				(name "PG4/A20")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 7.62)
				(name "PG5/A21")
				(number "18")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 7.62)
				(name "PH0/KWUH0")
				(number "75")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 7.62)
				(name "PH1/KWUH1")
				(number "76")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 7.62)
				(name "PH2/KWUH2")
				(number "77")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 7.62)
				(name "PH3/KWUH3")
				(number "78")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 7.62)
				(name "PH4/KWUH4")
				(number "81")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 7.62)
				(name "PH5/KWUH5")
				(number "82")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 7.62)
				(name "PH6/KWUH6")
				(number "83")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 7.62)
				(name "PH7/KWUH7")
				(number "84")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 7.62)
				(name "PJ0/KWUJ0")
				(number "3")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 7.62)
				(name "PJ1/KWUJ1")
				(number "4")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 7.62)
				(name "PJ2/KWUJ2")
				(number "5")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 7.62)
				(name "PJ3/KWUJ3")
				(number "6")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 7.62)
				(name "PJ4/KWUJ4")
				(number "7")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 7.62)
				(name "PJ5/KWUJ5")
				(number "8")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 7.62)
				(name "PJ6/KWUJ6")
				(number "9")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 7.62)
				(name "PJ7/KWUJ7")
				(number "10")
			)
			(pin input line
				(at 35.56 -22.86 180)
				(length 7.62)
				(name "PAD0")
				(number "87")
			)
			(pin input line
				(at 35.56 -25.4 180)
				(length 7.62)
				(name "PAD1")
				(number "88")
			)
			(pin input line
				(at 35.56 -27.94 180)
				(length 7.62)
				(name "PAD2")
				(number "89")
			)
			(pin input line
				(at 35.56 -30.48 180)
				(length 7.62)
				(name "PAD3")
				(number "90")
			)
			(pin input line
				(at 35.56 -33.02 180)
				(length 7.62)
				(name "PAD4")
				(number "91")
			)
			(pin input line
				(at 35.56 -35.56 180)
				(length 7.62)
				(name "PAD5")
				(number "92")
			)
			(pin input line
				(at 35.56 -38.1 180)
				(length 7.62)
				(name "PAD6")
				(number "93")
			)
			(pin input line
				(at 35.56 -40.64 180)
				(length 7.62)
				(name "VSTBY/PAD7")
				(number "94")
			)
			(pin input line
				(at 35.56 -48.26 180)
				(length 7.62)
				(name "VDDAD")
				(number "95")
			)
			(pin input line
				(at 35.56 -50.8 180)
				(length 7.62)
				(name "VSSAD")
				(number "96")
			)
			(pin input line
				(at 35.56 -55.88 180)
				(length 7.62)
				(name "VRH")
				(number "85")
			)
			(pin input line
				(at 35.56 -58.42 180)
				(length 7.62)
				(name "VRL")
				(number "86")
			)
			(pin input line
				(at 35.56 -63.5 180)
				(length 7.62)
				(name "VDDPLL")
				(number "43")
			)
			(pin passive line
				(at 35.56 -66.04 180)
				(length 7.62)
				(name "XFC")
				(number "44")
			)
			(pin input line
				(at 35.56 -68.58 180)
				(length 7.62)
				(name "VSSPLL")
				(number "45")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC68HC912"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 8.89 67.31 0)
		)
		(property "Value" "MC68HC912"
			(at 7.62 -62.23 0)
		)
		(property "Footprint" ""
			(at 0 2.54 0)
		)
		(property "Datasheet" ""
			(at 0 2.54 0)
		)
		(property "Description" "HC12 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_keywords" "68HC12 Microcontroller"
			(at 0 0 0)
		)
		(symbol "MC68HC912_0_1")
		(symbol "MC68HC912_1_1"
			(pin input line
				(at -27.94 60.96 0)
				(length 7.62)
				(name "VFP")
				(number "69")
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 7.62)
				(name "BKGD/SMODN/TAGHI")
				(number "17")
			)
			(pin input line
				(at -27.94 53.34 0)
				(length 7.62)
				(name "EXTAL")
				(number "33")
			)
			(pin output line
				(at -27.94 48.26 0)
				(length 7.62)
				(name "XTAL")
				(number "34")
			)
			(pin bidirectional input_low
				(at -27.94 43.18 0)
				(length 7.62)
				(name "RST")
				(number "32")
			)
			(pin input line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "PE0/XIRQ")
				(number "38")
			)
			(pin input line
				(at -27.94 35.56 0)
				(length 7.62)
				(name "PE1/IRQ")
				(number "37")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "PE2-R/W")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 7.62)
				(name "PE3/LSTRB/TAGLO")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 7.62)
				(name "PE4-ECLK")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "PE5-MODA/IPIPE0")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 7.62)
				(name "PE6-MODB/IPIPE1")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 7.62)
				(name "PE7/DBE")
				(number "26")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 7.62)
				(name "PA0/AD8")
				(number "39")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 7.62)
				(name "PA1/D9/A9")
				(number "40")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 7.62)
				(name "PA2/AD10")
				(number "41")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 7.62)
				(name "PA3/AD11")
				(number "42")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 7.62)
				(name "PA4/AD12")
				(number "43")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 7.62)
				(name "PA5/AD13")
				(number "44")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 7.62)
				(name "PA6/AD14")
				(number "45")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "PA7/AD15")
				(number "46")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 7.62)
				(name "PB0/AD0")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "PB1/AD1")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 7.62)
				(name "PB2/AD2")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "PB3/AD3")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "PB4/AD4")
				(number "22")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 7.62)
				(name "PB5/AD5")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 7.62)
				(name "PB6/AD6")
				(number "24")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "PB7/AD7")
				(number "25")
			)
			(pin power_in line
				(at -5.08 73.66 270)
				(length 7.62)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at -5.08 -68.58 90)
				(length 7.62)
				(name "VSS")
				(number "11")
			)
			(pin power_in line
				(at -2.54 73.66 270)
				(length 7.62)
				(name "VDD")
				(number "47")
			)
			(pin power_in line
				(at -2.54 -68.58 90)
				(length 7.62)
				(name "VSS")
				(number "48")
			)
			(pin power_in line
				(at 0 73.66 270)
				(length 7.62)
				(name "VDDX")
				(number "31")
			)
			(pin power_in line
				(at 0 -68.58 90)
				(length 7.62)
				(name "VSSX")
				(number "30")
			)
			(pin power_in line
				(at 2.54 73.66 270)
				(length 7.62)
				(name "VDDX")
				(number "78")
			)
			(pin power_in line
				(at 2.54 -68.58 90)
				(length 7.62)
				(name "VSSX")
				(number "77")
			)
			(pin input line
				(at 27.94 63.5 180)
				(length 7.62)
				(name "VRH")
				(number "49")
			)
			(pin input line
				(at 27.94 60.96 180)
				(length 7.62)
				(name "VRL")
				(number "50")
			)
			(pin input line
				(at 27.94 58.42 180)
				(length 7.62)
				(name "VDDA")
				(number "59")
			)
			(pin input line
				(at 27.94 55.88 180)
				(length 7.62)
				(name "VSSA")
				(number "60")
			)
			(pin input line
				(at 27.94 50.8 180)
				(length 7.62)
				(name "PAD0")
				(number "51")
			)
			(pin input line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "PAD1")
				(number "52")
			)
			(pin input line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "PAD2")
				(number "53")
			)
			(pin input line
				(at 27.94 43.18 180)
				(length 7.62)
				(name "PAD3")
				(number "54")
			)
			(pin input line
				(at 27.94 40.64 180)
				(length 7.62)
				(name "PAD4")
				(number "55")
			)
			(pin input line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "PAD5")
				(number "56")
			)
			(pin input line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "PAD6")
				(number "57")
			)
			(pin input line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "PAD7")
				(number "58")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "PT0-IOC0")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "PT1-IOC1")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 7.62)
				(name "PT2-IOC2")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "PT3-IOC3")
				(number "12")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 7.62)
				(name "PT4-IOC4")
				(number "13")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "PT5-IOC5")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "PT6-IOC6")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "PT7-IOC7-PAI")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "PS0/RxD")
				(number "61")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "PS1/TxD")
				(number "62")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 7.62)
				(name "PS2")
				(number "63")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "PS3")
				(number "64")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 7.62)
				(name "PS4SDI/MISO")
				(number "65")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "PS5/SD0/MOSI")
				(number "66")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "PS6/SCLK")
				(number "67")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 7.62)
				(name "PS7/CS/SS")
				(number "68")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "PP0/PW0")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "PP1/PW1")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 7.62)
				(name "PP2/PW3")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 7.62)
				(name "PP3/PW3")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 7.62)
				(name "PP4")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "PP5")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "PP6")
				(number "80")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "PP7")
				(number "79")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 7.62)
				(name "PDLC0/DLCRx")
				(number "76")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "PDLC1/DLCTx")
				(number "75")
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "PDLC2")
				(number "74")
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "PDLC3")
				(number "73")
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 7.62)
				(name "PDLC4")
				(number "72")
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 7.62)
				(name "PDLC5")
				(number "71")
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 7.62)
				(name "PDLC6")
				(number "70")
			)
		)
		(embedded_fonts no)
	)
)
