(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "MC9S12DT256"
		(pin_names
			(offset 0.762)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 17.78 86.36 0)
		)
		(property "Value" "MC9S12DT256"
			(at 20.32 -73.66 0)
		)
		(property "Footprint" ""
			(at 1.27 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/fact-sheet/MC9S12DT256FS.pdf"
			(at 1.27 0 0)
		)
		(property "Description" "HCS12 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_keywords" "HCS12 MCU"
			(at 0 0 0)
		)
		(symbol "MC9S12DT256_0_1")
		(symbol "MC9S12DT256_1_1"
			(pin input line
				(at -43.18 81.28 0)
				(length 7.62)
				(name "EXTAL")
				(number "46")
			)
			(pin output line
				(at -43.18 78.74 0)
				(length 7.62)
				(name "XTAL")
				(number "47")
			)
			(pin bidirectional line
				(at -43.18 73.66 0)
				(length 7.62)
				(name "BKGD/TAGHI/MODC")
				(number "23")
			)
			(pin bidirectional line
				(at -43.18 68.58 0)
				(length 7.62)
				(name "RESET")
				(number "42")
			)
			(pin bidirectional line
				(at -43.18 63.5 0)
				(length 7.62)
				(name "XFC")
				(number "44")
			)
			(pin power_in line
				(at -43.18 60.96 0)
				(length 7.62)
				(name "VDDPLL")
				(number "43")
			)
			(pin bidirectional line
				(at -43.18 58.42 0)
				(length 7.62)
				(name "VSSPLL")
				(number "45")
			)
			(pin input line
				(at -43.18 53.34 0)
				(length 7.62)
				(name "PE0/XIRQ")
				(number "56")
			)
			(pin input line
				(at -43.18 50.8 0)
				(length 7.62)
				(name "PE1/IRQ")
				(number "55")
			)
			(pin bidirectional line
				(at -43.18 48.26 0)
				(length 7.62)
				(name "PE2/RW")
				(number "54")
			)
			(pin bidirectional line
				(at -43.18 45.72 0)
				(length 7.62)
				(name "PE3/TAGLO/LSTRB")
				(number "53")
			)
			(pin bidirectional line
				(at -43.18 43.18 0)
				(length 7.62)
				(name "PE4/ECLK")
				(number "39")
			)
			(pin bidirectional line
				(at -43.18 40.64 0)
				(length 7.62)
				(name "PE5/MODA")
				(number "38")
			)
			(pin bidirectional line
				(at -43.18 38.1 0)
				(length 7.62)
				(name "PE6/MODB")
				(number "37")
			)
			(pin bidirectional line
				(at -43.18 35.56 0)
				(length 7.62)
				(name "PE7/NOACC/XCLKS")
				(number "36")
			)
			(pin input line
				(at -43.18 30.48 0)
				(length 7.62)
				(name "TEST")
				(number "48")
			)
			(pin bidirectional line
				(at -43.18 25.4 0)
				(length 7.62)
				(name "PT0/IOC0")
				(number "9")
			)
			(pin bidirectional line
				(at -43.18 22.86 0)
				(length 7.62)
				(name "PT1/IOC1")
				(number "10")
			)
			(pin bidirectional line
				(at -43.18 20.32 0)
				(length 7.62)
				(name "PT2/IOC2")
				(number "11")
			)
			(pin bidirectional line
				(at -43.18 17.78 0)
				(length 7.62)
				(name "PT3/IOC3")
				(number "12")
			)
			(pin bidirectional line
				(at -43.18 15.24 0)
				(length 7.62)
				(name "PT4/IOC4")
				(number "15")
			)
			(pin bidirectional line
				(at -43.18 12.7 0)
				(length 7.62)
				(name "PT5/IOC5")
				(number "16")
			)
			(pin bidirectional line
				(at -43.18 10.16 0)
				(length 7.62)
				(name "PT6/IOC6")
				(number "17")
			)
			(pin bidirectional line
				(at -43.18 7.62 0)
				(length 7.62)
				(name "PT7/IOC7")
				(number "18")
			)
			(pin passive line
				(at -43.18 2.54 0)
				(length 7.62)
				(name "VRH")
				(number "84")
			)
			(pin passive line
				(at -43.18 0 0)
				(length 7.62)
				(name "VRL")
				(number "85")
			)
			(pin input line
				(at -43.18 -5.08 0)
				(length 7.62)
				(name "PAD00/AN00")
				(number "67")
			)
			(pin input line
				(at -43.18 -7.62 0)
				(length 7.62)
				(name "PAD08/AN08")
				(number "68")
			)
			(pin input line
				(at -43.18 -10.16 0)
				(length 7.62)
				(name "PAD01/AN01")
				(number "69")
			)
			(pin input line
				(at -43.18 -12.7 0)
				(length 7.62)
				(name "PAD09/AN09")
				(number "70")
			)
			(pin input line
				(at -43.18 -15.24 0)
				(length 7.62)
				(name "PAD02/AN02")
				(number "71")
			)
			(pin input line
				(at -43.18 -17.78 0)
				(length 7.62)
				(name "PAD10/AN10")
				(number "72")
			)
			(pin input line
				(at -43.18 -20.32 0)
				(length 7.62)
				(name "PAD03/AN03")
				(number "73")
			)
			(pin input line
				(at -43.18 -22.86 0)
				(length 7.62)
				(name "PAD11/AN11")
				(number "74")
			)
			(pin input line
				(at -43.18 -25.4 0)
				(length 7.62)
				(name "PAD04/AN04")
				(number "75")
			)
			(pin input line
				(at -43.18 -27.94 0)
				(length 7.62)
				(name "PAD12/AN12")
				(number "76")
			)
			(pin input line
				(at -43.18 -30.48 0)
				(length 7.62)
				(name "PAD05/AN05")
				(number "77")
			)
			(pin input line
				(at -43.18 -33.02 0)
				(length 7.62)
				(name "PAD13/AN13")
				(number "78")
			)
			(pin input line
				(at -43.18 -35.56 0)
				(length 7.62)
				(name "PAD06/AN06")
				(number "79")
			)
			(pin input line
				(at -43.18 -38.1 0)
				(length 7.62)
				(name "PAD14/AN14")
				(number "80")
			)
			(pin input line
				(at -43.18 -40.64 0)
				(length 7.62)
				(name "PAD07/AN07/ETRIG0")
				(number "81")
			)
			(pin input line
				(at -43.18 -43.18 0)
				(length 7.62)
				(name "PAD15/AN15/ETRIG1")
				(number "82")
			)
			(pin bidirectional line
				(at -43.18 -48.26 0)
				(length 7.62)
				(name "PH0/KWH0/MISO1")
				(number "52")
			)
			(pin bidirectional line
				(at -43.18 -50.8 0)
				(length 7.62)
				(name "PH1/KWH1/MOSI1")
				(number "51")
			)
			(pin bidirectional line
				(at -43.18 -53.34 0)
				(length 7.62)
				(name "PH2/KWH2/SCK1")
				(number "50")
			)
			(pin bidirectional line
				(at -43.18 -55.88 0)
				(length 7.62)
				(name "PH3/KWH3/SS1")
				(number "49")
			)
			(pin bidirectional line
				(at -43.18 -58.42 0)
				(length 7.62)
				(name "PH4/KWH4")
				(number "35")
			)
			(pin bidirectional line
				(at -43.18 -60.96 0)
				(length 7.62)
				(name "PH5/KWH5")
				(number "34")
			)
			(pin bidirectional line
				(at -43.18 -63.5 0)
				(length 7.62)
				(name "PH6/KWH6")
				(number "33")
			)
			(pin bidirectional line
				(at -43.18 -66.04 0)
				(length 7.62)
				(name "PH7/KWH7")
				(number "32")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 7.62)
				(name "VDDR")
				(number "41")
			)
			(pin power_in line
				(at -5.08 91.44 270)
				(length 7.62)
				(name "VDDX")
				(number "107")
			)
			(pin power_in line
				(at -5.08 -78.74 90)
				(length 7.62)
				(name "VSSR")
				(number "40")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 7.62)
				(name "VDDA")
				(number "83")
			)
			(pin power_in line
				(at -2.54 -78.74 90)
				(length 7.62)
				(name "VSSX")
				(number "106")
			)
			(pin power_in line
				(at 0 91.44 270)
				(length 7.62)
				(name "VDD2")
				(number "65")
			)
			(pin power_in line
				(at 0 -78.74 90)
				(length 7.62)
				(name "VSSA")
				(number "86")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 7.62)
				(name "VDD1")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -78.74 90)
				(length 7.62)
				(name "VSS2")
				(number "66")
			)
			(pin power_in line
				(at 5.08 -78.74 90)
				(length 7.62)
				(name "VSS1")
				(number "14")
			)
			(pin input line
				(at 7.62 91.44 270)
				(length 7.62)
				(name "VREGEN")
				(number "97")
			)
			(pin bidirectional line
				(at 45.72 81.28 180)
				(length 7.62)
				(name "ADDR0/DATA0/PB0")
				(number "24")
			)
			(pin bidirectional line
				(at 45.72 78.74 180)
				(length 7.62)
				(name "ADDR1/DATA1/PB1")
				(number "25")
			)
			(pin bidirectional line
				(at 45.72 76.2 180)
				(length 7.62)
				(name "ADDR2/DATA2/PB2")
				(number "26")
			)
			(pin bidirectional line
				(at 45.72 73.66 180)
				(length 7.62)
				(name "ADDR3/DATA3/PB3")
				(number "27")
			)
			(pin bidirectional line
				(at 45.72 71.12 180)
				(length 7.62)
				(name "ADDR4/DATA4/PB4")
				(number "28")
			)
			(pin bidirectional line
				(at 45.72 68.58 180)
				(length 7.62)
				(name "ADDR5/DATA5/PB5")
				(number "29")
			)
			(pin bidirectional line
				(at 45.72 66.04 180)
				(length 7.62)
				(name "ADDR6/DATA6/PB6")
				(number "30")
			)
			(pin bidirectional line
				(at 45.72 63.5 180)
				(length 7.62)
				(name "ADDR7/DATA7/PB7")
				(number "31")
			)
			(pin bidirectional line
				(at 45.72 58.42 180)
				(length 7.62)
				(name "ADDR8/DATA8/PA0")
				(number "57")
			)
			(pin bidirectional line
				(at 45.72 55.88 180)
				(length 7.62)
				(name "ADDR9/DATA9/PA1")
				(number "58")
			)
			(pin bidirectional line
				(at 45.72 53.34 180)
				(length 7.62)
				(name "ADDR10/DATA10/PA2")
				(number "59")
			)
			(pin bidirectional line
				(at 45.72 50.8 180)
				(length 7.62)
				(name "ADDR11/DATA11/PA3")
				(number "60")
			)
			(pin bidirectional line
				(at 45.72 48.26 180)
				(length 7.62)
				(name "ADDR12/DATA12/PA4")
				(number "61")
			)
			(pin bidirectional line
				(at 45.72 45.72 180)
				(length 7.62)
				(name "ADDR13/DATA13/PA5")
				(number "62")
			)
			(pin bidirectional line
				(at 45.72 43.18 180)
				(length 7.62)
				(name "ADDR14/DATA14/PA6")
				(number "63")
			)
			(pin bidirectional line
				(at 45.72 40.64 180)
				(length 7.62)
				(name "ADDR15/DATA15/PA7")
				(number "64")
			)
			(pin bidirectional line
				(at 45.72 35.56 180)
				(length 7.62)
				(name "XADDR14/PK0")
				(number "8")
			)
			(pin bidirectional line
				(at 45.72 33.02 180)
				(length 7.62)
				(name "XADDR15/PK1")
				(number "7")
			)
			(pin bidirectional line
				(at 45.72 30.48 180)
				(length 7.62)
				(name "XADDR16/PK2")
				(number "6")
			)
			(pin bidirectional line
				(at 45.72 27.94 180)
				(length 7.62)
				(name "XADDR17/PK3")
				(number "5")
			)
			(pin bidirectional line
				(at 45.72 25.4 180)
				(length 7.62)
				(name "XADDR18/PK4")
				(number "20")
			)
			(pin bidirectional line
				(at 45.72 22.86 180)
				(length 7.62)
				(name "XADDR19/PK5")
				(number "19")
			)
			(pin bidirectional line
				(at 45.72 20.32 180)
				(length 7.62)
				(name "ECS/ROMCTL/PK7")
				(number "108")
			)
			(pin bidirectional line
				(at 45.72 15.24 180)
				(length 7.62)
				(name "RXD0/PS0")
				(number "89")
			)
			(pin bidirectional line
				(at 45.72 12.7 180)
				(length 7.62)
				(name "TXD0/PS1")
				(number "90")
			)
			(pin bidirectional line
				(at 45.72 10.16 180)
				(length 7.62)
				(name "RXD1/PS2")
				(number "91")
			)
			(pin bidirectional line
				(at 45.72 7.62 180)
				(length 7.62)
				(name "TXD1/PS3")
				(number "92")
			)
			(pin bidirectional line
				(at 45.72 5.08 180)
				(length 7.62)
				(name "MISO0/PS4")
				(number "93")
			)
			(pin bidirectional line
				(at 45.72 2.54 180)
				(length 7.62)
				(name "MOSI0/PS5")
				(number "94")
			)
			(pin bidirectional line
				(at 45.72 0 180)
				(length 7.62)
				(name "SCK0/PS6")
				(number "95")
			)
			(pin bidirectional line
				(at 45.72 -2.54 180)
				(length 7.62)
				(name "SS0/PS7")
				(number "96")
			)
			(pin bidirectional line
				(at 45.72 -7.62 180)
				(length 7.62)
				(name "RXCAN0/RXB/PM0")
				(number "105")
			)
			(pin bidirectional line
				(at 45.72 -10.16 180)
				(length 7.62)
				(name "TXCAN0/TXB/PM1")
				(number "104")
			)
			(pin bidirectional line
				(at 45.72 -12.7 180)
				(length 7.62)
				(name "RX_BF/RXCAN1/RXCAN0/MISO0/PM2")
				(number "103")
			)
			(pin bidirectional line
				(at 45.72 -15.24 180)
				(length 7.62)
				(name "TX_BF/TXCAN1/TXCAN0/SS0/PM3")
				(number "102")
			)
			(pin bidirectional line
				(at 45.72 -17.78 180)
				(length 7.62)
				(name "BF_PSYN/RXCAN0/RXCAN4/MOSI0/PM4")
				(number "101")
			)
			(pin bidirectional line
				(at 45.72 -20.32 180)
				(length 7.62)
				(name "BF_PROK/TXCAN0/TXCAN4/SCK0/PM5")
				(number "100")
			)
			(pin bidirectional line
				(at 45.72 -22.86 180)
				(length 7.62)
				(name "BF_PERR/RXCAN4/PM6")
				(number "88")
			)
			(pin bidirectional line
				(at 45.72 -25.4 180)
				(length 7.62)
				(name "BF_PSLM/TXCAN4/PM7")
				(number "87")
			)
			(pin bidirectional line
				(at 45.72 -30.48 180)
				(length 7.62)
				(name "KWJ0/PJ0")
				(number "22")
			)
			(pin bidirectional line
				(at 45.72 -33.02 180)
				(length 7.62)
				(name "KWJ1/PJ1")
				(number "21")
			)
			(pin bidirectional line
				(at 45.72 -35.56 180)
				(length 7.62)
				(name "KWJ6/RXCAN4/SDA/RXCAN0/PJ6")
				(number "99")
			)
			(pin bidirectional line
				(at 45.72 -38.1 180)
				(length 7.62)
				(name "KWJ7/TXCAN4/SCL/TXCAN0/PJ7")
				(number "98")
			)
			(pin bidirectional line
				(at 45.72 -43.18 180)
				(length 7.62)
				(name "MISO1/PWM0/KWP0/PP0")
				(number "4")
			)
			(pin bidirectional line
				(at 45.72 -45.72 180)
				(length 7.62)
				(name "MOSI1/PWM1/KWP1/PP1")
				(number "3")
			)
			(pin bidirectional line
				(at 45.72 -48.26 180)
				(length 7.62)
				(name "SCK1/PWM2/KWP2/PP2")
				(number "2")
			)
			(pin bidirectional line
				(at 45.72 -50.8 180)
				(length 7.62)
				(name "SS1/PWM3/KWP3/PP3")
				(number "1")
			)
			(pin bidirectional line
				(at 45.72 -53.34 180)
				(length 7.62)
				(name "PWM4/KWP4/PP4")
				(number "112")
			)
			(pin bidirectional line
				(at 45.72 -55.88 180)
				(length 7.62)
				(name "PWM5/KWP5/PP5")
				(number "111")
			)
			(pin bidirectional line
				(at 45.72 -58.42 180)
				(length 7.62)
				(name "PWM6/KWP6/PP6")
				(number "110")
			)
			(pin bidirectional line
				(at 45.72 -60.96 180)
				(length 7.62)
				(name "PWM7/KWP7/PP7")
				(number "109")
			)
		)
		(embedded_fonts no)
	)
)
