(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "MK20DX128VFM5"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 31.115 0)
		)
		(property "Value" "MK20DX128VFM5"
			(at 30.48 31.115 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 8.89 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/K20P32M50SF0.pdf"
			(at 10.16 -35.56 0)
		)
		(property "Description" "Kinetis K20 series, 50-MHz/32-bit ARM Cortex-M4, 128 kB flash/32 kB FlexNVM, 32 kB SRAM/2 kB FlexRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MK20DX128VFM5_0_1"
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PTA0")
				(number "12")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PTA1")
				(number "13")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PTA2")
				(number "14")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PTA3")
				(number "15")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PTA4/LLWU_P3")
				(number "16")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PTA18")
				(number "17")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PTA19")
				(number "18")
			)
			(pin input line
				(at -35.56 0 0)
				(length 5.08)
				(name "XTAL32")
				(number "9")
			)
			(pin input line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "EXTAL32")
				(number "10")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "USB0_DP")
				(number "3")
			)
			(pin input line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "~{RESET}")
				(number "19")
			)
			(pin power_out line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "VOUT33")
				(number "5")
			)
			(pin power_in line
				(at -10.16 35.56 270)
				(length 5.08)
				(name "VBAT")
				(number "11")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 5.08)
				(name "VREGIN")
				(number "6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 5.08 35.56 270)
				(length 5.08)
				(name "VDDA")
				(number "7")
			)
			(pin power_in line
				(at 5.08 -35.56 90)
				(length 5.08)
				(name "VSSA")
				(number "8")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "20")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PTB1")
				(number "21")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PTC1/LLWU_P6")
				(number "22")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PTC2")
				(number "23")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "24")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "25")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "26")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "27")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PTC7")
				(number "28")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "29")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PTD5")
				(number "30")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "31")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PTD7")
				(number "32")
			)
		)
		(symbol "MK20DX128VFM5_1_1"
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "USB0_DM")
				(number "4")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 5.08)
				(name "EPAD")
				(number "33")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MK20FX512VMD12"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -40.64 94.615 0)
		)
		(property "Value" "MK20FX512VMD12"
			(at 40.64 94.615 0)
		)
		(property "Footprint" "Package_BGA:BGA-144_13.0x13.0mm_Layout12x12_P1.0mm"
			(at 8.89 -94.615 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/K20P144M120SF3.pdf"
			(at 10.16 -104.14 0)
		)
		(property "Description" "Kinetis K20 series, 120-MHz/32-bit ARM Cortex-M4, 512 kB flash, 512 kB FlexNVM, 128 kB SRAM, 16 kB FlexRAM, USB HS+FS Device/OTG, MAPBGA-144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis K20 ARM Cortex M4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*13.0x13.0mm*Layout12x12*P1.0mm*"
			(at 0 0 0)
		)
		(symbol "MK20FX512VMD12_0_1")
		(symbol "MK20FX512VMD12_1_1"
			(pin bidirectional line
				(at -45.72 83.82 0)
				(length 5.08)
				(name "PTA0")
				(number "J5")
			)
			(pin bidirectional line
				(at -45.72 81.28 0)
				(length 5.08)
				(name "PTA1")
				(number "J6")
			)
			(pin bidirectional line
				(at -45.72 78.74 0)
				(length 5.08)
				(name "PTA2")
				(number "K6")
			)
			(pin bidirectional line
				(at -45.72 76.2 0)
				(length 5.08)
				(name "PTA3")
				(number "K7")
			)
			(pin bidirectional line
				(at -45.72 73.66 0)
				(length 5.08)
				(name "PTA4/LLWU_P3")
				(number "L7")
			)
			(pin bidirectional line
				(at -45.72 71.12 0)
				(length 5.08)
				(name "PTA5")
				(number "M8")
			)
			(pin bidirectional line
				(at -45.72 68.58 0)
				(length 5.08)
				(name "PTA6")
				(number "J7")
			)
			(pin bidirectional line
				(at -45.72 66.04 0)
				(length 5.08)
				(name "PTA7")
				(number "J8")
			)
			(pin bidirectional line
				(at -45.72 63.5 0)
				(length 5.08)
				(name "PTA8")
				(number "K8")
			)
			(pin bidirectional line
				(at -45.72 60.96 0)
				(length 5.08)
				(name "PTA9")
				(number "L8")
			)
			(pin bidirectional line
				(at -45.72 58.42 0)
				(length 5.08)
				(name "PTA10")
				(number "M9")
			)
			(pin bidirectional line
				(at -45.72 55.88 0)
				(length 5.08)
				(name "PTA11")
				(number "L9")
			)
			(pin bidirectional line
				(at -45.72 53.34 0)
				(length 5.08)
				(name "PTA12")
				(number "K9")
			)
			(pin bidirectional line
				(at -45.72 50.8 0)
				(length 5.08)
				(name "PTA13/LLWU_P4")
				(number "J9")
			)
			(pin bidirectional line
				(at -45.72 48.26 0)
				(length 5.08)
				(name "PTA14")
				(number "L10")
			)
			(pin bidirectional line
				(at -45.72 45.72 0)
				(length 5.08)
				(name "PTA15")
				(number "L11")
			)
			(pin bidirectional line
				(at -45.72 43.18 0)
				(length 5.08)
				(name "PTA16")
				(number "K10")
			)
			(pin bidirectional line
				(at -45.72 40.64 0)
				(length 5.08)
				(name "PTA17")
				(number "K11")
			)
			(pin bidirectional line
				(at -45.72 38.1 0)
				(length 5.08)
				(name "PTA18")
				(number "M12")
			)
			(pin bidirectional line
				(at -45.72 35.56 0)
				(length 5.08)
				(name "PTA19")
				(number "M11")
			)
			(pin bidirectional line
				(at -45.72 33.02 0)
				(length 5.08)
				(name "PTA24")
				(number "K12")
			)
			(pin bidirectional line
				(at -45.72 30.48 0)
				(length 5.08)
				(name "PTA25")
				(number "J12")
			)
			(pin bidirectional line
				(at -45.72 27.94 0)
				(length 5.08)
				(name "PTA26")
				(number "J11")
			)
			(pin bidirectional line
				(at -45.72 25.4 0)
				(length 5.08)
				(name "PTA27")
				(number "J10")
			)
			(pin bidirectional line
				(at -45.72 22.86 0)
				(length 5.08)
				(name "PTA28")
				(number "H12")
			)
			(pin bidirectional line
				(at -45.72 20.32 0)
				(length 5.08)
				(name "PTA29")
				(number "H11")
			)
			(pin bidirectional line
				(at -45.72 15.24 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "H10")
			)
			(pin bidirectional line
				(at -45.72 12.7 0)
				(length 5.08)
				(name "PTB1")
				(number "H9")
			)
			(pin bidirectional line
				(at -45.72 10.16 0)
				(length 5.08)
				(name "PTB2")
				(number "G12")
			)
			(pin bidirectional line
				(at -45.72 7.62 0)
				(length 5.08)
				(name "PTB3")
				(number "G11")
			)
			(pin bidirectional line
				(at -45.72 5.08 0)
				(length 5.08)
				(name "PTB4")
				(number "G10")
			)
			(pin bidirectional line
				(at -45.72 2.54 0)
				(length 5.08)
				(name "PTB5")
				(number "G9")
			)
			(pin bidirectional line
				(at -45.72 0 0)
				(length 5.08)
				(name "PTB6")
				(number "F12")
			)
			(pin bidirectional line
				(at -45.72 -2.54 0)
				(length 5.08)
				(name "PTB7")
				(number "F11")
			)
			(pin bidirectional line
				(at -45.72 -5.08 0)
				(length 5.08)
				(name "PTB8")
				(number "F10")
			)
			(pin bidirectional line
				(at -45.72 -7.62 0)
				(length 5.08)
				(name "PTB9")
				(number "F9")
			)
			(pin bidirectional line
				(at -45.72 -10.16 0)
				(length 5.08)
				(name "PTB10")
				(number "E12")
			)
			(pin bidirectional line
				(at -45.72 -12.7 0)
				(length 5.08)
				(name "PTB11")
				(number "E11")
			)
			(pin bidirectional line
				(at -45.72 -15.24 0)
				(length 5.08)
				(name "PTB16")
				(number "E10")
			)
			(pin bidirectional line
				(at -45.72 -17.78 0)
				(length 5.08)
				(name "PTB17")
				(number "E9")
			)
			(pin bidirectional line
				(at -45.72 -20.32 0)
				(length 5.08)
				(name "PTB18")
				(number "D12")
			)
			(pin bidirectional line
				(at -45.72 -22.86 0)
				(length 5.08)
				(name "PTB19")
				(number "D11")
			)
			(pin bidirectional line
				(at -45.72 -25.4 0)
				(length 5.08)
				(name "PTB20")
				(number "D10")
			)
			(pin bidirectional line
				(at -45.72 -27.94 0)
				(length 5.08)
				(name "PTB21")
				(number "D9")
			)
			(pin bidirectional line
				(at -45.72 -30.48 0)
				(length 5.08)
				(name "PTB22")
				(number "C12")
			)
			(pin bidirectional line
				(at -45.72 -33.02 0)
				(length 5.08)
				(name "PTB23")
				(number "C11")
			)
			(pin input line
				(at -45.72 -40.64 0)
				(length 5.08)
				(name "PGA2_DP/ADC2_DP0/ADC3_DP3/ADC0_DP1")
				(number "J1")
			)
			(pin input line
				(at -45.72 -43.18 0)
				(length 5.08)
				(name "PGA2_DM/ADC2_DM0/ADC3_DM3/ADC0_DM1")
				(number "J2")
			)
			(pin input line
				(at -45.72 -45.72 0)
				(length 5.08)
				(name "PGA3_DP/ADC3_DP0/ADC2_DP3/ADC1_DP1")
				(number "K1")
			)
			(pin input line
				(at -45.72 -48.26 0)
				(length 5.08)
				(name "PGA3_DM/ADC3_DM0/ADC2_DM3/ADC1_DM1")
				(number "K2")
			)
			(pin input line
				(at -45.72 -50.8 0)
				(length 5.08)
				(name "PGA0_DP/ADC0_DP0/ADC1_DP3")
				(number "L1")
			)
			(pin input line
				(at -45.72 -53.34 0)
				(length 5.08)
				(name "PGA0_DM/ADC0_DM0/ADC1_DM3")
				(number "L2")
			)
			(pin input line
				(at -45.72 -55.88 0)
				(length 5.08)
				(name "PGA1_DP/ADC1_DP0/ADC0_DP3")
				(number "M1")
			)
			(pin input line
				(at -45.72 -58.42 0)
				(length 5.08)
				(name "PGA1_DM/ADC1_DM0/ADC0_DM3")
				(number "M2")
			)
			(pin input line
				(at -45.72 -63.5 0)
				(length 5.08)
				(name "ADC0_SE16/CMP1_IN2/ADC0_SE21")
				(number "J3")
			)
			(pin input line
				(at -45.72 -66.04 0)
				(length 5.08)
				(name "ADC1_SE16/CMP2_IN2/ADC0_SE22")
				(number "K3")
			)
			(pin bidirectional line
				(at -45.72 -73.66 0)
				(length 5.08)
				(name "USB0_DP")
				(number "H1")
			)
			(pin bidirectional line
				(at -45.72 -76.2 0)
				(length 5.08)
				(name "USB0_DM")
				(number "H2")
			)
			(pin bidirectional line
				(at -45.72 -83.82 0)
				(length 5.08)
				(name "~{RESET}")
				(number "L12")
			)
			(pin no_connect line
				(at -12.7 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A10")
			)
			(pin power_in line
				(at -10.16 99.06 270)
				(length 5.08)
				(name "VBAT")
				(number "L6")
			)
			(pin no_connect line
				(at -10.16 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B10")
			)
			(pin no_connect line
				(at -7.62 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "C10")
			)
			(pin power_in line
				(at -5.08 99.06 270)
				(length 5.08)
				(name "VREGIN")
				(number "G2")
			)
			(pin no_connect line
				(at -5.08 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "M5")
			)
			(pin power_in line
				(at 0 99.06 270)
				(length 5.08)
				(name "VDD")
				(number "E5")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E6")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E7")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E8")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "F5")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "F8")
			)
			(pin power_in line
				(at 0 -99.06 90)
				(length 5.08)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H3")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H8")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M10")
			)
			(pin power_in line
				(at 5.08 99.06 270)
				(length 5.08)
				(name "VDDA")
				(number "H5")
			)
			(pin power_in line
				(at 5.08 -99.06 90)
				(length 5.08)
				(name "VSSA")
				(number "H6")
			)
			(pin power_in line
				(at 7.62 99.06 270)
				(length 5.08)
				(name "VREFH")
				(number "G5")
			)
			(pin power_in line
				(at 7.62 -99.06 90)
				(length 5.08)
				(name "VREFL")
				(number "G6")
			)
			(pin bidirectional line
				(at 45.72 83.82 180)
				(length 5.08)
				(name "PTC0")
				(number "B12")
			)
			(pin bidirectional line
				(at 45.72 81.28 180)
				(length 5.08)
				(name "PTC1/LLWU_P6")
				(number "B11")
			)
			(pin bidirectional line
				(at 45.72 78.74 180)
				(length 5.08)
				(name "PTC2")
				(number "A12")
			)
			(pin bidirectional line
				(at 45.72 76.2 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "A11")
			)
			(pin bidirectional line
				(at 45.72 73.66 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "A9")
			)
			(pin bidirectional line
				(at 45.72 71.12 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "D8")
			)
			(pin bidirectional line
				(at 45.72 68.58 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "C8")
			)
			(pin bidirectional line
				(at 45.72 66.04 180)
				(length 5.08)
				(name "PTC7")
				(number "B8")
			)
			(pin bidirectional line
				(at 45.72 63.5 180)
				(length 5.08)
				(name "PTC8")
				(number "A8")
			)
			(pin bidirectional line
				(at 45.72 60.96 180)
				(length 5.08)
				(name "PTC9")
				(number "D7")
			)
			(pin bidirectional line
				(at 45.72 58.42 180)
				(length 5.08)
				(name "PTC10")
				(number "C7")
			)
			(pin bidirectional line
				(at 45.72 55.88 180)
				(length 5.08)
				(name "PTC11/LLWU_P11")
				(number "B7")
			)
			(pin bidirectional line
				(at 45.72 53.34 180)
				(length 5.08)
				(name "PTC12")
				(number "A7")
			)
			(pin bidirectional line
				(at 45.72 50.8 180)
				(length 5.08)
				(name "PTC13")
				(number "D6")
			)
			(pin bidirectional line
				(at 45.72 48.26 180)
				(length 5.08)
				(name "PTC14")
				(number "C6")
			)
			(pin bidirectional line
				(at 45.72 45.72 180)
				(length 5.08)
				(name "PTC15")
				(number "B6")
			)
			(pin bidirectional line
				(at 45.72 43.18 180)
				(length 5.08)
				(name "PTC16")
				(number "A6")
			)
			(pin bidirectional line
				(at 45.72 40.64 180)
				(length 5.08)
				(name "PTC17")
				(number "D5")
			)
			(pin bidirectional line
				(at 45.72 38.1 180)
				(length 5.08)
				(name "PTC18")
				(number "C5")
			)
			(pin bidirectional line
				(at 45.72 35.56 180)
				(length 5.08)
				(name "PTC19")
				(number "B5")
			)
			(pin bidirectional line
				(at 45.72 30.48 180)
				(length 5.08)
				(name "PTD0/LLWU_P12")
				(number "A5")
			)
			(pin bidirectional line
				(at 45.72 27.94 180)
				(length 5.08)
				(name "PTD1")
				(number "D4")
			)
			(pin bidirectional line
				(at 45.72 25.4 180)
				(length 5.08)
				(name "PTD2/LLWU_P13")
				(number "C4")
			)
			(pin bidirectional line
				(at 45.72 22.86 180)
				(length 5.08)
				(name "PTD3")
				(number "B4")
			)
			(pin bidirectional line
				(at 45.72 20.32 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A4")
			)
			(pin bidirectional line
				(at 45.72 17.78 180)
				(length 5.08)
				(name "PTD5")
				(number "A3")
			)
			(pin bidirectional line
				(at 45.72 15.24 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "A2")
			)
			(pin bidirectional line
				(at 45.72 12.7 180)
				(length 5.08)
				(name "PTD7")
				(number "A1")
			)
			(pin bidirectional line
				(at 45.72 10.16 180)
				(length 5.08)
				(name "PTD8")
				(number "C9")
			)
			(pin bidirectional line
				(at 45.72 7.62 180)
				(length 5.08)
				(name "PTD9")
				(number "B9")
			)
			(pin bidirectional line
				(at 45.72 5.08 180)
				(length 5.08)
				(name "PTD10")
				(number "B3")
			)
			(pin bidirectional line
				(at 45.72 2.54 180)
				(length 5.08)
				(name "PTD11")
				(number "B2")
			)
			(pin bidirectional line
				(at 45.72 0 180)
				(length 5.08)
				(name "PTD12")
				(number "B1")
			)
			(pin bidirectional line
				(at 45.72 -2.54 180)
				(length 5.08)
				(name "PTD13")
				(number "C3")
			)
			(pin bidirectional line
				(at 45.72 -5.08 180)
				(length 5.08)
				(name "PTD14")
				(number "C2")
			)
			(pin bidirectional line
				(at 45.72 -7.62 180)
				(length 5.08)
				(name "PTD15")
				(number "C1")
			)
			(pin bidirectional line
				(at 45.72 -12.7 180)
				(length 5.08)
				(name "PTE0")
				(number "D3")
			)
			(pin bidirectional line
				(at 45.72 -15.24 180)
				(length 5.08)
				(name "PTE1/LLWU_P0")
				(number "D2")
			)
			(pin bidirectional line
				(at 45.72 -17.78 180)
				(length 5.08)
				(name "PTE2/LLWU_P1")
				(number "D1")
			)
			(pin bidirectional line
				(at 45.72 -20.32 180)
				(length 5.08)
				(name "PTE3")
				(number "E4")
			)
			(pin bidirectional line
				(at 45.72 -22.86 180)
				(length 5.08)
				(name "PTE4/LLWU_P2")
				(number "E3")
			)
			(pin bidirectional line
				(at 45.72 -25.4 180)
				(length 5.08)
				(name "PTE5")
				(number "E2")
			)
			(pin bidirectional line
				(at 45.72 -27.94 180)
				(length 5.08)
				(name "PTE6")
				(number "E1")
			)
			(pin bidirectional line
				(at 45.72 -30.48 180)
				(length 5.08)
				(name "PTE7")
				(number "F4")
			)
			(pin bidirectional line
				(at 45.72 -33.02 180)
				(length 5.08)
				(name "PTE8")
				(number "F3")
			)
			(pin bidirectional line
				(at 45.72 -35.56 180)
				(length 5.08)
				(name "PTE9")
				(number "F2")
			)
			(pin bidirectional line
				(at 45.72 -38.1 180)
				(length 5.08)
				(name "PTE10")
				(number "F1")
			)
			(pin bidirectional line
				(at 45.72 -40.64 180)
				(length 5.08)
				(name "PTE11")
				(number "G4")
			)
			(pin bidirectional line
				(at 45.72 -43.18 180)
				(length 5.08)
				(name "PTE12")
				(number "G3")
			)
			(pin bidirectional line
				(at 45.72 -45.72 180)
				(length 5.08)
				(name "PTE24")
				(number "M4")
			)
			(pin bidirectional line
				(at 45.72 -48.26 180)
				(length 5.08)
				(name "PTE25")
				(number "K5")
			)
			(pin bidirectional line
				(at 45.72 -50.8 180)
				(length 5.08)
				(name "PTE26")
				(number "K4")
			)
			(pin bidirectional line
				(at 45.72 -53.34 180)
				(length 5.08)
				(name "PTE27")
				(number "J4")
			)
			(pin bidirectional line
				(at 45.72 -55.88 180)
				(length 5.08)
				(name "PTE28")
				(number "H4")
			)
			(pin bidirectional line
				(at 45.72 -60.96 180)
				(length 5.08)
				(name "DAC0_OUT/CMP1_IN3/ADC0_SE23")
				(number "L3")
			)
			(pin bidirectional line
				(at 45.72 -63.5 180)
				(length 5.08)
				(name "DAC1_OUT/CMP0_IN4/CMP2_IN3/ADC1_SE23")
				(number "L4")
			)
			(pin bidirectional line
				(at 45.72 -66.04 180)
				(length 5.08)
				(name "VREF_OUT/CMP1_IN5/CMP0_IN5/ADC1_SE18")
				(number "M3")
			)
			(pin output line
				(at 45.72 -71.12 180)
				(length 5.08)
				(name "~{RTC_WAKEUP}")
				(number "L5")
			)
			(pin input line
				(at 45.72 -76.2 180)
				(length 5.08)
				(name "EXTAL32")
				(number "M6")
			)
			(pin output line
				(at 45.72 -78.74 180)
				(length 5.08)
				(name "XTAL32")
				(number "M7")
			)
			(pin power_out line
				(at 45.72 -83.82 180)
				(length 5.08)
				(name "VOUT33")
				(number "G1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MK26FN2M0VMD18"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -40.64 94.615 0)
		)
		(property "Value" "MK26FN2M0VMD18"
			(at 40.64 94.615 0)
		)
		(property "Footprint" "Package_BGA:BGA-144_13.0x13.0mm_Layout12x12_P1.0mm"
			(at 8.89 -94.615 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/K26P169M180SF5.pdf"
			(at 10.16 -104.14 0)
		)
		(property "Description" "Kinetis K26 series, 180-MHz/32-bit ARM Cortex-M4, 2048 kB flash, 256 kB SRAM, USB HS+FS Device/OTG, MAPBGA-144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis K26 ARM Cortex M4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*13.0x13.0mm*Layout12x12*P1.0mm*"
			(at 0 0 0)
		)
		(symbol "MK26FN2M0VMD18_0_1")
		(symbol "MK26FN2M0VMD18_1_1"
			(pin bidirectional line
				(at -45.72 83.82 0)
				(length 5.08)
				(name "PTA0")
				(number "J5")
			)
			(pin bidirectional line
				(at -45.72 81.28 0)
				(length 5.08)
				(name "PTA1")
				(number "J6")
			)
			(pin bidirectional line
				(at -45.72 78.74 0)
				(length 5.08)
				(name "PTA2")
				(number "K6")
			)
			(pin bidirectional line
				(at -45.72 76.2 0)
				(length 5.08)
				(name "PTA3")
				(number "K7")
			)
			(pin bidirectional line
				(at -45.72 73.66 0)
				(length 5.08)
				(name "PTA4/LLWU_P3")
				(number "L7")
			)
			(pin bidirectional line
				(at -45.72 71.12 0)
				(length 5.08)
				(name "PTA5")
				(number "M8")
			)
			(pin bidirectional line
				(at -45.72 68.58 0)
				(length 5.08)
				(name "PTA6")
				(number "J7")
			)
			(pin bidirectional line
				(at -45.72 66.04 0)
				(length 5.08)
				(name "PTA7")
				(number "J8")
			)
			(pin bidirectional line
				(at -45.72 63.5 0)
				(length 5.08)
				(name "PTA8")
				(number "K8")
			)
			(pin bidirectional line
				(at -45.72 60.96 0)
				(length 5.08)
				(name "PTA9")
				(number "L8")
			)
			(pin bidirectional line
				(at -45.72 58.42 0)
				(length 5.08)
				(name "PTA10/LLWU_P22")
				(number "M9")
			)
			(pin bidirectional line
				(at -45.72 55.88 0)
				(length 5.08)
				(name "PTA11/LLWU_P23")
				(number "L9")
			)
			(pin bidirectional line
				(at -45.72 53.34 0)
				(length 5.08)
				(name "PTA12")
				(number "K9")
			)
			(pin bidirectional line
				(at -45.72 50.8 0)
				(length 5.08)
				(name "PTA13/LLWU_P4")
				(number "J9")
			)
			(pin bidirectional line
				(at -45.72 48.26 0)
				(length 5.08)
				(name "PTA14")
				(number "L10")
			)
			(pin bidirectional line
				(at -45.72 45.72 0)
				(length 5.08)
				(name "PTA15")
				(number "L11")
			)
			(pin bidirectional line
				(at -45.72 43.18 0)
				(length 5.08)
				(name "PTA16")
				(number "K10")
			)
			(pin bidirectional line
				(at -45.72 40.64 0)
				(length 5.08)
				(name "PTA17")
				(number "K11")
			)
			(pin bidirectional line
				(at -45.72 38.1 0)
				(length 5.08)
				(name "PTA18")
				(number "M12")
			)
			(pin bidirectional line
				(at -45.72 35.56 0)
				(length 5.08)
				(name "PTA19")
				(number "M11")
			)
			(pin bidirectional line
				(at -45.72 33.02 0)
				(length 5.08)
				(name "PTA24")
				(number "K12")
			)
			(pin bidirectional line
				(at -45.72 30.48 0)
				(length 5.08)
				(name "PTA25")
				(number "J12")
			)
			(pin bidirectional line
				(at -45.72 27.94 0)
				(length 5.08)
				(name "PTA26")
				(number "J11")
			)
			(pin bidirectional line
				(at -45.72 25.4 0)
				(length 5.08)
				(name "PTA27")
				(number "J10")
			)
			(pin bidirectional line
				(at -45.72 22.86 0)
				(length 5.08)
				(name "PTA28")
				(number "H12")
			)
			(pin bidirectional line
				(at -45.72 20.32 0)
				(length 5.08)
				(name "PTA29")
				(number "H11")
			)
			(pin bidirectional line
				(at -45.72 15.24 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "H10")
			)
			(pin bidirectional line
				(at -45.72 12.7 0)
				(length 5.08)
				(name "PTB1")
				(number "H9")
			)
			(pin bidirectional line
				(at -45.72 10.16 0)
				(length 5.08)
				(name "PTB2")
				(number "G12")
			)
			(pin bidirectional line
				(at -45.72 7.62 0)
				(length 5.08)
				(name "PTB3")
				(number "G11")
			)
			(pin bidirectional line
				(at -45.72 5.08 0)
				(length 5.08)
				(name "PTB4")
				(number "G10")
			)
			(pin bidirectional line
				(at -45.72 2.54 0)
				(length 5.08)
				(name "PTB5")
				(number "G9")
			)
			(pin bidirectional line
				(at -45.72 0 0)
				(length 5.08)
				(name "PTB6")
				(number "F12")
			)
			(pin bidirectional line
				(at -45.72 -2.54 0)
				(length 5.08)
				(name "PTB7")
				(number "F11")
			)
			(pin bidirectional line
				(at -45.72 -5.08 0)
				(length 5.08)
				(name "PTB8")
				(number "F10")
			)
			(pin bidirectional line
				(at -45.72 -7.62 0)
				(length 5.08)
				(name "PTB9")
				(number "F9")
			)
			(pin bidirectional line
				(at -45.72 -10.16 0)
				(length 5.08)
				(name "PTB10")
				(number "E12")
			)
			(pin bidirectional line
				(at -45.72 -12.7 0)
				(length 5.08)
				(name "PTB11")
				(number "E11")
			)
			(pin bidirectional line
				(at -45.72 -15.24 0)
				(length 5.08)
				(name "PTB16")
				(number "E10")
			)
			(pin bidirectional line
				(at -45.72 -17.78 0)
				(length 5.08)
				(name "PTB17")
				(number "E9")
			)
			(pin bidirectional line
				(at -45.72 -20.32 0)
				(length 5.08)
				(name "PTB18")
				(number "D12")
			)
			(pin bidirectional line
				(at -45.72 -22.86 0)
				(length 5.08)
				(name "PTB19")
				(number "D11")
			)
			(pin bidirectional line
				(at -45.72 -25.4 0)
				(length 5.08)
				(name "PTB20")
				(number "D10")
			)
			(pin bidirectional line
				(at -45.72 -27.94 0)
				(length 5.08)
				(name "PTB21")
				(number "D9")
			)
			(pin bidirectional line
				(at -45.72 -30.48 0)
				(length 5.08)
				(name "PTB22")
				(number "C12")
			)
			(pin bidirectional line
				(at -45.72 -33.02 0)
				(length 5.08)
				(name "PTB23")
				(number "C11")
			)
			(pin input line
				(at -45.72 -40.64 0)
				(length 5.08)
				(name "PGA2_DP/ADC2_DP0/ADC3_DP3/ADC0_DP1")
				(number "J1")
			)
			(pin input line
				(at -45.72 -43.18 0)
				(length 5.08)
				(name "PGA2_DM/ADC2_DM0/ADC3_DM3/ADC0_DM1")
				(number "J2")
			)
			(pin input line
				(at -45.72 -45.72 0)
				(length 5.08)
				(name "PGA3_DP/ADC3_DP0/ADC2_DP3/ADC1_DP1")
				(number "K1")
			)
			(pin input line
				(at -45.72 -48.26 0)
				(length 5.08)
				(name "PGA3_DM/ADC3_DM0/ADC2_DM3/ADC1_DM1")
				(number "K2")
			)
			(pin input line
				(at -45.72 -50.8 0)
				(length 5.08)
				(name "PGA0_DP/ADC0_DP0/ADC1_DP3")
				(number "L1")
			)
			(pin input line
				(at -45.72 -53.34 0)
				(length 5.08)
				(name "PGA0_DM/ADC0_DM0/ADC1_DM3")
				(number "L2")
			)
			(pin input line
				(at -45.72 -55.88 0)
				(length 5.08)
				(name "PGA1_DP/ADC1_DP0/ADC0_DP3")
				(number "M1")
			)
			(pin input line
				(at -45.72 -58.42 0)
				(length 5.08)
				(name "PGA1_DM/ADC1_DM0/ADC0_DM3")
				(number "M2")
			)
			(pin input line
				(at -45.72 -63.5 0)
				(length 5.08)
				(name "ADC0_SE16/CMP1_IN2/ADC0_SE21")
				(number "J3")
			)
			(pin input line
				(at -45.72 -66.04 0)
				(length 5.08)
				(name "ADC1_SE16/CMP2_IN2/ADC0_SE22")
				(number "K3")
			)
			(pin bidirectional line
				(at -45.72 -73.66 0)
				(length 5.08)
				(name "USB0_DP")
				(number "H1")
			)
			(pin bidirectional line
				(at -45.72 -76.2 0)
				(length 5.08)
				(name "USB0_DM")
				(number "H2")
			)
			(pin bidirectional line
				(at -45.72 -83.82 0)
				(length 5.08)
				(name "~{RESET}")
				(number "L12")
			)
			(pin no_connect line
				(at -12.7 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A10")
			)
			(pin power_in line
				(at -10.16 99.06 270)
				(length 5.08)
				(name "VBAT")
				(number "L6")
			)
			(pin no_connect line
				(at -10.16 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B10")
			)
			(pin no_connect line
				(at -7.62 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "C10")
			)
			(pin power_in line
				(at -5.08 99.06 270)
				(length 5.08)
				(name "VREGIN")
				(number "G2")
			)
			(pin no_connect line
				(at -5.08 -93.98 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "M5")
			)
			(pin power_in line
				(at 0 99.06 270)
				(length 5.08)
				(name "VDD")
				(number "E5")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E6")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E7")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E8")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "F5")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "F8")
			)
			(pin power_in line
				(at 0 -99.06 90)
				(length 5.08)
				(name "VSS")
				(number "F6")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G8")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H3")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H8")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "M10")
			)
			(pin power_in line
				(at 5.08 99.06 270)
				(length 5.08)
				(name "VDDA")
				(number "H5")
			)
			(pin power_in line
				(at 5.08 -99.06 90)
				(length 5.08)
				(name "VSSA")
				(number "H6")
			)
			(pin power_in line
				(at 7.62 99.06 270)
				(length 5.08)
				(name "VREFH")
				(number "G5")
			)
			(pin power_in line
				(at 7.62 -99.06 90)
				(length 5.08)
				(name "VREFL")
				(number "G6")
			)
			(pin bidirectional line
				(at 45.72 83.82 180)
				(length 5.08)
				(name "PTC0")
				(number "B12")
			)
			(pin bidirectional line
				(at 45.72 81.28 180)
				(length 5.08)
				(name "PTC1/LLWU_P6")
				(number "B11")
			)
			(pin bidirectional line
				(at 45.72 78.74 180)
				(length 5.08)
				(name "PTC2")
				(number "A12")
			)
			(pin bidirectional line
				(at 45.72 76.2 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "A11")
			)
			(pin bidirectional line
				(at 45.72 73.66 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "A9")
			)
			(pin bidirectional line
				(at 45.72 71.12 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "D8")
			)
			(pin bidirectional line
				(at 45.72 68.58 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "C8")
			)
			(pin bidirectional line
				(at 45.72 66.04 180)
				(length 5.08)
				(name "PTC7")
				(number "B8")
			)
			(pin bidirectional line
				(at 45.72 63.5 180)
				(length 5.08)
				(name "PTC8")
				(number "A8")
			)
			(pin bidirectional line
				(at 45.72 60.96 180)
				(length 5.08)
				(name "PTC9")
				(number "D7")
			)
			(pin bidirectional line
				(at 45.72 58.42 180)
				(length 5.08)
				(name "PTC10")
				(number "C7")
			)
			(pin bidirectional line
				(at 45.72 55.88 180)
				(length 5.08)
				(name "PTC11/LLWU_P11")
				(number "B7")
			)
			(pin bidirectional line
				(at 45.72 53.34 180)
				(length 5.08)
				(name "PTC12")
				(number "A7")
			)
			(pin bidirectional line
				(at 45.72 50.8 180)
				(length 5.08)
				(name "PTC13")
				(number "D6")
			)
			(pin bidirectional line
				(at 45.72 48.26 180)
				(length 5.08)
				(name "PTC14")
				(number "C6")
			)
			(pin bidirectional line
				(at 45.72 45.72 180)
				(length 5.08)
				(name "PTC15")
				(number "B6")
			)
			(pin bidirectional line
				(at 45.72 43.18 180)
				(length 5.08)
				(name "PTC16")
				(number "A6")
			)
			(pin bidirectional line
				(at 45.72 40.64 180)
				(length 5.08)
				(name "PTC17")
				(number "D5")
			)
			(pin bidirectional line
				(at 45.72 38.1 180)
				(length 5.08)
				(name "PTC18")
				(number "C5")
			)
			(pin bidirectional line
				(at 45.72 35.56 180)
				(length 5.08)
				(name "PTC19")
				(number "B5")
			)
			(pin bidirectional line
				(at 45.72 30.48 180)
				(length 5.08)
				(name "PTD0/LLWU_P12")
				(number "A5")
			)
			(pin bidirectional line
				(at 45.72 27.94 180)
				(length 5.08)
				(name "PTD1")
				(number "D4")
			)
			(pin bidirectional line
				(at 45.72 25.4 180)
				(length 5.08)
				(name "PTD2/LLWU_P13")
				(number "C4")
			)
			(pin bidirectional line
				(at 45.72 22.86 180)
				(length 5.08)
				(name "PTD3")
				(number "B4")
			)
			(pin bidirectional line
				(at 45.72 20.32 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A4")
			)
			(pin bidirectional line
				(at 45.72 17.78 180)
				(length 5.08)
				(name "PTD5")
				(number "A3")
			)
			(pin bidirectional line
				(at 45.72 15.24 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "A2")
			)
			(pin bidirectional line
				(at 45.72 12.7 180)
				(length 5.08)
				(name "PTD7")
				(number "A1")
			)
			(pin bidirectional line
				(at 45.72 10.16 180)
				(length 5.08)
				(name "PTD8/LLWU_P24")
				(number "C9")
			)
			(pin bidirectional line
				(at 45.72 7.62 180)
				(length 5.08)
				(name "PTD9")
				(number "B9")
			)
			(pin bidirectional line
				(at 45.72 5.08 180)
				(length 5.08)
				(name "PTD10")
				(number "B3")
			)
			(pin bidirectional line
				(at 45.72 2.54 180)
				(length 5.08)
				(name "PTD11/LLWU_P25")
				(number "B2")
			)
			(pin bidirectional line
				(at 45.72 0 180)
				(length 5.08)
				(name "PTD12")
				(number "B1")
			)
			(pin bidirectional line
				(at 45.72 -2.54 180)
				(length 5.08)
				(name "PTD13")
				(number "C3")
			)
			(pin bidirectional line
				(at 45.72 -5.08 180)
				(length 5.08)
				(name "PTD14")
				(number "C2")
			)
			(pin bidirectional line
				(at 45.72 -7.62 180)
				(length 5.08)
				(name "PTD15")
				(number "C1")
			)
			(pin bidirectional line
				(at 45.72 -12.7 180)
				(length 5.08)
				(name "PTE0")
				(number "D3")
			)
			(pin bidirectional line
				(at 45.72 -15.24 180)
				(length 5.08)
				(name "PTE1/LLWU_P0")
				(number "D2")
			)
			(pin bidirectional line
				(at 45.72 -17.78 180)
				(length 5.08)
				(name "PTE2/LLWU_P1")
				(number "D1")
			)
			(pin bidirectional line
				(at 45.72 -20.32 180)
				(length 5.08)
				(name "PTE3")
				(number "E4")
			)
			(pin bidirectional line
				(at 45.72 -22.86 180)
				(length 5.08)
				(name "PTE4/LLWU_P2")
				(number "E3")
			)
			(pin bidirectional line
				(at 45.72 -25.4 180)
				(length 5.08)
				(name "PTE5")
				(number "E2")
			)
			(pin bidirectional line
				(at 45.72 -27.94 180)
				(length 5.08)
				(name "PTE6/LLWU_P16")
				(number "E1")
			)
			(pin bidirectional line
				(at 45.72 -30.48 180)
				(length 5.08)
				(name "PTE7")
				(number "F4")
			)
			(pin bidirectional line
				(at 45.72 -33.02 180)
				(length 5.08)
				(name "PTE8")
				(number "F3")
			)
			(pin bidirectional line
				(at 45.72 -35.56 180)
				(length 5.08)
				(name "PTE9/LLWU_P17")
				(number "F2")
			)
			(pin bidirectional line
				(at 45.72 -38.1 180)
				(length 5.08)
				(name "PTE10/LLWU_P18")
				(number "F1")
			)
			(pin bidirectional line
				(at 45.72 -40.64 180)
				(length 5.08)
				(name "PTE11")
				(number "G4")
			)
			(pin bidirectional line
				(at 45.72 -43.18 180)
				(length 5.08)
				(name "PTE12")
				(number "G3")
			)
			(pin bidirectional line
				(at 45.72 -45.72 180)
				(length 5.08)
				(name "PTE24")
				(number "M4")
			)
			(pin bidirectional line
				(at 45.72 -48.26 180)
				(length 5.08)
				(name "PTE25/LLWU_P21")
				(number "K5")
			)
			(pin bidirectional line
				(at 45.72 -50.8 180)
				(length 5.08)
				(name "PTE26/CLKOUT32K")
				(number "K4")
			)
			(pin bidirectional line
				(at 45.72 -53.34 180)
				(length 5.08)
				(name "PTE27")
				(number "J4")
			)
			(pin bidirectional line
				(at 45.72 -55.88 180)
				(length 5.08)
				(name "PTE28")
				(number "H4")
			)
			(pin bidirectional line
				(at 45.72 -60.96 180)
				(length 5.08)
				(name "DAC0_OUT/CMP1_IN3/ADC0_SE23")
				(number "L3")
			)
			(pin bidirectional line
				(at 45.72 -63.5 180)
				(length 5.08)
				(name "DAC1_OUT/CMP0_IN4/CMP2_IN3/ADC1_SE23")
				(number "L4")
			)
			(pin bidirectional line
				(at 45.72 -66.04 180)
				(length 5.08)
				(name "VREF_OUT/CMP1_IN5/CMP0_IN5/ADC1_SE18")
				(number "M3")
			)
			(pin output line
				(at 45.72 -71.12 180)
				(length 5.08)
				(name "~{RTC_WAKEUP}")
				(number "L5")
			)
			(pin input line
				(at 45.72 -76.2 180)
				(length 5.08)
				(name "EXTAL32")
				(number "M6")
			)
			(pin output line
				(at 45.72 -78.74 180)
				(length 5.08)
				(name "XTAL32")
				(number "M7")
			)
			(pin power_out line
				(at 45.72 -83.82 180)
				(length 5.08)
				(name "VOUT33")
				(number "G1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKE02Z64VLC4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 31.75 0)
		)
		(property "Value" "MKE02Z64VLC4"
			(at 17.78 31.75 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 8.89 -31.75 0)
		)
		(property "Datasheet" "https://www.nxp.com/files-static/microcontrollers/doc/ref_manual/MKE02P64M40SF0RM.pdf"
			(at 2.54 7.62 0)
		)
		(property "Description" "40 MHz, Entry-Level, High-Robustness, ESD/EMC performance Microcontroller, Cortex-M0+ core, 64kB Flash, 4kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP Kinetis Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MKE02Z64VLC4_0_1")
		(symbol "MKE02Z64VLC4_1_1"
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PTD0")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PTD1")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PTD2")
				(number "22")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PTD3")
				(number "21")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PTA4")
				(number "32")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PTA5")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PTC4")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PTB6")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PTB7")
				(number "7")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 5.08)
				(name "VSS/VSSA")
				(number "6")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 5.08)
				(name "VREFL")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 5.08)
				(name "PTA1")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PTA3")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA6")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA7")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTB0")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTB1")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTB2")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PTB3")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB4")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB5")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTC0")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTC1")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTC2")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PTC3")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 5.08)
				(name "PTC5")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PTC6")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PTC7")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKE02Z64VLD4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 45.72 0)
		)
		(property "Value" "MKE02Z64VLD4"
			(at 17.78 45.72 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 8.89 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/files-static/microcontrollers/doc/ref_manual/MKE02P64M40SF0RM.pdf"
			(at 2.54 17.78 0)
		)
		(property "Description" "40 MHz, Entry-Level, High-Robustness, ESD/EMC performance Microcontroller, Cortex-M0+ core, 64kB Flash, 4kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP Kinetis Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MKE02Z64VLD4_0_1")
		(symbol "MKE02Z64VLD4_1_1"
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PTE0")
				(number "40")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PTE1")
				(number "39")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PTE2")
				(number "38")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 5.08)
				(name "PTE7")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PTH2")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PTA4")
				(number "44")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PTA5")
				(number "43")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PTC4")
				(number "42")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PTB6")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 -27.94 0)
				(length 5.08)
				(name "PTB7")
				(number "9")
			)
			(pin passive line
				(at -2.54 48.26 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "28")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 5.08)
				(name "VSS")
				(number "11")
			)
			(pin passive line
				(at -2.54 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "27")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 5.08)
				(name "VSS/VSSA")
				(number "8")
			)
			(pin power_in line
				(at 5.08 -48.26 90)
				(length 5.08)
				(name "VREFL")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PTA0")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 5.08)
				(name "PTA1")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PTA2")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PTA3")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PTA6")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 5.08)
				(name "PTA7")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PTB0")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTB1")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTB2")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTB4")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTB5")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PTC0")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTC1")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTC2")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTC3")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTC5")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTC6")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTC7")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 5.08)
				(name "PTD0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PTD1")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PTD2")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 5.08)
				(name "PTD3")
				(number "30")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PTD4")
				(number "29")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PTD5")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PTD6")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PTD7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKE02Z64VLH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 55.88 0)
		)
		(property "Value" "MKE02Z64VLH4"
			(at 20.32 55.88 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 8.89 -54.61 0)
		)
		(property "Datasheet" "https://www.nxp.com/files-static/microcontrollers/doc/ref_manual/MKE02P64M40SF0RM.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "40 MHz, Entry-Level, High-Robustness, ESD/EMC performance Microcontroller, Cortex-M0+ core, 64kB Flash, 4kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP Kinetis Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKE02Z64VLH4_0_1")
		(symbol "MKE02Z64VLH4_1_1"
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 5.08)
				(name "PTF0")
				(number "43")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PTF1")
				(number "42")
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PTF2")
				(number "36")
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PTF3")
				(number "35")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PTF4")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PTF5")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PTF6")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PTF7")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PTG0")
				(number "58")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PTG1")
				(number "57")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PTG2")
				(number "56")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PTG3")
				(number "55")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PTH0")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PTH1")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTH2")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PTH6")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PTH7")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PTA4")
				(number "64")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PTA5")
				(number "63")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PTC4")
				(number "62")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PTB6")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PTB7")
				(number "11")
			)
			(pin passive line
				(at -2.54 58.42 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "41")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 5.08)
				(name "VSS")
				(number "13")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 5.08)
				(name "VSS/VSSA")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -58.42 90)
				(length 5.08)
				(name "VREFL")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PTA0")
				(number "50")
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PTA1")
				(number "49")
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PTA2")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PTA3")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PTA6")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PTA7")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PTB0")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PTB1")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PTB2")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 5.08)
				(name "PTB3")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PTB4")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PTB5")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTC0")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTC1")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTC2")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTC3")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTC5")
				(number "61")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PTC6")
				(number "52")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTC7")
				(number "51")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTD0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTD1")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTD2")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTD3")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PTD4")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 5.08)
				(name "PTD5")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PTD6")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PTD7")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PTE0")
				(number "60")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PTE1")
				(number "59")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PTE2")
				(number "54")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PTE3")
				(number "53")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PTE4")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PTE5")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PTE6")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PTE7")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKE02Z64VQH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 55.88 0)
		)
		(property "Value" "MKE02Z64VQH4"
			(at 20.32 55.88 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 8.89 -54.61 0)
		)
		(property "Datasheet" "https://www.nxp.com/files-static/microcontrollers/doc/ref_manual/MKE02P64M40SF0RM.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "40 MHz, Entry-Level, High-Robustness, ESD/EMC performance Microcontroller, Cortex-M0+ core, 64kB Flash, 4kB RAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP Kinetis Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MKE02Z64VQH4_0_1")
		(symbol "MKE02Z64VQH4_1_1"
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 5.08)
				(name "PTF0")
				(number "43")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 5.08)
				(name "PTF1")
				(number "42")
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 5.08)
				(name "PTF2")
				(number "36")
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 5.08)
				(name "PTF3")
				(number "35")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 5.08)
				(name "PTF4")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 5.08)
				(name "PTF5")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 5.08)
				(name "PTF6")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 5.08)
				(name "PTF7")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PTG0")
				(number "58")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PTG1")
				(number "57")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PTG2")
				(number "56")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PTG3")
				(number "55")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PTH0")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PTH1")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTH2")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PTH6")
				(number "4")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PTH7")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 -17.78 0)
				(length 5.08)
				(name "PTA4")
				(number "64")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PTA5")
				(number "63")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PTC4")
				(number "62")
			)
			(pin bidirectional line
				(at -22.86 -38.1 0)
				(length 5.08)
				(name "PTB6")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 -40.64 0)
				(length 5.08)
				(name "PTB7")
				(number "11")
			)
			(pin passive line
				(at -2.54 58.42 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "41")
			)
			(pin power_in line
				(at -2.54 58.42 270)
				(length 5.08)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -58.42 90)
				(length 5.08)
				(name "VSS")
				(number "13")
			)
			(pin passive line
				(at -2.54 -58.42 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "40")
			)
			(pin power_in line
				(at 2.54 58.42 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "8")
			)
			(pin power_in line
				(at 2.54 -58.42 90)
				(length 5.08)
				(name "VSS/VSSA")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -58.42 90)
				(length 5.08)
				(name "VREFL")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 5.08)
				(name "PTA0")
				(number "50")
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 5.08)
				(name "PTA1")
				(number "49")
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 5.08)
				(name "PTA2")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 5.08)
				(name "PTA3")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 5.08)
				(name "PTA6")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 5.08)
				(name "PTA7")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 5.08)
				(name "PTB0")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 5.08)
				(name "PTB1")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PTB2")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 5.08)
				(name "PTB3")
				(number "31")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PTB4")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PTB5")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTC0")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTC1")
				(number "25")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTC2")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTC3")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTC5")
				(number "61")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PTC6")
				(number "52")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTC7")
				(number "51")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTD0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTD1")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTD2")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTD3")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PTD4")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 5.08)
				(name "PTD5")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PTD6")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PTD7")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 5.08)
				(name "PTE0")
				(number "60")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 5.08)
				(name "PTE1")
				(number "59")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 5.08)
				(name "PTE2")
				(number "54")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 5.08)
				(name "PTE3")
				(number "53")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 5.08)
				(name "PTE4")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 -43.18 180)
				(length 5.08)
				(name "PTE5")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 5.08)
				(name "PTE6")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 5.08)
				(name "PTE7")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKE16Z64VLF4"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "MKE16Z64VLF4"
			(at 5.08 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 5.08 -34.29 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/KE1xZP48M48SF0.pdf"
			(at -1.27 6.35 0)
		)
		(property "Description" "Kinetis KE1xZ series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB RAM, Mainstream, Touch (TSI) and CAN control, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KE16 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKE16Z64VLF4_0_1")
		(symbol "MKE16Z64VLF4_1_1"
			(pin bidirectional line
				(at -15.24 33.02 0)
				(length 2.54)
				(name "PTA0")
				(number "38")
			)
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PTA1")
				(number "37")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PTA2")
				(number "36")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PTA3")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PTA4")
				(number "48")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PTA5")
				(number "47")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PTA6")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PTA7")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 10.16 0)
				(length 2.54)
				(name "PTB0")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PTB1")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PTB2")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PTB3")
				(number "24")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PTB4")
				(number "16")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PTB5")
				(number "15")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PTB6")
				(number "12")
			)
			(pin bidirectional line
				(at -15.24 -7.62 0)
				(length 2.54)
				(name "PTB7")
				(number "11")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PTC0")
				(number "23")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PTC1")
				(number "22")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PTC2")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PTC3")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PTC4")
				(number "46")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PTC5")
				(number "45")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PTC6")
				(number "40")
			)
			(pin bidirectional line
				(at -15.24 -30.48 0)
				(length 2.54)
				(name "PTC7")
				(number "39")
			)
			(pin power_in line
				(at -5.08 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 2.54)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 2.54)
				(name "VDDA")
				(number "8")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 2.54)
				(name "VREFH")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "VSS/VREFL")
				(number "10")
			)
			(pin bidirectional line
				(at 15.24 33.02 180)
				(length 2.54)
				(name "PTD0")
				(number "2")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PTD1")
				(number "1")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PTD2")
				(number "34")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PTD3")
				(number "33")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PTD4")
				(number "32")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PTD5")
				(number "21")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PTD6")
				(number "20")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PTD7")
				(number "19")
			)
			(pin bidirectional line
				(at 15.24 10.16 180)
				(length 2.54)
				(name "PTE0")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PTE1")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PTE2")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PTE3")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PTE4")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PTE5")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PTE6")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PTE8")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PTE10")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PTE11")
				(number "3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL02Z32CAF4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 31.115 0)
		)
		(property "Value" "MKL02Z32CAF4"
			(at 27.94 31.115 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-20_1.994x1.94mm_Layout4x5_P0.4mm"
			(at 3.81 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL02P20M48SF0.pdf"
			(at 7.62 -20.32 0)
		)
		(property "Description" "Kinetis KL02 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, WLCSP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL02 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*1.994x1.94mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MKL02Z32CAF4_0_1")
		(symbol "MKL02Z32CAF4_1_1"
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PTA0/IRQ_0")
				(number "A3")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "A4")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PTA2")
				(number "B3")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PTA3")
				(number "C4")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PTA4")
				(number "D4")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PTA5")
				(number "E3")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PTA6")
				(number "E4")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PTA7/IRQ_4")
				(number "E1")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PTA8")
				(number "D1")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PTA9")
				(number "C1")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PTA12/IRQ_13/LPTMR0_ALT2")
				(number "A1")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 5.08)
				(name "VDD/VREFH")
				(number "B4")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 5.08)
				(name "VSS/VREFL")
				(number "C3")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PTB0/IRQ_5")
				(number "E2")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PTB1/IRQ_6")
				(number "D3")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PTB2/IRQ_7")
				(number "D2")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PTB3/IRQ_10")
				(number "B1")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PTB4/IRQ_11")
				(number "C2")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PTB5/IRQ_12")
				(number "B2")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PTB13")
				(number "A2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL02Z32VFG4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 31.115 0)
		)
		(property "Value" "MKL02Z32VFG4"
			(at 27.94 31.115 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.9x1.9mm"
			(at 3.81 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL02P32M48SF0.pdf"
			(at 7.62 -20.32 0)
		)
		(property "Description" "Kinetis KL02 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL02 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL02Z32VFG4_0_1")
		(symbol "MKL02Z32VFG4_1_1"
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PTA0/IRQ_0")
				(number "14")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PTA2")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PTA3")
				(number "3")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PTA4")
				(number "4")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PTA5")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PTA6")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PTA7/IRQ_4")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 5.08)
				(name "EPAD")
				(number "17")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 5.08)
				(name "VDD/VREFH")
				(number "1")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 5.08)
				(name "VSS/VREFL")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PTB0/IRQ_5")
				(number "8")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PTB1/IRQ_6")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PTB2/IRQ_7")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PTB3/IRQ_10")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PTB4/IRQ_11")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PTB5/IRQ_12")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL02Z32VFK4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 31.115 0)
		)
		(property "Value" "MKL02Z32VFK4"
			(at 27.94 31.115 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 3.81 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL02P32M48SF0.pdf"
			(at 7.62 -20.32 0)
		)
		(property "Description" "Kinetis KL02 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL02 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL02Z32VFK4_0_1")
		(symbol "MKL02Z32VFK4_1_1"
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PTA0/IRQ_0")
				(number "22")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "23")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PTA3")
				(number "5")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PTA4")
				(number "6")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PTA5")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PTA6")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PTA7/IRQ_4")
				(number "11")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PTA8")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PTA9")
				(number "16")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PTA12/IRQ_13/LPTMR0_ALT2")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 5.08)
				(name "EPAD")
				(number "25")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 5.08)
				(name "VDD/VREFH")
				(number "3")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 5.08)
				(name "VSS/VREFL")
				(number "4")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PTB0/IRQ_5")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PTB1/IRQ_6")
				(number "13")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PTB2/IRQ_7")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PTB3/IRQ_10")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PTB4/IRQ_11")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PTB5/IRQ_12")
				(number "19")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "PTB6/IRQ_2/LPTMR0_ALT3")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PTB7/IRQ_3")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PTB10")
				(number "9")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PTB11")
				(number "10")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PTB13")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL02Z32VFM4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -27.94 31.115 0)
		)
		(property "Value" "MKL02Z32VFM4"
			(at 27.94 31.115 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 3.81 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL02P32M48SF0.pdf"
			(at 7.62 -20.32 0)
		)
		(property "Description" "Kinetis KL02 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL02 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL02Z32VFM4_0_1")
		(symbol "MKL02Z32VFM4_1_1"
			(pin bidirectional line
				(at -33.02 15.24 0)
				(length 5.08)
				(name "PTA0/IRQ_0")
				(number "30")
			)
			(pin bidirectional line
				(at -33.02 12.7 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "31")
			)
			(pin bidirectional line
				(at -33.02 10.16 0)
				(length 5.08)
				(name "PTA2")
				(number "32")
			)
			(pin bidirectional line
				(at -33.02 7.62 0)
				(length 5.08)
				(name "PTA3")
				(number "7")
			)
			(pin bidirectional line
				(at -33.02 5.08 0)
				(length 5.08)
				(name "PTA4")
				(number "8")
			)
			(pin bidirectional line
				(at -33.02 2.54 0)
				(length 5.08)
				(name "PTA5")
				(number "9")
			)
			(pin bidirectional line
				(at -33.02 0 0)
				(length 5.08)
				(name "PTA6")
				(number "10")
			)
			(pin bidirectional line
				(at -33.02 -2.54 0)
				(length 5.08)
				(name "PTA7/IRQ_4")
				(number "15")
			)
			(pin bidirectional line
				(at -33.02 -5.08 0)
				(length 5.08)
				(name "PTA8")
				(number "19")
			)
			(pin bidirectional line
				(at -33.02 -7.62 0)
				(length 5.08)
				(name "PTA9")
				(number "20")
			)
			(pin bidirectional line
				(at -33.02 -10.16 0)
				(length 5.08)
				(name "PTA10/IRQ_8")
				(number "21")
			)
			(pin bidirectional line
				(at -33.02 -12.7 0)
				(length 5.08)
				(name "PTA11/IRQ_9")
				(number "22")
			)
			(pin bidirectional line
				(at -33.02 -15.24 0)
				(length 5.08)
				(name "PTA12/IRQ_13/LPTMR0_ALT2")
				(number "26")
			)
			(pin bidirectional line
				(at -33.02 -17.78 0)
				(length 5.08)
				(name "PTA13")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 5.08)
				(name "EPAD")
				(number "33")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 5.08)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 5.08)
				(name "VREFH")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 5.08)
				(name "VREFL")
				(number "5")
			)
			(pin bidirectional line
				(at 33.02 15.24 180)
				(length 5.08)
				(name "PTB0/IRQ_5")
				(number "16")
			)
			(pin bidirectional line
				(at 33.02 12.7 180)
				(length 5.08)
				(name "PTB1/IRQ_6")
				(number "17")
			)
			(pin bidirectional line
				(at 33.02 10.16 180)
				(length 5.08)
				(name "PTB2/IRQ_7")
				(number "18")
			)
			(pin bidirectional line
				(at 33.02 7.62 180)
				(length 5.08)
				(name "PTB3/IRQ_10")
				(number "23")
			)
			(pin bidirectional line
				(at 33.02 5.08 180)
				(length 5.08)
				(name "PTB4/IRQ_11")
				(number "24")
			)
			(pin bidirectional line
				(at 33.02 2.54 180)
				(length 5.08)
				(name "PTB5/IRQ_12")
				(number "25")
			)
			(pin bidirectional line
				(at 33.02 0 180)
				(length 5.08)
				(name "PTB6/IRQ_2/LPTMR0_ALT3")
				(number "1")
			)
			(pin bidirectional line
				(at 33.02 -2.54 180)
				(length 5.08)
				(name "PTB7/IRQ_3")
				(number "2")
			)
			(pin bidirectional line
				(at 33.02 -5.08 180)
				(length 5.08)
				(name "PTB8")
				(number "11")
			)
			(pin bidirectional line
				(at 33.02 -7.62 180)
				(length 5.08)
				(name "PTB9")
				(number "12")
			)
			(pin bidirectional line
				(at 33.02 -10.16 180)
				(length 5.08)
				(name "PTB10")
				(number "13")
			)
			(pin bidirectional line
				(at 33.02 -12.7 180)
				(length 5.08)
				(name "PTB11")
				(number "14")
			)
			(pin bidirectional line
				(at 33.02 -15.24 180)
				(length 5.08)
				(name "PTB12")
				(number "28")
			)
			(pin bidirectional line
				(at 33.02 -17.78 180)
				(length 5.08)
				(name "PTB13")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL03Z32CAF4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 20.955 0)
		)
		(property "Value" "MKL03Z32CAF4"
			(at 30.48 20.955 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-20_1.994x1.609mm_Layout5x4_P0.4mm"
			(at 3.81 -20.955 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL03P24M48SF0.pdf"
			(at 7.62 -25.4 0)
		)
		(property "Description" "Kinetis KL03 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 2 kB SRAM, WLCSP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL03 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*1.994x1.609mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MKL03Z32CAF4_0_1")
		(symbol "MKL03Z32CAF4_1_1"
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PTA0/IRQ_0/LLWU_P7")
				(number "A4")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "B4")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PTA2")
				(number "A5")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PTA3")
				(number "C4")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PTA4")
				(number "C3")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PTA5/RTC_CLK_IN")
				(number "D3")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PTA6")
				(number "D5")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PTA7/IRQ_4")
				(number "D4")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PTA8")
				(number "D2")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PTA9")
				(number "C2")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PTA12/IRQ_13/LPTMR0_ALT2")
				(number "B3")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "B5")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "C5")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PTB0/IRQ_5/LLWU_P4")
				(number "C1")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PTB1/IRQ_6")
				(number "D1")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PTB2/IRQ_7")
				(number "B1")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PTB3/IRQ_10")
				(number "A1")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PTB4/IRQ_11")
				(number "B2")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PTB5/IRQ_12")
				(number "A2")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PTB13/CLKOUT32K")
				(number "A3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL03Z32VFG4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 20.955 0)
		)
		(property "Value" "MKL03Z32VFG4"
			(at 30.48 20.955 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.9x1.9mm"
			(at 3.81 -20.955 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL03P24M48SF0.pdf"
			(at 7.62 -48.26 0)
		)
		(property "Description" "Kinetis KL03 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 2 kB SRAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL03 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL03Z32VFG4_0_1")
		(symbol "MKL03Z32VFG4_1_1"
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PTA0/IRQ_0/LLWU_P7")
				(number "14")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "15")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PTA2")
				(number "16")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PTA3")
				(number "3")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PTA4")
				(number "4")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PTA5/RTC_CLK_IN")
				(number "5")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PTA6")
				(number "6")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PTA7/IRQ_4")
				(number "7")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 5.08)
				(name "EPAD")
				(number "17")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PTB0/IRQ_5/LLWU_P4")
				(number "8")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PTB1/IRQ_6")
				(number "9")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PTB2/IRQ_7")
				(number "10")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PTB3/IRQ_10")
				(number "11")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PTB4/IRQ_11")
				(number "12")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PTB5/IRQ_12")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL03Z32VFK4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 20.955 0)
		)
		(property "Value" "MKL03Z32VFK4"
			(at 30.48 20.955 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 3.81 -20.955 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL03P24M48SF0.pdf"
			(at 7.62 -25.4 0)
		)
		(property "Description" "Kinetis KL03 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 2 kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL03 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL03Z32VFK4_0_1")
		(symbol "MKL03Z32VFK4_1_1"
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PTA0/IRQ_0/LLWU_P7")
				(number "22")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "23")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PTA3")
				(number "5")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PTA4")
				(number "6")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PTA5/RTC_CLK_IN")
				(number "7")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PTA6")
				(number "8")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PTA7/IRQ_4")
				(number "11")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PTA8")
				(number "15")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PTA9")
				(number "16")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PTA12/IRQ_13/LPTMR0_ALT2")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 5.08)
				(name "EPAD")
				(number "25")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PTB0/IRQ_5/LLWU_P4")
				(number "12")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PTB1/IRQ_6")
				(number "13")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PTB2/IRQ_7")
				(number "14")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PTB3/IRQ_10")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PTB4/IRQ_11")
				(number "18")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PTB5/IRQ_12")
				(number "19")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PTB6/IRQ_2/LPTMR0_ALT3")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PTB7/IRQ_3")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PTB10")
				(number "9")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PTB11")
				(number "10")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PTB13/CLKOUT32K")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL04Z32VFK4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL04Z32VFK4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL04P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL04 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL04 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL04Z32VFK4_0_1")
		(symbol "MKL04Z32VFK4_1_1"
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PTA0/IRQ_0/LLWU_P7")
				(number "22")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "23")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PTA3")
				(number "5")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PTA4/LLWU_P0")
				(number "6")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PTA5/LLWU_P1/RTC_CLK_IN")
				(number "7")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PTA6/LLWU_P2")
				(number "8")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PTA7/IRQ_7/LLWU_P3")
				(number "11")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PTA8")
				(number "15")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PTA9")
				(number "16")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PTA12/IRQ_17/LPTMR0_ALT2")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 5.08)
				(name "EPAD")
				(number "25")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 5.08)
				(name "VDD/VREFH")
				(number "3")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 5.08)
				(name "VSS/VREFL")
				(number "4")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PTB0/IRQ_8/LLWU_P4")
				(number "12")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PTB1/IRQ_9")
				(number "13")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PTB2/IRQ_10/LLWU_P5")
				(number "14")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PTB3/IRQ_14")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PTB4/IRQ_15/LLWU_P6")
				(number "18")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PTB5/IRQ_16")
				(number "19")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PTB6/IRQ_2/LPTMR0_ALT3")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PTB7/IRQ_3")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PTB10")
				(number "9")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PTB11")
				(number "10")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PTB13")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL04Z32VFM4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL04Z32VFM4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL04P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL04 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL04 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL04Z32VFM4_0_1")
		(symbol "MKL04Z32VFM4_1_1"
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PTA0/IRQ_0/LLWU_P7")
				(number "30")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "31")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PTA2")
				(number "32")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PTA3")
				(number "7")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PTA4/LLWU_P0")
				(number "8")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PTA5/LLWU_P1/RTC_CLK_IN")
				(number "9")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PTA6/LLWU_P2")
				(number "10")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PTA7/IRQ_7/LLWU_P3")
				(number "15")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PTA8")
				(number "19")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PTA9")
				(number "20")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PTA10/IRQ_12")
				(number "21")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PTA11/IRQ_13")
				(number "22")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PTA12/IRQ_17/LPTMR0_ALT2")
				(number "26")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PTA13")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 5.08)
				(name "EPAD")
				(number "33")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 5.08)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 5.08)
				(name "VREFH")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 5.08)
				(name "VREFL")
				(number "5")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PTB0/IRQ_8/LLWU_P4")
				(number "16")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PTB1/IRQ_9")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PTB2/IRQ_10/LLWU_P5")
				(number "18")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PTB3/IRQ_14")
				(number "23")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PTB4/IRQ_15/LLWU_P6")
				(number "24")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PTB5/IRQ_16")
				(number "25")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PTB6/IRQ_2/LPTMR0_ALT3")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PTB7/IRQ_3")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PTB8")
				(number "11")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PTB9")
				(number "12")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PTB10")
				(number "13")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PTB11")
				(number "14")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PTB12")
				(number "28")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PTB13")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL04Z32VLC4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL04Z32VLC4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL04P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL04 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL04 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MKL04Z32VLC4_0_1")
		(symbol "MKL04Z32VLC4_1_1"
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PTA0/IRQ_0/LLWU_P7")
				(number "30")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "31")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PTA2")
				(number "32")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PTA3")
				(number "7")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PTA4/LLWU_P0")
				(number "8")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PTA5/LLWU_P1/RTC_CLK_IN")
				(number "9")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PTA6/LLWU_P2")
				(number "10")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PTA7/IRQ_7/LLWU_P3")
				(number "15")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PTA8")
				(number "19")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PTA9")
				(number "20")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PTA10/IRQ_12")
				(number "21")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PTA11/IRQ_13")
				(number "22")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PTA12/IRQ_17/LPTMR0_ALT2")
				(number "26")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PTA13")
				(number "27")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 5.08)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 5.08)
				(name "VREFH")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 5.08)
				(name "VREFL")
				(number "5")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PTB0/IRQ_8/LLWU_P4")
				(number "16")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PTB1/IRQ_9")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PTB2/IRQ_10/LLWU_P5")
				(number "18")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PTB3/IRQ_14")
				(number "23")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PTB4/IRQ_15/LLWU_P6")
				(number "24")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PTB5/IRQ_16")
				(number "25")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PTB6/IRQ_2/LPTMR0_ALT3")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PTB7/IRQ_3")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PTB8")
				(number "11")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PTB9")
				(number "12")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PTB10")
				(number "13")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PTB11")
				(number "14")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PTB12")
				(number "28")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PTB13")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL04Z32VLF4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL04Z32VLF4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL04P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL04 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL04 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL04Z32VLF4_0_1")
		(symbol "MKL04Z32VLF4_1_1"
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PTA0/IRQ_0/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "47")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PTA2")
				(number "48")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PTA3")
				(number "9")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PTA4/LLWU_P0")
				(number "10")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PTA5/LLWU_P1/RTC_CLK_IN")
				(number "14")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PTA6/LLWU_P2")
				(number "15")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PTA7/IRQ_7/LLWU_P3")
				(number "23")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PTA8")
				(number "27")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PTA9")
				(number "28")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PTA10/IRQ_12")
				(number "33")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PTA11/IRQ_13")
				(number "34")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PTA12/IRQ_17/LPTMR0_ALT2")
				(number "38")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PTA13")
				(number "39")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PTA14")
				(number "3")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PTA15")
				(number "4")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PTA16/IRQ_4")
				(number "18")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PTA17/IRQ_5")
				(number "19")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PTA18/IRQ_6")
				(number "20")
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PTA19")
				(number "41")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "11")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 5.08)
				(name "VREFH")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 5.08)
				(name "VREFL")
				(number "7")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PTB0/IRQ_8/LLWU_P4")
				(number "24")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PTB1/IRQ_9")
				(number "25")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PTB2/IRQ_10/LLWU_P5")
				(number "26")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PTB3/IRQ_14")
				(number "35")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PTB4/IRQ_15/LLWU_P6")
				(number "36")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PTB5/IRQ_16")
				(number "37")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PTB6/IRQ_2/LPTMR0_ALT3")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PTB7/IRQ_3")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PTB8")
				(number "16")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PTB9")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PTB10")
				(number "21")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PTB11")
				(number "22")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PTB12")
				(number "40")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PTB13")
				(number "45")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PTB14/IRQ_11")
				(number "32")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PTB15")
				(number "42")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PTB16")
				(number "43")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PTB17")
				(number "44")
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "PTB18")
				(number "12")
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PTB19")
				(number "13")
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PTB20")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL05Z32VFK4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL05Z32VFK4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL05P48M48SF1.pdf"
			(at 10.16 -45.72 0)
		)
		(property "Description" "Kinetis KL05 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL05 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL05Z32VFK4_0_1")
		(symbol "MKL05Z32VFK4_1_1"
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PTA0/IRQ_0/LLWU_P7")
				(number "22")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "23")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PTA3")
				(number "5")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PTA4/LLWU_P0")
				(number "6")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PTA5/LLWU_P1/RTC_CLK_IN")
				(number "7")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PTA6/LLWU_P2")
				(number "8")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PTA7/IRQ_7/LLWU_P3")
				(number "11")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PTA8")
				(number "15")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PTA9")
				(number "16")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PTA12/IRQ_17/LPTMR0_ALT2")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 5.08)
				(name "EPAD")
				(number "25")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 5.08)
				(name "VDD/VREFH")
				(number "3")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 5.08)
				(name "VSS/VREFL")
				(number "4")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PTB0/IRQ_8/LLWU_P4")
				(number "12")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PTB1/IRQ_9")
				(number "13")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PTB2/IRQ_10/LLWU_P5")
				(number "14")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PTB3/IRQ_14")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PTB4/IRQ_15/LLWU_P6")
				(number "18")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PTB5/IRQ_16")
				(number "19")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PTB6/IRQ_2/LPTMR0_ALT3")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PTB7/IRQ_3")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PTB10")
				(number "9")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PTB11")
				(number "10")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PTB13")
				(number "21")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL05Z32VFM4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL05Z32VFM4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL05P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL05 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL05 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL05Z32VFM4_0_1")
		(symbol "MKL05Z32VFM4_1_1"
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PTA0/IRQ_0/LLWU_P7")
				(number "30")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "31")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PTA2")
				(number "32")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PTA3")
				(number "7")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PTA4/LLWU_P0")
				(number "8")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PTA5/LLWU_P1/RTC_CLK_IN")
				(number "9")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PTA6/LLWU_P2")
				(number "10")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PTA7/IRQ_7/LLWU_P3")
				(number "15")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PTA8")
				(number "19")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PTA9")
				(number "20")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PTA10/IRQ_12")
				(number "21")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PTA11/IRQ_13")
				(number "22")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PTA12/IRQ_17/LPTMR0_ALT2")
				(number "26")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PTA13")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 5.08)
				(name "EPAD")
				(number "33")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 5.08)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 5.08)
				(name "VREFH")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 5.08)
				(name "VREFL")
				(number "5")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PTB0/IRQ_8/LLWU_P4")
				(number "16")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PTB1/IRQ_9")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PTB2/IRQ_10/LLWU_P5")
				(number "18")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PTB3/IRQ_14")
				(number "23")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PTB4/IRQ_15/LLWU_P6")
				(number "24")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PTB5/IRQ_16")
				(number "25")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PTB6/IRQ_2/LPTMR0_ALT3")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PTB7/IRQ_3")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PTB8")
				(number "11")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PTB9")
				(number "12")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PTB10")
				(number "13")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PTB11")
				(number "14")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PTB12")
				(number "28")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PTB13")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL05Z32VLC4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL05Z32VLC4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL05P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL05 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL05 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MKL05Z32VLC4_0_1")
		(symbol "MKL05Z32VLC4_1_1"
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PTA0/IRQ_0/LLWU_P7")
				(number "30")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "31")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PTA2")
				(number "32")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PTA3")
				(number "7")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PTA4/LLWU_P0")
				(number "8")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PTA5/LLWU_P1/RTC_CLK_IN")
				(number "9")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PTA6/LLWU_P2")
				(number "10")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PTA7/IRQ_7/LLWU_P3")
				(number "15")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PTA8")
				(number "19")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PTA9")
				(number "20")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PTA10/IRQ_12")
				(number "21")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PTA11/IRQ_13")
				(number "22")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PTA12/IRQ_17/LPTMR0_ALT2")
				(number "26")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PTA13")
				(number "27")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 5.08)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 5.08)
				(name "VREFH")
				(number "4")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 5.08)
				(name "VREFL")
				(number "5")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PTB0/IRQ_8/LLWU_P4")
				(number "16")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PTB1/IRQ_9")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PTB2/IRQ_10/LLWU_P5")
				(number "18")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PTB3/IRQ_14")
				(number "23")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PTB4/IRQ_15/LLWU_P6")
				(number "24")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PTB5/IRQ_16")
				(number "25")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PTB6/IRQ_2/LPTMR0_ALT3")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PTB7/IRQ_3")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PTB8")
				(number "11")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PTB9")
				(number "12")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PTB10")
				(number "13")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PTB11")
				(number "14")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PTB12")
				(number "28")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PTB13")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL05Z32VLF4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL05Z32VLF4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL05P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL05 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL05 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL05Z32VLF4_0_1")
		(symbol "MKL05Z32VLF4_1_1"
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 5.08)
				(name "PTA0/IRQ_0/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 5.08)
				(name "PTA1/IRQ_1/LPTMR0_ALT1")
				(number "47")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 5.08)
				(name "PTA2")
				(number "48")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 5.08)
				(name "PTA3")
				(number "9")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 5.08)
				(name "PTA4/LLWU_P0")
				(number "10")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 5.08)
				(name "PTA5/LLWU_P1/RTC_CLK_IN")
				(number "14")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 5.08)
				(name "PTA6/LLWU_P2")
				(number "15")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 5.08)
				(name "PTA7/IRQ_7/LLWU_P3")
				(number "23")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 5.08)
				(name "PTA8")
				(number "27")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 5.08)
				(name "PTA9")
				(number "28")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 5.08)
				(name "PTA10/IRQ_12")
				(number "33")
			)
			(pin bidirectional line
				(at -35.56 -2.54 0)
				(length 5.08)
				(name "PTA11/IRQ_13")
				(number "34")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 5.08)
				(name "PTA12/IRQ_17/LPTMR0_ALT2")
				(number "38")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 5.08)
				(name "PTA13")
				(number "39")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 5.08)
				(name "PTA14")
				(number "3")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 5.08)
				(name "PTA15")
				(number "4")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 5.08)
				(name "PTA16/IRQ_4")
				(number "18")
			)
			(pin bidirectional line
				(at -35.56 -17.78 0)
				(length 5.08)
				(name "PTA17/IRQ_5")
				(number "19")
			)
			(pin bidirectional line
				(at -35.56 -20.32 0)
				(length 5.08)
				(name "PTA18/IRQ_6")
				(number "20")
			)
			(pin bidirectional line
				(at -35.56 -22.86 0)
				(length 5.08)
				(name "PTA19")
				(number "41")
			)
			(pin passive line
				(at 0 45.72 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "31")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "11")
			)
			(pin passive line
				(at 0 -45.72 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 5.08)
				(name "VREFH")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 5.08)
				(name "VREFL")
				(number "7")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 5.08)
				(name "PTB0/IRQ_8/LLWU_P4")
				(number "24")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 5.08)
				(name "PTB1/IRQ_9")
				(number "25")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 5.08)
				(name "PTB2/IRQ_10/LLWU_P5")
				(number "26")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 5.08)
				(name "PTB3/IRQ_14")
				(number "35")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 5.08)
				(name "PTB4/IRQ_15/LLWU_P6")
				(number "36")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 5.08)
				(name "PTB5/IRQ_16")
				(number "37")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 5.08)
				(name "PTB6/IRQ_2/LPTMR0_ALT3")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 5.08)
				(name "PTB7/IRQ_3")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 5.08)
				(name "PTB8")
				(number "16")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 5.08)
				(name "PTB9")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 5.08)
				(name "PTB10")
				(number "21")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 5.08)
				(name "PTB11")
				(number "22")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 5.08)
				(name "PTB12")
				(number "40")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 5.08)
				(name "PTB13")
				(number "45")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 5.08)
				(name "PTB14/IRQ_11")
				(number "32")
			)
			(pin bidirectional line
				(at 35.56 -12.7 180)
				(length 5.08)
				(name "PTB15")
				(number "42")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 5.08)
				(name "PTB16")
				(number "43")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 5.08)
				(name "PTB17")
				(number "44")
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 5.08)
				(name "PTB18")
				(number "12")
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 5.08)
				(name "PTB19")
				(number "13")
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 5.08)
				(name "PTB20")
				(number "29")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL16Z128VFM4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL16Z128VFM4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL16P64M48SF5.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL16 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, I²S, TSI, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL16 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL16Z128VFM4_0_1")
		(symbol "MKL16Z128VFM4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "32")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL16Z128VFT4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL16Z128VFT4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL16P64M48SF5.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL16 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, I²S, TSI, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL16 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL16Z128VFT4_0_1")
		(symbol "MKL16Z128VFT4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB2")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB16")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB17")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTD0")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTD1")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PTD2")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PTD3")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "47")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "48")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "23")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VREFH")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VREFL")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC0")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE20")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE21")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE24")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE25")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE29")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL16Z128VLH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL16Z128VLH4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL16P64M48SF5.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL16 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, I²S, TSI, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL16 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL16Z128VLH4_0_1")
		(symbol "MKL16Z128VLH4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA12")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA13")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB2")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB16")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB17")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB18")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB19")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTD0")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTD1")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PTD2")
				(number "59")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PTD3")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "64")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VREFH")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VREFL")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC9")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTC10")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTC11")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE20")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE21")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE22")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE23")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE24")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE25")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE29")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE31")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL16Z256VLH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL16Z256VLH4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL16P64M48SF4.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL16 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, I²S, TSI, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL16 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL16Z256VLH4_0_1")
		(symbol "MKL16Z256VLH4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA12")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA13")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB2")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB16")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB17")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB18")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB19")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTD0")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTD1")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PTD2")
				(number "59")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PTD3")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "64")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VREFH")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VREFL")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC9")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTC10")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTC11")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE20")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE21")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE22")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE23")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE24")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE25")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE29")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE31")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL16Z256VMP4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL16Z256VMP4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-64_5.0x5.0mm_Layout8x8_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL16P64M48SF4.pdf"
			(at 5.08 -58.42 0)
		)
		(property "Description" "Kinetis KL16 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, I²S, TSI, MAPBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL16 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*5.0x5.0mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL16Z256VMP4_0_1")
		(symbol "MKL16Z256VMP4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "D3")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "D4")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "E5")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "D5")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "G5")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA5")
				(number "F5")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA12")
				(number "H6")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA13")
				(number "G6")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "H8")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "G8")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "F8")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "F7")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "F6")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB2")
				(number "E7")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "E8")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB16")
				(number "E6")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB17")
				(number "D7")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB18")
				(number "D6")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB19")
				(number "C7")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTD0")
				(number "C3")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTD1")
				(number "A4")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PTD2")
				(number "C2")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PTD3")
				(number "B3")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A3")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "C1")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "B2")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "A2")
			)
			(pin no_connect line
				(at -15.24 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "C5")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "E4")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "C4")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "F4")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "F3")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VREFH")
				(number "G4")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VREFL")
				(number "G3")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC0")
				(number "D8")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "C6")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "B7")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "C8")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "B8")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "A8")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "A7")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC8")
				(number "A6")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC9")
				(number "B5")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTC10")
				(number "B4")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTC11")
				(number "A5")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTE0")
				(number "A1")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTE1")
				(number "B1")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "E1")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "D1")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "E2")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "D2")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE20")
				(number "G1")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE21")
				(number "F1")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE22")
				(number "G2")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE23")
				(number "F2")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE24")
				(number "H4")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE25")
				(number "H5")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE29")
				(number "H1")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30")
				(number "H2")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE31")
				(number "H3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL17Z256CAL4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 36.195 0)
		)
		(property "Value" "MKL17Z256CAL4"
			(at 25.4 36.195 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-36_2.82x2.67mm_Layout6x6_P0.4mm"
			(at 3.81 -36.195 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF6.pdf"
			(at 96.52 50.8 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, FlexIO, WLCSP-36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.82x2.67mm*P0.4mm*"
			(at 0 0 0)
		)
		(symbol "MKL17Z256CAL4_0_1")
		(symbol "MKL17Z256CAL4_1_1"
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA0")
				(number "F5")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA1")
				(number "E4")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA2")
				(number "D4")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA3")
				(number "F4")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA4")
				(number "F3")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTA14")
				(number "E3")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTA15")
				(number "D3")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTA16")
				(number "C3")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTA17")
				(number "D2")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTA18")
				(number "F1")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTA19")
				(number "E1")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTA20")
				(number "D1")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "C2")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PTB1")
				(number "C1")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTE30")
				(number "E5")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 5.08)
				(name "VDD")
				(number "B3")
			)
			(pin passive line
				(at -2.54 40.64 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E2")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 5.08)
				(name "VSS")
				(number "C4")
			)
			(pin passive line
				(at -2.54 -40.64 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F2")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "E6")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "F6")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "B1")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC2")
				(number "B2")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "A1")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "A2")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "A3")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "B4")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTC7")
				(number "A4")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A5")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD5")
				(number "B5")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "A6")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD7")
				(number "B6")
			)
			(pin passive line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "Reserved")
				(number "C5")
			)
			(pin passive line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "Reserved")
				(number "C6")
			)
			(pin passive line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "Reserved")
				(number "D5")
			)
			(pin passive line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "Reserved")
				(number "D6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL17Z256VFM4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z256VFM4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF6.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, FlexIO, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL17Z256VFM4_0_1")
		(symbol "MKL17Z256VFM4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "32")
			)
			(pin power_in line
				(at -5.08 -53.34 90)
				(length 5.08)
				(name "EPAD")
				(number "33")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL17Z256VFT4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z256VFT4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF6.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, FlexIO, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL17Z256VFT4_0_1")
		(symbol "MKL17Z256VFT4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB2")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB16")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB17")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTD0")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTD1")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PTD2")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PTD3")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "47")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "48")
			)
			(pin power_in line
				(at -5.08 -53.34 90)
				(length 5.08)
				(name "EPAD")
				(number "49")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "23")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VREFH")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VREFL")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC0")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE20")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE21")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE24")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE25")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE29")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL17Z256VLH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z256VLH4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF6.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, FlexIO, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL17Z256VLH4_0_1")
		(symbol "MKL17Z256VLH4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA12")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA13")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB2")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB16")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB17")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB18")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB19")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTD0")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTD1")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PTD2")
				(number "59")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PTD3")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "64")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VREFH")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VREFL")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC9")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTC10")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTC11")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE20")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE21")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE22")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE23")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE24")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE25")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE29")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE31")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL17Z256VMP4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z256VMP4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-64_5.0x5.0mm_Layout8x8_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF6.pdf"
			(at 5.08 -58.42 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, FlexIO, MAPBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*5.0x5.0mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL17Z256VMP4_0_1")
		(symbol "MKL17Z256VMP4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "D3")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "D4")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "E5")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "D5")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "G5")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA5")
				(number "F5")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA12")
				(number "H6")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA13")
				(number "G6")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "H8")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "G8")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "F8")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "F7")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "F6")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB2")
				(number "E7")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "E8")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB16")
				(number "E6")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB17")
				(number "D7")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB18")
				(number "D6")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB19")
				(number "C7")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTD0")
				(number "C3")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTD1")
				(number "A4")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PTD2")
				(number "C2")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PTD3")
				(number "B3")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A3")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "C1")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "B2")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "A2")
			)
			(pin no_connect line
				(at -15.24 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "C5")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "E4")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "C4")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "F4")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "F3")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VREFH")
				(number "G4")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VREFL")
				(number "G3")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC0")
				(number "D8")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "C6")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "B7")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "C8")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "B8")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "A8")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "A7")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC8")
				(number "A6")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC9")
				(number "B5")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTC10")
				(number "B4")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTC11")
				(number "A5")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTE0")
				(number "A1")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTE1")
				(number "B1")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "E1")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "D1")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "E2")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "D2")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE20")
				(number "G1")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE21")
				(number "F1")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE22")
				(number "G2")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE23")
				(number "F2")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE24")
				(number "H4")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE25")
				(number "H5")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE29")
				(number "H1")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30")
				(number "H2")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE31")
				(number "H3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL17Z64VDA4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z64VDA4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-36_3.5x3.5mm_Layout6x6_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF2.pdf"
			(at 7.62 -60.96 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 16 kB SRAM, FlexIO, XFBGA-36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*3.5x3.5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL17Z64VDA4_0_1")
		(symbol "MKL17Z64VDA4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "F3")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "F4")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "E4")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "E5")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "F5")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "F6")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "E6")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "D5")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "D6")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "C6")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A3")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "B3")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "B2")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "A2")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "C3")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "C4")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "D3")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "D4")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "C5")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "B5")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "A6")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "A5")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "B4")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "A4")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTE0")
				(number "A1")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTE1")
				(number "B1")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "C2")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "C1")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "D1")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "D2")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE20")
				(number "E3")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE21")
				(number "E2")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE22")
				(number "E1")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE23")
				(number "F1")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30/VREF0")
				(number "F2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL17Z64VFM4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z64VFM4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF2.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 16 kB SRAM, FlexIO, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL17Z64VFM4_0_1")
		(symbol "MKL17Z64VFM4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "32")
			)
			(pin power_in line
				(at -5.08 -53.34 90)
				(length 5.08)
				(name "EPAD")
				(number "33")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30/VREF0")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL17Z64VFT4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z64VFT4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF6.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 16 kB SRAM, FlexIO, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL17Z64VFT4_0_1")
		(symbol "MKL17Z64VFT4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB2")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB16")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB17")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTD0")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTD1")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PTD2")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PTD3")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "47")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "48")
			)
			(pin power_in line
				(at -5.08 -53.34 90)
				(length 5.08)
				(name "EPAD")
				(number "49")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "23")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VREFH/VREFO")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VREFL")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC0")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE20")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE21")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE24")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE25")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE29")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL17Z64VLH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z64VLH4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF2.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 16 kB SRAM, FlexIO, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL17Z64VLH4_0_1")
		(symbol "MKL17Z64VLH4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA12")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA13")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB2")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB16")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB17")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB18")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB19")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTD0")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTD1")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PTD2")
				(number "59")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PTD3")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "64")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VREFH/VREFO")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VREFL")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC9")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTC10")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTC11")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE20")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE21")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE22")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE23")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE24")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE25")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE29")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE31")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL17Z64VMP4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z64VMP4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-64_5.0x5.0mm_Layout8x8_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF2.pdf"
			(at 5.08 -58.42 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 16 kB SRAM, FlexIO, MAPBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*5.0x5.0mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL17Z64VMP4_0_1")
		(symbol "MKL17Z64VMP4_1_1"
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA0")
				(number "D3")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA1")
				(number "D4")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA2")
				(number "E5")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA3")
				(number "D5")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA4")
				(number "G5")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA5")
				(number "F5")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA12")
				(number "H6")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA13")
				(number "G6")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA18")
				(number "H8")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA19")
				(number "G8")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA20")
				(number "F8")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "F7")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "F6")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB2")
				(number "E7")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "E8")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB16")
				(number "E6")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB17")
				(number "D7")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB18")
				(number "D6")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB19")
				(number "C7")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTD0")
				(number "C3")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTD1")
				(number "A4")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "PTD2")
				(number "C2")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PTD3")
				(number "B3")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A3")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTD5")
				(number "C1")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "B2")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTD7")
				(number "A2")
			)
			(pin no_connect line
				(at -15.24 -48.26 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "C5")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "E4")
			)
			(pin passive line
				(at -2.54 53.34 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "C4")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -53.34 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "F4")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "F3")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VREFH/VREFO")
				(number "G4")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VREFL")
				(number "G3")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC0")
				(number "D8")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "C6")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC2")
				(number "B7")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "C8")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "B8")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "A8")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "A7")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC8")
				(number "A6")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC9")
				(number "B5")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTC10")
				(number "B4")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTC11")
				(number "A5")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTE0")
				(number "A1")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTE1")
				(number "B1")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTE16")
				(number "E1")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTE17")
				(number "D1")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTE18")
				(number "E2")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE19")
				(number "D2")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE20")
				(number "G1")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE21")
				(number "F1")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE22")
				(number "G2")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE23")
				(number "F2")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE24")
				(number "H4")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE25")
				(number "H5")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE29")
				(number "H1")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE30")
				(number "H2")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE31")
				(number "H3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL24Z64VFM4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL24Z64VFM4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL24P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL24 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL24 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL24Z64VFM4_0_1")
		(symbol "MKL24Z64VFM4_1_1"
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA0")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA2")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA4")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA18")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA19")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA20")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB1")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "USB0_DP")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DM")
				(number "4")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VOUT33")
				(number "5")
			)
			(pin power_in line
				(at -7.62 66.04 270)
				(length 5.08)
				(name "VREGIN")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -66.04 90)
				(length 5.08)
				(name "EPAD")
				(number "33")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 5.08)
				(name "VDDA")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 5.08)
				(name "VSSA")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC2")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC7")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD7")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE30")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL24Z64VFT4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL24Z64VFT4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL24P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL24 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, USB FS Device/OTG, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL24 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL24Z64VFT4_0_1")
		(symbol "MKL24Z64VFT4_1_1"
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA0")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA1")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA2")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA3")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA4")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA18")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA19")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA20")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB1")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB2")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB16")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB17")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "USB0_DP")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DM")
				(number "4")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VOUT33")
				(number "5")
			)
			(pin power_in line
				(at -7.62 66.04 270)
				(length 5.08)
				(name "VREGIN")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -66.04 90)
				(length 5.08)
				(name "EPAD")
				(number "49")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "23")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 5.08)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 5.08)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 66.04 270)
				(length 5.08)
				(name "VREFH")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -66.04 90)
				(length 5.08)
				(name "VREFL")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PTC0")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC2")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC7")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD0")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD1")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD2")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD3")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD7")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE20")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE21")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE24")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE25")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE29")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE30")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL24Z64VLH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL24Z64VLH4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL24P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL24 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, USB FS Device/OTG, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL24 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL24Z64VLH4_0_1")
		(symbol "MKL24Z64VLH4_1_1"
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA3")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA4")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA12")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA13")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA18")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA19")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA20")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB2")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB16")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB17")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PTB18")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTB19")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "USB0_DP")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DM")
				(number "6")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VOUT33")
				(number "7")
			)
			(pin power_in line
				(at -7.62 66.04 270)
				(length 5.08)
				(name "VREGIN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at -2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 5.08)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 5.08)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 5.08 66.04 270)
				(length 5.08)
				(name "VREFH")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -66.04 90)
				(length 5.08)
				(name "VREFL")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC2")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC7")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC9")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC10")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC11")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD0")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD1")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD2")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD3")
				(number "60")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "62")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD7")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE20")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE21")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE22")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE23")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE24")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE25")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE29")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE30")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PTE31")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL24Z64VLK4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL24Z64VLK4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL24P80M48SF0.pdf"
			(at 7.62 -66.04 0)
		)
		(property "Description" "Kinetis KL24 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, USB FS Device/OTG, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL24 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL24Z64VLK4_0_1")
		(symbol "MKL24Z64VLK4_1_1"
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA1")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA2")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA3")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA4")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA5")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA12")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA13")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA14")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA15")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA16")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA17")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA18")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA19")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA20")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB1")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB2")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB8")
				(number "47")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB9")
				(number "48")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB10")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB11")
				(number "50")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB16")
				(number "51")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB17")
				(number "52")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PTB18")
				(number "53")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTB19")
				(number "54")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "USB0_DP")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DM")
				(number "10")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VOUT33")
				(number "11")
			)
			(pin power_in line
				(at -7.62 66.04 270)
				(length 5.08)
				(name "VREGIN")
				(number "12")
			)
			(pin passive line
				(at -2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "38")
			)
			(pin passive line
				(at -2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "60")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 5.08)
				(name "VDD")
				(number "7")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "39")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "59")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 5.08)
				(name "VDDA")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 66.04 270)
				(length 5.08)
				(name "VREFH")
				(number "18")
			)
			(pin power_in line
				(at 5.08 -66.04 90)
				(length 5.08)
				(name "VREFL")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PTC0")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC2")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "62")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC7")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC8")
				(number "65")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC9")
				(number "66")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC10")
				(number "67")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC11")
				(number "68")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC12")
				(number "69")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC13")
				(number "70")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC16")
				(number "71")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC17")
				(number "72")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD0")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD1")
				(number "74")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD2")
				(number "75")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD3")
				(number "76")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "77")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "78")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "79")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD7")
				(number "80")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE2")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE3")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE4")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE5")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE20")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE21")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE22")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE23")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE24")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE25")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE29")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE30")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PTE31")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL25Z128VFM4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL25Z128VFM4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL25P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL25 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL25 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL25Z128VFM4_0_1")
		(symbol "MKL25Z128VFM4_1_1"
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA0")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA2")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA4")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA18")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA19")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA20")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB1")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "USB0_DP")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DM")
				(number "4")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VOUT33")
				(number "5")
			)
			(pin power_in line
				(at -7.62 66.04 270)
				(length 5.08)
				(name "VREGIN")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -66.04 90)
				(length 5.08)
				(name "EPAD")
				(number "33")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 5.08)
				(name "VDDA")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 5.08)
				(name "VSSA")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC2")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC7")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD7")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE30")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL25Z128VFT4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL25Z128VFT4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL25P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL25 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device/OTG, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL25 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL25Z128VFT4_0_1")
		(symbol "MKL25Z128VFT4_1_1"
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA0")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA1")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA2")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA3")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA4")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA18")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA19")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA20")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB1")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB2")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB16")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB17")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "USB0_DP")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DM")
				(number "4")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VOUT33")
				(number "5")
			)
			(pin power_in line
				(at -7.62 66.04 270)
				(length 5.08)
				(name "VREGIN")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -66.04 90)
				(length 5.08)
				(name "EPAD")
				(number "49")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "23")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 5.08)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 5.08)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 66.04 270)
				(length 5.08)
				(name "VREFH")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -66.04 90)
				(length 5.08)
				(name "VREFL")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PTC0")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC2")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC7")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD0")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD1")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD2")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD3")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD7")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE20")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE21")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE24")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE25")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE29")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE30")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL25Z128VLH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL25Z128VLH4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL25P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL25 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device/OTG, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL25 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL25Z128VLH4_0_1")
		(symbol "MKL25Z128VLH4_1_1"
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA3")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA4")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA12")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA13")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA18")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA19")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA20")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB2")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB16")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB17")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PTB18")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTB19")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "USB0_DP")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DM")
				(number "6")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VOUT33")
				(number "7")
			)
			(pin power_in line
				(at -7.62 66.04 270)
				(length 5.08)
				(name "VREGIN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at -2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 5.08)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 5.08)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 5.08 66.04 270)
				(length 5.08)
				(name "VREFH")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -66.04 90)
				(length 5.08)
				(name "VREFL")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC2")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC7")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC9")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC10")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC11")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD0")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD1")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD2")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD3")
				(number "60")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "62")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD7")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE20")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE21")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE22")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE23")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE24")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE25")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE29")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE30")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PTE31")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL25Z128VLK4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL25Z128VLK4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL25P80M48SF0.pdf"
			(at 7.62 -66.04 0)
		)
		(property "Description" "Kinetis KL25 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device/OTG, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL25 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL25Z128VLK4_0_1")
		(symbol "MKL25Z128VLK4_1_1"
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA1")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA2")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA3")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA4")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA5")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA12")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA13")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA14")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA15")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA16")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA17")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA18")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA19")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA20")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB1")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB2")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB8")
				(number "47")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB9")
				(number "48")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB10")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB11")
				(number "50")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB16")
				(number "51")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB17")
				(number "52")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PTB18")
				(number "53")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTB19")
				(number "54")
			)
			(pin bidirectional line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "USB0_DP")
				(number "9")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DM")
				(number "10")
			)
			(pin power_out line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "VOUT33")
				(number "11")
			)
			(pin power_in line
				(at -7.62 66.04 270)
				(length 5.08)
				(name "VREGIN")
				(number "12")
			)
			(pin passive line
				(at -2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "38")
			)
			(pin passive line
				(at -2.54 66.04 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "60")
			)
			(pin power_in line
				(at -2.54 66.04 270)
				(length 5.08)
				(name "VDD")
				(number "7")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "39")
			)
			(pin passive line
				(at -2.54 -66.04 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "59")
			)
			(pin power_in line
				(at -2.54 -66.04 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 66.04 270)
				(length 5.08)
				(name "VDDA")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -66.04 90)
				(length 5.08)
				(name "VSSA")
				(number "20")
			)
			(pin power_in line
				(at 5.08 66.04 270)
				(length 5.08)
				(name "VREFH")
				(number "18")
			)
			(pin power_in line
				(at 5.08 -66.04 90)
				(length 5.08)
				(name "VREFL")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PTC0")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC2")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "62")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC7")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC8")
				(number "65")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC9")
				(number "66")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC10")
				(number "67")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC11")
				(number "68")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC12")
				(number "69")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC13")
				(number "70")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC16")
				(number "71")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC17")
				(number "72")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD0")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD1")
				(number "74")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD2")
				(number "75")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD3")
				(number "76")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "77")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "78")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "79")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD7")
				(number "80")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE2")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE3")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE4")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE5")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE20")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE21")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE22")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE23")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE24")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE25")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE29")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE30")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PTE31")
				(number "23")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL26Z128CAL4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 38.735 0)
		)
		(property "Value" "MKL26Z128CAL4"
			(at 25.4 38.735 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-36_2.374x2.459mm_Layout6x6_P0.35mm"
			(at 3.81 -38.735 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P36M48SF5.pdf"
			(at 96.52 50.8 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device/OTG, WLCSP-36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*2.374x2.459mm*P0.35mm*"
			(at 0 0 0)
		)
		(symbol "MKL26Z128CAL4_0_1")
		(symbol "MKL26Z128CAL4_1_1"
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA0")
				(number "F5")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA1")
				(number "E4")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA2")
				(number "F4")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA3")
				(number "E3")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA4")
				(number "F3")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTA18")
				(number "F1")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTA19")
				(number "E1")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTA20")
				(number "D1")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "C2")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB1")
				(number "C1")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "USB0_DP")
				(number "C4")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "USB0_DM")
				(number "C5")
			)
			(pin power_out line
				(at -30.48 -22.86 0)
				(length 5.08)
				(name "VOUT33")
				(number "C6")
			)
			(pin power_in line
				(at -7.62 43.18 270)
				(length 5.08)
				(name "VREGIN")
				(number "D4")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 5.08)
				(name "VDD")
				(number "F2")
			)
			(pin power_in line
				(at -2.54 -43.18 90)
				(length 5.08)
				(name "VSS")
				(number "C3")
			)
			(pin passive line
				(at -2.54 -43.18 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E2")
			)
			(pin power_in line
				(at 2.54 43.18 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "E6")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "F6")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "B1")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC2")
				(number "B2")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "B3")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "A1")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "B4")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "A2")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTC7")
				(number "A3")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A4")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD5")
				(number "A5")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "B5")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD7")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTE0")
				(number "A6")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE16")
				(number "D5")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE17")
				(number "D6")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE18")
				(number "D3")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE19")
				(number "D2")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE30")
				(number "E5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL26Z128VFM4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL26Z128VFM4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P64M48SF5.pdf"
			(at 12.7 -68.58 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL26Z128VFM4_0_1")
		(symbol "MKL26Z128VFM4_1_1"
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA0")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA2")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA4")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA18")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA19")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA20")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB1")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "USB0_DP")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "USB0_DM")
				(number "4")
			)
			(pin power_out line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "VOUT33")
				(number "5")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 5.08)
				(name "VREGIN")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -55.88 90)
				(length 5.08)
				(name "EPAD")
				(number "33")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VDDA")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC2")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC7")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD5")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTD7")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE30")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL26Z128VFT4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL26Z128VFT4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P64M48SF5.pdf"
			(at 7.62 -58.42 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device/OTG, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL26Z128VFT4_0_1")
		(symbol "MKL26Z128VFT4_1_1"
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA0")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA1")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA2")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA3")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA4")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA18")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA19")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA20")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB1")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB2")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB3")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "USB0_DP")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "USB0_DM")
				(number "4")
			)
			(pin power_out line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "VOUT33")
				(number "5")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 5.08)
				(name "VREGIN")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -55.88 90)
				(length 5.08)
				(name "EPAD")
				(number "49")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "23")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 5.08)
				(name "VREFH")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 5.08)
				(name "VREFL")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC0")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC2")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC7")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD0")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD1")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD2")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD3")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD5")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTD7")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE20")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE21")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE24")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE25")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE29")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE30")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL26Z128VLH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL26Z128VLH4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P64M48SF5.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device/OTG, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL26Z128VLH4_0_1")
		(symbol "MKL26Z128VLH4_1_1"
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA3")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA4")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA12")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA13")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA18")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA19")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA20")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB2")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB3")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB18")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB19")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "USB0_DP")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "USB0_DM")
				(number "6")
			)
			(pin power_out line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "VOUT33")
				(number "7")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 5.08)
				(name "VREGIN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 5.08)
				(name "VREFH")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 5.08)
				(name "VREFL")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC2")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC7")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC9")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC10")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTC11")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD0")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD1")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD2")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD3")
				(number "60")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD5")
				(number "62")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTD7")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE20")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE21")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE22")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE23")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE24")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE25")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE29")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE30")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE31")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL26Z256VLH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL26Z256VLH4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P121M48SF4.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, USB FS Device/OTG, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL26Z256VLH4_0_1")
		(symbol "MKL26Z256VLH4_1_1"
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA3")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA4")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA12")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA13")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA18")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA19")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA20")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB2")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB3")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB18")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB19")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "USB0_DP")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "USB0_DM")
				(number "6")
			)
			(pin power_out line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "VOUT33")
				(number "7")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 5.08)
				(name "VREGIN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 5.08)
				(name "VREFH")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 5.08)
				(name "VREFL")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC2")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC7")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC9")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC10")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTC11")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD0")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD1")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD2")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD3")
				(number "60")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD5")
				(number "62")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTD7")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE20")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE21")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE22")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE23")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE24")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE25")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE29")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE30")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE31")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL26Z256VLL4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 86.995 0)
		)
		(property "Value" "MKL26Z256VLL4"
			(at 25.4 86.995 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 6.35 -86.995 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P121M48SF4.pdf"
			(at 7.62 -91.44 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, USB FS Device/OTG, LQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL26Z256VLL4_0_1")
		(symbol "MKL26Z256VLL4_1_1"
			(pin bidirectional line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "PTA0")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "PTA1")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "PTA2")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "PTA3")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PTA4")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PTA5")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PTA6")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PTA7")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA12")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA13")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA14")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA15")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA16")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA17")
				(number "47")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA18")
				(number "50")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA19")
				(number "51")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA20")
				(number "52")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "53")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTB1")
				(number "54")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTB2")
				(number "55")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTB3")
				(number "56")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB7")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB8")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB9")
				(number "59")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB10")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB11")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB18")
				(number "64")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB19")
				(number "65")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB20")
				(number "66")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PTB21")
				(number "67")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTB22")
				(number "68")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTB23")
				(number "69")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DP")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "USB0_DM")
				(number "11")
			)
			(pin power_out line
				(at -30.48 -76.2 0)
				(length 5.08)
				(name "VOUT33")
				(number "12")
			)
			(pin no_connect line
				(at -25.4 -63.5 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "86")
			)
			(pin no_connect line
				(at -25.4 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "87")
			)
			(pin no_connect line
				(at -25.4 -68.58 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "88")
			)
			(pin no_connect line
				(at -25.4 -71.12 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "89")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VREGIN")
				(number "13")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "8")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "29")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin power_in line
				(at -2.54 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "25")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VREFH")
				(number "23")
			)
			(pin power_in line
				(at 5.08 -91.44 90)
				(length 5.08)
				(name "VREFL")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PTC0")
				(number "70")
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "71")
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PTC2")
				(number "72")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "76")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "77")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "78")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PTC7")
				(number "79")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PTC8")
				(number "80")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PTC9")
				(number "81")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PTC10")
				(number "82")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC11")
				(number "83")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC12")
				(number "84")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC13")
				(number "85")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC16")
				(number "90")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC17")
				(number "91")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC18")
				(number "92")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTD0")
				(number "93")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTD1")
				(number "94")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTD2")
				(number "95")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTD3")
				(number "96")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "97")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "98")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "99")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD7")
				(number "100")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE2")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE3")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE4")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE5")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE6")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE16")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE17")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE18")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PTE19")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PTE20")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PTE21")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PTE22")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PTE23")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PTE24")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PTE25")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PTE26")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PTE29")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PTE30")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PTE31")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL26Z256VMC4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 86.995 0)
		)
		(property "Value" "MKL26Z256VMC4"
			(at 25.4 86.995 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-121_8x8mm_Layout11x11_P0.65mm"
			(at 6.35 -86.995 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P121M48SF4.pdf"
			(at 7.62 -93.98 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, USB FS Device/OTG, XFBGA-121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MKL26Z256VMC4_0_1")
		(symbol "MKL26Z256VMC4_1_1"
			(pin bidirectional line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "PTA0")
				(number "J6")
			)
			(pin bidirectional line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "PTA1")
				(number "H8")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "PTA2")
				(number "J7")
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "PTA3")
				(number "H9")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PTA4")
				(number "J8")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PTA5")
				(number "K7")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PTA6")
				(number "K3")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PTA7")
				(number "H4")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA12")
				(number "K8")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA13/LLWU_P4")
				(number "L8")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA14")
				(number "K9")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA15")
				(number "L9")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA16")
				(number "J10")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA17")
				(number "H10")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA18")
				(number "L11")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA19")
				(number "K11")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA20")
				(number "J11")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "G11")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTB1")
				(number "G10")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTB2")
				(number "G9")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTB3")
				(number "G8")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB7")
				(number "E11")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB8")
				(number "D11")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB9")
				(number "E10")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB10")
				(number "D10")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB11")
				(number "C10")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "B10")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "E9")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB18")
				(number "D9")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB19")
				(number "C9")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB20")
				(number "F10")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PTB21")
				(number "F9")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTB22")
				(number "F8")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTB23")
				(number "E8")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DP")
				(number "F1")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "USB0_DM")
				(number "F2")
			)
			(pin power_out line
				(at -30.48 -76.2 0)
				(length 5.08)
				(name "VOUT33")
				(number "G1")
			)
			(pin no_connect line
				(at -25.4 55.88 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "J9")
			)
			(pin no_connect line
				(at -25.4 53.34 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "J4")
			)
			(pin no_connect line
				(at -25.4 27.94 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "H11")
			)
			(pin no_connect line
				(at -25.4 12.7 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "F11")
			)
			(pin no_connect line
				(at -25.4 -63.5 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "H3")
			)
			(pin no_connect line
				(at -25.4 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "J3")
			)
			(pin no_connect line
				(at -25.4 -68.58 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "K4")
			)
			(pin no_connect line
				(at -25.4 -71.12 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "L7")
			)
			(pin no_connect line
				(at -15.24 -86.36 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A11")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VREGIN")
				(number "G2")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "E5")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E6")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E7")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "K6")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "L10")
			)
			(pin power_in line
				(at -2.54 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G3")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L5")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L6")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "F5")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "F6")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VREFH")
				(number "G5")
			)
			(pin power_in line
				(at 5.08 -91.44 90)
				(length 5.08)
				(name "VREFL")
				(number "G6")
			)
			(pin no_connect line
				(at 25.4 40.64 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A5")
			)
			(pin no_connect line
				(at 25.4 38.1 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B5")
			)
			(pin no_connect line
				(at 25.4 27.94 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A4")
			)
			(pin no_connect line
				(at 25.4 -7.62 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B1")
			)
			(pin no_connect line
				(at 25.4 -10.16 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "C2")
			)
			(pin no_connect line
				(at 25.4 -12.7 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "C1")
			)
			(pin no_connect line
				(at 25.4 -15.24 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "D2")
			)
			(pin no_connect line
				(at 25.4 -17.78 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "D1")
			)
			(pin no_connect line
				(at 25.4 -20.32 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "E1")
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PTC0")
				(number "B9")
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "D8")
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PTC2")
				(number "C8")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "B8")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "A8")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "D7")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "C7")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PTC7")
				(number "B7")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PTC8")
				(number "A7")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PTC9")
				(number "D6")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PTC10")
				(number "C6")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC11")
				(number "C5")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC12")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC13")
				(number "A6")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC16")
				(number "D5")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC17")
				(number "C4")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC18")
				(number "B4")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC20")
				(number "A10")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC21")
				(number "A9")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC22")
				(number "B11")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC23")
				(number "C11")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTD0")
				(number "D4")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTD1")
				(number "D3")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD2")
				(number "C3")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD3")
				(number "B3")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A3")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD5")
				(number "A2")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "B2")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD7")
				(number "A1")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE0")
				(number "E4")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE1")
				(number "E3")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE2")
				(number "E2")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE3")
				(number "F4")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE4")
				(number "H7")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE5")
				(number "G4")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE6")
				(number "F3")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE16")
				(number "H1")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE17")
				(number "H2")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE18")
				(number "J1")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PTE19")
				(number "J2")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PTE20")
				(number "K1")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PTE21")
				(number "K2")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PTE22")
				(number "L1")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PTE23")
				(number "L2")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PTE24")
				(number "H5")
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PTE25")
				(number "J5")
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PTE26")
				(number "H6")
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PTE29")
				(number "L3")
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PTE30")
				(number "K5")
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PTE31")
				(number "L4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL26Z256VMP4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 86.995 0)
		)
		(property "Value" "MKL26Z256VMP4"
			(at 25.4 86.995 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-64_5.0x5.0mm_Layout8x8_P0.5mm"
			(at 6.35 -86.995 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P121M48SF4.pdf"
			(at 5.08 -96.52 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, USB FS Device/OTG, XFBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*5.0x5.0mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL26Z256VMP4_0_1")
		(symbol "MKL26Z256VMP4_1_1"
			(pin bidirectional line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "PTA0")
				(number "D3")
			)
			(pin bidirectional line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "PTA1")
				(number "D4")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "PTA2")
				(number "E5")
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "PTA3")
				(number "D5")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PTA4")
				(number "G5")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PTA5")
				(number "F5")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA12")
				(number "H6")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA13")
				(number "G6")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA18")
				(number "H8")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA19")
				(number "G8")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA20")
				(number "F8")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "F7")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTB1")
				(number "F6")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTB2")
				(number "E7")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTB3")
				(number "E8")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "E6")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "D7")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB18")
				(number "D6")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB19")
				(number "C7")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DP")
				(number "E1")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "USB0_DM")
				(number "D1")
			)
			(pin power_out line
				(at -30.48 -76.2 0)
				(length 5.08)
				(name "VOUT33")
				(number "E2")
			)
			(pin no_connect line
				(at -15.24 -86.36 90)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "C5")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VREGIN")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "E4")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at -2.54 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "C4")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "F4")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "F3")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VREFH")
				(number "G4")
			)
			(pin power_in line
				(at 5.08 -91.44 90)
				(length 5.08)
				(name "VREFL")
				(number "G3")
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PTC0")
				(number "D8")
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "C6")
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PTC2")
				(number "B7")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "C8")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "B8")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "A8")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "A7")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PTC7")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PTC8")
				(number "A6")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PTC9")
				(number "B5")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PTC10")
				(number "B4")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC11")
				(number "A5")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTD0")
				(number "C3")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTD1")
				(number "A4")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD2")
				(number "C2")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD3")
				(number "B3")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A3")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD5")
				(number "C1")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "B2")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD7")
				(number "A2")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE0")
				(number "A1")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE1")
				(number "B1")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PTE20")
				(number "G1")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PTE21")
				(number "F1")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PTE22")
				(number "G2")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PTE23")
				(number "F2")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PTE24")
				(number "H4")
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PTE25")
				(number "H5")
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PTE29")
				(number "H1")
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PTE30")
				(number "H2")
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PTE31")
				(number "H3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL27Z256VFT4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL27Z256VFT4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 8.89 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF6.pdf"
			(at 10.16 -55.88 0)
		)
		(property "Description" "Kinetis KL27 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, USB FS Device (xtal-less)/OTG, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL27Z256VFT4_0_1")
		(symbol "MKL27Z256VFT4_1_1"
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA0")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA1")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA2")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA3")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA4")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA18")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA19")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA20")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB1")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB2")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB3")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "USB0_DP")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "USB0_DM")
				(number "4")
			)
			(pin power_out line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "VOUT33")
				(number "5")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 5.08)
				(name "VREGIN")
				(number "6")
			)
			(pin power_in line
				(at -5.08 -55.88 90)
				(length 5.08)
				(name "EPAD")
				(number "49")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "23")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 5.08)
				(name "VREFH")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 5.08)
				(name "VREFL")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC0")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC2")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC7")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD0")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD1")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD2")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD3")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD5")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTD7")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE20")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE21")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE24")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE25")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE29")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE30")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL27Z256VLH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL27Z256VLH4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF6.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL27 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, USB FS Device (xtal-less)/OTG, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL27Z256VLH4_0_1")
		(symbol "MKL27Z256VLH4_1_1"
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA3")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA4")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA12")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA13")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA18")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA19")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA20")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB2")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB3")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB18")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB19")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "USB0_DP")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "USB0_DM")
				(number "6")
			)
			(pin power_out line
				(at -30.48 -45.72 0)
				(length 5.08)
				(name "VOUT33")
				(number "7")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 5.08)
				(name "VREGIN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 5.08)
				(name "VREFH")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 5.08)
				(name "VREFL")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC2")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC7")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC9")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC10")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTC11")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD0")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD1")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD2")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD3")
				(number "60")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD5")
				(number "62")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTD7")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE20")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE21")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE22")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE23")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE24")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE25")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE29")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE30")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE31")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL27Z64VFM4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL27Z64VFM4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF2.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL27 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 16 kB SRAM, USB FS Device (xtal-less)/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL27Z64VFM4_0_1")
		(symbol "MKL27Z64VFM4_1_1"
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA0")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA1")
				(number "11")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA2")
				(number "12")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA4")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA18")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA19")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA20")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB1")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "USB0_DP")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "USB0_DM")
				(number "4")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 5.08)
				(name "USB_VDD")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -55.88 90)
				(length 5.08)
				(name "EPAD")
				(number "33")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "22")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC2")
				(number "23")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "25")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC7")
				(number "28")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "29")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD5")
				(number "30")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTD7")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE16")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE30/VREF0")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL27Z64VFT4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL27Z64VFT4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF2.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL27 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 16 kB SRAM, USB FS Device (xtal-less)/OTG, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL27Z64VFT4_0_1")
		(symbol "MKL27Z64VFT4_1_1"
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA0")
				(number "17")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA1")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA2")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA3")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA4")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA18")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA19")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA20")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB1")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB2")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB3")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "USB0_DP")
				(number "3")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "USB0_DM")
				(number "4")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 5.08)
				(name "USB_VDD")
				(number "5")
			)
			(pin power_in line
				(at -5.08 -55.88 90)
				(length 5.08)
				(name "EPAD")
				(number "49")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "23")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 5.08)
				(name "VREFH/VREFO")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 5.08)
				(name "VREFL")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC0")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "34")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC2")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC7")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD0")
				(number "41")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD1")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD2")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD3")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD5")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTD7")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE16")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE20")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE21")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE24")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE25")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE29")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE30")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL27Z64VLH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL27Z64VLH4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF2.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL27 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 16 kB SRAM, USB FS Device (xtal-less)/OTG, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL27Z64VLH4_0_1")
		(symbol "MKL27Z64VLH4_1_1"
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA3")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA4")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA12")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA13")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA18")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA19")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTA20")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB2")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB3")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB18")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB19")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "USB0_DP")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "USB0_DM")
				(number "6")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 5.08)
				(name "USB_VDD")
				(number "7")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 5.08)
				(name "VREFH/VREFO")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 5.08)
				(name "VREFL")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC2")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC7")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC9")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTC10")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTC11")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD0")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD1")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD2")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD3")
				(number "60")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD5")
				(number "62")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTD7")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE16")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE20")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE21")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE22")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE23")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE24")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE25")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE29")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE30")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE31")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL28Z512VDC7"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 94.615 0)
		)
		(property "Value" "MKL28Z512VDC7"
			(at 25.4 94.615 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-121_8x8mm_Layout11x11_P0.65mm"
			(at 8.89 -94.615 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/MKL28Z512Vxx7.pdf"
			(at 10.16 -99.06 0)
		)
		(property "Description" "Kinetis KL28 series, 72...96-MHz/32-bit ARM Cortex-M0+, 512 kB flash, 128 kB SRAM, USB FS Device (xtal-less), XFBGA-121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL28 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MKL28Z512VDC7_0_1")
		(symbol "MKL28Z512VDC7_1_1"
			(pin bidirectional line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "PTA0")
				(number "J6")
			)
			(pin bidirectional line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "PTA1")
				(number "H8")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "PTA2")
				(number "J7")
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "PTA3")
				(number "H9")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PTA4/LLWU_P3")
				(number "J8")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PTA5")
				(number "K7")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PTA6")
				(number "K3")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PTA7")
				(number "H4")
			)
			(pin bidirectional line
				(at -30.48 55.88 0)
				(length 5.08)
				(name "PTA10/LLWU_P22")
				(number "J9")
			)
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PTA11/LLWU_P23")
				(number "J4")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA12")
				(number "K8")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA13/LLWU_P4")
				(number "L8")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA14")
				(number "K9")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA15")
				(number "L9")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA16")
				(number "J10")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA17")
				(number "H10")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA18")
				(number "L11")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA19")
				(number "K11")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA20")
				(number "J11")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA29")
				(number "H11")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "G11")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTB1")
				(number "G10")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTB2")
				(number "G9")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTB3")
				(number "G8")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTB6")
				(number "F11")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB7")
				(number "E11")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB8")
				(number "D11")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB9")
				(number "E10")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB10")
				(number "D10")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB11")
				(number "C10")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "B10")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "E9")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB18")
				(number "D9")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB19")
				(number "C9")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB20")
				(number "F10")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PTB21")
				(number "F9")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTB22")
				(number "F8")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTB23")
				(number "E8")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DP")
				(number "F1")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "USB0_DM")
				(number "F2")
			)
			(pin power_out line
				(at -30.48 -76.2 0)
				(length 5.08)
				(name "VOUT33")
				(number "G1")
			)
			(pin no_connect line
				(at -25.4 -63.5 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "H3")
			)
			(pin no_connect line
				(at -25.4 -66.04 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "J3")
			)
			(pin no_connect line
				(at -25.4 -68.58 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "K4")
			)
			(pin no_connect line
				(at -25.4 -71.12 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "L7")
			)
			(pin power_in line
				(at -5.08 99.06 270)
				(length 5.08)
				(name "VREGIN")
				(number "G2")
			)
			(pin power_in line
				(at 0 99.06 270)
				(length 5.08)
				(name "VDD")
				(number "E5")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E6")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E7")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "K6")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "L10")
			)
			(pin power_in line
				(at 0 -99.06 90)
				(length 5.08)
				(name "VSS")
				(number "A11")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G3")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L5")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L6")
			)
			(pin power_in line
				(at 5.08 99.06 270)
				(length 5.08)
				(name "VDDA")
				(number "F5")
			)
			(pin power_in line
				(at 5.08 -99.06 90)
				(length 5.08)
				(name "VSSA")
				(number "F6")
			)
			(pin power_in line
				(at 7.62 99.06 270)
				(length 5.08)
				(name "VREFH/VREF_OUT")
				(number "G5")
			)
			(pin power_in line
				(at 7.62 -99.06 90)
				(length 5.08)
				(name "VREFL")
				(number "G6")
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PTC0")
				(number "B9")
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "D8")
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PTC2")
				(number "C8")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "B8")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "A8")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "D7")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "C7")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PTC7")
				(number "B7")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PTC8")
				(number "A7")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PTC9")
				(number "D6")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PTC10")
				(number "C6")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC11/LLWU_P11")
				(number "C5")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC12")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC13")
				(number "A6")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTC14")
				(number "A5")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC15")
				(number "B5")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC16")
				(number "D5")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC17")
				(number "C4")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC18")
				(number "B4")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC19")
				(number "A4")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC22")
				(number "B11")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC23")
				(number "C11")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTD0/LLWU_P12")
				(number "D4")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTD1")
				(number "D3")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTD2/LLWU_P13")
				(number "C3")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTD3")
				(number "B3")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A3")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "A2")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "B2")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD7")
				(number "A1")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD8/LLWU_P24")
				(number "A10")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD9")
				(number "A9")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD10")
				(number "B1")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD11/LLWU_P25")
				(number "C2")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTD12")
				(number "C1")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTD13")
				(number "D2")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTD14")
				(number "D1")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTD15")
				(number "E1")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE0")
				(number "E4")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE1/LLWU_P0")
				(number "E3")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE2/LLWU_P1")
				(number "E2")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE3")
				(number "F4")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE4/LLWU_P2")
				(number "H7")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE5")
				(number "G4")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE6/LLWU_P16")
				(number "F3")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE16")
				(number "H1")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE17/LLWU_P19")
				(number "H2")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE18/LLWU_P20")
				(number "J1")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PTE19")
				(number "J2")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PTE20")
				(number "K1")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PTE21")
				(number "K2")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PTE22")
				(number "L1")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PTE23")
				(number "L2")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PTE24")
				(number "H5")
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PTE25/LLWU_P21")
				(number "J5")
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PTE26")
				(number "H6")
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PTE29")
				(number "L3")
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PTE30")
				(number "K5")
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PTE31")
				(number "L4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL28Z512VLL7"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 94.615 0)
		)
		(property "Value" "MKL28Z512VLL7"
			(at 25.4 94.615 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 8.89 -94.615 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/MKL28Z512Vxx7.pdf"
			(at 10.16 -99.06 0)
		)
		(property "Description" "Kinetis KL28 series, 72...96-MHz/32-bit ARM Cortex-M0+, 512 kB flash, 128 kB SRAM, USB FS Device (xtal-less), LQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL28 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL28Z512VLL7_0_1")
		(symbol "MKL28Z512VLL7_1_1"
			(pin bidirectional line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "PTA0")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "PTA1")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "PTA2")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "PTA3")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PTA4/LLWU_P3")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PTA5")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PTA6")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PTA7")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA12")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA13/LLWU_P4")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA14")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA15")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA16")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA17")
				(number "47")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA18")
				(number "50")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA19")
				(number "51")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA20")
				(number "52")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "53")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTB1")
				(number "54")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTB2")
				(number "55")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTB3")
				(number "56")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB7")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB8")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB9")
				(number "59")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB10")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB11")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB18")
				(number "64")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB19")
				(number "65")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB20")
				(number "66")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PTB21")
				(number "67")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTB22")
				(number "68")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTB23")
				(number "69")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DP")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "USB0_DM")
				(number "11")
			)
			(pin power_out line
				(at -30.48 -76.2 0)
				(length 5.08)
				(name "VOUT33")
				(number "12")
			)
			(pin power_in line
				(at -5.08 99.06 270)
				(length 5.08)
				(name "VREGIN")
				(number "13")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "75")
			)
			(pin power_in line
				(at 0 99.06 270)
				(length 5.08)
				(name "VDD")
				(number "8")
			)
			(pin passive line
				(at 0 99.06 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "89")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "29")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin passive line
				(at 0 -99.06 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "88")
			)
			(pin power_in line
				(at 0 -99.06 90)
				(length 5.08)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 5.08 99.06 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 5.08 -99.06 90)
				(length 5.08)
				(name "VSSA")
				(number "25")
			)
			(pin power_in line
				(at 7.62 99.06 270)
				(length 5.08)
				(name "VREFH/VREF_OUT")
				(number "23")
			)
			(pin power_in line
				(at 7.62 -99.06 90)
				(length 5.08)
				(name "VREFL")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PTC0")
				(number "70")
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PTC1/LLWU_P6")
				(number "71")
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PTC2")
				(number "72")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "76")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "77")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "78")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PTC7")
				(number "79")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PTC8")
				(number "80")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PTC9")
				(number "81")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PTC10")
				(number "82")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC11/LLWU_P11")
				(number "83")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC12")
				(number "84")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC13")
				(number "85")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTC14")
				(number "86")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC15")
				(number "87")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC16")
				(number "90")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC17")
				(number "91")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC18")
				(number "92")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTD0/LLWU_P12")
				(number "93")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTD1")
				(number "94")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTD2/LLWU_P13")
				(number "95")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTD3")
				(number "96")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "97")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "98")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "99")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD7")
				(number "100")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE1/LLWU_P0")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE2/LLWU_P1")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE3")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE4/LLWU_P2")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE5")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE6/LLWU_P16")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE16")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE17/LLWU_P19")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE18/LLWU_P20")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PTE19")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PTE20")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PTE21")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PTE22")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PTE23")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PTE24")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PTE25/LLWU_P21")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PTE26")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PTE29")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PTE30")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PTE31")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL43Z256VLH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL43Z256VLH4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL43P64M48SF6.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL43 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, USB FS Device (xtal-less), Segment LCD, FlexIO, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL43 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL43Z256VLH4_0_1")
		(symbol "MKL43Z256VLH4_1_1"
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA3")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA4")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA12")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA13")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA18")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA19")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA20")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB2")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB16")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB17")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB18")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB19")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "USB0_DP")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "USB0_DM")
				(number "6")
			)
			(pin power_out line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "VOUT33")
				(number "7")
			)
			(pin passive line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "VCAP1/PTC23")
				(number "52")
			)
			(pin passive line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "VCAP2/PTC22")
				(number "51")
			)
			(pin power_out line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "VLL1/PTC21")
				(number "50")
			)
			(pin power_out line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "VLL2/PTC20")
				(number "49")
			)
			(pin power_out line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "VLL3")
				(number "48")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 5.08)
				(name "VREGIN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 5.08)
				(name "VREFH")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 5.08)
				(name "VREFL")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC2")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC7")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD0")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD1")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD2")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD3")
				(number "60")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "62")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD7")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE20")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE21")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE22")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE23")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE24")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE25")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE29")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE30")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE31")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL43Z256VMP4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL43Z256VMP4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-64_5.0x5.0mm_Layout8x8_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL43P64M48SF6.pdf"
			(at 5.08 -60.96 0)
		)
		(property "Description" "Kinetis KL43 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, USB FS Device (xtal-less), Segment LCD, FlexIO, MAPBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL43 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*5.0x5.0mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL43Z256VMP4_0_1")
		(symbol "MKL43Z256VMP4_1_1"
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA0")
				(number "D3")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA1")
				(number "D4")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA2")
				(number "E5")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA3")
				(number "D5")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA4")
				(number "G5")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA5")
				(number "F5")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA12")
				(number "H6")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA13")
				(number "G6")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA18")
				(number "H8")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA19")
				(number "G8")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA20")
				(number "F8")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "F7")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB1")
				(number "F6")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB2")
				(number "E7")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "E8")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB16")
				(number "E6")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB17")
				(number "D7")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB18")
				(number "D6")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB19")
				(number "C7")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "USB0_DP")
				(number "E1")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "USB0_DM")
				(number "D1")
			)
			(pin power_out line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "VOUT33")
				(number "E2")
			)
			(pin passive line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "VCAP1/PTC23")
				(number "A5")
			)
			(pin passive line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "VCAP2/PTC22")
				(number "B4")
			)
			(pin power_out line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "VLL1/PTC21")
				(number "B5")
			)
			(pin power_out line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "VLL2/PTC20")
				(number "A6")
			)
			(pin power_out line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "VLL3")
				(number "C5")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 5.08)
				(name "VREGIN")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "VDD")
				(number "E4")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "VSS")
				(number "C4")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VDDA")
				(number "F4")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "F3")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 5.08)
				(name "VREFH")
				(number "G4")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 5.08)
				(name "VREFL")
				(number "G3")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTC0")
				(number "D8")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "C6")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC2")
				(number "B7")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "C8")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "B8")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "A8")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "A7")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC7")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD0")
				(number "C3")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD1")
				(number "A4")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD2")
				(number "C2")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD3")
				(number "B3")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A3")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "C1")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "B2")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD7")
				(number "A2")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE0")
				(number "A1")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE1")
				(number "B1")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE20")
				(number "G1")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE21")
				(number "F1")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE22")
				(number "G2")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE23")
				(number "F2")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE24")
				(number "H4")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE25")
				(number "H5")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE29")
				(number "H1")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE30")
				(number "H2")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE31")
				(number "H3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL46Z256VLH4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL46Z256VLH4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL46P121M48SF4.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL46 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, USB FS Device/OTG, Segment LCD, TSI, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL46 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL46Z256VLH4_0_1")
		(symbol "MKL46Z256VLH4_1_1"
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA3")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA4")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA5")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA12")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA13")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA18")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA19")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA20")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB2")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB3")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB16")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB17")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB18")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB19")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "USB0_DP")
				(number "5")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "USB0_DM")
				(number "6")
			)
			(pin power_out line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "VOUT33")
				(number "7")
			)
			(pin passive line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "VCAP1/PTC23")
				(number "52")
			)
			(pin passive line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "VCAP2/PTC22")
				(number "51")
			)
			(pin power_out line
				(at -30.48 -38.1 0)
				(length 5.08)
				(name "VLL1/PTC21")
				(number "50")
			)
			(pin power_out line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "VLL2/PTC20")
				(number "49")
			)
			(pin power_out line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "VLL3")
				(number "48")
			)
			(pin power_in line
				(at -7.62 55.88 270)
				(length 5.08)
				(name "VREGIN")
				(number "8")
			)
			(pin power_in line
				(at -2.54 55.88 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin passive line
				(at -2.54 55.88 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -55.88 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -55.88 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 2.54 55.88 270)
				(length 5.08)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -55.88 90)
				(length 5.08)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 5.08 55.88 270)
				(length 5.08)
				(name "VREFH")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -55.88 90)
				(length 5.08)
				(name "VREFL")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC2")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 27.94 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "55")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC7")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD0")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD1")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD2")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD3")
				(number "60")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "62")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 -10.16 180)
				(length 5.08)
				(name "PTD7")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE20")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE21")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE22")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE23")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE24")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE25")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE29")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE30")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE31")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL46Z256VLL4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 86.995 0)
		)
		(property "Value" "MKL46Z256VLL4"
			(at 25.4 86.995 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 8.89 -86.995 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL46P121M48SF4.pdf"
			(at 7.62 -91.44 0)
		)
		(property "Description" "Kinetis KL46 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, USB FS Device/OTG, Segment LCD, TSI, LQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL46 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL46Z256VLL4_0_1")
		(symbol "MKL46Z256VLL4_1_1"
			(pin bidirectional line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "PTA0")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "PTA1")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "PTA2")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "PTA3")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PTA4")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PTA5")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PTA6")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PTA7")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA12")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA13")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA14")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA15")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA16")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA17")
				(number "47")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA18")
				(number "50")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA19")
				(number "51")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA20")
				(number "52")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "53")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTB1")
				(number "54")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTB2")
				(number "55")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTB3")
				(number "56")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB7")
				(number "57")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB8")
				(number "58")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB9")
				(number "59")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB10")
				(number "60")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB11")
				(number "61")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "62")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "63")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB18")
				(number "64")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB19")
				(number "65")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB2")
				(number "66")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PTB21")
				(number "67")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTB22")
				(number "68")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTB23")
				(number "69")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DP")
				(number "10")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "USB0_DM")
				(number "11")
			)
			(pin power_out line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "VOUT33")
				(number "12")
			)
			(pin passive line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "VCAP1/PTC23")
				(number "79")
			)
			(pin passive line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "VCAP2/PTC22")
				(number "78")
			)
			(pin power_out line
				(at -30.48 -71.12 0)
				(length 5.08)
				(name "VLL1/PTC21")
				(number "77")
			)
			(pin power_out line
				(at -30.48 -73.66 0)
				(length 5.08)
				(name "VLL2/PTC20")
				(number "76")
			)
			(pin power_out line
				(at -30.48 -76.2 0)
				(length 5.08)
				(name "VLL3")
				(number "75")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VREGIN")
				(number "13")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "8")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "29")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "49")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "74")
			)
			(pin power_in line
				(at -2.54 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "22")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "25")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VREFH")
				(number "23")
			)
			(pin power_in line
				(at 5.08 -91.44 90)
				(length 5.08)
				(name "VREFL")
				(number "24")
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PTC0")
				(number "70")
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "71")
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PTC2")
				(number "72")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "80")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "81")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "82")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PTC7")
				(number "83")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PTC8")
				(number "84")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PTC9")
				(number "85")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PTC10")
				(number "86")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC11")
				(number "87")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC12")
				(number "88")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC13")
				(number "89")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC16")
				(number "90")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC17")
				(number "91")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC18")
				(number "92")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTD0")
				(number "93")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTD1")
				(number "94")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTD2")
				(number "95")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTD3")
				(number "96")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "97")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "98")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "99")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD7")
				(number "100")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE2")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE3")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE4")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE5")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE6")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE16")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE17")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE18")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PTE19")
				(number "17")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PTE20")
				(number "18")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PTE21")
				(number "19")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PTE22")
				(number "20")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PTE23")
				(number "21")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PTE24")
				(number "31")
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PTE25")
				(number "32")
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PTE26")
				(number "33")
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PTE29")
				(number "26")
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PTE30")
				(number "27")
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PTE31")
				(number "28")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL46Z256VMC4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 86.995 0)
		)
		(property "Value" "MKL46Z256VMC4"
			(at 25.4 86.995 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-121_8x8mm_Layout11x11_P0.65mm"
			(at 6.35 -86.995 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL46P121M48SF4.pdf"
			(at 7.62 -91.44 0)
		)
		(property "Description" "Kinetis KL46 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, USB FS Device/OTG, Segment LCD, TSI, MAPBGA-121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL46 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MKL46Z256VMC4_0_1")
		(symbol "MKL46Z256VMC4_1_1"
			(pin bidirectional line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "PTA0")
				(number "J6")
			)
			(pin bidirectional line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "PTA1")
				(number "H8")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "PTA2")
				(number "J7")
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "PTA3")
				(number "H9")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PTA4")
				(number "J8")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PTA5")
				(number "K7")
			)
			(pin bidirectional line
				(at -30.48 60.96 0)
				(length 5.08)
				(name "PTA6")
				(number "K3")
			)
			(pin bidirectional line
				(at -30.48 58.42 0)
				(length 5.08)
				(name "PTA7")
				(number "H4")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA12")
				(number "K8")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA13")
				(number "L8")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA14")
				(number "K9")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA15")
				(number "L9")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA16")
				(number "J10")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA17")
				(number "H10")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA18")
				(number "L11")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA19")
				(number "K11")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA20")
				(number "J11")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "G11")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTB1")
				(number "G10")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTB2")
				(number "G9")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTB3")
				(number "G8")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTB7")
				(number "E11")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTB8")
				(number "D11")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTB9")
				(number "E10")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTB10")
				(number "D10")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTB11")
				(number "C10")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "B10")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "E9")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB18")
				(number "D9")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB19")
				(number "C9")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTB2")
				(number "F10")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PTB21")
				(number "F9")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTB22")
				(number "F8")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTB23")
				(number "E8")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DP")
				(number "F1")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "USB0_DM")
				(number "F2")
			)
			(pin power_out line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "VOUT33")
				(number "G1")
			)
			(pin passive line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "VCAP1/PTC23")
				(number "C11")
			)
			(pin passive line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "VCAP2/PTC22")
				(number "B11")
			)
			(pin power_out line
				(at -30.48 -71.12 0)
				(length 5.08)
				(name "VLL1/PTC21")
				(number "A9")
			)
			(pin power_out line
				(at -30.48 -73.66 0)
				(length 5.08)
				(name "VLL2/PTC20")
				(number "A10")
			)
			(pin power_out line
				(at -30.48 -76.2 0)
				(length 5.08)
				(name "VLL3")
				(number "A11")
			)
			(pin no_connect line
				(at -25.4 55.88 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "J9")
			)
			(pin no_connect line
				(at -25.4 53.34 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "J4")
			)
			(pin no_connect line
				(at -25.4 27.94 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "H11")
			)
			(pin no_connect line
				(at -25.4 12.7 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "F11")
			)
			(pin no_connect line
				(at -25.4 -45.72 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "H3")
			)
			(pin no_connect line
				(at -25.4 -48.26 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "J3")
			)
			(pin no_connect line
				(at -25.4 -50.8 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "K4")
			)
			(pin no_connect line
				(at -25.4 -53.34 0)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "L7")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VREGIN")
				(number "G2")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "E5")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E6")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "E7")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "K6")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "L10")
			)
			(pin power_in line
				(at -2.54 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "F7")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G3")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "G7")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "K10")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L5")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "L6")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "F5")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "F6")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VREFH")
				(number "G5")
			)
			(pin power_in line
				(at 5.08 -91.44 90)
				(length 5.08)
				(name "VREFL")
				(number "G6")
			)
			(pin no_connect line
				(at 25.4 40.64 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A5")
			)
			(pin no_connect line
				(at 25.4 38.1 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B5")
			)
			(pin no_connect line
				(at 25.4 27.94 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "A4")
			)
			(pin no_connect line
				(at 25.4 -7.62 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "B1")
			)
			(pin no_connect line
				(at 25.4 -10.16 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "C2")
			)
			(pin no_connect line
				(at 25.4 -12.7 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "C1")
			)
			(pin no_connect line
				(at 25.4 -15.24 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "D2")
			)
			(pin no_connect line
				(at 25.4 -17.78 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "D1")
			)
			(pin no_connect line
				(at 25.4 -20.32 180)
				(length 5.08)
				(hide yes)
				(name "NC")
				(number "E1")
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PTC0")
				(number "B9")
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PTC1/LLWU_P6/RTC_CLKIN")
				(number "D8")
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PTC2")
				(number "C8")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "B8")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "A8")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "D7")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "C7")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PTC7")
				(number "B7")
			)
			(pin bidirectional line
				(at 30.48 55.88 180)
				(length 5.08)
				(name "PTC8")
				(number "A7")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PTC9")
				(number "D6")
			)
			(pin bidirectional line
				(at 30.48 50.8 180)
				(length 5.08)
				(name "PTC10")
				(number "C6")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTC11")
				(number "C5")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTC12")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTC13")
				(number "A6")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTC16")
				(number "D5")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTC17")
				(number "C4")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTC18")
				(number "B4")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTD0")
				(number "D4")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTD1")
				(number "D3")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTD2")
				(number "C3")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTD3")
				(number "B3")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A3")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD5")
				(number "A2")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "B2")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD7")
				(number "A1")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE0")
				(number "E4")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE1")
				(number "E3")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE2")
				(number "E2")
			)
			(pin bidirectional line
				(at 30.48 -33.02 180)
				(length 5.08)
				(name "PTE3")
				(number "F4")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTE4")
				(number "H7")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTE5")
				(number "G4")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTE6")
				(number "F3")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTE16")
				(number "H1")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTE17")
				(number "H2")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTE18")
				(number "J1")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PTE19")
				(number "J2")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PTE20")
				(number "K1")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PTE21")
				(number "K2")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PTE22")
				(number "L1")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PTE23")
				(number "L2")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PTE24")
				(number "H5")
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PTE25")
				(number "J5")
			)
			(pin bidirectional line
				(at 30.48 -68.58 180)
				(length 5.08)
				(name "PTE26")
				(number "H6")
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PTE29")
				(number "L3")
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PTE30")
				(number "K5")
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PTE31")
				(number "L4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKL46Z256VMP4"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -25.4 86.995 0)
		)
		(property "Value" "MKL46Z256VMP4"
			(at 25.4 86.995 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-64_5.0x5.0mm_Layout8x8_P0.5mm"
			(at 6.35 -86.995 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL46P121M48SF4.pdf"
			(at 7.62 -96.52 0)
		)
		(property "Description" "Kinetis KL46 series, 48-MHz/32-bit ARM Cortex-M0+, 256 kB flash, 32 kB SRAM, USB FS Device/OTG, Segment LCD, TSI, MAPBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL46 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*5.0x5.0mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKL46Z256VMP4_0_1")
		(symbol "MKL46Z256VMP4_1_1"
			(pin bidirectional line
				(at -30.48 76.2 0)
				(length 5.08)
				(name "PTA0")
				(number "D3")
			)
			(pin bidirectional line
				(at -30.48 73.66 0)
				(length 5.08)
				(name "PTA1")
				(number "D4")
			)
			(pin bidirectional line
				(at -30.48 71.12 0)
				(length 5.08)
				(name "PTA2")
				(number "E5")
			)
			(pin bidirectional line
				(at -30.48 68.58 0)
				(length 5.08)
				(name "PTA3")
				(number "D5")
			)
			(pin bidirectional line
				(at -30.48 66.04 0)
				(length 5.08)
				(name "PTA4")
				(number "G5")
			)
			(pin bidirectional line
				(at -30.48 63.5 0)
				(length 5.08)
				(name "PTA5")
				(number "F5")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA12")
				(number "H6")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA13")
				(number "G6")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA18")
				(number "H8")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA19")
				(number "G8")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA20")
				(number "F8")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTB0/LLWU_P5")
				(number "F7")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTB1")
				(number "F6")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTB2")
				(number "E7")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTB3")
				(number "E8")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTB16")
				(number "E6")
			)
			(pin bidirectional line
				(at -30.48 -5.08 0)
				(length 5.08)
				(name "PTB17")
				(number "D7")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTB18")
				(number "D6")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTB19")
				(number "C7")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "USB0_DP")
				(number "E1")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "USB0_DM")
				(number "D1")
			)
			(pin power_out line
				(at -30.48 -58.42 0)
				(length 5.08)
				(name "VOUT33")
				(number "E2")
			)
			(pin passive line
				(at -30.48 -63.5 0)
				(length 5.08)
				(name "VCAP1/PTC23")
				(number "A5")
			)
			(pin passive line
				(at -30.48 -66.04 0)
				(length 5.08)
				(name "VCAP2/PTC22")
				(number "B4")
			)
			(pin power_out line
				(at -30.48 -71.12 0)
				(length 5.08)
				(name "VLL1/PTC21")
				(number "B5")
			)
			(pin power_out line
				(at -30.48 -73.66 0)
				(length 5.08)
				(name "VLL2/PTC20")
				(number "A6")
			)
			(pin power_out line
				(at -30.48 -76.2 0)
				(length 5.08)
				(name "VLL3")
				(number "C5")
			)
			(pin power_in line
				(at -7.62 91.44 270)
				(length 5.08)
				(name "VREGIN")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 91.44 270)
				(length 5.08)
				(name "VDD")
				(number "E4")
			)
			(pin passive line
				(at -2.54 91.44 270)
				(length 5.08)
				(hide yes)
				(name "VDD")
				(number "G7")
			)
			(pin power_in line
				(at -2.54 -91.44 90)
				(length 5.08)
				(name "VSS")
				(number "C4")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "E3")
			)
			(pin passive line
				(at -2.54 -91.44 90)
				(length 5.08)
				(hide yes)
				(name "VSS")
				(number "H7")
			)
			(pin power_in line
				(at 2.54 91.44 270)
				(length 5.08)
				(name "VDDA")
				(number "F4")
			)
			(pin power_in line
				(at 2.54 -91.44 90)
				(length 5.08)
				(name "VSSA")
				(number "F3")
			)
			(pin power_in line
				(at 5.08 91.44 270)
				(length 5.08)
				(name "VREFH")
				(number "G4")
			)
			(pin power_in line
				(at 5.08 -91.44 90)
				(length 5.08)
				(name "VREFL")
				(number "G3")
			)
			(pin bidirectional line
				(at 30.48 76.2 180)
				(length 5.08)
				(name "PTC0")
				(number "D8")
			)
			(pin bidirectional line
				(at 30.48 73.66 180)
				(length 5.08)
				(name "PTC1/LLWU_P6")
				(number "C6")
			)
			(pin bidirectional line
				(at 30.48 71.12 180)
				(length 5.08)
				(name "PTC2")
				(number "B7")
			)
			(pin bidirectional line
				(at 30.48 68.58 180)
				(length 5.08)
				(name "PTC3/LLWU_P7")
				(number "C8")
			)
			(pin bidirectional line
				(at 30.48 66.04 180)
				(length 5.08)
				(name "PTC4/LLWU_P8")
				(number "B8")
			)
			(pin bidirectional line
				(at 30.48 63.5 180)
				(length 5.08)
				(name "PTC5/LLWU_P9")
				(number "A8")
			)
			(pin bidirectional line
				(at 30.48 60.96 180)
				(length 5.08)
				(name "PTC6/LLWU_P10")
				(number "A7")
			)
			(pin bidirectional line
				(at 30.48 58.42 180)
				(length 5.08)
				(name "PTC7")
				(number "B6")
			)
			(pin bidirectional line
				(at 30.48 12.7 180)
				(length 5.08)
				(name "PTD0")
				(number "C3")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTD1")
				(number "A4")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD2")
				(number "C2")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD3")
				(number "B3")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD4/LLWU_P14")
				(number "A3")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD5")
				(number "C1")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD6/LLWU_P15")
				(number "B2")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD7")
				(number "A2")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE0")
				(number "A1")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE1")
				(number "B1")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PTE20")
				(number "G1")
			)
			(pin bidirectional line
				(at 30.48 -55.88 180)
				(length 5.08)
				(name "PTE21")
				(number "F1")
			)
			(pin bidirectional line
				(at 30.48 -58.42 180)
				(length 5.08)
				(name "PTE22")
				(number "G2")
			)
			(pin bidirectional line
				(at 30.48 -60.96 180)
				(length 5.08)
				(name "PTE23")
				(number "F2")
			)
			(pin bidirectional line
				(at 30.48 -63.5 180)
				(length 5.08)
				(name "PTE24")
				(number "H4")
			)
			(pin bidirectional line
				(at 30.48 -66.04 180)
				(length 5.08)
				(name "PTE25")
				(number "H5")
			)
			(pin bidirectional line
				(at 30.48 -71.12 180)
				(length 5.08)
				(name "PTE29")
				(number "H1")
			)
			(pin bidirectional line
				(at 30.48 -73.66 180)
				(length 5.08)
				(name "PTE30")
				(number "H2")
			)
			(pin bidirectional line
				(at 30.48 -76.2 180)
				(length 5.08)
				(name "PTE31")
				(number "H3")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKV11Z128VLF7"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "MKV11Z128VLF7"
			(at 3.81 34.29 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 3.81 -31.75 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/KV11P64M75.pdf"
			(at -2.54 22.86 0)
		)
		(property "Description" "Kinetis KV11 series, 75-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB RAM, Entry-Level, Real-time Motor Control, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KV11 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKV11Z128VLF7_0_1")
		(symbol "MKV11Z128VLF7_1_1"
			(pin bidirectional line
				(at -15.24 30.48 0)
				(length 2.54)
				(name "PTA0")
				(number "17")
			)
			(pin bidirectional line
				(at -15.24 27.94 0)
				(length 2.54)
				(name "PTA1")
				(number "18")
			)
			(pin bidirectional line
				(at -15.24 25.4 0)
				(length 2.54)
				(name "PTA2")
				(number "19")
			)
			(pin bidirectional line
				(at -15.24 22.86 0)
				(length 2.54)
				(name "PTA3")
				(number "20")
			)
			(pin bidirectional line
				(at -15.24 20.32 0)
				(length 2.54)
				(name "PTA4")
				(number "21")
			)
			(pin bidirectional line
				(at -15.24 17.78 0)
				(length 2.54)
				(name "PTA18")
				(number "24")
			)
			(pin bidirectional line
				(at -15.24 15.24 0)
				(length 2.54)
				(name "PTA19")
				(number "25")
			)
			(pin bidirectional line
				(at -15.24 12.7 0)
				(length 2.54)
				(name "PTA20")
				(number "26")
			)
			(pin bidirectional line
				(at -15.24 7.62 0)
				(length 2.54)
				(name "PTB0")
				(number "27")
			)
			(pin bidirectional line
				(at -15.24 5.08 0)
				(length 2.54)
				(name "PTB1")
				(number "28")
			)
			(pin bidirectional line
				(at -15.24 2.54 0)
				(length 2.54)
				(name "PTB2")
				(number "29")
			)
			(pin bidirectional line
				(at -15.24 0 0)
				(length 2.54)
				(name "PTB3")
				(number "30")
			)
			(pin bidirectional line
				(at -15.24 -2.54 0)
				(length 2.54)
				(name "PTB16")
				(number "31")
			)
			(pin bidirectional line
				(at -15.24 -5.08 0)
				(length 2.54)
				(name "PTB17")
				(number "32")
			)
			(pin bidirectional line
				(at -15.24 -10.16 0)
				(length 2.54)
				(name "PTC0")
				(number "33")
			)
			(pin bidirectional line
				(at -15.24 -12.7 0)
				(length 2.54)
				(name "PTC1")
				(number "34")
			)
			(pin bidirectional line
				(at -15.24 -15.24 0)
				(length 2.54)
				(name "PTC2")
				(number "35")
			)
			(pin bidirectional line
				(at -15.24 -17.78 0)
				(length 2.54)
				(name "PTC3")
				(number "36")
			)
			(pin bidirectional line
				(at -15.24 -20.32 0)
				(length 2.54)
				(name "PTC4")
				(number "37")
			)
			(pin bidirectional line
				(at -15.24 -22.86 0)
				(length 2.54)
				(name "PTC5")
				(number "38")
			)
			(pin bidirectional line
				(at -15.24 -25.4 0)
				(length 2.54)
				(name "PTC6")
				(number "39")
			)
			(pin bidirectional line
				(at -15.24 -27.94 0)
				(length 2.54)
				(name "PTC7")
				(number "40")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 2.54)
				(name "VSS")
				(number "2")
			)
			(pin passive line
				(at -2.54 -33.02 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "23")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 2.54)
				(name "VDDA")
				(number "9")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 2.54)
				(name "VSSA")
				(number "12")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "VREFH")
				(number "10")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 2.54)
				(name "VREFL")
				(number "11")
			)
			(pin bidirectional line
				(at 15.24 30.48 180)
				(length 2.54)
				(name "PTD0")
				(number "41")
			)
			(pin bidirectional line
				(at 15.24 27.94 180)
				(length 2.54)
				(name "PTD1")
				(number "42")
			)
			(pin bidirectional line
				(at 15.24 25.4 180)
				(length 2.54)
				(name "PTD2")
				(number "43")
			)
			(pin bidirectional line
				(at 15.24 22.86 180)
				(length 2.54)
				(name "PTD3")
				(number "44")
			)
			(pin bidirectional line
				(at 15.24 20.32 180)
				(length 2.54)
				(name "PTD4")
				(number "45")
			)
			(pin bidirectional line
				(at 15.24 17.78 180)
				(length 2.54)
				(name "PTD5")
				(number "46")
			)
			(pin bidirectional line
				(at 15.24 15.24 180)
				(length 2.54)
				(name "PTD6")
				(number "47")
			)
			(pin bidirectional line
				(at 15.24 12.7 180)
				(length 2.54)
				(name "PTD7")
				(number "48")
			)
			(pin bidirectional line
				(at 15.24 7.62 180)
				(length 2.54)
				(name "PTE16")
				(number "3")
			)
			(pin bidirectional line
				(at 15.24 5.08 180)
				(length 2.54)
				(name "PTE17")
				(number "4")
			)
			(pin bidirectional line
				(at 15.24 2.54 180)
				(length 2.54)
				(name "PTE18")
				(number "5")
			)
			(pin bidirectional line
				(at 15.24 0 180)
				(length 2.54)
				(name "PTE19")
				(number "6")
			)
			(pin bidirectional line
				(at 15.24 -2.54 180)
				(length 2.54)
				(name "PTE20")
				(number "7")
			)
			(pin bidirectional line
				(at 15.24 -5.08 180)
				(length 2.54)
				(name "PTE21")
				(number "8")
			)
			(pin bidirectional line
				(at 15.24 -7.62 180)
				(length 2.54)
				(name "PTE29")
				(number "13")
			)
			(pin bidirectional line
				(at 15.24 -10.16 180)
				(length 2.54)
				(name "PTE30")
				(number "14")
			)
			(pin bidirectional line
				(at 15.24 -12.7 180)
				(length 2.54)
				(name "PTE24")
				(number "15")
			)
			(pin bidirectional line
				(at 15.24 -15.24 180)
				(length 2.54)
				(name "PTE25")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKV11Z128VLH7"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -15.24 44.45 0)
		)
		(property "Value" "MKV11Z128VLH7"
			(at 6.35 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 3.81 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/KV11P64M75.pdf"
			(at -96.52 17.78 0)
		)
		(property "Description" "Kinetis KV11 series, 75-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB RAM, Entry-Level, Real-time Motor Control, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KV11 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKV11Z128VLH7_0_1")
		(symbol "MKV11Z128VLH7_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PTA3")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PTA4")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PTA5")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PTA12")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PTA13")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PTA18")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PTA19")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PTA20")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PTB0")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PTB2")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PTB3")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PTB16")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PTB17")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PTB18")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PTB19")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PTC1")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PTC2")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PTC3")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PTC4")
				(number "49")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PTC5")
				(number "50")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PTC6")
				(number "51")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PTC7")
				(number "52")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PTC8")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PTC9")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PTC10")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -40.64 0)
				(length 2.54)
				(name "PTC11")
				(number "56")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "30")
			)
			(pin passive line
				(at -2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "4")
			)
			(pin passive line
				(at -2.54 -45.72 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "47")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "48")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "16")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VREFL")
				(number "15")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 2.54)
				(name "VREFH")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PTD0")
				(number "57")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PTD1")
				(number "58")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PTD2")
				(number "59")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "PTD3")
				(number "60")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PTD4")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PTD5")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PTD6")
				(number "63")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PTD7")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PTE0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PTE1")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PTE16")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PTR17")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PTE18")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PTE19")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PTE20")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PTE21")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PTE22")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PTE23")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PTE24")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PTE25")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PTE29")
				(number "17")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PTE30")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PTE31")
				(number "19")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MKW41Z512VHT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -20.32 44.45 0)
		)
		(property "Value" "MKW41Z512VHT"
			(at 21.59 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:NXP_LQFN-48-1EP_7x7mm_P0.5mm_EP3.5x3.5mm_16xMask0.45x0.45_ThermalVias"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MKW41Z512.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Kinetis KW41Z-2.4 GHz, Arm Cortex-M0+, 512kB Flash, 128kB SRAM, Multi Mode: Bluetooth LE and 802.15.4 Wireless Radio and generic FSK, LQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KW41Z ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NXP*LQFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MKW41Z512VHT_0_0"
			(pin input line
				(at -22.86 25.4 0)
				(length 2.54)
				(name "XTAL")
				(number "31")
			)
			(pin input line
				(at -22.86 22.86 0)
				(length 2.54)
				(name "EXTAL")
				(number "30")
			)
			(pin output line
				(at -22.86 20.32 0)
				(length 2.54)
				(name "XTAL_OUT")
				(number "29")
			)
			(pin input line
				(at -22.86 5.08 0)
				(length 2.54)
				(name "ADC0_DM0/CMP0_IN1")
				(number "25")
			)
			(pin input line
				(at -22.86 2.54 0)
				(length 2.54)
				(name "ADC0_DP0/CMP0_IN0")
				(number "24")
			)
			(pin input line
				(at -22.86 -5.08 0)
				(length 2.54)
				(name "PSWITCH")
				(number "8")
			)
			(pin input line
				(at -22.86 -10.16 0)
				(length 2.54)
				(name "DCDC_CFG")
				(number "9")
			)
			(pin power_in line
				(at -22.86 -15.24 0)
				(length 2.54)
				(name "VDCDC_IN")
				(number "10")
			)
			(pin passive line
				(at -22.86 -22.86 0)
				(length 2.54)
				(name "DCDC_LP")
				(number "11")
			)
			(pin passive line
				(at -22.86 -25.4 0)
				(length 2.54)
				(name "DCDC_LN")
				(number "12")
			)
			(pin bidirectional line
				(at -12.7 45.72 270)
				(length 2.54)
				(name "VREFH/VREF_OUT")
				(number "27")
			)
			(pin power_out line
				(at -7.62 45.72 270)
				(length 2.54)
				(name "VDD_1P8OUT")
				(number "14")
			)
			(pin power_out line
				(at -5.08 45.72 270)
				(length 2.54)
				(name "VDD_1P5OUT_PMCIN")
				(number "15")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD_RF3")
				(number "32")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 2.54)
				(name "VSS")
				(number "49")
			)
			(pin power_in line
				(at 0 45.72 270)
				(length 2.54)
				(name "VDD_RF2")
				(number "35")
			)
			(pin power_in line
				(at 0 -45.72 90)
				(length 2.54)
				(name "DCDC_GND")
				(number "13")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDD_RF1")
				(number "36")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 2.54)
				(name "VSSA")
				(number "26")
			)
			(pin power_in line
				(at 5.08 -45.72 90)
				(length 2.54)
				(name "GANT")
				(number "34")
			)
			(pin power_in line
				(at 7.62 45.72 270)
				(length 2.54)
				(name "VDD_1")
				(number "44")
			)
			(pin power_in line
				(at 10.16 45.72 270)
				(length 2.54)
				(name "VDD_0")
				(number "20")
			)
			(pin power_in line
				(at 12.7 45.72 270)
				(length 2.54)
				(name "VDDA")
				(number "28")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 2.54)
				(name "PTC1")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 2.54)
				(name "PTC2")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 2.54)
				(name "PTC3")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 2.54)
				(name "PTC4")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 2.54)
				(name "PTC5")
				(number "41")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 2.54)
				(name "PTC6")
				(number "42")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 2.54)
				(name "PTC7")
				(number "43")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 2.54)
				(name "PTC16")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 2.54)
				(name "PTC17")
				(number "46")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 2.54)
				(name "PTC18")
				(number "47")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 2.54)
				(name "PTC19")
				(number "48")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 2.54)
				(name "PTB0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 2.54)
				(name "PTB1")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 2.54)
				(name "PTB2")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 2.54)
				(name "PTB3")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 2.54)
				(name "PTB16")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 2.54)
				(name "PTB17")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 2.54)
				(name "PTB18")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 2.54)
				(name "PTA0")
				(number "1")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 2.54)
				(name "PTA1")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 2.54)
				(name "PTA2")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 2.54)
				(name "PTA16")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 2.54)
				(name "PTA17")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 2.54)
				(name "PTA18")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 2.54)
				(name "PTA19")
				(number "7")
			)
			(pin passive line
				(at 22.86 -35.56 180)
				(length 2.54)
				(name "ANT")
				(number "33")
			)
		)
		(symbol "MKW41Z512VHT_0_1")
		(embedded_fonts no)
	)
	(symbol "MK20DN128VFM5"
		(extends "MK20DX128VFM5")
		(property "Reference" "U"
			(at -30.48 31.115 0)
		)
		(property "Value" "MK20DN128VFM5"
			(at 30.48 31.115 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 8.89 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/K20P32M50SF0.pdf"
			(at 10.16 -35.56 0)
		)
		(property "Description" "Kinetis K20 series, 50-MHz/32-bit ARM Cortex-M4, 128 kB flash, 32 kB SRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MK20DN32VFM5"
		(extends "MK20DX128VFM5")
		(property "Reference" "U"
			(at -30.48 31.115 0)
		)
		(property "Value" "MK20DN32VFM5"
			(at 30.48 31.115 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 8.89 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/K20P32M50SF0.pdf"
			(at 10.16 -35.56 0)
		)
		(property "Description" "Kinetis K20 series, 50-MHz/32-bit ARM Cortex-M4, 32 kB flash, 8 kB SRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MK20DN64VFM5"
		(extends "MK20DX128VFM5")
		(property "Reference" "U"
			(at -30.48 31.115 0)
		)
		(property "Value" "MK20DN64VFM5"
			(at 30.48 31.115 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 8.89 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/K20P32M50SF0.pdf"
			(at 10.16 -35.56 0)
		)
		(property "Description" "Kinetis K20 series, 50-MHz/32-bit ARM Cortex-M4, 64 kB flash, 16 kB SRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MK20DX32VFM5"
		(extends "MK20DX128VFM5")
		(property "Reference" "U"
			(at -30.48 31.115 0)
		)
		(property "Value" "MK20DX32VFM5"
			(at 30.48 31.115 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 8.89 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/K20P32M50SF0.pdf"
			(at 10.16 -35.56 0)
		)
		(property "Description" "Kinetis K20 series, 50-MHz/32-bit ARM Cortex-M4, 32 kB flash/32 kB FlexNVM, 8 kB SRAM/2 kB FlexRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MK20DX64VFM5"
		(extends "MK20DX128VFM5")
		(property "Reference" "U"
			(at -30.48 31.115 0)
		)
		(property "Value" "MK20DX64VFM5"
			(at 30.48 31.115 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 8.89 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/K20P32M50SF0.pdf"
			(at 10.16 -35.56 0)
		)
		(property "Description" "Kinetis K20 series, 50-MHz/32-bit ARM Cortex-M4, 64 kB flash/32 kB FlexNVM, 16 kB SRAM/2 kB FlexRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MK20FN1M0VMD12"
		(extends "MK20FX512VMD12")
		(property "Reference" "U"
			(at -40.64 94.615 0)
		)
		(property "Value" "MK20FN1M0VMD12"
			(at 40.64 94.615 0)
		)
		(property "Footprint" "Package_BGA:BGA-144_13.0x13.0mm_Layout12x12_P1.0mm"
			(at 8.89 -94.615 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/K20P144M120SF3.pdf"
			(at 10.16 -104.14 0)
		)
		(property "Description" "Kinetis K20 series, 120-MHz/32-bit ARM Cortex-M4, 1024 kB flash, 128 kB SRAM, USB HS+FS Device/OTG, MAPBGA-144"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis K20 ARM Cortex M4"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "BGA*13.0x13.0mm*Layout12x12*P1.0mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKE02Z16VLC4"
		(extends "MKE02Z64VLC4")
		(property "Reference" "U"
			(at -17.78 31.75 0)
		)
		(property "Value" "MKE02Z16VLC4"
			(at 17.78 31.75 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 8.89 -31.75 0)
		)
		(property "Datasheet" "https://www.nxp.com/files-static/microcontrollers/doc/ref_manual/MKE02P64M40SF0RM.pdf"
			(at 2.54 7.62 0)
		)
		(property "Description" "40 MHz, Entry-Level, High-Robustness, ESD/EMC performance Microcontroller, Cortex-M0+ core, 16kB Flash, 2kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP Kinetis Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKE02Z16VLD4"
		(extends "MKE02Z64VLD4")
		(property "Reference" "U"
			(at -17.78 45.72 0)
		)
		(property "Value" "MKE02Z16VLD4"
			(at 17.78 45.72 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 8.89 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/files-static/microcontrollers/doc/ref_manual/MKE02P64M40SF0RM.pdf"
			(at 2.54 17.78 0)
		)
		(property "Description" "40 MHz, Entry-Level, High-Robustness, ESD/EMC performance Microcontroller, Cortex-M0+ core, 16kB Flash, 2kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP Kinetis Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKE02Z32VLC4"
		(extends "MKE02Z64VLC4")
		(property "Reference" "U"
			(at -17.78 31.75 0)
		)
		(property "Value" "MKE02Z32VLC4"
			(at 17.78 31.75 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 8.89 -31.75 0)
		)
		(property "Datasheet" "https://www.nxp.com/files-static/microcontrollers/doc/ref_manual/MKE02P64M40SF0RM.pdf"
			(at 2.54 7.62 0)
		)
		(property "Description" "40 MHz, Entry-Level, High-Robustness, ESD/EMC performance Microcontroller, Cortex-M0+ core, 32kB Flash, 4kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP Kinetis Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKE02Z32VLD4"
		(extends "MKE02Z64VLD4")
		(property "Reference" "U"
			(at -17.78 45.72 0)
		)
		(property "Value" "MKE02Z32VLD4"
			(at 17.78 45.72 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 8.89 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/files-static/microcontrollers/doc/ref_manual/MKE02P64M40SF0RM.pdf"
			(at 2.54 17.78 0)
		)
		(property "Description" "40 MHz, Entry-Level, High-Robustness, ESD/EMC performance Microcontroller, Cortex-M0+ core, 32kB Flash, 4kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP Kinetis Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKE02Z32VLH4"
		(extends "MKE02Z64VLH4")
		(property "Reference" "U"
			(at -17.78 55.88 0)
		)
		(property "Value" "MKE02Z32VLH4"
			(at 20.32 55.88 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 8.89 -54.61 0)
		)
		(property "Datasheet" "https://www.nxp.com/files-static/microcontrollers/doc/ref_manual/MKE02P64M40SF0RM.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "40 MHz, Entry-Level, High-Robustness, ESD/EMC performance Microcontroller, Cortex-M0+ core, 32kB Flash, 4kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP Kinetis Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKE02Z32VQH4"
		(extends "MKE02Z64VQH4")
		(property "Reference" "U"
			(at -17.78 55.88 0)
		)
		(property "Value" "MKE02Z32VQH4"
			(at 20.32 55.88 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_14x14mm_P0.8mm"
			(at 8.89 -54.61 0)
		)
		(property "Datasheet" "https://www.nxp.com/files-static/microcontrollers/doc/ref_manual/MKE02P64M40SF0RM.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "40 MHz, Entry-Level, High-Robustness, ESD/EMC performance Microcontroller, Cortex-M0+ core, 32kB Flash, 4kB RAM, TQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP Kinetis Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL02Z16VFG4"
		(extends "MKL02Z32VFG4")
		(property "Reference" "U"
			(at -27.94 31.115 0)
		)
		(property "Value" "MKL02Z16VFG4"
			(at 27.94 31.115 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.9x1.9mm"
			(at 3.81 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL02P32M48SF0.pdf"
			(at 7.62 -20.32 0)
		)
		(property "Description" "Kinetis KL02 series, 48-MHz/32-bit ARM Cortex-M0+, 16 kB flash, 2 kB SRAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL02 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL02Z16VFK4"
		(extends "MKL02Z32VFK4")
		(property "Reference" "U"
			(at -27.94 31.115 0)
		)
		(property "Value" "MKL02Z16VFK4"
			(at 27.94 31.115 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 3.81 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL02P32M48SF0.pdf"
			(at 7.62 -20.32 0)
		)
		(property "Description" "Kinetis KL02 series, 48-MHz/32-bit ARM Cortex-M0+, 16 kB flash, 2 kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL02 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL02Z16VFM4"
		(extends "MKL02Z32VFM4")
		(property "Reference" "U"
			(at -27.94 31.115 0)
		)
		(property "Value" "MKL02Z16VFM4"
			(at 27.94 31.115 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 3.81 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL02P32M48SF0.pdf"
			(at 7.62 -20.32 0)
		)
		(property "Description" "Kinetis KL02 series, 48-MHz/32-bit ARM Cortex-M0+, 16 kB flash, 2 kB SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL02 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL02Z8VFG4"
		(extends "MKL02Z32VFG4")
		(property "Reference" "U"
			(at -27.94 31.115 0)
		)
		(property "Value" "MKL02Z8VFG4"
			(at 27.94 31.115 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.9x1.9mm"
			(at 3.81 -31.115 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL02P32M48SF0.pdf"
			(at 7.62 -20.32 0)
		)
		(property "Description" "Kinetis KL02 series, 48-MHz/32-bit ARM Cortex-M0+, 8 kB flash, 1 kB SRAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL02 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL03Z16VFG4"
		(extends "MKL03Z32VFG4")
		(property "Reference" "U"
			(at -30.48 20.955 0)
		)
		(property "Value" "MKL03Z16VFG4"
			(at 30.48 20.955 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.9x1.9mm"
			(at 3.81 -20.955 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL03P24M48SF0.pdf"
			(at 7.62 -48.26 0)
		)
		(property "Description" "Kinetis KL03 series, 48-MHz/32-bit ARM Cortex-M0+, 16 kB flash, 2 kB SRAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL03 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL03Z16VFK4"
		(extends "MKL03Z32VFK4")
		(property "Reference" "U"
			(at -30.48 20.955 0)
		)
		(property "Value" "MKL03Z16VFK4"
			(at 30.48 20.955 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 3.81 -20.955 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL03P24M48SF0.pdf"
			(at 7.62 -25.4 0)
		)
		(property "Description" "Kinetis KL03 series, 48-MHz/32-bit ARM Cortex-M0+, 16 kB flash, 2 kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL03 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL03Z32CBF4"
		(extends "MKL03Z32CAF4")
		(property "Reference" "U"
			(at -30.48 20.955 0)
		)
		(property "Value" "MKL03Z32CBF4"
			(at 30.48 20.955 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-20_1.994x1.609mm_Layout5x4_P0.4mm"
			(at 3.81 -20.955 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL03P24M48SF0.pdf"
			(at 7.62 -25.4 0)
		)
		(property "Description" "Kinetis KL03 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 2 kB SRAM, WLCSP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL03 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*1.994x1.609mm*P0.4mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL03Z8VFG4"
		(extends "MKL03Z32VFG4")
		(property "Reference" "U"
			(at -30.48 20.955 0)
		)
		(property "Value" "MKL03Z8VFG4"
			(at 30.48 20.955 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-16-1EP_3x3mm_P0.5mm_EP1.9x1.9mm"
			(at 3.81 -20.955 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL03P24M48SF0.pdf"
			(at 7.62 -48.26 0)
		)
		(property "Description" "Kinetis KL03 series, 48-MHz/32-bit ARM Cortex-M0+, 8 kB flash, 2 kB SRAM, QFN-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL03 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*3x3mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL03Z8VFK4"
		(extends "MKL03Z32VFK4")
		(property "Reference" "U"
			(at -30.48 20.955 0)
		)
		(property "Value" "MKL03Z8VFK4"
			(at 30.48 20.955 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 3.81 -20.955 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL03P24M48SF0.pdf"
			(at 7.62 -25.4 0)
		)
		(property "Description" "Kinetis KL03 series, 48-MHz/32-bit ARM Cortex-M0+, 8 kB flash, 2 kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL03 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL04Z16VFK4"
		(extends "MKL04Z32VFK4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL04Z16VFK4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL04P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL04 series, 48-MHz/32-bit ARM Cortex-M0+, 16 kB flash, 2 kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL04 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL04Z16VFM4"
		(extends "MKL04Z32VFM4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL04Z16VFM4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL04P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL04 series, 48-MHz/32-bit ARM Cortex-M0+, 16 kB flash, 2 kB SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL04 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL04Z16VLC4"
		(extends "MKL04Z32VLC4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL04Z16VLC4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL04P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL04 series, 48-MHz/32-bit ARM Cortex-M0+, 16 kB flash, 2 kB SRAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL04 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL04Z16VLF4"
		(extends "MKL04Z32VLF4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL04Z16VLF4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL04P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL04 series, 48-MHz/32-bit ARM Cortex-M0+, 16 kB flash, 2 kB SRAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL04 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL04Z8VFK4"
		(extends "MKL04Z32VFK4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL04Z8VFK4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL04P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL04 series, 48-MHz/32-bit ARM Cortex-M0+, 8 kB flash, 1 kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL04 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL04Z8VFM4"
		(extends "MKL04Z32VFM4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL04Z8VFM4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL04P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL04 series, 48-MHz/32-bit ARM Cortex-M0+, 8 kB flash, 1 kB SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL04 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL04Z8VLC4"
		(extends "MKL04Z32VLC4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL04Z8VLC4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL04P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL04 series, 48-MHz/32-bit ARM Cortex-M0+, 8 kB flash, 1 kB SRAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL04 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL05Z16VFK4"
		(extends "MKL05Z32VFK4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL05Z16VFK4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL05P48M48SF1.pdf"
			(at 10.16 -45.72 0)
		)
		(property "Description" "Kinetis KL05 series, 48-MHz/32-bit ARM Cortex-M0+, 16 kB flash, 2 kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL05 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL05Z16VFM4"
		(extends "MKL05Z32VFM4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL05Z16VFM4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL05P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL05 series, 48-MHz/32-bit ARM Cortex-M0+, 16 kB flash, 2 kB SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL05 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL05Z16VLC4"
		(extends "MKL05Z32VLC4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL05Z16VLC4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL05P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL05 series, 48-MHz/32-bit ARM Cortex-M0+, 16 kB flash, 2 kB SRAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL05 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL05Z16VLF4"
		(extends "MKL05Z32VLF4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL05Z16VLF4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL05P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL05 series, 48-MHz/32-bit ARM Cortex-M0+, 16 kB flash, 2 kB SRAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL05 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL05Z8VFK4"
		(extends "MKL05Z32VFK4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL05Z8VFK4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL05P48M48SF1.pdf"
			(at 10.16 -45.72 0)
		)
		(property "Description" "Kinetis KL05 series, 48-MHz/32-bit ARM Cortex-M0+, 8 kB flash, 1 kB SRAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL05 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL05Z8VFM4"
		(extends "MKL05Z32VFM4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL05Z8VFM4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL05P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL05 series, 48-MHz/32-bit ARM Cortex-M0+, 8 kB flash, 1 kB SRAM, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL05 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL05Z8VLC4"
		(extends "MKL05Z32VLC4")
		(property "Reference" "U"
			(at -30.48 41.275 0)
		)
		(property "Value" "MKL05Z8VLC4"
			(at 30.48 41.275 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 3.81 -41.275 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL05P48M48SF1.pdf"
			(at 7.62 -45.72 0)
		)
		(property "Description" "Kinetis KL05 series, 48-MHz/32-bit ARM Cortex-M0+, 8 kB flash, 1 kB SRAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL05 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL16Z32VFM4"
		(extends "MKL16Z128VFM4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL16Z32VFM4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL16P64M48SF5.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL16 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, I²S, TSI, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL16 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL16Z32VFT4"
		(extends "MKL16Z128VFT4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL16Z32VFT4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL16P64M48SF5.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL16 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, I²S, TSI, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL16 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL16Z32VLH4"
		(extends "MKL16Z128VLH4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL16Z32VLH4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL16P64M48SF5.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL16 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, I²S, TSI, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL16 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL16Z64VFM4"
		(extends "MKL16Z128VFM4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL16Z64VFM4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL16P64M48SF5.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL16 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, I²S, TSI, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL16 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL16Z64VFT4"
		(extends "MKL16Z128VFT4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL16Z64VFT4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL16P64M48SF5.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL16 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, I²S, TSI, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL16 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL16Z64VLH4"
		(extends "MKL16Z128VLH4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL16Z64VLH4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL16P64M48SF5.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL16 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, I²S, TSI, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL16 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL17Z128VFM4"
		(extends "MKL17Z256VFM4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z128VFM4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF6.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 32 kB SRAM, FlexIO, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL17Z128VFT4"
		(extends "MKL17Z256VFT4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z128VFT4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF6.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 32 kB SRAM, FlexIO, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL17Z128VLH4"
		(extends "MKL17Z256VLH4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z128VLH4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF6.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 32 kB SRAM, FlexIO, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL17Z128VMP4"
		(extends "MKL17Z256VMP4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z128VMP4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-64_5.0x5.0mm_Layout8x8_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF6.pdf"
			(at 5.08 -58.42 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 32 kB SRAM, FlexIO, MAPBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*5.0x5.0mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL17Z32VDA4"
		(extends "MKL17Z64VDA4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z32VDA4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-36_3.5x3.5mm_Layout6x6_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF2.pdf"
			(at 7.62 -60.96 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 8 kB SRAM, FlexIO, XFBGA-36"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*3.5x3.5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL17Z32VFM4"
		(extends "MKL17Z64VFM4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z32VFM4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF2.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 8 kB SRAM, FlexIO, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL17Z32VFT4"
		(extends "MKL17Z64VFT4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z32VFT4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF6.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 8 kB SRAM, FlexIO, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL17Z32VLH4"
		(extends "MKL17Z64VLH4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z32VLH4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF2.pdf"
			(at 7.62 -53.34 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 8 kB SRAM, FlexIO, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL17Z32VMP4"
		(extends "MKL17Z64VMP4")
		(property "Reference" "U"
			(at -25.4 48.895 0)
		)
		(property "Value" "MKL17Z32VMP4"
			(at 25.4 48.895 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-64_5.0x5.0mm_Layout8x8_P0.5mm"
			(at 6.35 -48.895 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL17P64M48SF2.pdf"
			(at 5.08 -58.42 0)
		)
		(property "Description" "Kinetis KL17 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 8 kB SRAM, FlexIO, MAPBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL17 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*5.0x5.0mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL24Z32VFM4"
		(extends "MKL24Z64VFM4")
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL24Z32VFM4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL24P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL24 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL24 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL24Z32VFT4"
		(extends "MKL24Z64VFT4")
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL24Z32VFT4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL24P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL24 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, USB FS Device/OTG, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL24 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL24Z32VLH4"
		(extends "MKL24Z64VLH4")
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL24Z32VLH4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL24P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL24 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, USB FS Device/OTG, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL24 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL24Z32VLK4"
		(extends "MKL24Z64VLK4")
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL24Z32VLK4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL24P80M48SF0.pdf"
			(at 7.62 -66.04 0)
		)
		(property "Description" "Kinetis KL24 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, USB FS Device/OTG, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL24 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL25Z32VFM4"
		(extends "MKL25Z128VFM4")
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL25Z32VFM4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL25P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL25 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL25 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL25Z32VFT4"
		(extends "MKL25Z128VFT4")
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL25Z32VFT4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL25P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL25 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, USB FS Device/OTG, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL25 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL25Z32VLH4"
		(extends "MKL25Z128VLH4")
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL25Z32VLH4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL25P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL25 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, USB FS Device/OTG, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL25 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL25Z32VLK4"
		(extends "MKL25Z128VLK4")
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL25Z32VLK4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL25P80M48SF0.pdf"
			(at 7.62 -66.04 0)
		)
		(property "Description" "Kinetis KL25 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, USB FS Device/OTG, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL25 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL25Z64VFM4"
		(extends "MKL25Z128VFM4")
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL25Z64VFM4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL25P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL25 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL25 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL25Z64VFT4"
		(extends "MKL25Z128VFT4")
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL25Z64VFT4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL25P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL25 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, USB FS Device/OTG, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL25 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL25Z64VLH4"
		(extends "MKL25Z128VLH4")
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL25Z64VLH4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL25P80M48SF0.pdf"
			(at 7.62 -68.58 0)
		)
		(property "Description" "Kinetis KL25 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, USB FS Device/OTG, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL25 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL25Z64VLK4"
		(extends "MKL25Z128VLK4")
		(property "Reference" "U"
			(at -25.4 61.595 0)
		)
		(property "Value" "MKL25Z64VLK4"
			(at 25.4 61.595 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at 6.35 -61.595 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL25P80M48SF0.pdf"
			(at 7.62 -66.04 0)
		)
		(property "Description" "Kinetis KL25 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, USB FS Device/OTG, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL25 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL26Z128VLL4"
		(extends "MKL26Z256VLL4")
		(property "Reference" "U"
			(at -25.4 86.995 0)
		)
		(property "Value" "MKL26Z128VLL4"
			(at 25.4 86.995 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 6.35 -86.995 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P121M48SF4.pdf"
			(at 7.62 -91.44 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device/OTG, LQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL26Z128VMC4"
		(extends "MKL26Z256VMC4")
		(property "Reference" "U"
			(at -25.4 86.995 0)
		)
		(property "Value" "MKL26Z128VMC4"
			(at 25.4 86.995 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-121_8x8mm_Layout11x11_P0.65mm"
			(at 6.35 -86.995 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P121M48SF4.pdf"
			(at 7.62 -93.98 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device/OTG, XFBGA-121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL26Z32VFM4"
		(extends "MKL26Z128VFM4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL26Z32VFM4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P64M48SF5.pdf"
			(at 12.7 -68.58 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL26Z32VFT4"
		(extends "MKL26Z128VFT4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL26Z32VFT4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P64M48SF5.pdf"
			(at 7.62 -58.42 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, USB FS Device/OTG, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL26Z32VLH4"
		(extends "MKL26Z128VLH4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL26Z32VLH4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P64M48SF5.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 4 kB SRAM, USB FS Device/OTG, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL26Z64VFM4"
		(extends "MKL26Z128VFM4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL26Z64VFM4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P64M48SF5.pdf"
			(at 12.7 -68.58 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, USB FS Device/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL26Z64VFT4"
		(extends "MKL26Z128VFT4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL26Z64VFT4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P64M48SF5.pdf"
			(at 7.62 -58.42 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, USB FS Device/OTG, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL26Z64VLH4"
		(extends "MKL26Z128VLH4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL26Z64VLH4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL26P64M48SF5.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL26 series, 48-MHz/32-bit ARM Cortex-M0+, 64 kB flash, 8 kB SRAM, USB FS Device/OTG, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL26 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL27Z128VFT4"
		(extends "MKL27Z256VFT4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL27Z128VFT4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 8.89 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF6.pdf"
			(at 10.16 -55.88 0)
		)
		(property "Description" "Kinetis KL27 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 32 kB SRAM, USB FS Device (xtal-less)/OTG, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL27Z128VLH4"
		(extends "MKL27Z256VLH4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL27Z128VLH4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF6.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL27 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 32 kB SRAM, USB FS Device (xtal-less)/OTG, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL27Z32VFM4"
		(extends "MKL27Z64VFM4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL27Z32VFM4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF2.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL27 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 8 kB SRAM, USB FS Device (xtal-less)/OTG, QFN-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL27Z32VFT4"
		(extends "MKL27Z64VFT4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL27Z32VFT4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF2.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL27 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 8 kB SRAM, USB FS Device (xtal-less)/OTG, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL27Z32VLH4"
		(extends "MKL27Z64VLH4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL27Z32VLH4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL27P64M48SF2.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL27 series, 48-MHz/32-bit ARM Cortex-M0+, 32 kB flash, 8 kB SRAM, USB FS Device (xtal-less)/OTG, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL27 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL43Z128VLH4"
		(extends "MKL43Z256VLH4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL43Z128VLH4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL43P64M48SF6.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL43 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device (xtal-less), Segment LCD, FlexIO, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL43 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL43Z128VMP4"
		(extends "MKL43Z256VMP4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL43Z128VMP4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-64_5.0x5.0mm_Layout8x8_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL43P64M48SF6.pdf"
			(at 5.08 -60.96 0)
		)
		(property "Description" "Kinetis KL43 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device (xtal-less), Segment LCD, FlexIO, MAPBGA-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL43 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*5.0x5.0mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL46Z128VLH4"
		(extends "MKL46Z256VLH4")
		(property "Reference" "U"
			(at -25.4 51.435 0)
		)
		(property "Value" "MKL46Z128VLH4"
			(at 25.4 51.435 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 6.35 -51.435 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL46P121M48SF4.pdf"
			(at 7.62 -55.88 0)
		)
		(property "Description" "Kinetis KL46 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device/OTG, Segment LCD, TSI, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL46 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL46Z128VLL4"
		(extends "MKL46Z256VLL4")
		(property "Reference" "U"
			(at -25.4 86.995 0)
		)
		(property "Value" "MKL46Z128VLL4"
			(at 25.4 86.995 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 8.89 -86.995 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL46P121M48SF4.pdf"
			(at 7.62 -91.44 0)
		)
		(property "Description" "Kinetis KL46 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device/OTG, Segment LCD, TSI, LQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL46 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKL46Z128VMC4"
		(extends "MKL46Z256VMC4")
		(property "Reference" "U"
			(at -25.4 86.995 0)
		)
		(property "Value" "MKL46Z128VMC4"
			(at 25.4 86.995 0)
		)
		(property "Footprint" "Package_BGA:XFBGA-121_8x8mm_Layout11x11_P0.65mm"
			(at 6.35 -86.995 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/KL46P121M48SF4.pdf"
			(at 7.62 -91.44 0)
		)
		(property "Description" "Kinetis KL46 series, 48-MHz/32-bit ARM Cortex-M0+, 128 kB flash, 16 kB SRAM, USB FS Device/OTG, Segment LCD, TSI, MAPBGA-121"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KL46 ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "XFBGA*8x8mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKW21Z256VHT"
		(extends "MKW41Z512VHT")
		(property "Reference" "U"
			(at -20.32 44.45 0)
		)
		(property "Value" "MKW21Z256VHT"
			(at 21.59 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:NXP_LQFN-48-1EP_7x7mm_P0.5mm_EP3.5x3.5mm_16xMask0.45x0.45_ThermalVias"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MKW41Z512.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Kinetis KW41Z-2.4 GHz, Arm Cortex-M0+, 256kB Flash, 64kB SRAM, generic FSK, LQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KW21Z ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NXP*LQFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKW21Z512VHT"
		(extends "MKW41Z512VHT")
		(property "Reference" "U"
			(at -20.32 44.45 0)
		)
		(property "Value" "MKW21Z512VHT"
			(at 21.59 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:NXP_LQFN-48-1EP_7x7mm_P0.5mm_EP3.5x3.5mm_16xMask0.45x0.45_ThermalVias"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MKW41Z512.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Kinetis KW41Z-2.4 GHz, Arm Cortex-M0+, 512kB Flash, 128kB SRAM, generic FSK, LQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KW21Z ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NXP*LQFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKW31Z256VHT"
		(extends "MKW41Z512VHT")
		(property "Reference" "U"
			(at -20.32 44.45 0)
		)
		(property "Value" "MKW31Z256VHT"
			(at 21.59 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:NXP_LQFN-48-1EP_7x7mm_P0.5mm_EP3.5x3.5mm_16xMask0.45x0.45_ThermalVias"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MKW41Z512.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Kinetis KW31Z-2.4 GHz, Arm Cortex-M0+, 256kB Flash, 64kB SRAM, Dual Mode: Bluetooth LE and generic FSK, LQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KW31Z ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NXP*LQFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKW31Z512VHT"
		(extends "MKW41Z512VHT")
		(property "Reference" "U"
			(at -20.32 44.45 0)
		)
		(property "Value" "MKW31Z512VHT"
			(at 21.59 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:NXP_LQFN-48-1EP_7x7mm_P0.5mm_EP3.5x3.5mm_16xMask0.45x0.45_ThermalVias"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MKW41Z512.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Kinetis KW41Z-2.4 GHz, Arm Cortex-M0+, 512kB Flash, 128kB SRAM, Dual Mode: Bluetooth LE and generic FSK, LQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KW31Z ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NXP*LQFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MKW41Z256VHT"
		(extends "MKW41Z512VHT")
		(property "Reference" "U"
			(at -20.32 44.45 0)
		)
		(property "Value" "MKW41Z256VHT"
			(at 21.59 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:NXP_LQFN-48-1EP_7x7mm_P0.5mm_EP3.5x3.5mm_16xMask0.45x0.45_ThermalVias"
			(at -1.27 0 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MKW41Z512.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Kinetis KW41Z-2.4 GHz, Arm Cortex-M0+, 256kB Flash, 64kB SRAM, Multi Mode: Bluetooth LE and 802.15.4 Wireless Radio and generic FSK, LQFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "Kinetis KW41Z ARM Cortex M0+"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NXP*LQFN*1EP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
