(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "LPC1102UK"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 15.24 0)
		)
		(property "Value" "LPC1102UK"
			(at 10.16 15.24 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_4x4_B2.17x2.32mm_P0.5mm"
			(at 30.48 17.78 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC1102_1104.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32kB flash, 8kB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*4x4*B2.17x2.32mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LPC1102UK_0_1")
		(symbol "LPC1102UK_1_1"
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "PIO0_0")
				(number "C1")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PIO0_8")
				(number "A2")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "PIO0_9")
				(number "A3")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "PIO0_10")
				(number "A4")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "PIO0_11")
				(number "B4")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "XTALIN")
				(number "B2")
			)
			(pin power_in line
				(at -2.54 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at -2.54 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "D3")
			)
			(pin power_in line
				(at 2.54 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "A1")
			)
			(pin power_in line
				(at 2.54 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "B1")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PIO1_0")
				(number "B3")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PIO1_1")
				(number "C4")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PIO1_2")
				(number "C3")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PIO1_3")
				(number "D4")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "PIO1_6")
				(number "C2")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PIO1_7")
				(number "D1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC1104UK"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 15.24 0)
		)
		(property "Value" "LPC1104UK"
			(at 7.62 15.24 0)
		)
		(property "Footprint" "Package_CSP:WLCSP-16_4x4_B2.17x2.32mm_P0.5mm"
			(at 27.94 17.78 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC1102_1104.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32kB flash, 8kB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "WLCSP*4x4*B2.17x2.32mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LPC1104UK_0_1")
		(symbol "LPC1104UK_1_1"
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "PIO0_0")
				(number "B2")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PIO0_1")
				(number "C1")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "PIO0_6")
				(number "A1")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "PIO0_8")
				(number "A3")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "PIO0_9")
				(number "A4")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "PIO0_10")
				(number "A2")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "PIO0_11")
				(number "B4")
			)
			(pin input line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "XTALIN")
				(number "B1")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "D2")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "D3")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PIO1_0")
				(number "B3")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PIO1_1")
				(number "C4")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PIO1_2")
				(number "C3")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PIO1_3")
				(number "D4")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "PIO1_6")
				(number "C2")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PIO1_7")
				(number "D1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC1111FHN33-101"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1111FHN33-101"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 8KB flash, 2KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LPC1111FHN33-101_0_1")
		(symbol "LPC1111FHN33-101_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "PIO0_0")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "PIO0_1")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "PIO0_2")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "PIO0_3")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "PIO0_4")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PIO0_5")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "PIO0_6")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "PIO0_7")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "PIO0_8")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "PIO0_9")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "PIO0_10")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "PIO0_11")
				(number "21")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "XTALIN")
				(number "4")
			)
			(pin output line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "XTALOUT")
				(number "5")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "PIO1_0")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "PIO1_1")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "PIO1_2")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "PIO1_3")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PIO1_4")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PIO1_5")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PIO1_6")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PIO1_7")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "PIO1_8")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PIO1_9")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PIO1_10")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "PIO1_11")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "PIO2_0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "PIO3_2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "PIO3_4")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "PIO3_5")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC1112FHI33-102"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1112FHI33-102"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16KB flash, 2KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LPC1112FHI33-102_0_1")
		(symbol "LPC1112FHI33-102_1_1"
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "PIO0_0")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "PIO0_1")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "PIO0_2")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "PIO0_3")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "PIO0_4")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PIO0_5")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "PIO0_6")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "PIO0_7")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "PIO0_8")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "PIO0_9")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "PIO0_10")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "PIO0_11")
				(number "21")
			)
			(pin input line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "XTALIN")
				(number "4")
			)
			(pin output line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "XTALOUT")
				(number "5")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "6")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 3.81)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 3.81)
				(name "VDD")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "PIO1_0")
				(number "22")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "PIO1_1")
				(number "23")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "PIO1_2")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "PIO1_3")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PIO1_4")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PIO1_5")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PIO1_6")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PIO1_7")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "PIO1_8")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PIO1_9")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PIO1_10")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "PIO1_11")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "PIO2_0")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "PIO3_2")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "PIO3_4")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "PIO3_5")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC1113FBD48-301"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1113FBD48-301"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 24KB flash, 8KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LPC1113FBD48-301_0_1")
		(symbol "LPC1113FBD48-301_1_1"
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 3.81)
				(name "PIO0_0")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "PIO0_1")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 3.81)
				(name "PIO0_2")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "PIO0_3")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "PIO0_4")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "PIO0_5")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "PIO0_6")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "PIO0_7")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "PIO0_8")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PIO0_9")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "PIO0_10")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "PIO0_11")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "PIO1_0")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "PIO1_1")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "PIO1_2")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "PIO1_3")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "PIO1_4")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "PIO1_5")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "PIO1_6")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "PIO1_7")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "PIO1_8")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 3.81)
				(name "PIO1_9")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 3.81)
				(name "PIO1_10")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 3.81)
				(name "PIO1_11")
				(number "42")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 38.1 270)
				(length 3.81)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at 2.54 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "PIO2_0")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "PIO2_1")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "PIO2_2")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "PIO2_3")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "PIO2_4")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "PIO2_5")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "PIO2_6")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "PIO2_7")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PIO2_8")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PIO2_9")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PIO2_10")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PIO2_11")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PIO3_0")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PIO3_1")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "PIO3_2")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "PIO3_3")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "PIO3_4")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "PIO3_5")
				(number "21")
			)
			(pin input line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "XTALIN")
				(number "6")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 3.81)
				(name "XTALOUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC11E12FBD48-201"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "LPC11E12FBD48-201"
			(at 24.13 34.29 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 36.83 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11E1X.pdf"
			(at 1.27 34.29 0)
		)
		(property "Description" "LPC11E1x, 50MHz Cortex-M0 MCU, 16kB Flash, 1kB EEPROM, 6kB SRAM, USART, I2C, SSP, ADC, Power Profile, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "nxp lpc arm microcontroller cortex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LPC11E12FBD48-201_0_1")
		(symbol "LPC11E12FBD48-201_1_1"
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PIO0_0")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PIO0_1")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PIO0_2")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PIO0_3")
				(number "14")
			)
			(pin open_collector line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PIO0_4")
				(number "15")
			)
			(pin open_collector line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PIO0_5")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PIO0_6")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PIO0_7")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PIO0_8")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PIO0_9")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PIO0_10")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PIO0_11")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PIO0_12")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PIO0_13")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PIO0_14")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PIO0_15")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PIO0_16")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PIO0_17")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PIO0_18")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PIO0_19")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PIO0_20")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PIO0_21")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PIO0_22")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PIO0_23")
				(number "42")
			)
			(pin power_in line
				(at -2.54 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at 2.54 35.56 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at 2.54 -35.56 90)
				(length 2.54)
				(name "VSS")
				(number "41")
			)
			(pin no_connect line
				(at 15.24 -20.32 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "20")
			)
			(pin no_connect line
				(at 15.24 -22.86 180)
				(length 2.54)
				(hide yes)
				(name "NC")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PIO1_13")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PIO1_14")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PIO1_15")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 2.54)
				(name "PIO1_16")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PIO1_19")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PIO1_20")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PIO1_21")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PIO1_22")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PIO1_23")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PIO1_24")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PIO1_25")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PIO1_26")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PIO1_27")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PIO1_28")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PIO1_29")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PIO1_31")
				(number "25")
			)
			(pin passive line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "XTALOUT")
				(number "7")
			)
			(pin passive line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "XTALIN")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC11U12FBD48-201"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 35.56 0)
		)
		(property "Value" "LPC11U12FBD48-201"
			(at 12.7 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 21.59 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U1X.pdf"
			(at 0 -37.465 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, USB, 16KB flash, 6KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LPC11U12FBD48-201_0_1")
		(symbol "LPC11U12FBD48-201_1_1"
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 3.81)
				(name "PIO0_0")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "PIO0_1")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 3.81)
				(name "PIO0_2")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "PIO0_3")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "PIO0_4")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "PIO0_5")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "PIO0_6")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "PIO0_7")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "PIO0_8")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PIO0_9")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "PIO0_10")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "PIO0_11")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "PIO0_12")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "PIO0_13")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "PIO0_14")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "PIO0_15")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "PIO0_16")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "PIO0_17")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "PIO0_18")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "PIO0_19")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "PIO0_20")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "PIO0_21")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 3.81)
				(name "PIO0_22")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 3.81)
				(name "PIO0_23")
				(number "42")
			)
			(pin power_in line
				(at -2.54 38.1 270)
				(length 3.81)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at -2.54 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "41")
			)
			(pin power_in line
				(at 0 38.1 270)
				(length 3.81)
				(name "VDD")
				(number "8")
			)
			(pin power_in line
				(at 0 -38.1 90)
				(length 3.81)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "PIO1_13")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "PIO1_14")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "PIO1_15")
				(number "43")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "PIO1_16")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "PIO1_19")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "PIO1_20")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "PIO1_21")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "PIO1_22")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PIO1_23")
				(number "18")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PIO1_24")
				(number "21")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PIO1_25")
				(number "1")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PIO1_26")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "PIO1_27")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PIO1_28")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PIO1_29")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "PIO1_31")
				(number "25")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "USB_DP")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "USB_DM")
				(number "19")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "XTALIN")
				(number "6")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "XTALOUT")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC1224FBD48-101"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 44.45 0)
		)
		(property "Value" "LPC1224FBD48-101"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 15.24 46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC122X.pdf"
			(at -12.7 11.43 0)
		)
		(property "Description" "LPC122x 32-bit ARM Cortex-M0 microcontroller, 32 kB FLASH, 4 kB SRAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LPC1224FBD48-101_0_1")
		(symbol "LPC1224FBD48-101_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PIO0_0")
				(number "15")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PIO0_1")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PIO0_2")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PIO0_3")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PIO0_4")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PIO0_5")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PIO0_6")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PIO0_7")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PIO0_8")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PIO0_9")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PIO0_10")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PIO0_11")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PIO0_12/~{ISP}")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PIO0_13/~{RESET}")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PIO0_14")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PIO0_15")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PIO0_16")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PIO0_17")
				(number "32")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PIO0_18")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PIO0_19")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PIO0_20")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PIO0_21")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PIO0_22")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PIO0_23")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PIO0_24")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PIO0_25/SWDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PIO0_26/SWCLK")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PIO0_27")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PIO0_28")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PIO0_29")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PIO0_30")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PIO0_31")
				(number "35")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "44")
			)
			(pin power_in line
				(at -2.54 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "43")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "47")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSIO")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PIO1_0")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PIO1_1")
				(number "37")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PIO1_2")
				(number "38")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "WAKEUP/PIO1_3")
				(number "39")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PIO1_4")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PIO1_5")
				(number "41")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PIO1_6")
				(number "42")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "VREF_CMP")
				(number "3")
			)
			(pin input line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "XTALIN")
				(number "1")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "XTALOUT")
				(number "2")
			)
			(pin input line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "RTCXIN")
				(number "46")
			)
			(pin output line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "RTCXOUT")
				(number "45")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC1224FBD64-101"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 44.45 0)
		)
		(property "Value" "LPC1224FBD64-101"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 15.24 46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC122X.pdf"
			(at -12.7 11.43 0)
		)
		(property "Description" "LPC122x 32-bit ARM Cortex-M0 microcontroller, 32 kB FLASH, 4 kB SRAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LPC1224FBD64-101_0_1")
		(symbol "LPC1224FBD64-101_1_1"
			(pin bidirectional line
				(at -17.78 40.64 0)
				(length 2.54)
				(name "PIO0_0")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 38.1 0)
				(length 2.54)
				(name "PIO0_1")
				(number "20")
			)
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 2.54)
				(name "PIO0_2")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 2.54)
				(name "PIO0_3")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 2.54)
				(name "PIO0_4")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 2.54)
				(name "PIO0_5")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 2.54)
				(name "PIO0_6")
				(number "25")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 2.54)
				(name "PIO0_7")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 2.54)
				(name "PIO0_8")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 2.54)
				(name "PIO0_9")
				(number "28")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 2.54)
				(name "PIO0_10")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 2.54)
				(name "PIO0_11")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "PIO0_12/~{ISP}")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "PIO0_13/~{RESET}")
				(number "40")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "PIO0_14")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "PIO0_15")
				(number "42")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 2.54)
				(name "PIO0_16")
				(number "43")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "PIO0_17")
				(number "44")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "PIO0_18")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "PIO0_19")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "PIO0_20")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 2.54)
				(name "PIO0_21")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 2.54)
				(name "PIO0_22")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 2.54)
				(name "PIO0_23")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 2.54)
				(name "PIO0_24")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 2.54)
				(name "PIO0_25/SWDIO")
				(number "10")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 2.54)
				(name "PIO0_26/SWCLK")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 2.54)
				(name "PIO0_27")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 2.54)
				(name "PIO0_28")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 2.54)
				(name "PIO0_29")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -35.56 0)
				(length 2.54)
				(name "PIO0_30")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -38.1 0)
				(length 2.54)
				(name "PIO0_31")
				(number "47")
			)
			(pin power_in line
				(at -2.54 45.72 270)
				(length 2.54)
				(name "VDD")
				(number "56")
			)
			(pin power_in line
				(at -2.54 -43.18 90)
				(length 2.54)
				(name "VSS")
				(number "55")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 2.54)
				(name "VDDIO")
				(number "63")
			)
			(pin power_in line
				(at 2.54 -43.18 90)
				(length 2.54)
				(name "VSSIO")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 40.64 180)
				(length 2.54)
				(name "PIO1_0")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 38.1 180)
				(length 2.54)
				(name "PIO1_1")
				(number "49")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 2.54)
				(name "PIO1_2")
				(number "50")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 2.54)
				(name "WAKEUP/PIO1_3")
				(number "51")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 2.54)
				(name "PIO1_4")
				(number "52")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 2.54)
				(name "PIO1_5")
				(number "53")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 2.54)
				(name "PIO1_6")
				(number "54")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 2.54)
				(name "PIO2_0")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 2.54)
				(name "PIO2_1")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 2.54)
				(name "PIO2_2")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 2.54)
				(name "PIO2_3")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "PIO2_4")
				(number "33")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "PIO2_5")
				(number "34")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 2.54)
				(name "PIO2_6")
				(number "35")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "PIO2_7")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "PIO2_8")
				(number "59")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "PIO2_9")
				(number "60")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "PIO2_10")
				(number "61")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 2.54)
				(name "PIO2_11")
				(number "62")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "PIO2_12")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 2.54)
				(name "PIO2_13")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 2.54)
				(name "PIO2_14")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -17.78 180)
				(length 2.54)
				(name "PIO2_15")
				(number "16")
			)
			(pin input line
				(at 17.78 -22.86 180)
				(length 2.54)
				(name "VREF_CMP")
				(number "3")
			)
			(pin input line
				(at 17.78 -27.94 180)
				(length 2.54)
				(name "XTALIN")
				(number "1")
			)
			(pin output line
				(at 17.78 -30.48 180)
				(length 2.54)
				(name "XTALOUT")
				(number "2")
			)
			(pin input line
				(at 17.78 -35.56 180)
				(length 2.54)
				(name "RTCXIN")
				(number "58")
			)
			(pin output line
				(at 17.78 -38.1 180)
				(length 2.54)
				(name "RTCXOUT")
				(number "57")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC1763FBD100"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -17.78 62.23 0)
		)
		(property "Value" "LPC1763FBD100"
			(at 20.32 62.23 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 33.02 64.77 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC1769_68_67_66_65_64_63.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "32-bit ARM Cortex-M3 microcontroller, 256KB flash, 64KB RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM 32-bit Cortex-M3 M3 NXP microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LPC1763FBD100_0_1")
		(symbol "LPC1763FBD100_1_1"
			(pin bidirectional line
				(at -22.86 55.88 0)
				(length 3.81)
				(name "P0[0]")
				(number "46")
			)
			(pin bidirectional line
				(at -22.86 53.34 0)
				(length 3.81)
				(name "P0[1]")
				(number "47")
			)
			(pin bidirectional line
				(at -22.86 50.8 0)
				(length 3.81)
				(name "P0[2]")
				(number "98")
			)
			(pin bidirectional line
				(at -22.86 48.26 0)
				(length 3.81)
				(name "P0[3]")
				(number "99")
			)
			(pin bidirectional line
				(at -22.86 45.72 0)
				(length 3.81)
				(name "P0[4]")
				(number "81")
			)
			(pin bidirectional line
				(at -22.86 43.18 0)
				(length 3.81)
				(name "P0[5]")
				(number "80")
			)
			(pin bidirectional line
				(at -22.86 40.64 0)
				(length 3.81)
				(name "P0[6]")
				(number "79")
			)
			(pin bidirectional line
				(at -22.86 38.1 0)
				(length 3.81)
				(name "P0[7]")
				(number "78")
			)
			(pin bidirectional line
				(at -22.86 35.56 0)
				(length 3.81)
				(name "P0[8]")
				(number "77")
			)
			(pin bidirectional line
				(at -22.86 33.02 0)
				(length 3.81)
				(name "P0[9]")
				(number "76")
			)
			(pin bidirectional line
				(at -22.86 30.48 0)
				(length 3.81)
				(name "P0[10]")
				(number "48")
			)
			(pin bidirectional line
				(at -22.86 27.94 0)
				(length 3.81)
				(name "P0[11]")
				(number "49")
			)
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 3.81)
				(name "P0[15]")
				(number "62")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 3.81)
				(name "P0[16]")
				(number "63")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 3.81)
				(name "P0[17]")
				(number "61")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 3.81)
				(name "P0[18]")
				(number "60")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 3.81)
				(name "P0[19]")
				(number "59")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 3.81)
				(name "P0[20]")
				(number "58")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 3.81)
				(name "P0[21]")
				(number "57")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 3.81)
				(name "P0[22]")
				(number "56")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 3.81)
				(name "P0[23]")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 3.81)
				(name "P0[24]")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 3.81)
				(name "P0[25]")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 3.81)
				(name "P0[26]")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 3.81)
				(name "P0[27]")
				(number "25")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 3.81)
				(name "P0[28]")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 3.81)
				(name "P0[29]")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 3.81)
				(name "P0[30]")
				(number "30")
			)
			(pin output line
				(at -22.86 -17.78 0)
				(length 3.81)
				(name "RTCK")
				(number "100")
			)
			(pin output line
				(at -22.86 -20.32 0)
				(length 3.81)
				(name "TDO/SWO")
				(number "1")
			)
			(pin input line
				(at -22.86 -22.86 0)
				(length 3.81)
				(name "TDI")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 3.81)
				(name "TMS/SWDIO")
				(number "3")
			)
			(pin input line
				(at -22.86 -27.94 0)
				(length 3.81)
				(name "~{TRST}")
				(number "4")
			)
			(pin input line
				(at -22.86 -30.48 0)
				(length 3.81)
				(name "TCK/SWDCLK")
				(number "5")
			)
			(pin input line
				(at -22.86 -35.56 0)
				(length 3.81)
				(name "~{RESET}")
				(number "17")
			)
			(pin output line
				(at -22.86 -38.1 0)
				(length 3.81)
				(name "~{RSTOUT}")
				(number "14")
			)
			(pin input line
				(at -22.86 -43.18 0)
				(length 3.81)
				(name "XTAL1")
				(number "22")
			)
			(pin output line
				(at -22.86 -45.72 0)
				(length 3.81)
				(name "XTAL2")
				(number "23")
			)
			(pin input line
				(at -22.86 -48.26 0)
				(length 3.81)
				(name "RTCX1")
				(number "16")
			)
			(pin output line
				(at -22.86 -50.8 0)
				(length 3.81)
				(name "RTCX2")
				(number "18")
			)
			(pin no_connect line
				(at -19.05 -55.88 0)
				(length 3.81)
				(hide yes)
				(name "NC")
				(number "13")
			)
			(pin power_in line
				(at -10.16 63.5 270)
				(length 3.81)
				(name "VDD(3V3)")
				(number "28")
			)
			(pin power_in line
				(at -10.16 -63.5 90)
				(length 3.81)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -7.62 63.5 270)
				(length 3.81)
				(name "VDD(3V3)")
				(number "54")
			)
			(pin power_in line
				(at -7.62 -63.5 90)
				(length 3.81)
				(name "VSS")
				(number "41")
			)
			(pin power_in line
				(at -5.08 63.5 270)
				(length 3.81)
				(name "VDD(3V3)")
				(number "71")
			)
			(pin power_in line
				(at -5.08 -63.5 90)
				(length 3.81)
				(name "VSS")
				(number "55")
			)
			(pin power_in line
				(at -2.54 63.5 270)
				(length 3.81)
				(name "VDD(3V3)")
				(number "96")
			)
			(pin power_in line
				(at -2.54 -63.5 90)
				(length 3.81)
				(name "VSS")
				(number "72")
			)
			(pin power_in line
				(at 0 63.5 270)
				(length 3.81)
				(name "VDD(REG)(3V3)")
				(number "42")
			)
			(pin power_in line
				(at 0 -63.5 90)
				(length 3.81)
				(name "VSS")
				(number "83")
			)
			(pin power_in line
				(at 2.54 63.5 270)
				(length 3.81)
				(name "VDD(REG)(3V3)")
				(number "84")
			)
			(pin power_in line
				(at 2.54 -63.5 90)
				(length 3.81)
				(name "VSS")
				(number "97")
			)
			(pin power_in line
				(at 5.08 63.5 270)
				(length 3.81)
				(name "VBAT")
				(number "19")
			)
			(pin power_in line
				(at 5.08 -63.5 90)
				(length 3.81)
				(name "VREFN")
				(number "15")
			)
			(pin power_in line
				(at 7.62 63.5 270)
				(length 3.81)
				(name "VREFP")
				(number "12")
			)
			(pin power_in line
				(at 7.62 -63.5 90)
				(length 3.81)
				(name "VSSA")
				(number "11")
			)
			(pin power_in line
				(at 10.16 63.5 270)
				(length 3.81)
				(name "VDDA")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 55.88 180)
				(length 3.81)
				(name "P1[0]")
				(number "95")
			)
			(pin bidirectional line
				(at 22.86 53.34 180)
				(length 3.81)
				(name "P1[1]")
				(number "94")
			)
			(pin bidirectional line
				(at 22.86 50.8 180)
				(length 3.81)
				(name "P1[4]")
				(number "93")
			)
			(pin bidirectional line
				(at 22.86 48.26 180)
				(length 3.81)
				(name "P1[8]")
				(number "92")
			)
			(pin bidirectional line
				(at 22.86 45.72 180)
				(length 3.81)
				(name "P1[9]")
				(number "91")
			)
			(pin bidirectional line
				(at 22.86 43.18 180)
				(length 3.81)
				(name "P1[10]")
				(number "90")
			)
			(pin bidirectional line
				(at 22.86 40.64 180)
				(length 3.81)
				(name "P1[14]")
				(number "89")
			)
			(pin bidirectional line
				(at 22.86 38.1 180)
				(length 3.81)
				(name "P1[15]")
				(number "88")
			)
			(pin bidirectional line
				(at 22.86 35.56 180)
				(length 3.81)
				(name "P1[16]")
				(number "87")
			)
			(pin bidirectional line
				(at 22.86 33.02 180)
				(length 3.81)
				(name "P1[17]")
				(number "86")
			)
			(pin bidirectional line
				(at 22.86 30.48 180)
				(length 3.81)
				(name "P1[18]")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 27.94 180)
				(length 3.81)
				(name "P1[19]")
				(number "33")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 3.81)
				(name "P1[20]")
				(number "34")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 3.81)
				(name "P1[21]")
				(number "35")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 3.81)
				(name "P1[22]")
				(number "36")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 3.81)
				(name "P1[23]")
				(number "37")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 3.81)
				(name "P1[24]")
				(number "38")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 3.81)
				(name "P1[25]")
				(number "39")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 3.81)
				(name "P1[26]")
				(number "40")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 3.81)
				(name "P1[27]")
				(number "43")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 3.81)
				(name "P1[28]")
				(number "44")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 3.81)
				(name "P1[29]")
				(number "45")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 3.81)
				(name "P1[30]")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 3.81)
				(name "P1[31]")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 3.81)
				(name "P2[0]")
				(number "75")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 3.81)
				(name "P2[1]")
				(number "74")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 3.81)
				(name "P2[2]")
				(number "73")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 3.81)
				(name "P2[3]")
				(number "70")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 3.81)
				(name "P2[4]")
				(number "69")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 3.81)
				(name "P2[5]")
				(number "68")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 3.81)
				(name "P2[6]")
				(number "67")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 3.81)
				(name "P2[7]")
				(number "66")
			)
			(pin bidirectional line
				(at 22.86 -27.94 180)
				(length 3.81)
				(name "P2[8]")
				(number "65")
			)
			(pin bidirectional line
				(at 22.86 -30.48 180)
				(length 3.81)
				(name "P2[9]")
				(number "64")
			)
			(pin bidirectional line
				(at 22.86 -33.02 180)
				(length 3.81)
				(name "P2[10]")
				(number "53")
			)
			(pin bidirectional line
				(at 22.86 -35.56 180)
				(length 3.81)
				(name "P2[11]")
				(number "52")
			)
			(pin bidirectional line
				(at 22.86 -38.1 180)
				(length 3.81)
				(name "P2[12]")
				(number "51")
			)
			(pin bidirectional line
				(at 22.86 -40.64 180)
				(length 3.81)
				(name "P2[13]")
				(number "50")
			)
			(pin bidirectional line
				(at 22.86 -45.72 180)
				(length 3.81)
				(name "P3[25]")
				(number "27")
			)
			(pin bidirectional line
				(at 22.86 -48.26 180)
				(length 3.81)
				(name "P3[26]")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 -53.34 180)
				(length 3.81)
				(name "P4[28]")
				(number "82")
			)
			(pin bidirectional line
				(at 22.86 -55.88 180)
				(length 3.81)
				(name "P4[29]")
				(number "85")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC2141FBD64"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -12.7 46.99 0)
		)
		(property "Value" "LPC2141FBD64"
			(at 13.97 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 26.67 49.53 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC2141_42_44_46_48.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit/32-bit ARM7TDMI-S microcontroller, 32kB flash, 8kB RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 16-bit, 32-bit, ARM7, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LPC2141FBD64_0_1")
		(symbol "LPC2141FBD64_1_1"
			(pin bidirectional line
				(at -17.78 35.56 0)
				(length 3.81)
				(name "P0.0")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 33.02 0)
				(length 3.81)
				(name "P0.1")
				(number "21")
			)
			(pin bidirectional line
				(at -17.78 30.48 0)
				(length 3.81)
				(name "P0.2")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 27.94 0)
				(length 3.81)
				(name "P0.3")
				(number "26")
			)
			(pin bidirectional line
				(at -17.78 25.4 0)
				(length 3.81)
				(name "P0.4")
				(number "27")
			)
			(pin bidirectional line
				(at -17.78 22.86 0)
				(length 3.81)
				(name "P0.5")
				(number "29")
			)
			(pin bidirectional line
				(at -17.78 20.32 0)
				(length 3.81)
				(name "P0.6")
				(number "30")
			)
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "P0.7")
				(number "31")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "P0.8")
				(number "33")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "P0.9")
				(number "34")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "P0.10")
				(number "35")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "P0.11")
				(number "37")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "P0.12")
				(number "38")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "P0.13")
				(number "39")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "P0.14")
				(number "41")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "P0.15")
				(number "45")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "P0.16")
				(number "46")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "P0.17")
				(number "47")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "P0.18")
				(number "53")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "P0.19")
				(number "54")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "P0.20")
				(number "55")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "P0.21")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 -20.32 0)
				(length 3.81)
				(name "P0.22")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 -22.86 0)
				(length 3.81)
				(name "P0.23")
				(number "58")
			)
			(pin bidirectional line
				(at -17.78 -25.4 0)
				(length 3.81)
				(name "P0.25")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -27.94 0)
				(length 3.81)
				(name "P0.28")
				(number "13")
			)
			(pin bidirectional line
				(at -17.78 -30.48 0)
				(length 3.81)
				(name "P0.29")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 -33.02 0)
				(length 3.81)
				(name "P0.30")
				(number "15")
			)
			(pin output line
				(at -17.78 -35.56 0)
				(length 3.81)
				(name "P0.31")
				(number "17")
			)
			(pin power_in line
				(at -7.62 -48.26 90)
				(length 3.81)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 3.81)
				(name "VDD")
				(number "23")
			)
			(pin power_in line
				(at -5.08 -48.26 90)
				(length 3.81)
				(name "VSS")
				(number "18")
			)
			(pin power_in line
				(at -2.54 48.26 270)
				(length 3.81)
				(name "VDD")
				(number "43")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 3.81)
				(name "VSS")
				(number "25")
			)
			(pin power_in line
				(at 0 48.26 270)
				(length 3.81)
				(name "VDD")
				(number "51")
			)
			(pin power_in line
				(at 0 -48.26 90)
				(length 3.81)
				(name "VSS")
				(number "42")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 3.81)
				(name "VDDA")
				(number "7")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 3.81)
				(name "VSS")
				(number "50")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 3.81)
				(name "VBAT")
				(number "49")
			)
			(pin power_in line
				(at 5.08 -48.26 90)
				(length 3.81)
				(name "VSSA")
				(number "59")
			)
			(pin bidirectional line
				(at 17.78 35.56 180)
				(length 3.81)
				(name "P1.16")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 33.02 180)
				(length 3.81)
				(name "P1.17")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 30.48 180)
				(length 3.81)
				(name "P1.18")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 27.94 180)
				(length 3.81)
				(name "P1.19")
				(number "4")
			)
			(pin bidirectional line
				(at 17.78 25.4 180)
				(length 3.81)
				(name "P1.20")
				(number "48")
			)
			(pin bidirectional line
				(at 17.78 22.86 180)
				(length 3.81)
				(name "P1.21")
				(number "44")
			)
			(pin bidirectional line
				(at 17.78 20.32 180)
				(length 3.81)
				(name "P1.22")
				(number "40")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "P1.23")
				(number "36")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "P1.24")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "P1.25")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "P1.26")
				(number "24")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "P1.27")
				(number "64")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "P1.28")
				(number "60")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "P1.29")
				(number "56")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "P1.30")
				(number "52")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "P1.31")
				(number "20")
			)
			(pin input line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "~{RESET}")
				(number "57")
			)
			(pin input line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "VREF")
				(number "63")
			)
			(pin input line
				(at 17.78 -17.78 180)
				(length 3.81)
				(name "XTAL1")
				(number "62")
			)
			(pin output line
				(at 17.78 -20.32 180)
				(length 3.81)
				(name "XTAL2")
				(number "61")
			)
			(pin input line
				(at 17.78 -25.4 180)
				(length 3.81)
				(name "RTXC1")
				(number "3")
			)
			(pin output line
				(at 17.78 -27.94 180)
				(length 3.81)
				(name "RTXC2")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 -33.02 180)
				(length 3.81)
				(name "D+")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -35.56 180)
				(length 3.81)
				(name "D-")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC811M001JDH16"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 12.7 0)
		)
		(property "Value" "LPC811M001JDH16"
			(at 20.32 12.7 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 24.13 15.24 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC81XM.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 8kB flash, 2kB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LPC811M001JDH16_0_1")
		(symbol "LPC811M001JDH16_1_1"
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PIO0_0")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "PIO0_1")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "PIO0_2")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "PIO0_3")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "PIO0_4")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "PIO0_5")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "PIO0_6")
				(number "15")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PIO0_7")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PIO0_8")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PIO0_9")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "PIO0_10")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PIO0_11")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PIO0_12")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "PIO0_13")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC812M101JD20"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 15.24 0)
		)
		(property "Value" "LPC812M101JD20"
			(at 19.05 15.24 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 2.54 17.78 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC81XM.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16kB flash, 4kB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "LPC812M101JD20_0_1")
		(symbol "LPC812M101JD20_1_1"
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "PIO0_0")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PIO0_1")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "PIO0_2")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "PIO0_3")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "PIO0_4")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "PIO0_5")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "PIO0_6")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "PIO0_7")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "PIO0_8")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PIO0_9")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PIO0_10")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PIO0_11")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PIO0_12")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "PIO0_13")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PIO0_14")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PIO0_15")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "PIO0_16")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "PIO0_17")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC812M101JDH20"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 15.24 0)
		)
		(property "Value" "LPC812M101JDH20"
			(at 20.32 15.24 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 25.4 17.78 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC81XM.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16kB flash, 4kB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LPC812M101JDH20_0_1")
		(symbol "LPC812M101JDH20_1_1"
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "PIO0_0")
				(number "19")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PIO0_1")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "PIO0_2")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "PIO0_3")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "PIO0_4")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "PIO0_5")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "PIO0_6")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "PIO0_7")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "PIO0_8")
				(number "14")
			)
			(pin power_in line
				(at 0 17.78 270)
				(length 3.81)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at 0 -17.78 90)
				(length 3.81)
				(name "VSS")
				(number "16")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PIO0_9")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PIO0_10")
				(number "9")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PIO0_11")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PIO0_12")
				(number "3")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "PIO0_13")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PIO0_14")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PIO0_15")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "PIO0_16")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "PIO0_17")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC812M101JTB16"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 12.7 0)
		)
		(property "Value" "LPC812M101JTB16"
			(at 20.32 12.7 0)
		)
		(property "Footprint" "Package_SON:NXP_XSON-16"
			(at 2.54 15.24 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC81XM.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16kB flash, 4kB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "NXP*XSON*"
			(at 0 0 0)
		)
		(symbol "LPC812M101JTB16_0_1")
		(symbol "LPC812M101JTB16_1_1"
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PIO0_0")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "PIO0_1")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "PIO0_2")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "PIO0_3")
				(number "5")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "PIO0_4")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "PIO0_5")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "PIO0_6")
				(number "15")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 3.81)
				(name "VDD")
				(number "12")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 3.81)
				(name "VSS")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PIO0_7")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PIO0_8")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PIO0_9")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "PIO0_10")
				(number "8")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PIO0_11")
				(number "7")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PIO0_12")
				(number "2")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "PIO0_13")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC822M101JDH20"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 16.51 0)
		)
		(property "Value" "LPC822M101JDH20"
			(at 21.59 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 26.67 19.05 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC82X.pdf"
			(at 3.81 16.51 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16kB flash, 4kB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "LPC822M101JDH20_0_1")
		(symbol "LPC822M101JDH20_1_1"
			(pin bidirectional line
				(at -20.32 10.16 0)
				(length 5.08)
				(name "PIO0_0")
				(number "19")
			)
			(pin bidirectional line
				(at -20.32 7.62 0)
				(length 5.08)
				(name "PIO0_1")
				(number "12")
			)
			(pin bidirectional line
				(at -20.32 5.08 0)
				(length 5.08)
				(name "PIO0_2")
				(number "8")
			)
			(pin bidirectional line
				(at -20.32 2.54 0)
				(length 5.08)
				(name "PIO0_3")
				(number "7")
			)
			(pin bidirectional line
				(at -20.32 0 0)
				(length 5.08)
				(name "PIO0_4")
				(number "6")
			)
			(pin bidirectional line
				(at -20.32 -2.54 0)
				(length 5.08)
				(name "PIO0_5")
				(number "5")
			)
			(pin bidirectional line
				(at -20.32 -5.08 0)
				(length 5.08)
				(name "PIO0_8")
				(number "14")
			)
			(pin bidirectional line
				(at -20.32 -7.62 0)
				(length 5.08)
				(name "PIO0_9")
				(number "13")
			)
			(pin power_in line
				(at -2.54 20.32 270)
				(length 5.08)
				(name "VDD")
				(number "15")
			)
			(pin power_in line
				(at -2.54 -20.32 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at 2.54 20.32 270)
				(length 5.08)
				(name "VREFP")
				(number "18")
			)
			(pin power_in line
				(at 2.54 -20.32 90)
				(length 5.08)
				(name "VREFN")
				(number "17")
			)
			(pin bidirectional line
				(at 20.32 10.16 180)
				(length 5.08)
				(name "PIO0_10")
				(number "10")
			)
			(pin bidirectional line
				(at 20.32 7.62 180)
				(length 5.08)
				(name "PIO0_11")
				(number "9")
			)
			(pin bidirectional line
				(at 20.32 5.08 180)
				(length 5.08)
				(name "PIO0_12")
				(number "4")
			)
			(pin bidirectional line
				(at 20.32 2.54 180)
				(length 5.08)
				(name "PIO0_13")
				(number "3")
			)
			(pin bidirectional line
				(at 20.32 0 180)
				(length 5.08)
				(name "PIO0_14")
				(number "20")
			)
			(pin bidirectional line
				(at 20.32 -2.54 180)
				(length 5.08)
				(name "PIO0_15")
				(number "11")
			)
			(pin bidirectional line
				(at 20.32 -5.08 180)
				(length 5.08)
				(name "PIO0_17")
				(number "2")
			)
			(pin bidirectional line
				(at 20.32 -7.62 180)
				(length 5.08)
				(name "PIO0_23")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC822M101JHI33"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -11.43 22.86 0)
		)
		(property "Value" "LPC822M101JHI33"
			(at 19.05 22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 25.4 25.4 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC82X.pdf"
			(at 3.81 16.51 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16kB flash, 4kB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "LPC822M101JHI33_0_1")
		(symbol "LPC822M101JHI33_1_1"
			(pin bidirectional line
				(at -17.78 17.78 0)
				(length 3.81)
				(name "PIO0_0")
				(number "24")
			)
			(pin bidirectional line
				(at -17.78 15.24 0)
				(length 3.81)
				(name "PIO0_1")
				(number "16")
			)
			(pin bidirectional line
				(at -17.78 12.7 0)
				(length 3.81)
				(name "PIO0_2")
				(number "7")
			)
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 3.81)
				(name "PIO0_3")
				(number "6")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 3.81)
				(name "PIO0_4")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 3.81)
				(name "PIO0_5")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 3.81)
				(name "PIO0_6")
				(number "23")
			)
			(pin bidirectional line
				(at -17.78 0 0)
				(length 3.81)
				(name "PIO0_7")
				(number "22")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 3.81)
				(name "PIO0_8")
				(number "18")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 3.81)
				(name "PIO0_9")
				(number "17")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 3.81)
				(name "PIO0_10")
				(number "9")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 3.81)
				(name "PIO0_11")
				(number "8")
			)
			(pin bidirectional line
				(at -17.78 -12.7 0)
				(length 3.81)
				(name "PIO0_12")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 -15.24 0)
				(length 3.81)
				(name "PIO0_13")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 -17.78 0)
				(length 3.81)
				(name "PIO0_14")
				(number "25")
			)
			(pin power_in line
				(at -2.54 25.4 270)
				(length 3.81)
				(name "VDD")
				(number "19")
			)
			(pin power_in line
				(at -2.54 -25.4 90)
				(length 3.81)
				(name "VSS")
				(number "33")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 3.81)
				(name "VREFP")
				(number "21")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 3.81)
				(name "VREFN")
				(number "20")
			)
			(pin bidirectional line
				(at 17.78 17.78 180)
				(length 3.81)
				(name "PIO0_15")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 15.24 180)
				(length 3.81)
				(name "PIO0_16")
				(number "10")
			)
			(pin bidirectional line
				(at 17.78 12.7 180)
				(length 3.81)
				(name "PIO0_17")
				(number "32")
			)
			(pin bidirectional line
				(at 17.78 10.16 180)
				(length 3.81)
				(name "PIO0_18")
				(number "31")
			)
			(pin bidirectional line
				(at 17.78 7.62 180)
				(length 3.81)
				(name "PIO0_19")
				(number "30")
			)
			(pin bidirectional line
				(at 17.78 5.08 180)
				(length 3.81)
				(name "PIO0_20")
				(number "29")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 3.81)
				(name "PIO0_21")
				(number "28")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 3.81)
				(name "PIO0_22")
				(number "27")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 3.81)
				(name "PIO0_23")
				(number "26")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 3.81)
				(name "PIO0_24")
				(number "14")
			)
			(pin bidirectional line
				(at 17.78 -7.62 180)
				(length 3.81)
				(name "PIO0_25")
				(number "13")
			)
			(pin bidirectional line
				(at 17.78 -10.16 180)
				(length 3.81)
				(name "PIO0_26")
				(number "12")
			)
			(pin bidirectional line
				(at 17.78 -12.7 180)
				(length 3.81)
				(name "PIO0_27")
				(number "11")
			)
			(pin bidirectional line
				(at 17.78 -15.24 180)
				(length 3.81)
				(name "PIO0_28")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "LPC1111FHN33-102"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1111FHN33-102"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 8KB flash, 2KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1111FHN33-103"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1111FHN33-103"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 8KB flash, 2KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1111FHN33-201"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1111FHN33-201"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 8KB flash, 4KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1111FHN33-202"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1111FHN33-202"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 8KB flash, 4KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1111FHN33-203"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1111FHN33-203"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 8KB flash, 4KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1111JHN33-103"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1111JHN33-103"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 8KB flash, 2KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1111JHN33-203"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1111JHN33-203"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 8KB flash, 4KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1112FHI33-202"
		(extends "LPC1112FHI33-102")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1112FHI33-202"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16KB flash, 4KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1112FHI33-203"
		(extends "LPC1112FHI33-102")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1112FHI33-203"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16KB flash, 4KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1112FHN33-101"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1112FHN33-101"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16KB flash, 2KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1112FHN33-102"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1112FHN33-102"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16KB flash, 2KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1112FHN33-103"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1112FHN33-103"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16KB flash, 2KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1112FHN33-201"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1112FHN33-201"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16KB flash, 4KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1112FHN33-202"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1112FHN33-202"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16KB flash, 4KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1112FHN33-203"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1112FHN33-203"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16KB flash, 4KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1112JHI33-203"
		(extends "LPC1112FHI33-102")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1112JHI33-203"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16KB flash, 4KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1112JHN33-103"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1112JHN33-103"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16KB flash, 2KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1112JHN33-203"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1112JHN33-203"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16KB flash, 4KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1113FBD48-302"
		(extends "LPC1113FBD48-301")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1113FBD48-302"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 24KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1113FBD48-303"
		(extends "LPC1113FBD48-301")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1113FBD48-303"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 24KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1113FHN33-201"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1113FHN33-201"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 24KB flash, 4KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1113FHN33-202"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1113FHN33-202"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 24KB flash, 4KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1113FHN33-203"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1113FHN33-203"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 24KB flash, 4KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1113FHN33-301"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1113FHN33-301"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 24KB flash, 8KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1113FHN33-302"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1113FHN33-302"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 24KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1113FHN33-303"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1113FHN33-303"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 24KB flash, 8KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1113JBD48-303"
		(extends "LPC1113FBD48-301")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1113JBD48-303"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 24KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1113JHN33-203"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1113JHN33-203"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 24KB flash, 4KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1113JHN33-303"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1113JHN33-303"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 24KB flash, 8KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FBD48-301"
		(extends "LPC1113FBD48-301")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1114FBD48-301"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 8KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FBD48-302"
		(extends "LPC1113FBD48-301")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1114FBD48-302"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FBD48-303"
		(extends "LPC1113FBD48-301")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1114FBD48-303"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FBD48-323"
		(extends "LPC1113FBD48-301")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1114FBD48-323"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 48KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FBD48-333"
		(extends "LPC1113FBD48-301")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1114FBD48-333"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 56KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FHI33-302"
		(extends "LPC1112FHI33-102")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1114FHI33-302"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FHI33-303"
		(extends "LPC1112FHI33-102")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1114FHI33-303"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FHN33-201"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1114FHN33-201"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 4KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FHN33-202"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1114FHN33-202"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 4KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FHN33-203"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1114FHN33-203"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 4KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FHN33-301"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1114FHN33-301"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 8KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FHN33-302"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1114FHN33-302"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FHN33-303"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1114FHN33-303"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 8KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114FHN33-333"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1114FHN33-333"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 56KB flash, 8KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114JBD48-303"
		(extends "LPC1113FBD48-301")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1114JBD48-303"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114JBD48-323"
		(extends "LPC1113FBD48-301")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1114JBD48-323"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 48KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114JBD48-333"
		(extends "LPC1113FBD48-301")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1114JBD48-333"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 56KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114JHI33-303"
		(extends "LPC1112FHI33-102")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1114JHI33-303"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1114JHN33-203"
		(extends "LPC1111FHN33-101")
		(property "Reference" "U"
			(at -12.7 25.4 0)
		)
		(property "Value" "LPC1114JHN33-203"
			(at 13.97 25.4 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_7x7mm_P0.65mm_EP4.7x4.7mm_ThermalVias"
			(at 27.94 27.94 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 0 0 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32KB flash, 4KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*7x7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1115FBD48-303"
		(extends "LPC1113FBD48-301")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1115FBD48-303"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 64KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1115JBD48-303"
		(extends "LPC1113FBD48-301")
		(property "Reference" "U"
			(at -12.7 36.83 0)
		)
		(property "Value" "LPC1115JBD48-303"
			(at 13.97 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC111X.pdf"
			(at 48.26 15.24 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 64KB flash, 8KB SRAM, power profile"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC11E13FBD48-301"
		(extends "LPC11E12FBD48-201")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "LPC11E13FBD48-301"
			(at 24.13 34.29 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 36.83 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11E1X.pdf"
			(at 1.27 34.29 0)
		)
		(property "Description" "LPC11E1x, 50MHz Cortex-M0 MCU, 24kB Flash, 2kB EEPROM, 8kB SRAM, USART, I2C, SSP, ADC, Power Profile, LQFP48"
			(at 0 0 0)
		)
		(property "ki_keywords" "nxp lpc arm microcontroller cortex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC11E14FBD48-401"
		(extends "LPC11E12FBD48-201")
		(property "Reference" "U"
			(at -12.7 34.29 0)
		)
		(property "Value" "LPC11E14FBD48-401"
			(at 24.13 34.29 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 22.86 36.83 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U1X.pdf"
			(at 1.27 34.29 0)
		)
		(property "Description" "LPC11U00 USB series, 50MHz Cortex-M0 MCU, USB, ADC, USART, I2C, SPI, LQFP48 package"
			(at 0 0 0)
		)
		(property "ki_keywords" "nxp lpc arm microcontroller cortex"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC11U13FBD48-201"
		(extends "LPC11U12FBD48-201")
		(property "Reference" "U"
			(at -12.7 35.56 0)
		)
		(property "Value" "LPC11U13FBD48-201"
			(at 12.7 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 21.59 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U1X.pdf"
			(at 0 -37.465 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, USB, 24KB flash, 6KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC11U14FBD48-201"
		(extends "LPC11U12FBD48-201")
		(property "Reference" "U"
			(at -12.7 35.56 0)
		)
		(property "Value" "LPC11U14FBD48-201"
			(at 12.7 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 21.59 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U1X.pdf"
			(at 0 -37.465 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, USB, 32KB flash, 6KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC11U22FBD48-301"
		(extends "LPC11U12FBD48-201")
		(property "Reference" "U"
			(at -12.7 35.56 0)
		)
		(property "Value" "LPC11U22FBD48-301"
			(at 12.7 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 21.59 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U2X.pdf"
			(at 0 -37.465 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, USB, 16KB flash, 8KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC11U23FBD48-301"
		(extends "LPC11U12FBD48-201")
		(property "Reference" "U"
			(at -12.7 35.56 0)
		)
		(property "Value" "LPC11U23FBD48-301"
			(at 12.7 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 21.59 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U2X.pdf"
			(at 0 -37.465 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, USB, 24KB flash, 8KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC11U24FBD48-301"
		(extends "LPC11U12FBD48-201")
		(property "Reference" "U"
			(at -12.7 35.56 0)
		)
		(property "Value" "LPC11U24FBD48-301"
			(at 12.7 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 21.59 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U2X.pdf"
			(at 0 -37.465 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, USB, 32KB flash, 8KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC11U24FBD48-401"
		(extends "LPC11U12FBD48-201")
		(property "Reference" "U"
			(at -12.7 35.56 0)
		)
		(property "Value" "LPC11U24FBD48-401"
			(at 12.7 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 21.59 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U2X.pdf"
			(at 0 -37.465 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, USB, 32KB flash, 10KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC11U34FBD48-311"
		(extends "LPC11U12FBD48-201")
		(property "Reference" "U"
			(at -12.7 35.56 0)
		)
		(property "Value" "LPC11U34FBD48-311"
			(at 12.7 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 21.59 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U3X.pdf"
			(at 0 -37.465 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, USB, 40KB flash, 8KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC11U34FBD48-421"
		(extends "LPC11U12FBD48-201")
		(property "Reference" "U"
			(at -12.7 35.56 0)
		)
		(property "Value" "LPC11U34FBD48-421"
			(at 12.7 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 21.59 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U3X.pdf"
			(at 0 -37.465 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, USB, 48KB flash, 10KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC11U35FBD48-401"
		(extends "LPC11U12FBD48-201")
		(property "Reference" "U"
			(at -12.7 35.56 0)
		)
		(property "Value" "LPC11U35FBD48-401"
			(at 12.7 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 21.59 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U3X.pdf"
			(at 0 -37.465 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, USB, 64KB flash, 10KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC11U36FBD48-401"
		(extends "LPC11U12FBD48-201")
		(property "Reference" "U"
			(at -12.7 35.56 0)
		)
		(property "Value" "LPC11U36FBD48-401"
			(at 12.7 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 21.59 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U3X.pdf"
			(at 0 -37.465 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, USB, 96KB flash, 10KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC11U37FBD48-401_"
		(extends "LPC11U12FBD48-201")
		(property "Reference" "U"
			(at -12.7 35.56 0)
		)
		(property "Value" "LPC11U37FBD48-401_"
			(at 12.7 35.56 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 21.59 38.1 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC11U3X.pdf"
			(at 0 -37.465 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, USB, 128KB flash, 10KB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1224FBD48-121"
		(extends "LPC1224FBD48-101")
		(property "Reference" "U"
			(at -13.97 44.45 0)
		)
		(property "Value" "LPC1224FBD48-121"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 15.24 46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC122X.pdf"
			(at -12.7 11.43 0)
		)
		(property "Description" "LPC122x 32-bit ARM Cortex-M0 microcontroller, 48 kB FLASH, 4 kB SRAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1224FBD64-121"
		(extends "LPC1224FBD64-101")
		(property "Reference" "U"
			(at -13.97 44.45 0)
		)
		(property "Value" "LPC1224FBD64-121"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 15.24 46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC122X.pdf"
			(at -12.7 11.43 0)
		)
		(property "Description" "LPC122x 32-bit ARM Cortex-M0 microcontroller, 48 kB FLASH, 4 kB SRAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1225FBD48-301"
		(extends "LPC1224FBD48-101")
		(property "Reference" "U"
			(at -13.97 44.45 0)
		)
		(property "Value" "LPC1225FBD48-301"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 15.24 46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC122X.pdf"
			(at -12.7 11.43 0)
		)
		(property "Description" "LPC122x 32-bit ARM Cortex-M0 microcontroller, 64 kB FLASH, 8 kB SRAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1225FBD48-321"
		(extends "LPC1224FBD48-101")
		(property "Reference" "U"
			(at -13.97 44.45 0)
		)
		(property "Value" "LPC1225FBD48-321"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 15.24 46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC122X.pdf"
			(at -12.7 11.43 0)
		)
		(property "Description" "LPC122x 32-bit ARM Cortex-M0 microcontroller, 80 kB FLASH, 8 kB SRAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1225FBD64-301"
		(extends "LPC1224FBD64-101")
		(property "Reference" "U"
			(at -13.97 44.45 0)
		)
		(property "Value" "LPC1225FBD64-301"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 15.24 46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC122X.pdf"
			(at -12.7 11.43 0)
		)
		(property "Description" "LPC122x 32-bit ARM Cortex-M0 microcontroller, 64 kB FLASH, 8 kB SRAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1225FBD64-321"
		(extends "LPC1224FBD64-101")
		(property "Reference" "U"
			(at -13.97 44.45 0)
		)
		(property "Value" "LPC1225FBD64-321"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 15.24 46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC122X.pdf"
			(at -12.7 11.43 0)
		)
		(property "Description" "LPC122x 32-bit ARM Cortex-M0 microcontroller, 80 kB FLASH, 8 kB SRAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1226FBD48-301"
		(extends "LPC1224FBD48-101")
		(property "Reference" "U"
			(at -13.97 44.45 0)
		)
		(property "Value" "LPC1226FBD48-301"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 15.24 46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC122X.pdf"
			(at -12.7 11.43 0)
		)
		(property "Description" "LPC122x 32-bit ARM Cortex-M0 microcontroller, 96 kB FLASH, 8 kB SRAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1226FBD64-301"
		(extends "LPC1224FBD64-101")
		(property "Reference" "U"
			(at -13.97 44.45 0)
		)
		(property "Value" "LPC1226FBD64-301"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 15.24 46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC122X.pdf"
			(at -12.7 11.43 0)
		)
		(property "Description" "LPC122x 32-bit ARM Cortex-M0 microcontroller, 96 kB FLASH, 8 kB SRAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1227FBD48-301"
		(extends "LPC1224FBD48-101")
		(property "Reference" "U"
			(at -13.97 44.45 0)
		)
		(property "Value" "LPC1227FBD48-301"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 15.24 46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC122X.pdf"
			(at -12.7 11.43 0)
		)
		(property "Description" "LPC122x 32-bit ARM Cortex-M0 microcontroller, 128 kB FLASH, 8 kB SRAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1227FBD64-301"
		(extends "LPC1224FBD64-101")
		(property "Reference" "U"
			(at -13.97 44.45 0)
		)
		(property "Value" "LPC1227FBD64-301"
			(at 15.24 44.45 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 15.24 46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/LPC122X.pdf"
			(at -12.7 11.43 0)
		)
		(property "Description" "LPC122x 32-bit ARM Cortex-M0 microcontroller, 128 kB FLASH, 8 kB SRAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1764FBD100"
		(extends "LPC1763FBD100")
		(property "Reference" "U"
			(at -17.78 62.23 0)
		)
		(property "Value" "LPC1764FBD100"
			(at 20.32 62.23 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 33.02 64.77 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC1769_68_67_66_65_64_63.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "32-bit ARM Cortex-M3 microcontroller, 128KB flash, 32KB RAM, Ethernet, USB"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M3, M3, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1765FBD100"
		(extends "LPC1763FBD100")
		(property "Reference" "U"
			(at -17.78 62.23 0)
		)
		(property "Value" "LPC1765FBD100"
			(at 20.32 62.23 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 33.02 64.77 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC1769_68_67_66_65_64_63.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "32-bit ARM Cortex-M3 microcontroller, 256KB flash, 64KB RAM, USB"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M3, M3, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1766FBD100"
		(extends "LPC1763FBD100")
		(property "Reference" "U"
			(at -17.78 62.23 0)
		)
		(property "Value" "LPC1766FBD100"
			(at 20.32 62.23 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 33.02 64.77 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC1769_68_67_66_65_64_63.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "32-bit ARM Cortex-M3 microcontroller, 256KB flash, 64KB RAM, Ethernet, USB"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M3, M3, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1767FBD100"
		(extends "LPC1763FBD100")
		(property "Reference" "U"
			(at -17.78 62.23 0)
		)
		(property "Value" "LPC1767FBD100"
			(at 20.32 62.23 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 33.02 64.77 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC1769_68_67_66_65_64_63.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "32-bit ARM Cortex-M3 microcontroller, 512KB flash, 64KB RAM, Ethernet"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M3, M3, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1768FBD100"
		(extends "LPC1763FBD100")
		(property "Reference" "U"
			(at -17.78 62.23 0)
		)
		(property "Value" "LPC1768FBD100"
			(at 20.32 62.23 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 33.02 64.77 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC1769_68_67_66_65_64_63.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "32-bit ARM Cortex-M3 microcontroller, 512KB flash, 64KB RAM, Ethernet, USB"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M3, M3, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC1769FBD100"
		(extends "LPC1763FBD100")
		(property "Reference" "U"
			(at -17.78 62.23 0)
		)
		(property "Value" "LPC1769FBD100"
			(at 20.32 62.23 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 33.02 64.77 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC1769_68_67_66_65_64_63.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "32-bit ARM Cortex-M3 microcontroller, 512KB flash, 64KB RAM, Ethernet, USB"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M3, M3, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC2142FBD64"
		(extends "LPC2141FBD64")
		(property "Reference" "U"
			(at -12.7 46.99 0)
		)
		(property "Value" "LPC2142FBD64"
			(at 13.97 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 26.67 49.53 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC2141_42_44_46_48.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit/32-bit ARM7TDMI-S microcontroller, 64kB flash, 16kB RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 16-bit, 32-bit, ARM7, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC2144FBD64"
		(extends "LPC2141FBD64")
		(property "Reference" "U"
			(at -12.7 46.99 0)
		)
		(property "Value" "LPC2144FBD64"
			(at 13.97 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 26.67 49.53 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC2141_42_44_46_48.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit/32-bit ARM7TDMI-S microcontroller, 128kB flash, 16kB RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 16-bit, 32-bit, ARM7, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC2146FBD64"
		(extends "LPC2141FBD64")
		(property "Reference" "U"
			(at -12.7 46.99 0)
		)
		(property "Value" "LPC2146FBD64"
			(at 13.97 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 26.67 49.53 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC2141_42_44_46_48.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit/32-bit ARM7TDMI-S microcontroller, 256kB flash, 40kB RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 16-bit, 32-bit, ARM7, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC2148FBD64"
		(extends "LPC2141FBD64")
		(property "Reference" "U"
			(at -12.7 46.99 0)
		)
		(property "Value" "LPC2148FBD64"
			(at 13.97 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 26.67 49.53 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC2141_42_44_46_48.pdf"
			(at 0 0 0)
		)
		(property "Description" "16-bit/32-bit ARM7TDMI-S microcontroller, 512kB flash, 40kB RAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 16-bit, 32-bit, ARM7, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC812M001JDH16"
		(extends "LPC811M001JDH16")
		(property "Reference" "U"
			(at -11.43 12.7 0)
		)
		(property "Value" "LPC812M001JDH16"
			(at 20.32 12.7 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 24.13 15.24 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC81XM.pdf"
			(at 0 -12.7 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16kB flash, 4kB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC824M201JDH20"
		(extends "LPC822M101JDH20")
		(property "Reference" "U"
			(at -11.43 16.51 0)
		)
		(property "Value" "LPC824M201JDH20"
			(at 21.59 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 26.67 19.05 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC82X.pdf"
			(at 3.81 16.51 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32kB flash, 8kB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC824M201JHI33"
		(extends "LPC822M101JHI33")
		(property "Reference" "U"
			(at -11.43 22.86 0)
		)
		(property "Value" "LPC824M201JHI33"
			(at 19.05 22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 25.4 25.4 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC82X.pdf"
			(at 3.81 16.51 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32kB flash, 8kB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC832M101FDH20"
		(extends "LPC822M101JDH20")
		(property "Reference" "U"
			(at -11.43 16.51 0)
		)
		(property "Value" "LPC832M101FDH20"
			(at 21.59 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 26.67 19.05 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC83X.pdf"
			(at 3.81 16.51 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 16kB flash, 4kB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "LPC834M101FHI33"
		(extends "LPC822M101JHI33")
		(property "Reference" "U"
			(at -11.43 22.86 0)
		)
		(property "Value" "LPC834M101FHI33"
			(at 19.05 22.86 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-32-1EP_5x5mm_P0.5mm_EP3.45x3.45mm"
			(at 25.4 25.4 0)
		)
		(property "Datasheet" "http://www.nxp.com/docs/en/data-sheet/LPC83X.pdf"
			(at 3.81 16.51 0)
		)
		(property "Description" "32-bit ARM Cortex-M0 microcontroller, 32kB flash, 4kB SRAM"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM, 32-bit, Cortex-M0, M0, NXP, microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "*QFN*5x5mm*P0.5mm*"
			(at 0 0 0)
		)
	)
)
