(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "MAC7101"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 1.27 -44.45 0)
		)
		(property "Value" "MAC7101"
			(at 1.27 16.51 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at 1.27 -1.27 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MAC7100EC.pdf"
			(at 1.27 -1.27 0)
		)
		(property "Description" "Automotive ARM7TDMI-S-based Microcontroller, LQFP-144"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM7TDMI-S MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAC7101_0_1")
		(symbol "MAC7101_1_1"
			(pin input line
				(at -35.56 83.82 0)
				(length 7.62)
				(name "EXTAL")
				(number "60")
			)
			(pin output line
				(at -35.56 81.28 0)
				(length 7.62)
				(name "XTAL")
				(number "61")
			)
			(pin bidirectional inverted
				(at -35.56 78.74 0)
				(length 7.62)
				(name "RESET")
				(number "48")
			)
			(pin bidirectional line
				(at -35.56 76.2 0)
				(length 7.62)
				(name "PD0/MODB")
				(number "70")
			)
			(pin bidirectional line
				(at -35.56 73.66 0)
				(length 7.62)
				(name "PD1/MODA")
				(number "71")
			)
			(pin bidirectional line
				(at -35.56 71.12 0)
				(length 7.62)
				(name "PD2/CLKOUT/XCLKS")
				(number "80")
			)
			(pin bidirectional line
				(at -35.56 68.58 0)
				(length 7.62)
				(name "PD3/XIRQ")
				(number "81")
			)
			(pin bidirectional line
				(at -35.56 66.04 0)
				(length 7.62)
				(name "PD4/IRQ")
				(number "82")
			)
			(pin bidirectional line
				(at -35.56 58.42 0)
				(length 7.62)
				(name "PA0/MCKO")
				(number "138")
			)
			(pin bidirectional line
				(at -35.56 55.88 0)
				(length 7.62)
				(name "PA1/EVTO")
				(number "137")
			)
			(pin bidirectional line
				(at -35.56 53.34 0)
				(length 7.62)
				(name "PA2/EVTI")
				(number "136")
			)
			(pin bidirectional line
				(at -35.56 50.8 0)
				(length 7.62)
				(name "PA3/MDO0")
				(number "135")
			)
			(pin bidirectional line
				(at -35.56 48.26 0)
				(length 7.62)
				(name "PA4/MDO1")
				(number "134")
			)
			(pin bidirectional line
				(at -35.56 45.72 0)
				(length 7.62)
				(name "PA5/MSEO")
				(number "133")
			)
			(pin bidirectional line
				(at -35.56 43.18 0)
				(length 7.62)
				(name "PA6/RDY")
				(number "132")
			)
			(pin bidirectional line
				(at -35.56 38.1 0)
				(length 7.62)
				(name "PA13")
				(number "67")
			)
			(pin bidirectional line
				(at -35.56 35.56 0)
				(length 7.62)
				(name "PA14")
				(number "66")
			)
			(pin bidirectional line
				(at -35.56 33.02 0)
				(length 7.62)
				(name "PA15")
				(number "65")
			)
			(pin bidirectional line
				(at -35.56 27.94 0)
				(length 7.62)
				(name "PC0")
				(number "9")
			)
			(pin bidirectional line
				(at -35.56 25.4 0)
				(length 7.62)
				(name "PC1")
				(number "10")
			)
			(pin bidirectional line
				(at -35.56 22.86 0)
				(length 7.62)
				(name "PC2")
				(number "11")
			)
			(pin bidirectional line
				(at -35.56 20.32 0)
				(length 7.62)
				(name "PC3")
				(number "12")
			)
			(pin bidirectional line
				(at -35.56 17.78 0)
				(length 7.62)
				(name "PC4")
				(number "28")
			)
			(pin bidirectional line
				(at -35.56 15.24 0)
				(length 7.62)
				(name "PC5")
				(number "29")
			)
			(pin bidirectional line
				(at -35.56 12.7 0)
				(length 7.62)
				(name "PC6")
				(number "30")
			)
			(pin bidirectional line
				(at -35.56 10.16 0)
				(length 7.62)
				(name "PC7")
				(number "31")
			)
			(pin bidirectional line
				(at -35.56 7.62 0)
				(length 7.62)
				(name "PC8")
				(number "44")
			)
			(pin bidirectional line
				(at -35.56 5.08 0)
				(length 7.62)
				(name "PC9")
				(number "45")
			)
			(pin bidirectional line
				(at -35.56 2.54 0)
				(length 7.62)
				(name "PC10")
				(number "46")
			)
			(pin bidirectional line
				(at -35.56 0 0)
				(length 7.62)
				(name "PC11")
				(number "47")
			)
			(pin bidirectional line
				(at -35.56 -5.08 0)
				(length 7.62)
				(name "PD11")
				(number "68")
			)
			(pin bidirectional line
				(at -35.56 -7.62 0)
				(length 7.62)
				(name "PD12")
				(number "69")
			)
			(pin bidirectional line
				(at -35.56 -10.16 0)
				(length 7.62)
				(name "PD13")
				(number "83")
			)
			(pin bidirectional line
				(at -35.56 -12.7 0)
				(length 7.62)
				(name "PD14")
				(number "84")
			)
			(pin bidirectional line
				(at -35.56 -15.24 0)
				(length 7.62)
				(name "PD15")
				(number "85")
			)
			(pin bidirectional line
				(at -35.56 -30.48 0)
				(length 7.62)
				(name "PF0/NEXPS/eMIOS0")
				(number "43")
			)
			(pin bidirectional line
				(at -35.56 -33.02 0)
				(length 7.62)
				(name "PF1/NEXPR/eMIOS1")
				(number "42")
			)
			(pin bidirectional line
				(at -35.56 -35.56 0)
				(length 7.62)
				(name "PF2/eMIOS2")
				(number "41")
			)
			(pin bidirectional line
				(at -35.56 -38.1 0)
				(length 7.62)
				(name "PF3/eMIOS3")
				(number "40")
			)
			(pin bidirectional line
				(at -35.56 -40.64 0)
				(length 7.62)
				(name "PF4/eMIOS4")
				(number "39")
			)
			(pin bidirectional line
				(at -35.56 -43.18 0)
				(length 7.62)
				(name "PF5/eMIOS5")
				(number "38")
			)
			(pin bidirectional line
				(at -35.56 -45.72 0)
				(length 7.62)
				(name "PF6/eMIOS6")
				(number "37")
			)
			(pin bidirectional line
				(at -35.56 -48.26 0)
				(length 7.62)
				(name "PF7/eMIOS7")
				(number "36")
			)
			(pin bidirectional line
				(at -35.56 -50.8 0)
				(length 7.62)
				(name "PF8/eMIOS8")
				(number "35")
			)
			(pin bidirectional line
				(at -35.56 -53.34 0)
				(length 7.62)
				(name "PF9/eMIOS9")
				(number "34")
			)
			(pin bidirectional line
				(at -35.56 -55.88 0)
				(length 7.62)
				(name "PF10/eMIOS10")
				(number "33")
			)
			(pin bidirectional line
				(at -35.56 -58.42 0)
				(length 7.62)
				(name "PF11/eMIOS11")
				(number "32")
			)
			(pin bidirectional line
				(at -35.56 -60.96 0)
				(length 7.62)
				(name "PF12/eMIOS12")
				(number "27")
			)
			(pin bidirectional line
				(at -35.56 -63.5 0)
				(length 7.62)
				(name "PF13/eMIOS13")
				(number "26")
			)
			(pin bidirectional line
				(at -35.56 -66.04 0)
				(length 7.62)
				(name "PF14/eMIOS14")
				(number "25")
			)
			(pin bidirectional line
				(at -35.56 -68.58 0)
				(length 7.62)
				(name "PF15/eMIOS15")
				(number "24")
			)
			(pin passive line
				(at -35.56 -104.14 0)
				(length 7.62)
				(name "VRH")
				(number "111")
			)
			(pin passive line
				(at -35.56 -106.68 0)
				(length 7.62)
				(name "VRL")
				(number "110")
			)
			(pin bidirectional line
				(at -17.78 96.52 270)
				(length 7.62)
				(name "XFC")
				(number "58")
			)
			(pin power_in line
				(at -17.78 -116.84 90)
				(length 7.62)
				(name "VssX")
				(number "79")
			)
			(pin power_in line
				(at -15.24 -116.84 90)
				(length 7.62)
				(name "VssX")
				(number "13")
			)
			(pin passive line
				(at -12.7 96.52 270)
				(length 7.62)
				(name "VddPLL")
				(number "57")
			)
			(pin power_in line
				(at -12.7 -116.84 90)
				(length 7.62)
				(name "VssX")
				(number "49")
			)
			(pin power_in line
				(at -10.16 -116.84 90)
				(length 7.62)
				(name "VssX")
				(number "63")
			)
			(pin power_in line
				(at -7.62 -116.84 90)
				(length 7.62)
				(name "VssX")
				(number "86")
			)
			(pin passive line
				(at -5.08 96.52 270)
				(length 7.62)
				(name "Vdd2.5")
				(number "53")
			)
			(pin power_in line
				(at -5.08 -116.84 90)
				(length 7.62)
				(name "VssX")
				(number "125")
			)
			(pin power_in line
				(at -2.54 96.52 270)
				(length 7.62)
				(name "Vdd2.5")
				(number "127")
			)
			(pin power_in line
				(at 0 -116.84 90)
				(length 7.62)
				(name "Vss2.5")
				(number "126")
			)
			(pin passive line
				(at 2.54 -116.84 90)
				(length 7.62)
				(name "Vss2.5")
				(number "54")
			)
			(pin power_in line
				(at 5.08 96.52 270)
				(length 7.62)
				(name "VddX")
				(number "14")
			)
			(pin power_in line
				(at 7.62 96.52 270)
				(length 7.62)
				(name "VddX")
				(number "50")
			)
			(pin passive line
				(at 7.62 -116.84 90)
				(length 7.62)
				(name "VssPLL")
				(number "59")
			)
			(pin power_in line
				(at 10.16 96.52 270)
				(length 7.62)
				(name "VddX")
				(number "87")
			)
			(pin power_in line
				(at 12.7 96.52 270)
				(length 7.62)
				(name "VddX")
				(number "64")
			)
			(pin power_in line
				(at 12.7 -116.84 90)
				(length 7.62)
				(name "VssR")
				(number "55")
			)
			(pin power_in line
				(at 15.24 96.52 270)
				(length 7.62)
				(name "VddX")
				(number "124")
			)
			(pin power_in line
				(at 15.24 -116.84 90)
				(length 7.62)
				(name "VssA")
				(number "112")
			)
			(pin power_in line
				(at 20.32 96.52 270)
				(length 7.62)
				(name "VddR")
				(number "56")
			)
			(pin power_in line
				(at 22.86 96.52 270)
				(length 7.62)
				(name "VddA")
				(number "109")
			)
			(pin input line
				(at 38.1 83.82 180)
				(length 7.62)
				(name "TMS")
				(number "131")
			)
			(pin input line
				(at 38.1 81.28 180)
				(length 7.62)
				(name "TCK")
				(number "130")
			)
			(pin output line
				(at 38.1 78.74 180)
				(length 7.62)
				(name "TDO")
				(number "129")
			)
			(pin input line
				(at 38.1 76.2 180)
				(length 7.62)
				(name "TDI")
				(number "128")
			)
			(pin bidirectional line
				(at 38.1 71.12 180)
				(length 7.62)
				(name "PH0/AN0_B")
				(number "88")
			)
			(pin bidirectional line
				(at 38.1 68.58 180)
				(length 7.62)
				(name "MCKO'/PE0/AN0_A")
				(number "89")
			)
			(pin bidirectional line
				(at 38.1 66.04 180)
				(length 7.62)
				(name "PH1/AN1_B")
				(number "90")
			)
			(pin bidirectional line
				(at 38.1 63.5 180)
				(length 7.62)
				(name "EVTO'/PE1/AN1_A")
				(number "91")
			)
			(pin bidirectional line
				(at 38.1 60.96 180)
				(length 7.62)
				(name "PH2/AN2_B")
				(number "92")
			)
			(pin bidirectional line
				(at 38.1 58.42 180)
				(length 7.62)
				(name "EVTI'/PE2/AN2_A")
				(number "93")
			)
			(pin bidirectional line
				(at 38.1 55.88 180)
				(length 7.62)
				(name "PH3/AN3_B")
				(number "94")
			)
			(pin bidirectional line
				(at 38.1 53.34 180)
				(length 7.62)
				(name "MDO0'/PE3/AN3_A")
				(number "95")
			)
			(pin bidirectional line
				(at 38.1 50.8 180)
				(length 7.62)
				(name "PH4/AN4_B")
				(number "96")
			)
			(pin bidirectional line
				(at 38.1 48.26 180)
				(length 7.62)
				(name "MDO1'/PE4/AN4_A")
				(number "97")
			)
			(pin bidirectional line
				(at 38.1 45.72 180)
				(length 7.62)
				(name "PH5/AN5_B")
				(number "98")
			)
			(pin bidirectional line
				(at 38.1 43.18 180)
				(length 7.62)
				(name "MSEO'/PE5/AN5_A")
				(number "99")
			)
			(pin bidirectional line
				(at 38.1 40.64 180)
				(length 7.62)
				(name "PH6/AN6_B")
				(number "100")
			)
			(pin bidirectional line
				(at 38.1 38.1 180)
				(length 7.62)
				(name "RDY'/PE6/AN6_A")
				(number "101")
			)
			(pin bidirectional line
				(at 38.1 35.56 180)
				(length 7.62)
				(name "PH7/AN7_B")
				(number "102")
			)
			(pin bidirectional line
				(at 38.1 33.02 180)
				(length 7.62)
				(name "PE7/AN7_A")
				(number "103")
			)
			(pin bidirectional line
				(at 38.1 30.48 180)
				(length 7.62)
				(name "PH8/AN8_B")
				(number "104")
			)
			(pin bidirectional line
				(at 38.1 27.94 180)
				(length 7.62)
				(name "PE8/AN8_A")
				(number "105")
			)
			(pin bidirectional line
				(at 38.1 25.4 180)
				(length 7.62)
				(name "PH9/AN9_B")
				(number "106")
			)
			(pin bidirectional line
				(at 38.1 22.86 180)
				(length 7.62)
				(name "PE9/AN9_A")
				(number "107")
			)
			(pin bidirectional line
				(at 38.1 20.32 180)
				(length 7.62)
				(name "PH10/AN10_B")
				(number "108")
			)
			(pin bidirectional line
				(at 38.1 17.78 180)
				(length 7.62)
				(name "PE10/AN10_A")
				(number "113")
			)
			(pin bidirectional line
				(at 38.1 15.24 180)
				(length 7.62)
				(name "PH11/AN11_B")
				(number "114")
			)
			(pin bidirectional line
				(at 38.1 12.7 180)
				(length 7.62)
				(name "PE11/AN11_A")
				(number "115")
			)
			(pin bidirectional line
				(at 38.1 10.16 180)
				(length 7.62)
				(name "PH12/AN12_B")
				(number "116")
			)
			(pin bidirectional line
				(at 38.1 7.62 180)
				(length 7.62)
				(name "PE12/AN12_A")
				(number "117")
			)
			(pin bidirectional line
				(at 38.1 5.08 180)
				(length 7.62)
				(name "PH13/AN13_B")
				(number "118")
			)
			(pin bidirectional line
				(at 38.1 2.54 180)
				(length 7.62)
				(name "PE13/AN13_A")
				(number "119")
			)
			(pin bidirectional line
				(at 38.1 0 180)
				(length 7.62)
				(name "PH14/AN14_B")
				(number "120")
			)
			(pin bidirectional line
				(at 38.1 -2.54 180)
				(length 7.62)
				(name "PE14/AN14_A")
				(number "121")
			)
			(pin bidirectional line
				(at 38.1 -5.08 180)
				(length 7.62)
				(name "PH15/AN15_B")
				(number "122")
			)
			(pin bidirectional line
				(at 38.1 -7.62 180)
				(length 7.62)
				(name "PE15/AN15_A")
				(number "123")
			)
			(pin bidirectional line
				(at 38.1 -15.24 180)
				(length 7.62)
				(name "PG0/RXD_B")
				(number "141")
			)
			(pin bidirectional line
				(at 38.1 -17.78 180)
				(length 7.62)
				(name "PG1/TXD_B")
				(number "142")
			)
			(pin bidirectional line
				(at 38.1 -20.32 180)
				(length 7.62)
				(name "PG2/RXD_A")
				(number "143")
			)
			(pin bidirectional line
				(at 38.1 -22.86 180)
				(length 7.62)
				(name "PG3/TXD_A")
				(number "144")
			)
			(pin bidirectional line
				(at 38.1 -25.4 180)
				(length 7.62)
				(name "PG4/CANTXD_A")
				(number "1")
			)
			(pin bidirectional line
				(at 38.1 -27.94 180)
				(length 7.62)
				(name "PG5/CANRXD_A")
				(number "2")
			)
			(pin bidirectional line
				(at 38.1 -30.48 180)
				(length 7.62)
				(name "PG6/CANTXD_B")
				(number "7")
			)
			(pin bidirectional line
				(at 38.1 -33.02 180)
				(length 7.62)
				(name "PG7/CANRXD_B")
				(number "8")
			)
			(pin bidirectional line
				(at 38.1 -35.56 180)
				(length 7.62)
				(name "PG8/CANTXD_C")
				(number "3")
			)
			(pin bidirectional line
				(at 38.1 -38.1 180)
				(length 7.62)
				(name "PG9/CANRXD_C")
				(number "4")
			)
			(pin bidirectional line
				(at 38.1 -40.64 180)
				(length 7.62)
				(name "PG10/CANTXD_D")
				(number "5")
			)
			(pin bidirectional line
				(at 38.1 -43.18 180)
				(length 7.62)
				(name "PG11/CANRXD_D")
				(number "6")
			)
			(pin bidirectional line
				(at 38.1 -45.72 180)
				(length 7.62)
				(name "PG12/RXD_D")
				(number "51")
			)
			(pin bidirectional line
				(at 38.1 -48.26 180)
				(length 7.62)
				(name "PG13/TXD_D")
				(number "52")
			)
			(pin bidirectional line
				(at 38.1 -50.8 180)
				(length 7.62)
				(name "PG14/RXD_C")
				(number "139")
			)
			(pin bidirectional line
				(at 38.1 -53.34 180)
				(length 7.62)
				(name "PG15/TXD_C")
				(number "140")
			)
			(pin bidirectional line
				(at 38.1 -58.42 180)
				(length 7.62)
				(name "PB0/SDA")
				(number "15")
			)
			(pin bidirectional line
				(at 38.1 -60.96 180)
				(length 7.62)
				(name "PB1/SCL")
				(number "16")
			)
			(pin bidirectional line
				(at 38.1 -63.5 180)
				(length 7.62)
				(name "PB2/SIN_A")
				(number "17")
			)
			(pin bidirectional line
				(at 38.1 -66.04 180)
				(length 7.62)
				(name "PB3/SOUT_A")
				(number "18")
			)
			(pin bidirectional line
				(at 38.1 -68.58 180)
				(length 7.62)
				(name "PB4/SCK_A")
				(number "19")
			)
			(pin bidirectional line
				(at 38.1 -71.12 180)
				(length 7.62)
				(name "PB5/PCS0_A/SS_A")
				(number "20")
			)
			(pin bidirectional line
				(at 38.1 -73.66 180)
				(length 7.62)
				(name "PB6/PCS1_A")
				(number "21")
			)
			(pin bidirectional line
				(at 38.1 -76.2 180)
				(length 7.62)
				(name "PB7")
				(number "22")
			)
			(pin bidirectional line
				(at 38.1 -78.74 180)
				(length 7.62)
				(name "PB8/PCS5_A/PCSS_A")
				(number "23")
			)
			(pin bidirectional line
				(at 38.1 -81.28 180)
				(length 7.62)
				(name "PB9/PCS0_B/SS_B")
				(number "72")
			)
			(pin bidirectional line
				(at 38.1 -83.82 180)
				(length 7.62)
				(name "PB10/PCS5_B/PCSS_B")
				(number "73")
			)
			(pin bidirectional line
				(at 38.1 -86.36 180)
				(length 7.62)
				(name "PB11/PCS2_B")
				(number "74")
			)
			(pin bidirectional line
				(at 38.1 -88.9 180)
				(length 7.62)
				(name "PB12/PCS1_B")
				(number "75")
			)
			(pin bidirectional line
				(at 38.1 -91.44 180)
				(length 7.62)
				(name "PB13/PCSSCK_B")
				(number "76")
			)
			(pin bidirectional line
				(at 38.1 -93.98 180)
				(length 7.62)
				(name "PB14/SOUT_B")
				(number "77")
			)
			(pin bidirectional line
				(at 38.1 -96.52 180)
				(length 7.62)
				(name "PB15/SIN_B")
				(number "78")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MAC7111"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -1.27 -44.45 0)
		)
		(property "Value" "MAC7111"
			(at -1.27 16.51 0)
		)
		(property "Footprint" "Package_QFP:LQFP-144_20x20mm_P0.5mm"
			(at -1.27 -1.27 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MAC7100EC.pdf"
			(at -1.27 -1.27 0)
		)
		(property "Description" "Automotive ARM7TDMI-S-based Microcontroller, LQFP-144"
			(at 0 0 0)
		)
		(property "ki_keywords" "ARM7TDMI-S MCU"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*20x20mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MAC7111_0_1")
		(symbol "MAC7111_1_1"
			(pin input line
				(at -38.1 83.82 0)
				(length 7.62)
				(name "EXTAL")
				(number "60")
			)
			(pin output line
				(at -38.1 81.28 0)
				(length 7.62)
				(name "XTAL")
				(number "61")
			)
			(pin bidirectional inverted
				(at -38.1 78.74 0)
				(length 7.62)
				(name "RESET")
				(number "48")
			)
			(pin bidirectional line
				(at -38.1 71.12 0)
				(length 7.62)
				(name "PA0/DATA0/MCKO")
				(number "138")
			)
			(pin bidirectional line
				(at -38.1 68.58 0)
				(length 7.62)
				(name "PA1/DATA1/EVTO")
				(number "137")
			)
			(pin bidirectional line
				(at -38.1 66.04 0)
				(length 7.62)
				(name "PA2/DATA2/EVTI")
				(number "136")
			)
			(pin bidirectional line
				(at -38.1 63.5 0)
				(length 7.62)
				(name "PA3/DATA3/MDO0")
				(number "135")
			)
			(pin bidirectional line
				(at -38.1 60.96 0)
				(length 7.62)
				(name "PA4/DATA4/MDO1")
				(number "134")
			)
			(pin bidirectional line
				(at -38.1 58.42 0)
				(length 7.62)
				(name "PA5/DATA5/MSEO")
				(number "133")
			)
			(pin bidirectional line
				(at -38.1 55.88 0)
				(length 7.62)
				(name "PA6/DATA6/RDY")
				(number "132")
			)
			(pin bidirectional line
				(at -38.1 53.34 0)
				(length 7.62)
				(name "PA7/DATA7")
				(number "98")
			)
			(pin bidirectional line
				(at -38.1 50.8 0)
				(length 7.62)
				(name "PA8/DATA8")
				(number "97")
			)
			(pin bidirectional line
				(at -38.1 48.26 0)
				(length 7.62)
				(name "PA9/DATA9")
				(number "96")
			)
			(pin bidirectional line
				(at -38.1 45.72 0)
				(length 7.62)
				(name "PA10/DATA10")
				(number "95")
			)
			(pin bidirectional line
				(at -38.1 43.18 0)
				(length 7.62)
				(name "PA11/DATA11")
				(number "94")
			)
			(pin bidirectional line
				(at -38.1 40.64 0)
				(length 7.62)
				(name "PA12/DATA12")
				(number "93")
			)
			(pin bidirectional line
				(at -38.1 38.1 0)
				(length 7.62)
				(name "PA13/DATA13")
				(number "67")
			)
			(pin bidirectional line
				(at -38.1 35.56 0)
				(length 7.62)
				(name "PA14/DATA14")
				(number "66")
			)
			(pin bidirectional line
				(at -38.1 33.02 0)
				(length 7.62)
				(name "PA15/DATA15")
				(number "65")
			)
			(pin bidirectional line
				(at -38.1 27.94 0)
				(length 7.62)
				(name "PC0/ADDR0")
				(number "9")
			)
			(pin bidirectional line
				(at -38.1 25.4 0)
				(length 7.62)
				(name "PC1/ADDR1")
				(number "10")
			)
			(pin bidirectional line
				(at -38.1 22.86 0)
				(length 7.62)
				(name "PC2/ADDR2")
				(number "11")
			)
			(pin bidirectional line
				(at -38.1 20.32 0)
				(length 7.62)
				(name "PC3/ADDR3")
				(number "12")
			)
			(pin bidirectional line
				(at -38.1 17.78 0)
				(length 7.62)
				(name "PC4/ADDR4")
				(number "28")
			)
			(pin bidirectional line
				(at -38.1 15.24 0)
				(length 7.62)
				(name "PC5/ADDR5")
				(number "29")
			)
			(pin bidirectional line
				(at -38.1 12.7 0)
				(length 7.62)
				(name "PC6/ADDR6")
				(number "30")
			)
			(pin bidirectional line
				(at -38.1 10.16 0)
				(length 7.62)
				(name "PC7/ADDR7")
				(number "31")
			)
			(pin bidirectional line
				(at -38.1 7.62 0)
				(length 7.62)
				(name "PC8/ADDR8")
				(number "44")
			)
			(pin bidirectional line
				(at -38.1 5.08 0)
				(length 7.62)
				(name "PC9/ADDR9")
				(number "45")
			)
			(pin bidirectional line
				(at -38.1 2.54 0)
				(length 7.62)
				(name "PC10/ADDR10")
				(number "46")
			)
			(pin bidirectional line
				(at -38.1 0 0)
				(length 7.62)
				(name "PC11/ADDR11")
				(number "47")
			)
			(pin bidirectional line
				(at -38.1 -2.54 0)
				(length 7.62)
				(name "PC12/ADDR12")
				(number "88")
			)
			(pin bidirectional line
				(at -38.1 -5.08 0)
				(length 7.62)
				(name "PC13/ADDR13")
				(number "89")
			)
			(pin bidirectional line
				(at -38.1 -7.62 0)
				(length 7.62)
				(name "PC14/ADDR14")
				(number "90")
			)
			(pin bidirectional line
				(at -38.1 -10.16 0)
				(length 7.62)
				(name "PC15/ADDR15")
				(number "91")
			)
			(pin bidirectional line
				(at -38.1 -12.7 0)
				(length 7.62)
				(name "PD5/ADDR16")
				(number "92")
			)
			(pin bidirectional line
				(at -38.1 -15.24 0)
				(length 7.62)
				(name "PD6/ADDR17")
				(number "119")
			)
			(pin bidirectional line
				(at -38.1 -17.78 0)
				(length 7.62)
				(name "PD7/ADDR18")
				(number "120")
			)
			(pin bidirectional line
				(at -38.1 -20.32 0)
				(length 7.62)
				(name "PD8/ADDR19")
				(number "121")
			)
			(pin bidirectional line
				(at -38.1 -22.86 0)
				(length 7.62)
				(name "PD9/ADDR20")
				(number "122")
			)
			(pin bidirectional line
				(at -38.1 -25.4 0)
				(length 7.62)
				(name "PD10/ADDR21")
				(number "123")
			)
			(pin bidirectional line
				(at -38.1 -30.48 0)
				(length 7.62)
				(name "TA/AS")
				(number "79")
			)
			(pin bidirectional line
				(at -38.1 -33.02 0)
				(length 7.62)
				(name "PD15/R/W")
				(number "85")
			)
			(pin bidirectional line
				(at -38.1 -35.56 0)
				(length 7.62)
				(name "PD11/OE")
				(number "68")
			)
			(pin bidirectional line
				(at -38.1 -38.1 0)
				(length 7.62)
				(name "PD2/CLKOUT/XCLKS")
				(number "80")
			)
			(pin bidirectional line
				(at -38.1 -88.9 0)
				(length 7.62)
				(name "PD3/XIRQ")
				(number "81")
			)
			(pin bidirectional line
				(at -38.1 -91.44 0)
				(length 7.62)
				(name "PD4/IRQ")
				(number "82")
			)
			(pin bidirectional line
				(at -38.1 -96.52 0)
				(length 7.62)
				(name "PD0/BS0/MODB")
				(number "70")
			)
			(pin bidirectional line
				(at -38.1 -99.06 0)
				(length 7.62)
				(name "PD1/BS1/MODA")
				(number "71")
			)
			(pin passive line
				(at -38.1 -104.14 0)
				(length 7.62)
				(name "VRH")
				(number "111")
			)
			(pin passive line
				(at -38.1 -106.68 0)
				(length 7.62)
				(name "VRL")
				(number "110")
			)
			(pin bidirectional line
				(at -20.32 96.52 270)
				(length 7.62)
				(name "XFC")
				(number "58")
			)
			(pin power_in line
				(at -17.78 -116.84 90)
				(length 7.62)
				(name "VssX")
				(number "13")
			)
			(pin passive line
				(at -15.24 96.52 270)
				(length 7.62)
				(name "VddPLL")
				(number "57")
			)
			(pin power_in line
				(at -15.24 -116.84 90)
				(length 7.62)
				(name "VssX")
				(number "49")
			)
			(pin power_in line
				(at -12.7 -116.84 90)
				(length 7.62)
				(name "VssX")
				(number "63")
			)
			(pin power_in line
				(at -10.16 -116.84 90)
				(length 7.62)
				(name "VssX")
				(number "86")
			)
			(pin passive line
				(at -7.62 96.52 270)
				(length 7.62)
				(name "Vdd2.5")
				(number "53")
			)
			(pin power_in line
				(at -7.62 -116.84 90)
				(length 7.62)
				(name "VssX")
				(number "125")
			)
			(pin power_in line
				(at -5.08 96.52 270)
				(length 7.62)
				(name "Vdd2.5")
				(number "127")
			)
			(pin power_in line
				(at 0 -116.84 90)
				(length 7.62)
				(name "Vss2.5")
				(number "126")
			)
			(pin power_in line
				(at 2.54 96.52 270)
				(length 7.62)
				(name "VddX")
				(number "14")
			)
			(pin power_in line
				(at 2.54 -116.84 90)
				(length 7.62)
				(name "Vss2.5")
				(number "54")
			)
			(pin power_in line
				(at 5.08 96.52 270)
				(length 7.62)
				(name "VddX")
				(number "50")
			)
			(pin passive line
				(at 5.08 -116.84 90)
				(length 7.62)
				(name "VssPLL")
				(number "59")
			)
			(pin power_in line
				(at 7.62 96.52 270)
				(length 7.62)
				(name "VddX")
				(number "87")
			)
			(pin power_in line
				(at 10.16 96.52 270)
				(length 7.62)
				(name "VddX")
				(number "64")
			)
			(pin power_in line
				(at 10.16 -116.84 90)
				(length 7.62)
				(name "VssR")
				(number "55")
			)
			(pin power_in line
				(at 12.7 96.52 270)
				(length 7.62)
				(name "VddX")
				(number "124")
			)
			(pin power_in line
				(at 12.7 -116.84 90)
				(length 7.62)
				(name "VssA")
				(number "112")
			)
			(pin power_in line
				(at 17.78 96.52 270)
				(length 7.62)
				(name "VddR")
				(number "56")
			)
			(pin power_in line
				(at 20.32 96.52 270)
				(length 7.62)
				(name "VddA")
				(number "109")
			)
			(pin input line
				(at 35.56 83.82 180)
				(length 7.62)
				(name "TMS")
				(number "131")
			)
			(pin input line
				(at 35.56 81.28 180)
				(length 7.62)
				(name "TCK")
				(number "130")
			)
			(pin output line
				(at 35.56 78.74 180)
				(length 7.62)
				(name "TDO")
				(number "129")
			)
			(pin input line
				(at 35.56 76.2 180)
				(length 7.62)
				(name "TDI")
				(number "128")
			)
			(pin bidirectional line
				(at 35.56 71.12 180)
				(length 7.62)
				(name "PE0/MCKO'/AN0_A")
				(number "99")
			)
			(pin bidirectional line
				(at 35.56 68.58 180)
				(length 7.62)
				(name "PE1/EVTO'/AN1_A")
				(number "100")
			)
			(pin bidirectional line
				(at 35.56 66.04 180)
				(length 7.62)
				(name "PE2/EVTI'/AN2_A")
				(number "101")
			)
			(pin bidirectional line
				(at 35.56 63.5 180)
				(length 7.62)
				(name "PE3/MDO0'/AN3_A")
				(number "102")
			)
			(pin bidirectional line
				(at 35.56 60.96 180)
				(length 7.62)
				(name "PE4/MDO1'/AN4_A")
				(number "103")
			)
			(pin bidirectional line
				(at 35.56 58.42 180)
				(length 7.62)
				(name "PE5/MSEO'/AN5_A")
				(number "104")
			)
			(pin bidirectional line
				(at 35.56 55.88 180)
				(length 7.62)
				(name "PE6/RDY/AN6_A")
				(number "105")
			)
			(pin bidirectional line
				(at 35.56 53.34 180)
				(length 7.62)
				(name "PE7/AN7_A")
				(number "106")
			)
			(pin bidirectional line
				(at 35.56 50.8 180)
				(length 7.62)
				(name "PE8/AN8_A")
				(number "107")
			)
			(pin bidirectional line
				(at 35.56 48.26 180)
				(length 7.62)
				(name "PE9/AN9_A")
				(number "108")
			)
			(pin bidirectional line
				(at 35.56 45.72 180)
				(length 7.62)
				(name "PE10/AN10_A")
				(number "113")
			)
			(pin bidirectional line
				(at 35.56 43.18 180)
				(length 7.62)
				(name "PE11/AN11_A")
				(number "114")
			)
			(pin bidirectional line
				(at 35.56 40.64 180)
				(length 7.62)
				(name "PE12/AN12_A")
				(number "115")
			)
			(pin bidirectional line
				(at 35.56 38.1 180)
				(length 7.62)
				(name "PE13/AN13_A")
				(number "116")
			)
			(pin bidirectional line
				(at 35.56 35.56 180)
				(length 7.62)
				(name "PE14/AN14_A")
				(number "117")
			)
			(pin bidirectional line
				(at 35.56 33.02 180)
				(length 7.62)
				(name "PE15/AN15_A")
				(number "118")
			)
			(pin bidirectional line
				(at 35.56 27.94 180)
				(length 7.62)
				(name "PF0/NEXPS/eMIOS0")
				(number "43")
			)
			(pin bidirectional line
				(at 35.56 25.4 180)
				(length 7.62)
				(name "PF1/NEXPR/eMIOS1")
				(number "42")
			)
			(pin bidirectional line
				(at 35.56 22.86 180)
				(length 7.62)
				(name "PF2/eMIOS2")
				(number "41")
			)
			(pin bidirectional line
				(at 35.56 20.32 180)
				(length 7.62)
				(name "PF3/eMIOS3")
				(number "40")
			)
			(pin bidirectional line
				(at 35.56 17.78 180)
				(length 7.62)
				(name "PF4/eMIOS4")
				(number "39")
			)
			(pin bidirectional line
				(at 35.56 15.24 180)
				(length 7.62)
				(name "PF5/eMIOS5")
				(number "38")
			)
			(pin bidirectional line
				(at 35.56 12.7 180)
				(length 7.62)
				(name "PF6/eMIOS6")
				(number "37")
			)
			(pin bidirectional line
				(at 35.56 10.16 180)
				(length 7.62)
				(name "PF7/eMIOS7")
				(number "36")
			)
			(pin bidirectional line
				(at 35.56 7.62 180)
				(length 7.62)
				(name "PF8/eMIOS8")
				(number "35")
			)
			(pin bidirectional line
				(at 35.56 5.08 180)
				(length 7.62)
				(name "PF9/eMIOS9")
				(number "34")
			)
			(pin bidirectional line
				(at 35.56 2.54 180)
				(length 7.62)
				(name "PF10/eMIOS10")
				(number "33")
			)
			(pin bidirectional line
				(at 35.56 0 180)
				(length 7.62)
				(name "PF11/eMIOS11")
				(number "32")
			)
			(pin bidirectional line
				(at 35.56 -2.54 180)
				(length 7.62)
				(name "PF12/eMIOS12")
				(number "27")
			)
			(pin bidirectional line
				(at 35.56 -5.08 180)
				(length 7.62)
				(name "PF13/eMIOS13")
				(number "26")
			)
			(pin bidirectional line
				(at 35.56 -7.62 180)
				(length 7.62)
				(name "PF14/eMIOS14")
				(number "25")
			)
			(pin bidirectional line
				(at 35.56 -10.16 180)
				(length 7.62)
				(name "PF15/eMIOS15")
				(number "24")
			)
			(pin bidirectional line
				(at 35.56 -15.24 180)
				(length 7.62)
				(name "PG0/RXD_B")
				(number "141")
			)
			(pin bidirectional line
				(at 35.56 -17.78 180)
				(length 7.62)
				(name "PG1/TXD_B")
				(number "142")
			)
			(pin bidirectional line
				(at 35.56 -20.32 180)
				(length 7.62)
				(name "PG2/RXD_A")
				(number "143")
			)
			(pin bidirectional line
				(at 35.56 -22.86 180)
				(length 7.62)
				(name "PG3/TXD_A")
				(number "144")
			)
			(pin bidirectional line
				(at 35.56 -25.4 180)
				(length 7.62)
				(name "PG4/CANTXD_A")
				(number "1")
			)
			(pin bidirectional line
				(at 35.56 -27.94 180)
				(length 7.62)
				(name "PG5/CANRXD_A")
				(number "2")
			)
			(pin bidirectional line
				(at 35.56 -30.48 180)
				(length 7.62)
				(name "PG6/CANTXD_B")
				(number "7")
			)
			(pin bidirectional line
				(at 35.56 -33.02 180)
				(length 7.62)
				(name "PG7/CANRXD_B")
				(number "8")
			)
			(pin bidirectional line
				(at 35.56 -35.56 180)
				(length 7.62)
				(name "PG8/CANTXD_C")
				(number "3")
			)
			(pin bidirectional line
				(at 35.56 -38.1 180)
				(length 7.62)
				(name "PG9/CANRXD_C")
				(number "4")
			)
			(pin bidirectional line
				(at 35.56 -40.64 180)
				(length 7.62)
				(name "PG10/CANTXD_D")
				(number "5")
			)
			(pin bidirectional line
				(at 35.56 -43.18 180)
				(length 7.62)
				(name "PG11/CANRXD_D")
				(number "6")
			)
			(pin bidirectional line
				(at 35.56 -45.72 180)
				(length 7.62)
				(name "PG12/RXD_D")
				(number "51")
			)
			(pin bidirectional line
				(at 35.56 -48.26 180)
				(length 7.62)
				(name "PG13/TXD_D")
				(number "52")
			)
			(pin bidirectional line
				(at 35.56 -50.8 180)
				(length 7.62)
				(name "PG14/RXD_C")
				(number "139")
			)
			(pin bidirectional line
				(at 35.56 -53.34 180)
				(length 7.62)
				(name "PG15/TXD_C")
				(number "140")
			)
			(pin bidirectional line
				(at 35.56 -58.42 180)
				(length 7.62)
				(name "PB0/SDA")
				(number "15")
			)
			(pin bidirectional line
				(at 35.56 -60.96 180)
				(length 7.62)
				(name "PB1/SCL")
				(number "16")
			)
			(pin bidirectional line
				(at 35.56 -63.5 180)
				(length 7.62)
				(name "PB2/SIN_A")
				(number "17")
			)
			(pin bidirectional line
				(at 35.56 -66.04 180)
				(length 7.62)
				(name "PB3/SOUT_A")
				(number "18")
			)
			(pin bidirectional line
				(at 35.56 -68.58 180)
				(length 7.62)
				(name "PB4/SCK_A")
				(number "19")
			)
			(pin bidirectional line
				(at 35.56 -71.12 180)
				(length 7.62)
				(name "PB5/PCS0_A/SS_A")
				(number "20")
			)
			(pin bidirectional line
				(at 35.56 -73.66 180)
				(length 7.62)
				(name "PB6/PCS1_A")
				(number "21")
			)
			(pin bidirectional line
				(at 35.56 -76.2 180)
				(length 7.62)
				(name "PB7")
				(number "22")
			)
			(pin bidirectional line
				(at 35.56 -78.74 180)
				(length 7.62)
				(name "PB8/PCS5_A/PCSS_A")
				(number "23")
			)
			(pin bidirectional line
				(at 35.56 -81.28 180)
				(length 7.62)
				(name "PB9/PCS0_B/SS_B")
				(number "72")
			)
			(pin bidirectional line
				(at 35.56 -83.82 180)
				(length 7.62)
				(name "PB10/PCS5_B/PCSS_B")
				(number "73")
			)
			(pin bidirectional line
				(at 35.56 -86.36 180)
				(length 7.62)
				(name "PB11/PCS2_B")
				(number "74")
			)
			(pin bidirectional line
				(at 35.56 -88.9 180)
				(length 7.62)
				(name "PB12/PCS1_B")
				(number "75")
			)
			(pin bidirectional line
				(at 35.56 -91.44 180)
				(length 7.62)
				(name "PB13/PCSSCK_B")
				(number "76")
			)
			(pin bidirectional line
				(at 35.56 -93.98 180)
				(length 7.62)
				(name "PB14/SOUT_B")
				(number "77")
			)
			(pin bidirectional line
				(at 35.56 -96.52 180)
				(length 7.62)
				(name "PB15/SIN_B")
				(number "78")
			)
			(pin bidirectional line
				(at 35.56 -101.6 180)
				(length 7.62)
				(name "PD14/CS0")
				(number "84")
			)
			(pin bidirectional line
				(at 35.56 -104.14 180)
				(length 7.62)
				(name "PD13/CS1")
				(number "83")
			)
			(pin bidirectional line
				(at 35.56 -106.68 180)
				(length 7.62)
				(name "PD12/CS2")
				(number "69")
			)
		)
		(embedded_fonts no)
	)
)
