(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "MMC2114CFCPU"
		(pin_names
			(offset 1.016)
		)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at 13.97 67.31 0)
		)
		(property "Value" "MMC2114CFCPU"
			(at 8.89 -67.31 0)
		)
		(property "Footprint" ""
			(at 0 0 0)
		)
		(property "Datasheet" "motorola/mmc2114.pdf"
			(at 0 0 0)
		)
		(property "Description" "Motorola M*CORE  upro 100 pins"
			(at 0 0 0)
		)
		(symbol "MMC2114CFCPU_0_1")
		(symbol "MMC2114CFCPU_1_1"
			(pin input line
				(at -27.94 60.96 0)
				(length 7.62)
				(name "EXTAL")
				(number "87")
			)
			(pin output line
				(at -27.94 58.42 0)
				(length 7.62)
				(name "XTAL")
				(number "86")
			)
			(pin output line
				(at -27.94 53.34 0)
				(length 7.62)
				(name "CLKOUT")
				(number "90")
			)
			(pin input line
				(at -27.94 50.8 0)
				(length 7.62)
				(name "PLLEN")
				(number "85")
			)
			(pin output output_low
				(at -27.94 48.26 0)
				(length 7.62)
				(name "RSTOUT")
				(number "84")
			)
			(pin input input_low
				(at -27.94 45.72 0)
				(length 7.62)
				(name "RESET")
				(number "83")
			)
			(pin output line
				(at -27.94 40.64 0)
				(length 7.62)
				(name "TDO")
				(number "94")
			)
			(pin input line
				(at -27.94 38.1 0)
				(length 7.62)
				(name "TDI")
				(number "93")
			)
			(pin input line
				(at -27.94 35.56 0)
				(length 7.62)
				(name "TMS")
				(number "95")
			)
			(pin input line
				(at -27.94 33.02 0)
				(length 7.62)
				(name "TCLK")
				(number "92")
			)
			(pin input input_low
				(at -27.94 30.48 0)
				(length 7.62)
				(name "TRST")
				(number "98")
			)
			(pin output inverted
				(at -27.94 27.94 0)
				(length 7.62)
				(name "DE")
				(number "99")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 7.62)
				(name "TEST")
				(number "44")
			)
			(pin bidirectional inverted
				(at -27.94 20.32 0)
				(length 7.62)
				(name "PQA0")
				(number "78")
			)
			(pin bidirectional inverted
				(at -27.94 17.78 0)
				(length 7.62)
				(name "PQA1")
				(number "77")
			)
			(pin bidirectional inverted
				(at -27.94 15.24 0)
				(length 7.62)
				(name "PQA3")
				(number "76")
			)
			(pin bidirectional inverted
				(at -27.94 12.7 0)
				(length 7.62)
				(name "PQA4")
				(number "75")
			)
			(pin bidirectional inverted
				(at -27.94 10.16 0)
				(length 7.62)
				(name "PQB0")
				(number "74")
			)
			(pin bidirectional inverted
				(at -27.94 7.62 0)
				(length 7.62)
				(name "PQB1")
				(number "73")
			)
			(pin bidirectional inverted
				(at -27.94 5.08 0)
				(length 7.62)
				(name "PQB2")
				(number "72")
			)
			(pin bidirectional inverted
				(at -27.94 2.54 0)
				(length 7.62)
				(name "PQB3")
				(number "71")
			)
			(pin input line
				(at -27.94 -2.54 0)
				(length 7.62)
				(name "VrH")
				(number "80")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 7.62)
				(name "VrL")
				(number "79")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 7.62)
				(name "MOSI")
				(number "62")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 7.62)
				(name "MISO")
				(number "63")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 7.62)
				(name "SCK")
				(number "65")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 7.62)
				(name "SS")
				(number "66")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 7.62)
				(name "TXD1")
				(number "47")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 7.62)
				(name "RXD1")
				(number "48")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 7.62)
				(name "TXD2")
				(number "45")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 7.62)
				(name "RXD2")
				(number "46")
			)
			(pin bidirectional inverted
				(at -27.94 -38.1 0)
				(length 7.62)
				(name "INT0")
				(number "49")
			)
			(pin bidirectional inverted
				(at -27.94 -40.64 0)
				(length 7.62)
				(name "INT1")
				(number "50")
			)
			(pin bidirectional inverted
				(at -27.94 -43.18 0)
				(length 7.62)
				(name "INT2")
				(number "53")
			)
			(pin bidirectional inverted
				(at -27.94 -45.72 0)
				(length 7.62)
				(name "INT3")
				(number "56")
			)
			(pin bidirectional inverted
				(at -27.94 -48.26 0)
				(length 7.62)
				(name "INT4")
				(number "57")
			)
			(pin bidirectional inverted
				(at -27.94 -50.8 0)
				(length 7.62)
				(name "INT5")
				(number "58")
			)
			(pin bidirectional inverted
				(at -27.94 -53.34 0)
				(length 7.62)
				(name "INT6")
				(number "60")
			)
			(pin bidirectional inverted
				(at -27.94 -55.88 0)
				(length 7.62)
				(name "INT7")
				(number "61")
			)
			(pin power_in line
				(at -10.16 71.12 270)
				(length 7.62)
				(name "VSTBY")
				(number "64")
			)
			(pin power_in line
				(at -10.16 -71.12 90)
				(length 7.62)
				(name "VSSA")
				(number "81")
			)
			(pin power_in line
				(at -7.62 71.12 270)
				(length 7.62)
				(name "VDDA")
				(number "82")
			)
			(pin power_in line
				(at -7.62 -71.12 90)
				(length 7.62)
				(name "VSS")
				(number "12")
			)
			(pin power_in line
				(at -5.08 71.12 270)
				(length 7.62)
				(name "VDDH")
				(number "70")
			)
			(pin power_in line
				(at -5.08 -71.12 90)
				(length 7.62)
				(name "VSS")
				(number "21")
			)
			(pin power_in line
				(at -2.54 71.12 270)
				(length 7.62)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -71.12 90)
				(length 7.62)
				(name "VSS")
				(number "54")
			)
			(pin power_in line
				(at 0 71.12 270)
				(length 7.62)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at 0 -71.12 90)
				(length 7.62)
				(name "VSS")
				(number "88")
			)
			(pin power_in line
				(at 2.54 71.12 270)
				(length 7.62)
				(name "VDD")
				(number "55")
			)
			(pin power_in line
				(at 2.54 -71.12 90)
				(length 7.62)
				(name "VSS")
				(number "89")
			)
			(pin power_in line
				(at 5.08 71.12 270)
				(length 7.62)
				(name "VDD")
				(number "91")
			)
			(pin power_in line
				(at 5.08 -71.12 90)
				(length 7.62)
				(name "VSSF")
				(number "51")
			)
			(pin power_in line
				(at 7.62 71.12 270)
				(length 7.62)
				(name "VDD")
				(number "97")
			)
			(pin power_in line
				(at 7.62 -71.12 90)
				(length 7.62)
				(name "VSS")
				(number "96")
			)
			(pin power_in line
				(at 10.16 71.12 270)
				(length 7.62)
				(name "VDDF")
				(number "52")
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 7.62)
				(name "PA0")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 7.62)
				(name "PA1")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 7.62)
				(name "PA2")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 7.62)
				(name "PA3")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 7.62)
				(name "PA4")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 7.62)
				(name "PA5")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 7.62)
				(name "PA6")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 7.62)
				(name "PA7")
				(number "100")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 7.62)
				(name "PB0")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 7.62)
				(name "PB1")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 7.62)
				(name "PB2")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 7.62)
				(name "PB3")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 7.62)
				(name "PB4")
				(number "11")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 7.62)
				(name "PB5")
				(number "10")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 7.62)
				(name "PB6")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 7.62)
				(name "PB7")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 7.62)
				(name "PC0")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 7.62)
				(name "PC1")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 7.62)
				(name "PC2")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 7.62)
				(name "PC3")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 7.62)
				(name "PC4")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 7.62)
				(name "PC5")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 7.62)
				(name "PC6")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 7.62)
				(name "PC7")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 7.62)
				(name "PD0")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 7.62)
				(name "PD1")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 7.62)
				(name "PD2")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 7.62)
				(name "PD3")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 7.62)
				(name "PD4")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 7.62)
				(name "PD5")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 7.62)
				(name "PD6")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 7.62)
				(name "PD7")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 7.62)
				(name "PE5")
				(number "69")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 7.62)
				(name "PE6")
				(number "68")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 7.62)
				(name "PE7")
				(number "67")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 7.62)
				(name "ICOC10")
				(number "43")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 7.62)
				(name "IC0C11")
				(number "42")
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 7.62)
				(name "ICOC12")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 7.62)
				(name "ICOC13")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 7.62)
				(name "ICOC20")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 7.62)
				(name "ICOC21")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 7.62)
				(name "ICOC22")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 7.62)
				(name "ICOC23")
				(number "36")
			)
		)
		(embedded_fonts no)
	)
)
