(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "NHS3100"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "U"
			(at -13.97 13.97 0)
		)
		(property "Value" "NHS3100"
			(at 8.89 13.97 0)
		)
		(property "Footprint" "Package_DFN_QFN:HVQFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 33.02 -13.97 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/NHS3100.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "Temperature logger, VQFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "NFC Cortex-M0"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "HVQFN*1EP*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "NHS3100_0_1")
		(symbol "NHS3100_1_1"
			(pin bidirectional line
				(at -17.78 10.16 0)
				(length 2.54)
				(name "P0/WAKEUP")
				(number "1")
			)
			(pin bidirectional line
				(at -17.78 7.62 0)
				(length 2.54)
				(name "P1/CLKOUT")
				(number "2")
			)
			(pin bidirectional line
				(at -17.78 5.08 0)
				(length 2.54)
				(name "P2/SSEL")
				(number "3")
			)
			(pin bidirectional line
				(at -17.78 2.54 0)
				(length 2.54)
				(name "P3/CT16B_M0")
				(number "14")
			)
			(pin bidirectional line
				(at -17.78 -2.54 0)
				(length 2.54)
				(name "P4/SCL")
				(number "11")
			)
			(pin bidirectional line
				(at -17.78 -5.08 0)
				(length 2.54)
				(name "P5/SDA")
				(number "12")
			)
			(pin bidirectional line
				(at -17.78 -7.62 0)
				(length 2.54)
				(name "P6/SCLK")
				(number "4")
			)
			(pin bidirectional line
				(at -17.78 -10.16 0)
				(length 2.54)
				(name "P7/CT16B_M1")
				(number "13")
			)
			(pin no_connect line
				(at -15.24 0 0)
				(length 2.54)
				(hide yes)
				(name "reserved")
				(number "10")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 2.54)
				(name "VDDBAT")
				(number "7")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "17")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "18")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "21")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "22")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "23")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "24")
			)
			(pin passive line
				(at 0 -15.24 90)
				(length 2.54)
				(hide yes)
				(name "VSS")
				(number "25")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 2.54)
				(name "VSS")
				(number "8")
			)
			(pin passive line
				(at 17.78 10.16 180)
				(length 2.54)
				(name "LA")
				(number "20")
			)
			(pin passive line
				(at 17.78 7.62 180)
				(length 2.54)
				(name "LB")
				(number "19")
			)
			(pin bidirectional line
				(at 17.78 2.54 180)
				(length 2.54)
				(name "P8/MISO")
				(number "5")
			)
			(pin bidirectional line
				(at 17.78 0 180)
				(length 2.54)
				(name "P9/MOSI")
				(number "6")
			)
			(pin bidirectional line
				(at 17.78 -2.54 180)
				(length 2.54)
				(name "P10/SWCLK")
				(number "15")
			)
			(pin bidirectional line
				(at 17.78 -5.08 180)
				(length 2.54)
				(name "P11/SWDIO")
				(number "16")
			)
			(pin input line
				(at 17.78 -10.16 180)
				(length 2.54)
				(name "~{RESET}")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
)
