(kicad_symbol_lib
	(version 20241209)
	(generator "kicad_symbol_editor")
	(generator_version "9.0")
	(symbol "MC9S08AC128xFDE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 44.45 0)
		)
		(property "Value" "MC9S08AC128xFDE"
			(at 24.13 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC128.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 128kB Flash, 8kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08AC128xFDE_0_1")
		(symbol "MC9S08AC128xFDE_1_1"
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PTF0")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PTF1")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PTF4")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PTF5")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PTF6")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PTG0")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PTG1")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PTG2")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTG3")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PTG4")
				(number "37")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "40")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "IRQ/TPMCLK")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "PTG5/XTAL")
				(number "41")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "PTG6/EXTAL")
				(number "42")
			)
			(pin power_in line
				(at -5.08 48.26 270)
				(length 5.08)
				(name "VDD")
				(number "18")
			)
			(pin power_in line
				(at -5.08 -48.26 90)
				(length 5.08)
				(name "VSS")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -48.26 90)
				(length 5.08)
				(name "VSS")
				(number "43")
			)
			(pin power_in line
				(at 2.54 48.26 270)
				(length 5.08)
				(name "VDDA")
				(number "32")
			)
			(pin power_in line
				(at 2.54 -48.26 90)
				(length 5.08)
				(name "VSSA")
				(number "33")
			)
			(pin power_in line
				(at 5.08 48.26 270)
				(length 5.08)
				(name "VREFH")
				(number "38")
			)
			(pin power_in line
				(at 5.08 -48.26 90)
				(length 5.08)
				(name "VREFL")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PTA0")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PTA1")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PTA7")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PTB0")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PTB1")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PTB2")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTB3")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PTC0")
				(number "44")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTC1")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTC2")
				(number "46")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PTC3")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTC4")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PTC5")
				(number "48")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTD0")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTD1")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PTD2")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTD3")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTE0")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTE1")
				(number "10")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PTE2")
				(number "11")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PTE3")
				(number "12")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PTE4")
				(number "13")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PTE5")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PTE6")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PTE7")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08AC128xFGE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08AC128xFGE"
			(at 24.13 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC128.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 128kB Flash, 8kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08AC128xFGE_0_1")
		(symbol "MC9S08AC128xFGE_1_1"
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PTF0")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PTF1")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PTF4")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PTF5")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PTG0")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PTG1")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTG2")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PTG3")
				(number "33")
			)
			(pin input line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "36")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "IRQ/TPMCLK")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "PTG5/XTAL")
				(number "41")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "PTG6/EXTAL")
				(number "42")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -5.08 -45.72 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 5.08)
				(name "VSS")
				(number "43")
			)
			(pin power_in line
				(at 2.54 45.72 270)
				(length 5.08)
				(name "VDDA")
				(number "29")
			)
			(pin power_in line
				(at 2.54 -45.72 90)
				(length 5.08)
				(name "VSSA")
				(number "30")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 5.08)
				(name "VREFH")
				(number "34")
			)
			(pin power_in line
				(at 5.08 -45.72 90)
				(length 5.08)
				(name "VREFL")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PTA0")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PTA1")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PTB0")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PTB1")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PTB2")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTB3")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PTC0")
				(number "44")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTC1")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTC2")
				(number "46")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PTC3")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTC4")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PTC5")
				(number "48")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTD0")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTD1")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PTD2")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTD3")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTE0")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTE1")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PTE2")
				(number "10")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PTE3")
				(number "11")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PTE4")
				(number "12")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PTE5")
				(number "13")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PTE6")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PTE7")
				(number "15")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08AC128xFUE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AC128xFUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_14x14mm_P0.8mm"
			(at 10.16 -46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC128.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 128kB Flash, 8kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08AC128xFUE_0_1")
		(symbol "MC9S08AC128xFUE_1_1"
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PTE0")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PTE1")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PTE2")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PTE3")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PTE4")
				(number "17")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PTE5")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PTE6")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PTE7")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PTF0")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTF1")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PTF2")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PTF3")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PTF4")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PTF5")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PTF6")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PTF7")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PTG0")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PTG1")
				(number "24")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PTG2")
				(number "25")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PTG3")
				(number "48")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PTG4")
				(number "49")
			)
			(pin input line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "56")
			)
			(pin input line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "IRQ/TPMCLK")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "PTG5/XTAL")
				(number "57")
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "PTG6/EXTAL")
				(number "58")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 5.08)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 5.08)
				(name "VSS")
				(number "21")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 5.08)
				(name "VSS")
				(number "59")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 5.08)
				(name "VDDA")
				(number "44")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 5.08)
				(name "VSSA")
				(number "45")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 5.08)
				(name "VREFH")
				(number "54")
			)
			(pin power_in line
				(at 5.08 -50.8 90)
				(length 5.08)
				(name "VREFL")
				(number "55")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PTA1")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PTA2")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PTA3")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PTA4")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PTA5")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PTA6")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PTA7")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTB0")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PTB1")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PTB2")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTB4")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PTB5")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTB6")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PTB7")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTC0")
				(number "60")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTC1")
				(number "61")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PTC2")
				(number "62")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTC3")
				(number "63")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PTC4")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTC5")
				(number "64")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTC6")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PTD0")
				(number "42")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PTD1")
				(number "43")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PTD2")
				(number "46")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PTD3")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PTD4")
				(number "50")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PTD5")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PTD6")
				(number "52")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PTD7")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08AC128xLKE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 59.69 0)
		)
		(property "Value" "MC9S08AC128xLKE"
			(at 22.86 59.69 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at 10.16 -59.69 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC128.pdf"
			(at 2.54 35.56 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 128kB Flash, 8kB RAM, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08AC128xLKE_0_1")
		(symbol "MC9S08AC128xLKE_1_1"
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 5.08)
				(name "PTF0")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "PTF1")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "PTF2")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 45.72 0)
				(length 5.08)
				(name "PTF3")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "PTF4")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PTF5")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PTF6")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PTF7")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PTG0")
				(number "31")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PTG1")
				(number "32")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PTG2")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PTG3")
				(number "60")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PTG4")
				(number "61")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTH0")
				(number "42")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PTH1")
				(number "43")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PTH2")
				(number "44")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PTH3")
				(number "45")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PTH4")
				(number "75")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PTH5")
				(number "76")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PTH6")
				(number "77")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PTJ0")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PTJ1")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PTJ2")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PTJ3")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PTJ4")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PTJ5")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PTJ6")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PTJ7")
				(number "30")
			)
			(pin input line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "68")
			)
			(pin input line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "IRQ/TPMCLK")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 -50.8 0)
				(length 5.08)
				(name "PTG5/XTAL")
				(number "69")
			)
			(pin bidirectional line
				(at -27.94 -53.34 0)
				(length 5.08)
				(name "PTG6/EXTAL")
				(number "70")
			)
			(pin power_in line
				(at -5.08 63.5 270)
				(length 5.08)
				(name "VDD")
				(number "26")
			)
			(pin power_in line
				(at -5.08 -63.5 90)
				(length 5.08)
				(name "VSS")
				(number "25")
			)
			(pin power_in line
				(at -2.54 63.5 270)
				(length 5.08)
				(name "VDD")
				(number "72")
			)
			(pin power_in line
				(at -2.54 -63.5 90)
				(length 5.08)
				(name "VSS")
				(number "71")
			)
			(pin power_in line
				(at 2.54 63.5 270)
				(length 5.08)
				(name "VDDA")
				(number "56")
			)
			(pin power_in line
				(at 2.54 -63.5 90)
				(length 5.08)
				(name "VSSA")
				(number "57")
			)
			(pin power_in line
				(at 5.08 63.5 270)
				(length 5.08)
				(name "VREFH")
				(number "66")
			)
			(pin power_in line
				(at 5.08 -63.5 90)
				(length 5.08)
				(name "VREFL")
				(number "67")
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PTA0")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PTA1")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PTA2")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 45.72 180)
				(length 5.08)
				(name "PTA3")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PTA4")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PTA5")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PTA6")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PTA7")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PTB0")
				(number "46")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PTB1")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PTB2")
				(number "48")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PTB3")
				(number "49")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PTB4")
				(number "50")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTB5")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PTB6")
				(number "52")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PTB7")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTC0")
				(number "73")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PTC1")
				(number "74")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTC2")
				(number "78")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PTC3")
				(number "79")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PTC4")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTC5")
				(number "80")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTC6")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTD0")
				(number "54")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PTD1")
				(number "55")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTD2")
				(number "58")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTD3")
				(number "59")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PTD4")
				(number "62")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PTD5")
				(number "63")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PTD6")
				(number "64")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PTD7")
				(number "65")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PTE0")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PTE1")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PTE2")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PTE3")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 -45.72 180)
				(length 5.08)
				(name "PTE4")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "PTE5")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 5.08)
				(name "PTE6")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 5.08)
				(name "PTE7")
				(number "24")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08AC128xPUE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AC128xPUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC128.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 128kB Flash, 8kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08AC128xPUE_0_1")
		(symbol "MC9S08AC128xPUE_1_1"
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PTE0")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PTE1")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PTE2")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PTE3")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PTE4")
				(number "17")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PTE5")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PTE6")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PTE7")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PTF0")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTF1")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PTF2")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PTF3")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PTF4")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PTF5")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PTF6")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PTF7")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PTG0")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PTG1")
				(number "24")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PTG2")
				(number "25")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PTG3")
				(number "48")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PTG4")
				(number "49")
			)
			(pin input line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "56")
			)
			(pin input line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "IRQ/TPMCLK")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "PTG5/XTAL")
				(number "57")
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "PTG6/EXTAL")
				(number "58")
			)
			(pin power_in line
				(at -5.08 50.8 270)
				(length 5.08)
				(name "VDD")
				(number "22")
			)
			(pin power_in line
				(at -5.08 -50.8 90)
				(length 5.08)
				(name "VSS")
				(number "21")
			)
			(pin power_in line
				(at -2.54 -50.8 90)
				(length 5.08)
				(name "VSS")
				(number "59")
			)
			(pin power_in line
				(at 2.54 50.8 270)
				(length 5.08)
				(name "VDDA")
				(number "44")
			)
			(pin power_in line
				(at 2.54 -50.8 90)
				(length 5.08)
				(name "VSSA")
				(number "45")
			)
			(pin power_in line
				(at 5.08 50.8 270)
				(length 5.08)
				(name "VREFH")
				(number "54")
			)
			(pin power_in line
				(at 5.08 -50.8 90)
				(length 5.08)
				(name "VREFL")
				(number "55")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PTA1")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PTA2")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PTA3")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PTA4")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PTA5")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PTA6")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PTA7")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTB0")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PTB1")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PTB2")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTB4")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PTB5")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTB6")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PTB7")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTC0")
				(number "60")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTC1")
				(number "61")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PTC2")
				(number "62")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTC3")
				(number "63")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PTC4")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTC5")
				(number "64")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTC6")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PTD0")
				(number "42")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PTD1")
				(number "43")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PTD2")
				(number "46")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PTD3")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PTD4")
				(number "50")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PTD5")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PTD6")
				(number "52")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PTD7")
				(number "53")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08AC60xFJE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 29.21 0)
		)
		(property "Value" "MC9S08AC60xFJE"
			(at 22.86 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 10.16 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 11.43 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 60kB Flash, 2kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08AC60xFJE_0_1")
		(symbol "MC9S08AC60xFJE_1_1"
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PTF4")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PTF5")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTG0")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PTG1")
				(number "16")
			)
			(pin input line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "~{RESET}")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "27")
			)
			(pin input line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "IRQ/TPMCLK")
				(number "1")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PTG5/XTAL")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PTG6/EXTAL")
				(number "29")
			)
			(pin power_in line
				(at -5.08 33.02 270)
				(length 5.08)
				(name "VDD")
				(number "14")
			)
			(pin power_in line
				(at -5.08 -33.02 90)
				(length 5.08)
				(name "VSS")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 5.08)
				(name "VSS")
				(number "30")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 5.08)
				(name "VDDA")
				(number "21")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 5.08)
				(name "VSSA")
				(number "22")
			)
			(pin power_in line
				(at 5.08 33.02 270)
				(length 5.08)
				(name "VREFH")
				(number "25")
			)
			(pin power_in line
				(at 5.08 -33.02 90)
				(length 5.08)
				(name "VREFL")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PTB0")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PTB1")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTB2")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PTB3")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTC0")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTC1")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTD2")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PTD3")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTE0")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTE1")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PTE2")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTE3")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PTE4")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTE5")
				(number "10")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTE6")
				(number "11")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PTE7")
				(number "12")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08DZ128xLF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DZ128xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ128.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 128kB Flash, 8kB RAM, 2kB EEPROM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08DZ128xLF_0_1")
		(symbol "MC9S08DZ128xLF_1_1"
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PTE0")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PTE1")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PTE2")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PTE3")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PTE4")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PTE5")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PTE6")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTE7")
				(number "22")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PTF0")
				(number "17")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PTF1")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PTF2")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PTF3")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PTF4")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PTF5")
				(number "10")
			)
			(pin input line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "~{RESET}")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "33")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PTG0/EXTAL")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PTG1/XTAL")
				(number "7")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 5.08)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at -5.08 -43.18 90)
				(length 5.08)
				(name "VSS")
				(number "5")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 5.08)
				(name "VDD")
				(number "30")
			)
			(pin power_in line
				(at -2.54 -43.18 90)
				(length 5.08)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "43")
			)
			(pin power_in line
				(at 5.08 -43.18 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "42")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PTA0")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PTA1")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PTA2")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PTA3")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PTA4")
				(number "44")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PTA5")
				(number "46")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTA6")
				(number "48")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PTA7")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTB0")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTB1")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PTB2")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTB3")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PTB4")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PTB5")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTB6")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTB7")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTD0")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PTD1")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTD2")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTD3")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PTD4")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PTD5")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PTD6")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PTD7")
				(number "32")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08DZ128xLH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 49.53 0)
		)
		(property "Value" "MC9S08DZ128xLH"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ128.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 128kB Flash, 8kB RAM, 2kB EEPROM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08DZ128xLH_0_1")
		(symbol "MC9S08DZ128xLH_1_1"
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "PTE0")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PTE1")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PTE2")
				(number "17")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PTE3")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PTE4")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PTE5")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PTE6")
				(number "29")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PTE7")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PTF0")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PTF1")
				(number "24")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTF2")
				(number "25")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PTF3")
				(number "26")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PTF4")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PTF5")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PTF6")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PTF7")
				(number "37")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PTG0/EXTAL")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PTG1/XTAL")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PTG2")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PTG3")
				(number "22")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PTG4")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PTG5")
				(number "28")
			)
			(pin input line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "~{RESET}")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "42")
			)
			(pin power_in line
				(at -5.08 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "39")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "38")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "58")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "55")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VREFH")
				(number "57")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VREFL")
				(number "56")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PTA0")
				(number "46")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PTA1")
				(number "49")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PTA2")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PTA3")
				(number "54")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PTA4")
				(number "59")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PTA5")
				(number "62")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PTA6")
				(number "64")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PTA7")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PTB0")
				(number "44")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTB1")
				(number "48")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PTB2")
				(number "50")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PTB3")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTB4")
				(number "60")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTB5")
				(number "63")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PTB6")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTB7")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PTC0")
				(number "43")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTC1")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTC2")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PTC3")
				(number "52")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTC4")
				(number "61")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PTC5")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTC6")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTC7")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PTD0")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PTD1")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PTD2")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PTD3")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PTD4")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PTD5")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PTD6")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PTD7")
				(number "41")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08DZ128xLL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 72.39 0)
		)
		(property "Value" "MC9S08DZ128xLL"
			(at 22.86 72.39 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 10.16 -72.39 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ128.pdf"
			(at 2.54 48.26 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 128kB Flash, 8kB RAM, 2kB EEPROM, LQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08DZ128xLL_0_1")
		(symbol "MC9S08DZ128xLL_1_1"
			(pin bidirectional line
				(at -27.94 66.04 0)
				(length 5.08)
				(name "PTG0/EXTAL")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 63.5 0)
				(length 5.08)
				(name "PTG1/XTAL")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 60.96 0)
				(length 5.08)
				(name "PTG2")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 58.42 0)
				(length 5.08)
				(name "PTG3")
				(number "31")
			)
			(pin bidirectional line
				(at -27.94 55.88 0)
				(length 5.08)
				(name "PTG4")
				(number "40")
			)
			(pin bidirectional line
				(at -27.94 53.34 0)
				(length 5.08)
				(name "PTG5")
				(number "41")
			)
			(pin bidirectional line
				(at -27.94 50.8 0)
				(length 5.08)
				(name "PTG6")
				(number "42")
			)
			(pin bidirectional line
				(at -27.94 48.26 0)
				(length 5.08)
				(name "PTG7")
				(number "43")
			)
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "PTH0")
				(number "55")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PTH1")
				(number "56")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PTH2")
				(number "57")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PTH3")
				(number "58")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PTH4")
				(number "66")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PTH5")
				(number "67")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PTH6")
				(number "68")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PTH7")
				(number "69")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PTJ0")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PTJ1")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTJ2")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PTJ3")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PTJ4")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PTJ5")
				(number "21")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PTJ6")
				(number "22")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PTJ7")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PTK0")
				(number "83")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PTK1")
				(number "84")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PTK2")
				(number "85")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PTK3")
				(number "86")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "PTK4")
				(number "91")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PTK5")
				(number "92")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PTK6")
				(number "93")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PTK7")
				(number "94")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PTL0")
				(number "46")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PTL1")
				(number "47")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PTL2")
				(number "48")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "PTL3")
				(number "60")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "PTL4")
				(number "82")
			)
			(pin bidirectional line
				(at -27.94 -38.1 0)
				(length 5.08)
				(name "PTL5")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "PTL6")
				(number "32")
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "PTL7")
				(number "33")
			)
			(pin input line
				(at -27.94 -55.88 0)
				(length 5.08)
				(name "~{RESET}")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 -58.42 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "65")
			)
			(pin power_in line
				(at -5.08 76.2 270)
				(length 5.08)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at -5.08 -76.2 90)
				(length 5.08)
				(name "VSS")
				(number "10")
			)
			(pin power_in line
				(at -2.54 76.2 270)
				(length 5.08)
				(name "VDD")
				(number "38")
			)
			(pin power_in line
				(at -2.54 -76.2 90)
				(length 5.08)
				(name "VSS")
				(number "39")
			)
			(pin power_in line
				(at 0 76.2 270)
				(length 5.08)
				(name "VDD")
				(number "62")
			)
			(pin power_in line
				(at 0 -76.2 90)
				(length 5.08)
				(name "VSS")
				(number "61")
			)
			(pin power_in line
				(at 2.54 76.2 270)
				(length 5.08)
				(name "VDDA")
				(number "90")
			)
			(pin power_in line
				(at 2.54 -76.2 90)
				(length 5.08)
				(name "VSSA")
				(number "87")
			)
			(pin power_in line
				(at 5.08 76.2 270)
				(length 5.08)
				(name "VREFH")
				(number "89")
			)
			(pin power_in line
				(at 5.08 -76.2 90)
				(length 5.08)
				(name "VREFL")
				(number "88")
			)
			(pin bidirectional line
				(at 27.94 66.04 180)
				(length 5.08)
				(name "PTA0")
				(number "73")
			)
			(pin bidirectional line
				(at 27.94 63.5 180)
				(length 5.08)
				(name "PTA1")
				(number "76")
			)
			(pin bidirectional line
				(at 27.94 60.96 180)
				(length 5.08)
				(name "PTA2")
				(number "78")
			)
			(pin bidirectional line
				(at 27.94 58.42 180)
				(length 5.08)
				(name "PTA3")
				(number "81")
			)
			(pin bidirectional line
				(at 27.94 55.88 180)
				(length 5.08)
				(name "PTA4")
				(number "95")
			)
			(pin bidirectional line
				(at 27.94 53.34 180)
				(length 5.08)
				(name "PTA5")
				(number "98")
			)
			(pin bidirectional line
				(at 27.94 50.8 180)
				(length 5.08)
				(name "PTA6")
				(number "100")
			)
			(pin bidirectional line
				(at 27.94 48.26 180)
				(length 5.08)
				(name "PTA7")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PTB0")
				(number "71")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PTB1")
				(number "75")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PTB2")
				(number "77")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PTB3")
				(number "80")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PTB4")
				(number "96")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PTB5")
				(number "99")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PTB6")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PTB7")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PTC0")
				(number "70")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTC1")
				(number "72")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PTC2")
				(number "74")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PTC3")
				(number "79")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTC4")
				(number "97")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTC5")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PTC6")
				(number "4")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTC7")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PTD0")
				(number "49")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTD1")
				(number "50")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTD2")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PTD3")
				(number "52")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTD4")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PTD5")
				(number "54")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTD6")
				(number "63")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTD7")
				(number "64")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PTE0")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PTE1")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PTE2")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PTE3")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PTE4")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 -38.1 180)
				(length 5.08)
				(name "PTE5")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 -40.64 180)
				(length 5.08)
				(name "PTE6")
				(number "44")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "PTE7")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 -48.26 180)
				(length 5.08)
				(name "PTF0")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 -50.8 180)
				(length 5.08)
				(name "PTF1")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 -53.34 180)
				(length 5.08)
				(name "PTF2")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 -55.88 180)
				(length 5.08)
				(name "PTF3")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 -58.42 180)
				(length 5.08)
				(name "PTF4")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 -60.96 180)
				(length 5.08)
				(name "PTF5")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 -63.5 180)
				(length 5.08)
				(name "PTF6")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 -66.04 180)
				(length 5.08)
				(name "PTF7")
				(number "59")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08DZ60xLC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -20.32 29.21 0)
		)
		(property "Value" "MC9S08DZ60xLC"
			(at 20.32 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 7.62 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 60kB Flash, 4kB RAM, 2kB EEPROM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08DZ60xLC_0_1")
		(symbol "MC9S08DZ60xLC_1_1"
			(pin bidirectional line
				(at -25.4 22.86 0)
				(length 5.08)
				(name "PTE0")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PTE1")
				(number "8")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PTE2")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PTE3")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PTE4")
				(number "11")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PTE5")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PTE6")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PTE7")
				(number "14")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "~{RESET}")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PTG0/EXTAL")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 -20.32 0)
				(length 5.08)
				(name "PTG1/XTAL")
				(number "5")
			)
			(pin power_in line
				(at -2.54 33.02 270)
				(length 5.08)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at -2.54 -33.02 90)
				(length 5.08)
				(name "VSS")
				(number "3")
			)
			(pin power_in line
				(at 2.54 33.02 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "29")
			)
			(pin power_in line
				(at 2.54 -33.02 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 22.86 180)
				(length 5.08)
				(name "PTA0")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PTA1")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PTA2")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PTA3")
				(number "27")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PTA4")
				(number "30")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PTA5")
				(number "31")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PTA6")
				(number "32")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PTA7")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PTB0")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PTB1")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PTD0")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PTD1")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PTD2")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PTD3")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PTD4")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -20.32 180)
				(length 5.08)
				(name "PTD5")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08EL32xTJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -16.51 21.59 0)
		)
		(property "Value" "MC9S08EL32xTJ"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08EL32.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit EEPROM with LIN Microcontroller, S08 core, 32kB Flash, 1kB RAM, 512B EEPROM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08EL32xTJ_0_1")
		(symbol "MC9S08EL32xTJ_1_1"
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PTC0")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PTC1")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PTC2")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTC3")
				(number "9")
			)
			(pin input line
				(at -22.86 0 0)
				(length 5.08)
				(name "~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA0")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA1")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA2")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA3")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTB5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08EL32xTL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -19.05 24.13 0)
		)
		(property "Value" "MC9S08EL32xTL"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 6.35 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08EL32.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit EEPROM with LIN Microcontroller, S08 core, 32kB Flash, 1kB RAM, 512B EEPROM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08EL32xTL_0_1")
		(symbol "MC9S08EL32xTL_1_1"
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PTB0")
				(number "20")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PTB1")
				(number "19")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PTB2")
				(number "18")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PTB3")
				(number "17")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PTB4")
				(number "12")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PTB5")
				(number "11")
			)
			(pin input line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "9")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PTA1")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PTA3")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PTA6")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PTA7")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PTC0")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PTC1")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PTC2")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PTC3")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PTC5")
				(number "1")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PTC4")
				(number "2")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PTC6")
				(number "28")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PTC7")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08FL16xLC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 31.75 0)
		)
		(property "Value" "MC9S08FL16xLC"
			(at 17.78 31.75 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 5.08 -31.75 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08FL16RM.pdf"
			(at 2.54 7.62 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 16kB Flash, 1kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08FL16xLC_0_1")
		(symbol "MC9S08FL16xLC_1_1"
			(pin bidirectional line
				(at -22.86 25.4 0)
				(length 5.08)
				(name "PTC0")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PTC1")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PTC2")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PTC3")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PTC4")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PTC5")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PTC6")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTC7")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -20.32 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "6")
			)
			(pin power_in line
				(at 0 35.56 270)
				(length 5.08)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -35.56 90)
				(length 5.08)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 25.4 180)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 5.08)
				(name "PTA1")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PTA2")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PTA3")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA6")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA7")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTB0")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTB1")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTB2")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PTB3")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB4")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB5")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTD0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTD1")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTD2")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PTD3")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 5.08)
				(name "PTD4")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PTD5")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08JM16xLC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 31.75 0)
		)
		(property "Value" "MC9S08JM16xLC"
			(at 22.86 31.75 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 10.16 -31.75 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08JM16.pdf"
			(at 2.54 7.62 0)
		)
		(property "Description" "8-bit USB Cost-Effective Microcontroller, S08 core, 16kB Flash, 1kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08JM16xLC_0_1")
		(symbol "MC9S08JM16xLC_1_1"
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PTF4")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PTF5")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PTG2")
				(number "25")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTG3")
				(number "26")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "USBDN")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "USBDP")
				(number "16")
			)
			(pin input line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "~{RESET}")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "PTG4/XTAL")
				(number "28")
			)
			(pin bidirectional line
				(at -27.94 -25.4 0)
				(length 5.08)
				(name "PTG5/EXTAL")
				(number "29")
			)
			(pin power_in line
				(at -5.08 35.56 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at -5.08 -35.56 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin power_out line
				(at -2.54 35.56 270)
				(length 5.08)
				(name "VUSB33")
				(number "17")
			)
			(pin power_in line
				(at -2.54 -35.56 90)
				(length 5.08)
				(name "VSSOSC")
				(number "30")
			)
			(pin power_in line
				(at 5.08 35.56 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "22")
			)
			(pin power_in line
				(at 5.08 -35.56 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PTB4")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PTB5")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTC0")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PTC1")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTD0")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTD1")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PTD2")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PTE0")
				(number "5")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PTE1")
				(number "6")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTE2")
				(number "7")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTE3")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PTE4")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTE5")
				(number "10")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PTE6")
				(number "11")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTE7")
				(number "12")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "IRQ/TPMCLK")
				(number "1")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08JM60xGT"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08JM60xGT"
			(at 22.86 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08JM60.pdf"
			(at 2.54 17.78 0)
		)
		(property "Description" "8-bit USB Cost-Effective Microcontroller, S08 core, 60kB Flash, 4kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08JM60xGT_0_1")
		(symbol "MC9S08JM60xGT_1_1"
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PTE0")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PTE1")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PTE2")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PTE3")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PTE4")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PTE5")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PTE6")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PTE7")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PTF0")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PTF1")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PTF4")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PTF5")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PTF6")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "USBDN")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 -12.7 0)
				(length 5.08)
				(name "USBDP")
				(number "20")
			)
			(pin input line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 -22.86 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "40")
			)
			(pin bidirectional line
				(at -27.94 -33.02 0)
				(length 5.08)
				(name "PTG4/XTAL")
				(number "41")
			)
			(pin bidirectional line
				(at -27.94 -35.56 0)
				(length 5.08)
				(name "PTG5/EXTAL")
				(number "42")
			)
			(pin power_in line
				(at -5.08 45.72 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -5.08 -45.72 90)
				(length 5.08)
				(name "VSS")
				(number "18")
			)
			(pin power_out line
				(at -2.54 45.72 270)
				(length 5.08)
				(name "VUSB33")
				(number "21")
			)
			(pin power_in line
				(at -2.54 -45.72 90)
				(length 5.08)
				(name "VSSOSC")
				(number "43")
			)
			(pin power_in line
				(at 5.08 45.72 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "34")
			)
			(pin power_in line
				(at 5.08 -45.72 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PTA0")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PTA5")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PTB0")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PTB1")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PTB2")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PTB3")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTB4")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PTB5")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTC0")
				(number "44")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTC1")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PTC2")
				(number "46")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTC3")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PTC4")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PTC5")
				(number "48")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTD0")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PTD1")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTD2")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PTD7")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTG0")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PTG1")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PTG2")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PTG3")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "IRQ/TPMCLK")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08JM60xLD"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 36.83 0)
		)
		(property "Value" "MC9S08JM60xLD"
			(at 22.86 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -36.83 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08JM60.pdf"
			(at 2.54 12.7 0)
		)
		(property "Description" "8-bit USB Cost-Effective Microcontroller, S08 core, 60kB Flash, 4kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08JM60xLD_0_1")
		(symbol "MC9S08JM60xLD_1_1"
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PTE0")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PTE1")
				(number "9")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PTE2")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PTE3")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PTE4")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PTE5")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTE6")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PTE7")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PTF0")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PTF1")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PTF4")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PTF5")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "USBDN")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "USBDP")
				(number "19")
			)
			(pin input line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "36")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PTG4/XTAL")
				(number "37")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PTG5/EXTAL")
				(number "38")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 5.08)
				(name "VDD")
				(number "16")
			)
			(pin power_in line
				(at -5.08 -40.64 90)
				(length 5.08)
				(name "VSS")
				(number "17")
			)
			(pin power_out line
				(at -2.54 40.64 270)
				(length 5.08)
				(name "VUSB33")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 5.08)
				(name "VSSOSC")
				(number "39")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "31")
			)
			(pin power_in line
				(at 5.08 -40.64 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PTB0")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PTB1")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PTB2")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PTB3")
				(number "26")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PTB4")
				(number "27")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTB5")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PTC0")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTC1")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTC2")
				(number "42")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PTC3")
				(number "43")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTC4")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PTC5")
				(number "44")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTD0")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTD1")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PTD2")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PTG0")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTG1")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTG2")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PTG3")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "IRQ/TPMCLK")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08JM60xLH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 49.53 0)
		)
		(property "Value" "MC9S08JM60xLH"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08JM60.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit USB Cost-Effective Microcontroller, S08 core, 60kB Flash, 4kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08JM60xLH_0_1")
		(symbol "MC9S08JM60xLH_1_1"
			(pin bidirectional line
				(at -27.94 43.18 0)
				(length 5.08)
				(name "PTE0")
				(number "13")
			)
			(pin bidirectional line
				(at -27.94 40.64 0)
				(length 5.08)
				(name "PTE1")
				(number "14")
			)
			(pin bidirectional line
				(at -27.94 38.1 0)
				(length 5.08)
				(name "PTE2")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 35.56 0)
				(length 5.08)
				(name "PTE3")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PTE4")
				(number "17")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PTE5")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PTE6")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PTE7")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PTF0")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PTF1")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTF2")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PTF3")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PTF4")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PTF5")
				(number "11")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PTF6")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PTF7")
				(number "10")
			)
			(pin bidirectional line
				(at -27.94 -2.54 0)
				(length 5.08)
				(name "PTG0")
				(number "26")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PTG1")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PTG2")
				(number "54")
			)
			(pin bidirectional line
				(at -27.94 -10.16 0)
				(length 5.08)
				(name "PTG3")
				(number "55")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "USBDN")
				(number "23")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "USBDP")
				(number "24")
			)
			(pin input line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "56")
			)
			(pin bidirectional line
				(at -27.94 -40.64 0)
				(length 5.08)
				(name "PTG4/XTAL")
				(number "57")
			)
			(pin bidirectional line
				(at -27.94 -43.18 0)
				(length 5.08)
				(name "PTG5/EXTAL")
				(number "58")
			)
			(pin power_in line
				(at -5.08 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "21")
			)
			(pin power_in line
				(at -5.08 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "22")
			)
			(pin power_out line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VUSB33")
				(number "25")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSSOSC")
				(number "59")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VDDA")
				(number "44")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VSSA")
				(number "47")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VREFH")
				(number "45")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VREFL")
				(number "46")
			)
			(pin bidirectional line
				(at 27.94 43.18 180)
				(length 5.08)
				(name "PTA0")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 40.64 180)
				(length 5.08)
				(name "PTA1")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 38.1 180)
				(length 5.08)
				(name "PTA2")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 35.56 180)
				(length 5.08)
				(name "PTA3")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PTA4")
				(number "32")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PTA5")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PTB0")
				(number "34")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PTB1")
				(number "35")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PTB2")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTB3")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PTB4")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PTB5")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTB6")
				(number "40")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTB7")
				(number "41")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTC0")
				(number "60")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PTC1")
				(number "61")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PTC2")
				(number "62")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTC3")
				(number "63")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTC4")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PTC5")
				(number "64")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTC6")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTD0")
				(number "42")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTD1")
				(number "43")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PTD2")
				(number "48")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PTD3")
				(number "49")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PTD4")
				(number "50")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PTD5")
				(number "51")
			)
			(pin bidirectional line
				(at 27.94 -33.02 180)
				(length 5.08)
				(name "PTD6")
				(number "52")
			)
			(pin bidirectional line
				(at 27.94 -35.56 180)
				(length 5.08)
				(name "PTD7")
				(number "53")
			)
			(pin bidirectional line
				(at 27.94 -43.18 180)
				(length 5.08)
				(name "IRQ/TPMCLK")
				(number "2")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08JS16CFK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -19.05 24.13 0)
		)
		(property "Value" "MC9S08JS16CFK"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 6.35 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08JS16RM.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit USB Microcontroller, S08 core, 16kB Flash, 512B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08JS16CFK_0_1")
		(symbol "MC9S08JS16CFK_1_1"
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "USBDN")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "USBDP")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PTB1/~{RESET}")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PTB2/BKGD/MS")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PTB3/~{BLMS}")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PTB0/IRQ/TCLK")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PTB4/XTAL")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PTB5/EXTAL")
				(number "22")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "11")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "13")
			)
			(pin power_out line
				(at 2.54 27.94 270)
				(length 5.08)
				(name "VUSB33")
				(number "16")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "VSSOSC")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PTA1/KBIP1/MISO")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PTA2/KBIP2/MOSI")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PTA3/KBIP3/SPSCK")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PTA4/KBIP4/~{SS}")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PTA0/KBIP0/PTMCH0")
				(number "5")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PTA5/KBIP5/TPMCH1")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PTA6/KBIP6/RxD")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PTA7/KBIP7/TxD")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08JS16CWJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -19.05 24.13 0)
		)
		(property "Value" "MC9S08JS16CWJ"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 6.35 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08JS16RM.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit USB Microcontroller, S08 core, 16kB Flash, 512B RAM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08JS16CWJ_0_1")
		(symbol "MC9S08JS16CWJ_1_1"
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "USBDN")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "USBDP")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PTB1/~{RESET}")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PTB2/BKGD/MS")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 -2.54 0)
				(length 5.08)
				(name "PTB3/~{BLMS}")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PTB0/IRQ/TCLK")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PTB4/XTAL")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PTB5/EXTAL")
				(number "2")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "13")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "14")
			)
			(pin power_out line
				(at 2.54 27.94 270)
				(length 5.08)
				(name "VUSB33")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "VSSOSC")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PTA1/KBIP1/MISO")
				(number "9")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PTA2/KBIP2/MOSI")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PTA3/KBIP3/SPSCK")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PTA4/KBIP4/~{SS}")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PTA0/KBIP0/PTMCH0")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PTA5/KBIP5/TPMCH1")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PTA6/KBIP6/RxD")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PTA7/KBIP7/TxD")
				(number "20")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08LG32J0xLF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -25.4 36.83 0)
		)
		(property "Value" "MC9S08LG32J0xLF"
			(at 25.4 36.83 0)
		)
		(property "Footprint" "Package_QFP:TQFP-48-1EP_7x7mm_P0.5mm_EP3.5x3.5mm"
			(at 10.16 -36.83 0)
		)
		(property "Datasheet" "https://www.nxp.com/files-static/microcontrollers/doc/ref_manual/MC9S08LG32RM.pdf"
			(at 2.54 12.7 0)
		)
		(property "Description" "8-bit Segment LCD Microcontroller, S08 core, 32kB Flash, 1984B RAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08LG32J0xLF_0_1")
		(symbol "MC9S08LG32J0xLF_1_1"
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA1")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA2")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTA3")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTA4")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTA5")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTA6")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTA7")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTF0")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTF1")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTF2")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTF3")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTF4")
				(number "15")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTF5")
				(number "14")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTC6/~{RESET}")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PTC5/BKGD/MS")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTF6/XTAL")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 -30.48 0)
				(length 5.08)
				(name "PTF7/EXTAL")
				(number "18")
			)
			(pin power_in line
				(at -5.08 40.64 270)
				(length 5.08)
				(name "VDD")
				(number "17")
			)
			(pin power_in line
				(at -5.08 -40.64 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin power_in line
				(at -2.54 40.64 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "20")
			)
			(pin power_in line
				(at -2.54 -40.64 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "21")
			)
			(pin power_in line
				(at 0 -40.64 90)
				(length 5.08)
				(name "VLL1")
				(number "11")
			)
			(pin power_in line
				(at 2.54 40.64 270)
				(length 5.08)
				(name "VCAP1")
				(number "9")
			)
			(pin power_in line
				(at 2.54 -40.64 90)
				(length 5.08)
				(name "VLL2")
				(number "12")
			)
			(pin power_in line
				(at 5.08 40.64 270)
				(length 5.08)
				(name "VCAP2")
				(number "10")
			)
			(pin power_in line
				(at 5.08 -40.64 90)
				(length 5.08)
				(name "VLL3")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTA0/LCD21")
				(number "35")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC0/LCD16")
				(number "40")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC1/LCD17")
				(number "39")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC2/LCD18")
				(number "38")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC3/LCD19")
				(number "37")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC4/LCD20")
				(number "36")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTD0/LCD0")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD1/LCD1")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD2/LCD2")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD3/LCD3")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD4/LCD4")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD5/LCD5")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD6/LCD6")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD7/LCD7")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE0/LCD8")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE1/LCD9")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE2/LCD10")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE3/LCD11")
				(number "45")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE4/LCD12")
				(number "44")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE5/LCD13")
				(number "43")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE6/LCD14")
				(number "42")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE7/LCD15")
				(number "41")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08LG32J0xLH"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -25.4 49.53 0)
		)
		(property "Value" "MC9S08LG32J0xLH"
			(at 25.4 49.53 0)
		)
		(property "Footprint" "Package_QFP:TQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/files-static/microcontrollers/doc/ref_manual/MC9S08LG32RM.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit Segment LCD Microcontroller, S08 core, 32kB Flash, 1984B RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08LG32J0xLH_0_1")
		(symbol "MC9S08LG32J0xLH_1_1"
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA1")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA2")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA3")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 35.56 0)
				(length 5.08)
				(name "PTA4")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTA5")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTA6")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTA7")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTF0")
				(number "32")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTF1")
				(number "31")
			)
			(pin bidirectional line
				(at -30.48 17.78 0)
				(length 5.08)
				(name "PTF2")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTF3")
				(number "33")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTF4")
				(number "19")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTF5")
				(number "18")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTH4")
				(number "35")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTH5")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTH6")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTH7")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTI4")
				(number "21")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTI5")
				(number "20")
			)
			(pin bidirectional line
				(at -30.48 -25.4 0)
				(length 5.08)
				(name "PTC6/~{RESET}")
				(number "36")
			)
			(pin bidirectional line
				(at -30.48 -27.94 0)
				(length 5.08)
				(name "PTC5/BKGD/MS")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 -40.64 0)
				(length 5.08)
				(name "PTF6/XTAL")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 -43.18 0)
				(length 5.08)
				(name "PTF7/EXTAL")
				(number "25")
			)
			(pin power_in line
				(at -7.62 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "23")
			)
			(pin power_in line
				(at -5.08 53.34 270)
				(length 5.08)
				(name "VDD")
				(number "24")
			)
			(pin power_in line
				(at -5.08 -53.34 90)
				(length 5.08)
				(name "VSS")
				(number "55")
			)
			(pin power_in line
				(at -2.54 53.34 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "27")
			)
			(pin power_in line
				(at -2.54 -53.34 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "28")
			)
			(pin power_in line
				(at 0 -53.34 90)
				(length 5.08)
				(name "VLL1")
				(number "15")
			)
			(pin power_in line
				(at 2.54 53.34 270)
				(length 5.08)
				(name "VCAP1")
				(number "13")
			)
			(pin power_in line
				(at 2.54 -53.34 90)
				(length 5.08)
				(name "VLL2")
				(number "16")
			)
			(pin power_in line
				(at 5.08 53.34 270)
				(length 5.08)
				(name "VCAP2")
				(number "14")
			)
			(pin power_in line
				(at 5.08 -53.34 90)
				(length 5.08)
				(name "VLL3")
				(number "17")
			)
			(pin power_in line
				(at 7.62 -53.34 90)
				(length 5.08)
				(name "VLL3")
				(number "56")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTA0/LCD21")
				(number "47")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTB0/LCD29")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTB1/LCD30")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTB2/LCD31")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTB3/LCD32")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC0/LCD16")
				(number "52")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC1/LCD17")
				(number "51")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC2/LCD18")
				(number "50")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC3/LCD19")
				(number "49")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC4/LCD20")
				(number "48")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTD0/LCD0")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD1/LCD1")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD2/LCD2")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD3/LCD3")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD4/LCD4")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD5/LCD5")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD6/LCD6")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD7/LCD7")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE0/LCD8")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE1/LCD9")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE2/LCD10")
				(number "62")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE3/LCD11")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE4/LCD12")
				(number "60")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE5/LCD13")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE6/LCD14")
				(number "54")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE7/LCD15")
				(number "53")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTG0/LCD33")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTG1/LCD34")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTG2/LCD35")
				(number "46")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTG3/LCD36")
				(number "45")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08LG32J0xLK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -25.4 59.69 0)
		)
		(property "Value" "MC9S08LG32J0xLK"
			(at 25.4 59.69 0)
		)
		(property "Footprint" "Package_QFP:TQFP-80_14x14mm_P0.65mm"
			(at 10.16 -59.69 0)
		)
		(property "Datasheet" "https://www.nxp.com/files-static/microcontrollers/doc/ref_manual/MC9S08LG32RM.pdf"
			(at 2.54 35.56 0)
		)
		(property "Description" "8-bit Segment LCD Microcontroller, S08 core, 32kB Flash, 1984B RAM, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TQFP*14x14mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08LG32J0xLK_0_1")
		(symbol "MC9S08LG32J0xLK_1_1"
			(pin bidirectional line
				(at -30.48 53.34 0)
				(length 5.08)
				(name "PTA1")
				(number "56")
			)
			(pin bidirectional line
				(at -30.48 50.8 0)
				(length 5.08)
				(name "PTA2")
				(number "55")
			)
			(pin bidirectional line
				(at -30.48 48.26 0)
				(length 5.08)
				(name "PTA3")
				(number "54")
			)
			(pin bidirectional line
				(at -30.48 45.72 0)
				(length 5.08)
				(name "PTA4")
				(number "53")
			)
			(pin bidirectional line
				(at -30.48 43.18 0)
				(length 5.08)
				(name "PTA5")
				(number "52")
			)
			(pin bidirectional line
				(at -30.48 40.64 0)
				(length 5.08)
				(name "PTA6")
				(number "51")
			)
			(pin bidirectional line
				(at -30.48 38.1 0)
				(length 5.08)
				(name "PTA7")
				(number "50")
			)
			(pin bidirectional line
				(at -30.48 33.02 0)
				(length 5.08)
				(name "PTF0")
				(number "40")
			)
			(pin bidirectional line
				(at -30.48 30.48 0)
				(length 5.08)
				(name "PTF1")
				(number "39")
			)
			(pin bidirectional line
				(at -30.48 27.94 0)
				(length 5.08)
				(name "PTF2")
				(number "38")
			)
			(pin bidirectional line
				(at -30.48 25.4 0)
				(length 5.08)
				(name "PTF3")
				(number "41")
			)
			(pin bidirectional line
				(at -30.48 22.86 0)
				(length 5.08)
				(name "PTF4")
				(number "23")
			)
			(pin bidirectional line
				(at -30.48 20.32 0)
				(length 5.08)
				(name "PTF5")
				(number "22")
			)
			(pin bidirectional line
				(at -30.48 15.24 0)
				(length 5.08)
				(name "PTH0")
				(number "47")
			)
			(pin bidirectional line
				(at -30.48 12.7 0)
				(length 5.08)
				(name "PTH1")
				(number "46")
			)
			(pin bidirectional line
				(at -30.48 10.16 0)
				(length 5.08)
				(name "PTH2")
				(number "45")
			)
			(pin bidirectional line
				(at -30.48 7.62 0)
				(length 5.08)
				(name "PTH3")
				(number "44")
			)
			(pin bidirectional line
				(at -30.48 5.08 0)
				(length 5.08)
				(name "PTH4")
				(number "43")
			)
			(pin bidirectional line
				(at -30.48 2.54 0)
				(length 5.08)
				(name "PTH5")
				(number "42")
			)
			(pin bidirectional line
				(at -30.48 0 0)
				(length 5.08)
				(name "PTH6")
				(number "37")
			)
			(pin bidirectional line
				(at -30.48 -2.54 0)
				(length 5.08)
				(name "PTH7")
				(number "30")
			)
			(pin bidirectional line
				(at -30.48 -7.62 0)
				(length 5.08)
				(name "PTI0")
				(number "29")
			)
			(pin bidirectional line
				(at -30.48 -10.16 0)
				(length 5.08)
				(name "PTI1")
				(number "28")
			)
			(pin bidirectional line
				(at -30.48 -12.7 0)
				(length 5.08)
				(name "PTI2")
				(number "27")
			)
			(pin bidirectional line
				(at -30.48 -15.24 0)
				(length 5.08)
				(name "PTI3")
				(number "26")
			)
			(pin bidirectional line
				(at -30.48 -17.78 0)
				(length 5.08)
				(name "PTI4")
				(number "25")
			)
			(pin bidirectional line
				(at -30.48 -20.32 0)
				(length 5.08)
				(name "PTI5")
				(number "24")
			)
			(pin bidirectional line
				(at -30.48 -33.02 0)
				(length 5.08)
				(name "PTC6/~{RESET}")
				(number "48")
			)
			(pin bidirectional line
				(at -30.48 -35.56 0)
				(length 5.08)
				(name "PTC5/BKGD/MS")
				(number "49")
			)
			(pin bidirectional line
				(at -30.48 -50.8 0)
				(length 5.08)
				(name "PTF6/XTAL")
				(number "34")
			)
			(pin bidirectional line
				(at -30.48 -53.34 0)
				(length 5.08)
				(name "PTF7/EXTAL")
				(number "33")
			)
			(pin power_in line
				(at -7.62 -63.5 90)
				(length 5.08)
				(name "VSS")
				(number "31")
			)
			(pin power_in line
				(at -5.08 63.5 270)
				(length 5.08)
				(name "VDD")
				(number "32")
			)
			(pin power_in line
				(at -5.08 -63.5 90)
				(length 5.08)
				(name "VSS")
				(number "67")
			)
			(pin power_in line
				(at -2.54 63.5 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "35")
			)
			(pin power_in line
				(at -2.54 -63.5 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "36")
			)
			(pin power_in line
				(at 0 -63.5 90)
				(length 5.08)
				(name "VLL1")
				(number "19")
			)
			(pin power_in line
				(at 2.54 63.5 270)
				(length 5.08)
				(name "VCAP1")
				(number "17")
			)
			(pin power_in line
				(at 2.54 -63.5 90)
				(length 5.08)
				(name "VLL2")
				(number "20")
			)
			(pin power_in line
				(at 5.08 63.5 270)
				(length 5.08)
				(name "VCAP2")
				(number "18")
			)
			(pin power_in line
				(at 5.08 -63.5 90)
				(length 5.08)
				(name "VLL3")
				(number "21")
			)
			(pin power_in line
				(at 7.62 -63.5 90)
				(length 5.08)
				(name "VLL3")
				(number "68")
			)
			(pin bidirectional line
				(at 30.48 53.34 180)
				(length 5.08)
				(name "PTA0/LCD21")
				(number "59")
			)
			(pin bidirectional line
				(at 30.48 48.26 180)
				(length 5.08)
				(name "PTB0/LCD29")
				(number "14")
			)
			(pin bidirectional line
				(at 30.48 45.72 180)
				(length 5.08)
				(name "PTB1/LCD30")
				(number "13")
			)
			(pin bidirectional line
				(at 30.48 43.18 180)
				(length 5.08)
				(name "PTB2/LCD31")
				(number "8")
			)
			(pin bidirectional line
				(at 30.48 40.64 180)
				(length 5.08)
				(name "PTB3/LCD32")
				(number "7")
			)
			(pin bidirectional line
				(at 30.48 38.1 180)
				(length 5.08)
				(name "PTB4/LCD37")
				(number "12")
			)
			(pin bidirectional line
				(at 30.48 35.56 180)
				(length 5.08)
				(name "PTB5/LCD38")
				(number "11")
			)
			(pin bidirectional line
				(at 30.48 33.02 180)
				(length 5.08)
				(name "PTB6/LCD39")
				(number "10")
			)
			(pin bidirectional line
				(at 30.48 30.48 180)
				(length 5.08)
				(name "PTB7/LCD40")
				(number "9")
			)
			(pin bidirectional line
				(at 30.48 25.4 180)
				(length 5.08)
				(name "PTC0/LCD16")
				(number "64")
			)
			(pin bidirectional line
				(at 30.48 22.86 180)
				(length 5.08)
				(name "PTC1/LCD17")
				(number "63")
			)
			(pin bidirectional line
				(at 30.48 20.32 180)
				(length 5.08)
				(name "PTC2/LCD18")
				(number "62")
			)
			(pin bidirectional line
				(at 30.48 17.78 180)
				(length 5.08)
				(name "PTC3/LCD19")
				(number "61")
			)
			(pin bidirectional line
				(at 30.48 15.24 180)
				(length 5.08)
				(name "PTC4/LCD20")
				(number "60")
			)
			(pin bidirectional line
				(at 30.48 10.16 180)
				(length 5.08)
				(name "PTD0/LCD0")
				(number "16")
			)
			(pin bidirectional line
				(at 30.48 7.62 180)
				(length 5.08)
				(name "PTD1/LCD1")
				(number "15")
			)
			(pin bidirectional line
				(at 30.48 5.08 180)
				(length 5.08)
				(name "PTD2/LCD2")
				(number "6")
			)
			(pin bidirectional line
				(at 30.48 2.54 180)
				(length 5.08)
				(name "PTD3/LCD3")
				(number "5")
			)
			(pin bidirectional line
				(at 30.48 0 180)
				(length 5.08)
				(name "PTD4/LCD4")
				(number "4")
			)
			(pin bidirectional line
				(at 30.48 -2.54 180)
				(length 5.08)
				(name "PTD5/LCD5")
				(number "3")
			)
			(pin bidirectional line
				(at 30.48 -5.08 180)
				(length 5.08)
				(name "PTD6/LCD6")
				(number "2")
			)
			(pin bidirectional line
				(at 30.48 -7.62 180)
				(length 5.08)
				(name "PTD7/LCD7")
				(number "1")
			)
			(pin bidirectional line
				(at 30.48 -12.7 180)
				(length 5.08)
				(name "PTE0/LCD8")
				(number "80")
			)
			(pin bidirectional line
				(at 30.48 -15.24 180)
				(length 5.08)
				(name "PTE1/LCD9")
				(number "79")
			)
			(pin bidirectional line
				(at 30.48 -17.78 180)
				(length 5.08)
				(name "PTE2/LCD10")
				(number "78")
			)
			(pin bidirectional line
				(at 30.48 -20.32 180)
				(length 5.08)
				(name "PTE3/LCD11")
				(number "77")
			)
			(pin bidirectional line
				(at 30.48 -22.86 180)
				(length 5.08)
				(name "PTE4/LCD12")
				(number "76")
			)
			(pin bidirectional line
				(at 30.48 -25.4 180)
				(length 5.08)
				(name "PTE5/LCD13")
				(number "75")
			)
			(pin bidirectional line
				(at 30.48 -27.94 180)
				(length 5.08)
				(name "PTE6/LCD14")
				(number "66")
			)
			(pin bidirectional line
				(at 30.48 -30.48 180)
				(length 5.08)
				(name "PTE7/LCD15")
				(number "65")
			)
			(pin bidirectional line
				(at 30.48 -35.56 180)
				(length 5.08)
				(name "PTG0/LCD33")
				(number "74")
			)
			(pin bidirectional line
				(at 30.48 -38.1 180)
				(length 5.08)
				(name "PTG1/LCD34")
				(number "73")
			)
			(pin bidirectional line
				(at 30.48 -40.64 180)
				(length 5.08)
				(name "PTG2/LCD35")
				(number "58")
			)
			(pin bidirectional line
				(at 30.48 -43.18 180)
				(length 5.08)
				(name "PTG3/LCD36")
				(number "57")
			)
			(pin bidirectional line
				(at 30.48 -45.72 180)
				(length 5.08)
				(name "PTG4/LCD41")
				(number "72")
			)
			(pin bidirectional line
				(at 30.48 -48.26 180)
				(length 5.08)
				(name "PTG5/LCD42")
				(number "71")
			)
			(pin bidirectional line
				(at 30.48 -50.8 180)
				(length 5.08)
				(name "PTG6/LCD43")
				(number "70")
			)
			(pin bidirectional line
				(at 30.48 -53.34 180)
				(length 5.08)
				(name "PTG7/LCD44")
				(number "69")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08MP16xLC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 26.67 0)
		)
		(property "Value" "MC9S08MP16xLC"
			(at 22.86 26.67 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 10.16 -26.67 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08MP16RM.pdf"
			(at 2.54 2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 16kB Flash, 1kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08MP16xLC_0_1")
		(symbol "MC9S08MP16xLC_1_1"
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PTC0")
				(number "31")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PTC1")
				(number "32")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTC2")
				(number "1")
			)
			(pin bidirectional line
				(at -27.94 12.7 0)
				(length 5.08)
				(name "PTC3")
				(number "2")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PTC4")
				(number "3")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PTC5")
				(number "4")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PTC6")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PTF1/~{RESET}")
				(number "12")
			)
			(pin bidirectional line
				(at -27.94 -7.62 0)
				(length 5.08)
				(name "PTF0/BKGD/MS")
				(number "30")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PTE5/XTAL")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 -20.32 0)
				(length 5.08)
				(name "PTE6/EXTAL")
				(number "28")
			)
			(pin power_in line
				(at -5.08 30.48 270)
				(length 5.08)
				(name "VDD")
				(number "7")
			)
			(pin power_in line
				(at -5.08 -30.48 90)
				(length 5.08)
				(name "VSS")
				(number "6")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 5.08)
				(name "VSS")
				(number "29")
			)
			(pin power_in line
				(at 5.08 30.48 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "21")
			)
			(pin power_in line
				(at 5.08 -30.48 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PTA0")
				(number "8")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTA1")
				(number "9")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PTA2")
				(number "10")
			)
			(pin bidirectional line
				(at 27.94 12.7 180)
				(length 5.08)
				(name "PTA3")
				(number "11")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTA4")
				(number "13")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTA5")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PTA6")
				(number "15")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTA7")
				(number "16")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PTB0")
				(number "17")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTB1")
				(number "18")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTB2")
				(number "19")
			)
			(pin bidirectional line
				(at 27.94 -10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "20")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTB4")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PTB5")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTB6")
				(number "25")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTB7")
				(number "26")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08MP16xLF"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08MP16xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08MP16RM.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 16kB Flash, 1kB RAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08MP16xLF_0_1")
		(symbol "MC9S08MP16xLF_1_1"
			(pin bidirectional line
				(at -27.94 33.02 0)
				(length 5.08)
				(name "PTD0")
				(number "5")
			)
			(pin bidirectional line
				(at -27.94 30.48 0)
				(length 5.08)
				(name "PTD1")
				(number "6")
			)
			(pin bidirectional line
				(at -27.94 27.94 0)
				(length 5.08)
				(name "PTD2")
				(number "7")
			)
			(pin bidirectional line
				(at -27.94 25.4 0)
				(length 5.08)
				(name "PTD3")
				(number "8")
			)
			(pin bidirectional line
				(at -27.94 22.86 0)
				(length 5.08)
				(name "PTD4")
				(number "15")
			)
			(pin bidirectional line
				(at -27.94 20.32 0)
				(length 5.08)
				(name "PTD5")
				(number "16")
			)
			(pin bidirectional line
				(at -27.94 17.78 0)
				(length 5.08)
				(name "PTD6")
				(number "17")
			)
			(pin bidirectional line
				(at -27.94 15.24 0)
				(length 5.08)
				(name "PTD7")
				(number "18")
			)
			(pin bidirectional line
				(at -27.94 10.16 0)
				(length 5.08)
				(name "PTE0")
				(number "25")
			)
			(pin bidirectional line
				(at -27.94 7.62 0)
				(length 5.08)
				(name "PTE1")
				(number "26")
			)
			(pin bidirectional line
				(at -27.94 5.08 0)
				(length 5.08)
				(name "PTE2")
				(number "27")
			)
			(pin bidirectional line
				(at -27.94 2.54 0)
				(length 5.08)
				(name "PTE3")
				(number "34")
			)
			(pin bidirectional line
				(at -27.94 0 0)
				(length 5.08)
				(name "PTE4")
				(number "35")
			)
			(pin bidirectional line
				(at -27.94 -5.08 0)
				(length 5.08)
				(name "PTF2")
				(number "20")
			)
			(pin bidirectional line
				(at -27.94 -15.24 0)
				(length 5.08)
				(name "PTF1/~{RESET}")
				(number "19")
			)
			(pin bidirectional line
				(at -27.94 -17.78 0)
				(length 5.08)
				(name "PTF0/BKGD/MS")
				(number "44")
			)
			(pin bidirectional line
				(at -27.94 -27.94 0)
				(length 5.08)
				(name "PTE5/XTAL")
				(number "40")
			)
			(pin bidirectional line
				(at -27.94 -30.48 0)
				(length 5.08)
				(name "PTE6/EXTAL")
				(number "41")
			)
			(pin power_in line
				(at -5.08 43.18 270)
				(length 5.08)
				(name "VDD")
				(number "10")
			)
			(pin power_in line
				(at -5.08 -43.18 90)
				(length 5.08)
				(name "VSS")
				(number "9")
			)
			(pin power_in line
				(at -2.54 43.18 270)
				(length 5.08)
				(name "VDD")
				(number "43")
			)
			(pin power_in line
				(at -2.54 -43.18 90)
				(length 5.08)
				(name "VSS")
				(number "42")
			)
			(pin power_in line
				(at 5.08 43.18 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "32")
			)
			(pin power_in line
				(at 5.08 -43.18 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "33")
			)
			(pin bidirectional line
				(at 27.94 33.02 180)
				(length 5.08)
				(name "PTA0")
				(number "11")
			)
			(pin bidirectional line
				(at 27.94 30.48 180)
				(length 5.08)
				(name "PTA1")
				(number "12")
			)
			(pin bidirectional line
				(at 27.94 27.94 180)
				(length 5.08)
				(name "PTA2")
				(number "13")
			)
			(pin bidirectional line
				(at 27.94 25.4 180)
				(length 5.08)
				(name "PTA3")
				(number "14")
			)
			(pin bidirectional line
				(at 27.94 22.86 180)
				(length 5.08)
				(name "PTA4")
				(number "21")
			)
			(pin bidirectional line
				(at 27.94 20.32 180)
				(length 5.08)
				(name "PTA5")
				(number "22")
			)
			(pin bidirectional line
				(at 27.94 17.78 180)
				(length 5.08)
				(name "PTA6")
				(number "23")
			)
			(pin bidirectional line
				(at 27.94 15.24 180)
				(length 5.08)
				(name "PTA7")
				(number "24")
			)
			(pin bidirectional line
				(at 27.94 10.16 180)
				(length 5.08)
				(name "PTB0")
				(number "28")
			)
			(pin bidirectional line
				(at 27.94 7.62 180)
				(length 5.08)
				(name "PTB1")
				(number "29")
			)
			(pin bidirectional line
				(at 27.94 5.08 180)
				(length 5.08)
				(name "PTB2")
				(number "30")
			)
			(pin bidirectional line
				(at 27.94 2.54 180)
				(length 5.08)
				(name "PTB3")
				(number "31")
			)
			(pin bidirectional line
				(at 27.94 0 180)
				(length 5.08)
				(name "PTB4")
				(number "36")
			)
			(pin bidirectional line
				(at 27.94 -2.54 180)
				(length 5.08)
				(name "PTB5")
				(number "37")
			)
			(pin bidirectional line
				(at 27.94 -5.08 180)
				(length 5.08)
				(name "PTB6")
				(number "38")
			)
			(pin bidirectional line
				(at 27.94 -7.62 180)
				(length 5.08)
				(name "PTB7")
				(number "39")
			)
			(pin bidirectional line
				(at 27.94 -12.7 180)
				(length 5.08)
				(name "PTC0")
				(number "45")
			)
			(pin bidirectional line
				(at 27.94 -15.24 180)
				(length 5.08)
				(name "PTC1")
				(number "46")
			)
			(pin bidirectional line
				(at 27.94 -17.78 180)
				(length 5.08)
				(name "PTC2")
				(number "47")
			)
			(pin bidirectional line
				(at 27.94 -20.32 180)
				(length 5.08)
				(name "PTC3")
				(number "48")
			)
			(pin bidirectional line
				(at 27.94 -22.86 180)
				(length 5.08)
				(name "PTC4")
				(number "1")
			)
			(pin bidirectional line
				(at 27.94 -25.4 180)
				(length 5.08)
				(name "PTC5")
				(number "2")
			)
			(pin bidirectional line
				(at 27.94 -27.94 180)
				(length 5.08)
				(name "PTC6")
				(number "3")
			)
			(pin bidirectional line
				(at 27.94 -30.48 180)
				(length 5.08)
				(name "PTC7")
				(number "4")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08MP16xWL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -20.32 26.67 0)
		)
		(property "Value" "MC9S08MP16xWL"
			(at 20.32 26.67 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 7.62 -26.67 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08MP16RM.pdf"
			(at 0 2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 16kB Flash, 1kB RAM, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08MP16xWL_0_1")
		(symbol "MC9S08MP16xWL_1_1"
			(pin bidirectional line
				(at -25.4 20.32 0)
				(length 5.08)
				(name "PTC0")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PTC1")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PTC2")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PTC3")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PTC4")
				(number "5")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PTC5")
				(number "6")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PTC6")
				(number "7")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PTF1/~{RESET}")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PTF0/BKGD/MS")
				(number "28")
			)
			(pin power_in line
				(at -2.54 30.48 270)
				(length 5.08)
				(name "VDD")
				(number "9")
			)
			(pin power_in line
				(at -2.54 -30.48 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 30.48 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "23")
			)
			(pin power_in line
				(at 2.54 -30.48 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 20.32 180)
				(length 5.08)
				(name "PTA0")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PTA1")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PTA2")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PTA4")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PTA5")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PTA6")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 2.54 180)
				(length 5.08)
				(name "PTA7")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PTB0")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PTB1")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PTB2")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PTB4")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PTB5")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PTB6")
				(number "27")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QA4CDNE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QA4CDNE"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08QA4RM.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QA4CDNE_0_1")
		(symbol "MC9S08QA4CDNE_1_1"
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTA1")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTA2")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QA4CFQE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QA4CFQE"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_4x4mm_P0.8mm_EP2.5x3.6mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08QA4RM.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QA4CFQE_0_1")
		(symbol "MC9S08QA4CFQE_1_1"
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTA1")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTA2")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QA4CPAE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QA4CPAE"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08QA4RM.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QA4CPAE_0_1")
		(symbol "MC9S08QA4CPAE_1_1"
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTA1")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTA2")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QB8xGK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08QB8xGK"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 7.62 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08QB8RM.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 8kB Flash, 512B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QB8xGK_0_1")
		(symbol "MC9S08QB8xGK_1_1"
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PTC0")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PTC1")
				(number "9")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PTC6")
				(number "22")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PTC7")
				(number "21")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "23")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "24")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "2")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "3")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PTA0")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PTA1")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PTA2")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PTA3")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PTA6")
				(number "16")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PTA7")
				(number "15")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PTB0")
				(number "14")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PTB1")
				(number "13")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PTB2")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PTB3")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PTB4")
				(number "8")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PTB5")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "6")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QB8xTG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08QB8xTG"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 6.35 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08QB8RM.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 8kB Flash, 512B RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QB8xTG_0_1")
		(symbol "MC9S08QB8xTG_1_1"
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTB0")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PTB1")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB3")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QB8xWL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08QB8xWL"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 7.62 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08QB8RM.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 8kB Flash, 512B RAM, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QB8xWL_0_1")
		(symbol "MC9S08QB8xWL_1_1"
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PTC0")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PTC1")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PTC2")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PTC3")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PTC4")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PTC5")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PTC6")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PTC7")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "4")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PTA1")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PTA3")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PTA6")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PTA7")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PTB0")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PTB1")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PTB2")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PTB3")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PTB4")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PTB5")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QD4xPC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QD4xPC"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QD4.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QD4xPC_0_1")
		(symbol "MC9S08QD4xPC_1_1"
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTA1")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTA2")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QD4xSC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QD4xSC"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QD4.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QD4xSC_0_1")
		(symbol "MC9S08QD4xSC_1_1"
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTA1")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTA2")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QG4xPAE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QG4xPAE"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 5.08 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QG8.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QG4xPAE_0_1")
		(symbol "MC9S08QG4xPAE_1_1"
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTA1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTA2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QG8xDNE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QG8xDNE"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QG8.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 8kB Flash, 512B RAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QG8xDNE_0_1")
		(symbol "MC9S08QG8xDNE_1_1"
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTA1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTA2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QG8xDTE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 19.05 0)
		)
		(property "Value" "MC9S08QG8xDTE"
			(at 1.27 19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 5.08 -19.05 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QG8.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 8kB Flash, 512B RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QG8xDTE_0_1")
		(symbol "MC9S08QG8xDTE_1_1"
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "5")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PTB0")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB1")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB3")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QG8xFKE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 19.05 0)
		)
		(property "Value" "MC9S08QG8xFKE"
			(at 1.27 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 5.08 -19.05 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QG8.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 8kB Flash, 512B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QG8xFKE_0_1")
		(symbol "MC9S08QG8xFKE_1_1"
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "4")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VDD")
				(number "2")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "VSS")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA0")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA1")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA2")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PTB0")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB1")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB2")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB3")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB4")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB5")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QG8xFQE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QG8xFQE"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_4x4mm_P0.8mm_EP2.5x3.6mm"
			(at 5.08 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QG8.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 8kB Flash, 512B RAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QG8xFQE_0_1")
		(symbol "MC9S08QG8xFQE_1_1"
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTA1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTA2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08QG8xPBE"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 19.05 0)
		)
		(property "Value" "MC9S08QG8xPBE"
			(at 1.27 19.05 0)
		)
		(property "Footprint" "Package_DIP:DIP-16_W7.62mm"
			(at 5.08 -19.05 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QG8.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 8kB Flash, 512B RAM, DIP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08QG8xPBE_0_1")
		(symbol "MC9S08QG8xPBE_1_1"
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "5")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PTB0")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB1")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB3")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SC4xTG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SC4xTG"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SC4.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SC4xTG_0_1")
		(symbol "MC9S08SC4xTG_1_1"
			(pin input line
				(at -22.86 0 0)
				(length 5.08)
				(name "~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB0")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB1")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTB5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SE8xRL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08SE8xRL"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 7.62 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08SE8RM.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 8kB Flash, 512B RAM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*15.24mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SE8xRL_0_1")
		(symbol "MC9S08SE8xRL_1_1"
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PTC0")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PTC1")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PTC2")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PTC3")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PTC4")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PTC5")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PTC6")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PTC7")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "4")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PTA1")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PTA3")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PTA6")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PTA7")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PTB0")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PTB1")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PTB2")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PTB3")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PTB4")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PTB5")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SE8xTG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 16.51 0)
		)
		(property "Value" "MC9S08SE8xTG"
			(at 17.78 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 5.08 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08SE8RM.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 8kB Flash, 512B RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SE8xTG_0_1")
		(symbol "MC9S08SE8xTG_1_1"
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PTA0")
				(number "16")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTA1")
				(number "15")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PTA2")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin power_in line
				(at 0 20.32 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -20.32 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTB0")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTB1")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTB3")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PTB4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SE8xWL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08SE8xWL"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 7.62 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08SE8RM.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 8kB Flash, 512B RAM, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SE8xWL_0_1")
		(symbol "MC9S08SE8xWL_1_1"
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PTC0")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PTC1")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PTC2")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PTC3")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PTC4")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PTC5")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PTC6")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PTC7")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -10.16 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 -12.7 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "4")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PTA1")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PTA3")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PTA6")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PTA7")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 0 180)
				(length 5.08)
				(name "PTB0")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -2.54 180)
				(length 5.08)
				(name "PTB1")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PTB2")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PTB3")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PTB4")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PTB5")
				(number "11")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "10")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "9")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SF4xTG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SF4xTG"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 3.81 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08SF4RM.pdf"
			(at 2.54 2.54 0)
		)
		(property "Description" "8-bit Motor Control Microcontroller, S08 core, 4kB Flash, 128B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SF4xTG_0_1")
		(symbol "MC9S08SF4xTG_1_1"
			(pin bidirectional line
				(at -22.86 -5.08 0)
				(length 5.08)
				(name "PTA1/~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PTB7/BKGD/MS")
				(number "15")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA2")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA3")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA4")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PTB0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB1")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB3")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB4")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB5")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTB6")
				(number "14")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SF4xTJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 24.13 0)
		)
		(property "Value" "MC9S08SF4xTJ"
			(at 17.78 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 3.81 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08SF4RM.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "8-bit Motor Control Microcontroller, S08 core, 4kB Flash, 128B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SF4xTJ_0_1")
		(symbol "MC9S08SF4xTJ_1_1"
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PTC0")
				(number "18")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PTC1")
				(number "19")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PTA1/~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PTB7/BKGD/MS")
				(number "17")
			)
			(pin power_in line
				(at 0 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PTA0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA2")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA3")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA4")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA5")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA6")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTA7")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB0")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB1")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB2")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB4")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTB5")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PTB6")
				(number "16")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SG32xTG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SG32xTG"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SG32.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 32kB Flash, 1kB RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SG32xTG_0_1")
		(symbol "MC9S08SG32xTG_1_1"
			(pin input line
				(at -22.86 0 0)
				(length 5.08)
				(name "~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB0")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB1")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTB5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SG32xTJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SG32xTJ"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SG32.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 32kB Flash, 1kB RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SG32xTJ_0_1")
		(symbol "MC9S08SG32xTJ_1_1"
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PTC0")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PTC1")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PTC2")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTC3")
				(number "9")
			)
			(pin input line
				(at -22.86 0 0)
				(length 5.08)
				(name "~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA0")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA1")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA2")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA3")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTB5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SG32xTL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08SG32xTL"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 5.08 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SG32.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 32kB Flash, 1kB RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SG32xTL_0_1")
		(symbol "MC9S08SG32xTL_1_1"
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PTC0")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PTC1")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PTC2")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PTC3")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PTC4")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PTC5")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PTC6")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PTC7")
				(number "27")
			)
			(pin input line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "9")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PTA1")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PTA3")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PTA6")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PTA7")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PTB0")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PTB1")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PTB2")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PTB3")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PTB4")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PTB5")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SG8xSC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08SG8xSC"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SG8.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 8kB Flash, 512B RAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SG8xSC_0_1")
		(symbol "MC9S08SG8xSC_1_1"
			(pin input line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "BKGD/MS")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTA1")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTA2")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SH32xTG"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SH32xTG"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH32.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 32kB Flash, 1kB RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SH32xTG_0_1")
		(symbol "MC9S08SH32xTG_1_1"
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA3")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB0")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB1")
				(number "11")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB2")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTB5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SH32xTJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SH32xTJ"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH32.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 32kB Flash, 1kB RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SH32xTJ_0_1")
		(symbol "MC9S08SH32xTJ_1_1"
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PTC0")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PTC1")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PTC2")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTC3")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA0")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA1")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA2")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA3")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTB5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SH32xTL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08SH32xTL"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 5.08 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH32.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 32kB Flash, 1kB RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SH32xTL_0_1")
		(symbol "MC9S08SH32xTL_1_1"
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PTC0")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PTC1")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PTC2")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PTC3")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PTC4")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PTC5")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PTC6")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PTC7")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "9")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PTA1")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PTA3")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PTA6")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PTA7")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PTB0")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PTB1")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PTB2")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PTB3")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PTB4")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PTB5")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SH32xWL"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08SH32xWL"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 5.08 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH32.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 32kB Flash, 1kB RAM, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SH32xWL_0_1")
		(symbol "MC9S08SH32xWL_1_1"
			(pin bidirectional line
				(at -25.4 17.78 0)
				(length 5.08)
				(name "PTC0")
				(number "16")
			)
			(pin bidirectional line
				(at -25.4 15.24 0)
				(length 5.08)
				(name "PTC1")
				(number "15")
			)
			(pin bidirectional line
				(at -25.4 12.7 0)
				(length 5.08)
				(name "PTC2")
				(number "14")
			)
			(pin bidirectional line
				(at -25.4 10.16 0)
				(length 5.08)
				(name "PTC3")
				(number "13")
			)
			(pin bidirectional line
				(at -25.4 7.62 0)
				(length 5.08)
				(name "PTC4")
				(number "2")
			)
			(pin bidirectional line
				(at -25.4 5.08 0)
				(length 5.08)
				(name "PTC5")
				(number "1")
			)
			(pin bidirectional line
				(at -25.4 2.54 0)
				(length 5.08)
				(name "PTC6")
				(number "28")
			)
			(pin bidirectional line
				(at -25.4 0 0)
				(length 5.08)
				(name "PTC7")
				(number "27")
			)
			(pin bidirectional line
				(at -25.4 -5.08 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "3")
			)
			(pin bidirectional line
				(at -25.4 -7.62 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "4")
			)
			(pin bidirectional line
				(at -25.4 -15.24 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "10")
			)
			(pin bidirectional line
				(at -25.4 -17.78 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "9")
			)
			(pin power_in line
				(at -2.54 27.94 270)
				(length 5.08)
				(name "VDD")
				(number "5")
			)
			(pin power_in line
				(at -2.54 -27.94 90)
				(length 5.08)
				(name "VSS")
				(number "8")
			)
			(pin power_in line
				(at 2.54 27.94 270)
				(length 5.08)
				(name "VDDA/VREFH")
				(number "6")
			)
			(pin power_in line
				(at 2.54 -27.94 90)
				(length 5.08)
				(name "VSSA/VREFL")
				(number "7")
			)
			(pin bidirectional line
				(at 25.4 17.78 180)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at 25.4 15.24 180)
				(length 5.08)
				(name "PTA1")
				(number "25")
			)
			(pin bidirectional line
				(at 25.4 12.7 180)
				(length 5.08)
				(name "PTA2")
				(number "24")
			)
			(pin bidirectional line
				(at 25.4 10.16 180)
				(length 5.08)
				(name "PTA3")
				(number "23")
			)
			(pin bidirectional line
				(at 25.4 7.62 180)
				(length 5.08)
				(name "PTA6")
				(number "22")
			)
			(pin bidirectional line
				(at 25.4 5.08 180)
				(length 5.08)
				(name "PTA7")
				(number "21")
			)
			(pin bidirectional line
				(at 25.4 -5.08 180)
				(length 5.08)
				(name "PTB0")
				(number "20")
			)
			(pin bidirectional line
				(at 25.4 -7.62 180)
				(length 5.08)
				(name "PTB1")
				(number "19")
			)
			(pin bidirectional line
				(at 25.4 -10.16 180)
				(length 5.08)
				(name "PTB2")
				(number "18")
			)
			(pin bidirectional line
				(at 25.4 -12.7 180)
				(length 5.08)
				(name "PTB3")
				(number "17")
			)
			(pin bidirectional line
				(at 25.4 -15.24 180)
				(length 5.08)
				(name "PTB4")
				(number "12")
			)
			(pin bidirectional line
				(at 25.4 -17.78 180)
				(length 5.08)
				(name "PTB5")
				(number "11")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SH8xFK"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SH8xFK"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH8.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 8kB Flash, 512B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SH8xFK_0_1")
		(symbol "MC9S08SH8xFK_1_1"
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PTC0")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PTC1")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PTC2")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTC3")
				(number "8")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "23")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "24")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "5")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "4")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "1")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA0")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA1")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA2")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA3")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB0")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB1")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB2")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "12")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB4")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTB5")
				(number "6")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SH8xPJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SH8xPJ"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH8.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 8kB Flash, 512B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SH8xPJ_0_1")
		(symbol "MC9S08SH8xPJ_1_1"
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PTC0")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PTC1")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PTC2")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTC3")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -15.24 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "5")
			)
			(pin power_in line
				(at 0 25.4 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -25.4 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA0")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA1")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA2")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA3")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB3")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTB5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SH8xSC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08SH8xSC"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH8.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 8kB Flash, 512B RAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SH8xSC_0_1")
		(symbol "MC9S08SH8xSC_1_1"
			(pin bidirectional line
				(at -22.86 2.54 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin power_in line
				(at 0 15.24 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -15.24 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA0")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTA1")
				(number "7")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTA2")
				(number "6")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "5")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SH8xWJ"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 19.05 0)
		)
		(property "Value" "MC9S08SH8xWJ"
			(at 17.78 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 2.54 -19.05 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH8.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 8kB Flash, 512B RAM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SH8xWJ_0_1")
		(symbol "MC9S08SH8xWJ_1_1"
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PTC0")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PTC1")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTC2")
				(number "10")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PTC3")
				(number "9")
			)
			(pin bidirectional line
				(at -22.86 0 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -2.54 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "2")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "6")
			)
			(pin bidirectional line
				(at -22.86 -12.7 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "5")
			)
			(pin power_in line
				(at 0 22.86 270)
				(length 5.08)
				(name "VDD")
				(number "3")
			)
			(pin power_in line
				(at 0 -22.86 90)
				(length 5.08)
				(name "VSS")
				(number "4")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA0")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA1")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 7.62 180)
				(length 5.08)
				(name "PTA2")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTA3")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PTB0")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB1")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB2")
				(number "14")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB3")
				(number "13")
			)
			(pin bidirectional line
				(at 22.86 -10.16 180)
				(length 5.08)
				(name "PTB4")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTB5")
				(number "7")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08SV16CLC"
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(property "Reference" "IC"
			(at -17.78 29.21 0)
		)
		(property "Value" "MC9S08SV16CLC"
			(at 17.78 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 5.08 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08SV16RM.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit General Purpose Best-in-Class performance Microcontroller, S08 core, 16kB Flash, 1kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
		(symbol "MC9S08SV16CLC_0_1")
		(symbol "MC9S08SV16CLC_1_1"
			(pin bidirectional line
				(at -22.86 22.86 0)
				(length 5.08)
				(name "PTC0")
				(number "14")
			)
			(pin bidirectional line
				(at -22.86 20.32 0)
				(length 5.08)
				(name "PTC1")
				(number "13")
			)
			(pin bidirectional line
				(at -22.86 17.78 0)
				(length 5.08)
				(name "PTC2")
				(number "12")
			)
			(pin bidirectional line
				(at -22.86 15.24 0)
				(length 5.08)
				(name "PTC3")
				(number "11")
			)
			(pin bidirectional line
				(at -22.86 12.7 0)
				(length 5.08)
				(name "PTC4")
				(number "30")
			)
			(pin bidirectional line
				(at -22.86 10.16 0)
				(length 5.08)
				(name "PTC5")
				(number "29")
			)
			(pin bidirectional line
				(at -22.86 7.62 0)
				(length 5.08)
				(name "PTC6")
				(number "28")
			)
			(pin bidirectional line
				(at -22.86 5.08 0)
				(length 5.08)
				(name "PTC7")
				(number "27")
			)
			(pin bidirectional line
				(at -22.86 -7.62 0)
				(length 5.08)
				(name "PTA5/~{RESET}")
				(number "31")
			)
			(pin bidirectional line
				(at -22.86 -10.16 0)
				(length 5.08)
				(name "PTA4/BKGD/MS")
				(number "1")
			)
			(pin bidirectional line
				(at -22.86 -22.86 0)
				(length 5.08)
				(name "PTB6/XTAL")
				(number "7")
			)
			(pin bidirectional line
				(at -22.86 -25.4 0)
				(length 5.08)
				(name "PTB7/EXTAL")
				(number "6")
			)
			(pin power_in line
				(at 0 33.02 270)
				(length 5.08)
				(name "VDD")
				(number "4")
			)
			(pin power_in line
				(at 0 -33.02 90)
				(length 5.08)
				(name "VSS")
				(number "5")
			)
			(pin bidirectional line
				(at 22.86 22.86 180)
				(length 5.08)
				(name "PTA0")
				(number "26")
			)
			(pin bidirectional line
				(at 22.86 20.32 180)
				(length 5.08)
				(name "PTA1")
				(number "24")
			)
			(pin bidirectional line
				(at 22.86 17.78 180)
				(length 5.08)
				(name "PTA2")
				(number "23")
			)
			(pin bidirectional line
				(at 22.86 15.24 180)
				(length 5.08)
				(name "PTA3")
				(number "22")
			)
			(pin bidirectional line
				(at 22.86 12.7 180)
				(length 5.08)
				(name "PTA6")
				(number "21")
			)
			(pin bidirectional line
				(at 22.86 10.16 180)
				(length 5.08)
				(name "PTA7")
				(number "20")
			)
			(pin bidirectional line
				(at 22.86 5.08 180)
				(length 5.08)
				(name "PTB0")
				(number "19")
			)
			(pin bidirectional line
				(at 22.86 2.54 180)
				(length 5.08)
				(name "PTB1")
				(number "18")
			)
			(pin bidirectional line
				(at 22.86 0 180)
				(length 5.08)
				(name "PTB2")
				(number "17")
			)
			(pin bidirectional line
				(at 22.86 -2.54 180)
				(length 5.08)
				(name "PTB3")
				(number "15")
			)
			(pin bidirectional line
				(at 22.86 -5.08 180)
				(length 5.08)
				(name "PTB4")
				(number "10")
			)
			(pin bidirectional line
				(at 22.86 -7.62 180)
				(length 5.08)
				(name "PTB5")
				(number "8")
			)
			(pin bidirectional line
				(at 22.86 -12.7 180)
				(length 5.08)
				(name "PTD0")
				(number "2")
			)
			(pin bidirectional line
				(at 22.86 -15.24 180)
				(length 5.08)
				(name "PTD1")
				(number "3")
			)
			(pin bidirectional line
				(at 22.86 -17.78 180)
				(length 5.08)
				(name "PTD2")
				(number "32")
			)
			(pin bidirectional line
				(at 22.86 -20.32 180)
				(length 5.08)
				(name "PTD3")
				(number "9")
			)
			(pin bidirectional line
				(at 22.86 -22.86 180)
				(length 5.08)
				(name "PTD4")
				(number "16")
			)
			(pin bidirectional line
				(at 22.86 -25.4 180)
				(length 5.08)
				(name "PTD5")
				(number "25")
			)
		)
		(embedded_fonts no)
	)
	(symbol "MC9S08AC16xFDE"
		(extends "MC9S08AC128xFDE")
		(property "Reference" "IC"
			(at -22.86 44.45 0)
		)
		(property "Value" "MC9S08AC16xFDE"
			(at 24.13 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC16.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 16kB Flash, 1kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC16xFGE"
		(extends "MC9S08AC128xFGE")
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08AC16xFGE"
			(at 24.13 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC16.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 16kB Flash, 1kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC16xFJE"
		(extends "MC9S08AC60xFJE")
		(property "Reference" "IC"
			(at -22.86 29.21 0)
		)
		(property "Value" "MC9S08AC16xFJE"
			(at 22.86 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 10.16 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC16.pdf"
			(at 2.54 11.43 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 16kB Flash, 1kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC32xFDE"
		(extends "MC9S08AC128xFDE")
		(property "Reference" "IC"
			(at -22.86 44.45 0)
		)
		(property "Value" "MC9S08AC32xFDE"
			(at 24.13 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 32kB Flash, 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC32xFGE"
		(extends "MC9S08AC128xFGE")
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08AC32xFGE"
			(at 24.13 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 32kB Flash, 2kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC32xFJE"
		(extends "MC9S08AC60xFJE")
		(property "Reference" "IC"
			(at -22.86 29.21 0)
		)
		(property "Value" "MC9S08AC32xFJE"
			(at 22.86 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 10.16 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 11.43 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 32kB Flash, 2kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC32xFUE"
		(extends "MC9S08AC128xFUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AC32xFUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_14x14mm_P0.8mm"
			(at 10.16 -46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 32kB Flash, 2kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC32xPUE"
		(extends "MC9S08AC128xPUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AC32xPUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 32kB Flash, 2kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC48xFDE"
		(extends "MC9S08AC128xFDE")
		(property "Reference" "IC"
			(at -22.86 44.45 0)
		)
		(property "Value" "MC9S08AC48xFDE"
			(at 24.13 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 48kB Flash, 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC48xFGE"
		(extends "MC9S08AC128xFGE")
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08AC48xFGE"
			(at 24.13 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 48kB Flash, 2kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC48xFJE"
		(extends "MC9S08AC60xFJE")
		(property "Reference" "IC"
			(at -22.86 29.21 0)
		)
		(property "Value" "MC9S08AC48xFJE"
			(at 22.86 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 10.16 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 11.43 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 48kB Flash, 2kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC48xFUE"
		(extends "MC9S08AC128xFUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AC48xFUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_14x14mm_P0.8mm"
			(at 10.16 -46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 48kB Flash, 2kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC48xPUE"
		(extends "MC9S08AC128xPUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AC48xPUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 48kB Flash, 2kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC60xFDE"
		(extends "MC9S08AC128xFDE")
		(property "Reference" "IC"
			(at -22.86 44.45 0)
		)
		(property "Value" "MC9S08AC60xFDE"
			(at 24.13 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 60kB Flash, 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC60xFGE"
		(extends "MC9S08AC128xFGE")
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08AC60xFGE"
			(at 24.13 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 60kB Flash, 2kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC60xFUE"
		(extends "MC9S08AC128xFUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AC60xFUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_14x14mm_P0.8mm"
			(at 10.16 -46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 60kB Flash, 2kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC60xPUE"
		(extends "MC9S08AC128xPUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AC60xPUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 60kB Flash, 2kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC8xFDE"
		(extends "MC9S08AC128xFDE")
		(property "Reference" "IC"
			(at -22.86 44.45 0)
		)
		(property "Value" "MC9S08AC8xFDE"
			(at 24.13 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC16.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 8kB Flash, 768B RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC8xFGE"
		(extends "MC9S08AC128xFGE")
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08AC8xFGE"
			(at 24.13 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC16.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 8kB Flash, 768B RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC8xFJE"
		(extends "MC9S08AC60xFJE")
		(property "Reference" "IC"
			(at -22.86 29.21 0)
		)
		(property "Value" "MC9S08AC8xFJE"
			(at 22.86 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 10.16 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC16.pdf"
			(at 2.54 11.43 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 8kB Flash, 768B RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC96xFDE"
		(extends "MC9S08AC128xFDE")
		(property "Reference" "IC"
			(at -22.86 44.45 0)
		)
		(property "Value" "MC9S08AC96xFDE"
			(at 24.13 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC128.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 96kB Flash, 6kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC96xFGE"
		(extends "MC9S08AC128xFGE")
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08AC96xFGE"
			(at 24.13 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC128.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 96kB Flash, 6kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC96xFUE"
		(extends "MC9S08AC128xFUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AC96xFUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_14x14mm_P0.8mm"
			(at 10.16 -46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC128.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 96kB Flash, 6kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC96xLKE"
		(extends "MC9S08AC128xLKE")
		(property "Reference" "IC"
			(at -22.86 59.69 0)
		)
		(property "Value" "MC9S08AC96xLKE"
			(at 22.86 59.69 0)
		)
		(property "Footprint" "Package_QFP:LQFP-80_12x12mm_P0.5mm"
			(at 10.16 -59.69 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC128.pdf"
			(at 2.54 35.56 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 96kB Flash, 6kB RAM, LQFP-80"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*12x12mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AC96xPUE"
		(extends "MC9S08AC128xPUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AC96xPUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC128.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit Flexis Microcontroller, S08 core, 96kB Flash, 6kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW16AE0xLC"
		(extends "MC9S08AC60xFJE")
		(property "Reference" "IC"
			(at -22.86 29.21 0)
		)
		(property "Value" "MC9S08AW16AE0xLC"
			(at 22.86 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 10.16 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 11.43 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 96kB Flash, 6kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW16xFDE"
		(extends "MC9S08AC128xFDE")
		(property "Reference" "IC"
			(at -22.86 44.45 0)
		)
		(property "Value" "MC9S08AW16xFDE"
			(at 24.13 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 16kB Flash, 1kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW16xFGE"
		(extends "MC9S08AC128xFGE")
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08AW16xFGE"
			(at 24.13 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 16kB Flash, 1kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW16xFUE"
		(extends "MC9S08AC128xFUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AW16xFUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_14x14mm_P0.8mm"
			(at 10.16 -46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 16kB Flash, 1kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW16xPUE"
		(extends "MC9S08AC128xPUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AW16xPUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 16kB Flash, 1kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW32xFDE"
		(extends "MC9S08AC128xFDE")
		(property "Reference" "IC"
			(at -22.86 44.45 0)
		)
		(property "Value" "MC9S08AW32xFDE"
			(at 24.13 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 32kB Flash, 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW32xFGE"
		(extends "MC9S08AC128xFGE")
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08AW32xFGE"
			(at 24.13 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 32kB Flash, 2kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW32xFUE"
		(extends "MC9S08AC128xFUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AW32xFUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_14x14mm_P0.8mm"
			(at 10.16 -46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 32kB Flash, 2kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW32xPUE"
		(extends "MC9S08AC128xPUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AW32xPUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 32kB Flash, 2kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW48xFDE"
		(extends "MC9S08AC128xFDE")
		(property "Reference" "IC"
			(at -22.86 44.45 0)
		)
		(property "Value" "MC9S08AW48xFDE"
			(at 24.13 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 48kB Flash, 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW48xFGE"
		(extends "MC9S08AC128xFGE")
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08AW48xFGE"
			(at 24.13 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 48kB Flash, 2kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW48xFUE"
		(extends "MC9S08AC128xFUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AW48xFUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_14x14mm_P0.8mm"
			(at 10.16 -46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 48kB Flash, 2kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW48xPUE"
		(extends "MC9S08AC128xPUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AW48xPUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 48kB Flash, 2kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW60xFDE"
		(extends "MC9S08AC128xFDE")
		(property "Reference" "IC"
			(at -22.86 44.45 0)
		)
		(property "Value" "MC9S08AW60xFDE"
			(at 24.13 44.45 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -44.45 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 60kB Flash, 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW60xFGE"
		(extends "MC9S08AC128xFGE")
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08AW60xFGE"
			(at 24.13 41.91 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 20.32 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 60kB Flash, 2kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW60xFUE"
		(extends "MC9S08AC128xFUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AW60xFUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_14x14mm_P0.8mm"
			(at 10.16 -46.99 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 60kB Flash, 2kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW60xPUE"
		(extends "MC9S08AC128xPUE")
		(property "Reference" "IC"
			(at -22.86 46.99 0)
		)
		(property "Value" "MC9S08AW60xPUE"
			(at 22.86 46.99 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AW60.pdf"
			(at 2.54 22.86 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 60kB Flash, 2kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08AW8AE0xLC"
		(extends "MC9S08AC60xFJE")
		(property "Reference" "IC"
			(at -22.86 29.21 0)
		)
		(property "Value" "MC9S08AW8AE0xLC"
			(at 22.86 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 10.16 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08AC60.pdf"
			(at 2.54 11.43 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 8kB Flash, 768B RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DN16xLC"
		(extends "MC9S08DZ60xLC")
		(property "Reference" "IC"
			(at -20.32 29.21 0)
		)
		(property "Value" "MC9S08DN16xLC"
			(at 20.32 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 7.62 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 16kB Flash, 1kB RAM, 1kB EEPROM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DN16xLF"
		(extends "MC9S08DZ128xLF")
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DN16xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 16kB Flash, 1kB RAM, 1kB EEPROM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DN32xLC"
		(extends "MC9S08DZ60xLC")
		(property "Reference" "IC"
			(at -20.32 29.21 0)
		)
		(property "Value" "MC9S08DN32xLC"
			(at 20.32 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 7.62 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 32kB Flash, 1.5kB RAM, 1kB EEPROM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DN32xLF"
		(extends "MC9S08DZ128xLF")
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DN32xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 32kB Flash, 1.5kB RAM, 1kB EEPROM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DN32xLH"
		(extends "MC9S08DZ128xLH")
		(property "Reference" "IC"
			(at -22.86 49.53 0)
		)
		(property "Value" "MC9S08DN32xLH"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DN60.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 32kB Flash, 1.5kB RAM, 1kB EEPROM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DN48xLC"
		(extends "MC9S08DZ60xLC")
		(property "Reference" "IC"
			(at -20.32 29.21 0)
		)
		(property "Value" "MC9S08DN48xLC"
			(at 20.32 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 7.62 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 48kB Flash, 2kB RAM, 1.5kB EEPROM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DN48xLF"
		(extends "MC9S08DZ128xLF")
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DN48xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 48kB Flash, 2kB RAM, 1.5kB EEPROM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DN48xLH"
		(extends "MC9S08DZ128xLH")
		(property "Reference" "IC"
			(at -22.86 49.53 0)
		)
		(property "Value" "MC9S08DN48xLH"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DN60.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 48kB Flash, 2kB RAM, 1.5kB EEPROM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DN60xLC"
		(extends "MC9S08DZ60xLC")
		(property "Reference" "IC"
			(at -20.32 29.21 0)
		)
		(property "Value" "MC9S08DN60xLC"
			(at 20.32 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 7.62 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 60kB Flash, 2kB RAM, 2kB EEPROM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DN60xLF"
		(extends "MC9S08DZ128xLF")
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DN60xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 60kB Flash, 2kB RAM, 2kB EEPROM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DN60xLH"
		(extends "MC9S08DZ128xLH")
		(property "Reference" "IC"
			(at -22.86 49.53 0)
		)
		(property "Value" "MC9S08DN60xLH"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DN60.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 60kB Flash, 2kB RAM, 2kB EEPROM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DV16xLC"
		(extends "MC9S08DZ60xLC")
		(property "Reference" "IC"
			(at -20.32 29.21 0)
		)
		(property "Value" "MC9S08DV16xLC"
			(at 20.32 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 7.62 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 16kB Flash, 1kB RAM, 512B EEPROM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DV16xLF"
		(extends "MC9S08DZ128xLF")
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DV16xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 16kB Flash, 1kB RAM, 512B EEPROM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DV32xLC"
		(extends "MC9S08DZ60xLC")
		(property "Reference" "IC"
			(at -20.32 29.21 0)
		)
		(property "Value" "MC9S08DV32xLC"
			(at 20.32 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 7.62 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 32kB Flash, 1kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DV32xLF"
		(extends "MC9S08DZ128xLF")
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DV32xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 32kB Flash, 1kB RAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DV32xLH"
		(extends "MC9S08DZ128xLH")
		(property "Reference" "IC"
			(at -22.86 49.53 0)
		)
		(property "Value" "MC9S08DV32xLH"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DV60.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 32kB Flash, 1kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DV48xLC"
		(extends "MC9S08DZ60xLC")
		(property "Reference" "IC"
			(at -20.32 29.21 0)
		)
		(property "Value" "MC9S08DV48xLC"
			(at 20.32 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 7.62 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 48kB Flash, 3kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DV48xLF"
		(extends "MC9S08DZ128xLF")
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DV48xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 48kB Flash, 3kB RAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DV48xLH"
		(extends "MC9S08DZ128xLH")
		(property "Reference" "IC"
			(at -22.86 49.53 0)
		)
		(property "Value" "MC9S08DV48xLH"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DV60.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 48kB Flash, 3kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DV60xLC"
		(extends "MC9S08DZ60xLC")
		(property "Reference" "IC"
			(at -20.32 29.21 0)
		)
		(property "Value" "MC9S08DV60xLC"
			(at 20.32 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 7.62 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 60kB Flash, 3kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DV60xLF"
		(extends "MC9S08DZ128xLF")
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DV60xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 60kB Flash, 3kB RAM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DV60xLH"
		(extends "MC9S08DZ128xLH")
		(property "Reference" "IC"
			(at -22.86 49.53 0)
		)
		(property "Value" "MC9S08DV60xLH"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DV60.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 60kB Flash, 3kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DZ16xLC"
		(extends "MC9S08DZ60xLC")
		(property "Reference" "IC"
			(at -20.32 29.21 0)
		)
		(property "Value" "MC9S08DZ16xLC"
			(at 20.32 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 7.62 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 16kB Flash, 1kB RAM, 512B EEPROM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DZ16xLF"
		(extends "MC9S08DZ128xLF")
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DZ16xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 16kB Flash, 1kB RAM, 512B EEPROM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DZ32xLC"
		(extends "MC9S08DZ60xLC")
		(property "Reference" "IC"
			(at -20.32 29.21 0)
		)
		(property "Value" "MC9S08DZ32xLC"
			(at 20.32 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 7.62 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 32kB Flash, 2kB RAM, 1kB EEPROM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DZ32xLF"
		(extends "MC9S08DZ128xLF")
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DZ32xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 32kB Flash, 2kB RAM, 1kB EEPROM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DZ32xLH"
		(extends "MC9S08DZ128xLH")
		(property "Reference" "IC"
			(at -22.86 49.53 0)
		)
		(property "Value" "MC9S08DZ32xLH"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 32kB Flash, 2kB RAM, 1kB EEPROM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DZ48xLC"
		(extends "MC9S08DZ60xLC")
		(property "Reference" "IC"
			(at -20.32 29.21 0)
		)
		(property "Value" "MC9S08DZ48xLC"
			(at 20.32 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 7.62 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 48kB Flash, 3kB RAM, 1.5kB EEPROM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DZ48xLF"
		(extends "MC9S08DZ128xLF")
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DZ48xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 48kB Flash, 3kB RAM, 1.5kB EEPROM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DZ48xLH"
		(extends "MC9S08DZ128xLH")
		(property "Reference" "IC"
			(at -22.86 49.53 0)
		)
		(property "Value" "MC9S08DZ48xLH"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 48kB Flash, 3kB RAM, 1.5kB EEPROM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DZ60xLF"
		(extends "MC9S08DZ128xLF")
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DZ60xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 60kB Flash, 4kB RAM, 2kB EEPROM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DZ60xLH"
		(extends "MC9S08DZ128xLH")
		(property "Reference" "IC"
			(at -22.86 49.53 0)
		)
		(property "Value" "MC9S08DZ60xLH"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ60.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 60kB Flash, 4kB RAM, 2kB EEPROM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DZ96xLF"
		(extends "MC9S08DZ128xLF")
		(property "Reference" "IC"
			(at -22.86 39.37 0)
		)
		(property "Value" "MC9S08DZ96xLF"
			(at 22.86 39.37 0)
		)
		(property "Footprint" "Package_QFP:LQFP-48_7x7mm_P0.5mm"
			(at 10.16 -39.37 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ128.pdf"
			(at 2.54 15.24 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 96kB Flash, 6kB RAM, 2kB EEPROM, LQFP-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DZ96xLH"
		(extends "MC9S08DZ128xLH")
		(property "Reference" "IC"
			(at -22.86 49.53 0)
		)
		(property "Value" "MC9S08DZ96xLH"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ128.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 96kB Flash, 6kB RAM, 2kB EEPROM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08DZ96xLL"
		(extends "MC9S08DZ128xLL")
		(property "Reference" "IC"
			(at -22.86 72.39 0)
		)
		(property "Value" "MC9S08DZ96xLL"
			(at 22.86 72.39 0)
		)
		(property "Footprint" "Package_QFP:LQFP-100_14x14mm_P0.5mm"
			(at 10.16 -72.39 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08DZ128.pdf"
			(at 2.54 48.26 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 96kB Flash, 6kB RAM, 2kB EEPROM, LQFP-100"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*14x14mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08EL16xTJ"
		(extends "MC9S08EL32xTJ")
		(property "Reference" "IC"
			(at -16.51 21.59 0)
		)
		(property "Value" "MC9S08EL16xTJ"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08EL32.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit EEPROM with LIN Microcontroller, S08 core, 16kB Flash, 1kB RAM, 512B EEPROM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08EL16xTL"
		(extends "MC9S08EL32xTL")
		(property "Reference" "IC"
			(at -19.05 24.13 0)
		)
		(property "Value" "MC9S08EL16xTL"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 6.35 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08EL32.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit EEPROM with LIN Microcontroller, S08 core, 16kB Flash, 1kB RAM, 512B EEPROM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08FL8xLC"
		(extends "MC9S08FL16xLC")
		(property "Reference" "IC"
			(at -17.78 31.75 0)
		)
		(property "Value" "MC9S08FL8xLC"
			(at 17.78 31.75 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 5.08 -31.75 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08FL16RM.pdf"
			(at 2.54 7.62 0)
		)
		(property "Description" "8-bit Cost-Effective Microcontroller, S08 core, 8kB Flash, 768B RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08JM16xGT"
		(extends "MC9S08JM60xGT")
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08JM16xGT"
			(at 22.86 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08JM16.pdf"
			(at 2.54 17.78 0)
		)
		(property "Description" "8-bit USB Cost-Effective Microcontroller, S08 core, 16kB Flash, 1kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08JM16xLD"
		(extends "MC9S08JM60xLD")
		(property "Reference" "IC"
			(at -22.86 36.83 0)
		)
		(property "Value" "MC9S08JM16xLD"
			(at 22.86 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -36.83 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08JM16.pdf"
			(at 2.54 12.7 0)
		)
		(property "Description" "8-bit USB Cost-Effective Microcontroller, S08 core, 16kB Flash, 1kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08JM32xGT"
		(extends "MC9S08JM60xGT")
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08JM32xGT"
			(at 22.86 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08JM60.pdf"
			(at 2.54 17.78 0)
		)
		(property "Description" "8-bit USB Cost-Effective Microcontroller, S08 core, 32kB Flash, 2kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08JM32xLD"
		(extends "MC9S08JM60xLD")
		(property "Reference" "IC"
			(at -22.86 36.83 0)
		)
		(property "Value" "MC9S08JM32xLD"
			(at 22.86 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -36.83 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08JM60.pdf"
			(at 2.54 12.7 0)
		)
		(property "Description" "8-bit USB Cost-Effective Microcontroller, S08 core, 32kB Flash, 2kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08JM32xLH"
		(extends "MC9S08JM60xLH")
		(property "Reference" "IC"
			(at -22.86 49.53 0)
		)
		(property "Value" "MC9S08JM32xLH"
			(at 22.86 49.53 0)
		)
		(property "Footprint" "Package_QFP:LQFP-64_10x10mm_P0.5mm"
			(at 10.16 -49.53 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08JM60.pdf"
			(at 2.54 25.4 0)
		)
		(property "Description" "8-bit USB Cost-Effective Microcontroller, S08 core, 32kB Flash, 2kB RAM, LQFP-64"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08JM8xGT"
		(extends "MC9S08JM60xGT")
		(property "Reference" "IC"
			(at -22.86 41.91 0)
		)
		(property "Value" "MC9S08JM8xGT"
			(at 22.86 41.91 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.15x5.15mm"
			(at 10.16 -41.91 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08JM16.pdf"
			(at 2.54 17.78 0)
		)
		(property "Description" "8-bit USB Cost-Effective Microcontroller, S08 core, 8kB Flash, 1kB RAM, QFN-48"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*7x7mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08JM8xLC"
		(extends "MC9S08JM16xLC")
		(property "Reference" "IC"
			(at -22.86 31.75 0)
		)
		(property "Value" "MC9S08JM8xLC"
			(at 22.86 31.75 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 10.16 -31.75 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08JM16.pdf"
			(at 2.54 7.62 0)
		)
		(property "Description" "8-bit USB Cost-Effective Microcontroller, S08 core, 8kB Flash, 1kB RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08JM8xLD"
		(extends "MC9S08JM60xLD")
		(property "Reference" "IC"
			(at -22.86 36.83 0)
		)
		(property "Value" "MC9S08JM8xLD"
			(at 22.86 36.83 0)
		)
		(property "Footprint" "Package_QFP:LQFP-44_10x10mm_P0.8mm"
			(at 10.16 -36.83 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08JM16.pdf"
			(at 2.54 12.7 0)
		)
		(property "Description" "8-bit USB Cost-Effective Microcontroller, S08 core, 8kB Flash, 1kB RAM, LQFP-44"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*10x10mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08JS8CFK"
		(extends "MC9S08JS16CFK")
		(property "Reference" "IC"
			(at -19.05 24.13 0)
		)
		(property "Value" "MC9S08JS8CFK"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 6.35 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08JS16RM.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit USB Microcontroller, S08 core, 8kB Flash, 512B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08JS8CWJ"
		(extends "MC9S08JS16CWJ")
		(property "Reference" "IC"
			(at -19.05 24.13 0)
		)
		(property "Value" "MC9S08JS8CWJ"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 6.35 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08JS16RM.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit USB Microcontroller, S08 core, 8kB Flash, 512B RAM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08QA2CDNE"
		(extends "MC9S08QA4CDNE")
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QA2CDNE"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08QA4RM.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 2kB Flash, 160B RAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08QA2CFQE"
		(extends "MC9S08QA4CFQE")
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QA2CFQE"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_4x4mm_P0.8mm_EP2.5x3.6mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08QA4RM.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 2kB Flash, 160B RAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08QA2CPAE"
		(extends "MC9S08QA4CPAE")
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QA2CPAE"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08QA4RM.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 2kB Flash, 160B RAM, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08QB4xGK"
		(extends "MC9S08QB8xGK")
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08QB4xGK"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_5x5mm_P0.65mm_EP3.6x3.6mm"
			(at 7.62 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08QB8RM.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 4kB Flash, 256B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*1EP*5x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08QB4xTG"
		(extends "MC9S08QB8xTG")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08QB4xTG"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 6.35 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08QB8RM.pdf"
			(at 0 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 4kB Flash, 256B RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08QB4xWL"
		(extends "MC9S08QB8xWL")
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08QB4xWL"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 7.62 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08QB8RM.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 4kB Flash, 256B RAM, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08QD2xPC"
		(extends "MC9S08QD4xPC")
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QD2xPC"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QD4.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 2kB Flash, 128B RAM, DIP-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08QD2xSC"
		(extends "MC9S08QD4xSC")
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QD2xSC"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QD4.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 2kB Flash, 128B RAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08QG4xDNE"
		(extends "MC9S08QG8xDNE")
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QG4xDNE"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 5.08 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QG8.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08QG4xDTE"
		(extends "MC9S08QG8xDTE")
		(property "Reference" "IC"
			(at -17.78 19.05 0)
		)
		(property "Value" "MC9S08QG4xDTE"
			(at 1.27 19.05 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 5.08 -19.05 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QG8.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08QG4xFKE"
		(extends "MC9S08QG8xFKE")
		(property "Reference" "IC"
			(at -17.78 19.05 0)
		)
		(property "Value" "MC9S08QG4xFKE"
			(at 1.27 19.05 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 5.08 -19.05 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QG8.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08QG4xFQE"
		(extends "MC9S08QG8xFQE")
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08QG4xFQE"
			(at 1.27 11.43 0)
		)
		(property "Footprint" "Package_DFN_QFN:DFN-8-1EP_4x4mm_P0.8mm_EP2.5x3.6mm"
			(at 5.08 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08QG8.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, DFN-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DFN*4x4mm*P0.8mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SE4xRL"
		(extends "MC9S08SE8xRL")
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08SE4xRL"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_DIP:DIP-28_W15.24mm"
			(at 7.62 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08SE8RM.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 4kB Flash, 256B RAM, DIP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*15.24mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SE4xTG"
		(extends "MC9S08SE8xTG")
		(property "Reference" "IC"
			(at -17.78 16.51 0)
		)
		(property "Value" "MC9S08SE4xTG"
			(at 17.78 16.51 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 5.08 -16.51 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08SE8RM.pdf"
			(at 0 -10.16 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 4kB Flash, 256B RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SE4xWL"
		(extends "MC9S08SE8xWL")
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08SE4xWL"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 7.62 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08SE8RM.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 4kB Flash, 256B RAM, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SG16xTG"
		(extends "MC9S08SG32xTG")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SG16xTG"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SG32.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 16kB Flash, 1kB RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SG16xTJ"
		(extends "MC9S08SG32xTJ")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SG16xTJ"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SG32.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 16kB Flash, 1kB RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SG16xTL"
		(extends "MC9S08SG32xTL")
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08SG16xTL"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 5.08 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SG32.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 16kB Flash, 1kB RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SG4xSC"
		(extends "MC9S08SG8xSC")
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08SG4xSC"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SG8.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SG4xTG"
		(extends "MC9S08SG32xTG")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SG4xTG"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SG8.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SG4xTJ"
		(extends "MC9S08SG32xTJ")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SG4xTJ"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SG8.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 4kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SG8xTG"
		(extends "MC9S08SG32xTG")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SG8xTG"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SG8.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 8kB Flash, 512B RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SG8xTJ"
		(extends "MC9S08SG32xTJ")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SG8xTJ"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SG8.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit Small Package Microcontroller, S08 core, 8kB Flash, 512B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SH16xTG"
		(extends "MC9S08SH32xTG")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SH16xTG"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH32.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 16kB Flash, 1kB RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SH16xTJ"
		(extends "MC9S08SH32xTJ")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SH16xTJ"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH32.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 16kB Flash, 1kB RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SH16xTL"
		(extends "MC9S08SH32xTL")
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08SH16xTL"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 5.08 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH32.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 16kB Flash, 1kB RAM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SH16xWL"
		(extends "MC9S08SH32xWL")
		(property "Reference" "IC"
			(at -20.32 24.13 0)
		)
		(property "Value" "MC9S08SH16xWL"
			(at 20.32 24.13 0)
		)
		(property "Footprint" "Package_SO:SOIC-28W_7.5x17.9mm_P1.27mm"
			(at 5.08 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH32.pdf"
			(at 2.54 0 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 16kB Flash, 1kB RAM, SOIC-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x17.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SH4xFK"
		(extends "MC9S08SH8xFK")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SH4xFK"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_DFN_QFN:QFN-24-1EP_4x4mm_P0.5mm_EP2.6x2.6mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH8.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 4kB Flash, 256B RAM, QFN-24"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "QFN*4x4mm*P0.5mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SH4xPJ"
		(extends "MC9S08SH8xPJ")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SH4xPJ"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_DIP:DIP-20_W7.62mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH8.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 4kB Flash, 256B RAM, DIP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "DIP*7.62mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SH4xSC"
		(extends "MC9S08SH8xSC")
		(property "Reference" "IC"
			(at -17.78 11.43 0)
		)
		(property "Value" "MC9S08SH4xSC"
			(at 17.78 11.43 0)
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 2.54 -11.43 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH8.pdf"
			(at 2.54 -15.24 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 4kB Flash, 256B RAM, SOIC-8"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SH4xTG"
		(extends "MC9S08SH32xTG")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SH4xTG"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH8.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 4kB Flash, 256B RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SH4xTJ"
		(extends "MC9S08SH32xTJ")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SH4xTJ"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH8.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 4kB Flash, 256B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SH4xWJ"
		(extends "MC9S08SH8xWJ")
		(property "Reference" "IC"
			(at -17.78 19.05 0)
		)
		(property "Value" "MC9S08SH4xWJ"
			(at 17.78 19.05 0)
		)
		(property "Footprint" "Package_SO:SOIC-20W_7.5x12.8mm_P1.27mm"
			(at 2.54 -19.05 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH8.pdf"
			(at 2.54 -5.08 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 4kB Flash, 256B RAM, SOIC-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "SOIC*7.5x12.8mm*P1.27mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SH8xTG"
		(extends "MC9S08SH32xTG")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SH8xTG"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-16_4.4x5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH8.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 8kB Flash, 512B RAM, TSSOP-16"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SH8xTJ"
		(extends "MC9S08SH32xTJ")
		(property "Reference" "IC"
			(at -17.78 21.59 0)
		)
		(property "Value" "MC9S08SH8xTJ"
			(at 17.78 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08SH8.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit General Purpose Microcontroller, S08 core, 8kB Flash, 512B RAM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SL16xTJ"
		(extends "MC9S08EL32xTJ")
		(property "Reference" "IC"
			(at -16.51 21.59 0)
		)
		(property "Value" "MC9S08SL16xTJ"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08EL32.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit EEPROM with LIN Microcontroller, S08 core, 16kB Flash, 512B RAM, 256B EEPROM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SL16xTL"
		(extends "MC9S08EL32xTL")
		(property "Reference" "IC"
			(at -19.05 24.13 0)
		)
		(property "Value" "MC9S08SL16xTL"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 6.35 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08EL32.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit EEPROM with LIN Microcontroller, S08 core, 16kB Flash, 512B RAM, 256B EEPROM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SL32xTJ"
		(extends "MC9S08EL32xTJ")
		(property "Reference" "IC"
			(at -16.51 21.59 0)
		)
		(property "Value" "MC9S08SL32xTJ"
			(at 7.62 21.59 0)
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 2.54 -21.59 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08EL32.pdf"
			(at 2.54 -2.54 0)
		)
		(property "Description" "8-bit EEPROM with LIN Microcontroller, S08 core, 32kB Flash, 512B RAM, 256B EEPROM, TSSOP-20"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x6.5mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SL32xTL"
		(extends "MC9S08EL32xTL")
		(property "Reference" "IC"
			(at -19.05 24.13 0)
		)
		(property "Value" "MC9S08SL32xTL"
			(at 5.08 24.13 0)
		)
		(property "Footprint" "Package_SO:TSSOP-28_4.4x9.7mm_P0.65mm"
			(at 6.35 -24.13 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/data-sheet/MC9S08EL32.pdf"
			(at 0 0 0)
		)
		(property "Description" "8-bit EEPROM with LIN Microcontroller, S08 core, 32kB Flash, 512B RAM, 256B EEPROM, TSSOP-28"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "TSSOP*4.4x9.7mm*P0.65mm*"
			(at 0 0 0)
		)
	)
	(symbol "MC9S08SV8CLC"
		(extends "MC9S08SV16CLC")
		(property "Reference" "IC"
			(at -17.78 29.21 0)
		)
		(property "Value" "MC9S08SV8CLC"
			(at 17.78 29.21 0)
		)
		(property "Footprint" "Package_QFP:LQFP-32_7x7mm_P0.8mm"
			(at 5.08 -29.21 0)
		)
		(property "Datasheet" "https://www.nxp.com/docs/en/reference-manual/MC9S08SV16RM.pdf"
			(at 2.54 5.08 0)
		)
		(property "Description" "8-bit General Purpose Best-in-Class performance Microcontroller, S08 core, 8kB Flash, 768B RAM, LQFP-32"
			(at 0 0 0)
		)
		(property "ki_keywords" "NXP S08 Microcontroller"
			(at 0 0 0)
		)
		(property "ki_fp_filters" "LQFP*7x7mm*P0.8mm*"
			(at 0 0 0)
		)
	)
)
